<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MEGA">
<description>Full Arduino MEGA footprint</description>
</package>
<package name="ARDUINO_MEGA-PRO-3.3V">
<description>Arduino Mega Pro footprint</description>
</package>
<package name="ARDUINO_MINI">
</package>
<package name="DUEMILANOVE_SHIELD">
</package>
<package name="DUEMILANOVE_VIAS">
</package>
<package name="DUEMILANOVE_SHIELD_NOHOLES">
</package>
<package name="DUEMILANOVE_SHIELD_LONGPADS">
</package>
<package name="DUEMILANOVE_SHIELD_NOLABELS">
</package>
<package name="DUEMILANOVE_SHIELD_NOHOLES_NOLABELS">
</package>
<package name="1X06-SMD">
</package>
<package name="1X06">
</package>
<package name="MOLEX-1X6-RA_LOCK">
</package>
<package name="1X06_LONGPADS">
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X06-KIT">
<description>&lt;h3&gt;1X06-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="BREADBOARD-MINI">
</package>
<package name="MICRO-SDCARD">
</package>
<package name="SD-MMC-CARD">
</package>
<package name="WIZ811MJ">
<description>&lt;h3&gt;WIZnet W5100 Network Module with MagJack - WIZ811MJ&lt;/h3&gt;
WIZnet's WIZ811MJ is a breakout board for the W5100 embedded TCP/IP chip. Also included on the board is a RJ-45 MagJack Connector (RJ45 with X'FMR).&lt;br&gt;&lt;br&gt;

See http://www.sparkfun.com/commerce/product_info.php?products_id=9473 for more documentation and info.&lt;br&gt;
&lt;B&gt;**UNPROVEN&lt;/b&gt;</description>
</package>
<package name="XPORT">
</package>
<package name="XPORT_DIRECT_MODULE">
</package>
<package name="XPORT_DIRECT_MODULE-SMD">
</package>
</packages>
<symbols>
<symbol name="ARDUINO-MEGA">
<pin name="5V@0"/>
<pin name="RESET"/>
<pin name="5V@1"/>
<pin name="A0(RX0)"/>
<pin name="A1(TX0)"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="1(TX0)"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="GND@4"/>
<pin name="16(TX2)"/>
<pin name="17(RX2)"/>
<pin name="18(TX1)"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="40"/>
<pin name="39"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="15(RX3)"/>
<pin name="14(TX3)"/>
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="53"/>
<pin name="52"/>
<pin name="51"/>
<pin name="50"/>
<pin name="49"/>
<pin name="5V@2"/>
<pin name="3.3V"/>
<pin name="AREF"/>
<pin name="21(SCL)"/>
<pin name="20(SDA)"/>
<pin name="19(RX1)"/>
<pin name="VIN"/>
<pin name="0(RX0)"/>
</symbol>
<symbol name="ARDUINO_MINI">
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="GND"/>
<pin name="GND2"/>
<pin name="RAW"/>
<pin name="RST"/>
<pin name="RST2"/>
<pin name="RX1"/>
<pin name="TX0"/>
<pin name="VCC"/>
</symbol>
<symbol name="ARDUINO_SHIELD">
<pin name="RX"/>
<pin name="TX"/>
<pin name="D2"/>
<pin name="*D3"/>
<pin name="D4"/>
<pin name="*D5"/>
<pin name="*D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="*D9"/>
<pin name="*D10"/>
<pin name="*D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VIN"/>
<pin name="RES"/>
<pin name="5V"/>
<pin name="AREF"/>
<pin name="GND@2"/>
<pin name="GND@1"/>
<pin name="GND@0"/>
<pin name="3.3V"/>
</symbol>
<symbol name="ARDUINO_SERIAL_PROGRAM">
<pin name="DTR" direction="pas"/>
<pin name="RXI" direction="pas"/>
<pin name="TXO" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="CTS" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="BREADBOARD">
</symbol>
<symbol name="MICRO-SDCARD">
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="GND"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
</symbol>
<symbol name="SD-MMC-CARD">
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VSS1"/>
<pin name="VDD"/>
<pin name="DAT1"/>
<pin name="DAT0"/>
<pin name="VSS2"/>
<pin name="CLK"/>
</symbol>
<symbol name="WIZ811MJ">
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="SCLK"/>
<pin name="/SCS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A7"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="/RD"/>
<pin name="/CS"/>
<pin name="/WR"/>
<pin name="/INT"/>
<pin name="D0"/>
<pin name="/RESET"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
</symbol>
<symbol name="XPORT">
<pin name="GND"/>
<pin name="3.3V"/>
<pin name="RST" function="dot"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="DTR"/>
<pin name="CTS"/>
</symbol>
<symbol name="XPORT_DIRECT">
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="3.3V"/>
<pin name="RST"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="DTR"/>
<pin name="CTS"/>
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="GND@24"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO-MEGA" prefix="U">
<description>Arduino Mega board footprint</description>
<gates>
<gate name="G$1" symbol="ARDUINO-MEGA"/>
</gates>
<devices>
<device name="FULL" package="ARDUINO_MEGA">
<connects>
<connect gate="G$1" pin="0(RX0)" pad="0"/>
<connect gate="G$1" pin="1(TX0)" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14(TX3)" pad="14"/>
<connect gate="G$1" pin="15(RX3)" pad="15"/>
<connect gate="G$1" pin="16(TX2)" pad="16"/>
<connect gate="G$1" pin="17(RX2)" pad="17"/>
<connect gate="G$1" pin="18(TX1)" pad="18"/>
<connect gate="G$1" pin="19(RX1)" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20(SDA)" pad="20"/>
<connect gate="G$1" pin="21(SCL)" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V@0" pad="5V@0"/>
<connect gate="G$1" pin="5V@1" pad="5V@1"/>
<connect gate="G$1" pin="5V@2" pad="5V@2"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A0(RX0)" pad="A0"/>
<connect gate="G$1" pin="A1(TX0)" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="GND@4" pad="GND@4"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PRO" package="ARDUINO_MEGA-PRO-3.3V">
<connects>
<connect gate="G$1" pin="0(RX0)" pad="0"/>
<connect gate="G$1" pin="1(TX0)" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14(TX3)" pad="14"/>
<connect gate="G$1" pin="15(RX3)" pad="15"/>
<connect gate="G$1" pin="16(TX2)" pad="16"/>
<connect gate="G$1" pin="17(RX2)" pad="17"/>
<connect gate="G$1" pin="18(TX1)" pad="18"/>
<connect gate="G$1" pin="19(RX1)" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20(SDA)" pad="20"/>
<connect gate="G$1" pin="21(SCL)" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V@0" pad="5V@0"/>
<connect gate="G$1" pin="5V@1" pad="5V@1"/>
<connect gate="G$1" pin="5V@2" pad="5V@2"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A0(RX0)" pad="A0"/>
<connect gate="G$1" pin="A1(TX0)" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="GND@4" pad="GND@4"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MINI">
<description>Arduino Pro Mini footprint</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MINI"/>
</gates>
<devices>
<device name="" package="ARDUINO_MINI">
<connects>
<connect gate="G$1" pin="10" pad="13"/>
<connect gate="G$1" pin="11" pad="14"/>
<connect gate="G$1" pin="12" pad="15"/>
<connect gate="G$1" pin="13" pad="16"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="A3" pad="20"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND2" pad="23"/>
<connect gate="G$1" pin="RAW" pad="24"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="RST2" pad="22"/>
<connect gate="G$1" pin="RX1" pad="2"/>
<connect gate="G$1" pin="TX0" pad="1"/>
<connect gate="G$1" pin="VCC" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_SHIELD" prefix="U">
<description>Arduino shield footprint</description>
<gates>
<gate name="G$1" symbol="ARDUINO_SHIELD"/>
</gates>
<devices>
<device name="LABEL" package="DUEMILANOVE_SHIELD">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="DUEMILANOVE_VIAS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLES" package="DUEMILANOVE_SHIELD_NOHOLES">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="DUEMILANOVE_SHIELD_LONGPADS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOLABELS" package="DUEMILANOVE_SHIELD_NOLABELS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLESORLABELS" package="DUEMILANOVE_SHIELD_NOHOLES_NOLABELS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREADBOARD">
<description>&lt;b&gt;Breadboard Mini Self Adhesive&lt;/b&gt;&lt;p&gt;
This is the mechnical outline for the very small self adhesive breadboard from SparkFun Electronics. Good for very small proto areas. SKU : PRT-07916</description>
<gates>
<gate name="G$1" symbol="BREADBOARD"/>
</gates>
<devices>
<device name="MINI" package="BREADBOARD-MINI">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO-SDCARD">
<description>MicroSD footprint- NOT a socket for a MicroSD card!</description>
<gates>
<gate name="G$1" symbol="MICRO-SDCARD"/>
</gates>
<devices>
<device name="" package="MICRO-SDCARD">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="CD/DAT3"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="DAT0" pad="DAT0"/>
<connect gate="G$1" pin="DAT1" pad="DAT1"/>
<connect gate="G$1" pin="DAT2" pad="DAT2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VDD" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD_MMC_CARD">
<description>Mechanical size of an SD/MMC card- NOT a socket!</description>
<gates>
<gate name="G$1" symbol="SD-MMC-CARD"/>
</gates>
<devices>
<device name="SD_PCB" package="SD-MMC-CARD">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIZ811MJ" prefix="U">
<description>&lt;h3&gt;WIZnet W5100 Network Module with MagJack - WIZ811MJ&lt;/h3&gt;
WIZnet's WIZ811MJ is a breakout board for the W5100 embedded TCP/IP chip. Also included on the board is a RJ-45 MagJack Connector (RJ45 with X'FMR).&lt;br&gt;&lt;br&gt;

See http://www.sparkfun.com/commerce/product_info.php?products_id=9473 for more documentation and info.&lt;br&gt;
&lt;B&gt;**UNPROVEN&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="WIZ811MJ"/>
</gates>
<devices>
<device name="" package="WIZ811MJ">
<connects>
<connect gate="G$1" pin="/CS" pad="27"/>
<connect gate="G$1" pin="/INT" pad="28"/>
<connect gate="G$1" pin="/RD" pad="26"/>
<connect gate="G$1" pin="/RESET" pad="22"/>
<connect gate="G$1" pin="/SCS" pad="24"/>
<connect gate="G$1" pin="/WR" pad="25"/>
<connect gate="G$1" pin="A0" pad="31"/>
<connect gate="G$1" pin="A1" pad="32"/>
<connect gate="G$1" pin="A10" pad="15"/>
<connect gate="G$1" pin="A11" pad="16"/>
<connect gate="G$1" pin="A12" pad="17"/>
<connect gate="G$1" pin="A13" pad="18"/>
<connect gate="G$1" pin="A14" pad="19"/>
<connect gate="G$1" pin="A2" pad="33"/>
<connect gate="G$1" pin="A3" pad="34"/>
<connect gate="G$1" pin="A4" pad="35"/>
<connect gate="G$1" pin="A5" pad="36"/>
<connect gate="G$1" pin="A6" pad="37"/>
<connect gate="G$1" pin="A7" pad="38"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="A9" pad="14"/>
<connect gate="G$1" pin="D0" pad="4"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="6"/>
<connect gate="G$1" pin="D3" pad="5"/>
<connect gate="G$1" pin="D4" pad="8"/>
<connect gate="G$1" pin="D5" pad="7"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="29"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="GND@4" pad="40"/>
<connect gate="G$1" pin="GND@5" pad="30"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="SCLK" pad="23"/>
<connect gate="G$1" pin="VCC@1" pad="12"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPORT">
<description>TCP/IP stack and phy in RJ-45 jack footprint</description>
<gates>
<gate name="G$1" symbol="XPORT"/>
</gates>
<devices>
<device name="" package="XPORT">
<connects>
<connect gate="G$1" pin="3.3V" pad="P2"/>
<connect gate="G$1" pin="CTS" pad="P8"/>
<connect gate="G$1" pin="DTR" pad="P7"/>
<connect gate="G$1" pin="GND" pad="P1"/>
<connect gate="G$1" pin="RST" pad="P3"/>
<connect gate="G$1" pin="RTS" pad="P6"/>
<connect gate="G$1" pin="RX" pad="P5"/>
<connect gate="G$1" pin="TX" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPORT-DIRECT">
<description>TCP/IP phy and stack module</description>
<gates>
<gate name="G$1" symbol="XPORT_DIRECT"/>
</gates>
<devices>
<device name="" package="XPORT_DIRECT_MODULE">
<connects>
<connect gate="G$1" pin="3.3V" pad="P3"/>
<connect gate="G$1" pin="CP1" pad="P23"/>
<connect gate="G$1" pin="CP2" pad="P21"/>
<connect gate="G$1" pin="CTS" pad="P15"/>
<connect gate="G$1" pin="DTR" pad="P13"/>
<connect gate="G$1" pin="GND@1" pad="P1"/>
<connect gate="G$1" pin="GND@2" pad="P2"/>
<connect gate="G$1" pin="GND@24" pad="P24"/>
<connect gate="G$1" pin="RST" pad="P5"/>
<connect gate="G$1" pin="RTS" pad="P11"/>
<connect gate="G$1" pin="RX" pad="P9"/>
<connect gate="G$1" pin="TX" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="XPORT_DIRECT_MODULE-SMD">
<connects>
<connect gate="G$1" pin="3.3V" pad="P3"/>
<connect gate="G$1" pin="CP1" pad="P23"/>
<connect gate="G$1" pin="CP2" pad="P21"/>
<connect gate="G$1" pin="CTS" pad="P15"/>
<connect gate="G$1" pin="DTR" pad="P13"/>
<connect gate="G$1" pin="GND@1" pad="P1"/>
<connect gate="G$1" pin="GND@2" pad="P2"/>
<connect gate="G$1" pin="GND@24" pad="P24"/>
<connect gate="G$1" pin="RST" pad="P5"/>
<connect gate="G$1" pin="RTS" pad="P11"/>
<connect gate="G$1" pin="RX" pad="P9"/>
<connect gate="G$1" pin="TX" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
