<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
<package name="0805">
</package>
<package name="CAP-PTH-LARGE">
</package>
<package name="GRM43D">
</package>
<package name="0603-CAP">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CAP-PTH-5MM">
</package>
<package name="AXIAL-5MM">
</package>
<package name="1210">
</package>
<package name="1206">
</package>
<package name="CTZ3">
<description>CTZ3 Series land pattern for variable capacitor - CTZ3E-50C-W1-PF</description>
</package>
<package name="CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="EIA3216">
</package>
<package name="EIA3528">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="EIA7343">
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="NIPPON_F80">
</package>
<package name="PANASONIC_D">
</package>
<package name="CPOL-RADIAL-1000UF-63V">
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
<package name="VISHAY_C">
</package>
<package name="PANASONIC_H13">
</package>
<package name="EIA6032">
</package>
<package name="EN_J2">
<description>Type J2 package for SMD supercap PRT-10317 (p# EEC-EN0F204J2)</description>
</package>
<package name="EIA3528-KIT">
<description>&lt;h3&gt;EIA3528-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
<package name="EIA3216-KIT">
<description>&lt;h3&gt;EIA3216-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
<package name="0603">
</package>
<package name="FUSE_5MM">
</package>
<package name="INDUCTOR-1206">
</package>
<package name="CR54">
</package>
<package name="CDRH125">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="B82462G">
</package>
<package name="CR75">
</package>
<package name="1007">
<description>1007 (2518 metric) package</description>
</package>
<package name="COOPER_UP4B">
</package>
<package name="CDRH3D28">
</package>
<package name="CR75_V2">
</package>
<package name="CDRH2D09">
<description>1.3x1.3mm 1.7mm between. Fits Sumida CDRH2D09, CDRH2D18 inductor</description>
</package>
<package name="NPI75C">
</package>
<package name="SRU5028">
</package>
<package name="SRU1038">
</package>
<package name="CR54-KIT">
</package>
<package name="1X02">
</package>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
<package name="1X02_LOCK">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_2S-NO-NS">
</package>
<package name="SJ_3">
</package>
<package name="1X03">
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="SJ_3_PASTE2&amp;3">
</package>
<package name="AXIAL-0.3">
</package>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-RES">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="R2512">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.8">
<description>2W Resistor, 0.8" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.3-KIT">
<description>&lt;h3&gt;AXIAL-0.3-KIT&lt;/h3&gt;

Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.3 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="RPACK-SIP-PTH-5">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="SJ_2S-NOTRACE">
</package>
<package name="SJ_2W">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="PAD.02X.02">
</package>
<package name="PAD.03X.03">
</package>
<package name="PAD.03X.05">
</package>
<package name="GND_CONNECT">
</package>
<package name="DR1030">
<description>For Coiltronics/Cooper DR1030 series inductors</description>
</package>
</packages>
<symbols>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP_ADJ">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor&lt;/b&gt;
Standard 0603 ceramic capacitor, and 0.1" leaded capacitor.</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="PTH" package="CAP-PTH-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CAP-PTH-SMALL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CAP-PTH-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="GRM43D">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-CAP" package="0603-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-CAP" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CAP-PTH-5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="AXIAL-5MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ASMD" package="CTZ3">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="CAP-PTH-SMALL-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EZ" package="CAP-PTH-SMALLEZ">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_ADJ" prefix="C">
<description>Variable, non-polarized capacitor</description>
<gates>
<gate name="G$1" symbol="CAP_ADJ"/>
</gates>
<devices>
<device name="SMD" package="CTZ3">
<connects>
<connect gate="G$1" pin="3" pad="+"/>
<connect gate="G$1" pin="4" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_POL" prefix="C" uservalue="yes">
<description>&lt;b&gt;Capacitor Polarized&lt;/b&gt;
These are standard SMD and PTH capacitors. Normally 10uF, 47uF, and 100uF in electrolytic and tantalum varieties. Always verify the external diameter of the through hole cap, it varies with capacity, voltage, and manufacturer. The EIA devices should be standard.</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="1206" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="CPOL-RADIAL-100UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="CPOL-RADIAL-10UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7343" package="EIA7343">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F80" package="NIPPON_F80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="CPOL-RADIAL-1000UF-63V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="CPOL-RADIAL-1000UF-25V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="VISHAY_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H13" package="PANASONIC_H13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6032" package="EIA6032">
<connects>
<connect gate="G$1" pin="+" pad="P$1"/>
<connect gate="G$1" pin="-" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EN_J2" package="EN_J2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528-KIT" package="EIA3528-KIT">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206-KIT" package="EIA3216-KIT">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name=".1UF-CER" prefix="C">
<description>.1uF ceramic SMT&lt;br&gt;
CAP-00810- 25V +80%/-20% (0603)&lt;br&gt;
CAP-08390- 100V 10% (0603)&lt;br&gt;
CAP-08604- 25V 5% (0603)&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="CAP-08604" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="CAP-08390" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08390"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2UF-CER" prefix="C">
<description>2.2uF Ceramic SMT&lt;BR&gt;
CAP-07888- 10V, 20% (0603)&lt;br&gt;
CAP-10009- 50V, 10% (1206)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="CAP-07888" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
<device name="CAP-10009" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10009"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name=".22UF-CER" prefix="C" uservalue="yes">
<description>.22uF ceramic SMT&lt;br&gt;
CAP-09885- 50V +80%/-20% (0603)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="VALUE" value=".22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="100UF-ELECT" prefix="C" uservalue="yes">
<description>100uF electrolytic SMT&lt;br&gt;
CAP-08362- 63V 20%</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="PANASONIC_H13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08362"/>
<attribute name="VALUE" value="100uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10NF-CER" prefix="C" uservalue="yes">
<description>10nF/.01uF/10000pF ceramic SMT&lt;br&gt;
CAP-00867- 50V 10% (0603)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00867"/>
<attribute name="VALUE" value="10nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10UF-TANT" prefix="C" uservalue="yes">
<description>10uF Tantalum SMT&lt;br&gt;
CAP-00811- 16V 10% (EIA-3216)</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="47UF-TANT" prefix="C" uservalue="yes">
<description>47uF Tantalum SMT&lt;br&gt;
CAP-08310- 10V 10% (EIA-3528)</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08310"/>
<attribute name="VALUE" value="47uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name=".47UF-16V(-20/+80%)(0805)" prefix="C" uservalue="yes">
<description>CAP-08139</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name=".68UF-16V-20%,+80%(0603)" prefix="C" uservalue="yes">
<description>CAP-08708</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.018UF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08494</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.01UF-1000V-10%(1812)" prefix="C" uservalue="yes">
<description>CAP-09114</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.1UF-100V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08390</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.1UF-25V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08604</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.1UF-25V(+80/-20%)(0603)" prefix="C" uservalue="yes">
<description>Ceramic&lt;br&gt;
Standard decoupling cap &lt;br&gt;
CAP-00810</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.1UF-50V-20%(PTH)" prefix="C" uservalue="yes">
<description>CAP-08370</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.22UF-25V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-07822</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.22UF-50V-?20%(ELECT)(PTH)" prefix="C" uservalue="yes">
<description>CAP-09998</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.22UF50V-20%,+80%(0603)" prefix="C" uservalue="yes">
<description>CAP-09885</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.2F-3.3V--20%,+80%(COIN)" prefix="C" uservalue="yes">
<description>CAP-10408</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.33UF-50V-10%(0805)" prefix="C" uservalue="yes">
<description>CAP-08469</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.33UF-50V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08617</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.47UF-25V--20%,+80%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09152</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.68UF-16V--20%,+80%(0603)" prefix="C" uservalue="yes">
<description>CAP-08723</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.75PF-50V(-/+.25PF)(0603)" prefix="C" uservalue="yes">
<description>CAP-07878</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.0PF-50V(-/+.25PF)(0603)" prefix="C" uservalue="yes">
<description>CAP-07879</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.0UF50V10%(1206)" prefix="C" uservalue="yes">
<description>CAP-09822</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.0UF-100V-10%(1206)" prefix="C" uservalue="yes">
<description>CAP-10742</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.0UF-16V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-00868</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.0UF-50V-20%-(ELECT)" prefix="C" uservalue="yes">
<description>CAP-10222</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.2PF-50V-20%(0603)" prefix="C" uservalue="yes">
<description>CAP-09201</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.5PF-50V(+/-.25PF)(0603)" prefix="C" uservalue="yes">
<description>CAP-08763</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1000UF-10V-20%(PTH)" prefix="C" uservalue="yes">
<description>CAP-08514</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1000UF-25V-20%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09538</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1000UF-25V(PTH)" prefix="C" uservalue="yes">
<description>CAP-08070</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100PF-200V-5%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09181</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-07883</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100UF-10V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-07890</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100UF-16V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08702</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100UF-25V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08498</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100UF-25V-20%(PTH)" prefix="C" uservalue="yes">
<description>CAP-08439</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100UF-35V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09297</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100UF-63V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08362</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="100UF6.3V20%(1210)" prefix="C" uservalue="yes">
<description>CAP-09827</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10NF-100V-10%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09183</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10NF(0.01UF/10,000PF)-1000V-10%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09321</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10NF/10000PF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-00867</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10PF-200V-5%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09180</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF-16V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-00811&lt;BR&gt;
1206/EIA-3216 Tantalum capacitor</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10UF-16V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09575</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF-20V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08063</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF-25V-20%(PTH)" prefix="C" uservalue="yes">
<description>CAP-08440</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF-6.3V-20%(1206)" prefix="C" uservalue="yes">
<description>Ceramic&lt;br&gt;
CAP-10057</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10057"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10UF-6.3V-20%(0603)" prefix="C" uservalue="yes">
<description>CAP-11015</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF10V10%(0805)" prefix="C" uservalue="yes">
<description>CAP-11330</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF50V20%(1210)" prefix="C" uservalue="yes">
<description>CAP-09824</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09824"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12NF-200V-10%(0805)" prefix="C" uservalue="yes">
<description>CAP-11056</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="12PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-09137</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="15000PF(15NF)-25V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08710</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="15NF-250V-10%(0805)" prefix="C" uservalue="yes">
<description>CAP-11077</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="15PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-07881</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="18PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08267</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1NF-100V-5%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09182</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1NF/1000PF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-07886</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1UF-25V-10%(0805)" prefix="C" uservalue="yes">
<description>CAP-08064</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1UF-35V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09577</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1UF-50V--20,+80%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09184</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="2.2NF/2200PF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-07877</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="2.2UF-10V-20%(0603)" prefix="C" uservalue="yes">
<description>CAP-07888</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="2.2UF-25V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08706</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="2.2UF50V10%(1206)" prefix="C" uservalue="yes">
<description>CAP-10009</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="220PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08722</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="220UF-16V-20%(PTH)" prefix="C" uservalue="yes">
<description>CAP-10898</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="220UF-16V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09578</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="22NF/22,000PF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-07885</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="22PF-200V-5%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09128</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="22PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-07876</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="22UF-16V-20%-(1210)" prefix="C" uservalue="yes">
<description>CAP-10381</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10381"/>
<attribute name="VALUE" value="22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22UF-16V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09576</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="22UF-35V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08618</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="22UF-6.3V-20%(0805)" prefix="C" uservalue="yes">
<description>Ceramic&lt;BR&gt;
CAP-08402</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE" value="22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27PF50V5%(0603)" prefix="C" uservalue="yes">
<description>CAP-09989</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.3NF-100V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-09633</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.3UF-80V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08365</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="330PF-25V-10%-(0603)" prefix="C" uservalue="yes">
<description>CAP-10108</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="33NF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-07887</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="33PF-50V-5%-(0603)" prefix="C" uservalue="yes">
<description>CAP-10142</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="33UF-16V-20%(TANT)" prefix="C" uservalue="yes">
<description>CAP-09017</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="33UF-50V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08826</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="390NF-10V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-10986</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="4.7NF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-11378</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="4.7PF-50V(-/+.25PF)(0603)" prefix="C" uservalue="yes">
<description>CAP-07880</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="4.7UF-16V-20%,+80%-(1206)" prefix="C" uservalue="yes">
<description>CAP-10300</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="4.7UF-35V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08313</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="4.7UF-6.3V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08280</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE" value="4.7uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="430PF-100V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08709</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="470NF-16V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-09041</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="470PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-07884</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="470UF-25V(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08700</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="470UF-6.3V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08408</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="470UF16V?20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-10043</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="470UF16V(PTH)" prefix="C" uservalue="yes">
<description>CAP-08088</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47NF(0.047UF/47000PF)-25V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08605</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47PF-1500V-5%(0805)" prefix="C" uservalue="yes">
<description>CAP-09202</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47PF-500V-10%(PTH)" prefix="C" uservalue="yes">
<description>CAP-09326</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08913</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47UF-10V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08310</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47UF-25V(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08699</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47UF-35V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08478</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="47UF-50V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-10547</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="560PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08749</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="560UF25V20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09983</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="6.7PF" prefix="C" uservalue="yes">
<description>CAP-08429</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="6.8PF-50V-+/-.25PF(0603)" prefix="C" uservalue="yes">
<description>CAP-08620</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="680PF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-09232</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="680PF-50V-5%(0805)" prefix="C" uservalue="yes">
<description>CAP-08472</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="68PF-50V-5%(0603)" prefix="C" uservalue="yes">
<description>CAP-08804</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="68UF-10V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08312</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="68UF-10V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-10790</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="8200PF(PTH)" prefix="C" uservalue="yes">
<description>CAP-08081</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="8200PF/8.2NF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08309</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="9.0PF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-09341</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
