<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
<package name="1X06">
</package>
<package name="MOLEX-1X6-RA_LOCK">
</package>
<package name="1X06_LONGPADS">
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X06-KIT">
<description>&lt;h3&gt;1X06-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="ATARI_CONNECTOR">
</package>
<package name="ATX24_RIGHT_ANGLE">
</package>
<package name="AUDIO-JACK">
</package>
<package name="STEREOJACK2.5MM_STEREOJACK2.5MM">
</package>
<package name="STEREOJACK2.5MM_SPECIA_POGOPINS">
</package>
<package name="STEREOJACK2.5MM_SPECIAL_HOLES-ONLY">
</package>
<package name="STEREOJACK2.5MM_SMD">
</package>
<package name="AUDIO-JACK-3.5MM-SMD">
</package>
<package name="AVR_MINI_PROG">
</package>
<package name="2X3">
</package>
<package name="2X3-NS">
</package>
<package name="2X3_OFFSET">
</package>
<package name="2X3_LOCK">
</package>
<package name="AVR_ICSP">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X3-SHROUDED">
</package>
<package name="2X5-SHROUDED">
</package>
<package name="2X5-SHROUDED_LOCK">
</package>
<package name="2X5-SHROUDED_SMD">
</package>
<package name="BANANA_CONN">
</package>
<package name="BC9VPC">
</package>
<package name="BNC">
<description>Fits Mouser Part#5227161</description>
</package>
<package name="DB9">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="DB9_MALE">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25VP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25VB">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="DIN7">
</package>
<package name="DS_TOUCH_CONNECTOR">
<description>4-pin DS touch screen connector</description>
</package>
<package name="EB-85A">
</package>
<package name="EM406">
</package>
<package name="EM408_CON">
</package>
<package name="F25D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25VP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25VB">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="FTDI_BASIC">
</package>
<package name="IPOD_FEMALE_CONNECTOR">
</package>
<package name="IPOD_MALE_CONNECTOR">
</package>
<package name="FFC_16">
</package>
<package name="LITTLE_BITS_FEMALE">
</package>
<package name="LITTLE_BITS_MALE">
</package>
<package name="LITTLEBITS">
</package>
<package name="1X01_LONGPAD">
</package>
<package name="LUXEON-PAD">
</package>
<package name="SMTSO-256-ET">
</package>
<package name="SMTRA-256-8-6">
</package>
<package name="1X01NS">
</package>
<package name="1X01">
</package>
<package name="1X01_2MM">
</package>
<package name="1X01_OFFSET">
</package>
<package name="PAD-1.5X4.5">
</package>
<package name="1X01_POGOPIN_HOLE_LARGE">
</package>
<package name="1X01_POGOPIN_HOLE_0.58">
</package>
<package name="SNAP-FEMALE">
</package>
<package name="SNAP-MALE">
</package>
<package name="1X02">
</package>
<package name="MOLEX-1X2">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X02_BIG">
</package>
<package name="JST-2-SMD-VERT">
</package>
<package name="R_SW_TH">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X02_LOCK">
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="1X02_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1X02_NO_SILK">
</package>
<package name="JST-2-PTH">
</package>
<package name="1X02_XTRA_BIG">
</package>
<package name="1X02_PP_HOLES_ONLY">
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
</package>
<package name="JST-2-PTH-NS">
</package>
<package name="JST-2-PTH-KIT">
<description>&lt;H3&gt;JST-2-PTH-KIT&lt;/h3&gt;
2-Pin JST, through-hole connector&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="SPRINGTERMINAL-2.54MM-2">
</package>
<package name="1X03">
</package>
<package name="MOLEX-1X3">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="1X03_LOCK">
</package>
<package name="1X03_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X3_LOCK">
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S">
</package>
<package name="1X03_NO_SILK">
</package>
<package name="1X03_LONGPADS">
</package>
<package name="JST-3-PTH">
</package>
<package name="1X03_PP_HOLES_ONLY">
</package>
<package name="SCREWTERMINAL-5MM-3">
</package>
<package name="1X03_LOCK_NO_SILK">
</package>
<package name="JST-3-SMD">
</package>
<package name="1X03-1MM-RA">
</package>
<package name="1X04">
</package>
<package name="MOLEX-1X4">
</package>
<package name="SCREWTERMINAL-3.5MM-4">
</package>
<package name="1X04-1.27MM">
</package>
<package name="1X04_LOCK">
</package>
<package name="1X04_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X4_LOCK">
</package>
<package name="1X04-SMD">
</package>
<package name="1X04_LONGPADS">
</package>
<package name="1X04_NO_SILK">
</package>
<package name="JST-4-PTH">
</package>
<package name="SCREWTERMINAL-3.5MM-4_LOCK">
</package>
<package name="1X04-1MM-RA">
</package>
<package name="2X4">
</package>
<package name="1X05">
</package>
<package name="1X05-1.27MM">
<description>Header for OS4000-T</description>
</package>
<package name="1X05_LOCK">
</package>
<package name="1X05_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X05_LONGPADS">
</package>
<package name="1X05-1MM">
</package>
<package name="1X05-1MM-RA">
</package>
<package name="2X5-RA">
</package>
<package name="2X5-RAF">
</package>
<package name="MOLEX-1X6">
</package>
<package name="MOLEX-1X6-RA">
</package>
<package name="1X06_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="MOLEX-1X6_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X06-SIP_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X06_FEMALE_LOCK.010">
</package>
<package name="1X06-SMD_EDGE">
</package>
<package name="SCREWTERMINAL-3.5MM-6">
</package>
<package name="1X06-SMD-FEMALE">
</package>
<package name="1X06-SMD-FEMALE-V2">
<description>Package for 4UCONN part #19686 *UNPROVEN*</description>
</package>
<package name="1X06_HOLES_ONLY">
</package>
<package name="1X06_SMD_STRAIGHT">
</package>
<package name="1X06_SMD_STRAIGHT_ALT">
</package>
<package name="1X06_SMD_STRAIGHT_COMBO">
</package>
<package name="1X07">
</package>
<package name="1X07_LOCK">
</package>
<package name="1X07_LOCK_LONGPADS">
</package>
<package name="1X07_LONGPADS">
</package>
<package name="1X07_HOLES_ONLY">
</package>
<package name="1X08">
</package>
<package name="1X08_LOCK">
</package>
<package name="1X08_LOCK_LONGPADS">
</package>
<package name="1X08_LONGPADS">
</package>
<package name="SCREWTERMINAL-3.5MM-8">
</package>
<package name="1X08_SMD">
</package>
<package name="1X08_SMD_ALT">
</package>
<package name="1X08_SMD_COMBINED">
</package>
<package name="BM08B-SRSS-TB">
<description>JST crimp connector: 1mm pitch, top entry</description>
</package>
<package name="2X8">
</package>
<package name="1X09">
</package>
<package name="1X09_LOCK">
</package>
<package name="1X09_LOCK_LONGPADS">
</package>
<package name="1X09_LONGPADS">
</package>
<package name="1X10">
</package>
<package name="1X10-2MM">
</package>
<package name="1X10-2MM-SMD">
</package>
<package name="1X10_LOCK">
</package>
<package name="1X10_LOCK_LONGPADS">
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10_LOCK">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10_LOCK_SPECIAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10_NOSILK">
</package>
<package name="1X11">
</package>
<package name="1X11-1.27MM">
<description>Header for the OS4000-T</description>
</package>
<package name="1X11_LOCK">
</package>
<package name="1X11_LOCK_LONGPADS">
</package>
<package name="1X11_SMD_PTHCOMBO">
</package>
<package name="1X11_LONGPADS">
</package>
<package name="1X11_SMD_NO_HOLES">
</package>
<package name="1X11_HOLES_ONLY">
</package>
<package name="1X12">
</package>
<package name="1X12_LOCK">
</package>
<package name="1X12_LOCK_LONGPADS">
</package>
<package name="1X12_MACHINE-PIN-HEADER_LOCK.004">
</package>
<package name="1X12_LONGPADS">
</package>
<package name="1X12_HOLES_ONLY">
</package>
<package name="1X13">
</package>
<package name="1X13-LONGPADS">
</package>
<package name="1X14">
</package>
<package name="1X14_LOCK">
</package>
<package name="1X14_LOCK_LONGPADS">
</package>
<package name="1X14-LONGPADS">
</package>
<package name="1X15">
</package>
<package name="1X15_LOCK">
</package>
<package name="1X15_LOCK_LONGPADS">
</package>
<package name="1X16">
</package>
<package name="1X16_LOCK">
</package>
<package name="1X16_LOCK_LONGPADS">
</package>
<package name="1X16_MACHINE-PIN-HEADER_LOCK.004">
</package>
<package name="1X16_LONGPADS">
</package>
<package name="1X17">
</package>
<package name="1X18">
</package>
<package name="1X19">
</package>
<package name="1X20">
</package>
<package name="1X20_LOCK">
</package>
<package name="1X20_LOCK_LONGPADS">
</package>
<package name="1X20_LOCK_SPECIAL">
</package>
<package name="1X24">
</package>
<package name="1X24_LONGPADS">
</package>
<package name="1X25">
</package>
<package name="1X25_LOCK">
</package>
<package name="1X25_LOCK_LONGPADS">
</package>
<package name="1X25_LONGPAD">
</package>
<package name="1X27">
</package>
<package name="1X40_OFFSET">
</package>
<package name="1X40">
</package>
<package name="MAGJACK">
</package>
<package name="MAGJACK-19938">
</package>
<package name="MAGJACK-POE">
<description>&lt;h3&gt;PoE Compatible MagJack&lt;/h3&gt;
This RJ-45 jack with magnetics has 10 pins, gives you access to the unused twisted pair (10BASE-T, and 100BASE-T) which usually carries power in a power-over-ethernet system.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Footprint is Proven&lt;/b&gt;</description>
</package>
<package name="DIN_5_FEMALE_SUPPORT">
</package>
<package name="DIN_5_FEMALE">
</package>
<package name="MINI-DIN6">
</package>
<package name="MIRF">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="OBDII">
<description>OBDII Connector footprint, for your late model automotive needs</description>
</package>
<package name="PIC-ICSP-MINI">
</package>
<package name="2X12">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X26">
</package>
<package name="POWER_JACK_SMD">
</package>
<package name="POWER_JACK_SLOT">
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="POWER_JACK_COMBO">
</package>
<package name="POWER_JACK_PTH_LOCK">
</package>
<package name="PSP_CONNECTOR">
</package>
<package name="PSP_TOUCH_CONNECTOR">
<description>4-Pin connector for PSP touch screen</description>
</package>
<package name="RJ9">
<description>Footprint for RJ9 simple connector. Common with telephone handsets. SparkFun SKU: PRT-08694</description>
</package>
<package name="RJ11-6">
</package>
<package name="RJ45-8">
</package>
<package name="SCREENKEYMATINGCONNECTOR">
</package>
<package name="SD-MMC_SOCKET-PP">
</package>
<package name="SIMHOLDER">
</package>
<package name="SIMHOLDER2">
</package>
<package name="SIMHOLDER3">
</package>
<package name="SMARTCARD">
<description>&lt;b&gt;Description:&lt;/b&gt; S..m..r..t. I am so smrt!</description>
</package>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
<package name="STARBOARD_GROUND">
</package>
<package name="STARBOARD_GROUND_SMALL">
</package>
<package name="STARBOARD_GROUND_WIDE">
</package>
<package name="STARBOARD_GROUND_SMALL2">
</package>
<package name="STARBOARD_PWR_WIDE">
</package>
<package name="STARBOARD_PWR">
</package>
<package name="TOUCH-SCREEN">
</package>
<package name="U.FL">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="S4B-PH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-PCB">
</package>
<package name="USB-B-PTH-VERTICAL">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S-NOSILK">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="USB-A-S-SILK-FEMALE">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="MICRO-B-RA-SMT">
<description>Package for an SMT Micro-B connector.  Digikey part #H11613-ND
*** Unproven***</description>
</package>
<package name="MICRO-B-RA-TH">
<description>&lt;h3&gt;Micro B Right Angle through-hole PCB plug connector&lt;/h3&gt;
&lt;b&gt;**Unproven**&lt;/b&gt;&lt;br&gt;
See digikey part #H11673TR-ND</description>
</package>
<package name="MICRO-B-TH">
<description>&lt;h3&gt;Micro B USB Plug Assembly - Straight Through-hole&lt;/h3&gt;
&lt;b&gt;**UNPROVEN**&lt;/b&gt;&lt;Br&gt;
See Digikey part #H11497-ND</description>
</package>
<package name="MICRO-B-SMT">
<description>&lt;h3&gt;USB Micro-B Plug Connector&lt;/h3&gt;
Manufacturer part #: ZX80-B-5SA&lt;br&gt;
Manufacturer: Hirose&lt;br&gt;&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt; (Passed 1:1 printout test though!)</description>
</package>
<package name="USD-SOCKET-PP">
<description>OLD Production Socket. DO NOT USE for production boards.</description>
</package>
<package name="MICRO-SD-SOCKET-PP">
</package>
<package name="FFC26">
<description>&lt;b&gt;26-pin FFC connector&lt;/b&gt;
&lt;br&gt;See 4UCONN part #08630</description>
</package>
<package name="XLR3_NC3FAH2">
</package>
<package name="DIL28-3-ZIF_SOCKET">
</package>
<package name="DIL40-6-ZIF_SOCKET">
</package>
<package name="ZUNE_CONNECTOR_MALE">
</package>
<package name="50-PIN-CENTRONICS-F">
</package>
<package name="50-PIN-CENTRONICS-M">
</package>
<package name="RCA">
</package>
<package name="RCA_LOCK">
</package>
<package name="USB-AB-MICRO-SMD">
<description>micro USB AB connector for OTG support. 5-pins: USBVCC, GND, D+, D-, USBID. Can act as host or device</description>
</package>
<package name="1X16_NO_SILK">
</package>
<package name="1X19_NO_SILK">
</package>
<package name="1X11_NO_SILK">
</package>
<package name="SDCARD_4UCONN">
<description>4UConn part#19646</description>
</package>
<package name="COMPUTER-PERIPHERAL-POWER-RA">
</package>
<package name="COMPUTER-PERIPHERAL-POWER">
</package>
<package name="FTDI_DEVICE_SIDE">
<description>Package for devices meant to mate to an FTDI connector.</description>
</package>
<package name="3.81MM_TERMINAL_BLOCK_FEMALE_LOCKING">
</package>
<package name="1X04_SMD_STRAIGHT_COMBO">
</package>
<package name="DB15">
</package>
<package name="AUDIO-JACK-TRRS-SMD">
</package>
<package name="1X03_SMD_RA_FEMALE">
</package>
<package name="1X03_SMD_RA_MALE">
</package>
<package name="2X3_SMT_POSTS">
<description>4UCON 15881&lt;br&gt;
Male .1" spaced SMT&lt;br&gt;
Keying posts into board</description>
</package>
<package name="2X13">
</package>
<package name="USB-A-SMT-MALE">
</package>
<package name="2X3_POGO">
</package>
</packages>
<symbols>
<symbol name="ARDUINO_SERIAL_PROGRAM">
<pin name="DTR" direction="pas"/>
<pin name="RXI" direction="pas"/>
<pin name="TXO" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="CTS" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="ATARI_CONNECTOR">
<pin name="UP"/>
<pin name="DOWN"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="NC1"/>
<pin name="BUTTON"/>
<pin name="NC2"/>
<pin name="GND"/>
<pin name="NC3"/>
</symbol>
<symbol name="ATX24-1">
<pin name="-12V"/>
<pin name="3.3V@0"/>
<pin name="3.3V@1"/>
<pin name="3.3V@2"/>
<pin name="3.3V@3"/>
<pin name="5V@0"/>
<pin name="5V@1"/>
<pin name="5V@2"/>
<pin name="5V@3"/>
<pin name="5V@4"/>
<pin name="5V_STDBY"/>
<pin name="12V@0"/>
<pin name="12V@1"/>
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="NC"/>
<pin name="PS_ON"/>
<pin name="PWR_OK"/>
</symbol>
<symbol name="AUDIO-JACK">
<pin name="RIGHT"/>
<pin name="LEFT"/>
<pin name="SLEEVE"/>
</symbol>
<symbol name="AUDIO-JACK2">
<pin name="RING"/>
<pin name="TIP"/>
<pin name="SLEEVE"/>
<pin name="RSH"/>
<pin name="TSH"/>
</symbol>
<symbol name="AVR_MINI_PROGRAMMER">
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="RST" direction="pas"/>
<pin name="MOSI" direction="pas"/>
<pin name="SCK" direction="pas"/>
<pin name="MISO" direction="pas"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER_6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER-1">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="BANANA_CONN">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="BC9VPC">
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="BNC">
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="F09G">
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="DB25">
<pin name="1" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="DIN7">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
</symbol>
<symbol name="DS_TOUCH_CONNECTOR">
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="EB-85A">
<pin name="GND" direction="pwr"/>
<pin name="TX2" direction="out"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX2" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="BATT" direction="pwr"/>
</symbol>
<symbol name="EM406">
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="1PPS"/>
<pin name="VCC"/>
</symbol>
<symbol name="EM408_CON">
<pin name="EN"/>
<pin name="GND"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="VCC"/>
</symbol>
<symbol name="F25">
<pin name="1" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="M06">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="IPOD_CONNECTOR_FEMALE">
<pin name="LEFT_IN"/>
<pin name="VIDEO_OUT"/>
<pin name="RIGHT_IN"/>
<pin name="SCHROME_OUT"/>
<pin name="GND@1"/>
<pin name="SLUM_OUT"/>
<pin name="GND@2"/>
<pin name="GND@11"/>
<pin name="LEFT_OUT"/>
<pin name="GND@16"/>
<pin name="RIGHT_OUT"/>
<pin name="FW_12V@20"/>
<pin name="ACC_INDICATOR"/>
<pin name="FW_TPA-"/>
<pin name="USB_5V"/>
<pin name="17"/>
<pin name="3.3V"/>
<pin name="FW_12V@19"/>
<pin name="GND@15"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="FW_TPA+"/>
<pin name="USB_D-"/>
<pin name="FW_TPB-"/>
<pin name="USB_D+"/>
<pin name="FW_TPB+"/>
<pin name="GND@29"/>
<pin name="GND@30"/>
<pin name="14"/>
<pin name="7"/>
</symbol>
<symbol name="KENT_LCD_CONN">
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSS4"/>
<pin name="VCC"/>
<pin name="VPWR1"/>
<pin name="VPWR2"/>
<pin name="VPWR3"/>
<pin name="/RESET"/>
<pin name="BUSY"/>
<pin name="SCK"/>
<pin name="SO"/>
<pin name="SI"/>
<pin name="CS"/>
<pin name="NC1"/>
<pin name="NC2"/>
</symbol>
<symbol name="LITTLEBITS_FEMALE">
<pin name="VCC"/>
<pin name="SIG"/>
<pin name="GND"/>
</symbol>
<symbol name="LITTLEBITS_MALE">
<pin name="GND"/>
<pin name="SIG"/>
<pin name="VCC"/>
</symbol>
<symbol name="LITTLEBITS">
<pin name="GND"/>
<pin name="SIG"/>
<pin name="VCC"/>
</symbol>
<symbol name="M01">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="M02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="M04">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="M04X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="M05">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="M05X2">
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="M07">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="M08">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="M2X8">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="M09">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="M10">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="M10X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="M11">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="M12">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="M13">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="M14">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="M15">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="M16">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="M17">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
</symbol>
<symbol name="M18">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="M19">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
</symbol>
<symbol name="M20">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="M24">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="M25">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="M27">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
</symbol>
<symbol name="M40">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="MAGJACK">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD@0"/>
<pin name="SHIELD@1"/>
</symbol>
<symbol name="MAGJACK-2">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="MAGJACK-POE">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD@0"/>
<pin name="SHIELD@1"/>
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="MIDI_CONN_FEMALE">
<pin name="NC3"/>
<pin name="NC2"/>
<pin name="NC1"/>
<pin name="MIDI_OUT"/>
<pin name="MIDI_IN"/>
</symbol>
<symbol name="MIRF">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="MMA_CON">
<pin name="VCC" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="X" direction="pas" function="dot"/>
<pin name="Y" direction="pas" function="dot"/>
<pin name="Z" direction="pas" function="dot"/>
<pin name="GS1" direction="pas" function="dot"/>
<pin name="GS2" direction="pas" function="dot"/>
<pin name="SLP" direction="pas" function="dot"/>
</symbol>
<symbol name="OBDII">
<pin name="1"/>
<pin name="J1850BUS+"/>
<pin name="3"/>
<pin name="CHASGND"/>
<pin name="SIGGND"/>
<pin name="CANHIGH"/>
<pin name="ISOK-LINE"/>
<pin name="8"/>
<pin name="9"/>
<pin name="J1850BUS"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="CANLOW"/>
<pin name="ISOL-LINE"/>
<pin name="BATTPOWER"/>
</symbol>
<symbol name="ICSP-PIC">
<pin name="GND"/>
<pin name="PGC"/>
<pin name="PGD"/>
<pin name="PGM"/>
<pin name="VCC"/>
<pin name="VPP"/>
</symbol>
<symbol name="PIC-ISCP-MINI">
<pin name="VPP" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGD" direction="pas"/>
<pin name="PGC" direction="pas"/>
</symbol>
<symbol name="PINH2X12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X26">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="41" direction="pas" function="dot"/>
<pin name="43" direction="pas" function="dot"/>
<pin name="45" direction="pas" function="dot"/>
<pin name="47" direction="pas" function="dot"/>
<pin name="49" direction="pas" function="dot"/>
<pin name="51" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
<pin name="42" direction="pas" function="dot"/>
<pin name="44" direction="pas" function="dot"/>
<pin name="46" direction="pas" function="dot"/>
<pin name="48" direction="pas" function="dot"/>
<pin name="50" direction="pas" function="dot"/>
<pin name="52" direction="pas" function="dot"/>
</symbol>
<symbol name="POWERJACK">
<pin name="GNDBREAK"/>
<pin name="GND"/>
<pin name="PWR"/>
</symbol>
<symbol name="PSP_CONNECTOR">
<pin name="G7"/>
<pin name="G6"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="G3"/>
<pin name="G2"/>
<pin name="G1"/>
<pin name="G0"/>
<pin name="R7"/>
<pin name="R6"/>
<pin name="R5"/>
<pin name="R4"/>
<pin name="R3"/>
<pin name="R2"/>
<pin name="R1"/>
<pin name="R0"/>
<pin name="VCC2"/>
<pin name="VCC"/>
<pin name="GND2"/>
<pin name="GND"/>
<pin name="TEST3"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="NC2"/>
<pin name="AVDD2"/>
<pin name="AVDD"/>
<pin name="NC"/>
<pin name="VSYNC"/>
<pin name="HSYNC"/>
<pin name="DISP"/>
<pin name="CK"/>
<pin name="GND3"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="B0"/>
</symbol>
<symbol name="PSP_TOUCH_CONNECTOR">
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="M04-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="RJ45-8">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
</symbol>
<symbol name="SCREENKEYMATINGCONNECTOR">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
</symbol>
<symbol name="SDCARD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="GND1"/>
<pin name="DO"/>
<pin name="IRQ"/>
<pin name="WP"/>
<pin name="CD"/>
<pin name="SW"/>
<pin name="SHIELD"/>
<pin name="P9"/>
</symbol>
<symbol name="SIMHOLDER">
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="C7"/>
<pin name="C6"/>
<pin name="C5"/>
</symbol>
<symbol name="SIMHOLDER2">
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="SW1"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
<pin name="SW2"/>
</symbol>
<symbol name="SIMHOLDER3">
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="I/O"/>
</symbol>
<symbol name="SMARTCARD">
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="I/O"/>
<pin name="VPP"/>
<pin name="GND"/>
<pin name="C4"/>
<pin name="C8"/>
</symbol>
<symbol name="SMA_EDGE">
<pin name="GND@0"/>
<pin name="SIGNAL"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
</symbol>
<symbol name="STARBOARD_PAD">
<pin name="MOUNT" direction="pas"/>
</symbol>
<symbol name="STARBOARD_PAD+">
<pin name="MOUNT" direction="pas"/>
</symbol>
<symbol name="TOUCH-SCREEN">
<pin name="TS4"/>
<pin name="TS3"/>
<pin name="TS2"/>
<pin name="TS1"/>
</symbol>
<symbol name="U.FL">
<pin name="GND@0"/>
<pin name="SIGNAL"/>
<pin name="GND@1"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="USB+SHIELD">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="USB-5PIN">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="ID"/>
<pin name="MTN1"/>
<pin name="MTN2"/>
<pin name="MTN3"/>
<pin name="MTN4"/>
</symbol>
<symbol name="MICROB-PLUG">
<pin name="VCC"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="ID"/>
<pin name="GND"/>
</symbol>
<symbol name="USDCARD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="RSV"/>
<pin name="DO"/>
<pin name="NC"/>
<pin name="SHIELD@3"/>
<pin name="SHIELD@1"/>
<pin name="SHIELD@2"/>
<pin name="SHIELD@4"/>
</symbol>
<symbol name="WATN001001">
<pin name="V0@1"/>
<pin name="V1@1"/>
<pin name="V2@1"/>
<pin name="VSSE@1"/>
<pin name="VSS@1"/>
<pin name="EIO1"/>
<pin name="XCK"/>
<pin name="VDD"/>
<pin name="LATCH"/>
<pin name="RESERVED@1"/>
<pin name="SHL"/>
<pin name="SLEEPB"/>
<pin name="DLY0"/>
<pin name="DLY1"/>
<pin name="RESERVED@2"/>
<pin name="DI0"/>
<pin name="DI1"/>
<pin name="DI2"/>
<pin name="RESERVED@3"/>
<pin name="EIO2"/>
<pin name="VSS@2"/>
<pin name="VSSE@2"/>
<pin name="V0@2"/>
<pin name="V1@2"/>
<pin name="V2@2"/>
<pin name="RESERVED@4"/>
</symbol>
<symbol name="XLR3_NCFAH2">
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
<pin name="G"/>
</symbol>
<symbol name="DIL-28-3">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
</symbol>
<symbol name="DIL-40-6">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
</symbol>
<symbol name="ZUNE_CONNECTOR_MALE">
<pin name="USB_5V@1"/>
<pin name="USB_5V@2"/>
<pin name="USB_5V@3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="VIDEO+"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="AUDIO_L"/>
<pin name="AUDIO_R"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="GND@19"/>
<pin name="USB_DATA-"/>
<pin name="USB_DATA+"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
</symbol>
<symbol name="50-PIN-CENTRONICS">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
<pin name="P$41"/>
<pin name="P$42"/>
<pin name="P$43"/>
<pin name="P$44"/>
<pin name="P$45"/>
<pin name="P$46"/>
<pin name="P$47"/>
<pin name="P$48"/>
<pin name="P$49"/>
<pin name="P$50"/>
</symbol>
<symbol name="RCA">
<pin name="SWITCH"/>
<pin name="SHELL"/>
<pin name="PIN"/>
</symbol>
<symbol name="USB_AB">
<description>USB AB, 5-pins: USBVCC, GND, D+, D-, USBID.</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="USBID"/>
</symbol>
<symbol name="SDCARD-1">
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK"/>
<pin name="VSS2" direction="pwr"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="WP"/>
<pin name="CD"/>
<pin name="SH@1"/>
<pin name="SH@2"/>
</symbol>
<symbol name="COMPUTER-PERIPHERAL-POWER">
<pin name="12V" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="5V" direction="pas"/>
</symbol>
<symbol name="FTDI_DEVICE">
<pin name="DTR"/>
<pin name="TXO"/>
<pin name="RXI"/>
<pin name="VCC"/>
<pin name="CTS"/>
<pin name="GND"/>
</symbol>
<symbol name="MYDAQ_CONNECTOR">
<pin name="AN1-" direction="in"/>
<pin name="+15V" direction="pwr"/>
<pin name="-15V" direction="pwr"/>
<pin name="AGND_15V" direction="pwr"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="DIO4"/>
<pin name="DIO5"/>
<pin name="DIO6"/>
<pin name="DIO7"/>
<pin name="DGND" direction="pwr"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="5V" direction="pwr"/>
<pin name="AO0" direction="out"/>
<pin name="AO1" direction="out"/>
<pin name="AGND_IO" direction="pwr"/>
<pin name="AI0+" direction="in"/>
<pin name="AI0-" direction="in"/>
<pin name="AI1+" direction="in"/>
</symbol>
<symbol name="DB15">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="AUDIO-JACK3-TRRS">
<pin name="RING1"/>
<pin name="RING2"/>
<pin name="EARTH"/>
<pin name="TIP"/>
</symbol>
<symbol name="M03X2">
<pin name="1"/>
<pin name="3"/>
<pin name="5"/>
<pin name="6"/>
<pin name="4"/>
<pin name="2"/>
</symbol>
<symbol name="JST_2MM_MALE">
<pin name="-"/>
<pin name="+"/>
<pin name="PAD2"/>
<pin name="PAD1"/>
</symbol>
<symbol name="M13X2">
<pin name="26" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO_SERIAL_PROGRAM" prefix="JP" uservalue="yes">
<description>FTDI connector footprints</description>
<gates>
<gate name="G$1" symbol="ARDUINO_SERIAL_PROGRAM"/>
</gates>
<devices>
<device name="SMD" package="1X06-SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X06">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX-1X6-RA_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="DTR" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RXI" pad="5"/>
<connect gate="G$1" pin="TXO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-KIT" package="1X06-KIT">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATARI_CONNECTOR">
<description>DB9 labeled for Atari joystick</description>
<gates>
<gate name="G$1" symbol="ATARI_CONNECTOR"/>
</gates>
<devices>
<device name="" package="ATARI_CONNECTOR">
<connects>
<connect gate="G$1" pin="BUTTON" pad="P$1"/>
<connect gate="G$1" pin="DOWN" pad="P$6"/>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="LEFT" pad="P$7"/>
<connect gate="G$1" pin="NC1" pad="P$9"/>
<connect gate="G$1" pin="NC2" pad="P$2"/>
<connect gate="G$1" pin="NC3" pad="P$4"/>
<connect gate="G$1" pin="RIGHT" pad="P$8"/>
<connect gate="G$1" pin="UP" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATX24" prefix="J">
<description>&lt;b&gt;ATX24 Pin Power Supply Connector&lt;/b&gt; This is a good connector for connecting a computer power supply to a PCB. It's massive, but provides many amps of power at 5V and 12V. SKU: PRT-09498</description>
<gates>
<gate name="G$1" symbol="ATX24-1"/>
</gates>
<devices>
<device name="RH" package="ATX24_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="-12V" pad="14"/>
<connect gate="G$1" pin="12V@0" pad="10"/>
<connect gate="G$1" pin="12V@1" pad="11"/>
<connect gate="G$1" pin="3.3V@0" pad="1"/>
<connect gate="G$1" pin="3.3V@1" pad="2"/>
<connect gate="G$1" pin="3.3V@2" pad="12"/>
<connect gate="G$1" pin="3.3V@3" pad="13"/>
<connect gate="G$1" pin="5V@0" pad="4"/>
<connect gate="G$1" pin="5V@1" pad="6"/>
<connect gate="G$1" pin="5V@2" pad="21"/>
<connect gate="G$1" pin="5V@3" pad="22"/>
<connect gate="G$1" pin="5V@4" pad="23"/>
<connect gate="G$1" pin="5V_STDBY" pad="9"/>
<connect gate="G$1" pin="GND@0" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="15"/>
<connect gate="G$1" pin="GND@4" pad="17"/>
<connect gate="G$1" pin="GND@5" pad="18"/>
<connect gate="G$1" pin="GND@6" pad="19"/>
<connect gate="G$1" pin="GND@7" pad="24"/>
<connect gate="G$1" pin="NC" pad="20"/>
<connect gate="G$1" pin="PS_ON" pad="16"/>
<connect gate="G$1" pin="PWR_OK" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO-JACK" prefix="U" uservalue="yes">
<description>&lt;b&gt;3.5mm Audio Jack&lt;/b&gt;
Simple 3.5mm common PCB mount audio jack. SKU: PRT-08032</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK"/>
</gates>
<devices>
<device name="PTH" package="AUDIO-JACK">
<connects>
<connect gate="G$1" pin="LEFT" pad="TIP"/>
<connect gate="G$1" pin="RIGHT" pad="RING"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5MM" package="STEREOJACK2.5MM_STEREOJACK2.5MM">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL_POGO_PINS" package="STEREOJACK2.5MM_SPECIA_POGOPINS">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HOLESONLY" package="STEREOJACK2.5MM_SPECIAL_HOLES-ONLY">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="STEREOJACK2.5MM_SMD">
<connects>
<connect gate="G$1" pin="LEFT" pad="1"/>
<connect gate="G$1" pin="RIGHT" pad="4"/>
<connect gate="G$1" pin="SLEEVE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="AUDIO-JACK-3.5MM-SMD">
<connects>
<connect gate="G$1" pin="LEFT" pad="TIP"/>
<connect gate="G$1" pin="RIGHT" pad="RING"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO-JACK2">
<description>Stereo audio jack with bypass switches.</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK2"/>
</gates>
<devices>
<device name="PTH" package="AUDIO-JACK">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="AUDIO-JACK-3.5MM-SMD">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_MINI_PROG">
<description>AVR ISP 6-pin inline header</description>
<gates>
<gate name="G$1" symbol="AVR_MINI_PROGRAMMER"/>
</gates>
<devices>
<device name="SMD" package="AVR_MINI_PROG">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="6"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PRG_6" prefix="J">
<description>&lt;b&gt;AVR ISP 6 Pin&lt;/b&gt;
This is the reduced ISP connector for AVR programming. Common on Arduino. This footprint will take up less PCB space and can be used with a 10-pin to 6-pin adapter such as SKU: BOB-08508</description>
<gates>
<gate name="G$1" symbol="AVR_SPI_PROGRAMMER_6"/>
</gates>
<devices>
<device name="PTH" package="2X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NS" package="2X3-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OFFSET_PADS" package="2X3_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X3_LOCK" package="2X3_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PROG">
<description>&lt;b&gt;AVR 10-pin ICSP Header&lt;/b&gt; 
This is the standard AVR In Circuit Serial Programming header. Minimal, but includes pin one indicator. Works with standard Olimex programmers. Also look for the 6-pin reduced version. Spark Fun Electronics SKU: PRT-00778</description>
<gates>
<gate name="A" symbol="AVR_SPI_PROGRAMMER"/>
</gates>
<devices>
<device name="" package="AVR_ICSP">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PROG2">
<description>&lt;b&gt;AVR 10-pin ICSP Header&lt;/b&gt; 
This is the standard AVR In Circuit Serial Programming header. Minimal, but includes pin one indicator. Works with standard Olimex programmers. Also look for the 6-pin reduced version. Spark Fun Electronics SKU: PRT-00778</description>
<gates>
<gate name="A" symbol="AVR_SPI_PROGRAMMER-1"/>
</gates>
<devices>
<device name="PTH" package="AVR_ICSP">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="2X5-SHROUDED">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="2X5-SHROUDED_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="2X5-SHROUDED_SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BANANA_CONN" prefix="J" uservalue="yes">
<description>Through-hole banana jack</description>
<gates>
<gate name="G$1" symbol="BANANA_CONN"/>
</gates>
<devices>
<device name="" package="BANANA_CONN">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC9VPC" prefix="BAT" uservalue="yes">
<description>9V board-mount battery cradle</description>
<gates>
<gate name="G$1" symbol="BC9VPC"/>
</gates>
<devices>
<device name="" package="BC9VPC">
<connects>
<connect gate="G$1" pin="V+" pad="V+"/>
<connect gate="G$1" pin="V-" pad="V-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BNC">
<description>BNC Connector, Mouser Part# 5227161</description>
<gates>
<gate name="G$1" symbol="BNC"/>
</gates>
<devices>
<device name="PTH" package="BNC">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="OUT" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB9" prefix="X" uservalue="yes">
<description>&lt;b&gt;DB9 Connector&lt;/b&gt;
Standard DB9 (D-Sub 9) serial connector. Can be used for CAN bus as well as RS485 and RS232. Footprint production proven. Spark Fun Electronics SKU : PRT-00429</description>
<gates>
<gate name="G$1" symbol="F09G"/>
</gates>
<devices>
<device name="FEMALE" package="DB9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MALE" package="DB9_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB25" prefix="X" uservalue="yes">
<description>Various DB25 connectors</description>
<gates>
<gate name="-1" symbol="DB25"/>
</gates>
<devices>
<device name="D" package="M25D">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="M25H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HP" package="M25HP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="M25V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VP" package="M25VP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VB" package="M25VB">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIN7">
<description>Mini-DIN7 connector</description>
<gates>
<gate name="G$1" symbol="DIN7"/>
</gates>
<devices>
<device name="" package="DIN7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS_TOUCH_CONNECTOR" prefix="JP">
<description>4-pin DS touch screen connector (LCD-09105)</description>
<gates>
<gate name="G$1" symbol="DS_TOUCH_CONNECTOR"/>
</gates>
<devices>
<device name="" package="DS_TOUCH_CONNECTOR">
<connects>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="3"/>
<connect gate="G$1" pin="Y1" pad="4"/>
<connect gate="G$1" pin="Y2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EB-85A">
<description>&lt;b&gt;EB-85A Connector&lt;/b&gt;
Proven layout and schematic for ETek 5Hz GPS receiver connector. Spark Fun Electronics SKU : GPS-08297</description>
<gates>
<gate name="G$1" symbol="EB-85A"/>
</gates>
<devices>
<device name="SMD" package="EB-85A">
<connects>
<connect gate="G$1" pin="BATT" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PPS" pad="7"/>
<connect gate="G$1" pin="RX1" pad="4"/>
<connect gate="G$1" pin="RX2" pad="6"/>
<connect gate="G$1" pin="TX1" pad="3"/>
<connect gate="G$1" pin="TX2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM406" prefix="U">
<description>&lt;b&gt;EM406 GPS Connector&lt;/b&gt;
Proven layout and schematic for EM406 connector. Spark Fun Electronics SKU : GPS-00579</description>
<gates>
<gate name="G$1" symbol="EM406"/>
</gates>
<devices>
<device name="" package="EM406">
<connects>
<connect gate="G$1" pin="1PPS" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM408_CON" prefix="U">
<description>This is the mating connector for the EM408 GPS receiver.  The EM408 connects to the board via a cable, 
this connector footprint does not include the outline of the receiver.

You should include the "EM408_Outline" device in your schematic if you are to use the EM408 in your design.</description>
<gates>
<gate name="G$1" symbol="EM408_CON"/>
</gates>
<devices>
<device name="" package="EM408_CON">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="F25" prefix="X" uservalue="yes">
<description>25 Pin male connector. PCB edge mount for regular PCB thicknesses. This connector will connect directly to the back of a PC parallel port or through a normal DB25 extension cable (M/F). SKU: PRT-08287</description>
<gates>
<gate name="-1" symbol="F25"/>
</gates>
<devices>
<device name="D" package="F25D">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="F25H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HP" package="F25HP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="F25V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VP" package="F25VP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VB" package="F25VB">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI_BASIC" prefix="JP">
<description>FTDI Basic header with labels</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="PTH" package="FTDI_BASIC">
<connects>
<connect gate="G$1" pin="1" pad="DTR"/>
<connect gate="G$1" pin="2" pad="RXI"/>
<connect gate="G$1" pin="3" pad="TXO"/>
<connect gate="G$1" pin="4" pad="VCC"/>
<connect gate="G$1" pin="5" pad="CTS"/>
<connect gate="G$1" pin="6" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPOD_CONNECTOR_FEMALE">
<description>&lt;b&gt;iPod Female Connector&lt;/b&gt;
This is the connector found inside current iPods. Use this connector to attach to iPod accessories like Nike+iPods, etc. Schematic and footprint are not yet production proven. Spark Fun Electronics SKU : DEV-08035</description>
<gates>
<gate name="G$1" symbol="IPOD_CONNECTOR_FEMALE"/>
</gates>
<devices>
<device name="" package="IPOD_FEMALE_CONNECTOR">
<connects>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="3.3V" pad="18"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="ACC_INDICATOR" pad="21"/>
<connect gate="G$1" pin="FW_12V@19" pad="19"/>
<connect gate="G$1" pin="FW_12V@20" pad="20"/>
<connect gate="G$1" pin="FW_TPA+" pad="24"/>
<connect gate="G$1" pin="FW_TPA-" pad="22"/>
<connect gate="G$1" pin="FW_TPB+" pad="28"/>
<connect gate="G$1" pin="FW_TPB-" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="LEFT_IN" pad="6"/>
<connect gate="G$1" pin="LEFT_OUT" pad="4"/>
<connect gate="G$1" pin="RIGHT_IN" pad="5"/>
<connect gate="G$1" pin="RIGHT_OUT" pad="3"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCHROME_OUT" pad="9"/>
<connect gate="G$1" pin="SLUM_OUT" pad="10"/>
<connect gate="G$1" pin="TX" pad="12"/>
<connect gate="G$1" pin="USB_5V" pad="23"/>
<connect gate="G$1" pin="USB_D+" pad="27"/>
<connect gate="G$1" pin="USB_D-" pad="25"/>
<connect gate="G$1" pin="VIDEO_OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPOD_CONNECTOR_MALE">
<description>&lt;b&gt;iPod Male Connector&lt;/b&gt;
This is the connector that will insert into an iPods. Use this connector to gain access to the various iPod pins. Schematic and footprint are not yet production proven. The PCB thickness must be more thin than the standard 0.062" FR4. Spark Fun Electronics SKU : DEV-00633</description>
<gates>
<gate name="G$1" symbol="IPOD_CONNECTOR_FEMALE"/>
</gates>
<devices>
<device name="" package="IPOD_MALE_CONNECTOR">
<connects>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="3.3V" pad="18"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="ACC_INDICATOR" pad="21"/>
<connect gate="G$1" pin="FW_12V@19" pad="19"/>
<connect gate="G$1" pin="FW_12V@20" pad="20"/>
<connect gate="G$1" pin="FW_TPA+" pad="24"/>
<connect gate="G$1" pin="FW_TPA-" pad="22"/>
<connect gate="G$1" pin="FW_TPB+" pad="28"/>
<connect gate="G$1" pin="FW_TPB-" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="LEFT_IN" pad="6"/>
<connect gate="G$1" pin="LEFT_OUT" pad="4"/>
<connect gate="G$1" pin="RIGHT_IN" pad="5"/>
<connect gate="G$1" pin="RIGHT_OUT" pad="3"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCHROME_OUT" pad="9"/>
<connect gate="G$1" pin="SLUM_OUT" pad="10"/>
<connect gate="G$1" pin="TX" pad="12"/>
<connect gate="G$1" pin="USB_5V" pad="23"/>
<connect gate="G$1" pin="USB_D+" pad="27"/>
<connect gate="G$1" pin="USB_D-" pad="25"/>
<connect gate="G$1" pin="VIDEO_OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KENT_LCD_CONN">
<description>Connector for Kent display (LCD-09560)</description>
<gates>
<gate name="G$1" symbol="KENT_LCD_CONN"/>
</gates>
<devices>
<device name="" package="FFC_16">
<connects>
<connect gate="G$1" pin="/RESET" pad="1"/>
<connect gate="G$1" pin="BUSY" pad="2"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="NC1" pad="15"/>
<connect gate="G$1" pin="NC2" pad="16"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SI" pad="6"/>
<connect gate="G$1" pin="SO" pad="5"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VPWR1" pad="10"/>
<connect gate="G$1" pin="VPWR2" pad="11"/>
<connect gate="G$1" pin="VPWR3" pad="13"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="8"/>
<connect gate="G$1" pin="VSS3" pad="12"/>
<connect gate="G$1" pin="VSS4" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLEBITS_FEMALE" prefix="JP">
<description>Female end for LittleBits boards</description>
<gates>
<gate name="G$1" symbol="LITTLEBITS_FEMALE"/>
</gates>
<devices>
<device name="" package="LITTLE_BITS_FEMALE">
<connects>
<connect gate="G$1" pin="GND" pad="V-"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
<connect gate="G$1" pin="VCC" pad="V+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLEBITS_MALE">
<description>Male end for LittleBits boards</description>
<gates>
<gate name="G$1" symbol="LITTLEBITS_MALE"/>
</gates>
<devices>
<device name="" package="LITTLE_BITS_MALE">
<connects>
<connect gate="G$1" pin="GND" pad="V-"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
<connect gate="G$1" pin="VCC" pad="V+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLE_BITS_CONN">
<description>Connector used in LittleBits</description>
<gates>
<gate name="G$1" symbol="LITTLEBITS"/>
</gates>
<devices>
<device name="" package="LITTLEBITS">
<connects>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="SIG" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M01" prefix="JP">
<description>&lt;b&gt;Header 1&lt;/b&gt;
Standard 1-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M01"/>
</gates>
<devices>
<device name="PTH_LONGPAD" package="1X01_LONGPAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="LUXEON-PAD">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMTSO-256-ET" package="SMTSO-256-ET">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMTRA-256-8-6" package="SMTRA-256-8-6">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMDNS" package="1X01NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_2MM" package="1X01_2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OFFSET" package="1X01_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-4.5X1.5" package="PAD-1.5X4.5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLE_LARGE" package="1X01_POGOPIN_HOLE_LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLE_0.58" package="1X01_POGOPIN_HOLE_0.58">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SNAP-FEMALE" package="SNAP-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SNAP-MALE" package="SNAP-MALE">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M02" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 2&lt;/b&gt;
Standard 2-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08233 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08352"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROCKER" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="1" pad="P$3"/>
<connect gate="G$1" pin="2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 3&lt;/b&gt;
Standard 3-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08232 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X03_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X03_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X3_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X03_NO_SILK" package="1X03_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X03_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH" package="JST-3-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X03_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SCREW-5MM" package="SCREWTERMINAL-5MM-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X03_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="JST-3-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X03-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_RA_FEMALE" package="1X03_SMD_RA_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10926"/>
<attribute name="VALUE" value="1x3 RA Female .1&quot;"/>
</technology>
</technologies>
</device>
<device name="SMD_RA_MALE" package="1X03_SMD_RA_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 4&lt;/b&gt;
Standard 4-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208</description>
<gates>
<gate name="G$1" symbol="M04"/>
</gates>
<devices>
<device name="PTH" package="1X04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X04-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X04_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X04_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X4_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X04-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X04_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X04_NO_SILK" package="1X04_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH" package="JST-4-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-4_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="1X04-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_STRAIGHT_COMBO" package="1X04_SMD_STRAIGHT_COMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M04X2">
<description>.1" header, two rows of four.</description>
<gates>
<gate name="G$1" symbol="M04X2"/>
</gates>
<devices>
<device name="" package="2X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M05" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 5&lt;/b&gt;
Standard 5-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08230 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M05"/>
</gates>
<devices>
<device name="PTH" package="1X05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X05-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X05_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X05_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X05_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X05-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="1X05-1MM-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M05X2" prefix="JP">
<description>&lt;b&gt;Header 5x2&lt;/b&gt;
Standard 10-pin dual row 0.1" header. Commonly used with AVR-ISP. Use with Spark Fun Electronics SKU: PRT-00778</description>
<gates>
<gate name="G$1" symbol="M05X2"/>
</gates>
<devices>
<device name="PTH" package="AVR_ICSP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="2X5-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAF" package="2X5-RAF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD" package="2X5-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD_LOCK" package="2X5-SHROUDED_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD_SMD" package="2X5-SHROUDED_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M06" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 6&lt;/b&gt;
Standard 6-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08094 with associated crimp pins and housings.

NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="SIP" package="1X06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-1X6-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X06-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X06_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX-1X6-RA_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIP_LOCK" package="1X06-SIP_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_LOCK" package="1X06_FEMALE_LOCK.010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X06-SMD_EDGE_FEMALE" package="1X06-SMD_EDGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-6" package="SCREWTERMINAL-3.5MM-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMDF" package="1X06-SMD-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-FEMALE-V2" package="1X06-SMD-FEMALE-V2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X06_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT" package="1X06_SMD_STRAIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT" package="1X06_SMD_STRAIGHT_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT-COMBO" package="1X06_SMD_STRAIGHT_COMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EM406" package="EM406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M07" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 7&lt;/b&gt;
Standard 7-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).  NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS... This footprint was designed to help hold the alignment of a through-hole component (i.e. 7-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is usually a perfectly straight line). This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes. Because they are alternating, it causes a "brace" to hold the header in place. 0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice. Also, if you push a header all the way into place, it is covered up entirely on the bottom side. This idea of altering the position of holes to aid alignment will be further integrated into the Sparkfun Library for other footprints. It can help hold any component with 3 or more connection pins.</description>
<gates>
<gate name="G$1" symbol="M07"/>
</gates>
<devices>
<device name="" package="1X07">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X07_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X07_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X07_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPINS_HOLES_ONLY" package="1X07_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M08" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 8&lt;/b&gt;
Standard 8-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M08"/>
</gates>
<devices>
<device name="1X08" package="1X08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X08_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X08_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X08_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-8" package="SCREWTERMINAL-3.5MM-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT" package="1X08_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT" package="1X08_SMD_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-COMBO" package="1X08_SMD_COMBINED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BM08B-SRSS-TB" package="BM08B-SRSS-TB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M08X2">
<description>.1" headers, two rows of 8 each</description>
<gates>
<gate name="G$1" symbol="M2X8"/>
</gates>
<devices>
<device name="" package="2X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M09" prefix="JP">
<description>&lt;b&gt;Header 9&lt;/b&gt;
Standard 9-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M09"/>
</gates>
<devices>
<device name="" package="1X09">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X09_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK-LONGPADS" package="1X09_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X09_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M10" prefix="JP">
<description>&lt;b&gt;Header 10&lt;/b&gt;
Standard 10-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M10"/>
</gates>
<devices>
<device name="&quot;" package="1X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X10-2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MMSMD" package="1X10-2MM-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X10_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X10_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M10X2">
<description>This was SPECIALLY designed to be used with our Graphic LCD Backpack.  Be sure you want to use this!  It is not only staggered on each line of header holes, but IT IS ALSO offset of the center point of the top and bottom lines by 5 mil.  This causes the headers to lock into place on the "standard" footprint on the LCD screen.  The extra squares on the tdocu layer are there simply to reference other pins (if you were to actually populate a longer header than ten long - this is what we do with the backpacks).</description>
<gates>
<gate name="G$1" symbol="M10X2"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X10_LOCK" package="2X10_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="2X10_LOCK_SPECIAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="2X10_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M12" prefix="JP">
<description>&lt;b&gt;Header 12&lt;/b&gt;
Standard 12-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M12"/>
</gates>
<devices>
<device name="PTH" package="1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X12_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X12_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MACHINE-PIN_LOCK" package="1X12_MACHINE-PIN-HEADER_LOCK.004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X12_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X12_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M13" prefix="JP">
<description>13-pin single row .1" header</description>
<gates>
<gate name="G$1" symbol="M13"/>
</gates>
<devices>
<device name="" package="1X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X13-LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M14" prefix="JP">
<description>&lt;b&gt;Header 14&lt;/b&gt;
Standard 14-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M14"/>
</gates>
<devices>
<device name="" package="1X14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X14_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X14_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X14-LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M15" prefix="JP">
<description>&lt;b&gt;Header 15&lt;/b&gt;
Standard 15-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M15"/>
</gates>
<devices>
<device name="" package="1X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X15_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X15_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M17">
<description>1x17 .1" header</description>
<gates>
<gate name="G$1" symbol="M17"/>
</gates>
<devices>
<device name="" package="1X17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M18">
<description>1x18 .1" header</description>
<gates>
<gate name="G$1" symbol="M18"/>
</gates>
<devices>
<device name="_" package="1X18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M20" prefix="JP">
<description>1x20 .1" header&lt;br&gt;
This is just like the LOCK variant in that the holes are staggared by 5 mil, but except for the last two holes.  They are not altered from the "standard" footprint layout.  This is used for a special purpose on the layout of our Graphic LCD Backpack.  Make sure you want to use this device before selecting it for you project!</description>
<gates>
<gate name="G$1" symbol="M20"/>
</gates>
<devices>
<device name="" package="1X20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X20_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X20_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="1X20_LOCK_SPECIAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M24">
<description>1x24 .1" header</description>
<gates>
<gate name="G$1" symbol="M24"/>
</gates>
<devices>
<device name="" package="1X24">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X24_LONGPADS">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M25" prefix="JP">
<description>1x25 .1" header</description>
<gates>
<gate name="G$1" symbol="M25"/>
</gates>
<devices>
<device name="PTH" package="1X25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X25_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X25_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X25_LONGPAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M27">
<description>1x27 .1" header</description>
<gates>
<gate name="G$1" symbol="M27"/>
</gates>
<devices>
<device name="" package="1X27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M40">
<description>1x40 .1" header</description>
<gates>
<gate name="G$1" symbol="M40"/>
</gates>
<devices>
<device name="OFFSET" package="1X40_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK" prefix="J">
<description>RJ-45 with LEDs</description>
<gates>
<gate name="G$1" symbol="MAGJACK"/>
</gates>
<devices>
<device name="" package="MAGJACK">
<connects>
<connect gate="G$1" pin="GLED+" pad="11"/>
<connect gate="G$1" pin="GLED-" pad="12"/>
<connect gate="G$1" pin="RCT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD@0" pad="M1"/>
<connect gate="G$1" pin="SHIELD@1" pad="M2"/>
<connect gate="G$1" pin="TCT" pad="6"/>
<connect gate="G$1" pin="TD+" pad="7"/>
<connect gate="G$1" pin="TD-" pad="8"/>
<connect gate="G$1" pin="YLED+" pad="9"/>
<connect gate="G$1" pin="YLED-" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK-2" prefix="J">
<description>RJ-45 with LEDs</description>
<gates>
<gate name="G$1" symbol="MAGJACK-2"/>
</gates>
<devices>
<device name="" package="MAGJACK-19938">
<connects>
<connect gate="G$1" pin="GLED+" pad="10"/>
<connect gate="G$1" pin="GLED-" pad="9"/>
<connect gate="G$1" pin="RCT" pad="2"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="3"/>
<connect gate="G$1" pin="SHIELD" pad="8"/>
<connect gate="G$1" pin="TCT" pad="5"/>
<connect gate="G$1" pin="TD+" pad="4"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="YLED+" pad="12"/>
<connect gate="G$1" pin="YLED-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK-POE" prefix="U">
<description>&lt;h3&gt;PoE compatible MagJack&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="MAGJACK-POE"/>
</gates>
<devices>
<device name="" package="MAGJACK-POE">
<connects>
<connect gate="G$1" pin="GLED+" pad="13"/>
<connect gate="G$1" pin="GLED-" pad="14"/>
<connect gate="G$1" pin="RCT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD@0" pad="GND0"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND1"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="5"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
<connect gate="G$1" pin="YLED+" pad="11"/>
<connect gate="G$1" pin="YLED-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIDI_CONN_FEMALE_SUPPORT">
<description>MIDI connector with strain relief (DIN-5 female)</description>
<gates>
<gate name="G$1" symbol="MIDI_CONN_FEMALE"/>
</gates>
<devices>
<device name="" package="DIN_5_FEMALE_SUPPORT">
<connects>
<connect gate="G$1" pin="MIDI_IN" pad="4"/>
<connect gate="G$1" pin="MIDI_OUT" pad="5"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="NC3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIDI_CONN_FEMALE">
<description>MIDI connector, no strain relieve (DIN-5 female)</description>
<gates>
<gate name="G$1" symbol="MIDI_CONN_FEMALE"/>
</gates>
<devices>
<device name="" package="DIN_5_FEMALE">
<connects>
<connect gate="G$1" pin="MIDI_IN" pad="4"/>
<connect gate="G$1" pin="MIDI_OUT" pad="5"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="NC3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MINI-DIN6">
<description>&lt;b&gt;mini DIN 6 Connector&lt;/b&gt;
Commonly found on the back of a computer for PS2 keyboard and mice. Schematic and footprint are proven. Spark Fun Electronics SKU : PRT-08509</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="PTH" package="MINI-DIN6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA_ACCEL_CONNECTOR">
<gates>
<gate name="G$1" symbol="MMA_CON"/>
</gates>
<devices>
<device name="" package="1X08">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GS1" pad="6"/>
<connect gate="G$1" pin="GS2" pad="7"/>
<connect gate="G$1" pin="SLP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="X" pad="3"/>
<connect gate="G$1" pin="Y" pad="4"/>
<connect gate="G$1" pin="Z" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OBDII">
<description>OBDII connector footprint</description>
<gates>
<gate name="G$1" symbol="OBDII"/>
</gates>
<devices>
<device name="" package="OBDII">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="BATTPOWER" pad="16"/>
<connect gate="G$1" pin="CANHIGH" pad="6"/>
<connect gate="G$1" pin="CANLOW" pad="14"/>
<connect gate="G$1" pin="CHASGND" pad="4"/>
<connect gate="G$1" pin="ISOK-LINE" pad="7"/>
<connect gate="G$1" pin="ISOL-LINE" pad="15"/>
<connect gate="G$1" pin="J1850BUS" pad="10"/>
<connect gate="G$1" pin="J1850BUS+" pad="2"/>
<connect gate="G$1" pin="SIGGND" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC-ICSP">
<description>ISCP Programming connector for UAV, UBW Kit, etc.</description>
<gates>
<gate name="G$1" symbol="ICSP-PIC"/>
</gates>
<devices>
<device name="PTH" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGC" pad="2"/>
<connect gate="G$1" pin="PGD" pad="3"/>
<connect gate="G$1" pin="PGM" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGC" pad="2"/>
<connect gate="G$1" pin="PGD" pad="3"/>
<connect gate="G$1" pin="PGM" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC-ICSP-MINI">
<description>&lt;b&gt;PIC-ICSP-Mini&lt;/b&gt;
Miniature 5-pin connection for temporary programming of PICs. Use this device in your design to save space. Program the PIC with this adapter Spark Fun Electronics SKU : BOB-00194</description>
<gates>
<gate name="G$1" symbol="PIC-ISCP-MINI"/>
</gates>
<devices>
<device name="" package="PIC-ICSP-MINI">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PGC" pad="5"/>
<connect gate="G$1" pin="PGD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINH2X12">
<gates>
<gate name="G$1" symbol="PINH2X12"/>
</gates>
<devices>
<device name="" package="2X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X26">
<gates>
<gate name="G$1" symbol="PINH2X26"/>
</gates>
<devices>
<device name="" package="2X26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_JACK" prefix="J">
<description>&lt;b&gt;Power Jack&lt;/b&gt;
This is the standard 5.5mm barrel jack for power.&lt;br&gt;
The PTH is the most common, proven, reliable, footprint.&lt;br&gt;
The Slot footprint only works if the mill layer is transmitted to the PCB fab house so be warned.&lt;br&gt;
Spark Fun Electronics SKU : PRT-00119&lt;br&gt;
SMT: CONN-08106&lt;br&gt;

Mating wall wart : TOL-00298 (and others)</description>
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="SMD" package="POWER_JACK_SMD">
<connects>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="VIN0"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08106"/>
<attribute name="VALUE" value="5.5x2.1mm Barrel"/>
</technology>
</technologies>
</device>
<device name="SLT" package="POWER_JACK_SLOT">
<connects>
<connect gate="G$1" pin="GND" pad="GND@2"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND@1"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="POWER_JACK_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="COMBO" package="POWER_JACK_COMBO">
<connects>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="POWER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="POWER_JACK_PTH_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSP_CONNECTOR">
<description>Connector for LCD-08335</description>
<gates>
<gate name="G$1" symbol="PSP_CONNECTOR"/>
</gates>
<devices>
<device name="" package="PSP_CONNECTOR">
<connects>
<connect gate="G$1" pin="AVDD" pad="AVDD"/>
<connect gate="G$1" pin="AVDD2" pad="AVDD2"/>
<connect gate="G$1" pin="B0" pad="B0"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="CK" pad="CK"/>
<connect gate="G$1" pin="DISP" pad="DISP"/>
<connect gate="G$1" pin="G0" pad="G0"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="G3" pad="G3"/>
<connect gate="G$1" pin="G4" pad="G4"/>
<connect gate="G$1" pin="G5" pad="G5"/>
<connect gate="G$1" pin="G6" pad="G6"/>
<connect gate="G$1" pin="G7" pad="G7"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="HSYNC" pad="HSYNC"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="R0" pad="R0"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="R3" pad="R3"/>
<connect gate="G$1" pin="R4" pad="R4"/>
<connect gate="G$1" pin="R5" pad="R5"/>
<connect gate="G$1" pin="R6" pad="R6"/>
<connect gate="G$1" pin="R7" pad="R7"/>
<connect gate="G$1" pin="TEST1" pad="TEST1"/>
<connect gate="G$1" pin="TEST2" pad="TEST2"/>
<connect gate="G$1" pin="TEST3" pad="TEST3"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC2" pad="VCC2"/>
<connect gate="G$1" pin="VSYNC" pad="VSYNC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSP_TOUCH_CONNECTOR">
<description>4-Pin Connector for PSP Touch Screen (LCD-08448)</description>
<gates>
<gate name="G$1" symbol="PSP_TOUCH_CONNECTOR"/>
</gates>
<devices>
<device name="" package="PSP_TOUCH_CONNECTOR">
<connects>
<connect gate="G$1" pin="X1" pad="X1"/>
<connect gate="G$1" pin="X2" pad="X2"/>
<connect gate="G$1" pin="Y1" pad="Y1"/>
<connect gate="G$1" pin="Y2" pad="Y2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ9">
<description>RJ9 connector (e.g., phone handsets)</description>
<gates>
<gate name="G$1" symbol="M04-1"/>
</gates>
<devices>
<device name="PTH" package="RJ9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ11-6" prefix="J">
<description>&lt;b&gt;RJ11 Jack&lt;/b&gt;
Simple 6 pin RJ11 jack. Commonly found on CAT3 devices and Microchip programmers. SKU: PRT-00132</description>
<gates>
<gate name="G$1" symbol="M06"/>
</gates>
<devices>
<device name="PTH" package="RJ11-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45-8">
<description>&lt;b&gt;RJ45 Jack&lt;/b&gt;
Simple RJ45, 8-pin connection - connector for common Cat5, Cat5e, and Cat6 Ethernet cables. Footprint not yet proven in production. Connector sku is PRT-00643; Breakout PCB sku is BOB-00716.</description>
<gates>
<gate name="G$1" symbol="RJ45-8"/>
</gates>
<devices>
<device name="PTH" package="RJ45-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREENKEYMATINGCONNECTOR">
<description>ScreenKey mating connector- PRT-09586</description>
<gates>
<gate name="G$1" symbol="SCREENKEYMATINGCONNECTOR"/>
</gates>
<devices>
<device name="" package="SCREENKEYMATINGCONNECTOR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMHOLDER">
<description>&lt;b&gt;SIM Socket&lt;/b&gt;
Socket for SIM cellular cards. Schematic element and footprint production proven. Spark Fun Electronics SKU : PRT-00548</description>
<gates>
<gate name="G$1" symbol="SIMHOLDER"/>
</gates>
<devices>
<device name="" package="SIMHOLDER">
<connects>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="C3" pad="C3"/>
<connect gate="G$1" pin="C5" pad="C5"/>
<connect gate="G$1" pin="C6" pad="C6"/>
<connect gate="G$1" pin="C7" pad="C7"/>
<connect gate="G$1" pin="SW1" pad="SW1"/>
<connect gate="G$1" pin="SW2" pad="SW2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMHOLDER2">
<description>Alternate SIM card socket.</description>
<gates>
<gate name="G$1" symbol="SIMHOLDER2"/>
</gates>
<devices>
<device name="" package="SIMHOLDER2">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="I/O" pad="6"/>
<connect gate="G$1" pin="RST" pad="2"/>
<connect gate="G$1" pin="SW1" pad="4"/>
<connect gate="G$1" pin="SW2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VPP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMHOLDER3">
<description>Alternate SIM card socket</description>
<gates>
<gate name="G$1" symbol="SIMHOLDER3"/>
</gates>
<devices>
<device name="" package="SIMHOLDER3">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="I/O" pad="4"/>
<connect gate="G$1" pin="RST" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VPP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMARTCARD" prefix="JP">
<description>Smart card socket- PRT-09368</description>
<gates>
<gate name="G$1" symbol="SMARTCARD"/>
</gates>
<devices>
<device name="SMD" package="SMARTCARD">
<connects>
<connect gate="G$1" pin="C4" pad="C4"/>
<connect gate="G$1" pin="C8" pad="C8"/>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="I/O" pad="C7"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="SW1" pad="P1"/>
<connect gate="G$1" pin="SW2" pad="P2"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
<connect gate="G$1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA_EDGE" prefix="J$">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;
End launch SMA connector. The paste layer has been removed so that the connector can be hand soldered onto the board after reflow.</description>
<gates>
<gate name="1" symbol="SMA_EDGE"/>
</gates>
<devices>
<device name="" package="SMA-EDGE">
<connects>
<connect gate="1" pin="GND@0" pad="GND@0"/>
<connect gate="1" pin="GND@1" pad="GND@1"/>
<connect gate="1" pin="GND@2" pad="GND@2"/>
<connect gate="1" pin="GND@3" pad="GND@3"/>
<connect gate="1" pin="SIGNAL" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STARBOARD_GND" prefix="J" uservalue="yes">
<description>&lt;h3&gt;StarBoard ground Pad&lt;/h3&gt;
Starboard pads sans the star cutout in top layer</description>
<gates>
<gate name="G$1" symbol="STARBOARD_PAD"/>
</gates>
<devices>
<device name="" package="STARBOARD_GROUND">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMALL" package="STARBOARD_GROUND_SMALL">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-WIDE" package="STARBOARD_GROUND_WIDE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMALL2" package="STARBOARD_GROUND_SMALL2">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STARBOARD_PWR" prefix="J" uservalue="yes">
<description>&lt;h3&gt;StarbBoard Power pad&lt;/h3&gt;
Power pads are designated by the star cutout in the top layer.</description>
<gates>
<gate name="G$1" symbol="STARBOARD_PAD+"/>
</gates>
<devices>
<device name="-WIDE" package="STARBOARD_PWR_WIDE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="GROUND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TALL" package="STARBOARD_PWR">
<connects>
<connect gate="G$1" pin="MOUNT" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH-SCREEN">
<description>Nintendo DS touch screen connector LCD-09105</description>
<gates>
<gate name="G$1" symbol="TOUCH-SCREEN"/>
</gates>
<devices>
<device name="" package="TOUCH-SCREEN">
<connects>
<connect gate="G$1" pin="TS1" pad="P$4"/>
<connect gate="G$1" pin="TS2" pad="P$3"/>
<connect gate="G$1" pin="TS3" pad="P$2"/>
<connect gate="G$1" pin="TS4" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U.FL">
<description>SMD antenna connector- WRL-09144</description>
<gates>
<gate name="G$1" symbol="U.FL"/>
</gates>
<devices>
<device name="" package="U.FL">
<connects>
<connect gate="G$1" pin="GND@0" pad="P$1"/>
<connect gate="G$1" pin="GND@1" pad="P$2"/>
<connect gate="G$1" pin="SIGNAL" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="JP">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139/CONN-08278
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested
&lt;P&gt;USB-MICROB has been used. CONN-09505</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D-"/>
<connect gate="G$1" pin="D-" pad="D+"/>
<connect gate="G$1" pin="GND" pad="VBUS"/>
<connect gate="G$1" pin="VBUS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OLD" package="USB-MINIB-OLD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08278"/>
<attribute name="VALUE" value="USB-B"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCB" package="USB-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_P"/>
<connect gate="G$1" pin="D-" pad="USB_M"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="5V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-VERTICAL" package="USB-B-PTH-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-A-S-NOSILK" package="USB-A-S-NOSILK">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-SMD" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09520"/>
</technology>
</technologies>
</device>
<device name="-SMD-NS" package="USB-MINIB-NOSTOP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09505"/>
</technology>
</technologies>
</device>
<device name="A-SMD-MALE" package="USB-A-SMT-MALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB+SHIELD">
<description>&lt;h3&gt;USB+Shield&lt;/h3&gt;
USB connector with shield pins connectable</description>
<gates>
<gate name="G$1" symbol="USB+SHIELD"/>
</gates>
<devices>
<device name="" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="P$1" pad="S1"/>
<connect gate="G$1" pin="P$2" pad="S2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-MINIB">
<description>&lt;b&gt;Mini-USB "B" connector with 5th pin broken out.&lt;/b&gt;&lt;p&gt;
Created new symbol breaking out 5th "ID" pin in mini/micro USB connector spec.  See: http://en.wikipedia.org/wiki/Mini_usb#Cables.  Uses same footprint as 4-pin symbol.&lt;p&gt;
 

Also added pins to connect to mounting / shield pads if required (probably not generally needed as signals aren't shielded once they leave the connector).</description>
<gates>
<gate name="G$1" symbol="USB-5PIN"/>
</gates>
<devices>
<device name="-5PIN" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="MTN1" pad="MTN3"/>
<connect gate="G$1" pin="MTN2" pad="MTN1"/>
<connect gate="G$1" pin="MTN3" pad="MTN2"/>
<connect gate="G$1" pin="MTN4" pad="MTN4"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_MICROB_PLUG" prefix="JP">
<description>&lt;h3&gt;USB Micro-B Plug&lt;/h3&gt;
Comes in a variety of packages.  Check out Hirose's ZX-x0 line: http://www.hirose.co.jp/cataloge_hp/e24200011.pdf</description>
<gates>
<gate name="G$1" symbol="MICROB-PLUG"/>
</gates>
<devices>
<device name="" package="MICRO-B-RA-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH" package="MICRO-B-RA-TH">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH2" package="MICRO-B-TH">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT" package="MICRO-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USD-SOCKET" prefix="U">
<description>&lt;b&gt;microSD Socket&lt;/b&gt;
Push-push type uSD socket. Schematic element and footprint production proven. Spark Fun Electronics SKU : PRT-00127. tDoc lines correctly indicate media card edge positions when inserting (unlocked, locked, depressed).</description>
<gates>
<gate name="G$1" symbol="USDCARD"/>
</gates>
<devices>
<device name="USD" package="USD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="CD1"/>
<connect gate="G$1" pin="SHIELD@2" pad="CD2"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="SHIELD@4" pad="GND2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEW" package="MICRO-SD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND3"/>
<connect gate="G$1" pin="SHIELD@2" pad="CD1"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="SHIELD@4" pad="CD2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WATN001002BF" prefix="U">
<description>connector for 10x2 16-segment E-paper Display (LCD-10150)&lt;br&gt;
&lt;b&gt;***Unproven!!!***&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="WATN001001"/>
</gates>
<devices>
<device name="" package="FFC26">
<connects>
<connect gate="G$1" pin="DI0" pad="16"/>
<connect gate="G$1" pin="DI1" pad="17"/>
<connect gate="G$1" pin="DI2" pad="18"/>
<connect gate="G$1" pin="DLY0" pad="13"/>
<connect gate="G$1" pin="DLY1" pad="14"/>
<connect gate="G$1" pin="EIO1" pad="6"/>
<connect gate="G$1" pin="EIO2" pad="20"/>
<connect gate="G$1" pin="LATCH" pad="9"/>
<connect gate="G$1" pin="RESERVED@1" pad="10"/>
<connect gate="G$1" pin="RESERVED@2" pad="15"/>
<connect gate="G$1" pin="RESERVED@3" pad="19"/>
<connect gate="G$1" pin="RESERVED@4" pad="26"/>
<connect gate="G$1" pin="SHL" pad="11"/>
<connect gate="G$1" pin="SLEEPB" pad="12"/>
<connect gate="G$1" pin="V0@1" pad="1"/>
<connect gate="G$1" pin="V0@2" pad="25"/>
<connect gate="G$1" pin="V1@1" pad="2"/>
<connect gate="G$1" pin="V1@2" pad="24"/>
<connect gate="G$1" pin="V2@1" pad="3"/>
<connect gate="G$1" pin="V2@2" pad="23"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="21"/>
<connect gate="G$1" pin="VSSE@1" pad="4"/>
<connect gate="G$1" pin="VSSE@2" pad="22"/>
<connect gate="G$1" pin="XCK" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XLR3_NCFAH2" prefix="XLR">
<description>XLR connector</description>
<gates>
<gate name="G$1" symbol="XLR3_NCFAH2"/>
</gates>
<devices>
<device name="" package="XLR3_NC3FAH2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="G" pad="G"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZIFSOCKET-28-3">
<description>Lever-action ZIF socket for 28-pin ICs</description>
<gates>
<gate name="G$1" symbol="DIL-28-3"/>
</gates>
<devices>
<device name="ZIFFSOCKET-28-3" package="DIL28-3-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZIFSOCKET-40-6">
<description>Lever-action ZIF socket for 40-pin ICs</description>
<gates>
<gate name="G$1" symbol="DIL-40-6"/>
</gates>
<devices>
<device name="DIL40-6-ZIF_SOCKET" package="DIL40-6-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZUNE_CONNECTOR_MALE">
<description>Male connector for the Zune media player.  UNPROVEN FOOTPRINT!  This connector must be used only with a 1.2mm PCB thickness.</description>
<gates>
<gate name="G$1" symbol="ZUNE_CONNECTOR_MALE"/>
</gates>
<devices>
<device name="" package="ZUNE_CONNECTOR_MALE">
<connects>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="AUDIO_L" pad="P$13"/>
<connect gate="G$1" pin="AUDIO_R" pad="P$14"/>
<connect gate="G$1" pin="GND@19" pad="P$19"/>
<connect gate="G$1" pin="GND@22" pad="P$22"/>
<connect gate="G$1" pin="GND@23" pad="P$23"/>
<connect gate="G$1" pin="GND@24" pad="P$24"/>
<connect gate="G$1" pin="USB_5V@1" pad="P$1"/>
<connect gate="G$1" pin="USB_5V@2" pad="P$2"/>
<connect gate="G$1" pin="USB_5V@3" pad="P$3"/>
<connect gate="G$1" pin="USB_DATA+" pad="P$21"/>
<connect gate="G$1" pin="USB_DATA-" pad="P$20"/>
<connect gate="G$1" pin="VIDEO+" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-PIN-CENTRONICS-F">
<gates>
<gate name="G$1" symbol="50-PIN-CENTRONICS"/>
</gates>
<devices>
<device name="FEMALE" package="50-PIN-CENTRONICS-F">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$17" pad="P$17"/>
<connect gate="G$1" pin="P$18" pad="P$18"/>
<connect gate="G$1" pin="P$19" pad="P$19"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$20" pad="P$20"/>
<connect gate="G$1" pin="P$21" pad="P$21"/>
<connect gate="G$1" pin="P$22" pad="P$22"/>
<connect gate="G$1" pin="P$23" pad="P$23"/>
<connect gate="G$1" pin="P$24" pad="P$24"/>
<connect gate="G$1" pin="P$25" pad="P$25"/>
<connect gate="G$1" pin="P$26" pad="P$26"/>
<connect gate="G$1" pin="P$27" pad="P$27"/>
<connect gate="G$1" pin="P$28" pad="P$28"/>
<connect gate="G$1" pin="P$29" pad="P$29"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$30" pad="P$30"/>
<connect gate="G$1" pin="P$31" pad="P$31"/>
<connect gate="G$1" pin="P$32" pad="P$32"/>
<connect gate="G$1" pin="P$33" pad="P$33"/>
<connect gate="G$1" pin="P$34" pad="P$34"/>
<connect gate="G$1" pin="P$35" pad="P$35"/>
<connect gate="G$1" pin="P$36" pad="P$36"/>
<connect gate="G$1" pin="P$37" pad="P$37"/>
<connect gate="G$1" pin="P$38" pad="P$38"/>
<connect gate="G$1" pin="P$39" pad="P$39"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$40" pad="P$40"/>
<connect gate="G$1" pin="P$41" pad="P$41"/>
<connect gate="G$1" pin="P$42" pad="P$42"/>
<connect gate="G$1" pin="P$43" pad="P$43"/>
<connect gate="G$1" pin="P$44" pad="P$44"/>
<connect gate="G$1" pin="P$45" pad="P$45"/>
<connect gate="G$1" pin="P$46" pad="P$46"/>
<connect gate="G$1" pin="P$47" pad="P$47"/>
<connect gate="G$1" pin="P$48" pad="P$48"/>
<connect gate="G$1" pin="P$49" pad="P$49"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$50" pad="P$50"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="50-PIN-CENTRONICS-M">
<gates>
<gate name="G$1" symbol="50-PIN-CENTRONICS"/>
</gates>
<devices>
<device name="MALE" package="50-PIN-CENTRONICS-M">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$17" pad="P$17"/>
<connect gate="G$1" pin="P$18" pad="P$18"/>
<connect gate="G$1" pin="P$19" pad="P$19"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$20" pad="P$20"/>
<connect gate="G$1" pin="P$21" pad="P$21"/>
<connect gate="G$1" pin="P$22" pad="P$22"/>
<connect gate="G$1" pin="P$23" pad="P$23"/>
<connect gate="G$1" pin="P$24" pad="P$24"/>
<connect gate="G$1" pin="P$25" pad="P$25"/>
<connect gate="G$1" pin="P$26" pad="P$26"/>
<connect gate="G$1" pin="P$27" pad="P$27"/>
<connect gate="G$1" pin="P$28" pad="P$28"/>
<connect gate="G$1" pin="P$29" pad="P$29"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$30" pad="P$30"/>
<connect gate="G$1" pin="P$31" pad="P$31"/>
<connect gate="G$1" pin="P$32" pad="P$32"/>
<connect gate="G$1" pin="P$33" pad="P$33"/>
<connect gate="G$1" pin="P$34" pad="P$34"/>
<connect gate="G$1" pin="P$35" pad="P$35"/>
<connect gate="G$1" pin="P$36" pad="P$36"/>
<connect gate="G$1" pin="P$37" pad="P$37"/>
<connect gate="G$1" pin="P$38" pad="P$38"/>
<connect gate="G$1" pin="P$39" pad="P$39"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$40" pad="P$40"/>
<connect gate="G$1" pin="P$41" pad="P$41"/>
<connect gate="G$1" pin="P$42" pad="P$42"/>
<connect gate="G$1" pin="P$43" pad="P$43"/>
<connect gate="G$1" pin="P$44" pad="P$44"/>
<connect gate="G$1" pin="P$45" pad="P$45"/>
<connect gate="G$1" pin="P$46" pad="P$46"/>
<connect gate="G$1" pin="P$47" pad="P$47"/>
<connect gate="G$1" pin="P$48" pad="P$48"/>
<connect gate="G$1" pin="P$49" pad="P$49"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$50" pad="P$50"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCA" prefix="JP">
<gates>
<gate name="G$1" symbol="RCA"/>
</gates>
<devices>
<device name="" package="RCA">
<connects>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHELL" pad="SHELL"/>
<connect gate="G$1" pin="SWITCH" pad="SWITCH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LOCK" package="RCA_LOCK">
<connects>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHELL" pad="SHELL"/>
<connect gate="G$1" pin="SWITCH" pad="SWITCH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_AB">
<description>This is a USB AB connector that is compatible with USB OTG. i.e. this connector can serve as a host or device</description>
<gates>
<gate name="G$1" symbol="USB_AB"/>
</gates>
<devices>
<device name="" package="USB-AB-MICRO-SMD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="USBID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M16" prefix="JP">
<description>1x16 .1" header</description>
<gates>
<gate name="G$1" symbol="M16"/>
</gates>
<devices>
<device name="PTH" package="1X16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X16_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X16_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MACHIINE-PIN_LOCK" package="1X16_MACHINE-PIN-HEADER_LOCK.004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X16_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X16_NO_SILK" package="1X16_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M19">
<description>1x19 .1" header</description>
<gates>
<gate name="G$1" symbol="M19"/>
</gates>
<devices>
<device name="1X19" package="1X19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X19_NO_SILK" package="1X19_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M11" prefix="JP">
<description>&lt;b&gt;Header 11&lt;/b&gt;
Standard 11-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M11"/>
</gates>
<devices>
<device name="PTH" package="1X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X11-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X11_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X11_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X11_SMD_PTHCOMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X11_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_NO_HOLES" package="1X11_SMD_NO_HOLES">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X11_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X11_NO_SILK" package="1X11_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMPUTER-PERIPHERAL-POWER" prefix="J">
<gates>
<gate name="G$1" symbol="COMPUTER-PERIPHERAL-POWER"/>
</gates>
<devices>
<device name="RA" package="COMPUTER-PERIPHERAL-POWER-RA">
<connects>
<connect gate="G$1" pin="12V" pad="12V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="NC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VERTICAL" package="COMPUTER-PERIPHERAL-POWER">
<connects>
<connect gate="G$1" pin="12V" pad="12V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="NC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD_CARD_SOCKET" prefix="U">
<description>SD Memory Card Connector, push-push normal type, CD enable, WP enable</description>
<gates>
<gate name="G$1" symbol="SDCARD-1"/>
</gates>
<devices>
<device name="4UCON" package="SDCARD_4UCONN">
<connects>
<connect gate="G$1" pin="CD" pad="CD"/>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="SH@1" pad="SH@1"/>
<connect gate="G$1" pin="SH@2" pad="SH@2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WP" pad="WP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI_DEVICE" prefix="JP">
<description>Connector which mates to FTDI basic or FTDI cable.</description>
<gates>
<gate name="G$1" symbol="FTDI_DEVICE"/>
</gates>
<devices>
<device name="" package="FTDI_DEVICE_SIDE">
<connects>
<connect gate="G$1" pin="CTS" pad="P$5"/>
<connect gate="G$1" pin="DTR" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$6"/>
<connect gate="G$1" pin="RXI" pad="P$3"/>
<connect gate="G$1" pin="TXO" pad="P$2"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MYDAQ" prefix="JP">
<gates>
<gate name="G$1" symbol="MYDAQ_CONNECTOR"/>
</gates>
<devices>
<device name="" package="3.81MM_TERMINAL_BLOCK_FEMALE_LOCKING">
<connects>
<connect gate="G$1" pin="+15V" pad="1"/>
<connect gate="G$1" pin="-15V" pad="2"/>
<connect gate="G$1" pin="5V" pad="20"/>
<connect gate="G$1" pin="AGND_15V" pad="3"/>
<connect gate="G$1" pin="AGND_IO" pad="6"/>
<connect gate="G$1" pin="AI0+" pad="7"/>
<connect gate="G$1" pin="AI0-" pad="8"/>
<connect gate="G$1" pin="AI1+" pad="9"/>
<connect gate="G$1" pin="AN1-" pad="10"/>
<connect gate="G$1" pin="AO0" pad="4"/>
<connect gate="G$1" pin="AO1" pad="5"/>
<connect gate="G$1" pin="DGND" pad="19"/>
<connect gate="G$1" pin="DIO0" pad="11"/>
<connect gate="G$1" pin="DIO1" pad="12"/>
<connect gate="G$1" pin="DIO2" pad="13"/>
<connect gate="G$1" pin="DIO3" pad="14"/>
<connect gate="G$1" pin="DIO4" pad="15"/>
<connect gate="G$1" pin="DIO5" pad="16"/>
<connect gate="G$1" pin="DIO6" pad="17"/>
<connect gate="G$1" pin="DIO7" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-AB" prefix="U" uservalue="yes">
<description>This is a USB AB connector that is compatible with USB OTG. i.e. this connector can serve as a host or device</description>
<gates>
<gate name="G$1" symbol="USB_AB"/>
</gates>
<devices>
<device name="" package="USB-AB-MICRO-SMD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="USBID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB15">
<description>DB15 / VGA right angle through-hole female connector.</description>
<gates>
<gate name="G$1" symbol="DB15"/>
</gates>
<devices>
<device name="" package="DB15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M03X2" prefix="JP" uservalue="yes">
<description>2x3 .1" header.&lt;br&gt;
Shrouded, with keying- CONN-10681&lt;br&gt;
SMT- CONN-11415&lt;br&gt;
Pogo pins- HW-11044</description>
<gates>
<gate name="G$1" symbol="M03X2"/>
</gates>
<devices>
<device name="" package="2X3-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10681"/>
</technology>
</technologies>
</device>
<device name="SMT" package="2X3_SMT_POSTS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11415"/>
</technology>
</technologies>
</device>
<device name="POGO_PINS" package="2X3_POGO">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="HW-11044"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO-JACK3">
<description>Audio jack - 3.5mm TRRS variety - two rings.</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK3-TRRS"/>
</gates>
<devices>
<device name="" package="AUDIO-JACK-TRRS-SMD">
<connects>
<connect gate="G$1" pin="EARTH" pad="EARTH"/>
<connect gate="G$1" pin="RING1" pad="RING1"/>
<connect gate="G$1" pin="RING2" pad="RING2"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_2MM_MALE" prefix="J" uservalue="yes">
<description>Mates to single-cell LiPo batteries.&lt;br&gt;
CONN-08352</description>
<gates>
<gate name="G$1" symbol="JST_2MM_MALE"/>
</gates>
<devices>
<device name="" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
<connect gate="G$1" pin="PAD1" pad="NC1"/>
<connect gate="G$1" pin="PAD2" pad="NC2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08352"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M13X2" prefix="JP">
<description>0.1" spaced headers</description>
<gates>
<gate name="G$1" symbol="M13X2"/>
</gates>
<devices>
<device name="2X13" package="2X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
