<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08WIDE">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="QFN-44">
</package>
<package name="QFN-44-NOPAD">
</package>
<package name="TQFP64">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
<package name="TQFP64_14X14MM">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 14x14x1mm Body</description>
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;100-lead Thin Quad Flat Pack Package Outline&lt;/b&gt;</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="QFN20">
</package>
<package name="DIL28-EZ">
<description>28-pin "EZ" package.&lt;br&gt;
Pin 28 is clipped during kitting to key the chip.&lt;br&gt;
Pins are spaced a little wider than normal to ease insertion.&lt;br&gt;
Top mask deleted so solder can ONLY be applied on bottom.</description>
</package>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
<package name="DIL28-3-SIMON">
</package>
<package name="DIL28-3-ZIF_SOCKET">
</package>
<package name="DIL28-3-SIMON-KIT">
<description>&lt;h3&gt;DIL-28-3-SIMON-KIT&lt;/h3&gt;
28-pin DIL package&lt;br&gt;
Used for the ATmega328 on our Simon Kit&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="MLP28">
<description>&lt;b&gt;MLP 28&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP2101.pdf</description>
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="LQFP-32">
<description>&lt;b&gt;Quad Flat Package&lt;/b&gt; 32 LD LQFP&lt;p&gt;
Source: ds232b12.pdf&lt;br&gt;
http://www.ftdichip.com</description>
</package>
<package name="QFN-24">
</package>
<package name="QFN-24_ALT1.PAC">
</package>
<package name="DIL40">
<description>Dual In Line Package: 40-pin PDIP</description>
</package>
<package name="TQFP44">
</package>
<package name="TQFP-100-12X12MM">
</package>
<package name="PQFP208">
</package>
<package name="QFN-32">
<description>&lt;h3&gt;QFN 32-Pin package w/ Thermal Pad&lt;/h3&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
&lt;B&gt;Applicable Parts:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;TLC5940&lt;/ul&gt;</description>
</package>
<package name="LQFP-48">
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO016">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SC70">
</package>
<package name="TSSOP5">
</package>
<package name="SO-28W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="SQFP-S-10X10-64">
<description>&lt;b&gt;QFP64&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="TQFP32-5MM">
</package>
<package name="DIL24">
</package>
<package name="TSSOP28">
</package>
<package name="TSSOP28-GROUNDPAD">
</package>
<package name="SOT23-3">
</package>
<package name="TSOP48">
</package>
<package name="SC70-6">
</package>
<package name="P8X32A-Q44">
</package>
<package name="PSOP-8">
</package>
<package name="SO-24DW">
<description>300-mil body, package type SO</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="SOIC-14">
</package>
<package name="PIC24FXXX_TQFP64">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
<package name="_STN_SCANTOOL_QFN-28-S">
<description>&lt;H1&gt;Quad Flat No Leads package, 28 pin&lt;/H1&gt;
  &lt;tr
&lt;table align=left&gt;
  &lt;tr&gt;&lt;td&gt;&lt;h2&gt;Change Log&lt;/h2&gt;&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;
    &lt;th&gt;Date&lt;/th&gt;&lt;th&gt;Author&lt;/th&gt;&lt;th&gt;Change&lt;/th&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 23, 2010&lt;/td&gt;&lt;td&gt;joe@scantool.net&lt;/td&gt;&lt;td&gt;Added t-keepout layer.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 22, 2010&lt;/td&gt;&lt;td&gt;engineering@scantool.net&lt;/td&gt;&lt;td&gt;Resized per PIC24HJ64GPx02 (QFN-S) datasheet. Fixed tStop and tCream layers. Redesigned silkscreen.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 17, 2010&lt;/td&gt;&lt;td&gt;vitaliy@scantool.net&lt;/td&gt;&lt;td&gt;Verified package.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 17, 2010&lt;/td&gt;&lt;td&gt;jason@scantool.net&lt;/td&gt;&lt;td&gt;Increased silkscreen ratio.&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt;
    &lt;td&gt;March 02, 2010&lt;/td&gt;&lt;td&gt;jason@scantool.net&lt;/td&gt;&lt;td&gt;Copied from Microchip Library.&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;</description>
</package>
<package name="SOIC-18">
</package>
<package name="SOT143">
<description>&lt;h3&gt;SOT143&lt;/h3&gt;
Package is used for the STM811 (also APX811)&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Proven&lt;/b&gt;</description>
</package>
<package name="TSSOP30">
</package>
<package name="UBW32_TQFP100">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="SOIC18-W">
</package>
<package name="QFN-24-USB">
</package>
<package name="LQFP-80">
<description>&lt;h3&gt;LQFP-80&lt;/h3&gt;
80-pin, 10x10mm, 0.4mm pitch, SMD package&lt;br&gt;
Used for WIZnet W5100 (COM-09471)&lt;br&gt;
http://www.sparkfun.com/products/9471
&lt;br&gt;&lt;br&gt;
&lt;b&gt;***UNPROVEN***&lt;/b&gt;</description>
</package>
<package name="SOP-14">
<description>&lt;h3&gt;14-pin SOP-14 package&lt;/h3&gt;
Used on WS2801 RGB controller</description>
</package>
<package name="PQ208">
</package>
<package name="TQFP-100-14X14MM">
</package>
<package name="SQFP-S-10X10-64-XS1">
</package>
<package name="SOT353">
<description>&lt;h3&gt;SOT353 aka SC70-5&lt;/h3&gt;
Used on single circuit logic gates</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;TSOP16&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="SO014">
</package>
<package name="DIL14">
</package>
<package name="TSSOP-24">
<description>&lt;h3&gt;24-pin TSSOP with Exposed Thermal Pad&lt;/h3&gt;
Used on: &lt;ul&gt;
&lt;li&gt;Allegro A6282 16-bit LED driver&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/21/10&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="QFN-24_ALT2">
<description>&lt;h3&gt;24-pin QFN with Exposed Thermal pad&lt;/h3&gt;
Parts that use this package:
&lt;ul&gt;
&lt;li&gt;A6282&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;br&gt;
&lt;b&gt;***UNPROVEN***&lt;/b&gt;&lt;BR&gt;</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
<package name="SOP20">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
<package name="SOP20W">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL24-4">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.4 inch</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL24-9">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.9 inch</description>
</package>
<package name="SSOP_20">
<description>20-pin .65mm pitch/5.2mm body SMT</description>
</package>
<package name="DIL40_0.9">
<description>Dual inline 40 pin package for mbed microcontroller development platform.</description>
</package>
<package name="SO14">
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SPARKFUN-DIGITALIC_QFN-44">
</package>
<package name="SPARKFUN-DIGITALIC_QFN-44-NOPAD">
</package>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
<package name="QFN-28">
</package>
</packages>
<symbols>
<symbol name="AT25FS010">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="HOLD" function="dot"/>
<pin name="CS" function="dot"/>
<pin name="WP" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="AT45DB041B">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="RST" function="dot"/>
<pin name="CS" function="dot"/>
<pin name="WP" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="AT45DB161D">
<pin name="CS" function="dot"/>
<pin name="RST" function="dot"/>
<pin name="SCK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="WP" function="dot"/>
</symbol>
<symbol name="ATMEGA8U2">
<pin name="AVCC"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="PB0"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6(RTS)"/>
<pin name="PD7(CTS)"/>
<pin name="RESET/PC1"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VCC"/>
<pin name="XTAL1"/>
<pin name="XTAL2/PC0"/>
</symbol>
<symbol name="ATMEGA32U4">
<pin name="!RESET"/>
<pin name="AREF"/>
<pin name="AVCC@24"/>
<pin name="AVCC@44"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND@15"/>
<pin name="GND@23"/>
<pin name="GND@35"/>
<pin name="GND@43"/>
<pin name="PB0(SS)"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4(ADC11)"/>
<pin name="PB5(ADC12)"/>
<pin name="PB6(ADC13)"/>
<pin name="PB7"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0(SCL)"/>
<pin name="PD1(SDA)"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4(ADC8)"/>
<pin name="PD5"/>
<pin name="PD6(ADC9)"/>
<pin name="PD7(ADC10)"/>
<pin name="PE2/!HWB"/>
<pin name="PE6"/>
<pin name="PF0(ADC0)"/>
<pin name="PF1(ADC1)"/>
<pin name="PF4(ADC4)"/>
<pin name="PF5(ADC5)"/>
<pin name="PF6(ADC6)"/>
<pin name="PF7(ADC7)"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VBUS"/>
<pin name="VCC@14"/>
<pin name="VCC@34"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
</symbol>
<symbol name="ATMEGA128">
<pin name="VCC@21"/>
<pin name="VCC@52"/>
<pin name="AVCC"/>
<pin name="AREF"/>
<pin name="RESET"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AGND"/>
<pin name="GND@53"/>
<pin name="GND@22"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PE0(RXD)"/>
<pin name="PE1(TXD)"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1(SDA)"/>
<pin name="PD0(SCL)"/>
<pin name="PC7"/>
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="PB7"/>
<pin name="PB6"/>
<pin name="PB5"/>
<pin name="PB4"/>
<pin name="PB3(MISO)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB1(SCK)"/>
<pin name="PB0(SS)"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
</symbol>
<symbol name="ATMEGAXX8-28PIN">
<description>Symbol for Atmega328/168/88/48 chips, 28-pin versions</description>
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="ATMEGAXX8-28PIN_EZ">
<description>Symbol for Atmega328/168/88/48 chips, 28-pin versions</description>
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="ATMEGAXX8-32PIN">
<description>Symbol for Atmega328/168/88/48 chips, 32-pin version</description>
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="ATMEGA2560">
<pin name="(A8)PC0"/>
<pin name="(A9)PC1"/>
<pin name="(A10)PC2"/>
<pin name="(A11)PC3"/>
<pin name="(A12)PC4"/>
<pin name="(A13)PC5"/>
<pin name="(A14)PC6"/>
<pin name="(A15)PC7"/>
<pin name="(AD0)PA0"/>
<pin name="(AD1)PA1"/>
<pin name="(AD2)PA2"/>
<pin name="(AD3)PA3"/>
<pin name="(AD4)PA4"/>
<pin name="(AD5)PA5"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(ADC0)PF0"/>
<pin name="(ADC1)PF1"/>
<pin name="(ADC2)PF2"/>
<pin name="(ADC3)PF3"/>
<pin name="(ADC4/TCK)PF4"/>
<pin name="(ADC5/TMS)PF5"/>
<pin name="(ADC6/TDO)PF6"/>
<pin name="(ADC7/TDI)PF7"/>
<pin name="(ALE)PG2"/>
<pin name="(CLKO/ICP3/INT7)PE7"/>
<pin name="(ICP1)PD4"/>
<pin name="(MISO/PCINT3)PB3"/>
<pin name="(MOSI/PCINT2)PB2"/>
<pin name="(OC0A/OC1C/PCINT7)PB7"/>
<pin name="(OC0B)PG5"/>
<pin name="(OC1A/PCINT5)PB5"/>
<pin name="(OC1B/PCINT6)PB6"/>
<pin name="(OC2A/PCINT4)PB4"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(RD)PG1"/>
<pin name="(RXD0/PCIN8)PE0"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SCK/PCINT1)PB1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SS/PCINT0)PB0"/>
<pin name="(T0)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(TOSC1)PG4"/>
<pin name="(TOSC2)PG3"/>
<pin name="(TXD0)PE1"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(WR)PG0"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(XCK1)PD5"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="PH0(RXD2)"/>
<pin name="PH1(TXD2)"/>
<pin name="PH2(XCK2)"/>
<pin name="PH3(OC4A)"/>
<pin name="PH4(OC4B)"/>
<pin name="PH5(OC4C)"/>
<pin name="PH6(OC2B)"/>
<pin name="PH7(T4)"/>
<pin name="PJ0(RXD3/PCINT9)"/>
<pin name="PJ1(TXD3/PCINT10)"/>
<pin name="PJ2(XCK3/PCINT11)"/>
<pin name="PJ3(PCINT12)"/>
<pin name="PJ4(PCINT13)"/>
<pin name="PJ5(PCINT14)"/>
<pin name="PJ6(PCINT15)"/>
<pin name="PJ7"/>
<pin name="PK0(ADC8/PCINT16)"/>
<pin name="PK1(ADC9/PCINT17)"/>
<pin name="PK2(ADC10/PCINT18)"/>
<pin name="PK3(ADC11/PCINT19)"/>
<pin name="PK4(ADC12/PCINT20)"/>
<pin name="PK5(ADC13/PCINT21)"/>
<pin name="PK6(ADC14/PCINT22)"/>
<pin name="PK7(ADC15/PCINT23)"/>
<pin name="PL0(ICP4)"/>
<pin name="PL1(ICP5)"/>
<pin name="PL2(T5)"/>
<pin name="PL3(OC5A)"/>
<pin name="PL4(OC5B)"/>
<pin name="PL5(OC5C)"/>
<pin name="PL6"/>
<pin name="PL7"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
</symbol>
<symbol name="ATTINY13">
<pin name="VCC"/>
<pin name="PB1(MISO)"/>
<pin name="PB5(NRES)"/>
<pin name="GND"/>
<pin name="PB0(MOSI)"/>
<pin name="PB2(SCK/ADC1)"/>
<pin name="PB3(ADC3)"/>
<pin name="PB4(ADC2)"/>
</symbol>
<symbol name="ATTINY24">
<pin name="VCC"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3/RESET"/>
<pin name="PA7/ADC7"/>
<pin name="PA6/MOSI"/>
<pin name="PA5/MISO"/>
<pin name="PA4/SCL"/>
<pin name="PA3/ADC3"/>
<pin name="PA2/ADC2"/>
<pin name="PA1/ADC1"/>
<pin name="PA0/ADC0"/>
<pin name="GND"/>
<pin name="GND@0"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="23-I/O-2">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="VCC@1"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="CP2101">
<pin name="REGIN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VBUS" direction="in"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="!RST"/>
<pin name="SUSPEND" direction="out"/>
<pin name="!SUSPEND" direction="out"/>
<pin name="RI" direction="in"/>
<pin name="DCD" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="DSR" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="GND@EXP" direction="pwr"/>
<pin name="GND@M" direction="pwr"/>
</symbol>
<symbol name="CP2103">
<pin name="REGIN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VBUS" direction="in"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="!RST"/>
<pin name="SUSPEND" direction="out"/>
<pin name="!SUSPEND" direction="out"/>
<pin name="RI" direction="in"/>
<pin name="DCD" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="DSR" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="GND@EXP" direction="pwr"/>
<pin name="GND@M" direction="pwr"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
<pin name="GPIO_3"/>
<pin name="VIO" direction="pwr"/>
</symbol>
<symbol name="CY7C64215">
<pin name="VSS@1"/>
<pin name="P07"/>
<pin name="P05"/>
<pin name="P03"/>
<pin name="P01"/>
<pin name="P25"/>
<pin name="P23"/>
<pin name="P21"/>
<pin name="P17"/>
<pin name="P15"/>
<pin name="P13"/>
<pin name="P11"/>
<pin name="VSS@13"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VDD@16"/>
<pin name="P10"/>
<pin name="P12"/>
<pin name="P14"/>
<pin name="P16"/>
<pin name="P20"/>
<pin name="P22"/>
<pin name="P24"/>
<pin name="P00"/>
<pin name="P02"/>
<pin name="P04"/>
<pin name="P06"/>
<pin name="VDD@28"/>
</symbol>
<symbol name="DOSONCHIP-IC">
<pin name="UART_TX" direction="out"/>
<pin name="CARD_SCLK" direction="out"/>
<pin name="SPI_CS" direction="in" function="dot"/>
<pin name="CARD_DIN"/>
<pin name="CARD_WP" direction="in"/>
<pin name="CARD_CD" direction="in" function="dot"/>
<pin name="XTAL_OUT" direction="out"/>
<pin name="XTAL_IN" direction="in"/>
<pin name="SPI_MOSI" direction="in"/>
<pin name="UART_RX" direction="in"/>
<pin name="SPI_MISO" direction="out"/>
<pin name="SPI_SCLK" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="MODE0" direction="in"/>
<pin name="CARD_DOUT" direction="out"/>
<pin name="CARD_CS" direction="in" function="dot"/>
<pin name="MODE1" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="UART_CTS" direction="in"/>
<pin name="UART_RTS/BUSY" direction="out"/>
<pin name="I2C_SCL"/>
<pin name="I2C_SDA"/>
</symbol>
<symbol name="DSPIC30F4011">
<pin name="MCLR"/>
<pin name="RB0/AREF+"/>
<pin name="RB1/AREF-"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4/IC7"/>
<pin name="RB5/IC8"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RB8"/>
<pin name="VDD0"/>
<pin name="VSS0"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="RC13/TX1"/>
<pin name="RC14/RX1"/>
<pin name="INT0/RE8"/>
<pin name="OC2/RD1"/>
<pin name="RD3"/>
<pin name="VSS1"/>
<pin name="VDD1"/>
<pin name="RD2"/>
<pin name="OC1/RD0"/>
<pin name="RF6/SCK1"/>
<pin name="PGD/SCL"/>
<pin name="PGC/SDA"/>
<pin name="RF5/TX2"/>
<pin name="RF4/RX2"/>
<pin name="RF1"/>
<pin name="RF0"/>
<pin name="VSS2"/>
<pin name="VDD2"/>
<pin name="RE5"/>
<pin name="RE4"/>
<pin name="RE3"/>
<pin name="RE2"/>
<pin name="RE1"/>
<pin name="RE0"/>
<pin name="AVSS"/>
<pin name="AVDD"/>
</symbol>
<symbol name="DSPIC30F6015">
<pin name="VDD@10"/>
<pin name="VDD@26"/>
<pin name="VDD@38"/>
<pin name="VDD@57"/>
<pin name="AVDD@19"/>
<pin name="MCLR@7"/>
<pin name="PGC@17"/>
<pin name="PGD@18"/>
<pin name="OSC1@39"/>
<pin name="OSC2@40"/>
<pin name="RX1@34"/>
<pin name="TX1@33"/>
<pin name="VREF+/RB0@16"/>
<pin name="VREF-/RB1@15"/>
<pin name="RB2@14"/>
<pin name="RB3@13"/>
<pin name="RB4@12"/>
<pin name="RB5@11"/>
<pin name="RB8@21"/>
<pin name="RB9@22"/>
<pin name="RB10@23"/>
<pin name="RB11@24"/>
<pin name="RB12@27"/>
<pin name="RB13@28"/>
<pin name="RB14@29"/>
<pin name="RB15@30"/>
<pin name="GND@56"/>
<pin name="GND@41"/>
<pin name="GND@25"/>
<pin name="GND@9"/>
<pin name="AGND@20"/>
<pin name="RC13@47"/>
<pin name="RC14@48"/>
<pin name="RD0@46"/>
<pin name="RD1@49"/>
<pin name="RD2@50"/>
<pin name="RD3@51"/>
<pin name="RD4@52"/>
<pin name="RD5@53"/>
<pin name="RD6@54"/>
<pin name="RD7@55"/>
<pin name="RG8@6"/>
<pin name="RG9@8"/>
<pin name="RG2@37"/>
<pin name="RD8@42"/>
<pin name="RF6@35"/>
<pin name="RG3@36"/>
<pin name="RD9@43"/>
<pin name="RD10@44"/>
<pin name="RD11@45"/>
<pin name="RF0@58"/>
<pin name="RF1@59"/>
<pin name="RE0@60"/>
<pin name="RE1@61"/>
<pin name="RE2@62"/>
<pin name="RE3@63"/>
<pin name="RG7@5"/>
<pin name="RG6@4"/>
<pin name="RE7@3"/>
<pin name="RE6@2"/>
<pin name="RE5@1"/>
<pin name="RE4@64"/>
<pin name="TX2@31"/>
<pin name="RX2@32"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_POWER">
<pin name="VSS@75"/>
<pin name="VDD@2"/>
<pin name="VDD@86"/>
<pin name="VCAP"/>
<pin name="VDD@46"/>
<pin name="VSS@45"/>
<pin name="VDD@37"/>
<pin name="VSS@36"/>
<pin name="RA9/VREF-"/>
<pin name="RA10/VREF+"/>
<pin name="VDD@16"/>
<pin name="VSS@15"/>
<pin name="VSS@65"/>
<pin name="VDD@62"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_CONTROL">
<pin name="RB0/AN0"/>
<pin name="RB1/AN1"/>
<pin name="RB3/AN3"/>
<pin name="RB4/AN4"/>
<pin name="RB5/AN5"/>
<pin name="RB6/AN6"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RG2/SCL1"/>
<pin name="RG3/SDA1"/>
<pin name="RD8/IC1"/>
<pin name="RD9/IC2"/>
<pin name="RD14/U1CTS/IC7"/>
<pin name="RD15/U1RTS/IC8"/>
<pin name="RD10/IC3"/>
<pin name="RD11/IC4"/>
<pin name="RD0/OC1"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5"/>
<pin name="RD12/IC5"/>
<pin name="RD13/IC6"/>
<pin name="RD5/OC6"/>
<pin name="RD6/OC7"/>
<pin name="RD7/OC8"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RF2/U1RX"/>
<pin name="RF3/U1TX"/>
<pin name="RB14/AN14"/>
<pin name="RC4/AN19"/>
<pin name="RA6/AN22"/>
<pin name="RE4"/>
<pin name="RE3"/>
<pin name="RE2"/>
<pin name="RE1/AN25"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_EXTERNAL">
<pin name="RB15/AN15"/>
<pin name="RC1/AN16"/>
<pin name="RC2/AN17"/>
<pin name="RC3/AN18"/>
<pin name="RA12/INT1"/>
<pin name="RA13/INT2"/>
<pin name="RA7/AN23"/>
<pin name="RG6/SCK2"/>
<pin name="RG7/SDI2"/>
<pin name="RG8/SDO2"/>
<pin name="RG9/SS2"/>
<pin name="RF4/U2RX"/>
<pin name="RF5/U2TX"/>
<pin name="RF13/U2RTS"/>
<pin name="RF12/U2CTS"/>
<pin name="RC14/PGEC2"/>
<pin name="RC13/PGED2"/>
<pin name="MCLR"/>
<pin name="RF1/C1TX1"/>
<pin name="RF0/C1RX1"/>
<pin name="RF6/SCK1"/>
<pin name="RF7/SDI1"/>
<pin name="RF8/SDO1"/>
<pin name="RA2/SCL2"/>
<pin name="RA3/SDA2"/>
<pin name="RB2/SS1"/>
<pin name="RE0/AN24"/>
<pin name="RA1"/>
<pin name="RA5/TDO"/>
<pin name="RA4/TDI"/>
<pin name="RA14"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_EXTRA">
<pin name="RE5/AN29"/>
<pin name="RE6/AN30"/>
<pin name="RE7/AN31"/>
<pin name="RG0/C2RX"/>
<pin name="RG1/C2TX"/>
<pin name="RG13/CSDO"/>
<pin name="RG12/CSDI"/>
<pin name="RG14/CSCK"/>
<pin name="RA0/TMS"/>
<pin name="RA15"/>
<pin name="RC15/OSC2"/>
<pin name="RC12/OSC1"/>
<pin name="RG15/COFS"/>
</symbol>
<symbol name="EEPROM-I2C">
<pin name="VSS" direction="pwr"/>
<pin name="WP"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A2"/>
<pin name="A0"/>
<pin name="A1"/>
</symbol>
<symbol name="ENC28J60">
<pin name="VCAP"/>
<pin name="VSS"/>
<pin name="CLKOUT"/>
<pin name="/INT"/>
<pin name="NC"/>
<pin name="SO"/>
<pin name="SI"/>
<pin name="SCK"/>
<pin name="CS"/>
<pin name="RESET"/>
<pin name="VSSRX"/>
<pin name="TPIN-"/>
<pin name="TPIN+"/>
<pin name="RBIAS"/>
<pin name="VDDTX"/>
<pin name="TPOUT-"/>
<pin name="TPOUT+"/>
<pin name="VSSTX"/>
<pin name="VDDRX"/>
<pin name="VDDPLL"/>
<pin name="VSSPLL"/>
<pin name="VSSOSC"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="VDDOSC"/>
<pin name="LEDB"/>
<pin name="LEDA"/>
<pin name="VDD"/>
</symbol>
<symbol name="EP2C20_PQ208_PLL">
<pin name="GND_PLL1" direction="pwr"/>
<pin name="GND_PLL1@1" direction="pwr"/>
<pin name="GND_PLL2" direction="pwr"/>
<pin name="GND_PLL2@1" direction="pwr"/>
<pin name="GNDA_PLL1" direction="pwr"/>
<pin name="GNDA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
</symbol>
<symbol name="EP2C20_PQ208_B3">
<pin name="IO_LVDS56N"/>
<pin name="IO_LVDS56P"/>
<pin name="VCCIO3@1"/>
<pin name="IO_LVDS53N"/>
<pin name="IO_LVDS53P"/>
<pin name="IO_LVDS52N"/>
<pin name="IO_LVDS52P"/>
<pin name="IO_LVDS51N"/>
<pin name="IO_LVDS51P"/>
<pin name="IO_VREFB3N1"/>
<pin name="VCCIO3@2"/>
<pin name="IO_LVDS48N"/>
<pin name="IO_LVDS48P"/>
<pin name="CLK7_LVDSCLK3N"/>
<pin name="CLK6_LVDSCLK3P"/>
<pin name="CLK5_LVDSCLK2N"/>
<pin name="CLK4_LVDSCLK2P"/>
<pin name="IO_LVDS47N"/>
<pin name="IO_LVDS47P"/>
<pin name="IO_LVDS46N"/>
<pin name="VCCIO3@3"/>
<pin name="IO_LVDS46P"/>
<pin name="IO_LVDS45N"/>
<pin name="IO_LVDS45P"/>
<pin name="IO_LVDS44N"/>
<pin name="IO_LVDS44P"/>
<pin name="IO_LVDS42N"/>
<pin name="IO_LVDS42P"/>
<pin name="IO_VREFB3N0"/>
<pin name="IO_LVDS39N"/>
<pin name="IO_LVDS39P"/>
<pin name="VCCIO3@4"/>
<pin name="IO_LVDS38N"/>
<pin name="IO_LVDS38P"/>
<pin name="IO_PLL2_OUTP"/>
<pin name="IO_PLL2_OUTN"/>
<pin name="IO@1"/>
</symbol>
<symbol name="EP2C20_PQ208_B1">
<pin name="IO_LVDS14P"/>
<pin name="IO_LVDS14N"/>
<pin name="VCCIO1@1"/>
<pin name="IO_LVDS13P"/>
<pin name="IO_LVDS13N"/>
<pin name="IO_LVDS12P"/>
<pin name="IO_LVDS12N"/>
<pin name="IO_VREFB1N0"/>
<pin name="IO_LVDS8P"/>
<pin name="IO_LVDS8N"/>
<pin name="CLK0_LVDSCLK0P"/>
<pin name="CLK1_LVDSCLK0N"/>
<pin name="CLK2_LVDSCLK1P"/>
<pin name="CLK3_LVDSCLK1N"/>
<pin name="VCCIO1@4"/>
<pin name="IO_LVDS7P"/>
<pin name="IO_LVDS7N"/>
<pin name="IO_LVDS6N"/>
<pin name="IO@2"/>
<pin name="IO_LVDS5P"/>
<pin name="IO_VREFB1N1"/>
<pin name="IO_LVDS3N"/>
<pin name="IO_LVDS2P"/>
<pin name="IO_LVDS2N"/>
<pin name="VCCIO1@6"/>
<pin name="IO@3"/>
<pin name="IO_LVDS0P"/>
<pin name="IO_LVDS0N"/>
<pin name="IO@4"/>
<pin name="IO_PLL1_OUTP"/>
<pin name="IO_PLL1_OUTN"/>
</symbol>
<symbol name="EP2C20_PQ208_B4">
<pin name="IO_LVDS77P"/>
<pin name="IO_LVDS76P"/>
<pin name="IO_LVDS76N"/>
<pin name="IO_LVDS75P"/>
<pin name="IO_LVDS75N"/>
<pin name="VCCIO4@1"/>
<pin name="IO_LVDS74P"/>
<pin name="IO_LVDS74N"/>
<pin name="IO_VREFB4N1"/>
<pin name="IO_LVDS70P"/>
<pin name="IO_LVDS70N"/>
<pin name="IO_LVDS68P"/>
<pin name="IO_LVDS68N"/>
<pin name="VCCIO4@2"/>
<pin name="IO_LVDS67P"/>
<pin name="IO_LVDS67N"/>
<pin name="IO_LVDS66P"/>
<pin name="IO_LVDS66N"/>
<pin name="IO_LVDS64P"/>
<pin name="IO_LVDS64N"/>
<pin name="VCCIO4@3"/>
<pin name="IO_LVDS63P"/>
<pin name="IO_LVDS63N"/>
<pin name="IO_LVDS62P"/>
<pin name="IO_LVDS62N"/>
<pin name="IO_VREFB4N0"/>
<pin name="IO_LVDS61P"/>
<pin name="VCCIO4@4"/>
<pin name="IO_LVDS61N"/>
<pin name="IO_LVDS60P"/>
<pin name="IO_LVDS60N"/>
<pin name="IO@2"/>
<pin name="IO_LVDS59P"/>
<pin name="VCCIO4@5"/>
<pin name="IO_LVDS59N"/>
<pin name="IO_LVDS58P"/>
<pin name="IO_LVDS58N"/>
<pin name="IO_LVDS57P"/>
<pin name="IO_LVDS57N"/>
<pin name="IO@1"/>
</symbol>
<symbol name="EP2C20_PQ208_POWER">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="VCCINT@1" direction="pwr"/>
<pin name="VCCINT@2" direction="pwr"/>
<pin name="VCCINT@3" direction="pwr"/>
<pin name="VCCINT@4" direction="pwr"/>
<pin name="VCCINT@5" direction="pwr"/>
<pin name="VCCINT@6" direction="pwr"/>
<pin name="GND@15"/>
<pin name="GND@16"/>
<pin name="GND@17"/>
<pin name="GND@18"/>
<pin name="GND@19"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
<pin name="GND@25"/>
</symbol>
<symbol name="EP2C20_PQ208_B2">
<pin name="IO_LVDS37N"/>
<pin name="IO_LVDS37P"/>
<pin name="IO_LVDS36N"/>
<pin name="IO_LVDS36P"/>
<pin name="IO_LVDS35N"/>
<pin name="IO_LVDS35P"/>
<pin name="VCCIO2@1"/>
<pin name="IO_LVDS34N"/>
<pin name="IO_LVDS34P"/>
<pin name="IO_VREFB2N0"/>
<pin name="IO_LVDS33N"/>
<pin name="VCCIO2@2"/>
<pin name="IO_LVDS33P"/>
<pin name="IO_LVDS31N"/>
<pin name="IO_LVDS31P"/>
<pin name="IO_LVDS29N"/>
<pin name="IO_LVDS29P"/>
<pin name="IO_LVDS28N"/>
<pin name="IO_LVDS28P"/>
<pin name="VCCIO2@3"/>
<pin name="IO_LVDS26P"/>
<pin name="IO_LVDS25N"/>
<pin name="IO_LVDS25P"/>
<pin name="IO_LVDS24N"/>
<pin name="IO_LVDS24P"/>
<pin name="IO_VREFB2N1"/>
<pin name="IO_LVDS23N"/>
<pin name="VCCIO2@4"/>
<pin name="IO_LVDS23P"/>
<pin name="IO_LVDS21N"/>
<pin name="IO_LVDS21P"/>
<pin name="IO_LVDS19N"/>
<pin name="IO_LVDS19P"/>
<pin name="IO_LVDS18N"/>
<pin name="VCCIO2@5"/>
<pin name="IO_LVDS18P"/>
<pin name="IO_LVDS17P"/>
<pin name="IO_LVDS16N"/>
<pin name="IO_LVDS16P"/>
<pin name="IO_LVDS17N"/>
</symbol>
<symbol name="EP2C20_PQ208_CONFIG">
<pin name="ASDO"/>
<pin name="CRC_ERROR"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="DATA0"/>
<pin name="NCSO"/>
<pin name="CLKUSR"/>
<pin name="TMS"/>
<pin name="TDI"/>
<pin name="NCE"/>
<pin name="NCONFIG"/>
<pin name="DEV_OE"/>
<pin name="INIT_DONE"/>
<pin name="NCEO"/>
<pin name="NSTATUS"/>
<pin name="CONF_DONE"/>
<pin name="MSEL1"/>
<pin name="MSEL0"/>
<pin name="DCLK"/>
</symbol>
<symbol name="FT232R">
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="DSR" direction="in" function="dot"/>
<pin name="DCD" direction="in" function="dot"/>
<pin name="RI" direction="in" function="dot"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND7" direction="pwr"/>
<pin name="GND18" direction="pwr"/>
<pin name="GND21" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="TXLED" direction="in" function="dot"/>
<pin name="RXLED" direction="in" function="dot"/>
<pin name="RTS" direction="out" function="dot"/>
<pin name="CTS" direction="in" function="dot"/>
<pin name="DTR" direction="out" function="dot"/>
<pin name="PWREN" direction="in" function="dot"/>
<pin name="TXDEN" direction="in"/>
<pin name="SLEEP" direction="in" function="dot"/>
</symbol>
<symbol name="FT232R-BASIC">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="TXLED" function="dot"/>
<pin name="RXLED" function="dot"/>
<pin name="RTS" function="dot"/>
<pin name="CTS" function="dot"/>
<pin name="DTR" function="dot"/>
</symbol>
<symbol name="FT232RQ">
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="DSR" direction="in" function="dot"/>
<pin name="DCD" direction="in" function="dot"/>
<pin name="RI" direction="in" function="dot"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="TXLED" direction="in" function="dot"/>
<pin name="RXLED" direction="in" function="dot"/>
<pin name="RTS" direction="out" function="dot"/>
<pin name="CTS" direction="in" function="dot"/>
<pin name="DTR" direction="out" function="dot"/>
<pin name="PWREN" direction="in" function="dot"/>
<pin name="TXDEN" direction="in"/>
<pin name="SLEEP" direction="in" function="dot"/>
</symbol>
<symbol name="FT245R">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="RXF" function="dot"/>
<pin name="TXE" function="dot"/>
<pin name="RD" function="dot"/>
<pin name="WR"/>
<pin name="PWEN"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="FT2232D">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="BDBUS0" direction="out"/>
<pin name="BDBUS1" direction="in"/>
<pin name="BDBUS2" direction="out"/>
<pin name="BDBUS3" direction="in"/>
<pin name="BDBUS4" direction="out"/>
<pin name="BDBUS5" direction="in"/>
<pin name="BDBUS6" direction="in"/>
<pin name="BDBUS7" direction="in"/>
<pin name="PWEN#"/>
<pin name="VCCIOA" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC2" direction="pwr"/>
<pin name="RSTOUT#"/>
<pin name="RESET#"/>
<pin name="XTIN"/>
<pin name="XTOUT"/>
<pin name="EECS"/>
<pin name="EESK"/>
<pin name="EEDATA"/>
<pin name="GND4"/>
<pin name="SI/WUB"/>
<pin name="BCBUS3"/>
<pin name="BCBUS2"/>
<pin name="BCBUS1"/>
<pin name="BCBUS0"/>
<pin name="ACBUS2"/>
<pin name="ACBUS1"/>
<pin name="ACBUS0"/>
<pin name="ADBUS7"/>
<pin name="ADBUS6"/>
<pin name="ADBUS5"/>
<pin name="SI/WUA"/>
<pin name="ACBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS3"/>
<pin name="ADBUS2"/>
<pin name="ADBUS1"/>
<pin name="ADBUS0"/>
<pin name="VCC1" direction="pwr"/>
<pin name="AVCC"/>
<pin name="VCCIOB"/>
</symbol>
<symbol name="HEF4543">
<pin name="A"/>
<pin name="B"/>
<pin name="BL"/>
<pin name="C"/>
<pin name="D"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="GND"/>
<pin name="LD"/>
<pin name="PH"/>
<pin name="VCC"/>
</symbol>
<symbol name="M74HC4050">
<pin name="VCC"/>
<pin name="1A"/>
<pin name="2A"/>
<pin name="3A"/>
<pin name="4A"/>
<pin name="5A"/>
<pin name="6A"/>
<pin name="1Y"/>
<pin name="2Y"/>
<pin name="3Y"/>
<pin name="4Y"/>
<pin name="5Y"/>
<pin name="6Y"/>
<pin name="GND"/>
</symbol>
<symbol name="ICL3232">
<pin name="C1+"/>
<pin name="V+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="V-"/>
<pin name="T2OUT"/>
<pin name="R2IN"/>
<pin name="R2OUT"/>
<pin name="T2IN"/>
<pin name="T1IN"/>
<pin name="R1OUT"/>
<pin name="R1IN"/>
<pin name="T1OUT"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="INVERTER">
<pin name="NC"/>
<pin name="A"/>
<pin name="GND"/>
<pin name="Y"/>
<pin name="VCC"/>
</symbol>
<symbol name="INVERTING_SCHMITT_TRIGGER">
<pin name="NC"/>
<pin name="A"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="Y"/>
</symbol>
<symbol name="ISD1932">
<pin name="_REC"/>
<pin name="_PLAYE/FMC2"/>
<pin name="_PLAYL/FMC1"/>
<pin name="S3/_M4"/>
<pin name="S2/_M3"/>
<pin name="S1/_M2"/>
<pin name="S0/_M1"/>
<pin name="E3/_M8"/>
<pin name="E2/_M7"/>
<pin name="E1/_M6"/>
<pin name="E0/_M5"/>
<pin name="_FT"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="AGC"/>
<pin name="ROSC"/>
<pin name="SP-"/>
<pin name="SP+"/>
<pin name="VSSP2"/>
<pin name="VSSP1"/>
<pin name="VCCP"/>
<pin name="VSSA"/>
<pin name="VCCA"/>
<pin name="VSSD"/>
<pin name="VCCD"/>
<pin name="XCLK/FMC3"/>
<pin name="_LED"/>
<pin name="ADDR/_DRCT"/>
</symbol>
<symbol name="LPC213X">
<pin name="P1.16(TRACEPKT0)"/>
<pin name="P1.17(TRACEPKT1)"/>
<pin name="P1.18(TRACEPKT2)"/>
<pin name="P1.19(TRACEPKT3)"/>
<pin name="P1.20(TRACESYNC)"/>
<pin name="P1.21(PIPESTAT0)"/>
<pin name="P1.22(PIPESTAT1)"/>
<pin name="P1.23(PIPESTAT2)"/>
<pin name="(MISO0/MAT0.1/A0.7)P0.5"/>
<pin name="(SSEL0/PWM2/EINT2)P0.7"/>
<pin name="(TXD1/PWM4/A1.1)P0.8"/>
<pin name="(RXD1/PWM6/EINT3)P0.9"/>
<pin name="(RTS1/CAP1.0/AD1.2)P0.10"/>
<pin name="(CTS1/CAP1.1/SCL1)P0.11"/>
<pin name="P1.24(TRACECLK)"/>
<pin name="P1.25(EXTIN0)"/>
<pin name="P1.26(RTCK)"/>
<pin name="P1.27(TDO)"/>
<pin name="P1.28(TDI)"/>
<pin name="P1.29(TCK)"/>
<pin name="P1.30(TMS)"/>
<pin name="P1.31(/TRST)"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="(DSR1/MAT1.0/AD1.3)P0.12"/>
<pin name="(DTR1/MAT1.1/AD1.4)P0.13"/>
<pin name="(DCD1/EINT1/SDA1)P0.14"/>
<pin name="(RI1/EINT2/AD1.5)P0.15"/>
<pin name="(EINT0/MAT0.2/CAP0.2)P0.16"/>
<pin name="(CAP1.2/SCK1/MAT1.2)P0.17"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA3" direction="pwr"/>
<pin name="VDD3-1" direction="pwr"/>
<pin name="VDD3-2" direction="pwr"/>
<pin name="VDD3-3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="(TXD0/PWM1)P0.0"/>
<pin name="(RXD0/PWM3/EINT0)P0.1"/>
<pin name="(SCL0/CAP0.0)P0.2"/>
<pin name="(SDA0/MAT0.0/EINT1)P0.3"/>
<pin name="(SCK0/CAP0.1/AD0.6)P0.4"/>
<pin name="(MOSI0/CAP0.2/AD1.0)P0.6"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="RTXC1" direction="in"/>
<pin name="RTXC2" direction="out"/>
<pin name="(CAP1.3/MISO1/MAT1.3)P0.18"/>
<pin name="(MAT1.2/MOSI1/CAP1.2)P0.19"/>
<pin name="(MAT1.3/SSEL1/EINT3)P0.20"/>
<pin name="(PWM5/AD1.6/CAP1.3)P0.21"/>
<pin name="(AD1.7/CAP0.0/MAT0.0)P0.22"/>
<pin name="P0.23"/>
<pin name="(AD0.4/AOUT)P0.25"/>
<pin name="(AD0.5)P0.26"/>
<pin name="(AD0.0/CAP0.1/MAT0.1)P0.27"/>
<pin name="(AD0.1/CAP0.2/MAT0.2)P0.28"/>
<pin name="(AD0.2/CAP0.3/MAT0.3)P0.29"/>
<pin name="(AD0.3/EINT3/CAP0.0)P0.30"/>
<pin name="P0.31" direction="out"/>
</symbol>
<symbol name="LPC2103">
<pin name="P0.19/MAT1.2/MISO1"/>
<pin name="P0.20/MAT1.3/MOSI1"/>
<pin name="P0.21/SSEL1/MAT3.0"/>
<pin name="VBAT"/>
<pin name="VDD(1V8)"/>
<pin name="RST"/>
<pin name="VSS@7"/>
<pin name="P0.27/TRST/CAP2.0"/>
<pin name="P0.28/TMS/CAP2.1"/>
<pin name="P0.29/TCK/CAP2.2"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0.0/TXD0/MAT3.1"/>
<pin name="P0.1/RXD0/MAT3.2"/>
<pin name="P0.30/TDI/MAT3.3"/>
<pin name="P0.31/TDO"/>
<pin name="VDD(3V3)@17"/>
<pin name="P0.2/SCL0/CAP0.0"/>
<pin name="VSS@19"/>
<pin name="RTCX1"/>
<pin name="P0.3/SDA0/MAT0.0"/>
<pin name="P0.4/SCK0/CAP0.1"/>
<pin name="P0.5/MISO0/MAT0.1"/>
<pin name="P0.6/MOSI0/CAP0.2"/>
<pin name="RTCX2"/>
<pin name="RTCK"/>
<pin name="DBGSEL"/>
<pin name="P0.7/SSEL0/MAT2.0"/>
<pin name="P0.8/TXD1/MAT2.1"/>
<pin name="P0.9/RXD1/MAT2.2"/>
<pin name="VSSA"/>
<pin name="P0.22/AD0.0"/>
<pin name="P0.23/AD0.1"/>
<pin name="P0.24/AD0.2"/>
<pin name="P0.10/RTS1/CAP1.0/AD0.3"/>
<pin name="P0.11/CTS1/CAP1.1/AD0.4"/>
<pin name="P0.12/DSR1/MAT1.0/AD0.5"/>
<pin name="P0.25/AD0.6"/>
<pin name="P0.26/AD0.7"/>
<pin name="VDD(3V3)@40"/>
<pin name="P0.13/DTR1/MAT1.1"/>
<pin name="VDDA"/>
<pin name="VSS@43"/>
<pin name="P0.14/DCD1/SCK1/EINT1"/>
<pin name="P0.15/RI1/EINT2"/>
<pin name="P0.16/EINT0/MAT0.2"/>
<pin name="P0.17/CAP1.2/SCL1"/>
<pin name="P0.18/CAP1.3/SDA1"/>
</symbol>
<symbol name="M74HC238">
<pin name="VCC"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="G1"/>
<pin name="~G2B"/>
<pin name="~G2A"/>
<pin name="GND"/>
<pin name="Y7"/>
<pin name="Y6"/>
<pin name="Y5"/>
<pin name="Y4"/>
<pin name="Y3"/>
<pin name="Y2"/>
<pin name="Y1"/>
<pin name="Y0"/>
</symbol>
<symbol name="M93C46">
<pin name="CS"/>
<pin name="SK"/>
<pin name="DIN"/>
<pin name="DOUT"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="MAX232">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="MAX485">
<pin name="RO"/>
<pin name="RE" function="dot"/>
<pin name="DE"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="A"/>
<pin name="B"/>
<pin name="VCC"/>
</symbol>
<symbol name="MAX3421E-1">
<pin name="VCC"/>
<pin name="VL"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBCOMP"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="INT"/>
<pin name="RES"/>
<pin name="GPX"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="SS"/>
<pin name="GND@3"/>
<pin name="GND@19"/>
<pin name="GOUT7"/>
<pin name="GOUT6"/>
<pin name="GOUT5"/>
<pin name="GOUT4"/>
<pin name="GOUT3"/>
<pin name="GOUT2"/>
<pin name="GOUT1"/>
<pin name="GOUT0"/>
<pin name="GPIN7"/>
<pin name="GPIN6"/>
<pin name="GPIN5"/>
<pin name="GPIN4"/>
<pin name="GPIN3"/>
<pin name="GPIN2"/>
<pin name="GPIN1"/>
<pin name="GPIN0"/>
</symbol>
<symbol name="MAX7219">
<pin name="DIN"/>
<pin name="DIG0"/>
<pin name="DIG4"/>
<pin name="GND"/>
<pin name="DIG6"/>
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG7"/>
<pin name="GND2"/>
<pin name="DIG5"/>
<pin name="DIG1"/>
<pin name="LOAD"/>
<pin name="CLK"/>
<pin name="SEGA"/>
<pin name="SEGF"/>
<pin name="SEGB"/>
<pin name="SEGG"/>
<pin name="ISET"/>
<pin name="VCC"/>
<pin name="SEGC"/>
<pin name="SEGE"/>
<pin name="SEGDP"/>
<pin name="SEGD"/>
<pin name="DOUT"/>
</symbol>
<symbol name="MAX7456">
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="CLKIN"/>
<pin name="XFB"/>
<pin name="CLKOUT"/>
<pin name="~CS"/>
<pin name="DIN"/>
<pin name="SCK"/>
<pin name="DOUT"/>
<pin name="LOS"/>
<pin name="~VSYNC"/>
<pin name="~HSYNC"/>
<pin name="~RESET"/>
<pin name="AGND"/>
<pin name="AVDD"/>
<pin name="VIN"/>
<pin name="PGND"/>
<pin name="PVDD"/>
<pin name="SAG"/>
<pin name="VOUT"/>
</symbol>
<symbol name="MC9S12XS64">
<pin name="PWM3/KWP3/PP3"/>
<pin name="TXD1/IOC2/PWM2/KWP2/PP2"/>
<pin name="IOC1/PWM1/KWP1/PP1"/>
<pin name="RXD1/IOC0/PWM0/KWP0/PP0"/>
<pin name="IOC0/PT0"/>
<pin name="IOC1/PT1"/>
<pin name="IOC2/PT2"/>
<pin name="IOC3/PT3"/>
<pin name="VDDF"/>
<pin name="VSS1"/>
<pin name="PWM4/IOC4/PT4"/>
<pin name="VREG_API/PWM5/IOC5/PT"/>
<pin name="PWM6/IOC6/PT6"/>
<pin name="PWM7/IOC7/PT7"/>
<pin name="MODC/BKGD"/>
<pin name="PB0"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="XCLKS/ECLKX2/PE7"/>
<pin name="ECLK/PE4"/>
<pin name="VSSX2"/>
<pin name="VDDX2"/>
<pin name="RESET"/>
<pin name="VDDR"/>
<pin name="VSS3"/>
<pin name="VSSPLL"/>
<pin name="EXTAL"/>
<pin name="XTAL"/>
<pin name="VDDPLL"/>
<pin name="IRQ/PE1"/>
<pin name="XIRQ/PE0"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="VDD"/>
<pin name="VSS2"/>
<pin name="PAD00/AN00"/>
<pin name="PAD01/AN01"/>
<pin name="PAD02/AN02"/>
<pin name="PAD03/AN03"/>
<pin name="PAD04/AN04"/>
<pin name="PAD05/AN05"/>
<pin name="PAD06/AN06"/>
<pin name="PAD07/AN07"/>
<pin name="VDDA"/>
<pin name="VRH"/>
<pin name="VSSA/VRL"/>
<pin name="PS0/RXD0"/>
<pin name="PS1/TXD0"/>
<pin name="PS2/RXD1"/>
<pin name="PS3/TXD1"/>
<pin name="TEST"/>
<pin name="PM5/SCK0"/>
<pin name="PM4/MOSI0"/>
<pin name="PM3/SS0"/>
<pin name="PM2/MISO0"/>
<pin name="PM1/TXCAN0/TXD1"/>
<pin name="PM0/RXCAN0/RXD1"/>
<pin name="VSSX1"/>
<pin name="VDDX1"/>
<pin name="PP7/KWP7/PWM7"/>
<pin name="PP5/KPW5/PWM5"/>
</symbol>
<symbol name="MCP130">
<pin name="RESET"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="MCP2551">
<pin name="TXD"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="RXD"/>
<pin name="VREF"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="RS"/>
</symbol>
<symbol name="NAND256">
<pin name="RXB"/>
<pin name="XR"/>
<pin name="XE"/>
<pin name="CL"/>
<pin name="AL"/>
<pin name="XW"/>
<pin name="XWP"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VSS1"/>
<pin name="IO7"/>
<pin name="IO6"/>
<pin name="IO5"/>
<pin name="IO4"/>
<pin name="IO3"/>
<pin name="IO2"/>
<pin name="IO1"/>
<pin name="IO0"/>
<pin name="VSS2"/>
</symbol>
<symbol name="BUFFER-DUAL">
<pin name="A2"/>
<pin name="A1"/>
<pin name="GND"/>
<pin name="Y1"/>
<pin name="VCC"/>
<pin name="Y2"/>
</symbol>
<symbol name="NCP303LSN09">
<pin name="RST"/>
<pin name="IN"/>
<pin name="GND"/>
<pin name="CD"/>
<pin name="NC"/>
</symbol>
<symbol name="4VDD4VSS">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="P8X32A">
<pin name="BOE/" direction="in"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="RES/"/>
<pin name="XI" direction="in"/>
<pin name="XO" direction="out"/>
</symbol>
<symbol name="PCA9306">
<pin name="SDA1"/>
<pin name="SCL1"/>
<pin name="EN"/>
<pin name="VREF1"/>
<pin name="VREF2"/>
<pin name="SCL2"/>
<pin name="SDA2"/>
<pin name="GND"/>
</symbol>
<symbol name="PCF8575C">
<pin name="INT"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="PO0"/>
<pin name="PO1"/>
<pin name="PO2"/>
<pin name="PO3"/>
<pin name="PO4"/>
<pin name="PO5"/>
<pin name="PO6"/>
<pin name="PO7"/>
<pin name="GND"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="A0"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC"/>
</symbol>
<symbol name="PIC16F88-DIP">
<pin name="RA5/MCLR" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/AN4"/>
<pin name="RB0/INT"/>
<pin name="RB1/SDA"/>
<pin name="RB2/RX"/>
<pin name="RB3"/>
<pin name="RB4/SCL"/>
<pin name="RB5/TX"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RA6/OSC2"/>
<pin name="RA7/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
</symbol>
<symbol name="PIC16F88-SSOP">
<pin name="RA5/MCLR" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/AN4"/>
<pin name="RB0/INT"/>
<pin name="RB1/SDA"/>
<pin name="RB2/RX"/>
<pin name="RB3"/>
<pin name="RB4/SCL"/>
<pin name="RB5/TX"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RA6/OSC2"/>
<pin name="RA7/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
</symbol>
<symbol name="PIC16F688">
<pin name="RA3/MCLR"/>
<pin name="RA5/OSC1"/>
<pin name="RA0/PGD"/>
<pin name="RC2/AN6"/>
<pin name="RC1/AN5"/>
<pin name="RC0/AN4"/>
<pin name="RA2/AN2"/>
<pin name="RA1/PGC"/>
<pin name="RC3/AN7"/>
<pin name="RC4/TX"/>
<pin name="RC5/RX"/>
<pin name="RA4/OSC2"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PIC16F883">
<pin name="RX/RC7" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="TX/RC6"/>
<pin name="RC5/SDO"/>
<pin name="RB0/INT0"/>
<pin name="RC4/SDI"/>
<pin name="RB4/AN11"/>
<pin name="RB5/PGM"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2/INT2/AN8"/>
<pin name="RB1/INT1/AN10"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3/AN9"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3/SCK"/>
<pin name="RC0"/>
</symbol>
<symbol name="PIC16F913">
<pin name="RX/RC7/SDA" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="TX/RC6/SCL"/>
<pin name="RC5"/>
<pin name="RB0/INT0"/>
<pin name="RC4/SD0"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RA6/OSC2"/>
<pin name="RA7/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC0"/>
</symbol>
<symbol name="PIC18F2550">
<pin name="RX/RC7" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/AN4"/>
<pin name="TX/RC6"/>
<pin name="RC5/D+"/>
<pin name="RB0/INT0"/>
<pin name="RC4/D-"/>
<pin name="RB4/AN11"/>
<pin name="RB5/PGM"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2/INT2/AN8"/>
<pin name="RB1/INT1/AN10"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3/AN9"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="V-USB"/>
<pin name="RC0"/>
</symbol>
<symbol name="PIC24FJXXXDAX06">
<pin name="!MCLR" direction="in"/>
<pin name="AN2/C2INB/VMIO/RP13/CN4/RB2"/>
<pin name="AN3/C2INA/VPIO/CN5/RB3"/>
<pin name="AN8/RP8/CN26/RB8"/>
<pin name="AN9/RP9/CN27/RB9"/>
<pin name="AN14/CTPLS/RP14/CN32/RB14"/>
<pin name="AN15/RP29/REFO/CN12/RB15"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="C1INC/RP26/CN9/RG7"/>
<pin name="C1IND/RP21/CN8/RG6"/>
<pin name="C2INC/RP27/GD15/CN11/RG9"/>
<pin name="C2IND/RP19/GD14/CN10/RG8"/>
<pin name="C3INA/SESSEND/CN16/RD7"/>
<pin name="C3INB/CN15/RD6"/>
<pin name="D+/CN83/RG2"/>
<pin name="D-/CN84/RG3"/>
<pin name="DMH/RP11/INT0/CN49/RD0"/>
<pin name="DPH/RP23/CN51/RD2"/>
<pin name="DPLN/SDA1/RP4/GD8/CN54/RD9"/>
<pin name="ENVREG" direction="in"/>
<pin name="GD0/CN58/RE0"/>
<pin name="GD1/CN59/RE1"/>
<pin name="GD2/CN60/RE2"/>
<pin name="GD3/CN61/RE3"/>
<pin name="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0"/>
<pin name="GD11/VCMPST2/SESSVLD/CN69/RF1"/>
<pin name="GD12/SCL3/CN64/RE6"/>
<pin name="GD13/SDA3/CN65/RE7"/>
<pin name="HSYNC/CN62/RE4"/>
<pin name="OSCI/CLKI/CN23/RC12"/>
<pin name="OSCO/CLKO/CN22/RC15"/>
<pin name="PGEC1/AN1/VREF-/RP1/CN3/RB1"/>
<pin name="PGEC2/AN6/RP6/CN24/RB6"/>
<pin name="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5"/>
<pin name="PGED1/AN0/VREF+/RP0/CN2/RB0"/>
<pin name="PGED2/AN7/RP7/RCV/CN25/RB7"/>
<pin name="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4"/>
<pin name="RP12/GD7/CN56/RD11"/>
<pin name="RP16/USBID/CN71/RF3"/>
<pin name="RP20/GPWR/CN14/RD5"/>
<pin name="RP22/GEN/CN52/RD3"/>
<pin name="RP25/GCLK/CN13/RD4"/>
<pin name="RTCC/DMLN/RP2/CN53/RD8"/>
<pin name="SCL1/RP3/GD6/CN55/RD10"/>
<pin name="SCL2/RP17/GD5/CN18/RF5"/>
<pin name="SDA2/RP10/GD4/CN17/RF4"/>
<pin name="SOSCI/C3IND/CN1/RC13"/>
<pin name="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14"/>
<pin name="TCK/AN12/CTEDG2/CN30/RB12"/>
<pin name="TDI/AN13/CTEDG1/CN31/RB13"/>
<pin name="TDO/AN11/CN29/RB11"/>
<pin name="TMS/CVREF/AN10/CN28/RB10"/>
<pin name="VBUS/RF7" direction="in"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSYNC/CN63/RE5"/>
<pin name="VUSB" direction="pwr"/>
</symbol>
<symbol name="PIC24HJ32GP202">
<pin name="AN0/VREF+/CN2/RA0"/>
<pin name="AN1/VREF-/CN2/RA1"/>
<pin name="AN4/RP2/CN6/RB2"/>
<pin name="AN5/RP3/CN7/RB3"/>
<pin name="AN9/RP15/CN11/RB15"/>
<pin name="AN10/RP14/CN12/RB14"/>
<pin name="AN11/RP13/CN13/RB13"/>
<pin name="AN12/RP12/CN14/RB12"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="INT0/RP7/CN23/RB7"/>
<pin name="MCLR" direction="in"/>
<pin name="OSCO/CLKO/CN29/RA3" direction="out"/>
<pin name="OSCI/CLKI/CN30/RA2" direction="in"/>
<pin name="PGEC1/AN3/C2IN+/RP1/CN5/RB1"/>
<pin name="PGEC2/TMS/RP11/CN15/RB11"/>
<pin name="PGEC3/ASCL1/RP6/CN24/RB6"/>
<pin name="PGED1/AN2/C2IN-/RP0/CN4/RB0"/>
<pin name="PGED2/TDI/RP10/CN16/RB10"/>
<pin name="PGED3/ASDA1/RP5/CN27/RB5"/>
<pin name="SOSCI/RP4/CN1/RB4"/>
<pin name="SOSCO/T1CK/CN0/RA4"/>
<pin name="TCK/SCL/RP8/CN22/RB8"/>
<pin name="TDO/SDA1/RP9/CN12/RB9"/>
<pin name="VCAP/VDDCORE" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="PIC32MX440F512H">
<pin name="RE5/PMD5"/>
<pin name="RE6/PMD6"/>
<pin name="RE7/PMD7"/>
<pin name="RG6/PMA5/SCK2/CN8"/>
<pin name="RG7/PMA4/SDI2/CN9"/>
<pin name="RG8/PMA3/SDO2/CN10"/>
<pin name="~MCLR"/>
<pin name="RG9/PMA2/~SS2/CN11"/>
<pin name="VSS@9"/>
<pin name="VDD@10"/>
<pin name="RB5/AN5/VBUSON/C1IN+/CN7"/>
<pin name="RB4/AN4/C1IN-/CN6"/>
<pin name="RB3/AN3/C2IN+/CN5"/>
<pin name="RB2/AN2/C2IN-/CN4"/>
<pin name="RB1/AN1/PGEC1/VREF-/CVREF-/CN3"/>
<pin name="RB0/AN0/PGED1/EMUD1/PMA6/VREF+/CVREF+/CN2"/>
<pin name="RB6/AN6/PGEC2/OCFA"/>
<pin name="RB7/AN7/PGED2"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="RB8/AN8/~U2CTS/C1OUT"/>
<pin name="RB9/AN9/PMA7/C2OUT"/>
<pin name="RB10/AN10/TMS/CVREFOUT/PMA13"/>
<pin name="RB11/AN11/TDO/PMA12"/>
<pin name="VSS@25"/>
<pin name="VDD@26"/>
<pin name="RB12/AN12/TCK/PMA11"/>
<pin name="RB13/AN13/TDI/PMA10"/>
<pin name="RB14/AN14/PMALH/PMA1/~U2RTS/BCLK2"/>
<pin name="RB15/AN15/PMALL/PMA0/OCFB/CN12"/>
<pin name="RF4/PMA9/U2RX/SDA2/CN17"/>
<pin name="RF5/PMA8/U2TX/SCL2/CN18"/>
<pin name="RF3/USBID"/>
<pin name="VBUS"/>
<pin name="VUSB"/>
<pin name="D-/RG3"/>
<pin name="D+/RG2"/>
<pin name="VDD@38"/>
<pin name="RC12/OSC1/CLKI"/>
<pin name="RC15/OSC2/CLKO"/>
<pin name="VSS@41"/>
<pin name="RD8/IC1/RTCC/INT1"/>
<pin name="RD9/IC2/~U1CTS//INT2/SDA1"/>
<pin name="RD10/IC3/PMCS2/PMA15/INT3/SCL1"/>
<pin name="RD11/IC4/PMCS1/PMA14/INT4"/>
<pin name="RD0/OC1/INT0"/>
<pin name="RC13/SOSCI/CN1"/>
<pin name="RC14/SOSCO/T1CK/CN0"/>
<pin name="RD1/OC2/~U1RTS/BCLK1"/>
<pin name="RD2/OC3/U1RX"/>
<pin name="RD3/OC4/U1TX"/>
<pin name="RD4/PMWR/OC5/IC5/CN13"/>
<pin name="RD5/PMRD/CN14"/>
<pin name="RD6/CN15"/>
<pin name="RD7/CN16"/>
<pin name="VCAP/VDDCORE"/>
<pin name="ENVREG"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0/PMD0"/>
<pin name="RE1/PMD1"/>
<pin name="RE2/PMD2"/>
<pin name="RE3/PMD3"/>
<pin name="RE4/PMD4"/>
</symbol>
<symbol name="PL-2303XA">
<pin name="TXD"/>
<pin name="DTR_N"/>
<pin name="RTS_N"/>
<pin name="VDD_325"/>
<pin name="RXD"/>
<pin name="RI_N"/>
<pin name="GND@7"/>
<pin name="VDD_33"/>
<pin name="DSR_N"/>
<pin name="DCD_N"/>
<pin name="CTS_N"/>
<pin name="SHTD_N"/>
<pin name="EE_CLK"/>
<pin name="EE_DATA"/>
<pin name="DP"/>
<pin name="DM"/>
<pin name="VO_33"/>
<pin name="GND@18"/>
<pin name="RESET_N"/>
<pin name="VDD_5"/>
<pin name="GND@21"/>
<pin name="GP0"/>
<pin name="GP1"/>
<pin name="VDD_33A"/>
<pin name="GND_A"/>
<pin name="PLL_TEST"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
</symbol>
<symbol name="RS485">
<pin name="RO"/>
<pin name="/RE"/>
<pin name="DE"/>
<pin name="DI"/>
<pin name="VCC"/>
<pin name="B"/>
<pin name="A"/>
<pin name="GND"/>
</symbol>
<symbol name="RS485_SP491">
<pin name="A"/>
<pin name="B"/>
<pin name="Z"/>
<pin name="Y"/>
<pin name="R"/>
<pin name="/RE"/>
<pin name="DE"/>
<pin name="D"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="VCC"/>
<pin name="NC2"/>
<pin name="NC1"/>
<pin name="NC3"/>
</symbol>
<symbol name="SC16IS750">
<pin name="RESET"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VDD"/>
<pin name="I2C-/SPI"/>
<pin name="A0-/CS"/>
<pin name="A1-SI"/>
<pin name="NC-SO"/>
<pin name="SCL-SCLK"/>
<pin name="SDA-VSS"/>
<pin name="/IRQ"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="VSS"/>
<pin name="GPIO4-/DSR"/>
<pin name="GPIO5-/DTR"/>
<pin name="GPIO6-/CD"/>
<pin name="GPIO7-/RI"/>
<pin name="/RTS"/>
<pin name="/CTS"/>
<pin name="TX"/>
<pin name="RX"/>
</symbol>
<symbol name="STN1110-QFN">
<pin name="!VPW_RX" direction="in"/>
<pin name="PWM_RX" direction="in"/>
<pin name="J1850_BUS+_TX" direction="out"/>
<pin name="!J1850_BUS-_TX" direction="out"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="!ISO_RX" direction="in"/>
<pin name="!SLEEP" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="CAN_RX" direction="in"/>
<pin name="CAN_TX" direction="out"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="PWR_CTRL" direction="out"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="!OBD_TX_LED!/!RST_NVM"/>
<pin name="!OBD_RX_LED!/!INT" direction="out"/>
<pin name="!UART_TX_LED" direction="out"/>
<pin name="!UART_RX_LED" direction="out"/>
<pin name="!ISO_K_TX" direction="out"/>
<pin name="!ISO_L_TX" direction="out"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="ANALOG_IN" direction="in"/>
<pin name="PWM/!VPW" direction="out"/>
<pin name="PAD" direction="pas"/>
</symbol>
<symbol name="SN74HC251">
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="Y"/>
<pin name="W"/>
<pin name="OE"/>
<pin name="GND"/>
<pin name="C"/>
<pin name="B"/>
<pin name="A"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="VCC"/>
</symbol>
<symbol name="SN74LVC1G08">
<pin name="A"/>
<pin name="B"/>
<pin name="GND"/>
<pin name="Y"/>
<pin name="+V"/>
</symbol>
<symbol name="SPEAKJET">
<pin name="E0"/>
<pin name="E1"/>
<pin name="E2"/>
<pin name="E3"/>
<pin name="E4"/>
<pin name="E5"/>
<pin name="E6/RC0"/>
<pin name="E7/RC1"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="RX"/>
<pin name="RST"/>
<pin name="M0"/>
<pin name="M1"/>
<pin name="D0/RDY"/>
<pin name="D1/SPK"/>
<pin name="D2/BHF"/>
<pin name="VOICE"/>
</symbol>
<symbol name="SPI_FLASH">
<pin name="CS"/>
<pin name="MISO"/>
<pin name="WP"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="HOLD"/>
<pin name="SCK"/>
<pin name="MOSI"/>
</symbol>
<symbol name="STM811">
<pin name="VCC"/>
<pin name="VSS"/>
<pin name="~RST"/>
<pin name="~MR"/>
</symbol>
<symbol name="STP16CP05/A6282">
<pin name="GND"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="VDD"/>
<pin name="REXT"/>
<pin name="SDO"/>
<pin name="~OE"/>
<pin name="OUT15"/>
<pin name="OUT14"/>
<pin name="OUT13"/>
<pin name="OUT12"/>
<pin name="OUT11"/>
<pin name="OUT10"/>
<pin name="OUT8"/>
<pin name="OUT9"/>
</symbol>
<symbol name="STW5093">
<pin name="VCC"/>
<pin name="REMOUT"/>
<pin name="REMIN"/>
<pin name="MIC3+"/>
<pin name="MIC3-"/>
<pin name="MBIAS"/>
<pin name="VCCA"/>
<pin name="MIC1+"/>
<pin name="MIC1-"/>
<pin name="GNDA"/>
<pin name="MIC2+"/>
<pin name="MIC2-"/>
<pin name="VCCP"/>
<pin name="VLR-"/>
<pin name="VLR+"/>
<pin name="GNDP"/>
<pin name="VFR"/>
<pin name="LO"/>
<pin name="BZ"/>
<pin name="CCLK"/>
<pin name="CS-"/>
<pin name="CI"/>
<pin name="AUXCLK"/>
<pin name="VCCIO"/>
<pin name="CO"/>
<pin name="GND"/>
<pin name="DX"/>
<pin name="DR"/>
<pin name="FS"/>
<pin name="MCLK"/>
</symbol>
<symbol name="TC7SU04F">
<pin name="NC"/>
<pin name="GND"/>
<pin name="IN"/>
<pin name="OUT"/>
<pin name="+V"/>
</symbol>
<symbol name="TJA1040TD-T">
<pin name="TXD"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="RXD"/>
<pin name="SPLIT"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="STB"/>
</symbol>
<symbol name="TLC5940">
<pin name="GND"/>
<pin name="BLANK"/>
<pin name="SCLK"/>
<pin name="SIN"/>
<pin name="VPRG"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="OUT8"/>
<pin name="XLAT"/>
<pin name="OUT9"/>
<pin name="OUT10"/>
<pin name="OUT11"/>
<pin name="OUT12"/>
<pin name="OUT13"/>
<pin name="OUT14"/>
<pin name="OUT15"/>
<pin name="XERR"/>
<pin name="SOUT"/>
<pin name="GSCLK"/>
<pin name="DCPRG"/>
<pin name="IREF"/>
<pin name="VCC"/>
</symbol>
<symbol name="UBW32_PIC32MX4XXL">
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="C1IN-/AN4/CN6/RB4"/>
<pin name="C1OUT/AN8/RB8"/>
<pin name="C2IN+/AN3/CN5/RB3"/>
<pin name="C2IN-/AN2/CN4/RB2"/>
<pin name="C2OUT/AN9/RB9"/>
<pin name="CN20/U1CTS/RD14"/>
<pin name="CVREFOUT/PMA13/AN10/RB10"/>
<pin name="D+/RG2"/>
<pin name="D-/RG3"/>
<pin name="ENVREG"/>
<pin name="IC1/RTCC/RD8"/>
<pin name="IC2/SS1/RD9"/>
<pin name="IC3/SCKI/PMCS2/PMA15/RD10"/>
<pin name="IC4/PMCS1/PMA14/RD11"/>
<pin name="INT1/RE8"/>
<pin name="INT2/RE9"/>
<pin name="MCLR"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="PGC1/EMUC1/AN1/CN3/RB1"/>
<pin name="PGC2/EMUC2/AN6/OCFA/RB6"/>
<pin name="PGD1/EMUD1/AN0/CN2/RB0"/>
<pin name="PGD2/EMUD2/AN7/RB7"/>
<pin name="PMA2/SS2/CN11/RG9"/>
<pin name="PMA3/SDO2/CN10/RG8"/>
<pin name="PMA4/SDI2/CN9/RG7"/>
<pin name="PMA5/SCK2/CN8/RG6"/>
<pin name="PMA6/VREF+/CVREF+/RA10"/>
<pin name="PMA7/VREF-/CVREF-/RA9"/>
<pin name="PMA8/U2TX/CN18/RF5"/>
<pin name="PMA9/U2RX/CN17/RF4"/>
<pin name="PMA10/AN13/RB13"/>
<pin name="PMA11/AN12/RB12"/>
<pin name="PMA12/AN11/RB11"/>
<pin name="PMALH/PMA1/AN14/RB14"/>
<pin name="PMALL/PMA0/AN15/OCFB/CN12/RB15"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="PMD4/RE4"/>
<pin name="PMD5/RE5"/>
<pin name="PMD6/RE6"/>
<pin name="PMD7/RE7"/>
<pin name="PMD8/RG0"/>
<pin name="PMD9/RG1"/>
<pin name="PMD10/RF1"/>
<pin name="PMD11/RF0"/>
<pin name="PMD12/IC5/RD12"/>
<pin name="PMD13/CN19/RD13"/>
<pin name="PMD14/CN15/RD6"/>
<pin name="PMD15/CN16/RD7"/>
<pin name="PMRD/CN14/RD5"/>
<pin name="PMWR/OC5/CN13/RD4"/>
<pin name="RG15"/>
<pin name="SCL1/INT3/RA14"/>
<pin name="SCL2/RA2"/>
<pin name="SDA1/INT4/RA15"/>
<pin name="SDA2/RA3"/>
<pin name="SDI1/T5CK/RC4"/>
<pin name="SDO1/OC1/INT0/RD0"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="T2CK/RC1"/>
<pin name="T3CK/RC2"/>
<pin name="T4CK/RC3"/>
<pin name="TCK/RA1"/>
<pin name="TDI/RA4"/>
<pin name="TDO/RA5"/>
<pin name="TMS/RA0"/>
<pin name="TRCLK/RA6"/>
<pin name="TRD0/RG13"/>
<pin name="TRD1/RG12"/>
<pin name="TRD2/RG14"/>
<pin name="TRD3/RA7"/>
<pin name="U1RTS/BCLK1/CN21/RD15"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF8"/>
<pin name="U2CTS/RF12"/>
<pin name="U2RTS/BCLK2/RF13"/>
<pin name="USBID/RF3"/>
<pin name="VBUS"/>
<pin name="VBUSON/C1IN+/AN5/CN7/RB5"/>
<pin name="VCAP/VDDCORE"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDD3"/>
<pin name="VDD4"/>
<pin name="VDD5"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSS4"/>
<pin name="VSS6"/>
<pin name="VUSB"/>
</symbol>
<symbol name="UM-FPU_V3_1">
<pin name="CS" direction="in"/>
<pin name="!MCLR" direction="in" function="dot"/>
<pin name="AN0" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="in"/>
<pin name="SEROUT" direction="out"/>
<pin name="SERIN" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="SOUT/SCL" direction="out"/>
<pin name="SIN/SDA" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="EXTIN" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT0" direction="out"/>
<pin name="SCLK" direction="in"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
</symbol>
<symbol name="USB3318">
<pin name="DATA7"/>
<pin name="DATA6"/>
<pin name="DATA5"/>
<pin name="DATA4"/>
<pin name="DATA3"/>
<pin name="DATA2"/>
<pin name="DATA1"/>
<pin name="DATA0"/>
<pin name="STP"/>
<pin name="NXT"/>
<pin name="DIR"/>
<pin name="CLKOUT"/>
<pin name="RESETB"/>
<pin name="REFCLK"/>
<pin name="RBIAS"/>
<pin name="VBUS"/>
<pin name="VBAT"/>
<pin name="VDD33"/>
<pin name="VDDIO"/>
<pin name="VDD18"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="ID"/>
<pin name="CPEN"/>
<pin name="GND1"/>
<pin name="GND2"/>
</symbol>
<symbol name="VS1000">
<pin name="XRESET"/>
<pin name="TEST"/>
<pin name="XTAL1"/>
<pin name="XTAL0"/>
<pin name="NFDIO0/IO0_0"/>
<pin name="NFDIO1/IO0_1"/>
<pin name="NFDIO2/IO0_2"/>
<pin name="NFDIO3/IO0_3"/>
<pin name="NFDIO4/IO0_4"/>
<pin name="NFDIO5/IO0_5"/>
<pin name="NFDIO6/IO0_6"/>
<pin name="NFDIO7/IO0_7"/>
<pin name="NFRDY/GPIO0_8"/>
<pin name="NFRD/GPIO0_9"/>
<pin name="CS1/GPIO0_10"/>
<pin name="NFCLE/GPIO0_12"/>
<pin name="NFALE/GPIO0_13"/>
<pin name="NFWR/GPIO0_11"/>
<pin name="CS2/GPIO0_14"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DGND1"/>
<pin name="VHIGH"/>
<pin name="POWBTN"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="XCS/GPIO1_0"/>
<pin name="SCLK/GPIO1_1"/>
<pin name="SI/GPIO1_2"/>
<pin name="SO/GPIO1_3"/>
<pin name="RX/GPIO1_4"/>
<pin name="TX/GPIO1_5"/>
<pin name="USBN"/>
<pin name="USBP"/>
<pin name="CVDD"/>
<pin name="IOVDD2"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="AVDD3"/>
<pin name="AVDD4"/>
<pin name="IOVDD3"/>
<pin name="IOVDD1"/>
</symbol>
<symbol name="VS1002">
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="XRESET"/>
<pin name="D_REQ"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="XDCS/BSYNC"/>
<pin name="XTAL0"/>
<pin name="XTAL1"/>
<pin name="XCS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="TEST"/>
<pin name="SPIBOOT/GPIO0"/>
<pin name="GPIO1"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="LEFT"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD3" direction="pwr"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DVDD1" direction="pwr"/>
<pin name="DVDD2" direction="pwr"/>
<pin name="DVDD3" direction="pwr"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="DGND1" direction="pwr"/>
</symbol>
<symbol name="VS1033D">
<pin name="S0"/>
<pin name="SI"/>
<pin name="SCLK"/>
<pin name="XCS"/>
<pin name="XDCS/BSYNC"/>
<pin name="DREQ"/>
<pin name="XRESET"/>
<pin name="TEST"/>
<pin name="XTAL1/MCLK"/>
<pin name="XTAL2"/>
<pin name="VCO"/>
<pin name="GPIO0/I2S_SCLK"/>
<pin name="GPIO1/I2S_SDATA"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="GPIO4/I2S_LROUT"/>
<pin name="GPIO5/I2C_MCLK"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="IOVDD1"/>
<pin name="IOVDD2"/>
<pin name="IOVDD3"/>
<pin name="CVDD1"/>
<pin name="CVDD2"/>
<pin name="CVDD3"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="AVDD3"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="LINEIN"/>
<pin name="RCAP"/>
<pin name="DGND6"/>
<pin name="DGND1"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="AGND4"/>
<pin name="CVDD4"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
</symbol>
<symbol name="VS1103">
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="XRESET"/>
<pin name="D_REQ"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="XDCS/BSYNC"/>
<pin name="XTAL0"/>
<pin name="XTAL1"/>
<pin name="XCS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="TEST"/>
<pin name="SPIBOOT/GPIO0"/>
<pin name="GPIO1"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="LEFT"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD3" direction="pwr"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DVDD1" direction="pwr"/>
<pin name="DVDD2" direction="pwr"/>
<pin name="DVDD3" direction="pwr"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="DGND1" direction="pwr"/>
<pin name="CVDD1"/>
<pin name="CVDD2"/>
<pin name="CVDD3"/>
<pin name="CVDD4"/>
</symbol>
<symbol name="W5100">
<pin name="RSET_BG"/>
<pin name="3V3A"/>
<pin name="NC@0"/>
<pin name="GNDA@0"/>
<pin name="RXIP"/>
<pin name="RXIN"/>
<pin name="1V8A@0"/>
<pin name="TXOP"/>
<pin name="TXON"/>
<pin name="GNDA@1"/>
<pin name="1V8OUT"/>
<pin name="3V3D@0"/>
<pin name="GNDD@0"/>
<pin name="GNDD@1"/>
<pin name="1V8D@0"/>
<pin name="1V8D@1"/>
<pin name="GNDD@2"/>
<pin name="3V3D@1"/>
<pin name="DATA7"/>
<pin name="DATA6"/>
<pin name="DATA5"/>
<pin name="DATA4"/>
<pin name="DATA3"/>
<pin name="DATA2"/>
<pin name="DATA1"/>
<pin name="DATA0"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="*SCS"/>
<pin name="SCLK"/>
<pin name="SEN"/>
<pin name="GNDD@3"/>
<pin name="1V8D@2"/>
<pin name="TEST3"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="TEST0"/>
<pin name="ADDR14"/>
<pin name="ADDR13"/>
<pin name="ADDR12"/>
<pin name="ADDR11"/>
<pin name="ADDR10"/>
<pin name="GNDD@4"/>
<pin name="3V3D@2"/>
<pin name="ADDR9"/>
<pin name="ADDR8"/>
<pin name="ADDR7"/>
<pin name="ADDR6"/>
<pin name="ADDR5"/>
<pin name="ADDR4"/>
<pin name="ADDR3"/>
<pin name="ADDR2"/>
<pin name="ADDR1"/>
<pin name="ADDR0"/>
<pin name="*CS"/>
<pin name="*INT"/>
<pin name="*WR"/>
<pin name="*RD"/>
<pin name="*RESET"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="OPMODE0"/>
<pin name="OPMODE1"/>
<pin name="OPMODE2"/>
<pin name="LINKLED"/>
<pin name="SPDLED"/>
<pin name="GNDD@5"/>
<pin name="1V8D@3"/>
<pin name="FDXLED"/>
<pin name="COLLED"/>
<pin name="RXLED"/>
<pin name="TXLED"/>
<pin name="1V8A@1"/>
<pin name="XTLN"/>
<pin name="XTLP"/>
<pin name="GNDA@2"/>
<pin name="NC@4"/>
<pin name="NC@5"/>
<pin name="NC@6"/>
</symbol>
<symbol name="WS2801">
<pin name="CKI"/>
<pin name="SDI"/>
<pin name="VCC"/>
<pin name="POL"/>
<pin name="CKO"/>
<pin name="SDO"/>
<pin name="BOUT"/>
<pin name="GOUT"/>
<pin name="ROUT"/>
<pin name="BFB"/>
<pin name="GFB"/>
<pin name="RFB"/>
<pin name="GND"/>
</symbol>
<symbol name="XC3S250/500E-PQ208">
<pin name="GND"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@12"/>
<pin name="GND@13"/>
<pin name="GND@14"/>
<pin name="GND@15"/>
<pin name="GND@16"/>
<pin name="GND@17"/>
<pin name="GND@18"/>
<pin name="GND@19"/>
<pin name="GND@20"/>
<pin name="VCCAUX"/>
<pin name="VCCAUX@2"/>
<pin name="VCCAUX@3"/>
<pin name="VCCAUX@4"/>
<pin name="VCCAUX@5"/>
<pin name="VCCAUX@6"/>
<pin name="VCCAUX@7"/>
<pin name="VCCAUX@8"/>
<pin name="VCCINT"/>
<pin name="VCCINT@2"/>
<pin name="VCCINT@3"/>
<pin name="VCCINT@4"/>
<pin name="DONE"/>
<pin name="PROG_B"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="IO"/>
<pin name="IO/VREF_0"/>
<pin name="IO_L01N_0"/>
<pin name="IO_L01P_0"/>
<pin name="IO_L02N_0/VREF_0"/>
<pin name="IO_L02P_0"/>
<pin name="IO_L03N_0"/>
<pin name="IO_L03P_0"/>
<pin name="IO_L04N_0/VREF_0"/>
<pin name="IO_L04P_0"/>
<pin name="IO_L05N_0"/>
<pin name="IO_L05P_0"/>
<pin name="IO_L07N_0/GCLK5"/>
<pin name="IO_LO7P_0/GCLK4"/>
<pin name="IO_L08N_0/GCLK7"/>
<pin name="IO_L08P_0/GCLK6"/>
<pin name="IO_L10N_0/GCLK11"/>
<pin name="IO_L10P_0/GCLK10"/>
<pin name="IO_L11N_0"/>
<pin name="IO_L11P_0"/>
<pin name="IO_L12N_0/VREF_0"/>
<pin name="IO_L12P_0"/>
<pin name="IO_L13N_0"/>
<pin name="IO_L13P_0"/>
<pin name="IO_L14N_0/VREF_0"/>
<pin name="IO_L15N_0"/>
<pin name="IO_L14P_0"/>
<pin name="IO_L15P_0"/>
<pin name="IO_L16N_0/HSWAP"/>
<pin name="IO_L16P_0"/>
<pin name="IP"/>
<pin name="IP@2"/>
<pin name="IP@3"/>
<pin name="IP@4"/>
<pin name="IP_L06N_0"/>
<pin name="IP_L06P_0"/>
<pin name="IP_LO9N_0/GCLK9"/>
<pin name="IP_L09P_0/GCLK8"/>
<pin name="VCCO_0"/>
<pin name="VCCO_0@2"/>
<pin name="VCCO_0@3"/>
<pin name="IO_L01N_1/A15"/>
<pin name="IO_L01P_1/A16"/>
<pin name="IO_L02N_1/A13"/>
<pin name="IO_L02P_1/A14"/>
<pin name="IO_L03N_1/VREF_1"/>
<pin name="IO_L03P_1"/>
<pin name="IO_L04N_1"/>
<pin name="IO_L04P_1"/>
<pin name="IO_L05N_1/A11"/>
<pin name="IO_L05P_1/A12"/>
<pin name="IO_L06N_1/VREF_1"/>
<pin name="IO_L06P_1"/>
<pin name="IO_L07N_1/A7/RHCLK1"/>
<pin name="IO_L07P_1/A10/RHCLK0"/>
<pin name="IO_L08N_1/A7/RHCLK3"/>
<pin name="IO_L08P_1/A8/RHCLK2"/>
<pin name="IO_L09N_1/A5/RHCLK5"/>
<pin name="IO_L09P_1/A6/RHCLK4"/>
<pin name="IO_L10N_1/A3/RHCLK7"/>
<pin name="IO_L10P_1/A4/RHCLK6"/>
<pin name="IO_L11N_1/A1"/>
<pin name="IO_L11P_1/A2"/>
<pin name="IO_L12N_1/A0"/>
<pin name="IO_L12P_1"/>
<pin name="IO_L13N_1"/>
<pin name="IO_L13P_1"/>
<pin name="IO_L14N_1"/>
<pin name="IO_L14P_1"/>
<pin name="IO_L15_1/LDC0"/>
<pin name="IO_L15P_1/HDC"/>
<pin name="IO_L16N_1/LDC2"/>
<pin name="IO_16P_1/LDC1"/>
<pin name="IP@5"/>
<pin name="IP@6"/>
<pin name="IP@7"/>
<pin name="IP@8"/>
<pin name="IP@9"/>
<pin name="IP@10"/>
<pin name="IP@11"/>
<pin name="IP/VREF_1"/>
<pin name="VCC0_1"/>
<pin name="VCC0_1@2"/>
<pin name="VCC0_1@3"/>
<pin name="IO/D5"/>
<pin name="IO/M1"/>
<pin name="IO/VREF_2"/>
<pin name="IO/L01N_2/INIT_B"/>
<pin name="IO_L01P_2/CSO_B"/>
<pin name="IO_L03N_2/MOSI/CSI_B"/>
<pin name="IO_L03P_2/DOUT/BUSY"/>
<pin name="IO_L04N_2"/>
<pin name="IO_L04P_2"/>
<pin name="IO_L05N_2"/>
<pin name="IO_L05P_2"/>
<pin name="IO_L06N_2"/>
<pin name="IO_L06P_2"/>
<pin name="IO_L08N_2/D6/GCLK13"/>
<pin name="10_L08P_2/D7/GCLK12"/>
<pin name="IO_L09N_2/D3/GCLK15"/>
<pin name="IO_L09P_2/D4/GCLK14"/>
<pin name="IO_L11N_2/D1/GCLK3"/>
<pin name="IO_L11P_2/D2/GCLK2"/>
<pin name="IO_L12N_2/DIN/D0"/>
<pin name="IO_L12P_2/M0"/>
<pin name="IO_L13N_2"/>
<pin name="IO_L13P_2"/>
<pin name="IO_L14N_2/A22"/>
<pin name="IO_L14P_2/A23"/>
<pin name="IO_L15N_2/A20"/>
<pin name="IO_L15P_2/A21"/>
<pin name="IO_L16N_2/VS1/A18"/>
<pin name="IO_L16P_2/VS2/A19"/>
<pin name="IO_L17N_2/CCLK"/>
<pin name="IO_L17P_2/VS0/A17"/>
<pin name="IP@12"/>
<pin name="IP@13"/>
<pin name="IP@14"/>
<pin name="IP_L02N_2"/>
<pin name="IP_L02P_2"/>
<pin name="IP_L07N_2/VREF_2"/>
<pin name="IP_L07P_2"/>
<pin name="IP_L10N_2/M2/GCLK1"/>
<pin name="IP_L10P_2/RDWR_B/GCLK0"/>
<pin name="VCCO_2"/>
<pin name="VCCO_2@2"/>
<pin name="VCCO_2@3"/>
<pin name="IO/VREF_3"/>
<pin name="IO_L01N_3"/>
<pin name="IO_L01P_3"/>
<pin name="IO_L02N_3/VREF_3"/>
<pin name="IO_L02P_3"/>
<pin name="IO_L03N_3"/>
<pin name="IO_L03P_3"/>
<pin name="IO_L04N_3"/>
<pin name="IO_L04P_3"/>
<pin name="IO_L05N_3"/>
<pin name="IO_L05P_3"/>
<pin name="IO_L06N_3"/>
<pin name="IO_L06P_3"/>
<pin name="IO_L07N_3/LHCLK1"/>
<pin name="IO_L07P_3/LHCLK0"/>
<pin name="IO_L08N_3/LHCLK3"/>
<pin name="IO_L08P_3/LHCLK2"/>
<pin name="IO_L09N_3/LHCLK5"/>
<pin name="IO_L09P_3/LHCLK4"/>
<pin name="IO_L10N_3/LHCLK7"/>
<pin name="IO_L10P_3/LHCLK6"/>
<pin name="IO_L11N_3"/>
<pin name="IO_L11P_3"/>
<pin name="IO_L12N_3"/>
<pin name="IO_L12P_3"/>
<pin name="IO_L13N_3"/>
<pin name="IO_L13P_3"/>
<pin name="IO_L14N_3"/>
<pin name="IO_L14P_3"/>
<pin name="IO_L15N_3"/>
<pin name="IO_L15P_3"/>
<pin name="IO_L16N_3"/>
<pin name="IO_L16P_3"/>
<pin name="IP@15"/>
<pin name="IP@16"/>
<pin name="IP@17"/>
<pin name="IP@18"/>
<pin name="IP@19"/>
<pin name="IP@20"/>
<pin name="IP/VREF_3"/>
<pin name="VCCO_3"/>
<pin name="VCCO_3@2"/>
<pin name="VCCO_3@3"/>
</symbol>
<symbol name="XMEGA">
<pin name="GND@84"/>
<pin name="GND@93"/>
<pin name="AVCC@4"/>
<pin name="AVCC@94"/>
<pin name="GND@3"/>
<pin name="GND@13"/>
<pin name="GND@23"/>
<pin name="GND@33"/>
<pin name="GND@43"/>
<pin name="GND@53"/>
<pin name="GND@63"/>
<pin name="GND@73"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PDI/PDI_DATA"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PJ5"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="RESET/PDI_CLOCK"/>
<pin name="VCC@14"/>
<pin name="VCC@24"/>
<pin name="VCC@34"/>
<pin name="VCC@44"/>
<pin name="VCC@54"/>
<pin name="VCC@64"/>
<pin name="VCC@74"/>
<pin name="VCC@83"/>
</symbol>
<symbol name="XMEGA-A3B">
<pin name="/RESET_PDI_CLK"/>
<pin name="PDI_DATA"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="VCC3"/>
<pin name="VCC4"/>
<pin name="VCC5"/>
<pin name="PF5"/>
<pin name="PR0(XTAL2)"/>
<pin name="PR1(XTAL1)"/>
<pin name="PA0(ADC0/AC0/AREF)"/>
<pin name="PA1(ADC1/AC1)"/>
<pin name="PA2(ADC2/AC2)"/>
<pin name="PA3(ADC3/AC3)"/>
<pin name="PA4(ADC4/AC4)"/>
<pin name="PA5(ADC5/AC5)"/>
<pin name="PA6(ADC6/AC6)"/>
<pin name="PA7(ADC7/AC7/AC0OUT)"/>
<pin name="PB0(ADC0/AC0/AREF)"/>
<pin name="PB1(ADC1/AC1)"/>
<pin name="PB2(ADC2/AC2/DAC0)"/>
<pin name="PB3(ADC3/AC3/DAC1)"/>
<pin name="PB4(ADC4/AC4/TMS)"/>
<pin name="PB5(ADC5/AC5/TDI)"/>
<pin name="PB6(ADC6/AC6/TCK)"/>
<pin name="PB7(ADC7/AC7/AC0OUT/TDO)"/>
<pin name="PC1(OC0B/AC0AH/XCK0/SCL)"/>
<pin name="PC0(OC0A/OC0AL/SDA)"/>
<pin name="PC2(OC0C/OC0BL/RXD0)"/>
<pin name="PC3(OC0D/OX0BH/TXD0)"/>
<pin name="PC4(AC1A/OC0CL/SS)"/>
<pin name="PC5(OC1B/OC0CH/XCK1/MOSI)"/>
<pin name="PC6(OC0DL/RXD1/MISO)"/>
<pin name="PC7(OC0DH/CKOUT/EVO/TXD1/SCK)"/>
<pin name="PD0(OC0A)"/>
<pin name="PD1(OC0B/XCK0)"/>
<pin name="PD2(OC0C/RXD0)"/>
<pin name="PD3(OX0D/TXD0)"/>
<pin name="PD4(OC1A/SS)"/>
<pin name="PD5(OC1B/XCK1/MOSI)"/>
<pin name="PD6(RXD1/MISO)"/>
<pin name="PD7(CKOUT/EVO/TXD1/SCK)"/>
<pin name="PE0(OC0A/SDA)"/>
<pin name="PE1(OC0B/XCK0/SCL)"/>
<pin name="PE2(OC0C/RXD0)"/>
<pin name="PE3(OC0D/TXD0)"/>
<pin name="PE4(OC1A/SS)"/>
<pin name="PE5(OC1B/XCK1/MOSI)"/>
<pin name="PE6(TOSC2/RXD1/MISO)"/>
<pin name="PE7(TOSC1/CKOUT/EVO/TXD1/SCK)"/>
<pin name="PF0(OC0A)"/>
<pin name="PF1(OC0B/XCK0)"/>
<pin name="PF2(OC0C/RXD0)"/>
<pin name="PF3(OC0D/TXD0)"/>
<pin name="PF4"/>
<pin name="PF6"/>
<pin name="PF7"/>
</symbol>
<symbol name="XR2206">
<pin name="AMSI" direction="in"/>
<pin name="STO" direction="out"/>
<pin name="MO" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="TC1" direction="in"/>
<pin name="TC2" direction="in"/>
<pin name="TR1" direction="out"/>
<pin name="TR2" direction="out"/>
<pin name="FSKI" direction="in"/>
<pin name="BIAS" direction="out"/>
<pin name="SYNCO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="WAVEA1" direction="in"/>
<pin name="WAVEA2" direction="in"/>
<pin name="SYMA1" direction="in"/>
<pin name="SYMA2" direction="in"/>
</symbol>
<symbol name="XS1-L1-64LQFP">
<pin name="VDDIO_6"/>
<pin name="VDDIO_18"/>
<pin name="VDDIO_32"/>
<pin name="VDDIO_40"/>
<pin name="VDDIO_53"/>
<pin name="VDDIO_60"/>
<pin name="VDD_4"/>
<pin name="VDD_13"/>
<pin name="VDD_21"/>
<pin name="VDD_28"/>
<pin name="VDD_37"/>
<pin name="VDD_43"/>
<pin name="VDD_52"/>
<pin name="VDD_61"/>
<pin name="PLL_AVDD"/>
<pin name="PLL_AGND"/>
<pin name="MODE0"/>
<pin name="MODE1"/>
<pin name="MODE2"/>
<pin name="MODE3"/>
<pin name="DEBUG"/>
<pin name="RST_N"/>
<pin name="CLK"/>
<pin name="TDO"/>
<pin name="TDI"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="TRST_N"/>
<pin name="GND"/>
<pin name="X0D0"/>
<pin name="X0D1"/>
<pin name="X0D2"/>
<pin name="X0D3"/>
<pin name="X0D4"/>
<pin name="X0D5"/>
<pin name="X0D6"/>
<pin name="X0D7"/>
<pin name="X0D8"/>
<pin name="X0D9"/>
<pin name="X0D10"/>
<pin name="X0D11"/>
<pin name="X0D12"/>
<pin name="X0D13"/>
<pin name="X0D14"/>
<pin name="X0D15"/>
<pin name="X0D16"/>
<pin name="X0D17"/>
<pin name="X0D18"/>
<pin name="X0D19"/>
<pin name="X0D20"/>
<pin name="X0D21"/>
<pin name="X0D22"/>
<pin name="X0D23"/>
<pin name="X0D24"/>
<pin name="X0D25"/>
<pin name="X0D26"/>
<pin name="X0D32"/>
<pin name="X0D33"/>
<pin name="X0D34"/>
<pin name="X0D35"/>
<pin name="X0D36"/>
<pin name="X0D37"/>
<pin name="X0D38"/>
<pin name="X0D27"/>
<pin name="X0D39"/>
</symbol>
<symbol name="74AHC1G08">
<pin name="B"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="Y"/>
</symbol>
<symbol name="OR-SINGLE">
<pin name="B"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="Y"/>
</symbol>
<symbol name="74157">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
<pin name="3A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3Y" direction="out"/>
<pin name="4A" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74595">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QH*" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74ACT125D">
<pin name="VCC"/>
<pin name="A0"/>
<pin name="B0"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="A2"/>
<pin name="B2"/>
<pin name="GND"/>
<pin name="B3"/>
<pin name="A3"/>
<pin name="O3"/>
<pin name="O2"/>
<pin name="O1"/>
<pin name="O0"/>
</symbol>
<symbol name="74HC04_HEX_INVERTER">
<pin name="VCC" direction="pwr"/>
<pin name="2A" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="5A" direction="in"/>
<pin name="6A" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="6Y" direction="out"/>
<pin name="5Y" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="1A" direction="in"/>
<pin name="1Y" direction="out"/>
</symbol>
<symbol name="74LVC138AD">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="/E1"/>
<pin name="/E2"/>
<pin name="E3"/>
<pin name="/Y7"/>
<pin name="GND"/>
<pin name="/Y6"/>
<pin name="/Y5"/>
<pin name="/Y4"/>
<pin name="/Y3"/>
<pin name="/Y2"/>
<pin name="/Y1"/>
<pin name="/Y0"/>
<pin name="VCC"/>
</symbol>
<symbol name="A6282">
<pin name="GND@1"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="VDD"/>
<pin name="REXT"/>
<pin name="SDO"/>
<pin name="~OE"/>
<pin name="OUT15"/>
<pin name="OUT14"/>
<pin name="OUT13"/>
<pin name="OUT12"/>
<pin name="OUT11"/>
<pin name="OUT10"/>
<pin name="OUT8"/>
<pin name="OUT9"/>
<pin name="GND@2"/>
</symbol>
<symbol name="AD725">
<pin name="STND"/>
<pin name="AGND"/>
<pin name="4FSC"/>
<pin name="APOS"/>
<pin name="CE"/>
<pin name="RIN"/>
<pin name="GIN"/>
<pin name="BIN"/>
<pin name="HSYNC"/>
<pin name="VSYNC"/>
<pin name="DPOS"/>
<pin name="DGND"/>
<pin name="YTRAP"/>
<pin name="LUMA"/>
<pin name="COMP"/>
<pin name="CRMA"/>
</symbol>
<symbol name="WTV020SD-20S">
<pin name="P03"/>
<pin name="P04"/>
<pin name="P05"/>
<pin name="P06"/>
<pin name="P07"/>
<pin name="VCC"/>
<pin name="SPK_P"/>
<pin name="SPK_N"/>
<pin name="NC"/>
<pin name="PAD_EQO"/>
<pin name="PAD_EQI"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="VDD"/>
<pin name="OSCI/P10"/>
<pin name="OSCO/P11"/>
<pin name="RESET"/>
<pin name="P00"/>
<pin name="P01"/>
<pin name="P02"/>
</symbol>
<symbol name="DIL40">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="DIL24">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="MBED_NXP_LPC1768">
<description>&lt;h3&gt;mbed NXP LPC1768&lt;/h3&gt;
&lt;p&gt;Microcontroller development board featuring an ARM cortex M3 and an online IDE with driverless USB programming.&lt;/p&gt;</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
</symbol>
<symbol name="ATTINY2313A">
<pin name="PA2/!RESET"/>
<pin name="PD0/RXD"/>
<pin name="PD1/TXD"/>
<pin name="PA1/XTAL2"/>
<pin name="PA0/XTAL1"/>
<pin name="PD2/INT0"/>
<pin name="PD3/INT1"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="PB7/SCK/SCL"/>
<pin name="PB6/MISO/DO"/>
<pin name="PB5/MOSI/SDA/DI"/>
<pin name="PB4"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="PB1"/>
<pin name="PB0"/>
<pin name="PD6"/>
</symbol>
<symbol name="ATTINY84">
<pin name="VCC"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT11/~RESET/DW)PB3"/>
<pin name="GND"/>
</symbol>
<symbol name="74165">
<pin name="B" direction="hiz"/>
<pin name="C" direction="hiz"/>
<pin name="D" direction="hiz"/>
<pin name="E" direction="hiz"/>
<pin name="F" direction="hiz"/>
<pin name="G" direction="hiz"/>
<pin name="H" direction="hiz"/>
<pin name="!QH" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLK_INH" direction="in"/>
<pin name="SH/!LD" direction="in"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TXB0104PWR">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="OE"/>
</symbol>
<symbol name="SPARKFUN-DIGITALIC_ATMEGA32U4">
<pin name="!RESET"/>
<pin name="AREF"/>
<pin name="AVCC@24"/>
<pin name="AVCC@44"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND@15"/>
<pin name="GND@23"/>
<pin name="GND@35"/>
<pin name="GND@43"/>
<pin name="PB0(SS)"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4(ADC11)"/>
<pin name="PB5(ADC12)"/>
<pin name="PB6(ADC13)"/>
<pin name="PB7"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0(SCL)"/>
<pin name="PD1(SDA)"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4(ADC8)"/>
<pin name="PD5"/>
<pin name="PD6(ADC9)"/>
<pin name="PD7(ADC10)"/>
<pin name="PE2/!HWB"/>
<pin name="PE6"/>
<pin name="PF0(ADC0)"/>
<pin name="PF1(ADC1)"/>
<pin name="PF4(ADC4)"/>
<pin name="PF5(ADC5)"/>
<pin name="PF6(ADC6)"/>
<pin name="PF7(ADC7)"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VBUS"/>
<pin name="VCC@14"/>
<pin name="VCC@34"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
</symbol>
<symbol name="ATSHA204">
<pin name="SDA"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="SX1509">
<description>&lt;h3&gt;Semtech SX1509&lt;/h3&gt;
Level Shifting GPIO Expander w/ LED Driver and Keypad Engine</description>
<pin name="VDDM"/>
<pin name="!RESET"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="!INT"/>
<pin name="GND"/>
<pin name="VCC1"/>
<pin name="I/O[0]"/>
<pin name="I/O[1]"/>
<pin name="I/O[2]"/>
<pin name="I/O[3]"/>
<pin name="I/O[4]"/>
<pin name="I/O[5]"/>
<pin name="I/O[6]"/>
<pin name="I/O[7]"/>
<pin name="VCC2"/>
<pin name="I/O[8]"/>
<pin name="I/O[9]"/>
<pin name="I/O[10]"/>
<pin name="I/O[11]"/>
<pin name="I/O[12]"/>
<pin name="I/O[13]"/>
<pin name="I/O[14]"/>
<pin name="I/O[15]"/>
<pin name="OSCIO"/>
<pin name="ADDR0"/>
<pin name="ADDR1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AT25FS010">
<description>1-Mbit SPI flash memory</description>
<gates>
<gate name="G$1" symbol="AT25FS010"/>
</gates>
<devices>
<device name="" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB041B">
<description>4-Mbit SPI flash memory</description>
<gates>
<gate name="G$1" symbol="AT45DB041B"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB161D">
<description>16-Mbit SPI flash memory</description>
<gates>
<gate name="G$1" symbol="AT45DB161D"/>
</gates>
<devices>
<device name="" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8U2" prefix="U">
<description>Atmel 32-pin 8-bit Microcontroller with 8/16/32K Bystes of ISP Flash and USB Controller. ATmega8U2, ATmega16U2, and ATmega32U2</description>
<gates>
<gate name="G$1" symbol="ATMEGA8U2"/>
</gates>
<devices>
<device name="AU" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PB0" pad="14"/>
<connect gate="G$1" pin="PB1(SCK)" pad="15"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="16"/>
<connect gate="G$1" pin="PB3(MISO)" pad="17"/>
<connect gate="G$1" pin="PB4" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="20"/>
<connect gate="G$1" pin="PB7" pad="21"/>
<connect gate="G$1" pin="PC2" pad="5"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="25"/>
<connect gate="G$1" pin="PC6" pad="23"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="6"/>
<connect gate="G$1" pin="PD1" pad="7"/>
<connect gate="G$1" pin="PD2(RX)" pad="8"/>
<connect gate="G$1" pin="PD3(TX)" pad="9"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="PD5" pad="11"/>
<connect gate="G$1" pin="PD6(RTS)" pad="12"/>
<connect gate="G$1" pin="PD7(CTS)" pad="13"/>
<connect gate="G$1" pin="RESET/PC1" pad="24"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
<connect gate="G$1" pin="XTAL2/PC0" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA128" prefix="U">
<description>ATmega128/128L/1281/2561. Note: The ATmega128 pin 1 is PEN and the ATmega256/1281 pin 1 is PG5.</description>
<gates>
<gate name="G$1" symbol="ATMEGA128"/>
</gates>
<devices>
<device name="_SMD" package="TQFP64">
<connects>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PB0(SS)" pad="10"/>
<connect gate="G$1" pin="PB1(SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(MISO)" pad="13"/>
<connect gate="G$1" pin="PB4" pad="14"/>
<connect gate="G$1" pin="PB5" pad="15"/>
<connect gate="G$1" pin="PB6" pad="16"/>
<connect gate="G$1" pin="PB7" pad="17"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD0(SCL)" pad="25"/>
<connect gate="G$1" pin="PD1(SDA)" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PE0(RXD)" pad="2"/>
<connect gate="G$1" pin="PE1(TXD)" pad="3"/>
<connect gate="G$1" pin="PE2" pad="4"/>
<connect gate="G$1" pin="PE3" pad="5"/>
<connect gate="G$1" pin="PE4" pad="6"/>
<connect gate="G$1" pin="PE5" pad="7"/>
<connect gate="G$1" pin="PE6" pad="8"/>
<connect gate="G$1" pin="PE7" pad="9"/>
<connect gate="G$1" pin="PF0" pad="61"/>
<connect gate="G$1" pin="PF1" pad="60"/>
<connect gate="G$1" pin="PF2" pad="59"/>
<connect gate="G$1" pin="PF3" pad="58"/>
<connect gate="G$1" pin="PF4" pad="57"/>
<connect gate="G$1" pin="PF5" pad="56"/>
<connect gate="G$1" pin="PF6" pad="55"/>
<connect gate="G$1" pin="PF7" pad="54"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="PG3" pad="18"/>
<connect gate="G$1" pin="PG4" pad="19"/>
<connect gate="G$1" pin="PG5" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@21" pad="21"/>
<connect gate="G$1" pin="VCC@52" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="TQFP64_14X14MM">
<connects>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PB0(SS)" pad="10"/>
<connect gate="G$1" pin="PB1(SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(MISO)" pad="13"/>
<connect gate="G$1" pin="PB4" pad="14"/>
<connect gate="G$1" pin="PB5" pad="15"/>
<connect gate="G$1" pin="PB6" pad="16"/>
<connect gate="G$1" pin="PB7" pad="17"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD0(SCL)" pad="25"/>
<connect gate="G$1" pin="PD1(SDA)" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PE0(RXD)" pad="2"/>
<connect gate="G$1" pin="PE1(TXD)" pad="3"/>
<connect gate="G$1" pin="PE2" pad="4"/>
<connect gate="G$1" pin="PE3" pad="5"/>
<connect gate="G$1" pin="PE4" pad="6"/>
<connect gate="G$1" pin="PE5" pad="7"/>
<connect gate="G$1" pin="PE6" pad="8"/>
<connect gate="G$1" pin="PE7" pad="9"/>
<connect gate="G$1" pin="PF0" pad="61"/>
<connect gate="G$1" pin="PF1" pad="60"/>
<connect gate="G$1" pin="PF2" pad="59"/>
<connect gate="G$1" pin="PF3" pad="58"/>
<connect gate="G$1" pin="PF4" pad="57"/>
<connect gate="G$1" pin="PF5" pad="56"/>
<connect gate="G$1" pin="PF6" pad="55"/>
<connect gate="G$1" pin="PF7" pad="54"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="PG3" pad="18"/>
<connect gate="G$1" pin="PG4" pad="19"/>
<connect gate="G$1" pin="PG5" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@21" pad="21"/>
<connect gate="G$1" pin="VCC@52" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA168" prefix="U">
<description>Atmel 32-pin 8-bit micro, 16k flash.</description>
<gates>
<gate name="G$1" symbol="ATMEGAXX8-32PIN"/>
</gates>
<devices>
<device name="MLF" package="MLF32">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA2560" prefix="U">
<description>Atmel 100-pin 8-bit uC&lt;BR&gt;
64/128/256 Kbytes FLASH&lt;BR&gt;
4 Kbytes EEPROM&lt;BR&gt;
8 Kbytes SRAM&lt;BR&gt;
86 General Purpose I/O pins&lt;BR&gt;
12-channels16-bit PWM&lt;BR&gt;
4 x Serial USARTs&lt;BR&gt;
16-channels 10-bit A/D&lt;BR&gt;</description>
<gates>
<gate name="1" symbol="ATMEGA2560"/>
</gates>
<devices>
<device name="AU" package="TQFP100">
<connects>
<connect gate="1" pin="(A10)PC2" pad="55"/>
<connect gate="1" pin="(A11)PC3" pad="56"/>
<connect gate="1" pin="(A12)PC4" pad="57"/>
<connect gate="1" pin="(A13)PC5" pad="58"/>
<connect gate="1" pin="(A14)PC6" pad="59"/>
<connect gate="1" pin="(A15)PC7" pad="60"/>
<connect gate="1" pin="(A8)PC0" pad="53"/>
<connect gate="1" pin="(A9)PC1" pad="54"/>
<connect gate="1" pin="(AD0)PA0" pad="78"/>
<connect gate="1" pin="(AD1)PA1" pad="77"/>
<connect gate="1" pin="(AD2)PA2" pad="76"/>
<connect gate="1" pin="(AD3)PA3" pad="75"/>
<connect gate="1" pin="(AD4)PA4" pad="74"/>
<connect gate="1" pin="(AD5)PA5" pad="73"/>
<connect gate="1" pin="(AD6)PA6" pad="72"/>
<connect gate="1" pin="(AD7)PA7" pad="71"/>
<connect gate="1" pin="(ADC0)PF0" pad="97"/>
<connect gate="1" pin="(ADC1)PF1" pad="96"/>
<connect gate="1" pin="(ADC2)PF2" pad="95"/>
<connect gate="1" pin="(ADC3)PF3" pad="94"/>
<connect gate="1" pin="(ADC4/TCK)PF4" pad="93"/>
<connect gate="1" pin="(ADC5/TMS)PF5" pad="92"/>
<connect gate="1" pin="(ADC6/TDO)PF6" pad="91"/>
<connect gate="1" pin="(ADC7/TDI)PF7" pad="90"/>
<connect gate="1" pin="(ALE)PG2" pad="70"/>
<connect gate="1" pin="(CLKO/ICP3/INT7)PE7" pad="9"/>
<connect gate="1" pin="(ICP1)PD4" pad="47"/>
<connect gate="1" pin="(MISO/PCINT3)PB3" pad="22"/>
<connect gate="1" pin="(MOSI/PCINT2)PB2" pad="21"/>
<connect gate="1" pin="(OC0A/OC1C/PCINT7)PB7" pad="26"/>
<connect gate="1" pin="(OC0B)PG5" pad="1"/>
<connect gate="1" pin="(OC1A/PCINT5)PB5" pad="24"/>
<connect gate="1" pin="(OC1B/PCINT6)PB6" pad="25"/>
<connect gate="1" pin="(OC2A/PCINT4)PB4" pad="23"/>
<connect gate="1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="1" pin="(RD)PG1" pad="52"/>
<connect gate="1" pin="(RXD0/PCIN8)PE0" pad="2"/>
<connect gate="1" pin="(RXD1/INT2)PD2" pad="45"/>
<connect gate="1" pin="(SCK/PCINT1)PB1" pad="20"/>
<connect gate="1" pin="(SCL/INT0)PD0" pad="43"/>
<connect gate="1" pin="(SDA/INT1)PD1" pad="44"/>
<connect gate="1" pin="(SS/PCINT0)PB0" pad="19"/>
<connect gate="1" pin="(T0)PD7" pad="50"/>
<connect gate="1" pin="(T1)PD6" pad="49"/>
<connect gate="1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="1" pin="(TOSC1)PG4" pad="29"/>
<connect gate="1" pin="(TOSC2)PG3" pad="28"/>
<connect gate="1" pin="(TXD0)PE1" pad="3"/>
<connect gate="1" pin="(TXD1/INT3)PD3" pad="46"/>
<connect gate="1" pin="(WR)PG0" pad="51"/>
<connect gate="1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="1" pin="(XCK1)PD5" pad="48"/>
<connect gate="1" pin="AGND" pad="99"/>
<connect gate="1" pin="AREF" pad="98"/>
<connect gate="1" pin="AVCC" pad="100"/>
<connect gate="1" pin="GND" pad="11"/>
<connect gate="1" pin="GND1" pad="32"/>
<connect gate="1" pin="GND2" pad="62"/>
<connect gate="1" pin="GND3" pad="81"/>
<connect gate="1" pin="PH0(RXD2)" pad="12"/>
<connect gate="1" pin="PH1(TXD2)" pad="13"/>
<connect gate="1" pin="PH2(XCK2)" pad="14"/>
<connect gate="1" pin="PH3(OC4A)" pad="15"/>
<connect gate="1" pin="PH4(OC4B)" pad="16"/>
<connect gate="1" pin="PH5(OC4C)" pad="17"/>
<connect gate="1" pin="PH6(OC2B)" pad="18"/>
<connect gate="1" pin="PH7(T4)" pad="27"/>
<connect gate="1" pin="PJ0(RXD3/PCINT9)" pad="63"/>
<connect gate="1" pin="PJ1(TXD3/PCINT10)" pad="64"/>
<connect gate="1" pin="PJ2(XCK3/PCINT11)" pad="65"/>
<connect gate="1" pin="PJ3(PCINT12)" pad="66"/>
<connect gate="1" pin="PJ4(PCINT13)" pad="67"/>
<connect gate="1" pin="PJ5(PCINT14)" pad="68"/>
<connect gate="1" pin="PJ6(PCINT15)" pad="69"/>
<connect gate="1" pin="PJ7" pad="79"/>
<connect gate="1" pin="PK0(ADC8/PCINT16)" pad="89"/>
<connect gate="1" pin="PK1(ADC9/PCINT17)" pad="88"/>
<connect gate="1" pin="PK2(ADC10/PCINT18)" pad="87"/>
<connect gate="1" pin="PK3(ADC11/PCINT19)" pad="86"/>
<connect gate="1" pin="PK4(ADC12/PCINT20)" pad="85"/>
<connect gate="1" pin="PK5(ADC13/PCINT21)" pad="84"/>
<connect gate="1" pin="PK6(ADC14/PCINT22)" pad="83"/>
<connect gate="1" pin="PK7(ADC15/PCINT23)" pad="82"/>
<connect gate="1" pin="PL0(ICP4)" pad="35"/>
<connect gate="1" pin="PL1(ICP5)" pad="36"/>
<connect gate="1" pin="PL2(T5)" pad="37"/>
<connect gate="1" pin="PL3(OC5A)" pad="38"/>
<connect gate="1" pin="PL4(OC5B)" pad="39"/>
<connect gate="1" pin="PL5(OC5C)" pad="40"/>
<connect gate="1" pin="PL6" pad="41"/>
<connect gate="1" pin="PL7" pad="42"/>
<connect gate="1" pin="RESET" pad="30"/>
<connect gate="1" pin="VCC" pad="10"/>
<connect gate="1" pin="VCC1" pad="31"/>
<connect gate="1" pin="VCC2" pad="61"/>
<connect gate="1" pin="VCC3" pad="80"/>
<connect gate="1" pin="XTAL1" pad="34"/>
<connect gate="1" pin="XTAL2" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13">
<description>Atmel 8-pin 1kB flash uC</description>
<gates>
<gate name="G$1" symbol="ATTINY13"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP" package="DIP08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY24">
<description>Atmel 20-pin 2kB flash uC</description>
<gates>
<gate name="G$1" symbol="ATTINY24"/>
</gates>
<devices>
<device name="QFN" package="QFN20">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@0" pad="0"/>
<connect gate="G$1" pin="PA0/ADC0" pad="5"/>
<connect gate="G$1" pin="PA1/ADC1" pad="4"/>
<connect gate="G$1" pin="PA2/ADC2" pad="3"/>
<connect gate="G$1" pin="PA3/ADC3" pad="2"/>
<connect gate="G$1" pin="PA4/SCL" pad="1"/>
<connect gate="G$1" pin="PA5/MISO" pad="20"/>
<connect gate="G$1" pin="PA6/MOSI" pad="16"/>
<connect gate="G$1" pin="PA7/ADC7" pad="15"/>
<connect gate="G$1" pin="PB0" pad="11"/>
<connect gate="G$1" pin="PB1" pad="12"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3/RESET" pad="13"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45" prefix="U" uservalue="yes">
<description>Atmel 8-pin 2/4/8kB flash uC</description>
<gates>
<gate name="G$1" symbol="ATTINY13"/>
</gates>
<devices>
<device name="TINY45-20-SMT" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08922"/>
<attribute name="VALUE" value="Tiny45-20-SMT"/>
</technology>
</technologies>
</device>
<device name="TINY45-20-DIP" package="DIP08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09439"/>
<attribute name="VALUE" value="TINY45-20-DIP"/>
</technology>
</technologies>
</device>
<device name="TINY85-20-DIP" package="DIP08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE" value="TINY85-20-DIP"/>
</technology>
</technologies>
</device>
<device name="TINY85-20-SMT" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09092"/>
<attribute name="VALUE" value="Tiny85-20-SMT"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-MEGA8" prefix="U$">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
6-channel 10 bit ADC&lt;p&gt;
2-channel 8 bit ADC</description>
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="-MI" package="MLF32">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AI" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-MEGA8-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
2-channel 8 bit ADC</description>
<gates>
<gate name="G$1" symbol="23-I/O-2"/>
</gates>
<devices>
<device name="PTH" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIM" package="DIL28-3-SIMON">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ZIF_SOCKET" package="DIL28-3-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="DIL28-3-SIMON-KIT">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP210X_USB_UART" prefix="IC">
<description>&lt;b&gt;Single-Chip USB to UART Bridge&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP2101.pdf / cp2102.pdf. Spark Fun Electronics SKU : COM-00310</description>
<gates>
<gate name="G$1" symbol="CP2101"/>
</gates>
<devices>
<device name="" package="MLP28">
<connects>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="!SUSPEND" pad="11"/>
<connect gate="G$1" pin="CTS" pad="23"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="DCD" pad="1"/>
<connect gate="G$1" pin="DSR" pad="27"/>
<connect gate="G$1" pin="DTR" pad="28"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@M" pad="M"/>
<connect gate="G$1" pin="REGIN" pad="7"/>
<connect gate="G$1" pin="RI" pad="2"/>
<connect gate="G$1" pin="RTS" pad="24"/>
<connect gate="G$1" pin="RXD" pad="25"/>
<connect gate="G$1" pin="SUSPEND" pad="12"/>
<connect gate="G$1" pin="TXD" pad="26"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP2103_USB_UART" prefix="IC">
<description>&lt;b&gt;Single-Chip USB to UART Bridge&lt;/b&gt;
Source: www.silabs.com .. CP2103.pdf. Spark Fun Electronics SKU : COM-00309</description>
<gates>
<gate name="G$1" symbol="CP2103"/>
</gates>
<devices>
<device name="" package="MLP28">
<connects>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="!SUSPEND" pad="11"/>
<connect gate="G$1" pin="CTS" pad="22"/>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="4"/>
<connect gate="G$1" pin="DCD" pad="28"/>
<connect gate="G$1" pin="DSR" pad="26"/>
<connect gate="G$1" pin="DTR" pad="27"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@M" pad="M"/>
<connect gate="G$1" pin="GPIO_0" pad="19"/>
<connect gate="G$1" pin="GPIO_1" pad="18"/>
<connect gate="G$1" pin="GPIO_2" pad="17"/>
<connect gate="G$1" pin="GPIO_3" pad="16"/>
<connect gate="G$1" pin="REGIN" pad="7"/>
<connect gate="G$1" pin="RI" pad="1"/>
<connect gate="G$1" pin="RTS" pad="23"/>
<connect gate="G$1" pin="RXD" pad="24"/>
<connect gate="G$1" pin="SUSPEND" pad="12"/>
<connect gate="G$1" pin="TXD" pad="25"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VIO" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C64215">
<description>Cypress PSOC uC with USB</description>
<gates>
<gate name="G$1" symbol="CY7C64215"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="D+" pad="14"/>
<connect gate="G$1" pin="D-" pad="15"/>
<connect gate="G$1" pin="P00" pad="24"/>
<connect gate="G$1" pin="P01" pad="5"/>
<connect gate="G$1" pin="P02" pad="25"/>
<connect gate="G$1" pin="P03" pad="4"/>
<connect gate="G$1" pin="P04" pad="26"/>
<connect gate="G$1" pin="P05" pad="3"/>
<connect gate="G$1" pin="P06" pad="27"/>
<connect gate="G$1" pin="P07" pad="2"/>
<connect gate="G$1" pin="P10" pad="17"/>
<connect gate="G$1" pin="P11" pad="12"/>
<connect gate="G$1" pin="P12" pad="18"/>
<connect gate="G$1" pin="P13" pad="11"/>
<connect gate="G$1" pin="P14" pad="19"/>
<connect gate="G$1" pin="P15" pad="10"/>
<connect gate="G$1" pin="P16" pad="20"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20" pad="21"/>
<connect gate="G$1" pin="P21" pad="8"/>
<connect gate="G$1" pin="P22" pad="22"/>
<connect gate="G$1" pin="P23" pad="7"/>
<connect gate="G$1" pin="P24" pad="23"/>
<connect gate="G$1" pin="P25" pad="6"/>
<connect gate="G$1" pin="VDD@16" pad="16"/>
<connect gate="G$1" pin="VDD@28" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="1"/>
<connect gate="G$1" pin="VSS@13" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DOSONCHIP-IC">
<description>&lt;b&gt;DOSonCHIP IC&lt;/b&gt;
This is the tested schematic and footprint for the DOSonCHIP FAT16 FAT32 IC. Spark Fun Electronics SKU : COM-07956. QFN package also tested/proven.</description>
<gates>
<gate name="G$1" symbol="DOSONCHIP-IC"/>
</gates>
<devices>
<device name="LQFP" package="LQFP-32">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="13"/>
<connect gate="G$1" pin="CARD_CS" pad="18"/>
<connect gate="G$1" pin="CARD_DIN" pad="15"/>
<connect gate="G$1" pin="CARD_DOUT" pad="17"/>
<connect gate="G$1" pin="CARD_SCLK" pad="16"/>
<connect gate="G$1" pin="CARD_WP" pad="14"/>
<connect gate="G$1" pin="DIR" pad="22"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="25"/>
<connect gate="G$1" pin="I2C_SDA" pad="26"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="21"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="27"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="28"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="23"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="24"/>
<connect gate="G$1" pin="UART_RX" pad="29"/>
<connect gate="G$1" pin="UART_TX" pad="30"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="32"/>
<connect gate="G$1" pin="XTAL_OUT" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN" package="QFN-24">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="7"/>
<connect gate="G$1" pin="CARD_CS" pad="12"/>
<connect gate="G$1" pin="CARD_DIN" pad="9"/>
<connect gate="G$1" pin="CARD_DOUT" pad="11"/>
<connect gate="G$1" pin="CARD_SCLK" pad="10"/>
<connect gate="G$1" pin="CARD_WP" pad="8"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="17"/>
<connect gate="G$1" pin="I2C_SDA" pad="18"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="13"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="19"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="20"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="15"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="16"/>
<connect gate="G$1" pin="UART_RX" pad="21"/>
<connect gate="G$1" pin="UART_TX" pad="22"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="24"/>
<connect gate="G$1" pin="XTAL_OUT" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN_ALT1" package="QFN-24_ALT1.PAC">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="7"/>
<connect gate="G$1" pin="CARD_CS" pad="12"/>
<connect gate="G$1" pin="CARD_DIN" pad="9"/>
<connect gate="G$1" pin="CARD_DOUT" pad="11"/>
<connect gate="G$1" pin="CARD_SCLK" pad="10"/>
<connect gate="G$1" pin="CARD_WP" pad="8"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="17"/>
<connect gate="G$1" pin="I2C_SDA" pad="18"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="13"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="19"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="20"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="15"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="16"/>
<connect gate="G$1" pin="UART_RX" pad="21"/>
<connect gate="G$1" pin="UART_TX" pad="22"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="24"/>
<connect gate="G$1" pin="XTAL_OUT" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F4011">
<description>Microchip 16-bit DSP for UAVv2x, not tested</description>
<gates>
<gate name="G$1" symbol="DSPIC30F4011"/>
</gates>
<devices>
<device name="DIL" package="DIL40">
<connects>
<connect gate="G$1" pin="AVDD" pad="40"/>
<connect gate="G$1" pin="AVSS" pad="39"/>
<connect gate="G$1" pin="INT0/RE8" pad="17"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OC1/RD0" pad="23"/>
<connect gate="G$1" pin="OC2/RD1" pad="18"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="PGC/SDA" pad="26"/>
<connect gate="G$1" pin="PGD/SCL" pad="25"/>
<connect gate="G$1" pin="RB0/AREF+" pad="2"/>
<connect gate="G$1" pin="RB1/AREF-" pad="3"/>
<connect gate="G$1" pin="RB2" pad="4"/>
<connect gate="G$1" pin="RB3" pad="5"/>
<connect gate="G$1" pin="RB4/IC7" pad="6"/>
<connect gate="G$1" pin="RB5/IC8" pad="7"/>
<connect gate="G$1" pin="RB6" pad="8"/>
<connect gate="G$1" pin="RB7" pad="9"/>
<connect gate="G$1" pin="RB8" pad="10"/>
<connect gate="G$1" pin="RC13/TX1" pad="15"/>
<connect gate="G$1" pin="RC14/RX1" pad="16"/>
<connect gate="G$1" pin="RD2" pad="22"/>
<connect gate="G$1" pin="RD3" pad="19"/>
<connect gate="G$1" pin="RE0" pad="38"/>
<connect gate="G$1" pin="RE1" pad="37"/>
<connect gate="G$1" pin="RE2" pad="36"/>
<connect gate="G$1" pin="RE3" pad="35"/>
<connect gate="G$1" pin="RE4" pad="34"/>
<connect gate="G$1" pin="RE5" pad="33"/>
<connect gate="G$1" pin="RF0" pad="30"/>
<connect gate="G$1" pin="RF1" pad="29"/>
<connect gate="G$1" pin="RF4/RX2" pad="28"/>
<connect gate="G$1" pin="RF5/TX2" pad="27"/>
<connect gate="G$1" pin="RF6/SCK1" pad="24"/>
<connect gate="G$1" pin="VDD0" pad="11"/>
<connect gate="G$1" pin="VDD1" pad="21"/>
<connect gate="G$1" pin="VDD2" pad="32"/>
<connect gate="G$1" pin="VSS0" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="20"/>
<connect gate="G$1" pin="VSS2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="16"/>
<connect gate="G$1" pin="INT0/RE8" pad="36"/>
<connect gate="G$1" pin="MCLR" pad="18"/>
<connect gate="G$1" pin="OC1/RD0" pad="42"/>
<connect gate="G$1" pin="OC2/RD1" pad="37"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="PGC/SDA" pad="1"/>
<connect gate="G$1" pin="PGD/SCL" pad="44"/>
<connect gate="G$1" pin="RB0/AREF+" pad="19"/>
<connect gate="G$1" pin="RB1/AREF-" pad="20"/>
<connect gate="G$1" pin="RB2" pad="21"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4/IC7" pad="23"/>
<connect gate="G$1" pin="RB5/IC8" pad="24"/>
<connect gate="G$1" pin="RB6" pad="25"/>
<connect gate="G$1" pin="RB7" pad="26"/>
<connect gate="G$1" pin="RB8" pad="27"/>
<connect gate="G$1" pin="RC13/TX1" pad="32"/>
<connect gate="G$1" pin="RC14/RX1" pad="35"/>
<connect gate="G$1" pin="RD2" pad="41"/>
<connect gate="G$1" pin="RD3" pad="38"/>
<connect gate="G$1" pin="RE0" pad="15"/>
<connect gate="G$1" pin="RE1" pad="14"/>
<connect gate="G$1" pin="RE2" pad="11"/>
<connect gate="G$1" pin="RE3" pad="10"/>
<connect gate="G$1" pin="RE4" pad="9"/>
<connect gate="G$1" pin="RE5" pad="8"/>
<connect gate="G$1" pin="RF0" pad="5"/>
<connect gate="G$1" pin="RF1" pad="4"/>
<connect gate="G$1" pin="RF4/RX2" pad="3"/>
<connect gate="G$1" pin="RF5/TX2" pad="2"/>
<connect gate="G$1" pin="RF6/SCK1" pad="43"/>
<connect gate="G$1" pin="VDD0" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="28"/>
<connect gate="G$1" pin="VDD2" pad="40"/>
<connect gate="G$1" pin="VSS0" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="29"/>
<connect gate="G$1" pin="VSS2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6015" prefix="U">
<description>Microchip 16-bit DSP</description>
<gates>
<gate name="G$1" symbol="DSPIC30F6015"/>
</gates>
<devices>
<device name="SMD" package="TQFP64">
<connects>
<connect gate="G$1" pin="AGND@20" pad="20"/>
<connect gate="G$1" pin="AVDD@19" pad="19"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@41" pad="41"/>
<connect gate="G$1" pin="GND@56" pad="56"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="MCLR@7" pad="7"/>
<connect gate="G$1" pin="OSC1@39" pad="39"/>
<connect gate="G$1" pin="OSC2@40" pad="40"/>
<connect gate="G$1" pin="PGC@17" pad="17"/>
<connect gate="G$1" pin="PGD@18" pad="18"/>
<connect gate="G$1" pin="RB10@23" pad="23"/>
<connect gate="G$1" pin="RB11@24" pad="24"/>
<connect gate="G$1" pin="RB12@27" pad="27"/>
<connect gate="G$1" pin="RB13@28" pad="28"/>
<connect gate="G$1" pin="RB14@29" pad="29"/>
<connect gate="G$1" pin="RB15@30" pad="30"/>
<connect gate="G$1" pin="RB2@14" pad="14"/>
<connect gate="G$1" pin="RB3@13" pad="13"/>
<connect gate="G$1" pin="RB4@12" pad="12"/>
<connect gate="G$1" pin="RB5@11" pad="11"/>
<connect gate="G$1" pin="RB8@21" pad="21"/>
<connect gate="G$1" pin="RB9@22" pad="22"/>
<connect gate="G$1" pin="RC13@47" pad="47"/>
<connect gate="G$1" pin="RC14@48" pad="48"/>
<connect gate="G$1" pin="RD0@46" pad="46"/>
<connect gate="G$1" pin="RD10@44" pad="44"/>
<connect gate="G$1" pin="RD11@45" pad="45"/>
<connect gate="G$1" pin="RD1@49" pad="49"/>
<connect gate="G$1" pin="RD2@50" pad="50"/>
<connect gate="G$1" pin="RD3@51" pad="51"/>
<connect gate="G$1" pin="RD4@52" pad="52"/>
<connect gate="G$1" pin="RD5@53" pad="53"/>
<connect gate="G$1" pin="RD6@54" pad="54"/>
<connect gate="G$1" pin="RD7@55" pad="55"/>
<connect gate="G$1" pin="RD8@42" pad="42"/>
<connect gate="G$1" pin="RD9@43" pad="43"/>
<connect gate="G$1" pin="RE0@60" pad="60"/>
<connect gate="G$1" pin="RE1@61" pad="61"/>
<connect gate="G$1" pin="RE2@62" pad="62"/>
<connect gate="G$1" pin="RE3@63" pad="63"/>
<connect gate="G$1" pin="RE4@64" pad="64"/>
<connect gate="G$1" pin="RE5@1" pad="1"/>
<connect gate="G$1" pin="RE6@2" pad="2"/>
<connect gate="G$1" pin="RE7@3" pad="3"/>
<connect gate="G$1" pin="RF0@58" pad="58"/>
<connect gate="G$1" pin="RF1@59" pad="59"/>
<connect gate="G$1" pin="RF6@35" pad="35"/>
<connect gate="G$1" pin="RG2@37" pad="37"/>
<connect gate="G$1" pin="RG3@36" pad="36"/>
<connect gate="G$1" pin="RG6@4" pad="4"/>
<connect gate="G$1" pin="RG7@5" pad="5"/>
<connect gate="G$1" pin="RG8@6" pad="6"/>
<connect gate="G$1" pin="RG9@8" pad="8"/>
<connect gate="G$1" pin="RX1@34" pad="34"/>
<connect gate="G$1" pin="RX2@32" pad="32"/>
<connect gate="G$1" pin="TX1@33" pad="33"/>
<connect gate="G$1" pin="TX2@31" pad="31"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@26" pad="26"/>
<connect gate="G$1" pin="VDD@38" pad="38"/>
<connect gate="G$1" pin="VDD@57" pad="57"/>
<connect gate="G$1" pin="VREF+/RB0@16" pad="16"/>
<connect gate="G$1" pin="VREF-/RB1@15" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ256GP710" prefix="U">
<description>Microchip 16-bit DSP</description>
<gates>
<gate name="G1" symbol="DSPIC33FJ256GP710_POWER"/>
<gate name="G2" symbol="DSPIC33FJ256GP710_CONTROL"/>
<gate name="G3" symbol="DSPIC33FJ256GP710_EXTERNAL"/>
<gate name="G4" symbol="DSPIC33FJ256GP710_EXTRA"/>
</gates>
<devices>
<device name="_" package="TQFP-100-12X12MM">
<connects>
<connect gate="G1" pin="AVDD" pad="30"/>
<connect gate="G1" pin="AVSS" pad="31"/>
<connect gate="G1" pin="RA10/VREF+" pad="29"/>
<connect gate="G1" pin="RA9/VREF-" pad="28"/>
<connect gate="G1" pin="VCAP" pad="85"/>
<connect gate="G1" pin="VDD@16" pad="16"/>
<connect gate="G1" pin="VDD@2" pad="2"/>
<connect gate="G1" pin="VDD@37" pad="37"/>
<connect gate="G1" pin="VDD@46" pad="46"/>
<connect gate="G1" pin="VDD@62" pad="62"/>
<connect gate="G1" pin="VDD@86" pad="86"/>
<connect gate="G1" pin="VSS@15" pad="15"/>
<connect gate="G1" pin="VSS@36" pad="36"/>
<connect gate="G1" pin="VSS@45" pad="45"/>
<connect gate="G1" pin="VSS@65" pad="65"/>
<connect gate="G1" pin="VSS@75" pad="75"/>
<connect gate="G2" pin="RA6/AN22" pad="91"/>
<connect gate="G2" pin="RB0/AN0" pad="25"/>
<connect gate="G2" pin="RB1/AN1" pad="24"/>
<connect gate="G2" pin="RB10/AN10" pad="34"/>
<connect gate="G2" pin="RB11/AN11" pad="35"/>
<connect gate="G2" pin="RB12/AN12" pad="41"/>
<connect gate="G2" pin="RB13/AN13" pad="42"/>
<connect gate="G2" pin="RB14/AN14" pad="43"/>
<connect gate="G2" pin="RB3/AN3" pad="22"/>
<connect gate="G2" pin="RB4/AN4" pad="21"/>
<connect gate="G2" pin="RB5/AN5" pad="20"/>
<connect gate="G2" pin="RB6/AN6" pad="26"/>
<connect gate="G2" pin="RB7/AN7" pad="27"/>
<connect gate="G2" pin="RB8/AN8" pad="32"/>
<connect gate="G2" pin="RB9/AN9" pad="33"/>
<connect gate="G2" pin="RC4/AN19" pad="9"/>
<connect gate="G2" pin="RD0/OC1" pad="72"/>
<connect gate="G2" pin="RD1/OC2" pad="76"/>
<connect gate="G2" pin="RD10/IC3" pad="70"/>
<connect gate="G2" pin="RD11/IC4" pad="71"/>
<connect gate="G2" pin="RD12/IC5" pad="79"/>
<connect gate="G2" pin="RD13/IC6" pad="80"/>
<connect gate="G2" pin="RD14/U1CTS/IC7" pad="47"/>
<connect gate="G2" pin="RD15/U1RTS/IC8" pad="48"/>
<connect gate="G2" pin="RD2/OC3" pad="77"/>
<connect gate="G2" pin="RD3/OC4" pad="78"/>
<connect gate="G2" pin="RD4/OC5" pad="81"/>
<connect gate="G2" pin="RD5/OC6" pad="82"/>
<connect gate="G2" pin="RD6/OC7" pad="83"/>
<connect gate="G2" pin="RD7/OC8" pad="84"/>
<connect gate="G2" pin="RD8/IC1" pad="68"/>
<connect gate="G2" pin="RD9/IC2" pad="69"/>
<connect gate="G2" pin="RE1/AN25" pad="94"/>
<connect gate="G2" pin="RE2" pad="98"/>
<connect gate="G2" pin="RE3" pad="99"/>
<connect gate="G2" pin="RE4" pad="100"/>
<connect gate="G2" pin="RF2/U1RX" pad="52"/>
<connect gate="G2" pin="RF3/U1TX" pad="51"/>
<connect gate="G2" pin="RG2/SCL1" pad="57"/>
<connect gate="G2" pin="RG3/SDA1" pad="56"/>
<connect gate="G3" pin="MCLR" pad="13"/>
<connect gate="G3" pin="RA1" pad="38"/>
<connect gate="G3" pin="RA12/INT1" pad="18"/>
<connect gate="G3" pin="RA13/INT2" pad="19"/>
<connect gate="G3" pin="RA14" pad="66"/>
<connect gate="G3" pin="RA2/SCL2" pad="58"/>
<connect gate="G3" pin="RA3/SDA2" pad="59"/>
<connect gate="G3" pin="RA4/TDI" pad="60"/>
<connect gate="G3" pin="RA5/TDO" pad="61"/>
<connect gate="G3" pin="RA7/AN23" pad="92"/>
<connect gate="G3" pin="RB15/AN15" pad="44"/>
<connect gate="G3" pin="RB2/SS1" pad="23"/>
<connect gate="G3" pin="RC1/AN16" pad="6"/>
<connect gate="G3" pin="RC13/PGED2" pad="73"/>
<connect gate="G3" pin="RC14/PGEC2" pad="74"/>
<connect gate="G3" pin="RC2/AN17" pad="7"/>
<connect gate="G3" pin="RC3/AN18" pad="8"/>
<connect gate="G3" pin="RE0/AN24" pad="93"/>
<connect gate="G3" pin="RF0/C1RX1" pad="87"/>
<connect gate="G3" pin="RF1/C1TX1" pad="88"/>
<connect gate="G3" pin="RF12/U2CTS" pad="40"/>
<connect gate="G3" pin="RF13/U2RTS" pad="39"/>
<connect gate="G3" pin="RF4/U2RX" pad="49"/>
<connect gate="G3" pin="RF5/U2TX" pad="50"/>
<connect gate="G3" pin="RF6/SCK1" pad="55"/>
<connect gate="G3" pin="RF7/SDI1" pad="54"/>
<connect gate="G3" pin="RF8/SDO1" pad="53"/>
<connect gate="G3" pin="RG6/SCK2" pad="10"/>
<connect gate="G3" pin="RG7/SDI2" pad="11"/>
<connect gate="G3" pin="RG8/SDO2" pad="12"/>
<connect gate="G3" pin="RG9/SS2" pad="14"/>
<connect gate="G4" pin="RA0/TMS" pad="17"/>
<connect gate="G4" pin="RA15" pad="67"/>
<connect gate="G4" pin="RC12/OSC1" pad="63"/>
<connect gate="G4" pin="RC15/OSC2" pad="64"/>
<connect gate="G4" pin="RE5/AN29" pad="3"/>
<connect gate="G4" pin="RE6/AN30" pad="4"/>
<connect gate="G4" pin="RE7/AN31" pad="5"/>
<connect gate="G4" pin="RG0/C2RX" pad="90"/>
<connect gate="G4" pin="RG1/C2TX" pad="89"/>
<connect gate="G4" pin="RG12/CSDI" pad="96"/>
<connect gate="G4" pin="RG13/CSDO" pad="97"/>
<connect gate="G4" pin="RG14/CSCK" pad="95"/>
<connect gate="G4" pin="RG15/COFS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM-I2C" prefix="U">
<description>I2C EEPROM chips, 24LC256 (and others)</description>
<gates>
<gate name="G$1" symbol="EEPROM-I2C"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EIAJ" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENC28J60" prefix="U" uservalue="yes">
<description>Microchip SPI 10Base ethernet IC</description>
<gates>
<gate name="G$1" symbol="ENC28J60"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="/INT" pad="4"/>
<connect gate="G$1" pin="CLKOUT" pad="3"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="LEDA" pad="27"/>
<connect gate="G$1" pin="LEDB" pad="26"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="23"/>
<connect gate="G$1" pin="OSC2" pad="24"/>
<connect gate="G$1" pin="RBIAS" pad="14"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SCK" pad="8"/>
<connect gate="G$1" pin="SI" pad="7"/>
<connect gate="G$1" pin="SO" pad="6"/>
<connect gate="G$1" pin="TPIN+" pad="13"/>
<connect gate="G$1" pin="TPIN-" pad="12"/>
<connect gate="G$1" pin="TPOUT+" pad="17"/>
<connect gate="G$1" pin="TPOUT-" pad="16"/>
<connect gate="G$1" pin="VCAP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VDDOSC" pad="25"/>
<connect gate="G$1" pin="VDDPLL" pad="20"/>
<connect gate="G$1" pin="VDDRX" pad="19"/>
<connect gate="G$1" pin="VDDTX" pad="15"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSSOSC" pad="22"/>
<connect gate="G$1" pin="VSSPLL" pad="21"/>
<connect gate="G$1" pin="VSSRX" pad="11"/>
<connect gate="G$1" pin="VSSTX" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C8_PQ208">
<description>Altera Cyclone2 FPGA, PQFP-208</description>
<gates>
<gate name="G$2" symbol="EP2C20_PQ208_PLL"/>
<gate name="G$6" symbol="EP2C20_PQ208_B3"/>
<gate name="G$4" symbol="EP2C20_PQ208_B1"/>
<gate name="G$3" symbol="EP2C20_PQ208_B4"/>
<gate name="G$7" symbol="EP2C20_PQ208_POWER"/>
<gate name="G$5" symbol="EP2C20_PQ208_B2"/>
<gate name="G$1" symbol="EP2C20_PQ208_CONFIG"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="G$1" pin="ASDO" pad="1"/>
<connect gate="G$1" pin="CLKUSR" pad="4"/>
<connect gate="G$1" pin="CONF_DONE" pad="123"/>
<connect gate="G$1" pin="CRC_ERROR" pad="3"/>
<connect gate="G$1" pin="DATA0" pad="20"/>
<connect gate="G$1" pin="DCLK" pad="21"/>
<connect gate="G$1" pin="DEV_OE" pad="56"/>
<connect gate="G$1" pin="INIT_DONE" pad="107"/>
<connect gate="G$1" pin="MSEL0" pad="126"/>
<connect gate="G$1" pin="MSEL1" pad="125"/>
<connect gate="G$1" pin="NCE" pad="22"/>
<connect gate="G$1" pin="NCEO" pad="108"/>
<connect gate="G$1" pin="NCONFIG" pad="26"/>
<connect gate="G$1" pin="NCSO" pad="2"/>
<connect gate="G$1" pin="NSTATUS" pad="121"/>
<connect gate="G$1" pin="TCK" pad="18"/>
<connect gate="G$1" pin="TDI" pad="19"/>
<connect gate="G$1" pin="TDO" pad="16"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$2" pin="GNDA_PLL1" pad="54"/>
<connect gate="G$2" pin="GNDA_PLL2" pad="158"/>
<connect gate="G$2" pin="GND_PLL1" pad="50"/>
<connect gate="G$2" pin="GND_PLL1@1" pad="52"/>
<connect gate="G$2" pin="GND_PLL2" pad="154"/>
<connect gate="G$2" pin="GND_PLL2@1" pad="156"/>
<connect gate="G$2" pin="VCCA_PLL1" pad="53"/>
<connect gate="G$2" pin="VCCA_PLL2" pad="157"/>
<connect gate="G$2" pin="VCCD_PLL1" pad="51"/>
<connect gate="G$2" pin="VCCD_PLL2" pad="155"/>
<connect gate="G$3" pin="IO@1" pad="80"/>
<connect gate="G$3" pin="IO@2" pad="96"/>
<connect gate="G$3" pin="IO_LVDS57N" pad="104"/>
<connect gate="G$3" pin="IO_LVDS57P" pad="103"/>
<connect gate="G$3" pin="IO_LVDS58N" pad="102"/>
<connect gate="G$3" pin="IO_LVDS58P" pad="101"/>
<connect gate="G$3" pin="IO_LVDS59N" pad="99"/>
<connect gate="G$3" pin="IO_LVDS59P" pad="97"/>
<connect gate="G$3" pin="IO_LVDS60N" pad="95"/>
<connect gate="G$3" pin="IO_LVDS60P" pad="94"/>
<connect gate="G$3" pin="IO_LVDS61N" pad="92"/>
<connect gate="G$3" pin="IO_LVDS61P" pad="90"/>
<connect gate="G$3" pin="IO_LVDS62N" pad="88"/>
<connect gate="G$3" pin="IO_LVDS62P" pad="87"/>
<connect gate="G$3" pin="IO_LVDS63N" pad="86"/>
<connect gate="G$3" pin="IO_LVDS63P" pad="84"/>
<connect gate="G$3" pin="IO_LVDS64N" pad="82"/>
<connect gate="G$3" pin="IO_LVDS64P" pad="81"/>
<connect gate="G$3" pin="IO_LVDS66N" pad="77"/>
<connect gate="G$3" pin="IO_LVDS66P" pad="76"/>
<connect gate="G$3" pin="IO_LVDS67N" pad="75"/>
<connect gate="G$3" pin="IO_LVDS67P" pad="74"/>
<connect gate="G$3" pin="IO_LVDS68N" pad="72"/>
<connect gate="G$3" pin="IO_LVDS68P" pad="70"/>
<connect gate="G$3" pin="IO_LVDS70N" pad="69"/>
<connect gate="G$3" pin="IO_LVDS70P" pad="68"/>
<connect gate="G$3" pin="IO_LVDS74N" pad="64"/>
<connect gate="G$3" pin="IO_LVDS74P" pad="63"/>
<connect gate="G$3" pin="IO_LVDS75N" pad="61"/>
<connect gate="G$3" pin="IO_LVDS75P" pad="60"/>
<connect gate="G$3" pin="IO_LVDS76N" pad="59"/>
<connect gate="G$3" pin="IO_LVDS76P" pad="58"/>
<connect gate="G$3" pin="IO_LVDS77P" pad="57"/>
<connect gate="G$3" pin="IO_VREFB4N0" pad="89"/>
<connect gate="G$3" pin="IO_VREFB4N1" pad="67"/>
<connect gate="G$3" pin="VCCIO4@1" pad="62"/>
<connect gate="G$3" pin="VCCIO4@2" pad="71"/>
<connect gate="G$3" pin="VCCIO4@3" pad="83"/>
<connect gate="G$3" pin="VCCIO4@4" pad="91"/>
<connect gate="G$3" pin="VCCIO4@5" pad="98"/>
<connect gate="G$4" pin="CLK0_LVDSCLK0P" pad="23"/>
<connect gate="G$4" pin="CLK1_LVDSCLK0N" pad="24"/>
<connect gate="G$4" pin="CLK2_LVDSCLK1P" pad="27"/>
<connect gate="G$4" pin="CLK3_LVDSCLK1N" pad="28"/>
<connect gate="G$4" pin="IO@2" pad="34"/>
<connect gate="G$4" pin="IO@3" pad="43"/>
<connect gate="G$4" pin="IO@4" pad="46"/>
<connect gate="G$4" pin="IO_LVDS0N" pad="45"/>
<connect gate="G$4" pin="IO_LVDS0P" pad="44"/>
<connect gate="G$4" pin="IO_LVDS12N" pad="12"/>
<connect gate="G$4" pin="IO_LVDS12P" pad="11"/>
<connect gate="G$4" pin="IO_LVDS13N" pad="10"/>
<connect gate="G$4" pin="IO_LVDS13P" pad="8"/>
<connect gate="G$4" pin="IO_LVDS14N" pad="6"/>
<connect gate="G$4" pin="IO_LVDS14P" pad="5"/>
<connect gate="G$4" pin="IO_LVDS2N" pad="41"/>
<connect gate="G$4" pin="IO_LVDS2P" pad="40"/>
<connect gate="G$4" pin="IO_LVDS3N" pad="39"/>
<connect gate="G$4" pin="IO_LVDS5P" pad="35"/>
<connect gate="G$4" pin="IO_LVDS6N" pad="33"/>
<connect gate="G$4" pin="IO_LVDS7N" pad="31"/>
<connect gate="G$4" pin="IO_LVDS7P" pad="30"/>
<connect gate="G$4" pin="IO_LVDS8N" pad="15"/>
<connect gate="G$4" pin="IO_LVDS8P" pad="14"/>
<connect gate="G$4" pin="IO_PLL1_OUTN" pad="48"/>
<connect gate="G$4" pin="IO_PLL1_OUTP" pad="47"/>
<connect gate="G$4" pin="IO_VREFB1N0" pad="13"/>
<connect gate="G$4" pin="IO_VREFB1N1" pad="37"/>
<connect gate="G$4" pin="VCCIO1@1" pad="7"/>
<connect gate="G$4" pin="VCCIO1@4" pad="29"/>
<connect gate="G$4" pin="VCCIO1@6" pad="42"/>
<connect gate="G$5" pin="IO_LVDS16N" pad="208"/>
<connect gate="G$5" pin="IO_LVDS16P" pad="207"/>
<connect gate="G$5" pin="IO_LVDS17N" pad="206"/>
<connect gate="G$5" pin="IO_LVDS17P" pad="205"/>
<connect gate="G$5" pin="IO_LVDS18N" pad="201"/>
<connect gate="G$5" pin="IO_LVDS18P" pad="203"/>
<connect gate="G$5" pin="IO_LVDS19N" pad="199"/>
<connect gate="G$5" pin="IO_LVDS19P" pad="200"/>
<connect gate="G$5" pin="IO_LVDS21N" pad="197"/>
<connect gate="G$5" pin="IO_LVDS21P" pad="198"/>
<connect gate="G$5" pin="IO_LVDS23N" pad="193"/>
<connect gate="G$5" pin="IO_LVDS23P" pad="195"/>
<connect gate="G$5" pin="IO_LVDS24N" pad="189"/>
<connect gate="G$5" pin="IO_LVDS24P" pad="191"/>
<connect gate="G$5" pin="IO_LVDS25N" pad="187"/>
<connect gate="G$5" pin="IO_LVDS25P" pad="188"/>
<connect gate="G$5" pin="IO_LVDS26P" pad="185"/>
<connect gate="G$5" pin="IO_LVDS28N" pad="181"/>
<connect gate="G$5" pin="IO_LVDS28P" pad="182"/>
<connect gate="G$5" pin="IO_LVDS29N" pad="179"/>
<connect gate="G$5" pin="IO_LVDS29P" pad="180"/>
<connect gate="G$5" pin="IO_LVDS31N" pad="175"/>
<connect gate="G$5" pin="IO_LVDS31P" pad="176"/>
<connect gate="G$5" pin="IO_LVDS33N" pad="171"/>
<connect gate="G$5" pin="IO_LVDS33P" pad="173"/>
<connect gate="G$5" pin="IO_LVDS34N" pad="168"/>
<connect gate="G$5" pin="IO_LVDS34P" pad="169"/>
<connect gate="G$5" pin="IO_LVDS35N" pad="164"/>
<connect gate="G$5" pin="IO_LVDS35P" pad="165"/>
<connect gate="G$5" pin="IO_LVDS36N" pad="162"/>
<connect gate="G$5" pin="IO_LVDS36P" pad="163"/>
<connect gate="G$5" pin="IO_LVDS37N" pad="160"/>
<connect gate="G$5" pin="IO_LVDS37P" pad="161"/>
<connect gate="G$5" pin="IO_VREFB2N0" pad="170"/>
<connect gate="G$5" pin="IO_VREFB2N1" pad="192"/>
<connect gate="G$5" pin="VCCIO2@1" pad="166"/>
<connect gate="G$5" pin="VCCIO2@2" pad="172"/>
<connect gate="G$5" pin="VCCIO2@3" pad="183"/>
<connect gate="G$5" pin="VCCIO2@4" pad="194"/>
<connect gate="G$5" pin="VCCIO2@5" pad="202"/>
<connect gate="G$6" pin="CLK4_LVDSCLK2P" pad="132"/>
<connect gate="G$6" pin="CLK5_LVDSCLK2N" pad="131"/>
<connect gate="G$6" pin="CLK6_LVDSCLK3P" pad="130"/>
<connect gate="G$6" pin="CLK7_LVDSCLK3N" pad="129"/>
<connect gate="G$6" pin="IO@1" pad="118"/>
<connect gate="G$6" pin="IO_LVDS38N" pad="149"/>
<connect gate="G$6" pin="IO_LVDS38P" pad="150"/>
<connect gate="G$6" pin="IO_LVDS39N" pad="146"/>
<connect gate="G$6" pin="IO_LVDS39P" pad="147"/>
<connect gate="G$6" pin="IO_LVDS42N" pad="143"/>
<connect gate="G$6" pin="IO_LVDS42P" pad="144"/>
<connect gate="G$6" pin="IO_LVDS44N" pad="141"/>
<connect gate="G$6" pin="IO_LVDS44P" pad="142"/>
<connect gate="G$6" pin="IO_LVDS45N" pad="138"/>
<connect gate="G$6" pin="IO_LVDS45P" pad="139"/>
<connect gate="G$6" pin="IO_LVDS46N" pad="135"/>
<connect gate="G$6" pin="IO_LVDS46P" pad="137"/>
<connect gate="G$6" pin="IO_LVDS47N" pad="133"/>
<connect gate="G$6" pin="IO_LVDS47P" pad="134"/>
<connect gate="G$6" pin="IO_LVDS48N" pad="127"/>
<connect gate="G$6" pin="IO_LVDS48P" pad="128"/>
<connect gate="G$6" pin="IO_LVDS51N" pad="115"/>
<connect gate="G$6" pin="IO_LVDS51P" pad="116"/>
<connect gate="G$6" pin="IO_LVDS52N" pad="113"/>
<connect gate="G$6" pin="IO_LVDS52P" pad="114"/>
<connect gate="G$6" pin="IO_LVDS53N" pad="110"/>
<connect gate="G$6" pin="IO_LVDS53P" pad="112"/>
<connect gate="G$6" pin="IO_LVDS56N" pad="105"/>
<connect gate="G$6" pin="IO_LVDS56P" pad="106"/>
<connect gate="G$6" pin="IO_PLL2_OUTN" pad="152"/>
<connect gate="G$6" pin="IO_PLL2_OUTP" pad="151"/>
<connect gate="G$6" pin="IO_VREFB3N0" pad="145"/>
<connect gate="G$6" pin="IO_VREFB3N1" pad="117"/>
<connect gate="G$6" pin="VCCIO3@1" pad="109"/>
<connect gate="G$6" pin="VCCIO3@2" pad="122"/>
<connect gate="G$6" pin="VCCIO3@3" pad="136"/>
<connect gate="G$6" pin="VCCIO3@4" pad="148"/>
<connect gate="G$7" pin="GND@1" pad="9"/>
<connect gate="G$7" pin="GND@10" pad="85"/>
<connect gate="G$7" pin="GND@11" pad="93"/>
<connect gate="G$7" pin="GND@12" pad="100"/>
<connect gate="G$7" pin="GND@13" pad="111"/>
<connect gate="G$7" pin="GND@14" pad="119"/>
<connect gate="G$7" pin="GND@15" pad="124"/>
<connect gate="G$7" pin="GND@16" pad="140"/>
<connect gate="G$7" pin="GND@17" pad="153"/>
<connect gate="G$7" pin="GND@18" pad="159"/>
<connect gate="G$7" pin="GND@19" pad="167"/>
<connect gate="G$7" pin="GND@2" pad="25"/>
<connect gate="G$7" pin="GND@20" pad="174"/>
<connect gate="G$7" pin="GND@21" pad="177"/>
<connect gate="G$7" pin="GND@22" pad="184"/>
<connect gate="G$7" pin="GND@23" pad="186"/>
<connect gate="G$7" pin="GND@24" pad="196"/>
<connect gate="G$7" pin="GND@25" pad="204"/>
<connect gate="G$7" pin="GND@3" pad="36"/>
<connect gate="G$7" pin="GND@4" pad="38"/>
<connect gate="G$7" pin="GND@5" pad="49"/>
<connect gate="G$7" pin="GND@6" pad="55"/>
<connect gate="G$7" pin="GND@7" pad="65"/>
<connect gate="G$7" pin="GND@8" pad="73"/>
<connect gate="G$7" pin="GND@9" pad="78"/>
<connect gate="G$7" pin="VCCINT@1" pad="32"/>
<connect gate="G$7" pin="VCCINT@2" pad="66"/>
<connect gate="G$7" pin="VCCINT@3" pad="79"/>
<connect gate="G$7" pin="VCCINT@4" pad="120"/>
<connect gate="G$7" pin="VCCINT@5" pad="178"/>
<connect gate="G$7" pin="VCCINT@6" pad="190"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RL" prefix="U">
<description>&lt;b&gt;USB UART&lt;/b&gt;
FT232RL 4&lt;sup&gt;th&lt;/sup&gt; Generation USB UART (USB &amp;lt;-&amp;gt; Serial) Controller. &lt;br&gt;
Spark Fun Electronics SKU : COM-00650&lt;br&gt;
Production SKU IC-00870</description>
<gates>
<gate name="G$1" symbol="FT232R"/>
</gates>
<devices>
<device name="SSOP" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DCD" pad="10"/>
<connect gate="G$1" pin="DSR" pad="9"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND18" pad="18"/>
<connect gate="G$1" pin="GND21" pad="21"/>
<connect gate="G$1" pin="GND7" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN" pad="14"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="22"/>
<connect gate="G$1" pin="SLEEP" pad="12"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXDEN" pad="13"/>
<connect gate="G$1" pin="TXLED" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-00870"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RL-BASIC" prefix="U">
<description>&lt;b&gt;USB UART&lt;/b&gt;
This is the simplified version of the FT232RL unit. Only what you need, nothing you don't. Spark Fun Electronics SKU : COM-00650</description>
<gates>
<gate name="G$1" symbol="FT232R-BASIC"/>
</gates>
<devices>
<device name="SSOP" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="22"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXLED" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RQ">
<description>USB to USART. Non-stock item, unproven FP for this part.</description>
<gates>
<gate name="G$1" symbol="FT232RQ"/>
</gates>
<devices>
<device name="" package="QFN-32">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="16"/>
<connect gate="G$1" pin="AGND" pad="24"/>
<connect gate="G$1" pin="CTS" pad="8"/>
<connect gate="G$1" pin="DCD" pad="7"/>
<connect gate="G$1" pin="DSR" pad="6"/>
<connect gate="G$1" pin="DTR" pad="31"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN" pad="11"/>
<connect gate="G$1" pin="RESET" pad="18"/>
<connect gate="G$1" pin="RI" pad="3"/>
<connect gate="G$1" pin="RTS" pad="32"/>
<connect gate="G$1" pin="RXD" pad="2"/>
<connect gate="G$1" pin="RXLED" pad="21"/>
<connect gate="G$1" pin="SLEEP" pad="9"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="30"/>
<connect gate="G$1" pin="TXDEN" pad="10"/>
<connect gate="G$1" pin="TXLED" pad="22"/>
<connect gate="G$1" pin="USBDM" pad="15"/>
<connect gate="G$1" pin="USBDP" pad="14"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VCCIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT245RL">
<description>&lt;b&gt;USB FIFO Controller&lt;/b&gt;
4&lt;sup&gt;th&lt;/sup&gt; Generation USB Controller (USB &amp;lt;-&amp;gt; Parallel) - FIFO. Spark Fun Electronics SKU : COM-00787</description>
<gates>
<gate name="G$1" symbol="FT245R"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="D0" pad="1"/>
<connect gate="G$1" pin="D1" pad="5"/>
<connect gate="G$1" pin="D2" pad="3"/>
<connect gate="G$1" pin="D3" pad="11"/>
<connect gate="G$1" pin="D4" pad="2"/>
<connect gate="G$1" pin="D5" pad="9"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="6"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWEN" pad="12"/>
<connect gate="G$1" pin="RD" pad="13"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RXF" pad="23"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXE" pad="22"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
<connect gate="G$1" pin="WR" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT2232D">
<description>USB to USART/FIFO/JTAG/SPI/I2C</description>
<gates>
<gate name="G$1" symbol="FT2232D"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="ACBUS0" pad="15"/>
<connect gate="G$1" pin="ACBUS1" pad="13"/>
<connect gate="G$1" pin="ACBUS2" pad="12"/>
<connect gate="G$1" pin="ACBUS3" pad="11"/>
<connect gate="G$1" pin="ADBUS0" pad="24"/>
<connect gate="G$1" pin="ADBUS1" pad="23"/>
<connect gate="G$1" pin="ADBUS2" pad="22"/>
<connect gate="G$1" pin="ADBUS3" pad="21"/>
<connect gate="G$1" pin="ADBUS4" pad="20"/>
<connect gate="G$1" pin="ADBUS5" pad="19"/>
<connect gate="G$1" pin="ADBUS6" pad="17"/>
<connect gate="G$1" pin="ADBUS7" pad="16"/>
<connect gate="G$1" pin="AGND" pad="45"/>
<connect gate="G$1" pin="AVCC" pad="46"/>
<connect gate="G$1" pin="BCBUS0" pad="30"/>
<connect gate="G$1" pin="BCBUS1" pad="29"/>
<connect gate="G$1" pin="BCBUS2" pad="28"/>
<connect gate="G$1" pin="BCBUS3" pad="27"/>
<connect gate="G$1" pin="BDBUS0" pad="40"/>
<connect gate="G$1" pin="BDBUS1" pad="39"/>
<connect gate="G$1" pin="BDBUS2" pad="38"/>
<connect gate="G$1" pin="BDBUS3" pad="37"/>
<connect gate="G$1" pin="BDBUS4" pad="36"/>
<connect gate="G$1" pin="BDBUS5" pad="35"/>
<connect gate="G$1" pin="BDBUS6" pad="33"/>
<connect gate="G$1" pin="BDBUS7" pad="32"/>
<connect gate="G$1" pin="EECS" pad="48"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="GND3" pad="34"/>
<connect gate="G$1" pin="GND4" pad="9"/>
<connect gate="G$1" pin="PWEN#" pad="41"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="SI/WUA" pad="10"/>
<connect gate="G$1" pin="SI/WUB" pad="26"/>
<connect gate="G$1" pin="TEST" pad="47"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="42"/>
<connect gate="G$1" pin="VCCIOA" pad="14"/>
<connect gate="G$1" pin="VCCIOB" pad="31"/>
<connect gate="G$1" pin="XTIN" pad="43"/>
<connect gate="G$1" pin="XTOUT" pad="44"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEF4543">
<description>BCD to 7-seg decoder/driver</description>
<gates>
<gate name="G$1" symbol="HEF4543"/>
</gates>
<devices>
<device name="PTH" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="9"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="BL" pad="7"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="D" pad="12"/>
<connect gate="G$1" pin="D0" pad="5"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="E" pad="13"/>
<connect gate="G$1" pin="F" pad="15"/>
<connect gate="G$1" pin="G" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LD" pad="1"/>
<connect gate="G$1" pin="PH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEX_CONVERTER" prefix="U">
<description>Just what it says.</description>
<gates>
<gate name="G$1" symbol="M74HC4050"/>
</gates>
<devices>
<device name="" package="SO016">
<connects>
<connect gate="G$1" pin="1A" pad="3"/>
<connect gate="G$1" pin="1Y" pad="2"/>
<connect gate="G$1" pin="2A" pad="5"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="3A" pad="7"/>
<connect gate="G$1" pin="3Y" pad="6"/>
<connect gate="G$1" pin="4A" pad="9"/>
<connect gate="G$1" pin="4Y" pad="10"/>
<connect gate="G$1" pin="5A" pad="11"/>
<connect gate="G$1" pin="5Y" pad="12"/>
<connect gate="G$1" pin="6A" pad="14"/>
<connect gate="G$1" pin="6Y" pad="15"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL3232">
<description>3V to RS-232 transceiver</description>
<gates>
<gate name="G$1" symbol="ICL3232"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INVERTER">
<description>Single inverter, SOT23-5</description>
<gates>
<gate name="G$1" symbol="INVERTER"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="&quot;&quot;" package="SC70">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INVERTING_SCHMITT_TRIGGER">
<description>FAIRCHILD Inverting Schmitt Trigger

UNTESTED FOOTPRINT!!
Used in External Clock Sources.
Digikey P/N NC7SZ14M5XCT-ND</description>
<gates>
<gate name="G$1" symbol="INVERTING_SCHMITT_TRIGGER"/>
</gates>
<devices>
<device name="" package="TSSOP5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISD1900" prefix="U">
<description>Voice recorder IC</description>
<gates>
<gate name="G$1" symbol="ISD1932"/>
</gates>
<devices>
<device name="ISD1932" package="SO-28W">
<connects>
<connect gate="G$1" pin="ADDR/_DRCT" pad="27"/>
<connect gate="G$1" pin="AGC" pad="17"/>
<connect gate="G$1" pin="E0/_M5" pad="7"/>
<connect gate="G$1" pin="E1/_M6" pad="9"/>
<connect gate="G$1" pin="E2/_M7" pad="10"/>
<connect gate="G$1" pin="E3/_M8" pad="11"/>
<connect gate="G$1" pin="MIC+" pad="18"/>
<connect gate="G$1" pin="MIC-" pad="19"/>
<connect gate="G$1" pin="ROSC" pad="20"/>
<connect gate="G$1" pin="S0/_M1" pad="2"/>
<connect gate="G$1" pin="S1/_M2" pad="3"/>
<connect gate="G$1" pin="S2/_M3" pad="4"/>
<connect gate="G$1" pin="S3/_M4" pad="5"/>
<connect gate="G$1" pin="SP+" pad="15"/>
<connect gate="G$1" pin="SP-" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="21"/>
<connect gate="G$1" pin="VCCD" pad="28"/>
<connect gate="G$1" pin="VCCP" pad="14"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="VSSD" pad="1"/>
<connect gate="G$1" pin="VSSP1" pad="16"/>
<connect gate="G$1" pin="VSSP2" pad="12"/>
<connect gate="G$1" pin="XCLK/FMC3" pad="25"/>
<connect gate="G$1" pin="_FT" pad="26"/>
<connect gate="G$1" pin="_LED" pad="22"/>
<connect gate="G$1" pin="_PLAYE/FMC2" pad="23"/>
<connect gate="G$1" pin="_PLAYL/FMC1" pad="6"/>
<connect gate="G$1" pin="_REC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC213X" prefix="IC">
<description>Schematic element and footprint for NXP LPC213x uC. Spark Fun Electronics SKU : COM-00520</description>
<gates>
<gate name="G$1" symbol="LPC213X"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="(AD0.0/CAP0.1/MAT0.1)P0.27" pad="11"/>
<connect gate="G$1" pin="(AD0.1/CAP0.2/MAT0.2)P0.28" pad="13"/>
<connect gate="G$1" pin="(AD0.2/CAP0.3/MAT0.3)P0.29" pad="14"/>
<connect gate="G$1" pin="(AD0.3/EINT3/CAP0.0)P0.30" pad="15"/>
<connect gate="G$1" pin="(AD0.4/AOUT)P0.25" pad="9"/>
<connect gate="G$1" pin="(AD0.5)P0.26" pad="10"/>
<connect gate="G$1" pin="(AD1.7/CAP0.0/MAT0.0)P0.22" pad="2"/>
<connect gate="G$1" pin="(CAP1.2/SCK1/MAT1.2)P0.17" pad="47"/>
<connect gate="G$1" pin="(CAP1.3/MISO1/MAT1.3)P0.18" pad="53"/>
<connect gate="G$1" pin="(CTS1/CAP1.1/SCL1)P0.11" pad="37"/>
<connect gate="G$1" pin="(DCD1/EINT1/SDA1)P0.14" pad="41"/>
<connect gate="G$1" pin="(DSR1/MAT1.0/AD1.3)P0.12" pad="38"/>
<connect gate="G$1" pin="(DTR1/MAT1.1/AD1.4)P0.13" pad="39"/>
<connect gate="G$1" pin="(EINT0/MAT0.2/CAP0.2)P0.16" pad="46"/>
<connect gate="G$1" pin="(MAT1.2/MOSI1/CAP1.2)P0.19" pad="54"/>
<connect gate="G$1" pin="(MAT1.3/SSEL1/EINT3)P0.20" pad="55"/>
<connect gate="G$1" pin="(MISO0/MAT0.1/A0.7)P0.5" pad="29"/>
<connect gate="G$1" pin="(MOSI0/CAP0.2/AD1.0)P0.6" pad="30"/>
<connect gate="G$1" pin="(PWM5/AD1.6/CAP1.3)P0.21" pad="1"/>
<connect gate="G$1" pin="(RI1/EINT2/AD1.5)P0.15" pad="45"/>
<connect gate="G$1" pin="(RTS1/CAP1.0/AD1.2)P0.10" pad="35"/>
<connect gate="G$1" pin="(RXD0/PWM3/EINT0)P0.1" pad="21"/>
<connect gate="G$1" pin="(RXD1/PWM6/EINT3)P0.9" pad="34"/>
<connect gate="G$1" pin="(SCK0/CAP0.1/AD0.6)P0.4" pad="27"/>
<connect gate="G$1" pin="(SCL0/CAP0.0)P0.2" pad="22"/>
<connect gate="G$1" pin="(SDA0/MAT0.0/EINT1)P0.3" pad="26"/>
<connect gate="G$1" pin="(SSEL0/PWM2/EINT2)P0.7" pad="31"/>
<connect gate="G$1" pin="(TXD0/PWM1)P0.0" pad="19"/>
<connect gate="G$1" pin="(TXD1/PWM4/A1.1)P0.8" pad="33"/>
<connect gate="G$1" pin="P0.23" pad="58"/>
<connect gate="G$1" pin="P0.31" pad="17"/>
<connect gate="G$1" pin="P1.16(TRACEPKT0)" pad="16"/>
<connect gate="G$1" pin="P1.17(TRACEPKT1)" pad="12"/>
<connect gate="G$1" pin="P1.18(TRACEPKT2)" pad="8"/>
<connect gate="G$1" pin="P1.19(TRACEPKT3)" pad="4"/>
<connect gate="G$1" pin="P1.20(TRACESYNC)" pad="48"/>
<connect gate="G$1" pin="P1.21(PIPESTAT0)" pad="44"/>
<connect gate="G$1" pin="P1.22(PIPESTAT1)" pad="40"/>
<connect gate="G$1" pin="P1.23(PIPESTAT2)" pad="36"/>
<connect gate="G$1" pin="P1.24(TRACECLK)" pad="32"/>
<connect gate="G$1" pin="P1.25(EXTIN0)" pad="28"/>
<connect gate="G$1" pin="P1.26(RTCK)" pad="24"/>
<connect gate="G$1" pin="P1.27(TDO)" pad="64"/>
<connect gate="G$1" pin="P1.28(TDI)" pad="60"/>
<connect gate="G$1" pin="P1.29(TCK)" pad="56"/>
<connect gate="G$1" pin="P1.30(TMS)" pad="52"/>
<connect gate="G$1" pin="P1.31(/TRST)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="57"/>
<connect gate="G$1" pin="RTXC1" pad="3"/>
<connect gate="G$1" pin="RTXC2" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="49"/>
<connect gate="G$1" pin="VDD3-1" pad="23"/>
<connect gate="G$1" pin="VDD3-2" pad="43"/>
<connect gate="G$1" pin="VDD3-3" pad="51"/>
<connect gate="G$1" pin="VDDA3" pad="7"/>
<connect gate="G$1" pin="VREF" pad="63"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="18"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="42"/>
<connect gate="G$1" pin="VSS@4" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="59"/>
<connect gate="G$1" pin="XTAL1" pad="62"/>
<connect gate="G$1" pin="XTAL2" pad="61"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2103">
<description>NXP LPC2103 ARM7 based MCU</description>
<gates>
<gate name="G$1" symbol="LPC2103"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="DBGSEL" pad="27"/>
<connect gate="G$1" pin="P0.0/TXD0/MAT3.1" pad="13"/>
<connect gate="G$1" pin="P0.1/RXD0/MAT3.2" pad="14"/>
<connect gate="G$1" pin="P0.10/RTS1/CAP1.0/AD0.3" pad="35"/>
<connect gate="G$1" pin="P0.11/CTS1/CAP1.1/AD0.4" pad="36"/>
<connect gate="G$1" pin="P0.12/DSR1/MAT1.0/AD0.5" pad="37"/>
<connect gate="G$1" pin="P0.13/DTR1/MAT1.1" pad="41"/>
<connect gate="G$1" pin="P0.14/DCD1/SCK1/EINT1" pad="44"/>
<connect gate="G$1" pin="P0.15/RI1/EINT2" pad="45"/>
<connect gate="G$1" pin="P0.16/EINT0/MAT0.2" pad="46"/>
<connect gate="G$1" pin="P0.17/CAP1.2/SCL1" pad="47"/>
<connect gate="G$1" pin="P0.18/CAP1.3/SDA1" pad="48"/>
<connect gate="G$1" pin="P0.19/MAT1.2/MISO1" pad="1"/>
<connect gate="G$1" pin="P0.2/SCL0/CAP0.0" pad="18"/>
<connect gate="G$1" pin="P0.20/MAT1.3/MOSI1" pad="2"/>
<connect gate="G$1" pin="P0.21/SSEL1/MAT3.0" pad="3"/>
<connect gate="G$1" pin="P0.22/AD0.0" pad="32"/>
<connect gate="G$1" pin="P0.23/AD0.1" pad="33"/>
<connect gate="G$1" pin="P0.24/AD0.2" pad="34"/>
<connect gate="G$1" pin="P0.25/AD0.6" pad="38"/>
<connect gate="G$1" pin="P0.26/AD0.7" pad="39"/>
<connect gate="G$1" pin="P0.27/TRST/CAP2.0" pad="8"/>
<connect gate="G$1" pin="P0.28/TMS/CAP2.1" pad="9"/>
<connect gate="G$1" pin="P0.29/TCK/CAP2.2" pad="10"/>
<connect gate="G$1" pin="P0.3/SDA0/MAT0.0" pad="21"/>
<connect gate="G$1" pin="P0.30/TDI/MAT3.3" pad="15"/>
<connect gate="G$1" pin="P0.31/TDO" pad="16"/>
<connect gate="G$1" pin="P0.4/SCK0/CAP0.1" pad="22"/>
<connect gate="G$1" pin="P0.5/MISO0/MAT0.1" pad="23"/>
<connect gate="G$1" pin="P0.6/MOSI0/CAP0.2" pad="24"/>
<connect gate="G$1" pin="P0.7/SSEL0/MAT2.0" pad="28"/>
<connect gate="G$1" pin="P0.8/TXD1/MAT2.1" pad="29"/>
<connect gate="G$1" pin="P0.9/RXD1/MAT2.2" pad="30"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="RTCK" pad="26"/>
<connect gate="G$1" pin="RTCX1" pad="20"/>
<connect gate="G$1" pin="RTCX2" pad="25"/>
<connect gate="G$1" pin="VBAT" pad="4"/>
<connect gate="G$1" pin="VDD(1V8)" pad="5"/>
<connect gate="G$1" pin="VDD(3V3)@17" pad="17"/>
<connect gate="G$1" pin="VDD(3V3)@40" pad="40"/>
<connect gate="G$1" pin="VDDA" pad="42"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
<connect gate="G$1" pin="VSS@43" pad="43"/>
<connect gate="G$1" pin="VSS@7" pad="7"/>
<connect gate="G$1" pin="VSSA" pad="31"/>
<connect gate="G$1" pin="XTAL1" pad="11"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74HC238">
<description>M74HC238 - CMOS 3 TO 8 LINE DECODER</description>
<gates>
<gate name="G$1" symbol="M74HC238"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="G1" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y0" pad="15"/>
<connect gate="G$1" pin="Y1" pad="14"/>
<connect gate="G$1" pin="Y2" pad="13"/>
<connect gate="G$1" pin="Y3" pad="12"/>
<connect gate="G$1" pin="Y4" pad="11"/>
<connect gate="G$1" pin="Y5" pad="10"/>
<connect gate="G$1" pin="Y6" pad="9"/>
<connect gate="G$1" pin="Y7" pad="7"/>
<connect gate="G$1" pin="~G2A" pad="4"/>
<connect gate="G$1" pin="~G2B" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M93C46">
<description>1kbit SPI EEPROM</description>
<gates>
<gate name="G$1" symbol="M93C46"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX232" prefix="U">
<description>&lt;b&gt;RS232 Transceiver&lt;/b&gt;
Very common IC. This is generically called 'MAX232', but works with the 3V equivalent MAX3232 generic ICs. Field tested and mother approved. Spark Fun Electronics SKU : COM-00316 (DIP) and COM-00589 (SMD)</description>
<gates>
<gate name="G$1" symbol="MAX232"/>
</gates>
<devices>
<device name="SOIC16" package="SO016">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TSSOP" package="TSSOP16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX485">
<description>RS-485 transceiver</description>
<gates>
<gate name="G$1" symbol="MAX485"/>
</gates>
<devices>
<device name="DIL" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RE" pad="2"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3421E" prefix="U">
<description>USB Peripheral/Host Controller w/ SPI</description>
<gates>
<gate name="G$1" symbol="MAX3421E-1"/>
</gates>
<devices>
<device name="SMD" package="TQFP32-5MM">
<connects>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="20"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GOUT0" pad="4"/>
<connect gate="G$1" pin="GOUT1" pad="5"/>
<connect gate="G$1" pin="GOUT2" pad="6"/>
<connect gate="G$1" pin="GOUT3" pad="7"/>
<connect gate="G$1" pin="GOUT4" pad="8"/>
<connect gate="G$1" pin="GOUT5" pad="9"/>
<connect gate="G$1" pin="GOUT6" pad="10"/>
<connect gate="G$1" pin="GOUT7" pad="11"/>
<connect gate="G$1" pin="GPIN0" pad="26"/>
<connect gate="G$1" pin="GPIN1" pad="27"/>
<connect gate="G$1" pin="GPIN2" pad="28"/>
<connect gate="G$1" pin="GPIN3" pad="29"/>
<connect gate="G$1" pin="GPIN4" pad="30"/>
<connect gate="G$1" pin="GPIN5" pad="31"/>
<connect gate="G$1" pin="GPIN6" pad="32"/>
<connect gate="G$1" pin="GPIN7" pad="1"/>
<connect gate="G$1" pin="GPX" pad="17"/>
<connect gate="G$1" pin="INT" pad="18"/>
<connect gate="G$1" pin="MISO" pad="15"/>
<connect gate="G$1" pin="MOSI" pad="16"/>
<connect gate="G$1" pin="RES" pad="12"/>
<connect gate="G$1" pin="SCK" pad="13"/>
<connect gate="G$1" pin="SS" pad="14"/>
<connect gate="G$1" pin="VBCOMP" pad="22"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VL" pad="2"/>
<connect gate="G$1" pin="X0" pad="25"/>
<connect gate="G$1" pin="X1" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7219">
<description>8-digit, 8-segment LED display driver, serial input</description>
<gates>
<gate name="G$1" symbol="MAX7219"/>
</gates>
<devices>
<device name="DIP" package="DIL24">
<connects>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="DIG0" pad="2"/>
<connect gate="G$1" pin="DIG1" pad="11"/>
<connect gate="G$1" pin="DIG2" pad="6"/>
<connect gate="G$1" pin="DIG3" pad="7"/>
<connect gate="G$1" pin="DIG4" pad="3"/>
<connect gate="G$1" pin="DIG5" pad="10"/>
<connect gate="G$1" pin="DIG6" pad="5"/>
<connect gate="G$1" pin="DIG7" pad="8"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="24"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND2" pad="9"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="LOAD" pad="12"/>
<connect gate="G$1" pin="SEGA" pad="14"/>
<connect gate="G$1" pin="SEGB" pad="16"/>
<connect gate="G$1" pin="SEGC" pad="20"/>
<connect gate="G$1" pin="SEGD" pad="23"/>
<connect gate="G$1" pin="SEGDP" pad="22"/>
<connect gate="G$1" pin="SEGE" pad="21"/>
<connect gate="G$1" pin="SEGF" pad="15"/>
<connect gate="G$1" pin="SEGG" pad="17"/>
<connect gate="G$1" pin="VCC" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7456">
<description>Monochrome NTSC/PAL on-screen display generator (SPI)</description>
<gates>
<gate name="G$1" symbol="MAX7456"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="CLKIN" pad="5"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DVDD" pad="3"/>
<connect gate="G$1" pin="LOS" pad="12"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="PVDD" pad="24"/>
<connect gate="G$1" pin="SAG" pad="25"/>
<connect gate="G$1" pin="SCK" pad="10"/>
<connect gate="G$1" pin="VIN" pad="22"/>
<connect gate="G$1" pin="VOUT" pad="26"/>
<connect gate="G$1" pin="XFB" pad="6"/>
<connect gate="G$1" pin="~CS" pad="8"/>
<connect gate="G$1" pin="~HSYNC" pad="18"/>
<connect gate="G$1" pin="~RESET" pad="19"/>
<connect gate="G$1" pin="~VSYNC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GROUNDPAD" package="TSSOP28-GROUNDPAD">
<connects>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="CLKIN" pad="5"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DVDD" pad="3"/>
<connect gate="G$1" pin="LOS" pad="12"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="PVDD" pad="24"/>
<connect gate="G$1" pin="SAG" pad="25"/>
<connect gate="G$1" pin="SCK" pad="10"/>
<connect gate="G$1" pin="VIN" pad="22"/>
<connect gate="G$1" pin="VOUT" pad="26"/>
<connect gate="G$1" pin="XFB" pad="6"/>
<connect gate="G$1" pin="~CS" pad="8"/>
<connect gate="G$1" pin="~HSYNC" pad="18"/>
<connect gate="G$1" pin="~RESET" pad="19"/>
<connect gate="G$1" pin="~VSYNC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S12XS64">
<description>Freescale 16-bit uC</description>
<gates>
<gate name="G$1" symbol="MC9S12XS64"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="ECLK/PE4" pad="21"/>
<connect gate="G$1" pin="EXTAL" pad="28"/>
<connect gate="G$1" pin="IOC0/PT0" pad="5"/>
<connect gate="G$1" pin="IOC1/PT1" pad="6"/>
<connect gate="G$1" pin="IOC1/PWM1/KWP1/PP1" pad="3"/>
<connect gate="G$1" pin="IOC2/PT2" pad="7"/>
<connect gate="G$1" pin="IOC3/PT3" pad="8"/>
<connect gate="G$1" pin="IRQ/PE1" pad="31"/>
<connect gate="G$1" pin="MODC/BKGD" pad="15"/>
<connect gate="G$1" pin="PA0" pad="33"/>
<connect gate="G$1" pin="PA1" pad="34"/>
<connect gate="G$1" pin="PA2" pad="35"/>
<connect gate="G$1" pin="PA3" pad="36"/>
<connect gate="G$1" pin="PAD00/AN00" pad="39"/>
<connect gate="G$1" pin="PAD01/AN01" pad="40"/>
<connect gate="G$1" pin="PAD02/AN02" pad="41"/>
<connect gate="G$1" pin="PAD03/AN03" pad="42"/>
<connect gate="G$1" pin="PAD04/AN04" pad="43"/>
<connect gate="G$1" pin="PAD05/AN05" pad="44"/>
<connect gate="G$1" pin="PAD06/AN06" pad="45"/>
<connect gate="G$1" pin="PAD07/AN07" pad="46"/>
<connect gate="G$1" pin="PB0" pad="16"/>
<connect gate="G$1" pin="PB5" pad="17"/>
<connect gate="G$1" pin="PB6" pad="18"/>
<connect gate="G$1" pin="PB7" pad="19"/>
<connect gate="G$1" pin="PM0/RXCAN0/RXD1" pad="60"/>
<connect gate="G$1" pin="PM1/TXCAN0/TXD1" pad="59"/>
<connect gate="G$1" pin="PM2/MISO0" pad="58"/>
<connect gate="G$1" pin="PM3/SS0" pad="57"/>
<connect gate="G$1" pin="PM4/MOSI0" pad="56"/>
<connect gate="G$1" pin="PM5/SCK0" pad="55"/>
<connect gate="G$1" pin="PP5/KPW5/PWM5" pad="64"/>
<connect gate="G$1" pin="PP7/KWP7/PWM7" pad="63"/>
<connect gate="G$1" pin="PS0/RXD0" pad="50"/>
<connect gate="G$1" pin="PS1/TXD0" pad="51"/>
<connect gate="G$1" pin="PS2/RXD1" pad="52"/>
<connect gate="G$1" pin="PS3/TXD1" pad="53"/>
<connect gate="G$1" pin="PWM3/KWP3/PP3" pad="1"/>
<connect gate="G$1" pin="PWM4/IOC4/PT4" pad="11"/>
<connect gate="G$1" pin="PWM6/IOC6/PT6" pad="13"/>
<connect gate="G$1" pin="PWM7/IOC7/PT7" pad="14"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="G$1" pin="RXD1/IOC0/PWM0/KWP0/PP0" pad="4"/>
<connect gate="G$1" pin="TEST" pad="54"/>
<connect gate="G$1" pin="TXD1/IOC2/PWM2/KWP2/PP2" pad="2"/>
<connect gate="G$1" pin="VDD" pad="37"/>
<connect gate="G$1" pin="VDDA" pad="47"/>
<connect gate="G$1" pin="VDDF" pad="9"/>
<connect gate="G$1" pin="VDDPLL" pad="30"/>
<connect gate="G$1" pin="VDDR" pad="25"/>
<connect gate="G$1" pin="VDDX1" pad="62"/>
<connect gate="G$1" pin="VDDX2" pad="23"/>
<connect gate="G$1" pin="VREG_API/PWM5/IOC5/PT" pad="12"/>
<connect gate="G$1" pin="VRH" pad="48"/>
<connect gate="G$1" pin="VSS1" pad="10"/>
<connect gate="G$1" pin="VSS2" pad="38"/>
<connect gate="G$1" pin="VSS3" pad="26"/>
<connect gate="G$1" pin="VSSA/VRL" pad="49"/>
<connect gate="G$1" pin="VSSPLL" pad="27"/>
<connect gate="G$1" pin="VSSX1" pad="61"/>
<connect gate="G$1" pin="VSSX2" pad="22"/>
<connect gate="G$1" pin="XCLKS/ECLKX2/PE7" pad="20"/>
<connect gate="G$1" pin="XIRQ/PE0" pad="32"/>
<connect gate="G$1" pin="XTAL" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP130" prefix="U">
<description>Open-drain microcontroller supervisor chip</description>
<gates>
<gate name="G$1" symbol="MCP130"/>
</gates>
<devices>
<device name="SOT" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP2551" prefix="U">
<description>CAN transceiver</description>
<gates>
<gate name="G$1" symbol="MCP2551"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAND256">
<description>NAND flash</description>
<gates>
<gate name="G$1" symbol="NAND256"/>
</gates>
<devices>
<device name="" package="TSOP48">
<connects>
<connect gate="G$1" pin="AL" pad="17"/>
<connect gate="G$1" pin="CL" pad="16"/>
<connect gate="G$1" pin="IO0" pad="29"/>
<connect gate="G$1" pin="IO1" pad="30"/>
<connect gate="G$1" pin="IO2" pad="31"/>
<connect gate="G$1" pin="IO3" pad="32"/>
<connect gate="G$1" pin="IO4" pad="41"/>
<connect gate="G$1" pin="IO5" pad="42"/>
<connect gate="G$1" pin="IO6" pad="43"/>
<connect gate="G$1" pin="IO7" pad="44"/>
<connect gate="G$1" pin="RXB" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="12"/>
<connect gate="G$1" pin="VDD2" pad="37"/>
<connect gate="G$1" pin="VSS1" pad="13"/>
<connect gate="G$1" pin="VSS2" pad="36"/>
<connect gate="G$1" pin="XE" pad="9"/>
<connect gate="G$1" pin="XR" pad="8"/>
<connect gate="G$1" pin="XW" pad="18"/>
<connect gate="G$1" pin="XWP" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7WZ07">
<description>Ultra-high speed dual open-drain output buffer (non-inverting)</description>
<gates>
<gate name="G$1" symbol="BUFFER-DUAL"/>
</gates>
<devices>
<device name="" package="SC70-6">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y1" pad="6"/>
<connect gate="G$1" pin="Y2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP303LSN09">
<description>Power-on uC reset controller</description>
<gates>
<gate name="G$1" symbol="NCP303LSN09"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CD" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9306">
<description>Bidirectional I2C level shifter.&lt;br&gt;
NOT compatible with all available part number pinout schemes- DOUBLE CHECK!!!</description>
<gates>
<gate name="G$1" symbol="PCA9306"/>
</gates>
<devices>
<device name="" package="PSOP-8">
<connects>
<connect gate="G$1" pin="EN" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL1" pad="2"/>
<connect gate="G$1" pin="SCL2" pad="6"/>
<connect gate="G$1" pin="SDA1" pad="3"/>
<connect gate="G$1" pin="SDA2" pad="5"/>
<connect gate="G$1" pin="VREF1" pad="1"/>
<connect gate="G$1" pin="VREF2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8575C">
<description>PCF8575C I/O Expander.</description>
<gates>
<gate name="G$1" symbol="PCF8575C"/>
</gates>
<devices>
<device name="" package="SO-24DW">
<connects>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INT" pad="1"/>
<connect gate="G$1" pin="P10" pad="13"/>
<connect gate="G$1" pin="P11" pad="14"/>
<connect gate="G$1" pin="P12" pad="15"/>
<connect gate="G$1" pin="P13" pad="16"/>
<connect gate="G$1" pin="P14" pad="17"/>
<connect gate="G$1" pin="P15" pad="18"/>
<connect gate="G$1" pin="P16" pad="19"/>
<connect gate="G$1" pin="P17" pad="20"/>
<connect gate="G$1" pin="PO0" pad="4"/>
<connect gate="G$1" pin="PO1" pad="5"/>
<connect gate="G$1" pin="PO2" pad="6"/>
<connect gate="G$1" pin="PO3" pad="7"/>
<connect gate="G$1" pin="PO4" pad="8"/>
<connect gate="G$1" pin="PO5" pad="9"/>
<connect gate="G$1" pin="PO6" pad="10"/>
<connect gate="G$1" pin="PO7" pad="11"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F88-DIP">
<description>8-bit PIC uC</description>
<gates>
<gate name="G$1" symbol="PIC16F88-DIP"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="17"/>
<connect gate="G$1" pin="RA1/AN1" pad="18"/>
<connect gate="G$1" pin="RA2/AN2" pad="1"/>
<connect gate="G$1" pin="RA3/AN3" pad="2"/>
<connect gate="G$1" pin="RA4/AN4" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2" pad="15"/>
<connect gate="G$1" pin="RA7/OSC1" pad="16"/>
<connect gate="G$1" pin="RB0/INT" pad="6"/>
<connect gate="G$1" pin="RB1/SDA" pad="7"/>
<connect gate="G$1" pin="RB2/RX" pad="8"/>
<connect gate="G$1" pin="RB3" pad="9"/>
<connect gate="G$1" pin="RB4/SCL" pad="10"/>
<connect gate="G$1" pin="RB5/TX" pad="11"/>
<connect gate="G$1" pin="RB6/PGC" pad="12"/>
<connect gate="G$1" pin="RB7/PGD" pad="13"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F88-SSOP" prefix="IC">
<description>&lt;b&gt;PIC 16F8x&lt;/b&gt;
8-Bit PIC16F8X Family

&lt;p&gt;Pin Compatible : PIC16F83, PIC16CR83, PIC16F84A, PIC16CR84</description>
<gates>
<gate name="G$1" symbol="PIC16F88-SSOP"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2" pad="1"/>
<connect gate="G$1" pin="RA3/AN3" pad="2"/>
<connect gate="G$1" pin="RA4/AN4" pad="3"/>
<connect gate="G$1" pin="RA5/MCLR" pad="4"/>
<connect gate="G$1" pin="RA6/OSC2" pad="17"/>
<connect gate="G$1" pin="RA7/OSC1" pad="18"/>
<connect gate="G$1" pin="RB0/INT" pad="7"/>
<connect gate="G$1" pin="RB1/SDA" pad="8"/>
<connect gate="G$1" pin="RB2/RX" pad="9"/>
<connect gate="G$1" pin="RB3" pad="10"/>
<connect gate="G$1" pin="RB4/SCL" pad="11"/>
<connect gate="G$1" pin="RB5/TX" pad="12"/>
<connect gate="G$1" pin="RB6/PGC" pad="13"/>
<connect gate="G$1" pin="RB7/PGD" pad="14"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VDD@1" pad="16"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F688">
<description>&lt;b&gt;PIC 16F688&lt;/b&gt;
8-Bit PIC16F88</description>
<gates>
<gate name="G$1" symbol="PIC16F688"/>
</gates>
<devices>
<device name="SMD" package="SOIC-14">
<connects>
<connect gate="G$1" pin="RA0/PGD" pad="13"/>
<connect gate="G$1" pin="RA1/PGC" pad="12"/>
<connect gate="G$1" pin="RA2/AN2" pad="11"/>
<connect gate="G$1" pin="RA3/MCLR" pad="4"/>
<connect gate="G$1" pin="RA4/OSC2" pad="3"/>
<connect gate="G$1" pin="RA5/OSC1" pad="2"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4/TX" pad="6"/>
<connect gate="G$1" pin="RC5/RX" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F883">
<gates>
<gate name="G$1" symbol="PIC16F883"/>
</gates>
<devices>
<device name="" package="SO-28W">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC4/SDI" pad="15"/>
<connect gate="G$1" pin="RC5/SDO" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F913">
<gates>
<gate name="G$1" symbol="PIC16F913"/>
</gates>
<devices>
<device name="SOIC28" package="SO-28W">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2" pad="10"/>
<connect gate="G$1" pin="RA7/OSC1" pad="9"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4/SD0" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RX/RC7/SDA" pad="18"/>
<connect gate="G$1" pin="TX/RC6/SCL" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2455">
<gates>
<gate name="G$1" symbol="PIC18F2550"/>
</gates>
<devices>
<device name="SMD" package="SO-28W">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/AN4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC4/D-" pad="15"/>
<connect gate="G$1" pin="RC5/D+" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="V-USB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2550">
<gates>
<gate name="G$1" symbol="PIC18F2550"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/AN4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC4/D-" pad="15"/>
<connect gate="G$1" pin="RC5/D+" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="V-USB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXXDAX06" prefix="U">
<description>&lt;b&gt;PIC24FXXXDAX06&lt;/b&gt;&lt;br&gt;
PIC24FXXXDA106 / PIC24FXXXDA206&lt;br&gt;
PIC24FJ256DA206-I/PT for IOIO&lt;br&gt;
IC-10386</description>
<gates>
<gate name="G$1" symbol="PIC24FJXXXDAX06"/>
</gates>
<devices>
<device name="" package="PIC24FXXX_TQFP64">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AN14/CTPLS/RP14/CN32/RB14" pad="29"/>
<connect gate="G$1" pin="AN15/RP29/REFO/CN12/RB15" pad="30"/>
<connect gate="G$1" pin="AN2/C2INB/VMIO/RP13/CN4/RB2" pad="14"/>
<connect gate="G$1" pin="AN3/C2INA/VPIO/CN5/RB3" pad="13"/>
<connect gate="G$1" pin="AN8/RP8/CN26/RB8" pad="21"/>
<connect gate="G$1" pin="AN9/RP9/CN27/RB9" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="C1INC/RP26/CN9/RG7" pad="5"/>
<connect gate="G$1" pin="C1IND/RP21/CN8/RG6" pad="4"/>
<connect gate="G$1" pin="C2INC/RP27/GD15/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="C2IND/RP19/GD14/CN10/RG8" pad="6"/>
<connect gate="G$1" pin="C3INA/SESSEND/CN16/RD7" pad="55"/>
<connect gate="G$1" pin="C3INB/CN15/RD6" pad="54"/>
<connect gate="G$1" pin="D+/CN83/RG2" pad="37"/>
<connect gate="G$1" pin="D-/CN84/RG3" pad="36"/>
<connect gate="G$1" pin="DMH/RP11/INT0/CN49/RD0" pad="46"/>
<connect gate="G$1" pin="DPH/RP23/CN51/RD2" pad="50"/>
<connect gate="G$1" pin="DPLN/SDA1/RP4/GD8/CN54/RD9" pad="43"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="GD0/CN58/RE0" pad="60"/>
<connect gate="G$1" pin="GD1/CN59/RE1" pad="61"/>
<connect gate="G$1" pin="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0" pad="58"/>
<connect gate="G$1" pin="GD11/VCMPST2/SESSVLD/CN69/RF1" pad="59"/>
<connect gate="G$1" pin="GD12/SCL3/CN64/RE6" pad="2"/>
<connect gate="G$1" pin="GD13/SDA3/CN65/RE7" pad="3"/>
<connect gate="G$1" pin="GD2/CN60/RE2" pad="62"/>
<connect gate="G$1" pin="GD3/CN61/RE3" pad="63"/>
<connect gate="G$1" pin="HSYNC/CN62/RE4" pad="64"/>
<connect gate="G$1" pin="OSCI/CLKI/CN23/RC12" pad="39"/>
<connect gate="G$1" pin="OSCO/CLKO/CN22/RC15" pad="40"/>
<connect gate="G$1" pin="PGEC1/AN1/VREF-/RP1/CN3/RB1" pad="15"/>
<connect gate="G$1" pin="PGEC2/AN6/RP6/CN24/RB6" pad="17"/>
<connect gate="G$1" pin="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5" pad="11"/>
<connect gate="G$1" pin="PGED1/AN0/VREF+/RP0/CN2/RB0" pad="16"/>
<connect gate="G$1" pin="PGED2/AN7/RP7/RCV/CN25/RB7" pad="18"/>
<connect gate="G$1" pin="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4" pad="12"/>
<connect gate="G$1" pin="RP12/GD7/CN56/RD11" pad="45"/>
<connect gate="G$1" pin="RP16/USBID/CN71/RF3" pad="33"/>
<connect gate="G$1" pin="RP20/GPWR/CN14/RD5" pad="53"/>
<connect gate="G$1" pin="RP22/GEN/CN52/RD3" pad="51"/>
<connect gate="G$1" pin="RP25/GCLK/CN13/RD4" pad="52"/>
<connect gate="G$1" pin="RTCC/DMLN/RP2/CN53/RD8" pad="42"/>
<connect gate="G$1" pin="SCL1/RP3/GD6/CN55/RD10" pad="44"/>
<connect gate="G$1" pin="SCL2/RP17/GD5/CN18/RF5" pad="32"/>
<connect gate="G$1" pin="SDA2/RP10/GD4/CN17/RF4" pad="31"/>
<connect gate="G$1" pin="SOSCI/C3IND/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="TCK/AN12/CTEDG2/CN30/RB12" pad="27"/>
<connect gate="G$1" pin="TDI/AN13/CTEDG1/CN31/RB13" pad="28"/>
<connect gate="G$1" pin="TDO/AN11/CN29/RB11" pad="24"/>
<connect gate="G$1" pin="TMS/CVREF/AN10/CN28/RB10" pad="23"/>
<connect gate="G$1" pin="VBUS/RF7" pad="34"/>
<connect gate="G$1" pin="VCAP" pad="56"/>
<connect gate="G$1" pin="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1" pad="49"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSYNC/CN63/RE5" pad="1"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10386"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ32GP202">
<gates>
<gate name="G$1" symbol="PIC24HJ32GP202"/>
</gates>
<devices>
<device name="DIP" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AN0/VREF+/CN2/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/VREF-/CN2/RA1" pad="3"/>
<connect gate="G$1" pin="AN10/RP14/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/RP13/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/RP12/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN4/RP2/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/RP3/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/RP15/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="28"/>
<connect gate="G$1" pin="AVSS" pad="27"/>
<connect gate="G$1" pin="INT0/RP7/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OSCI/CLKI/CN30/RA2" pad="9"/>
<connect gate="G$1" pin="OSCO/CLKO/CN29/RA3" pad="10"/>
<connect gate="G$1" pin="PGEC1/AN3/C2IN+/RP1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/TMS/RP11/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/RP6/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/AN2/C2IN-/RP0/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/TDI/RP10/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/RP5/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="SOSCI/RP4/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RA4" pad="12"/>
<connect gate="G$1" pin="TCK/SCL/RP8/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="TDO/SDA1/RP9/CN12/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SO-28W">
<connects>
<connect gate="G$1" pin="AN0/VREF+/CN2/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/VREF-/CN2/RA1" pad="3"/>
<connect gate="G$1" pin="AN10/RP14/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/RP13/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/RP12/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN4/RP2/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/RP3/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/RP15/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="28"/>
<connect gate="G$1" pin="AVSS" pad="27"/>
<connect gate="G$1" pin="INT0/RP7/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OSCI/CLKI/CN30/RA2" pad="9"/>
<connect gate="G$1" pin="OSCO/CLKO/CN29/RA3" pad="10"/>
<connect gate="G$1" pin="PGEC1/AN3/C2IN+/RP1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/TMS/RP11/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/RP6/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/AN2/C2IN-/RP0/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/TDI/RP10/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/RP5/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="SOSCI/RP4/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RA4" pad="12"/>
<connect gate="G$1" pin="TCK/SCL/RP8/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="TDO/SDA1/RP9/CN12/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX440F512H">
<gates>
<gate name="G$1" symbol="PIC32MX440F512H"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="D+/RG2" pad="37"/>
<connect gate="G$1" pin="D-/RG3" pad="36"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="RB0/AN0/PGED1/EMUD1/PMA6/VREF+/CVREF+/CN2" pad="16"/>
<connect gate="G$1" pin="RB1/AN1/PGEC1/VREF-/CVREF-/CN3" pad="15"/>
<connect gate="G$1" pin="RB10/AN10/TMS/CVREFOUT/PMA13" pad="23"/>
<connect gate="G$1" pin="RB11/AN11/TDO/PMA12" pad="24"/>
<connect gate="G$1" pin="RB12/AN12/TCK/PMA11" pad="27"/>
<connect gate="G$1" pin="RB13/AN13/TDI/PMA10" pad="28"/>
<connect gate="G$1" pin="RB14/AN14/PMALH/PMA1/~U2RTS/BCLK2" pad="29"/>
<connect gate="G$1" pin="RB15/AN15/PMALL/PMA0/OCFB/CN12" pad="30"/>
<connect gate="G$1" pin="RB2/AN2/C2IN-/CN4" pad="14"/>
<connect gate="G$1" pin="RB3/AN3/C2IN+/CN5" pad="13"/>
<connect gate="G$1" pin="RB4/AN4/C1IN-/CN6" pad="12"/>
<connect gate="G$1" pin="RB5/AN5/VBUSON/C1IN+/CN7" pad="11"/>
<connect gate="G$1" pin="RB6/AN6/PGEC2/OCFA" pad="17"/>
<connect gate="G$1" pin="RB7/AN7/PGED2" pad="18"/>
<connect gate="G$1" pin="RB8/AN8/~U2CTS/C1OUT" pad="21"/>
<connect gate="G$1" pin="RB9/AN9/PMA7/C2OUT" pad="22"/>
<connect gate="G$1" pin="RC12/OSC1/CLKI" pad="39"/>
<connect gate="G$1" pin="RC13/SOSCI/CN1" pad="47"/>
<connect gate="G$1" pin="RC14/SOSCO/T1CK/CN0" pad="48"/>
<connect gate="G$1" pin="RC15/OSC2/CLKO" pad="40"/>
<connect gate="G$1" pin="RD0/OC1/INT0" pad="46"/>
<connect gate="G$1" pin="RD1/OC2/~U1RTS/BCLK1" pad="49"/>
<connect gate="G$1" pin="RD10/IC3/PMCS2/PMA15/INT3/SCL1" pad="44"/>
<connect gate="G$1" pin="RD11/IC4/PMCS1/PMA14/INT4" pad="45"/>
<connect gate="G$1" pin="RD2/OC3/U1RX" pad="50"/>
<connect gate="G$1" pin="RD3/OC4/U1TX" pad="51"/>
<connect gate="G$1" pin="RD4/PMWR/OC5/IC5/CN13" pad="52"/>
<connect gate="G$1" pin="RD5/PMRD/CN14" pad="53"/>
<connect gate="G$1" pin="RD6/CN15" pad="54"/>
<connect gate="G$1" pin="RD7/CN16" pad="55"/>
<connect gate="G$1" pin="RD8/IC1/RTCC/INT1" pad="42"/>
<connect gate="G$1" pin="RD9/IC2/~U1CTS//INT2/SDA1" pad="43"/>
<connect gate="G$1" pin="RE0/PMD0" pad="60"/>
<connect gate="G$1" pin="RE1/PMD1" pad="61"/>
<connect gate="G$1" pin="RE2/PMD2" pad="62"/>
<connect gate="G$1" pin="RE3/PMD3" pad="63"/>
<connect gate="G$1" pin="RE4/PMD4" pad="64"/>
<connect gate="G$1" pin="RE5/PMD5" pad="1"/>
<connect gate="G$1" pin="RE6/PMD6" pad="2"/>
<connect gate="G$1" pin="RE7/PMD7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF3/USBID" pad="33"/>
<connect gate="G$1" pin="RF4/PMA9/U2RX/SDA2/CN17" pad="31"/>
<connect gate="G$1" pin="RF5/PMA8/U2TX/SCL2/CN18" pad="32"/>
<connect gate="G$1" pin="RG6/PMA5/SCK2/CN8" pad="4"/>
<connect gate="G$1" pin="RG7/PMA4/SDI2/CN9" pad="5"/>
<connect gate="G$1" pin="RG8/PMA3/SDO2/CN10" pad="6"/>
<connect gate="G$1" pin="RG9/PMA2/~SS2/CN11" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="56"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@26" pad="26"/>
<connect gate="G$1" pin="VDD@38" pad="38"/>
<connect gate="G$1" pin="VSS@25" pad="25"/>
<connect gate="G$1" pin="VSS@41" pad="41"/>
<connect gate="G$1" pin="VSS@9" pad="9"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
<connect gate="G$1" pin="~MCLR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PL-2303XA">
<description>Prolific USB chip, requires 12MHz xtal</description>
<gates>
<gate name="G$1" symbol="PL-2303XA"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="CTS_N" pad="11"/>
<connect gate="G$1" pin="DCD_N" pad="10"/>
<connect gate="G$1" pin="DM" pad="16"/>
<connect gate="G$1" pin="DP" pad="15"/>
<connect gate="G$1" pin="DSR_N" pad="9"/>
<connect gate="G$1" pin="DTR_N" pad="2"/>
<connect gate="G$1" pin="EE_CLK" pad="13"/>
<connect gate="G$1" pin="EE_DATA" pad="14"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND_A" pad="25"/>
<connect gate="G$1" pin="GP0" pad="22"/>
<connect gate="G$1" pin="GP1" pad="23"/>
<connect gate="G$1" pin="OSC1" pad="27"/>
<connect gate="G$1" pin="OSC2" pad="28"/>
<connect gate="G$1" pin="PLL_TEST" pad="26"/>
<connect gate="G$1" pin="RESET_N" pad="19"/>
<connect gate="G$1" pin="RI_N" pad="6"/>
<connect gate="G$1" pin="RTS_N" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="SHTD_N" pad="12"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VDD_325" pad="4"/>
<connect gate="G$1" pin="VDD_33" pad="8"/>
<connect gate="G$1" pin="VDD_33A" pad="24"/>
<connect gate="G$1" pin="VDD_5" pad="20"/>
<connect gate="G$1" pin="VO_33" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS485">
<description>RS485 transceiver</description>
<gates>
<gate name="G$1" symbol="RS485"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="/RE" pad="2"/>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS485_SP491">
<description>RS485 transceiver</description>
<gates>
<gate name="G$1" symbol="RS485_SP491"/>
</gates>
<devices>
<device name="" package="SOIC-14">
<connects>
<connect gate="G$1" pin="/RE" pad="3"/>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="D" pad="5"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="8"/>
<connect gate="G$1" pin="NC3" pad="13"/>
<connect gate="G$1" pin="R" pad="2"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SC16IS750" prefix="IC">
<description>SPI/I2C/IrDA to UART</description>
<gates>
<gate name="G$1" symbol="SC16IS750"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="/CTS" pad="22"/>
<connect gate="G$1" pin="/IRQ" pad="11"/>
<connect gate="G$1" pin="/RTS" pad="21"/>
<connect gate="G$1" pin="A0-/CS" pad="6"/>
<connect gate="G$1" pin="A1-SI" pad="7"/>
<connect gate="G$1" pin="GPIO0" pad="12"/>
<connect gate="G$1" pin="GPIO1" pad="13"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4-/DSR" pad="17"/>
<connect gate="G$1" pin="GPIO5-/DTR" pad="18"/>
<connect gate="G$1" pin="GPIO6-/CD" pad="19"/>
<connect gate="G$1" pin="GPIO7-/RI" pad="20"/>
<connect gate="G$1" pin="I2C-/SPI" pad="5"/>
<connect gate="G$1" pin="NC-SO" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="RX" pad="24"/>
<connect gate="G$1" pin="SCL-SCLK" pad="9"/>
<connect gate="G$1" pin="SDA-VSS" pad="10"/>
<connect gate="G$1" pin="TX" pad="23"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCANTOOL" prefix="U">
<description>&lt;h1&gt;STN1110 - Multiprotocol OBD II to UART Interpreter, QFN Package&lt;/h1&gt;

&lt;p&gt;
&lt;table&gt;
  &lt;tr&gt;&lt;td&gt;&lt;h2&gt;Change Log&lt;/h2&gt;&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;
    &lt;th&gt;Date&lt;/th&gt;&lt;th&gt;Author&lt;/th&gt;&lt;th&gt;Change&lt;/th&gt;
  &lt;tr&gt;
    &lt;td&gt;Aug 23, 2010&lt;/td&gt;&lt;td&gt;vit@scantool.net&lt;/td&gt;&lt;td&gt;Created device&lt;/td&gt;
  &lt;/tr&gt;
 &lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;

&lt;br /&gt;</description>
<gates>
<gate name="G$1" symbol="STN1110-QFN"/>
</gates>
<devices>
<device name="" package="_STN_SCANTOOL_QFN-28-S">
<connects>
<connect gate="G$1" pin="!ISO_K_TX" pad="22"/>
<connect gate="G$1" pin="!ISO_L_TX" pad="23"/>
<connect gate="G$1" pin="!ISO_RX" pad="8"/>
<connect gate="G$1" pin="!J1850_BUS-_TX" pad="4"/>
<connect gate="G$1" pin="!OBD_RX_LED!/!INT" pad="19"/>
<connect gate="G$1" pin="!OBD_TX_LED!/!RST_NVM" pad="18"/>
<connect gate="G$1" pin="!RESET" pad="26"/>
<connect gate="G$1" pin="!SLEEP" pad="9"/>
<connect gate="G$1" pin="!UART_RX_LED" pad="21"/>
<connect gate="G$1" pin="!UART_TX_LED" pad="20"/>
<connect gate="G$1" pin="!VPW_RX" pad="1"/>
<connect gate="G$1" pin="ANALOG_IN" pad="27"/>
<connect gate="G$1" pin="AVDD" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="24"/>
<connect gate="G$1" pin="CAN_RX" pad="11"/>
<connect gate="G$1" pin="CAN_TX" pad="12"/>
<connect gate="G$1" pin="J1850_BUS+_TX" pad="3"/>
<connect gate="G$1" pin="OSC1" pad="6"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="PAD" pad="EXP"/>
<connect gate="G$1" pin="PWM/!VPW" pad="28"/>
<connect gate="G$1" pin="PWM_RX" pad="2"/>
<connect gate="G$1" pin="PWR_CTRL" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCAP" pad="17"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VSS@16" pad="16"/>
<connect gate="G$1" pin="VSS@5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74HC251" prefix="U">
<description>SN54HC251 Data Selector/Multiplexer</description>
<gates>
<gate name="G$1" symbol="SN74HC251"/>
</gates>
<devices>
<device name="_SMD" package="SO016">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="9"/>
<connect gate="G$1" pin="D0" pad="4"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="1"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="12"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OE" pad="7"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="W" pad="6"/>
<connect gate="G$1" pin="Y" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC1G08">
<description>Single-gate AND logic</description>
<gates>
<gate name="G$1" symbol="SN74LVC1G08"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+V" pad="5"/>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPEAKJET" prefix="U">
<description>Speech synthesis chip- COM-09578</description>
<gates>
<gate name="G$1" symbol="SPEAKJET"/>
</gates>
<devices>
<device name="DIP" package="DIL18">
<connects>
<connect gate="G$1" pin="D0/RDY" pad="17"/>
<connect gate="G$1" pin="D1/SPK" pad="16"/>
<connect gate="G$1" pin="D2/BHF" pad="15"/>
<connect gate="G$1" pin="E0" pad="9"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="7"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="E4" pad="4"/>
<connect gate="G$1" pin="E5" pad="3"/>
<connect gate="G$1" pin="E6/RC0" pad="2"/>
<connect gate="G$1" pin="E7/RC1" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="M0" pad="13"/>
<connect gate="G$1" pin="M1" pad="12"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VOICE" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOIC-18">
<connects>
<connect gate="G$1" pin="D0/RDY" pad="17"/>
<connect gate="G$1" pin="D1/SPK" pad="16"/>
<connect gate="G$1" pin="D2/BHF" pad="15"/>
<connect gate="G$1" pin="E0" pad="9"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="7"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="E4" pad="4"/>
<connect gate="G$1" pin="E5" pad="3"/>
<connect gate="G$1" pin="E6/RC0" pad="2"/>
<connect gate="G$1" pin="E7/RC1" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="M0" pad="13"/>
<connect gate="G$1" pin="M1" pad="12"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VOICE" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPI_FLASH-X25XX">
<description>8pin SPI Flash series x25xx. Works with devices like W25X32 and BR25L32</description>
<gates>
<gate name="G$1" symbol="SPI_FLASH"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD1" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM811" prefix="U">
<description>&lt;h3&gt;STM811 Reset Circuit&lt;/h3&gt;
Used in the Ethernet Shield</description>
<gates>
<gate name="G$1" symbol="STM811"/>
</gates>
<devices>
<device name="" package="SOT143">
<connects>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="~MR" pad="3"/>
<connect gate="G$1" pin="~RST" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STP16CP05">
<description>16-pin constant current sink shift register LED driver</description>
<gates>
<gate name="G$1" symbol="STP16CP05/A6282"/>
</gates>
<devices>
<device name="" package="SO-24DW">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LE" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="15"/>
<connect gate="G$1" pin="OUT11" pad="16"/>
<connect gate="G$1" pin="OUT12" pad="17"/>
<connect gate="G$1" pin="OUT13" pad="18"/>
<connect gate="G$1" pin="OUT14" pad="19"/>
<connect gate="G$1" pin="OUT15" pad="20"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="13"/>
<connect gate="G$1" pin="OUT9" pad="14"/>
<connect gate="G$1" pin="REXT" pad="23"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="22"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="~OE" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STW5093">
<description>STW5093 - PCM Audio Codec</description>
<gates>
<gate name="G$1" symbol="STW5093"/>
</gates>
<devices>
<device name="" package="TSSOP30">
<connects>
<connect gate="G$1" pin="AUXCLK" pad="P$23"/>
<connect gate="G$1" pin="BZ" pad="P$19"/>
<connect gate="G$1" pin="CCLK" pad="P$20"/>
<connect gate="G$1" pin="CI" pad="P$22"/>
<connect gate="G$1" pin="CO" pad="P$25"/>
<connect gate="G$1" pin="CS-" pad="P$21"/>
<connect gate="G$1" pin="DR" pad="P$28"/>
<connect gate="G$1" pin="DX" pad="P$27"/>
<connect gate="G$1" pin="FS" pad="P$29"/>
<connect gate="G$1" pin="GND" pad="P$26"/>
<connect gate="G$1" pin="GNDA" pad="P$10"/>
<connect gate="G$1" pin="GNDP" pad="P$16"/>
<connect gate="G$1" pin="LO" pad="P$18"/>
<connect gate="G$1" pin="MBIAS" pad="P$6"/>
<connect gate="G$1" pin="MCLK" pad="P$30"/>
<connect gate="G$1" pin="MIC1+" pad="P$8"/>
<connect gate="G$1" pin="MIC1-" pad="P$9"/>
<connect gate="G$1" pin="MIC2+" pad="P$11"/>
<connect gate="G$1" pin="MIC2-" pad="P$12"/>
<connect gate="G$1" pin="MIC3+" pad="P$4"/>
<connect gate="G$1" pin="MIC3-" pad="P$5"/>
<connect gate="G$1" pin="REMIN" pad="P$3"/>
<connect gate="G$1" pin="REMOUT" pad="P$2"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
<connect gate="G$1" pin="VCCA" pad="P$7"/>
<connect gate="G$1" pin="VCCIO" pad="P$24"/>
<connect gate="G$1" pin="VCCP" pad="P$13"/>
<connect gate="G$1" pin="VFR" pad="P$17"/>
<connect gate="G$1" pin="VLR+" pad="P$15"/>
<connect gate="G$1" pin="VLR-" pad="P$14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC7SU04F">
<description>Single gate inverter</description>
<gates>
<gate name="G$1" symbol="TC7SU04F"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+V" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TJA1040">
<description>CAN Tranceiver</description>
<gates>
<gate name="G$1" symbol="TJA1040TD-T"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SPLIT" pad="5"/>
<connect gate="G$1" pin="STB" pad="8"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5940" prefix="U">
<description>16-channel LED Driver with Dot Correction and Grayscale PWM Control
&lt;hr&gt;
&lt;p&gt;The TLC5940 is a 16-channel, constant-current sink LED driver. Each channel has an individually adjustable 4096-step grayscale PWM brightness control and a 64-step, constant-current sink (dot correction). The dot correction adjusts the brightness variations between LED channels and other LED drivers. The dot correction data is stored in an integrated EEPROM. Both grayscale control and dot correction are accessible via a serial interface. A single external resistor sets the maximum current value of all 16 channels.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;28-pin HTSSOP
&lt;li&gt;32-pin 5x5mm QFN
&lt;li&gt;28-pin DIP&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TLC5940"/>
</gates>
<devices>
<device name="-NT" package="DIL28-3">
<connects>
<connect gate="G$1" pin="BLANK" pad="23"/>
<connect gate="G$1" pin="DCPRG" pad="19"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GSCLK" pad="18"/>
<connect gate="G$1" pin="IREF" pad="20"/>
<connect gate="G$1" pin="OUT0" pad="28"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT10" pad="10"/>
<connect gate="G$1" pin="OUT11" pad="11"/>
<connect gate="G$1" pin="OUT12" pad="12"/>
<connect gate="G$1" pin="OUT13" pad="13"/>
<connect gate="G$1" pin="OUT14" pad="14"/>
<connect gate="G$1" pin="OUT15" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="3"/>
<connect gate="G$1" pin="OUT4" pad="4"/>
<connect gate="G$1" pin="OUT5" pad="5"/>
<connect gate="G$1" pin="OUT6" pad="6"/>
<connect gate="G$1" pin="OUT7" pad="7"/>
<connect gate="G$1" pin="OUT8" pad="8"/>
<connect gate="G$1" pin="OUT9" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="25"/>
<connect gate="G$1" pin="SIN" pad="26"/>
<connect gate="G$1" pin="SOUT" pad="17"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VPRG" pad="27"/>
<connect gate="G$1" pin="XERR" pad="16"/>
<connect gate="G$1" pin="XLAT" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RHB" package="QFN-32">
<connects>
<connect gate="G$1" pin="BLANK" pad="31"/>
<connect gate="G$1" pin="DCPRG" pad="25"/>
<connect gate="G$1" pin="GND" pad="30"/>
<connect gate="G$1" pin="GSCLK" pad="24"/>
<connect gate="G$1" pin="IREF" pad="26"/>
<connect gate="G$1" pin="OUT0" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT10" pad="16"/>
<connect gate="G$1" pin="OUT11" pad="17"/>
<connect gate="G$1" pin="OUT12" pad="18"/>
<connect gate="G$1" pin="OUT13" pad="19"/>
<connect gate="G$1" pin="OUT14" pad="20"/>
<connect gate="G$1" pin="OUT15" pad="21"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="8"/>
<connect gate="G$1" pin="OUT5" pad="9"/>
<connect gate="G$1" pin="OUT6" pad="10"/>
<connect gate="G$1" pin="OUT7" pad="11"/>
<connect gate="G$1" pin="OUT8" pad="14"/>
<connect gate="G$1" pin="OUT9" pad="15"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="SIN" pad="2"/>
<connect gate="G$1" pin="SOUT" pad="23"/>
<connect gate="G$1" pin="VCC" pad="27"/>
<connect gate="G$1" pin="VPRG" pad="3"/>
<connect gate="G$1" pin="XERR" pad="22"/>
<connect gate="G$1" pin="XLAT" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PWP" package="TSSOP28-GROUNDPAD">
<connects>
<connect gate="G$1" pin="BLANK" pad="2"/>
<connect gate="G$1" pin="DCPRG" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GSCLK" pad="25"/>
<connect gate="G$1" pin="IREF" pad="27"/>
<connect gate="G$1" pin="OUT0" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="8"/>
<connect gate="G$1" pin="OUT10" pad="17"/>
<connect gate="G$1" pin="OUT11" pad="18"/>
<connect gate="G$1" pin="OUT12" pad="19"/>
<connect gate="G$1" pin="OUT13" pad="20"/>
<connect gate="G$1" pin="OUT14" pad="21"/>
<connect gate="G$1" pin="OUT15" pad="22"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="OUT3" pad="10"/>
<connect gate="G$1" pin="OUT4" pad="11"/>
<connect gate="G$1" pin="OUT5" pad="12"/>
<connect gate="G$1" pin="OUT6" pad="13"/>
<connect gate="G$1" pin="OUT7" pad="14"/>
<connect gate="G$1" pin="OUT8" pad="15"/>
<connect gate="G$1" pin="OUT9" pad="16"/>
<connect gate="G$1" pin="SCLK" pad="4"/>
<connect gate="G$1" pin="SIN" pad="5"/>
<connect gate="G$1" pin="SOUT" pad="24"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPRG" pad="6"/>
<connect gate="G$1" pin="XERR" pad="23"/>
<connect gate="G$1" pin="XLAT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UBW32_PIC32MX4XXL">
<gates>
<gate name="G$1" symbol="UBW32_PIC32MX4XXL"/>
</gates>
<devices>
<device name="TQFP100" package="UBW32_TQFP100">
<connects>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="C1IN-/AN4/CN6/RB4" pad="21"/>
<connect gate="G$1" pin="C1OUT/AN8/RB8" pad="32"/>
<connect gate="G$1" pin="C2IN+/AN3/CN5/RB3" pad="22"/>
<connect gate="G$1" pin="C2IN-/AN2/CN4/RB2" pad="23"/>
<connect gate="G$1" pin="C2OUT/AN9/RB9" pad="33"/>
<connect gate="G$1" pin="CN20/U1CTS/RD14" pad="47"/>
<connect gate="G$1" pin="CVREFOUT/PMA13/AN10/RB10" pad="34"/>
<connect gate="G$1" pin="D+/RG2" pad="57"/>
<connect gate="G$1" pin="D-/RG3" pad="56"/>
<connect gate="G$1" pin="ENVREG" pad="86"/>
<connect gate="G$1" pin="IC1/RTCC/RD8" pad="68"/>
<connect gate="G$1" pin="IC2/SS1/RD9" pad="69"/>
<connect gate="G$1" pin="IC3/SCKI/PMCS2/PMA15/RD10" pad="70"/>
<connect gate="G$1" pin="IC4/PMCS1/PMA14/RD11" pad="71"/>
<connect gate="G$1" pin="INT1/RE8" pad="18"/>
<connect gate="G$1" pin="INT2/RE9" pad="19"/>
<connect gate="G$1" pin="MCLR" pad="13"/>
<connect gate="G$1" pin="OC2/RD1" pad="76"/>
<connect gate="G$1" pin="OC3/RD2" pad="77"/>
<connect gate="G$1" pin="OC4/RD3" pad="78"/>
<connect gate="G$1" pin="OSC1/CLKI/RC12" pad="63"/>
<connect gate="G$1" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="G$1" pin="PGC1/EMUC1/AN1/CN3/RB1" pad="24"/>
<connect gate="G$1" pin="PGC2/EMUC2/AN6/OCFA/RB6" pad="26"/>
<connect gate="G$1" pin="PGD1/EMUD1/AN0/CN2/RB0" pad="25"/>
<connect gate="G$1" pin="PGD2/EMUD2/AN7/RB7" pad="27"/>
<connect gate="G$1" pin="PMA10/AN13/RB13" pad="42"/>
<connect gate="G$1" pin="PMA11/AN12/RB12" pad="41"/>
<connect gate="G$1" pin="PMA12/AN11/RB11" pad="35"/>
<connect gate="G$1" pin="PMA2/SS2/CN11/RG9" pad="14"/>
<connect gate="G$1" pin="PMA3/SDO2/CN10/RG8" pad="12"/>
<connect gate="G$1" pin="PMA4/SDI2/CN9/RG7" pad="11"/>
<connect gate="G$1" pin="PMA5/SCK2/CN8/RG6" pad="10"/>
<connect gate="G$1" pin="PMA6/VREF+/CVREF+/RA10" pad="29"/>
<connect gate="G$1" pin="PMA7/VREF-/CVREF-/RA9" pad="28"/>
<connect gate="G$1" pin="PMA8/U2TX/CN18/RF5" pad="50"/>
<connect gate="G$1" pin="PMA9/U2RX/CN17/RF4" pad="49"/>
<connect gate="G$1" pin="PMALH/PMA1/AN14/RB14" pad="43"/>
<connect gate="G$1" pin="PMALL/PMA0/AN15/OCFB/CN12/RB15" pad="44"/>
<connect gate="G$1" pin="PMD0/RE0" pad="93"/>
<connect gate="G$1" pin="PMD1/RE1" pad="94"/>
<connect gate="G$1" pin="PMD10/RF1" pad="88"/>
<connect gate="G$1" pin="PMD11/RF0" pad="87"/>
<connect gate="G$1" pin="PMD12/IC5/RD12" pad="79"/>
<connect gate="G$1" pin="PMD13/CN19/RD13" pad="80"/>
<connect gate="G$1" pin="PMD14/CN15/RD6" pad="83"/>
<connect gate="G$1" pin="PMD15/CN16/RD7" pad="84"/>
<connect gate="G$1" pin="PMD2/RE2" pad="98"/>
<connect gate="G$1" pin="PMD3/RE3" pad="99"/>
<connect gate="G$1" pin="PMD4/RE4" pad="100"/>
<connect gate="G$1" pin="PMD5/RE5" pad="3"/>
<connect gate="G$1" pin="PMD6/RE6" pad="4"/>
<connect gate="G$1" pin="PMD7/RE7" pad="5"/>
<connect gate="G$1" pin="PMD8/RG0" pad="90"/>
<connect gate="G$1" pin="PMD9/RG1" pad="89"/>
<connect gate="G$1" pin="PMRD/CN14/RD5" pad="82"/>
<connect gate="G$1" pin="PMWR/OC5/CN13/RD4" pad="81"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="SCL1/INT3/RA14" pad="66"/>
<connect gate="G$1" pin="SCL2/RA2" pad="58"/>
<connect gate="G$1" pin="SDA1/INT4/RA15" pad="67"/>
<connect gate="G$1" pin="SDA2/RA3" pad="59"/>
<connect gate="G$1" pin="SDI1/T5CK/RC4" pad="9"/>
<connect gate="G$1" pin="SDO1/OC1/INT0/RD0" pad="72"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="73"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="74"/>
<connect gate="G$1" pin="T2CK/RC1" pad="6"/>
<connect gate="G$1" pin="T3CK/RC2" pad="7"/>
<connect gate="G$1" pin="T4CK/RC3" pad="8"/>
<connect gate="G$1" pin="TCK/RA1" pad="38"/>
<connect gate="G$1" pin="TDI/RA4" pad="60"/>
<connect gate="G$1" pin="TDO/RA5" pad="61"/>
<connect gate="G$1" pin="TMS/RA0" pad="17"/>
<connect gate="G$1" pin="TRCLK/RA6" pad="91"/>
<connect gate="G$1" pin="TRD0/RG13" pad="97"/>
<connect gate="G$1" pin="TRD1/RG12" pad="96"/>
<connect gate="G$1" pin="TRD2/RG14" pad="95"/>
<connect gate="G$1" pin="TRD3/RA7" pad="92"/>
<connect gate="G$1" pin="U1RTS/BCLK1/CN21/RD15" pad="48"/>
<connect gate="G$1" pin="U1RX/RF2" pad="52"/>
<connect gate="G$1" pin="U1TX/RF8" pad="53"/>
<connect gate="G$1" pin="U2CTS/RF12" pad="40"/>
<connect gate="G$1" pin="U2RTS/BCLK2/RF13" pad="39"/>
<connect gate="G$1" pin="USBID/RF3" pad="51"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VBUSON/C1IN+/AN5/CN7/RB5" pad="20"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="85"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VDD3" pad="37"/>
<connect gate="G$1" pin="VDD4" pad="46"/>
<connect gate="G$1" pin="VDD5" pad="62"/>
<connect gate="G$1" pin="VSS1" pad="15"/>
<connect gate="G$1" pin="VSS2" pad="36"/>
<connect gate="G$1" pin="VSS3" pad="45"/>
<connect gate="G$1" pin="VSS4" pad="65"/>
<connect gate="G$1" pin="VSS6" pad="75"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UNBUFFERED_INVERTER">
<description>FAIRCHILD Unbuffered Inverter.
Used for external clock sources
Digikey P/N NC7SPU04P5XCT-ND</description>
<gates>
<gate name="G$1" symbol="INVERTER"/>
</gates>
<devices>
<device name="" package="SC70">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UM-FPU_V3_1" uservalue="yes">
<description>Micromega floating point coprocessor</description>
<gates>
<gate name="G$1" symbol="UM-FPU_V3_1"/>
</gates>
<devices>
<device name="DIL" package="DIL18">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="AN0" pad="2"/>
<connect gate="G$1" pin="AN1" pad="3"/>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="AVSS" pad="17"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="EXTIN" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="6"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="OUT0" pad="15"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="SCLK" pad="16"/>
<connect gate="G$1" pin="SERIN" pad="9"/>
<connect gate="G$1" pin="SEROUT" pad="8"/>
<connect gate="G$1" pin="SIN/SDA" pad="12"/>
<connect gate="G$1" pin="SOUT/SCL" pad="11"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SOIC18-W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="AN0" pad="2"/>
<connect gate="G$1" pin="AN1" pad="3"/>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="AVSS" pad="17"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="EXTIN" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="6"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="OUT0" pad="15"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="SCLK" pad="16"/>
<connect gate="G$1" pin="SERIN" pad="9"/>
<connect gate="G$1" pin="SEROUT" pad="8"/>
<connect gate="G$1" pin="SIN/SDA" pad="12"/>
<connect gate="G$1" pin="SOUT/SCL" pad="11"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3318">
<description>Hi-speed USB transceiver</description>
<gates>
<gate name="G$1" symbol="USB3318"/>
</gates>
<devices>
<device name="" package="QFN-24-USB">
<connects>
<connect gate="G$1" pin="CLKOUT" pad="12"/>
<connect gate="G$1" pin="CPEN" pad="7"/>
<connect gate="G$1" pin="DATA0" pad="16"/>
<connect gate="G$1" pin="DATA1" pad="15"/>
<connect gate="G$1" pin="DATA2" pad="14"/>
<connect gate="G$1" pin="DATA3" pad="13"/>
<connect gate="G$1" pin="DATA4" pad="11"/>
<connect gate="G$1" pin="DATA5" pad="10"/>
<connect gate="G$1" pin="DATA6" pad="9"/>
<connect gate="G$1" pin="DATA7" pad="8"/>
<connect gate="G$1" pin="DIR" pad="19"/>
<connect gate="G$1" pin="DM" pad="5"/>
<connect gate="G$1" pin="DP" pad="6"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="ID" pad="1"/>
<connect gate="G$1" pin="NXT" pad="18"/>
<connect gate="G$1" pin="RBIAS" pad="24"/>
<connect gate="G$1" pin="REFCLK" pad="23"/>
<connect gate="G$1" pin="RESETB" pad="22"/>
<connect gate="G$1" pin="STP" pad="20"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VBUS" pad="2"/>
<connect gate="G$1" pin="VDD18" pad="21"/>
<connect gate="G$1" pin="VDD33" pad="4"/>
<connect gate="G$1" pin="VDDIO" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1000">
<description>OGG Vorbis codec</description>
<gates>
<gate name="G$1" symbol="VS1000"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="38"/>
<connect gate="G$1" pin="AGND2" pad="41"/>
<connect gate="G$1" pin="AGND3" pad="42"/>
<connect gate="G$1" pin="AGND4" pad="48"/>
<connect gate="G$1" pin="AVDD1" pad="34"/>
<connect gate="G$1" pin="AVDD2" pad="39"/>
<connect gate="G$1" pin="AVDD3" pad="44"/>
<connect gate="G$1" pin="AVDD4" pad="46"/>
<connect gate="G$1" pin="CS1/GPIO0_10" pad="15"/>
<connect gate="G$1" pin="CS2/GPIO0_14" pad="21"/>
<connect gate="G$1" pin="CVDD" pad="32"/>
<connect gate="G$1" pin="DGND1" pad="6"/>
<connect gate="G$1" pin="DGND2" pad="18"/>
<connect gate="G$1" pin="DGND3" pad="31"/>
<connect gate="G$1" pin="GBUF" pad="43"/>
<connect gate="G$1" pin="IOVDD1" pad="30"/>
<connect gate="G$1" pin="IOVDD2" pad="19"/>
<connect gate="G$1" pin="IOVDD3" pad="7"/>
<connect gate="G$1" pin="LEFT" pad="47"/>
<connect gate="G$1" pin="NFALE/GPIO0_13" pad="17"/>
<connect gate="G$1" pin="NFCLE/GPIO0_12" pad="16"/>
<connect gate="G$1" pin="NFDIO0/IO0_0" pad="2"/>
<connect gate="G$1" pin="NFDIO1/IO0_1" pad="3"/>
<connect gate="G$1" pin="NFDIO2/IO0_2" pad="4"/>
<connect gate="G$1" pin="NFDIO3/IO0_3" pad="5"/>
<connect gate="G$1" pin="NFDIO4/IO0_4" pad="9"/>
<connect gate="G$1" pin="NFDIO5/IO0_5" pad="10"/>
<connect gate="G$1" pin="NFDIO6/IO0_6" pad="11"/>
<connect gate="G$1" pin="NFDIO7/IO0_7" pad="12"/>
<connect gate="G$1" pin="NFRD/GPIO0_9" pad="14"/>
<connect gate="G$1" pin="NFRDY/GPIO0_8" pad="13"/>
<connect gate="G$1" pin="NFWR/GPIO0_11" pad="20"/>
<connect gate="G$1" pin="POWBTN" pad="37"/>
<connect gate="G$1" pin="RCAP" pad="45"/>
<connect gate="G$1" pin="RIGHT" pad="40"/>
<connect gate="G$1" pin="RX/GPIO1_4" pad="27"/>
<connect gate="G$1" pin="SCLK/GPIO1_1" pad="23"/>
<connect gate="G$1" pin="SI/GPIO1_2" pad="24"/>
<connect gate="G$1" pin="SO/GPIO1_3" pad="25"/>
<connect gate="G$1" pin="TEST" pad="8"/>
<connect gate="G$1" pin="TX/GPIO1_5" pad="26"/>
<connect gate="G$1" pin="USBN" pad="36"/>
<connect gate="G$1" pin="USBP" pad="35"/>
<connect gate="G$1" pin="VHIGH" pad="33"/>
<connect gate="G$1" pin="XCS/GPIO1_0" pad="22"/>
<connect gate="G$1" pin="XRESET" pad="1"/>
<connect gate="G$1" pin="XTAL0" pad="29"/>
<connect gate="G$1" pin="XTAL1" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1002">
<description>MP3 deecoder</description>
<gates>
<gate name="G$1" symbol="VS1002"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DVDD1" pad="6"/>
<connect gate="G$1" pin="DVDD2" pad="14"/>
<connect gate="G$1" pin="DVDD3" pad="19"/>
<connect gate="G$1" pin="D_REQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="SPIBOOT/GPIO0" pad="33"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL0" pad="17"/>
<connect gate="G$1" pin="XTAL1" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1033" prefix="U">
<description>MP3 codec</description>
<gates>
<gate name="G$1" symbol="VS1033D"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="CVDD1" pad="5"/>
<connect gate="G$1" pin="CVDD2" pad="7"/>
<connect gate="G$1" pin="CVDD3" pad="24"/>
<connect gate="G$1" pin="CVDD4" pad="31"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DGND6" pad="35"/>
<connect gate="G$1" pin="DREQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO0/I2S_SCLK" pad="33"/>
<connect gate="G$1" pin="GPIO1/I2S_SDATA" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="GPIO4/I2S_LROUT" pad="36"/>
<connect gate="G$1" pin="GPIO5/I2C_MCLK" pad="25"/>
<connect gate="G$1" pin="GPIO6" pad="11"/>
<connect gate="G$1" pin="GPIO7" pad="12"/>
<connect gate="G$1" pin="IOVDD1" pad="6"/>
<connect gate="G$1" pin="IOVDD2" pad="14"/>
<connect gate="G$1" pin="IOVDD3" pad="19"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="LINEIN" pad="48"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="S0" pad="30"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="VCO" pad="15"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL1/MCLK" pad="18"/>
<connect gate="G$1" pin="XTAL2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1103">
<description>MIDI/ADPCM/WAV codec, MIDI synth</description>
<gates>
<gate name="G$1" symbol="VS1103"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="CVDD1" pad="5"/>
<connect gate="G$1" pin="CVDD2" pad="7"/>
<connect gate="G$1" pin="CVDD3" pad="24"/>
<connect gate="G$1" pin="CVDD4" pad="31"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DVDD1" pad="6"/>
<connect gate="G$1" pin="DVDD2" pad="14"/>
<connect gate="G$1" pin="DVDD3" pad="19"/>
<connect gate="G$1" pin="D_REQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="SPIBOOT/GPIO0" pad="33"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL0" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W5100" prefix="U" uservalue="yes">
<description>&lt;h3&gt;WIZnet W5100&lt;/h3&gt;
TCP/IP PHY Embedded Chip&lt;br&gt;
See SparkFun catalog # COM-09471&lt;br&gt;
&lt;br&gt;
Package: &lt;b&gt;LQFP-80&lt;/b&gt;,10x10mm,  0.4mm pitch</description>
<gates>
<gate name="G$1" symbol="W5100"/>
</gates>
<devices>
<device name="" package="LQFP-80">
<connects>
<connect gate="G$1" pin="*CS" pad="55"/>
<connect gate="G$1" pin="*INT" pad="56"/>
<connect gate="G$1" pin="*RD" pad="58"/>
<connect gate="G$1" pin="*RESET" pad="59"/>
<connect gate="G$1" pin="*SCS" pad="29"/>
<connect gate="G$1" pin="*WR" pad="57"/>
<connect gate="G$1" pin="1V8A@0" pad="7"/>
<connect gate="G$1" pin="1V8A@1" pad="74"/>
<connect gate="G$1" pin="1V8D@0" pad="15"/>
<connect gate="G$1" pin="1V8D@1" pad="16"/>
<connect gate="G$1" pin="1V8D@2" pad="33"/>
<connect gate="G$1" pin="1V8D@3" pad="69"/>
<connect gate="G$1" pin="1V8OUT" pad="11"/>
<connect gate="G$1" pin="3V3A" pad="2"/>
<connect gate="G$1" pin="3V3D@0" pad="12"/>
<connect gate="G$1" pin="3V3D@1" pad="18"/>
<connect gate="G$1" pin="3V3D@2" pad="44"/>
<connect gate="G$1" pin="ADDR0" pad="54"/>
<connect gate="G$1" pin="ADDR1" pad="53"/>
<connect gate="G$1" pin="ADDR10" pad="42"/>
<connect gate="G$1" pin="ADDR11" pad="41"/>
<connect gate="G$1" pin="ADDR12" pad="40"/>
<connect gate="G$1" pin="ADDR13" pad="39"/>
<connect gate="G$1" pin="ADDR14" pad="38"/>
<connect gate="G$1" pin="ADDR2" pad="52"/>
<connect gate="G$1" pin="ADDR3" pad="51"/>
<connect gate="G$1" pin="ADDR4" pad="50"/>
<connect gate="G$1" pin="ADDR5" pad="49"/>
<connect gate="G$1" pin="ADDR6" pad="48"/>
<connect gate="G$1" pin="ADDR7" pad="47"/>
<connect gate="G$1" pin="ADDR8" pad="46"/>
<connect gate="G$1" pin="ADDR9" pad="45"/>
<connect gate="G$1" pin="COLLED" pad="71"/>
<connect gate="G$1" pin="DATA0" pad="26"/>
<connect gate="G$1" pin="DATA1" pad="25"/>
<connect gate="G$1" pin="DATA2" pad="24"/>
<connect gate="G$1" pin="DATA3" pad="23"/>
<connect gate="G$1" pin="DATA4" pad="22"/>
<connect gate="G$1" pin="DATA5" pad="21"/>
<connect gate="G$1" pin="DATA6" pad="20"/>
<connect gate="G$1" pin="DATA7" pad="19"/>
<connect gate="G$1" pin="FDXLED" pad="70"/>
<connect gate="G$1" pin="GNDA@0" pad="4"/>
<connect gate="G$1" pin="GNDA@1" pad="10"/>
<connect gate="G$1" pin="GNDA@2" pad="77"/>
<connect gate="G$1" pin="GNDD@0" pad="13"/>
<connect gate="G$1" pin="GNDD@1" pad="14"/>
<connect gate="G$1" pin="GNDD@2" pad="17"/>
<connect gate="G$1" pin="GNDD@3" pad="32"/>
<connect gate="G$1" pin="GNDD@4" pad="43"/>
<connect gate="G$1" pin="GNDD@5" pad="68"/>
<connect gate="G$1" pin="LINKLED" pad="66"/>
<connect gate="G$1" pin="MISO" pad="27"/>
<connect gate="G$1" pin="MOSI" pad="28"/>
<connect gate="G$1" pin="NC@0" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="60"/>
<connect gate="G$1" pin="NC@2" pad="61"/>
<connect gate="G$1" pin="NC@3" pad="62"/>
<connect gate="G$1" pin="NC@4" pad="78"/>
<connect gate="G$1" pin="NC@5" pad="79"/>
<connect gate="G$1" pin="NC@6" pad="80"/>
<connect gate="G$1" pin="OPMODE0" pad="63"/>
<connect gate="G$1" pin="OPMODE1" pad="64"/>
<connect gate="G$1" pin="OPMODE2" pad="65"/>
<connect gate="G$1" pin="RSET_BG" pad="1"/>
<connect gate="G$1" pin="RXIN" pad="6"/>
<connect gate="G$1" pin="RXIP" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="72"/>
<connect gate="G$1" pin="SCLK" pad="30"/>
<connect gate="G$1" pin="SEN" pad="31"/>
<connect gate="G$1" pin="SPDLED" pad="67"/>
<connect gate="G$1" pin="TEST0" pad="37"/>
<connect gate="G$1" pin="TEST1" pad="36"/>
<connect gate="G$1" pin="TEST2" pad="35"/>
<connect gate="G$1" pin="TEST3" pad="34"/>
<connect gate="G$1" pin="TXLED" pad="73"/>
<connect gate="G$1" pin="TXON" pad="9"/>
<connect gate="G$1" pin="TXOP" pad="8"/>
<connect gate="G$1" pin="XTLN" pad="75"/>
<connect gate="G$1" pin="XTLP" pad="76"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2801" prefix="U">
<description>&lt;h3&gt;WS2801&lt;/h3&gt;
3 Channel Constant Current LED Driver with programmable PWM outputs.
&lt;br&gt;
&lt;br&gt;
Datasheet:  http://www.sparkfun.com/datasheets/Components/LED/WS2801.pdf</description>
<gates>
<gate name="G$1" symbol="WS2801"/>
</gates>
<devices>
<device name="" package="SOP-14">
<connects>
<connect gate="G$1" pin="BFB" pad="6"/>
<connect gate="G$1" pin="BOUT" pad="8"/>
<connect gate="G$1" pin="CKI" pad="1"/>
<connect gate="G$1" pin="CKO" pad="13"/>
<connect gate="G$1" pin="GFB" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GOUT" pad="9"/>
<connect gate="G$1" pin="POL" pad="3"/>
<connect gate="G$1" pin="RFB" pad="4"/>
<connect gate="G$1" pin="ROUT" pad="10"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XC3S250/500E-PQ208">
<description>Xilinx Spartan3E FPGA</description>
<gates>
<gate name="G$1" symbol="XC3S250/500E-PQ208"/>
</gates>
<devices>
<device name="" package="PQ208">
<connects>
<connect gate="G$1" pin="10_L08P_2/D7/GCLK12" pad="74"/>
<connect gate="G$1" pin="DONE" pad="104"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="GND@10" pad="95"/>
<connect gate="G$1" pin="GND@11" pad="105"/>
<connect gate="G$1" pin="GND@12" pad="121"/>
<connect gate="G$1" pin="GND@13" pad="131"/>
<connect gate="G$1" pin="GND@14" pad="141"/>
<connect gate="G$1" pin="GND@15" pad="156"/>
<connect gate="G$1" pin="GND@16" pad="173"/>
<connect gate="G$1" pin="GND@17" pad="182"/>
<connect gate="G$1" pin="GND@18" pad="188"/>
<connect gate="G$1" pin="GND@19" pad="198"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@20" pad="208"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="37"/>
<connect gate="G$1" pin="GND@5" pad="52"/>
<connect gate="G$1" pin="GND@6" pad="53"/>
<connect gate="G$1" pin="GND@7" pad="70"/>
<connect gate="G$1" pin="GND@8" pad="79"/>
<connect gate="G$1" pin="GND@9" pad="85"/>
<connect gate="G$1" pin="IO" pad="187"/>
<connect gate="G$1" pin="IO/D5" pad="76"/>
<connect gate="G$1" pin="IO/L01N_2/INIT_B" pad="56"/>
<connect gate="G$1" pin="IO/M1" pad="84"/>
<connect gate="G$1" pin="IO/VREF_0" pad="179"/>
<connect gate="G$1" pin="IO/VREF_2" pad="98"/>
<connect gate="G$1" pin="IO/VREF_3" pad="45"/>
<connect gate="G$1" pin="IO_16P_1/LDC1" pad="152"/>
<connect gate="G$1" pin="IO_L01N_0" pad="161"/>
<connect gate="G$1" pin="IO_L01N_1/A15" pad="107"/>
<connect gate="G$1" pin="IO_L01N_3" pad="3"/>
<connect gate="G$1" pin="IO_L01P_0" pad="160"/>
<connect gate="G$1" pin="IO_L01P_1/A16" pad="106"/>
<connect gate="G$1" pin="IO_L01P_2/CSO_B" pad="55"/>
<connect gate="G$1" pin="IO_L01P_3" pad="2"/>
<connect gate="G$1" pin="IO_L02N_0/VREF_0" pad="163"/>
<connect gate="G$1" pin="IO_L02N_1/A13" pad="109"/>
<connect gate="G$1" pin="IO_L02N_3/VREF_3" pad="5"/>
<connect gate="G$1" pin="IO_L02P_0" pad="162"/>
<connect gate="G$1" pin="IO_L02P_1/A14" pad="108"/>
<connect gate="G$1" pin="IO_L02P_3" pad="4"/>
<connect gate="G$1" pin="IO_L03N_0" pad="165"/>
<connect gate="G$1" pin="IO_L03N_1/VREF_1" pad="113"/>
<connect gate="G$1" pin="IO_L03N_2/MOSI/CSI_B" pad="61"/>
<connect gate="G$1" pin="IO_L03N_3" pad="9"/>
<connect gate="G$1" pin="IO_L03P_0" pad="164"/>
<connect gate="G$1" pin="IO_L03P_1" pad="112"/>
<connect gate="G$1" pin="IO_L03P_2/DOUT/BUSY" pad="60"/>
<connect gate="G$1" pin="IO_L03P_3" pad="8"/>
<connect gate="G$1" pin="IO_L04N_0/VREF_0" pad="168"/>
<connect gate="G$1" pin="IO_L04N_1" pad="116"/>
<connect gate="G$1" pin="IO_L04N_2" pad="63"/>
<connect gate="G$1" pin="IO_L04N_3" pad="12"/>
<connect gate="G$1" pin="IO_L04P_0" pad="167"/>
<connect gate="G$1" pin="IO_L04P_1" pad="115"/>
<connect gate="G$1" pin="IO_L04P_2" pad="62"/>
<connect gate="G$1" pin="IO_L04P_3" pad="11"/>
<connect gate="G$1" pin="IO_L05N_0" pad="172"/>
<connect gate="G$1" pin="IO_L05N_1/A11" pad="120"/>
<connect gate="G$1" pin="IO_L05N_2" pad="65"/>
<connect gate="G$1" pin="IO_L05N_3" pad="16"/>
<connect gate="G$1" pin="IO_L05P_0" pad="171"/>
<connect gate="G$1" pin="IO_L05P_1/A12" pad="119"/>
<connect gate="G$1" pin="IO_L05P_2" pad="64"/>
<connect gate="G$1" pin="IO_L05P_3" pad="15"/>
<connect gate="G$1" pin="IO_L06N_1/VREF_1" pad="123"/>
<connect gate="G$1" pin="IO_L06N_2" pad="69"/>
<connect gate="G$1" pin="IO_L06N_3" pad="19"/>
<connect gate="G$1" pin="IO_L06P_1" pad="122"/>
<connect gate="G$1" pin="IO_L06P_2" pad="68"/>
<connect gate="G$1" pin="IO_L06P_3" pad="18"/>
<connect gate="G$1" pin="IO_L07N_0/GCLK5" pad="178"/>
<connect gate="G$1" pin="IO_L07N_1/A7/RHCLK1" pad="127"/>
<connect gate="G$1" pin="IO_L07N_3/LHCLK1" pad="23"/>
<connect gate="G$1" pin="IO_L07P_1/A10/RHCLK0" pad="126"/>
<connect gate="G$1" pin="IO_L07P_3/LHCLK0" pad="22"/>
<connect gate="G$1" pin="IO_L08N_0/GCLK7" pad="181"/>
<connect gate="G$1" pin="IO_L08N_1/A7/RHCLK3" pad="129"/>
<connect gate="G$1" pin="IO_L08N_2/D6/GCLK13" pad="75"/>
<connect gate="G$1" pin="IO_L08N_3/LHCLK3" pad="25"/>
<connect gate="G$1" pin="IO_L08P_0/GCLK6" pad="180"/>
<connect gate="G$1" pin="IO_L08P_1/A8/RHCLK2" pad="128"/>
<connect gate="G$1" pin="IO_L08P_3/LHCLK2" pad="24"/>
<connect gate="G$1" pin="IO_L09N_1/A5/RHCLK5" pad="133"/>
<connect gate="G$1" pin="IO_L09N_2/D3/GCLK15" pad="78"/>
<connect gate="G$1" pin="IO_L09N_3/LHCLK5" pad="29"/>
<connect gate="G$1" pin="IO_L09P_1/A6/RHCLK4" pad="132"/>
<connect gate="G$1" pin="IO_L09P_2/D4/GCLK14" pad="77"/>
<connect gate="G$1" pin="IO_L09P_3/LHCLK4" pad="28"/>
<connect gate="G$1" pin="IO_L10N_0/GCLK11" pad="186"/>
<connect gate="G$1" pin="IO_L10N_1/A3/RHCLK7" pad="135"/>
<connect gate="G$1" pin="IO_L10N_3/LHCLK7" pad="31"/>
<connect gate="G$1" pin="IO_L10P_0/GCLK10" pad="185"/>
<connect gate="G$1" pin="IO_L10P_1/A4/RHCLK6" pad="134"/>
<connect gate="G$1" pin="IO_L10P_3/LHCLK6" pad="30"/>
<connect gate="G$1" pin="IO_L11N_0" pad="190"/>
<connect gate="G$1" pin="IO_L11N_1/A1" pad="138"/>
<connect gate="G$1" pin="IO_L11N_2/D1/GCLK3" pad="83"/>
<connect gate="G$1" pin="IO_L11N_3" pad="34"/>
<connect gate="G$1" pin="IO_L11P_0" pad="189"/>
<connect gate="G$1" pin="IO_L11P_1/A2" pad="137"/>
<connect gate="G$1" pin="IO_L11P_2/D2/GCLK2" pad="82"/>
<connect gate="G$1" pin="IO_L11P_3" pad="33"/>
<connect gate="G$1" pin="IO_L12N_0/VREF_0" pad="193"/>
<connect gate="G$1" pin="IO_L12N_1/A0" pad="140"/>
<connect gate="G$1" pin="IO_L12N_2/DIN/D0" pad="87"/>
<connect gate="G$1" pin="IO_L12N_3" pad="36"/>
<connect gate="G$1" pin="IO_L12P_0" pad="192"/>
<connect gate="G$1" pin="IO_L12P_1" pad="139"/>
<connect gate="G$1" pin="IO_L12P_2/M0" pad="86"/>
<connect gate="G$1" pin="IO_L12P_3" pad="35"/>
<connect gate="G$1" pin="IO_L13N_0" pad="197"/>
<connect gate="G$1" pin="IO_L13N_1" pad="145"/>
<connect gate="G$1" pin="IO_L13N_2" pad="90"/>
<connect gate="G$1" pin="IO_L13N_3" pad="40"/>
<connect gate="G$1" pin="IO_L13P_0" pad="196"/>
<connect gate="G$1" pin="IO_L13P_1" pad="144"/>
<connect gate="G$1" pin="IO_L13P_2" pad="89"/>
<connect gate="G$1" pin="IO_L13P_3" pad="39"/>
<connect gate="G$1" pin="IO_L14N_0/VREF_0" pad="200"/>
<connect gate="G$1" pin="IO_L14N_1" pad="147"/>
<connect gate="G$1" pin="IO_L14N_2/A22" pad="94"/>
<connect gate="G$1" pin="IO_L14N_3" pad="42"/>
<connect gate="G$1" pin="IO_L14P_0" pad="199"/>
<connect gate="G$1" pin="IO_L14P_1" pad="146"/>
<connect gate="G$1" pin="IO_L14P_2/A23" pad="93"/>
<connect gate="G$1" pin="IO_L14P_3" pad="41"/>
<connect gate="G$1" pin="IO_L15N_0" pad="203"/>
<connect gate="G$1" pin="IO_L15N_2/A20" pad="97"/>
<connect gate="G$1" pin="IO_L15N_3" pad="48"/>
<connect gate="G$1" pin="IO_L15P_0" pad="202"/>
<connect gate="G$1" pin="IO_L15P_1/HDC" pad="150"/>
<connect gate="G$1" pin="IO_L15P_2/A21" pad="96"/>
<connect gate="G$1" pin="IO_L15P_3" pad="47"/>
<connect gate="G$1" pin="IO_L15_1/LDC0" pad="151"/>
<connect gate="G$1" pin="IO_L16N_0/HSWAP" pad="206"/>
<connect gate="G$1" pin="IO_L16N_1/LDC2" pad="153"/>
<connect gate="G$1" pin="IO_L16N_2/VS1/A18" pad="100"/>
<connect gate="G$1" pin="IO_L16N_3" pad="50"/>
<connect gate="G$1" pin="IO_L16P_0" pad="205"/>
<connect gate="G$1" pin="IO_L16P_2/VS2/A19" pad="99"/>
<connect gate="G$1" pin="IO_L16P_3" pad="49"/>
<connect gate="G$1" pin="IO_L17N_2/CCLK" pad="103"/>
<connect gate="G$1" pin="IO_L17P_2/VS0/A17" pad="102"/>
<connect gate="G$1" pin="IO_LO7P_0/GCLK4" pad="177"/>
<connect gate="G$1" pin="IP" pad="159"/>
<connect gate="G$1" pin="IP/VREF_1" pad="136"/>
<connect gate="G$1" pin="IP/VREF_3" pad="20"/>
<connect gate="G$1" pin="IP@10" pad="148"/>
<connect gate="G$1" pin="IP@11" pad="154"/>
<connect gate="G$1" pin="IP@12" pad="54"/>
<connect gate="G$1" pin="IP@13" pad="91"/>
<connect gate="G$1" pin="IP@14" pad="101"/>
<connect gate="G$1" pin="IP@15" pad="6"/>
<connect gate="G$1" pin="IP@16" pad="14"/>
<connect gate="G$1" pin="IP@17" pad="26"/>
<connect gate="G$1" pin="IP@18" pad="32"/>
<connect gate="G$1" pin="IP@19" pad="43"/>
<connect gate="G$1" pin="IP@2" pad="169"/>
<connect gate="G$1" pin="IP@20" pad="51"/>
<connect gate="G$1" pin="IP@3" pad="194"/>
<connect gate="G$1" pin="IP@4" pad="204"/>
<connect gate="G$1" pin="IP@5" pad="110"/>
<connect gate="G$1" pin="IP@6" pad="118"/>
<connect gate="G$1" pin="IP@7" pad="124"/>
<connect gate="G$1" pin="IP@8" pad="130"/>
<connect gate="G$1" pin="IP@9" pad="142"/>
<connect gate="G$1" pin="IP_L02N_2" pad="58"/>
<connect gate="G$1" pin="IP_L02P_2" pad="57"/>
<connect gate="G$1" pin="IP_L06N_0" pad="175"/>
<connect gate="G$1" pin="IP_L06P_0" pad="174"/>
<connect gate="G$1" pin="IP_L07N_2/VREF_2" pad="72"/>
<connect gate="G$1" pin="IP_L07P_2" pad="71"/>
<connect gate="G$1" pin="IP_L09P_0/GCLK8" pad="183"/>
<connect gate="G$1" pin="IP_L10N_2/M2/GCLK1" pad="81"/>
<connect gate="G$1" pin="IP_L10P_2/RDWR_B/GCLK0" pad="80"/>
<connect gate="G$1" pin="IP_LO9N_0/GCLK9" pad="184"/>
<connect gate="G$1" pin="PROG_B" pad="1"/>
<connect gate="G$1" pin="TCK" pad="158"/>
<connect gate="G$1" pin="TDI" pad="207"/>
<connect gate="G$1" pin="TDO" pad="157"/>
<connect gate="G$1" pin="TMS" pad="155"/>
<connect gate="G$1" pin="VCC0_1" pad="114"/>
<connect gate="G$1" pin="VCC0_1@2" pad="125"/>
<connect gate="G$1" pin="VCC0_1@3" pad="143"/>
<connect gate="G$1" pin="VCCAUX" pad="7"/>
<connect gate="G$1" pin="VCCAUX@2" pad="44"/>
<connect gate="G$1" pin="VCCAUX@3" pad="66"/>
<connect gate="G$1" pin="VCCAUX@4" pad="92"/>
<connect gate="G$1" pin="VCCAUX@5" pad="111"/>
<connect gate="G$1" pin="VCCAUX@6" pad="149"/>
<connect gate="G$1" pin="VCCAUX@7" pad="166"/>
<connect gate="G$1" pin="VCCAUX@8" pad="195"/>
<connect gate="G$1" pin="VCCINT" pad="13"/>
<connect gate="G$1" pin="VCCINT@2" pad="67"/>
<connect gate="G$1" pin="VCCINT@3" pad="117"/>
<connect gate="G$1" pin="VCCINT@4" pad="170"/>
<connect gate="G$1" pin="VCCO_0" pad="176"/>
<connect gate="G$1" pin="VCCO_0@2" pad="191"/>
<connect gate="G$1" pin="VCCO_0@3" pad="201"/>
<connect gate="G$1" pin="VCCO_2" pad="59"/>
<connect gate="G$1" pin="VCCO_2@2" pad="73"/>
<connect gate="G$1" pin="VCCO_2@3" pad="88"/>
<connect gate="G$1" pin="VCCO_3" pad="21"/>
<connect gate="G$1" pin="VCCO_3@2" pad="38"/>
<connect gate="G$1" pin="VCCO_3@3" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA-100">
<description>Atmel XMega uC</description>
<gates>
<gate name="G$1" symbol="XMEGA"/>
</gates>
<devices>
<device name="SMD" package="TQFP-100-14X14MM">
<connects>
<connect gate="G$1" pin="AVCC@4" pad="4"/>
<connect gate="G$1" pin="AVCC@94" pad="94"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@33" pad="33"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="GND@63" pad="63"/>
<connect gate="G$1" pin="GND@73" pad="73"/>
<connect gate="G$1" pin="GND@84" pad="84"/>
<connect gate="G$1" pin="GND@93" pad="93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI/PDI_DATA" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="RESET/PDI_CLOCK" pad="90"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@24" pad="24"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="VCC@44" pad="44"/>
<connect gate="G$1" pin="VCC@54" pad="54"/>
<connect gate="G$1" pin="VCC@64" pad="64"/>
<connect gate="G$1" pin="VCC@74" pad="74"/>
<connect gate="G$1" pin="VCC@83" pad="83"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA-A3">
<description>Atmel's 8/16-bit AVR XMEGA A3 Microcontroller - ATxmega256A3, etc.</description>
<gates>
<gate name="G$1" symbol="XMEGA-A3B"/>
</gates>
<devices>
<device name="-AU" package="TQFP64_14X14MM">
<connects>
<connect gate="G$1" pin="/RESET_PDI_CLK" pad="57"/>
<connect gate="G$1" pin="AGND" pad="60"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND1" pad="14"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="GND3" pad="34"/>
<connect gate="G$1" pin="GND4" pad="44"/>
<connect gate="G$1" pin="GND5" pad="52"/>
<connect gate="G$1" pin="PA0(ADC0/AC0/AREF)" pad="62"/>
<connect gate="G$1" pin="PA1(ADC1/AC1)" pad="63"/>
<connect gate="G$1" pin="PA2(ADC2/AC2)" pad="64"/>
<connect gate="G$1" pin="PA3(ADC3/AC3)" pad="1"/>
<connect gate="G$1" pin="PA4(ADC4/AC4)" pad="2"/>
<connect gate="G$1" pin="PA5(ADC5/AC5)" pad="3"/>
<connect gate="G$1" pin="PA6(ADC6/AC6)" pad="4"/>
<connect gate="G$1" pin="PA7(ADC7/AC7/AC0OUT)" pad="5"/>
<connect gate="G$1" pin="PB0(ADC0/AC0/AREF)" pad="6"/>
<connect gate="G$1" pin="PB1(ADC1/AC1)" pad="7"/>
<connect gate="G$1" pin="PB2(ADC2/AC2/DAC0)" pad="8"/>
<connect gate="G$1" pin="PB3(ADC3/AC3/DAC1)" pad="9"/>
<connect gate="G$1" pin="PB4(ADC4/AC4/TMS)" pad="10"/>
<connect gate="G$1" pin="PB5(ADC5/AC5/TDI)" pad="11"/>
<connect gate="G$1" pin="PB6(ADC6/AC6/TCK)" pad="12"/>
<connect gate="G$1" pin="PB7(ADC7/AC7/AC0OUT/TDO)" pad="13"/>
<connect gate="G$1" pin="PC0(OC0A/OC0AL/SDA)" pad="16"/>
<connect gate="G$1" pin="PC1(OC0B/AC0AH/XCK0/SCL)" pad="17"/>
<connect gate="G$1" pin="PC2(OC0C/OC0BL/RXD0)" pad="18"/>
<connect gate="G$1" pin="PC3(OC0D/OX0BH/TXD0)" pad="19"/>
<connect gate="G$1" pin="PC4(AC1A/OC0CL/SS)" pad="20"/>
<connect gate="G$1" pin="PC5(OC1B/OC0CH/XCK1/MOSI)" pad="21"/>
<connect gate="G$1" pin="PC6(OC0DL/RXD1/MISO)" pad="22"/>
<connect gate="G$1" pin="PC7(OC0DH/CKOUT/EVO/TXD1/SCK)" pad="23"/>
<connect gate="G$1" pin="PD0(OC0A)" pad="26"/>
<connect gate="G$1" pin="PD1(OC0B/XCK0)" pad="27"/>
<connect gate="G$1" pin="PD2(OC0C/RXD0)" pad="28"/>
<connect gate="G$1" pin="PD3(OX0D/TXD0)" pad="29"/>
<connect gate="G$1" pin="PD4(OC1A/SS)" pad="30"/>
<connect gate="G$1" pin="PD5(OC1B/XCK1/MOSI)" pad="31"/>
<connect gate="G$1" pin="PD6(RXD1/MISO)" pad="32"/>
<connect gate="G$1" pin="PD7(CKOUT/EVO/TXD1/SCK)" pad="33"/>
<connect gate="G$1" pin="PDI_DATA" pad="56"/>
<connect gate="G$1" pin="PE0(OC0A/SDA)" pad="36"/>
<connect gate="G$1" pin="PE1(OC0B/XCK0/SCL)" pad="37"/>
<connect gate="G$1" pin="PE2(OC0C/RXD0)" pad="38"/>
<connect gate="G$1" pin="PE3(OC0D/TXD0)" pad="39"/>
<connect gate="G$1" pin="PE4(OC1A/SS)" pad="40"/>
<connect gate="G$1" pin="PE5(OC1B/XCK1/MOSI)" pad="41"/>
<connect gate="G$1" pin="PE6(TOSC2/RXD1/MISO)" pad="42"/>
<connect gate="G$1" pin="PE7(TOSC1/CKOUT/EVO/TXD1/SCK)" pad="43"/>
<connect gate="G$1" pin="PF0(OC0A)" pad="46"/>
<connect gate="G$1" pin="PF1(OC0B/XCK0)" pad="47"/>
<connect gate="G$1" pin="PF2(OC0C/RXD0)" pad="48"/>
<connect gate="G$1" pin="PF3(OC0D/TXD0)" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0(XTAL2)" pad="58"/>
<connect gate="G$1" pin="PR1(XTAL1)" pad="59"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VCC2" pad="25"/>
<connect gate="G$1" pin="VCC3" pad="35"/>
<connect gate="G$1" pin="VCC4" pad="45"/>
<connect gate="G$1" pin="VCC5" pad="53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XR2206" prefix="U">
<description>XR2206 Monolithic Function Generator</description>
<gates>
<gate name="G$1" symbol="XR2206"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="AMSI" pad="1"/>
<connect gate="G$1" pin="BIAS" pad="10"/>
<connect gate="G$1" pin="FSKI" pad="9"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="MO" pad="3"/>
<connect gate="G$1" pin="STO" pad="2"/>
<connect gate="G$1" pin="SYMA1" pad="15"/>
<connect gate="G$1" pin="SYMA2" pad="16"/>
<connect gate="G$1" pin="SYNCO" pad="11"/>
<connect gate="G$1" pin="TC1" pad="5"/>
<connect gate="G$1" pin="TC2" pad="6"/>
<connect gate="G$1" pin="TR1" pad="7"/>
<connect gate="G$1" pin="TR2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="WAVEA1" pad="13"/>
<connect gate="G$1" pin="WAVEA2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XS1_L1_64LQFP">
<description>XMos processor (multicore)</description>
<gates>
<gate name="G$1" symbol="XS1-L1-64LQFP"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64-XS1">
<connects>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="DEBUG" pad="17"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MODE0" pad="22"/>
<connect gate="G$1" pin="MODE1" pad="23"/>
<connect gate="G$1" pin="MODE2" pad="24"/>
<connect gate="G$1" pin="MODE3" pad="25"/>
<connect gate="G$1" pin="PLL_AGND" pad="19"/>
<connect gate="G$1" pin="PLL_AVDD" pad="20"/>
<connect gate="G$1" pin="RST_N" pad="8"/>
<connect gate="G$1" pin="TCK" pad="29"/>
<connect gate="G$1" pin="TDI" pad="30"/>
<connect gate="G$1" pin="TDO" pad="31"/>
<connect gate="G$1" pin="TMS" pad="27"/>
<connect gate="G$1" pin="TRST_N" pad="26"/>
<connect gate="G$1" pin="VDDIO_18" pad="18"/>
<connect gate="G$1" pin="VDDIO_32" pad="32"/>
<connect gate="G$1" pin="VDDIO_40" pad="40"/>
<connect gate="G$1" pin="VDDIO_53" pad="53"/>
<connect gate="G$1" pin="VDDIO_6" pad="6"/>
<connect gate="G$1" pin="VDDIO_60" pad="60"/>
<connect gate="G$1" pin="VDD_13" pad="13"/>
<connect gate="G$1" pin="VDD_21" pad="21"/>
<connect gate="G$1" pin="VDD_28" pad="28"/>
<connect gate="G$1" pin="VDD_37" pad="37"/>
<connect gate="G$1" pin="VDD_4" pad="4"/>
<connect gate="G$1" pin="VDD_43" pad="43"/>
<connect gate="G$1" pin="VDD_52" pad="52"/>
<connect gate="G$1" pin="VDD_61" pad="61"/>
<connect gate="G$1" pin="X0D0" pad="16"/>
<connect gate="G$1" pin="X0D1" pad="15"/>
<connect gate="G$1" pin="X0D10" pad="1"/>
<connect gate="G$1" pin="X0D11" pad="64"/>
<connect gate="G$1" pin="X0D12" pad="63"/>
<connect gate="G$1" pin="X0D13" pad="62"/>
<connect gate="G$1" pin="X0D14" pad="59"/>
<connect gate="G$1" pin="X0D15" pad="58"/>
<connect gate="G$1" pin="X0D16" pad="57"/>
<connect gate="G$1" pin="X0D17" pad="56"/>
<connect gate="G$1" pin="X0D18" pad="55"/>
<connect gate="G$1" pin="X0D19" pad="54"/>
<connect gate="G$1" pin="X0D2" pad="14"/>
<connect gate="G$1" pin="X0D20" pad="51"/>
<connect gate="G$1" pin="X0D21" pad="50"/>
<connect gate="G$1" pin="X0D22" pad="49"/>
<connect gate="G$1" pin="X0D23" pad="48"/>
<connect gate="G$1" pin="X0D24" pad="47"/>
<connect gate="G$1" pin="X0D25" pad="46"/>
<connect gate="G$1" pin="X0D26" pad="45"/>
<connect gate="G$1" pin="X0D27" pad="44"/>
<connect gate="G$1" pin="X0D3" pad="12"/>
<connect gate="G$1" pin="X0D32" pad="36"/>
<connect gate="G$1" pin="X0D33" pad="35"/>
<connect gate="G$1" pin="X0D34" pad="34"/>
<connect gate="G$1" pin="X0D35" pad="33"/>
<connect gate="G$1" pin="X0D36" pad="42"/>
<connect gate="G$1" pin="X0D37" pad="41"/>
<connect gate="G$1" pin="X0D38" pad="39"/>
<connect gate="G$1" pin="X0D39" pad="38"/>
<connect gate="G$1" pin="X0D4" pad="11"/>
<connect gate="G$1" pin="X0D5" pad="10"/>
<connect gate="G$1" pin="X0D6" pad="7"/>
<connect gate="G$1" pin="X0D7" pad="5"/>
<connect gate="G$1" pin="X0D8" pad="3"/>
<connect gate="G$1" pin="X0D9" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*08" prefix="U">
<description>Single 2-input AND gate</description>
<gates>
<gate name="G$1" symbol="74AHC1G08"/>
</gates>
<devices>
<device name="SE" package="SOT353">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*32" prefix="U">
<description>Single 2-input OR gate</description>
<gates>
<gate name="G$1" symbol="OR-SINGLE"/>
</gates>
<devices>
<device name="SE" package="SOT353">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*157" prefix="IC">
<description>Quadruple 2-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74157"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="SO" package="SO016">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*595" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch</description>
<gates>
<gate name="A" symbol="74595"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="3"/>
<connect gate="A" pin="QD" pad="4"/>
<connect gate="A" pin="QE" pad="5"/>
<connect gate="A" pin="QF" pad="7"/>
<connect gate="A" pin="QG" pad="8"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="QH*" pad="12"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCK" pad="14"/>
<connect gate="A" pin="SCL" pad="13"/>
<connect gate="A" pin="SER" pad="18"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="" package="TSSOP16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74ACT125D">
<description>Quad Buffer with 3-State Outputs-
ON Semi Conductor:

Digikey P/N MC74ACT125DR2GOSTR-ND</description>
<gates>
<gate name="G$1" symbol="74ACT125D"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="B0" pad="2"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="O0" pad="3"/>
<connect gate="G$1" pin="O1" pad="6"/>
<connect gate="G$1" pin="O2" pad="11"/>
<connect gate="G$1" pin="O3" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AHC1G08">
<description>Single 2-input AND gate</description>
<gates>
<gate name="G$1" symbol="74AHC1G08"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC04_HEX_INVERTER" prefix="U">
<description>74HC04 Hex Inverter</description>
<gates>
<gate name="G$1" symbol="74HC04_HEX_INVERTER"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1Y" pad="2"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="3A" pad="5"/>
<connect gate="G$1" pin="3Y" pad="6"/>
<connect gate="G$1" pin="4A" pad="9"/>
<connect gate="G$1" pin="4Y" pad="8"/>
<connect gate="G$1" pin="5A" pad="11"/>
<connect gate="G$1" pin="5Y" pad="10"/>
<connect gate="G$1" pin="6A" pad="13"/>
<connect gate="G$1" pin="6Y" pad="12"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC138AD">
<description>3-to-8 decoder</description>
<gates>
<gate name="G$1" symbol="74LVC138AD"/>
</gates>
<devices>
<device name="" package="SO016">
<connects>
<connect gate="G$1" pin="/E1" pad="4"/>
<connect gate="G$1" pin="/E2" pad="5"/>
<connect gate="G$1" pin="/Y0" pad="15"/>
<connect gate="G$1" pin="/Y1" pad="14"/>
<connect gate="G$1" pin="/Y2" pad="13"/>
<connect gate="G$1" pin="/Y3" pad="12"/>
<connect gate="G$1" pin="/Y4" pad="11"/>
<connect gate="G$1" pin="/Y5" pad="10"/>
<connect gate="G$1" pin="/Y6" pad="9"/>
<connect gate="G$1" pin="/Y7" pad="7"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A6282" prefix="U">
<description>16-Channel Constant-Current LED Driver&lt;br&gt;
Packages: TSSOP-24, 24-pin QFN&lt;br&gt;
&lt;br&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;B&gt;Unproven!&lt;/b&gt;&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="A6282"/>
</gates>
<devices>
<device name="-LP" package="TSSOP-24">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="EP"/>
<connect gate="G$1" pin="LE" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="15"/>
<connect gate="G$1" pin="OUT11" pad="16"/>
<connect gate="G$1" pin="OUT12" pad="17"/>
<connect gate="G$1" pin="OUT13" pad="18"/>
<connect gate="G$1" pin="OUT14" pad="19"/>
<connect gate="G$1" pin="OUT15" pad="20"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="13"/>
<connect gate="G$1" pin="OUT9" pad="14"/>
<connect gate="G$1" pin="REXT" pad="23"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="22"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="~OE" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ES" package="QFN-24_ALT2">
<connects>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="EP"/>
<connect gate="G$1" pin="LE" pad="7"/>
<connect gate="G$1" pin="OUT0" pad="8"/>
<connect gate="G$1" pin="OUT1" pad="9"/>
<connect gate="G$1" pin="OUT10" pad="18"/>
<connect gate="G$1" pin="OUT11" pad="19"/>
<connect gate="G$1" pin="OUT12" pad="20"/>
<connect gate="G$1" pin="OUT13" pad="21"/>
<connect gate="G$1" pin="OUT14" pad="22"/>
<connect gate="G$1" pin="OUT15" pad="23"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="OUT5" pad="13"/>
<connect gate="G$1" pin="OUT6" pad="14"/>
<connect gate="G$1" pin="OUT7" pad="15"/>
<connect gate="G$1" pin="OUT8" pad="16"/>
<connect gate="G$1" pin="OUT9" pad="17"/>
<connect gate="G$1" pin="REXT" pad="2"/>
<connect gate="G$1" pin="SDI" pad="5"/>
<connect gate="G$1" pin="SDO" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="~OE" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WTV020SD" prefix="IC" uservalue="yes">
<description>SD audio playback IC&lt;br&gt;
Can play back .wav or .ad4 files from an SD card&lt;br&gt;
SPI control or digital input trigger control&lt;br&gt;
available in SSOP-20 or DIP-20</description>
<gates>
<gate name="G$1" symbol="WTV020SD-20S"/>
</gates>
<devices>
<device name="" package="SSOP_20">
<connects>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="OSCI/P10" pad="15"/>
<connect gate="G$1" pin="OSCO/P11" pad="16"/>
<connect gate="G$1" pin="P00" pad="18"/>
<connect gate="G$1" pin="P01" pad="19"/>
<connect gate="G$1" pin="P02" pad="20"/>
<connect gate="G$1" pin="P03" pad="1"/>
<connect gate="G$1" pin="P04" pad="2"/>
<connect gate="G$1" pin="P05" pad="3"/>
<connect gate="G$1" pin="P06" pad="4"/>
<connect gate="G$1" pin="P07" pad="5"/>
<connect gate="G$1" pin="PAD_EQI" pad="11"/>
<connect gate="G$1" pin="PAD_EQO" pad="10"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="SPK_N" pad="8"/>
<connect gate="G$1" pin="SPK_P" pad="7"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VPP" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_#" value="NA"/>
<attribute name="SKU" value="NA"/>
<attribute name="SPARKLE_ID" value="6000"/>
<attribute name="VALUE" value="WTV020SD-20S"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328P_PDIP" prefix="U">
<description>uC used in the Arduino&lt;br&gt;
32kb flash, 1k EEPROM, 2k SRAM&lt;br&gt;
This is the through-hole version of this chip.</description>
<gates>
<gate name="G$1" symbol="ATMEGAXX8-28PIN"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328P_PDIP_EZ" prefix="U">
<description>uC used in the Arduino&lt;br&gt;
32kb flash, 1k EEPROM, 2k SRAM&lt;br&gt;
This is the through-hole version of this chip.</description>
<gates>
<gate name="G$1" symbol="ATMEGAXX8-28PIN_EZ"/>
</gates>
<devices>
<device name="" package="DIL28-EZ">
<connects>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY2313A" prefix="U" uservalue="yes">
<description>ATTINY2313A&lt;br&gt;
2kB 20MHz I2C/SPI/UART</description>
<gates>
<gate name="G$1" symbol="ATTINY2313A"/>
</gates>
<devices>
<device name="" package="SOP20W">
<connects>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PA0/XTAL1" pad="5"/>
<connect gate="G$1" pin="PA1/XTAL2" pad="4"/>
<connect gate="G$1" pin="PA2/!RESET" pad="1"/>
<connect gate="G$1" pin="PB0" pad="12"/>
<connect gate="G$1" pin="PB1" pad="13"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PB5/MOSI/SDA/DI" pad="17"/>
<connect gate="G$1" pin="PB6/MISO/DO" pad="18"/>
<connect gate="G$1" pin="PB7/SCK/SCL" pad="19"/>
<connect gate="G$1" pin="PD0/RXD" pad="2"/>
<connect gate="G$1" pin="PD1/TXD" pad="3"/>
<connect gate="G$1" pin="PD2/INT0" pad="6"/>
<connect gate="G$1" pin="PD3/INT1" pad="7"/>
<connect gate="G$1" pin="PD4" pad="8"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11305"/>
<attribute name="VALUE" value="ATTINY2313A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBED_NXP_LPC1768">
<gates>
<gate name="G$1" symbol="MBED_NXP_LPC1768"/>
</gates>
<devices>
<device name="" package="DIL40_0.9">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY84">
<description>Atmel 14-pin 2/4/8kB flash uC</description>
<gates>
<gate name="G$1" symbol="ATTINY84"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="G$1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="G$1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="G$1" pin="(PCINT11/~RESET/DW)PB3" pad="4"/>
<connect gate="G$1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="G$1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="G$1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="G$1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="G$1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="G$1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="G$1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="G$1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*165">
<gates>
<gate name="A" symbol="74165"/>
</gates>
<devices>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!QH" pad="7"/>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="CLK_INH" pad="15"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="A" pin="F" pad="4"/>
<connect gate="A" pin="G" pad="5"/>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="H" pad="6"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="SER" pad="10"/>
<connect gate="A" pin="SH/!LD" pad="1"/>
<connect gate="A" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0104PWR" prefix="U" uservalue="yes">
<description>&lt;b&gt;4-Bit Bi-Directional Level Shifter&lt;/b&gt;
&lt;ul&gt;
  &lt;li&gt;1.2V-3.6V (VCCA) to 1.65V-5.5V (VCCB) bi-directional level shifter with auto direction sensing.&lt;/li&gt;
  &lt;li&gt;Max data rate - VCCA 1.8V:  20Mbps (50ns), VCCA 3.3V: 100Mbps (10ns)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey: 296-21929-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TXB0104PWR"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="B1" pad="13"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="11"/>
<connect gate="G$1" pin="B4" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OE" pad="8"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC14" package="SO14">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="B1" pad="13"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="11"/>
<connect gate="G$1" pin="B4" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OE" pad="8"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P8X32A-Q44" prefix="U" uservalue="yes">
<description>Propellor uC</description>
<gates>
<gate name="P" symbol="4VDD4VSS"/>
<gate name="P8X32A-Q44" symbol="P8X32A"/>
</gates>
<devices>
<device name="" package="P8X32A-Q44">
<connects>
<connect gate="P" pin="VDD@1" pad="8"/>
<connect gate="P" pin="VDD@2" pad="18"/>
<connect gate="P" pin="VDD@3" pad="30"/>
<connect gate="P" pin="VDD@4" pad="40"/>
<connect gate="P" pin="VSS@1" pad="5"/>
<connect gate="P" pin="VSS@2" pad="17"/>
<connect gate="P" pin="VSS@3" pad="27"/>
<connect gate="P" pin="VSS@4" pad="39"/>
<connect gate="P8X32A-Q44" pin="BOE/" pad="6"/>
<connect gate="P8X32A-Q44" pin="P0" pad="41"/>
<connect gate="P8X32A-Q44" pin="P1" pad="42"/>
<connect gate="P8X32A-Q44" pin="P10" pad="11"/>
<connect gate="P8X32A-Q44" pin="P11" pad="12"/>
<connect gate="P8X32A-Q44" pin="P12" pad="13"/>
<connect gate="P8X32A-Q44" pin="P13" pad="14"/>
<connect gate="P8X32A-Q44" pin="P14" pad="15"/>
<connect gate="P8X32A-Q44" pin="P15" pad="16"/>
<connect gate="P8X32A-Q44" pin="P16" pad="19"/>
<connect gate="P8X32A-Q44" pin="P17" pad="20"/>
<connect gate="P8X32A-Q44" pin="P18" pad="21"/>
<connect gate="P8X32A-Q44" pin="P19" pad="22"/>
<connect gate="P8X32A-Q44" pin="P2" pad="43"/>
<connect gate="P8X32A-Q44" pin="P20" pad="23"/>
<connect gate="P8X32A-Q44" pin="P21" pad="24"/>
<connect gate="P8X32A-Q44" pin="P22" pad="25"/>
<connect gate="P8X32A-Q44" pin="P23" pad="26"/>
<connect gate="P8X32A-Q44" pin="P24" pad="31"/>
<connect gate="P8X32A-Q44" pin="P25" pad="32"/>
<connect gate="P8X32A-Q44" pin="P26" pad="33"/>
<connect gate="P8X32A-Q44" pin="P27" pad="34"/>
<connect gate="P8X32A-Q44" pin="P28" pad="35"/>
<connect gate="P8X32A-Q44" pin="P29" pad="36"/>
<connect gate="P8X32A-Q44" pin="P3" pad="44"/>
<connect gate="P8X32A-Q44" pin="P30" pad="37"/>
<connect gate="P8X32A-Q44" pin="P31" pad="38"/>
<connect gate="P8X32A-Q44" pin="P4" pad="1"/>
<connect gate="P8X32A-Q44" pin="P5" pad="2"/>
<connect gate="P8X32A-Q44" pin="P6" pad="3"/>
<connect gate="P8X32A-Q44" pin="P7" pad="4"/>
<connect gate="P8X32A-Q44" pin="P8" pad="9"/>
<connect gate="P8X32A-Q44" pin="P9" pad="10"/>
<connect gate="P8X32A-Q44" pin="RES/" pad="7"/>
<connect gate="P8X32A-Q44" pin="XI" pad="28"/>
<connect gate="P8X32A-Q44" pin="XO" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328_SMT" prefix="U" uservalue="yes">
<description>32-Pin Atmega328 part&lt;BR&gt;
Commonly used on Arduino compatible boards&lt;br&gt;
Available in QFP and QFN packages&lt;br&gt;
TQFP is IC-09069
QFN is non-stock</description>
<gates>
<gate name="G$1" symbol="ATMEGAXX8-32PIN"/>
</gates>
<devices>
<device name="" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE" value="ATMEGA328P"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32U4">
<description>Atmel 44-pin 8-bit Microcontroller with 32KBytes of ISP Flash and USB Controller</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-DIGITALIC_ATMEGA32U4"/>
</gates>
<devices>
<device name="QFN" package="SPARKFUN-DIGITALIC_QFN-44">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN2" package="SPARKFUN-DIGITALIC_QFN-44-NOPAD">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQFP" package="SPARKFUN-DIGITALIC_TQFP44">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSHA204" prefix="U">
<description>&lt;h3&gt;Atmel ATSHA204&lt;/h3&gt;

The Atmel ATSHA204 is an optimized authentication chip that includes a 4.5Kb EEPROM. This array can be used for storage of keys, miscellaneous read/write, read-only, password or secret data, and consumption tracking. Access to the various sections of memory can be restricted in a variety of ways and then the configuration locked to prevent changes.</description>
<gates>
<gate name="G$1" symbol="ATSHA204"/>
</gates>
<devices>
<device name="-TSU" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SX1509" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Semtech SX1509&lt;/h3&gt;

The SX1509 is a complete ultra low voltage 1.2V to 3.6V General Purpose parallel Input/Output (GPIO) expanders ideal for low power handheld battery powered equipment. This version comes in a 16-channel configuration and allows easy serial expansion of I/O through a standard 400kHz I2C interface. GPIO devices can provide additional control and monitoring when the microcontroller or chipset has insufficient I/O ports, or in systems where serial communication and control from a remote location is advantageous.</description>
<gates>
<gate name="G$1" symbol="SX1509"/>
</gates>
<devices>
<device name="" package="QFN-28">
<connects>
<connect gate="G$1" pin="!INT" pad="9"/>
<connect gate="G$1" pin="!RESET" pad="23"/>
<connect gate="G$1" pin="ADDR0" pad="26"/>
<connect gate="G$1" pin="ADDR1" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 17 29"/>
<connect gate="G$1" pin="I/O[0]" pad="27"/>
<connect gate="G$1" pin="I/O[10]" pad="15"/>
<connect gate="G$1" pin="I/O[11]" pad="16"/>
<connect gate="G$1" pin="I/O[12]" pad="19"/>
<connect gate="G$1" pin="I/O[13]" pad="20"/>
<connect gate="G$1" pin="I/O[14]" pad="21"/>
<connect gate="G$1" pin="I/O[15]" pad="22"/>
<connect gate="G$1" pin="I/O[1]" pad="28"/>
<connect gate="G$1" pin="I/O[2]" pad="1"/>
<connect gate="G$1" pin="I/O[3]" pad="2"/>
<connect gate="G$1" pin="I/O[4]" pad="5"/>
<connect gate="G$1" pin="I/O[5]" pad="6"/>
<connect gate="G$1" pin="I/O[6]" pad="7"/>
<connect gate="G$1" pin="I/O[7]" pad="8"/>
<connect gate="G$1" pin="I/O[8]" pad="13"/>
<connect gate="G$1" pin="I/O[9]" pad="14"/>
<connect gate="G$1" pin="OSCIO" pad="11"/>
<connect gate="G$1" pin="SCL" pad="25"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VCC1" pad="4"/>
<connect gate="G$1" pin="VCC2" pad="18"/>
<connect gate="G$1" pin="VDDM" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
