<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="BATTERY-AAA">
</package>
<package name="BATTERY">
<description>&lt;B&gt;BATTERY&lt;/B&gt;&lt;p&gt;
22 mm</description>
</package>
<package name="BATTERY-AA">
</package>
<package name="BATTCON_12MM_PTH">
</package>
<package name="BATTCON_20MM">
</package>
<package name="BATTCON_245MM">
</package>
<package name="BATTCOM_20MM_PTH">
</package>
<package name="BATTCON_245MM_PTH">
</package>
<package name="LIPO-1100MAH">
</package>
<package name="BATTERY-AA-PANEL">
</package>
<package name="BATTERY_20MM_PTH_COMPACT">
</package>
<package name="BATTCON_12MM">
</package>
<package name="BATTCON_20MM_4LEGS">
</package>
<package name="BATTERY-AA-KIT">
<description>&lt;h3&gt;BATTERY-AA-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="BUTTON-CONDUCTIVE">
</package>
<package name="BUTTON-CONDUCTIVE-0.1">
</package>
<package name="BUTTON-CONDUCTIVE-MINI">
</package>
<package name="BUTTON-10MM">
</package>
<package name="BUTTON-18MM">
</package>
<package name="BUTTONPAD-2X2">
</package>
<package name="BUTTONPAD-2X2-SPECIAL">
</package>
<package name="BUTTONPAD-2X2SINGLE">
</package>
<package name="BUTTONPAD-2X2SINGLE-KIT">
<description>&lt;h3&gt;BUTTONPAD-2X2SINGLE-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="BUTTONPAD-4X4">
</package>
<package name="BUTTONPAD-4X4-SPECIAL">
</package>
<package name="BUZZER-12MM">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
<package name="BUZZER-CMT1603">
</package>
<package name="BUZZER-CCV">
</package>
<package name="BUZZER-CMT1102">
</package>
<package name="BUZZER-12MM-NS">
</package>
<package name="BUZZER-12MM-NS-KIT">
<description>&lt;h3&gt;BUZZER-12MM-NS-KIT&lt;/h3&gt;
Through-hole buzzer&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="BUZZER-CCV-KIT">
<description>&lt;h3&gt;BUZZER-CCV-KIT&lt;/h3&gt;
SMD Buzzer&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to aid in hand soldering.</description>
</package>
<package name="CAPSENSE_PAD">
</package>
<package name="ENCODER_LED_2">
<description>&lt;h3&gt;2-color Illuminated Rotary Encoder&lt;/h3&gt;</description>
</package>
<package name="ENCODER_LED_3">
</package>
<package name="FKIT-LIR2450-H">
</package>
<package name="FKIT-RIBBON_CONNECTOR_03_2MM_L">
</package>
<package name="FKIT-RIBBON_CONNECTOR_03_2MM_R">
</package>
<package name="FKIT-SNAP_FEMALE">
</package>
<package name="FKIT-SNAP_MALE">
</package>
<package name="G3VM-61E1">
</package>
<package name="JOYSTICK">
</package>
<package name="JOYSTICK-PSP1000">
</package>
<package name="JOYSTICK_MINI">
</package>
<package name="LIPO-1100">
</package>
<package name="LIPO-2000">
</package>
<package name="LIPO-100">
</package>
<package name="MAGNET-18MM">
</package>
<package name="VIBE-MOTOR-10MM">
</package>
<package name="N35P112">
</package>
<package name="NAV_SWITCH">
</package>
<package name="ALPS_POT">
</package>
<package name="TRIM_POT">
</package>
<package name="3362U">
</package>
<package name="POT_ALPHA_RV16AF-20">
<description>Package for Alpha RV16AF-20 potentiometer</description>
</package>
<package name="POT_MAMMOTH">
</package>
<package name="POT_PTH">
</package>
<package name="RELAY-G5V">
<description>G5Q SPDT Relay (SparkFun SKU: COM-00100). Footprint should also work with SPST-NO relay.</description>
</package>
<package name="RELAY-G5Q">
</package>
<package name="TACTILE-PTH-SIDEEZ">
</package>
<package name="TACTILE-PTH-SIDE">
</package>
<package name="RELAY-T9A">
<description>Big relay. 220V/30A. SparkFun SKU: COM-00101</description>
</package>
<package name="RELAY-T9A-2">
</package>
<package name="RELAY-JZC">
</package>
<package name="RELAY-S108T02">
</package>
<package name="SLIDER">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="SWITCH-4PDT-CNK">
</package>
<package name="MSS22">
<description>MSS22 DPDT Switch</description>
</package>
<package name="MS">
<description>Series S Slide Switch</description>
</package>
<package name="ES">
<description>Right Angle Slide Switch. Works with part#ES21MABE</description>
</package>
<package name="OS">
</package>
<package name="EG2211">
</package>
<package name="GPI-152-3013">
<description>Switch with part number: GPI-152-3013</description>
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="TACTILE_SWITCH_SMD-2">
</package>
<package name="TACTILE-PTH-12MM">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
<package name="REED_SWITCH_PTH">
</package>
<package name="TACTILE_SWITCH_TALL">
</package>
<package name="REED_SWITCH_PLASTIC">
</package>
<package name="SWITCH-SP3T-SMD">
</package>
<package name="SWITCH-SPDT">
</package>
<package name="SWITCHE-DPDT">
</package>
<package name="R_SW_TH">
</package>
<package name="SWITCH-SPDT-SMD">
</package>
<package name="SWITCH-SPDT_LOCK.007S">
</package>
<package name="SWITCH-SPDT_KIT">
<description>&lt;h3&gt;SWITCH-SPDT_KIT&lt;/h3&gt;
Through-hole SPDT Switch&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="SWITCH-SPST-SMD-A">
</package>
<package name="SWITCH-SPST-VERTICAL">
</package>
<package name="KPS-1290">
</package>
<package name="DIPSWITCH-02">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="DIPSWITCH-08">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="KSA_SEALED_TAC_SWITCH">
</package>
<package name="TRACKBALL">
</package>
<package name="TRIMPOT-3MM">
</package>
<package name="3362U-2">
</package>
<package name="TRIM_POT_PTH">
</package>
<package name="TRIMPOT_PTH_S3_LOCK">
</package>
<package name="3386U">
<description>&lt;h3&gt;TSR-3386U Trimpot&lt;/h3&gt;
Trimpot with a knob&lt;br&gt;
For COM-09806 in the SparkFun catalog&lt;br&gt;</description>
</package>
<package name="TRIMPOT_TC33">
</package>
<package name="TRIMPOT-3MM-2">
</package>
<package name="1X01_TURRET">
<description>0.08" Drill, 0.13" tDoc</description>
</package>
<package name="6400BG_HEATSINK">
</package>
<package name="PCB_MOUNT_SPEAKER">
</package>
<package name="ROTARY_ENC_PLAIN">
<description>Simple rotary encoder, no LED, push center&lt;br&gt;
COM-09117</description>
</package>
<package name="ENCODER-16MM-QUAD">
<description>16mm top width</description>
</package>
<package name="POT_PTH_SWITCH">
<description>topup part# 16M1SHB-B3-20KM-A2K-16Y</description>
</package>
<package name="QFN16-3X3MM">
<description>3mm x 3mm QFN 16 pin</description>
</package>
<package name="USB-AB-MICRO-SMD">
<description>micro USB AB connector for OTG support. 5-pins: USBVCC, GND, D+, D-, USBID. Can act as host or device</description>
</package>
<package name="TRIMPOT-5MM">
</package>
<package name="LIPO-110-TABS">
</package>
</packages>
<symbols>
<symbol name="AYZ0202">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="BATTERY">
<pin name="-" direction="pwr"/>
<pin name="+" direction="pwr"/>
</symbol>
<symbol name="BATTERY-2">
<pin name="-1" direction="pwr"/>
<pin name="+2" direction="pwr"/>
<pin name="+1" direction="pwr"/>
<pin name="-2" direction="pwr"/>
</symbol>
<symbol name="BUTTON-CONDUCTIVE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEWTAP">
<pin name="1"/>
</symbol>
<symbol name="BUTTONPAD_SINGLE">
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="GND"/>
<pin name="RED"/>
<pin name="SIG2"/>
<pin name="SIG1"/>
</symbol>
<symbol name="BUTTONPAD_1LED">
<pin name="A"/>
<pin name="K"/>
<pin name="SIG2"/>
<pin name="SIG1"/>
</symbol>
<symbol name="BUZZER">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CAPSENSE_PAD">
<pin name="RES"/>
<pin name="RECEIVE"/>
</symbol>
<symbol name="ENCODER_LED_2-1">
<pin name="-" direction="pas"/>
<pin name="+R" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="+G" direction="pas"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="ENCODER_LED_3_CA">
<pin name="+" direction="pas"/>
<pin name="-G" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="-R" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="-B" direction="pas"/>
</symbol>
<symbol name="FKIT-BATTERY">
<pin name="NEG"/>
<pin name="POS"/>
</symbol>
<symbol name="FKIT-CONNECTOR_COND_03">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="FKIT-SNAP_CONNECTOR">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="G3VM-61E1">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
<symbol name="JOYSTICK">
<pin name="V+"/>
<pin name="V"/>
<pin name="V-"/>
<pin name="H+"/>
<pin name="H"/>
<pin name="H-"/>
<pin name="SEL+"/>
<pin name="SEL-"/>
</symbol>
<symbol name="JOYSTICK-PSP1000">
<pin name="X"/>
<pin name="Y"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="JOYSTICK_MINI">
<pin name="CENT"/>
<pin name="DOWN"/>
<pin name="GND"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="UP"/>
</symbol>
<symbol name="LIPO-1100">
</symbol>
<symbol name="MAGNET">
</symbol>
<symbol name="MOTOR">
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="N35P112">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="RESETN"/>
<pin name="ADDR"/>
<pin name="VDDP"/>
<pin name="VDD"/>
<pin name="INTN"/>
<pin name="SWITCHN"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
</symbol>
<symbol name="NAV_SWITCH">
<pin name="1" direction="in"/>
<pin name="T" direction="in"/>
<pin name="2" direction="in"/>
<pin name="C" direction="pwr"/>
</symbol>
<symbol name="POT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RELAY-SPDT-2">
<pin name="9"/>
<pin name="6"/>
<pin name="10"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
</symbol>
<symbol name="RELAY-SPDT">
<pin name="COIL2"/>
<pin name="MAIN"/>
<pin name="NO"/>
<pin name="NC"/>
<pin name="COIL1"/>
</symbol>
<symbol name="RELAY-SOLIDSTATE">
<pin name="T1"/>
<pin name="T2"/>
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="STAND-OFF">
</symbol>
<symbol name="SWITCH-4PDT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SWITCH-SP3T">
<pin name="1"/>
<pin name="3"/>
<pin name="2"/>
<pin name="4"/>
</symbol>
<symbol name="TOGGLE">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SPST">
<pin name="P" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SW_SPDT">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SW_DIP-2">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SW_DIP-8">
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TRACKBALL">
</symbol>
<symbol name="TRIMPOT">
<pin name="WIPER" direction="pas"/>
<pin name="CCW" direction="pas"/>
<pin name="CW" direction="pas"/>
</symbol>
<symbol name="TURRET">
<pin name="1"/>
</symbol>
<symbol name="6400GB_HEATSINK">
</symbol>
<symbol name="SPEAKER">
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="ENCODER-QUADRATURE">
<pin name="C"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="ROT_ENCODER">
<description>Simple rotary encode&lt;br&gt;
Center push button&lt;br&gt;
Gray code output&lt;br&gt;
No illumination</description>
<pin name="SW+"/>
<pin name="SW-"/>
<pin name="B"/>
<pin name="C"/>
<pin name="A"/>
</symbol>
<symbol name="TPS62143">
<pin name="PVIN@11"/>
<pin name="PVIN@12"/>
<pin name="AVIN"/>
<pin name="EN"/>
<pin name="FSW"/>
<pin name="PGND@15"/>
<pin name="PGND@16"/>
<pin name="EXT"/>
<pin name="SW@1"/>
<pin name="SW@2"/>
<pin name="SW@3"/>
<pin name="PG"/>
<pin name="VOS"/>
<pin name="SS_TR"/>
<pin name="AGND"/>
<pin name="DEF"/>
<pin name="FB"/>
</symbol>
<symbol name="USB_AB">
<description>USB AB, 5-pins: USBVCC, GND, D+, D-, USBID.</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="USBID"/>
</symbol>
<symbol name="VIN">
<pin name="VIN" direction="sup"/>
</symbol>
<symbol name="TRIMPOT-1">
<pin name="CCW" direction="pas"/>
<pin name="CW" direction="pas"/>
<pin name="WIPER" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AYZ0202">
<description>&lt;b&gt;SPDT Slide Switch&lt;/b&gt;
Simple SMD single-pull double-throw slide switch. Good for  less than 350mA power switch, switching UARTs between devices, etc. Spark Fun Electronics SKU : COM-00597</description>
<gates>
<gate name="G$1" symbol="AYZ0202"/>
</gates>
<devices>
<device name="" package="AYZ0202">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="1"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY" prefix="BAT" uservalue="yes">
<description>&lt;b&gt;Battery Holders&lt;/b&gt;&lt;br&gt;
Various common sizes : AA, AAA, 20mm coin cell and 12mm coin cell.&lt;br&gt;
20MM_4LEGS, BATT-10373</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="AAA" package="BATTERY-AAA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20PTH2" package="BATTERY">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AA" package="BATTERY-AA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12PTH" package="BATTCON_12MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="VCC@1"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20SMD" package="BATTCON_20MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="245MM" package="BATTCON_245MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20PTH" package="BATTCOM_20MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="245PTH" package="BATTCON_245MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1100" package="LIPO-1100MAH">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AA-PANEL" package="BATTERY-AA-PANEL">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FOB" package="BATTERY_20MM_PTH_COMPACT">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12MM" package="BATTCON_12MM">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="20MM_4LEGS" package="BATTCON_20MM_4LEGS">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-10373"/>
<attribute name="VALUE" value="20mm coincell"/>
</technology>
</technologies>
</device>
<device name="AA-KIT" package="BATTERY-AA-KIT">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LIPO-TABS" package="LIPO-110-TABS">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-2">
<description>AA and AAA battery holders</description>
<gates>
<gate name="G$1" symbol="BATTERY-2"/>
</gates>
<devices>
<device name="AA" package="BATTERY-AA">
<connects>
<connect gate="G$1" pin="+1" pad="PWR@1"/>
<connect gate="G$1" pin="+2" pad="PWR@2"/>
<connect gate="G$1" pin="-1" pad="GND@1"/>
<connect gate="G$1" pin="-2" pad="GND@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AAA" package="BATTERY-AAA">
<connects>
<connect gate="G$1" pin="+1" pad="PWR@1"/>
<connect gate="G$1" pin="+2" pad="PWR@2"/>
<connect gate="G$1" pin="-1" pad="GND@1"/>
<connect gate="G$1" pin="-2" pad="GND@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-CONDUCTIVE">
<description>Used with rubber key pads. This one was designed and proven to work with the PolyCase Key FOB enclosures.</description>
<gates>
<gate name="G$1" symbol="BUTTON-CONDUCTIVE"/>
</gates>
<devices>
<device name="SMD" package="BUTTON-CONDUCTIVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-0.1&quot;" package="BUTTON-CONDUCTIVE-0.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="BUTTON-CONDUCTIVE-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-MAGNETIC">
<description>Magnetic metal snaps. 18mm is DEV-08682.</description>
<gates>
<gate name="G$1" symbol="SEWTAP"/>
</gates>
<devices>
<device name="10MM" package="BUTTON-10MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="18MM" package="BUTTON-18MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-2X2">
<description>Proven layout and schematic for 2x2 button pad. Panelize this device/fp to a 4x4 pad if needed. Spark Fun Electronics SKU : COM-07835. Compatible common cathode tri-color LED SKU : COM-00105</description>
<gates>
<gate name="-C1" symbol="BUTTONPAD_SINGLE"/>
<gate name="-C2" symbol="BUTTONPAD_SINGLE"/>
<gate name="-C3" symbol="BUTTONPAD_SINGLE"/>
<gate name="-C4" symbol="BUTTONPAD_SINGLE"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-2X2">
<connects>
<connect gate="-C1" pin="BLU" pad="BLU1"/>
<connect gate="-C1" pin="GND" pad="GND1"/>
<connect gate="-C1" pin="GRN" pad="GRN1"/>
<connect gate="-C1" pin="RED" pad="RED1"/>
<connect gate="-C1" pin="SIG1" pad="SIG1"/>
<connect gate="-C1" pin="SIG2" pad="SIG2"/>
<connect gate="-C2" pin="BLU" pad="BLU2"/>
<connect gate="-C2" pin="GND" pad="GND2"/>
<connect gate="-C2" pin="GRN" pad="GRN2"/>
<connect gate="-C2" pin="RED" pad="RED2"/>
<connect gate="-C2" pin="SIG1" pad="SIG3"/>
<connect gate="-C2" pin="SIG2" pad="SIG4"/>
<connect gate="-C3" pin="BLU" pad="BLU3"/>
<connect gate="-C3" pin="GND" pad="GND3"/>
<connect gate="-C3" pin="GRN" pad="GRN3"/>
<connect gate="-C3" pin="RED" pad="RED3"/>
<connect gate="-C3" pin="SIG1" pad="SIG5"/>
<connect gate="-C3" pin="SIG2" pad="SIG6"/>
<connect gate="-C4" pin="BLU" pad="BLU4"/>
<connect gate="-C4" pin="GND" pad="GND4"/>
<connect gate="-C4" pin="GRN" pad="GRN4"/>
<connect gate="-C4" pin="RED" pad="RED4"/>
<connect gate="-C4" pin="SIG1" pad="SIG7"/>
<connect gate="-C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SPECIAL" package="BUTTONPAD-2X2-SPECIAL">
<connects>
<connect gate="-C1" pin="BLU" pad="BLU1"/>
<connect gate="-C1" pin="GND" pad="GND1"/>
<connect gate="-C1" pin="GRN" pad="GRN1"/>
<connect gate="-C1" pin="RED" pad="RED1"/>
<connect gate="-C1" pin="SIG1" pad="SIG1"/>
<connect gate="-C1" pin="SIG2" pad="SIG2"/>
<connect gate="-C2" pin="BLU" pad="BLU2"/>
<connect gate="-C2" pin="GND" pad="GND2"/>
<connect gate="-C2" pin="GRN" pad="GRN2"/>
<connect gate="-C2" pin="RED" pad="RED2"/>
<connect gate="-C2" pin="SIG1" pad="SIG3"/>
<connect gate="-C2" pin="SIG2" pad="SIG4"/>
<connect gate="-C3" pin="BLU" pad="BLU3"/>
<connect gate="-C3" pin="GND" pad="GND3"/>
<connect gate="-C3" pin="GRN" pad="GRN3"/>
<connect gate="-C3" pin="RED" pad="RED3"/>
<connect gate="-C3" pin="SIG1" pad="SIG5"/>
<connect gate="-C3" pin="SIG2" pad="SIG6"/>
<connect gate="-C4" pin="BLU" pad="BLU4"/>
<connect gate="-C4" pin="GND" pad="GND4"/>
<connect gate="-C4" pin="GRN" pad="GRN4"/>
<connect gate="-C4" pin="RED" pad="RED4"/>
<connect gate="-C4" pin="SIG1" pad="SIG7"/>
<connect gate="-C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-2X2SINGLE">
<description>Proto layout and schematic for 2x2 button pad with single color LEDs (used on Simon board). Panelize this device/fp to a 4x4 pad if needed. Any single-color 5mm LED should be compatible. Spark Fun Electronics SKU : COM-07835.</description>
<gates>
<gate name="C1" symbol="BUTTONPAD_1LED"/>
<gate name="C2" symbol="BUTTONPAD_1LED"/>
<gate name="C3" symbol="BUTTONPAD_1LED"/>
<gate name="C4" symbol="BUTTONPAD_1LED"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-2X2SINGLE">
<connects>
<connect gate="C1" pin="A" pad="A1"/>
<connect gate="C1" pin="K" pad="K1"/>
<connect gate="C1" pin="SIG1" pad="SIG1"/>
<connect gate="C1" pin="SIG2" pad="SIG2"/>
<connect gate="C2" pin="A" pad="A2"/>
<connect gate="C2" pin="K" pad="K2"/>
<connect gate="C2" pin="SIG1" pad="SIG3"/>
<connect gate="C2" pin="SIG2" pad="SIG4"/>
<connect gate="C3" pin="A" pad="A3"/>
<connect gate="C3" pin="K" pad="K3"/>
<connect gate="C3" pin="SIG1" pad="SIG5"/>
<connect gate="C3" pin="SIG2" pad="SIG6"/>
<connect gate="C4" pin="A" pad="A4"/>
<connect gate="C4" pin="K" pad="K4"/>
<connect gate="C4" pin="SIG1" pad="SIG7"/>
<connect gate="C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="BUTTONPAD-2X2SINGLE-KIT">
<connects>
<connect gate="C1" pin="A" pad="A1"/>
<connect gate="C1" pin="K" pad="K1"/>
<connect gate="C1" pin="SIG1" pad="SIG1"/>
<connect gate="C1" pin="SIG2" pad="SIG2"/>
<connect gate="C2" pin="A" pad="A2"/>
<connect gate="C2" pin="K" pad="K2"/>
<connect gate="C2" pin="SIG1" pad="SIG3"/>
<connect gate="C2" pin="SIG2" pad="SIG4"/>
<connect gate="C3" pin="A" pad="A3"/>
<connect gate="C3" pin="K" pad="K3"/>
<connect gate="C3" pin="SIG1" pad="SIG5"/>
<connect gate="C3" pin="SIG2" pad="SIG6"/>
<connect gate="C4" pin="A" pad="A4"/>
<connect gate="C4" pin="K" pad="K4"/>
<connect gate="C4" pin="SIG1" pad="SIG7"/>
<connect gate="C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-4X4">
<description>Proto layout and schematic for 4x4 button pad. Spark Fun Electronics SKU : COM-07835. Compatible common cathode tri-color LED SKU : COM-00105</description>
<gates>
<gate name="G$0" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$1" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$2" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$3" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$4" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$5" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$6" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$7" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$8" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$9" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$10" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$11" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$12" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$13" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$14" symbol="BUTTONPAD_SINGLE"/>
<gate name="G$15" symbol="BUTTONPAD_SINGLE"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-4X4">
<connects>
<connect gate="G$0" pin="BLU" pad="BLU0"/>
<connect gate="G$0" pin="GND" pad="GND0"/>
<connect gate="G$0" pin="GRN" pad="GRN0"/>
<connect gate="G$0" pin="RED" pad="RED0"/>
<connect gate="G$0" pin="SIG1" pad="SIG0"/>
<connect gate="G$0" pin="SIG2" pad="SIG1"/>
<connect gate="G$1" pin="BLU" pad="BLU1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GRN" pad="GRN1"/>
<connect gate="G$1" pin="RED" pad="RED1"/>
<connect gate="G$1" pin="SIG1" pad="SIG2"/>
<connect gate="G$1" pin="SIG2" pad="SIG3"/>
<connect gate="G$10" pin="BLU" pad="BLU10"/>
<connect gate="G$10" pin="GND" pad="GND10"/>
<connect gate="G$10" pin="GRN" pad="GRN10"/>
<connect gate="G$10" pin="RED" pad="RED10"/>
<connect gate="G$10" pin="SIG1" pad="SIG20"/>
<connect gate="G$10" pin="SIG2" pad="SIG21"/>
<connect gate="G$11" pin="BLU" pad="BLU11"/>
<connect gate="G$11" pin="GND" pad="GND11"/>
<connect gate="G$11" pin="GRN" pad="GRN11"/>
<connect gate="G$11" pin="RED" pad="RED11"/>
<connect gate="G$11" pin="SIG1" pad="SIG22"/>
<connect gate="G$11" pin="SIG2" pad="SIG23"/>
<connect gate="G$12" pin="BLU" pad="BLU12"/>
<connect gate="G$12" pin="GND" pad="GND12"/>
<connect gate="G$12" pin="GRN" pad="GRN12"/>
<connect gate="G$12" pin="RED" pad="RED12"/>
<connect gate="G$12" pin="SIG1" pad="SIG24"/>
<connect gate="G$12" pin="SIG2" pad="SIG25"/>
<connect gate="G$13" pin="BLU" pad="BLU13"/>
<connect gate="G$13" pin="GND" pad="GND13"/>
<connect gate="G$13" pin="GRN" pad="GRN13"/>
<connect gate="G$13" pin="RED" pad="RED13"/>
<connect gate="G$13" pin="SIG1" pad="SIG26"/>
<connect gate="G$13" pin="SIG2" pad="SIG27"/>
<connect gate="G$14" pin="BLU" pad="BLU14"/>
<connect gate="G$14" pin="GND" pad="GND14"/>
<connect gate="G$14" pin="GRN" pad="GRN14"/>
<connect gate="G$14" pin="RED" pad="RED14"/>
<connect gate="G$14" pin="SIG1" pad="SIG28"/>
<connect gate="G$14" pin="SIG2" pad="SIG29"/>
<connect gate="G$15" pin="BLU" pad="BLU15"/>
<connect gate="G$15" pin="GND" pad="GND15"/>
<connect gate="G$15" pin="GRN" pad="GRN15"/>
<connect gate="G$15" pin="RED" pad="RED15"/>
<connect gate="G$15" pin="SIG1" pad="SIG30"/>
<connect gate="G$15" pin="SIG2" pad="SIG31"/>
<connect gate="G$2" pin="BLU" pad="BLU2"/>
<connect gate="G$2" pin="GND" pad="GND2"/>
<connect gate="G$2" pin="GRN" pad="GRN2"/>
<connect gate="G$2" pin="RED" pad="RED2"/>
<connect gate="G$2" pin="SIG1" pad="SIG4"/>
<connect gate="G$2" pin="SIG2" pad="SIG5"/>
<connect gate="G$3" pin="BLU" pad="BLU3"/>
<connect gate="G$3" pin="GND" pad="GND3"/>
<connect gate="G$3" pin="GRN" pad="GRN3"/>
<connect gate="G$3" pin="RED" pad="RED3"/>
<connect gate="G$3" pin="SIG1" pad="SIG6"/>
<connect gate="G$3" pin="SIG2" pad="SIG7"/>
<connect gate="G$4" pin="BLU" pad="BLU4"/>
<connect gate="G$4" pin="GND" pad="GND4"/>
<connect gate="G$4" pin="GRN" pad="GRN4"/>
<connect gate="G$4" pin="RED" pad="RED4"/>
<connect gate="G$4" pin="SIG1" pad="SIG8"/>
<connect gate="G$4" pin="SIG2" pad="SIG9"/>
<connect gate="G$5" pin="BLU" pad="BLU5"/>
<connect gate="G$5" pin="GND" pad="GND5"/>
<connect gate="G$5" pin="GRN" pad="GRN6"/>
<connect gate="G$5" pin="RED" pad="RED5"/>
<connect gate="G$5" pin="SIG1" pad="SIG10"/>
<connect gate="G$5" pin="SIG2" pad="SIG11"/>
<connect gate="G$6" pin="BLU" pad="BLU6"/>
<connect gate="G$6" pin="GND" pad="GND6"/>
<connect gate="G$6" pin="GRN" pad="GRN5"/>
<connect gate="G$6" pin="RED" pad="RED6"/>
<connect gate="G$6" pin="SIG1" pad="SIG12"/>
<connect gate="G$6" pin="SIG2" pad="SIG13"/>
<connect gate="G$7" pin="BLU" pad="BLU7"/>
<connect gate="G$7" pin="GND" pad="GND7"/>
<connect gate="G$7" pin="GRN" pad="GRN7"/>
<connect gate="G$7" pin="RED" pad="RED7"/>
<connect gate="G$7" pin="SIG1" pad="SIG14"/>
<connect gate="G$7" pin="SIG2" pad="SIG15"/>
<connect gate="G$8" pin="BLU" pad="BLU8"/>
<connect gate="G$8" pin="GND" pad="GND8"/>
<connect gate="G$8" pin="GRN" pad="GRN8"/>
<connect gate="G$8" pin="RED" pad="RED8"/>
<connect gate="G$8" pin="SIG1" pad="SIG16"/>
<connect gate="G$8" pin="SIG2" pad="SIG17"/>
<connect gate="G$9" pin="BLU" pad="BLU9"/>
<connect gate="G$9" pin="GND" pad="GND9"/>
<connect gate="G$9" pin="GRN" pad="GRN9"/>
<connect gate="G$9" pin="RED" pad="RED9"/>
<connect gate="G$9" pin="SIG1" pad="SIG18"/>
<connect gate="G$9" pin="SIG2" pad="SIG19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="BUTTONPAD-4X4-SPECIAL">
<connects>
<connect gate="G$0" pin="BLU" pad="BLU0"/>
<connect gate="G$0" pin="GND" pad="GND0"/>
<connect gate="G$0" pin="GRN" pad="GRN0"/>
<connect gate="G$0" pin="RED" pad="RED0"/>
<connect gate="G$0" pin="SIG1" pad="SIG0"/>
<connect gate="G$0" pin="SIG2" pad="SIG1"/>
<connect gate="G$1" pin="BLU" pad="BLU1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GRN" pad="GRN1"/>
<connect gate="G$1" pin="RED" pad="RED1"/>
<connect gate="G$1" pin="SIG1" pad="SIG2"/>
<connect gate="G$1" pin="SIG2" pad="SIG3"/>
<connect gate="G$10" pin="BLU" pad="BLU10"/>
<connect gate="G$10" pin="GND" pad="GND10"/>
<connect gate="G$10" pin="GRN" pad="GRN10"/>
<connect gate="G$10" pin="RED" pad="RED10"/>
<connect gate="G$10" pin="SIG1" pad="SIG20"/>
<connect gate="G$10" pin="SIG2" pad="SIG21"/>
<connect gate="G$11" pin="BLU" pad="BLU11"/>
<connect gate="G$11" pin="GND" pad="GND11"/>
<connect gate="G$11" pin="GRN" pad="GRN11"/>
<connect gate="G$11" pin="RED" pad="RED11"/>
<connect gate="G$11" pin="SIG1" pad="SIG22"/>
<connect gate="G$11" pin="SIG2" pad="SIG23"/>
<connect gate="G$12" pin="BLU" pad="BLU12"/>
<connect gate="G$12" pin="GND" pad="GND12"/>
<connect gate="G$12" pin="GRN" pad="GRN12"/>
<connect gate="G$12" pin="RED" pad="RED12"/>
<connect gate="G$12" pin="SIG1" pad="SIG24"/>
<connect gate="G$12" pin="SIG2" pad="SIG25"/>
<connect gate="G$13" pin="BLU" pad="BLU13"/>
<connect gate="G$13" pin="GND" pad="GND13"/>
<connect gate="G$13" pin="GRN" pad="GRN13"/>
<connect gate="G$13" pin="RED" pad="RED13"/>
<connect gate="G$13" pin="SIG1" pad="SIG26"/>
<connect gate="G$13" pin="SIG2" pad="SIG27"/>
<connect gate="G$14" pin="BLU" pad="BLU14"/>
<connect gate="G$14" pin="GND" pad="GND14"/>
<connect gate="G$14" pin="GRN" pad="GRN14"/>
<connect gate="G$14" pin="RED" pad="RED14"/>
<connect gate="G$14" pin="SIG1" pad="SIG28"/>
<connect gate="G$14" pin="SIG2" pad="SIG29"/>
<connect gate="G$15" pin="BLU" pad="BLU15"/>
<connect gate="G$15" pin="GND" pad="GND15"/>
<connect gate="G$15" pin="GRN" pad="GRN15"/>
<connect gate="G$15" pin="RED" pad="RED15"/>
<connect gate="G$15" pin="SIG1" pad="SIG30"/>
<connect gate="G$15" pin="SIG2" pad="SIG31"/>
<connect gate="G$2" pin="BLU" pad="BLU2"/>
<connect gate="G$2" pin="GND" pad="GND2"/>
<connect gate="G$2" pin="GRN" pad="GRN2"/>
<connect gate="G$2" pin="RED" pad="RED2"/>
<connect gate="G$2" pin="SIG1" pad="SIG4"/>
<connect gate="G$2" pin="SIG2" pad="SIG5"/>
<connect gate="G$3" pin="BLU" pad="BLU3"/>
<connect gate="G$3" pin="GND" pad="GND3"/>
<connect gate="G$3" pin="GRN" pad="GRN3"/>
<connect gate="G$3" pin="RED" pad="RED3"/>
<connect gate="G$3" pin="SIG1" pad="SIG6"/>
<connect gate="G$3" pin="SIG2" pad="SIG7"/>
<connect gate="G$4" pin="BLU" pad="BLU4"/>
<connect gate="G$4" pin="GND" pad="GND4"/>
<connect gate="G$4" pin="GRN" pad="GRN4"/>
<connect gate="G$4" pin="RED" pad="RED4"/>
<connect gate="G$4" pin="SIG1" pad="SIG8"/>
<connect gate="G$4" pin="SIG2" pad="SIG9"/>
<connect gate="G$5" pin="BLU" pad="BLU5"/>
<connect gate="G$5" pin="GND" pad="GND5"/>
<connect gate="G$5" pin="GRN" pad="GRN6"/>
<connect gate="G$5" pin="RED" pad="RED5"/>
<connect gate="G$5" pin="SIG1" pad="SIG10"/>
<connect gate="G$5" pin="SIG2" pad="SIG11"/>
<connect gate="G$6" pin="BLU" pad="BLU6"/>
<connect gate="G$6" pin="GND" pad="GND6"/>
<connect gate="G$6" pin="GRN" pad="GRN5"/>
<connect gate="G$6" pin="RED" pad="RED6"/>
<connect gate="G$6" pin="SIG1" pad="SIG12"/>
<connect gate="G$6" pin="SIG2" pad="SIG13"/>
<connect gate="G$7" pin="BLU" pad="BLU7"/>
<connect gate="G$7" pin="GND" pad="GND7"/>
<connect gate="G$7" pin="GRN" pad="GRN7"/>
<connect gate="G$7" pin="RED" pad="RED7"/>
<connect gate="G$7" pin="SIG1" pad="SIG14"/>
<connect gate="G$7" pin="SIG2" pad="SIG15"/>
<connect gate="G$8" pin="BLU" pad="BLU8"/>
<connect gate="G$8" pin="GND" pad="GND8"/>
<connect gate="G$8" pin="GRN" pad="GRN8"/>
<connect gate="G$8" pin="RED" pad="RED8"/>
<connect gate="G$8" pin="SIG1" pad="SIG16"/>
<connect gate="G$8" pin="SIG2" pad="SIG17"/>
<connect gate="G$9" pin="BLU" pad="BLU9"/>
<connect gate="G$9" pin="GND" pad="GND9"/>
<connect gate="G$9" pin="GRN" pad="GRN9"/>
<connect gate="G$9" pin="RED" pad="RED9"/>
<connect gate="G$9" pin="SIG1" pad="SIG18"/>
<connect gate="G$9" pin="SIG2" pad="SIG19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUZZER" prefix="SG">
<description>&lt;b&gt;Buzzer 12mm&lt;/b&gt;
Spark Fun Electronics SKU : Comp-Buzzer</description>
<gates>
<gate name="G$1" symbol="BUZZER"/>
</gates>
<devices>
<device name="PTH" package="BUZZER-12MM">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="BUZZER-CMT1603">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="BUZZER-CCV">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD3" package="BUZZER-CMT1102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NS" package="BUZZER-12MM-NS">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-NS-KIT" package="BUZZER-12MM-NS-KIT">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2-KIT" package="BUZZER-CCV-KIT">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPSENSE_PAD">
<description>Generic copper pad for a capacitive touch sensor.</description>
<gates>
<gate name="G$1" symbol="CAPSENSE_PAD"/>
</gates>
<devices>
<device name="" package="CAPSENSE_PAD">
<connects>
<connect gate="G$1" pin="RECEIVE" pad="P$1"/>
<connect gate="G$1" pin="RES" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER_2LED" prefix="U">
<description>&lt;H3&gt;Illuminated Rotary Encoder w/ 2 LEDs&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="ENCODER_LED_2-1"/>
</gates>
<devices>
<device name="" package="ENCODER_LED_2">
<connects>
<connect gate="G$1" pin="+G" pad="+G"/>
<connect gate="G$1" pin="+R" pad="+R"/>
<connect gate="G$1" pin="-" pad="GND"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="SW"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER_RGB_CA" prefix="SW" uservalue="yes">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ RGB LED and select switch&lt;/h3&gt;

EC12PLRGBSDVBF-D: http://top-up.so-buy.com/front/bin/ptdetail.phtml?Part=EC12PLRGBSDVBF-D</description>
<gates>
<gate name="G$1" symbol="ENCODER_LED_3_CA"/>
</gates>
<devices>
<device name="" package="ENCODER_LED_3">
<connects>
<connect gate="G$1" pin="+" pad="5"/>
<connect gate="G$1" pin="-B" pad="4"/>
<connect gate="G$1" pin="-G" pad="2"/>
<connect gate="G$1" pin="-R" pad="1"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-COIN_CELL" prefix="BATT">
<description>&lt;h3&gt;Fabrick.it Coin Cell Holder&lt;/h3&gt;
Coin cell holder for 24.5mm rechargable coin cell</description>
<gates>
<gate name="G$1" symbol="FKIT-BATTERY"/>
</gates>
<devices>
<device name="LIR2450-H" package="FKIT-LIR2450-H">
<connects>
<connect gate="G$1" pin="NEG" pad="NEG"/>
<connect gate="G$1" pin="POS" pad="POS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-RIBBON_CONNECTOR" prefix="J">
<description>&lt;h3&gt;fabrick.it Conductive Ribbon Connector&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="FKIT-CONNECTOR_COND_03"/>
</gates>
<devices>
<device name="-2MM_L_REV2" package="FKIT-RIBBON_CONNECTOR_03_2MM_L">
<connects>
<connect gate="G$1" pin="P$1" pad="P1A"/>
<connect gate="G$1" pin="P$2" pad="P2A"/>
<connect gate="G$1" pin="P$3" pad="P3A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2MM_R_REV2" package="FKIT-RIBBON_CONNECTOR_03_2MM_R">
<connects>
<connect gate="G$1" pin="P$1" pad="P1A"/>
<connect gate="G$1" pin="P$2" pad="P2A"/>
<connect gate="G$1" pin="P$3" pad="P3A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-SNAP_CONNECTOR">
<description>Snap connector for Fabrick.it products</description>
<gates>
<gate name="G$1" symbol="FKIT-SNAP_CONNECTOR"/>
</gates>
<devices>
<device name="-FEMALE" package="FKIT-SNAP_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MALE" package="FKIT-SNAP_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G3VM-61E1">
<description>Omron NO solid state relay</description>
<gates>
<gate name="G$1" symbol="G3VM-61E1"/>
</gates>
<devices>
<device name="" package="G3VM-61E1">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK" prefix="U">
<description>&lt;b&gt;Thumb Joystick&lt;/b&gt;
Joystick commonly found in PS2 controllers. Two pots and a select switch. Footprint proven. Spark Fun Electronics SKU : COM-09032</description>
<gates>
<gate name="G$1" symbol="JOYSTICK"/>
</gates>
<devices>
<device name="PTH" package="JOYSTICK">
<connects>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="H+" pad="H1"/>
<connect gate="G$1" pin="H-" pad="H3"/>
<connect gate="G$1" pin="SEL+" pad="B1A"/>
<connect gate="G$1" pin="SEL-" pad="B2A"/>
<connect gate="G$1" pin="V" pad="V2"/>
<connect gate="G$1" pin="V+" pad="V1"/>
<connect gate="G$1" pin="V-" pad="V3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK-PSP1000">
<description>This is a footprint for the PSP-1000 Joystick.  4-pins: X, Y, Vcc and GND</description>
<gates>
<gate name="G$1" symbol="JOYSTICK-PSP1000"/>
</gates>
<devices>
<device name="" package="JOYSTICK-PSP1000">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="X" pad="X"/>
<connect gate="G$1" pin="Y" pad="Y"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK_MINI" prefix="S" uservalue="yes">
<description>Small 5-way tactile joystick, COM-10063&lt;p&gt;
4UCON SF303GJ26</description>
<gates>
<gate name="G$1" symbol="JOYSTICK_MINI"/>
</gates>
<devices>
<device name="" package="JOYSTICK_MINI">
<connects>
<connect gate="G$1" pin="CENT" pad="CTR"/>
<connect gate="G$1" pin="DOWN" pad="D"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="LEFT" pad="C"/>
<connect gate="G$1" pin="RIGHT" pad="B"/>
<connect gate="G$1" pin="UP" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIPO-OUTLINE">
<description>Outlines for common LiPo batteries sold by SparkFun.&lt;br&gt;
For fit only- no pads or connectors!</description>
<gates>
<gate name="G$1" symbol="LIPO-1100"/>
</gates>
<devices>
<device name="1100" package="LIPO-1100">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2000" package="LIPO-2000">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="100" package="LIPO-100">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGNET">
<description>Ceramic disc magnet, COM-08890</description>
<gates>
<gate name="G$1" symbol="MAGNET"/>
</gates>
<devices>
<device name="18MM" package="MAGNET-18MM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOTOR">
<description>&lt;b&gt;Vibration Motor- ROB-08449&lt;/b&gt;
Physical dimension and wire connections for this powerful vibration motor. Motor has a self adhesive backing.</description>
<gates>
<gate name="G$1" symbol="MOTOR"/>
</gates>
<devices>
<device name="10MM" package="VIBE-MOTOR-10MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N35P112" prefix="U" uservalue="yes">
<description>Hall-effect based I2C analog mini-joystick with button</description>
<gates>
<gate name="G$1" symbol="N35P112"/>
</gates>
<devices>
<device name="" package="N35P112">
<connects>
<connect gate="G$1" pin="ADDR" pad="9"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="11"/>
<connect gate="G$1" pin="GND4" pad="12"/>
<connect gate="G$1" pin="GND5" pad="13"/>
<connect gate="G$1" pin="INTN" pad="7"/>
<connect gate="G$1" pin="RESETN" pad="6"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SWITCHN" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAV_SWITCH">
<description>&lt;b&gt;Navigation Switch&lt;/b&gt;
Three way navigation switch. Commonly used as up/down/select on MP3 players. Schematic element and footprint production proven. Spark Fun Electronics SKU : COM-08184</description>
<gates>
<gate name="G$1" symbol="NAV_SWITCH"/>
</gates>
<devices>
<device name="SMD" package="NAV_SWITCH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="T" pad="T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT" uservalue="yes">
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="" package="ALPS_POT">
<connects>
<connect gate="G$1" pin="A" pad="P$3"/>
<connect gate="G$1" pin="E" pad="P$1"/>
<connect gate="G$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRIM" package="TRIM_POT">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="100K_3362U" package="3362U">
<connects>
<connect gate="G$1" pin="A" pad="P$3"/>
<connect gate="G$1" pin="E" pad="P$1"/>
<connect gate="G$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RV16AF-20" package="POT_ALPHA_RV16AF-20">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MAM" package="POT_MAMMOTH">
<connects>
<connect gate="G$1" pin="A" pad="P$2"/>
<connect gate="G$1" pin="E" pad="P$3"/>
<connect gate="G$1" pin="S" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-2">
<description>SPDT relay (COM-00100)</description>
<gates>
<gate name="G$1" symbol="RELAY-SPDT-2"/>
</gates>
<devices>
<device name="G5Q" package="RELAY-G5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY">
<description>SPDT relay (COM-00101)</description>
<gates>
<gate name="G$1" symbol="RELAY-SPDT"/>
</gates>
<devices>
<device name="PTH" package="RELAY-G5Q">
<connects>
<connect gate="G$1" pin="COIL1" pad="5"/>
<connect gate="G$1" pin="COIL2" pad="1"/>
<connect gate="G$1" pin="MAIN" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="RELAY-T9A">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="MAIN"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="RELAY-T9A-2">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="MAIN"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="RELAY-JZC">
<connects>
<connect gate="G$1" pin="COIL1" pad="5"/>
<connect gate="G$1" pin="COIL2" pad="1"/>
<connect gate="G$1" pin="MAIN" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-SOLIDSTATE" prefix="U">
<description>SPST SS relay</description>
<gates>
<gate name="G$1" symbol="RELAY-SOLIDSTATE"/>
</gates>
<devices>
<device name="PTH" package="RELAY-S108T02">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="4"/>
<connect gate="G$1" pin="T1" pad="1"/>
<connect gate="G$1" pin="T2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDER">
<description>Slide-type potentiometer- COM-9119</description>
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="" package="SLIDER">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="S" pad="2A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STAND-OFF" prefix="STANDOFF">
<description>&lt;b&gt;#4 Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
<gates>
<gate name="G$1" symbol="STAND-OFF"/>
</gates>
<devices>
<device name="" package="STAND-OFF">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TIGHT" package="STAND-OFF-TIGHT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-4PDT">
<description>For use with a push-button switch made by CnK components.</description>
<gates>
<gate name="G$1" symbol="SWITCH-4PDT"/>
</gates>
<devices>
<device name="CNK_LOCK" package="SWITCH-4PDT-CNK">
<connects>
<connect gate="G$1" pin="1" pad="PP$1"/>
<connect gate="G$1" pin="10" pad="PP$10"/>
<connect gate="G$1" pin="11" pad="PP$11"/>
<connect gate="G$1" pin="12" pad="PP$12"/>
<connect gate="G$1" pin="2" pad="PP$2"/>
<connect gate="G$1" pin="3" pad="PP$3"/>
<connect gate="G$1" pin="4" pad="PP$4"/>
<connect gate="G$1" pin="5" pad="PP$5"/>
<connect gate="G$1" pin="6" pad="PP$6"/>
<connect gate="G$1" pin="7" pad="PP$7"/>
<connect gate="G$1" pin="8" pad="PP$8"/>
<connect gate="G$1" pin="9" pad="PP$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-DPDT" prefix="S" uservalue="yes">
<description>DPDT Version of the COM-00597</description>
<gates>
<gate name="G$1" symbol="AYZ0202"/>
</gates>
<devices>
<device name="AYZ0202" package="AYZ0202">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08179"/>
<attribute name="VALUE" value="DPDT"/>
</technology>
</technologies>
</device>
<device name="PTH" package="MSS22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH1" package="MS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ES" package="ES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OS" package="OS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EG2211" package="EG2211">
<connects>
<connect gate="G$1" pin="1" pad="P1-TA"/>
<connect gate="G$1" pin="2" pad="P1"/>
<connect gate="G$1" pin="3" pad="P1-TB"/>
<connect gate="G$1" pin="4" pad="P2-TA"/>
<connect gate="G$1" pin="5" pad="P2"/>
<connect gate="G$1" pin="6" pad="P2-TB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GPI" package="GPI-152-3013">
<connects>
<connect gate="G$1" pin="1" pad="10"/>
<connect gate="G$1" pin="2" pad="C@1"/>
<connect gate="G$1" pin="3" pad="20"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="C@2"/>
<connect gate="G$1" pin="6" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-MOMENTARY-2" prefix="S">
<description>Various NO switches- pushbuttons, reed, etc</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-2" package="TACTILE_SWITCH_SMD-2">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12MM" package="TACTILE-PTH-12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-1101NE" package="TACTILE-SWITCH-1101NE">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_REED" package="REED_SWITCH_PTH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TACTILE_SWITCH_TALL">
<connects>
<connect gate="G$1" pin="1" pad="A2"/>
<connect gate="G$1" pin="2" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_REED2" package="REED_SWITCH_PLASTIC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDE_EZ" package="TACTILE-PTH-SIDEEZ">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SP3T" prefix="S" uservalue="yes">
<gates>
<gate name="G$1" symbol="SWITCH-SP3T"/>
</gates>
<devices>
<device name="" package="SWITCH-SP3T-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPDT" prefix="S" uservalue="yes">
<description>&lt;b&gt;SPDT Switch&lt;/b&gt;&lt;br&gt;
Simple slide switch, Spark Fun Electronics SKU : COM-00102&lt;br&gt;
DPDT SMT slide switch, AYZ0202, SWCH-08179</description>
<gates>
<gate name="1" symbol="TOGGLE"/>
</gates>
<devices>
<device name="PTH" package="SWITCH-SPDT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="AYZ0202">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08179"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="SWITCHE-DPDT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="R_SW_TH">
<connects>
<connect gate="1" pin="O" pad="P$1"/>
<connect gate="1" pin="P" pad="P$2"/>
<connect gate="1" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SWITCH-SPDT-SMD">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="SWITCH-SPDT_LOCK.007S">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="SWITCH-SPDT_KIT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-A" package="SWITCH-SPST-SMD-A">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPST-2">
<gates>
<gate name="G$1" symbol="SPST"/>
</gates>
<devices>
<device name="RA" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="O" pad="P$3"/>
<connect gate="G$1" pin="P" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TV" package="SWITCH-SPST-VERTICAL">
<connects>
<connect gate="G$1" pin="O" pad="1"/>
<connect gate="G$1" pin="P" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_SPDT">
<description>Side-actuated SPDT slide switch, as used on the Arduino Pro</description>
<gates>
<gate name="G$1" symbol="SW_SPDT"/>
</gates>
<devices>
<device name="" package="KPS-1290">
<connects>
<connect gate="G$1" pin="O" pad="O"/>
<connect gate="G$1" pin="P" pad="P"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_DIP-2" prefix="SW" uservalue="yes">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SW_DIP-2"/>
</gates>
<devices>
<device name="" package="DIPSWITCH-02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_DIP-8" prefix="SW" uservalue="yes">
<description>&lt;b&gt;DIP Switch 8 Position&lt;/b&gt;
Spark Fun Electronics SKU : COM-08034</description>
<gates>
<gate name="A" symbol="SW_DIP-8"/>
</gates>
<devices>
<device name="" package="DIPSWITCH-08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAC_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;Momentary Switch&lt;/b&gt;&lt;br&gt;
Button commonly used for reset or general input.&lt;br&gt;
Spark Fun Electronics SKU : COM-00097&lt;br&gt;
SMT- SWCH-08247</description>
<gates>
<gate name="S" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
</technology>
</technologies>
</device>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KSA_SEALED" package="KSA_SEALED_TAC_SWITCH">
<connects>
<connect gate="S" pin="1" pad="P$1"/>
<connect gate="S" pin="2" pad="P$2"/>
<connect gate="S" pin="3" pad="P$3"/>
<connect gate="S" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRACKBALL">
<description>Mechanical footprint for trackball</description>
<gates>
<gate name="G$1" symbol="TRACKBALL"/>
</gates>
<devices>
<device name="MECH" package="TRACKBALL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TURRET-1520" uservalue="yes">
<description>Turret FP for Keystone Electronics Part#1520</description>
<gates>
<gate name="G$1" symbol="TURRET"/>
</gates>
<devices>
<device name="PTH" package="1X01_TURRET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6400BG_HEATSINK">
<description>Multiwatt heatsink, PRT-09576</description>
<gates>
<gate name="G$1" symbol="6400GB_HEATSINK"/>
</gates>
<devices>
<device name="" package="6400BG_HEATSINK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPEAKER" prefix="SP">
<description>General speakers.</description>
<gates>
<gate name="G$1" symbol="SPEAKER"/>
</gates>
<devices>
<device name="" package="PCB_MOUNT_SPEAKER">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="PCB_MOUNT">
<attribute name="MFG" value="SANCO"/>
<attribute name="PROD_#" value="NA"/>
<attribute name="SKU" value="COM-11089"/>
<attribute name="SPARKLE_ID" value="6504"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER-QUADRATURE" prefix="U" uservalue="yes">
<description>quadrature encoder from Top-Up, part#EC16PHBF-B-20F-24-24C-16Y</description>
<gates>
<gate name="G$1" symbol="ENCODER-QUADRATURE"/>
</gates>
<devices>
<device name="" package="ENCODER-16MM-QUAD">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT_SWITCH" prefix="U" uservalue="yes">
<description>Potentiometer w/ switch.</description>
<gates>
<gate name="G$1" symbol="POT"/>
<gate name="G$2" symbol="SWITCH-MOMENTARY-2-1"/>
</gates>
<devices>
<device name="POT_PTH" package="POT_PTH">
<connects>
<connect gate="G$1" pin="A" pad="E@1"/>
<connect gate="G$1" pin="E" pad="E@2"/>
<connect gate="G$1" pin="S" pad="WAND"/>
<connect gate="G$2" pin="1" pad="S1"/>
<connect gate="G$2" pin="2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POT_PTH_SWITCH" package="POT_PTH_SWITCH">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
<connect gate="G$2" pin="1" pad="S1"/>
<connect gate="G$2" pin="2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT" prefix="R">
<description>Various small potentiometers for "set-and-forget" applications</description>
<gates>
<gate name="R?" symbol="TRIMPOT-1"/>
</gates>
<devices>
<device name="-2" package="TRIMPOT_TC33">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH-KNOB" package="3386U">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM-2" package="TRIMPOT-3MM-2">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3362U-2" package="3362U-2">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="TRIM_POT_PTH">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TRIMPOT-3MM">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRIMPOT-5MM" package="TRIMPOT-5MM">
<connects>
<connect gate="R?" pin="CCW" pad="A"/>
<connect gate="R?" pin="CW" pad="C"/>
<connect gate="R?" pin="WIPER" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRIMPOT_PTH_S3_LOCK" package="TRIMPOT_PTH_S3_LOCK">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ROTARTY_ENCODER" prefix="SW">
<description>Simple no LED rotary encoder&lt;br&gt;
Example: COM-09117</description>
<gates>
<gate name="G$1" symbol="ROT_ENCODER"/>
</gates>
<devices>
<device name="" package="ROTARY_ENC_PLAIN">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW+" pad="SW+"/>
<connect gate="G$1" pin="SW-" pad="SW-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
