<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SC-70">
</package>
<package name="SO08WIDE">
</package>
<package name="DRC-10">
<description>&lt;h3&gt;10-pin QFN/SON package&lt;/h3&gt;
Package Type: SON&lt;br&gt;
Package Drawing: DRC&lt;Br&gt;
Pitch: 0.5mm&lt;br&gt;
Overall Dimensions: 3.15x3.15mm&lt;br&gt;
Pins: 10 (+1 exposed heatsink pin)&lt;br&gt;
&lt;br&gt;Related ICs:&lt;ul&gt;&lt;li&gt; TI's BQ2402x - http://focus.ti.com/lit/ds/symlink/bq24023.pdf&lt;br&gt;
&lt;/ul&gt;

Last modified: 8/16/10&lt;br&gt;
&lt;B&gt;Unproven!!!&lt;/B&gt;&lt;br&gt;</description>
</package>
<package name="DC-DC_CONVERTER">
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="MULTIWATT15">
<description>Multiwatt15V package for the L298 dual full bridge driver</description>
</package>
<package name="MULTIWATT15_6400BGHEATSINK">
</package>
<package name="POWERSO20">
</package>
<package name="HTSSOP28">
</package>
<package name="MSOP-8">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="DPAK">
</package>
<package name="SOT23-3">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="MSOP-8-EP">
</package>
<package name="TSSOP-16">
</package>
<package name="TO-220-11LEAD">
<description>TO-220 11 Pin Package</description>
</package>
<package name="TO-PMOD-7">
<description>7-Lead package for National voltage switchers (LMZ14203)</description>
</package>
<package name="Q5-DD">
<description>&lt;b&gt;Q5-DD&lt;/b&gt;</description>
</package>
<package name="MSOP-10-GNDPAD">
<description>10-lead MSOP w/ center GND pad</description>
</package>
<package name="TDFN-8">
<description>TDFN - 8pin, 2mmx3mm</description>
</package>
<package name="8-TDFN-EP">
<description>TDFN - 8pin, 2mmx3mm</description>
</package>
<package name="14-TDFN">
</package>
<package name="MSOP-10">
</package>
<package name="SO-24W">
</package>
<package name="Q5-DD_SPX29300">
</package>
<package name="PTC">
</package>
<package name="PTC-1206">
</package>
<package name="0603">
</package>
<package name="MULTIWATT15_YB324GHEATSINK">
</package>
<package name="MULTIWATT15_6400BGHEATSINK_2">
</package>
<package name="SSOP24">
</package>
<package name="QFN16-4X4">
<description>&lt;b&gt;16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9mm Body [QFN]&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41203E.pdf</description>
</package>
<package name="QFN-10_PAD">
</package>
<package name="TRANSFORMER">
</package>
<package name="TRANSFORMER_SMD">
<description>TTC-5023</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO018">
</package>
<package name="SO18L">
</package>
<package name="VNH2SP30">
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="TO220-IGO">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="TO-220-ALT">
</package>
<package name="TO220-ADJ">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="V-REG_DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 369C-01&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
</package>
<package name="D2PACK/A">
<description>&lt;h3&gt;D&lt;sup&gt;2&lt;/sup&gt;PAK/A V-reg Package&lt;/h3&gt;
3-pins w/ tab&lt;br&gt;&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;&lt;br&gt;&lt;br&gt;
&lt;b&gt;Used on:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;LD1085xx Adjustable 3A Regulator
&lt;/ul&gt;</description>
</package>
<package name="SC70">
</package>
<package name="DPAK-5">
<description>DPAK 5, center lead crop, case 175AA</description>
</package>
<package name="QFN-28-5MM">
</package>
<package name="QFN16-3X3MM">
<description>3mm x 3mm QFN 16 pin</description>
</package>
<package name="WSON-8-PAD">
</package>
</packages>
<symbols>
<symbol name="ADM1087">
<pin name="ENIN"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="ENOUT"/>
<pin name="CEXT"/>
<pin name="VCC"/>
</symbol>
<symbol name="BD10KA5WF-E2">
<pin name="OUT"/>
<pin name="VCC"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="CTL"/>
</symbol>
<symbol name="BQ24022">
<pin name="AC"/>
<pin name="USB"/>
<pin name="STAT1"/>
<pin name="STAT2"/>
<pin name="GND"/>
<pin name="ISET1"/>
<pin name="ISET2"/>
<pin name="~PG"/>
<pin name="~CE"/>
<pin name="OUT"/>
<pin name="ETP"/>
</symbol>
<symbol name="DC-DC_CONVERTER">
<pin name="VIN"/>
<pin name="GND1"/>
<pin name="ON/OFF"/>
<pin name="PGOOD"/>
<pin name="SEQ"/>
<pin name="VOUT"/>
<pin name="SENSE"/>
<pin name="TRIM"/>
<pin name="GND2"/>
</symbol>
<symbol name="HV826MG_BACKLIGHT">
<pin name="RSW"/>
<pin name="VA"/>
<pin name="VCC"/>
<pin name="VB"/>
<pin name="CS"/>
<pin name="LX"/>
<pin name="REL" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="L298">
<pin name="OUT1"/>
<pin name="VS"/>
<pin name="ENA"/>
<pin name="GND"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="OUT4"/>
<pin name="CSA"/>
<pin name="OUT2"/>
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="VLS"/>
<pin name="ENB"/>
<pin name="OUT3"/>
<pin name="CSB"/>
</symbol>
<symbol name="L298_BRIDGE_DRIVER">
<pin name="GND@1"/>
<pin name="SENSE_A"/>
<pin name="NC@3"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="VS"/>
<pin name="IN1"/>
<pin name="ENA"/>
<pin name="IN2"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="VSS"/>
<pin name="IN3"/>
<pin name="ENB"/>
<pin name="IN4"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="NC@18"/>
<pin name="SENSE_B"/>
<pin name="GND@20"/>
</symbol>
<symbol name="L6470">
<pin name="BUSYN/SYNC"/>
<pin name="DGND"/>
<pin name="PGNDB"/>
<pin name="PGNDA"/>
<pin name="AGND"/>
<pin name="OSCOUT"/>
<pin name="OSCIN"/>
<pin name="FLAGN"/>
<pin name="STCK"/>
<pin name="STBYN/RESETN"/>
<pin name="CSN"/>
<pin name="CK"/>
<pin name="SDI"/>
<pin name="SDO"/>
<pin name="VSA"/>
<pin name="VSB"/>
<pin name="OUT1A"/>
<pin name="OUT2A"/>
<pin name="OUT1B"/>
<pin name="OUT2B"/>
<pin name="VDD"/>
<pin name="CP"/>
<pin name="VBOOT"/>
<pin name="VREG"/>
<pin name="SW"/>
<pin name="ADCIN"/>
<pin name="VSB2"/>
<pin name="VSA2"/>
<pin name="EPAD"/>
</symbol>
<symbol name="LM2621">
<pin name="PGND"/>
<pin name="EN"/>
<pin name="FREQ"/>
<pin name="FB"/>
<pin name="SGND"/>
<pin name="VDD"/>
<pin name="BOOT"/>
<pin name="SW"/>
</symbol>
<symbol name="LM2931">
<pin name="OUT"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="ADJ"/>
<pin name="INH"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="IN"/>
</symbol>
<symbol name="LM2931_FIXED">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="LM3480IM4">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="LM4128-2.5VREF">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="LM4871">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="BYPASS"/>
<pin name="SHUTDWN"/>
<pin name="V02"/>
<pin name="V01"/>
</symbol>
<symbol name="LM5007">
<pin name="SW"/>
<pin name="BST"/>
<pin name="RCL"/>
<pin name="RTN"/>
<pin name="FB"/>
<pin name="RON"/>
<pin name="VCC"/>
<pin name="VIN"/>
<pin name="EP"/>
</symbol>
<symbol name="LM5574">
<pin name="VCC"/>
<pin name="SD"/>
<pin name="VIN"/>
<pin name="SYNC"/>
<pin name="COMP"/>
<pin name="FB"/>
<pin name="RT"/>
<pin name="RAMP"/>
<pin name="AGND"/>
<pin name="SS"/>
<pin name="OUT"/>
<pin name="PGND"/>
<pin name="IS"/>
<pin name="SW"/>
<pin name="PRE"/>
<pin name="BST"/>
</symbol>
<symbol name="LMD1820X">
<pin name="BS1"/>
<pin name="OUT1"/>
<pin name="DIR"/>
<pin name="BRK"/>
<pin name="PWM"/>
<pin name="PWR"/>
<pin name="PGND"/>
<pin name="SGND"/>
<pin name="TF"/>
<pin name="OUT2"/>
<pin name="BS2"/>
</symbol>
<symbol name="LMZ14203">
<pin name="VIN"/>
<pin name="RON"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="SS"/>
<pin name="FB"/>
<pin name="VOUT"/>
<pin name="EP"/>
</symbol>
<symbol name="LT1528">
<pin name="OUT"/>
<pin name="SENSE"/>
<pin name="GND"/>
<pin name="SHDN"/>
<pin name="IN"/>
</symbol>
<symbol name="LTC3588">
<pin name="PZ1"/>
<pin name="PZ2"/>
<pin name="CAP"/>
<pin name="VIN"/>
<pin name="SW"/>
<pin name="VOUT"/>
<pin name="VIN2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="PGOOD"/>
<pin name="GND"/>
</symbol>
<symbol name="MAX1555">
<pin name="USB"/>
<pin name="GND"/>
<pin name="CHG"/>
<pin name="BATT"/>
<pin name="DC"/>
</symbol>
<symbol name="MAX1704X">
<pin name="CTG"/>
<pin name="CELL"/>
<pin name="VDD"/>
<pin name="GND@4"/>
<pin name="ALT"/>
<pin name="QST"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND@EP"/>
</symbol>
<symbol name="MAX98300">
<pin name="VDD" direction="pwr"/>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GAIN" direction="pwr"/>
</symbol>
<symbol name="MAX98306">
<pin name="VDD@2" direction="pwr"/>
<pin name="INL+"/>
<pin name="INL-"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OUTL+"/>
<pin name="OUTL-"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GAIN" direction="pas"/>
<pin name="INR+"/>
<pin name="INR-"/>
<pin name="OUTR+"/>
<pin name="OUTR-"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
</symbol>
<symbol name="MC34063">
<pin name="DVR"/>
<pin name="COMP"/>
<pin name="TC"/>
<pin name="SWC"/>
<pin name="GND"/>
<pin name="SWE"/>
<pin name="VCC"/>
<pin name="SEN"/>
</symbol>
<symbol name="MCP73842">
<pin name="SENSE"/>
<pin name="VDD"/>
<pin name="STAT1"/>
<pin name="EN"/>
<pin name="TIMER"/>
<pin name="VSS"/>
<pin name="VBAT"/>
<pin name="DRV"/>
</symbol>
<symbol name="MCP73831">
<pin name="VIN" direction="pwr"/>
<pin name="STAT" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PROG" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MCP73833">
<pin name="VDD@1"/>
<pin name="VDD@2"/>
<pin name="STAT1"/>
<pin name="STAT2"/>
<pin name="VSS"/>
<pin name="PROG"/>
<pin name="~PG"/>
<pin name="THERM"/>
<pin name="VBAT@1"/>
<pin name="VBAT@2"/>
</symbol>
<symbol name="MIC2571-1">
<pin name="IN"/>
<pin name="GND"/>
<pin name="SW"/>
<pin name="2.85V"/>
<pin name="3.3V"/>
<pin name="5V"/>
<pin name="SYNC"/>
</symbol>
<symbol name="NJM2670">
<pin name="NC@1" direction="in"/>
<pin name="SENSEA"/>
<pin name="INA1"/>
<pin name="ENABLEA"/>
<pin name="GND@2"/>
<pin name="INB1"/>
<pin name="ENABLEB"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="TSDARM"/>
<pin name="INB2"/>
<pin name="GND@3"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OUTA1" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="OUTA2" direction="pwr"/>
<pin name="NC@4"/>
<pin name="INA2"/>
<pin name="VCC"/>
<pin name="VSA"/>
<pin name="OUTB1"/>
<pin name="SENSEB"/>
<pin name="OUTB2"/>
<pin name="VSB"/>
</symbol>
<symbol name="PQ1CY1032Z">
<pin name="VIN"/>
<pin name="VOUT"/>
<pin name="GND"/>
<pin name="ADJ"/>
<pin name="VS"/>
</symbol>
<symbol name="PTC">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="SPX29300">
<pin name="ENABLE"/>
<pin name="VIN"/>
<pin name="GND@1"/>
<pin name="VOUT"/>
<pin name="ADJUST"/>
<pin name="GND@0"/>
</symbol>
<symbol name="STA540">
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="IN3"/>
<pin name="SVR"/>
<pin name="IN4"/>
<pin name="P-GND"/>
<pin name="S-GND"/>
<pin name="DIAG"/>
<pin name="OUT4"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="STBY"/>
</symbol>
<symbol name="TB6612FNG">
<pin name="A01@1"/>
<pin name="A01@2"/>
<pin name="PGND1@3"/>
<pin name="PGND1@4"/>
<pin name="A02@5"/>
<pin name="A02@6"/>
<pin name="B02@7"/>
<pin name="B02@8"/>
<pin name="PGND2@9"/>
<pin name="PGND2@10"/>
<pin name="B01@11"/>
<pin name="B01@12"/>
<pin name="VM2"/>
<pin name="VM3"/>
<pin name="PWMB"/>
<pin name="BIN2"/>
<pin name="BIN1"/>
<pin name="GND"/>
<pin name="STBY"/>
<pin name="VCC"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="PWMA"/>
<pin name="VM1"/>
</symbol>
<symbol name="TPS6211*">
<pin name="AGND" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="LBI" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="PG" direction="out"/>
<pin name="PGND@1" direction="pwr"/>
<pin name="PGND@2" direction="pwr"/>
<pin name="PWPD" direction="pwr"/>
<pin name="SW@1" direction="out"/>
<pin name="SW@2" direction="out"/>
<pin name="SYNC" direction="in"/>
<pin name="VIN@1" direction="pwr"/>
<pin name="VIN@2" direction="pwr"/>
<pin name="VINA" direction="pwr"/>
</symbol>
<symbol name="TPS61200">
<pin name="EN" direction="in"/>
<pin name="FB" direction="pas"/>
<pin name="GND" direction="sup"/>
<pin name="L" direction="pas"/>
<pin name="PAD@1" direction="sup"/>
<pin name="PAD@2" direction="sup"/>
<pin name="PAD@3" direction="sup"/>
<pin name="PAD@4" direction="sup"/>
<pin name="PAD@5" direction="sup"/>
<pin name="PGND" direction="sup"/>
<pin name="PS" direction="in"/>
<pin name="UVLO" direction="pas"/>
<pin name="VAUX" direction="pas"/>
<pin name="VIN" direction="sup"/>
<pin name="VOUT" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER">
<pin name="1"/>
<pin name="4"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="ULN2803">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
</symbol>
<symbol name="VNH2SP30">
<pin name="OUTB@15"/>
<pin name="INB"/>
<pin name="VCC@13"/>
<pin name="EN/DIAB"/>
<pin name="CS"/>
<pin name="PWM"/>
<pin name="EN/DIAA"/>
<pin name="INA"/>
<pin name="VCC@3"/>
<pin name="OUTA@1"/>
<pin name="OUTA@30"/>
<pin name="GNDA@28"/>
<pin name="GNDA@27"/>
<pin name="GNDA@26"/>
<pin name="OUTA@25"/>
<pin name="VCC@23"/>
<pin name="OUTB@21"/>
<pin name="GNDB@20"/>
<pin name="GNDB@19"/>
<pin name="GNDB@18"/>
<pin name="OUTB@16"/>
<pin name="VCC@SLUG1"/>
<pin name="OUTA@SLUG3"/>
<pin name="OUTB@SLUG2"/>
</symbol>
<symbol name="MIC5216">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="VOUT"/>
<pin name="FLAG"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
</symbol>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="78ADJ-2">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
</symbol>
<symbol name="V-REG-LDO">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="BP" direction="in"/>
</symbol>
<symbol name="V-REG-LDO-ADJ">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="ADJ" direction="in"/>
</symbol>
<symbol name="78ADJ-3">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND"/>
<pin name="EN"/>
</symbol>
<symbol name="NCP1400">
<pin name="LX" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="in"/>
</symbol>
<symbol name="TPS61040">
<pin name="EN"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="SW"/>
<pin name="FB"/>
</symbol>
<symbol name="TPS76433DBVT">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="in"/>
</symbol>
<symbol name="ZXLD1360">
<pin name="LX"/>
<pin name="GND"/>
<pin name="ADJ"/>
<pin name="SENSE"/>
<pin name="VIN"/>
</symbol>
<symbol name="A4983">
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="DIR" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND_PAD" direction="pwr"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="MS3" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="OUT1A"/>
<pin name="OUT1B"/>
<pin name="OUT2A"/>
<pin name="OUT2B"/>
<pin name="REF"/>
<pin name="RESET" direction="in"/>
<pin name="ROSC"/>
<pin name="SENSE1"/>
<pin name="SENSE2"/>
<pin name="SLEEP" direction="in"/>
<pin name="STEP" direction="in"/>
<pin name="VBB1"/>
<pin name="VBB2"/>
<pin name="VCP"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREG"/>
</symbol>
<symbol name="TPS62143">
<pin name="PVIN@11"/>
<pin name="PVIN@12"/>
<pin name="AVIN"/>
<pin name="EN"/>
<pin name="FSW"/>
<pin name="PGND@15"/>
<pin name="PGND@16"/>
<pin name="EXT"/>
<pin name="SW@1"/>
<pin name="SW@2"/>
<pin name="SW@3"/>
<pin name="PG"/>
<pin name="VOS"/>
<pin name="SS_TR"/>
<pin name="AGND"/>
<pin name="DEF"/>
<pin name="FB"/>
</symbol>
<symbol name="HV816">
<pin name="VDD"/>
<pin name="REL-OSC"/>
<pin name="RSW-OSC"/>
<pin name="RSLEW-OUT"/>
<pin name="GND"/>
<pin name="HVGND"/>
<pin name="SEL"/>
<pin name="EN"/>
<pin name="VB"/>
<pin name="VA"/>
<pin name="CS"/>
<pin name="VREG"/>
<pin name="VOUT"/>
<pin name="VDRIVE"/>
<pin name="LX"/>
<pin name="GATE"/>
</symbol>
<symbol name="ADP160">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="VOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="MIC5216-1">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="VOUT"/>
<pin name="FLAG"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
</symbol>
<symbol name="TPS62172">
<description>&lt;h3&gt;TPS62172&lt;/h3&gt;

3-17V 0.5A Step-Down Converter w/ DCS-Control</description>
<pin name="VIN"/>
<pin name="EN"/>
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="SW"/>
<pin name="VOS"/>
<pin name="PG"/>
<pin name="FB"/>
<pin name="PAD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADM1087">
<description>Power supply sequencer</description>
<gates>
<gate name="G$1" symbol="ADM1087"/>
</gates>
<devices>
<device name="SC-70" package="SC-70">
<connects>
<connect gate="G$1" pin="CEXT" pad="5"/>
<connect gate="G$1" pin="ENIN" pad="1"/>
<connect gate="G$1" pin="ENOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD10KA5WF-E2">
<description>500mA LDO, 1.0V SO-8 (COM-10827)</description>
<gates>
<gate name="G$1" symbol="BD10KA5WF-E2"/>
</gates>
<devices>
<device name="" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CTL" pad="5"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24022" prefix="U">
<description>Single-chip, Li-ion and Li-pol charger IC with autonomous USB-port and AC-adapter supply management.&lt;br&gt;
Datasheet: http://focus.ti.com/lit/ds/symlink/bq24022.pdf&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;&lt;br&gt;
Last modified: 8/16/10&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="BQ24022"/>
</gates>
<devices>
<device name="" package="DRC-10">
<connects>
<connect gate="G$1" pin="AC" pad="1"/>
<connect gate="G$1" pin="ETP" pad="EP"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISET1" pad="6"/>
<connect gate="G$1" pin="ISET2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="USB" pad="2"/>
<connect gate="G$1" pin="~CE" pad="9"/>
<connect gate="G$1" pin="~PG" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC_CONVERTER">
<description>APTS006A0X-SRZ Step-down 6A variable voltage switching module (TOL-09275)</description>
<gates>
<gate name="G$1" symbol="DC-DC_CONVERTER"/>
</gates>
<devices>
<device name="" package="DC-DC_CONVERTER">
<connects>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="ON/OFF" pad="1"/>
<connect gate="G$1" pin="PGOOD" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="SEQ" pad="9"/>
<connect gate="G$1" pin="TRIM" pad="6"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HV826MG_BACKLIGHT">
<description>Small EL backlight driver for the CFAX 128x64 graphical display.</description>
<gates>
<gate name="G$1" symbol="HV826MG_BACKLIGHT"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="REL" pad="3"/>
<connect gate="G$1" pin="RSW" pad="2"/>
<connect gate="G$1" pin="VA" pad="8"/>
<connect gate="G$1" pin="VB" pad="7"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298" prefix="U">
<description>L298 Dual Full Bridge Driver</description>
<gates>
<gate name="G$1" symbol="L298"/>
</gates>
<devices>
<device name="" package="MULTIWATT15">
<connects>
<connect gate="G$1" pin="CSA" pad="1"/>
<connect gate="G$1" pin="CSB" pad="15"/>
<connect gate="G$1" pin="ENA" pad="6"/>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="VLS" pad="9"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HEATSINK" package="MULTIWATT15_6400BGHEATSINK">
<connects>
<connect gate="G$1" pin="CSA" pad="1"/>
<connect gate="G$1" pin="CSB" pad="15"/>
<connect gate="G$1" pin="ENA" pad="6"/>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="VLS" pad="9"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298_BRIDGE_DRIVER">
<description>Full-bridge power driver IC</description>
<gates>
<gate name="G$1" symbol="L298_BRIDGE_DRIVER"/>
</gates>
<devices>
<device name="" package="POWERSO20">
<connects>
<connect gate="G$1" pin="ENA" pad="8"/>
<connect gate="G$1" pin="ENB" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="13"/>
<connect gate="G$1" pin="IN4" pad="15"/>
<connect gate="G$1" pin="NC@18" pad="18"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="OUT3" pad="16"/>
<connect gate="G$1" pin="OUT4" pad="17"/>
<connect gate="G$1" pin="SENSE_A" pad="2"/>
<connect gate="G$1" pin="SENSE_B" pad="19"/>
<connect gate="G$1" pin="VS" pad="6"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6470" prefix="U" uservalue="yes">
<description>3A RMS/7A peak bipolar stepper motor driver with SPI control&lt;br&gt;
and step input in HTSSOP-28 package.&lt;br&gt;
IC-10648</description>
<gates>
<gate name="G$1" symbol="L6470"/>
</gates>
<devices>
<device name="" package="HTSSOP28">
<connects>
<connect gate="G$1" pin="ADCIN" pad="5"/>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="BUSYN/SYNC" pad="22"/>
<connect gate="G$1" pin="CK" pad="19"/>
<connect gate="G$1" pin="CP" pad="10"/>
<connect gate="G$1" pin="CSN" pad="23"/>
<connect gate="G$1" pin="DGND" pad="21"/>
<connect gate="G$1" pin="EPAD" pad="29"/>
<connect gate="G$1" pin="FLAGN" pad="24"/>
<connect gate="G$1" pin="OSCIN" pad="7"/>
<connect gate="G$1" pin="OSCOUT" pad="8"/>
<connect gate="G$1" pin="OUT1A" pad="1"/>
<connect gate="G$1" pin="OUT1B" pad="14"/>
<connect gate="G$1" pin="OUT2A" pad="28"/>
<connect gate="G$1" pin="OUT2B" pad="15"/>
<connect gate="G$1" pin="PGNDA" pad="27"/>
<connect gate="G$1" pin="PGNDB" pad="13"/>
<connect gate="G$1" pin="SDI" pad="20"/>
<connect gate="G$1" pin="SDO" pad="18"/>
<connect gate="G$1" pin="STBYN/RESETN" pad="3"/>
<connect gate="G$1" pin="STCK" pad="25"/>
<connect gate="G$1" pin="SW" pad="4"/>
<connect gate="G$1" pin="VBOOT" pad="11"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VREG" pad="6"/>
<connect gate="G$1" pin="VSA" pad="2"/>
<connect gate="G$1" pin="VSA2" pad="26"/>
<connect gate="G$1" pin="VSB" pad="12"/>
<connect gate="G$1" pin="VSB2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10648"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2621">
<description>Step-up switching regulator IC</description>
<gates>
<gate name="G$1" symbol="LM2621"/>
</gates>
<devices>
<device name="SMD" package="MSOP-8">
<connects>
<connect gate="G$1" pin="BOOT" pad="7"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="FREQ" pad="3"/>
<connect gate="G$1" pin="PGND" pad="1"/>
<connect gate="G$1" pin="SGND" pad="5"/>
<connect gate="G$1" pin="SW" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931">
<description>LDO regulator with reverse battery protection- very durable!</description>
<gates>
<gate name="G$1" symbol="LM2931"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="INH" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931_FIXED">
<description>LDO regulator with reverse battery protection- very durable!</description>
<gates>
<gate name="G$1" symbol="LM2931_FIXED"/>
</gates>
<devices>
<device name="" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3480IM4">
<description>Small package linear regulator</description>
<gates>
<gate name="G$1" symbol="LM3480IM4"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4128-2.5VREF">
<description>.1% accurate low-current voltage reference</description>
<gates>
<gate name="G$1" symbol="LM4128-2.5VREF"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4871">
<description>3W audio amplifier</description>
<gates>
<gate name="G$1" symbol="LM4871"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="BYPASS" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="SHUTDWN" pad="1"/>
<connect gate="G$1" pin="V01" pad="5"/>
<connect gate="G$1" pin="V02" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5007" prefix="U">
<description>High Voltage (80V) Step-down switching regulator&lt;br&gt;

http://www.national.com/ds/LM/LM5007.pdf&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LM5007"/>
</gates>
<devices>
<device name="" package="MSOP-8-EP">
<connects>
<connect gate="G$1" pin="BST" pad="2"/>
<connect gate="G$1" pin="EP" pad="EP"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="RCL" pad="3"/>
<connect gate="G$1" pin="RON" pad="6"/>
<connect gate="G$1" pin="RTN" pad="4"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5574" prefix="U">
<description>Simple Switcher 75V, 0.5A Step-down switching regulator</description>
<gates>
<gate name="G$1" symbol="LM5574"/>
</gates>
<devices>
<device name="" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="BST" pad="16"/>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="IS" pad="13"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="PGND" pad="12"/>
<connect gate="G$1" pin="PRE" pad="15"/>
<connect gate="G$1" pin="RAMP" pad="8"/>
<connect gate="G$1" pin="RT" pad="7"/>
<connect gate="G$1" pin="SD" pad="2"/>
<connect gate="G$1" pin="SS" pad="10"/>
<connect gate="G$1" pin="SW" pad="14"/>
<connect gate="G$1" pin="SYNC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMD1820X">
<description>LMD1820X H-Bridge - BOB-00747</description>
<gates>
<gate name="G$1" symbol="LMD1820X"/>
</gates>
<devices>
<device name="" package="TO-220-11LEAD">
<connects>
<connect gate="G$1" pin="BRK" pad="4"/>
<connect gate="G$1" pin="BS1" pad="1"/>
<connect gate="G$1" pin="BS2" pad="11"/>
<connect gate="G$1" pin="DIR" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="PGND" pad="7"/>
<connect gate="G$1" pin="PWM" pad="5"/>
<connect gate="G$1" pin="PWR" pad="6"/>
<connect gate="G$1" pin="SGND" pad="8"/>
<connect gate="G$1" pin="TF" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMZ14203" prefix="U">
<description>3A, Simple Switcher Power Module with 42V Maximum Input</description>
<gates>
<gate name="G$1" symbol="LMZ14203"/>
</gates>
<devices>
<device name="" package="TO-PMOD-7">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="EP" pad="EP"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1528">
<description>High current voltage regulator commonly used with GM862 cellular module. Spark Fun Electronics SKU : COM-00311. Footprint may need to have the large paste aperature reduced.</description>
<gates>
<gate name="G$1" symbol="LT1528"/>
</gates>
<devices>
<device name="" package="Q5-DD">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3588" prefix="U">
<description>Energy Harvesting Power Supply</description>
<gates>
<gate name="G$1" symbol="LTC3588"/>
</gates>
<devices>
<device name="_" package="MSOP-10-GNDPAD">
<connects>
<connect gate="G$1" pin="CAP" pad="3"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PGOOD" pad="10"/>
<connect gate="G$1" pin="PZ1" pad="1"/>
<connect gate="G$1" pin="PZ2" pad="2"/>
<connect gate="G$1" pin="SW" pad="5"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VIN2" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1555" prefix="U">
<description>&lt;b&gt;MAX1555 Lithium Charger IC&lt;/b&gt;
SOT-23 Lithium Polymer charging IC. Schematic element and footprint proven. Spark Fun Electronics SKU : COM-00674</description>
<gates>
<gate name="G$1" symbol="MAX1555"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BATT" pad="5"/>
<connect gate="G$1" pin="CHG" pad="3"/>
<connect gate="G$1" pin="DC" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="USB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1704X" prefix="U">
<description>MAX17043/MAX17044: Battery Fuel Guage (43 is 1cell, 44 is 2cell)</description>
<gates>
<gate name="G$1" symbol="MAX1704X"/>
</gates>
<devices>
<device name="" package="TDFN-8">
<connects>
<connect gate="G$1" pin="ALT" pad="5"/>
<connect gate="G$1" pin="CELL" pad="2"/>
<connect gate="G$1" pin="CTG" pad="1"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@EP" pad="EP"/>
<connect gate="G$1" pin="QST" pad="6"/>
<connect gate="G$1" pin="SCL" pad="7"/>
<connect gate="G$1" pin="SDA" pad="8"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX98300" prefix="U" uservalue="yes">
<description>&lt;b&gt;Mono 2.6W Class D Amplifier&lt;/b&gt;&lt;p&gt;

Datasheet: &lt;a href="http://datasheets.maxim-ic.com/en/ds/MAX98300.pdf"&gt;http://datasheets.maxim-ic.com/en/ds/MAX98300.pdf&lt;/a&gt;&lt;p&gt;

The MAX98300 mono 2.6W Class D amplifier provides
Class AB audio performance with Class D efficiency.
This device offers five selectable gain settings (0dB,
3dB, 6dB, 9dB, and 12dB) set by a single gain-select
input (GAIN).
Active emissions-limiting edge-rate and overshoot control
circuitry greatly reduces EMI. A patented filterless
spread-spectrum modulation scheme eliminates the need
for output filtering found in traditional Class D devices.
These features reduce application component count.
The MAX98300 industry-leading 0.78mA at 3.7V (1.1mA
at 5V) quiescent current extends battery life in portable
applications.
The MAX98300 is available in an 8-pin TDFN-EP (2mm
x 2mm x 0.8mm) and a 9-bump (1.2mm x 1.2mm) WLP.
Both packages are specified over the extended -40NC to
+85NC temperature range.</description>
<gates>
<gate name="G$1" symbol="MAX98300"/>
</gates>
<devices>
<device name="ETA+" package="8-TDFN-EP">
<connects>
<connect gate="G$1" pin="GAIN" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="IN+" pad="1"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="7"/>
<connect gate="G$1" pin="OUT-" pad="6"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX98306" prefix="U">
<description>&lt;b&gt;Stereo 3.7W Class D Amplifier&lt;/b&gt;&lt;p&gt;

Datasheet: &lt;a href="http://datasheets.maxim-ic.com/en/ds/MAX98306.pdf"&gt;http://datasheets.maxim-ic.com/en/ds/MAX98306.pdf&lt;/a&gt;&lt;p&gt;

The MAX98306 stereo 3.7W Class D amplifier provides
Class AB audio performance with Class D efficiency.
This device offers five selectable gain settings (6dB,
9dB, 12dB, 15dB, and 18dB) set by a single gain-select
input (GAIN).
Active emissions limiting, edge-rate, and overshoot control
circuitry combined with a filterless spread-spectrum
modulation scheme (SSM) provide excellent EMI performance
while eliminating the need for output filtering found
in traditional Class D devices. These features reduce
application component count.
The IC's 2.0mA quiescent current with a 3.7V supply
extends battery life in portable applications.
The IC is available in a 14-pin TDFN (3mm x 3mm x
0.75mm) package specified over the extended -40NC to
+85NC temperature range.</description>
<gates>
<gate name="G$1" symbol="MAX98306"/>
</gates>
<devices>
<device name="ETD+" package="14-TDFN">
<connects>
<connect gate="G$1" pin="GAIN" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="GND@3" pad="15"/>
<connect gate="G$1" pin="INL+" pad="3"/>
<connect gate="G$1" pin="INL-" pad="4"/>
<connect gate="G$1" pin="INR+" pad="7"/>
<connect gate="G$1" pin="INR-" pad="6"/>
<connect gate="G$1" pin="OUTL+" pad="13"/>
<connect gate="G$1" pin="OUTL-" pad="14"/>
<connect gate="G$1" pin="OUTR+" pad="10"/>
<connect gate="G$1" pin="OUTR-" pad="9"/>
<connect gate="G$1" pin="SHDN" pad="2"/>
<connect gate="G$1" pin="VDD@1" pad="11"/>
<connect gate="G$1" pin="VDD@2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34063" prefix="U">
<description>Jellybean switching supply controller</description>
<gates>
<gate name="G$1" symbol="MC34063"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="DVR" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SEN" pad="7"/>
<connect gate="G$1" pin="SWC" pad="1"/>
<connect gate="G$1" pin="SWE" pad="2"/>
<connect gate="G$1" pin="TC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP7384XX" prefix="U">
<description>Li-Ion charge controller family from Microchip</description>
<gates>
<gate name="G$1" symbol="MCP73842"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="DRV" pad="8"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="TIMER" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="7"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73831" prefix="U">
<description>Miniature single cell, fully integrated Li-Ion, Li-polymer charge management controller&lt;br&gt;
http://ww1.microchip.com/downloads/en/DeviceDoc/21984a.pdf&lt;br&gt;
IC-09995</description>
<gates>
<gate name="G$1" symbol="MCP73831"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="STAT" pad="1"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09995"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73833" prefix="U">
<description>Stand-alone Linear Li-ion/Li-polymer Charge Management Controller&lt;br&gt;
Packages: DFN-10, MSOP-10&lt;br&gt;
&lt;br&gt;
Last modified: 8/17/10&lt;br&gt;
&lt;b&gt;Unproven!&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MCP73833"/>
</gates>
<devices>
<device name="" package="MSOP-10">
<connects>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="THERM" pad="8"/>
<connect gate="G$1" pin="VBAT@1" pad="9"/>
<connect gate="G$1" pin="VBAT@2" pad="10"/>
<connect gate="G$1" pin="VDD@1" pad="1"/>
<connect gate="G$1" pin="VDD@2" pad="2"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="~PG" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC2571" prefix="U">
<description>Single Cell Switching Regulator - MIC2571</description>
<gates>
<gate name="G$1" symbol="MIC2571-1"/>
</gates>
<devices>
<device name="SMD" package="MSOP-8">
<connects>
<connect gate="G$1" pin="2.85V" pad="6"/>
<connect gate="G$1" pin="3.3V" pad="5"/>
<connect gate="G$1" pin="5V" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="SYNC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NJM2670">
<description>Dual H-bridge driver</description>
<gates>
<gate name="G$1" symbol="NJM2670"/>
</gates>
<devices>
<device name="SMD" package="SO-24W">
<connects>
<connect gate="G$1" pin="ENABLEA" pad="3"/>
<connect gate="G$1" pin="ENABLEB" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="18"/>
<connect gate="G$1" pin="GND@4" pad="19"/>
<connect gate="G$1" pin="INA1" pad="2"/>
<connect gate="G$1" pin="INA2" pad="22"/>
<connect gate="G$1" pin="INB1" pad="8"/>
<connect gate="G$1" pin="INB2" pad="17"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="10"/>
<connect gate="G$1" pin="NC@3" pad="15"/>
<connect gate="G$1" pin="NC@4" pad="21"/>
<connect gate="G$1" pin="OUTA1" pad="5"/>
<connect gate="G$1" pin="OUTA2" pad="20"/>
<connect gate="G$1" pin="OUTB1" pad="11"/>
<connect gate="G$1" pin="OUTB2" pad="14"/>
<connect gate="G$1" pin="SENSEA" pad="1"/>
<connect gate="G$1" pin="SENSEB" pad="12"/>
<connect gate="G$1" pin="TSDARM" pad="16"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VSA" pad="24"/>
<connect gate="G$1" pin="VSB" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PQ1CY1032Z">
<description>3.5A Switching Regulator</description>
<gates>
<gate name="G$1" symbol="PQ1CY1032Z"/>
</gates>
<devices>
<device name="" package="Q5-DD_SPX29300">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTC" prefix="F">
<description>&lt;b&gt;Resettable Fuse PTC&lt;/b&gt;
Resettable Fuse. Spark Fun Electronics SKU : COM-08357</description>
<gates>
<gate name="G$1" symbol="PTC"/>
</gates>
<devices>
<device name="PTH" package="PTC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="PTC-1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPX29302">
<description>3A LDO regulator</description>
<gates>
<gate name="G$1" symbol="SPX29300"/>
</gates>
<devices>
<device name="" package="Q5-DD_SPX29300">
<connects>
<connect gate="G$1" pin="ADJUST" pad="5"/>
<connect gate="G$1" pin="ENABLE" pad="1"/>
<connect gate="G$1" pin="GND@0" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA540">
<description>Multiwatt package for L298 bridge driver</description>
<gates>
<gate name="G$1" symbol="STA540"/>
</gates>
<devices>
<device name="" package="MULTIWATT15">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W/6400BG_HEATSINK" package="MULTIWATT15_6400BGHEATSINK">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W/YB324G_HEATSINK" package="MULTIWATT15_YB324GHEATSINK">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6400BG_W/SOLDERPOSTS" package="MULTIWATT15_6400BGHEATSINK_2">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TB6621FNG" prefix="U" uservalue="yes">
<description>Toshiba 1A dual motor driver&lt;br&gt;
IC-09363</description>
<gates>
<gate name="G$1" symbol="TB6612FNG"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="A01@1" pad="1"/>
<connect gate="G$1" pin="A01@2" pad="2"/>
<connect gate="G$1" pin="A02@5" pad="5"/>
<connect gate="G$1" pin="A02@6" pad="6"/>
<connect gate="G$1" pin="AIN1" pad="21"/>
<connect gate="G$1" pin="AIN2" pad="22"/>
<connect gate="G$1" pin="B01@11" pad="11"/>
<connect gate="G$1" pin="B01@12" pad="12"/>
<connect gate="G$1" pin="B02@7" pad="7"/>
<connect gate="G$1" pin="B02@8" pad="8"/>
<connect gate="G$1" pin="BIN1" pad="17"/>
<connect gate="G$1" pin="BIN2" pad="16"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="PGND1@3" pad="3"/>
<connect gate="G$1" pin="PGND1@4" pad="4"/>
<connect gate="G$1" pin="PGND2@10" pad="10"/>
<connect gate="G$1" pin="PGND2@9" pad="9"/>
<connect gate="G$1" pin="PWMA" pad="23"/>
<connect gate="G$1" pin="PWMB" pad="15"/>
<connect gate="G$1" pin="STBY" pad="19"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VM1" pad="24"/>
<connect gate="G$1" pin="VM2" pad="13"/>
<connect gate="G$1" pin="VM3" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09363"/>
<attribute name="VALUE" value="TB6612FNG"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6211*" prefix="U">
<description>TPS62112: 1.5A Step-Down Converter</description>
<gates>
<gate name="G$1" symbol="TPS6211*"/>
</gates>
<devices>
<device name="" package="QFN16-4X4">
<connects>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="LBI" pad="7"/>
<connect gate="G$1" pin="LBO" pad="6"/>
<connect gate="G$1" pin="PG" pad="13"/>
<connect gate="G$1" pin="PGND@1" pad="1"/>
<connect gate="G$1" pin="PGND@2" pad="16"/>
<connect gate="G$1" pin="PWPD" pad="EXP"/>
<connect gate="G$1" pin="SW@1" pad="14"/>
<connect gate="G$1" pin="SW@2" pad="15"/>
<connect gate="G$1" pin="SYNC" pad="5"/>
<connect gate="G$1" pin="VIN@1" pad="2"/>
<connect gate="G$1" pin="VIN@2" pad="3"/>
<connect gate="G$1" pin="VINA" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS61200" prefix="U">
<description>DC to DC Booster&lt;br&gt;
IC-10035</description>
<gates>
<gate name="G$1" symbol="TPS61200"/>
</gates>
<devices>
<device name="" package="QFN-10_PAD">
<connects>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="L" pad="3"/>
<connect gate="G$1" pin="PAD@1" pad="15"/>
<connect gate="G$1" pin="PAD@2" pad="11"/>
<connect gate="G$1" pin="PAD@3" pad="12"/>
<connect gate="G$1" pin="PAD@4" pad="13"/>
<connect gate="G$1" pin="PAD@5" pad="14"/>
<connect gate="G$1" pin="PGND" pad="4"/>
<connect gate="G$1" pin="PS" pad="8"/>
<connect gate="G$1" pin="UVLO" pad="7"/>
<connect gate="G$1" pin="VAUX" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10035"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSFORMER">
<description>Small transformers</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER"/>
</gates>
<devices>
<device name="PTH" package="TRANSFORMER">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TRANSFORMER_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULN2803" prefix="ULN2803" uservalue="yes">
<description>&lt;b&gt;Darlington Driver&lt;/b&gt;
ULN2803 Darlington array. 500mA max per channel, 8-channel package. Spark Fun Electronics SKU : COM-00312</description>
<gates>
<gate name="G$1" symbol="ULN2803"/>
</gates>
<devices>
<device name="DIP" package="DIL18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SO018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOICW" package="SO18L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNH2SP30">
<description>30A motor driver IC</description>
<gates>
<gate name="G$1" symbol="VNH2SP30"/>
</gates>
<devices>
<device name="" package="VNH2SP30">
<connects>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="EN/DIAA" pad="6"/>
<connect gate="G$1" pin="EN/DIAB" pad="10"/>
<connect gate="G$1" pin="GNDA@26" pad="26"/>
<connect gate="G$1" pin="GNDA@27" pad="27"/>
<connect gate="G$1" pin="GNDA@28" pad="28"/>
<connect gate="G$1" pin="GNDB@18" pad="18"/>
<connect gate="G$1" pin="GNDB@19" pad="19"/>
<connect gate="G$1" pin="GNDB@20" pad="20"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="11"/>
<connect gate="G$1" pin="OUTA@1" pad="1"/>
<connect gate="G$1" pin="OUTA@25" pad="25"/>
<connect gate="G$1" pin="OUTA@30" pad="30"/>
<connect gate="G$1" pin="OUTA@SLUG3" pad="SLUG3"/>
<connect gate="G$1" pin="OUTB@15" pad="15"/>
<connect gate="G$1" pin="OUTB@16" pad="16"/>
<connect gate="G$1" pin="OUTB@21" pad="21"/>
<connect gate="G$1" pin="OUTB@SLUG2" pad="SLUG2"/>
<connect gate="G$1" pin="PWM" pad="8"/>
<connect gate="G$1" pin="VCC@13" pad="13"/>
<connect gate="G$1" pin="VCC@23" pad="23"/>
<connect gate="G$1" pin="VCC@3" pad="3"/>
<connect gate="G$1" pin="VCC@SLUG1" pad="SLUG1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_78XX" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;
Standard 7805 5V regulator. IGO (Input Ground Output). Spark Fun Electronics SKU : COM-00107</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="SIDE" package="78XXL">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SINK" package="TO220-IGO">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-92" package="TO-92">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-220" package="TO-220-ALT">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_317" prefix="U">
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;
Standard LM317 adjustable voltage regulator. AOI (Adjust Output Input). Google 'LM317 Calculator' for easy to use app to get the two resistor values needed. 240/720 for 5V output. 240/390 for 3.3V output. Spark Fun Electronics SKU : COM-00527</description>
<gates>
<gate name="G$1" symbol="78ADJ-2"/>
</gates>
<devices>
<device name="SINK" package="TO220-ADJ">
<connects>
<connect gate="G$1" pin="ADJ" pad="ADJ"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DPACK" package="V-REG_DPACK">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LD1085" prefix="U">
<description>&lt;h3&gt;LD1085 3A low-drop positive voltage regulator, adjustable&lt;/h3&gt;

The LD1085xx is a low drop voltage regulator able to provide up to 3 A of output current. Dropout is guaranteed at a maximum of 1.2 V at the maximum output current, decreasing at lower loads. The LD1085xx is pin to pin compatible with the older 3-terminal adjustable regulators, but has better performances in term of drop and output tolerance.&lt;br&gt;
&lt;br&gt;
&lt;B&gt;Available Packages&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;D&lt;sup&gt;2&lt;/sup&gt;PAK/A - 3-pin w/ tabs, SMD</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="D2" package="D2PACK/A">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="TAB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LD1117VXX">
<description>LD1117VXX voltage regulator. We carry the 3.3V version (COM-00526) in TO-220 package.</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="78XXL">
<connects>
<connect gate="G$1" pin="GND" pad="IN"/>
<connect gate="G$1" pin="IN" pad="OUT"/>
<connect gate="G$1" pin="OUT" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LDO" prefix="U">
<description>&lt;b&gt;Voltage Regulator LDO&lt;/b&gt;
Standard 150mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5205. BP (by-pass) pin is used to lower output noise with 470pF cap.</description>
<gates>
<gate name="G$1" symbol="V-REG-LDO"/>
</gates>
<devices>
<device name="SMD" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SC70">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LM1117" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator LM1117&lt;/b&gt;
Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MC33269" prefix="U">
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="DT" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MIC2920">
<description>MIC2920A (http://www.micrel.com/_PDF/mic2920.pdf) - 400mA output LDO Regulator</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MIC5219" prefix="U" uservalue="yes">
<description>&lt;b&gt;V_REG MIC5219&lt;/b&gt;
Standard 500mA LDO voltage regulator in SOT-23 layout. Micrel part MIC5219. BP (by-pass) pin is used to lower output noise with 470pF cap,
may be left open.</description>
<gates>
<gate name="G$1" symbol="V-REG-LDO"/>
</gates>
<devices>
<device name="3.3V" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="VREG-09872"/>
<attribute name="VALUE" value="MIC5219 3.3V"/>
</technology>
</technologies>
</device>
<device name="5V" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="VREG-10107"/>
<attribute name="VALUE" value="MIC5219 5V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MIC5235" prefix="U">
<gates>
<gate name="G$1" symbol="V-REG-LDO-ADJ"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_NCP50X" prefix="U">
<description>NCP550x 500mA LDO Voltage Regulator</description>
<gates>
<gate name="G$1" symbol="78ADJ-3"/>
</gates>
<devices>
<device name="" package="DPAK-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="ADJ"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="VIN"/>
<connect gate="G$1" pin="OUT" pad="VOUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_NCP1400" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Switching step-up voltage regulator&lt;/b&gt;
NCP1400 switiching regulator takes single cell AA and outputs 100mA at 3.3V or 5V with minimal number of external components.</description>
<gates>
<gate name="G$1" symbol="NCP1400"/>
</gates>
<devices>
<device name="SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_TPS61040">
<gates>
<gate name="G$1" symbol="TPS61040"/>
</gates>
<devices>
<device name="SMD" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_TPS76433" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator&lt;/b&gt;
Older TI part. LDO 150mA regulator. No output by-pass cap option. See V_REG_LDO for a better part.</description>
<gates>
<gate name="G$1" symbol="TPS76433DBVT"/>
</gates>
<devices>
<device name="SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZXLD1360">
<description>Adjustable constant current switching driver for high-power LEDs</description>
<gates>
<gate name="G$1" symbol="ZXLD1360"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="LX" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="4"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4983" prefix="U">
<description>DMOS Microstepping Driver with Translator</description>
<gates>
<gate name="G$1" symbol="A4983"/>
</gates>
<devices>
<device name="" package="QFN-28-5MM">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_MIC5216" prefix="U">
<description>500mA LDO, MSOP8 for better dissipation</description>
<gates>
<gate name="G$1" symbol="MIC5216-1"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="FLAG" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HV816">
<description>High-drive dimmable EL inverter&lt;br&gt;
Supertex, available in SOW16 and QFN16</description>
<gates>
<gate name="G$1" symbol="HV816"/>
</gates>
<devices>
<device name="K6" package="QFN16-4X4">
<connects>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="EN" pad="9"/>
<connect gate="G$1" pin="GATE" pad="15"/>
<connect gate="G$1" pin="GND" pad="7 EXP"/>
<connect gate="G$1" pin="HVGND" pad="13"/>
<connect gate="G$1" pin="LX" pad="16"/>
<connect gate="G$1" pin="REL-OSC" pad="2"/>
<connect gate="G$1" pin="RSLEW-OUT" pad="8"/>
<connect gate="G$1" pin="RSW-OSC" pad="1"/>
<connect gate="G$1" pin="SEL" pad="3"/>
<connect gate="G$1" pin="VA" pad="10"/>
<connect gate="G$1" pin="VB" pad="11"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VDRIVE" pad="14"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
<connect gate="G$1" pin="VREG" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADP160" prefix="U" uservalue="yes">
<description>Nanopower LDO&lt;br&gt;
Iq less than 1uA for low Iload</description>
<gates>
<gate name="G$1" symbol="ADP160"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="VREG-11306"/>
<attribute name="VALUE" value="ADP160"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6214X" prefix="U">
<description>3-17V, 2A Step Down Converter</description>
<gates>
<gate name="G$1" symbol="TPS62143"/>
</gates>
<devices>
<device name="" package="QFN16-3X3MM">
<connects>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AVIN" pad="10"/>
<connect gate="G$1" pin="DEF" pad="8"/>
<connect gate="G$1" pin="EN" pad="13"/>
<connect gate="G$1" pin="EXT" pad="EXT"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="FSW" pad="7"/>
<connect gate="G$1" pin="PG" pad="4"/>
<connect gate="G$1" pin="PGND@15" pad="15"/>
<connect gate="G$1" pin="PGND@16" pad="16"/>
<connect gate="G$1" pin="PVIN@11" pad="11"/>
<connect gate="G$1" pin="PVIN@12" pad="12"/>
<connect gate="G$1" pin="SS_TR" pad="9"/>
<connect gate="G$1" pin="SW@1" pad="1"/>
<connect gate="G$1" pin="SW@2" pad="2"/>
<connect gate="G$1" pin="SW@3" pad="3"/>
<connect gate="G$1" pin="VOS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS62172" prefix="U">
<description>&lt;h3&gt;Texas Instruments TPS62172&lt;/h3&gt;
3-17V 0.5A Step-Down Converter with DCS control. Available in adjustable and fixed output voltage versions.&lt;br&gt;&lt;br&gt;

Is packaged in an 8-pin WSON package measuring 2 × 2 mm (DSG).&lt;br&gt; &lt;br&gt;

See a 3.3V fixed output version of this chip in action on the &lt;a href="https://www.sparkfun.com/products/11400"&gt;Electric Imp Breakout Board&lt;/a&gt;.&lt;br&gt;&lt;br&gt;
&lt;a href="http://www.ti.com/lit/gpn/tps62172"&gt;Datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TPS62172"/>
</gates>
<devices>
<device name="" package="WSON-8-PAD">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="PAD" pad="PAD"/>
<connect gate="G$1" pin="PG" pad="8"/>
<connect gate="G$1" pin="PGND" pad="1"/>
<connect gate="G$1" pin="SW" pad="7"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
