<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ALM-1412">
</package>
<package name="ANTENNA-CHIP">
</package>
<package name="ANTENNA-CHIP2">
</package>
<package name="ANTENNA-CHIP3">
</package>
<package name="ANTENNA-CHIP4">
</package>
<package name="ANTENNA-CHIP5">
</package>
<package name="ANTENNA-CHIP6">
<description>Footprint for Part#1575AT43A40</description>
</package>
<package name="QFN-64">
<description>QFN package with a 6x8 pin configuration.</description>
</package>
<package name="BALUN">
</package>
<package name="BGB203_ORIGINAL">
</package>
<package name="BGB203">
</package>
<package name="BLUERADIO_BR-C40A">
</package>
<package name="BLUERADIO_BR-C40N">
</package>
<package name="BLUETOOTH-SMD-FP">
</package>
<package name="BLUETOOTH-INTERNAL-FP">
</package>
<package name="BLUETOOTH-INTERNAL-FP2">
</package>
<package name="RN41">
</package>
<package name="BTM182">
<description>BTM-182 Class2 Bluetooth Module from Rayson</description>
</package>
<package name="COPERNICUS">
</package>
<package name="COPERNICUS-DIP">
</package>
<package name="EM406">
</package>
<package name="EMB001">
</package>
<package name="EM406_OUTLINE">
</package>
<package name="EM408_OUTLINE">
</package>
<package name="ET312">
</package>
<package name="GE863">
</package>
<package name="GE864">
</package>
<package name="GE865">
</package>
<package name="GM862">
</package>
<package name="GM862_CONNECTOR">
</package>
<package name="GP-2106">
</package>
<package name="GR-10">
</package>
<package name="GS406SMD">
<description>50 Channel GS406 Helical GPS Receiver - SMD Connector

sku: GPS-09079</description>
</package>
<package name="GS406-MATING_SMD_***SPECIAL">
</package>
<package name="GS1011MXX">
<description>SMD GS1011Mxx</description>
</package>
<package name="ID-12">
<description>ID12 Footprint (works with ID2, ID12, and ID20)</description>
</package>
<package name="ID-12_LOCK">
<description>ID12 Footprint (works with ID2, ID12, and ID20)</description>
</package>
<package name="ID-12_SMD">
<description>ID12 Footprint (works with ID2, ID12, and ID20)</description>
</package>
<package name="LASSEN_IQ_GPS">
</package>
<package name="LS20126">
<description>&lt;h3&gt;LS20126 GPS Receiver&lt;/h3&gt;
Package for LOCOSYS LS20126 GPS smart antenna module.&lt;br&gt;
SparkFun Sku# GPS-09838&lt;br&gt;&lt;br&gt;
Note: PCB cannot extend past top tPlace border @ 25mm&lt;br&gt;
&lt;b&gt;Unproven!&lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="MIRF">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="MN5010HS">
<description>MN5010HS GPS Module</description>
</package>
<package name="MLP-24">
</package>
<package name="QFN20">
</package>
<package name="QFN-32">
<description>&lt;h3&gt;QFN 32-Pin package w/ Thermal Pad&lt;/h3&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
&lt;B&gt;Applicable Parts:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;TLC5940&lt;/ul&gt;</description>
</package>
<package name="QFN-36">
</package>
<package name="NS73M">
</package>
<package name="RF-LINK_RX">
<description>RF-LINK receivers WRL-8947, 8948, 8949, 8950</description>
</package>
<package name="RF-LINK_TX">
<description>RF-LINK transmitters WRL-8945, 8946</description>
</package>
<package name="RF24G-2X5">
<description>test</description>
</package>
<package name="RFM22-XXX-S2">
<description>Package for Hope RF s RFM22-xxx-S2 SMD wireless transciever, xxx is module s frequency band.
*Unproven*''</description>
</package>
<package name="RMCM01">
</package>
<package name="RN-131G">
</package>
<package name="RN171">
<description>RN-171, FP pad size: 40mil x 90mil</description>
</package>
<package name="RS9110-N-11-22-SHORT">
<description>Redpine WiFi module: short FP (doesn't include the NC pads around the antenna)</description>
</package>
<package name="SI470X">
</package>
<package name="SI4700/01-GM">
</package>
<package name="SM130">
<description>30-pin DIL with 100mil spacing between headers</description>
</package>
<package name="SM5100B">
</package>
<package name="SM5100B-SPECIAL_FOR_TESTING">
</package>
<package name="SOT666">
</package>
<package name="SUP500F">
</package>
<package name="TFM-511">
</package>
<package name="TRF-24G-SOCKET">
</package>
<package name="LGA44">
<description>LGA44 - Used for Venus GPS</description>
</package>
<package name="VENUS638FLPX">
</package>
<package name="WIFLY_GSX">
</package>
<package name="WLANMODULE">
</package>
<package name="WT32">
</package>
<package name="XBEE-1">
</package>
<package name="XBEE-SILK">
</package>
<package name="XBEE-SMD">
</package>
<package name="XBEE-1_LOCK">
</package>
<package name="XTEND-DIGI-MODEM">
<description>Package for the Xtend Digi Modem 40 mile range</description>
</package>
<package name="ZG2100M">
</package>
<package name="BLE112-A">
<description>BLE112-A&lt;BR&gt;
Bluetooth 4.0 module with built-in chip antenna.</description>
</package>
<package name="BLUERADIO_BR-LE4.0-S2">
</package>
<package name="SD_MMC_SOCKET">
<description>&lt;h3&gt;SD/Multi-Media Card Socket&lt;/h3&gt;
4UCONN part # 19646</description>
</package>
</packages>
<symbols>
<symbol name="ALM-1412">
<pin name="RF_IN"/>
<pin name="GND"/>
<pin name="SD"/>
<pin name="RF_OUT"/>
<pin name="VDD"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
</symbol>
<symbol name="ANTENNA">
<pin name="GND"/>
<pin name="SIGNAL"/>
</symbol>
<symbol name="ANTENNA2">
<pin name="SIGNAL"/>
</symbol>
<symbol name="ATMEGA128RFA1">
<pin name="EVDD"/>
<pin name="DEVDD@23"/>
<pin name="AVDD"/>
<pin name="DVDD@21"/>
<pin name="AVSS@58"/>
<pin name="DVSS@20"/>
<pin name="PB0"/>
<pin name="PB1/SCK"/>
<pin name="PB2/PDI"/>
<pin name="PB3/PDO"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="PF5"/>
<pin name="PF4"/>
<pin name="PF3"/>
<pin name="PF2"/>
<pin name="PF1"/>
<pin name="PF0"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="AVSS_RFN"/>
<pin name="AVSS_RFP"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="RSTN"/>
<pin name="RSTON"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AREF"/>
<pin name="TST"/>
<pin name="CLKI"/>
<pin name="DVDD@22"/>
<pin name="DVSS@24"/>
<pin name="DVSS@35"/>
<pin name="DVSS@45"/>
<pin name="DVSS@55"/>
<pin name="DEVDD@34"/>
<pin name="DEVDD@44"/>
<pin name="DEVDD@54"/>
<pin name="AVSS@61"/>
</symbol>
<symbol name="BALUN">
<pin name="IN"/>
<pin name="OUT1"/>
<pin name="GND@5"/>
<pin name="OUT2"/>
<pin name="GND@2"/>
</symbol>
<symbol name="BGB203_BLUETOOTH">
<pin name="GND@1"/>
<pin name="ANT"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
<pin name="GND@10"/>
<pin name="GPIO[14]"/>
<pin name="GPIO[12]"/>
<pin name="VDDRF"/>
<pin name="BTACT/GPIO[17]"/>
<pin name="VANLO"/>
<pin name="I2C_SDA/GPIO[1]"/>
<pin name="I2C_SCL/GPIO[0]"/>
<pin name="VDDA/VDDO"/>
<pin name="XTAL2_SYS"/>
<pin name="XTAL1_SYS"/>
<pin name="GPIO[13]"/>
<pin name="GPIO[11]"/>
<pin name="GPIO[10]"/>
<pin name="VDDC/VDDIO1"/>
<pin name="GPIO[16]"/>
<pin name="VDDIO1"/>
<pin name="XTAL1_LP"/>
<pin name="XTAL2_LP"/>
<pin name="VBUS_USB"/>
<pin name="GPIO[15]"/>
<pin name="GPIO[7]"/>
<pin name="GPIO[9]"/>
<pin name="GPIO[6]"/>
<pin name="GPIO[8]"/>
<pin name="VDDC"/>
<pin name="VDDIO2"/>
<pin name="DN_USB"/>
<pin name="DP_USB"/>
<pin name="RTS/GPIO[3]"/>
<pin name="RX/GPIO[5]"/>
<pin name="TX/GPIO[4]"/>
<pin name="CTS/GPIO[2]"/>
<pin name="RESET_N"/>
<pin name="VDDIORF"/>
<pin name="TMS_JTAG"/>
<pin name="TDO_JTAG"/>
<pin name="TDI_JTAG"/>
<pin name="TCK_JTAG"/>
<pin name="GND@49"/>
</symbol>
<symbol name="BLUERADIO_BR-C40A">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCC"/>
<pin name="SPI_CSB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="PIO_2/CONNECT" direction="out"/>
<pin name="PIO_3/INT" direction="in"/>
<pin name="PIO_4/FACRST"/>
<pin name="PIO_5/STATUS" direction="out"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="PCM_OUT"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="UART_RTS" direction="out" function="dot"/>
<pin name="UART_CTS" direction="in" function="dot"/>
<pin name="RESET"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="BLUERADIO_BR-C40N">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCC"/>
<pin name="SPI_CSB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="PIO_2/CONNECT" direction="out"/>
<pin name="PIO_3/INT" direction="in"/>
<pin name="PIO_4/FACRST"/>
<pin name="PIO_5/STATUS" direction="out"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="PCM_OUT"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="UART_RTS" direction="out" function="dot"/>
<pin name="UART_CTS" direction="in" function="dot"/>
<pin name="RESET"/>
<pin name="GND@4" direction="pwr"/>
<pin name="ANT"/>
</symbol>
<symbol name="RN41">
<pin name="GND"/>
<pin name="SPIMOSI"/>
<pin name="PIO6"/>
<pin name="PIO7"/>
<pin name="RESET"/>
<pin name="SPICLK"/>
<pin name="PCMCLK"/>
<pin name="PCMSYNC"/>
<pin name="PCMIN"/>
<pin name="PCMOUT"/>
<pin name="VDD"/>
<pin name="GND1"/>
<pin name="UARTRX"/>
<pin name="UARTTX"/>
<pin name="UARTRTS"/>
<pin name="UARTCTS"/>
<pin name="USBD+"/>
<pin name="USBD-"/>
<pin name="PIO2"/>
<pin name="PIO3"/>
<pin name="PIO5"/>
<pin name="PIO4"/>
<pin name="SPICSB"/>
<pin name="SPIMISO"/>
<pin name="GND2"/>
<pin name="NC"/>
<pin name="GND3"/>
<pin name="PIO9"/>
<pin name="GND4"/>
<pin name="PIO8"/>
<pin name="PIO10"/>
<pin name="PIO11"/>
<pin name="AIO1"/>
<pin name="AIO2"/>
<pin name="GND5"/>
</symbol>
<symbol name="BTM182">
<pin name="VDD"/>
<pin name="VDD_USB"/>
<pin name="USB_DP"/>
<pin name="USB_DN"/>
<pin name="PCM_OUT"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="UART_CTS"/>
<pin name="UART_TX"/>
<pin name="UART_RX"/>
<pin name="UART_RTS"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_CSB"/>
<pin name="SPI_MISO"/>
<pin name="SPI_CLK"/>
<pin name="GND"/>
<pin name="RESET"/>
<pin name="AIO1"/>
<pin name="AIO0"/>
<pin name="PIO11"/>
<pin name="PIO10"/>
<pin name="PIO9"/>
<pin name="PIO8"/>
<pin name="PIO7"/>
<pin name="PIO6"/>
<pin name="PIO5"/>
<pin name="PIO4"/>
<pin name="PIO3"/>
<pin name="PIO2"/>
<pin name="PIO1"/>
<pin name="PIO0"/>
</symbol>
<symbol name="COPERNICUS">
<pin name="BOOT"/>
<pin name="SHORT"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="RFIN"/>
<pin name="GND@3"/>
<pin name="LNA"/>
<pin name="GND@6"/>
<pin name="XSTANDBY"/>
<pin name="RESERVED3"/>
<pin name="RESERVED4"/>
<pin name="PPS"/>
<pin name="RXD-A"/>
<pin name="RESERVED5"/>
<pin name="TXD-A"/>
<pin name="TXD-B"/>
<pin name="RESERVED6"/>
<pin name="RESERVED7"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="RESERVED1"/>
<pin name="OPEN"/>
<pin name="RESERVED2"/>
<pin name="XRESET"/>
<pin name="RXD-B"/>
<pin name="VCC"/>
</symbol>
<symbol name="COPERNICUS-DIP">
<pin name="BOOT"/>
<pin name="SHORT"/>
<pin name="GND"/>
<pin name="LNA"/>
<pin name="XSTANDBY"/>
<pin name="RESERVED3"/>
<pin name="RESERVED4"/>
<pin name="PPS"/>
<pin name="RXD-A"/>
<pin name="RESERVED5"/>
<pin name="TXD-A"/>
<pin name="TXD-B"/>
<pin name="RESERVED6"/>
<pin name="RESERVED7"/>
<pin name="RESERVED1"/>
<pin name="OPEN"/>
<pin name="RESERVED2"/>
<pin name="XRESET"/>
<pin name="RXD-B"/>
<pin name="VCC"/>
</symbol>
<symbol name="D2523T">
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="VBAT"/>
<pin name="LED"/>
</symbol>
<symbol name="EMB001">
<pin name="ANT"/>
<pin name="GND@0"/>
<pin name="PIO2"/>
<pin name="PIO3"/>
<pin name="PIO4"/>
<pin name="PIO5"/>
<pin name="PIO6"/>
<pin name="PIO7"/>
<pin name="PIO8"/>
<pin name="PIO9"/>
<pin name="PIO10"/>
<pin name="PIO11"/>
<pin name="USB_DN"/>
<pin name="USB_DP"/>
<pin name="PCM_CLK"/>
<pin name="PCM_IN"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_OUT"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="VSUP"/>
<pin name="1V8"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="TX"/>
<pin name="CTS"/>
<pin name="MOSI"/>
<pin name="SPI_CLK"/>
<pin name="SPI_CSB"/>
<pin name="MISO"/>
<pin name="RST"/>
<pin name="AIO1"/>
<pin name="AIO0"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="PIO1"/>
<pin name="PIO0"/>
<pin name="GND@9"/>
</symbol>
<symbol name="EM406_OUTLINE">
</symbol>
<symbol name="EM408_OUTLINE">
</symbol>
<symbol name="ET312">
<pin name="GND6" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="TX" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="GND7" direction="pwr"/>
<pin name="RF"/>
<pin name="GPIO1"/>
<pin name="VCC" direction="pwr"/>
<pin name="BATT" direction="pwr"/>
</symbol>
<symbol name="GE863">
<pin name="GPIO13"/>
<pin name="GPIO12"/>
<pin name="GPIO11"/>
<pin name="GPIO10"/>
<pin name="GPIO9/CAM_RST"/>
<pin name="GPIO8/CAM_ON"/>
<pin name="CAM_CLK"/>
<pin name="GND@0"/>
<pin name="EAR_MT-"/>
<pin name="EAR_MT+"/>
<pin name="EAR_HF+"/>
<pin name="EAR_HF-"/>
<pin name="MIC_MT+"/>
<pin name="MIN_MT-"/>
<pin name="MIC_HF+"/>
<pin name="MIC_HF-"/>
<pin name="GND@1"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="ADC_IN1"/>
<pin name="VRTC"/>
<pin name="TX_TRACE"/>
<pin name="RX_TRACE"/>
<pin name="VBATT"/>
<pin name="GND@2"/>
<pin name="STAT_LED"/>
<pin name="AXE"/>
<pin name="VAUX1"/>
<pin name="GPIO4/CAM_SDA"/>
<pin name="GPIO2/JDR"/>
<pin name="GPIO1"/>
<pin name="CHARGE"/>
<pin name="GND@3"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="GND@4"/>
<pin name="ON/OFF"/>
<pin name="RESET"/>
<pin name="GND@5"/>
<pin name="ANT"/>
<pin name="GND@6"/>
<pin name="GPIO7/BUZZER"/>
<pin name="PWRMON"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO3/CAM_SCL"/>
<pin name="GND@7"/>
<pin name="GPIO17"/>
<pin name="GPIO14"/>
<pin name="DAC_OUT"/>
<pin name="GPIO16"/>
<pin name="GND@8"/>
<pin name="TX_GPS"/>
<pin name="GND@9"/>
<pin name="GPIO15"/>
<pin name="GND@10"/>
<pin name="RX_GPS"/>
<pin name="PPS"/>
<pin name="GPIO18"/>
<pin name="GND@11"/>
<pin name="RX_GPS_BIN"/>
<pin name="GND@12"/>
<pin name="TX_GPS_BIN"/>
<pin name="GND@13"/>
<pin name="GPS_ANT"/>
<pin name="GND_GPS"/>
</symbol>
<symbol name="GE864">
<pin name="EAR_MT-"/>
<pin name="EAR_MT+"/>
<pin name="EAR_HF+"/>
<pin name="EAR_HF-"/>
<pin name="MIC_MT+"/>
<pin name="MIC_MT-"/>
<pin name="MIC_HF+"/>
<pin name="MIC_HF-"/>
<pin name="AXE"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TX_TRACE"/>
<pin name="RX_TRACE"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="ADC_IN3"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="CHARGE@G1"/>
<pin name="CHARGE@G2"/>
<pin name="ON_OFF"/>
<pin name="VAUX1"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="DV12_CLK"/>
<pin name="TGPIO_12"/>
<pin name="TGPIO_03"/>
<pin name="TGPIO_04"/>
<pin name="TGPIO_20"/>
<pin name="TGPIO_14"/>
<pin name="TGPIO_11"/>
<pin name="TGPIO_19"/>
<pin name="TGPIO_01"/>
<pin name="TGPIO_18"/>
<pin name="TGPIO_17"/>
<pin name="TGPIO_15"/>
<pin name="TGPIO_08"/>
<pin name="TGPIO_06/ALARM"/>
<pin name="TGPIO_09"/>
<pin name="TGPIO_02/JDR"/>
<pin name="TGPIO_07/BUZZER"/>
<pin name="TGPIO_16"/>
<pin name="TGPIO_13"/>
<pin name="TGPIO_05/RFTXMON"/>
<pin name="TGPIO_21"/>
<pin name="TGPIO_22"/>
<pin name="TGPIO_10"/>
<pin name="VBATT@J1"/>
<pin name="VBATT@K1"/>
<pin name="VBATT@J2"/>
<pin name="VBATT@K2"/>
<pin name="GND@A1"/>
<pin name="GND@F1"/>
<pin name="GND@H1"/>
<pin name="GND@L1"/>
<pin name="GND@H2"/>
<pin name="GND@L2"/>
<pin name="GND@J3"/>
<pin name="GND@K3"/>
<pin name="GND@L3"/>
<pin name="GND@K4"/>
<pin name="GND@K5"/>
<pin name="GND@D6"/>
<pin name="GND@K6"/>
<pin name="GND@L6"/>
<pin name="GND@A11"/>
<pin name="GND@F11"/>
<pin name="GND@L11"/>
</symbol>
<symbol name="GE865">
<pin name="EAR-"/>
<pin name="EAR+"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TXD_AUX"/>
<pin name="RXD_AUX"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="ON_OFF"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="GPIO_03"/>
<pin name="GPIO_04/TX_DISAB"/>
<pin name="GPIO_01"/>
<pin name="GPIO_08"/>
<pin name="GPIO_06/ALARM"/>
<pin name="GPIO_09"/>
<pin name="GPIO_02/JDR"/>
<pin name="GPIO_07/BUZZER"/>
<pin name="GPIO_05/RFTXMON"/>
<pin name="GPIO_10"/>
<pin name="VBATT@F1"/>
<pin name="VBATT@F2"/>
<pin name="VBATT@F3"/>
<pin name="GND@G1"/>
<pin name="GND@C2"/>
<pin name="GND@C7"/>
<pin name="GND@E5"/>
<pin name="GND@E7"/>
<pin name="GND@G5"/>
<pin name="GND@G4"/>
<pin name="GND@G3"/>
<pin name="GND@H3"/>
<pin name="GND@H6"/>
</symbol>
<symbol name="GE865_2">
<pin name="EAR-"/>
<pin name="EAR+"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TXD_AUX"/>
<pin name="RXD_AUX"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="ON_OFF"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="GPIO_03"/>
<pin name="GPIO_04/TX_DISAB"/>
<pin name="GPIO_01"/>
<pin name="GPIO_08"/>
<pin name="GPIO_06/ALARM"/>
<pin name="GPIO_09"/>
<pin name="GPIO_02/JDR"/>
<pin name="GPIO_07/BUZZER"/>
<pin name="GPIO_05/RFTXMON"/>
<pin name="GPIO_10"/>
<pin name="VBATT@F1"/>
<pin name="VBATT@F2"/>
<pin name="VBATT@F3"/>
<pin name="GND@G1"/>
<pin name="GND@C2"/>
<pin name="GND@C7"/>
<pin name="GND@E5"/>
<pin name="GND@E7"/>
<pin name="GND@G5"/>
<pin name="GND@G4"/>
<pin name="GND@G3"/>
<pin name="GND@H3"/>
<pin name="GND@H6"/>
<pin name="SERVICE"/>
</symbol>
<symbol name="GM862">
<pin name="VBATT@0" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="VBATT@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VBATT@2" direction="pwr"/>
<pin name="GND/ADC" direction="pwr"/>
<pin name="VBATT@3" direction="pwr"/>
<pin name="CHARGE" direction="in"/>
<pin name="EAR_HF+" direction="out"/>
<pin name="EAR_MT-" direction="out"/>
<pin name="EAR_HF-" direction="out"/>
<pin name="EAR_MT+" direction="out"/>
<pin name="MIC_HF-" direction="in"/>
<pin name="MIC_MT+" direction="in"/>
<pin name="MIC_HF+" direction="in"/>
<pin name="MIC_MT-" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="AXE" direction="in"/>
<pin name="SIMIO"/>
<pin name="C103/TXD" direction="in"/>
<pin name="PWRMON" direction="out"/>
<pin name="SIMVCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="SIMRST" direction="out"/>
<pin name="RES@25"/>
<pin name="SIMCLK" direction="out"/>
<pin name="CCIN/SIMIN"/>
<pin name="GPO2/JDR" direction="out"/>
<pin name="C106/CTS"/>
<pin name="C125/RING" direction="out"/>
<pin name="GPI1" direction="in"/>
<pin name="GPIO8/PD[0]/CAM_ON"/>
<pin name="C107/DSR" direction="out"/>
<pin name="GPIO9/PD[1]/CAM_RST"/>
<pin name="EMMI_TX/TX_GPS" direction="out"/>
<pin name="C109/DCD" direction="out"/>
<pin name="C104/RXD" direction="out"/>
<pin name="GPIO10/PD[2]"/>
<pin name="STAT_LED" direction="out"/>
<pin name="GPIO11/PD[3]"/>
<pin name="EMMI_RX/RX_GPS" direction="in"/>
<pin name="GPIO12/PD[4]"/>
<pin name="C108/DTR" direction="in"/>
<pin name="GPIO13/PD[5]"/>
<pin name="C105/RTS" direction="in"/>
<pin name="GPIO3/PD[6]/CAM_SCL"/>
<pin name="GPIO4/IICSDA/CAM_SDA"/>
<pin name="GPIO5/CAM_RDY/RFTXMON"/>
<pin name="GPIO6/ALARM/PD[7]"/>
<pin name="GPIO7/BUZZER/CAM_PWR_ON"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
</symbol>
<symbol name="GP-2106">
<pin name="VCC"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="ONOFF"/>
<pin name="1PPS"/>
<pin name="GND"/>
</symbol>
<symbol name="GR-10">
<pin name="FREF"/>
<pin name="GND@2" direction="pwr"/>
<pin name="1.8V@3" direction="pwr"/>
<pin name="SB" direction="in"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX0" direction="in"/>
<pin name="TX0" direction="out"/>
<pin name="1PPS" direction="out"/>
<pin name="1.8V@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GPIO_A11"/>
<pin name="GPIO_A5"/>
<pin name="GPIO_A6"/>
<pin name="GPIO_A9"/>
<pin name="APIO_A4"/>
<pin name="RTC_XIN"/>
<pin name="RTC_XOUT"/>
<pin name="GPIO_B19"/>
<pin name="VALID_FIX" direction="out"/>
<pin name="1.8V@21" direction="pwr"/>
<pin name="GPIO_B16"/>
<pin name="RESET" direction="in"/>
<pin name="GND@24" direction="pwr"/>
<pin name="1.8VVCO" direction="pwr"/>
<pin name="1.8VIF" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="1.8VLNA" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="ANT" direction="in"/>
<pin name="GND@31" direction="pwr"/>
<pin name="RFEN" direction="out"/>
<pin name="3V" direction="pwr"/>
<pin name="1.8VRF" direction="pwr"/>
<pin name="TPI" direction="in"/>
<pin name="TPQ" direction="in"/>
</symbol>
<symbol name="GS406SMD">
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
</symbol>
<symbol name="GS1011">
<pin name="GND@1"/>
<pin name="JTAG_TCK"/>
<pin name="JTAG_TDO"/>
<pin name="JTAG_TDI"/>
<pin name="JTAG_TMS"/>
<pin name="JTAG_RST"/>
<pin name="ALARM1"/>
<pin name="RTC_OUT1"/>
<pin name="VBAT"/>
<pin name="DC_CNTL"/>
<pin name="ADC1"/>
<pin name="ADC2"/>
<pin name="ALARM2"/>
<pin name="MSPI_DIN"/>
<pin name="MSPI_DOUT"/>
<pin name="VOUT_1.8V"/>
<pin name="GND@17"/>
<pin name="MSPI_CLK"/>
<pin name="MSPI_CS0"/>
<pin name="MSPI_CS1"/>
<pin name="GPIO21_11MHZ"/>
<pin name="GPIO20_22MHZ"/>
<pin name="GPIO19_44MHZ"/>
<pin name="PWM0/GPIO10"/>
<pin name="I2C_CLK"/>
<pin name="I2C_DATA"/>
<pin name="SSPI_DOUT"/>
<pin name="SSPI_CLK"/>
<pin name="SSPI_CS"/>
<pin name="SSPI_DIN"/>
<pin name="VIN_3V3"/>
<pin name="GND@32"/>
<pin name="EN_1.8V"/>
<pin name="VDDIO"/>
<pin name="UART1_CTS/GPIO26"/>
<pin name="UART1_RTS/GPIO27"/>
<pin name="UART1_RX/GPIO3"/>
<pin name="UART1_TX/GPIO2"/>
<pin name="UART0_TX/GPIO1"/>
<pin name="UART0_RTS/GPIO25"/>
<pin name="UART0_RX/GPIO0"/>
<pin name="UART0_CTS/GPIO24"/>
<pin name="GPIO31_LED2"/>
<pin name="GPIO30_LED1"/>
<pin name="GPIO29"/>
<pin name="GPIO28"/>
<pin name="EXT_RESET"/>
<pin name="GND@48"/>
</symbol>
<symbol name="ID-12">
<pin name="GNDT"/>
<pin name="RES"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="CP"/>
<pin name="FUTURE"/>
<pin name="+/-"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="LED"/>
<pin name="5V"/>
</symbol>
<symbol name="LASSEN_IQ_GPS">
<pin name="RXA" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="TXA" direction="out"/>
<pin name="PPS" direction="out"/>
<pin name="RXB" direction="in"/>
<pin name="BATT" direction="pwr"/>
<pin name="TXB" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LS20126">
<pin name="GND@1"/>
<pin name="VSTBY"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="GPIO"/>
<pin name="BOOTSL"/>
<pin name="EN"/>
<pin name="VCC"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
</symbol>
<symbol name="MIRF">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="MLX90121">
<pin name="VDD1"/>
<pin name="TX"/>
<pin name="MOD"/>
<pin name="VSS1"/>
<pin name="XOUT"/>
<pin name="XIN"/>
<pin name="VSS2"/>
<pin name="XBUF"/>
<pin name="RES1"/>
<pin name="RTB"/>
<pin name="DOUT"/>
<pin name="VDD2"/>
<pin name="DIN"/>
<pin name="MODE"/>
<pin name="CK"/>
<pin name="DSYC"/>
<pin name="VDD3"/>
<pin name="RES2(DNC)"/>
<pin name="VSS3"/>
<pin name="RX"/>
</symbol>
<symbol name="MN5010HS">
<pin name="1PPS"/>
<pin name="ANT"/>
<pin name="BATT"/>
<pin name="GND2"/>
<pin name="GND11"/>
<pin name="GND24"/>
<pin name="GND27"/>
<pin name="GND29"/>
<pin name="GND31"/>
<pin name="NAV"/>
<pin name="NMR"/>
<pin name="ONOFF"/>
<pin name="OPT1"/>
<pin name="OPT2"/>
<pin name="RX-I"/>
<pin name="TX-O"/>
<pin name="VIO"/>
<pin name="GND4"/>
</symbol>
<symbol name="NRF24AP1">
<pin name="BR2"/>
<pin name="BR1" direction="in"/>
<pin name="EXT32K" direction="in"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="SLEEP" direction="in"/>
<pin name="SUSPEND" direction="in" function="dot"/>
<pin name="RTS" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VSS_PA" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="PORTSEL" direction="in"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VSS@0" direction="out"/>
</symbol>
<symbol name="NRF24L01-1">
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="IRQ" direction="out" function="dot"/>
<pin name="DVDD" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="CSN" direction="in"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
</symbol>
<symbol name="NRF24LE1">
<pin name="P0.1"/>
<pin name="VDD1"/>
<pin name="DEC1"/>
<pin name="DEC2"/>
<pin name="P0.2"/>
<pin name="PROG"/>
<pin name="P0.3"/>
<pin name="VSS1"/>
<pin name="VDD2"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="RESET"/>
<pin name="VDD_PA"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="VSS2"/>
<pin name="VDD3"/>
<pin name="IREF"/>
<pin name="VSS3"/>
<pin name="VDD4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="XC2"/>
<pin name="XC1"/>
<pin name="P0.0"/>
</symbol>
<symbol name="NRF24LU1">
<pin name="VDD3"/>
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="VSS2"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="/RESET"/>
<pin name="PROG"/>
<pin name="VSS1"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="VDD2"/>
<pin name="VBUS"/>
<pin name="VDD1"/>
<pin name="XC1"/>
<pin name="XC2"/>
<pin name="VSS7"/>
<pin name="DEC2"/>
<pin name="DEC1"/>
<pin name="VDD6"/>
<pin name="VSS6"/>
<pin name="IREF"/>
<pin name="VDD5"/>
<pin name="VSS5"/>
<pin name="ANT2"/>
<pin name="ANT1"/>
<pin name="VDD_PA"/>
<pin name="VDD4"/>
<pin name="VSS4"/>
<pin name="VSS3"/>
</symbol>
<symbol name="NRF24Z1">
<pin name="SSEL"/>
<pin name="SMISO"/>
<pin name="SSCK"/>
<pin name="SCSN"/>
<pin name="VDD"/>
<pin name="SMOSI"/>
<pin name="DD1"/>
<pin name="DD0"/>
<pin name="REQ"/>
<pin name="CLK"/>
<pin name="WS"/>
<pin name="DATA"/>
<pin name="SPDIO"/>
<pin name="MCLK"/>
<pin name="DVDD"/>
<pin name="VSS"/>
<pin name="XC2"/>
<pin name="XC1"/>
<pin name="VDD1"/>
<pin name="VDD_PA"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="VSS_PA"/>
<pin name="IREF"/>
<pin name="VSS1"/>
<pin name="MODE"/>
<pin name="MSDA"/>
<pin name="MSCL"/>
<pin name="MCSN"/>
<pin name="MMISO"/>
<pin name="MMOSI"/>
<pin name="VSS2"/>
<pin name="VDD2"/>
<pin name="VSS3"/>
<pin name="MSCK"/>
<pin name="IRQ"/>
</symbol>
<symbol name="NRF2401A">
<pin name="DATA"/>
<pin name="DVDD" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="DR1" direction="out"/>
<pin name="CLK2"/>
<pin name="DOUT2" direction="out"/>
<pin name="CLK1"/>
<pin name="PWR_UP" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VSS_PA" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="DR2" direction="out"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
</symbol>
<symbol name="NS73M">
<pin name="RFO"/>
<pin name="GND@14"/>
<pin name="RIN"/>
<pin name="LIN"/>
<pin name="GND@11"/>
<pin name="X1"/>
<pin name="VCC"/>
<pin name="GND@1"/>
<pin name="VDRF"/>
<pin name="TEB"/>
<pin name="PWE"/>
<pin name="CK"/>
<pin name="DA"/>
<pin name="LA"/>
<pin name="IIC"/>
</symbol>
<symbol name="RF-LINK_RX">
<pin name="GND" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="+5V" direction="pwr"/>
<pin name="DATA" direction="in"/>
</symbol>
<symbol name="RF-LINK_TX">
<pin name="GND" direction="pwr"/>
<pin name="DATA" direction="in"/>
<pin name="ANT" direction="pas"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="RF24G">
<pin name="GND"/>
<pin name="CE"/>
<pin name="CLK2"/>
<pin name="CS"/>
<pin name="CLK1"/>
<pin name="VCC"/>
<pin name="DR2"/>
<pin name="DOUT2"/>
<pin name="DR1"/>
<pin name="DATA"/>
</symbol>
<symbol name="RFM22">
<pin name="ANT"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="NIRQ" direction="out"/>
<pin name="NSEL" direction="in"/>
<pin name="RXANT" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDN" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="TXANT" direction="in"/>
<pin name="VCC"/>
</symbol>
<symbol name="RMCM01">
<pin name="FPLS"/>
<pin name="HR"/>
<pin name="OSC"/>
<pin name="F32KIN"/>
<pin name="OSC_ON"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="LX1"/>
<pin name="LX2"/>
<pin name="WIDB_DET"/>
<pin name="RESET"/>
</symbol>
<symbol name="RN-131G">
<pin name="SEN6"/>
<pin name="SEN4"/>
<pin name="SEN5"/>
<pin name="SEN7"/>
<pin name="RESET"/>
<pin name="EPC-A"/>
<pin name="EPC-B"/>
<pin name="S_CAP"/>
<pin name="F_AWAKE"/>
<pin name="GPIO-13"/>
<pin name="GPIO-12"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="MOSI"/>
<pin name="CLK"/>
<pin name="MISO"/>
<pin name="3.3V-ROUT"/>
<pin name="3.3V-RIN"/>
<pin name="GND@19"/>
<pin name="VDD-BATT"/>
<pin name="VDD-IN"/>
<pin name="DMA-TX"/>
<pin name="DMA-RX"/>
<pin name="GPIO-9"/>
<pin name="GPIO-8"/>
<pin name="GPIO-7"/>
<pin name="GPIO-6"/>
<pin name="GPIO-5"/>
<pin name="GPIO-4"/>
<pin name="SEN1"/>
<pin name="SEN2"/>
<pin name="SEN3"/>
<pin name="SENSE-PWR"/>
<pin name="SEN0"/>
<pin name="GND@36"/>
<pin name="GND@37"/>
<pin name="GND@38"/>
<pin name="GND@39"/>
<pin name="GND@40"/>
<pin name="GND@41"/>
<pin name="GND@42"/>
<pin name="GND@43"/>
<pin name="GND@44"/>
</symbol>
<symbol name="RN171">
<pin name="GND@1"/>
<pin name="CLK"/>
<pin name="CS"/>
<pin name="GPIO7"/>
<pin name="INT/GPIO6"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="VDD"/>
<pin name="GPIO3"/>
<pin name="GPIO2"/>
<pin name="GPIO1"/>
<pin name="GND@14"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="ANT"/>
<pin name="GND@25"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="SEN0"/>
<pin name="SEN1"/>
<pin name="SEN2"/>
<pin name="SEN3"/>
<pin name="SPOWER"/>
<pin name="VDD_RF"/>
<pin name="SEN4"/>
<pin name="SEN5"/>
<pin name="SEN6"/>
<pin name="SEN7"/>
<pin name="GND@39"/>
<pin name="RESET"/>
<pin name="AWAKE"/>
<pin name="GPIO14"/>
<pin name="RTS"/>
<pin name="CTS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND@47"/>
<pin name="SREG"/>
<pin name="VDD_BATT"/>
</symbol>
<symbol name="RS9110-N-11-22">
<pin name="VIN@46"/>
<pin name="VIN@47"/>
<pin name="JPD0"/>
<pin name="JPD1"/>
<pin name="JPD2"/>
<pin name="INTR"/>
<pin name="RST"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="SD3"/>
<pin name="CLK"/>
<pin name="CS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="MODE"/>
<pin name="GND@10"/>
<pin name="GND@16"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@48"/>
<pin name="GND@PAD"/>
</symbol>
<symbol name="SI470X">
<pin name="!RST"/>
<pin name="!SEN"/>
<pin name="DOUT"/>
<pin name="FMIP"/>
<pin name="GND@12"/>
<pin name="GND@PAD"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="LOUT"/>
<pin name="LPI"/>
<pin name="RCLK"/>
<pin name="RFGND"/>
<pin name="ROUT"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VA"/>
<pin name="VD"/>
<pin name="VIO"/>
</symbol>
<symbol name="SI4700/01-GM">
<pin name="GND"/>
<pin name="VA" direction="pwr"/>
<pin name="FMIP" direction="in"/>
<pin name="RFGND"/>
<pin name="FMIN" direction="in"/>
<pin name="RST" function="dot"/>
<pin name="SEN" function="dot"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="RCLK"/>
<pin name="VIO" direction="pwr"/>
<pin name="LOUT"/>
<pin name="ROUT"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="VD" direction="pwr"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="GND@0"/>
</symbol>
<symbol name="SM130">
<pin name="VCC"/>
<pin name="RFVCC"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="OK"/>
<pin name="ERROR"/>
<pin name="RESET"/>
<pin name="I1"/>
<pin name="I2"/>
<pin name="GND"/>
<pin name="RFGND@23"/>
<pin name="RFGND@25"/>
<pin name="RFGND@27"/>
<pin name="ANT2"/>
<pin name="ANT1"/>
<pin name="O2"/>
<pin name="O1"/>
<pin name="RX-I"/>
<pin name="TX-O"/>
</symbol>
<symbol name="SM5100B">
<pin name="VBAT@0"/>
<pin name="VCHG@0"/>
<pin name="VBAT@1"/>
<pin name="VCHG@1"/>
<pin name="VBAT@2"/>
<pin name="ADIN1"/>
<pin name="VBAT@3"/>
<pin name="ADIN2"/>
<pin name="GND@0"/>
<pin name="GPIO_19"/>
<pin name="GND@1"/>
<pin name="EAR_MICN"/>
<pin name="GND@2"/>
<pin name="EAR_MICP"/>
<pin name="GND@3"/>
<pin name="EAR_SPKN"/>
<pin name="GND@4"/>
<pin name="EAR_SPKP"/>
<pin name="TXD0"/>
<pin name="RXD0"/>
<pin name="SIM_RST"/>
<pin name="GPIO_17"/>
<pin name="KEY_DRV3"/>
<pin name="KEY_DRV0"/>
<pin name="KEY_DRV4"/>
<pin name="KEY_DRV2"/>
<pin name="SIM_CLK"/>
<pin name="KEY_DRV1"/>
<pin name="SIM_DA"/>
<pin name="KEY_DRV5"/>
<pin name="KEY_SEN2"/>
<pin name="KEY_SEN1"/>
<pin name="GPO42/NBOOT"/>
<pin name="RESET"/>
<pin name="GPIO_4"/>
<pin name="KEY_SEN0"/>
<pin name="GPIO_10"/>
<pin name="GPIO_6"/>
<pin name="GPIO_1"/>
<pin name="KEY_SEN3"/>
<pin name="GPIO_9"/>
<pin name="AUX_MICP"/>
<pin name="RXD1"/>
<pin name="AUX_SPKP"/>
<pin name="GPIO_18"/>
<pin name="TXD1"/>
<pin name="VCC@0"/>
<pin name="RTC_BATT"/>
<pin name="GPIO_26"/>
<pin name="AUX_MICN"/>
<pin name="SIM_VCC"/>
<pin name="GPIO_16"/>
<pin name="GPO_11"/>
<pin name="GPIO_8"/>
<pin name="GPIO_3"/>
<pin name="GPIO_20"/>
<pin name="GPIO_46"/>
<pin name="AUX_SPKN"/>
<pin name="POWER_ON"/>
<pin name="VCC@1"/>
</symbol>
<symbol name="SMA661AS">
<pin name="IN"/>
<pin name="GND@2"/>
<pin name="PD"/>
<pin name="OUT"/>
<pin name="GND@5"/>
<pin name="VCC"/>
</symbol>
<symbol name="SUP500F">
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="PSEL"/>
<pin name="GND"/>
<pin name="PPS"/>
<pin name="TX-O"/>
<pin name="RX-I"/>
</symbol>
<symbol name="TFM-511">
<pin name="ANT"/>
<pin name="NC"/>
<pin name="ROUT"/>
<pin name="LOUT"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="BUSEN"/>
<pin name="BUSMOD"/>
<pin name="CLK"/>
<pin name="DAT"/>
</symbol>
<symbol name="TRF-24G">
<pin name="VCC"/>
<pin name="DR2"/>
<pin name="DOUT2"/>
<pin name="DR1"/>
<pin name="DATA"/>
<pin name="CLK1"/>
<pin name="CS"/>
<pin name="CLK2"/>
<pin name="CE"/>
<pin name="GND"/>
</symbol>
<symbol name="VENUS634FLPX">
<pin name="LED"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="PPS"/>
<pin name="CLK"/>
<pin name="CSN"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@19"/>
<pin name="GND@15"/>
<pin name="GNDRF@21"/>
<pin name="GNDRF@22"/>
<pin name="GNDRF@24"/>
<pin name="GNDRF@25"/>
<pin name="GNDRF@27"/>
<pin name="GNDRF@28"/>
<pin name="GNDRF@29"/>
<pin name="GNDRF@31"/>
<pin name="GNDRF@33"/>
<pin name="RTC"/>
<pin name="BTSEL"/>
<pin name="RSTN"/>
<pin name="RFIN"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="GPIO1"/>
<pin name="REGEN"/>
<pin name="GPIO2"/>
<pin name="GPIO20"/>
<pin name="PIO12"/>
<pin name="PIO14"/>
<pin name="GPIO24"/>
</symbol>
<symbol name="VENUS638FLPX-L">
<pin name="LED/GPIO0"/>
<pin name="TXD0"/>
<pin name="RXD0"/>
<pin name="PPS"/>
<pin name="CLK"/>
<pin name="CSN"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@19"/>
<pin name="GND@15"/>
<pin name="GNDRF@21"/>
<pin name="GNDRF@22"/>
<pin name="GNDRF@24"/>
<pin name="GNDRF@25"/>
<pin name="GNDRF@27"/>
<pin name="GNDRF@28"/>
<pin name="GNDRF@29"/>
<pin name="GNDRF@31"/>
<pin name="GNDRF@33"/>
<pin name="RTC"/>
<pin name="BTSEL"/>
<pin name="RSTN"/>
<pin name="RFIN"/>
<pin name="VCC"/>
<pin name="VBAT"/>
<pin name="GPIO1"/>
<pin name="REGEN"/>
<pin name="GPIO2"/>
<pin name="GPIO20"/>
<pin name="PIO12"/>
<pin name="PIO14"/>
<pin name="GPIO24"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPIO4"/>
<pin name="GPIO3"/>
<pin name="GND@49"/>
<pin name="PIO5"/>
<pin name="PIO11"/>
<pin name="RXD1"/>
<pin name="GPIO25"/>
<pin name="GPIO30"/>
<pin name="PIO15"/>
<pin name="TXD1"/>
<pin name="VCC@58"/>
<pin name="GPIO28"/>
<pin name="GND@60"/>
<pin name="GNDRF@61"/>
<pin name="GNDRF@62"/>
<pin name="GPIO6"/>
<pin name="GND@64"/>
<pin name="GNDRF@65"/>
<pin name="GNDRF@69"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO29"/>
</symbol>
<symbol name="WIFLY_GSX">
<pin name="EPCB"/>
<pin name="EPCA"/>
<pin name="FORCE_WAKE"/>
<pin name="RESET_L"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MISO"/>
<pin name="GPIO9"/>
<pin name="GPIO8"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO_13"/>
<pin name="GPIO_12"/>
<pin name="URX"/>
<pin name="UTX"/>
<pin name="VD_BAT"/>
<pin name="VD_3V_IN"/>
<pin name="SENS0"/>
<pin name="SENS1"/>
<pin name="SENS2"/>
<pin name="SENS3"/>
<pin name="SENS4"/>
<pin name="SENS5"/>
<pin name="SENS6"/>
<pin name="SENS7"/>
<pin name="SENSPWR"/>
<pin name="DMA_RX"/>
<pin name="DMA_TX"/>
<pin name="SUPCAP"/>
<pin name="3V3_OUT"/>
<pin name="3V3_IN"/>
<pin name="G9"/>
<pin name="G8"/>
<pin name="G7"/>
<pin name="G6"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="G3"/>
<pin name="G2"/>
<pin name="G1"/>
<pin name="G10"/>
<pin name="NC"/>
</symbol>
<symbol name="WLANMODULE">
<pin name="VSS@0"/>
<pin name="TSI"/>
<pin name="DVDD@0"/>
<pin name="DVDD@2"/>
<pin name="V2.5"/>
<pin name="RFU"/>
<pin name="/RST"/>
<pin name="/TSS"/>
<pin name="G6"/>
<pin name="TSO"/>
<pin name="G3"/>
<pin name="F5"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="VSS@1"/>
<pin name="VSS@2"/>
<pin name="G2"/>
<pin name="F4"/>
<pin name="G1"/>
<pin name="TSCK"/>
<pin name="G7"/>
<pin name="G0"/>
<pin name="F6"/>
<pin name="F7"/>
<pin name="F0"/>
<pin name="F3"/>
<pin name="F2"/>
<pin name="F1"/>
<pin name="E6"/>
<pin name="E5"/>
<pin name="E7"/>
<pin name="E4"/>
<pin name="DVDD@1"/>
<pin name="DVDD@3"/>
<pin name="/RF_LED"/>
<pin name="VSS@3"/>
</symbol>
<symbol name="WT32">
<pin name="VDDIO@17"/>
<pin name="VDD_BAT@37"/>
<pin name="VDD_CHG@38"/>
<pin name="AIO0@5"/>
<pin name="AIO1@6"/>
<pin name="VREG_ENA@1"/>
<pin name="PIO0@7"/>
<pin name="PIO1@8"/>
<pin name="PIO2@9"/>
<pin name="PIO3@10"/>
<pin name="PIO4@26"/>
<pin name="PIO5@25"/>
<pin name="PIO6@24"/>
<pin name="PIO7@23"/>
<pin name="PIO8@22"/>
<pin name="PIO9@13"/>
<pin name="PIO10@14"/>
<pin name="USB_DN@11"/>
<pin name="USB_DP@12"/>
<pin name="RXD@15"/>
<pin name="TXD@16"/>
<pin name="PCM_IN@27"/>
<pin name="PCM_OUT@28"/>
<pin name="PCM_SYNC@29"/>
<pin name="PCM_CLK@30"/>
<pin name="RESET@19"/>
<pin name="RTS@20"/>
<pin name="CTS@21"/>
<pin name="SPI_CS@32"/>
<pin name="SPI_MISO@34"/>
<pin name="SPI_CLK@33"/>
<pin name="SPI_MOSI@35"/>
<pin name="LED0@36"/>
<pin name="MIC_BIAS@40"/>
<pin name="AUDIO_IN_P_RIGHT@41"/>
<pin name="AUDIO_IN_N_RIGHT@42"/>
<pin name="AUDIO_IN_P_LEFT@44"/>
<pin name="AUDIO_IN_N_LEFT@45"/>
<pin name="AUDIO_OUT_N_RIGHT@46"/>
<pin name="AUDIO_OUT_P_RIGHT@47"/>
<pin name="AUDIO_OUT_N_LEFT@49"/>
<pin name="AUDIO_OUT_P_LEFT@50"/>
<pin name="DGND@2"/>
<pin name="DGND@3"/>
<pin name="DGND@4"/>
<pin name="DGND@18"/>
<pin name="DGND@31"/>
<pin name="AGND@39"/>
<pin name="AGND@43"/>
<pin name="AGND@48"/>
</symbol>
<symbol name="XBEE-1">
<pin name="VDD" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="DIO12"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="RSSI"/>
<pin name="DIO11"/>
<pin name="RES@8"/>
<pin name="DTR" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="DIO4"/>
<pin name="CTS" direction="out" function="dot"/>
<pin name="DIO9"/>
<pin name="RES@14"/>
<pin name="DIO5"/>
<pin name="RTS" direction="in" function="dot"/>
<pin name="DIO3"/>
<pin name="DIO2"/>
<pin name="DIO1"/>
<pin name="DIO0"/>
</symbol>
<symbol name="XTEND-DIGI-MODEM">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="GPO2"/>
<pin name="TX_PWR"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="SHDN"/>
<pin name="SLEEP"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="CONFIG"/>
</symbol>
<symbol name="ZG2100M">
<pin name="GND1"/>
<pin name="VDD_1.8_1"/>
<pin name="JTAG_TDO"/>
<pin name="JTAG_TCK"/>
<pin name="JTAG_TMS"/>
<pin name="JTAG_TDI"/>
<pin name="RST_N"/>
<pin name="NC6"/>
<pin name="JTAG_RST_N"/>
<pin name="GND2"/>
<pin name="VDD_1.8_2"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="RES"/>
<pin name="VDD_3.3_1"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="CE_N"/>
<pin name="JTAG_EN"/>
<pin name="NC5"/>
<pin name="SCS_N"/>
<pin name="VDD_1.8_3"/>
<pin name="GND5"/>
<pin name="UART_RX"/>
<pin name="UART_TX"/>
<pin name="GND6"/>
<pin name="VDD_3.3_2"/>
<pin name="GND7"/>
<pin name="VDD_1.8_4"/>
<pin name="SDO"/>
<pin name="INT_NX"/>
<pin name="SCK"/>
<pin name="SDI"/>
<pin name="GND8"/>
</symbol>
<symbol name="BLE112-A">
<description>BlueGiga BLE112-A module&lt;BR&gt;
Bluetooth 4.0 module with chip antenna.</description>
<pin name="GND1"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="P2_2"/>
<pin name="P2_1"/>
<pin name="P2_0"/>
<pin name="P1_7"/>
<pin name="P1_6"/>
<pin name="VDD_USB"/>
<pin name="GND2"/>
<pin name="USB+"/>
<pin name="USB-"/>
<pin name="P1_5"/>
<pin name="P1_4"/>
<pin name="P1_3"/>
<pin name="P1_2"/>
<pin name="P1_1"/>
<pin name="P1_0"/>
<pin name="P0_7"/>
<pin name="DVDD"/>
<pin name="GND3"/>
<pin name="P0_6"/>
<pin name="P0_5"/>
<pin name="P0_4"/>
<pin name="P0_3"/>
<pin name="P0_2"/>
<pin name="P0_1"/>
<pin name="P0_0"/>
<pin name="RESET"/>
<pin name="GND4"/>
</symbol>
<symbol name="BLUERADIO_BR-LE4.0-S2">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC(2.0-3.6V)" direction="pwr"/>
<pin name="SPI_CSB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="PIO_2"/>
<pin name="PIO_3/INT"/>
<pin name="PIO_4"/>
<pin name="PIO_5"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="USB_VBUS"/>
<pin name="USB_GND"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="UART_RTS" direction="out" function="dot"/>
<pin name="UART_CTS" direction="in" function="dot"/>
<pin name="RESET" direction="in"/>
<pin name="PIO_9"/>
<pin name="PIO_14"/>
<pin name="ADC_0" direction="in"/>
<pin name="ADC_1" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="PIO_8"/>
</symbol>
<symbol name="ELECTRIC_IMP">
<description>&lt;h3&gt;Electric Imp&lt;/h3&gt;

A wi-fi enabled microcontroller, in an SD card package.</description>
<pin name="1(CLK2/CTS1/TX3/SCL2)"/>
<pin name="2(MISO1/MOSI2/RTS1/RX3/SDA2)"/>
<pin name="5(SCLK1/SCLK2/TX2)"/>
<pin name="7(MOSI1/MISO2/RX2)"/>
<pin name="8(MOSI2/TX1/SCL1)"/>
<pin name="9(MISO2/RX1/SDA1)"/>
<pin name="CD"/>
<pin name="WP"/>
<pin name="VDD"/>
<pin name="ID"/>
<pin name="GND"/>
<pin name="S1"/>
<pin name="S2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ALM-1412">
<description>&lt;b&gt;GPS Antenna Amp&lt;/b&gt;
Filter and Amp built into one. Very small package.</description>
<gates>
<gate name="G$1" symbol="ALM-1412"/>
</gates>
<devices>
<device name="SMD" package="ALM-1412">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="5"/>
<connect gate="G$1" pin="RF_OUT" pad="3"/>
<connect gate="G$1" pin="SD" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA">
<description>&lt;b&gt;Chip antenna&lt;/b&gt;&lt;p&gt;
Chip antenna with ground or secondary connection. Common with larger metal RF connectors.</description>
<gates>
<gate name="G$1" symbol="ANTENNA"/>
</gates>
<devices>
<device name="SMD1" package="ANTENNA-CHIP">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA2">
<description>&lt;b&gt;Chip antenna&lt;/b&gt;&lt;p&gt;
Single endded antenna. Common with smaller chip antennas. CHIP4 package is the GPS Chip Antenna &lt;b&gt;SKU:&lt;/b&gt; GPS-08418. CHIP5 package is 2.4GHz chip antenna &lt;b&gt;SKU:&lt;/b&gt; WRL-00144.</description>
<gates>
<gate name="G$1" symbol="ANTENNA2"/>
</gates>
<devices>
<device name="SMD" package="ANTENNA-CHIP2">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="ANTENNA-CHIP3">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD3" package="ANTENNA-CHIP4">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD5" package="ANTENNA-CHIP5">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD6" package="ANTENNA-CHIP6">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA128RFA1" prefix="U">
<description>Atmel 8-bit micro with 802.15.4 wireless support and 128k flash</description>
<gates>
<gate name="G$1" symbol="ATMEGA128RFA1"/>
</gates>
<devices>
<device name="" package="QFN-64">
<connects>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVDD" pad="60"/>
<connect gate="G$1" pin="AVSS@58" pad="58"/>
<connect gate="G$1" pin="AVSS@61" pad="61"/>
<connect gate="G$1" pin="AVSS_RFN" pad="10"/>
<connect gate="G$1" pin="AVSS_RFP" pad="7"/>
<connect gate="G$1" pin="CLKI" pad="33"/>
<connect gate="G$1" pin="DEVDD@23" pad="23"/>
<connect gate="G$1" pin="DEVDD@34" pad="34"/>
<connect gate="G$1" pin="DEVDD@44" pad="44"/>
<connect gate="G$1" pin="DEVDD@54" pad="54"/>
<connect gate="G$1" pin="DVDD@21" pad="21"/>
<connect gate="G$1" pin="DVDD@22" pad="22"/>
<connect gate="G$1" pin="DVSS@20" pad="20"/>
<connect gate="G$1" pin="DVSS@24" pad="24"/>
<connect gate="G$1" pin="DVSS@35" pad="35"/>
<connect gate="G$1" pin="DVSS@45" pad="45"/>
<connect gate="G$1" pin="DVSS@55" pad="55"/>
<connect gate="G$1" pin="EVDD" pad="59"/>
<connect gate="G$1" pin="PB0" pad="36"/>
<connect gate="G$1" pin="PB1/SCK" pad="37"/>
<connect gate="G$1" pin="PB2/PDI" pad="38"/>
<connect gate="G$1" pin="PB3/PDO" pad="39"/>
<connect gate="G$1" pin="PB4" pad="40"/>
<connect gate="G$1" pin="PB5" pad="41"/>
<connect gate="G$1" pin="PB6" pad="42"/>
<connect gate="G$1" pin="PB7" pad="43"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PE0" pad="46"/>
<connect gate="G$1" pin="PE1" pad="47"/>
<connect gate="G$1" pin="PE2" pad="48"/>
<connect gate="G$1" pin="PE3" pad="49"/>
<connect gate="G$1" pin="PE4" pad="50"/>
<connect gate="G$1" pin="PE5" pad="51"/>
<connect gate="G$1" pin="PE6" pad="52"/>
<connect gate="G$1" pin="PE7" pad="53"/>
<connect gate="G$1" pin="PF0" pad="63"/>
<connect gate="G$1" pin="PF1" pad="64"/>
<connect gate="G$1" pin="PF2" pad="1"/>
<connect gate="G$1" pin="PF3" pad="2"/>
<connect gate="G$1" pin="PF4" pad="3"/>
<connect gate="G$1" pin="PF5" pad="4"/>
<connect gate="G$1" pin="PF6" pad="5"/>
<connect gate="G$1" pin="PF7" pad="6"/>
<connect gate="G$1" pin="PG0" pad="14"/>
<connect gate="G$1" pin="PG1" pad="15"/>
<connect gate="G$1" pin="PG2" pad="16"/>
<connect gate="G$1" pin="PG3" pad="17"/>
<connect gate="G$1" pin="PG4" pad="18"/>
<connect gate="G$1" pin="PG5" pad="19"/>
<connect gate="G$1" pin="RFN" pad="9"/>
<connect gate="G$1" pin="RFP" pad="8"/>
<connect gate="G$1" pin="RSTN" pad="12"/>
<connect gate="G$1" pin="RSTON" pad="13"/>
<connect gate="G$1" pin="TST" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="57"/>
<connect gate="G$1" pin="XTAL2" pad="56"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BALUN" prefix="B">
<description>0805 footprint balun- Ember 351/357</description>
<gates>
<gate name="G$1" symbol="BALUN"/>
</gates>
<devices>
<device name="0805" package="BALUN">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BGB203_BLUETOOTH">
<description>Bluetooth SMD IC</description>
<gates>
<gate name="G$1" symbol="BGB203_BLUETOOTH"/>
</gates>
<devices>
<device name="OLD" package="BGB203_ORIGINAL">
<connects>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="BTACT/GPIO[17]" pad="14"/>
<connect gate="G$1" pin="CTS/GPIO[2]" pad="42"/>
<connect gate="G$1" pin="DN_USB" pad="37"/>
<connect gate="G$1" pin="DP_USB" pad="38"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="GPIO[10]" pad="23"/>
<connect gate="G$1" pin="GPIO[11]" pad="22"/>
<connect gate="G$1" pin="GPIO[12]" pad="12"/>
<connect gate="G$1" pin="GPIO[13]" pad="21"/>
<connect gate="G$1" pin="GPIO[14]" pad="11"/>
<connect gate="G$1" pin="GPIO[15]" pad="30"/>
<connect gate="G$1" pin="GPIO[16]" pad="25"/>
<connect gate="G$1" pin="GPIO[6]" pad="33"/>
<connect gate="G$1" pin="GPIO[7]" pad="31"/>
<connect gate="G$1" pin="GPIO[8]" pad="34"/>
<connect gate="G$1" pin="GPIO[9]" pad="32"/>
<connect gate="G$1" pin="I2C_SCL/GPIO[0]" pad="17"/>
<connect gate="G$1" pin="I2C_SDA/GPIO[1]" pad="16"/>
<connect gate="G$1" pin="RESET_N" pad="43"/>
<connect gate="G$1" pin="RTS/GPIO[3]" pad="39"/>
<connect gate="G$1" pin="RX/GPIO[5]" pad="40"/>
<connect gate="G$1" pin="TCK_JTAG" pad="48"/>
<connect gate="G$1" pin="TDI_JTAG" pad="47"/>
<connect gate="G$1" pin="TDO_JTAG" pad="46"/>
<connect gate="G$1" pin="TMS_JTAG" pad="45"/>
<connect gate="G$1" pin="TX/GPIO[4]" pad="41"/>
<connect gate="G$1" pin="VANLO" pad="15"/>
<connect gate="G$1" pin="VBUS_USB" pad="29"/>
<connect gate="G$1" pin="VDDA/VDDO" pad="18"/>
<connect gate="G$1" pin="VDDC" pad="35"/>
<connect gate="G$1" pin="VDDC/VDDIO1" pad="24"/>
<connect gate="G$1" pin="VDDIO1" pad="26"/>
<connect gate="G$1" pin="VDDIO2" pad="36"/>
<connect gate="G$1" pin="VDDIORF" pad="44"/>
<connect gate="G$1" pin="VDDRF" pad="13"/>
<connect gate="G$1" pin="XTAL1_LP" pad="27"/>
<connect gate="G$1" pin="XTAL1_SYS" pad="20"/>
<connect gate="G$1" pin="XTAL2_LP" pad="28"/>
<connect gate="G$1" pin="XTAL2_SYS" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="BGB203">
<connects>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="BTACT/GPIO[17]" pad="14"/>
<connect gate="G$1" pin="CTS/GPIO[2]" pad="42"/>
<connect gate="G$1" pin="DN_USB" pad="37"/>
<connect gate="G$1" pin="DP_USB" pad="38"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="GPIO[10]" pad="23"/>
<connect gate="G$1" pin="GPIO[11]" pad="22"/>
<connect gate="G$1" pin="GPIO[12]" pad="12"/>
<connect gate="G$1" pin="GPIO[13]" pad="21"/>
<connect gate="G$1" pin="GPIO[14]" pad="11"/>
<connect gate="G$1" pin="GPIO[15]" pad="30"/>
<connect gate="G$1" pin="GPIO[16]" pad="25"/>
<connect gate="G$1" pin="GPIO[6]" pad="33"/>
<connect gate="G$1" pin="GPIO[7]" pad="31"/>
<connect gate="G$1" pin="GPIO[8]" pad="34"/>
<connect gate="G$1" pin="GPIO[9]" pad="32"/>
<connect gate="G$1" pin="I2C_SCL/GPIO[0]" pad="17"/>
<connect gate="G$1" pin="I2C_SDA/GPIO[1]" pad="16"/>
<connect gate="G$1" pin="RESET_N" pad="43"/>
<connect gate="G$1" pin="RTS/GPIO[3]" pad="39"/>
<connect gate="G$1" pin="RX/GPIO[5]" pad="40"/>
<connect gate="G$1" pin="TCK_JTAG" pad="48"/>
<connect gate="G$1" pin="TDI_JTAG" pad="47"/>
<connect gate="G$1" pin="TDO_JTAG" pad="46"/>
<connect gate="G$1" pin="TMS_JTAG" pad="45"/>
<connect gate="G$1" pin="TX/GPIO[4]" pad="41"/>
<connect gate="G$1" pin="VANLO" pad="15"/>
<connect gate="G$1" pin="VBUS_USB" pad="29"/>
<connect gate="G$1" pin="VDDA/VDDO" pad="18"/>
<connect gate="G$1" pin="VDDC" pad="35"/>
<connect gate="G$1" pin="VDDC/VDDIO1" pad="24"/>
<connect gate="G$1" pin="VDDIO1" pad="26"/>
<connect gate="G$1" pin="VDDIO2" pad="36"/>
<connect gate="G$1" pin="VDDIORF" pad="44"/>
<connect gate="G$1" pin="VDDRF" pad="13"/>
<connect gate="G$1" pin="XTAL1_LP" pad="27"/>
<connect gate="G$1" pin="XTAL1_SYS" pad="20"/>
<connect gate="G$1" pin="XTAL2_LP" pad="28"/>
<connect gate="G$1" pin="XTAL2_SYS" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUERADIO_BR-C40A">
<description>&lt;b&gt;Bluetooth SMD Module&lt;/b&gt;
Footprint fully proven. Spark Fun Electronics SKU : WRL-00149</description>
<gates>
<gate name="G$1" symbol="BLUERADIO_BR-C40A"/>
</gates>
<devices>
<device name="BAS" package="BLUERADIO_BR-C40A">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUERADIO_BR-C40N">
<description>&lt;b&gt;Bluetooth SMD Module&lt;/b&gt;
BR-C40A with antenna cut off. 50 Ohm antenna trace and connector required. Footprint fully proven. Spark Fun Electronics SKU : WRL-00149</description>
<gates>
<gate name="G$1" symbol="BLUERADIO_BR-C40N"/>
</gates>
<devices>
<device name="BAS" package="BLUERADIO_BR-C40N">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFE" package="BLUETOOTH-SMD-FP">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="INTERNAL" package="BLUETOOTH-INTERNAL-FP">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="INT2" package="BLUETOOTH-INTERNAL-FP2">
<connects>
<connect gate="G$1" pin="ANT" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="29"/>
<connect gate="G$1" pin="PCM_CLK" pad="7"/>
<connect gate="G$1" pin="PCM_IN" pad="9"/>
<connect gate="G$1" pin="PCM_OUT" pad="10"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_2/CONNECT" pad="19"/>
<connect gate="G$1" pin="PIO_3/INT" pad="20"/>
<connect gate="G$1" pin="PIO_4/FACRST" pad="22"/>
<connect gate="G$1" pin="PIO_5/STATUS" pad="21"/>
<connect gate="G$1" pin="PIO_6" pad="3"/>
<connect gate="G$1" pin="PIO_7" pad="4"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CLK" pad="6"/>
<connect gate="G$1" pin="SPI_CSB" pad="23"/>
<connect gate="G$1" pin="SPI_MISO" pad="24"/>
<connect gate="G$1" pin="SPI_MOSI" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="16"/>
<connect gate="G$1" pin="UART_RTS" pad="15"/>
<connect gate="G$1" pin="UART_RX" pad="13"/>
<connect gate="G$1" pin="UART_TX" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUETOOTH-RN41">
<description>Bluetooth SMD module</description>
<gates>
<gate name="G$1" symbol="RN41"/>
</gates>
<devices>
<device name="&quot;" package="RN41">
<connects>
<connect gate="G$1" pin="AIO1" pad="35"/>
<connect gate="G$1" pin="AIO2" pad="30"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="GND3" pad="27"/>
<connect gate="G$1" pin="GND4" pad="28"/>
<connect gate="G$1" pin="GND5" pad="29"/>
<connect gate="G$1" pin="NC" pad="26"/>
<connect gate="G$1" pin="PCMCLK" pad="7"/>
<connect gate="G$1" pin="PCMIN" pad="9"/>
<connect gate="G$1" pin="PCMOUT" pad="10"/>
<connect gate="G$1" pin="PCMSYNC" pad="8"/>
<connect gate="G$1" pin="PIO10" pad="33"/>
<connect gate="G$1" pin="PIO11" pad="34"/>
<connect gate="G$1" pin="PIO2" pad="19"/>
<connect gate="G$1" pin="PIO3" pad="20"/>
<connect gate="G$1" pin="PIO4" pad="22"/>
<connect gate="G$1" pin="PIO5" pad="21"/>
<connect gate="G$1" pin="PIO6" pad="3"/>
<connect gate="G$1" pin="PIO7" pad="4"/>
<connect gate="G$1" pin="PIO8" pad="31"/>
<connect gate="G$1" pin="PIO9" pad="32"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPICLK" pad="6"/>
<connect gate="G$1" pin="SPICSB" pad="23"/>
<connect gate="G$1" pin="SPIMISO" pad="24"/>
<connect gate="G$1" pin="SPIMOSI" pad="2"/>
<connect gate="G$1" pin="UARTCTS" pad="16"/>
<connect gate="G$1" pin="UARTRTS" pad="15"/>
<connect gate="G$1" pin="UARTRX" pad="13"/>
<connect gate="G$1" pin="UARTTX" pad="14"/>
<connect gate="G$1" pin="USBD+" pad="17"/>
<connect gate="G$1" pin="USBD-" pad="18"/>
<connect gate="G$1" pin="VDD" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTM182" prefix="U">
<description>BTM-182 Bluetooth Module from Rayson</description>
<gates>
<gate name="G$1" symbol="BTM182"/>
</gates>
<devices>
<device name="_" package="BTM182">
<connects>
<connect gate="G$1" pin="AIO0" pad="2"/>
<connect gate="G$1" pin="AIO1" pad="3"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="PCM_CLK" pad="5"/>
<connect gate="G$1" pin="PCM_IN" pad="7"/>
<connect gate="G$1" pin="PCM_OUT" pad="4"/>
<connect gate="G$1" pin="PCM_SYNC" pad="6"/>
<connect gate="G$1" pin="PIO0" pad="31"/>
<connect gate="G$1" pin="PIO1" pad="32"/>
<connect gate="G$1" pin="PIO10" pad="30"/>
<connect gate="G$1" pin="PIO11" pad="1"/>
<connect gate="G$1" pin="PIO2" pad="27"/>
<connect gate="G$1" pin="PIO3" pad="26"/>
<connect gate="G$1" pin="PIO4" pad="25"/>
<connect gate="G$1" pin="PIO5" pad="24"/>
<connect gate="G$1" pin="PIO6" pad="23"/>
<connect gate="G$1" pin="PIO7" pad="22"/>
<connect gate="G$1" pin="PIO8" pad="28"/>
<connect gate="G$1" pin="PIO9" pad="29"/>
<connect gate="G$1" pin="RESET" pad="21"/>
<connect gate="G$1" pin="SPI_CLK" pad="20"/>
<connect gate="G$1" pin="SPI_CSB" pad="18"/>
<connect gate="G$1" pin="SPI_MISO" pad="19"/>
<connect gate="G$1" pin="SPI_MOSI" pad="17"/>
<connect gate="G$1" pin="UART_CTS" pad="8"/>
<connect gate="G$1" pin="UART_RTS" pad="11"/>
<connect gate="G$1" pin="UART_RX" pad="10"/>
<connect gate="G$1" pin="UART_TX" pad="9"/>
<connect gate="G$1" pin="USB_DN" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="12"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDD_USB" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COPERNICUS" prefix="IC">
<description>Copernicus II GPS-  Trimble recommended layout and paste layer. Footprint production proven. Spark Fun Electronics SKU : GPS-07951</description>
<gates>
<gate name="G$2" symbol="COPERNICUS"/>
</gates>
<devices>
<device name="SMD" package="COPERNICUS">
<connects>
<connect gate="G$2" pin="BOOT" pad="10"/>
<connect gate="G$2" pin="GND@1" pad="1"/>
<connect gate="G$2" pin="GND@2" pad="2"/>
<connect gate="G$2" pin="GND@3" pad="4"/>
<connect gate="G$2" pin="GND@4" pad="13"/>
<connect gate="G$2" pin="GND@5" pad="14"/>
<connect gate="G$2" pin="GND@6" pad="15"/>
<connect gate="G$2" pin="GND@7" pad="27"/>
<connect gate="G$2" pin="GND@8" pad="28"/>
<connect gate="G$2" pin="LNA" pad="5"/>
<connect gate="G$2" pin="OPEN" pad="7"/>
<connect gate="G$2" pin="PPS" pad="19"/>
<connect gate="G$2" pin="RESERVED1" pad="6"/>
<connect gate="G$2" pin="RESERVED2" pad="9"/>
<connect gate="G$2" pin="RESERVED3" pad="17"/>
<connect gate="G$2" pin="RESERVED4" pad="18"/>
<connect gate="G$2" pin="RESERVED5" pad="22"/>
<connect gate="G$2" pin="RESERVED6" pad="25"/>
<connect gate="G$2" pin="RESERVED7" pad="26"/>
<connect gate="G$2" pin="RFIN" pad="3"/>
<connect gate="G$2" pin="RXD-A" pad="21"/>
<connect gate="G$2" pin="RXD-B" pad="20"/>
<connect gate="G$2" pin="SHORT" pad="8"/>
<connect gate="G$2" pin="TXD-A" pad="23"/>
<connect gate="G$2" pin="TXD-B" pad="24"/>
<connect gate="G$2" pin="VCC" pad="12"/>
<connect gate="G$2" pin="XRESET" pad="11"/>
<connect gate="G$2" pin="XSTANDBY" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COPERNICUS-DIP">
<description>Copernicus II dip module, SKU GPS-10923</description>
<gates>
<gate name="G$1" symbol="COPERNICUS-DIP"/>
</gates>
<devices>
<device name="PTH" package="COPERNICUS-DIP">
<connects>
<connect gate="G$1" pin="BOOT" pad="6"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="LNA" pad="1"/>
<connect gate="G$1" pin="OPEN" pad="3"/>
<connect gate="G$1" pin="PPS" pad="13"/>
<connect gate="G$1" pin="RESERVED1" pad="2"/>
<connect gate="G$1" pin="RESERVED2" pad="5"/>
<connect gate="G$1" pin="RESERVED3" pad="11"/>
<connect gate="G$1" pin="RESERVED4" pad="12"/>
<connect gate="G$1" pin="RESERVED5" pad="16"/>
<connect gate="G$1" pin="RESERVED6" pad="19"/>
<connect gate="G$1" pin="RESERVED7" pad="20"/>
<connect gate="G$1" pin="RXD-A" pad="15"/>
<connect gate="G$1" pin="RXD-B" pad="14"/>
<connect gate="G$1" pin="SHORT" pad="4"/>
<connect gate="G$1" pin="TXD-A" pad="17"/>
<connect gate="G$1" pin="TXD-B" pad="18"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XRESET" pad="7"/>
<connect gate="G$1" pin="XSTANDBY" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="D2523T" prefix="U">
<description>D2523T GPS Module</description>
<gates>
<gate name="G$1" symbol="D2523T"/>
</gates>
<devices>
<device name="_" package="EM406">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LED" pad="1"/>
<connect gate="G$1" pin="RX" pad="6"/>
<connect gate="G$1" pin="TX" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="2"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EBM001">
<description>Bluetooth module</description>
<gates>
<gate name="G$1" symbol="EMB001"/>
</gates>
<devices>
<device name="" package="EMB001">
<connects>
<connect gate="G$1" pin="1V8" pad="23"/>
<connect gate="G$1" pin="AIO0" pad="34"/>
<connect gate="G$1" pin="AIO1" pad="33"/>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="CTS" pad="27"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="19"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="GND@3" pad="21"/>
<connect gate="G$1" pin="GND@4" pad="35"/>
<connect gate="G$1" pin="GND@5" pad="36"/>
<connect gate="G$1" pin="GND@6" pad="37"/>
<connect gate="G$1" pin="GND@7" pad="38"/>
<connect gate="G$1" pin="GND@8" pad="39"/>
<connect gate="G$1" pin="GND@9" pad="42"/>
<connect gate="G$1" pin="MISO" pad="31"/>
<connect gate="G$1" pin="MOSI" pad="28"/>
<connect gate="G$1" pin="PCM_CLK" pad="15"/>
<connect gate="G$1" pin="PCM_IN" pad="16"/>
<connect gate="G$1" pin="PCM_OUT" pad="18"/>
<connect gate="G$1" pin="PCM_SYNC" pad="17"/>
<connect gate="G$1" pin="PIO0" pad="41"/>
<connect gate="G$1" pin="PIO1" pad="40"/>
<connect gate="G$1" pin="PIO10" pad="11"/>
<connect gate="G$1" pin="PIO11" pad="12"/>
<connect gate="G$1" pin="PIO2" pad="3"/>
<connect gate="G$1" pin="PIO3" pad="4"/>
<connect gate="G$1" pin="PIO4" pad="5"/>
<connect gate="G$1" pin="PIO5" pad="6"/>
<connect gate="G$1" pin="PIO6" pad="7"/>
<connect gate="G$1" pin="PIO7" pad="8"/>
<connect gate="G$1" pin="PIO8" pad="9"/>
<connect gate="G$1" pin="PIO9" pad="10"/>
<connect gate="G$1" pin="RST" pad="32"/>
<connect gate="G$1" pin="RTS" pad="25"/>
<connect gate="G$1" pin="RX" pad="24"/>
<connect gate="G$1" pin="SPI_CLK" pad="29"/>
<connect gate="G$1" pin="SPI_CSB" pad="30"/>
<connect gate="G$1" pin="TX" pad="26"/>
<connect gate="G$1" pin="USB_DN" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="14"/>
<connect gate="G$1" pin="VSUP" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM406_OUTLINE">
<description>Package outline for EM406 GPS module</description>
<gates>
<gate name="G$1" symbol="EM406_OUTLINE"/>
</gates>
<devices>
<device name="" package="EM406_OUTLINE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM408_OUTLINE">
<description>This device is only the outline of the EM408 GPS receiver.  The device is intended to give the
designer an idea of what how the receiver will fit on the board.  THIS DEVICE DOES NOT PROVIDE ANY ELECTRICAL CONNECTION TO THE BOARD!  Include the "EM408_CON" device in order to connect the EM408 to your design.</description>
<gates>
<gate name="G$1" symbol="EM408_OUTLINE"/>
</gates>
<devices>
<device name="" package="EM408_OUTLINE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ET312">
<description>&lt;b&gt;ET312 GPS Receiver&lt;/b&gt;
Proven layout and schematic for SiRF III ET312 GPS receiver. This footprint has been tweaked significantly to work with the ET312. This footprint has been fully qualified. Spark Fun Electronics SKU : GPS-08268.</description>
<gates>
<gate name="G$1" symbol="ET312"/>
</gates>
<devices>
<device name="SMD" package="ET312">
<connects>
<connect gate="G$1" pin="BATT" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="2"/>
<connect gate="G$1" pin="GND3" pad="8"/>
<connect gate="G$1" pin="GND4" pad="9"/>
<connect gate="G$1" pin="GND5" pad="10"/>
<connect gate="G$1" pin="GND6" pad="11"/>
<connect gate="G$1" pin="GND7" pad="13"/>
<connect gate="G$1" pin="GPIO1" pad="5"/>
<connect gate="G$1" pin="RF" pad="12"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE863_GPS">
<description>&lt;b&gt;GE863 Cellular Module with GPS&lt;/b&gt;
Proto layout and schematic for GE863 cellular module with SiRF III GPS. Spark Fun Electronics SKU : CEL-08246</description>
<gates>
<gate name="G$1" symbol="GE863"/>
</gates>
<devices>
<device name="" package="GE863">
<connects>
<connect gate="G$1" pin="ADC_IN1" pad="23"/>
<connect gate="G$1" pin="ANT" pad="49"/>
<connect gate="G$1" pin="AXE" pad="30"/>
<connect gate="G$1" pin="C103/TXD" pad="37"/>
<connect gate="G$1" pin="C104/RXD" pad="38"/>
<connect gate="G$1" pin="C105/RTS" pad="40"/>
<connect gate="G$1" pin="C106/CTS" pad="41"/>
<connect gate="G$1" pin="C107/DSR" pad="43"/>
<connect gate="G$1" pin="C108/DTR" pad="39"/>
<connect gate="G$1" pin="C109/DCD" pad="42"/>
<connect gate="G$1" pin="C125/RING" pad="44"/>
<connect gate="G$1" pin="CAM_CLK" pad="7"/>
<connect gate="G$1" pin="CHARGE" pad="35"/>
<connect gate="G$1" pin="DAC_OUT" pad="63"/>
<connect gate="G$1" pin="EAR_HF+" pad="11"/>
<connect gate="G$1" pin="EAR_HF-" pad="12"/>
<connect gate="G$1" pin="EAR_MT+" pad="10"/>
<connect gate="G$1" pin="EAR_MT-" pad="9"/>
<connect gate="G$1" pin="GND@0" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="17"/>
<connect gate="G$1" pin="GND@10" pad="72"/>
<connect gate="G$1" pin="GND@11" pad="77"/>
<connect gate="G$1" pin="GND@12" pad="79"/>
<connect gate="G$1" pin="GND@13" pad="82"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="36"/>
<connect gate="G$1" pin="GND@4" pad="45"/>
<connect gate="G$1" pin="GND@5" pad="48"/>
<connect gate="G$1" pin="GND@6" pad="50"/>
<connect gate="G$1" pin="GND@7" pad="56"/>
<connect gate="G$1" pin="GND@8" pad="67"/>
<connect gate="G$1" pin="GND@9" pad="69"/>
<connect gate="G$1" pin="GND_GPS" pad="84"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO10" pad="4"/>
<connect gate="G$1" pin="GPIO11" pad="3"/>
<connect gate="G$1" pin="GPIO12" pad="2"/>
<connect gate="G$1" pin="GPIO13" pad="1"/>
<connect gate="G$1" pin="GPIO14" pad="60"/>
<connect gate="G$1" pin="GPIO15" pad="71"/>
<connect gate="G$1" pin="GPIO16" pad="64"/>
<connect gate="G$1" pin="GPIO17" pad="59"/>
<connect gate="G$1" pin="GPIO18" pad="76"/>
<connect gate="G$1" pin="GPIO2/JDR" pad="33"/>
<connect gate="G$1" pin="GPIO3/CAM_SCL" pad="55"/>
<connect gate="G$1" pin="GPIO4/CAM_SDA" pad="32"/>
<connect gate="G$1" pin="GPIO5" pad="53"/>
<connect gate="G$1" pin="GPIO6" pad="54"/>
<connect gate="G$1" pin="GPIO7/BUZZER" pad="51"/>
<connect gate="G$1" pin="GPIO8/CAM_ON" pad="6"/>
<connect gate="G$1" pin="GPIO9/CAM_RST" pad="5"/>
<connect gate="G$1" pin="GPS_ANT" pad="83"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="16"/>
<connect gate="G$1" pin="MIC_MT+" pad="13"/>
<connect gate="G$1" pin="MIN_MT-" pad="14"/>
<connect gate="G$1" pin="ON/OFF" pad="46"/>
<connect gate="G$1" pin="PPS" pad="75"/>
<connect gate="G$1" pin="PWRMON" pad="52"/>
<connect gate="G$1" pin="RESET" pad="47"/>
<connect gate="G$1" pin="RX_GPS" pad="73"/>
<connect gate="G$1" pin="RX_GPS_BIN" pad="78"/>
<connect gate="G$1" pin="RX_TRACE" pad="26"/>
<connect gate="G$1" pin="SIMCLK" pad="18"/>
<connect gate="G$1" pin="SIMIN" pad="21"/>
<connect gate="G$1" pin="SIMIO" pad="20"/>
<connect gate="G$1" pin="SIMRST" pad="19"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="29"/>
<connect gate="G$1" pin="TX_GPS" pad="68"/>
<connect gate="G$1" pin="TX_GPS_BIN" pad="80"/>
<connect gate="G$1" pin="TX_TRACE" pad="25"/>
<connect gate="G$1" pin="VAUX1" pad="31"/>
<connect gate="G$1" pin="VBATT" pad="27"/>
<connect gate="G$1" pin="VRTC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE864">
<description>Telit quad cell module (see CEL-09296)</description>
<gates>
<gate name="G$1" symbol="GE864"/>
</gates>
<devices>
<device name="" package="GE864">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="J11"/>
<connect gate="G$1" pin="ADC_IN2" pad="H11"/>
<connect gate="G$1" pin="ADC_IN3" pad="G11"/>
<connect gate="G$1" pin="ANTENNA" pad="L4"/>
<connect gate="G$1" pin="AXE" pad="F9"/>
<connect gate="G$1" pin="C103/TXD" pad="E7"/>
<connect gate="G$1" pin="C104/RXD" pad="H8"/>
<connect gate="G$1" pin="C105/RTS" pad="F7"/>
<connect gate="G$1" pin="C106/CTS" pad="F6"/>
<connect gate="G$1" pin="C107/DSR" pad="E11"/>
<connect gate="G$1" pin="C108/DTR" pad="B7"/>
<connect gate="G$1" pin="C109/DCD" pad="D9"/>
<connect gate="G$1" pin="C125/RING" pad="B6"/>
<connect gate="G$1" pin="CHARGE@G1" pad="G1"/>
<connect gate="G$1" pin="CHARGE@G2" pad="G2"/>
<connect gate="G$1" pin="DAC_OUT" pad="C7"/>
<connect gate="G$1" pin="DV12_CLK" pad="D7"/>
<connect gate="G$1" pin="EAR_HF+" pad="H10"/>
<connect gate="G$1" pin="EAR_HF-" pad="J10"/>
<connect gate="G$1" pin="EAR_MT+" pad="G10"/>
<connect gate="G$1" pin="EAR_MT-" pad="H9"/>
<connect gate="G$1" pin="GND@A1" pad="A1"/>
<connect gate="G$1" pin="GND@A11" pad="A11"/>
<connect gate="G$1" pin="GND@D6" pad="D6"/>
<connect gate="G$1" pin="GND@F1" pad="F1"/>
<connect gate="G$1" pin="GND@F11" pad="F11"/>
<connect gate="G$1" pin="GND@H1" pad="H1"/>
<connect gate="G$1" pin="GND@H2" pad="H2"/>
<connect gate="G$1" pin="GND@J3" pad="J3"/>
<connect gate="G$1" pin="GND@K3" pad="K3"/>
<connect gate="G$1" pin="GND@K4" pad="K4"/>
<connect gate="G$1" pin="GND@K5" pad="K5"/>
<connect gate="G$1" pin="GND@K6" pad="K6"/>
<connect gate="G$1" pin="GND@L1" pad="L1"/>
<connect gate="G$1" pin="GND@L11" pad="L11"/>
<connect gate="G$1" pin="GND@L2" pad="L2"/>
<connect gate="G$1" pin="GND@L3" pad="L3"/>
<connect gate="G$1" pin="GND@L6" pad="L6"/>
<connect gate="G$1" pin="MIC_HF+" pad="G8"/>
<connect gate="G$1" pin="MIC_HF-" pad="J9"/>
<connect gate="G$1" pin="MIC_MT+" pad="J8"/>
<connect gate="G$1" pin="MIC_MT-" pad="G9"/>
<connect gate="G$1" pin="ON_OFF" pad="J5"/>
<connect gate="G$1" pin="PWRMON" pad="L8"/>
<connect gate="G$1" pin="RESET" pad="A2"/>
<connect gate="G$1" pin="RX_TRACE" pad="F10"/>
<connect gate="G$1" pin="SIMCLK" pad="C10"/>
<connect gate="G$1" pin="SIMIN" pad="C11"/>
<connect gate="G$1" pin="SIMIO" pad="D10"/>
<connect gate="G$1" pin="SIMRST" pad="E9"/>
<connect gate="G$1" pin="SIMVCC" pad="D4"/>
<connect gate="G$1" pin="STAT_LED" pad="D8"/>
<connect gate="G$1" pin="TGPIO_01" pad="C1"/>
<connect gate="G$1" pin="TGPIO_02/JDR" pad="E6"/>
<connect gate="G$1" pin="TGPIO_03" pad="C2"/>
<connect gate="G$1" pin="TGPIO_04" pad="B3"/>
<connect gate="G$1" pin="TGPIO_05/RFTXMON" pad="K8"/>
<connect gate="G$1" pin="TGPIO_06/ALARM" pad="B5"/>
<connect gate="G$1" pin="TGPIO_07/BUZZER" pad="L9"/>
<connect gate="G$1" pin="TGPIO_08" pad="K11"/>
<connect gate="G$1" pin="TGPIO_09" pad="C9"/>
<connect gate="G$1" pin="TGPIO_10" pad="H3"/>
<connect gate="G$1" pin="TGPIO_11" pad="D1"/>
<connect gate="G$1" pin="TGPIO_12" pad="G4"/>
<connect gate="G$1" pin="TGPIO_13" pad="K10"/>
<connect gate="G$1" pin="TGPIO_14" pad="B4"/>
<connect gate="G$1" pin="TGPIO_15" pad="F5"/>
<connect gate="G$1" pin="TGPIO_16" pad="H6"/>
<connect gate="G$1" pin="TGPIO_17" pad="H5"/>
<connect gate="G$1" pin="TGPIO_18" pad="K7"/>
<connect gate="G$1" pin="TGPIO_19" pad="B1"/>
<connect gate="G$1" pin="TGPIO_20" pad="C3"/>
<connect gate="G$1" pin="TGPIO_21" pad="L10"/>
<connect gate="G$1" pin="TGPIO_22" pad="E8"/>
<connect gate="G$1" pin="TX_TRACE" pad="D11"/>
<connect gate="G$1" pin="VAUX1" pad="D5"/>
<connect gate="G$1" pin="VBATT@J1" pad="J1"/>
<connect gate="G$1" pin="VBATT@J2" pad="J2"/>
<connect gate="G$1" pin="VBATT@K1" pad="K1"/>
<connect gate="G$1" pin="VBATT@K2" pad="K2"/>
<connect gate="G$1" pin="VRTC" pad="E2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE865">
<description>Telit quad cell module (CEL-09720)</description>
<gates>
<gate name="G$1" symbol="GE865"/>
</gates>
<devices>
<device name="" package="GE865">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="F5"/>
<connect gate="G$1" pin="ADC_IN2" pad="F6"/>
<connect gate="G$1" pin="ANTENNA" pad="H5"/>
<connect gate="G$1" pin="C103/TXD" pad="A3"/>
<connect gate="G$1" pin="C104/RXD" pad="A4"/>
<connect gate="G$1" pin="C105/RTS" pad="A1"/>
<connect gate="G$1" pin="C106/CTS" pad="A2"/>
<connect gate="G$1" pin="C107/DSR" pad="B2"/>
<connect gate="G$1" pin="C108/DTR" pad="B3"/>
<connect gate="G$1" pin="C109/DCD" pad="B5"/>
<connect gate="G$1" pin="C125/RING" pad="B4"/>
<connect gate="G$1" pin="DAC_OUT" pad="G7"/>
<connect gate="G$1" pin="EAR+" pad="D8"/>
<connect gate="G$1" pin="EAR-" pad="E8"/>
<connect gate="G$1" pin="GND@C2" pad="C2"/>
<connect gate="G$1" pin="GND@C7" pad="C7"/>
<connect gate="G$1" pin="GND@E5" pad="E5"/>
<connect gate="G$1" pin="GND@E7" pad="E7"/>
<connect gate="G$1" pin="GND@G1" pad="G1"/>
<connect gate="G$1" pin="GND@G3" pad="G3"/>
<connect gate="G$1" pin="GND@G4" pad="G4"/>
<connect gate="G$1" pin="GND@G5" pad="G5"/>
<connect gate="G$1" pin="GND@H3" pad="H3"/>
<connect gate="G$1" pin="GND@H6" pad="H6"/>
<connect gate="G$1" pin="GPIO_01" pad="D3"/>
<connect gate="G$1" pin="GPIO_02/JDR" pad="D2"/>
<connect gate="G$1" pin="GPIO_03" pad="E4"/>
<connect gate="G$1" pin="GPIO_04/TX_DISAB" pad="H7"/>
<connect gate="G$1" pin="GPIO_05/RFTXMON" pad="G2"/>
<connect gate="G$1" pin="GPIO_06/ALARM" pad="H8"/>
<connect gate="G$1" pin="GPIO_07/BUZZER" pad="G6"/>
<connect gate="G$1" pin="GPIO_08" pad="D4"/>
<connect gate="G$1" pin="GPIO_09" pad="F4"/>
<connect gate="G$1" pin="GPIO_10" pad="E3"/>
<connect gate="G$1" pin="MIC+" pad="B8"/>
<connect gate="G$1" pin="MIC-" pad="C8"/>
<connect gate="G$1" pin="ON_OFF" pad="B1"/>
<connect gate="G$1" pin="PWRMON" pad="E2"/>
<connect gate="G$1" pin="RESET" pad="C1"/>
<connect gate="G$1" pin="RXD_AUX" pad="E1"/>
<connect gate="G$1" pin="SIMCLK" pad="A5"/>
<connect gate="G$1" pin="SIMIN" pad="B7"/>
<connect gate="G$1" pin="SIMIO" pad="A6"/>
<connect gate="G$1" pin="SIMRST" pad="A8"/>
<connect gate="G$1" pin="SIMVCC" pad="A7"/>
<connect gate="G$1" pin="STAT_LED" pad="G8"/>
<connect gate="G$1" pin="TXD_AUX" pad="D1"/>
<connect gate="G$1" pin="VBATT@F1" pad="F1"/>
<connect gate="G$1" pin="VBATT@F2" pad="F2"/>
<connect gate="G$1" pin="VBATT@F3" pad="F3"/>
<connect gate="G$1" pin="VRTC" pad="H2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GE865_2">
<description>Telit quad cell module (CEL-09720)</description>
<gates>
<gate name="G$1" symbol="GE865_2"/>
</gates>
<devices>
<device name="" package="GE865">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="F5"/>
<connect gate="G$1" pin="ADC_IN2" pad="F6"/>
<connect gate="G$1" pin="ANTENNA" pad="H5"/>
<connect gate="G$1" pin="C103/TXD" pad="A3"/>
<connect gate="G$1" pin="C104/RXD" pad="A4"/>
<connect gate="G$1" pin="C105/RTS" pad="A1"/>
<connect gate="G$1" pin="C106/CTS" pad="A2"/>
<connect gate="G$1" pin="C107/DSR" pad="B2"/>
<connect gate="G$1" pin="C108/DTR" pad="B3"/>
<connect gate="G$1" pin="C109/DCD" pad="B5"/>
<connect gate="G$1" pin="C125/RING" pad="B4"/>
<connect gate="G$1" pin="DAC_OUT" pad="G7"/>
<connect gate="G$1" pin="EAR+" pad="D8"/>
<connect gate="G$1" pin="EAR-" pad="E8"/>
<connect gate="G$1" pin="GND@C2" pad="C2"/>
<connect gate="G$1" pin="GND@C7" pad="C7"/>
<connect gate="G$1" pin="GND@E5" pad="E5"/>
<connect gate="G$1" pin="GND@E7" pad="E7"/>
<connect gate="G$1" pin="GND@G1" pad="G1"/>
<connect gate="G$1" pin="GND@G3" pad="G3"/>
<connect gate="G$1" pin="GND@G4" pad="G4"/>
<connect gate="G$1" pin="GND@G5" pad="G5"/>
<connect gate="G$1" pin="GND@H3" pad="H3"/>
<connect gate="G$1" pin="GND@H6" pad="H6"/>
<connect gate="G$1" pin="GPIO_01" pad="D3"/>
<connect gate="G$1" pin="GPIO_02/JDR" pad="D2"/>
<connect gate="G$1" pin="GPIO_03" pad="E4"/>
<connect gate="G$1" pin="GPIO_04/TX_DISAB" pad="H7"/>
<connect gate="G$1" pin="GPIO_05/RFTXMON" pad="G2"/>
<connect gate="G$1" pin="GPIO_06/ALARM" pad="H8"/>
<connect gate="G$1" pin="GPIO_07/BUZZER" pad="G6"/>
<connect gate="G$1" pin="GPIO_08" pad="D4"/>
<connect gate="G$1" pin="GPIO_09" pad="F4"/>
<connect gate="G$1" pin="GPIO_10" pad="E3"/>
<connect gate="G$1" pin="MIC+" pad="B8"/>
<connect gate="G$1" pin="MIC-" pad="C8"/>
<connect gate="G$1" pin="ON_OFF" pad="B1"/>
<connect gate="G$1" pin="PWRMON" pad="E2"/>
<connect gate="G$1" pin="RESET" pad="C1"/>
<connect gate="G$1" pin="RXD_AUX" pad="E1"/>
<connect gate="G$1" pin="SERVICE" pad="H1"/>
<connect gate="G$1" pin="SIMCLK" pad="A5"/>
<connect gate="G$1" pin="SIMIN" pad="B7"/>
<connect gate="G$1" pin="SIMIO" pad="A6"/>
<connect gate="G$1" pin="SIMRST" pad="A8"/>
<connect gate="G$1" pin="SIMVCC" pad="A7"/>
<connect gate="G$1" pin="STAT_LED" pad="G8"/>
<connect gate="G$1" pin="TXD_AUX" pad="D1"/>
<connect gate="G$1" pin="VBATT@F1" pad="F1"/>
<connect gate="G$1" pin="VBATT@F2" pad="F2"/>
<connect gate="G$1" pin="VBATT@F3" pad="F3"/>
<connect gate="G$1" pin="VRTC" pad="H2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GM862">
<description>&lt;b&gt;GM862 Cellular Module with GPS&lt;/b&gt;
Proven layout and schematic for GM862 cellular module with SiRF III GPS. Spark Fun Electronics SKU : CEL-07917</description>
<gates>
<gate name="G$1" symbol="GM862"/>
</gates>
<devices>
<device name="GND" package="GM862">
<connects>
<connect gate="G$1" pin="AXE" pad="18"/>
<connect gate="G$1" pin="C103/TXD" pad="20"/>
<connect gate="G$1" pin="C104/RXD" pad="37"/>
<connect gate="G$1" pin="C105/RTS" pad="45"/>
<connect gate="G$1" pin="C106/CTS" pad="29"/>
<connect gate="G$1" pin="C107/DSR" pad="33"/>
<connect gate="G$1" pin="C108/DTR" pad="43"/>
<connect gate="G$1" pin="C109/DCD" pad="36"/>
<connect gate="G$1" pin="C125/RING" pad="30"/>
<connect gate="G$1" pin="CCIN/SIMIN" pad="27"/>
<connect gate="G$1" pin="CHARGE" pad="8"/>
<connect gate="G$1" pin="EAR_HF+" pad="9"/>
<connect gate="G$1" pin="EAR_HF-" pad="11"/>
<connect gate="G$1" pin="EAR_MT+" pad="12"/>
<connect gate="G$1" pin="EAR_MT-" pad="10"/>
<connect gate="G$1" pin="EMMI_RX/RX_GPS" pad="41"/>
<connect gate="G$1" pin="EMMI_TX/TX_GPS" pad="35"/>
<connect gate="G$1" pin="GND/ADC" pad="6"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="G1"/>
<connect gate="G$1" pin="GND@3" pad="G2"/>
<connect gate="G$1" pin="GND@4" pad="G3"/>
<connect gate="G$1" pin="GND@5" pad="G8"/>
<connect gate="G$1" pin="GND@6" pad="G4"/>
<connect gate="G$1" pin="GND@7" pad="G5"/>
<connect gate="G$1" pin="GND@8" pad="G6"/>
<connect gate="G$1" pin="GND@9" pad="G7"/>
<connect gate="G$1" pin="GPI1" pad="31"/>
<connect gate="G$1" pin="GPIO10/PD[2]" pad="38"/>
<connect gate="G$1" pin="GPIO11/PD[3]" pad="40"/>
<connect gate="G$1" pin="GPIO12/PD[4]" pad="42"/>
<connect gate="G$1" pin="GPIO13/PD[5]" pad="44"/>
<connect gate="G$1" pin="GPIO3/PD[6]/CAM_SCL" pad="46"/>
<connect gate="G$1" pin="GPIO4/IICSDA/CAM_SDA" pad="47"/>
<connect gate="G$1" pin="GPIO5/CAM_RDY/RFTXMON" pad="48"/>
<connect gate="G$1" pin="GPIO6/ALARM/PD[7]" pad="49"/>
<connect gate="G$1" pin="GPIO7/BUZZER/CAM_PWR_ON" pad="50"/>
<connect gate="G$1" pin="GPIO8/PD[0]/CAM_ON" pad="32"/>
<connect gate="G$1" pin="GPIO9/PD[1]/CAM_RST" pad="34"/>
<connect gate="G$1" pin="GPO2/JDR" pad="28"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="13"/>
<connect gate="G$1" pin="MIC_MT+" pad="14"/>
<connect gate="G$1" pin="MIC_MT-" pad="16"/>
<connect gate="G$1" pin="ON/OFF" pad="17"/>
<connect gate="G$1" pin="PWRMON" pad="21"/>
<connect gate="G$1" pin="RES@25" pad="25"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="SIMCLK" pad="26"/>
<connect gate="G$1" pin="SIMIO" pad="19"/>
<connect gate="G$1" pin="SIMRST" pad="24"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="39"/>
<connect gate="G$1" pin="VBATT@0" pad="1"/>
<connect gate="G$1" pin="VBATT@1" pad="3"/>
<connect gate="G$1" pin="VBATT@2" pad="5"/>
<connect gate="G$1" pin="VBATT@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM862_CONNECTOR" package="GM862_CONNECTOR">
<connects>
<connect gate="G$1" pin="AXE" pad="18"/>
<connect gate="G$1" pin="C103/TXD" pad="20"/>
<connect gate="G$1" pin="C104/RXD" pad="37"/>
<connect gate="G$1" pin="C105/RTS" pad="45"/>
<connect gate="G$1" pin="C106/CTS" pad="29"/>
<connect gate="G$1" pin="C107/DSR" pad="33"/>
<connect gate="G$1" pin="C108/DTR" pad="43"/>
<connect gate="G$1" pin="C109/DCD" pad="36"/>
<connect gate="G$1" pin="C125/RING" pad="30"/>
<connect gate="G$1" pin="CCIN/SIMIN" pad="27"/>
<connect gate="G$1" pin="CHARGE" pad="8"/>
<connect gate="G$1" pin="EAR_HF+" pad="9"/>
<connect gate="G$1" pin="EAR_HF-" pad="11"/>
<connect gate="G$1" pin="EAR_MT+" pad="12"/>
<connect gate="G$1" pin="EAR_MT-" pad="10"/>
<connect gate="G$1" pin="EMMI_RX/RX_GPS" pad="41"/>
<connect gate="G$1" pin="EMMI_TX/TX_GPS" pad="35"/>
<connect gate="G$1" pin="GND/ADC" pad="6"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="G1"/>
<connect gate="G$1" pin="GND@3" pad="G2"/>
<connect gate="G$1" pin="GND@4" pad="G3"/>
<connect gate="G$1" pin="GND@5" pad="G8"/>
<connect gate="G$1" pin="GND@6" pad="G4"/>
<connect gate="G$1" pin="GND@7" pad="G5"/>
<connect gate="G$1" pin="GND@8" pad="G6"/>
<connect gate="G$1" pin="GND@9" pad="G7"/>
<connect gate="G$1" pin="GPI1" pad="31"/>
<connect gate="G$1" pin="GPIO10/PD[2]" pad="38"/>
<connect gate="G$1" pin="GPIO11/PD[3]" pad="40"/>
<connect gate="G$1" pin="GPIO12/PD[4]" pad="42"/>
<connect gate="G$1" pin="GPIO13/PD[5]" pad="44"/>
<connect gate="G$1" pin="GPIO3/PD[6]/CAM_SCL" pad="46"/>
<connect gate="G$1" pin="GPIO4/IICSDA/CAM_SDA" pad="47"/>
<connect gate="G$1" pin="GPIO5/CAM_RDY/RFTXMON" pad="48"/>
<connect gate="G$1" pin="GPIO6/ALARM/PD[7]" pad="49"/>
<connect gate="G$1" pin="GPIO7/BUZZER/CAM_PWR_ON" pad="50"/>
<connect gate="G$1" pin="GPIO8/PD[0]/CAM_ON" pad="32"/>
<connect gate="G$1" pin="GPIO9/PD[1]/CAM_RST" pad="34"/>
<connect gate="G$1" pin="GPO2/JDR" pad="28"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="13"/>
<connect gate="G$1" pin="MIC_MT+" pad="14"/>
<connect gate="G$1" pin="MIC_MT-" pad="16"/>
<connect gate="G$1" pin="ON/OFF" pad="17"/>
<connect gate="G$1" pin="PWRMON" pad="21"/>
<connect gate="G$1" pin="RES@25" pad="25"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="SIMCLK" pad="26"/>
<connect gate="G$1" pin="SIMIO" pad="19"/>
<connect gate="G$1" pin="SIMRST" pad="24"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="39"/>
<connect gate="G$1" pin="VBATT@0" pad="1"/>
<connect gate="G$1" pin="VBATT@1" pad="3"/>
<connect gate="G$1" pin="VBATT@2" pad="5"/>
<connect gate="G$1" pin="VBATT@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GP-2106" prefix="U">
<description>GP-2106 GPS SiRF IV</description>
<gates>
<gate name="G$1" symbol="GP-2106"/>
</gates>
<devices>
<device name="" package="GP-2106">
<connects>
<connect gate="G$1" pin="1PPS" pad="1PPS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ONOFF" pad="ONOFF"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GR-10">
<description>&lt;b&gt;GR-10 GPS Receiver Module&lt;/b&gt;
Proto layout and schematic for GR-10 GPS receiver. Spark Fun Electronics SKU : GPS-08291</description>
<gates>
<gate name="G$1" symbol="GR-10"/>
</gates>
<devices>
<device name="SMD" package="GR-10">
<connects>
<connect gate="G$1" pin="1.8V@10" pad="10"/>
<connect gate="G$1" pin="1.8V@21" pad="21"/>
<connect gate="G$1" pin="1.8V@3" pad="3"/>
<connect gate="G$1" pin="1.8VIF" pad="26"/>
<connect gate="G$1" pin="1.8VLNA" pad="28"/>
<connect gate="G$1" pin="1.8VRF" pad="34"/>
<connect gate="G$1" pin="1.8VVCO" pad="25"/>
<connect gate="G$1" pin="1PPS" pad="9"/>
<connect gate="G$1" pin="3V" pad="33"/>
<connect gate="G$1" pin="ANT" pad="30"/>
<connect gate="G$1" pin="APIO_A4" pad="16"/>
<connect gate="G$1" pin="FREF" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@31" pad="31"/>
<connect gate="G$1" pin="GPIO_A11" pad="12"/>
<connect gate="G$1" pin="GPIO_A5" pad="13"/>
<connect gate="G$1" pin="GPIO_A6" pad="14"/>
<connect gate="G$1" pin="GPIO_A9" pad="15"/>
<connect gate="G$1" pin="GPIO_B16" pad="22"/>
<connect gate="G$1" pin="GPIO_B19" pad="19"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="RFEN" pad="32"/>
<connect gate="G$1" pin="RTC_XIN" pad="17"/>
<connect gate="G$1" pin="RTC_XOUT" pad="18"/>
<connect gate="G$1" pin="RX0" pad="7"/>
<connect gate="G$1" pin="RX1" pad="5"/>
<connect gate="G$1" pin="SB" pad="4"/>
<connect gate="G$1" pin="TPI" pad="35"/>
<connect gate="G$1" pin="TPQ" pad="36"/>
<connect gate="G$1" pin="TX0" pad="8"/>
<connect gate="G$1" pin="TX1" pad="6"/>
<connect gate="G$1" pin="VALID_FIX" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GS406SMD" prefix="U">
<description>50 Channel GS406 Helical GPS Receiver - SMD Connector.  The Mating SMD SPECIAL is called SPECIAL for a reason. This package was only made in order to make a dummy gs407 PCB with mating connector (used for testing).

sku: GPS-09079</description>
<gates>
<gate name="CONNECTOR" symbol="GS406SMD"/>
</gates>
<devices>
<device name="SOCKET" package="GS406SMD">
<connects>
<connect gate="CONNECTOR" pin="P1" pad="1"/>
<connect gate="CONNECTOR" pin="P10" pad="10"/>
<connect gate="CONNECTOR" pin="P2" pad="2"/>
<connect gate="CONNECTOR" pin="P3" pad="3"/>
<connect gate="CONNECTOR" pin="P4" pad="4"/>
<connect gate="CONNECTOR" pin="P5" pad="5"/>
<connect gate="CONNECTOR" pin="P6" pad="6"/>
<connect gate="CONNECTOR" pin="P7" pad="7"/>
<connect gate="CONNECTOR" pin="P8" pad="8"/>
<connect gate="CONNECTOR" pin="P9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MATING_SMD_***SPECIAL" package="GS406-MATING_SMD_***SPECIAL">
<connects>
<connect gate="CONNECTOR" pin="P1" pad="1"/>
<connect gate="CONNECTOR" pin="P10" pad="10"/>
<connect gate="CONNECTOR" pin="P2" pad="2"/>
<connect gate="CONNECTOR" pin="P3" pad="3"/>
<connect gate="CONNECTOR" pin="P4" pad="4"/>
<connect gate="CONNECTOR" pin="P5" pad="5"/>
<connect gate="CONNECTOR" pin="P6" pad="6"/>
<connect gate="CONNECTOR" pin="P7" pad="7"/>
<connect gate="CONNECTOR" pin="P8" pad="8"/>
<connect gate="CONNECTOR" pin="P9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GS1011" prefix="U">
<description>GainSpan GS1011M Low-Power Wireless SOC Wi-Fi Module</description>
<gates>
<gate name="G$1" symbol="GS1011"/>
</gates>
<devices>
<device name="GS1011MXX" package="GS1011MXX">
<connects>
<connect gate="G$1" pin="ADC1" pad="11"/>
<connect gate="G$1" pin="ADC2" pad="12"/>
<connect gate="G$1" pin="ALARM1" pad="7"/>
<connect gate="G$1" pin="ALARM2" pad="13"/>
<connect gate="G$1" pin="DC_CNTL" pad="10"/>
<connect gate="G$1" pin="EN_1.8V" pad="33"/>
<connect gate="G$1" pin="EXT_RESET" pad="47"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@32" pad="32"/>
<connect gate="G$1" pin="GND@48" pad="48"/>
<connect gate="G$1" pin="GPIO19_44MHZ" pad="23"/>
<connect gate="G$1" pin="GPIO20_22MHZ" pad="22"/>
<connect gate="G$1" pin="GPIO21_11MHZ" pad="21"/>
<connect gate="G$1" pin="GPIO28" pad="46"/>
<connect gate="G$1" pin="GPIO29" pad="45"/>
<connect gate="G$1" pin="GPIO30_LED1" pad="44"/>
<connect gate="G$1" pin="GPIO31_LED2" pad="43"/>
<connect gate="G$1" pin="I2C_CLK" pad="25"/>
<connect gate="G$1" pin="I2C_DATA" pad="26"/>
<connect gate="G$1" pin="JTAG_RST" pad="6"/>
<connect gate="G$1" pin="JTAG_TCK" pad="2"/>
<connect gate="G$1" pin="JTAG_TDI" pad="4"/>
<connect gate="G$1" pin="JTAG_TDO" pad="3"/>
<connect gate="G$1" pin="JTAG_TMS" pad="5"/>
<connect gate="G$1" pin="MSPI_CLK" pad="18"/>
<connect gate="G$1" pin="MSPI_CS0" pad="19"/>
<connect gate="G$1" pin="MSPI_CS1" pad="20"/>
<connect gate="G$1" pin="MSPI_DIN" pad="14"/>
<connect gate="G$1" pin="MSPI_DOUT" pad="15"/>
<connect gate="G$1" pin="PWM0/GPIO10" pad="24"/>
<connect gate="G$1" pin="RTC_OUT1" pad="8"/>
<connect gate="G$1" pin="SSPI_CLK" pad="28"/>
<connect gate="G$1" pin="SSPI_CS" pad="29"/>
<connect gate="G$1" pin="SSPI_DIN" pad="30"/>
<connect gate="G$1" pin="SSPI_DOUT" pad="27"/>
<connect gate="G$1" pin="UART0_CTS/GPIO24" pad="42"/>
<connect gate="G$1" pin="UART0_RTS/GPIO25" pad="40"/>
<connect gate="G$1" pin="UART0_RX/GPIO0" pad="41"/>
<connect gate="G$1" pin="UART0_TX/GPIO1" pad="39"/>
<connect gate="G$1" pin="UART1_CTS/GPIO26" pad="35"/>
<connect gate="G$1" pin="UART1_RTS/GPIO27" pad="36"/>
<connect gate="G$1" pin="UART1_RX/GPIO3" pad="37"/>
<connect gate="G$1" pin="UART1_TX/GPIO2" pad="38"/>
<connect gate="G$1" pin="VBAT" pad="9"/>
<connect gate="G$1" pin="VDDIO" pad="34"/>
<connect gate="G$1" pin="VIN_3V3" pad="31"/>
<connect gate="G$1" pin="VOUT_1.8V" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ID-12/20">
<description>RFID reader for ID2, ID12, and ID20 Package</description>
<gates>
<gate name="G$1" symbol="ID-12"/>
</gates>
<devices>
<device name="" package="ID-12">
<connects>
<connect gate="G$1" pin="+/-" pad="7"/>
<connect gate="G$1" pin="5V" pad="11"/>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="FUTURE" pad="6"/>
<connect gate="G$1" pin="GNDT" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ID-12_LOCK" package="ID-12_LOCK">
<connects>
<connect gate="G$1" pin="+/-" pad="7"/>
<connect gate="G$1" pin="5V" pad="11"/>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="FUTURE" pad="6"/>
<connect gate="G$1" pin="GNDT" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="ID-12_SMD">
<connects>
<connect gate="G$1" pin="+/-" pad="7"/>
<connect gate="G$1" pin="5V" pad="11"/>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="FUTURE" pad="6"/>
<connect gate="G$1" pin="GNDT" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LASSEN_IQ_GPS">
<description>Lassen iq 
12-Channel GPS receiver. Schematic and footprint production proven. Spark Fun Electronics SKU : GPS-00163. Surface mount mating connector : GPS-00170</description>
<gates>
<gate name="G$1" symbol="LASSEN_IQ_GPS"/>
</gates>
<devices>
<device name="LASSEN" package="LASSEN_IQ_GPS">
<connects>
<connect gate="G$1" pin="BATT" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PPS" pad="4"/>
<connect gate="G$1" pin="RXA" pad="3"/>
<connect gate="G$1" pin="RXB" pad="6"/>
<connect gate="G$1" pin="TXA" pad="1"/>
<connect gate="G$1" pin="TXB" pad="5"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LS20126" prefix="U">
<description>&lt;h3&gt; LS20126 20-Channel GPS Module&lt;/h3&gt;&lt;br&gt;
SparkFun SKU# &lt;b&gt;GPS-09838&lt;/b&gt;&lt;br&gt;
The LOCOSYS LS20126 GPS smart antenna module is a high sensitivity, low power, SMD type, 20 channels with built-in magnetic sensor, 3-axial acceleration sensor L1 GPS receiver and 10mm patch antenna designed for portable applications.</description>
<gates>
<gate name="G$1" symbol="LS20126"/>
</gates>
<devices>
<device name="" package="LS20126">
<connects>
<connect gate="G$1" pin="BOOTSL" pad="6"/>
<connect gate="G$1" pin="EN" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="10"/>
<connect gate="G$1" pin="GPIO" pad="5"/>
<connect gate="G$1" pin="RX" pad="4"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSTBY" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIRF" prefix="MIRF" uservalue="yes">
<description>nRF2401A 2.4GHz transceiver module, WRL-00153</description>
<gates>
<gate name="A" symbol="MIRF"/>
</gates>
<devices>
<device name="" package="MIRF">
<connects>
<connect gate="A" pin="1" pad="7"/>
<connect gate="A" pin="2" pad="6"/>
<connect gate="A" pin="3" pad="5"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="3"/>
<connect gate="A" pin="6" pad="2"/>
<connect gate="A" pin="7" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MLX90121" prefix="U">
<description>MLX90121 13.56MHz RFID Transceiver</description>
<gates>
<gate name="G$1" symbol="MLX90121"/>
</gates>
<devices>
<device name="_" package="SSOP20">
<connects>
<connect gate="G$1" pin="CK" pad="15"/>
<connect gate="G$1" pin="DIN" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DSYC" pad="16"/>
<connect gate="G$1" pin="MOD" pad="3"/>
<connect gate="G$1" pin="MODE" pad="14"/>
<connect gate="G$1" pin="RES1" pad="9"/>
<connect gate="G$1" pin="RES2(DNC)" pad="18"/>
<connect gate="G$1" pin="RTB" pad="10"/>
<connect gate="G$1" pin="RX" pad="20"/>
<connect gate="G$1" pin="TX" pad="2"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="12"/>
<connect gate="G$1" pin="VDD3" pad="17"/>
<connect gate="G$1" pin="VSS1" pad="4"/>
<connect gate="G$1" pin="VSS2" pad="7"/>
<connect gate="G$1" pin="VSS3" pad="19"/>
<connect gate="G$1" pin="XBUF" pad="8"/>
<connect gate="G$1" pin="XIN" pad="6"/>
<connect gate="G$1" pin="XOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MN5010HS">
<description>MN5010HS GPS Receiver Module. Packagse GR-10 and MN5010HS are NOT tested with this device.</description>
<gates>
<gate name="G$1" symbol="MN5010HS"/>
</gates>
<devices>
<device name="SMD" package="MN5010HS">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="GR-10">
<connects>
<connect gate="G$1" pin="1PPS" pad="9"/>
<connect gate="G$1" pin="ANT" pad="30"/>
<connect gate="G$1" pin="BATT" pad="33"/>
<connect gate="G$1" pin="GND11" pad="11"/>
<connect gate="G$1" pin="GND2" pad="2"/>
<connect gate="G$1" pin="GND24" pad="24"/>
<connect gate="G$1" pin="GND27" pad="27"/>
<connect gate="G$1" pin="GND29" pad="29"/>
<connect gate="G$1" pin="GND31" pad="31"/>
<connect gate="G$1" pin="GND4" pad="4"/>
<connect gate="G$1" pin="NAV" pad="20"/>
<connect gate="G$1" pin="NMR" pad="23"/>
<connect gate="G$1" pin="ONOFF" pad="22"/>
<connect gate="G$1" pin="OPT1" pad="13"/>
<connect gate="G$1" pin="OPT2" pad="14"/>
<connect gate="G$1" pin="RX-I" pad="7"/>
<connect gate="G$1" pin="TX-O" pad="8"/>
<connect gate="G$1" pin="VIO" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24AP1" prefix="U">
<description>&lt;b&gt;2.4GHz ANT IC&lt;/b&gt;
Nordic Semiconductor 2.4GHz transceiver that implements the ANT protocol.</description>
<gates>
<gate name="G$1" symbol="NRF24AP1"/>
</gates>
<devices>
<device name="SMD" package="MLP-24">
<connects>
<connect gate="G$1" pin="ANT1" pad="14"/>
<connect gate="G$1" pin="ANT2" pad="15"/>
<connect gate="G$1" pin="BR1" pad="2"/>
<connect gate="G$1" pin="BR2" pad="1"/>
<connect gate="G$1" pin="DVDD" pad="9"/>
<connect gate="G$1" pin="EXT32K" pad="3"/>
<connect gate="G$1" pin="IREF" pad="19"/>
<connect gate="G$1" pin="PORTSEL" pad="23"/>
<connect gate="G$1" pin="RTS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SLEEP" pad="6"/>
<connect gate="G$1" pin="SUSPEND" pad="7"/>
<connect gate="G$1" pin="TXD" pad="5"/>
<connect gate="G$1" pin="VDD@17" pad="17"/>
<connect gate="G$1" pin="VDD@21" pad="21"/>
<connect gate="G$1" pin="VDD@24" pad="24"/>
<connect gate="G$1" pin="VDD_PA" pad="13"/>
<connect gate="G$1" pin="VSS@0" pad="0"/>
<connect gate="G$1" pin="VSS@10" pad="10"/>
<connect gate="G$1" pin="VSS@18" pad="18"/>
<connect gate="G$1" pin="VSS@20" pad="20"/>
<connect gate="G$1" pin="VSS@22" pad="22"/>
<connect gate="G$1" pin="VSS_PA" pad="16"/>
<connect gate="G$1" pin="XC1" pad="12"/>
<connect gate="G$1" pin="XC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24L01">
<description>&lt;b&gt;2.4GHz Low Power Transceiver&lt;/b&gt;
This is the very popular, low cost, very low power RF transceiver from Nordic Semiconductor. Simple SPI interface. SKU: COM-00690</description>
<gates>
<gate name="G$1" symbol="NRF24L01-1"/>
</gates>
<devices>
<device name="SMD" package="QFN20">
<connects>
<connect gate="G$1" pin="ANT1" pad="12"/>
<connect gate="G$1" pin="ANT2" pad="13"/>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="CSN" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="19"/>
<connect gate="G$1" pin="IREF" pad="16"/>
<connect gate="G$1" pin="IRQ" pad="6"/>
<connect gate="G$1" pin="MISO" pad="5"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VDD@15" pad="15"/>
<connect gate="G$1" pin="VDD@18" pad="18"/>
<connect gate="G$1" pin="VDD@7" pad="7"/>
<connect gate="G$1" pin="VDD_PA" pad="11"/>
<connect gate="G$1" pin="VSS@0" pad="0"/>
<connect gate="G$1" pin="VSS@14" pad="14"/>
<connect gate="G$1" pin="VSS@17" pad="17"/>
<connect gate="G$1" pin="VSS@20" pad="20"/>
<connect gate="G$1" pin="VSS@8" pad="8"/>
<connect gate="G$1" pin="XC1" pad="10"/>
<connect gate="G$1" pin="XC2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24LE1">
<description>2.4GHz transceiver</description>
<gates>
<gate name="G$1" symbol="NRF24LE1"/>
</gates>
<devices>
<device name="" package="QFN-32">
<connects>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="DEC1" pad="3"/>
<connect gate="G$1" pin="DEC2" pad="4"/>
<connect gate="G$1" pin="IREF" pad="25"/>
<connect gate="G$1" pin="P0.0" pad="32"/>
<connect gate="G$1" pin="P0.1" pad="1"/>
<connect gate="G$1" pin="P0.2" pad="5"/>
<connect gate="G$1" pin="P0.3" pad="7"/>
<connect gate="G$1" pin="P0.4" pad="10"/>
<connect gate="G$1" pin="P0.5" pad="11"/>
<connect gate="G$1" pin="P0.6" pad="12"/>
<connect gate="G$1" pin="P0.7" pad="13"/>
<connect gate="G$1" pin="P1.0" pad="14"/>
<connect gate="G$1" pin="P1.1" pad="15"/>
<connect gate="G$1" pin="P1.2" pad="16"/>
<connect gate="G$1" pin="P1.3" pad="17"/>
<connect gate="G$1" pin="P1.4" pad="18"/>
<connect gate="G$1" pin="P1.5" pad="28"/>
<connect gate="G$1" pin="P1.6" pad="29"/>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="9"/>
<connect gate="G$1" pin="VDD3" pad="24"/>
<connect gate="G$1" pin="VDD4" pad="27"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="23"/>
<connect gate="G$1" pin="VSS3" pad="26"/>
<connect gate="G$1" pin="XC1" pad="31"/>
<connect gate="G$1" pin="XC2" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24LU1">
<description>2.4GHz transceiver</description>
<gates>
<gate name="G$1" symbol="NRF24LU1"/>
</gates>
<devices>
<device name="" package="QFN-32">
<connects>
<connect gate="G$1" pin="/RESET" pad="8"/>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="DEC1" pad="28"/>
<connect gate="G$1" pin="DEC2" pad="29"/>
<connect gate="G$1" pin="IREF" pad="25"/>
<connect gate="G$1" pin="P0.0" pad="10"/>
<connect gate="G$1" pin="P0.1" pad="11"/>
<connect gate="G$1" pin="P0.2" pad="13"/>
<connect gate="G$1" pin="P0.3" pad="14"/>
<connect gate="G$1" pin="P0.4" pad="15"/>
<connect gate="G$1" pin="P0.5" pad="16"/>
<connect gate="G$1" pin="PROG" pad="7"/>
<connect gate="G$1" pin="VBUS" pad="2"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="3"/>
<connect gate="G$1" pin="VDD3" pad="9"/>
<connect gate="G$1" pin="VDD4" pad="19"/>
<connect gate="G$1" pin="VDD5" pad="24"/>
<connect gate="G$1" pin="VDD6" pad="27"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="6"/>
<connect gate="G$1" pin="VSS2" pad="12"/>
<connect gate="G$1" pin="VSS3" pad="17"/>
<connect gate="G$1" pin="VSS4" pad="18"/>
<connect gate="G$1" pin="VSS5" pad="23"/>
<connect gate="G$1" pin="VSS6" pad="26"/>
<connect gate="G$1" pin="VSS7" pad="30"/>
<connect gate="G$1" pin="XC1" pad="32"/>
<connect gate="G$1" pin="XC2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24Z1">
<description>2.4GHz transceiver</description>
<gates>
<gate name="G$1" symbol="NRF24Z1"/>
</gates>
<devices>
<device name="" package="QFN-36">
<connects>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="DATA" pad="12"/>
<connect gate="G$1" pin="DD0" pad="8"/>
<connect gate="G$1" pin="DD1" pad="7"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="IREF" pad="24"/>
<connect gate="G$1" pin="IRQ" pad="36"/>
<connect gate="G$1" pin="MCLK" pad="14"/>
<connect gate="G$1" pin="MCSN" pad="29"/>
<connect gate="G$1" pin="MMISO" pad="30"/>
<connect gate="G$1" pin="MMOSI" pad="31"/>
<connect gate="G$1" pin="MODE" pad="26"/>
<connect gate="G$1" pin="MSCK" pad="35"/>
<connect gate="G$1" pin="MSCL" pad="28"/>
<connect gate="G$1" pin="MSDA" pad="27"/>
<connect gate="G$1" pin="REQ" pad="9"/>
<connect gate="G$1" pin="SCSN" pad="4"/>
<connect gate="G$1" pin="SMISO" pad="2"/>
<connect gate="G$1" pin="SMOSI" pad="6"/>
<connect gate="G$1" pin="SPDIO" pad="13"/>
<connect gate="G$1" pin="SSCK" pad="3"/>
<connect gate="G$1" pin="SSEL" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VDD1" pad="19"/>
<connect gate="G$1" pin="VDD2" pad="33"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="VSS1" pad="25"/>
<connect gate="G$1" pin="VSS2" pad="32"/>
<connect gate="G$1" pin="VSS3" pad="34"/>
<connect gate="G$1" pin="VSS_PA" pad="23"/>
<connect gate="G$1" pin="WS" pad="11"/>
<connect gate="G$1" pin="XC1" pad="18"/>
<connect gate="G$1" pin="XC2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF2401A">
<description>&lt;b&gt;2.4GHz Transceiver&lt;/b&gt;
This is the very popular, low power RF transceiver from Nordic Semiconductor. Used in the Nike+iPod product. SKU: COM-00300</description>
<gates>
<gate name="G$1" symbol="NRF2401A"/>
</gates>
<devices>
<device name="SMD" package="MLP-24">
<connects>
<connect gate="G$1" pin="ANT1" pad="14"/>
<connect gate="G$1" pin="ANT2" pad="15"/>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="CLK1" pad="7"/>
<connect gate="G$1" pin="CLK2" pad="3"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="DOUT2" pad="4"/>
<connect gate="G$1" pin="DR1" pad="6"/>
<connect gate="G$1" pin="DR2" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="9"/>
<connect gate="G$1" pin="IREF" pad="19"/>
<connect gate="G$1" pin="PWR_UP" pad="23"/>
<connect gate="G$1" pin="VDD@17" pad="17"/>
<connect gate="G$1" pin="VDD@21" pad="21"/>
<connect gate="G$1" pin="VDD@24" pad="24"/>
<connect gate="G$1" pin="VDD_PA" pad="13"/>
<connect gate="G$1" pin="VSS@0" pad="0"/>
<connect gate="G$1" pin="VSS@10" pad="10"/>
<connect gate="G$1" pin="VSS@18" pad="18"/>
<connect gate="G$1" pin="VSS@20" pad="20"/>
<connect gate="G$1" pin="VSS@22" pad="22"/>
<connect gate="G$1" pin="VSS_PA" pad="16"/>
<connect gate="G$1" pin="XC1" pad="12"/>
<connect gate="G$1" pin="XC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NS73M" prefix="U">
<description>&lt;b&gt;FM Transmitter&lt;/b&gt;
2mW transmitter NS73M. Easy SPI interface. Digital tuning. SKU: WRL-08452</description>
<gates>
<gate name="G$1" symbol="NS73M"/>
</gates>
<devices>
<device name="SMD" package="NS73M">
<connects>
<connect gate="G$1" pin="CK" pad="5"/>
<connect gate="G$1" pin="DA" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="IIC" pad="8"/>
<connect gate="G$1" pin="LA" pad="7"/>
<connect gate="G$1" pin="LIN" pad="12"/>
<connect gate="G$1" pin="PWE" pad="4"/>
<connect gate="G$1" pin="RFO" pad="15"/>
<connect gate="G$1" pin="RIN" pad="13"/>
<connect gate="G$1" pin="TEB" pad="3"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VDRF" pad="2"/>
<connect gate="G$1" pin="X1" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF-LINK_RX">
<description>RF Link receivers- WRL-8947, 8948, 8949, 8950</description>
<gates>
<gate name="G$1" symbol="RF-LINK_RX"/>
</gates>
<devices>
<device name="" package="RF-LINK_RX">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V@1"/>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA" pad="DATA@1"/>
<connect gate="G$1" pin="GND" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF-LINK_TX">
<description>RF Link transmitters WRL-8945, 8946</description>
<gates>
<gate name="G$1" symbol="RF-LINK_TX"/>
</gates>
<devices>
<device name="" package="RF-LINK_TX">
<connects>
<connect gate="G$1" pin="+5V" pad="VCC"/>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF24G">
<description>&lt;b&gt;RF24G Header&lt;/b&gt; This is the header for connections to the RF24G Transceiver (SparkFun Electronics SKU: WRL-00151), used in the Breakout Board for RF24G Transceiver (SparkFun Electronics SKU: BOB-00196). This footprint has not yet been proven in production.</description>
<gates>
<gate name="G$1" symbol="RF24G"/>
</gates>
<devices>
<device name="" package="RF24G-2X5">
<connects>
<connect gate="G$1" pin="CE" pad="2"/>
<connect gate="G$1" pin="CLK1" pad="5"/>
<connect gate="G$1" pin="CLK2" pad="3"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="DATA" pad="6"/>
<connect gate="G$1" pin="DOUT2" pad="8"/>
<connect gate="G$1" pin="DR1" pad="7"/>
<connect gate="G$1" pin="DR2" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM22">
<description>The RFM22 is a low-power, low cost radio that is capable of operating in the 434MHz and 900MHz open bands. It's frequency is software defined and there are some very good libraries written for it.</description>
<gates>
<gate name="G$1" symbol="RFM22"/>
</gates>
<devices>
<device name="SMD" package="RFM22-XXX-S2">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="16"/>
<connect gate="G$1" pin="GPIO0" pad="6"/>
<connect gate="G$1" pin="GPIO1" pad="7"/>
<connect gate="G$1" pin="GPIO2" pad="8"/>
<connect gate="G$1" pin="NIRQ" pad="14"/>
<connect gate="G$1" pin="NSEL" pad="13"/>
<connect gate="G$1" pin="RXANT" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="12"/>
<connect gate="G$1" pin="SDI" pad="11"/>
<connect gate="G$1" pin="SDN" pad="15"/>
<connect gate="G$1" pin="SDO" pad="10"/>
<connect gate="G$1" pin="TXANT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RMCM01">
<description>Polar Heart Rate Monitor module</description>
<gates>
<gate name="G$1" symbol="RMCM01"/>
</gates>
<devices>
<device name="SMD" package="RMCM01">
<connects>
<connect gate="G$1" pin="F32KIN" pad="3"/>
<connect gate="G$1" pin="FPLS" pad="6"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="HR" pad="5"/>
<connect gate="G$1" pin="LX1" pad="10"/>
<connect gate="G$1" pin="LX2" pad="9"/>
<connect gate="G$1" pin="OSC" pad="4"/>
<connect gate="G$1" pin="OSC_ON" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="WIDB_DET" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN-131G">
<description>Roving Netowrks WiFLy GSX Module</description>
<gates>
<gate name="G$1" symbol="RN-131G"/>
</gates>
<devices>
<device name="" package="RN-131G">
<connects>
<connect gate="G$1" pin="3.3V-RIN" pad="P$18"/>
<connect gate="G$1" pin="3.3V-ROUT" pad="P$17"/>
<connect gate="G$1" pin="CLK" pad="P$15"/>
<connect gate="G$1" pin="DMA-RX" pad="P$23"/>
<connect gate="G$1" pin="DMA-TX" pad="P$22"/>
<connect gate="G$1" pin="EPC-A" pad="P$6"/>
<connect gate="G$1" pin="EPC-B" pad="P$7"/>
<connect gate="G$1" pin="F_AWAKE" pad="P$9"/>
<connect gate="G$1" pin="GND@19" pad="P$19"/>
<connect gate="G$1" pin="GND@36" pad="P$36"/>
<connect gate="G$1" pin="GND@37" pad="P$37"/>
<connect gate="G$1" pin="GND@38" pad="P$38"/>
<connect gate="G$1" pin="GND@39" pad="P$39"/>
<connect gate="G$1" pin="GND@40" pad="P$40"/>
<connect gate="G$1" pin="GND@41" pad="P$41"/>
<connect gate="G$1" pin="GND@42" pad="P$42"/>
<connect gate="G$1" pin="GND@43" pad="P$43"/>
<connect gate="G$1" pin="GND@44" pad="P$44"/>
<connect gate="G$1" pin="GPIO-12" pad="P$11"/>
<connect gate="G$1" pin="GPIO-13" pad="P$10"/>
<connect gate="G$1" pin="GPIO-4" pad="P$29"/>
<connect gate="G$1" pin="GPIO-5" pad="P$28"/>
<connect gate="G$1" pin="GPIO-6" pad="P$27"/>
<connect gate="G$1" pin="GPIO-7" pad="P$26"/>
<connect gate="G$1" pin="GPIO-8" pad="P$25"/>
<connect gate="G$1" pin="GPIO-9" pad="P$24"/>
<connect gate="G$1" pin="MISO" pad="P$16"/>
<connect gate="G$1" pin="MOSI" pad="P$14"/>
<connect gate="G$1" pin="RESET" pad="P$5"/>
<connect gate="G$1" pin="RX" pad="P$12"/>
<connect gate="G$1" pin="SEN0" pad="P$34"/>
<connect gate="G$1" pin="SEN1" pad="P$30"/>
<connect gate="G$1" pin="SEN2" pad="P$31"/>
<connect gate="G$1" pin="SEN3" pad="P$32"/>
<connect gate="G$1" pin="SEN4" pad="P$2"/>
<connect gate="G$1" pin="SEN5" pad="P$3"/>
<connect gate="G$1" pin="SEN6" pad="P$1"/>
<connect gate="G$1" pin="SEN7" pad="P$4"/>
<connect gate="G$1" pin="SENSE-PWR" pad="P$33"/>
<connect gate="G$1" pin="S_CAP" pad="P$8"/>
<connect gate="G$1" pin="TX" pad="P$13"/>
<connect gate="G$1" pin="VDD-BATT" pad="P$20"/>
<connect gate="G$1" pin="VDD-IN" pad="P$21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN171" prefix="U">
<description>WiFi Module</description>
<gates>
<gate name="G$1" symbol="RN171"/>
</gates>
<devices>
<device name="RN171" package="RN171">
<connects>
<connect gate="G$1" pin="ANT" pad="24"/>
<connect gate="G$1" pin="AWAKE" pad="41"/>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="CTS" pad="44"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@39" pad="39"/>
<connect gate="G$1" pin="GND@47" pad="47"/>
<connect gate="G$1" pin="GPIO1" pad="13"/>
<connect gate="G$1" pin="GPIO14" pad="42"/>
<connect gate="G$1" pin="GPIO2" pad="12"/>
<connect gate="G$1" pin="GPIO3" pad="11"/>
<connect gate="G$1" pin="GPIO7" pad="6"/>
<connect gate="G$1" pin="INT/GPIO6" pad="7"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="9"/>
<connect gate="G$1" pin="RESET" pad="40"/>
<connect gate="G$1" pin="RTS" pad="43"/>
<connect gate="G$1" pin="RX" pad="45"/>
<connect gate="G$1" pin="SEN0" pad="29"/>
<connect gate="G$1" pin="SEN1" pad="30"/>
<connect gate="G$1" pin="SEN2" pad="31"/>
<connect gate="G$1" pin="SEN3" pad="32"/>
<connect gate="G$1" pin="SEN4" pad="35"/>
<connect gate="G$1" pin="SEN5" pad="36"/>
<connect gate="G$1" pin="SEN6" pad="37"/>
<connect gate="G$1" pin="SEN7" pad="38"/>
<connect gate="G$1" pin="SPOWER" pad="33"/>
<connect gate="G$1" pin="SREG" pad="48"/>
<connect gate="G$1" pin="TX" pad="46"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDD_BATT" pad="49"/>
<connect gate="G$1" pin="VDD_RF" pad="34"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS9110" prefix="U">
<description>Redpine WiFi module</description>
<gates>
<gate name="G$1" symbol="RS9110-N-11-22"/>
</gates>
<devices>
<device name="" package="RS9110-N-11-22-SHORT">
<connects>
<connect gate="G$1" pin="CLK" pad="51"/>
<connect gate="G$1" pin="CS" pad="52"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@48" pad="48"/>
<connect gate="G$1" pin="GND@PAD" pad="GND"/>
<connect gate="G$1" pin="INTR" pad="3"/>
<connect gate="G$1" pin="JPD0" pad="42"/>
<connect gate="G$1" pin="JPD1" pad="43"/>
<connect gate="G$1" pin="JPD2" pad="44"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MODE" pad="22"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RX" pad="7"/>
<connect gate="G$1" pin="SD3" pad="6"/>
<connect gate="G$1" pin="TX" pad="5"/>
<connect gate="G$1" pin="VIN@46" pad="46"/>
<connect gate="G$1" pin="VIN@47" pad="47"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI470X" prefix="U">
<description>FM receiver IC. Tested with Si4703. You really only need SEN, RST, SCLK, and SDIO to get a full FM radio working. Antenna comes from headphone jack. See BOB-10344.</description>
<gates>
<gate name="G$1" symbol="SI470X"/>
</gates>
<devices>
<device name="" package="SI470X">
<connects>
<connect gate="G$1" pin="!RST" pad="5"/>
<connect gate="G$1" pin="!SEN" pad="6"/>
<connect gate="G$1" pin="DOUT" pad="15"/>
<connect gate="G$1" pin="FMIP" pad="2"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@PAD" pad="21"/>
<connect gate="G$1" pin="GPIO1" pad="19"/>
<connect gate="G$1" pin="GPIO2" pad="18"/>
<connect gate="G$1" pin="GPIO3" pad="17"/>
<connect gate="G$1" pin="LOUT" pad="14"/>
<connect gate="G$1" pin="LPI" pad="4"/>
<connect gate="G$1" pin="RCLK" pad="9"/>
<connect gate="G$1" pin="RFGND" pad="3"/>
<connect gate="G$1" pin="ROUT" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="SDIO" pad="8"/>
<connect gate="G$1" pin="VA" pad="16"/>
<connect gate="G$1" pin="VD" pad="11"/>
<connect gate="G$1" pin="VIO" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI4700">
<description>&lt;b&gt;Silicon Labs FM Receiver&lt;/b&gt;&lt;p&gt;
76-108 MHz FM band support with integrated VCO, automatic gain control, automatic frequency control and seek tuning.</description>
<gates>
<gate name="G$1" symbol="SI4700/01-GM"/>
</gates>
<devices>
<device name="SMD" package="SI4700/01-GM">
<connects>
<connect gate="G$1" pin="FMIN" pad="4"/>
<connect gate="G$1" pin="FMIP" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="6"/>
<connect gate="G$1" pin="GND3" pad="14"/>
<connect gate="G$1" pin="GND4" pad="17"/>
<connect gate="G$1" pin="GND5" pad="24"/>
<connect gate="G$1" pin="GND@0" pad="0"/>
<connect gate="G$1" pin="GPIO1" pad="21"/>
<connect gate="G$1" pin="GPIO2" pad="20"/>
<connect gate="G$1" pin="GPIO3" pad="19"/>
<connect gate="G$1" pin="LOUT" pad="16"/>
<connect gate="G$1" pin="RCLK" pad="11"/>
<connect gate="G$1" pin="RFGND" pad="3"/>
<connect gate="G$1" pin="ROUT" pad="15"/>
<connect gate="G$1" pin="RST" pad="7"/>
<connect gate="G$1" pin="SCLK" pad="9"/>
<connect gate="G$1" pin="SDIO" pad="10"/>
<connect gate="G$1" pin="SEN" pad="8"/>
<connect gate="G$1" pin="VA" pad="18"/>
<connect gate="G$1" pin="VD" pad="13"/>
<connect gate="G$1" pin="VIO" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SM130" prefix="U">
<description>13.56MHz RFID Mifare Read/Write Module</description>
<gates>
<gate name="G$1" symbol="SM130"/>
</gates>
<devices>
<device name="" package="SM130">
<connects>
<connect gate="G$1" pin="ANT1" pad="24"/>
<connect gate="G$1" pin="ANT2" pad="26"/>
<connect gate="G$1" pin="ERROR" pad="17"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="I1" pad="19"/>
<connect gate="G$1" pin="I2" pad="20"/>
<connect gate="G$1" pin="O1" pad="21"/>
<connect gate="G$1" pin="O2" pad="22"/>
<connect gate="G$1" pin="OK" pad="16"/>
<connect gate="G$1" pin="RESET" pad="18"/>
<connect gate="G$1" pin="RFGND@23" pad="23"/>
<connect gate="G$1" pin="RFGND@25" pad="25"/>
<connect gate="G$1" pin="RFGND@27" pad="27"/>
<connect gate="G$1" pin="RFVCC" pad="1"/>
<connect gate="G$1" pin="RX-I" pad="11"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="TX-O" pad="12"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SM5100B">
<description>Quad-band GSM modem</description>
<gates>
<gate name="G$1" symbol="SM5100B"/>
</gates>
<devices>
<device name="" package="SM5100B">
<connects>
<connect gate="G$1" pin="ADIN1" pad="6"/>
<connect gate="G$1" pin="ADIN2" pad="8"/>
<connect gate="G$1" pin="AUX_MICN" pad="50"/>
<connect gate="G$1" pin="AUX_MICP" pad="42"/>
<connect gate="G$1" pin="AUX_SPKN" pad="58"/>
<connect gate="G$1" pin="AUX_SPKP" pad="44"/>
<connect gate="G$1" pin="EAR_MICN" pad="12"/>
<connect gate="G$1" pin="EAR_MICP" pad="14"/>
<connect gate="G$1" pin="EAR_SPKN" pad="16"/>
<connect gate="G$1" pin="EAR_SPKP" pad="18"/>
<connect gate="G$1" pin="GND@0" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GPIO_1" pad="39"/>
<connect gate="G$1" pin="GPIO_10" pad="37"/>
<connect gate="G$1" pin="GPIO_16" pad="52"/>
<connect gate="G$1" pin="GPIO_17" pad="22"/>
<connect gate="G$1" pin="GPIO_18" pad="45"/>
<connect gate="G$1" pin="GPIO_19" pad="10"/>
<connect gate="G$1" pin="GPIO_20" pad="56"/>
<connect gate="G$1" pin="GPIO_26" pad="49"/>
<connect gate="G$1" pin="GPIO_3" pad="55"/>
<connect gate="G$1" pin="GPIO_4" pad="35"/>
<connect gate="G$1" pin="GPIO_46" pad="57"/>
<connect gate="G$1" pin="GPIO_6" pad="38"/>
<connect gate="G$1" pin="GPIO_8" pad="54"/>
<connect gate="G$1" pin="GPIO_9" pad="41"/>
<connect gate="G$1" pin="GPO42/NBOOT" pad="33"/>
<connect gate="G$1" pin="GPO_11" pad="53"/>
<connect gate="G$1" pin="KEY_DRV0" pad="24"/>
<connect gate="G$1" pin="KEY_DRV1" pad="28"/>
<connect gate="G$1" pin="KEY_DRV2" pad="26"/>
<connect gate="G$1" pin="KEY_DRV3" pad="23"/>
<connect gate="G$1" pin="KEY_DRV4" pad="25"/>
<connect gate="G$1" pin="KEY_DRV5" pad="30"/>
<connect gate="G$1" pin="KEY_SEN0" pad="36"/>
<connect gate="G$1" pin="KEY_SEN1" pad="32"/>
<connect gate="G$1" pin="KEY_SEN2" pad="31"/>
<connect gate="G$1" pin="KEY_SEN3" pad="40"/>
<connect gate="G$1" pin="POWER_ON" pad="59"/>
<connect gate="G$1" pin="RESET" pad="34"/>
<connect gate="G$1" pin="RTC_BATT" pad="48"/>
<connect gate="G$1" pin="RXD0" pad="20"/>
<connect gate="G$1" pin="RXD1" pad="43"/>
<connect gate="G$1" pin="SIM_CLK" pad="27"/>
<connect gate="G$1" pin="SIM_DA" pad="29"/>
<connect gate="G$1" pin="SIM_RST" pad="21"/>
<connect gate="G$1" pin="SIM_VCC" pad="51"/>
<connect gate="G$1" pin="TXD0" pad="19"/>
<connect gate="G$1" pin="TXD1" pad="46"/>
<connect gate="G$1" pin="VBAT@0" pad="7"/>
<connect gate="G$1" pin="VBAT@1" pad="1"/>
<connect gate="G$1" pin="VBAT@2" pad="3"/>
<connect gate="G$1" pin="VBAT@3" pad="5"/>
<connect gate="G$1" pin="VCC@0" pad="47"/>
<connect gate="G$1" pin="VCC@1" pad="60"/>
<connect gate="G$1" pin="VCHG@0" pad="2"/>
<connect gate="G$1" pin="VCHG@1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL_FOR_TESTING!!" package="SM5100B-SPECIAL_FOR_TESTING">
<connects>
<connect gate="G$1" pin="ADIN1" pad="6"/>
<connect gate="G$1" pin="ADIN2" pad="8"/>
<connect gate="G$1" pin="AUX_MICN" pad="50"/>
<connect gate="G$1" pin="AUX_MICP" pad="42"/>
<connect gate="G$1" pin="AUX_SPKN" pad="58"/>
<connect gate="G$1" pin="AUX_SPKP" pad="44"/>
<connect gate="G$1" pin="EAR_MICN" pad="12"/>
<connect gate="G$1" pin="EAR_MICP" pad="14"/>
<connect gate="G$1" pin="EAR_SPKN" pad="16"/>
<connect gate="G$1" pin="EAR_SPKP" pad="18"/>
<connect gate="G$1" pin="GND@0" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GPIO_1" pad="39"/>
<connect gate="G$1" pin="GPIO_10" pad="37"/>
<connect gate="G$1" pin="GPIO_16" pad="52"/>
<connect gate="G$1" pin="GPIO_17" pad="22"/>
<connect gate="G$1" pin="GPIO_18" pad="45"/>
<connect gate="G$1" pin="GPIO_19" pad="10"/>
<connect gate="G$1" pin="GPIO_20" pad="56"/>
<connect gate="G$1" pin="GPIO_26" pad="49"/>
<connect gate="G$1" pin="GPIO_3" pad="55"/>
<connect gate="G$1" pin="GPIO_4" pad="35"/>
<connect gate="G$1" pin="GPIO_46" pad="57"/>
<connect gate="G$1" pin="GPIO_6" pad="38"/>
<connect gate="G$1" pin="GPIO_8" pad="54"/>
<connect gate="G$1" pin="GPIO_9" pad="41"/>
<connect gate="G$1" pin="GPO42/NBOOT" pad="33"/>
<connect gate="G$1" pin="GPO_11" pad="53"/>
<connect gate="G$1" pin="KEY_DRV0" pad="24"/>
<connect gate="G$1" pin="KEY_DRV1" pad="28"/>
<connect gate="G$1" pin="KEY_DRV2" pad="26"/>
<connect gate="G$1" pin="KEY_DRV3" pad="23"/>
<connect gate="G$1" pin="KEY_DRV4" pad="25"/>
<connect gate="G$1" pin="KEY_DRV5" pad="30"/>
<connect gate="G$1" pin="KEY_SEN0" pad="36"/>
<connect gate="G$1" pin="KEY_SEN1" pad="32"/>
<connect gate="G$1" pin="KEY_SEN2" pad="31"/>
<connect gate="G$1" pin="KEY_SEN3" pad="40"/>
<connect gate="G$1" pin="POWER_ON" pad="59"/>
<connect gate="G$1" pin="RESET" pad="34"/>
<connect gate="G$1" pin="RTC_BATT" pad="48"/>
<connect gate="G$1" pin="RXD0" pad="20"/>
<connect gate="G$1" pin="RXD1" pad="43"/>
<connect gate="G$1" pin="SIM_CLK" pad="27"/>
<connect gate="G$1" pin="SIM_DA" pad="29"/>
<connect gate="G$1" pin="SIM_RST" pad="21"/>
<connect gate="G$1" pin="SIM_VCC" pad="51"/>
<connect gate="G$1" pin="TXD0" pad="19"/>
<connect gate="G$1" pin="TXD1" pad="46"/>
<connect gate="G$1" pin="VBAT@0" pad="7"/>
<connect gate="G$1" pin="VBAT@1" pad="1"/>
<connect gate="G$1" pin="VBAT@2" pad="3"/>
<connect gate="G$1" pin="VBAT@3" pad="5"/>
<connect gate="G$1" pin="VCC@0" pad="47"/>
<connect gate="G$1" pin="VCC@1" pad="60"/>
<connect gate="G$1" pin="VCHG@0" pad="2"/>
<connect gate="G$1" pin="VCHG@1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA661AS">
<description>GPS low noise amplifier, 18dB gain, low external parts count</description>
<gates>
<gate name="G$1" symbol="SMA661AS"/>
</gates>
<devices>
<device name="" package="SOT666">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="PD" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUP500F" prefix="U">
<description>SUP500F Venus GPS</description>
<gates>
<gate name="G$1" symbol="SUP500F"/>
</gates>
<devices>
<device name="" package="SUP500F">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PPS" pad="6"/>
<connect gate="G$1" pin="PSEL" pad="7"/>
<connect gate="G$1" pin="RX-I" pad="1"/>
<connect gate="G$1" pin="TX-O" pad="2"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TFM-511P">
<gates>
<gate name="G$1" symbol="TFM-511"/>
</gates>
<devices>
<device name="" package="TFM-511">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="BUSEN" pad="7"/>
<connect gate="G$1" pin="BUSMOD" pad="8"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="DAT" pad="10"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LOUT" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="ROUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRF-24G">
<description>2.4GHz wireless module</description>
<gates>
<gate name="G$1" symbol="TRF-24G"/>
</gates>
<devices>
<device name="" package="TRF-24G-SOCKET">
<connects>
<connect gate="G$1" pin="CE" pad="P$9"/>
<connect gate="G$1" pin="CLK1" pad="P$6"/>
<connect gate="G$1" pin="CLK2" pad="P$8"/>
<connect gate="G$1" pin="CS" pad="P$7"/>
<connect gate="G$1" pin="DATA" pad="P$5"/>
<connect gate="G$1" pin="DOUT2" pad="P$3"/>
<connect gate="G$1" pin="DR1" pad="P$4"/>
<connect gate="G$1" pin="DR2" pad="P$2"/>
<connect gate="G$1" pin="GND" pad="P$10"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VENUS634">
<description>Venus634 from SkyTraq</description>
<gates>
<gate name="G$1" symbol="VENUS634FLPX"/>
</gates>
<devices>
<device name="SMD" package="LGA44">
<connects>
<connect gate="G$1" pin="BTSEL" pad="9"/>
<connect gate="G$1" pin="CLK" pad="41"/>
<connect gate="G$1" pin="CSN" pad="43"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GNDRF@21" pad="21"/>
<connect gate="G$1" pin="GNDRF@22" pad="22"/>
<connect gate="G$1" pin="GNDRF@24" pad="24"/>
<connect gate="G$1" pin="GNDRF@25" pad="25"/>
<connect gate="G$1" pin="GNDRF@27" pad="27"/>
<connect gate="G$1" pin="GNDRF@28" pad="28"/>
<connect gate="G$1" pin="GNDRF@29" pad="29"/>
<connect gate="G$1" pin="GNDRF@31" pad="31"/>
<connect gate="G$1" pin="GNDRF@33" pad="33"/>
<connect gate="G$1" pin="GPIO1" pad="6"/>
<connect gate="G$1" pin="GPIO2" pad="5"/>
<connect gate="G$1" pin="GPIO20" pad="14"/>
<connect gate="G$1" pin="GPIO24" pad="8"/>
<connect gate="G$1" pin="LED" pad="7"/>
<connect gate="G$1" pin="MISO" pad="39"/>
<connect gate="G$1" pin="MOSI" pad="38"/>
<connect gate="G$1" pin="PIO12" pad="4"/>
<connect gate="G$1" pin="PIO14" pad="37"/>
<connect gate="G$1" pin="PPS" pad="40"/>
<connect gate="G$1" pin="REGEN" pad="36"/>
<connect gate="G$1" pin="RFIN" pad="32"/>
<connect gate="G$1" pin="RSTN" pad="1"/>
<connect gate="G$1" pin="RTC" pad="17"/>
<connect gate="G$1" pin="RX" pad="42"/>
<connect gate="G$1" pin="TX" pad="44"/>
<connect gate="G$1" pin="VBAT" pad="18"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VENUS638FLPX-L" prefix="U">
<description>&lt;b&gt;Venus638FLPX-L GPS Receiver&lt;/b&gt;&lt;p&gt;

Venus638FLPx is a high performance, low cost, single
chip GPS receiver targeting mobile consumer and cellular
handset applications. It offers very low power
consumption, high sensitivity, and best in class signal
acquisition and time-to-first-fix performance.&lt;p&gt;
Venus638FLPx contains all the necessary components of
a complete GPS receiver, includes 1.2dB cascaded
system NF RF front-end, GPS baseband signal processor,
0.5ppm TCXO, 32.768kHz RTC crystal, RTC LDO
regulator, and passive components. It requires very low
external component count and takes up only 100mm2
PCB footprint.&lt;p&gt;
Dedicated massive-correlator signal parameter search
engine within the baseband enables rapid search of all the
available satellites and acquisition of very weak signal. An
advanced track engine allows weak signal tracking and
positioning in harsh environments such as urban canyons
and under deep foliage. The self-contained architecture keeps GPS processing off
the host and allows integration into applications with very
little resource.&lt;p&gt;
FEATURES&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;20Hz update rate&lt;/li&gt;
&lt;li&gt;-148dBm cold start sensitivity&lt;/li&gt;
&lt;li&gt;-165dBm tracking sensitivity&lt;/li&gt;
&lt;li&gt;29 second cold start TTFF&lt;/li&gt;
&lt;li&gt;3.5 second TTFF with AGPS&lt;/li&gt;
&lt;li&gt;1 second hot start&lt;/li&gt;
&lt;li&gt;2.5m accuracy&lt;/li&gt;
&lt;li&gt;Multipath detection and suppression&lt;/li&gt;
&lt;li&gt;Jamming detection and mitigation&lt;/li&gt;
&lt;li&gt;SBAS (WAAS / EGNOS) support&lt;/li&gt;
&lt;li&gt;7-day extended ephemeris AGPS&lt;/li&gt;
&lt;li&gt;67mW full power navigation&lt;/li&gt;
&lt;li&gt;Works directly with active or passive antenna&lt;/li&gt;
&lt;li&gt;Internal flash for optional 75K point data logging&lt;/li&gt;
&lt;li&gt;Supports external SPI flash memory data logging&lt;/li&gt;
&lt;li&gt;Complete receiver in 10mm x 10mm x 1.3mm size&lt;/li&gt;
&lt;li&gt;Contains LNA, SAW Filter, TCXO, RTC Xtal, LDO&lt;/li&gt;
&lt;li&gt;Pb-free RoHS compliant&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="VENUS638FLPX-L"/>
</gates>
<devices>
<device name="" package="VENUS638FLPX">
<connects>
<connect gate="G$1" pin="BTSEL" pad="9"/>
<connect gate="G$1" pin="CLK" pad="41"/>
<connect gate="G$1" pin="CSN" pad="43"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@49" pad="49"/>
<connect gate="G$1" pin="GND@60" pad="60"/>
<connect gate="G$1" pin="GND@64" pad="64"/>
<connect gate="G$1" pin="GNDRF@21" pad="21"/>
<connect gate="G$1" pin="GNDRF@22" pad="22"/>
<connect gate="G$1" pin="GNDRF@24" pad="24"/>
<connect gate="G$1" pin="GNDRF@25" pad="25"/>
<connect gate="G$1" pin="GNDRF@27" pad="27"/>
<connect gate="G$1" pin="GNDRF@28" pad="28"/>
<connect gate="G$1" pin="GNDRF@29" pad="29"/>
<connect gate="G$1" pin="GNDRF@31" pad="31"/>
<connect gate="G$1" pin="GNDRF@33" pad="33"/>
<connect gate="G$1" pin="GNDRF@61" pad="61"/>
<connect gate="G$1" pin="GNDRF@62" pad="62"/>
<connect gate="G$1" pin="GNDRF@65" pad="65"/>
<connect gate="G$1" pin="GNDRF@69" pad="69"/>
<connect gate="G$1" pin="GPIO1" pad="6"/>
<connect gate="G$1" pin="GPIO2" pad="5"/>
<connect gate="G$1" pin="GPIO20" pad="14"/>
<connect gate="G$1" pin="GPIO22" pad="12"/>
<connect gate="G$1" pin="GPIO23" pad="13"/>
<connect gate="G$1" pin="GPIO24" pad="8"/>
<connect gate="G$1" pin="GPIO25" pad="53"/>
<connect gate="G$1" pin="GPIO28" pad="59"/>
<connect gate="G$1" pin="GPIO29" pad="16"/>
<connect gate="G$1" pin="GPIO3" pad="48"/>
<connect gate="G$1" pin="GPIO30" pad="54"/>
<connect gate="G$1" pin="GPIO4" pad="47"/>
<connect gate="G$1" pin="GPIO6" pad="63"/>
<connect gate="G$1" pin="LED/GPIO0" pad="7"/>
<connect gate="G$1" pin="MISO" pad="39"/>
<connect gate="G$1" pin="MOSI" pad="38"/>
<connect gate="G$1" pin="PIO11" pad="51"/>
<connect gate="G$1" pin="PIO12" pad="4"/>
<connect gate="G$1" pin="PIO14" pad="37"/>
<connect gate="G$1" pin="PIO15" pad="55"/>
<connect gate="G$1" pin="PIO5" pad="50"/>
<connect gate="G$1" pin="PPS" pad="40"/>
<connect gate="G$1" pin="REGEN" pad="36"/>
<connect gate="G$1" pin="RFIN" pad="32"/>
<connect gate="G$1" pin="RSTN" pad="1"/>
<connect gate="G$1" pin="RTC" pad="17"/>
<connect gate="G$1" pin="RXD0" pad="42"/>
<connect gate="G$1" pin="RXD1" pad="52"/>
<connect gate="G$1" pin="SCL" pad="46"/>
<connect gate="G$1" pin="SDA" pad="45"/>
<connect gate="G$1" pin="TXD0" pad="44"/>
<connect gate="G$1" pin="TXD1" pad="57"/>
<connect gate="G$1" pin="VBAT" pad="18"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VCC@58" pad="58"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIFLY_GSX">
<description>WiFi module</description>
<gates>
<gate name="G$1" symbol="WIFLY_GSX"/>
</gates>
<devices>
<device name="" package="WIFLY_GSX">
<connects>
<connect gate="G$1" pin="3V3_IN" pad="18"/>
<connect gate="G$1" pin="3V3_OUT" pad="17"/>
<connect gate="G$1" pin="DMA_RX" pad="23"/>
<connect gate="G$1" pin="DMA_TX" pad="22"/>
<connect gate="G$1" pin="EPCA" pad="6"/>
<connect gate="G$1" pin="EPCB" pad="7"/>
<connect gate="G$1" pin="FORCE_WAKE" pad="9"/>
<connect gate="G$1" pin="G1" pad="19"/>
<connect gate="G$1" pin="G10" pad="44"/>
<connect gate="G$1" pin="G2" pad="36"/>
<connect gate="G$1" pin="G3" pad="37"/>
<connect gate="G$1" pin="G4" pad="38"/>
<connect gate="G$1" pin="G5" pad="39"/>
<connect gate="G$1" pin="G6" pad="40"/>
<connect gate="G$1" pin="G7" pad="41"/>
<connect gate="G$1" pin="G8" pad="42"/>
<connect gate="G$1" pin="G9" pad="43"/>
<connect gate="G$1" pin="GPIO4" pad="29"/>
<connect gate="G$1" pin="GPIO5" pad="28"/>
<connect gate="G$1" pin="GPIO6" pad="27"/>
<connect gate="G$1" pin="GPIO7" pad="26"/>
<connect gate="G$1" pin="GPIO8" pad="25"/>
<connect gate="G$1" pin="GPIO9" pad="24"/>
<connect gate="G$1" pin="GPIO_12" pad="11"/>
<connect gate="G$1" pin="GPIO_13" pad="10"/>
<connect gate="G$1" pin="NC" pad="35"/>
<connect gate="G$1" pin="RESET_L" pad="5"/>
<connect gate="G$1" pin="SENS0" pad="34"/>
<connect gate="G$1" pin="SENS1" pad="30"/>
<connect gate="G$1" pin="SENS2" pad="31"/>
<connect gate="G$1" pin="SENS3" pad="32"/>
<connect gate="G$1" pin="SENS4" pad="2"/>
<connect gate="G$1" pin="SENS5" pad="3"/>
<connect gate="G$1" pin="SENS6" pad="1"/>
<connect gate="G$1" pin="SENS7" pad="4"/>
<connect gate="G$1" pin="SENSPWR" pad="33"/>
<connect gate="G$1" pin="SPI_CLK" pad="15"/>
<connect gate="G$1" pin="SPI_MISO" pad="16"/>
<connect gate="G$1" pin="SPI_MOSI" pad="14"/>
<connect gate="G$1" pin="SUPCAP" pad="8"/>
<connect gate="G$1" pin="URX" pad="12"/>
<connect gate="G$1" pin="UTX" pad="13"/>
<connect gate="G$1" pin="VD_3V_IN" pad="21"/>
<connect gate="G$1" pin="VD_BAT" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WLANMODULE">
<description>&lt;b&gt;DPAC WiFi Module&lt;/b&gt;
Footprint for DPAC wireless module. Not fully tested so double check it. Spark Fun Electronics SKU : (Module) WRL-00665, (Connector) WRL-00673</description>
<gates>
<gate name="G$1" symbol="WLANMODULE"/>
</gates>
<devices>
<device name="" package="WLANMODULE">
<connects>
<connect gate="G$1" pin="/RF_LED" pad="P35"/>
<connect gate="G$1" pin="/RST" pad="P7"/>
<connect gate="G$1" pin="/TSS" pad="P8"/>
<connect gate="G$1" pin="DVDD@0" pad="P3"/>
<connect gate="G$1" pin="DVDD@1" pad="P33"/>
<connect gate="G$1" pin="DVDD@2" pad="P4"/>
<connect gate="G$1" pin="DVDD@3" pad="P34"/>
<connect gate="G$1" pin="E4" pad="P32"/>
<connect gate="G$1" pin="E5" pad="P30"/>
<connect gate="G$1" pin="E6" pad="P29"/>
<connect gate="G$1" pin="E7" pad="P31"/>
<connect gate="G$1" pin="F0" pad="P25"/>
<connect gate="G$1" pin="F1" pad="P28"/>
<connect gate="G$1" pin="F2" pad="P27"/>
<connect gate="G$1" pin="F3" pad="P26"/>
<connect gate="G$1" pin="F4" pad="P18"/>
<connect gate="G$1" pin="F5" pad="P12"/>
<connect gate="G$1" pin="F6" pad="P23"/>
<connect gate="G$1" pin="F7" pad="P24"/>
<connect gate="G$1" pin="G0" pad="P22"/>
<connect gate="G$1" pin="G1" pad="P19"/>
<connect gate="G$1" pin="G2" pad="P17"/>
<connect gate="G$1" pin="G3" pad="P11"/>
<connect gate="G$1" pin="G4" pad="P14"/>
<connect gate="G$1" pin="G5" pad="P13"/>
<connect gate="G$1" pin="G6" pad="P9"/>
<connect gate="G$1" pin="G7" pad="P21"/>
<connect gate="G$1" pin="RFU" pad="P6"/>
<connect gate="G$1" pin="TSCK" pad="P20"/>
<connect gate="G$1" pin="TSI" pad="P2"/>
<connect gate="G$1" pin="TSO" pad="P10"/>
<connect gate="G$1" pin="V2.5" pad="P5"/>
<connect gate="G$1" pin="VSS@0" pad="P1"/>
<connect gate="G$1" pin="VSS@1" pad="P15"/>
<connect gate="G$1" pin="VSS@2" pad="P16"/>
<connect gate="G$1" pin="VSS@3" pad="P36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WT32">
<description>Blue Giga Audio Bluetooth Module

Footprint is not confirmed yet.</description>
<gates>
<gate name="G$1" symbol="WT32"/>
</gates>
<devices>
<device name="" package="WT32">
<connects>
<connect gate="G$1" pin="AGND@39" pad="39"/>
<connect gate="G$1" pin="AGND@43" pad="43"/>
<connect gate="G$1" pin="AGND@48" pad="48"/>
<connect gate="G$1" pin="AIO0@5" pad="5"/>
<connect gate="G$1" pin="AIO1@6" pad="6"/>
<connect gate="G$1" pin="AUDIO_IN_N_LEFT@45" pad="45"/>
<connect gate="G$1" pin="AUDIO_IN_N_RIGHT@42" pad="42"/>
<connect gate="G$1" pin="AUDIO_IN_P_LEFT@44" pad="44"/>
<connect gate="G$1" pin="AUDIO_IN_P_RIGHT@41" pad="41"/>
<connect gate="G$1" pin="AUDIO_OUT_N_LEFT@49" pad="49"/>
<connect gate="G$1" pin="AUDIO_OUT_N_RIGHT@46" pad="46"/>
<connect gate="G$1" pin="AUDIO_OUT_P_LEFT@50" pad="50"/>
<connect gate="G$1" pin="AUDIO_OUT_P_RIGHT@47" pad="47"/>
<connect gate="G$1" pin="CTS@21" pad="21"/>
<connect gate="G$1" pin="DGND@18" pad="18"/>
<connect gate="G$1" pin="DGND@2" pad="2"/>
<connect gate="G$1" pin="DGND@3" pad="3"/>
<connect gate="G$1" pin="DGND@31" pad="31"/>
<connect gate="G$1" pin="DGND@4" pad="4"/>
<connect gate="G$1" pin="LED0@36" pad="36"/>
<connect gate="G$1" pin="MIC_BIAS@40" pad="40"/>
<connect gate="G$1" pin="PCM_CLK@30" pad="30"/>
<connect gate="G$1" pin="PCM_IN@27" pad="27"/>
<connect gate="G$1" pin="PCM_OUT@28" pad="28"/>
<connect gate="G$1" pin="PCM_SYNC@29" pad="29"/>
<connect gate="G$1" pin="PIO0@7" pad="7"/>
<connect gate="G$1" pin="PIO10@14" pad="14"/>
<connect gate="G$1" pin="PIO1@8" pad="8"/>
<connect gate="G$1" pin="PIO2@9" pad="9"/>
<connect gate="G$1" pin="PIO3@10" pad="10"/>
<connect gate="G$1" pin="PIO4@26" pad="26"/>
<connect gate="G$1" pin="PIO5@25" pad="25"/>
<connect gate="G$1" pin="PIO6@24" pad="24"/>
<connect gate="G$1" pin="PIO7@23" pad="23"/>
<connect gate="G$1" pin="PIO8@22" pad="22"/>
<connect gate="G$1" pin="PIO9@13" pad="13"/>
<connect gate="G$1" pin="RESET@19" pad="19"/>
<connect gate="G$1" pin="RTS@20" pad="20"/>
<connect gate="G$1" pin="RXD@15" pad="15"/>
<connect gate="G$1" pin="SPI_CLK@33" pad="33"/>
<connect gate="G$1" pin="SPI_CS@32" pad="32"/>
<connect gate="G$1" pin="SPI_MISO@34" pad="34"/>
<connect gate="G$1" pin="SPI_MOSI@35" pad="35"/>
<connect gate="G$1" pin="TXD@16" pad="16"/>
<connect gate="G$1" pin="USB_DN@11" pad="11"/>
<connect gate="G$1" pin="USB_DP@12" pad="12"/>
<connect gate="G$1" pin="VDDIO@17" pad="17"/>
<connect gate="G$1" pin="VDD_BAT@37" pad="37"/>
<connect gate="G$1" pin="VDD_CHG@38" pad="38"/>
<connect gate="G$1" pin="VREG_ENA@1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE-1">
<description>Xbee module footprints&lt;br&gt;
SMT header is CONN-09042.</description>
<gates>
<gate name="G$1" symbol="XBEE-1"/>
</gates>
<devices>
<device name="B1" package="XBEE-1">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B2" package="XBEE-SILK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B3" package="XBEE-SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09042"/>
</technology>
</technologies>
</device>
<device name="XBEE-1_LOCK" package="XBEE-1_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTEND-DIGI-MODEM">
<description>Xtend Digi Modem WRL-09411</description>
<gates>
<gate name="G$1" symbol="XTEND-DIGI-MODEM"/>
</gates>
<devices>
<device name="" package="XTEND-DIGI-MODEM">
<connects>
<connect gate="G$1" pin="CONFIG" pad="11"/>
<connect gate="G$1" pin="CTS" pad="9"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="DO" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GPO2" pad="3"/>
<connect gate="G$1" pin="RTS" pad="10"/>
<connect gate="G$1" pin="SHDN" pad="7"/>
<connect gate="G$1" pin="SLEEP" pad="8"/>
<connect gate="G$1" pin="TX_PWR" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZG2100M">
<description>WiFi transceiver module</description>
<gates>
<gate name="G$1" symbol="ZG2100M"/>
</gates>
<devices>
<device name="" package="ZG2100M">
<connects>
<connect gate="G$1" pin="CE_N" pad="20"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="18"/>
<connect gate="G$1" pin="GND4" pad="19"/>
<connect gate="G$1" pin="GND5" pad="36"/>
<connect gate="G$1" pin="GND6" pad="25"/>
<connect gate="G$1" pin="GND7" pad="28"/>
<connect gate="G$1" pin="GND8" pad="30"/>
<connect gate="G$1" pin="INT_NX" pad="33"/>
<connect gate="G$1" pin="JTAG_EN" pad="21"/>
<connect gate="G$1" pin="JTAG_RST_N" pad="9"/>
<connect gate="G$1" pin="JTAG_TCK" pad="4"/>
<connect gate="G$1" pin="JTAG_TDI" pad="6"/>
<connect gate="G$1" pin="JTAG_TDO" pad="3"/>
<connect gate="G$1" pin="JTAG_TMS" pad="5"/>
<connect gate="G$1" pin="NC1" pad="8"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="13"/>
<connect gate="G$1" pin="NC4" pad="14"/>
<connect gate="G$1" pin="NC5" pad="15"/>
<connect gate="G$1" pin="NC6" pad="22"/>
<connect gate="G$1" pin="RES" pad="16"/>
<connect gate="G$1" pin="RST_N" pad="7"/>
<connect gate="G$1" pin="SCK" pad="34"/>
<connect gate="G$1" pin="SCS_N" pad="23"/>
<connect gate="G$1" pin="SDI" pad="35"/>
<connect gate="G$1" pin="SDO" pad="32"/>
<connect gate="G$1" pin="UART_RX" pad="26"/>
<connect gate="G$1" pin="UART_TX" pad="27"/>
<connect gate="G$1" pin="VDD_1.8_1" pad="2"/>
<connect gate="G$1" pin="VDD_1.8_2" pad="11"/>
<connect gate="G$1" pin="VDD_1.8_3" pad="24"/>
<connect gate="G$1" pin="VDD_1.8_4" pad="31"/>
<connect gate="G$1" pin="VDD_3.3_1" pad="17"/>
<connect gate="G$1" pin="VDD_3.3_2" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLE112-A" prefix="U">
<description>BlueGiga Bluetooth 4.0 module&lt;br&gt;
with integrated chip antenna and onboard&lt;br&gt;
8051 processor and peripherals</description>
<gates>
<gate name="G$1" symbol="BLE112-A"/>
</gates>
<devices>
<device name="" package="BLE112-A">
<connects>
<connect gate="G$1" pin="AVDD1" pad="2"/>
<connect gate="G$1" pin="AVDD2" pad="3"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="GND4" pad="30"/>
<connect gate="G$1" pin="P0_0" pad="28"/>
<connect gate="G$1" pin="P0_1" pad="27"/>
<connect gate="G$1" pin="P0_2" pad="26"/>
<connect gate="G$1" pin="P0_3" pad="25"/>
<connect gate="G$1" pin="P0_4" pad="24"/>
<connect gate="G$1" pin="P0_5" pad="23"/>
<connect gate="G$1" pin="P0_6" pad="22"/>
<connect gate="G$1" pin="P0_7" pad="19"/>
<connect gate="G$1" pin="P1_0" pad="18"/>
<connect gate="G$1" pin="P1_1" pad="17"/>
<connect gate="G$1" pin="P1_2" pad="16"/>
<connect gate="G$1" pin="P1_3" pad="15"/>
<connect gate="G$1" pin="P1_4" pad="14"/>
<connect gate="G$1" pin="P1_5" pad="13"/>
<connect gate="G$1" pin="P1_6" pad="8"/>
<connect gate="G$1" pin="P1_7" pad="7"/>
<connect gate="G$1" pin="P2_0" pad="6"/>
<connect gate="G$1" pin="P2_1" pad="5"/>
<connect gate="G$1" pin="P2_2" pad="4"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="USB+" pad="11"/>
<connect gate="G$1" pin="USB-" pad="12"/>
<connect gate="G$1" pin="VDD_USB" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUERADIO_BR-LE4.0-S2" uservalue="yes">
<description>BlueRadios BlueTooth 4.0 Module&lt;br&gt;
BR-LE4.0-S2A&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="BLUERADIO_BR-LE4.0-S2"/>
</gates>
<devices>
<device name="" package="BLUERADIO_BR-LE4.0-S2">
<connects>
<connect gate="G$1" pin="ADC_0" pad="21"/>
<connect gate="G$1" pin="ADC_1" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="GND@3" pad="30"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="PIO_14" pad="19"/>
<connect gate="G$1" pin="PIO_2" pad="23"/>
<connect gate="G$1" pin="PIO_3/INT" pad="26"/>
<connect gate="G$1" pin="PIO_4" pad="28"/>
<connect gate="G$1" pin="PIO_5" pad="24"/>
<connect gate="G$1" pin="PIO_6" pad="25"/>
<connect gate="G$1" pin="PIO_7" pad="29"/>
<connect gate="G$1" pin="PIO_8" pad="27"/>
<connect gate="G$1" pin="PIO_9" pad="22"/>
<connect gate="G$1" pin="RESET" pad="3"/>
<connect gate="G$1" pin="SPI_CLK" pad="7"/>
<connect gate="G$1" pin="SPI_CSB" pad="6"/>
<connect gate="G$1" pin="SPI_MISO" pad="5"/>
<connect gate="G$1" pin="SPI_MOSI" pad="8"/>
<connect gate="G$1" pin="UART_CTS" pad="11"/>
<connect gate="G$1" pin="UART_RTS" pad="12"/>
<connect gate="G$1" pin="UART_RX" pad="14"/>
<connect gate="G$1" pin="UART_TX" pad="13"/>
<connect gate="G$1" pin="USB_DM" pad="18"/>
<connect gate="G$1" pin="USB_DP" pad="17"/>
<connect gate="G$1" pin="USB_GND" pad="16"/>
<connect gate="G$1" pin="USB_VBUS" pad="15"/>
<connect gate="G$1" pin="VCC(2.0-3.6V)" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11328"/>
<attribute name="VALUE" value="BR-LE4.0-S2A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELECTRIC_IMP" prefix="U">
<description>&lt;h3&gt;Electric Imp SD Socket&lt;/h3&gt;
This symbol matches the &lt;a href="https://www.sparkfun.com/products/11395"&gt;Electric Imp&lt;/a&gt; pinout to a 4UCONN SD MMC connector.&lt;br&gt;
&lt;br&gt;
The 4UCONN part number is &lt;a href="http://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19646&amp;seriesno_a=12"&gt;19646&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
See this part in action on the &lt;a href="https://www.sparkfun.com/products/11400"&gt;Electric Imp Breakout&lt;/a&gt;.</description>
<gates>
<gate name="G$1" symbol="ELECTRIC_IMP"/>
</gates>
<devices>
<device name="" package="SD_MMC_SOCKET">
<connects>
<connect gate="G$1" pin="1(CLK2/CTS1/TX3/SCL2)" pad="1"/>
<connect gate="G$1" pin="2(MISO1/MOSI2/RTS1/RX3/SDA2)" pad="2"/>
<connect gate="G$1" pin="5(SCLK1/SCLK2/TX2)" pad="5"/>
<connect gate="G$1" pin="7(MOSI1/MISO2/RX2)" pad="7"/>
<connect gate="G$1" pin="8(MOSI2/TX1/SCL1)" pad="8"/>
<connect gate="G$1" pin="9(MISO2/RX1/SDA1)" pad="9"/>
<connect gate="G$1" pin="CD" pad="CD"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="ID" pad="6"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="WP" pad="WP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
