<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ADMP401">
</package>
<package name="ADMP421">
</package>
<package name="ADNS2610">
</package>
<package name="ADXL180">
</package>
<package name="ADXL193">
</package>
<package name="LFCSP-16">
</package>
<package name="LGA14">
</package>
<package name="BC-32">
<description>ADXRS6xx and ADXRS150, 300, and 401</description>
</package>
<package name="SOT-23-6">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="SO08WIDE">
</package>
<package name="LGA12">
</package>
<package name="BMP085">
</package>
<package name="CAMERA_CMOS_CON">
</package>
<package name="CAMERA_CMOS_PLUG">
</package>
<package name="CMA3000">
</package>
<package name="DCM01">
</package>
<package name="MQ-3">
<description>MQ-3 in Configuration B</description>
</package>
<package name="GEIGER_TUBE">
</package>
<package name="SC70">
</package>
<package name="QFN-16">
</package>
<package name="QFN-16-(ROUNDED0THERMAL-PAD)">
</package>
<package name="HIH-4030">
<description>HIH-4030 Humidity Sensor</description>
</package>
<package name="HMC1041Z">
</package>
<package name="HMC1051Z_2">
</package>
<package name="HMC1051Z3">
</package>
<package name="16LPCC">
</package>
<package name="LPCC20">
</package>
<package name="HMC6042">
</package>
<package name="LCC36">
</package>
<package name="LCC24">
</package>
<package name="IDG300">
</package>
<package name="SPARKFUN_IDG500">
</package>
<package name="IDG500">
</package>
<package name="QFN-24">
</package>
<package name="TSOP8523">
</package>
<package name="ODFN6">
</package>
<package name="QFN-28_6X8">
<description>QFN package with a 6x8 pin configuration.</description>
</package>
<package name="LGA16-4X4">
<description>&lt;h3&gt;16-pin LGA Package&lt;/h3&gt;
4x4x1.1mm&lt;br&gt;
0.65mm pitch&lt;br&gt;
4pins-by-4pins&lt;br&gt;
&lt;br&gt;
Package used by L3G4200D 3-axis gyro&lt;br&gt;
&lt;br&gt;
&lt;B&gt;***UNPROVEN***&lt;/b&gt;</description>
</package>
<package name="QFN-28">
</package>
<package name="LGA16-3MM">
<description>LGA16 (3x3x1mm)</description>
</package>
<package name="LGA28">
<description>Untested fp for LGA28 package</description>
</package>
<package name="1X03">
</package>
<package name="LGA28-5X5">
</package>
<package name="LTR-301">
</package>
<package name="LGA16">
<description>LGA16 for LY530AL</description>
</package>
<package name="LGA28L">
</package>
<package name="DFN-10">
<description>10-pin DFN, 2mm x 2mm x 0.85mm</description>
</package>
<package name="SOT23-3">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="MIC-9.7MM">
</package>
<package name="MIC_ELECTRET_SMD">
</package>
<package name="MEMS-MIC">
</package>
<package name="MLX90609">
</package>
<package name="TO-39">
</package>
<package name="MMA7260">
</package>
<package name="QFN-16_0.5MM">
<description>&lt;h3&gt;QFN-16 0.5mm Pitch&lt;/h3&gt;
3 x 3mm Outline&lt;br&gt;
16-pin&lt;br&gt;
Used on the MMA8452Q accelerometer&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Layout in accordance with App note AN4077&lt;br&gt;
http://cache.freescale.com/files/sensors/doc/app_note/AN4077.pdf</description>
</package>
<package name="LGA8">
<description>&lt;h4&gt;LGA8 Package&lt;/h4&gt; &lt;B&gt;**UNPROVEN**&lt;/b&gt;
&lt;ul&gt;&lt;li&gt; 5.0x3.0x1.2mm&lt;/li&gt;
&lt;li&gt;8-pad&lt;/li&gt;&lt;br&gt;&lt;/ul&gt;
Used in MPL115A1 -</description>
</package>
<package name="QFN-20-0.4MM">
<description>** 20-pin QFN ** 
initially designed for MPR121 | 
0.4mm pitch | 
3x3x0.65mm |
** VERY UNPROVEN **</description>
</package>
<package name="OS4000-T">
<description>Footprint for the OS4000-T</description>
</package>
<package name="PHOTOCELL">
</package>
<package name="PHOTOCELL-KIT">
<description>&lt;h3&gt;PHOTOCELL-KIT&lt;/h3&gt;
Through-hole photocell (http://www.sparkfun.com/products/9088)&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="QRB1114-SIDE">
</package>
<package name="QRD1114">
</package>
<package name="QRE1113">
</package>
<package name="SCA1000">
</package>
<package name="SCA3000">
</package>
<package name="SCP1000">
</package>
<package name="SCP1000-LG">
</package>
<package name="SHT1X">
<description>&lt;b&gt;SHT1x&lt;/b&gt;
Sensirion Humdity Sensor</description>
</package>
<package name="ODFN">
<description>ODFN: 1.5mm x 1.5mm. Used on the Si1120</description>
</package>
<package name="SOLARBIT-12X1">
</package>
<package name="SPM0204UD5">
</package>
<package name="ST-GYRO">
</package>
<package name="LGA28-4X5">
</package>
<package name="TCM8240MD">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="TEMT6000-SEN">
</package>
<package name="TO-92-KIT">
</package>
<package name="SOT563">
</package>
<package name="TOUCH1">
</package>
<package name="TOUCH2">
</package>
<package name="CAMERA_SFV24R-2ST_2">
</package>
<package name="VCNL4000">
<description>&lt;h3&gt;VCNL4000 Footprint&lt;/h3&gt;
For Vishay VNCL4000 proximity and ambient light sensor.&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;</description>
</package>
<package name="ADXL362">
</package>
<package name="QFN-24-NP">
</package>
</packages>
<symbols>
<symbol name="ADMP401">
<pin name="VDD"/>
<pin name="OUT"/>
<pin name="GND@6"/>
<pin name="GND@2"/>
<pin name="GND@4"/>
</symbol>
<symbol name="ADMP421">
<pin name="VDD"/>
<pin name="DATA"/>
<pin name="GND@2"/>
<pin name="CLK"/>
<pin name="L/R"/>
<pin name="GND@1"/>
<pin name="GND@3"/>
</symbol>
<symbol name="ADNS2610">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="OSC_OUT"/>
<pin name="OSC_IN"/>
<pin name="SCK"/>
<pin name="SDIO"/>
<pin name="LED_CNTL"/>
<pin name="REFA"/>
</symbol>
<symbol name="ADXL180">
<pin name="VBN@3"/>
<pin name="VDD"/>
<pin name="VBN@8"/>
<pin name="VBC"/>
<pin name="VBN@10"/>
<pin name="VBP"/>
<pin name="VSCI"/>
<pin name="VBN@18"/>
</symbol>
<symbol name="ADXL193">
<pin name="VDD"/>
<pin name="VDD2"/>
<pin name="ST"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="ADXL330">
<pin name="ST"/>
<pin name="COM@3"/>
<pin name="COM@2"/>
<pin name="COM@1"/>
<pin name="COM"/>
<pin name="ZOUT"/>
<pin name="YOUT"/>
<pin name="XOUT"/>
<pin name="VS@1"/>
<pin name="VS"/>
</symbol>
<symbol name="ADXL335">
<pin name="ST"/>
<pin name="COM@6"/>
<pin name="ZOUT"/>
<pin name="YOUT"/>
<pin name="XOUT"/>
<pin name="VS@14"/>
<pin name="VS@15"/>
<pin name="COM@5"/>
<pin name="COM@3"/>
<pin name="COM@7"/>
</symbol>
<symbol name="ADXL345">
<pin name="VDD"/>
<pin name="NC@11"/>
<pin name="NC@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="VSS"/>
<pin name="CS"/>
<pin name="INT1"/>
<pin name="INT2"/>
<pin name="GND@2"/>
<pin name="NC@10"/>
<pin name="SDO"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="ADXRS">
<pin name="AVCC"/>
<pin name="VDD"/>
<pin name="AGND"/>
<pin name="PGND"/>
<pin name="VRATIO"/>
<pin name="RATEOUT"/>
<pin name="SUMJ"/>
<pin name="NC"/>
<pin name="ST1"/>
<pin name="ST2"/>
<pin name="TEMP"/>
<pin name="CP5"/>
<pin name="CP4"/>
<pin name="CP3"/>
<pin name="CP2"/>
<pin name="CP1"/>
</symbol>
<symbol name="AT42QT1012">
<pin name="VDD"/>
<pin name="SNSK"/>
<pin name="GND"/>
<pin name="SNS"/>
<pin name="OUT"/>
<pin name="TIME"/>
</symbol>
<symbol name="AT45DB041B">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="RST" function="dot"/>
<pin name="CS" function="dot"/>
<pin name="WP" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="BMA180">
<pin name="NC"/>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="INT"/>
<pin name="CSB"/>
<pin name="NC1"/>
<pin name="SCK"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="VDDIO"/>
<pin name="NC2"/>
<pin name="NC3"/>
</symbol>
<symbol name="BMP085">
<pin name="XCLR" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="NC"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="EOC" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CAMERA_CMOS_CON">
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
<pin name="Y4"/>
<pin name="Y5"/>
<pin name="Y6"/>
<pin name="Y7"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="ENB"/>
<pin name="RST"/>
<pin name="GND@1"/>
<pin name="VCC@1"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="FVL"/>
<pin name="LVL"/>
<pin name="PCK"/>
<pin name="MCK"/>
</symbol>
<symbol name="CMA3000-A01">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="VDD1"/>
<pin name="Z"/>
<pin name="PD"/>
<pin name="RANGE"/>
<pin name="X"/>
<pin name="Y"/>
</symbol>
<symbol name="CMA3000-D01">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="DVIO"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="CS"/>
<pin name="INT"/>
</symbol>
<symbol name="DCM01">
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FC30">
<pin name="VDD_IO" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="RES@7" direction="nc"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="RES@4" direction="pwr"/>
<pin name="RES@10" direction="pwr"/>
<pin name="RES@13" direction="nc"/>
<pin name="RES@14" direction="nc"/>
<pin name="PD" direction="in"/>
<pin name="SIGN" direction="out"/>
<pin name="LC" direction="out"/>
<pin name="PC" direction="out"/>
</symbol>
<symbol name="MQ-3">
<pin name="A1"/>
<pin name="H1"/>
<pin name="B1"/>
<pin name="H2"/>
</symbol>
<symbol name="GEIGER_TUBE">
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="HALL-EFFECT">
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="HDJD-S822-QR999">
<pin name="VROUT"/>
<pin name="VGOUT"/>
<pin name="VBOUT"/>
<pin name="GSBLUE1"/>
<pin name="GSGRN0"/>
<pin name="VDD3"/>
<pin name="GND"/>
<pin name="TEST_EN"/>
<pin name="VDD5"/>
<pin name="GSRED1"/>
<pin name="GSGRN1"/>
<pin name="GSBLUE0"/>
<pin name="GSRED0"/>
</symbol>
<symbol name="HIH-4030">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="HMC1041Z">
<pin name="S/R+"/>
<pin name="S/R-"/>
<pin name="GND"/>
<pin name="OUT-"/>
<pin name="OUT+"/>
<pin name="OFFSET+"/>
<pin name="VBRIDGE"/>
<pin name="OFFSET-"/>
</symbol>
<symbol name="HMC1051Z">
<pin name="GND@1"/>
<pin name="V0+"/>
<pin name="VCC"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="S/R+"/>
<pin name="S/R-"/>
<pin name="VO-"/>
</symbol>
<symbol name="HMC1052L">
<pin name="GND2A"/>
<pin name="OFF+"/>
<pin name="OUT+A"/>
<pin name="VB"/>
<pin name="NC"/>
<pin name="OFF-"/>
<pin name="GND2B"/>
<pin name="S/R+"/>
<pin name="NC2"/>
<pin name="OUT-B"/>
<pin name="S/R-"/>
<pin name="NC3"/>
<pin name="GND1A"/>
<pin name="OUT-A"/>
<pin name="GND1B"/>
<pin name="OUT+B"/>
</symbol>
<symbol name="HMC5843">
<pin name="AVDD"/>
<pin name="DRDY"/>
<pin name="SDA"/>
<pin name="AGND"/>
<pin name="VREN"/>
<pin name="SCLP"/>
<pin name="SDAP"/>
<pin name="SCL"/>
<pin name="C1"/>
<pin name="SETC"/>
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="SVDD"/>
<pin name="SETN"/>
<pin name="SETP"/>
<pin name="OFFN"/>
<pin name="OFFP"/>
</symbol>
<symbol name="HMC5883L">
<pin name="SCL"/>
<pin name="VDD"/>
<pin name="NC@1"/>
<pin name="S1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
<pin name="SETP"/>
<pin name="GND@1"/>
<pin name="C1"/>
<pin name="GND@2"/>
<pin name="SETC"/>
<pin name="VDDIO"/>
<pin name="NC@5"/>
<pin name="DRDY"/>
<pin name="SDA"/>
</symbol>
<symbol name="HMC6042">
<pin name="C1"/>
<pin name="S/R-IN" direction="in"/>
<pin name="INZ+" direction="in"/>
<pin name="INZ-" direction="in"/>
<pin name="VDD1"/>
<pin name="S/R+"/>
<pin name="S/R-"/>
<pin name="S/R-C"/>
<pin name="FBY"/>
<pin name="OUTY" direction="out"/>
<pin name="FBX"/>
<pin name="OUTX" direction="out"/>
<pin name="OUTZ" direction="out"/>
<pin name="FBZ"/>
<pin name="VDD2"/>
<pin name="GND"/>
</symbol>
<symbol name="HMC6343">
<pin name="VDD@3"/>
<pin name="VDD@21"/>
<pin name="VDD@11"/>
<pin name="GND@25"/>
<pin name="GND@29"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="CS"/>
<pin name="CSC"/>
</symbol>
<symbol name="HMC6352">
<pin name="CA1"/>
<pin name="CA2"/>
<pin name="CB1"/>
<pin name="CB2"/>
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC"/>
</symbol>
<symbol name="IDG300">
<pin name="GND@0"/>
<pin name="X_RO"/>
<pin name="XAGC"/>
<pin name="VDD@0"/>
<pin name="CPOUT"/>
<pin name="GND@1"/>
<pin name="YAGC"/>
<pin name="GND@2"/>
<pin name="Y_RO"/>
<pin name="VDD@1"/>
<pin name="VREF"/>
<pin name="VDD@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
</symbol>
<symbol name="IDG500-1">
<pin name="GND@2"/>
<pin name="GND@8"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="CPOUT"/>
<pin name="YAGC"/>
<pin name="XAGC"/>
<pin name="VDD@19"/>
<pin name="VDD@9"/>
<pin name="X4.5IN"/>
<pin name="XOUT"/>
<pin name="X4.5OUT"/>
<pin name="Y4.5IN"/>
<pin name="YOUT"/>
<pin name="Y4.5OUT"/>
<pin name="PTATS"/>
<pin name="AZ"/>
<pin name="VREF"/>
</symbol>
<symbol name="IDG1215">
<pin name="GND@2"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="CPOUT"/>
<pin name="YAGC"/>
<pin name="XAGC"/>
<pin name="VDD@19"/>
<pin name="VDD@9"/>
<pin name="XHP1"/>
<pin name="XOUT"/>
<pin name="XHP2"/>
<pin name="YHP1"/>
<pin name="YOUT"/>
<pin name="YHP2"/>
<pin name="PTATS"/>
<pin name="AZ"/>
<pin name="VREF"/>
</symbol>
<symbol name="IMU3000">
<pin name="VDD"/>
<pin name="GND@18"/>
<pin name="INT"/>
<pin name="CPOUT"/>
<pin name="VLOG"/>
<pin name="CLKOUT"/>
<pin name="REGOUT"/>
<pin name="GND@11"/>
<pin name="SDA"/>
<pin name="AD0"/>
<pin name="CLKIN"/>
<pin name="AUX_DA"/>
<pin name="AUX_CL"/>
<pin name="SCL"/>
</symbol>
<symbol name="TSOP8523">
<pin name="GND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="OUT"/>
<pin name="VS"/>
</symbol>
<symbol name="ISL29102">
<pin name="VDD"/>
<pin name="GND"/>
<pin name="NC"/>
<pin name="REXT"/>
<pin name="NC1"/>
<pin name="VOUT"/>
</symbol>
<symbol name="ISZ-500">
<pin name="GND@28"/>
<pin name="GND@27"/>
<pin name="GND@26"/>
<pin name="GND@8"/>
<pin name="GND@2"/>
<pin name="VDD@9"/>
<pin name="VDD@19"/>
<pin name="CPOUT"/>
<pin name="Z4.5OUT"/>
<pin name="ZAGC"/>
<pin name="Z4.5IN"/>
<pin name="Z-OUT"/>
<pin name="VREF"/>
<pin name="PTATS"/>
<pin name="AZ"/>
</symbol>
<symbol name="ITG-3200">
<pin name="CLKIN"/>
<pin name="VLOGIC"/>
<pin name="AD0"/>
<pin name="REGOUT"/>
<pin name="RESV-G"/>
<pin name="INT"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="CPOUT"/>
<pin name="GND"/>
<pin name="VDD"/>
</symbol>
<symbol name="IXZ500">
<pin name="GND@2"/>
<pin name="GND@8"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="CPOUT"/>
<pin name="ZAGC"/>
<pin name="XAGC"/>
<pin name="VDD@19"/>
<pin name="VDD@9"/>
<pin name="X4.5IN"/>
<pin name="XOUT"/>
<pin name="X4.5OUT"/>
<pin name="Z4.5IN"/>
<pin name="ZOUT"/>
<pin name="Z4.5OUT"/>
<pin name="PTATS"/>
<pin name="AZ"/>
<pin name="VREF"/>
</symbol>
<symbol name="L3G4200D">
<pin name="VDDIO"/>
<pin name="SCL"/>
<pin name="SDA/SDI"/>
<pin name="SDO"/>
<pin name="CS"/>
<pin name="INT2"/>
<pin name="INT1"/>
<pin name="RSVDG@0"/>
<pin name="VDD"/>
<pin name="RSVDV@0"/>
<pin name="PLL"/>
<pin name="GND"/>
<pin name="RSVDG@4"/>
<pin name="RSDVG@3"/>
<pin name="RSVDG@2"/>
<pin name="RSVDG@1"/>
</symbol>
<symbol name="LIS3LV02DQ">
<pin name="INT" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="SDA/SDI"/>
<pin name="SCL/SPC" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="CK" direction="in"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD_IO" direction="pwr"/>
</symbol>
<symbol name="LIS302DL">
<pin name="VDD_IO" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="INT1" direction="out"/>
<pin name="INT2" direction="out"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="SDO" direction="out"/>
<pin name="SDA/SDI" direction="in"/>
<pin name="SCL/SPC" direction="in"/>
</symbol>
<symbol name="LIS331-1">
<pin name="VDD"/>
<pin name="SCL/SPC"/>
<pin name="GND@5"/>
<pin name="GND@13"/>
<pin name="GND@12"/>
<pin name="INT1"/>
<pin name="GNDR"/>
<pin name="INT2"/>
<pin name="VDDIO"/>
<pin name="VDDR"/>
<pin name="GND@16"/>
<pin name="CS"/>
<pin name="SA0/SDO"/>
<pin name="SDA/SDI"/>
</symbol>
<symbol name="LISY300AL">
<pin name="CACT"/>
<pin name="VDD"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="GND1"/>
<pin name="GND"/>
<pin name="AOUT"/>
<pin name="PD"/>
<pin name="ST"/>
<pin name="VCONT"/>
<pin name="FVDD"/>
</symbol>
<symbol name="LM34">
<pin name="V+"/>
<pin name="VOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="LOAD_CELL">
<pin name="B" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="W" direction="pas"/>
</symbol>
<symbol name="LSM303DLH">
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="SA0_A"/>
<pin name="VDD_I2C"/>
<pin name="VDD"/>
<pin name="VDD@7"/>
<pin name="SET2"/>
<pin name="C1"/>
<pin name="SET1"/>
<pin name="GND@17"/>
<pin name="DRDY_M"/>
<pin name="SDA_M"/>
<pin name="SCL_M"/>
<pin name="VDD_M"/>
<pin name="VDD_IO@22"/>
<pin name="VDD_IO@23"/>
<pin name="SCL_A"/>
<pin name="SDA_A"/>
<pin name="INT1"/>
<pin name="INT2"/>
<pin name="GND@28"/>
</symbol>
<symbol name="LTR-301">
<pin name="C"/>
<pin name="E"/>
</symbol>
<symbol name="LY530AL">
<pin name="VDDD"/>
<pin name="VDDA"/>
<pin name="RES"/>
<pin name="PD"/>
<pin name="AOUT"/>
<pin name="ST"/>
<pin name="PLL2"/>
<pin name="PLL1"/>
<pin name="DIS"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="SDO"/>
<pin name="CS"/>
<pin name="DR"/>
<pin name="CACT"/>
<pin name="GND"/>
</symbol>
<symbol name="LYPR540AH">
<pin name="RESGND1"/>
<pin name="ST"/>
<pin name="GND"/>
<pin name="VCONT_1G"/>
<pin name="VCONT_2G"/>
<pin name="FILTVDD_2G"/>
<pin name="4XZ"/>
<pin name="4XY"/>
<pin name="4XX"/>
<pin name="Z"/>
<pin name="Y"/>
<pin name="X"/>
<pin name="RESGND2"/>
<pin name="RESVDD1"/>
<pin name="RESVDD2"/>
<pin name="RESVDD3"/>
<pin name="RESVDD4"/>
<pin name="VDD"/>
</symbol>
<symbol name="MAG3110">
<pin name="CAP-A"/>
<pin name="CAP-R"/>
<pin name="GND@5"/>
<pin name="GND@10"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="INT1"/>
<pin name="VDDIO"/>
<pin name="VDD"/>
</symbol>
<symbol name="MCP9700">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="VO"/>
</symbol>
<symbol name="MCP73831">
<pin name="VIN" direction="pwr"/>
<pin name="STAT" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="PROG" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="BUZZER">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MEMS-MIC">
<pin name="VIN"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="OUT"/>
</symbol>
<symbol name="MLX90609">
<pin name="TOPCAP@1"/>
<pin name="GND"/>
<pin name="VDD"/>
<pin name="SCLK"/>
<pin name="SS"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="TEST"/>
<pin name="ERROR"/>
<pin name="SELFTEST"/>
<pin name="HVIN"/>
<pin name="OUTTEMP"/>
<pin name="FLT"/>
<pin name="OUTAR"/>
<pin name="VREF"/>
<pin name="VSSA"/>
<pin name="VDDA"/>
<pin name="CASE"/>
<pin name="TESTIN"/>
<pin name="TESTOUT"/>
<pin name="TOPCAP@2"/>
</symbol>
<symbol name="MLX90614">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="SCL/VZ"/>
<pin name="PWM/SDA"/>
</symbol>
<symbol name="MMA7260">
<pin name="VCC"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
<pin name="GS1"/>
<pin name="GS2"/>
<pin name="SLP"/>
<pin name="GND"/>
<pin name="PAD"/>
</symbol>
<symbol name="MMA7361">
<pin name="XOUT"/>
<pin name="YOUT"/>
<pin name="ZOUT"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="SLEEP"/>
<pin name="0GD"/>
<pin name="GSELECT"/>
<pin name="ST"/>
</symbol>
<symbol name="MMA8452Q">
<pin name="VDDIO"/>
<pin name="BYP"/>
<pin name="SCL"/>
<pin name="GND@0"/>
<pin name="SDA"/>
<pin name="SA0"/>
<pin name="INT2"/>
<pin name="GND@1"/>
<pin name="INT1"/>
<pin name="GND@2"/>
<pin name="VDD"/>
</symbol>
<symbol name="MPL115A">
<pin name="VDD"/>
<pin name="CAP"/>
<pin name="GND"/>
<pin name="SHDN"/>
<pin name="RST/CS"/>
<pin name="NC/DOUT"/>
<pin name="SDA/DIN"/>
<pin name="SCLK"/>
</symbol>
<symbol name="MPL3115A2">
<pin name="VDD"/>
<pin name="CAP"/>
<pin name="GND"/>
<pin name="VDDIO"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="INT1"/>
<pin name="INT2"/>
</symbol>
<symbol name="MPR121">
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="VREG"/>
<pin name="~IRQ"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="ADDR"/>
<pin name="REXT"/>
<pin name="ELE11/LED7"/>
<pin name="ELE10/LED6"/>
<pin name="ELE9/LED5"/>
<pin name="ELE8/LED4"/>
<pin name="ELE7/LED3"/>
<pin name="ELE6/LED2"/>
<pin name="ELE5/LED1"/>
<pin name="ELE4/LED0"/>
<pin name="ELE3"/>
<pin name="ELE2"/>
<pin name="ELE1"/>
<pin name="ELE0"/>
</symbol>
<symbol name="OS4000-T">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="20"/>
<pin name="19"/>
<pin name="18"/>
<pin name="17"/>
<pin name="16"/>
<pin name="14"/>
<pin name="13"/>
<pin name="12"/>
<pin name="15"/>
</symbol>
<symbol name="PHOTOCELL">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="QRE1113">
<pin name="A"/>
<pin name="E"/>
<pin name="C"/>
<pin name="K"/>
</symbol>
<symbol name="QRD1114">
<pin name="C"/>
<pin name="E"/>
<pin name="K"/>
<pin name="A"/>
</symbol>
<symbol name="SCA1000">
<pin name="SCK"/>
<pin name="N/C@2"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="OUTY"/>
<pin name="GND"/>
<pin name="CSB"/>
<pin name="N/C@8"/>
<pin name="ST2"/>
<pin name="ST1"/>
<pin name="OUTX"/>
<pin name="VDD"/>
</symbol>
<symbol name="SCA3000">
<pin name="RST"/>
<pin name="INT"/>
<pin name="CLK"/>
<pin name="DVSS"/>
<pin name="DVDD"/>
<pin name="DVIO"/>
<pin name="CSB"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="AVDD"/>
<pin name="AVSS@15"/>
<pin name="AVSS@16"/>
</symbol>
<symbol name="SCP1000_D01">
<pin name="TRIG"/>
<pin name="AVSS"/>
<pin name="ATST"/>
<pin name="AVDD"/>
<pin name="CSB"/>
<pin name="MISO"/>
<pin name="DRDY"/>
<pin name="CLK"/>
<pin name="DVDD"/>
<pin name="DVSS"/>
<pin name="DVDDS"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="PD"/>
</symbol>
<symbol name="SHT1X">
<pin name="DATA"/>
<pin name="GND" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="SI1120">
<pin name="VDD"/>
<pin name="TXGD"/>
<pin name="TXO"/>
<pin name="VSS"/>
<pin name="PRX"/>
<pin name="MD"/>
<pin name="SC"/>
<pin name="STX"/>
</symbol>
<symbol name="SOLARCELL_SINGLE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SPM0204UD5">
<pin name="VS"/>
<pin name="OUT"/>
<pin name="GND"/>
<pin name="GND#"/>
</symbol>
<symbol name="ST-GYRO-PR">
<pin name="4XINX"/>
<pin name="4XINY"/>
<pin name="4XOUTX"/>
<pin name="4XOUTY"/>
<pin name="FILTVDD"/>
<pin name="GND"/>
<pin name="HP"/>
<pin name="OUTX"/>
<pin name="OUTY"/>
<pin name="PD"/>
<pin name="RES@14"/>
<pin name="RES@15"/>
<pin name="ST"/>
<pin name="VCONT"/>
<pin name="VDD"/>
<pin name="VREF"/>
</symbol>
<symbol name="ST-GYRO-PY">
<pin name="4XINZ"/>
<pin name="4XINX"/>
<pin name="4XOUTZ"/>
<pin name="4XOUTX"/>
<pin name="FILTVDD"/>
<pin name="GND"/>
<pin name="HP"/>
<pin name="OUTZ"/>
<pin name="OUTX"/>
<pin name="PD"/>
<pin name="RES@14"/>
<pin name="RES@15"/>
<pin name="ST"/>
<pin name="VCONT"/>
<pin name="VDD"/>
<pin name="VREF"/>
</symbol>
<symbol name="TCM8240MD">
<pin name="DOUT3"/>
<pin name="DOUT2"/>
<pin name="DOUT1"/>
<pin name="DOUT0"/>
<pin name="GND@5"/>
<pin name="PVDD(2.8V)"/>
<pin name="RESET"/>
<pin name="SCL"/>
<pin name="GND@9"/>
<pin name="SDA"/>
<pin name="GND@11"/>
<pin name="DVDD(1.6V)"/>
<pin name="EXTCLK"/>
<pin name="STROBE"/>
<pin name="HBLK"/>
<pin name="VBLK"/>
<pin name="GND@17"/>
<pin name="IOVDD"/>
<pin name="DCLK"/>
<pin name="GND@20"/>
<pin name="DOUT7"/>
<pin name="DOUT6"/>
<pin name="DOUT5"/>
<pin name="DOUT4"/>
</symbol>
<symbol name="TEMPERATURE-SENSOR">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="ADJ"/>
</symbol>
<symbol name="TEMT6000-SEN">
<pin name="E1" direction="pas"/>
<pin name="C1" direction="pas"/>
</symbol>
<symbol name="TMP36">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="TMP102">
<pin name="SCL"/>
<pin name="GND"/>
<pin name="ALERT"/>
<pin name="ADD0"/>
<pin name="VCC"/>
<pin name="SDA"/>
</symbol>
<symbol name="TOUCH">
<pin name="T1"/>
<pin name="T2"/>
</symbol>
<symbol name="CAMERA_SFV24R-2ST">
<pin name="SCLK"/>
<pin name="AGND"/>
<pin name="AVDD28"/>
<pin name="RESET_N"/>
<pin name="CLK_IN"/>
<pin name="DGND"/>
<pin name="DOUT_0"/>
<pin name="DOUT_1"/>
<pin name="DOUT_2"/>
<pin name="DOUT_3"/>
<pin name="DOUT_4"/>
<pin name="DOUT_5"/>
<pin name="DOUT_6"/>
<pin name="DOUT_7"/>
<pin name="DOUT_8"/>
<pin name="VCLK_OUT"/>
<pin name="VALIDH"/>
<pin name="VALIDV"/>
<pin name="DVDD28"/>
<pin name="SDIN"/>
<pin name="PS1"/>
<pin name="PS2"/>
<pin name="SHIELD"/>
<pin name="LED_CTRL"/>
</symbol>
<symbol name="VCNL4000">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="IR-@1"/>
<pin name="IR-@0"/>
<pin name="IR+"/>
<pin name="VDD"/>
<pin name="GND@1"/>
<pin name="GND@0"/>
</symbol>
<symbol name="ADXL362">
<pin name="VDDIO"/>
<pin name="VS"/>
<pin name="SCLK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="!CS"/>
<pin name="GND"/>
<pin name="INT2"/>
<pin name="INT1"/>
</symbol>
<symbol name="GEIGER_TUBE-1">
<pin name="A"/>
<pin name="C"/>
</symbol>
<symbol name="MQ-4">
<description>MQ-4 Methane gas sensor</description>
<pin name="A1"/>
<pin name="HB"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="HA"/>
<pin name="B2"/>
</symbol>
<symbol name="MPU-9150">
<description>MPU-9150: 9DOF (3mag, 3accel, 3rotat)</description>
<pin name="VLOGIC"/>
<pin name="VDD@3"/>
<pin name="VDD@13"/>
<pin name="AD0"/>
<pin name="CPOUT"/>
<pin name="GND@18"/>
<pin name="GND@17"/>
<pin name="GND@15"/>
<pin name="FSYNC"/>
<pin name="REGOUT"/>
<pin name="CLKIN"/>
<pin name="E_SDA"/>
<pin name="E_SCL"/>
<pin name="CLKOUT"/>
<pin name="INT"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ADMP401">
<description>Omnidirection bottom-port MEMS microphone</description>
<gates>
<gate name="G$1" symbol="ADMP401"/>
</gates>
<devices>
<device name="" package="ADMP401">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADMP421">
<description>Omnidirectional bottom-port MEMS microphone (digital output)</description>
<gates>
<gate name="G$1" symbol="ADMP421"/>
</gates>
<devices>
<device name="" package="ADMP421">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DATA" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="L/R" pad="2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADNS2610" prefix="U">
<description>Optical mouse sensor (SPI)</description>
<gates>
<gate name="G$1" symbol="ADNS2610"/>
</gates>
<devices>
<device name="PTH" package="ADNS2610">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LED_CNTL" pad="5"/>
<connect gate="G$1" pin="OSC_IN" pad="1"/>
<connect gate="G$1" pin="OSC_OUT" pad="2"/>
<connect gate="G$1" pin="REFA" pad="8"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SDIO" pad="3"/>
<connect gate="G$1" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL180">
<description>Configurable 50-500g 1-axis MEMS accelerometer, digital output</description>
<gates>
<gate name="G$1" symbol="ADXL180"/>
</gates>
<devices>
<device name="" package="ADXL180">
<connects>
<connect gate="G$1" pin="VBC" pad="9"/>
<connect gate="G$1" pin="VBN@10" pad="10"/>
<connect gate="G$1" pin="VBN@18" pad="18"/>
<connect gate="G$1" pin="VBN@3" pad="3"/>
<connect gate="G$1" pin="VBN@8" pad="8"/>
<connect gate="G$1" pin="VBP" pad="12"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSCI" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL193">
<description>250g accelerometer analog out</description>
<gates>
<gate name="G$1" symbol="ADXL193"/>
</gates>
<devices>
<device name="" package="ADXL193">
<connects>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="OUT" pad="P$6"/>
<connect gate="G$1" pin="ST" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$7"/>
<connect gate="G$1" pin="VDD2" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL330">
<description>&lt;b&gt;Triple Axis Accelerometer&lt;/b&gt;
Analog Devices ADXL330 +/-3g 2.4V-5.25V Analog output. Spark Fun Electronics SKU : COM-00730. Center pad paste layer has been reduced to avoid shorting.</description>
<gates>
<gate name="G$1" symbol="ADXL330"/>
</gates>
<devices>
<device name="SMD" package="LFCSP-16">
<connects>
<connect gate="G$1" pin="COM" pad="3"/>
<connect gate="G$1" pin="COM@1" pad="5"/>
<connect gate="G$1" pin="COM@2" pad="6"/>
<connect gate="G$1" pin="COM@3" pad="7"/>
<connect gate="G$1" pin="ST" pad="2"/>
<connect gate="G$1" pin="VS" pad="14"/>
<connect gate="G$1" pin="VS@1" pad="15"/>
<connect gate="G$1" pin="XOUT" pad="12"/>
<connect gate="G$1" pin="YOUT" pad="10"/>
<connect gate="G$1" pin="ZOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL335" prefix="U">
<description>3-axis, 3g accelerometer, analog out</description>
<gates>
<gate name="G$1" symbol="ADXL335"/>
</gates>
<devices>
<device name="" package="LFCSP-16">
<connects>
<connect gate="G$1" pin="COM@3" pad="3"/>
<connect gate="G$1" pin="COM@5" pad="5"/>
<connect gate="G$1" pin="COM@6" pad="6"/>
<connect gate="G$1" pin="COM@7" pad="7"/>
<connect gate="G$1" pin="ST" pad="2"/>
<connect gate="G$1" pin="VS@14" pad="14"/>
<connect gate="G$1" pin="VS@15" pad="15"/>
<connect gate="G$1" pin="XOUT" pad="12"/>
<connect gate="G$1" pin="YOUT" pad="10"/>
<connect gate="G$1" pin="ZOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL345" prefix="U">
<description>3-axis SPI/I2C 2/4/8/16g accelerometer</description>
<gates>
<gate name="G$1" symbol="ADXL345"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC@10" pad="10"/>
<connect gate="G$1" pin="NC@11" pad="11"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXRSXXX">
<description>Various MEMS gyros- ADXRS6xx, 150, 300, 401</description>
<gates>
<gate name="G$1" symbol="ADXRS"/>
</gates>
<devices>
<device name="SMD" package="BC-32">
<connects>
<connect gate="G$1" pin="AGND" pad="AGND"/>
<connect gate="G$1" pin="AVCC" pad="AVCC"/>
<connect gate="G$1" pin="CP1" pad="CP1"/>
<connect gate="G$1" pin="CP2" pad="CP2"/>
<connect gate="G$1" pin="CP3" pad="CP3"/>
<connect gate="G$1" pin="CP4" pad="CP4"/>
<connect gate="G$1" pin="CP5" pad="CP5"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="PGND" pad="PGND"/>
<connect gate="G$1" pin="RATEOUT" pad="RATEOUT"/>
<connect gate="G$1" pin="ST1" pad="ST1"/>
<connect gate="G$1" pin="ST2" pad="ST2"/>
<connect gate="G$1" pin="SUMJ" pad="SUMJ"/>
<connect gate="G$1" pin="TEMP" pad="TEMP"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VRATIO" pad="VRATIO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT42QT1012" prefix="U">
<description>One channel capacitive touch sense</description>
<gates>
<gate name="G$1" symbol="AT42QT1012"/>
</gates>
<devices>
<device name="" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SNS" pad="4"/>
<connect gate="G$1" pin="SNSK" pad="3"/>
<connect gate="G$1" pin="TIME" pad="6"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMA180">
<description>3-axis, 14-bit SPI/I2C accelerometer.&lt;br&gt;
Range 1/1.5/2/3/4/8/16g.</description>
<gates>
<gate name="G$1" symbol="BMA180"/>
</gates>
<devices>
<device name="" package="LGA12">
<connects>
<connect gate="G$1" pin="CSB" pad="5"/>
<connect gate="G$1" pin="INT" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="11"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="SDI" pad="9"/>
<connect gate="G$1" pin="SDO" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="10"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMP085">
<description>&lt;b&gt;BMP085 Pressure Sensor&lt;/b&gt; Great little MEMS pressure sensor. SKU: COM-09603</description>
<gates>
<gate name="G$1" symbol="BMP085"/>
</gates>
<devices>
<device name="" package="BMP085">
<connects>
<connect gate="G$1" pin="EOC" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="3"/>
<connect gate="G$1" pin="VDDD" pad="4"/>
<connect gate="G$1" pin="XCLR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAMERA_CMOS_CON">
<description>&lt;b&gt;640x480 CMOS Color Camera&lt;/b&gt;
Footprint proven. Spark Fun Electronics Camera SKU : SEN-00637, Mating Connector SKU : SEN-00638</description>
<gates>
<gate name="G$1" symbol="CAMERA_CMOS_CON"/>
</gates>
<devices>
<device name="SMD" package="CAMERA_CMOS_CON">
<connects>
<connect gate="G$1" pin="ENB" pad="ENB"/>
<connect gate="G$1" pin="FVL" pad="FVLD"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="LVL" pad="LVLD"/>
<connect gate="G$1" pin="MCK" pad="MCLK"/>
<connect gate="G$1" pin="PCK" pad="PCLK"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC@1" pad="VCC@1"/>
<connect gate="G$1" pin="Y0" pad="Y0"/>
<connect gate="G$1" pin="Y1" pad="Y1"/>
<connect gate="G$1" pin="Y2" pad="Y2"/>
<connect gate="G$1" pin="Y3" pad="Y3"/>
<connect gate="G$1" pin="Y4" pad="Y4"/>
<connect gate="G$1" pin="Y5" pad="Y5"/>
<connect gate="G$1" pin="Y6" pad="Y6"/>
<connect gate="G$1" pin="Y7" pad="Y7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PLUG" package="CAMERA_CMOS_PLUG">
<connects>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="FVL" pad="17"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="LVL" pad="18"/>
<connect gate="G$1" pin="MCK" pad="20"/>
<connect gate="G$1" pin="PCK" pad="19"/>
<connect gate="G$1" pin="RST" pad="12"/>
<connect gate="G$1" pin="SCL" pad="15"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC@1" pad="14"/>
<connect gate="G$1" pin="Y0" pad="1"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="3"/>
<connect gate="G$1" pin="Y3" pad="4"/>
<connect gate="G$1" pin="Y4" pad="5"/>
<connect gate="G$1" pin="Y5" pad="6"/>
<connect gate="G$1" pin="Y6" pad="7"/>
<connect gate="G$1" pin="Y7" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CMA3000-A01">
<description>3-axis 2/8g analog output accelerometer</description>
<gates>
<gate name="G$1" symbol="CMA3000-A01"/>
</gates>
<devices>
<device name="" package="CMA3000">
<connects>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="PD" pad="P$5"/>
<connect gate="G$1" pin="RANGE" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
<connect gate="G$1" pin="VDD1" pad="P$3"/>
<connect gate="G$1" pin="X" pad="P$7"/>
<connect gate="G$1" pin="Y" pad="P$8"/>
<connect gate="G$1" pin="Z" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CMA3000-D01">
<description>3-axis 2/8g I2c/SPI accelerometer</description>
<gates>
<gate name="G$1" symbol="CMA3000-D01"/>
</gates>
<devices>
<device name="" package="CMA3000">
<connects>
<connect gate="G$1" pin="CS" pad="P$7"/>
<connect gate="G$1" pin="DVIO" pad="P$3"/>
<connect gate="G$1" pin="INT" pad="P$8"/>
<connect gate="G$1" pin="MISO" pad="P$4"/>
<connect gate="G$1" pin="MOSI" pad="P$6"/>
<connect gate="G$1" pin="SCK" pad="P$5"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
<connect gate="G$1" pin="VSS" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCM01" prefix="U">
<description>&lt;b&gt;DCM01 Reflective Blood Sensor&lt;/b&gt;&lt;br&gt;
UNPROVEN&lt;br&gt;
Sensor head for Pulse Oximeter.  Contains IR and visible red LEDs, and PIN photodiode.&lt;br&gt;
&lt;href="http://www.apmkr.com/bio-device/DCM01_datasheet.pdf"&gt;http://www.apmkr.com/bio-device/DCM01_datasheet.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="DCM01"/>
</gates>
<devices>
<device name="" package="DCM01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FC30">
<description>STMicro 3-axis accelerometer with tap detection- orientation output only.</description>
<gates>
<gate name="G$1" symbol="FC30"/>
</gates>
<devices>
<device name="SMD" package="LGA14">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="LC" pad="9"/>
<connect gate="G$1" pin="PC" pad="8"/>
<connect gate="G$1" pin="PD" pad="11"/>
<connect gate="G$1" pin="RES@10" pad="10"/>
<connect gate="G$1" pin="RES@13" pad="13"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@4" pad="4"/>
<connect gate="G$1" pin="RES@7" pad="7"/>
<connect gate="G$1" pin="SIGN" pad="12"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
<connect gate="G$1" pin="VDD@6" pad="6"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GAS_SENSOR" prefix="U">
<description>MQ-3 alcohol gas sensor . FP not tested. SEN-08880.</description>
<gates>
<gate name="G$1" symbol="MQ-3"/>
</gates>
<devices>
<device name="" package="MQ-3">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="H1" pad="HA"/>
<connect gate="G$1" pin="H2" pad="HB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HALL-EFFECT">
<description>Hall effect sensor in SC70 package</description>
<gates>
<gate name="G$1" symbol="HALL-EFFECT"/>
</gates>
<devices>
<device name="SMD" package="SC70">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HDJD-S822-QR999">
<description>Avago RGB color sensor, analog out</description>
<gates>
<gate name="G$1" symbol="HDJD-S822-QR999"/>
</gates>
<devices>
<device name="" package="QFN-16">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GSBLUE0" pad="11"/>
<connect gate="G$1" pin="GSBLUE1" pad="13"/>
<connect gate="G$1" pin="GSGRN0" pad="3"/>
<connect gate="G$1" pin="GSGRN1" pad="8"/>
<connect gate="G$1" pin="GSRED0" pad="16"/>
<connect gate="G$1" pin="GSRED1" pad="6"/>
<connect gate="G$1" pin="TEST_EN" pad="5"/>
<connect gate="G$1" pin="VBOUT" pad="12"/>
<connect gate="G$1" pin="VDD3" pad="4"/>
<connect gate="G$1" pin="VDD5" pad="1"/>
<connect gate="G$1" pin="VGOUT" pad="10"/>
<connect gate="G$1" pin="VROUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHPIC" package="QFN-16-(ROUNDED0THERMAL-PAD)">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GSBLUE0" pad="11"/>
<connect gate="G$1" pin="GSBLUE1" pad="13"/>
<connect gate="G$1" pin="GSGRN0" pad="3"/>
<connect gate="G$1" pin="GSGRN1" pad="8"/>
<connect gate="G$1" pin="GSRED0" pad="16"/>
<connect gate="G$1" pin="GSRED1" pad="6"/>
<connect gate="G$1" pin="TEST_EN" pad="5"/>
<connect gate="G$1" pin="VBOUT" pad="12"/>
<connect gate="G$1" pin="VDD3" pad="4"/>
<connect gate="G$1" pin="VDD5" pad="1"/>
<connect gate="G$1" pin="VGOUT" pad="10"/>
<connect gate="G$1" pin="VROUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HIH-4030" prefix="U">
<description>Humidity Sensor</description>
<gates>
<gate name="G$1" symbol="HIH-4030"/>
</gates>
<devices>
<device name="SMD" package="HIH-4030">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC1041Z">
<description>Honeywell 1-axis magnetometer</description>
<gates>
<gate name="G$1" symbol="HMC1041Z"/>
</gates>
<devices>
<device name="" package="HMC1041Z">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="OFFSET+" pad="3"/>
<connect gate="G$1" pin="OFFSET-" pad="1"/>
<connect gate="G$1" pin="OUT+" pad="4"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
<connect gate="G$1" pin="S/R+" pad="8"/>
<connect gate="G$1" pin="S/R-" pad="7"/>
<connect gate="G$1" pin="VBRIDGE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC1051Z">
<description>Honeywell 1-axis magnetometer</description>
<gates>
<gate name="G$1" symbol="HMC1051Z"/>
</gates>
<devices>
<device name="2" package="HMC1051Z_2">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="S/R+" pad="6"/>
<connect gate="G$1" pin="S/R-" pad="7"/>
<connect gate="G$1" pin="V0+" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VO-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="HMC1051Z3">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="S/R+" pad="6"/>
<connect gate="G$1" pin="S/R-" pad="7"/>
<connect gate="G$1" pin="V0+" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VO-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC1052L">
<description>&lt;b&gt;HMC1052L&lt;/b&gt;
Dual axis magnetic sensor. Used for compass and magnetometer applications. Schematic and footprint are not tested and probably need fixing. Spark Fun Electronics SKU : COM-00708</description>
<gates>
<gate name="G$1" symbol="HMC1052L"/>
</gates>
<devices>
<device name="" package="16LPCC">
<connects>
<connect gate="G$1" pin="GND1A" pad="13"/>
<connect gate="G$1" pin="GND1B" pad="15"/>
<connect gate="G$1" pin="GND2A" pad="1"/>
<connect gate="G$1" pin="GND2B" pad="7"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NC2" pad="9"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="OFF+" pad="2"/>
<connect gate="G$1" pin="OFF-" pad="6"/>
<connect gate="G$1" pin="OUT+A" pad="3"/>
<connect gate="G$1" pin="OUT+B" pad="16"/>
<connect gate="G$1" pin="OUT-A" pad="14"/>
<connect gate="G$1" pin="OUT-B" pad="10"/>
<connect gate="G$1" pin="S/R+" pad="8"/>
<connect gate="G$1" pin="S/R-" pad="11"/>
<connect gate="G$1" pin="VB" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC5843" prefix="U">
<description>Honeywell 3-axis digital compass IC, SEN-09371</description>
<gates>
<gate name="G$1" symbol="HMC5843"/>
</gates>
<devices>
<device name="SMD" package="LPCC20">
<connects>
<connect gate="G$1" pin="AGND" pad="17"/>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="C1" pad="13"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DRDY" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="OFFN" pad="7"/>
<connect gate="G$1" pin="OFFP" pad="6"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SCLP" pad="3"/>
<connect gate="G$1" pin="SDA" pad="20"/>
<connect gate="G$1" pin="SDAP" pad="2"/>
<connect gate="G$1" pin="SETC" pad="14"/>
<connect gate="G$1" pin="SETN" pad="10"/>
<connect gate="G$1" pin="SETP" pad="9"/>
<connect gate="G$1" pin="SVDD" pad="11"/>
<connect gate="G$1" pin="VREN" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC5883L">
<description>3 Axis Digital Compass IC</description>
<gates>
<gate name="G$1" symbol="HMC5883L"/>
</gates>
<devices>
<device name="SMD" package="16LPCC">
<connects>
<connect gate="G$1" pin="C1" pad="10"/>
<connect gate="G$1" pin="DRDY" pad="15"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="5"/>
<connect gate="G$1" pin="NC@3" pad="6"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="NC@5" pad="14"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="SETC" pad="12"/>
<connect gate="G$1" pin="SETP" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC6042">
<description>Honeywell 2-axis magnetic sensor</description>
<gates>
<gate name="G$1" symbol="HMC6042"/>
</gates>
<devices>
<device name="" package="HMC6042">
<connects>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="FBX" pad="15"/>
<connect gate="G$1" pin="FBY" pad="13"/>
<connect gate="G$1" pin="FBZ" pad="11"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="INZ+" pad="6"/>
<connect gate="G$1" pin="INZ-" pad="7"/>
<connect gate="G$1" pin="OUTX" pad="16"/>
<connect gate="G$1" pin="OUTY" pad="14"/>
<connect gate="G$1" pin="OUTZ" pad="12"/>
<connect gate="G$1" pin="S/R+" pad="4"/>
<connect gate="G$1" pin="S/R-" pad="5"/>
<connect gate="G$1" pin="S/R-C" pad="9"/>
<connect gate="G$1" pin="S/R-IN" pad="10"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC6343">
<description>Honeywell compass IC with tilt compensation, SEN-08656</description>
<gates>
<gate name="G$1" symbol="HMC6343"/>
</gates>
<devices>
<device name="A" package="LCC36">
<connects>
<connect gate="G$1" pin="CS" pad="22"/>
<connect gate="G$1" pin="CSC" pad="35"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="SCL" pad="32"/>
<connect gate="G$1" pin="SDA" pad="36"/>
<connect gate="G$1" pin="VDD@11" pad="11"/>
<connect gate="G$1" pin="VDD@21" pad="21"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC6352">
<description>Compass module from Honeywell. Works very well. Schematic and footprint are production proven. Spark Fun Electronics SKU : COM-07892</description>
<gates>
<gate name="G$1" symbol="HMC6352"/>
</gates>
<devices>
<device name="" package="LCC24">
<connects>
<connect gate="G$1" pin="CA1" pad="23"/>
<connect gate="G$1" pin="CA2" pad="22"/>
<connect gate="G$1" pin="CB1" pad="20"/>
<connect gate="G$1" pin="CB2" pad="19"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDG300">
<description>Invensense 300deg/s dual axis gyro. Works very well. Schematic and footprint are not yet production proven. Spark Fun Electronics SKU : COM-00700</description>
<gates>
<gate name="G$1" symbol="IDG300"/>
</gates>
<devices>
<device name="SMD" package="IDG300">
<connects>
<connect gate="G$1" pin="CPOUT" pad="17"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="38"/>
<connect gate="G$1" pin="GND@4" pad="39"/>
<connect gate="G$1" pin="GND@5" pad="40"/>
<connect gate="G$1" pin="GND@6" pad="GND"/>
<connect gate="G$1" pin="VDD@0" pad="14"/>
<connect gate="G$1" pin="VDD@1" pad="29"/>
<connect gate="G$1" pin="VDD@2" pad="34"/>
<connect gate="G$1" pin="VREF" pad="32"/>
<connect gate="G$1" pin="XAGC" pad="8"/>
<connect gate="G$1" pin="X_RO" pad="3"/>
<connect gate="G$1" pin="YAGC" pad="23"/>
<connect gate="G$1" pin="Y_RO" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDG500" prefix="U">
<description>Invensense 500 deg/s MEMS Gyro, COM-09070</description>
<gates>
<gate name="G$1" symbol="IDG500-1"/>
</gates>
<devices>
<device name="" package="SPARKFUN_IDG500">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="X4.5IN" pad="5"/>
<connect gate="G$1" pin="X4.5OUT" pad="7"/>
<connect gate="G$1" pin="XAGC" pad="6"/>
<connect gate="G$1" pin="XOUT" pad="1"/>
<connect gate="G$1" pin="Y4.5IN" pad="16"/>
<connect gate="G$1" pin="Y4.5OUT" pad="14"/>
<connect gate="G$1" pin="YAGC" pad="15"/>
<connect gate="G$1" pin="YOUT" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IDG1215">
<description>Invensense dual-axis 67 deg/s gyro, COM-09071</description>
<gates>
<gate name="G$1" symbol="IDG1215"/>
</gates>
<devices>
<device name="-1215" package="IDG500">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="XAGC" pad="6"/>
<connect gate="G$1" pin="XHP1" pad="1"/>
<connect gate="G$1" pin="XHP2" pad="5"/>
<connect gate="G$1" pin="XOUT" pad="7"/>
<connect gate="G$1" pin="YAGC" pad="15"/>
<connect gate="G$1" pin="YHP1" pad="20"/>
<connect gate="G$1" pin="YHP2" pad="16"/>
<connect gate="G$1" pin="YOUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IMU3000" prefix="U">
<description>3-axis I2C programmable gyro.&lt;BR&gt;
Can interface with an I2C accelerometer to provide 6-axis motion information.</description>
<gates>
<gate name="G$1" symbol="IMU3000"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="AUX_CL" pad="7"/>
<connect gate="G$1" pin="AUX_DA" pad="6"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CLKOUT" pad="22"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VLOG" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRRECEIVER">
<description>TSOP85238 38kHz IR receiver with built in demodulation and filtering- SEN-08545</description>
<gates>
<gate name="G$1" symbol="TSOP8523"/>
</gates>
<devices>
<device name="SMD" package="TSOP8523">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="4"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISL29102">
<description>Light-to-voltage converter.</description>
<gates>
<gate name="G$1" symbol="ISL29102"/>
</gates>
<devices>
<device name="" package="ODFN6">
<connects>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="NC" pad="P$3"/>
<connect gate="G$1" pin="NC1" pad="P$5"/>
<connect gate="G$1" pin="REXT" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
<connect gate="G$1" pin="VOUT" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISZ500" prefix="U">
<description>ISZ500 Single axis gyro</description>
<gates>
<gate name="G$1" symbol="ISZ-500"/>
</gates>
<devices>
<device name="SMD" package="QFN-28_6X8">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="Z-OUT" pad="20"/>
<connect gate="G$1" pin="Z4.5IN" pad="16"/>
<connect gate="G$1" pin="Z4.5OUT" pad="14"/>
<connect gate="G$1" pin="ZAGC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ITG-3200" prefix="U">
<description>ITG-3200 3-axis gyro, digital output, qfn24 package</description>
<gates>
<gate name="G$1" symbol="ITG-3200"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV-G" pad="11"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VLOGIC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IXZ500" prefix="U">
<description>IXZ-500 Dual Axis (X/Z) Gyro</description>
<gates>
<gate name="G$1" symbol="IXZ500"/>
</gates>
<devices>
<device name="SMD" package="QFN-28_6X8">
<connects>
<connect gate="G$1" pin="AZ" pad="24"/>
<connect gate="G$1" pin="CPOUT" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="8"/>
<connect gate="G$1" pin="PTATS" pad="23"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@9" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
<connect gate="G$1" pin="X4.5IN" pad="5"/>
<connect gate="G$1" pin="X4.5OUT" pad="7"/>
<connect gate="G$1" pin="XAGC" pad="6"/>
<connect gate="G$1" pin="XOUT" pad="1"/>
<connect gate="G$1" pin="Z4.5IN" pad="16"/>
<connect gate="G$1" pin="Z4.5OUT" pad="14"/>
<connect gate="G$1" pin="ZAGC" pad="15"/>
<connect gate="G$1" pin="ZOUT" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L3G4200D" prefix="U">
<description>&lt;h3&gt;L3G4200D Three-axis, digital output gyroscope&lt;/h3&gt;
The L3G4200D is a low-power three-axis angular rate sensor, has a full scale of ±250/±500/±2000 dps and is capable of measuring rates with a user-selectable bandwidth.&lt;br&gt;&lt;br&gt;
It includes a sensing element and an IC interface capable of providing the measured angular rate to the external world through a digital interface (I2C/SPI).
&lt;hr&gt;
&lt;b&gt;Package:&lt;/b&gt; 4x4x1.1 LGA-16 (LGA16-4x4.PAC)&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L3G4200D"/>
</gates>
<devices>
<device name="" package="LGA16-4X4">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="INT2" pad="6"/>
<connect gate="G$1" pin="PLL" pad="14"/>
<connect gate="G$1" pin="RSDVG@3" pad="11"/>
<connect gate="G$1" pin="RSVDG@0" pad="8"/>
<connect gate="G$1" pin="RSVDG@1" pad="9"/>
<connect gate="G$1" pin="RSVDG@2" pad="10"/>
<connect gate="G$1" pin="RSVDG@4" pad="12"/>
<connect gate="G$1" pin="RSVDV@0" pad="15"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA/SDI" pad="3"/>
<connect gate="G$1" pin="SDO" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS3LV02DQ">
<description>3-axis 2/6g I2C/SPI accelerometer</description>
<gates>
<gate name="G$1" symbol="LIS3LV02DQ"/>
</gates>
<devices>
<device name="SMD" package="QFN-28">
<connects>
<connect gate="G$1" pin="CK" pad="16"/>
<connect gate="G$1" pin="CS" pad="13"/>
<connect gate="G$1" pin="GND@0" pad="0"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT" pad="6"/>
<connect gate="G$1" pin="SCL/SPC" pad="12"/>
<connect gate="G$1" pin="SDA/SDI" pad="10"/>
<connect gate="G$1" pin="SDO" pad="9"/>
<connect gate="G$1" pin="VDD@19" pad="19"/>
<connect gate="G$1" pin="VDD@20" pad="20"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
<connect gate="G$1" pin="VDD_IO" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS302DL">
<description>3-axis I2C/SPI 2/8g accelerometer</description>
<gates>
<gate name="G$1" symbol="LIS302DL"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="SCL/SPC" pad="14"/>
<connect gate="G$1" pin="SDA/SDI" pad="13"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
<connect gate="G$1" pin="VDD@6" pad="6"/>
<connect gate="G$1" pin="VDD_IO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS331" prefix="U">
<description>3-axis 6/12/24g SPI/I2C accelerometer</description>
<gates>
<gate name="G$1" symbol="LIS331-1"/>
</gates>
<devices>
<device name="" package="LGA16-3MM">
<connects>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GNDR" pad="10"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="SA0/SDO" pad="7"/>
<connect gate="G$1" pin="SCL/SPC" pad="4"/>
<connect gate="G$1" pin="SDA/SDI" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
<connect gate="G$1" pin="VDDR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LISY300AL">
<description>Single-axis 300 deg/s analog gyroscope.&lt;br&gt;
Untested part.</description>
<gates>
<gate name="G$1" symbol="LISY300AL"/>
</gates>
<devices>
<device name="SMD" package="LGA28">
<connects>
<connect gate="G$1" pin="AOUT" pad="6"/>
<connect gate="G$1" pin="CACT" pad="5"/>
<connect gate="G$1" pin="FVDD" pad="24"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="PD" pad="10"/>
<connect gate="G$1" pin="ST" pad="11"/>
<connect gate="G$1" pin="VCONT" pad="23"/>
<connect gate="G$1" pin="VDD" pad="25"/>
<connect gate="G$1" pin="VDD1" pad="26"/>
<connect gate="G$1" pin="VDD2" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM34">
<description>10mV/degF, 1 degF accurate analog temp sensor</description>
<gates>
<gate name="G$1" symbol="LM34"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOAD_CELL" prefix="J">
<description>&lt;h3&gt;Half-wheatstone bridge Load Cell&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="LOAD_CELL"/>
</gates>
<devices>
<device name="1X03-PTH" package="1X03">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="R" pad="3"/>
<connect gate="G$1" pin="W" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LSM303DLH" prefix="U">
<description>I2C accelerometer/magnetometer/tilt compensated compass</description>
<gates>
<gate name="G$1" symbol="LSM303DLH"/>
</gates>
<devices>
<device name="SMD" package="LGA28-5X5">
<connects>
<connect gate="G$1" pin="C1" pad="15"/>
<connect gate="G$1" pin="DRDY_M" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="INT1" pad="26"/>
<connect gate="G$1" pin="INT2" pad="27"/>
<connect gate="G$1" pin="SA0_A" pad="4"/>
<connect gate="G$1" pin="SCL_A" pad="24"/>
<connect gate="G$1" pin="SCL_M" pad="20"/>
<connect gate="G$1" pin="SDA_A" pad="25"/>
<connect gate="G$1" pin="SDA_M" pad="19"/>
<connect gate="G$1" pin="SET1" pad="16"/>
<connect gate="G$1" pin="SET2" pad="12"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VDD@7" pad="7"/>
<connect gate="G$1" pin="VDD_I2C" pad="5"/>
<connect gate="G$1" pin="VDD_IO@22" pad="22"/>
<connect gate="G$1" pin="VDD_IO@23" pad="23"/>
<connect gate="G$1" pin="VDD_M" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTR-301" prefix="Q" uservalue="yes">
<description>Through-hole side-receiving IR phototransistor</description>
<gates>
<gate name="G$1" symbol="LTR-301"/>
</gates>
<devices>
<device name="" package="LTR-301">
<connects>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LY530AL">
<description>Single-axis 300deg/s gyro w/available 4x amplified output</description>
<gates>
<gate name="G$1" symbol="LY530AL"/>
</gates>
<devices>
<device name="SMD" package="LGA16">
<connects>
<connect gate="G$1" pin="AOUT" pad="4"/>
<connect gate="G$1" pin="CACT" pad="3"/>
<connect gate="G$1" pin="CS" pad="10"/>
<connect gate="G$1" pin="DIS" pad="5"/>
<connect gate="G$1" pin="DR" pad="11"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="PD" pad="8"/>
<connect gate="G$1" pin="PLL1" pad="2"/>
<connect gate="G$1" pin="PLL2" pad="1"/>
<connect gate="G$1" pin="RES" pad="14"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="ST" pad="7"/>
<connect gate="G$1" pin="VDDA" pad="16"/>
<connect gate="G$1" pin="VDDD" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LYPR540AH">
<description>3-axis 400/1600 deg/s analog output gyroscope</description>
<gates>
<gate name="G$1" symbol="LYPR540AH"/>
</gates>
<devices>
<device name="" package="LGA28L">
<connects>
<connect gate="G$1" pin="4XX" pad="17"/>
<connect gate="G$1" pin="4XY" pad="16"/>
<connect gate="G$1" pin="4XZ" pad="15"/>
<connect gate="G$1" pin="FILTVDD_2G" pad="14"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESGND1" pad="8"/>
<connect gate="G$1" pin="RESGND2" pad="23"/>
<connect gate="G$1" pin="RESVDD1" pad="24"/>
<connect gate="G$1" pin="RESVDD2" pad="25"/>
<connect gate="G$1" pin="RESVDD3" pad="26"/>
<connect gate="G$1" pin="RESVDD4" pad="27"/>
<connect gate="G$1" pin="ST" pad="9"/>
<connect gate="G$1" pin="VCONT_1G" pad="12"/>
<connect gate="G$1" pin="VCONT_2G" pad="13"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="X" pad="22"/>
<connect gate="G$1" pin="Y" pad="21"/>
<connect gate="G$1" pin="Z" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAG3110" prefix="U">
<description>3-axis digital (I2C) magnetometer</description>
<gates>
<gate name="G$1" symbol="MAG3110"/>
</gates>
<devices>
<device name="" package="DFN-10">
<connects>
<connect gate="G$1" pin="CAP-A" pad="1"/>
<connect gate="G$1" pin="CAP-R" pad="4"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="INT1" pad="9"/>
<connect gate="G$1" pin="SCL" pad="7"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP9700">
<description>Analog-output temperature sensor</description>
<gates>
<gate name="G$1" symbol="MCP9700"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC">
<description>Omni-directional electret microphone. 9.7mm standard diameter.</description>
<gates>
<gate name="G$1" symbol="BUZZER"/>
</gates>
<devices>
<device name="9.7MM" package="MIC-9.7MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ELECTRET_SMD" package="MIC_ELECTRET_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MLX90609">
<description>Single axis 150 deg/s analog and SPI MEMs gyroscope. Spark Fun Electronics SKU: COM-08336 and others</description>
<gates>
<gate name="G$1" symbol="MLX90609"/>
</gates>
<devices>
<device name="SMD" package="MLX90609">
<connects>
<connect gate="G$1" pin="CASE" pad="28"/>
<connect gate="G$1" pin="ERROR" pad="11"/>
<connect gate="G$1" pin="FLT" pad="23"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="HVIN" pad="21"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="9"/>
<connect gate="G$1" pin="OUTAR" pad="24"/>
<connect gate="G$1" pin="OUTTEMP" pad="22"/>
<connect gate="G$1" pin="SCLK" pad="6"/>
<connect gate="G$1" pin="SELFTEST" pad="12"/>
<connect gate="G$1" pin="SS" pad="7"/>
<connect gate="G$1" pin="TEST" pad="10"/>
<connect gate="G$1" pin="TESTIN" pad="29"/>
<connect gate="G$1" pin="TESTOUT" pad="30"/>
<connect gate="G$1" pin="TOPCAP@1" pad="1"/>
<connect gate="G$1" pin="TOPCAP@2" pad="32"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VDDA" pad="27"/>
<connect gate="G$1" pin="VREF" pad="25"/>
<connect gate="G$1" pin="VSSA" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MLX90614" prefix="U">
<description>Non-contact PIR I2C interface temperature sensor</description>
<gates>
<gate name="G$1" symbol="MLX90614"/>
</gates>
<devices>
<device name="_" package="TO-39">
<connects>
<connect gate="G$1" pin="PWM/SDA" pad="2"/>
<connect gate="G$1" pin="SCL/VZ" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA7260" prefix="U">
<description>Freescale 3-axis 1.5/2/4/6g analog output accelerometer.&lt;BR&gt;
Schematic element and footprint production proven. Center pad has reduced paste layer for solder short reduction. Spark Fun Electronics SKU : COM-00308</description>
<gates>
<gate name="G$1" symbol="MMA7260"/>
</gates>
<devices>
<device name="" package="MMA7260">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GS1" pad="1"/>
<connect gate="G$1" pin="GS2" pad="2"/>
<connect gate="G$1" pin="PAD" pad="PAD"/>
<connect gate="G$1" pin="SLP" pad="12"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="X" pad="15"/>
<connect gate="G$1" pin="Y" pad="14"/>
<connect gate="G$1" pin="Z" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA7361" prefix="U" uservalue="yes">
<description>3-axis 1.5/6g analog output accelerometer&lt;br&gt;
IC-09489</description>
<gates>
<gate name="G$1" symbol="MMA7361"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="0GD" pad="9"/>
<connect gate="G$1" pin="GSELECT" pad="10"/>
<connect gate="G$1" pin="SLEEP" pad="7"/>
<connect gate="G$1" pin="ST" pad="13"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="XOUT" pad="2"/>
<connect gate="G$1" pin="YOUT" pad="3"/>
<connect gate="G$1" pin="ZOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09489"/>
<attribute name="VALUE" value="IC-09489"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMA8452Q" prefix="U">
<description>&lt;h3&gt;MMA8452Q 3-Axis, 12/8-bit Digital Accelerometer&lt;/h3&gt;
&lt;ul&gt;
&lt;li&gt;&lt;B&gt;Supply Voltage:&lt;/b&gt; 1.6-3.6V&lt;/li&gt;
&lt;li&gt;&lt;B&gt;Range:&lt;/b&gt; +/- 2g, 4g, 8g&lt;/li&gt;
&lt;li&gt;&lt;B&gt;Interface:&lt;/b&gt; I&lt;sup&gt;2&lt;/sup&gt;C, 12-bit and 8-bit&lt;/li&gt;
&lt;li&gt;&lt;b&gt;ODR:&lt;/b&gt; 1.56 Hz - 800 Hz&lt;/li&gt;
&lt;li&gt;&lt;B&gt;Package:&lt;/b&gt; QFN-16&lt;/li&gt;
&lt;/ul&gt;
&lt;br&gt;
&lt;br&gt;
http://cache.freescale.com/files/sensors/doc/data_sheet/MMA8452Q.pdf</description>
<gates>
<gate name="G$1" symbol="MMA8452Q"/>
</gates>
<devices>
<device name="" package="QFN-16_0.5MM">
<connects>
<connect gate="G$1" pin="BYP" pad="2"/>
<connect gate="G$1" pin="GND@0" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="SA0" pad="7"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPL115A" prefix="U">
<description>&lt;b&gt;&lt;h3&gt;MPL115A1 (SPI) and MPL115A2 (I2C) Miniature Digital Barometer&lt;/h3&gt;&lt;/b&gt;
&lt;br&gt;
5.0x3.0x1.2mm LGA Package</description>
<gates>
<gate name="G$1" symbol="MPL115A"/>
</gates>
<devices>
<device name="" package="LGA8">
<connects>
<connect gate="G$1" pin="CAP" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC/DOUT" pad="6"/>
<connect gate="G$1" pin="RST/CS" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="8"/>
<connect gate="G$1" pin="SDA/DIN" pad="7"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPL3115A2" prefix="U">
<description>Altimeter/Pressure Sensor, I2C, 1.95V-3.6V supply, 50 to 110kPa</description>
<gates>
<gate name="G$1" symbol="MPL3115A2"/>
</gates>
<devices>
<device name="LGA8" package="LGA8">
<connects>
<connect gate="G$1" pin="CAP" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="INT1" pad="6"/>
<connect gate="G$1" pin="INT2" pad="5"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDDIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPR121">
<description>MPR121 Capacitive Touch Sensor Controller</description>
<gates>
<gate name="G$1" symbol="MPR121"/>
</gates>
<devices>
<device name="QFN20" package="QFN-20-0.4MM">
<connects>
<connect gate="G$1" pin="ADDR" pad="4"/>
<connect gate="G$1" pin="ELE0" pad="8"/>
<connect gate="G$1" pin="ELE1" pad="9"/>
<connect gate="G$1" pin="ELE10/LED6" pad="18"/>
<connect gate="G$1" pin="ELE11/LED7" pad="19"/>
<connect gate="G$1" pin="ELE2" pad="10"/>
<connect gate="G$1" pin="ELE3" pad="11"/>
<connect gate="G$1" pin="ELE4/LED0" pad="12"/>
<connect gate="G$1" pin="ELE5/LED1" pad="13"/>
<connect gate="G$1" pin="ELE6/LED2" pad="14"/>
<connect gate="G$1" pin="ELE7/LED3" pad="15"/>
<connect gate="G$1" pin="ELE8/LED4" pad="16"/>
<connect gate="G$1" pin="ELE9/LED5" pad="17"/>
<connect gate="G$1" pin="REXT" pad="7"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VREG" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="~IRQ" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OS4000-T">
<description>OS4000-T tilt-compensated compass module</description>
<gates>
<gate name="G$1" symbol="OS4000-T"/>
</gates>
<devices>
<device name="" package="OS4000-T">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PHOTOCELL" prefix="R">
<description>CdS photoresistor. This is a low cost way to detect light levels. Resistance decreases with more incoming light. SparkFun SKU: SEN-09088</description>
<gates>
<gate name="G$1" symbol="PHOTOCELL"/>
</gates>
<devices>
<device name="PTH" package="PHOTOCELL">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-KIT" package="PHOTOCELL-KIT">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QRB1114" prefix="Q">
<description>&lt;b&gt;PHOTOTRANSISTOR REFLECTIVE OBJECT SENSOR&lt;/b&gt;
&lt;p&gt;
The QRB1113/1114 consists of an infrared emitting diode and an NPN silicon phototransistor mounted side by side on a converging
optical axis in a black plastic housing. The phototransistor responds to radiation from the emitting diode only when a reflective
object passes within its field of view. The area of the optimum response approximates a circle .200" in diameter.
&lt;p&gt;Datasheet: http://www.sparkfun.com/datasheets/Sensors/QRB1114.pdf
&lt;p&gt;MAX RATINGS:
&lt;p&gt;EMITTER
&lt;br&gt;Continuous Forward Current (IF) 50 mA
&lt;br&gt;Reverse Voltage (VR) 5 V
&lt;br&gt;Power Dissipation (PD) 100 mW
&lt;p&gt;SENSOR
&lt;br&gt;Collector-Emitter Voltage (VCEO) 30 V
&lt;br&gt;Emitter-Collector Voltage (VECO) 4.5 V
&lt;br&gt;Collector Current 20 mA
&lt;br&gt;Power Dissipation (PD) 100 mW</description>
<gates>
<gate name="G$1" symbol="QRE1113"/>
</gates>
<devices>
<device name="" package="QRB1114-SIDE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="K" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QRD1114">
<description>Reflective object sensor</description>
<gates>
<gate name="G$1" symbol="QRD1114"/>
</gates>
<devices>
<device name="" package="QRD1114">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QRE1113">
<description>Reflective object sensor</description>
<gates>
<gate name="G$1" symbol="QRE1113"/>
</gates>
<devices>
<device name="" package="QRE1113">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCA1000">
<description>Dual 4g accelerometer, SPI and analog out</description>
<gates>
<gate name="G$1" symbol="SCA1000"/>
</gates>
<devices>
<device name="" package="SCA1000">
<connects>
<connect gate="G$1" pin="CSB" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="3"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="N/C@2" pad="2"/>
<connect gate="G$1" pin="N/C@8" pad="8"/>
<connect gate="G$1" pin="OUTX" pad="11"/>
<connect gate="G$1" pin="OUTY" pad="5"/>
<connect gate="G$1" pin="SCK" pad="1"/>
<connect gate="G$1" pin="ST1" pad="10"/>
<connect gate="G$1" pin="ST2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCA3000">
<description>2g SPI accelerometer with interrrupt</description>
<gates>
<gate name="G$1" symbol="SCA3000"/>
</gates>
<devices>
<device name="" package="SCA3000">
<connects>
<connect gate="G$1" pin="AVDD" pad="P$14"/>
<connect gate="G$1" pin="AVSS@15" pad="P$15"/>
<connect gate="G$1" pin="AVSS@16" pad="P$16"/>
<connect gate="G$1" pin="CLK" pad="P$4"/>
<connect gate="G$1" pin="CSB" pad="P$8"/>
<connect gate="G$1" pin="DVDD" pad="P$6"/>
<connect gate="G$1" pin="DVIO" pad="P$7"/>
<connect gate="G$1" pin="DVSS" pad="P$5"/>
<connect gate="G$1" pin="INT" pad="P$3"/>
<connect gate="G$1" pin="MISO" pad="P$12"/>
<connect gate="G$1" pin="MOSI" pad="P$13"/>
<connect gate="G$1" pin="RST" pad="P$2"/>
<connect gate="G$1" pin="SCK" pad="P$11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCP1000_D01" prefix="U">
<description>Barometric pressure sensor. Schematic elements and footprint production proven. Spark Fun Electronics SKU : COM-08128</description>
<gates>
<gate name="G$1" symbol="SCP1000_D01"/>
</gates>
<devices>
<device name="SMD" package="SCP1000">
<connects>
<connect gate="G$1" pin="ATST" pad="ATST"/>
<connect gate="G$1" pin="AVDD" pad="AVDD"/>
<connect gate="G$1" pin="AVSS" pad="AVSS"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CSB" pad="CSB"/>
<connect gate="G$1" pin="DRDY" pad="DRDY"/>
<connect gate="G$1" pin="DVDD" pad="DVDD"/>
<connect gate="G$1" pin="DVDDS" pad="DVDDS"/>
<connect gate="G$1" pin="DVSS" pad="DVSS"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI/SDA"/>
<connect gate="G$1" pin="PD" pad="PD"/>
<connect gate="G$1" pin="SCK" pad="SCK/SCL"/>
<connect gate="G$1" pin="TRIG" pad="TRIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="SCP1000-LG">
<connects>
<connect gate="G$1" pin="ATST" pad="ATST"/>
<connect gate="G$1" pin="AVDD" pad="AVDD"/>
<connect gate="G$1" pin="AVSS" pad="AVSS"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CSB" pad="CSB"/>
<connect gate="G$1" pin="DRDY" pad="DRDY"/>
<connect gate="G$1" pin="DVDD" pad="DVDD"/>
<connect gate="G$1" pin="DVDDS" pad="DVDDS"/>
<connect gate="G$1" pin="DVSS" pad="DVSS"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI/SDA"/>
<connect gate="G$1" pin="PD" pad="PD"/>
<connect gate="G$1" pin="SCK" pad="SCK/SCL"/>
<connect gate="G$1" pin="TRIG" pad="TRIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SHT1X">
<description>&lt;b&gt;SHT1x Humdity Sensor&lt;/b&gt;
Sensirion humdity sensor. Schematic element and footprint proven. Spark Fun Electronics SKU : COM-08227</description>
<gates>
<gate name="G$1" symbol="SHT1X"/>
</gates>
<devices>
<device name="SMD" package="SHT1X">
<connects>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI1120">
<description>Si1120: Proximity/Ambient Light Sensor</description>
<gates>
<gate name="G$1" symbol="SI1120"/>
</gates>
<devices>
<device name="" package="ODFN">
<connects>
<connect gate="G$1" pin="MD" pad="7"/>
<connect gate="G$1" pin="PRX" pad="1"/>
<connect gate="G$1" pin="SC" pad="6"/>
<connect gate="G$1" pin="STX" pad="4"/>
<connect gate="G$1" pin="TXGD" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLAR-IXYS" prefix="D">
<gates>
<gate name="G$1" symbol="SOLARCELL_SINGLE"/>
</gates>
<devices>
<device name="_" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="C" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-" package="SOLARBIT-12X1">
<connects>
<connect gate="G$1" pin="A" pad="+"/>
<connect gate="G$1" pin="C" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPM0204UD5">
<description>Ultrasonic range sensor</description>
<gates>
<gate name="G$1" symbol="SPM0204UD5"/>
</gates>
<devices>
<device name="SMD" package="SPM0204UD5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND#" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST-GYRO-PR">
<gates>
<gate name="G$1" symbol="ST-GYRO-PR"/>
</gates>
<devices>
<device name="LGA" package="ST-GYRO">
<connects>
<connect gate="G$1" pin="4XINX" pad="9"/>
<connect gate="G$1" pin="4XINY" pad="5"/>
<connect gate="G$1" pin="4XOUTX" pad="8"/>
<connect gate="G$1" pin="4XOUTY" pad="6"/>
<connect gate="G$1" pin="FILTVDD" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HP" pad="13"/>
<connect gate="G$1" pin="OUTX" pad="10"/>
<connect gate="G$1" pin="OUTY" pad="4"/>
<connect gate="G$1" pin="PD" pad="12"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@15" pad="15"/>
<connect gate="G$1" pin="ST" pad="11"/>
<connect gate="G$1" pin="VCONT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LGA28" package="LGA28-4X5">
<connects>
<connect gate="G$1" pin="4XINX" pad="5"/>
<connect gate="G$1" pin="4XINY" pad="16"/>
<connect gate="G$1" pin="4XOUTX" pad="7"/>
<connect gate="G$1" pin="4XOUTY" pad="14"/>
<connect gate="G$1" pin="FILTVDD" pad="18"/>
<connect gate="G$1" pin="GND" pad="26"/>
<connect gate="G$1" pin="HP" pad="24"/>
<connect gate="G$1" pin="OUTX" pad="1"/>
<connect gate="G$1" pin="OUTY" pad="20"/>
<connect gate="G$1" pin="PD" pad="28"/>
<connect gate="G$1" pin="RES@14" pad="19"/>
<connect gate="G$1" pin="RES@15" pad="25"/>
<connect gate="G$1" pin="ST" pad="27"/>
<connect gate="G$1" pin="VCONT" pad="17"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VREF" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ST-GYRO-PY">
<gates>
<gate name="G$1" symbol="ST-GYRO-PY"/>
</gates>
<devices>
<device name="SMD" package="ST-GYRO">
<connects>
<connect gate="G$1" pin="4XINX" pad="5"/>
<connect gate="G$1" pin="4XINZ" pad="9"/>
<connect gate="G$1" pin="4XOUTX" pad="6"/>
<connect gate="G$1" pin="4XOUTZ" pad="8"/>
<connect gate="G$1" pin="FILTVDD" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HP" pad="13"/>
<connect gate="G$1" pin="OUTX" pad="4"/>
<connect gate="G$1" pin="OUTZ" pad="10"/>
<connect gate="G$1" pin="PD" pad="12"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@15" pad="15"/>
<connect gate="G$1" pin="ST" pad="11"/>
<connect gate="G$1" pin="VCONT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCM8240MD" uservalue="yes">
<description>1.3MP color image sensor</description>
<gates>
<gate name="G$1" symbol="TCM8240MD"/>
</gates>
<devices>
<device name="" package="TCM8240MD">
<connects>
<connect gate="G$1" pin="DCLK" pad="P$19"/>
<connect gate="G$1" pin="DOUT0" pad="P$4"/>
<connect gate="G$1" pin="DOUT1" pad="P$3"/>
<connect gate="G$1" pin="DOUT2" pad="P$2"/>
<connect gate="G$1" pin="DOUT3" pad="P$1"/>
<connect gate="G$1" pin="DOUT4" pad="P$24"/>
<connect gate="G$1" pin="DOUT5" pad="P$23"/>
<connect gate="G$1" pin="DOUT6" pad="P$22"/>
<connect gate="G$1" pin="DOUT7" pad="P$21"/>
<connect gate="G$1" pin="DVDD(1.6V)" pad="P$12"/>
<connect gate="G$1" pin="EXTCLK" pad="P$13"/>
<connect gate="G$1" pin="GND@11" pad="P$11"/>
<connect gate="G$1" pin="GND@17" pad="P$17"/>
<connect gate="G$1" pin="GND@20" pad="P$20"/>
<connect gate="G$1" pin="GND@5" pad="P$5"/>
<connect gate="G$1" pin="GND@9" pad="P$9"/>
<connect gate="G$1" pin="HBLK" pad="P$15"/>
<connect gate="G$1" pin="IOVDD" pad="P$18"/>
<connect gate="G$1" pin="PVDD(2.8V)" pad="P$6"/>
<connect gate="G$1" pin="RESET" pad="P$7"/>
<connect gate="G$1" pin="SCL" pad="P$8"/>
<connect gate="G$1" pin="SDA" pad="P$10"/>
<connect gate="G$1" pin="STROBE" pad="P$14"/>
<connect gate="G$1" pin="VBLK" pad="P$16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMPERATURE-SENSOR">
<description>TO-92 temp sensor</description>
<gates>
<gate name="G$1" symbol="TEMPERATURE-SENSOR"/>
</gates>
<devices>
<device name="" package="TO-92">
<connects>
<connect gate="G$1" pin="ADJ" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMT6000">
<description>&lt;b&gt;Ambient Light Sensor&lt;/b&gt;
Simple light detection sensor. Output varies with light intensity input. Spark Fun Electronics SKU : COM-08348</description>
<gates>
<gate name="G$1" symbol="TEMT6000-SEN"/>
</gates>
<devices>
<device name="" package="TEMT6000-SEN">
<connects>
<connect gate="G$1" pin="C1" pad="COLLECTOR"/>
<connect gate="G$1" pin="E1" pad="EMITTER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMP36" prefix="U" uservalue="yes">
<description>Precision degC temp sensor, analog out</description>
<gates>
<gate name="G$1" symbol="TMP36"/>
</gates>
<devices>
<device name="GT9" package="TO-92">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-92-KIT" package="TO-92-KIT">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMP102" prefix="U">
<description>I2C degC temp sensor</description>
<gates>
<gate name="G$1" symbol="TMP102"/>
</gates>
<devices>
<device name="" package="SOT563">
<connects>
<connect gate="G$1" pin="ADD0" pad="4"/>
<connect gate="G$1" pin="ALERT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH">
<description>Electrode for resistive touch detection</description>
<gates>
<gate name="G$1" symbol="TOUCH"/>
</gates>
<devices>
<device name="" package="TOUCH1">
<connects>
<connect gate="G$1" pin="T1" pad="P$1"/>
<connect gate="G$1" pin="T2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="TOUCH2">
<connects>
<connect gate="G$1" pin="T1" pad="P$1"/>
<connect gate="G$1" pin="T2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSCHIPTC5747">
<description>CMOS image sensor</description>
<gates>
<gate name="G$1" symbol="CAMERA_SFV24R-2ST"/>
</gates>
<devices>
<device name="" package="CAMERA_SFV24R-2ST_2">
<connects>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="AVDD28" pad="3"/>
<connect gate="G$1" pin="CLK_IN" pad="5"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="DOUT_0" pad="7"/>
<connect gate="G$1" pin="DOUT_1" pad="8"/>
<connect gate="G$1" pin="DOUT_2" pad="9"/>
<connect gate="G$1" pin="DOUT_3" pad="10"/>
<connect gate="G$1" pin="DOUT_4" pad="11"/>
<connect gate="G$1" pin="DOUT_5" pad="12"/>
<connect gate="G$1" pin="DOUT_6" pad="13"/>
<connect gate="G$1" pin="DOUT_7" pad="14"/>
<connect gate="G$1" pin="DOUT_8" pad="15"/>
<connect gate="G$1" pin="DVDD28" pad="19"/>
<connect gate="G$1" pin="LED_CTRL" pad="24"/>
<connect gate="G$1" pin="PS1" pad="21"/>
<connect gate="G$1" pin="PS2" pad="22"/>
<connect gate="G$1" pin="RESET_N" pad="4"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="SDIN" pad="20"/>
<connect gate="G$1" pin="SHIELD" pad="23"/>
<connect gate="G$1" pin="VALIDH" pad="17"/>
<connect gate="G$1" pin="VALIDV" pad="18"/>
<connect gate="G$1" pin="VCLK_OUT" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCNL4000" prefix="U" uservalue="yes">
<description>Fully integrated proximity and ambient light sensor with infrared emitter and I2C interface&lt;br&gt;
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="VCNL4000"/>
</gates>
<devices>
<device name="" package="VCNL4000">
<connects>
<connect gate="G$1" pin="GND@0" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="IR+" pad="1"/>
<connect gate="G$1" pin="IR-@0" pad="2"/>
<connect gate="G$1" pin="IR-@1" pad="3"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GEIGER_TUBE" prefix="U" uservalue="yes">
<description>LND712 Geiger Tube (COM-08875)</description>
<gates>
<gate name="G$1" symbol="GEIGER_TUBE-1"/>
</gates>
<devices>
<device name="LND712" package="GEIGER_TUBE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL362" prefix="U" uservalue="yes">
<description>Micropower 3-axis accelerometer&lt;BR&gt;
2/4/8g digital output (SPI)&lt;br&gt;
IC-11297</description>
<gates>
<gate name="G$1" symbol="ADXL362"/>
</gates>
<devices>
<device name="" package="ADXL362">
<connects>
<connect gate="G$1" pin="!CS" pad="P$8"/>
<connect gate="G$1" pin="GND" pad="P$12 P$13 P$16"/>
<connect gate="G$1" pin="INT1" pad="P$11"/>
<connect gate="G$1" pin="INT2" pad="P$9"/>
<connect gate="G$1" pin="MISO" pad="P$7"/>
<connect gate="G$1" pin="MOSI" pad="P$6"/>
<connect gate="G$1" pin="SCLK" pad="P$4"/>
<connect gate="G$1" pin="VDDIO" pad="P$1"/>
<connect gate="G$1" pin="VS" pad="P$14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11297"/>
<attribute name="VALUE" value="ADXL362"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="METHANE_SENSOR">
<description>MQ-4 Methane Gas Sensor&lt;br&gt;
SEN-09404</description>
<gates>
<gate name="G$1" symbol="MQ-4"/>
</gates>
<devices>
<device name="" package="MQ-3">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="HA" pad="HA"/>
<connect gate="G$1" pin="HB" pad="HB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPU-9150" prefix="U" uservalue="yes">
<description>9DOF (3mag, 3accel, 3rotat). I2C interface.</description>
<gates>
<gate name="G$1" symbol="MPU-9150"/>
</gates>
<devices>
<device name="QFN-24-NP" package="QFN-24-NP">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CLKOUT" pad="22"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="E_SCL" pad="7"/>
<connect gate="G$1" pin="E_SDA" pad="6"/>
<connect gate="G$1" pin="FSYNC" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD@13" pad="13"/>
<connect gate="G$1" pin="VDD@3" pad="3"/>
<connect gate="G$1" pin="VLOGIC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
