<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<packages>
<package name="LAUNCHPAD-COMPATIBLE">
<description>Stellaris LaunchPad layout.</description>
</package>
<package name="LAUNCHPAD-XL">
<description>Stellaris LaunchPad layout.</description>
</package>
</packages>
<symbols>
<symbol name="STELLARIS-LM4F120H5QR-COMPATIBLE">
<description>TI Stellaris Launchpad LM4F120
Using only pins connected to outer header rows to maintain compatability with MSP430 booster packs</description>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PE0"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="3.3V" direction="pwr"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PF0"/>
<pin name="RST" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
</symbol>
<symbol name="STELLARIS-LM4F120H5QR-XL">
<description>TI Stellaris Launchpad LM4F120
Using all header pins to connect to XL booster packs.</description>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="3.3V" direction="pwr"/>
<pin name="VBUS" direction="pwr"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF4"/>
<pin name="RST" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="PF3"/>
<pin name="GND1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="STELLARIS-LAUNCHPAD">
<gates>
<gate name="G$1" symbol="STELLARIS-LM4F120H5QR-XL"/>
</gates>
<devices>
<device name="STELLARIS-LAUNCHPAD-XL" package="LAUNCHPAD-XL">
<connects>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="PA2" pad="PA2"/>
<connect gate="G$1" pin="PA3" pad="PA3"/>
<connect gate="G$1" pin="PA4" pad="PA4"/>
<connect gate="G$1" pin="PA5" pad="PA5"/>
<connect gate="G$1" pin="PA6" pad="PA6"/>
<connect gate="G$1" pin="PA7" pad="PA7"/>
<connect gate="G$1" pin="PB0" pad="PB0"/>
<connect gate="G$1" pin="PB1" pad="PB1"/>
<connect gate="G$1" pin="PB2" pad="PB2"/>
<connect gate="G$1" pin="PB3" pad="PB3"/>
<connect gate="G$1" pin="PB4" pad="PB4"/>
<connect gate="G$1" pin="PB5" pad="PB5"/>
<connect gate="G$1" pin="PB6" pad="PB6"/>
<connect gate="G$1" pin="PB7" pad="PB7"/>
<connect gate="G$1" pin="PC4" pad="PC4"/>
<connect gate="G$1" pin="PC5" pad="PC5"/>
<connect gate="G$1" pin="PC6" pad="PC6"/>
<connect gate="G$1" pin="PC7" pad="PC7"/>
<connect gate="G$1" pin="PD0" pad="PD0"/>
<connect gate="G$1" pin="PD1" pad="PD1"/>
<connect gate="G$1" pin="PD2" pad="PD2"/>
<connect gate="G$1" pin="PD3" pad="PD3"/>
<connect gate="G$1" pin="PD6" pad="PD6"/>
<connect gate="G$1" pin="PD7" pad="PD7"/>
<connect gate="G$1" pin="PE0" pad="PE0"/>
<connect gate="G$1" pin="PE1" pad="PE1"/>
<connect gate="G$1" pin="PE2" pad="PE2"/>
<connect gate="G$1" pin="PE3" pad="PE3"/>
<connect gate="G$1" pin="PE4" pad="PE4"/>
<connect gate="G$1" pin="PE5" pad="PE5"/>
<connect gate="G$1" pin="PF0" pad="PF0"/>
<connect gate="G$1" pin="PF1" pad="PF1"/>
<connect gate="G$1" pin="PF2" pad="PF2"/>
<connect gate="G$1" pin="PF3" pad="PF3"/>
<connect gate="G$1" pin="PF4" pad="PF4"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STELLARIS-LAUNCHPAD-COMPATIBLE">
<gates>
<gate name="G$1" symbol="STELLARIS-LM4F120H5QR-COMPATIBLE"/>
</gates>
<devices>
<device name="STELLARIS-LAUNCHPAD-COMPATIBLE" package="LAUNCHPAD-COMPATIBLE">
<connects>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="PA2" pad="PA2"/>
<connect gate="G$1" pin="PA3" pad="PA3"/>
<connect gate="G$1" pin="PA4" pad="PA4"/>
<connect gate="G$1" pin="PA5" pad="PA5"/>
<connect gate="G$1" pin="PA6" pad="PA6"/>
<connect gate="G$1" pin="PA7" pad="PA7"/>
<connect gate="G$1" pin="PB0" pad="PB0"/>
<connect gate="G$1" pin="PB1" pad="PB1"/>
<connect gate="G$1" pin="PB2" pad="PB2"/>
<connect gate="G$1" pin="PB4" pad="PB4"/>
<connect gate="G$1" pin="PB5" pad="PB5"/>
<connect gate="G$1" pin="PB6" pad="PB6"/>
<connect gate="G$1" pin="PB7" pad="PB7"/>
<connect gate="G$1" pin="PE0" pad="PE0"/>
<connect gate="G$1" pin="PE4" pad="PE4"/>
<connect gate="G$1" pin="PE5" pad="PE5"/>
<connect gate="G$1" pin="PF0" pad="PF0"/>
<connect gate="G$1" pin="RST" pad="RST"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
