<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO52A">
<description>&lt;b&gt;TO-52&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SOIC 150 mil</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="TO99">
<description>&lt;b&gt;TO-99&lt;/b&gt;</description>
</package>
<package name="TO52">
<description>&lt;b&gt;TO-52&lt;/b&gt;</description>
</package>
<package name="SO18L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO20L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO24L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO28L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;&lt;p&gt;
MAX3221-MAX3243.pdf; SO28W</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="UMAX8">
<description>&lt;b&gt;micro MAX Package&lt;/b&gt;</description>
</package>
<package name="PLCC20">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="UMAX10">
<description>&lt;b&gt;micro MAX Package&lt;/b&gt;</description>
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOT23-6L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SC70-6L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="SC70-5L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="SC70-3L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="QSOP20">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="TSOC6">
<description>&lt;b&gt;TSOC 6&lt;/b&gt;</description>
</package>
<package name="TO92-">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
DALLAS Semiconductor (DS2405.pdf)&lt;/b&gt;</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;TQFP100&lt;/b&gt;&lt;p&gt;
thin quad flat pack, square 14 x14 mm</description>
</package>
<package name="QSOP16">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="TSSOP28">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 28&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="SSOP16">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="SSOP14">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;
http://www.maxim-ic.com .. MAX3223-MAX3243.pdf</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .150 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/package_drawings/21-0041B.pdf</description>
</package>
<package name="MQFP80-2">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;&lt;p&gt;
Source: refpackages.lbr</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="68LQFN">
<description>&lt;b&gt;68L QFN&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX12527.pdf&lt;br&gt;
http://pdfserv.maxim-ic.com/package_dwgs/21-0142D.PDF</description>
</package>
<package name="UCSP6">
<description>&lt;b&gt;UCSP 6 pol.&lt;/b&gt; 3 x 2 mm&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX985-MAX994.pdf</description>
</package>
<package name="SOT23-8L">
<description>&lt;b&gt;SC70/SOT23-8&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4335-MAX4338.pdf</description>
</package>
<package name="QFN32">
<description>&lt;b&gt;QFN 32&lt;/b&gt; 5 x 5 mm&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7042.pdf</description>
</package>
<package name="SSOP36">
<description>&lt;b&gt;36L SSOP, 0.80 MM PITCH&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7042.pdf</description>
</package>
<package name="SO08-208">
<description>&lt;b&gt;SOIC .208" 8 LEAD&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/package_dwgs/G4010-001.PDF</description>
</package>
<package name="UCSP25">
<description>&lt;b&gt;UCSP-25&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4947-MAX4948.pdf</description>
</package>
<package name="TQFN24-EP">
<description>&lt;b&gt;24 TQFN-EP 24&lt;/b&gt; T2444-4&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4947-MAX4948.pdf</description>
</package>
<package name="UDFN8">
<description>&lt;b&gt;uDFN 8&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4906-MAX4907F.pdf</description>
</package>
<package name="UDFN10">
<description>&lt;b&gt;10 uDFN&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4906-MAX4907F.pdf</description>
</package>
<package name="UMAX8-THERMAL">
<description>&lt;b&gt;micro MAX Package&lt;/b&gt;
Source: MAX1792.pdf</description>
</package>
<package name="QSOP24">
<description>&lt;b&gt;QSOP 24&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7313.pdf</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="TQFN32">
<description>&lt;b&gt;TQFN 7x7 mm&lt;/b&gt;&lt;p&gt;
Source: www.maxim-ic.com/packages .. 90-0125.pdf</description>
</package>
<package name="TQFN20-5X5">
<description>&lt;b&gt;THIN QFN 20&lt;/b&gt; 5x5x0.75mm&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/package_dwgs/21-0140.PDF</description>
</package>
</packages>
<symbols>
<symbol name="MAX130">
<pin name="D1" direction="hiz"/>
<pin name="C1" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="F1" direction="hiz"/>
<pin name="G1" direction="hiz"/>
<pin name="E1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="C2" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="F2" direction="hiz"/>
<pin name="E2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="F3" direction="hiz"/>
<pin name="E3" direction="hiz"/>
<pin name="AB4" direction="hiz"/>
<pin name="G3" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="C3" direction="hiz"/>
<pin name="G2" direction="hiz"/>
<pin name="POL" direction="out"/>
<pin name="BP" direction="out"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="OSC3" direction="pas"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="COMM" direction="pwr"/>
<pin name="CREF+" direction="pas"/>
<pin name="CREF-" direction="pas"/>
<pin name="REF-LO" direction="in"/>
<pin name="REF-HI" direction="in"/>
<pin name="TEST" direction="pas"/>
<pin name="A/Z" direction="pas"/>
<pin name="BUFF" direction="pas"/>
<pin name="INT" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX133">
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="AC-OUT" direction="out"/>
<pin name="INT-OUT" direction="out"/>
<pin name="FA-OUT" direction="out"/>
<pin name="FR-OUT" direction="out"/>
<pin name="BUFFOUT1" direction="out"/>
<pin name="BUFFOUT2" direction="out"/>
<pin name="BCL-OUT" direction="out"/>
<pin name="AC-IN" direction="in"/>
<pin name="INT-IN" direction="in"/>
<pin name="FA-IN" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="BEEPER" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="FR-IN" direction="in"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="10M" direction="pas"/>
<pin name="1,11M" direction="pas"/>
<pin name="101K" direction="pas"/>
<pin name="10K" direction="pas"/>
<pin name="1K" direction="pas"/>
<pin name="VREF" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="DGND" direction="pwr"/>
<pin name="CUR-IN" direction="in"/>
<pin name="OS" direction="in"/>
<pin name="400MV-IN" direction="in"/>
<pin name="COMMON" direction="pwr"/>
<pin name="ALE" direction="in"/>
<pin name="EOC" direction="in"/>
</symbol>
<symbol name="MAX136">
<pin name="D1" direction="hiz"/>
<pin name="C1" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="F1" direction="hiz"/>
<pin name="G1" direction="hiz"/>
<pin name="E1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="C2" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="F2" direction="hiz"/>
<pin name="E2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="F3" direction="hiz"/>
<pin name="E3" direction="hiz"/>
<pin name="AB4" direction="hiz"/>
<pin name="G3" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="C3" direction="hiz"/>
<pin name="G2" direction="hiz"/>
<pin name="POL" direction="out"/>
<pin name="BP" direction="out"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="OSC3" direction="pas"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="COMM" direction="pwr"/>
<pin name="CREF+" direction="pas"/>
<pin name="CREF-" direction="pas"/>
<pin name="HOLD" direction="in"/>
<pin name="REF-HI" direction="in"/>
<pin name="TEST" direction="pas"/>
<pin name="A/Z" direction="pas"/>
<pin name="BUFF" direction="pas"/>
<pin name="INT" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX138">
<pin name="D1" direction="hiz"/>
<pin name="C1" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="F1" direction="hiz"/>
<pin name="G1" direction="hiz"/>
<pin name="E1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="C2" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="F2" direction="hiz"/>
<pin name="E2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="F3" direction="hiz"/>
<pin name="E3" direction="hiz"/>
<pin name="AB4" direction="hiz"/>
<pin name="G3" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="C3" direction="hiz"/>
<pin name="G2" direction="hiz"/>
<pin name="POL" direction="out"/>
<pin name="BP" direction="out"/>
<pin name="CAP+" direction="pas"/>
<pin name="CAP-" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="COMM" direction="pwr"/>
<pin name="CREF+" direction="pas"/>
<pin name="CREF-" direction="pas"/>
<pin name="REF-LO" direction="in"/>
<pin name="REF-HI" direction="in"/>
<pin name="TEST" direction="pas"/>
<pin name="A/Z" direction="pas"/>
<pin name="BUFF" direction="pas"/>
<pin name="INT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX150">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="REF-OUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="OFL" direction="out" function="dot"/>
<pin name="V-IN" direction="in"/>
<pin name="WR/RDY" function="dot"/>
<pin name="MODE" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
</symbol>
<symbol name="MAX154">
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="REF-OUT" direction="out"/>
<pin name="RDY" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VREF+" direction="pas"/>
<pin name="VREF-" direction="pas"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="MAX158">
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="REF-OUT" direction="out"/>
<pin name="RDY" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VREF+" direction="pas"/>
<pin name="VREF-" direction="pas"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="AIN8" direction="in"/>
</symbol>
<symbol name="MAX160">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="VREF" direction="in"/>
<pin name="BOFS" direction="in"/>
<pin name="AIN" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="MAX161">
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="VREF" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="BOFS" direction="in"/>
<pin name="STAT" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="ALE" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="MAX162">
<pin name="D0/8" direction="hiz"/>
<pin name="D1/9" direction="hiz"/>
<pin name="D2/10" direction="hiz"/>
<pin name="D3/11" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="VSS" direction="pwr"/>
<pin name="AGND" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="AIN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="CLK-IN" direction="in" function="clk"/>
<pin name="CLK-OUT" direction="out"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="BUSY" direction="in" function="dot"/>
<pin name="HBEN" direction="in"/>
</symbol>
<symbol name="MAX578">
<pin name="B1@" direction="hiz" function="dot"/>
<pin name="B1" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="B4" direction="hiz"/>
<pin name="B5" direction="hiz"/>
<pin name="B6" direction="hiz"/>
<pin name="B7" direction="hiz"/>
<pin name="B8" direction="hiz"/>
<pin name="B9" direction="hiz"/>
<pin name="B10" direction="hiz"/>
<pin name="B11" direction="hiz"/>
<pin name="B12" direction="hiz"/>
<pin name="REF-OUT" direction="out"/>
<pin name="SER-OUT@" direction="out"/>
<pin name="CLK-OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="SER-OUT" direction="out"/>
<pin name="DGND" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="CLK-ADJ" direction="in"/>
<pin name="CLK-IN" direction="in"/>
<pin name="10V-IN" direction="in"/>
<pin name="20V-IN" direction="in"/>
<pin name="REF-IN" direction="in"/>
<pin name="SHCY" direction="in"/>
<pin name="ZERO-ADJ" direction="in"/>
<pin name="EOC" direction="out"/>
<pin name="CONST" direction="in"/>
<pin name="BIOFF" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="in"/>
</symbol>
<symbol name="ADC0820">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="WR/RDY" function="dot"/>
<pin name="MODE" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="INT" direction="out" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="VREF-" direction="pas"/>
<pin name="VREF+" direction="pas"/>
<pin name="OFL" direction="out" function="dot"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="ICL7106">
<pin name="D1" direction="hiz"/>
<pin name="C1" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="F1" direction="hiz"/>
<pin name="G1" direction="hiz"/>
<pin name="E1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="C2" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="F2" direction="hiz"/>
<pin name="E2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="F3" direction="hiz"/>
<pin name="E3" direction="hiz"/>
<pin name="AB4" direction="hiz"/>
<pin name="G3" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="C3" direction="hiz"/>
<pin name="G2" direction="hiz"/>
<pin name="POL" direction="out"/>
<pin name="BP" direction="out"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="OSC3" direction="pas"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="COMM" direction="pwr"/>
<pin name="CREF+" direction="pas"/>
<pin name="CREF-" direction="pas"/>
<pin name="REF-LO" direction="in"/>
<pin name="REF-HI" direction="in"/>
<pin name="TEST" direction="pas"/>
<pin name="A/Z" direction="pas"/>
<pin name="BUFF" direction="pas"/>
<pin name="INT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="ICL7109">
<pin name="B1" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="B4" direction="hiz"/>
<pin name="B5" direction="hiz"/>
<pin name="B6" direction="hiz"/>
<pin name="B7" direction="hiz"/>
<pin name="B8" direction="hiz"/>
<pin name="B9" direction="hiz"/>
<pin name="B10" direction="hiz"/>
<pin name="B11" direction="hiz"/>
<pin name="B12" direction="hiz"/>
<pin name="STATUS" direction="out"/>
<pin name="POL" direction="out"/>
<pin name="OR" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="LBEN" function="dot"/>
<pin name="HBEN" function="dot"/>
<pin name="CE/LOAD"/>
<pin name="MODE" direction="in"/>
<pin name="OSC-IN" direction="in"/>
<pin name="OSC-OUT" direction="out"/>
<pin name="REF-OUT" direction="in"/>
<pin name="BOSC-OUT" direction="out"/>
<pin name="BUFFER" direction="out"/>
<pin name="R/H" direction="in"/>
<pin name="SEND" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="AZ" direction="pas"/>
<pin name="INT" direction="out"/>
<pin name="COMM" direction="pwr"/>
<pin name="IN-LO" direction="in"/>
<pin name="IN-HI" direction="in"/>
<pin name="REF-IN+" direction="in"/>
<pin name="REF-IN-" direction="in"/>
<pin name="REF-CAP+" direction="pas"/>
<pin name="REF-CAP-" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OSC-SEL" direction="in"/>
</symbol>
<symbol name="ICL7116">
<pin name="D1" direction="hiz"/>
<pin name="C1" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="F1" direction="hiz"/>
<pin name="G1" direction="hiz"/>
<pin name="E1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="C2" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="F2" direction="hiz"/>
<pin name="E2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="F3" direction="hiz"/>
<pin name="E3" direction="hiz"/>
<pin name="AB4" direction="hiz"/>
<pin name="G3" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="C3" direction="hiz"/>
<pin name="G2" direction="hiz"/>
<pin name="POL" direction="out"/>
<pin name="BP/GND"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="OSC3" direction="pas"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="COMM" direction="pwr"/>
<pin name="CREF+" direction="pas"/>
<pin name="CREF-" direction="pas"/>
<pin name="HOLD" direction="in"/>
<pin name="REF-HI" direction="in"/>
<pin name="TEST" direction="pas"/>
<pin name="A/Z" direction="pas"/>
<pin name="BUFF" direction="pas"/>
<pin name="INT" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="ICL7135">
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="ANA-COM" direction="pwr"/>
<pin name="INT-OUT" direction="out"/>
<pin name="BUFF-OUT" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="BUSY" direction="out"/>
<pin name="POL" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="AZ-IN" direction="in"/>
<pin name="REFCAP-" direction="pas"/>
<pin name="REFCAP+" direction="pas"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="DIGI-GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="STROBE" direction="out" function="dot"/>
<pin name="O/R" direction="out"/>
<pin name="U/R" direction="out"/>
<pin name="R/H" direction="in"/>
<pin name="CLK-IN" direction="in" function="clk"/>
</symbol>
<symbol name="MX565A">
<pin name="BIT1" direction="in"/>
<pin name="BIT2" direction="in"/>
<pin name="BIT3" direction="in"/>
<pin name="BIT4" direction="in"/>
<pin name="BIT5" direction="in"/>
<pin name="BIT6" direction="in"/>
<pin name="BIT7" direction="in"/>
<pin name="BIT8" direction="in"/>
<pin name="BIT9" direction="in"/>
<pin name="BIT10" direction="in"/>
<pin name="BIT11" direction="in"/>
<pin name="BIT12" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="REF-GND" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="REF-OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="REF-IN" direction="in"/>
<pin name="BIOFF-IN" direction="in"/>
<pin name="10V-SPAN" direction="pas"/>
<pin name="20V-SPAN" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="DAC-OUT" direction="out"/>
</symbol>
<symbol name="MX7224">
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="V-OUT" direction="out"/>
<pin name="V-REF" direction="in"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="RESET" direction="in" function="dot"/>
</symbol>
<symbol name="MX7225">
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="VREF-A" direction="in"/>
<pin name="VREF-B" direction="in"/>
<pin name="VREF-C" direction="in"/>
<pin name="VREF-D" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VOUT-D" direction="out"/>
<pin name="VOUT-C" direction="out"/>
<pin name="VOUT-B" direction="out"/>
<pin name="VOUT-A" direction="out"/>
</symbol>
<symbol name="MX7520">
<pin name="BIT1" direction="in"/>
<pin name="BIT2" direction="in"/>
<pin name="BIT3" direction="in"/>
<pin name="BIT4" direction="in"/>
<pin name="BIT5" direction="in"/>
<pin name="BIT6" direction="in"/>
<pin name="BIT7" direction="in"/>
<pin name="BIT8" direction="in"/>
<pin name="BIT9" direction="in"/>
<pin name="BIT10" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="MX7523">
<pin name="BIT1" direction="in"/>
<pin name="BIT2" direction="in"/>
<pin name="BIT3" direction="in"/>
<pin name="BIT4" direction="in"/>
<pin name="BIT5" direction="in"/>
<pin name="BIT6" direction="in"/>
<pin name="BIT7" direction="in"/>
<pin name="BIT8" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="MX7524">
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="MX7528">
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="VREF-A" direction="in"/>
<pin name="VREF-B" direction="in"/>
<pin name="RFB-A" direction="in"/>
<pin name="RFB-B" direction="in"/>
<pin name="DAA/DAB" direction="in"/>
<pin name="WR" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="OUT-A" direction="out"/>
<pin name="OUT-B" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MX7530">
<pin name="BIT1" direction="in"/>
<pin name="BIT4" direction="in"/>
<pin name="BIT2" direction="in"/>
<pin name="BIT3" direction="in"/>
<pin name="BIT5" direction="in"/>
<pin name="BIT6" direction="in"/>
<pin name="BIT7" direction="in"/>
<pin name="BIT8" direction="in"/>
<pin name="BIT9" direction="in"/>
<pin name="BIT10" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OUT-1" direction="out"/>
<pin name="OUT-2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MX7531">
<pin name="BIT1" direction="in"/>
<pin name="BIT4" direction="in"/>
<pin name="BIT2" direction="in"/>
<pin name="BIT3" direction="in"/>
<pin name="BIT5" direction="in"/>
<pin name="BIT6" direction="in"/>
<pin name="BIT7" direction="in"/>
<pin name="BIT8" direction="in"/>
<pin name="BIT9" direction="in"/>
<pin name="BIT10" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OUT-1" direction="out"/>
<pin name="OUT-2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="BIT11" direction="in"/>
<pin name="BIT12" direction="in"/>
</symbol>
<symbol name="MX7542">
<pin name="D0" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="DGND" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OUT-1" direction="out"/>
<pin name="OUT-2" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MX7543">
<pin name="STB1" direction="in"/>
<pin name="STB4" direction="in"/>
<pin name="STB2" direction="in"/>
<pin name="STB3" direction="in" function="dot"/>
<pin name="LD1" direction="in" function="dot"/>
<pin name="LD2" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="SRI" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="DGND" direction="pwr"/>
<pin name="RFB" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OUT-1" direction="out"/>
<pin name="OUT-2" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MX7545">
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="DB8" direction="in"/>
<pin name="DB9" direction="in"/>
<pin name="DB10" direction="in"/>
<pin name="DB11" direction="in"/>
<pin name="RFB" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
</symbol>
<symbol name="MAX670">
<pin name="VOUT-S1" direction="out"/>
<pin name="VOUT-S2" direction="out"/>
<pin name="OUT-F" direction="out"/>
<pin name="GND-F" direction="pwr"/>
<pin name="GND-S1" direction="pwr"/>
<pin name="GND-S2" direction="pwr"/>
<pin name="+15V" direction="pwr"/>
<pin name="OADJ" direction="in"/>
<pin name="FADJ" direction="in"/>
<pin name="FADJ@1" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="TP" direction="pas"/>
</symbol>
<symbol name="MAX672">
<pin name="VIN" direction="in"/>
<pin name="TRIM" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
<symbol name="MX580CS">
<pin name="+VS" direction="in"/>
<pin name="+2,5V" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="MX580H">
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
</symbol>
<symbol name="MX584N">
<pin name="10,0V" direction="out"/>
<pin name="5,0V" direction="out"/>
<pin name="2,5V" direction="out"/>
<pin name="COMMON" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="CAP" direction="pas"/>
<pin name="VBG" direction="pas"/>
<pin name="STROBE" direction="in"/>
</symbol>
<symbol name="MX2700">
<pin name="NC@7" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="FADJ" direction="in"/>
<pin name="FADJ@1" direction="in"/>
<pin name="TP" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="+15V" direction="pwr"/>
<pin name="10V-OUT" direction="out"/>
</symbol>
<symbol name="MX2701">
<pin name="NC@7" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="FADJ" direction="in"/>
<pin name="FADJ@1" direction="in"/>
<pin name="TP" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="-15V" direction="pwr"/>
<pin name="-10V-OUT" direction="out"/>
</symbol>
<symbol name="REF01">
<pin name="TRIM" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="V-IN" direction="pwr"/>
<pin name="V-OUT" direction="out"/>
</symbol>
<symbol name="REF02">
<pin name="TRIM" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="TEMP" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-IN" direction="pwr"/>
<pin name="V-OUT" direction="out"/>
</symbol>
<symbol name="MX536A">
<pin name="BUF-IN" direction="in"/>
<pin name="CAV" direction="pas"/>
<pin name="RL" direction="pas"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="BUF-OUT" direction="out"/>
<pin name="I-OUT" direction="out"/>
<pin name="DB" direction="out"/>
<pin name="COMM" direction="pwr"/>
<pin name="V-IN" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
</symbol>
<symbol name="MAX400">
<pin name="NC" direction="nc"/>
<pin name="VOS" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VOS@1" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX420">
<pin name="CRETN" direction="pas"/>
<pin name="CEXTA" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="CEXTB" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX421">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="CEXTA" direction="pas"/>
<pin name="CEXTB" direction="pas"/>
<pin name="CRETN" direction="pas"/>
<pin name="CLK-IN" direction="in"/>
<pin name="INT/EXT" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="CLK-OUT" direction="out"/>
<pin name="OUT-CLP" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OPAMP2NC">
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX450">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BIAS-ADJ" direction="in"/>
<pin name="FCOMP" direction="pas"/>
<pin name="FCOMP@1" direction="pas"/>
<pin name="FCOMP@2" direction="pas"/>
<pin name="FCOMP@3" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MAX453">
<pin name="A0" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="IN1" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX454">
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX455">
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="V-" direction="pwr"/>
<pin name="NC@3" direction="nc"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="OP2OFF+-">
<pin name="IQS" direction="pas"/>
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OP2OFF">
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
<pin name="IQS" direction="pas"/>
</symbol>
<symbol name="2V+V-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+@1" direction="pwr"/>
</symbol>
<symbol name="OPOFF+NC">
<pin name="NC" direction="pas"/>
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
</symbol>
<symbol name="OPOFF+-">
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="ICL7650">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="CEXTA" direction="pas"/>
<pin name="CEXTB" direction="pas"/>
<pin name="CRETN" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="ICL7650/">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="INT/EXT" direction="in"/>
<pin name="CLK-IN" direction="in" function="clk"/>
<pin name="CEXTA" direction="pas"/>
<pin name="CEXTB" direction="pas"/>
<pin name="CRETN" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="OUT-CLP" direction="out"/>
<pin name="CLK-OUT" direction="out" function="clk"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="MAX600">
<pin name="AC1" direction="in"/>
<pin name="AC2" direction="in"/>
<pin name="OUV" direction="in" function="dot"/>
<pin name="VSET" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="VSENSE" direction="in"/>
</symbol>
<symbol name="MAX601">
<pin name="AC1" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="OUV" direction="in" function="dot"/>
<pin name="VSENSE" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="RD" direction="pas"/>
</symbol>
<symbol name="MAX630">
<pin name="VFB" direction="in"/>
<pin name="LBR" direction="in"/>
<pin name="IC" direction="in"/>
<pin name="CX" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="LBD" direction="out"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX631">
<pin name="VFB" direction="in"/>
<pin name="LBI" direction="in"/>
<pin name="CP" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX634">
<pin name="VFB" direction="in"/>
<pin name="LBR" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="CX" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="LBD" direction="out"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX635">
<pin name="VFB" direction="in"/>
<pin name="LBI" direction="in"/>
<pin name="VREF" direction="out"/>
<pin name="-VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="LBO" direction="out"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX638">
<pin name="VFB" direction="in"/>
<pin name="LBI" direction="in"/>
<pin name="+VS" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX641">
<pin name="VFB" direction="in"/>
<pin name="LBI" direction="in"/>
<pin name="EXT" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX663">
<pin name="SENSE" direction="in"/>
<pin name="VIN(POS)" direction="pwr"/>
<pin name="VTC" direction="out"/>
<pin name="VOUT2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="VOUT1" direction="out"/>
<pin name="VSET" direction="in"/>
</symbol>
<symbol name="MAX664">
<pin name="SENSE" direction="in"/>
<pin name="VIN(NEG)" direction="pwr"/>
<pin name="SHDN@1" direction="in"/>
<pin name="VOUT2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="VOUT1" direction="out"/>
<pin name="VSET" direction="in"/>
</symbol>
<symbol name="MAX666">
<pin name="SENSE" direction="in"/>
<pin name="LBI" direction="in"/>
<pin name="VIN(POS)" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="VSET" direction="in"/>
</symbol>
<symbol name="VCC-GND">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX680">
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="V+" direction="out"/>
<pin name="V-" direction="out"/>
</symbol>
<symbol name="MAX690">
<pin name="WDI" direction="in"/>
<pin name="PFI" direction="in"/>
<pin name="RESET" direction="out" function="dot"/>
<pin name="VBATT" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="PFO" direction="out" function="dot"/>
</symbol>
<symbol name="MAX691">
<pin name="VBATT" direction="in"/>
<pin name="BATT-ON" direction="out"/>
<pin name="PFO" direction="out" function="dot"/>
<pin name="VOUT" direction="out"/>
<pin name="LOW-LINE" direction="out"/>
<pin name="OSC-IN" direction="pas"/>
<pin name="OSC-SEL" direction="pas"/>
<pin name="CE-OUT" direction="out"/>
<pin name="PFI" direction="in"/>
<pin name="WDI" direction="in"/>
<pin name="WDO" direction="out" function="dot"/>
<pin name="RESET" direction="out"/>
<pin name="CE-IN" direction="in"/>
<pin name="RESET@" direction="out" function="dot"/>
</symbol>
<symbol name="MAX696">
<pin name="VBATT" direction="in"/>
<pin name="BATT-ON" direction="out"/>
<pin name="PFO" direction="out" function="dot"/>
<pin name="VOUT" direction="out"/>
<pin name="LOW-LINE" direction="out"/>
<pin name="OSC-IN" direction="pas"/>
<pin name="OSC-SEL" direction="pas"/>
<pin name="LLIN" direction="in"/>
<pin name="PFI" direction="in"/>
<pin name="WDI" direction="in"/>
<pin name="WDO" direction="out" function="dot"/>
<pin name="RESET" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="RESET@" direction="out" function="dot"/>
</symbol>
<symbol name="MAX697">
<pin name="NC" direction="nc"/>
<pin name="OSC-IN" direction="pas"/>
<pin name="PFO" direction="out" function="dot"/>
<pin name="TEST" direction="pas"/>
<pin name="LOW-LINE" direction="out"/>
<pin name="LLIN" direction="in"/>
<pin name="OSC-SEL" direction="pas"/>
<pin name="CE-OUT" direction="out"/>
<pin name="PFI" direction="in"/>
<pin name="WDI" direction="in"/>
<pin name="WDO" direction="out" function="dot"/>
<pin name="RESET" direction="out"/>
<pin name="CE-IN" direction="in"/>
<pin name="RESET@" direction="out" function="dot"/>
</symbol>
<symbol name="MAX8211">
<pin name="THRESH" direction="in"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="HYSTER" direction="out"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="ICL7660">
<pin name="LV" direction="pas"/>
<pin name="CAP-" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OSC" direction="out"/>
<pin name="CAP+" direction="pas"/>
</symbol>
<symbol name="ICL7663">
<pin name="SHDN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="VTC" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="VSET" direction="in"/>
</symbol>
<symbol name="ICL7664">
<pin name="SHDN" direction="in" function="dot"/>
<pin name="SENSE" direction="in"/>
<pin name="SHDN@1" direction="in" function="dot"/>
<pin name="OUT1" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="VSET" direction="in"/>
</symbol>
<symbol name="ICL7665">
<pin name="HYST1" direction="in"/>
<pin name="SET1" direction="in"/>
<pin name="SET2" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="HYST2" direction="in"/>
</symbol>
<symbol name="MAX7231">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="BD0" direction="in"/>
<pin name="BD1" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="BD3" direction="in"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="VDISP" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="COM1" direction="out"/>
<pin name="COM2" direction="out"/>
<pin name="COM3" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="1X" direction="out"/>
<pin name="1Y" direction="out"/>
<pin name="1Z" direction="out"/>
<pin name="2X" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="3X" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="4X" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="4Z" direction="out"/>
<pin name="8Z" direction="out"/>
<pin name="8Y" direction="out"/>
<pin name="8X" direction="out"/>
<pin name="7Z" direction="out"/>
<pin name="7Y" direction="out"/>
<pin name="7X" direction="out"/>
<pin name="6Z" direction="out"/>
<pin name="6Y" direction="out"/>
<pin name="6X" direction="out"/>
<pin name="5Z" direction="out"/>
<pin name="5Y" direction="out"/>
<pin name="5X" direction="out"/>
</symbol>
<symbol name="MAX7232">
<pin name="CLK" direction="in" function="clk"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="DATA" direction="in"/>
<pin name="DATAACC" direction="out"/>
<pin name="10Z" direction="out"/>
<pin name="10Y" direction="out"/>
<pin name="10X" direction="out"/>
<pin name="9Z" direction="out"/>
<pin name="VDISP" direction="in"/>
<pin name="9X" direction="out"/>
<pin name="9Y" direction="out"/>
<pin name="COM1" direction="out"/>
<pin name="COM2" direction="out"/>
<pin name="COM3" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="1X" direction="out"/>
<pin name="1Y" direction="out"/>
<pin name="1Z" direction="out"/>
<pin name="2X" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="3X" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="4X" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="4Z" direction="out"/>
<pin name="8Z" direction="out"/>
<pin name="8Y" direction="out"/>
<pin name="8X" direction="out"/>
<pin name="7Z" direction="out"/>
<pin name="7Y" direction="out"/>
<pin name="7X" direction="out"/>
<pin name="6Z" direction="out"/>
<pin name="6Y" direction="out"/>
<pin name="6X" direction="out"/>
<pin name="5Z" direction="out"/>
<pin name="5Y" direction="out"/>
<pin name="5X" direction="out"/>
</symbol>
<symbol name="MAX7233">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="CS1" direction="in" function="dot"/>
<pin name="CS2" direction="in" function="dot"/>
<pin name="D3" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="VDISP" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="COM1" direction="out"/>
<pin name="COM2" direction="out"/>
<pin name="COM3" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="1U" direction="out"/>
<pin name="1V" direction="out"/>
<pin name="1W" direction="out"/>
<pin name="1X" direction="out"/>
<pin name="1Y" direction="out"/>
<pin name="1Z" direction="out"/>
<pin name="2U" direction="out"/>
<pin name="2V" direction="out"/>
<pin name="2W" direction="out"/>
<pin name="2X" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="4Z" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="4X" direction="out"/>
<pin name="4W" direction="out"/>
<pin name="4V" direction="out"/>
<pin name="4U" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3X" direction="out"/>
<pin name="3W" direction="out"/>
<pin name="3V" direction="out"/>
<pin name="3U" direction="out"/>
</symbol>
<symbol name="MAX7234">
<pin name="CLK" direction="in" function="clk"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="DATA" direction="in"/>
<pin name="DATAACC" direction="out"/>
<pin name="5Z" direction="out"/>
<pin name="5Y" direction="out"/>
<pin name="5X" direction="out"/>
<pin name="5W" direction="out"/>
<pin name="VDISP" direction="in"/>
<pin name="5U" direction="out"/>
<pin name="5V" direction="out"/>
<pin name="COM1" direction="out"/>
<pin name="COM2" direction="out"/>
<pin name="COM3" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="1U" direction="out"/>
<pin name="1V" direction="out"/>
<pin name="1W" direction="out"/>
<pin name="1X" direction="out"/>
<pin name="1Y" direction="out"/>
<pin name="1Z" direction="out"/>
<pin name="2U" direction="out"/>
<pin name="2V" direction="out"/>
<pin name="2W" direction="out"/>
<pin name="2X" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="2Z" direction="out"/>
<pin name="4Z" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="4X" direction="out"/>
<pin name="4W" direction="out"/>
<pin name="4V" direction="out"/>
<pin name="4U" direction="out"/>
<pin name="3Z" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3X" direction="out"/>
<pin name="3W" direction="out"/>
<pin name="3V" direction="out"/>
<pin name="3U" direction="out"/>
</symbol>
<symbol name="ICM7211">
<pin name="D1-IN" direction="in"/>
<pin name="D2-IN" direction="in"/>
<pin name="D3-IN" direction="in"/>
<pin name="G1" direction="out"/>
<pin name="F4" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="D4-IN" direction="in"/>
<pin name="E3" direction="out"/>
<pin name="E4" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="B0-IN" direction="in"/>
<pin name="B1-IN" direction="in"/>
<pin name="B2-IN" direction="in"/>
<pin name="B3-IN" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="BP"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="E2" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="C4" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="C2" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B3" direction="out"/>
</symbol>
<symbol name="ICM7211M">
<pin name="DIGSEL1" direction="in"/>
<pin name="DIGSEL2" direction="in"/>
<pin name="CS1" direction="in" function="dot"/>
<pin name="G1" direction="out"/>
<pin name="F4" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="CS2" direction="in" function="dot"/>
<pin name="E3" direction="out"/>
<pin name="E4" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="B0-IN" direction="in"/>
<pin name="B1-IN" direction="in"/>
<pin name="B2-IN" direction="in"/>
<pin name="B3-IN" direction="in"/>
<pin name="BP" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="E2" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="C4" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="C2" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B3" direction="out"/>
</symbol>
<symbol name="ICM7212M">
<pin name="DIGSEL1" direction="in"/>
<pin name="DIGSEL2" direction="in"/>
<pin name="CS1" direction="in" function="dot"/>
<pin name="G1" direction="out"/>
<pin name="F4" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="CS2" direction="in" function="dot"/>
<pin name="E3" direction="out"/>
<pin name="E4" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="B0-IN" direction="in"/>
<pin name="B1-IN" direction="in"/>
<pin name="B2-IN" direction="in"/>
<pin name="B3-IN" direction="in"/>
<pin name="BRT" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="E2" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="C4" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="C2" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B3" direction="out"/>
</symbol>
<symbol name="ICM7217A">
<pin name="D1" direction="out" function="dot"/>
<pin name="D2" direction="out" function="dot"/>
<pin name="D3" direction="out" function="dot"/>
<pin name="D4" direction="out" function="dot"/>
<pin name="C/B" direction="out"/>
<pin name="ZERO" direction="out" function="dot"/>
<pin name="EQUAL" direction="out" function="dot"/>
<pin name="SEG-G" direction="out"/>
<pin name="SEG-F" direction="out"/>
<pin name="SEG-E" direction="out"/>
<pin name="SEG-D" direction="out"/>
<pin name="BCD1S"/>
<pin name="BCD2S"/>
<pin name="BCD4S"/>
<pin name="BCD8S"/>
<pin name="SEG-C" direction="out"/>
<pin name="SEG-B" direction="out"/>
<pin name="SEG-A" direction="out"/>
<pin name="C-OUT" direction="out"/>
<pin name="U/D" direction="in"/>
<pin name="LR/OFF" direction="in"/>
<pin name="LC/OFF"/>
<pin name="SCAN" direction="pas"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="DISP-CON" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="STORE" direction="in" function="dot"/>
</symbol>
<symbol name="ICM7217">
<pin name="BCD1S"/>
<pin name="BCD2S"/>
<pin name="BCD4S"/>
<pin name="BCD8S"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="SEGG" direction="out"/>
<pin name="SEGF" direction="out"/>
<pin name="SEGE" direction="out"/>
<pin name="SEGD" direction="out"/>
<pin name="SEGC" direction="out"/>
<pin name="SEGB" direction="out"/>
<pin name="SEGA" direction="out"/>
<pin name="C/B" direction="out"/>
<pin name="ZERO" direction="out" function="dot"/>
<pin name="EQUAL" direction="out" function="dot"/>
<pin name="CO" direction="out"/>
<pin name="STORE" direction="in" function="dot"/>
<pin name="UP/DOWN" direction="in"/>
<pin name="LR/OFF" direction="in"/>
<pin name="LC/OFF"/>
<pin name="SCAN" direction="pas"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="DISP-CON" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ICM7218A">
<pin name="DIG-1" direction="out"/>
<pin name="DIG-2" direction="out"/>
<pin name="DIG-3" direction="out"/>
<pin name="DIG-4" direction="out"/>
<pin name="DIG-5" direction="out"/>
<pin name="DIG-6" direction="out"/>
<pin name="DIG-7" direction="out"/>
<pin name="DIG-8" direction="out"/>
<pin name="SEG-A" direction="out"/>
<pin name="SEG-B" direction="out"/>
<pin name="SEG-C" direction="out"/>
<pin name="SEG-F" direction="out"/>
<pin name="SEG-G" direction="out"/>
<pin name="SEG-D" direction="out"/>
<pin name="SEG-E" direction="out"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="ID2" direction="in"/>
<pin name="ID3" direction="in"/>
<pin name="ID4" direction="in"/>
<pin name="ID5" direction="in"/>
<pin name="ID6" direction="in"/>
<pin name="ID7" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="MODE" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DP" direction="out"/>
</symbol>
<symbol name="ICM7218C">
<pin name="DIG-1" direction="out"/>
<pin name="DIG-2" direction="out"/>
<pin name="DIG-3" direction="out"/>
<pin name="DIG-4" direction="out"/>
<pin name="DIG-5" direction="out"/>
<pin name="DIG-6" direction="out"/>
<pin name="DIG-7" direction="out"/>
<pin name="DIG-8" direction="out"/>
<pin name="SEG-A" direction="out"/>
<pin name="SEG-B" direction="out"/>
<pin name="SEG-C" direction="out"/>
<pin name="SEG-F" direction="out"/>
<pin name="SEG-G" direction="out"/>
<pin name="SEG-D" direction="out"/>
<pin name="SEG-E" direction="out"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="ID2" direction="in"/>
<pin name="ID3" direction="in"/>
<pin name="DA2" direction="in"/>
<pin name="DA0" direction="in"/>
<pin name="DA1" direction="in"/>
<pin name="ID7-DP" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DP" direction="out"/>
</symbol>
<symbol name="ICM7218D">
<pin name="DIG-1" direction="out"/>
<pin name="DIG-2" direction="out"/>
<pin name="DIG-3" direction="out"/>
<pin name="DIG-4" direction="out"/>
<pin name="DIG-5" direction="out"/>
<pin name="DIG-6" direction="out"/>
<pin name="DIG-7" direction="out"/>
<pin name="DIG-8" direction="out"/>
<pin name="SEG-A" direction="out"/>
<pin name="SEG-B" direction="out"/>
<pin name="SEG-C" direction="out"/>
<pin name="SEG-F" direction="out"/>
<pin name="SEG-G" direction="out"/>
<pin name="SEG-D" direction="out"/>
<pin name="SEG-E" direction="out"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="ID2" direction="in"/>
<pin name="ID3" direction="in"/>
<pin name="DA2" direction="in"/>
<pin name="DA0" direction="in"/>
<pin name="DA1" direction="in"/>
<pin name="ID7-DP" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DP" direction="out"/>
</symbol>
<symbol name="ICM7224">
<pin name="A2" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="C2" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="E2" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="E3" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="C4" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="E4" direction="out"/>
<pin name="F4" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="(BRT)BP"/>
<pin name="1/2-DIG" direction="out"/>
<pin name="LZB-OUT" direction="out"/>
<pin name="LZB-IN" direction="in"/>
<pin name="!CNTINH" direction="in"/>
<pin name="CNT" direction="in" function="dot"/>
<pin name="CARRY" direction="out" function="dot"/>
<pin name="STORE" direction="pas" function="dot"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OSC-GND" direction="pwr"/>
</symbol>
<symbol name="MM74C945">
<pin name="A2" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="C2" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="E2" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="E3" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="C4" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="E4" direction="out"/>
<pin name="F4" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="OSC" direction="pas"/>
<pin name="BP"/>
<pin name="LZB-OUT" direction="out"/>
<pin name="LZB-IN" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CARRY" direction="out"/>
<pin name="STORE" direction="in"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="UP/DOWN" direction="in"/>
</symbol>
<symbol name="ICM7242">
<pin name="RESET" direction="in"/>
<pin name="TRIG"/>
<pin name="128/256" direction="out"/>
<pin name="TB"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT-2" direction="out"/>
<pin name="RC" direction="pas"/>
</symbol>
<symbol name="ICM7240">
<pin name="1" direction="out"/>
<pin name="2" direction="out"/>
<pin name="4" direction="out"/>
<pin name="8" direction="out"/>
<pin name="16" direction="out"/>
<pin name="32" direction="out"/>
<pin name="64" direction="out"/>
<pin name="128" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="TRIGGER" direction="in"/>
<pin name="MOD" direction="in"/>
<pin name="RC" direction="pas"/>
<pin name="BU-RES" direction="in"/>
<pin name="TB"/>
</symbol>
<symbol name="ICM7556">
<pin name="DISCH2" direction="in"/>
<pin name="TRSH2" direction="in"/>
<pin name="RESET2" direction="in" function="dot"/>
<pin name="CV2" direction="pas"/>
<pin name="TRIGG2" function="dot"/>
<pin name="OUT2" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="DISCH1" direction="in"/>
<pin name="TRSH1" direction="in"/>
<pin name="RESET1" direction="in" function="dot"/>
<pin name="CV1" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="TRIGG1" function="dot"/>
</symbol>
<symbol name="ICM7555">
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DISCH" direction="in"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="CV" direction="pas"/>
<pin name="TRIG" function="dot"/>
<pin name="TRSH" direction="in"/>
</symbol>
<symbol name="ICL7126">
<pin name="D1" direction="hiz"/>
<pin name="C1" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="F1" direction="hiz"/>
<pin name="G1" direction="hiz"/>
<pin name="E1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="C2" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="F2" direction="hiz"/>
<pin name="E2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="F3" direction="hiz"/>
<pin name="E3" direction="hiz"/>
<pin name="AB4" direction="hiz"/>
<pin name="G3" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="C3" direction="hiz"/>
<pin name="G2" direction="hiz"/>
<pin name="POL" direction="out"/>
<pin name="BP"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="OSC3" direction="pas"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="COMM" direction="pwr"/>
<pin name="CREF+" direction="pas"/>
<pin name="CREF-" direction="pas"/>
<pin name="REF-LO" direction="in"/>
<pin name="REF-HI" direction="in"/>
<pin name="TEST" direction="pas"/>
<pin name="A/Z" direction="pas"/>
<pin name="BUFF" direction="pas"/>
<pin name="INT" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="ICL7129">
<pin name="BC2,LOBA" direction="out"/>
<pin name="FEDP1" direction="out"/>
<pin name="AGD1" direction="out"/>
<pin name="BC1,CONT" direction="out"/>
<pin name="FEDP2" direction="out"/>
<pin name="BC3,MIN" direction="out"/>
<pin name="AGD2" direction="out"/>
<pin name="AGD4" direction="out"/>
<pin name="BC4,BC5" direction="out"/>
<pin name="FEDP3" direction="out"/>
<pin name="AGD3" direction="out"/>
<pin name="BP1" direction="out"/>
<pin name="FEDP4" direction="out"/>
<pin name="CONT" direction="in"/>
<pin name="INT-OUT" direction="out"/>
<pin name="DP3/UR" direction="in"/>
<pin name="LAT/HOL" direction="in"/>
<pin name="VDISP" direction="in"/>
<pin name="DP4/OR" direction="in"/>
<pin name="BP3" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="BP2" direction="out"/>
<pin name="ANNDR" direction="out"/>
<pin name="DP1" direction="in"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="OSC3" direction="pas"/>
<pin name="IN-HI" direction="in"/>
<pin name="IN-LO" direction="in"/>
<pin name="COMM" direction="pwr"/>
<pin name="CREF+" direction="pas"/>
<pin name="CREF-" direction="pas"/>
<pin name="REF-LO" direction="in"/>
<pin name="REF-HI" direction="in"/>
<pin name="DP2" direction="in"/>
<pin name="RANGE" direction="pas"/>
<pin name="BUFF" direction="out"/>
<pin name="INT-IN" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX260">
<pin name="INA" direction="in"/>
<pin name="HPA" direction="out"/>
<pin name="HPB" direction="out"/>
<pin name="BPB" direction="out"/>
<pin name="BPA" direction="out"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="CLKA" direction="in" function="clk"/>
<pin name="CLKB" direction="in" function="clk"/>
<pin name="CLK-OUT" direction="out"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="OSC-OUT" direction="in"/>
<pin name="LPA" direction="out"/>
<pin name="LPB" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="INB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="MAX261">
<pin name="INA" direction="in"/>
<pin name="HPA" direction="out"/>
<pin name="HPB" direction="out"/>
<pin name="BPB" direction="out"/>
<pin name="BPA" direction="out"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="CLKA" direction="in" function="clk"/>
<pin name="CLKB" direction="in" function="clk"/>
<pin name="CLK-OUT" direction="out"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="OSC-OUT" direction="in"/>
<pin name="LPA" direction="out"/>
<pin name="LPB" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="INB" direction="in"/>
<pin name="OP-OUT" direction="out"/>
<pin name="OP-IN" direction="in"/>
</symbol>
<symbol name="MAX263">
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="LPA" direction="out"/>
<pin name="LPB" direction="out"/>
<pin name="BPA" direction="out"/>
<pin name="BPB" direction="out"/>
<pin name="N/HPA" direction="out"/>
<pin name="N/HPB" direction="out"/>
<pin name="Q0" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="M0" direction="in"/>
<pin name="M1" direction="in"/>
<pin name="F0" direction="in"/>
<pin name="F1" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="F3" direction="in"/>
<pin name="F4" direction="in"/>
<pin name="CLK-A" direction="in" function="clk"/>
<pin name="CLK-B" direction="in" function="clk"/>
<pin name="OSC-OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX267">
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="BPA" direction="out"/>
<pin name="BPB" direction="out"/>
<pin name="OP-OUT" direction="out"/>
<pin name="Q0" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="OP-IN" direction="in"/>
<pin name="F0" direction="in"/>
<pin name="F1" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="F3" direction="in"/>
<pin name="F4" direction="in"/>
<pin name="CLK-A" direction="in" function="clk"/>
<pin name="CLK-B" direction="in" function="clk"/>
<pin name="OSC-OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MF10">
<pin name="LPA" direction="out"/>
<pin name="BPA" direction="out"/>
<pin name="N/AP/HPA" direction="out"/>
<pin name="LPB" direction="out"/>
<pin name="BPB" direction="out"/>
<pin name="N/AP/HPB" direction="out"/>
<pin name="INVA" direction="in"/>
<pin name="INVB" direction="in"/>
<pin name="S1A" direction="in"/>
<pin name="S1B" direction="in"/>
<pin name="SA/B" direction="in"/>
<pin name="VA+" direction="pwr"/>
<pin name="VD-" direction="pwr"/>
<pin name="VA-" direction="pwr"/>
<pin name="VD+" direction="pwr"/>
<pin name="LSH" direction="in"/>
<pin name="CLK-A" direction="in" function="clk"/>
<pin name="CLK-B" direction="in" function="clk"/>
<pin name="50/100/C" direction="in"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="MAX310">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="S5" direction="pas"/>
<pin name="S6" direction="pas"/>
<pin name="S7" direction="pas"/>
<pin name="S8" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX311">
<pin name="S1A" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S3A" direction="pas"/>
<pin name="S4A" direction="pas"/>
<pin name="S1B" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="S3B" direction="pas"/>
<pin name="S4B" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="OUT-B" direction="pas"/>
<pin name="OUT-A" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX358">
<pin name="IN1" direction="pas"/>
<pin name="IN2" direction="pas"/>
<pin name="IN3" direction="pas"/>
<pin name="IN4" direction="pas"/>
<pin name="IN5" direction="pas"/>
<pin name="IN6" direction="pas"/>
<pin name="IN7" direction="pas"/>
<pin name="IN8" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX359">
<pin name="IN1A" direction="pas"/>
<pin name="IN2A" direction="pas"/>
<pin name="IN3A" direction="pas"/>
<pin name="IN4A" direction="pas"/>
<pin name="IN1B" direction="pas"/>
<pin name="IN2B" direction="pas"/>
<pin name="IN3B" direction="pas"/>
<pin name="IN4B" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="OUT-A" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="OUT-B" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="DG506A">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="S5" direction="pas"/>
<pin name="S6" direction="pas"/>
<pin name="S7" direction="pas"/>
<pin name="S8" direction="pas"/>
<pin name="S9" direction="pas"/>
<pin name="S10" direction="pas"/>
<pin name="S11" direction="pas"/>
<pin name="S12" direction="pas"/>
<pin name="S13" direction="pas"/>
<pin name="S14" direction="pas"/>
<pin name="S15" direction="pas"/>
<pin name="S16" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="D" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="DG507AC">
<pin name="S1A" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S3A" direction="pas"/>
<pin name="S4A" direction="pas"/>
<pin name="S5A" direction="pas"/>
<pin name="S6A" direction="pas"/>
<pin name="S7A" direction="pas"/>
<pin name="S8A" direction="pas"/>
<pin name="S1B" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="S3B" direction="pas"/>
<pin name="S4B" direction="pas"/>
<pin name="S5B" direction="pas"/>
<pin name="S6B" direction="pas"/>
<pin name="S7B" direction="pas"/>
<pin name="S8B" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="DB" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="DA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="DG508A">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="S5" direction="pas"/>
<pin name="S6" direction="pas"/>
<pin name="S7" direction="pas"/>
<pin name="S8" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="D" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="DG509A">
<pin name="S1A" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S3A" direction="pas"/>
<pin name="S4A" direction="pas"/>
<pin name="S1B" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="S3B" direction="pas"/>
<pin name="S4B" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="DB" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="DA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="DG201">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX333">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="MAX341">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX343">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="D4" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DG200">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="MAX232">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
</symbol>
<symbol name="MAX242">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="EN" direction="pas" function="dot"/>
<pin name="SHDN" direction="pas" function="dot"/>
</symbol>
<symbol name="MAX230">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="SHUTDOWN" direction="pas"/>
<pin name="T5OUT" direction="out"/>
<pin name="T5IN" direction="in"/>
</symbol>
<symbol name="MAX231">
<pin name="C+"/>
<pin name="C-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
</symbol>
<symbol name="MAX233">
<pin name="V-@2"/>
<pin name="V-@1"/>
<pin name="C1-"/>
<pin name="C1+"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="C2+@2"/>
<pin name="C2+@1"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="V+"/>
<pin name="C2-@2"/>
<pin name="C2-@1"/>
</symbol>
<symbol name="PWR2GND">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="MAX234">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
</symbol>
<symbol name="MAX235">
<pin name="EN" direction="pas" function="dot"/>
<pin name="T5IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="R3IN" direction="in"/>
<pin name="T5OUT" direction="out"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
<pin name="R5OUT" direction="out"/>
<pin name="R4OUT" direction="out"/>
<pin name="R3OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="R1IN" direction="in"/>
<pin name="SHDN" direction="pas"/>
<pin name="R5IN" direction="in"/>
<pin name="R4IN" direction="in"/>
</symbol>
<symbol name="MAX236">
<pin name="EN" direction="pas" function="dot"/>
<pin name="C2-"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="R3IN" direction="in"/>
<pin name="V+"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="R3OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="R1IN" direction="in"/>
<pin name="SHDN" direction="pas"/>
<pin name="C1+"/>
<pin name="V-"/>
</symbol>
<symbol name="MAX237">
<pin name="T5IN" direction="in"/>
<pin name="C2-"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="R3IN" direction="in"/>
<pin name="V+"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="R3OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="R1IN" direction="in"/>
<pin name="T5OUT" direction="out"/>
<pin name="C1+"/>
<pin name="V-"/>
</symbol>
<symbol name="MAX238">
<pin name="R4OUT" direction="out"/>
<pin name="C2-"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="R3IN" direction="in"/>
<pin name="V+"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="R3OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="R1IN" direction="in"/>
<pin name="R4IN" direction="in"/>
<pin name="C1+"/>
<pin name="V-"/>
</symbol>
<symbol name="MAX239">
<pin name="R4OUT" direction="out"/>
<pin name="C-"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="R5OUT" direction="out"/>
<pin name="R3IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="R5IN" direction="in"/>
<pin name="C+"/>
<pin name="R3OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="R1IN" direction="in"/>
<pin name="R4IN" direction="in"/>
<pin name="V-"/>
<pin name="EN" direction="pas" function="dot"/>
<pin name="NC" direction="nc"/>
<pin name="V+" direction="pas"/>
</symbol>
<symbol name="MAX243">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
</symbol>
<symbol name="MAX244">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="TA1OUT" direction="out"/>
<pin name="TA1IN" direction="in"/>
<pin name="TA2IN" direction="in"/>
<pin name="TA3OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="TB1OUT" direction="out"/>
<pin name="TB1IN" direction="in"/>
<pin name="TB2IN" direction="in"/>
<pin name="TB3OUT" direction="out"/>
<pin name="TA2OUT" direction="out"/>
<pin name="TA3IN" direction="in"/>
<pin name="TA4OUT" direction="out"/>
<pin name="TA4IN" direction="in"/>
<pin name="RA1IN" direction="in"/>
<pin name="RA1OUT" direction="out"/>
<pin name="RA2IN" direction="in"/>
<pin name="RA2OUT" direction="out"/>
<pin name="RA3IN" direction="in"/>
<pin name="RA3OUT" direction="out"/>
<pin name="RA4IN" direction="in"/>
<pin name="RA4OUT" direction="out"/>
<pin name="RA5IN" direction="in"/>
<pin name="RA5OUT" direction="out"/>
<pin name="RB5OUT" direction="out"/>
<pin name="RB5IN" direction="in"/>
<pin name="RB4OUT" direction="out"/>
<pin name="RB4IN" direction="in"/>
<pin name="RB3OUT" direction="out"/>
<pin name="RB3IN" direction="in"/>
<pin name="RB2OUT" direction="out"/>
<pin name="RB2IN" direction="in"/>
<pin name="RB1OUT" direction="out"/>
<pin name="RB1IN" direction="in"/>
<pin name="TB4IN" direction="in"/>
<pin name="TB4OUT" direction="out"/>
<pin name="TB3IN" direction="in"/>
<pin name="TB2OUT" direction="out"/>
</symbol>
<symbol name="MAX245">
<pin name="ENR" direction="pas" function="dot"/>
<pin name="TA1OUT" direction="out"/>
<pin name="TA1IN" direction="in"/>
<pin name="TA2IN" direction="in"/>
<pin name="TA3OUT" direction="out"/>
<pin name="ENT" direction="pas" function="dot"/>
<pin name="TB1OUT" direction="out"/>
<pin name="TB1IN" direction="in"/>
<pin name="TB2IN" direction="in"/>
<pin name="TB3OUT" direction="out"/>
<pin name="TA2OUT" direction="out"/>
<pin name="TA3IN" direction="in"/>
<pin name="TA4OUT" direction="out"/>
<pin name="TA4IN" direction="in"/>
<pin name="RA1IN" direction="in"/>
<pin name="RA1OUT" direction="out"/>
<pin name="RA2IN" direction="in"/>
<pin name="RA2OUT" direction="out"/>
<pin name="RA3IN" direction="in"/>
<pin name="RA3OUT" direction="out"/>
<pin name="RA4IN" direction="in"/>
<pin name="RA4OUT" direction="out"/>
<pin name="RA5IN" direction="in"/>
<pin name="RA5OUT" direction="out"/>
<pin name="RB5OUT" direction="out"/>
<pin name="RB5IN" direction="in"/>
<pin name="RB4OUT" direction="out"/>
<pin name="RB4IN" direction="in"/>
<pin name="RB3OUT" direction="out"/>
<pin name="RB3IN" direction="in"/>
<pin name="RB2OUT" direction="out"/>
<pin name="RB2IN" direction="in"/>
<pin name="RB1OUT" direction="out"/>
<pin name="RB1IN" direction="in"/>
<pin name="TB4IN" direction="in"/>
<pin name="TB4OUT" direction="out"/>
<pin name="TB3IN" direction="in"/>
<pin name="TB2OUT" direction="out"/>
</symbol>
<symbol name="MAX247">
<pin name="RB5OUT" direction="out"/>
<pin name="TA1OUT" direction="out"/>
<pin name="TA1IN" direction="in"/>
<pin name="TA2IN" direction="in"/>
<pin name="TA3OUT" direction="out"/>
<pin name="RB5IN" direction="in"/>
<pin name="TB1OUT" direction="out"/>
<pin name="TB1IN" direction="in"/>
<pin name="TB2IN" direction="in"/>
<pin name="TB3OUT" direction="out"/>
<pin name="TA2OUT" direction="out"/>
<pin name="TA3IN" direction="in"/>
<pin name="TA4OUT" direction="out"/>
<pin name="TA4IN" direction="in"/>
<pin name="RA1IN" direction="in"/>
<pin name="RA1OUT" direction="out"/>
<pin name="RA2IN" direction="in"/>
<pin name="RA2OUT" direction="out"/>
<pin name="RA3IN" direction="in"/>
<pin name="RA3OUT" direction="out"/>
<pin name="RA4IN" direction="in"/>
<pin name="RA4OUT" direction="out"/>
<pin name="ENRA" direction="pas" function="dot"/>
<pin name="ENRB" direction="pas" function="dot"/>
<pin name="RB4OUT" direction="out"/>
<pin name="RB4IN" direction="in"/>
<pin name="RB3OUT" direction="out"/>
<pin name="RB3IN" direction="in"/>
<pin name="RB2OUT" direction="out"/>
<pin name="RB2IN" direction="in"/>
<pin name="RB1OUT" direction="out"/>
<pin name="RB1IN" direction="in"/>
<pin name="TB4IN" direction="in"/>
<pin name="TB4OUT" direction="out"/>
<pin name="TB3IN" direction="in"/>
<pin name="TB2OUT" direction="out"/>
<pin name="ENTA" direction="pas" function="dot"/>
<pin name="ENTB" direction="pas" function="dot"/>
</symbol>
<symbol name="MAX246">
<pin name="ENA" direction="pas" function="dot"/>
<pin name="TA1OUT" direction="out"/>
<pin name="TA1IN" direction="in"/>
<pin name="TA2IN" direction="in"/>
<pin name="TA3OUT" direction="out"/>
<pin name="ENB" direction="pas" function="dot"/>
<pin name="TB1OUT" direction="out"/>
<pin name="TB1IN" direction="in"/>
<pin name="TB2IN" direction="in"/>
<pin name="TB3OUT" direction="out"/>
<pin name="TA2OUT" direction="out"/>
<pin name="TA3IN" direction="in"/>
<pin name="TA4OUT" direction="out"/>
<pin name="TA4IN" direction="in"/>
<pin name="RA1IN" direction="in"/>
<pin name="RA1OUT" direction="out"/>
<pin name="RA2IN" direction="in"/>
<pin name="RA2OUT" direction="out"/>
<pin name="RA3IN" direction="in"/>
<pin name="RA3OUT" direction="out"/>
<pin name="RA4IN" direction="in"/>
<pin name="RA4OUT" direction="out"/>
<pin name="RA5IN" direction="in"/>
<pin name="RA5OUT" direction="out"/>
<pin name="RB5OUT" direction="out"/>
<pin name="RB5IN" direction="in"/>
<pin name="RB4OUT" direction="out"/>
<pin name="RB4IN" direction="in"/>
<pin name="RB3OUT" direction="out"/>
<pin name="RB3IN" direction="in"/>
<pin name="RB2OUT" direction="out"/>
<pin name="RB2IN" direction="in"/>
<pin name="RB1OUT" direction="out"/>
<pin name="RB1IN" direction="in"/>
<pin name="TB4IN" direction="in"/>
<pin name="TB4OUT" direction="out"/>
<pin name="TB3IN" direction="in"/>
<pin name="TB2OUT" direction="out"/>
</symbol>
<symbol name="MAX248">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="TA1OUT" direction="out"/>
<pin name="TA1IN" direction="in"/>
<pin name="TA2IN" direction="in"/>
<pin name="TA3OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="TB1OUT" direction="out"/>
<pin name="TB1IN" direction="in"/>
<pin name="TB2IN" direction="in"/>
<pin name="TB3OUT" direction="out"/>
<pin name="TA2OUT" direction="out"/>
<pin name="TA3IN" direction="in"/>
<pin name="TA4OUT" direction="out"/>
<pin name="TA4IN" direction="in"/>
<pin name="RA1IN" direction="in"/>
<pin name="RA1OUT" direction="out"/>
<pin name="RA2IN" direction="in"/>
<pin name="RA2OUT" direction="out"/>
<pin name="RA3IN" direction="in"/>
<pin name="RA3OUT" direction="out"/>
<pin name="RA4IN" direction="in"/>
<pin name="RA4OUT" direction="out"/>
<pin name="ENRA" direction="pas" function="dot"/>
<pin name="ENTA" direction="pas" function="dot"/>
<pin name="ENTB" direction="pas" function="dot"/>
<pin name="ENRB" direction="pas" function="dot"/>
<pin name="RB4OUT" direction="out"/>
<pin name="RB4IN" direction="in"/>
<pin name="RB3OUT" direction="out"/>
<pin name="RB3IN" direction="in"/>
<pin name="RB2OUT" direction="out"/>
<pin name="RB2IN" direction="in"/>
<pin name="RB1OUT" direction="out"/>
<pin name="RB1IN" direction="in"/>
<pin name="TB4IN" direction="in"/>
<pin name="TB4OUT" direction="out"/>
<pin name="TB3IN" direction="in"/>
<pin name="TB2OUT" direction="out"/>
</symbol>
<symbol name="MAX249">
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="TA1OUT" direction="out"/>
<pin name="TA1IN" direction="in"/>
<pin name="TA2IN" direction="in"/>
<pin name="TA3OUT" direction="out"/>
<pin name="V+"/>
<pin name="V-"/>
<pin name="TB1OUT" direction="out"/>
<pin name="TB1IN" direction="in"/>
<pin name="TB2IN" direction="in"/>
<pin name="TB3OUT" direction="out"/>
<pin name="TA2OUT" direction="out"/>
<pin name="TA3IN" direction="in"/>
<pin name="RA5IN" direction="out"/>
<pin name="RA5OUT" direction="in"/>
<pin name="RA1IN" direction="in"/>
<pin name="RA1OUT" direction="out"/>
<pin name="RA2IN" direction="in"/>
<pin name="RA2OUT" direction="out"/>
<pin name="RA3IN" direction="in"/>
<pin name="RA3OUT" direction="out"/>
<pin name="RA4IN" direction="in"/>
<pin name="RA4OUT" direction="out"/>
<pin name="ENRA" direction="pas" function="dot"/>
<pin name="ENTA" direction="pas" function="dot"/>
<pin name="ENTB" direction="pas" function="dot"/>
<pin name="ENRB" direction="pas" function="dot"/>
<pin name="RB4OUT" direction="out"/>
<pin name="RB4IN" direction="in"/>
<pin name="RB3OUT" direction="out"/>
<pin name="RB3IN" direction="in"/>
<pin name="RB2OUT" direction="out"/>
<pin name="RB2IN" direction="in"/>
<pin name="RB1OUT" direction="out"/>
<pin name="RB1IN" direction="in"/>
<pin name="RB5OUT" direction="in"/>
<pin name="RB5IN" direction="out"/>
<pin name="TB3IN" direction="in"/>
<pin name="TB2OUT" direction="out"/>
</symbol>
<symbol name="MAX910">
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="RA" direction="pas"/>
<pin name="TH_OUT" direction="out"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="TH_CTRL" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="REFOUT" direction="out"/>
<pin name="REFIN" direction="in"/>
<pin name="CMP_OUT" direction="out"/>
<pin name="CMP_GND" direction="pwr"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="RB" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="LATCH" direction="pas"/>
</symbol>
<symbol name="MAX625">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="S1" direction="out"/>
<pin name="D2" direction="in"/>
<pin name="S2" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="S3" direction="out"/>
<pin name="D4" direction="in"/>
<pin name="S4" direction="out"/>
<pin name="PR" direction="out"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX639">
<pin name="V+" direction="pwr"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="LBI" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="LX" direction="out"/>
<pin name="VFB" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX665">
<pin name="FC" direction="pas"/>
<pin name="CAP+"/>
<pin name="GND" direction="pwr"/>
<pin name="CAP-"/>
<pin name="V+" direction="pwr"/>
<pin name="OSC" direction="out"/>
<pin name="LV" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX291">
<pin name="CLK" direction="in" function="clk"/>
<pin name="OPO" direction="out"/>
<pin name="OPI-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OPAMP1">
<pin name="CEXT2" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="CRET" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="CEXT1" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP2">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="ICM7212">
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="DI3" direction="in"/>
<pin name="DI4" direction="in"/>
<pin name="BD0" direction="in"/>
<pin name="BD1" direction="in"/>
<pin name="A1" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="G1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="C2" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="E2" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="G2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="E3" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="G3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="C4" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="E4" direction="out"/>
<pin name="F4" direction="out"/>
<pin name="G4" direction="out"/>
<pin name="BD2" direction="in"/>
<pin name="BD3" direction="in"/>
<pin name="BRT"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="MAX7219">
<pin name="DIG2" direction="out"/>
<pin name="DIG3" direction="out"/>
<pin name="DIG4" direction="out"/>
<pin name="DIG5" direction="out"/>
<pin name="DIG6" direction="out"/>
<pin name="DIG7" direction="out"/>
<pin name="SEGA" direction="out"/>
<pin name="SEGB" direction="out"/>
<pin name="SEGC" direction="out"/>
<pin name="SEGD" direction="out"/>
<pin name="SEGE" direction="out"/>
<pin name="SEGF" direction="out"/>
<pin name="SEGG" direction="out"/>
<pin name="SEGDP" direction="out"/>
<pin name="DIG1" direction="out"/>
<pin name="DIG0" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="LOAD" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="ISET" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="MAX151">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="REF-OUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="V-IN" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="DB8" direction="hiz"/>
<pin name="DB9" direction="hiz"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="TP" direction="in"/>
<pin name="DBX@1" direction="pas"/>
<pin name="DBX" direction="pas"/>
</symbol>
<symbol name="MAX764">
<pin name="SHDN" direction="in" function="dot"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="LX" direction="out"/>
<pin name="REF" direction="in"/>
<pin name="AV+" direction="pwr"/>
<pin name="OUT" direction="sup"/>
</symbol>
<symbol name="MAX471">
<pin name="BATT" direction="in"/>
<pin name="RS+" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="LOAD" direction="out"/>
<pin name="SIGN" direction="oc"/>
<pin name="RS-" direction="in"/>
<pin name="IOUT" direction="out"/>
</symbol>
<symbol name="OPUB">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX505">
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="VOUT-A" direction="out"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VOUT-B" direction="out"/>
<pin name="VOUT-C" direction="out"/>
<pin name="VOUT-D" direction="out"/>
<pin name="VREF-A" direction="in"/>
<pin name="VREF-B" direction="in"/>
<pin name="VREF-C" direction="in"/>
<pin name="VREF-D" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="OP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MAX326">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX328">
<pin name="S5" direction="pas"/>
<pin name="S6" direction="pas"/>
<pin name="S7" direction="pas"/>
<pin name="S8" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="MAX368">
<pin name="IN5" direction="pas"/>
<pin name="IN6" direction="pas"/>
<pin name="IN7" direction="pas"/>
<pin name="IN8" direction="pas"/>
<pin name="IN1" direction="pas"/>
<pin name="IN2" direction="pas"/>
<pin name="IN3" direction="pas"/>
<pin name="IN4" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="EN" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="RS" direction="in" function="dot"/>
</symbol>
<symbol name="MAX369">
<pin name="IN3A" direction="pas"/>
<pin name="IN3B" direction="pas"/>
<pin name="IN4A" direction="pas"/>
<pin name="IN4B" direction="pas"/>
<pin name="IN1A" direction="pas"/>
<pin name="IN1B" direction="pas"/>
<pin name="IN2A" direction="pas"/>
<pin name="IN2B" direction="pas"/>
<pin name="OUTA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="EN" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="RS" direction="in" function="dot"/>
<pin name="OUTB" direction="pas"/>
</symbol>
<symbol name="MAX329">
<pin name="S3A" direction="pas"/>
<pin name="S3B" direction="pas"/>
<pin name="S4A" direction="pas"/>
<pin name="S4B" direction="pas"/>
<pin name="S1A" direction="pas"/>
<pin name="S1B" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="OUTA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="OUTB" direction="pas"/>
</symbol>
<symbol name="MAX378">
<pin name="IN5" direction="pas"/>
<pin name="IN6" direction="pas"/>
<pin name="IN7" direction="pas"/>
<pin name="IN8" direction="pas"/>
<pin name="IN1" direction="pas"/>
<pin name="IN2" direction="pas"/>
<pin name="IN3" direction="pas"/>
<pin name="IN4" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="MAX379">
<pin name="IN3A" direction="pas"/>
<pin name="IN3B" direction="pas"/>
<pin name="IN4A" direction="pas"/>
<pin name="IN4B" direction="pas"/>
<pin name="IN1A" direction="pas"/>
<pin name="IN1B" direction="pas"/>
<pin name="IN2A" direction="pas"/>
<pin name="IN2B" direction="pas"/>
<pin name="OUTA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="OUTB" direction="pas"/>
</symbol>
<symbol name="MAX220">
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="C2-" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="C2+" direction="pas"/>
</symbol>
<symbol name="MAX222">
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="C2-" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="C2+" direction="pas"/>
<pin name="SHDN" direction="in" function="dot"/>
</symbol>
<symbol name="MAX250">
<pin name="R1DIN" direction="in"/>
<pin name="R2DIN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T1LDR" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="D2" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="T2LDR" direction="out"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="D1" direction="pas"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="SHDN" direction="in"/>
</symbol>
<symbol name="MAX251">
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T1DIN" direction="in"/>
<pin name="T2DIN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="ISO-GND" direction="pas"/>
<pin name="BYP" direction="pas"/>
<pin name="V+" direction="sup"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1LDR" direction="out"/>
<pin name="R2LDR" direction="out"/>
<pin name="RTRI" direction="in"/>
<pin name="AC" direction="pas"/>
<pin name="V-" direction="sup"/>
</symbol>
<symbol name="MAX252">
<pin name="R1DIN" direction="in"/>
<pin name="R2DIN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T1LDR" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="D2" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="T2LDR" direction="out"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="D1" direction="pas"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="SHDN" direction="in"/>
<pin name="T1LED" direction="pas"/>
<pin name="LEDCOM" direction="pas"/>
<pin name="T2LED" direction="pas"/>
<pin name="R1DET" direction="pas"/>
<pin name="DETCOM" direction="pas"/>
<pin name="R2DET" direction="pas"/>
<pin name="ISOGND" direction="pwr"/>
<pin name="T1DET" direction="pas"/>
<pin name="T2DET" direction="pas"/>
<pin name="IDCOM" direction="pas"/>
<pin name="R1LED" direction="pas"/>
<pin name="ILCOM" direction="pas"/>
<pin name="R2LED" direction="pas"/>
<pin name="T1DIN" direction="in"/>
<pin name="T2DIN" direction="in"/>
<pin name="R1LDR" direction="out"/>
<pin name="R2LDR" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="AC" direction="pas"/>
<pin name="V+" direction="sup"/>
<pin name="V+@1" direction="sup"/>
<pin name="BYP" direction="pas"/>
<pin name="V-" direction="sup"/>
</symbol>
<symbol name="MAX406">
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="BW" direction="pas"/>
</symbol>
<symbol name="MAX425">
<pin name="CLK" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="LG" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="AZ" direction="pas"/>
</symbol>
<symbol name="MAX620">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="C2-" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="OUT2" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="C2+" direction="pas"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="PR" direction="out"/>
<pin name="CE" direction="in" function="dot"/>
</symbol>
<symbol name="MAX622">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="C2-" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="C2+" direction="pas"/>
<pin name="PR" direction="out"/>
</symbol>
<symbol name="MAX623">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="PR" direction="out"/>
<pin name="VOUT@1" direction="out"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="MAX654">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="HPGND" direction="pas"/>
<pin name="LX1" direction="pas"/>
<pin name="CTL" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="LX2" direction="pas"/>
<pin name="PR" direction="out"/>
<pin name="VREF" direction="sup"/>
<pin name="V+" direction="sup"/>
<pin name="OUT" direction="sup"/>
<pin name="LBI" direction="in"/>
<pin name="HPGND@1" direction="pas"/>
</symbol>
<symbol name="MAX656">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LX1" direction="pas"/>
<pin name="CTL" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="PR" direction="out"/>
<pin name="VREF" direction="sup"/>
<pin name="V+" direction="sup"/>
<pin name="OUT" direction="sup"/>
<pin name="LBI" direction="in"/>
<pin name="D" direction="out"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="MAX660">
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="C+" direction="pas"/>
<pin name="FC" direction="in"/>
<pin name="C-" direction="pas"/>
<pin name="OSC" direction="out"/>
<pin name="OUT" direction="sup"/>
<pin name="LV" direction="pas"/>
</symbol>
<symbol name="MAX667">
<pin name="GND" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="LBO" direction="pas"/>
<pin name="OUT" direction="sup"/>
<pin name="DD" direction="pas"/>
<pin name="SHDN" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="LBI" direction="in"/>
</symbol>
<symbol name="MAX742">
<pin name="GND" direction="pwr"/>
<pin name="FB+" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="VREF" direction="sup"/>
<pin name="CC+" direction="pas"/>
<pin name="AV+" direction="in"/>
<pin name="12/15" direction="in"/>
<pin name="100/200" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="EXT-" direction="hiz"/>
<pin name="CC-" direction="pas"/>
<pin name="FB-" direction="in"/>
<pin name="CSL-" direction="in"/>
<pin name="CSH-" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="PDRV" direction="in"/>
<pin name="CSL+" direction="in"/>
<pin name="CSH+" direction="in"/>
<pin name="PUMP" direction="out"/>
<pin name="EXT+" direction="hiz"/>
</symbol>
<symbol name="MAX743">
<pin name="GND" direction="pwr"/>
<pin name="FB+" direction="in"/>
<pin name="SS" direction="pas"/>
<pin name="VREF" direction="sup"/>
<pin name="CC+" direction="pas"/>
<pin name="AV+" direction="in"/>
<pin name="12/15" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="LX-" direction="pas"/>
<pin name="CC-" direction="pas"/>
<pin name="FB-" direction="in"/>
<pin name="V+@1" direction="in"/>
<pin name="LX+" direction="pas"/>
<pin name="V+" direction="in"/>
<pin name="V+@3" direction="in"/>
<pin name="V+@2" direction="in"/>
</symbol>
<symbol name="MAX1232">
<pin name="GND" direction="pwr"/>
<pin name="PBRST" direction="in" function="dot"/>
<pin name="TD" direction="in"/>
<pin name="TOL" direction="in"/>
<pin name="RST" direction="out" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="RST@1" direction="out"/>
<pin name="ST" direction="in" function="dot"/>
</symbol>
<symbol name="MAX698">
<pin name="GND" direction="pwr"/>
<pin name="RST" direction="out" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="MAX699">
<pin name="GND" direction="pwr"/>
<pin name="RST" direction="out" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="WDI" direction="in"/>
</symbol>
<symbol name="MAX700">
<pin name="GND" direction="pwr"/>
<pin name="RST" direction="out" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="MR" direction="in"/>
<pin name="CTL" direction="in"/>
<pin name="HYST" direction="pas"/>
<pin name="RST@1" direction="out"/>
<pin name="SENSE" direction="in"/>
</symbol>
<symbol name="MAX701">
<pin name="GND" direction="pwr"/>
<pin name="RST" direction="out" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="MR" direction="in"/>
<pin name="RST@1" direction="out"/>
</symbol>
<symbol name="MAX702">
<pin name="GND" direction="pwr"/>
<pin name="RST" direction="out" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="MR" direction="in"/>
</symbol>
<symbol name="MAX270">
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="OPOUT" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="OPIN" direction="in"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
</symbol>
<symbol name="MAX271">
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="D0" direction="in"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="T/HOUT" direction="out"/>
<pin name="MODE" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="T/H" direction="in"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="T/HEN" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="T/HA/B" direction="in"/>
</symbol>
<symbol name="MAX280">
<pin name="AGND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="BOUT" direction="out"/>
<pin name="DIR" direction="in"/>
<pin name="OUT" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="COSC" direction="in"/>
</symbol>
<symbol name="MAX171">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CK+" direction="pas"/>
<pin name="I_DGND@" direction="pas"/>
<pin name="CK-" direction="pas"/>
<pin name="S-" direction="pas"/>
<pin name="S+" direction="pas"/>
<pin name="I_V+" direction="in"/>
<pin name="REF" direction="sup"/>
<pin name="I_AGND" direction="pas"/>
<pin name="AIN" direction="in"/>
<pin name="I_DGND" direction="pas"/>
<pin name="I_V-" direction="in"/>
<pin name="DATA" direction="out"/>
<pin name="TP" direction="in"/>
</symbol>
<symbol name="MAX174">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="REFOUT" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="REFIN" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="12/8" direction="in"/>
<pin name="R/C" direction="in"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="VL+" direction="pwr"/>
<pin name="STS" direction="out"/>
<pin name="BIPOFF" direction="in"/>
<pin name="10VIN" direction="in"/>
<pin name="20VIN" direction="in"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
</symbol>
<symbol name="MAX178">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="REFOUT" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="REFIN" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="CAZ" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="VDD" direction="pwr"/>
<pin name="BYSL" direction="in"/>
<pin name="AIN" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="MAX180">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="REFOUT" direction="sup"/>
<pin name="VSS" direction="pwr"/>
<pin name="REFIN" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DIFF" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="OFFADJ" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="REFADJ" direction="in"/>
<pin name="CLKIN" direction="in" function="clk"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="BIP" direction="in"/>
<pin name="HBEN" direction="in"/>
</symbol>
<symbol name="MAX182">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="REFOUT" direction="sup"/>
<pin name="VSS" direction="pwr"/>
<pin name="REFIN" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="BYSL" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CAZ" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="MAX183">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="CLKOUT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="AIN2" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AIN1" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="VREF" direction="in"/>
<pin name="CLKIN" direction="in" function="clk"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
</symbol>
<symbol name="MAX404">
<pin name="VT1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VT2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX405">
<pin name="VC+" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="VC-" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NULL" direction="pas"/>
</symbol>
<symbol name="PWR1">
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MAX900">
<pin name="LATCH" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MAX500">
<pin name="AGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUTC" direction="sup"/>
<pin name="SDA" direction="in"/>
<pin name="OUTD" direction="sup"/>
<pin name="OUTB" direction="sup"/>
<pin name="OUTA" direction="sup"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="REFA/B" direction="in"/>
<pin name="REFD" direction="in"/>
<pin name="REFC" direction="in"/>
<pin name="LOAD" direction="in" function="dot"/>
<pin name="SRO" direction="out"/>
<pin name="SCL" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MAX516">
<pin name="VDD" direction="pwr"/>
<pin name="C2" direction="out"/>
<pin name="C3" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="C0" direction="out"/>
<pin name="D0" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="REF" direction="in"/>
</symbol>
<symbol name="MAX543">
<pin name="GND" direction="pwr"/>
<pin name="RFB" direction="in"/>
<pin name="IOUT" direction="out"/>
<pin name="LOAD" direction="in" function="dot"/>
<pin name="VREF" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="SRI" direction="in"/>
</symbol>
<symbol name="DG401">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
</symbol>
<symbol name="DG403">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="D4" direction="pas"/>
<pin name="S4" direction="pas"/>
</symbol>
<symbol name="DG406">
<pin name="S5" direction="pas"/>
<pin name="S6" direction="pas"/>
<pin name="S7" direction="pas"/>
<pin name="S8" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="S9" direction="pas"/>
<pin name="S10" direction="pas"/>
<pin name="S11" direction="pas"/>
<pin name="S12" direction="pas"/>
<pin name="S13" direction="pas"/>
<pin name="S14" direction="pas"/>
<pin name="S15" direction="pas"/>
<pin name="S16" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="DG407">
<pin name="S5A" direction="pas"/>
<pin name="S6A" direction="pas"/>
<pin name="S7A" direction="pas"/>
<pin name="S8A" direction="pas"/>
<pin name="S1A" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S3A" direction="pas"/>
<pin name="S4A" direction="pas"/>
<pin name="DA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="S1B" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="S3B" direction="pas"/>
<pin name="S4B" direction="pas"/>
<pin name="S5B" direction="pas"/>
<pin name="S6B" direction="pas"/>
<pin name="S7B" direction="pas"/>
<pin name="S8B" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="DB" direction="pas"/>
</symbol>
<symbol name="DG408">
<pin name="S5" direction="pas"/>
<pin name="S6" direction="pas"/>
<pin name="S7" direction="pas"/>
<pin name="S8" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="DG409">
<pin name="S1B" direction="pas"/>
<pin name="S2B" direction="pas"/>
<pin name="S3B" direction="pas"/>
<pin name="S4B" direction="pas"/>
<pin name="S1A" direction="pas"/>
<pin name="S2A" direction="pas"/>
<pin name="S3A" direction="pas"/>
<pin name="S4A" direction="pas"/>
<pin name="DA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="DB" direction="pas"/>
</symbol>
<symbol name="DG411">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="D4" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
</symbol>
<symbol name="DG417">
<pin name="IN1" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
</symbol>
<symbol name="DG419">
<pin name="IN1" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="DG441">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S3" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="D4" direction="pas"/>
<pin name="S4" direction="pas"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
</symbol>
<symbol name="MAX905">
<pin name="CLK@" direction="in" function="clk"/>
<pin name="CLK" direction="in" function="dotclk"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT@" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="VEES" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="MAX906">
<pin name="CLK@" direction="in" function="clk"/>
<pin name="CLK" direction="in" function="dotclk"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="QA@" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="QA" direction="out" function="dot"/>
<pin name="VEES" direction="pwr"/>
<pin name="VEEA" direction="pwr"/>
<pin name="QB" direction="out" function="dot"/>
<pin name="QB@" direction="out"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="VEEB" direction="pwr"/>
</symbol>
<symbol name="MAX911">
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="RA" direction="pas"/>
<pin name="TH_OUT" direction="out"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="TH_CTRL" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="REFOUT" direction="out"/>
<pin name="REFIN" direction="in"/>
<pin name="Q_OUT" direction="out" function="dot"/>
<pin name="CMP_GND" direction="pwr"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="RB" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LATCH" direction="pas"/>
<pin name="Q_OUT@" direction="out"/>
</symbol>
<symbol name="MAX662">
<pin name="SHDN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VOUT" direction="sup"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
</symbol>
<symbol name="MAX714">
<pin name="RS_O" direction="out" function="dot"/>
<pin name="ON" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LBO" direction="out"/>
<pin name="BAT" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="S1" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="S2" direction="in"/>
<pin name="B2" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="S6" direction="in"/>
<pin name="U6" direction="out"/>
<pin name="E6" direction="pas"/>
<pin name="B6N" direction="out"/>
</symbol>
<symbol name="MAX715">
<pin name="RS_O" direction="out" function="dot"/>
<pin name="ON" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LBO" direction="out"/>
<pin name="BAT" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="S1" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="S2" direction="in"/>
<pin name="B2" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="S6" direction="in"/>
<pin name="U6" direction="out"/>
<pin name="E6" direction="pas"/>
<pin name="B7" direction="out"/>
<pin name="S3" direction="in"/>
<pin name="B3" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="S5" direction="in"/>
<pin name="S7" direction="in"/>
<pin name="E5" direction="pas"/>
<pin name="E3" direction="pas"/>
<pin name="E7" direction="pas"/>
</symbol>
<symbol name="MAX716">
<pin name="RS_O" direction="out" function="dot"/>
<pin name="ON" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LBO" direction="out"/>
<pin name="BAT" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="S1" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="S2" direction="in"/>
<pin name="B2" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="S6" direction="in"/>
<pin name="U6" direction="out"/>
<pin name="E6" direction="pas"/>
<pin name="B7" direction="out"/>
<pin name="S3" direction="in"/>
<pin name="S4" direction="in"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="S5" direction="in"/>
<pin name="S7" direction="in"/>
<pin name="E5" direction="pas"/>
<pin name="E4" direction="pas"/>
<pin name="E3" direction="pas"/>
<pin name="E7" direction="pas"/>
</symbol>
<symbol name="MAX722">
<pin name="VREF" direction="out"/>
<pin name="3/5" direction="in"/>
<pin name="NEGON" direction="in"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="CS+" direction="in"/>
<pin name="FBN" direction="in"/>
<pin name="FB3" direction="in"/>
<pin name="LIN" direction="out"/>
<pin name="DLOW" direction="out"/>
<pin name="DHI" direction="out"/>
<pin name="PFO" direction="out" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="CS-" direction="in"/>
<pin name="LX3" direction="out"/>
</symbol>
<symbol name="MAX730">
<pin name="VREF" direction="out"/>
<pin name="CC" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX736">
<pin name="VREF" direction="out"/>
<pin name="CC" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="LX" direction="out"/>
<pin name="DRV-" direction="in"/>
<pin name="LX@" direction="out"/>
<pin name="V+@" direction="pwr"/>
<pin name="V+@1" direction="pwr"/>
</symbol>
<symbol name="MAX741">
<pin name="VREF" direction="out"/>
<pin name="SLOPE" direction="pas"/>
<pin name="VSEL" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="SYNC" direction="pas"/>
<pin name="P/Z/N" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="UVLO" direction="out"/>
<pin name="SS" direction="in"/>
<pin name="EAO" direction="out"/>
<pin name="EAIN" direction="in"/>
<pin name="DUTY" direction="in"/>
<pin name="P/N" direction="in"/>
<pin name="CSA" direction="in"/>
<pin name="CSB" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="DRV-" direction="out"/>
</symbol>
<symbol name="MAX705">
<pin name="PFO" direction="out"/>
<pin name="PFI" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="WDO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="WDI" direction="in"/>
<pin name="RESET" direction="out"/>
</symbol>
<symbol name="MAX707">
<pin name="PFO" direction="out" function="dot"/>
<pin name="PFI" direction="in"/>
<pin name="MR" direction="in" function="dot"/>
<pin name="RESET@" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="out" function="dot"/>
</symbol>
<symbol name="MAX274">
<pin name="INA" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="BPOA" direction="out"/>
<pin name="V-" direction="pwr"/>
<pin name="LPIA" direction="in"/>
<pin name="BPIA" direction="in"/>
<pin name="LPOA" direction="out"/>
<pin name="INB" direction="in"/>
<pin name="BPOB" direction="out"/>
<pin name="LPIB" direction="in"/>
<pin name="BPIB" direction="in"/>
<pin name="LPOB" direction="out"/>
<pin name="INC" direction="out"/>
<pin name="BPOC" direction="in"/>
<pin name="LPOC" direction="out"/>
<pin name="LPIC" direction="in"/>
<pin name="BPIC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="BPOD" direction="out"/>
<pin name="LPID" direction="in"/>
<pin name="BPID" direction="in"/>
<pin name="LPOD" direction="out"/>
<pin name="FC" direction="pas"/>
</symbol>
<symbol name="MAX275">
<pin name="INA" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="BPOA" direction="out"/>
<pin name="V-" direction="pwr"/>
<pin name="LPIA" direction="in"/>
<pin name="BPIA" direction="in"/>
<pin name="LPOA" direction="out"/>
<pin name="INB" direction="in"/>
<pin name="BPOB" direction="out"/>
<pin name="LPIB" direction="in"/>
<pin name="BPIB" direction="in"/>
<pin name="LPOB" direction="out"/>
<pin name="FCB" direction="pas"/>
<pin name="FCA" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@" direction="pwr"/>
</symbol>
<symbol name="MAX120">
<pin name="AIN" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="CONVST" direction="in" function="dot"/>
<pin name="CLKIN" direction="in"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="VREF" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="INT/BU" direction="out" function="dot"/>
</symbol>
<symbol name="MAX132">
<pin name="DIN" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="SCLK" direction="in" function="clk"/>
<pin name="P1" direction="out"/>
<pin name="P0" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="P2" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="CREF-" direction="pas"/>
<pin name="CREF+" direction="pas"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="P3" direction="out"/>
<pin name="BUFOUT" direction="out"/>
<pin name="INTOUT" direction="out"/>
<pin name="INLO" direction="in"/>
<pin name="INHI" direction="in"/>
<pin name="EOC" direction="out"/>
<pin name="REF+" direction="in"/>
<pin name="REF-" direction="in"/>
<pin name="INTIN" direction="in"/>
</symbol>
<symbol name="MAX135">
<pin name="DGND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="CREF-" direction="pas"/>
<pin name="CREF+" direction="pas"/>
<pin name="OSC1" direction="pas"/>
<pin name="OSC2" direction="pas"/>
<pin name="D4" direction="out"/>
<pin name="BUFOUT" direction="out"/>
<pin name="INTOUT" direction="out"/>
<pin name="INLO" direction="in"/>
<pin name="INHI" direction="in"/>
<pin name="EOC" direction="out"/>
<pin name="REF+" direction="in"/>
<pin name="REF-" direction="in"/>
<pin name="INTIN" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="AGND@" direction="pwr"/>
</symbol>
<symbol name="MAX155">
<pin name="DGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="D2/A2" direction="out"/>
<pin name="D1/A1" direction="out"/>
<pin name="D0/A0" direction="out"/>
<pin name="D3/PD" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="D4/INH" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="REFIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="D5/BIP" direction="out"/>
<pin name="D6/DIFF" direction="out"/>
<pin name="D7/ALL" direction="out"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="MAX156">
<pin name="DGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="D2" direction="out"/>
<pin name="D1/A1" direction="out"/>
<pin name="D0/A0" direction="out"/>
<pin name="D3/PD" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="D4/INH" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="REFIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="D5/BIP" direction="out"/>
<pin name="D6/DIFF" direction="out"/>
<pin name="D7/ALL" direction="out"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="MAX165">
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB0/LSB" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="AGND" direction="pwr"/>
<pin name="DB4" direction="hiz"/>
<pin name="REFOUT" direction="out"/>
<pin name="AIN" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="REFIN" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7/MSB" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="MAX166">
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="D2" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D0/LSB" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="AGND" direction="pwr"/>
<pin name="D4" direction="hiz"/>
<pin name="REFOUT" direction="out"/>
<pin name="AIN-" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="REFIN" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7/MSB" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="MODE" direction="in" function="clk"/>
<pin name="AIN+" direction="in"/>
</symbol>
<symbol name="MAX190">
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="D2/D10" direction="hiz"/>
<pin name="D1/D9" direction="hiz"/>
<pin name="D0/D8" direction="hiz"/>
<pin name="D3/D11" direction="hiz"/>
<pin name="AGND" direction="pwr"/>
<pin name="D4" direction="hiz"/>
<pin name="VREF" direction="out"/>
<pin name="AIN-" direction="in"/>
<pin name="BUSY" direction="out" function="dot"/>
<pin name="REFADJ" direction="in"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="D5/SSTB" direction="hiz"/>
<pin name="D6/SCLK" direction="hiz"/>
<pin name="D7/SDATA" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="BIP" direction="in"/>
<pin name="HBEN" direction="in"/>
<pin name="PAR" direction="in"/>
<pin name="AIN+" direction="in"/>
<pin name="AGND@" direction="pwr"/>
<pin name="PD" direction="in"/>
</symbol>
<symbol name="MAX440">
<pin name="GND@" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="COMP" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VNS" direction="pas"/>
<pin name="IN0" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="LEV/ED" direction="in"/>
<pin name="V+@" direction="pwr"/>
<pin name="V+@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="V-@1" direction="pwr"/>
<pin name="V-@" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="LATCH" direction="in"/>
</symbol>
<symbol name="MAX441">
<pin name="GND@" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="COMP" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VNS" direction="pas"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="LEV/ED" direction="in"/>
<pin name="V+@" direction="pwr"/>
<pin name="V-@" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="LATCH" direction="in"/>
</symbol>
<symbol name="MAX442">
<pin name="V+" direction="pwr"/>
<pin name="IN-" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX456">
<pin name="AGND@" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="OUT0" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="IN0" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="SER/PAR" direction="in"/>
<pin name="V+@" direction="pwr"/>
<pin name="V+@1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="V-@" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="LATCH" direction="in"/>
<pin name="DGND@" direction="pwr"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="EDGE/LEV" direction="in"/>
<pin name="CE@" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="LOAD" direction="in"/>
<pin name="A0" direction="out"/>
<pin name="D0/SIN" direction="in"/>
<pin name="D1/SOUT" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
</symbol>
<symbol name="MAX502">
<pin name="VDD" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="RA" direction="pas"/>
<pin name="D0" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="VSS" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="RB" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="RFB" direction="pas"/>
</symbol>
<symbol name="MAX501">
<pin name="VDD" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="RA" direction="pas"/>
<pin name="D0/D8" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D1/D9" direction="in"/>
<pin name="D2/D10" direction="in"/>
<pin name="D3/D11" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="VSS" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="RB" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="RFB" direction="pas"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="SET" direction="in" function="dot"/>
<pin name="CSLSB" direction="in" function="dot"/>
<pin name="CSMSB" direction="in" function="dot"/>
</symbol>
<symbol name="MAX506">
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="VOUT-A" direction="out"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VOUT-B" direction="out"/>
<pin name="VOUT-C" direction="out"/>
<pin name="VOUT-D" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MAX507">
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="VOUT" direction="out"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="REF-O" direction="out"/>
<pin name="ROFS" direction="pas"/>
<pin name="RFB" direction="pas"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CS" direction="in" function="dot"/>
</symbol>
<symbol name="MAX508">
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D0/D8" direction="in"/>
<pin name="D1/D9" direction="in"/>
<pin name="D2/D10" direction="in"/>
<pin name="D3/D11" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="VOUT" direction="out"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="REF-O" direction="out"/>
<pin name="ROFS" direction="pas"/>
<pin name="RFB" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="CSMSB" direction="in" function="dot"/>
<pin name="CSLSB" direction="in" function="dot"/>
</symbol>
<symbol name="MAX514">
<pin name="SRIC" direction="in"/>
<pin name="LOADC" direction="in" function="dot"/>
<pin name="SRIA" direction="in"/>
<pin name="SRIB" direction="in"/>
<pin name="LOADB" direction="in" function="dot"/>
<pin name="SRID" direction="in"/>
<pin name="LOADA" direction="in" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="IOUTB" direction="out"/>
<pin name="RFBB" direction="pas"/>
<pin name="RFBA" direction="pas"/>
<pin name="LOADD" direction="in" function="dot"/>
<pin name="VREFA" direction="in"/>
<pin name="IOUTA" direction="out"/>
<pin name="VREFB" direction="in"/>
<pin name="VREFC" direction="in"/>
<pin name="VREFD" direction="in"/>
<pin name="CLK@" direction="pas" function="clk"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="RFBC" direction="pas"/>
<pin name="IOUTC" direction="out"/>
<pin name="RFBD" direction="pas"/>
<pin name="IOUTD" direction="out"/>
</symbol>
<symbol name="MAX514SO">
<pin name="SRIC" direction="in"/>
<pin name="CLKC" direction="in"/>
<pin name="LOADC" direction="in" function="dot"/>
<pin name="SRIA" direction="in"/>
<pin name="CLKA" direction="in"/>
<pin name="SRIB" direction="in"/>
<pin name="CLKB" direction="in"/>
<pin name="LOADB" direction="in" function="dot"/>
<pin name="SRID" direction="in"/>
<pin name="LOADA" direction="in" function="dot"/>
<pin name="IOUTA" direction="out" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="IOUTB@" direction="out"/>
<pin name="RFBB" direction="pas"/>
<pin name="RFBA" direction="pas"/>
<pin name="CLKD" direction="in"/>
<pin name="LOADD" direction="in" function="dot"/>
<pin name="VREFA" direction="in"/>
<pin name="IOUTA@" direction="out"/>
<pin name="IOUTB" direction="out" function="dot"/>
<pin name="VREFB" direction="in"/>
<pin name="VREFC" direction="in"/>
<pin name="VREFD" direction="in"/>
<pin name="RFBC" direction="pas"/>
<pin name="IOUTC" direction="out" function="dot"/>
<pin name="IOUTC@" direction="out"/>
<pin name="RFBD" direction="pas"/>
<pin name="IOUTD" direction="out" function="dot"/>
<pin name="IOUTD@" direction="out"/>
</symbol>
<symbol name="MAX526">
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D0/D8" direction="in"/>
<pin name="D1/D9" direction="in"/>
<pin name="D2/D10" direction="in"/>
<pin name="D3/D11" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="VOUTA" direction="out"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VOUTB" direction="out"/>
<pin name="VOUTC" direction="out"/>
<pin name="VOUTD" direction="out"/>
<pin name="VREFAB" direction="in"/>
<pin name="VREFCD" direction="in"/>
<pin name="CSLSB" direction="in" function="dot"/>
<pin name="CSMSB" direction="in" function="dot"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MAX528">
<pin name="CLK" direction="in" function="clk"/>
<pin name="DIN" direction="in"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="OUT0" direction="out"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="REFL1" direction="in"/>
<pin name="REFH1" direction="in"/>
<pin name="REFL2" direction="in"/>
<pin name="REFH2" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="MAX872">
<pin name="VIN" direction="in"/>
<pin name="TRIM" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="COMP" direction="pas"/>
<pin name="TEMP" direction="out"/>
</symbol>
<symbol name="MAX200">
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="C2-" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="T2OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
<pin name="T5OUT" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="C2+" direction="pas"/>
<pin name="T3OUT" direction="out"/>
<pin name="T5IN" direction="in"/>
<pin name="SHDN" direction="in"/>
</symbol>
<symbol name="MAX201">
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="C-" direction="pas"/>
<pin name="C+" direction="pas"/>
<pin name="T2OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="R1OUT" direction="out"/>
</symbol>
<symbol name="MAX202">
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="C1-" direction="pas"/>
<pin name="C1+" direction="pas"/>
<pin name="T2OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="R1OUT" direction="out"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
</symbol>
<symbol name="MAX306">
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="NO5" direction="pas"/>
<pin name="NO6" direction="pas"/>
<pin name="NO7" direction="pas"/>
<pin name="NO8" direction="pas"/>
<pin name="NO9" direction="pas"/>
<pin name="NO10" direction="pas"/>
<pin name="NO11" direction="pas"/>
<pin name="NO12" direction="pas"/>
<pin name="NO13" direction="pas"/>
<pin name="NO14" direction="pas"/>
<pin name="NO15" direction="pas"/>
<pin name="NO16" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
</symbol>
<symbol name="MAX307">
<pin name="NO1A" direction="pas"/>
<pin name="NO2A" direction="pas"/>
<pin name="NO3A" direction="pas"/>
<pin name="NO4A" direction="pas"/>
<pin name="NO5A" direction="pas"/>
<pin name="NO6A" direction="pas"/>
<pin name="NO7A" direction="pas"/>
<pin name="NO8A" direction="pas"/>
<pin name="NO8B" direction="pas"/>
<pin name="NO1B" direction="pas"/>
<pin name="NO2B" direction="pas"/>
<pin name="NO3B" direction="pas"/>
<pin name="NO4B" direction="pas"/>
<pin name="NO5B" direction="pas"/>
<pin name="NO6B" direction="pas"/>
<pin name="NO7B" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="NC@2" direction="nc"/>
<pin name="COMA" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="COMB" direction="pas"/>
</symbol>
<symbol name="MAX308">
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="NO6" direction="pas"/>
<pin name="NO7" direction="pas"/>
<pin name="NO8" direction="pas"/>
<pin name="NO5" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX309">
<pin name="NO1B" direction="pas"/>
<pin name="NO2B" direction="pas"/>
<pin name="NO3B" direction="pas"/>
<pin name="NO4B" direction="pas"/>
<pin name="NO2A" direction="pas"/>
<pin name="NO3A" direction="pas"/>
<pin name="NO4A" direction="pas"/>
<pin name="NO1A" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="COMB" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="COMA" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX317">
<pin name="IN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX318">
<pin name="IN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NO" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX335">
<pin name="SCLK" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="DIN" direction="in"/>
<pin name="NO0" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="NO5" direction="pas"/>
<pin name="NO6" direction="pas"/>
<pin name="NO7" direction="pas"/>
<pin name="COM0" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="VL" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="COM4" direction="pas"/>
<pin name="COM5" direction="pas"/>
<pin name="COM6" direction="pas"/>
<pin name="COM7" direction="pas"/>
</symbol>
<symbol name="MAX338">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="NO5" direction="pas"/>
<pin name="NO6" direction="pas"/>
<pin name="NO7" direction="pas"/>
<pin name="NO8" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX339">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="COMB" direction="pas"/>
<pin name="NO1A" direction="pas"/>
<pin name="NO2A" direction="pas"/>
<pin name="NO3A" direction="pas"/>
<pin name="NO4A" direction="pas"/>
<pin name="NO1B" direction="pas"/>
<pin name="NO2B" direction="pas"/>
<pin name="NO3B" direction="pas"/>
<pin name="NO4B" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="COMA" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX351">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX352">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX353">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX361">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX362">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX366">
<pin name="IN1" direction="pas"/>
<pin name="IN2" direction="pas"/>
<pin name="IN3" direction="pas"/>
<pin name="OUT1" direction="pas"/>
<pin name="OUT2" direction="pas"/>
<pin name="OUT3" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX367">
<pin name="IN1" direction="pas"/>
<pin name="IN2" direction="pas"/>
<pin name="IN3" direction="pas"/>
<pin name="IN4" direction="pas"/>
<pin name="IN5" direction="pas"/>
<pin name="IN6" direction="pas"/>
<pin name="IN7" direction="pas"/>
<pin name="IN8" direction="pas"/>
<pin name="OUT1" direction="pas"/>
<pin name="OUT2" direction="pas"/>
<pin name="OUT3" direction="pas"/>
<pin name="OUT4" direction="pas"/>
<pin name="OUT5" direction="pas"/>
<pin name="OUT6" direction="pas"/>
<pin name="OUT7" direction="pas"/>
<pin name="OUT8" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX381">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
</symbol>
<symbol name="MAX383">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
</symbol>
<symbol name="MAX385">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
</symbol>
<symbol name="MAX391">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
</symbol>
<symbol name="MAX392">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NO3" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
</symbol>
<symbol name="MAX393">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="COM4" direction="pas"/>
</symbol>
<symbol name="MAX398">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="NO1" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NO6" direction="pas"/>
<pin name="NO4" direction="pas"/>
<pin name="NO5" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="NO8" direction="pas"/>
<pin name="NO7" direction="pas"/>
</symbol>
<symbol name="MAX399">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="NO1A" direction="pas"/>
<pin name="NO2A" direction="pas"/>
<pin name="COMA" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NO3B" direction="pas"/>
<pin name="NO1B" direction="pas"/>
<pin name="NO2B" direction="pas"/>
<pin name="NO3A" direction="pas"/>
<pin name="NO4A" direction="pas"/>
<pin name="COMB" direction="pas"/>
<pin name="NO4B" direction="pas"/>
</symbol>
<symbol name="MAX388">
<pin name="IN1" direction="pas"/>
<pin name="IN2" direction="pas"/>
<pin name="IN3" direction="pas"/>
<pin name="IN4" direction="pas"/>
<pin name="IN5" direction="pas"/>
<pin name="IN6" direction="pas"/>
<pin name="IN7" direction="pas"/>
<pin name="IN8" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="!RS" direction="in" function="dot"/>
<pin name="!WR" direction="in" function="dot"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX389">
<pin name="IN1A" direction="pas"/>
<pin name="IN1B" direction="pas"/>
<pin name="IN2A" direction="pas"/>
<pin name="IN2B" direction="pas"/>
<pin name="IN3A" direction="pas"/>
<pin name="IN3B" direction="pas"/>
<pin name="IN4A" direction="pas"/>
<pin name="IN4B" direction="pas"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="OUTB" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="!RS" direction="in" function="dot"/>
<pin name="!WR" direction="in" function="dot"/>
<pin name="OUTA" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX752">
<pin name="!SHDN" direction="in"/>
<pin name="VREF" direction="out"/>
<pin name="SS" direction="pas"/>
<pin name="CC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX765">
<pin name="V+" direction="pwr"/>
<pin name="V+@0" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="LX" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="REF" direction="out"/>
</symbol>
<symbol name="MAX687">
<pin name="OUT" direction="out"/>
<pin name="PFO" direction="out" function="dot"/>
<pin name="CC" direction="out"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SHDN" direction="in" function="dot"/>
<pin name="BASE" direction="out"/>
<pin name="BLIM" direction="in"/>
</symbol>
<symbol name="OPOFF">
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
</symbol>
<symbol name="MXD1000">
<pin name="IN" direction="in"/>
<pin name="TAP1" direction="out"/>
<pin name="TAP2" direction="out"/>
<pin name="TAP3" direction="out"/>
<pin name="TAP4" direction="out"/>
<pin name="TAP5" direction="out"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="MAX3222">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="SHDN/" direction="in"/>
<pin name="EN/" direction="in"/>
</symbol>
<symbol name="MAX3237">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T4IN" direction="in"/>
<pin name="T5IN" direction="in"/>
<pin name="T3OUT" direction="out"/>
<pin name="T4OUT" direction="out"/>
<pin name="T5OUT" direction="out"/>
<pin name="R1OUTB" direction="out"/>
<pin name="R3OUT" direction="out"/>
<pin name="R3IN" direction="in"/>
<pin name="MBOUD" direction="in"/>
<pin name="SHDN/" direction="in"/>
<pin name="EN/" direction="in"/>
</symbol>
<symbol name="MAX3241">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T3OUT" direction="out"/>
<pin name="R1OUTB" direction="out"/>
<pin name="R3OUT" direction="out"/>
<pin name="R3IN" direction="in"/>
<pin name="SHDN/" direction="in"/>
<pin name="EN/" direction="in"/>
<pin name="R2OUTB" direction="out"/>
<pin name="R4OUT" direction="out"/>
<pin name="R5OUT" direction="out"/>
<pin name="R4IN" direction="in"/>
<pin name="R5IN" direction="in"/>
</symbol>
<symbol name="MAX3232">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
</symbol>
<symbol name="MAX481">
<pin name="RO" direction="out"/>
<pin name="RE/" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="MAX488">
<pin name="DI" direction="in"/>
<pin name="RO" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="Z" direction="out"/>
</symbol>
<symbol name="MAX489">
<pin name="RO" direction="out"/>
<pin name="RE/" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="Z" direction="pas"/>
<pin name="Y" direction="pas"/>
</symbol>
<symbol name="MAX1674">
<pin name="SHDN/" direction="in"/>
<pin name="LBI" direction="in"/>
<pin name="LBO/" direction="out"/>
<pin name="REF" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="LX" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX1676">
<pin name="SHDN/" direction="in"/>
<pin name="LBI" direction="in"/>
<pin name="LBO/" direction="out"/>
<pin name="REF" direction="pas"/>
<pin name="FB" direction="in"/>
<pin name="LX" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="BATT" direction="in"/>
<pin name="CSEL" direction="in"/>
</symbol>
<symbol name="MAX813L">
<pin name="PFO" direction="out"/>
<pin name="PFI" direction="in"/>
<pin name="MR" direction="in"/>
<pin name="WDO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="WDI" direction="in"/>
</symbol>
<symbol name="VCC-VEE">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="MAX4137">
<pin name="NC1" direction="nc"/>
<pin name="VCCO@1" direction="pwr"/>
<pin name="VCCO@2" direction="pwr"/>
<pin name="VEEO@1" direction="pwr"/>
<pin name="VEEO@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCCI" direction="pwr"/>
<pin name="VEEI" direction="pwr"/>
<pin name="NC12" direction="nc"/>
<pin name="NC13" direction="nc"/>
<pin name="NC24" direction="nc"/>
<pin name="/SEL1" direction="in"/>
<pin name="/SEL2" direction="in"/>
<pin name="/SEL3" direction="in"/>
<pin name="/SEL4" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="NC17" direction="nc"/>
<pin name="AGND@4" direction="pwr"/>
</symbol>
<symbol name="MAX4138">
<pin name="NC1" direction="nc"/>
<pin name="VCCO@1" direction="pwr"/>
<pin name="VCCO@2" direction="pwr"/>
<pin name="VEEO@1" direction="pwr"/>
<pin name="VEEO@2" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VCCI" direction="pwr"/>
<pin name="VEEI" direction="pwr"/>
<pin name="NC12" direction="nc"/>
<pin name="NC13" direction="nc"/>
<pin name="NC24" direction="nc"/>
<pin name="/SEL1" direction="in"/>
<pin name="/SEL2" direction="in"/>
<pin name="/SEL3" direction="in"/>
<pin name="/SEL4" direction="in"/>
<pin name="RF" direction="pas"/>
<pin name="RG" direction="pas"/>
<pin name="IN+" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="AGND@4" direction="pwr"/>
</symbol>
<symbol name="MAX203E">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+/1" direction="pas"/>
<pin name="C2-/1" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-/1" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="C2+/2" direction="pas"/>
<pin name="C2-/2" direction="pas"/>
<pin name="V-/2" direction="pas"/>
</symbol>
<symbol name="MAX211E">
<pin name="R4OUT" direction="out"/>
<pin name="C1-" direction="pas"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="R5OUT" direction="out"/>
<pin name="R3IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="R5IN" direction="in"/>
<pin name="C1+" direction="pas"/>
<pin name="R3OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="R1IN" direction="in"/>
<pin name="R4IN" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="T4IN" direction="in"/>
<pin name="T4OUT" direction="out"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
</symbol>
<symbol name="MAX213E">
<pin name="R4OUT" direction="out"/>
<pin name="C1-" direction="pas"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="R5OUT" direction="out"/>
<pin name="R3IN" direction="in"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="T3OUT" direction="out"/>
<pin name="R5IN" direction="in"/>
<pin name="C1+" direction="pas"/>
<pin name="R3OUT" direction="out"/>
<pin name="R2IN" direction="in"/>
<pin name="R1IN" direction="in"/>
<pin name="R4IN" direction="in"/>
<pin name="V-" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="SHDN" direction="in"/>
<pin name="V+" direction="pas"/>
<pin name="T4IN" direction="in"/>
<pin name="T4OUT" direction="out"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
</symbol>
<symbol name="OPBUFF">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="G_VCCVEE">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="BUFF3P">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="MAX807">
<pin name="BATT" direction="in"/>
<pin name="PFI" direction="in"/>
<pin name="!CEIN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="BATT_ON" direction="out"/>
<pin name="!LOWLINE" direction="out"/>
<pin name="BATT_OK" direction="out"/>
<pin name="!PFO" direction="out"/>
<pin name="!CEOUT" direction="out"/>
<pin name="RESET" direction="out"/>
<pin name="!RESET" direction="out"/>
<pin name="!WDO" direction="out"/>
<pin name="!MR" direction="in"/>
<pin name="WDI" direction="in"/>
</symbol>
<symbol name="MAX038">
<pin name="REF" direction="out"/>
<pin name="DADJ" direction="in"/>
<pin name="IIN" direction="pas"/>
<pin name="FADJ" direction="in"/>
<pin name="COSC" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DV+" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="SYNC" direction="out"/>
<pin name="PDI" direction="in"/>
<pin name="PDO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="MAX3965">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GNDO" direction="pwr"/>
<pin name="VCCO" direction="pwr"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="INV" direction="in"/>
<pin name="VTH" direction="out"/>
<pin name="CZP" direction="pas"/>
<pin name="CZN" direction="pas"/>
<pin name="RSSI" direction="out"/>
<pin name="SQUELCH" direction="in"/>
<pin name="LOS+" direction="out"/>
<pin name="LOS-" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="OUT+" direction="out"/>
<pin name="SUB" direction="pas"/>
<pin name="FILTER" direction="out"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="MAX6342">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PFI" direction="in"/>
<pin name="!MR" direction="in"/>
<pin name="!RESET" direction="out"/>
<pin name="!PFO" direction="out"/>
</symbol>
<symbol name="MAX712">
<pin name="GND" direction="pwr"/>
<pin name="BATT+" direction="in"/>
<pin name="THI" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="VLIMIT" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="TEMP" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="BATT-" direction="in"/>
<pin name="TLO" direction="in"/>
<pin name="DRV" direction="out"/>
<pin name="PGM0" direction="in"/>
<pin name="PGM1" direction="in"/>
<pin name="PGM2" direction="in"/>
<pin name="PGM3" direction="in"/>
<pin name="!FASTCHG" direction="oc"/>
</symbol>
<symbol name="DS2890">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DATA"/>
<pin name="RH" direction="pas"/>
<pin name="RL" direction="pas"/>
<pin name="WIPER" direction="pas"/>
</symbol>
<symbol name="DS2405">
<pin name="DATA" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="PIO" direction="pas"/>
</symbol>
<symbol name="MAX4355">
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="IN9" direction="in"/>
<pin name="IN10" direction="in"/>
<pin name="IN11" direction="in"/>
<pin name="IN12" direction="in"/>
<pin name="IN13" direction="in"/>
<pin name="IN14" direction="in"/>
<pin name="IN15" direction="in"/>
<pin name="OUT0" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="OUT9" direction="out"/>
<pin name="OUT10" direction="out"/>
<pin name="OUT11" direction="out"/>
<pin name="OUT12" direction="out"/>
<pin name="OUT13" direction="out"/>
<pin name="OUT14" direction="out"/>
<pin name="OUT15" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!UPDATE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="!AOUT" direction="out"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="VEE">
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="DGND">
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="AGND">
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MAX4313">
<pin name="IN1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!SHDN" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A0" direction="in"/>
</symbol>
<symbol name="MAX4310">
<pin name="IN1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="FB" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="!SHDN" direction="in"/>
</symbol>
<symbol name="MAX4311">
<pin name="IN1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="FB" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="A1" direction="in"/>
</symbol>
<symbol name="MAX4312">
<pin name="IN1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="FB" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="MAX4314">
<pin name="IN1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!SHDN" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="MAX4315">
<pin name="IN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!SHDN" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="IN0" direction="in"/>
</symbol>
<symbol name="MAX3243">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="T3IN" direction="in"/>
<pin name="T3OUT" direction="out"/>
<pin name="R2OUTB" direction="out"/>
<pin name="R3OUT" direction="out"/>
<pin name="R3IN" direction="in"/>
<pin name="!INVALID" direction="in"/>
<pin name="!FORCEOFF" direction="in"/>
<pin name="FORCEON" direction="in"/>
<pin name="R4OUT" direction="out"/>
<pin name="R5OUT" direction="out"/>
<pin name="R4IN" direction="in"/>
<pin name="R5IN" direction="in"/>
</symbol>
<symbol name="MAX3223">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="!INVALID" direction="out"/>
<pin name="!FORCEOFF" direction="in"/>
<pin name="FORCEON" direction="in"/>
<pin name="!EN" direction="in"/>
</symbol>
<symbol name="MAX3221">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="!INVALID" direction="in"/>
<pin name="!FORCEOFF" direction="in"/>
<pin name="FORCEON" direction="in"/>
<pin name="!EN" direction="in"/>
</symbol>
<symbol name="MAX1150">
<pin name="D1B" direction="out"/>
<pin name="D2B" direction="out"/>
<pin name="D3B" direction="out"/>
<pin name="D4B" direction="out"/>
<pin name="D5B" direction="out"/>
<pin name="D6B" direction="out"/>
<pin name="D7B" direction="out"/>
<pin name="D0B" direction="out"/>
<pin name="D0A" direction="out"/>
<pin name="D1A" direction="out"/>
<pin name="D2A" direction="out"/>
<pin name="D3A" direction="out"/>
<pin name="D4A" direction="out"/>
<pin name="D5A" direction="out"/>
<pin name="D6A" direction="out"/>
<pin name="D7A" direction="out"/>
<pin name="VEE" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VRBF" direction="in"/>
<pin name="VRBS" direction="in"/>
<pin name="VIN@1" direction="in"/>
<pin name="VRM" direction="in"/>
<pin name="VRTF" direction="in"/>
<pin name="VRTS" direction="in"/>
<pin name="NCLK" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="DRA" direction="out"/>
<pin name="NDRA" direction="out"/>
<pin name="DRB" direction="out"/>
<pin name="NDRB" direction="out"/>
<pin name="VIN" direction="in"/>
<pin name="D8B" direction="out"/>
<pin name="D8A" direction="out"/>
</symbol>
<symbol name="MAX1150-P">
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="DGND@5" direction="pwr"/>
<pin name="DGND@6" direction="pwr"/>
<pin name="DGND@7" direction="pwr"/>
<pin name="DGND@8" direction="pwr"/>
<pin name="DGND@9" direction="pwr"/>
<pin name="DGND@10" direction="pwr"/>
<pin name="NC@3" direction="nc"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AGND@5" direction="pwr"/>
<pin name="AGND@6" direction="pwr"/>
<pin name="AGND@7" direction="pwr"/>
<pin name="AGND@8" direction="pwr"/>
<pin name="AGND@9" direction="pwr"/>
<pin name="AGND@10" direction="pwr"/>
<pin name="AGND@11" direction="pwr"/>
<pin name="AGND@12" direction="pwr"/>
<pin name="AGND@13" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="VEE@1" direction="pwr"/>
<pin name="VEE@2" direction="pwr"/>
<pin name="VEE@3" direction="pwr"/>
<pin name="VEE@4" direction="pwr"/>
<pin name="VEE@5" direction="pwr"/>
<pin name="VEE@6" direction="pwr"/>
<pin name="VEE@7" direction="pwr"/>
<pin name="VEE@8" direction="pwr"/>
<pin name="VEE@9" direction="pwr"/>
<pin name="VEE@10" direction="pwr"/>
<pin name="VEE@11" direction="pwr"/>
<pin name="VEE@12" direction="pwr"/>
<pin name="VEE@13" direction="pwr"/>
<pin name="VEE@14" direction="pwr"/>
<pin name="VEE@15" direction="pwr"/>
<pin name="VEE@16" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
</symbol>
<symbol name="MAX3465">
<pin name="RO" direction="out"/>
<pin name="RE/" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="Z" direction="out"/>
<pin name="Y" direction="out"/>
<pin name="TXP" direction="pas"/>
<pin name="RXP" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SHDN" direction="in"/>
</symbol>
<symbol name="MAX3467">
<pin name="RO" direction="out"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="DI" direction="in"/>
<pin name="Z" direction="pas"/>
<pin name="Y" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="MAX3468">
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RO" direction="out"/>
<pin name="RE/" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="DI" direction="in"/>
</symbol>
<symbol name="MAX3043">
<pin name="T1IN" direction="in"/>
<pin name="Z1" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="EN" direction="in"/>
<pin name="!EB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="T2IN" direction="in"/>
<pin name="Z2" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="T3IN" direction="in"/>
<pin name="Z3" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="T4IN" direction="in"/>
<pin name="Z4" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MAX3095">
<pin name="Y1" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="G" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="A4" direction="out"/>
</symbol>
<symbol name="MAX3040">
<pin name="T1IN" direction="in"/>
<pin name="Z1" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="EN12" direction="in"/>
<pin name="EN34" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="T2IN" direction="in"/>
<pin name="Z2" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="T3IN" direction="in"/>
<pin name="Z3" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="T4IN" direction="in"/>
<pin name="Z4" direction="out"/>
<pin name="Y4" direction="out"/>
</symbol>
<symbol name="MAX12527">
<pin name="INAP" direction="in"/>
<pin name="INAN" direction="in"/>
<pin name="REFAP" direction="pas"/>
<pin name="COMA" direction="pas"/>
<pin name="REFAN" direction="pas"/>
<pin name="REFIN" direction="in"/>
<pin name="REFOUT" direction="out"/>
<pin name="SHREF" direction="in"/>
<pin name="REFBP" direction="pas"/>
<pin name="COMB" direction="pas"/>
<pin name="REFBN" direction="pas"/>
<pin name="INBP" direction="in"/>
<pin name="INBN" direction="in"/>
<pin name="DIFFCLK/!SECLK" direction="in"/>
<pin name="CLKP" direction="in"/>
<pin name="CLKN" direction="in"/>
<pin name="DIV2" direction="in"/>
<pin name="DIV4" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="PD" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="DORB" direction="out"/>
<pin name="D0B" direction="out"/>
<pin name="D1B" direction="out"/>
<pin name="D2B" direction="out"/>
<pin name="D3B" direction="out"/>
<pin name="D4B" direction="out"/>
<pin name="D5B" direction="out"/>
<pin name="D6B" direction="out"/>
<pin name="D7B" direction="out"/>
<pin name="D8B" direction="out"/>
<pin name="D9B" direction="out"/>
<pin name="D10B" direction="out"/>
<pin name="D11B" direction="out"/>
<pin name="OVDD" direction="pwr"/>
<pin name="DAV" direction="out"/>
<pin name="G/!T" direction="in"/>
<pin name="DORA" direction="out"/>
<pin name="D0A" direction="out"/>
<pin name="D1A" direction="out"/>
<pin name="D2A" direction="out"/>
<pin name="D3A" direction="out"/>
<pin name="D4A" direction="out"/>
<pin name="D5A" direction="out"/>
<pin name="D6A" direction="out"/>
<pin name="D7A" direction="out"/>
<pin name="D8A" direction="out"/>
<pin name="D9A" direction="out"/>
<pin name="D10A" direction="out"/>
<pin name="D11A" direction="out"/>
<pin name="THPAD" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="OVDD@1" direction="pwr"/>
<pin name="OVDD@2" direction="pwr"/>
</symbol>
<symbol name="MAX3766">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="BIASMAX" direction="in"/>
<pin name="POWERSET" direction="in"/>
<pin name="REF1" direction="pas"/>
<pin name="TC" direction="pas"/>
<pin name="REF2" direction="pas"/>
<pin name="MOD" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GNDOUT" direction="pas"/>
<pin name="SAFETY" direction="in"/>
<pin name="!FAIL" direction="out"/>
<pin name="BIAS" direction="pas"/>
<pin name="OUT+" direction="out"/>
<pin name="MD" direction="in"/>
<pin name="OUT-" direction="out"/>
<pin name="ENABLE" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCCOUT" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="MAX3233">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+@2" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="!INVALID" direction="out"/>
<pin name="!FORCEOFF" direction="in"/>
<pin name="FORCEON" direction="in"/>
<pin name="V+@1" direction="pas"/>
</symbol>
<symbol name="MAX3380">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="T1IN" direction="in"/>
<pin name="T2IN" direction="in"/>
<pin name="R1OUT" direction="out"/>
<pin name="R2OUT" direction="out"/>
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="T1OUT" direction="out"/>
<pin name="T2OUT" direction="out"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="!INVALID" direction="out"/>
<pin name="!FORCEOFF" direction="in"/>
<pin name="FORCEON" direction="in"/>
<pin name="VL" direction="pas"/>
</symbol>
<symbol name="ICL76XX">
<pin name="IOSET" direction="pas"/>
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="ICL762XX">
<pin name="OFF1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OFF2" direction="pas"/>
</symbol>
<symbol name="PWR2+-">
<pin name="V+@1" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+@2" direction="pwr"/>
</symbol>
<symbol name="ICL763XX">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="IOSET" direction="pas"/>
</symbol>
<symbol name="OP-SHDOWN">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="SHUTDOWN" direction="pas"/>
</symbol>
<symbol name="PWR+-GATE">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MAX7042">
<pin name="LNAIN" direction="in"/>
<pin name="LNASRC" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="HVIN" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DATA" direction="out"/>
<pin name="DS-" direction="in"/>
<pin name="PDMAX" direction="out"/>
<pin name="PDMIN" direction="out"/>
<pin name="DS+" direction="in"/>
<pin name="OP+" direction="in"/>
<pin name="DF" direction="in"/>
<pin name="LNASEL" direction="in"/>
<pin name="FSEL2" direction="in"/>
<pin name="FSEL1" direction="in"/>
<pin name="RSSI" direction="out"/>
<pin name="FIN+" direction="in"/>
<pin name="FIN-" direction="in"/>
<pin name="MIXIN+" direction="in"/>
<pin name="MIXIN-" direction="in"/>
<pin name="MIXOUT" direction="out"/>
<pin name="LNAOUT" direction="in"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="DS1621">
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="TOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MAX4947">
<pin name="COM1"/>
<pin name="NO1"/>
<pin name="NC1"/>
<pin name="COM2"/>
<pin name="NO2"/>
<pin name="NC2"/>
<pin name="CB" direction="in"/>
</symbol>
<symbol name="MAX4948">
<pin name="COM1"/>
<pin name="NO1"/>
<pin name="NC1"/>
<pin name="COM2"/>
<pin name="NO2"/>
<pin name="NC2"/>
<pin name="CB" direction="in"/>
<pin name="COM3"/>
<pin name="NO3"/>
<pin name="NC3"/>
<pin name="COM4"/>
<pin name="NO4"/>
<pin name="NC4"/>
<pin name="COM5"/>
<pin name="NO5"/>
<pin name="NC5"/>
<pin name="COM6"/>
<pin name="NO6"/>
<pin name="NC6"/>
<pin name="!EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="EXPOSED">
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="MAX4906">
<pin name="SHDN/!EN" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="COM1"/>
<pin name="NO1"/>
<pin name="NC1"/>
<pin name="COM2"/>
<pin name="NO2"/>
<pin name="NC2"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX4907">
<pin name="SHDN/!EN" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="COM1"/>
<pin name="NO1"/>
<pin name="COM2"/>
<pin name="NO2"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX6173">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="in"/>
<pin name="TRIM" direction="in"/>
<pin name="TEMP" direction="nc"/>
</symbol>
<symbol name="MAX1792">
<pin name="IN@1" direction="in"/>
<pin name="IN@2" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="!RST" direction="out"/>
<pin name="OUT@1" direction="pas"/>
<pin name="OUT@2" direction="pas"/>
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="MAX1759">
<pin name="IN@1" direction="in"/>
<pin name="IN@2" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="POK" direction="oc"/>
<pin name="GND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="PGND" direction="pwr"/>
<pin name="CXP" direction="in"/>
<pin name="CXN" direction="in"/>
</symbol>
<symbol name="MAX1555">
<pin name="USB" direction="in"/>
<pin name="DC" direction="in"/>
<pin name="BAT" direction="pas"/>
<pin name="!CHG" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX1551">
<pin name="USB" direction="in"/>
<pin name="DC" direction="in"/>
<pin name="BAT" direction="pas"/>
<pin name="!POK" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DS275">
<pin name="TXIN" direction="in"/>
<pin name="VDRV" direction="in"/>
<pin name="TXOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RXOUT" direction="out"/>
<pin name="RXIN" direction="in"/>
</symbol>
<symbol name="MAX3311">
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TIN" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="ROUT" direction="out"/>
<pin name="V-" direction="pas"/>
<pin name="TOUT" direction="out"/>
<pin name="RIN" direction="in"/>
</symbol>
<symbol name="MAX7313AEG">
<pin name="SLC" direction="in"/>
<pin name="SDA"/>
<pin name="!INT!/O16" direction="oc"/>
<pin name="AD0" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="MAX7313">
<pin name="SLC" direction="in"/>
<pin name="SDA"/>
<pin name="!INT!/O16" direction="oc"/>
<pin name="AD0" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="GND" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="MAX6520">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="in"/>
</symbol>
<symbol name="MAX1038">
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="AIN8" direction="in"/>
<pin name="AIN9" direction="in"/>
<pin name="AIN10" direction="in"/>
<pin name="AIN11/REF" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX1036">
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3/REF" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX312">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="NC4" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
</symbol>
<symbol name="MAX313">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NO3" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="NO4" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
</symbol>
<symbol name="MAX314">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="NO4" direction="pas"/>
<pin name="COM4" direction="pas"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
</symbol>
<symbol name="DS2726">
<pin name="PKP" direction="in"/>
<pin name="CC" direction="out"/>
<pin name="SNS" direction="in"/>
<pin name="DC" direction="out"/>
<pin name="VIN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="OVS0" direction="in"/>
<pin name="OVS1" direction="in"/>
<pin name="CBS0" direction="in"/>
<pin name="CBS1" direction="in"/>
<pin name="CBCFG" direction="in"/>
<pin name="SLEEP" direction="in"/>
<pin name="CSCD" direction="in"/>
<pin name="RSC" direction="in"/>
<pin name="RDOC" direction="in"/>
<pin name="DCOCD" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="V00" direction="pas"/>
<pin name="V01" direction="pas"/>
<pin name="V02" direction="pas"/>
<pin name="V03" direction="pas"/>
<pin name="V04" direction="pas"/>
<pin name="V05" direction="pas"/>
<pin name="V06" direction="pas"/>
<pin name="V07" direction="pas"/>
<pin name="V08" direction="pas"/>
<pin name="V09" direction="pas"/>
<pin name="V10" direction="pas"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="DS8500">
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="!RST"/>
<pin name="OCD" direction="out"/>
<pin name="RTS" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="XCEN" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="FSK_OUT" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="FSK_IN" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="DGND@5" direction="pwr"/>
<pin name="D_OUT" direction="out"/>
<pin name="D_IN" direction="in"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="MAX31855">
<pin name="VCC"/>
<pin name="T+"/>
<pin name="T-"/>
<pin name="SO"/>
<pin name="!CS"/>
<pin name="SCK"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX130CPL" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX130"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A/Z" pad="29"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="23"/>
<connect gate="G$1" pin="AB4" pad="19"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="BP" pad="21"/>
<connect gate="G$1" pin="BUFF" pad="28"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="24"/>
<connect gate="G$1" pin="COMM" pad="32"/>
<connect gate="G$1" pin="CREF+" pad="34"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="14"/>
<connect gate="G$1" pin="E3" pad="18"/>
<connect gate="G$1" pin="F1" pad="6"/>
<connect gate="G$1" pin="F2" pad="13"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="25"/>
<connect gate="G$1" pin="G3" pad="22"/>
<connect gate="G$1" pin="IN-HI" pad="31"/>
<connect gate="G$1" pin="IN-LO" pad="30"/>
<connect gate="G$1" pin="INT" pad="27"/>
<connect gate="G$1" pin="OSC1" pad="40"/>
<connect gate="G$1" pin="OSC2" pad="39"/>
<connect gate="G$1" pin="OSC3" pad="38"/>
<connect gate="G$1" pin="POL" pad="20"/>
<connect gate="G$1" pin="REF-HI" pad="36"/>
<connect gate="G$1" pin="REF-LO" pad="35"/>
<connect gate="G$1" pin="TEST" pad="37"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX133CPL" prefix="IC">
<description>3 3/4-digit &lt;b&gt;DMM CIRCUIT&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX133"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="1,11M" pad="17"/>
<connect gate="G$1" pin="101K" pad="18"/>
<connect gate="G$1" pin="10K" pad="19"/>
<connect gate="G$1" pin="10M" pad="16"/>
<connect gate="G$1" pin="1K" pad="20"/>
<connect gate="G$1" pin="400MV-IN" pad="27"/>
<connect gate="G$1" pin="AC-IN" pad="29"/>
<connect gate="G$1" pin="AC-OUT" pad="28"/>
<connect gate="G$1" pin="ALE" pad="4"/>
<connect gate="G$1" pin="BCL-OUT" pad="5"/>
<connect gate="G$1" pin="BEEPER" pad="10"/>
<connect gate="G$1" pin="BUFFOUT1" pad="34"/>
<connect gate="G$1" pin="BUFFOUT2" pad="35"/>
<connect gate="G$1" pin="COMMON" pad="22"/>
<connect gate="G$1" pin="CS" pad="3"/>
<connect gate="G$1" pin="CUR-IN" pad="33"/>
<connect gate="G$1" pin="D0" pad="39"/>
<connect gate="G$1" pin="D1" pad="38"/>
<connect gate="G$1" pin="D2" pad="37"/>
<connect gate="G$1" pin="D3" pad="36"/>
<connect gate="G$1" pin="DGND" pad="2"/>
<connect gate="G$1" pin="EOC" pad="9"/>
<connect gate="G$1" pin="FA-IN" pad="14"/>
<connect gate="G$1" pin="FA-OUT" pad="15"/>
<connect gate="G$1" pin="FR-IN" pad="31"/>
<connect gate="G$1" pin="FR-OUT" pad="23"/>
<connect gate="G$1" pin="IN-LO" pad="11"/>
<connect gate="G$1" pin="INT-IN" pad="13"/>
<connect gate="G$1" pin="INT-OUT" pad="12"/>
<connect gate="G$1" pin="NC" pad="21"/>
<connect gate="G$1" pin="NC@1" pad="24"/>
<connect gate="G$1" pin="NC@2" pad="25"/>
<connect gate="G$1" pin="OS" pad="32"/>
<connect gate="G$1" pin="OSC1" pad="7"/>
<connect gate="G$1" pin="OSC2" pad="8"/>
<connect gate="G$1" pin="RD" pad="40"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="30"/>
<connect gate="G$1" pin="VREF" pad="26"/>
<connect gate="G$1" pin="WR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX136CPL" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX136"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A/Z" pad="29"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="23"/>
<connect gate="G$1" pin="AB4" pad="19"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="BP" pad="21"/>
<connect gate="G$1" pin="BUFF" pad="28"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="24"/>
<connect gate="G$1" pin="COMM" pad="32"/>
<connect gate="G$1" pin="CREF+" pad="34"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="14"/>
<connect gate="G$1" pin="E3" pad="18"/>
<connect gate="G$1" pin="F1" pad="6"/>
<connect gate="G$1" pin="F2" pad="13"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="25"/>
<connect gate="G$1" pin="G3" pad="22"/>
<connect gate="G$1" pin="HOLD" pad="1"/>
<connect gate="G$1" pin="IN-HI" pad="31"/>
<connect gate="G$1" pin="IN-LO" pad="30"/>
<connect gate="G$1" pin="INT" pad="27"/>
<connect gate="G$1" pin="OSC1" pad="40"/>
<connect gate="G$1" pin="OSC2" pad="39"/>
<connect gate="G$1" pin="OSC3" pad="38"/>
<connect gate="G$1" pin="POL" pad="20"/>
<connect gate="G$1" pin="REF-HI" pad="36"/>
<connect gate="G$1" pin="TEST" pad="37"/>
<connect gate="G$1" pin="V+" pad="35"/>
<connect gate="G$1" pin="V-" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX138CPL" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX138"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A/Z" pad="29"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="23"/>
<connect gate="G$1" pin="AB4" pad="19"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="BP" pad="21"/>
<connect gate="G$1" pin="BUFF" pad="28"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="24"/>
<connect gate="G$1" pin="CAP+" pad="40"/>
<connect gate="G$1" pin="CAP-" pad="38"/>
<connect gate="G$1" pin="COMM" pad="32"/>
<connect gate="G$1" pin="CREF+" pad="34"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="14"/>
<connect gate="G$1" pin="E3" pad="18"/>
<connect gate="G$1" pin="F1" pad="6"/>
<connect gate="G$1" pin="F2" pad="13"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="25"/>
<connect gate="G$1" pin="G3" pad="22"/>
<connect gate="G$1" pin="GND" pad="39"/>
<connect gate="G$1" pin="IN-HI" pad="31"/>
<connect gate="G$1" pin="IN-LO" pad="30"/>
<connect gate="G$1" pin="INT" pad="27"/>
<connect gate="G$1" pin="POL" pad="20"/>
<connect gate="G$1" pin="REF-HI" pad="36"/>
<connect gate="G$1" pin="REF-LO" pad="35"/>
<connect gate="G$1" pin="TEST" pad="37"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX150ACP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX150"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="CS" pad="13"/>
<connect gate="G$1" pin="DB0" pad="2"/>
<connect gate="G$1" pin="DB1" pad="3"/>
<connect gate="G$1" pin="DB2" pad="4"/>
<connect gate="G$1" pin="DB3" pad="5"/>
<connect gate="G$1" pin="DB4" pad="14"/>
<connect gate="G$1" pin="DB5" pad="15"/>
<connect gate="G$1" pin="DB6" pad="16"/>
<connect gate="G$1" pin="DB7" pad="17"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="INT" pad="9"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="OFL" pad="18"/>
<connect gate="G$1" pin="RD" pad="8"/>
<connect gate="G$1" pin="REF-OUT" pad="19"/>
<connect gate="G$1" pin="V-IN" pad="1"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VREF+" pad="12"/>
<connect gate="G$1" pin="VREF-" pad="11"/>
<connect gate="G$1" pin="WR/RDY" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX154ACN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX154"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="A0" pad="22"/>
<connect gate="G$1" pin="A1" pad="21"/>
<connect gate="G$1" pin="AIN1" pad="4"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="2"/>
<connect gate="G$1" pin="AIN4" pad="1"/>
<connect gate="G$1" pin="CS" pad="16"/>
<connect gate="G$1" pin="DB0" pad="6"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB2" pad="8"/>
<connect gate="G$1" pin="DB3" pad="9"/>
<connect gate="G$1" pin="DB4" pad="17"/>
<connect gate="G$1" pin="DB5" pad="18"/>
<connect gate="G$1" pin="DB6" pad="19"/>
<connect gate="G$1" pin="DB7" pad="20"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INT" pad="11"/>
<connect gate="G$1" pin="NC" pad="23"/>
<connect gate="G$1" pin="RD" pad="10"/>
<connect gate="G$1" pin="RDY" pad="15"/>
<connect gate="G$1" pin="REF-OUT" pad="5"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VREF+" pad="14"/>
<connect gate="G$1" pin="VREF-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX158ACN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX158"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="25"/>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="A2" pad="23"/>
<connect gate="G$1" pin="AIN1" pad="6"/>
<connect gate="G$1" pin="AIN2" pad="5"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AIN4" pad="3"/>
<connect gate="G$1" pin="AIN5" pad="2"/>
<connect gate="G$1" pin="AIN6" pad="1"/>
<connect gate="G$1" pin="AIN7" pad="28"/>
<connect gate="G$1" pin="AIN8" pad="27"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="DB0" pad="8"/>
<connect gate="G$1" pin="DB1" pad="9"/>
<connect gate="G$1" pin="DB2" pad="10"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="DB4" pad="19"/>
<connect gate="G$1" pin="DB5" pad="20"/>
<connect gate="G$1" pin="DB6" pad="21"/>
<connect gate="G$1" pin="DB7" pad="22"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="INT" pad="13"/>
<connect gate="G$1" pin="RD" pad="12"/>
<connect gate="G$1" pin="RDY" pad="17"/>
<connect gate="G$1" pin="REF-OUT" pad="7"/>
<connect gate="G$1" pin="VDD" pad="26"/>
<connect gate="G$1" pin="VREF+" pad="16"/>
<connect gate="G$1" pin="VREF-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX160CPN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX160"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="AIN" pad="4"/>
<connect gate="G$1" pin="BOFS" pad="3"/>
<connect gate="G$1" pin="BUSY" pad="14"/>
<connect gate="G$1" pin="CLK" pad="17"/>
<connect gate="G$1" pin="CS" pad="16"/>
<connect gate="G$1" pin="DB0" pad="13"/>
<connect gate="G$1" pin="DB1" pad="12"/>
<connect gate="G$1" pin="DB2" pad="11"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="9"/>
<connect gate="G$1" pin="DB5" pad="8"/>
<connect gate="G$1" pin="DB6" pad="7"/>
<connect gate="G$1" pin="DB7" pad="6"/>
<connect gate="G$1" pin="DGND" pad="18"/>
<connect gate="G$1" pin="RD" pad="15"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX161ACP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX161"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="AIN0" pad="9"/>
<connect gate="G$1" pin="AIN1" pad="8"/>
<connect gate="G$1" pin="AIN2" pad="7"/>
<connect gate="G$1" pin="AIN3" pad="6"/>
<connect gate="G$1" pin="AIN4" pad="5"/>
<connect gate="G$1" pin="AIN5" pad="4"/>
<connect gate="G$1" pin="AIN6" pad="3"/>
<connect gate="G$1" pin="AIN7" pad="2"/>
<connect gate="G$1" pin="ALE" pad="16"/>
<connect gate="G$1" pin="BOFS" pad="1"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="CS" pad="13"/>
<connect gate="G$1" pin="DB0" pad="27"/>
<connect gate="G$1" pin="DB1" pad="26"/>
<connect gate="G$1" pin="DB2" pad="25"/>
<connect gate="G$1" pin="DB3" pad="24"/>
<connect gate="G$1" pin="DB4" pad="23"/>
<connect gate="G$1" pin="DB5" pad="22"/>
<connect gate="G$1" pin="DB6" pad="21"/>
<connect gate="G$1" pin="DB7" pad="20"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="STAT" pad="12"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VREF" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX162ACN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX162"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AIN" pad="1"/>
<connect gate="G$1" pin="BUSY" pad="22"/>
<connect gate="G$1" pin="CLK-IN" pad="17"/>
<connect gate="G$1" pin="CLK-OUT" pad="18"/>
<connect gate="G$1" pin="CS" pad="21"/>
<connect gate="G$1" pin="D0/8" pad="16"/>
<connect gate="G$1" pin="D1/9" pad="15"/>
<connect gate="G$1" pin="D10" pad="5"/>
<connect gate="G$1" pin="D11" pad="4"/>
<connect gate="G$1" pin="D2/10" pad="14"/>
<connect gate="G$1" pin="D3/11" pad="13"/>
<connect gate="G$1" pin="D4" pad="11"/>
<connect gate="G$1" pin="D5" pad="10"/>
<connect gate="G$1" pin="D6" pad="9"/>
<connect gate="G$1" pin="D7" pad="8"/>
<connect gate="G$1" pin="D8" pad="7"/>
<connect gate="G$1" pin="D9" pad="6"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="HBEN" pad="19"/>
<connect gate="G$1" pin="RD" pad="20"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VREF" pad="2"/>
<connect gate="G$1" pin="VSS" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX578JN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX578"/>
</gates>
<devices>
<device name="" package="DIL32">
<connects>
<connect gate="G$1" pin="10V-IN" pad="27"/>
<connect gate="G$1" pin="20V-IN" pad="28"/>
<connect gate="G$1" pin="AGND" pad="30"/>
<connect gate="G$1" pin="B1" pad="12"/>
<connect gate="G$1" pin="B10" pad="3"/>
<connect gate="G$1" pin="B11" pad="2"/>
<connect gate="G$1" pin="B12" pad="1"/>
<connect gate="G$1" pin="B1@" pad="13"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="10"/>
<connect gate="G$1" pin="B4" pad="9"/>
<connect gate="G$1" pin="B5" pad="8"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="6"/>
<connect gate="G$1" pin="B8" pad="5"/>
<connect gate="G$1" pin="B9" pad="4"/>
<connect gate="G$1" pin="BIOFF" pad="26"/>
<connect gate="G$1" pin="CLK-ADJ" pad="17"/>
<connect gate="G$1" pin="CLK-IN" pad="19"/>
<connect gate="G$1" pin="CLK-OUT" pad="18"/>
<connect gate="G$1" pin="CONST" pad="21"/>
<connect gate="G$1" pin="DGND" pad="15"/>
<connect gate="G$1" pin="EOC" pad="20"/>
<connect gate="G$1" pin="REF-IN" pad="25"/>
<connect gate="G$1" pin="REF-OUT" pad="24"/>
<connect gate="G$1" pin="SER-OUT" pad="23"/>
<connect gate="G$1" pin="SER-OUT@" pad="22"/>
<connect gate="G$1" pin="SHCY" pad="14"/>
<connect gate="G$1" pin="V+" pad="31"/>
<connect gate="G$1" pin="V-" pad="32"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="ZERO-ADJ" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0820BCN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADC0820"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="CS" pad="13"/>
<connect gate="G$1" pin="DB0" pad="2"/>
<connect gate="G$1" pin="DB1" pad="3"/>
<connect gate="G$1" pin="DB2" pad="4"/>
<connect gate="G$1" pin="DB3" pad="5"/>
<connect gate="G$1" pin="DB4" pad="14"/>
<connect gate="G$1" pin="DB5" pad="15"/>
<connect gate="G$1" pin="DB6" pad="16"/>
<connect gate="G$1" pin="DB7" pad="17"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="INT" pad="9"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="OFL" pad="18"/>
<connect gate="G$1" pin="RD" pad="8"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VREF+" pad="12"/>
<connect gate="G$1" pin="VREF-" pad="11"/>
<connect gate="G$1" pin="WR/RDY" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7106CPL" prefix="IC">
<description>&lt;b&gt;LCD DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7106"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A/Z" pad="29"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="23"/>
<connect gate="G$1" pin="AB4" pad="19"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="BP" pad="21"/>
<connect gate="G$1" pin="BUFF" pad="28"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="24"/>
<connect gate="G$1" pin="COMM" pad="32"/>
<connect gate="G$1" pin="CREF+" pad="34"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="14"/>
<connect gate="G$1" pin="E3" pad="18"/>
<connect gate="G$1" pin="F1" pad="6"/>
<connect gate="G$1" pin="F2" pad="13"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="25"/>
<connect gate="G$1" pin="G3" pad="22"/>
<connect gate="G$1" pin="IN-HI" pad="31"/>
<connect gate="G$1" pin="IN-LO" pad="30"/>
<connect gate="G$1" pin="INT" pad="27"/>
<connect gate="G$1" pin="OSC1" pad="40"/>
<connect gate="G$1" pin="OSC2" pad="39"/>
<connect gate="G$1" pin="OSC3" pad="38"/>
<connect gate="G$1" pin="POL" pad="20"/>
<connect gate="G$1" pin="REF-HI" pad="36"/>
<connect gate="G$1" pin="REF-LO" pad="35"/>
<connect gate="G$1" pin="TEST" pad="37"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7109MJL" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7109"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="AZ" pad="31"/>
<connect gate="G$1" pin="B1" pad="16"/>
<connect gate="G$1" pin="B10" pad="7"/>
<connect gate="G$1" pin="B11" pad="6"/>
<connect gate="G$1" pin="B12" pad="5"/>
<connect gate="G$1" pin="B2" pad="15"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="B4" pad="13"/>
<connect gate="G$1" pin="B5" pad="12"/>
<connect gate="G$1" pin="B6" pad="11"/>
<connect gate="G$1" pin="B7" pad="10"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="8"/>
<connect gate="G$1" pin="BOSC-OUT" pad="25"/>
<connect gate="G$1" pin="BUFFER" pad="30"/>
<connect gate="G$1" pin="CE/LOAD" pad="20"/>
<connect gate="G$1" pin="COMM" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HBEN" pad="19"/>
<connect gate="G$1" pin="IN-HI" pad="35"/>
<connect gate="G$1" pin="IN-LO" pad="34"/>
<connect gate="G$1" pin="INT" pad="32"/>
<connect gate="G$1" pin="LBEN" pad="18"/>
<connect gate="G$1" pin="MODE" pad="21"/>
<connect gate="G$1" pin="OR" pad="4"/>
<connect gate="G$1" pin="OSC-IN" pad="22"/>
<connect gate="G$1" pin="OSC-OUT" pad="23"/>
<connect gate="G$1" pin="OSC-SEL" pad="24"/>
<connect gate="G$1" pin="POL" pad="3"/>
<connect gate="G$1" pin="R/H" pad="26"/>
<connect gate="G$1" pin="REF-CAP+" pad="37"/>
<connect gate="G$1" pin="REF-CAP-" pad="38"/>
<connect gate="G$1" pin="REF-IN+" pad="36"/>
<connect gate="G$1" pin="REF-IN-" pad="39"/>
<connect gate="G$1" pin="REF-OUT" pad="29"/>
<connect gate="G$1" pin="SEND" pad="27"/>
<connect gate="G$1" pin="STATUS" pad="2"/>
<connect gate="G$1" pin="TEST" pad="17"/>
<connect gate="G$1" pin="V+" pad="40"/>
<connect gate="G$1" pin="V-" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7116CPL" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7116"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A/Z" pad="29"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="23"/>
<connect gate="G$1" pin="AB4" pad="19"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="BP/GND" pad="21"/>
<connect gate="G$1" pin="BUFF" pad="28"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="24"/>
<connect gate="G$1" pin="COMM" pad="32"/>
<connect gate="G$1" pin="CREF+" pad="34"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="14"/>
<connect gate="G$1" pin="E3" pad="18"/>
<connect gate="G$1" pin="F1" pad="6"/>
<connect gate="G$1" pin="F2" pad="13"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="25"/>
<connect gate="G$1" pin="G3" pad="22"/>
<connect gate="G$1" pin="HOLD" pad="1"/>
<connect gate="G$1" pin="IN-HI" pad="31"/>
<connect gate="G$1" pin="IN-LO" pad="30"/>
<connect gate="G$1" pin="INT" pad="27"/>
<connect gate="G$1" pin="OSC1" pad="40"/>
<connect gate="G$1" pin="OSC2" pad="39"/>
<connect gate="G$1" pin="OSC3" pad="38"/>
<connect gate="G$1" pin="POL" pad="20"/>
<connect gate="G$1" pin="REF-HI" pad="36"/>
<connect gate="G$1" pin="TEST" pad="37"/>
<connect gate="G$1" pin="V+" pad="35"/>
<connect gate="G$1" pin="V-" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7135CJI" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7135"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="ANA-COM" pad="3"/>
<connect gate="G$1" pin="AZ-IN" pad="5"/>
<connect gate="G$1" pin="B1" pad="13"/>
<connect gate="G$1" pin="B2" pad="14"/>
<connect gate="G$1" pin="B4" pad="15"/>
<connect gate="G$1" pin="B8" pad="16"/>
<connect gate="G$1" pin="BUFF-OUT" pad="6"/>
<connect gate="G$1" pin="BUSY" pad="21"/>
<connect gate="G$1" pin="CLK-IN" pad="22"/>
<connect gate="G$1" pin="D1" pad="20"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="DIGI-GND" pad="24"/>
<connect gate="G$1" pin="IN-HI" pad="10"/>
<connect gate="G$1" pin="IN-LO" pad="9"/>
<connect gate="G$1" pin="INT-OUT" pad="4"/>
<connect gate="G$1" pin="O/R" pad="27"/>
<connect gate="G$1" pin="POL" pad="23"/>
<connect gate="G$1" pin="R/H" pad="25"/>
<connect gate="G$1" pin="REF" pad="2"/>
<connect gate="G$1" pin="REFCAP+" pad="8"/>
<connect gate="G$1" pin="REFCAP-" pad="7"/>
<connect gate="G$1" pin="STROBE" pad="26"/>
<connect gate="G$1" pin="U/R" pad="28"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX565AJN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX565A"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="10V-SPAN" pad="10"/>
<connect gate="G$1" pin="20V-SPAN" pad="11"/>
<connect gate="G$1" pin="BIOFF-IN" pad="8"/>
<connect gate="G$1" pin="BIT1" pad="24"/>
<connect gate="G$1" pin="BIT10" pad="15"/>
<connect gate="G$1" pin="BIT11" pad="14"/>
<connect gate="G$1" pin="BIT12" pad="13"/>
<connect gate="G$1" pin="BIT2" pad="23"/>
<connect gate="G$1" pin="BIT3" pad="22"/>
<connect gate="G$1" pin="BIT4" pad="21"/>
<connect gate="G$1" pin="BIT5" pad="20"/>
<connect gate="G$1" pin="BIT6" pad="19"/>
<connect gate="G$1" pin="BIT7" pad="18"/>
<connect gate="G$1" pin="BIT8" pad="17"/>
<connect gate="G$1" pin="BIT9" pad="16"/>
<connect gate="G$1" pin="DAC-OUT" pad="9"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="REF-GND" pad="5"/>
<connect gate="G$1" pin="REF-IN" pad="6"/>
<connect gate="G$1" pin="REF-OUT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VEE" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7224KN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7224"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="CS" pad="14"/>
<connect gate="G$1" pin="DB0" pad="13"/>
<connect gate="G$1" pin="DB1" pad="12"/>
<connect gate="G$1" pin="DB2" pad="11"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="9"/>
<connect gate="G$1" pin="DB5" pad="8"/>
<connect gate="G$1" pin="DB6" pad="7"/>
<connect gate="G$1" pin="DB7" pad="6"/>
<connect gate="G$1" pin="DGND" pad="5"/>
<connect gate="G$1" pin="LDAC" pad="16"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="V-OUT" pad="2"/>
<connect gate="G$1" pin="V-REF" pad="3"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="WR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7225KN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7225"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="A0" pad="19"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="DB0" pad="16"/>
<connect gate="G$1" pin="DB1" pad="15"/>
<connect gate="G$1" pin="DB2" pad="14"/>
<connect gate="G$1" pin="DB3" pad="13"/>
<connect gate="G$1" pin="DB4" pad="12"/>
<connect gate="G$1" pin="DB5" pad="11"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="9"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="LDAC" pad="8"/>
<connect gate="G$1" pin="VDD" pad="22"/>
<connect gate="G$1" pin="VOUT-A" pad="2"/>
<connect gate="G$1" pin="VOUT-B" pad="1"/>
<connect gate="G$1" pin="VOUT-C" pad="24"/>
<connect gate="G$1" pin="VOUT-D" pad="23"/>
<connect gate="G$1" pin="VREF-A" pad="5"/>
<connect gate="G$1" pin="VREF-B" pad="4"/>
<connect gate="G$1" pin="VREF-C" pad="21"/>
<connect gate="G$1" pin="VREF-D" pad="20"/>
<connect gate="G$1" pin="VSS" pad="3"/>
<connect gate="G$1" pin="WR" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7520JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7520"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="BIT1" pad="4"/>
<connect gate="G$1" pin="BIT10" pad="13"/>
<connect gate="G$1" pin="BIT2" pad="5"/>
<connect gate="G$1" pin="BIT3" pad="6"/>
<connect gate="G$1" pin="BIT4" pad="7"/>
<connect gate="G$1" pin="BIT5" pad="8"/>
<connect gate="G$1" pin="BIT6" pad="9"/>
<connect gate="G$1" pin="BIT7" pad="10"/>
<connect gate="G$1" pin="BIT8" pad="11"/>
<connect gate="G$1" pin="BIT9" pad="12"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7523JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7523"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="BIT1" pad="4"/>
<connect gate="G$1" pin="BIT2" pad="5"/>
<connect gate="G$1" pin="BIT3" pad="6"/>
<connect gate="G$1" pin="BIT4" pad="7"/>
<connect gate="G$1" pin="BIT5" pad="8"/>
<connect gate="G$1" pin="BIT6" pad="9"/>
<connect gate="G$1" pin="BIT7" pad="10"/>
<connect gate="G$1" pin="BIT8" pad="11"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7524JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7524"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="DB0" pad="11"/>
<connect gate="G$1" pin="DB1" pad="10"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="8"/>
<connect gate="G$1" pin="DB4" pad="7"/>
<connect gate="G$1" pin="DB5" pad="6"/>
<connect gate="G$1" pin="DB6" pad="5"/>
<connect gate="G$1" pin="DB7" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
<connect gate="G$1" pin="WR" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7528JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7528"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="CS" pad="15"/>
<connect gate="G$1" pin="DAA/DAB" pad="6"/>
<connect gate="G$1" pin="DB0" pad="14"/>
<connect gate="G$1" pin="DB1" pad="13"/>
<connect gate="G$1" pin="DB2" pad="12"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="DB4" pad="10"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="8"/>
<connect gate="G$1" pin="DB7" pad="7"/>
<connect gate="G$1" pin="DGND" pad="5"/>
<connect gate="G$1" pin="OUT-A" pad="2"/>
<connect gate="G$1" pin="OUT-B" pad="20"/>
<connect gate="G$1" pin="RFB-A" pad="3"/>
<connect gate="G$1" pin="RFB-B" pad="19"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VREF-A" pad="4"/>
<connect gate="G$1" pin="VREF-B" pad="18"/>
<connect gate="G$1" pin="WR" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7530JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7530"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="BIT1" pad="4"/>
<connect gate="G$1" pin="BIT10" pad="13"/>
<connect gate="G$1" pin="BIT2" pad="5"/>
<connect gate="G$1" pin="BIT3" pad="6"/>
<connect gate="G$1" pin="BIT4" pad="7"/>
<connect gate="G$1" pin="BIT5" pad="8"/>
<connect gate="G$1" pin="BIT6" pad="9"/>
<connect gate="G$1" pin="BIT7" pad="10"/>
<connect gate="G$1" pin="BIT8" pad="11"/>
<connect gate="G$1" pin="BIT9" pad="12"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT-1" pad="1"/>
<connect gate="G$1" pin="OUT-2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7531JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7531"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="BIT1" pad="4"/>
<connect gate="G$1" pin="BIT10" pad="13"/>
<connect gate="G$1" pin="BIT11" pad="14"/>
<connect gate="G$1" pin="BIT12" pad="15"/>
<connect gate="G$1" pin="BIT2" pad="5"/>
<connect gate="G$1" pin="BIT3" pad="6"/>
<connect gate="G$1" pin="BIT4" pad="7"/>
<connect gate="G$1" pin="BIT5" pad="8"/>
<connect gate="G$1" pin="BIT6" pad="9"/>
<connect gate="G$1" pin="BIT7" pad="10"/>
<connect gate="G$1" pin="BIT8" pad="11"/>
<connect gate="G$1" pin="BIT9" pad="12"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT-1" pad="1"/>
<connect gate="G$1" pin="OUT-2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="18"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7542JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7542"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="CLR" pad="13"/>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="D0" pad="7"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="D2" pad="5"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="OUT-1" pad="1"/>
<connect gate="G$1" pin="OUT-2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
<connect gate="G$1" pin="WR" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7543JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7543"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="CLR" pad="13"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="LD1" pad="5"/>
<connect gate="G$1" pin="LD2" pad="9"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="OUT-1" pad="1"/>
<connect gate="G$1" pin="OUT-2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="SRI" pad="7"/>
<connect gate="G$1" pin="STB1" pad="4"/>
<connect gate="G$1" pin="STB2" pad="8"/>
<connect gate="G$1" pin="STB3" pad="10"/>
<connect gate="G$1" pin="STB4" pad="11"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX7545JN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX7545"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="CS" pad="16"/>
<connect gate="G$1" pin="DB0" pad="15"/>
<connect gate="G$1" pin="DB1" pad="14"/>
<connect gate="G$1" pin="DB10" pad="5"/>
<connect gate="G$1" pin="DB11" pad="4"/>
<connect gate="G$1" pin="DB2" pad="13"/>
<connect gate="G$1" pin="DB3" pad="12"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="10"/>
<connect gate="G$1" pin="DB6" pad="9"/>
<connect gate="G$1" pin="DB7" pad="8"/>
<connect gate="G$1" pin="DB8" pad="7"/>
<connect gate="G$1" pin="DB9" pad="6"/>
<connect gate="G$1" pin="DGND" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="RFB" pad="20"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VREF" pad="19"/>
<connect gate="G$1" pin="WR" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX670CDD" prefix="IC">
<description>&lt;b&gt;VOLATAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX670"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+15V" pad="11"/>
<connect gate="G$1" pin="FADJ" pad="12"/>
<connect gate="G$1" pin="FADJ@1" pad="14"/>
<connect gate="G$1" pin="GND-F" pad="5"/>
<connect gate="G$1" pin="GND-S1" pad="6"/>
<connect gate="G$1" pin="GND-S2" pad="7"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="NC@2" pad="9"/>
<connect gate="G$1" pin="OADJ" pad="3"/>
<connect gate="G$1" pin="OUT-F" pad="13"/>
<connect gate="G$1" pin="TP" pad="10"/>
<connect gate="G$1" pin="VOUT-S1" pad="1"/>
<connect gate="G$1" pin="VOUT-S2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX672CPA" prefix="IC">
<description>&lt;b&gt;VOLATAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX672"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="NC@3" pad="8"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX580JCSA" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX580CS"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+2,5V" pad="1"/>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="5"/>
<connect gate="G$1" pin="NC@3" pad="6"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX580KH" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX580H"/>
</gates>
<devices>
<device name="" package="TO52A">
<connects>
<connect gate="G$1" pin="+VS" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX584JN" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX584N"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="10,0V" pad="1"/>
<connect gate="G$1" pin="2,5V" pad="3"/>
<connect gate="G$1" pin="5,0V" pad="2"/>
<connect gate="G$1" pin="CAP" pad="7"/>
<connect gate="G$1" pin="COMMON" pad="4"/>
<connect gate="G$1" pin="STROBE" pad="5"/>
<connect gate="G$1" pin="VBG" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX2700JD" prefix="IC">
<description>&lt;b&gt;RECEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX2700"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+15V" pad="11"/>
<connect gate="G$1" pin="10V-OUT" pad="13"/>
<connect gate="G$1" pin="FADJ" pad="12"/>
<connect gate="G$1" pin="FADJ@1" pad="14"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="NC@3" pad="4"/>
<connect gate="G$1" pin="NC@4" pad="5"/>
<connect gate="G$1" pin="NC@5" pad="6"/>
<connect gate="G$1" pin="NC@6" pad="8"/>
<connect gate="G$1" pin="NC@7" pad="9"/>
<connect gate="G$1" pin="TP" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX2701JD" prefix="IC">
<description>&lt;b&gt;RECEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX2701"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="-10V-OUT" pad="13"/>
<connect gate="G$1" pin="-15V" pad="11"/>
<connect gate="G$1" pin="FADJ" pad="12"/>
<connect gate="G$1" pin="FADJ@1" pad="14"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="NC@3" pad="4"/>
<connect gate="G$1" pin="NC@4" pad="5"/>
<connect gate="G$1" pin="NC@5" pad="6"/>
<connect gate="G$1" pin="NC@6" pad="8"/>
<connect gate="G$1" pin="NC@7" pad="9"/>
<connect gate="G$1" pin="TP" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF01HP" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="REF01"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="NC@3" pad="8"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="V-IN" pad="2"/>
<connect gate="G$1" pin="V-OUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF02HCSA" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="REF02"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="7"/>
<connect gate="G$1" pin="NC@2" pad="8"/>
<connect gate="G$1" pin="TEMP" pad="3"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="V-IN" pad="2"/>
<connect gate="G$1" pin="V-OUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX536AJN" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MX536A"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+VS" pad="14"/>
<connect gate="G$1" pin="-VS" pad="3"/>
<connect gate="G$1" pin="BUF-IN" pad="7"/>
<connect gate="G$1" pin="BUF-OUT" pad="6"/>
<connect gate="G$1" pin="CAV" pad="4"/>
<connect gate="G$1" pin="COMM" pad="10"/>
<connect gate="G$1" pin="DB" pad="5"/>
<connect gate="G$1" pin="I-OUT" pad="8"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="11"/>
<connect gate="G$1" pin="NC@2" pad="12"/>
<connect gate="G$1" pin="NC@3" pad="13"/>
<connect gate="G$1" pin="RL" pad="9"/>
<connect gate="G$1" pin="V-IN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX400MJA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX400"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VOS" pad="1"/>
<connect gate="G$1" pin="VOS@1" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX420CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX420"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CEXTA" pad="1"/>
<connect gate="G$1" pin="CEXTB" pad="8"/>
<connect gate="G$1" pin="CRETN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX421EPD" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX421"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CEXTA" pad="2"/>
<connect gate="G$1" pin="CEXTB" pad="1"/>
<connect gate="G$1" pin="CLK-IN" pad="13"/>
<connect gate="G$1" pin="CLK-OUT" pad="12"/>
<connect gate="G$1" pin="CRETN" pad="8"/>
<connect gate="G$1" pin="IN+" pad="5"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="INT/EXT" pad="14"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="OUT-CLP" pad="9"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX430CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP2NC"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="5"/>
<connect gate="G$1" pin="NC@2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX450CPD" prefix="IC">
<description>&lt;b&gt;VIDEO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX450"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="14"/>
<connect gate="G$1" pin="BIAS-ADJ" pad="5"/>
<connect gate="G$1" pin="FCOMP" pad="4"/>
<connect gate="G$1" pin="FCOMP@1" pad="6"/>
<connect gate="G$1" pin="FCOMP@2" pad="9"/>
<connect gate="G$1" pin="FCOMP@3" pad="11"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="7"/>
<connect gate="G$1" pin="NC@2" pad="12"/>
<connect gate="G$1" pin="NC@3" pad="13"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX452CPA" prefix="IC">
<description>&lt;b&gt;VIDEO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP2NC"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="7"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@2" pad="4"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX453EPA" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX453"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="-IN" pad="7"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN0" pad="4"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX454CPD" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX454"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="-IN" pad="13"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN0" pad="7"/>
<connect gate="G$1" pin="IN1" pad="8"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="IN3" pad="11"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="9"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="V+" pad="12"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX454CSD" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX454"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="-IN" pad="13"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN0" pad="7"/>
<connect gate="G$1" pin="IN1" pad="8"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="IN3" pad="11"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="9"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="V+" pad="12"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX455CPP" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX455"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="-IN" pad="19"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN0" pad="5"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="IN5" pad="13"/>
<connect gate="G$1" pin="IN6" pad="15"/>
<connect gate="G$1" pin="IN7" pad="17"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="NC@3" pad="16"/>
<connect gate="G$1" pin="OUT" pad="20"/>
<connect gate="G$1" pin="V+" pad="18"/>
<connect gate="G$1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7621" prefix="IC">
<description>&lt;b&gt;Dual Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/ICL7612-ICL764X.pdf</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
<gate name="B" symbol="OPAMP"/>
</gates>
<devices>
<device name="PA" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TV" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SA" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7622" prefix="IC">
<description>&lt;b&gt;Dual Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/ICL7612-ICL764X.pdf</description>
<gates>
<gate name="A" symbol="OPOFF+NC"/>
<gate name="P" symbol="2V+V-"/>
<gate name="B" symbol="OPOFF"/>
</gates>
<devices>
<device name="PD" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="OFF1" pad="3"/>
<connect gate="A" pin="OFF2" pad="14"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OFF1" pad="5"/>
<connect gate="B" pin="OFF2" pad="8"/>
<connect gate="B" pin="OUT" pad="10"/>
<connect gate="P" pin="V+" pad="9"/>
<connect gate="P" pin="V+@1" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SA" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="OFF1" pad="3"/>
<connect gate="A" pin="OFF2" pad="14"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OFF1" pad="5"/>
<connect gate="B" pin="OFF2" pad="8"/>
<connect gate="B" pin="OUT" pad="10"/>
<connect gate="P" pin="V+" pad="9"/>
<connect gate="P" pin="V+@1" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7650CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7650"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CEXTA" pad="1"/>
<connect gate="G$1" pin="CEXTB" pad="8"/>
<connect gate="G$1" pin="CRETN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7650CPD" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7650/"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="CEXTA" pad="2"/>
<connect gate="G$1" pin="CEXTB" pad="1"/>
<connect gate="G$1" pin="CLK-IN" pad="13"/>
<connect gate="G$1" pin="CLK-OUT" pad="12"/>
<connect gate="G$1" pin="CRETN" pad="8"/>
<connect gate="G$1" pin="INT/EXT" pad="14"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="OUT-CLP" pad="9"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX600LPA" prefix="IC">
<description>&lt;b&gt;AC-DC REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX600"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="AC1" pad="7"/>
<connect gate="G$1" pin="AC2" pad="1"/>
<connect gate="G$1" pin="OUV" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
<connect gate="G$1" pin="VSENSE" pad="5"/>
<connect gate="G$1" pin="VSET" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX601LPA" prefix="IC">
<description>&lt;b&gt;AC-DC REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX601"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="AC1" pad="7"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="OUV" pad="3"/>
<connect gate="G$1" pin="RD" pad="4"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
<connect gate="G$1" pin="VSENSE" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX630CPA" prefix="IC">
<description>Step-up &lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX630"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="5"/>
<connect gate="G$1" pin="CX" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IC" pad="6"/>
<connect gate="G$1" pin="LBD" pad="8"/>
<connect gate="G$1" pin="LBR" pad="1"/>
<connect gate="G$1" pin="LX" pad="3"/>
<connect gate="G$1" pin="VFB" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4193SA" prefix="IC">
<description>Step-up &lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX630"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+VS" pad="5"/>
<connect gate="G$1" pin="CX" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IC" pad="6"/>
<connect gate="G$1" pin="LBD" pad="8"/>
<connect gate="G$1" pin="LBR" pad="1"/>
<connect gate="G$1" pin="LX" pad="3"/>
<connect gate="G$1" pin="VFB" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX631CPA" prefix="IC">
<description>Step-up &lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX631"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="CP" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LBI" pad="1"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="4"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX634CPA" prefix="IC">
<description>&lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX634"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="CX" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBD" pad="2"/>
<connect gate="G$1" pin="LBR" pad="1"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="VFB" pad="8"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX634CSA" prefix="IC">
<description>&lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX634"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="CX" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBD" pad="2"/>
<connect gate="G$1" pin="LBR" pad="1"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="VFB" pad="8"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX635CPA" prefix="IC">
<description>&lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX635"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="-VOUT" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="VFB" pad="8"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX635CSA" prefix="IC">
<description>&lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX635"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="-VOUT" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="VFB" pad="8"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX638CPA" prefix="IC">
<description>Step-down &lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX638"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX638CSA" prefix="IC">
<description>Step-down &lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX638"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX641CPA" prefix="IC">
<description>Step-up &lt;b&gt;SWITCHING REGULATOR CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX641"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="EXT" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LBI" pad="1"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="4"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX641CSA" prefix="IC">
<description>Step-up &lt;b&gt;SWITCHING REGULATOR CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX641"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="EXT" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LBI" pad="1"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="4"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX663CPA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX663"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="VIN(POS)" pad="8"/>
<connect gate="G$1" pin="VOUT1" pad="3"/>
<connect gate="G$1" pin="VOUT2" pad="2"/>
<connect gate="G$1" pin="VSET" pad="6"/>
<connect gate="G$1" pin="VTC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX663CSA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX663"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="VIN(POS)" pad="8"/>
<connect gate="G$1" pin="VOUT1" pad="3"/>
<connect gate="G$1" pin="VOUT2" pad="2"/>
<connect gate="G$1" pin="VSET" pad="6"/>
<connect gate="G$1" pin="VTC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX664CPA" prefix="IC">
<description>Negative &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX664"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="SHDN@1" pad="5"/>
<connect gate="G$1" pin="VIN(NEG)" pad="4"/>
<connect gate="G$1" pin="VOUT1" pad="7"/>
<connect gate="G$1" pin="VOUT2" pad="1"/>
<connect gate="G$1" pin="VSET" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX664CSA" prefix="IC">
<description>Negative &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX664"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="SHDN@1" pad="5"/>
<connect gate="G$1" pin="VIN(NEG)" pad="4"/>
<connect gate="G$1" pin="VOUT1" pad="7"/>
<connect gate="G$1" pin="VOUT2" pad="1"/>
<connect gate="G$1" pin="VSET" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX666CPA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX666"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="VIN(POS)" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="VSET" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX666CSA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX666"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="VIN(POS)" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="VSET" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX680CPA" prefix="IC">
<description>Switched-capcitor &lt;b&gt;VOLTAGE CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX680"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="C1+" pad="7"/>
<connect gate="G$1" pin="C1-" pad="1"/>
<connect gate="G$1" pin="C2+" pad="2"/>
<connect gate="G$1" pin="C2-" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX680CSA" prefix="IC">
<description>Switched-capcitor &lt;b&gt;VOLTAGE CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX680"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="C1+" pad="7"/>
<connect gate="G$1" pin="C1-" pad="1"/>
<connect gate="G$1" pin="C2+" pad="2"/>
<connect gate="G$1" pin="C2-" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX690ACPA" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX690"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VBATT" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="G$1" pin="WDI" pad="6"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX691ACPE" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX691"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="BATT-ON" pad="5"/>
<connect gate="G$1" pin="CE-IN" pad="13"/>
<connect gate="G$1" pin="CE-OUT" pad="12"/>
<connect gate="G$1" pin="LOW-LINE" pad="6"/>
<connect gate="G$1" pin="OSC-IN" pad="7"/>
<connect gate="G$1" pin="OSC-SEL" pad="8"/>
<connect gate="G$1" pin="PFI" pad="9"/>
<connect gate="G$1" pin="PFO" pad="10"/>
<connect gate="G$1" pin="RESET" pad="16"/>
<connect gate="G$1" pin="RESET@" pad="15"/>
<connect gate="G$1" pin="VBATT" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="WDI" pad="11"/>
<connect gate="G$1" pin="WDO" pad="14"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX696CPE" prefix="IC">
<description>&lt;b&gt;SUPERVISORY CIRCUIT&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX696"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="BATT-ON" pad="5"/>
<connect gate="G$1" pin="LLIN" pad="13"/>
<connect gate="G$1" pin="LOW-LINE" pad="6"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="OSC-IN" pad="7"/>
<connect gate="G$1" pin="OSC-SEL" pad="8"/>
<connect gate="G$1" pin="PFI" pad="9"/>
<connect gate="G$1" pin="PFO" pad="10"/>
<connect gate="G$1" pin="RESET" pad="16"/>
<connect gate="G$1" pin="RESET@" pad="15"/>
<connect gate="G$1" pin="VBATT" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="WDI" pad="11"/>
<connect gate="G$1" pin="WDO" pad="14"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX697CPE" prefix="IC">
<description>&lt;b&gt;SUPERVISORY CIRCUIT&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX697"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="CE-IN" pad="13"/>
<connect gate="G$1" pin="CE-OUT" pad="12"/>
<connect gate="G$1" pin="LLIN" pad="4"/>
<connect gate="G$1" pin="LOW-LINE" pad="6"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="OSC-IN" pad="7"/>
<connect gate="G$1" pin="OSC-SEL" pad="8"/>
<connect gate="G$1" pin="PFI" pad="9"/>
<connect gate="G$1" pin="PFO" pad="10"/>
<connect gate="G$1" pin="RESET" pad="16"/>
<connect gate="G$1" pin="RESET@" pad="15"/>
<connect gate="G$1" pin="TEST" pad="1"/>
<connect gate="G$1" pin="WDI" pad="11"/>
<connect gate="G$1" pin="WDO" pad="14"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX8211CP" prefix="IC">
<description>&lt;b&gt;VOLTAGE MONITOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX8211"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="HYSTER" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="THRESH" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX8211CS" prefix="IC">
<description>&lt;b&gt;VOLTAGE MONITOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX8211"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="HYSTER" pad="2"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="THRESH" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7660CPA" prefix="IC">
<description>&lt;b&gt;VOLTAGE CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7660"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LV" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7660CSA" prefix="IC">
<description>&lt;b&gt;VOLTAGE CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7660"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LV" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7663CPA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7663"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VSET" pad="6"/>
<connect gate="G$1" pin="VTC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7663CSA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7663"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VSET" pad="6"/>
<connect gate="G$1" pin="VTC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7664CPA" prefix="IC">
<description>Negative &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7664"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT2" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="SHDN@1" pad="5"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VSET" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7664CSA" prefix="IC">
<description>Negative &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7664"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT2" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="SHDN@1" pad="5"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VSET" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7665CPA" prefix="IC">
<description>&lt;b&gt;UNDER/OVER VOLTAGE DETECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7665"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HYST1" pad="2"/>
<connect gate="G$1" pin="HYST2" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="SET1" pad="3"/>
<connect gate="G$1" pin="SET2" pad="6"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7665CSA" prefix="IC">
<description>&lt;b&gt;UNDER/OVER VOLTAGE DETECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7665"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HYST1" pad="2"/>
<connect gate="G$1" pin="HYST2" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="SET1" pad="3"/>
<connect gate="G$1" pin="SET2" pad="6"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7231PL" prefix="IC">
<description>&lt;b&gt;LCD DISPLAY DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX7231"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="1X" pad="8"/>
<connect gate="G$1" pin="1Y" pad="7"/>
<connect gate="G$1" pin="1Z" pad="6"/>
<connect gate="G$1" pin="2X" pad="11"/>
<connect gate="G$1" pin="2Y" pad="10"/>
<connect gate="G$1" pin="2Z" pad="9"/>
<connect gate="G$1" pin="3X" pad="14"/>
<connect gate="G$1" pin="3Y" pad="13"/>
<connect gate="G$1" pin="3Z" pad="12"/>
<connect gate="G$1" pin="4X" pad="17"/>
<connect gate="G$1" pin="4Y" pad="16"/>
<connect gate="G$1" pin="4Z" pad="15"/>
<connect gate="G$1" pin="5X" pad="20"/>
<connect gate="G$1" pin="5Y" pad="19"/>
<connect gate="G$1" pin="5Z" pad="18"/>
<connect gate="G$1" pin="6X" pad="23"/>
<connect gate="G$1" pin="6Y" pad="22"/>
<connect gate="G$1" pin="6Z" pad="21"/>
<connect gate="G$1" pin="7X" pad="26"/>
<connect gate="G$1" pin="7Y" pad="25"/>
<connect gate="G$1" pin="7Z" pad="24"/>
<connect gate="G$1" pin="8X" pad="29"/>
<connect gate="G$1" pin="8Y" pad="28"/>
<connect gate="G$1" pin="8Z" pad="27"/>
<connect gate="G$1" pin="A0" pad="37"/>
<connect gate="G$1" pin="A1" pad="38"/>
<connect gate="G$1" pin="A2" pad="39"/>
<connect gate="G$1" pin="AN1" pad="30"/>
<connect gate="G$1" pin="AN2" pad="31"/>
<connect gate="G$1" pin="BD0" pad="32"/>
<connect gate="G$1" pin="BD1" pad="33"/>
<connect gate="G$1" pin="BD2" pad="34"/>
<connect gate="G$1" pin="BD3" pad="35"/>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="4"/>
<connect gate="G$1" pin="COM3" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="36"/>
<connect gate="G$1" pin="V+" pad="40"/>
<connect gate="G$1" pin="VDISP" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7232PL" prefix="IC">
<description>&lt;b&gt;LCD DISPLAY DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX7232"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="10X" pad="35"/>
<connect gate="G$1" pin="10Y" pad="34"/>
<connect gate="G$1" pin="10Z" pad="33"/>
<connect gate="G$1" pin="1X" pad="8"/>
<connect gate="G$1" pin="1Y" pad="7"/>
<connect gate="G$1" pin="1Z" pad="6"/>
<connect gate="G$1" pin="2X" pad="11"/>
<connect gate="G$1" pin="2Y" pad="10"/>
<connect gate="G$1" pin="2Z" pad="9"/>
<connect gate="G$1" pin="3X" pad="14"/>
<connect gate="G$1" pin="3Y" pad="13"/>
<connect gate="G$1" pin="3Z" pad="12"/>
<connect gate="G$1" pin="4X" pad="17"/>
<connect gate="G$1" pin="4Y" pad="16"/>
<connect gate="G$1" pin="4Z" pad="15"/>
<connect gate="G$1" pin="5X" pad="20"/>
<connect gate="G$1" pin="5Y" pad="19"/>
<connect gate="G$1" pin="5Z" pad="18"/>
<connect gate="G$1" pin="6X" pad="23"/>
<connect gate="G$1" pin="6Y" pad="22"/>
<connect gate="G$1" pin="6Z" pad="21"/>
<connect gate="G$1" pin="7X" pad="26"/>
<connect gate="G$1" pin="7Y" pad="25"/>
<connect gate="G$1" pin="7Z" pad="24"/>
<connect gate="G$1" pin="8X" pad="29"/>
<connect gate="G$1" pin="8Y" pad="28"/>
<connect gate="G$1" pin="8Z" pad="27"/>
<connect gate="G$1" pin="9X" pad="32"/>
<connect gate="G$1" pin="9Y" pad="31"/>
<connect gate="G$1" pin="9Z" pad="30"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="4"/>
<connect gate="G$1" pin="COM3" pad="5"/>
<connect gate="G$1" pin="DATA" pad="38"/>
<connect gate="G$1" pin="DATAACC" pad="37"/>
<connect gate="G$1" pin="GND" pad="36"/>
<connect gate="G$1" pin="V+" pad="40"/>
<connect gate="G$1" pin="VDISP" pad="2"/>
<connect gate="G$1" pin="WR" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7233PL" prefix="IC">
<description>&lt;b&gt;LCD DISPLAY DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX7233"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="1U" pad="11"/>
<connect gate="G$1" pin="1V" pad="10"/>
<connect gate="G$1" pin="1W" pad="9"/>
<connect gate="G$1" pin="1X" pad="8"/>
<connect gate="G$1" pin="1Y" pad="7"/>
<connect gate="G$1" pin="1Z" pad="6"/>
<connect gate="G$1" pin="2U" pad="17"/>
<connect gate="G$1" pin="2V" pad="16"/>
<connect gate="G$1" pin="2W" pad="15"/>
<connect gate="G$1" pin="2X" pad="14"/>
<connect gate="G$1" pin="2Y" pad="13"/>
<connect gate="G$1" pin="2Z" pad="12"/>
<connect gate="G$1" pin="3U" pad="23"/>
<connect gate="G$1" pin="3V" pad="22"/>
<connect gate="G$1" pin="3W" pad="21"/>
<connect gate="G$1" pin="3X" pad="20"/>
<connect gate="G$1" pin="3Y" pad="19"/>
<connect gate="G$1" pin="3Z" pad="18"/>
<connect gate="G$1" pin="4U" pad="29"/>
<connect gate="G$1" pin="4V" pad="28"/>
<connect gate="G$1" pin="4W" pad="27"/>
<connect gate="G$1" pin="4X" pad="26"/>
<connect gate="G$1" pin="4Y" pad="25"/>
<connect gate="G$1" pin="4Z" pad="24"/>
<connect gate="G$1" pin="A0" pad="37"/>
<connect gate="G$1" pin="A1" pad="38"/>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="4"/>
<connect gate="G$1" pin="COM3" pad="5"/>
<connect gate="G$1" pin="CS1" pad="1"/>
<connect gate="G$1" pin="CS2" pad="39"/>
<connect gate="G$1" pin="D0" pad="30"/>
<connect gate="G$1" pin="D1" pad="31"/>
<connect gate="G$1" pin="D2" pad="32"/>
<connect gate="G$1" pin="D3" pad="33"/>
<connect gate="G$1" pin="D4" pad="34"/>
<connect gate="G$1" pin="D5" pad="35"/>
<connect gate="G$1" pin="GND" pad="36"/>
<connect gate="G$1" pin="V+" pad="40"/>
<connect gate="G$1" pin="VDISP" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7234PL" prefix="IC">
<description>&lt;b&gt;LCD DISPLAY DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX7234"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="1U" pad="11"/>
<connect gate="G$1" pin="1V" pad="10"/>
<connect gate="G$1" pin="1W" pad="9"/>
<connect gate="G$1" pin="1X" pad="8"/>
<connect gate="G$1" pin="1Y" pad="7"/>
<connect gate="G$1" pin="1Z" pad="6"/>
<connect gate="G$1" pin="2U" pad="17"/>
<connect gate="G$1" pin="2V" pad="16"/>
<connect gate="G$1" pin="2W" pad="15"/>
<connect gate="G$1" pin="2X" pad="14"/>
<connect gate="G$1" pin="2Y" pad="13"/>
<connect gate="G$1" pin="2Z" pad="12"/>
<connect gate="G$1" pin="3U" pad="23"/>
<connect gate="G$1" pin="3V" pad="22"/>
<connect gate="G$1" pin="3W" pad="21"/>
<connect gate="G$1" pin="3X" pad="20"/>
<connect gate="G$1" pin="3Y" pad="19"/>
<connect gate="G$1" pin="3Z" pad="18"/>
<connect gate="G$1" pin="4U" pad="29"/>
<connect gate="G$1" pin="4V" pad="28"/>
<connect gate="G$1" pin="4W" pad="27"/>
<connect gate="G$1" pin="4X" pad="26"/>
<connect gate="G$1" pin="4Y" pad="25"/>
<connect gate="G$1" pin="4Z" pad="24"/>
<connect gate="G$1" pin="5U" pad="35"/>
<connect gate="G$1" pin="5V" pad="34"/>
<connect gate="G$1" pin="5W" pad="33"/>
<connect gate="G$1" pin="5X" pad="32"/>
<connect gate="G$1" pin="5Y" pad="31"/>
<connect gate="G$1" pin="5Z" pad="30"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="4"/>
<connect gate="G$1" pin="COM3" pad="5"/>
<connect gate="G$1" pin="DATA" pad="38"/>
<connect gate="G$1" pin="DATAACC" pad="37"/>
<connect gate="G$1" pin="GND" pad="36"/>
<connect gate="G$1" pin="V+" pad="40"/>
<connect gate="G$1" pin="VDISP" pad="2"/>
<connect gate="G$1" pin="WR" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7211PL" prefix="IC">
<description>&lt;b&gt;LCD DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7211"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A1" pad="37"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="13"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="B0-IN" pad="27"/>
<connect gate="G$1" pin="B1" pad="38"/>
<connect gate="G$1" pin="B1-IN" pad="28"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B2-IN" pad="29"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="B3-IN" pad="30"/>
<connect gate="G$1" pin="B4" pad="21"/>
<connect gate="G$1" pin="BP" pad="5"/>
<connect gate="G$1" pin="C1" pad="39"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="15"/>
<connect gate="G$1" pin="C4" pad="22"/>
<connect gate="G$1" pin="D1" pad="40"/>
<connect gate="G$1" pin="D1-IN" pad="31"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D2-IN" pad="32"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D3-IN" pad="33"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="D4-IN" pad="34"/>
<connect gate="G$1" pin="E1" pad="2"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="E3" pad="17"/>
<connect gate="G$1" pin="E4" pad="24"/>
<connect gate="G$1" pin="F1" pad="4"/>
<connect gate="G$1" pin="F2" pad="12"/>
<connect gate="G$1" pin="F3" pad="19"/>
<connect gate="G$1" pin="F4" pad="26"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="18"/>
<connect gate="G$1" pin="G4" pad="25"/>
<connect gate="G$1" pin="GND" pad="35"/>
<connect gate="G$1" pin="OSC" pad="36"/>
<connect gate="G$1" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7211M" prefix="IC">
<description>&lt;b&gt;LCD DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7211M"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A1" pad="37"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="13"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="B0-IN" pad="27"/>
<connect gate="G$1" pin="B1" pad="38"/>
<connect gate="G$1" pin="B1-IN" pad="28"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B2-IN" pad="29"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="B3-IN" pad="30"/>
<connect gate="G$1" pin="B4" pad="21"/>
<connect gate="G$1" pin="BP" pad="5"/>
<connect gate="G$1" pin="C1" pad="39"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="15"/>
<connect gate="G$1" pin="C4" pad="22"/>
<connect gate="G$1" pin="CS1" pad="33"/>
<connect gate="G$1" pin="CS2" pad="34"/>
<connect gate="G$1" pin="D1" pad="40"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="DIGSEL1" pad="31"/>
<connect gate="G$1" pin="DIGSEL2" pad="32"/>
<connect gate="G$1" pin="E1" pad="2"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="E3" pad="17"/>
<connect gate="G$1" pin="E4" pad="24"/>
<connect gate="G$1" pin="F1" pad="4"/>
<connect gate="G$1" pin="F2" pad="12"/>
<connect gate="G$1" pin="F3" pad="19"/>
<connect gate="G$1" pin="F4" pad="26"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="18"/>
<connect gate="G$1" pin="G4" pad="25"/>
<connect gate="G$1" pin="GND" pad="35"/>
<connect gate="G$1" pin="OSC" pad="36"/>
<connect gate="G$1" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7212M" prefix="IC">
<description>&lt;b&gt;LCD DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7212M"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A1" pad="37"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="13"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="B0-IN" pad="27"/>
<connect gate="G$1" pin="B1" pad="38"/>
<connect gate="G$1" pin="B1-IN" pad="28"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B2-IN" pad="29"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="B3-IN" pad="30"/>
<connect gate="G$1" pin="B4" pad="21"/>
<connect gate="G$1" pin="BRT" pad="5"/>
<connect gate="G$1" pin="C1" pad="39"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="15"/>
<connect gate="G$1" pin="C4" pad="22"/>
<connect gate="G$1" pin="CS1" pad="33"/>
<connect gate="G$1" pin="CS2" pad="34"/>
<connect gate="G$1" pin="D1" pad="40"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="DIGSEL1" pad="31"/>
<connect gate="G$1" pin="DIGSEL2" pad="32"/>
<connect gate="G$1" pin="E1" pad="2"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="E3" pad="17"/>
<connect gate="G$1" pin="E4" pad="24"/>
<connect gate="G$1" pin="F1" pad="4"/>
<connect gate="G$1" pin="F2" pad="12"/>
<connect gate="G$1" pin="F3" pad="19"/>
<connect gate="G$1" pin="F4" pad="26"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="18"/>
<connect gate="G$1" pin="G4" pad="25"/>
<connect gate="G$1" pin="GND" pad="35"/>
<connect gate="G$1" pin="GND@1" pad="36"/>
<connect gate="G$1" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7217" prefix="IC">
<description>&lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7217A"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="BCD1S" pad="7"/>
<connect gate="G$1" pin="BCD2S" pad="6"/>
<connect gate="G$1" pin="BCD4S" pad="5"/>
<connect gate="G$1" pin="BCD8S" pad="4"/>
<connect gate="G$1" pin="C-OUT" pad="8"/>
<connect gate="G$1" pin="C/B" pad="1"/>
<connect gate="G$1" pin="D1" pad="28"/>
<connect gate="G$1" pin="D2" pad="27"/>
<connect gate="G$1" pin="D3" pad="26"/>
<connect gate="G$1" pin="D4" pad="25"/>
<connect gate="G$1" pin="DISP-CON" pad="23"/>
<connect gate="G$1" pin="EQUAL" pad="3"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="LC/OFF" pad="12"/>
<connect gate="G$1" pin="LR/OFF" pad="11"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="SCAN" pad="13"/>
<connect gate="G$1" pin="SEG-A" pad="16"/>
<connect gate="G$1" pin="SEG-B" pad="21"/>
<connect gate="G$1" pin="SEG-C" pad="15"/>
<connect gate="G$1" pin="SEG-D" pad="17"/>
<connect gate="G$1" pin="SEG-E" pad="19"/>
<connect gate="G$1" pin="SEG-F" pad="18"/>
<connect gate="G$1" pin="SEG-G" pad="22"/>
<connect gate="G$1" pin="STORE" pad="9"/>
<connect gate="G$1" pin="U/D" pad="10"/>
<connect gate="G$1" pin="V+" pad="24"/>
<connect gate="G$1" pin="ZERO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7217A" prefix="IC">
<description>&lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7217A"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="BCD1S" pad="7"/>
<connect gate="G$1" pin="BCD2S" pad="6"/>
<connect gate="G$1" pin="BCD4S" pad="5"/>
<connect gate="G$1" pin="BCD8S" pad="4"/>
<connect gate="G$1" pin="C-OUT" pad="8"/>
<connect gate="G$1" pin="C/B" pad="1"/>
<connect gate="G$1" pin="D1" pad="18"/>
<connect gate="G$1" pin="D2" pad="17"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="DISP-CON" pad="20"/>
<connect gate="G$1" pin="EQUAL" pad="3"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="LC/OFF" pad="12"/>
<connect gate="G$1" pin="LR/OFF" pad="11"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="SCAN" pad="13"/>
<connect gate="G$1" pin="SEG-A" pad="23"/>
<connect gate="G$1" pin="SEG-B" pad="27"/>
<connect gate="G$1" pin="SEG-C" pad="25"/>
<connect gate="G$1" pin="SEG-D" pad="28"/>
<connect gate="G$1" pin="SEG-E" pad="22"/>
<connect gate="G$1" pin="SEG-F" pad="26"/>
<connect gate="G$1" pin="SEG-G" pad="21"/>
<connect gate="G$1" pin="STORE" pad="9"/>
<connect gate="G$1" pin="U/D" pad="10"/>
<connect gate="G$1" pin="V+" pad="24"/>
<connect gate="G$1" pin="ZERO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7218A" prefix="IC">
<description>&lt;b&gt;LED DECODER DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7218A"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="DIG-1" pad="15"/>
<connect gate="G$1" pin="DIG-2" pad="16"/>
<connect gate="G$1" pin="DIG-3" pad="23"/>
<connect gate="G$1" pin="DIG-4" pad="20"/>
<connect gate="G$1" pin="DIG-5" pad="17"/>
<connect gate="G$1" pin="DIG-6" pad="22"/>
<connect gate="G$1" pin="DIG-7" pad="21"/>
<connect gate="G$1" pin="DIG-8" pad="18"/>
<connect gate="G$1" pin="DP" pad="4"/>
<connect gate="G$1" pin="GND" pad="28"/>
<connect gate="G$1" pin="ID0" pad="12"/>
<connect gate="G$1" pin="ID1" pad="11"/>
<connect gate="G$1" pin="ID2" pad="13"/>
<connect gate="G$1" pin="ID3" pad="14"/>
<connect gate="G$1" pin="ID4" pad="10"/>
<connect gate="G$1" pin="ID5" pad="6"/>
<connect gate="G$1" pin="ID6" pad="5"/>
<connect gate="G$1" pin="ID7" pad="7"/>
<connect gate="G$1" pin="MODE" pad="9"/>
<connect gate="G$1" pin="SEG-A" pad="27"/>
<connect gate="G$1" pin="SEG-B" pad="3"/>
<connect gate="G$1" pin="SEG-C" pad="1"/>
<connect gate="G$1" pin="SEG-D" pad="25"/>
<connect gate="G$1" pin="SEG-E" pad="2"/>
<connect gate="G$1" pin="SEG-F" pad="24"/>
<connect gate="G$1" pin="SEG-G" pad="26"/>
<connect gate="G$1" pin="V+" pad="19"/>
<connect gate="G$1" pin="WR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7218B" prefix="IC">
<description>&lt;b&gt;LED DECODER DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7218A"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="DIG-1" pad="4"/>
<connect gate="G$1" pin="DIG-2" pad="25"/>
<connect gate="G$1" pin="DIG-3" pad="3"/>
<connect gate="G$1" pin="DIG-4" pad="1"/>
<connect gate="G$1" pin="DIG-5" pad="26"/>
<connect gate="G$1" pin="DIG-6" pad="2"/>
<connect gate="G$1" pin="DIG-7" pad="27"/>
<connect gate="G$1" pin="DIG-8" pad="24"/>
<connect gate="G$1" pin="DP" pad="15"/>
<connect gate="G$1" pin="GND" pad="28"/>
<connect gate="G$1" pin="ID0" pad="12"/>
<connect gate="G$1" pin="ID1" pad="11"/>
<connect gate="G$1" pin="ID2" pad="13"/>
<connect gate="G$1" pin="ID3" pad="14"/>
<connect gate="G$1" pin="ID4" pad="10"/>
<connect gate="G$1" pin="ID5" pad="6"/>
<connect gate="G$1" pin="ID6" pad="5"/>
<connect gate="G$1" pin="ID7" pad="7"/>
<connect gate="G$1" pin="MODE" pad="9"/>
<connect gate="G$1" pin="SEG-A" pad="16"/>
<connect gate="G$1" pin="SEG-B" pad="17"/>
<connect gate="G$1" pin="SEG-C" pad="20"/>
<connect gate="G$1" pin="SEG-D" pad="18"/>
<connect gate="G$1" pin="SEG-E" pad="21"/>
<connect gate="G$1" pin="SEG-F" pad="22"/>
<connect gate="G$1" pin="SEG-G" pad="23"/>
<connect gate="G$1" pin="V+" pad="19"/>
<connect gate="G$1" pin="WR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7218C" prefix="IC">
<description>&lt;b&gt;LED DECODER DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7218C"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="DA0" pad="5"/>
<connect gate="G$1" pin="DA1" pad="6"/>
<connect gate="G$1" pin="DA2" pad="10"/>
<connect gate="G$1" pin="DIG-1" pad="15"/>
<connect gate="G$1" pin="DIG-2" pad="16"/>
<connect gate="G$1" pin="DIG-3" pad="23"/>
<connect gate="G$1" pin="DIG-4" pad="20"/>
<connect gate="G$1" pin="DIG-5" pad="17"/>
<connect gate="G$1" pin="DIG-6" pad="22"/>
<connect gate="G$1" pin="DIG-7" pad="21"/>
<connect gate="G$1" pin="DIG-8" pad="18"/>
<connect gate="G$1" pin="DP" pad="4"/>
<connect gate="G$1" pin="GND" pad="28"/>
<connect gate="G$1" pin="ID0" pad="12"/>
<connect gate="G$1" pin="ID1" pad="11"/>
<connect gate="G$1" pin="ID2" pad="13"/>
<connect gate="G$1" pin="ID3" pad="14"/>
<connect gate="G$1" pin="ID7-DP" pad="7"/>
<connect gate="G$1" pin="SEG-A" pad="27"/>
<connect gate="G$1" pin="SEG-B" pad="3"/>
<connect gate="G$1" pin="SEG-C" pad="1"/>
<connect gate="G$1" pin="SEG-D" pad="25"/>
<connect gate="G$1" pin="SEG-E" pad="2"/>
<connect gate="G$1" pin="SEG-F" pad="24"/>
<connect gate="G$1" pin="SEG-G" pad="26"/>
<connect gate="G$1" pin="SHDN" pad="9"/>
<connect gate="G$1" pin="V+" pad="19"/>
<connect gate="G$1" pin="WR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7218D" prefix="IC">
<description>&lt;b&gt;LED DECODER DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7218D"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="DA0" pad="5"/>
<connect gate="G$1" pin="DA1" pad="6"/>
<connect gate="G$1" pin="DA2" pad="10"/>
<connect gate="G$1" pin="DIG-1" pad="4"/>
<connect gate="G$1" pin="DIG-2" pad="25"/>
<connect gate="G$1" pin="DIG-3" pad="3"/>
<connect gate="G$1" pin="DIG-4" pad="1"/>
<connect gate="G$1" pin="DIG-5" pad="26"/>
<connect gate="G$1" pin="DIG-6" pad="2"/>
<connect gate="G$1" pin="DIG-7" pad="27"/>
<connect gate="G$1" pin="DIG-8" pad="24"/>
<connect gate="G$1" pin="DP" pad="15"/>
<connect gate="G$1" pin="GND" pad="28"/>
<connect gate="G$1" pin="ID0" pad="12"/>
<connect gate="G$1" pin="ID1" pad="11"/>
<connect gate="G$1" pin="ID2" pad="13"/>
<connect gate="G$1" pin="ID3" pad="14"/>
<connect gate="G$1" pin="ID7-DP" pad="7"/>
<connect gate="G$1" pin="SEG-A" pad="16"/>
<connect gate="G$1" pin="SEG-B" pad="17"/>
<connect gate="G$1" pin="SEG-C" pad="20"/>
<connect gate="G$1" pin="SEG-D" pad="18"/>
<connect gate="G$1" pin="SEG-E" pad="21"/>
<connect gate="G$1" pin="SEG-F" pad="22"/>
<connect gate="G$1" pin="SEG-G" pad="23"/>
<connect gate="G$1" pin="SHDN" pad="9"/>
<connect gate="G$1" pin="V+" pad="19"/>
<connect gate="G$1" pin="WR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7224PL" prefix="IC">
<description>&lt;b&gt;LCD COUNTER/DECODER/ DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7224"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!CNTINH" pad="31"/>
<connect gate="G$1" pin="(BRT)BP" pad="5"/>
<connect gate="G$1" pin="1/2-DIG" pad="27"/>
<connect gate="G$1" pin="A1" pad="37"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="13"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="B1" pad="38"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="B4" pad="21"/>
<connect gate="G$1" pin="C1" pad="39"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="15"/>
<connect gate="G$1" pin="C4" pad="22"/>
<connect gate="G$1" pin="CARRY" pad="28"/>
<connect gate="G$1" pin="CNT" pad="32"/>
<connect gate="G$1" pin="D1" pad="40"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="E1" pad="2"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="E3" pad="17"/>
<connect gate="G$1" pin="E4" pad="24"/>
<connect gate="G$1" pin="F1" pad="4"/>
<connect gate="G$1" pin="F2" pad="12"/>
<connect gate="G$1" pin="F3" pad="19"/>
<connect gate="G$1" pin="F4" pad="26"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="18"/>
<connect gate="G$1" pin="G4" pad="25"/>
<connect gate="G$1" pin="GND" pad="35"/>
<connect gate="G$1" pin="LZB-IN" pad="29"/>
<connect gate="G$1" pin="LZB-OUT" pad="30"/>
<connect gate="G$1" pin="OSC-GND" pad="36"/>
<connect gate="G$1" pin="RESET" pad="33"/>
<connect gate="G$1" pin="STORE" pad="34"/>
<connect gate="G$1" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MM74C945" prefix="IC">
<description>&lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MM74C945"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A1" pad="37"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="13"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="B1" pad="38"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="B4" pad="21"/>
<connect gate="G$1" pin="BP" pad="5"/>
<connect gate="G$1" pin="C1" pad="39"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="15"/>
<connect gate="G$1" pin="C4" pad="22"/>
<connect gate="G$1" pin="CARRY" pad="28"/>
<connect gate="G$1" pin="CLK" pad="32"/>
<connect gate="G$1" pin="D1" pad="40"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="E1" pad="2"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="E3" pad="17"/>
<connect gate="G$1" pin="E4" pad="24"/>
<connect gate="G$1" pin="ENABLE" pad="31"/>
<connect gate="G$1" pin="F1" pad="4"/>
<connect gate="G$1" pin="F2" pad="12"/>
<connect gate="G$1" pin="F3" pad="19"/>
<connect gate="G$1" pin="F4" pad="26"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="18"/>
<connect gate="G$1" pin="G4" pad="25"/>
<connect gate="G$1" pin="LZB-IN" pad="29"/>
<connect gate="G$1" pin="LZB-OUT" pad="30"/>
<connect gate="G$1" pin="OSC" pad="36"/>
<connect gate="G$1" pin="RESET" pad="33"/>
<connect gate="G$1" pin="STORE" pad="34"/>
<connect gate="G$1" pin="UP/DOWN" pad="27"/>
<connect gate="P" pin="GND" pad="35"/>
<connect gate="P" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7242PA" prefix="IC">
<description>&lt;b&gt;TIMER/COUNTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7242"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="128/256" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT-2" pad="2"/>
<connect gate="G$1" pin="RC" pad="7"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="TB" pad="8"/>
<connect gate="G$1" pin="TRIG" pad="6"/>
<connect gate="G$1" pin="V+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7240PE" prefix="IC">
<description>&lt;b&gt;LCD COUNTER/DECODER/ DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7240"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="128" pad="8"/>
<connect gate="G$1" pin="16" pad="5"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="32" pad="6"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="64" pad="7"/>
<connect gate="G$1" pin="8" pad="4"/>
<connect gate="G$1" pin="BU-RES" pad="15"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="MOD" pad="12"/>
<connect gate="G$1" pin="RC" pad="13"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="TB" pad="14"/>
<connect gate="G$1" pin="TRIGGER" pad="11"/>
<connect gate="G$1" pin="V+" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7556PD" prefix="IC">
<description>&lt;b&gt;TIMER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7556"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CV1" pad="3"/>
<connect gate="G$1" pin="CV2" pad="11"/>
<connect gate="G$1" pin="DISCH1" pad="1"/>
<connect gate="G$1" pin="DISCH2" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="RESET1" pad="4"/>
<connect gate="G$1" pin="RESET2" pad="10"/>
<connect gate="G$1" pin="TRIGG1" pad="6"/>
<connect gate="G$1" pin="TRIGG2" pad="8"/>
<connect gate="G$1" pin="TRSH1" pad="2"/>
<connect gate="G$1" pin="TRSH2" pad="12"/>
<connect gate="G$1" pin="V+" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7555" prefix="IC">
<description>&lt;b&gt;TIMER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7555"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CV" pad="5"/>
<connect gate="G$1" pin="DISCH" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="TRIG" pad="2"/>
<connect gate="G$1" pin="TRSH" pad="6"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7126PL" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7126"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A/Z" pad="29"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="23"/>
<connect gate="G$1" pin="AB4" pad="19"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="BP" pad="21"/>
<connect gate="G$1" pin="BUFF" pad="28"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="10"/>
<connect gate="G$1" pin="C3" pad="24"/>
<connect gate="G$1" pin="COMM" pad="32"/>
<connect gate="G$1" pin="CREF+" pad="34"/>
<connect gate="G$1" pin="CREF-" pad="33"/>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="14"/>
<connect gate="G$1" pin="E3" pad="18"/>
<connect gate="G$1" pin="F1" pad="6"/>
<connect gate="G$1" pin="F2" pad="13"/>
<connect gate="G$1" pin="F3" pad="17"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="25"/>
<connect gate="G$1" pin="G3" pad="22"/>
<connect gate="G$1" pin="IN-HI" pad="31"/>
<connect gate="G$1" pin="IN-LO" pad="30"/>
<connect gate="G$1" pin="INT" pad="27"/>
<connect gate="G$1" pin="OSC1" pad="40"/>
<connect gate="G$1" pin="OSC2" pad="39"/>
<connect gate="G$1" pin="OSC3" pad="38"/>
<connect gate="G$1" pin="POL" pad="20"/>
<connect gate="G$1" pin="REF-HI" pad="36"/>
<connect gate="G$1" pin="REF-LO" pad="35"/>
<connect gate="G$1" pin="TEST" pad="37"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7129ACP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICL7129"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="AGD1" pad="5"/>
<connect gate="G$1" pin="AGD2" pad="8"/>
<connect gate="G$1" pin="AGD3" pad="11"/>
<connect gate="G$1" pin="AGD4" pad="14"/>
<connect gate="G$1" pin="ANNDR" pad="3"/>
<connect gate="G$1" pin="BC1,CONT" pad="4"/>
<connect gate="G$1" pin="BC2,LOBA" pad="7"/>
<connect gate="G$1" pin="BC3,MIN" pad="10"/>
<connect gate="G$1" pin="BC4,BC5" pad="13"/>
<connect gate="G$1" pin="BP1" pad="18"/>
<connect gate="G$1" pin="BP2" pad="17"/>
<connect gate="G$1" pin="BP3" pad="16"/>
<connect gate="G$1" pin="BUFF" pad="31"/>
<connect gate="G$1" pin="COMM" pad="28"/>
<connect gate="G$1" pin="CONT" pad="27"/>
<connect gate="G$1" pin="CREF+" pad="29"/>
<connect gate="G$1" pin="CREF-" pad="30"/>
<connect gate="G$1" pin="DGND" pad="36"/>
<connect gate="G$1" pin="DP1" pad="39"/>
<connect gate="G$1" pin="DP2" pad="38"/>
<connect gate="G$1" pin="DP3/UR" pad="21"/>
<connect gate="G$1" pin="DP4/OR" pad="20"/>
<connect gate="G$1" pin="FEDP1" pad="6"/>
<connect gate="G$1" pin="FEDP2" pad="9"/>
<connect gate="G$1" pin="FEDP3" pad="12"/>
<connect gate="G$1" pin="FEDP4" pad="15"/>
<connect gate="G$1" pin="IN-HI" pad="33"/>
<connect gate="G$1" pin="IN-LO" pad="32"/>
<connect gate="G$1" pin="INT-IN" pad="25"/>
<connect gate="G$1" pin="INT-OUT" pad="26"/>
<connect gate="G$1" pin="LAT/HOL" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="1"/>
<connect gate="G$1" pin="OSC2" pad="40"/>
<connect gate="G$1" pin="OSC3" pad="2"/>
<connect gate="G$1" pin="RANGE" pad="37"/>
<connect gate="G$1" pin="REF-HI" pad="34"/>
<connect gate="G$1" pin="REF-LO" pad="35"/>
<connect gate="G$1" pin="V+" pad="24"/>
<connect gate="G$1" pin="V-" pad="23"/>
<connect gate="G$1" pin="VDISP" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX260NG" prefix="IC">
<description>Switched-capacitor &lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX260"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="BPA" pad="1"/>
<connect gate="G$1" pin="BPB" pad="21"/>
<connect gate="G$1" pin="CLK-OUT" pad="8"/>
<connect gate="G$1" pin="CLKA" pad="11"/>
<connect gate="G$1" pin="CLKB" pad="12"/>
<connect gate="G$1" pin="D0" pad="20"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="HPA" pad="3"/>
<connect gate="G$1" pin="HPB" pad="14"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="23"/>
<connect gate="G$1" pin="LPA" pad="24"/>
<connect gate="G$1" pin="LPB" pad="22"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="OSC-OUT" pad="19"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="17"/>
<connect gate="G$1" pin="WR" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX261NG" prefix="IC">
<description>Switched-capacitor &lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX261"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="A0" pad="14"/>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="BPA" pad="1"/>
<connect gate="G$1" pin="BPB" pad="21"/>
<connect gate="G$1" pin="CLK-OUT" pad="8"/>
<connect gate="G$1" pin="CLKA" pad="11"/>
<connect gate="G$1" pin="CLKB" pad="12"/>
<connect gate="G$1" pin="D0" pad="19"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="HPA" pad="3"/>
<connect gate="G$1" pin="HPB" pad="20"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="23"/>
<connect gate="G$1" pin="LPA" pad="24"/>
<connect gate="G$1" pin="LPB" pad="22"/>
<connect gate="G$1" pin="OP-IN" pad="4"/>
<connect gate="G$1" pin="OP-OUT" pad="2"/>
<connect gate="G$1" pin="OSC-OUT" pad="18"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="16"/>
<connect gate="G$1" pin="WR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX263PI" prefix="IC">
<description>Switched-capacitor &lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX263"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="BPA" pad="3"/>
<connect gate="G$1" pin="BPB" pad="27"/>
<connect gate="G$1" pin="CLK-A" pad="13"/>
<connect gate="G$1" pin="CLK-B" pad="14"/>
<connect gate="G$1" pin="F0" pad="24"/>
<connect gate="G$1" pin="F1" pad="17"/>
<connect gate="G$1" pin="F2" pad="23"/>
<connect gate="G$1" pin="F3" pad="12"/>
<connect gate="G$1" pin="F4" pad="11"/>
<connect gate="G$1" pin="GND" pad="19"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="1"/>
<connect gate="G$1" pin="LPA" pad="2"/>
<connect gate="G$1" pin="LPB" pad="28"/>
<connect gate="G$1" pin="M0" pad="8"/>
<connect gate="G$1" pin="M1" pad="7"/>
<connect gate="G$1" pin="N/HPA" pad="4"/>
<connect gate="G$1" pin="N/HPB" pad="26"/>
<connect gate="G$1" pin="OSC-OUT" pad="20"/>
<connect gate="G$1" pin="Q0" pad="15"/>
<connect gate="G$1" pin="Q1" pad="16"/>
<connect gate="G$1" pin="Q2" pad="21"/>
<connect gate="G$1" pin="Q3" pad="22"/>
<connect gate="G$1" pin="Q4" pad="25"/>
<connect gate="G$1" pin="Q5" pad="6"/>
<connect gate="G$1" pin="Q6" pad="9"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="V-" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX267NG" prefix="IC">
<description>Switched-capacitor &lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX267"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="BPA" pad="2"/>
<connect gate="G$1" pin="BPB" pad="24"/>
<connect gate="G$1" pin="CLK-A" pad="11"/>
<connect gate="G$1" pin="CLK-B" pad="12"/>
<connect gate="G$1" pin="F0" pad="22"/>
<connect gate="G$1" pin="F1" pad="15"/>
<connect gate="G$1" pin="F2" pad="21"/>
<connect gate="G$1" pin="F3" pad="10"/>
<connect gate="G$1" pin="F4" pad="9"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="1"/>
<connect gate="G$1" pin="OP-IN" pad="4"/>
<connect gate="G$1" pin="OP-OUT" pad="3"/>
<connect gate="G$1" pin="OSC-OUT" pad="18"/>
<connect gate="G$1" pin="Q0" pad="13"/>
<connect gate="G$1" pin="Q1" pad="14"/>
<connect gate="G$1" pin="Q2" pad="19"/>
<connect gate="G$1" pin="Q3" pad="20"/>
<connect gate="G$1" pin="Q4" pad="23"/>
<connect gate="G$1" pin="Q5" pad="6"/>
<connect gate="G$1" pin="Q6" pad="7"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MF10BN" prefix="IC">
<description>&lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MF10"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="50/100/C" pad="12"/>
<connect gate="G$1" pin="AGND" pad="15"/>
<connect gate="G$1" pin="BPA" pad="2"/>
<connect gate="G$1" pin="BPB" pad="19"/>
<connect gate="G$1" pin="CLK-A" pad="10"/>
<connect gate="G$1" pin="CLK-B" pad="11"/>
<connect gate="G$1" pin="INVA" pad="4"/>
<connect gate="G$1" pin="INVB" pad="17"/>
<connect gate="G$1" pin="LPA" pad="1"/>
<connect gate="G$1" pin="LPB" pad="20"/>
<connect gate="G$1" pin="LSH" pad="9"/>
<connect gate="G$1" pin="N/AP/HPA" pad="3"/>
<connect gate="G$1" pin="N/AP/HPB" pad="18"/>
<connect gate="G$1" pin="S1A" pad="5"/>
<connect gate="G$1" pin="S1B" pad="16"/>
<connect gate="G$1" pin="SA/B" pad="6"/>
<connect gate="G$1" pin="VA+" pad="7"/>
<connect gate="G$1" pin="VA-" pad="14"/>
<connect gate="G$1" pin="VD+" pad="8"/>
<connect gate="G$1" pin="VD-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX310CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX310"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="13"/>
<connect gate="G$1" pin="A1" pad="14"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="EN" pad="12"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="S1" pad="1"/>
<connect gate="G$1" pin="S2" pad="2"/>
<connect gate="G$1" pin="S3" pad="3"/>
<connect gate="G$1" pin="S4" pad="4"/>
<connect gate="G$1" pin="S5" pad="5"/>
<connect gate="G$1" pin="S6" pad="6"/>
<connect gate="G$1" pin="S7" pad="7"/>
<connect gate="G$1" pin="S8" pad="8"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX311CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX311"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="13"/>
<connect gate="G$1" pin="A1" pad="14"/>
<connect gate="G$1" pin="EN" pad="12"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="OUT-A" pad="16"/>
<connect gate="G$1" pin="OUT-B" pad="10"/>
<connect gate="G$1" pin="S1A" pad="1"/>
<connect gate="G$1" pin="S1B" pad="5"/>
<connect gate="G$1" pin="S2A" pad="2"/>
<connect gate="G$1" pin="S2B" pad="6"/>
<connect gate="G$1" pin="S3A" pad="3"/>
<connect gate="G$1" pin="S3B" pad="7"/>
<connect gate="G$1" pin="S4A" pad="4"/>
<connect gate="G$1" pin="S4B" pad="8"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX358CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX358"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="6"/>
<connect gate="G$1" pin="IN4" pad="7"/>
<connect gate="G$1" pin="IN5" pad="12"/>
<connect gate="G$1" pin="IN6" pad="11"/>
<connect gate="G$1" pin="IN7" pad="10"/>
<connect gate="G$1" pin="IN8" pad="9"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX359CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX359"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IN1A" pad="4"/>
<connect gate="G$1" pin="IN1B" pad="13"/>
<connect gate="G$1" pin="IN2A" pad="5"/>
<connect gate="G$1" pin="IN2B" pad="12"/>
<connect gate="G$1" pin="IN3A" pad="6"/>
<connect gate="G$1" pin="IN3B" pad="11"/>
<connect gate="G$1" pin="IN4A" pad="7"/>
<connect gate="G$1" pin="IN4B" pad="10"/>
<connect gate="G$1" pin="OUT-A" pad="8"/>
<connect gate="G$1" pin="OUT-B" pad="9"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG506ACJ" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG506A"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="D" pad="28"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="S1" pad="19"/>
<connect gate="G$1" pin="S10" pad="10"/>
<connect gate="G$1" pin="S11" pad="9"/>
<connect gate="G$1" pin="S12" pad="8"/>
<connect gate="G$1" pin="S13" pad="7"/>
<connect gate="G$1" pin="S14" pad="6"/>
<connect gate="G$1" pin="S15" pad="5"/>
<connect gate="G$1" pin="S16" pad="4"/>
<connect gate="G$1" pin="S2" pad="20"/>
<connect gate="G$1" pin="S3" pad="21"/>
<connect gate="G$1" pin="S4" pad="22"/>
<connect gate="G$1" pin="S5" pad="23"/>
<connect gate="G$1" pin="S6" pad="24"/>
<connect gate="G$1" pin="S7" pad="25"/>
<connect gate="G$1" pin="S8" pad="26"/>
<connect gate="G$1" pin="S9" pad="11"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG507ACJ" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG507AC"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="DA" pad="28"/>
<connect gate="G$1" pin="DB" pad="2"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="S1A" pad="19"/>
<connect gate="G$1" pin="S1B" pad="11"/>
<connect gate="G$1" pin="S2A" pad="20"/>
<connect gate="G$1" pin="S2B" pad="10"/>
<connect gate="G$1" pin="S3A" pad="21"/>
<connect gate="G$1" pin="S3B" pad="9"/>
<connect gate="G$1" pin="S4A" pad="22"/>
<connect gate="G$1" pin="S4B" pad="8"/>
<connect gate="G$1" pin="S5A" pad="23"/>
<connect gate="G$1" pin="S5B" pad="7"/>
<connect gate="G$1" pin="S6A" pad="24"/>
<connect gate="G$1" pin="S6B" pad="6"/>
<connect gate="G$1" pin="S7A" pad="25"/>
<connect gate="G$1" pin="S7B" pad="5"/>
<connect gate="G$1" pin="S8A" pad="26"/>
<connect gate="G$1" pin="S8B" pad="4"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG508ACJ" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG508A"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="6"/>
<connect gate="G$1" pin="S4" pad="7"/>
<connect gate="G$1" pin="S5" pad="12"/>
<connect gate="G$1" pin="S6" pad="11"/>
<connect gate="G$1" pin="S7" pad="10"/>
<connect gate="G$1" pin="S8" pad="9"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG509ACJ" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG509A"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DA" pad="8"/>
<connect gate="G$1" pin="DB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="S1A" pad="4"/>
<connect gate="G$1" pin="S1B" pad="13"/>
<connect gate="G$1" pin="S2A" pad="5"/>
<connect gate="G$1" pin="S2B" pad="12"/>
<connect gate="G$1" pin="S3A" pad="6"/>
<connect gate="G$1" pin="S3B" pad="11"/>
<connect gate="G$1" pin="S4A" pad="7"/>
<connect gate="G$1" pin="S4B" pad="10"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG201ACJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG201"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="S1" pad="3"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="11"/>
<connect gate="G$1" pin="S4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX333ACPP" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX333"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="8"/>
<connect gate="G$1" pin="COM3" pad="13"/>
<connect gate="G$1" pin="COM4" pad="18"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="IN3" pad="11"/>
<connect gate="G$1" pin="IN4" pad="20"/>
<connect gate="G$1" pin="NC" pad="15"/>
<connect gate="G$1" pin="NC1" pad="4"/>
<connect gate="G$1" pin="NC2" pad="7"/>
<connect gate="G$1" pin="NC3" pad="14"/>
<connect gate="G$1" pin="NC4" pad="17"/>
<connect gate="G$1" pin="NO1" pad="2"/>
<connect gate="G$1" pin="NO2" pad="9"/>
<connect gate="G$1" pin="NO3" pad="12"/>
<connect gate="G$1" pin="NO4" pad="19"/>
<connect gate="G$1" pin="V+" pad="16"/>
<connect gate="G$1" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX341CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX341"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A1" pad="15"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="4"/>
<connect gate="G$1" pin="NC@3" pad="5"/>
<connect gate="G$1" pin="NC@4" pad="6"/>
<connect gate="G$1" pin="NC@5" pad="7"/>
<connect gate="G$1" pin="NC@6" pad="12"/>
<connect gate="G$1" pin="S1" pad="1"/>
<connect gate="G$1" pin="S2" pad="8"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX343CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX343"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A1" pad="15"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="7"/>
<connect gate="G$1" pin="NC@2" pad="12"/>
<connect gate="G$1" pin="S1" pad="1"/>
<connect gate="G$1" pin="S2" pad="8"/>
<connect gate="G$1" pin="S3" pad="3"/>
<connect gate="G$1" pin="S4" pad="5"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG200ACJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG200"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="D1" pad="9"/>
<connect gate="G$1" pin="D2" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="14"/>
<connect gate="G$1" pin="IN2" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="8"/>
<connect gate="G$1" pin="NC@3" pad="11"/>
<connect gate="G$1" pin="NC@4" pad="13"/>
<connect gate="G$1" pin="S1" pad="10"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="V+" pad="12"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX232" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX232"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX242" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX242"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="R1IN" pad="14"/>
<connect gate="G$1" pin="R1OUT" pad="13"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="SHDN" pad="18"/>
<connect gate="G$1" pin="T1IN" pad="12"/>
<connect gate="G$1" pin="T1OUT" pad="15"/>
<connect gate="G$1" pin="T2IN" pad="11"/>
<connect gate="G$1" pin="T2OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX230" prefix="IC">
<description>&lt;b&gt;RS232 TRANMITTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX230"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="C1+" pad="8"/>
<connect gate="G$1" pin="C1-" pad="10"/>
<connect gate="G$1" pin="C2+" pad="11"/>
<connect gate="G$1" pin="C2-" pad="12"/>
<connect gate="G$1" pin="NC" pad="18"/>
<connect gate="G$1" pin="SHUTDOWN" pad="17"/>
<connect gate="G$1" pin="T1IN" pad="5"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="4"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="14"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="T4OUT" pad="20"/>
<connect gate="G$1" pin="T5IN" pad="19"/>
<connect gate="G$1" pin="T5OUT" pad="16"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="13"/>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX231" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX231"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="2"/>
<connect gate="G$1" pin="R1IN" pad="10"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="6"/>
<connect gate="G$1" pin="T1IN" pad="8"/>
<connect gate="G$1" pin="T1OUT" pad="11"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T2OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX233" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX233"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="C1+" pad="8"/>
<connect gate="G$1" pin="C1-" pad="13"/>
<connect gate="G$1" pin="C2+@1" pad="11"/>
<connect gate="G$1" pin="C2+@2" pad="15"/>
<connect gate="G$1" pin="C2-@1" pad="10"/>
<connect gate="G$1" pin="C2-@2" pad="16"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="3"/>
<connect gate="G$1" pin="R2IN" pad="19"/>
<connect gate="G$1" pin="R2OUT" pad="20"/>
<connect gate="G$1" pin="T1IN" pad="2"/>
<connect gate="G$1" pin="T1OUT" pad="5"/>
<connect gate="G$1" pin="T2IN" pad="1"/>
<connect gate="G$1" pin="T2OUT" pad="18"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-@1" pad="12"/>
<connect gate="G$1" pin="V-@2" pad="17"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="9"/>
<connect gate="P" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX234" prefix="IC">
<description>&lt;b&gt;RS232 TRANSMITTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX234"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="7"/>
<connect gate="G$1" pin="C1-" pad="9"/>
<connect gate="G$1" pin="C2+" pad="10"/>
<connect gate="G$1" pin="C2-" pad="11"/>
<connect gate="G$1" pin="T1IN" pad="4"/>
<connect gate="G$1" pin="T1OUT" pad="1"/>
<connect gate="G$1" pin="T2IN" pad="3"/>
<connect gate="G$1" pin="T2OUT" pad="2"/>
<connect gate="G$1" pin="T3IN" pad="13"/>
<connect gate="G$1" pin="T3OUT" pad="16"/>
<connect gate="G$1" pin="T4IN" pad="14"/>
<connect gate="G$1" pin="T4OUT" pad="15"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="12"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX235" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX235"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="EN" pad="20"/>
<connect gate="G$1" pin="R1IN" pad="10"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="6"/>
<connect gate="G$1" pin="R3IN" pad="24"/>
<connect gate="G$1" pin="R3OUT" pad="23"/>
<connect gate="G$1" pin="R4IN" pad="18"/>
<connect gate="G$1" pin="R4OUT" pad="17"/>
<connect gate="G$1" pin="R5IN" pad="13"/>
<connect gate="G$1" pin="R5OUT" pad="14"/>
<connect gate="G$1" pin="SHDN" pad="21"/>
<connect gate="G$1" pin="T1IN" pad="8"/>
<connect gate="G$1" pin="T1OUT" pad="3"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T2OUT" pad="4"/>
<connect gate="G$1" pin="T3IN" pad="15"/>
<connect gate="G$1" pin="T3OUT" pad="2"/>
<connect gate="G$1" pin="T4IN" pad="16"/>
<connect gate="G$1" pin="T4OUT" pad="1"/>
<connect gate="G$1" pin="T5IN" pad="22"/>
<connect gate="G$1" pin="T5OUT" pad="19"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX236" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX236"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="12"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="14"/>
<connect gate="G$1" pin="EN" pad="20"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="5"/>
<connect gate="G$1" pin="R2IN" pad="23"/>
<connect gate="G$1" pin="R2OUT" pad="22"/>
<connect gate="G$1" pin="R3IN" pad="16"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="SHDN" pad="21"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="6"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="18"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="19"/>
<connect gate="G$1" pin="T4OUT" pad="24"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX237" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX237"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="12"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="5"/>
<connect gate="G$1" pin="R2IN" pad="23"/>
<connect gate="G$1" pin="R2OUT" pad="22"/>
<connect gate="G$1" pin="R3IN" pad="16"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="6"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="18"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="19"/>
<connect gate="G$1" pin="T4OUT" pad="24"/>
<connect gate="G$1" pin="T5IN" pad="21"/>
<connect gate="G$1" pin="T5OUT" pad="20"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX238" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX238"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="12"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="7"/>
<connect gate="G$1" pin="R1OUT" pad="6"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R2OUT" pad="4"/>
<connect gate="G$1" pin="R3IN" pad="23"/>
<connect gate="G$1" pin="R3OUT" pad="22"/>
<connect gate="G$1" pin="R4IN" pad="16"/>
<connect gate="G$1" pin="R4OUT" pad="17"/>
<connect gate="G$1" pin="T1IN" pad="5"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="18"/>
<connect gate="G$1" pin="T2OUT" pad="1"/>
<connect gate="G$1" pin="T3IN" pad="19"/>
<connect gate="G$1" pin="T3OUT" pad="24"/>
<connect gate="G$1" pin="T4IN" pad="21"/>
<connect gate="G$1" pin="T4OUT" pad="20"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX239" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="VCC-GND"/>
<gate name="G$1" symbol="MAX239"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="C+" pad="6"/>
<connect gate="G$1" pin="C-" pad="7"/>
<connect gate="G$1" pin="EN" pad="14"/>
<connect gate="G$1" pin="NC" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="2"/>
<connect gate="G$1" pin="R1OUT" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="21"/>
<connect gate="G$1" pin="R2OUT" pad="22"/>
<connect gate="G$1" pin="R3IN" pad="18"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="R4IN" pad="12"/>
<connect gate="G$1" pin="R4OUT" pad="11"/>
<connect gate="G$1" pin="R5IN" pad="9"/>
<connect gate="G$1" pin="R5OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="24"/>
<connect gate="G$1" pin="T1OUT" pad="19"/>
<connect gate="G$1" pin="T2IN" pad="23"/>
<connect gate="G$1" pin="T2OUT" pad="20"/>
<connect gate="G$1" pin="T3IN" pad="16"/>
<connect gate="G$1" pin="T3OUT" pad="13"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX243" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX243"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX244" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX244"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="C1+" pad="21"/>
<connect gate="G$1" pin="C1-" pad="23"/>
<connect gate="G$1" pin="C2+" pad="24"/>
<connect gate="G$1" pin="C2-" pad="25"/>
<connect gate="G$1" pin="RA1IN" pad="9"/>
<connect gate="G$1" pin="RA1OUT" pad="10"/>
<connect gate="G$1" pin="RA2IN" pad="8"/>
<connect gate="G$1" pin="RA2OUT" pad="11"/>
<connect gate="G$1" pin="RA3IN" pad="7"/>
<connect gate="G$1" pin="RA3OUT" pad="12"/>
<connect gate="G$1" pin="RA4IN" pad="6"/>
<connect gate="G$1" pin="RA4OUT" pad="13"/>
<connect gate="G$1" pin="RA5IN" pad="5"/>
<connect gate="G$1" pin="RA5OUT" pad="14"/>
<connect gate="G$1" pin="RB1IN" pad="36"/>
<connect gate="G$1" pin="RB1OUT" pad="35"/>
<connect gate="G$1" pin="RB2IN" pad="37"/>
<connect gate="G$1" pin="RB2OUT" pad="34"/>
<connect gate="G$1" pin="RB3IN" pad="38"/>
<connect gate="G$1" pin="RB3OUT" pad="33"/>
<connect gate="G$1" pin="RB4IN" pad="39"/>
<connect gate="G$1" pin="RB4OUT" pad="32"/>
<connect gate="G$1" pin="RB5IN" pad="40"/>
<connect gate="G$1" pin="RB5OUT" pad="31"/>
<connect gate="G$1" pin="TA1IN" pad="15"/>
<connect gate="G$1" pin="TA1OUT" pad="1"/>
<connect gate="G$1" pin="TA2IN" pad="16"/>
<connect gate="G$1" pin="TA2OUT" pad="2"/>
<connect gate="G$1" pin="TA3IN" pad="17"/>
<connect gate="G$1" pin="TA3OUT" pad="3"/>
<connect gate="G$1" pin="TA4IN" pad="18"/>
<connect gate="G$1" pin="TA4OUT" pad="4"/>
<connect gate="G$1" pin="TB1IN" pad="30"/>
<connect gate="G$1" pin="TB1OUT" pad="44"/>
<connect gate="G$1" pin="TB2IN" pad="29"/>
<connect gate="G$1" pin="TB2OUT" pad="43"/>
<connect gate="G$1" pin="TB3IN" pad="28"/>
<connect gate="G$1" pin="TB3OUT" pad="42"/>
<connect gate="G$1" pin="TB4IN" pad="27"/>
<connect gate="G$1" pin="TB4OUT" pad="41"/>
<connect gate="G$1" pin="V+" pad="22"/>
<connect gate="G$1" pin="V-" pad="26"/>
<connect gate="P" pin="GND" pad="19"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX245" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX245"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="ENR" pad="1"/>
<connect gate="G$1" pin="ENT" pad="39"/>
<connect gate="G$1" pin="RA1IN" pad="11"/>
<connect gate="G$1" pin="RA1OUT" pad="10"/>
<connect gate="G$1" pin="RA2IN" pad="12"/>
<connect gate="G$1" pin="RA2OUT" pad="9"/>
<connect gate="G$1" pin="RA3IN" pad="13"/>
<connect gate="G$1" pin="RA3OUT" pad="8"/>
<connect gate="G$1" pin="RA4IN" pad="14"/>
<connect gate="G$1" pin="RA4OUT" pad="7"/>
<connect gate="G$1" pin="RA5IN" pad="15"/>
<connect gate="G$1" pin="RA5OUT" pad="6"/>
<connect gate="G$1" pin="RB1IN" pad="29"/>
<connect gate="G$1" pin="RB1OUT" pad="30"/>
<connect gate="G$1" pin="RB2IN" pad="28"/>
<connect gate="G$1" pin="RB2OUT" pad="31"/>
<connect gate="G$1" pin="RB3IN" pad="27"/>
<connect gate="G$1" pin="RB3OUT" pad="32"/>
<connect gate="G$1" pin="RB4IN" pad="26"/>
<connect gate="G$1" pin="RB4OUT" pad="33"/>
<connect gate="G$1" pin="RB5IN" pad="25"/>
<connect gate="G$1" pin="RB5OUT" pad="34"/>
<connect gate="G$1" pin="TA1IN" pad="2"/>
<connect gate="G$1" pin="TA1OUT" pad="16"/>
<connect gate="G$1" pin="TA2IN" pad="3"/>
<connect gate="G$1" pin="TA2OUT" pad="17"/>
<connect gate="G$1" pin="TA3IN" pad="4"/>
<connect gate="G$1" pin="TA3OUT" pad="18"/>
<connect gate="G$1" pin="TA4IN" pad="5"/>
<connect gate="G$1" pin="TA4OUT" pad="19"/>
<connect gate="G$1" pin="TB1IN" pad="38"/>
<connect gate="G$1" pin="TB1OUT" pad="24"/>
<connect gate="G$1" pin="TB2IN" pad="37"/>
<connect gate="G$1" pin="TB2OUT" pad="23"/>
<connect gate="G$1" pin="TB3IN" pad="36"/>
<connect gate="G$1" pin="TB3OUT" pad="22"/>
<connect gate="G$1" pin="TB4IN" pad="35"/>
<connect gate="G$1" pin="TB4OUT" pad="21"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX247" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX247"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="ENRA" pad="11"/>
<connect gate="G$1" pin="ENRB" pad="30"/>
<connect gate="G$1" pin="ENTA" pad="1"/>
<connect gate="G$1" pin="ENTB" pad="39"/>
<connect gate="G$1" pin="RA1IN" pad="12"/>
<connect gate="G$1" pin="RA1OUT" pad="10"/>
<connect gate="G$1" pin="RA2IN" pad="13"/>
<connect gate="G$1" pin="RA2OUT" pad="9"/>
<connect gate="G$1" pin="RA3IN" pad="14"/>
<connect gate="G$1" pin="RA3OUT" pad="8"/>
<connect gate="G$1" pin="RA4IN" pad="15"/>
<connect gate="G$1" pin="RA4OUT" pad="7"/>
<connect gate="G$1" pin="RB1IN" pad="29"/>
<connect gate="G$1" pin="RB1OUT" pad="31"/>
<connect gate="G$1" pin="RB2IN" pad="28"/>
<connect gate="G$1" pin="RB2OUT" pad="32"/>
<connect gate="G$1" pin="RB3IN" pad="27"/>
<connect gate="G$1" pin="RB3OUT" pad="33"/>
<connect gate="G$1" pin="RB4IN" pad="26"/>
<connect gate="G$1" pin="RB4OUT" pad="34"/>
<connect gate="G$1" pin="RB5IN" pad="25"/>
<connect gate="G$1" pin="RB5OUT" pad="6"/>
<connect gate="G$1" pin="TA1IN" pad="2"/>
<connect gate="G$1" pin="TA1OUT" pad="16"/>
<connect gate="G$1" pin="TA2IN" pad="3"/>
<connect gate="G$1" pin="TA2OUT" pad="17"/>
<connect gate="G$1" pin="TA3IN" pad="4"/>
<connect gate="G$1" pin="TA3OUT" pad="18"/>
<connect gate="G$1" pin="TA4IN" pad="5"/>
<connect gate="G$1" pin="TA4OUT" pad="19"/>
<connect gate="G$1" pin="TB1IN" pad="38"/>
<connect gate="G$1" pin="TB1OUT" pad="24"/>
<connect gate="G$1" pin="TB2IN" pad="37"/>
<connect gate="G$1" pin="TB2OUT" pad="23"/>
<connect gate="G$1" pin="TB3IN" pad="36"/>
<connect gate="G$1" pin="TB3OUT" pad="22"/>
<connect gate="G$1" pin="TB4IN" pad="35"/>
<connect gate="G$1" pin="TB4OUT" pad="21"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX246" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX246"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="ENA" pad="1"/>
<connect gate="G$1" pin="ENB" pad="39"/>
<connect gate="G$1" pin="RA1IN" pad="11"/>
<connect gate="G$1" pin="RA1OUT" pad="10"/>
<connect gate="G$1" pin="RA2IN" pad="12"/>
<connect gate="G$1" pin="RA2OUT" pad="9"/>
<connect gate="G$1" pin="RA3IN" pad="13"/>
<connect gate="G$1" pin="RA3OUT" pad="8"/>
<connect gate="G$1" pin="RA4IN" pad="14"/>
<connect gate="G$1" pin="RA4OUT" pad="7"/>
<connect gate="G$1" pin="RA5IN" pad="15"/>
<connect gate="G$1" pin="RA5OUT" pad="6"/>
<connect gate="G$1" pin="RB1IN" pad="29"/>
<connect gate="G$1" pin="RB1OUT" pad="30"/>
<connect gate="G$1" pin="RB2IN" pad="28"/>
<connect gate="G$1" pin="RB2OUT" pad="31"/>
<connect gate="G$1" pin="RB3IN" pad="27"/>
<connect gate="G$1" pin="RB3OUT" pad="32"/>
<connect gate="G$1" pin="RB4IN" pad="26"/>
<connect gate="G$1" pin="RB4OUT" pad="33"/>
<connect gate="G$1" pin="RB5IN" pad="25"/>
<connect gate="G$1" pin="RB5OUT" pad="34"/>
<connect gate="G$1" pin="TA1IN" pad="2"/>
<connect gate="G$1" pin="TA1OUT" pad="16"/>
<connect gate="G$1" pin="TA2IN" pad="3"/>
<connect gate="G$1" pin="TA2OUT" pad="17"/>
<connect gate="G$1" pin="TA3IN" pad="4"/>
<connect gate="G$1" pin="TA3OUT" pad="18"/>
<connect gate="G$1" pin="TA4IN" pad="5"/>
<connect gate="G$1" pin="TA4OUT" pad="19"/>
<connect gate="G$1" pin="TB1IN" pad="38"/>
<connect gate="G$1" pin="TB1OUT" pad="24"/>
<connect gate="G$1" pin="TB2IN" pad="37"/>
<connect gate="G$1" pin="TB2OUT" pad="23"/>
<connect gate="G$1" pin="TB3IN" pad="36"/>
<connect gate="G$1" pin="TB3OUT" pad="22"/>
<connect gate="G$1" pin="TB4IN" pad="35"/>
<connect gate="G$1" pin="TB4OUT" pad="21"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX248" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX248"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="C1+" pad="21"/>
<connect gate="G$1" pin="C1-" pad="23"/>
<connect gate="G$1" pin="C2+" pad="24"/>
<connect gate="G$1" pin="C2-" pad="25"/>
<connect gate="G$1" pin="ENRA" pad="9"/>
<connect gate="G$1" pin="ENRB" pad="36"/>
<connect gate="G$1" pin="ENTA" pad="18"/>
<connect gate="G$1" pin="ENTB" pad="27"/>
<connect gate="G$1" pin="RA1IN" pad="8"/>
<connect gate="G$1" pin="RA1OUT" pad="10"/>
<connect gate="G$1" pin="RA2IN" pad="7"/>
<connect gate="G$1" pin="RA2OUT" pad="11"/>
<connect gate="G$1" pin="RA3IN" pad="6"/>
<connect gate="G$1" pin="RA3OUT" pad="12"/>
<connect gate="G$1" pin="RA4IN" pad="5"/>
<connect gate="G$1" pin="RA4OUT" pad="13"/>
<connect gate="G$1" pin="RB1IN" pad="37"/>
<connect gate="G$1" pin="RB1OUT" pad="35"/>
<connect gate="G$1" pin="RB2IN" pad="38"/>
<connect gate="G$1" pin="RB2OUT" pad="34"/>
<connect gate="G$1" pin="RB3IN" pad="39"/>
<connect gate="G$1" pin="RB3OUT" pad="33"/>
<connect gate="G$1" pin="RB4IN" pad="40"/>
<connect gate="G$1" pin="RB4OUT" pad="32"/>
<connect gate="G$1" pin="TA1IN" pad="14"/>
<connect gate="G$1" pin="TA1OUT" pad="1"/>
<connect gate="G$1" pin="TA2IN" pad="15"/>
<connect gate="G$1" pin="TA2OUT" pad="2"/>
<connect gate="G$1" pin="TA3IN" pad="16"/>
<connect gate="G$1" pin="TA3OUT" pad="3"/>
<connect gate="G$1" pin="TA4IN" pad="17"/>
<connect gate="G$1" pin="TA4OUT" pad="4"/>
<connect gate="G$1" pin="TB1IN" pad="31"/>
<connect gate="G$1" pin="TB1OUT" pad="44"/>
<connect gate="G$1" pin="TB2IN" pad="30"/>
<connect gate="G$1" pin="TB2OUT" pad="43"/>
<connect gate="G$1" pin="TB3IN" pad="29"/>
<connect gate="G$1" pin="TB3OUT" pad="42"/>
<connect gate="G$1" pin="TB4IN" pad="28"/>
<connect gate="G$1" pin="TB4OUT" pad="41"/>
<connect gate="G$1" pin="V+" pad="22"/>
<connect gate="G$1" pin="V-" pad="26"/>
<connect gate="P" pin="GND" pad="19"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX249" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX249"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="C1+" pad="21"/>
<connect gate="G$1" pin="C1-" pad="23"/>
<connect gate="G$1" pin="C2+" pad="24"/>
<connect gate="G$1" pin="C2-" pad="25"/>
<connect gate="G$1" pin="ENRA" pad="9"/>
<connect gate="G$1" pin="ENRB" pad="36"/>
<connect gate="G$1" pin="ENTA" pad="18"/>
<connect gate="G$1" pin="ENTB" pad="27"/>
<connect gate="G$1" pin="RA1IN" pad="8"/>
<connect gate="G$1" pin="RA1OUT" pad="10"/>
<connect gate="G$1" pin="RA2IN" pad="7"/>
<connect gate="G$1" pin="RA2OUT" pad="11"/>
<connect gate="G$1" pin="RA3IN" pad="6"/>
<connect gate="G$1" pin="RA3OUT" pad="12"/>
<connect gate="G$1" pin="RA4IN" pad="5"/>
<connect gate="G$1" pin="RA4OUT" pad="13"/>
<connect gate="G$1" pin="RA5IN" pad="4"/>
<connect gate="G$1" pin="RA5OUT" pad="14"/>
<connect gate="G$1" pin="RB1IN" pad="37"/>
<connect gate="G$1" pin="RB1OUT" pad="35"/>
<connect gate="G$1" pin="RB2IN" pad="38"/>
<connect gate="G$1" pin="RB2OUT" pad="34"/>
<connect gate="G$1" pin="RB3IN" pad="39"/>
<connect gate="G$1" pin="RB3OUT" pad="33"/>
<connect gate="G$1" pin="RB4IN" pad="40"/>
<connect gate="G$1" pin="RB4OUT" pad="32"/>
<connect gate="G$1" pin="RB5IN" pad="41"/>
<connect gate="G$1" pin="RB5OUT" pad="31"/>
<connect gate="G$1" pin="TA1IN" pad="15"/>
<connect gate="G$1" pin="TA1OUT" pad="1"/>
<connect gate="G$1" pin="TA2IN" pad="16"/>
<connect gate="G$1" pin="TA2OUT" pad="2"/>
<connect gate="G$1" pin="TA3IN" pad="17"/>
<connect gate="G$1" pin="TA3OUT" pad="3"/>
<connect gate="G$1" pin="TB1IN" pad="30"/>
<connect gate="G$1" pin="TB1OUT" pad="44"/>
<connect gate="G$1" pin="TB2IN" pad="29"/>
<connect gate="G$1" pin="TB2OUT" pad="43"/>
<connect gate="G$1" pin="TB3IN" pad="28"/>
<connect gate="G$1" pin="TB3OUT" pad="42"/>
<connect gate="G$1" pin="V+" pad="22"/>
<connect gate="G$1" pin="V-" pad="26"/>
<connect gate="P" pin="GND" pad="19"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX910" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX910"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="CMP_GND" pad="18"/>
<connect gate="G$1" pin="CMP_OUT" pad="17"/>
<connect gate="G$1" pin="D0" pad="21"/>
<connect gate="G$1" pin="D1" pad="22"/>
<connect gate="G$1" pin="D2" pad="23"/>
<connect gate="G$1" pin="D3" pad="24"/>
<connect gate="G$1" pin="D4" pad="1"/>
<connect gate="G$1" pin="D5" pad="2"/>
<connect gate="G$1" pin="D6" pad="3"/>
<connect gate="G$1" pin="D7" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="IN+" pad="13"/>
<connect gate="G$1" pin="IN-" pad="14"/>
<connect gate="G$1" pin="LATCH" pad="5"/>
<connect gate="G$1" pin="RA" pad="10"/>
<connect gate="G$1" pin="RB" pad="11"/>
<connect gate="G$1" pin="REFIN" pad="8"/>
<connect gate="G$1" pin="REFOUT" pad="9"/>
<connect gate="G$1" pin="TH_CTRL" pad="16"/>
<connect gate="G$1" pin="TH_OUT" pad="12"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VDD" pad="19"/>
<connect gate="G$1" pin="VEE" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX625" prefix="IC">
<description>&lt;b&gt;POWER SUPPLY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX625"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="CE" pad="8"/>
<connect gate="G$1" pin="D1" pad="23"/>
<connect gate="G$1" pin="D2" pad="21"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="D4" pad="2"/>
<connect gate="G$1" pin="IN1" pad="18"/>
<connect gate="G$1" pin="IN2" pad="19"/>
<connect gate="G$1" pin="IN3" pad="6"/>
<connect gate="G$1" pin="IN4" pad="7"/>
<connect gate="G$1" pin="PR" pad="9"/>
<connect gate="G$1" pin="S1" pad="24"/>
<connect gate="G$1" pin="S2" pad="22"/>
<connect gate="G$1" pin="S3" pad="3"/>
<connect gate="G$1" pin="S4" pad="1"/>
<connect gate="G$1" pin="V+" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX639" prefix="IC">
<description>Step-down &lt;b&gt;SWITCHING REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX639"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="2"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="SHDN" pad="8"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="VFB" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX665" prefix="IC">
<description>Switched-capcitor &lt;b&gt;VOLTAGE CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX665"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="FC" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LV" pad="6"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX291" prefix="IC">
<description>&lt;b&gt;DIGITAL FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX291"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OPI-" pad="4"/>
<connect gate="G$1" pin="OPO" pad="3"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX420PA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP1"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CEXT1" pad="1"/>
<connect gate="G$1" pin="CEXT2" pad="8"/>
<connect gate="G$1" pin="CRET" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX420MTV" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP1"/>
</gates>
<devices>
<device name="" package="TO99">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CEXT1" pad="1"/>
<connect gate="G$1" pin="CEXT2" pad="8"/>
<connect gate="G$1" pin="CRET" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX430PA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP2"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICM7212" prefix="IC">
<description>&lt;b&gt;LCD DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ICM7212"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A1" pad="37"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="13"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="B1" pad="38"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="B4" pad="21"/>
<connect gate="G$1" pin="BD0" pad="27"/>
<connect gate="G$1" pin="BD1" pad="28"/>
<connect gate="G$1" pin="BD2" pad="29"/>
<connect gate="G$1" pin="BD3" pad="30"/>
<connect gate="G$1" pin="BRT" pad="5"/>
<connect gate="G$1" pin="C1" pad="39"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="C3" pad="15"/>
<connect gate="G$1" pin="C4" pad="22"/>
<connect gate="G$1" pin="D1" pad="40"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="23"/>
<connect gate="G$1" pin="DI1" pad="31"/>
<connect gate="G$1" pin="DI2" pad="32"/>
<connect gate="G$1" pin="DI3" pad="33"/>
<connect gate="G$1" pin="DI4" pad="34"/>
<connect gate="G$1" pin="E1" pad="2"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="E3" pad="17"/>
<connect gate="G$1" pin="E4" pad="24"/>
<connect gate="G$1" pin="F1" pad="4"/>
<connect gate="G$1" pin="F2" pad="12"/>
<connect gate="G$1" pin="F3" pad="19"/>
<connect gate="G$1" pin="F4" pad="26"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="18"/>
<connect gate="G$1" pin="G4" pad="25"/>
<connect gate="G$1" pin="GND@1" pad="35"/>
<connect gate="G$1" pin="GND@2" pad="36"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX358E" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX358"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="6"/>
<connect gate="G$1" pin="IN4" pad="7"/>
<connect gate="G$1" pin="IN5" pad="12"/>
<connect gate="G$1" pin="IN6" pad="11"/>
<connect gate="G$1" pin="IN7" pad="10"/>
<connect gate="G$1" pin="IN8" pad="9"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX359E" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX359"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IN1A" pad="4"/>
<connect gate="G$1" pin="IN1B" pad="13"/>
<connect gate="G$1" pin="IN2A" pad="5"/>
<connect gate="G$1" pin="IN2B" pad="12"/>
<connect gate="G$1" pin="IN3A" pad="6"/>
<connect gate="G$1" pin="IN3B" pad="11"/>
<connect gate="G$1" pin="IN4A" pad="7"/>
<connect gate="G$1" pin="IN4B" pad="10"/>
<connect gate="G$1" pin="OUT-A" pad="8"/>
<connect gate="G$1" pin="OUT-B" pad="9"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7219CNG" prefix="IC">
<description>&lt;b&gt;LED DISPLAY DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX7219"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="DIG0" pad="2"/>
<connect gate="G$1" pin="DIG1" pad="11"/>
<connect gate="G$1" pin="DIG2" pad="6"/>
<connect gate="G$1" pin="DIG3" pad="7"/>
<connect gate="G$1" pin="DIG4" pad="3"/>
<connect gate="G$1" pin="DIG5" pad="10"/>
<connect gate="G$1" pin="DIG6" pad="5"/>
<connect gate="G$1" pin="DIG7" pad="8"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="24"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="LOAD" pad="12"/>
<connect gate="G$1" pin="SEGA" pad="14"/>
<connect gate="G$1" pin="SEGB" pad="16"/>
<connect gate="G$1" pin="SEGC" pad="20"/>
<connect gate="G$1" pin="SEGD" pad="23"/>
<connect gate="G$1" pin="SEGDP" pad="22"/>
<connect gate="G$1" pin="SEGE" pad="21"/>
<connect gate="G$1" pin="SEGF" pad="15"/>
<connect gate="G$1" pin="SEGG" pad="17"/>
<connect gate="G$1" pin="VCC" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX260" prefix="IC">
<description>Switched-capacitor &lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX260"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="BPA" pad="1"/>
<connect gate="G$1" pin="BPB" pad="21"/>
<connect gate="G$1" pin="CLK-OUT" pad="8"/>
<connect gate="G$1" pin="CLKA" pad="11"/>
<connect gate="G$1" pin="CLKB" pad="12"/>
<connect gate="G$1" pin="D0" pad="20"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="HPA" pad="3"/>
<connect gate="G$1" pin="HPB" pad="14"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="23"/>
<connect gate="G$1" pin="LPA" pad="24"/>
<connect gate="G$1" pin="LPB" pad="22"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="OSC-OUT" pad="19"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="17"/>
<connect gate="G$1" pin="WR" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX261" prefix="IC">
<description>Switched-capacitor &lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX261"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="A0" pad="14"/>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="BPA" pad="1"/>
<connect gate="G$1" pin="BPB" pad="21"/>
<connect gate="G$1" pin="CLK-OUT" pad="8"/>
<connect gate="G$1" pin="CLKA" pad="11"/>
<connect gate="G$1" pin="CLKB" pad="12"/>
<connect gate="G$1" pin="D0" pad="19"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="HPA" pad="3"/>
<connect gate="G$1" pin="HPB" pad="20"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="23"/>
<connect gate="G$1" pin="LPA" pad="24"/>
<connect gate="G$1" pin="LPB" pad="22"/>
<connect gate="G$1" pin="OP-IN" pad="4"/>
<connect gate="G$1" pin="OP-OUT" pad="2"/>
<connect gate="G$1" pin="OSC-OUT" pad="18"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="16"/>
<connect gate="G$1" pin="WR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX690ACSA" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX690"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VBATT" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="G$1" pin="WDI" pad="6"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX691ACSE" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX691"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="BATT-ON" pad="5"/>
<connect gate="G$1" pin="CE-IN" pad="13"/>
<connect gate="G$1" pin="CE-OUT" pad="12"/>
<connect gate="G$1" pin="LOW-LINE" pad="6"/>
<connect gate="G$1" pin="OSC-IN" pad="7"/>
<connect gate="G$1" pin="OSC-SEL" pad="8"/>
<connect gate="G$1" pin="PFI" pad="9"/>
<connect gate="G$1" pin="PFO" pad="10"/>
<connect gate="G$1" pin="RESET" pad="16"/>
<connect gate="G$1" pin="RESET@" pad="15"/>
<connect gate="G$1" pin="VBATT" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="WDI" pad="11"/>
<connect gate="G$1" pin="WDO" pad="14"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX326CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG201"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="S1" pad="3"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="11"/>
<connect gate="G$1" pin="S4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX328CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="DG508A"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="1" pin="A0" pad="1"/>
<connect gate="1" pin="A1" pad="16"/>
<connect gate="1" pin="A2" pad="15"/>
<connect gate="1" pin="D" pad="8"/>
<connect gate="1" pin="EN" pad="2"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="S1" pad="4"/>
<connect gate="1" pin="S2" pad="5"/>
<connect gate="1" pin="S3" pad="6"/>
<connect gate="1" pin="S4" pad="7"/>
<connect gate="1" pin="S5" pad="12"/>
<connect gate="1" pin="S6" pad="11"/>
<connect gate="1" pin="S7" pad="10"/>
<connect gate="1" pin="S8" pad="9"/>
<connect gate="1" pin="V+" pad="13"/>
<connect gate="1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX151CNG" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX151"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="A" pin="AGND" pad="23"/>
<connect gate="A" pin="BUSY" pad="11"/>
<connect gate="A" pin="CS" pad="14"/>
<connect gate="A" pin="DB0" pad="7"/>
<connect gate="A" pin="DB1" pad="8"/>
<connect gate="A" pin="DB2" pad="9"/>
<connect gate="A" pin="DB3" pad="10"/>
<connect gate="A" pin="DB4" pad="16"/>
<connect gate="A" pin="DB5" pad="17"/>
<connect gate="A" pin="DB6" pad="18"/>
<connect gate="A" pin="DB7" pad="19"/>
<connect gate="A" pin="DB8" pad="20"/>
<connect gate="A" pin="DB9" pad="21"/>
<connect gate="A" pin="DBX" pad="5"/>
<connect gate="A" pin="DBX@1" pad="6"/>
<connect gate="A" pin="DGND" pad="12"/>
<connect gate="A" pin="RD" pad="15"/>
<connect gate="A" pin="REF-OUT" pad="4"/>
<connect gate="A" pin="TP" pad="1"/>
<connect gate="A" pin="V-IN" pad="3"/>
<connect gate="A" pin="VDD" pad="22"/>
<connect gate="A" pin="VREF+" pad="2"/>
<connect gate="A" pin="VREF-" pad="24"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX764CPA" prefix="IC">
<description>&lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX764"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="AV+" pad="6"/>
<connect gate="A" pin="FB" pad="2"/>
<connect gate="A" pin="GND" pad="5"/>
<connect gate="A" pin="LX" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="SHDN" pad="3"/>
<connect gate="A" pin="V+" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX471CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX471"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="BATT" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="IOUT" pad="8"/>
<connect gate="A" pin="LOAD" pad="6"/>
<connect gate="A" pin="RS+" pad="3"/>
<connect gate="A" pin="RS-" pad="7"/>
<connect gate="A" pin="SHDN" pad="1"/>
<connect gate="A" pin="SIGN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX427CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OPOFF+-"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OFF1" pad="1"/>
<connect gate="G$1" pin="OFF2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX505CNG" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX505"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="A" pin="A0" pad="19"/>
<connect gate="A" pin="A1" pad="18"/>
<connect gate="A" pin="AGND" pad="6"/>
<connect gate="A" pin="D0" pad="16"/>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D2" pad="14"/>
<connect gate="A" pin="D3" pad="13"/>
<connect gate="A" pin="D4" pad="12"/>
<connect gate="A" pin="D5" pad="11"/>
<connect gate="A" pin="D6" pad="10"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="DGND" pad="7"/>
<connect gate="A" pin="LDAC" pad="8"/>
<connect gate="A" pin="VDD" pad="22"/>
<connect gate="A" pin="VOUT-A" pad="2"/>
<connect gate="A" pin="VOUT-B" pad="1"/>
<connect gate="A" pin="VOUT-C" pad="24"/>
<connect gate="A" pin="VOUT-D" pad="23"/>
<connect gate="A" pin="VREF-A" pad="5"/>
<connect gate="A" pin="VREF-B" pad="4"/>
<connect gate="A" pin="VREF-C" pad="21"/>
<connect gate="A" pin="VREF-D" pad="20"/>
<connect gate="A" pin="VSS" pad="3"/>
<connect gate="A" pin="WR" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX907CPA" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPUB"/>
<gate name="B" symbol="OP"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX368CPN" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX368"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="17"/>
<connect gate="G$1" pin="A2" pad="16"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="6"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="IN5" pad="13"/>
<connect gate="G$1" pin="IN6" pad="12"/>
<connect gate="G$1" pin="IN7" pad="11"/>
<connect gate="G$1" pin="IN8" pad="10"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="RS" pad="18"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="WR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX369CPN" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX369"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="17"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="IN1A" pad="5"/>
<connect gate="G$1" pin="IN1B" pad="14"/>
<connect gate="G$1" pin="IN2A" pad="6"/>
<connect gate="G$1" pin="IN2B" pad="13"/>
<connect gate="G$1" pin="IN3A" pad="7"/>
<connect gate="G$1" pin="IN3B" pad="12"/>
<connect gate="G$1" pin="IN4A" pad="8"/>
<connect gate="G$1" pin="IN4B" pad="11"/>
<connect gate="G$1" pin="OUTA" pad="9"/>
<connect gate="G$1" pin="OUTB" pad="10"/>
<connect gate="G$1" pin="RS" pad="18"/>
<connect gate="G$1" pin="V+" pad="15"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="WR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX329CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX329"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="OUTA" pad="8"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
<connect gate="G$1" pin="S1A" pad="4"/>
<connect gate="G$1" pin="S1B" pad="13"/>
<connect gate="G$1" pin="S2A" pad="5"/>
<connect gate="G$1" pin="S2B" pad="12"/>
<connect gate="G$1" pin="S3A" pad="6"/>
<connect gate="G$1" pin="S3B" pad="11"/>
<connect gate="G$1" pin="S4A" pad="7"/>
<connect gate="G$1" pin="S4B" pad="10"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX378CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX378"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="6"/>
<connect gate="G$1" pin="IN4" pad="7"/>
<connect gate="G$1" pin="IN5" pad="12"/>
<connect gate="G$1" pin="IN6" pad="11"/>
<connect gate="G$1" pin="IN7" pad="10"/>
<connect gate="G$1" pin="IN8" pad="9"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX379CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX379"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IN1A" pad="4"/>
<connect gate="G$1" pin="IN1B" pad="13"/>
<connect gate="G$1" pin="IN2A" pad="5"/>
<connect gate="G$1" pin="IN2B" pad="12"/>
<connect gate="G$1" pin="IN3A" pad="6"/>
<connect gate="G$1" pin="IN3B" pad="11"/>
<connect gate="G$1" pin="IN4A" pad="7"/>
<connect gate="G$1" pin="IN4B" pad="10"/>
<connect gate="G$1" pin="OUTA" pad="8"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX220CPE" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX220"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX222CPN" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX222"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="R1IN" pad="14"/>
<connect gate="G$1" pin="R1OUT" pad="13"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="SHDN" pad="18"/>
<connect gate="G$1" pin="T1IN" pad="12"/>
<connect gate="G$1" pin="T1OUT" pad="15"/>
<connect gate="G$1" pin="T2IN" pad="11"/>
<connect gate="G$1" pin="T2OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VCC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX250CPD" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX250"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="EN" pad="8"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="R1DIN" pad="10"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="R2DIN" pad="11"/>
<connect gate="G$1" pin="R2OUT" pad="12"/>
<connect gate="G$1" pin="SHDN" pad="1"/>
<connect gate="G$1" pin="T1IN" pad="4"/>
<connect gate="G$1" pin="T1LDR" pad="3"/>
<connect gate="G$1" pin="T2IN" pad="5"/>
<connect gate="G$1" pin="T2LDR" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX251CPD" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX251"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="AC" pad="1"/>
<connect gate="G$1" pin="BYP" pad="7"/>
<connect gate="G$1" pin="ISO-GND" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="10"/>
<connect gate="G$1" pin="R1LDR" pad="5"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2LDR" pad="6"/>
<connect gate="G$1" pin="RTRI" pad="8"/>
<connect gate="G$1" pin="T1DIN" pad="3"/>
<connect gate="G$1" pin="T1OUT" pad="12"/>
<connect gate="G$1" pin="T2DIN" pad="4"/>
<connect gate="G$1" pin="T2OUT" pad="11"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX252A" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX252"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="AC" pad="40"/>
<connect gate="G$1" pin="BYP" pad="31"/>
<connect gate="G$1" pin="D1" pad="4"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="DETCOM" pad="19"/>
<connect gate="G$1" pin="EN" pad="11"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="IDCOM" pad="25"/>
<connect gate="G$1" pin="ILCOM" pad="22"/>
<connect gate="G$1" pin="ISOGND" pad="38"/>
<connect gate="G$1" pin="LEDCOM" pad="16"/>
<connect gate="G$1" pin="R1DET" pad="18"/>
<connect gate="G$1" pin="R1DIN" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="34"/>
<connect gate="G$1" pin="R1LDR" pad="29"/>
<connect gate="G$1" pin="R1LED" pad="23"/>
<connect gate="G$1" pin="R1OUT" pad="1"/>
<connect gate="G$1" pin="R2DET" pad="20"/>
<connect gate="G$1" pin="R2DIN" pad="13"/>
<connect gate="G$1" pin="R2IN" pad="33"/>
<connect gate="G$1" pin="R2LDR" pad="30"/>
<connect gate="G$1" pin="R2LED" pad="21"/>
<connect gate="G$1" pin="R2OUT" pad="12"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="T1DET" pad="26"/>
<connect gate="G$1" pin="T1DIN" pad="27"/>
<connect gate="G$1" pin="T1IN" pad="8"/>
<connect gate="G$1" pin="T1LDR" pad="9"/>
<connect gate="G$1" pin="T1LED" pad="15"/>
<connect gate="G$1" pin="T1OUT" pad="36"/>
<connect gate="G$1" pin="T2DET" pad="24"/>
<connect gate="G$1" pin="T2DIN" pad="28"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T2LDR" pad="6"/>
<connect gate="G$1" pin="T2LED" pad="17"/>
<connect gate="G$1" pin="T2OUT" pad="35"/>
<connect gate="G$1" pin="V+" pad="37"/>
<connect gate="G$1" pin="V+@1" pad="32"/>
<connect gate="G$1" pin="V-" pad="39"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX406CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX406"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BW" pad="8"/>
<connect gate="G$1" pin="OFF1" pad="1"/>
<connect gate="G$1" pin="OFF2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX412CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPUB"/>
<gate name="B" symbol="OP"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX620CPN" prefix="IC">
<description>&lt;b&gt;MOSFET DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX620"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="A" pin="C1+" pad="11"/>
<connect gate="A" pin="C1-" pad="10"/>
<connect gate="A" pin="C2+" pad="9"/>
<connect gate="A" pin="C2-" pad="13"/>
<connect gate="A" pin="CE" pad="5"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN1" pad="15"/>
<connect gate="A" pin="IN2" pad="16"/>
<connect gate="A" pin="IN3" pad="3"/>
<connect gate="A" pin="IN4" pad="4"/>
<connect gate="A" pin="OUT1" pad="18"/>
<connect gate="A" pin="OUT2" pad="17"/>
<connect gate="A" pin="OUT3" pad="2"/>
<connect gate="A" pin="OUT4" pad="1"/>
<connect gate="A" pin="PR" pad="6"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX622CPA" prefix="IC">
<description>&lt;b&gt;POWER SUPPLY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX622"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="7"/>
<connect gate="G$1" pin="C2+" pad="6"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PR" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX623CPE" prefix="IC">
<description>&lt;b&gt;POWER SUPPLY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX623"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PR" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VOUT" pad="9"/>
<connect gate="G$1" pin="VOUT@1" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX654CPD" prefix="IC">
<description>Step-up &lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX654"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CTL" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="HPGND" pad="12"/>
<connect gate="G$1" pin="HPGND@1" pad="14"/>
<connect gate="G$1" pin="LBI" pad="6"/>
<connect gate="G$1" pin="LBO" pad="5"/>
<connect gate="G$1" pin="LX1" pad="9"/>
<connect gate="G$1" pin="LX2" pad="1"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="PR" pad="11"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX656CPD" prefix="IC">
<description>Step-up &lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX656"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CTL" pad="13"/>
<connect gate="G$1" pin="D" pad="12"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="LBI" pad="6"/>
<connect gate="G$1" pin="LBO" pad="5"/>
<connect gate="G$1" pin="LX1" pad="9"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="PR" pad="11"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX660CPA" prefix="IC">
<description>Charge-pump &lt;b&gt;VOLTAGE CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX660"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="C+" pad="2"/>
<connect gate="G$1" pin="C-" pad="4"/>
<connect gate="G$1" pin="FC" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LV" pad="6"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX667CPA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX667"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="DD" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="LBI" pad="3"/>
<connect gate="G$1" pin="LBO" pad="7"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="SET" pad="6"/>
<connect gate="G$1" pin="SHDN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX742CPP" prefix="IC">
<description>&lt;b&gt;PWM SWITCH-MODE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX742"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="100/200" pad="5"/>
<connect gate="G$1" pin="12/15" pad="6"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AV+" pad="4"/>
<connect gate="G$1" pin="CC+" pad="2"/>
<connect gate="G$1" pin="CC-" pad="9"/>
<connect gate="G$1" pin="CSH+" pad="20"/>
<connect gate="G$1" pin="CSH-" pad="12"/>
<connect gate="G$1" pin="CSL+" pad="19"/>
<connect gate="G$1" pin="CSL-" pad="11"/>
<connect gate="G$1" pin="EXT+" pad="17"/>
<connect gate="G$1" pin="EXT-" pad="14"/>
<connect gate="G$1" pin="FB+" pad="1"/>
<connect gate="G$1" pin="FB-" pad="10"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="PDRV" pad="15"/>
<connect gate="G$1" pin="PUMP" pad="16"/>
<connect gate="G$1" pin="SS" pad="8"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX743CPE" prefix="IC">
<description>&lt;b&gt;PWM SWITCH-MODE REGULATOR&lt;/b&gt;r</description>
<gates>
<gate name="G$1" symbol="MAX743"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="12/15" pad="11"/>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="AV+" pad="3"/>
<connect gate="G$1" pin="CC+" pad="1"/>
<connect gate="G$1" pin="CC-" pad="8"/>
<connect gate="G$1" pin="FB+" pad="16"/>
<connect gate="G$1" pin="FB-" pad="9"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="LX+" pad="15"/>
<connect gate="G$1" pin="LX-" pad="10"/>
<connect gate="G$1" pin="SS" pad="7"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V+@1" pad="12"/>
<connect gate="G$1" pin="V+@2" pad="4"/>
<connect gate="G$1" pin="V+@3" pad="5"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1232CPA" prefix="IC">
<description>MONITOR DEVICE</description>
<gates>
<gate name="G$1" symbol="MAX1232"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PBRST" pad="1"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="RST@1" pad="5"/>
<connect gate="G$1" pin="ST" pad="7"/>
<connect gate="G$1" pin="TD" pad="2"/>
<connect gate="G$1" pin="TOL" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX687CPA" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX687"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="BASE" pad="7"/>
<connect gate="G$1" pin="BLIM" pad="6"/>
<connect gate="G$1" pin="CC" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="PFO" pad="3"/>
<connect gate="G$1" pin="SHDN" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX699CPA" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX699"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="RST" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="WDI" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX700CPA" prefix="IC">
<description>&lt;b&gt;POWER SUPPLY MONITOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX700"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CTL" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HYST" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="RST@1" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX701CPA" prefix="IC">
<description>&lt;b&gt;POWER SUPPLY MONITOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX701"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="RST@1" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX702CPA" prefix="IC">
<description>&lt;b&gt;POWER SUPPLY MONITOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX702"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="RST" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX270CPP" prefix="IC">
<description>&lt;b&gt;DIGITAL FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX270"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="CS" pad="11"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="18"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="7"/>
<connect gate="G$1" pin="OPIN" pad="20"/>
<connect gate="G$1" pin="OPOUT" pad="1"/>
<connect gate="G$1" pin="OUTA" pad="3"/>
<connect gate="G$1" pin="OUTB" pad="8"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="WR" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX271CNG" prefix="IC">
<description>&lt;b&gt;DIGITAL FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX271"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="A0" pad="16"/>
<connect gate="G$1" pin="A1" pad="15"/>
<connect gate="G$1" pin="CS" pad="14"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="18"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="20"/>
<connect gate="G$1" pin="D4" pad="21"/>
<connect gate="G$1" pin="D5" pad="22"/>
<connect gate="G$1" pin="D6" pad="23"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="7"/>
<connect gate="G$1" pin="MODE" pad="8"/>
<connect gate="G$1" pin="OUTA" pad="3"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
<connect gate="G$1" pin="T/H" pad="24"/>
<connect gate="G$1" pin="T/HA/B" pad="11"/>
<connect gate="G$1" pin="T/HEN" pad="13"/>
<connect gate="G$1" pin="T/HOUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="WR" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX280CP" prefix="IC">
<description>Switched-capacitor &lt;b&gt;FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX280"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="BOUT" pad="8"/>
<connect gate="G$1" pin="COSC" pad="5"/>
<connect gate="G$1" pin="DIR" pad="4"/>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX171ACP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX171"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="AIN" pad="4"/>
<connect gate="G$1" pin="CK+" pad="13"/>
<connect gate="G$1" pin="CK-" pad="12"/>
<connect gate="G$1" pin="DATA" pad="11"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I_AGND" pad="6"/>
<connect gate="G$1" pin="I_DGND" pad="1"/>
<connect gate="G$1" pin="I_DGND@" pad="8"/>
<connect gate="G$1" pin="I_V+" pad="3"/>
<connect gate="G$1" pin="I_V-" pad="2"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="S+" pad="14"/>
<connect gate="G$1" pin="S-" pad="15"/>
<connect gate="G$1" pin="TP" pad="7"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX174AC" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX174"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="10VIN" pad="13"/>
<connect gate="G$1" pin="12/8" pad="2"/>
<connect gate="G$1" pin="20VIN" pad="14"/>
<connect gate="G$1" pin="A0" pad="4"/>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="BIPOFF" pad="12"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="CS" pad="3"/>
<connect gate="G$1" pin="D0" pad="16"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="26"/>
<connect gate="G$1" pin="D11" pad="27"/>
<connect gate="G$1" pin="D2" pad="18"/>
<connect gate="G$1" pin="D3" pad="19"/>
<connect gate="G$1" pin="D4" pad="20"/>
<connect gate="G$1" pin="D5" pad="21"/>
<connect gate="G$1" pin="D6" pad="22"/>
<connect gate="G$1" pin="D7" pad="23"/>
<connect gate="G$1" pin="D8" pad="24"/>
<connect gate="G$1" pin="D9" pad="25"/>
<connect gate="G$1" pin="DGND" pad="15"/>
<connect gate="G$1" pin="R/C" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="STS" pad="28"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VEE" pad="11"/>
<connect gate="G$1" pin="VL+" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX178ACN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX178"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="AIN" pad="2"/>
<connect gate="G$1" pin="BUSY" pad="20"/>
<connect gate="G$1" pin="BYSL" pad="19"/>
<connect gate="G$1" pin="CAZ" pad="1"/>
<connect gate="G$1" pin="CLK" pad="21"/>
<connect gate="G$1" pin="CS" pad="17"/>
<connect gate="G$1" pin="DB0" pad="15"/>
<connect gate="G$1" pin="DB1" pad="14"/>
<connect gate="G$1" pin="DB2" pad="13"/>
<connect gate="G$1" pin="DB3" pad="12"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="10"/>
<connect gate="G$1" pin="DB6" pad="9"/>
<connect gate="G$1" pin="DB7" pad="8"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="RD" pad="16"/>
<connect gate="G$1" pin="REFIN" pad="4"/>
<connect gate="G$1" pin="REFOUT" pad="22"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="23"/>
<connect gate="G$1" pin="WR" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX180ACP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX180"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A0" pad="37"/>
<connect gate="G$1" pin="A1" pad="38"/>
<connect gate="G$1" pin="A2" pad="39"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AIN4" pad="5"/>
<connect gate="G$1" pin="AIN5" pad="6"/>
<connect gate="G$1" pin="AIN6" pad="7"/>
<connect gate="G$1" pin="AIN7" pad="8"/>
<connect gate="G$1" pin="BIP" pad="36"/>
<connect gate="G$1" pin="BUSY" pad="34"/>
<connect gate="G$1" pin="CLKIN" pad="29"/>
<connect gate="G$1" pin="CS" pad="33"/>
<connect gate="G$1" pin="D0" pad="28"/>
<connect gate="G$1" pin="D1" pad="27"/>
<connect gate="G$1" pin="D10" pad="17"/>
<connect gate="G$1" pin="D11" pad="16"/>
<connect gate="G$1" pin="D2" pad="26"/>
<connect gate="G$1" pin="D3" pad="25"/>
<connect gate="G$1" pin="D4" pad="24"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="22"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="D8" pad="19"/>
<connect gate="G$1" pin="D9" pad="18"/>
<connect gate="G$1" pin="DGND" pad="20"/>
<connect gate="G$1" pin="DIFF" pad="35"/>
<connect gate="G$1" pin="HBEN" pad="30"/>
<connect gate="G$1" pin="MODE" pad="14"/>
<connect gate="G$1" pin="OFFADJ" pad="13"/>
<connect gate="G$1" pin="RD" pad="31"/>
<connect gate="G$1" pin="REFADJ" pad="12"/>
<connect gate="G$1" pin="REFIN" pad="9"/>
<connect gate="G$1" pin="REFOUT" pad="11"/>
<connect gate="G$1" pin="VDD" pad="40"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="WR" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX182ACP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX182"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="25"/>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="BUSY" pad="22"/>
<connect gate="G$1" pin="BYSL" pad="21"/>
<connect gate="G$1" pin="CAZ" pad="1"/>
<connect gate="G$1" pin="CLK" pad="23"/>
<connect gate="G$1" pin="CS" pad="19"/>
<connect gate="G$1" pin="DB0" pad="17"/>
<connect gate="G$1" pin="DB1" pad="16"/>
<connect gate="G$1" pin="DB2" pad="15"/>
<connect gate="G$1" pin="DB3" pad="14"/>
<connect gate="G$1" pin="DB4" pad="13"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="11"/>
<connect gate="G$1" pin="DB7" pad="10"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="RD" pad="18"/>
<connect gate="G$1" pin="REFIN" pad="6"/>
<connect gate="G$1" pin="REFOUT" pad="26"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS" pad="27"/>
<connect gate="G$1" pin="WR" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX183ACN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX183"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AIN1" pad="1"/>
<connect gate="G$1" pin="AIN2" pad="24"/>
<connect gate="G$1" pin="BUSY" pad="21"/>
<connect gate="G$1" pin="CLKIN" pad="17"/>
<connect gate="G$1" pin="CLKOUT" pad="18"/>
<connect gate="G$1" pin="CS" pad="20"/>
<connect gate="G$1" pin="D0" pad="16"/>
<connect gate="G$1" pin="D1" pad="15"/>
<connect gate="G$1" pin="D10" pad="5"/>
<connect gate="G$1" pin="D11" pad="4"/>
<connect gate="G$1" pin="D2" pad="14"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="11"/>
<connect gate="G$1" pin="D5" pad="10"/>
<connect gate="G$1" pin="D6" pad="9"/>
<connect gate="G$1" pin="D7" pad="8"/>
<connect gate="G$1" pin="D8" pad="7"/>
<connect gate="G$1" pin="D9" pad="6"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="RD" pad="19"/>
<connect gate="G$1" pin="VDD" pad="23"/>
<connect gate="G$1" pin="VREF" pad="2"/>
<connect gate="G$1" pin="VSS" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX404CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX404"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VT1" pad="1"/>
<connect gate="G$1" pin="VT2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX405CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX405"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="NULL" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VC+" pad="8"/>
<connect gate="G$1" pin="VC-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX457CPA" prefix="IC">
<description>&lt;b&gt;VIDEO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPUB"/>
<gate name="B" symbol="OP"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX900ACP" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX900"/>
<gate name="B" symbol="MAX900"/>
<gate name="C" symbol="MAX900"/>
<gate name="D" symbol="MAX900"/>
<gate name="P" symbol="PWR1"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="LATCH" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="B" pin="+IN" pad="9"/>
<connect gate="B" pin="-IN" pad="10"/>
<connect gate="B" pin="LATCH" pad="7"/>
<connect gate="B" pin="OUT" pad="6"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="LATCH" pad="14"/>
<connect gate="C" pin="OUT" pad="15"/>
<connect gate="D" pin="+IN" pad="19"/>
<connect gate="D" pin="-IN" pad="20"/>
<connect gate="D" pin="LATCH" pad="17"/>
<connect gate="D" pin="OUT" pad="16"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="18"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VEE" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX901ACP" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
<gate name="P" symbol="PWR1"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="8"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="12"/>
<connect gate="D" pin="+IN" pad="15"/>
<connect gate="D" pin="-IN" pad="16"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="14"/>
<connect gate="P" pin="VDD" pad="11"/>
<connect gate="P" pin="VEE" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX902CPD" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX900"/>
<gate name="B" symbol="MAX900"/>
<gate name="P" symbol="PWR1"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="LATCH" pad="4"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="B" pin="+IN" pad="9"/>
<connect gate="B" pin="-IN" pad="8"/>
<connect gate="B" pin="LATCH" pad="11"/>
<connect gate="B" pin="OUT" pad="12"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="14"/>
<connect gate="P" pin="VDD" pad="10"/>
<connect gate="P" pin="VEE" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX903CPA" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MAX900"/>
<gate name="P" symbol="PWR1"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="LATCH" pad="5"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="VCC" pad="1"/>
<connect gate="P" pin="VDD" pad="8"/>
<connect gate="P" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX500ACP" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX500"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="LDAC" pad="7"/>
<connect gate="G$1" pin="LOAD" pad="9"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="1"/>
<connect gate="G$1" pin="OUTC" pad="16"/>
<connect gate="G$1" pin="OUTD" pad="15"/>
<connect gate="G$1" pin="REFA/B" pad="4"/>
<connect gate="G$1" pin="REFC" pad="13"/>
<connect gate="G$1" pin="REFD" pad="12"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="8"/>
<connect gate="G$1" pin="SRO" pad="11"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX516ACN" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX516"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="AIN0" pad="5"/>
<connect gate="G$1" pin="AIN1" pad="4"/>
<connect gate="G$1" pin="AIN2" pad="21"/>
<connect gate="G$1" pin="AIN3" pad="20"/>
<connect gate="G$1" pin="C0" pad="2"/>
<connect gate="G$1" pin="C1" pad="1"/>
<connect gate="G$1" pin="C2" pad="24"/>
<connect gate="G$1" pin="C3" pad="23"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="14"/>
<connect gate="G$1" pin="D5" pad="13"/>
<connect gate="G$1" pin="D6" pad="12"/>
<connect gate="G$1" pin="D7" pad="11"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="REF" pad="19"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VDD" pad="22"/>
<connect gate="G$1" pin="WR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX543AC" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX543"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IOUT" pad="3"/>
<connect gate="G$1" pin="LOAD" pad="5"/>
<connect gate="G$1" pin="RFB" pad="2"/>
<connect gate="G$1" pin="SRI" pad="6"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX414CPD" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPUB"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG401DJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG401"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="8"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="IN1" pad="15"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="S1" pad="16"/>
<connect gate="G$1" pin="S2" pad="9"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="14"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG403DJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG403"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="8"/>
<connect gate="G$1" pin="D3" pad="3"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="IN1" pad="15"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="S1" pad="16"/>
<connect gate="G$1" pin="S2" pad="9"/>
<connect gate="G$1" pin="S3" pad="4"/>
<connect gate="G$1" pin="S4" pad="5"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="14"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG406DJ" prefix="IC">
<description>&lt;b&gt;ANALOG MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG406"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="D" pad="28"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="S1" pad="19"/>
<connect gate="G$1" pin="S10" pad="10"/>
<connect gate="G$1" pin="S11" pad="9"/>
<connect gate="G$1" pin="S12" pad="8"/>
<connect gate="G$1" pin="S13" pad="7"/>
<connect gate="G$1" pin="S14" pad="6"/>
<connect gate="G$1" pin="S15" pad="5"/>
<connect gate="G$1" pin="S16" pad="4"/>
<connect gate="G$1" pin="S2" pad="20"/>
<connect gate="G$1" pin="S3" pad="21"/>
<connect gate="G$1" pin="S4" pad="22"/>
<connect gate="G$1" pin="S5" pad="23"/>
<connect gate="G$1" pin="S6" pad="24"/>
<connect gate="G$1" pin="S7" pad="25"/>
<connect gate="G$1" pin="S8" pad="26"/>
<connect gate="G$1" pin="S9" pad="11"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG407DJ" prefix="IC">
<description>&lt;b&gt;ANALOG MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG407"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="DA" pad="28"/>
<connect gate="G$1" pin="DB" pad="2"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="S1A" pad="19"/>
<connect gate="G$1" pin="S1B" pad="11"/>
<connect gate="G$1" pin="S2A" pad="20"/>
<connect gate="G$1" pin="S2B" pad="10"/>
<connect gate="G$1" pin="S3A" pad="21"/>
<connect gate="G$1" pin="S3B" pad="9"/>
<connect gate="G$1" pin="S4A" pad="22"/>
<connect gate="G$1" pin="S4B" pad="8"/>
<connect gate="G$1" pin="S5A" pad="23"/>
<connect gate="G$1" pin="S5B" pad="7"/>
<connect gate="G$1" pin="S6A" pad="24"/>
<connect gate="G$1" pin="S6B" pad="6"/>
<connect gate="G$1" pin="S7A" pad="25"/>
<connect gate="G$1" pin="S7B" pad="5"/>
<connect gate="G$1" pin="S8A" pad="26"/>
<connect gate="G$1" pin="S8B" pad="4"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG408DJ" prefix="IC">
<description>&lt;b&gt;ANALOG MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG408"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="6"/>
<connect gate="G$1" pin="S4" pad="7"/>
<connect gate="G$1" pin="S5" pad="12"/>
<connect gate="G$1" pin="S6" pad="11"/>
<connect gate="G$1" pin="S7" pad="10"/>
<connect gate="G$1" pin="S8" pad="9"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG409DJ" prefix="IC">
<description>&lt;b&gt;ANALOG MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG409"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DA" pad="8"/>
<connect gate="G$1" pin="DB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="S1A" pad="4"/>
<connect gate="G$1" pin="S1B" pad="13"/>
<connect gate="G$1" pin="S2A" pad="5"/>
<connect gate="G$1" pin="S2B" pad="12"/>
<connect gate="G$1" pin="S3A" pad="6"/>
<connect gate="G$1" pin="S3B" pad="11"/>
<connect gate="G$1" pin="S4A" pad="7"/>
<connect gate="G$1" pin="S4B" pad="10"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG411DJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG411"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="S1" pad="3"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="11"/>
<connect gate="G$1" pin="S4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG417CJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG417"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="6"/>
<connect gate="G$1" pin="S1" pad="1"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG418CJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG417"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="6"/>
<connect gate="G$1" pin="S1" pad="8"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG419CJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG419"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN1" pad="6"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="8"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG441DJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG441"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="S1" pad="3"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="11"/>
<connect gate="G$1" pin="S4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX407CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPUB"/>
<gate name="B" symbol="OP"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX905CPD" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX905"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="CLK@" pad="11"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="OUT@" pad="13"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VEE" pad="1"/>
<connect gate="G$1" pin="VEES" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX906CPE" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MAX906"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="1" pin="+INA" pad="2"/>
<connect gate="1" pin="+INB" pad="7"/>
<connect gate="1" pin="-INA" pad="3"/>
<connect gate="1" pin="-INB" pad="6"/>
<connect gate="1" pin="AGND" pad="4"/>
<connect gate="1" pin="CLK" pad="12"/>
<connect gate="1" pin="CLK@" pad="13"/>
<connect gate="1" pin="DGND" pad="14"/>
<connect gate="1" pin="QA" pad="16"/>
<connect gate="1" pin="QA@" pad="15"/>
<connect gate="1" pin="QB" pad="9"/>
<connect gate="1" pin="QB@" pad="10"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="1" pin="VEEA" pad="1"/>
<connect gate="1" pin="VEEB" pad="8"/>
<connect gate="1" pin="VEES" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX911CNG" prefix="IC">
<description>&lt;b&gt;VOLTAGE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MAX911"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="1" pin="CMP_GND" pad="18"/>
<connect gate="1" pin="D0" pad="21"/>
<connect gate="1" pin="D1" pad="22"/>
<connect gate="1" pin="D2" pad="23"/>
<connect gate="1" pin="D3" pad="24"/>
<connect gate="1" pin="D4" pad="1"/>
<connect gate="1" pin="D5" pad="2"/>
<connect gate="1" pin="D6" pad="3"/>
<connect gate="1" pin="D7" pad="4"/>
<connect gate="1" pin="GND@1" pad="15"/>
<connect gate="1" pin="GND@2" pad="20"/>
<connect gate="1" pin="IN+" pad="13"/>
<connect gate="1" pin="IN-" pad="14"/>
<connect gate="1" pin="LATCH" pad="5"/>
<connect gate="1" pin="Q_OUT" pad="19"/>
<connect gate="1" pin="Q_OUT@" pad="17"/>
<connect gate="1" pin="RA" pad="10"/>
<connect gate="1" pin="RB" pad="11"/>
<connect gate="1" pin="REFIN" pad="8"/>
<connect gate="1" pin="REFOUT" pad="9"/>
<connect gate="1" pin="TH_CTRL" pad="16"/>
<connect gate="1" pin="TH_OUT" pad="12"/>
<connect gate="1" pin="VCC" pad="6"/>
<connect gate="1" pin="VEE" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX662CPA" prefix="IC">
<description>&lt;b&gt;SUPPLY CHARGE PUMP&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MAX662"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="1" pin="C1+" pad="2"/>
<connect gate="1" pin="C1-" pad="1"/>
<connect gate="1" pin="C2+" pad="4"/>
<connect gate="1" pin="C2-" pad="3"/>
<connect gate="1" pin="GND" pad="7"/>
<connect gate="1" pin="SHDN" pad="8"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX714CPE" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MAX714"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="1" pin="AGND" pad="16"/>
<connect gate="1" pin="B1" pad="6"/>
<connect gate="1" pin="B2" pad="8"/>
<connect gate="1" pin="B6" pad="9"/>
<connect gate="1" pin="B6N" pad="10"/>
<connect gate="1" pin="BAT" pad="15"/>
<connect gate="1" pin="E6" pad="14"/>
<connect gate="1" pin="LBO" pad="3"/>
<connect gate="1" pin="ON" pad="4"/>
<connect gate="1" pin="PGND" pad="1"/>
<connect gate="1" pin="RS_O" pad="12"/>
<connect gate="1" pin="S1" pad="5"/>
<connect gate="1" pin="S2" pad="7"/>
<connect gate="1" pin="S6" pad="11"/>
<connect gate="1" pin="U6" pad="13"/>
<connect gate="1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX715CNG" prefix="IC">
<description>&lt;b&gt;SUPPLY SYSTEM&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MAX715"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="1" pin="AGND" pad="2"/>
<connect gate="1" pin="B1" pad="8"/>
<connect gate="1" pin="B2" pad="10"/>
<connect gate="1" pin="B3" pad="11"/>
<connect gate="1" pin="B5" pad="13"/>
<connect gate="1" pin="B6" pad="15"/>
<connect gate="1" pin="B7" pad="17"/>
<connect gate="1" pin="BAT" pad="1"/>
<connect gate="1" pin="E3" pad="20"/>
<connect gate="1" pin="E5" pad="22"/>
<connect gate="1" pin="E6" pad="23"/>
<connect gate="1" pin="E7" pad="24"/>
<connect gate="1" pin="LBO" pad="5"/>
<connect gate="1" pin="ON" pad="6"/>
<connect gate="1" pin="PGND" pad="3"/>
<connect gate="1" pin="RS_O" pad="19"/>
<connect gate="1" pin="S1" pad="7"/>
<connect gate="1" pin="S2" pad="9"/>
<connect gate="1" pin="S3" pad="12"/>
<connect gate="1" pin="S5" pad="14"/>
<connect gate="1" pin="S6" pad="16"/>
<connect gate="1" pin="S7" pad="18"/>
<connect gate="1" pin="U6" pad="21"/>
<connect gate="1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX716CPI" prefix="IC">
<description>&lt;b&gt;SUPPLY SYSTEM&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="MAX716"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="1" pin="AGND" pad="2"/>
<connect gate="1" pin="B1" pad="10"/>
<connect gate="1" pin="B2" pad="12"/>
<connect gate="1" pin="B3" pad="13"/>
<connect gate="1" pin="B4" pad="8"/>
<connect gate="1" pin="B5" pad="15"/>
<connect gate="1" pin="B6" pad="17"/>
<connect gate="1" pin="B7" pad="19"/>
<connect gate="1" pin="BAT" pad="1"/>
<connect gate="1" pin="E3" pad="22"/>
<connect gate="1" pin="E4" pad="24"/>
<connect gate="1" pin="E5" pad="26"/>
<connect gate="1" pin="E6" pad="27"/>
<connect gate="1" pin="E7" pad="28"/>
<connect gate="1" pin="LBO" pad="5"/>
<connect gate="1" pin="ON" pad="6"/>
<connect gate="1" pin="PGND" pad="3"/>
<connect gate="1" pin="RS_O" pad="21"/>
<connect gate="1" pin="S1" pad="9"/>
<connect gate="1" pin="S2" pad="11"/>
<connect gate="1" pin="S3" pad="14"/>
<connect gate="1" pin="S4" pad="7"/>
<connect gate="1" pin="S5" pad="16"/>
<connect gate="1" pin="S6" pad="18"/>
<connect gate="1" pin="S7" pad="20"/>
<connect gate="1" pin="U6" pad="25"/>
<connect gate="1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX722CSE" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX722"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="3/5" pad="3"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="CS+" pad="9"/>
<connect gate="G$1" pin="CS-" pad="10"/>
<connect gate="G$1" pin="DHI" pad="11"/>
<connect gate="G$1" pin="DLOW" pad="12"/>
<connect gate="G$1" pin="FB3" pad="7"/>
<connect gate="G$1" pin="FBN" pad="8"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="LIN" pad="13"/>
<connect gate="G$1" pin="LX3" pad="15"/>
<connect gate="G$1" pin="NEGON" pad="2"/>
<connect gate="G$1" pin="PFO" pad="4"/>
<connect gate="G$1" pin="SHDN" pad="1"/>
<connect gate="G$1" pin="V+" pad="16"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX730CPA" prefix="IC">
<description>&lt;b&gt;DC/DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX730"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CC" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LX" pad="7"/>
<connect gate="G$1" pin="SHDN" pad="1"/>
<connect gate="G$1" pin="SS" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX731CPA" prefix="IC">
<description>&lt;b&gt;DC/DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX730"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CC" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LX" pad="6"/>
<connect gate="G$1" pin="SHDN" pad="1"/>
<connect gate="G$1" pin="SS" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX736CPD" prefix="IC">
<description>&lt;b&gt;DC/DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX736"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="CC" pad="7"/>
<connect gate="G$1" pin="DRV-" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LX" pad="11"/>
<connect gate="G$1" pin="LX@" pad="12"/>
<connect gate="G$1" pin="SHDN" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V+@" pad="13"/>
<connect gate="G$1" pin="V+@1" pad="14"/>
<connect gate="G$1" pin="VOUT" pad="8"/>
<connect gate="G$1" pin="VREF" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX741UCP" prefix="IC">
<description>&lt;b&gt;PWM CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX741"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="CSA" pad="15"/>
<connect gate="G$1" pin="CSB" pad="14"/>
<connect gate="G$1" pin="DRV-" pad="16"/>
<connect gate="G$1" pin="DUTY" pad="12"/>
<connect gate="G$1" pin="EAIN" pad="11"/>
<connect gate="G$1" pin="EAO" pad="10"/>
<connect gate="G$1" pin="FREQ" pad="20"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="OUTA" pad="18"/>
<connect gate="G$1" pin="OUTB" pad="17"/>
<connect gate="G$1" pin="P/N" pad="13"/>
<connect gate="G$1" pin="P/Z/N" pad="4"/>
<connect gate="G$1" pin="SLOPE" pad="1"/>
<connect gate="G$1" pin="SS" pad="8"/>
<connect gate="G$1" pin="SYNC" pad="2"/>
<connect gate="G$1" pin="UVLO" pad="7"/>
<connect gate="G$1" pin="V+" pad="19"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
<connect gate="G$1" pin="VREF" pad="6"/>
<connect gate="G$1" pin="VSEL" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX705CPA" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX705"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="WDI" pad="6"/>
<connect gate="G$1" pin="WDO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX707CPA" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX707"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="RESET@" pad="8"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX274ACN" prefix="IC">
<description>&lt;b&gt;ANALOG FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX274"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="BPIA" pad="3"/>
<connect gate="G$1" pin="BPIB" pad="10"/>
<connect gate="G$1" pin="BPIC" pad="15"/>
<connect gate="G$1" pin="BPID" pad="22"/>
<connect gate="G$1" pin="BPOA" pad="4"/>
<connect gate="G$1" pin="BPOB" pad="9"/>
<connect gate="G$1" pin="BPOC" pad="16"/>
<connect gate="G$1" pin="BPOD" pad="21"/>
<connect gate="G$1" pin="FC" pad="8"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="INA" pad="2"/>
<connect gate="G$1" pin="INB" pad="11"/>
<connect gate="G$1" pin="INC" pad="14"/>
<connect gate="G$1" pin="IND" pad="23"/>
<connect gate="G$1" pin="LPIA" pad="6"/>
<connect gate="G$1" pin="LPIB" pad="7"/>
<connect gate="G$1" pin="LPIC" pad="18"/>
<connect gate="G$1" pin="LPID" pad="19"/>
<connect gate="G$1" pin="LPOA" pad="1"/>
<connect gate="G$1" pin="LPOB" pad="12"/>
<connect gate="G$1" pin="LPOC" pad="13"/>
<connect gate="G$1" pin="LPOD" pad="24"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX275ACP" prefix="IC">
<description>&lt;b&gt;ANALOG FILTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX275"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="BPIA" pad="7"/>
<connect gate="G$1" pin="BPIB" pad="15"/>
<connect gate="G$1" pin="BPOA" pad="4"/>
<connect gate="G$1" pin="BPOB" pad="18"/>
<connect gate="G$1" pin="FCA" pad="9"/>
<connect gate="G$1" pin="FCB" pad="12"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="INA" pad="8"/>
<connect gate="G$1" pin="INB" pad="14"/>
<connect gate="G$1" pin="LPIA" pad="6"/>
<connect gate="G$1" pin="LPIB" pad="16"/>
<connect gate="G$1" pin="LPOA" pad="2"/>
<connect gate="G$1" pin="LPOB" pad="19"/>
<connect gate="G$1" pin="V+" pad="20"/>
<connect gate="G$1" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX120" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX120"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN" pad="4"/>
<connect gate="G$1" pin="CLKIN" pad="21"/>
<connect gate="G$1" pin="CONVST" pad="20"/>
<connect gate="G$1" pin="CS" pad="23"/>
<connect gate="G$1" pin="D0" pad="19"/>
<connect gate="G$1" pin="D1" pad="18"/>
<connect gate="G$1" pin="D10" pad="8"/>
<connect gate="G$1" pin="D11" pad="7"/>
<connect gate="G$1" pin="D2" pad="17"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="11"/>
<connect gate="G$1" pin="D8" pad="10"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="INT/BU" pad="22"/>
<connect gate="G$1" pin="MODE" pad="1"/>
<connect gate="G$1" pin="RD" pad="24"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX132CNG" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX132"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="16"/>
<connect gate="G$1" pin="BUFOUT" pad="23"/>
<connect gate="G$1" pin="CREF+" pad="19"/>
<connect gate="G$1" pin="CREF-" pad="20"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="3"/>
<connect gate="G$1" pin="EOC" pad="11"/>
<connect gate="G$1" pin="INHI" pad="14"/>
<connect gate="G$1" pin="INLO" pad="15"/>
<connect gate="G$1" pin="INTIN" pad="21"/>
<connect gate="G$1" pin="INTOUT" pad="22"/>
<connect gate="G$1" pin="OSC1" pad="6"/>
<connect gate="G$1" pin="OSC2" pad="5"/>
<connect gate="G$1" pin="P0" pad="7"/>
<connect gate="G$1" pin="P1" pad="8"/>
<connect gate="G$1" pin="P2" pad="9"/>
<connect gate="G$1" pin="P3" pad="10"/>
<connect gate="G$1" pin="REF+" pad="18"/>
<connect gate="G$1" pin="REF-" pad="17"/>
<connect gate="G$1" pin="SCLK" pad="4"/>
<connect gate="G$1" pin="V+" pad="24"/>
<connect gate="G$1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX135CPI" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX135"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="AGND@" pad="20"/>
<connect gate="G$1" pin="BUFOUT" pad="27"/>
<connect gate="G$1" pin="CREF+" pad="23"/>
<connect gate="G$1" pin="CREF-" pad="24"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0" pad="6"/>
<connect gate="G$1" pin="D1" pad="7"/>
<connect gate="G$1" pin="D2" pad="8"/>
<connect gate="G$1" pin="D3" pad="9"/>
<connect gate="G$1" pin="D4" pad="10"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="12"/>
<connect gate="G$1" pin="D7" pad="13"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="EOC" pad="15"/>
<connect gate="G$1" pin="INHI" pad="17"/>
<connect gate="G$1" pin="INLO" pad="19"/>
<connect gate="G$1" pin="INTIN" pad="25"/>
<connect gate="G$1" pin="INTOUT" pad="26"/>
<connect gate="G$1" pin="OSC1" pad="5"/>
<connect gate="G$1" pin="OSC2" pad="4"/>
<connect gate="G$1" pin="RD" pad="2"/>
<connect gate="G$1" pin="REF+" pad="22"/>
<connect gate="G$1" pin="REF-" pad="21"/>
<connect gate="G$1" pin="V+" pad="28"/>
<connect gate="G$1" pin="V-" pad="16"/>
<connect gate="G$1" pin="WR" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX155ACP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX155"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="AGND" pad="23"/>
<connect gate="G$1" pin="AIN0" pad="4"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="2"/>
<connect gate="G$1" pin="AIN3" pad="1"/>
<connect gate="G$1" pin="AIN4" pad="28"/>
<connect gate="G$1" pin="AIN5" pad="27"/>
<connect gate="G$1" pin="AIN6" pad="26"/>
<connect gate="G$1" pin="AIN7" pad="25"/>
<connect gate="G$1" pin="BUSY" pad="10"/>
<connect gate="G$1" pin="CLK" pad="11"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="D0/A0" pad="20"/>
<connect gate="G$1" pin="D1/A1" pad="19"/>
<connect gate="G$1" pin="D2/A2" pad="18"/>
<connect gate="G$1" pin="D3/PD" pad="17"/>
<connect gate="G$1" pin="D4/INH" pad="16"/>
<connect gate="G$1" pin="D5/BIP" pad="15"/>
<connect gate="G$1" pin="D6/DIFF" pad="13"/>
<connect gate="G$1" pin="D7/ALL" pad="12"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="MODE" pad="5"/>
<connect gate="G$1" pin="RD" pad="8"/>
<connect gate="G$1" pin="REFIN" pad="22"/>
<connect gate="G$1" pin="REFOUT" pad="21"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="WR" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX156CNG" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX156"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="1"/>
<connect gate="G$1" pin="AIN2" pad="24"/>
<connect gate="G$1" pin="AIN3" pad="23"/>
<connect gate="G$1" pin="BUSY" pad="8"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="D0/A0" pad="18"/>
<connect gate="G$1" pin="D1/A1" pad="17"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3/PD" pad="15"/>
<connect gate="G$1" pin="D4/INH" pad="14"/>
<connect gate="G$1" pin="D5/BIP" pad="13"/>
<connect gate="G$1" pin="D6/DIFF" pad="11"/>
<connect gate="G$1" pin="D7/ALL" pad="10"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="MODE" pad="3"/>
<connect gate="G$1" pin="RD" pad="6"/>
<connect gate="G$1" pin="REFIN" pad="20"/>
<connect gate="G$1" pin="REFOUT" pad="19"/>
<connect gate="G$1" pin="VDD" pad="22"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX165CPN" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX165"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="AGND" pad="15"/>
<connect gate="G$1" pin="AIN" pad="16"/>
<connect gate="G$1" pin="BUSY" pad="4"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DB0/LSB" pad="14"/>
<connect gate="G$1" pin="DB1" pad="13"/>
<connect gate="G$1" pin="DB2" pad="12"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="DB4" pad="10"/>
<connect gate="G$1" pin="DB5" pad="8"/>
<connect gate="G$1" pin="DB6" pad="7"/>
<connect gate="G$1" pin="DB7/MSB" pad="6"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="RD" pad="2"/>
<connect gate="G$1" pin="REFIN" pad="17"/>
<connect gate="G$1" pin="REFOUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX166CPP" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX166"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="AGND" pad="16"/>
<connect gate="G$1" pin="AIN+" pad="18"/>
<connect gate="G$1" pin="AIN-" pad="17"/>
<connect gate="G$1" pin="BUSY" pad="5"/>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0/LSB" pad="15"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="12"/>
<connect gate="G$1" pin="D4" pad="11"/>
<connect gate="G$1" pin="D5" pad="9"/>
<connect gate="G$1" pin="D6" pad="8"/>
<connect gate="G$1" pin="D7/MSB" pad="7"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="MODE" pad="4"/>
<connect gate="G$1" pin="RD" pad="2"/>
<connect gate="G$1" pin="REFIN" pad="19"/>
<connect gate="G$1" pin="REFOUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX190CNG" prefix="IC">
<description>&lt;b&gt;ANALOG/DIGITAL CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX190"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="AGND@" pad="7"/>
<connect gate="G$1" pin="AIN+" pad="3"/>
<connect gate="G$1" pin="AIN-" pad="4"/>
<connect gate="G$1" pin="BIP" pad="8"/>
<connect gate="G$1" pin="BUSY" pad="9"/>
<connect gate="G$1" pin="CLK" pad="23"/>
<connect gate="G$1" pin="CS" pad="20"/>
<connect gate="G$1" pin="D0/D8" pad="10"/>
<connect gate="G$1" pin="D1/D9" pad="11"/>
<connect gate="G$1" pin="D2/D10" pad="13"/>
<connect gate="G$1" pin="D3/D11" pad="14"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5/SSTB" pad="16"/>
<connect gate="G$1" pin="D6/SCLK" pad="17"/>
<connect gate="G$1" pin="D7/SDATA" pad="18"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="HBEN" pad="21"/>
<connect gate="G$1" pin="PAR" pad="22"/>
<connect gate="G$1" pin="PD" pad="1"/>
<connect gate="G$1" pin="RD" pad="19"/>
<connect gate="G$1" pin="REFADJ" pad="6"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX440CPI" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX440"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="25"/>
<connect gate="G$1" pin="A2" pad="26"/>
<connect gate="G$1" pin="COMP" pad="20"/>
<connect gate="G$1" pin="EN" pad="27"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="IN-" pad="18"/>
<connect gate="G$1" pin="IN0" pad="1"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="9"/>
<connect gate="G$1" pin="IN5" pad="11"/>
<connect gate="G$1" pin="IN6" pad="13"/>
<connect gate="G$1" pin="IN7" pad="15"/>
<connect gate="G$1" pin="LATCH" pad="23"/>
<connect gate="G$1" pin="LEV/ED" pad="2"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V+@" pad="22"/>
<connect gate="G$1" pin="V+@1" pad="21"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="V-@" pad="17"/>
<connect gate="G$1" pin="V-@1" pad="16"/>
<connect gate="G$1" pin="VNS" pad="28"/>
<connect gate="G$1" pin="VOUT" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX441CPP" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX441"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="A0" pad="18"/>
<connect gate="G$1" pin="A1" pad="19"/>
<connect gate="G$1" pin="COMP" pad="15"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@" pad="9"/>
<connect gate="G$1" pin="IN-" pad="13"/>
<connect gate="G$1" pin="IN0" pad="1"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="LATCH" pad="17"/>
<connect gate="G$1" pin="LEV/ED" pad="2"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V+@" pad="16"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="V-@" pad="12"/>
<connect gate="G$1" pin="VNS" pad="20"/>
<connect gate="G$1" pin="VOUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX442CPA" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX442"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN-" pad="5"/>
<connect gate="G$1" pin="IN0" pad="1"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX456CPL" prefix="IC">
<description>8 x 8 crosspoint &lt;b&gt;VIDEO SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX456"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="AGND" pad="32"/>
<connect gate="G$1" pin="AGND@" pad="30"/>
<connect gate="G$1" pin="AGND@1" pad="28"/>
<connect gate="G$1" pin="CE" pad="23"/>
<connect gate="G$1" pin="CE@" pad="24"/>
<connect gate="G$1" pin="D0/SIN" pad="2"/>
<connect gate="G$1" pin="D1/SOUT" pad="1"/>
<connect gate="G$1" pin="D2" pad="38"/>
<connect gate="G$1" pin="D3" pad="36"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="DGND@" pad="12"/>
<connect gate="G$1" pin="EDGE/LEV" pad="14"/>
<connect gate="G$1" pin="IN0" pad="5"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="11"/>
<connect gate="G$1" pin="IN4" pad="13"/>
<connect gate="G$1" pin="IN5" pad="15"/>
<connect gate="G$1" pin="IN6" pad="17"/>
<connect gate="G$1" pin="IN7" pad="19"/>
<connect gate="G$1" pin="LATCH" pad="22"/>
<connect gate="G$1" pin="LOAD" pad="8"/>
<connect gate="G$1" pin="OUT0" pad="39"/>
<connect gate="G$1" pin="OUT1" pad="37"/>
<connect gate="G$1" pin="OUT2" pad="35"/>
<connect gate="G$1" pin="OUT3" pad="33"/>
<connect gate="G$1" pin="OUT4" pad="31"/>
<connect gate="G$1" pin="OUT5" pad="29"/>
<connect gate="G$1" pin="OUT6" pad="27"/>
<connect gate="G$1" pin="OUT7" pad="25"/>
<connect gate="G$1" pin="SER/PAR" pad="18"/>
<connect gate="G$1" pin="V+" pad="40"/>
<connect gate="G$1" pin="V+@" pad="26"/>
<connect gate="G$1" pin="V+@1" pad="16"/>
<connect gate="G$1" pin="V-" pad="34"/>
<connect gate="G$1" pin="V-@" pad="20"/>
<connect gate="G$1" pin="WR" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX502CNG" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX502"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="CS" pad="16"/>
<connect gate="G$1" pin="D0" pad="14"/>
<connect gate="G$1" pin="D1" pad="13"/>
<connect gate="G$1" pin="D10" pad="3"/>
<connect gate="G$1" pin="D11" pad="2"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="9"/>
<connect gate="G$1" pin="D5" pad="8"/>
<connect gate="G$1" pin="D6" pad="7"/>
<connect gate="G$1" pin="D7" pad="6"/>
<connect gate="G$1" pin="D8" pad="5"/>
<connect gate="G$1" pin="D9" pad="4"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="RA" pad="21"/>
<connect gate="G$1" pin="RB" pad="22"/>
<connect gate="G$1" pin="RC" pad="23"/>
<connect gate="G$1" pin="RFB" pad="24"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="G$1" pin="VREF" pad="17"/>
<connect gate="G$1" pin="VSS" pad="19"/>
<connect gate="G$1" pin="WR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX501CNG" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX501"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="CLR" pad="4"/>
<connect gate="G$1" pin="CSLSB" pad="14"/>
<connect gate="G$1" pin="CSMSB" pad="16"/>
<connect gate="G$1" pin="D0/D8" pad="13"/>
<connect gate="G$1" pin="D1/D9" pad="11"/>
<connect gate="G$1" pin="D2/D10" pad="10"/>
<connect gate="G$1" pin="D3/D11" pad="9"/>
<connect gate="G$1" pin="D4" pad="8"/>
<connect gate="G$1" pin="D5" pad="7"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D7" pad="5"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="LDAC" pad="2"/>
<connect gate="G$1" pin="RA" pad="21"/>
<connect gate="G$1" pin="RB" pad="22"/>
<connect gate="G$1" pin="RC" pad="23"/>
<connect gate="G$1" pin="RFB" pad="24"/>
<connect gate="G$1" pin="SET" pad="3"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="G$1" pin="VREF" pad="17"/>
<connect gate="G$1" pin="VSS" pad="19"/>
<connect gate="G$1" pin="WR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX506CPP" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX506"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="D0" pad="14"/>
<connect gate="G$1" pin="D1" pad="13"/>
<connect gate="G$1" pin="D2" pad="12"/>
<connect gate="G$1" pin="D3" pad="11"/>
<connect gate="G$1" pin="D4" pad="10"/>
<connect gate="G$1" pin="D5" pad="9"/>
<connect gate="G$1" pin="D6" pad="8"/>
<connect gate="G$1" pin="D7" pad="7"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VOUT-A" pad="2"/>
<connect gate="G$1" pin="VOUT-B" pad="1"/>
<connect gate="G$1" pin="VOUT-C" pad="20"/>
<connect gate="G$1" pin="VOUT-D" pad="19"/>
<connect gate="G$1" pin="VREF" pad="4"/>
<connect gate="G$1" pin="VSS" pad="3"/>
<connect gate="G$1" pin="WR" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX507CNG" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX507"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="CLR" pad="21"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D10" pad="6"/>
<connect gate="G$1" pin="D11" pad="5"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="14"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="7"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="LDAC" pad="20"/>
<connect gate="G$1" pin="REF-O" pad="3"/>
<connect gate="G$1" pin="RFB" pad="23"/>
<connect gate="G$1" pin="ROFS" pad="2"/>
<connect gate="G$1" pin="VDD" pad="22"/>
<connect gate="G$1" pin="VOUT" pad="24"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="WR" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX508CPP" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX508"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="CSLSB" pad="15"/>
<connect gate="G$1" pin="CSMSB" pad="14"/>
<connect gate="G$1" pin="D0/D8" pad="13"/>
<connect gate="G$1" pin="D1/D9" pad="12"/>
<connect gate="G$1" pin="D2/D10" pad="11"/>
<connect gate="G$1" pin="D3/D11" pad="9"/>
<connect gate="G$1" pin="D4" pad="8"/>
<connect gate="G$1" pin="D5" pad="7"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D7" pad="5"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="LDAC" pad="17"/>
<connect gate="G$1" pin="REF-O" pad="3"/>
<connect gate="G$1" pin="RFB" pad="19"/>
<connect gate="G$1" pin="ROFS" pad="2"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VOUT" pad="20"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="WR" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX514CNG" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX514"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="CLK" pad="21"/>
<connect gate="G$1" pin="CLK@" pad="16"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="IOUTA" pad="3"/>
<connect gate="G$1" pin="IOUTB" pad="6"/>
<connect gate="G$1" pin="IOUTC" pad="9"/>
<connect gate="G$1" pin="IOUTD" pad="11"/>
<connect gate="G$1" pin="LOADA" pad="22"/>
<connect gate="G$1" pin="LOADB" pad="19"/>
<connect gate="G$1" pin="LOADC" pad="17"/>
<connect gate="G$1" pin="LOADD" pad="13"/>
<connect gate="G$1" pin="RFBA" pad="2"/>
<connect gate="G$1" pin="RFBB" pad="5"/>
<connect gate="G$1" pin="RFBC" pad="8"/>
<connect gate="G$1" pin="RFBD" pad="10"/>
<connect gate="G$1" pin="SRIA" pad="23"/>
<connect gate="G$1" pin="SRIB" pad="20"/>
<connect gate="G$1" pin="SRIC" pad="18"/>
<connect gate="G$1" pin="SRID" pad="14"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VREFA" pad="1"/>
<connect gate="G$1" pin="VREFB" pad="4"/>
<connect gate="G$1" pin="VREFC" pad="7"/>
<connect gate="G$1" pin="VREFD" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX526CNG" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX526"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="A0" pad="18"/>
<connect gate="G$1" pin="A1" pad="17"/>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="CSLSB" pad="21"/>
<connect gate="G$1" pin="CSMSB" pad="22"/>
<connect gate="G$1" pin="D0/D8" pad="16"/>
<connect gate="G$1" pin="D1/D9" pad="15"/>
<connect gate="G$1" pin="D2/D10" pad="14"/>
<connect gate="G$1" pin="D3/D11" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="LDAC" pad="8"/>
<connect gate="G$1" pin="VDD" pad="23"/>
<connect gate="G$1" pin="VOUTA" pad="3"/>
<connect gate="G$1" pin="VOUTB" pad="2"/>
<connect gate="G$1" pin="VOUTC" pad="1"/>
<connect gate="G$1" pin="VOUTD" pad="24"/>
<connect gate="G$1" pin="VREFAB" pad="6"/>
<connect gate="G$1" pin="VREFCD" pad="19"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WR" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX528CPP" prefix="IC">
<description>&lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX528"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="8"/>
<connect gate="G$1" pin="DOUT" pad="10"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OUT0" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="OUT3" pad="6"/>
<connect gate="G$1" pin="OUT4" pad="15"/>
<connect gate="G$1" pin="OUT5" pad="16"/>
<connect gate="G$1" pin="OUT6" pad="17"/>
<connect gate="G$1" pin="OUT7" pad="18"/>
<connect gate="G$1" pin="REFH1" pad="2"/>
<connect gate="G$1" pin="REFH2" pad="19"/>
<connect gate="G$1" pin="REFL1" pad="1"/>
<connect gate="G$1" pin="REFL2" pad="20"/>
<connect gate="G$1" pin="SHDN" pad="13"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX872CPA" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX872"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@" pad="7"/>
<connect gate="G$1" pin="TEMP" pad="3"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX200CPP" prefix="IC">
<description>&lt;b&gt;RS232 TRANSMITTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX200"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="C1+" pad="8"/>
<connect gate="G$1" pin="C1-" pad="10"/>
<connect gate="G$1" pin="C2+" pad="11"/>
<connect gate="G$1" pin="C2-" pad="12"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SHDN" pad="17"/>
<connect gate="G$1" pin="T1IN" pad="5"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="4"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="14"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="T4OUT" pad="20"/>
<connect gate="G$1" pin="T5IN" pad="19"/>
<connect gate="G$1" pin="T5OUT" pad="16"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="13"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX201CPD" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX201"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="2"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="R1IN" pad="10"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="6"/>
<connect gate="G$1" pin="T1IN" pad="8"/>
<connect gate="G$1" pin="T1OUT" pad="11"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T2OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
<connect gate="G$1" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX201CWE" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX201"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="C+" pad="1"/>
<connect gate="G$1" pin="C-" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="12"/>
<connect gate="G$1" pin="R1OUT" pad="11"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="6"/>
<connect gate="G$1" pin="T1IN" pad="10"/>
<connect gate="G$1" pin="T1OUT" pad="13"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T2OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="16"/>
<connect gate="G$1" pin="V-" pad="3"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX202CPE" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX202"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX306CPI" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX306"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="COM" pad="28"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="NO1" pad="19"/>
<connect gate="G$1" pin="NO10" pad="10"/>
<connect gate="G$1" pin="NO11" pad="9"/>
<connect gate="G$1" pin="NO12" pad="8"/>
<connect gate="G$1" pin="NO13" pad="7"/>
<connect gate="G$1" pin="NO14" pad="6"/>
<connect gate="G$1" pin="NO15" pad="5"/>
<connect gate="G$1" pin="NO16" pad="4"/>
<connect gate="G$1" pin="NO2" pad="20"/>
<connect gate="G$1" pin="NO3" pad="21"/>
<connect gate="G$1" pin="NO4" pad="22"/>
<connect gate="G$1" pin="NO5" pad="23"/>
<connect gate="G$1" pin="NO6" pad="24"/>
<connect gate="G$1" pin="NO7" pad="25"/>
<connect gate="G$1" pin="NO8" pad="26"/>
<connect gate="G$1" pin="NO9" pad="11"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX307CPI" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX307"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="COMA" pad="28"/>
<connect gate="G$1" pin="COMB" pad="2"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="NO1A" pad="19"/>
<connect gate="G$1" pin="NO1B" pad="11"/>
<connect gate="G$1" pin="NO2A" pad="20"/>
<connect gate="G$1" pin="NO2B" pad="10"/>
<connect gate="G$1" pin="NO3A" pad="21"/>
<connect gate="G$1" pin="NO3B" pad="9"/>
<connect gate="G$1" pin="NO4A" pad="22"/>
<connect gate="G$1" pin="NO4B" pad="8"/>
<connect gate="G$1" pin="NO5A" pad="23"/>
<connect gate="G$1" pin="NO5B" pad="7"/>
<connect gate="G$1" pin="NO6A" pad="24"/>
<connect gate="G$1" pin="NO6B" pad="6"/>
<connect gate="G$1" pin="NO7A" pad="25"/>
<connect gate="G$1" pin="NO7B" pad="5"/>
<connect gate="G$1" pin="NO8A" pad="26"/>
<connect gate="G$1" pin="NO8B" pad="4"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX307EQI" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX307"/>
</gates>
<devices>
<device name="" package="PLCC28">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="COMA" pad="28"/>
<connect gate="G$1" pin="COMB" pad="2"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="NO1A" pad="19"/>
<connect gate="G$1" pin="NO1B" pad="11"/>
<connect gate="G$1" pin="NO2A" pad="20"/>
<connect gate="G$1" pin="NO2B" pad="10"/>
<connect gate="G$1" pin="NO3A" pad="21"/>
<connect gate="G$1" pin="NO3B" pad="9"/>
<connect gate="G$1" pin="NO4A" pad="22"/>
<connect gate="G$1" pin="NO4B" pad="8"/>
<connect gate="G$1" pin="NO5A" pad="23"/>
<connect gate="G$1" pin="NO5B" pad="7"/>
<connect gate="G$1" pin="NO6A" pad="24"/>
<connect gate="G$1" pin="NO6B" pad="6"/>
<connect gate="G$1" pin="NO7A" pad="25"/>
<connect gate="G$1" pin="NO7B" pad="5"/>
<connect gate="G$1" pin="NO8A" pad="26"/>
<connect gate="G$1" pin="NO8B" pad="4"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX308CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX308"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="COM" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="NO1" pad="4"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="NO3" pad="6"/>
<connect gate="G$1" pin="NO4" pad="7"/>
<connect gate="G$1" pin="NO5" pad="12"/>
<connect gate="G$1" pin="NO6" pad="11"/>
<connect gate="G$1" pin="NO7" pad="10"/>
<connect gate="G$1" pin="NO8" pad="9"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX309CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX309"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="COMA" pad="8"/>
<connect gate="G$1" pin="COMB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="NO1A" pad="4"/>
<connect gate="G$1" pin="NO1B" pad="13"/>
<connect gate="G$1" pin="NO2A" pad="5"/>
<connect gate="G$1" pin="NO2B" pad="12"/>
<connect gate="G$1" pin="NO3A" pad="6"/>
<connect gate="G$1" pin="NO3B" pad="11"/>
<connect gate="G$1" pin="NO4A" pad="7"/>
<connect gate="G$1" pin="NO4B" pad="10"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX317CPA" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX317"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX318CPA" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX318"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NO" pad="8"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX318CSA" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX318"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NO" pad="8"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX317CSA" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX317"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX306CWI" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX306"/>
</gates>
<devices>
<device name="" package="SO28L">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="COM" pad="28"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="NO1" pad="19"/>
<connect gate="G$1" pin="NO10" pad="10"/>
<connect gate="G$1" pin="NO11" pad="9"/>
<connect gate="G$1" pin="NO12" pad="8"/>
<connect gate="G$1" pin="NO13" pad="7"/>
<connect gate="G$1" pin="NO14" pad="6"/>
<connect gate="G$1" pin="NO15" pad="5"/>
<connect gate="G$1" pin="NO16" pad="4"/>
<connect gate="G$1" pin="NO2" pad="20"/>
<connect gate="G$1" pin="NO3" pad="21"/>
<connect gate="G$1" pin="NO4" pad="22"/>
<connect gate="G$1" pin="NO5" pad="23"/>
<connect gate="G$1" pin="NO6" pad="24"/>
<connect gate="G$1" pin="NO7" pad="25"/>
<connect gate="G$1" pin="NO8" pad="26"/>
<connect gate="G$1" pin="NO9" pad="11"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX306EQI" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX306"/>
</gates>
<devices>
<device name="" package="PLCC28">
<connects>
<connect gate="G$2" pin="A0" pad="17"/>
<connect gate="G$2" pin="A1" pad="16"/>
<connect gate="G$2" pin="A2" pad="15"/>
<connect gate="G$2" pin="A3" pad="14"/>
<connect gate="G$2" pin="COM" pad="28"/>
<connect gate="G$2" pin="EN" pad="18"/>
<connect gate="G$2" pin="GND" pad="12"/>
<connect gate="G$2" pin="NC" pad="2"/>
<connect gate="G$2" pin="NC@1" pad="3"/>
<connect gate="G$2" pin="NC@2" pad="13"/>
<connect gate="G$2" pin="NO1" pad="19"/>
<connect gate="G$2" pin="NO10" pad="10"/>
<connect gate="G$2" pin="NO11" pad="9"/>
<connect gate="G$2" pin="NO12" pad="8"/>
<connect gate="G$2" pin="NO13" pad="7"/>
<connect gate="G$2" pin="NO14" pad="6"/>
<connect gate="G$2" pin="NO15" pad="5"/>
<connect gate="G$2" pin="NO16" pad="4"/>
<connect gate="G$2" pin="NO2" pad="20"/>
<connect gate="G$2" pin="NO3" pad="21"/>
<connect gate="G$2" pin="NO4" pad="22"/>
<connect gate="G$2" pin="NO5" pad="23"/>
<connect gate="G$2" pin="NO6" pad="24"/>
<connect gate="G$2" pin="NO7" pad="25"/>
<connect gate="G$2" pin="NO8" pad="26"/>
<connect gate="G$2" pin="NO9" pad="11"/>
<connect gate="G$2" pin="V+" pad="1"/>
<connect gate="G$2" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX307CWI" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="MAX307"/>
</gates>
<devices>
<device name="" package="SO28L">
<connects>
<connect gate="G$3" pin="A0" pad="17"/>
<connect gate="G$3" pin="A1" pad="16"/>
<connect gate="G$3" pin="A2" pad="15"/>
<connect gate="G$3" pin="COMA" pad="28"/>
<connect gate="G$3" pin="COMB" pad="2"/>
<connect gate="G$3" pin="EN" pad="18"/>
<connect gate="G$3" pin="GND" pad="12"/>
<connect gate="G$3" pin="NC" pad="3"/>
<connect gate="G$3" pin="NC@1" pad="13"/>
<connect gate="G$3" pin="NC@2" pad="14"/>
<connect gate="G$3" pin="NO1A" pad="19"/>
<connect gate="G$3" pin="NO1B" pad="11"/>
<connect gate="G$3" pin="NO2A" pad="20"/>
<connect gate="G$3" pin="NO2B" pad="10"/>
<connect gate="G$3" pin="NO3A" pad="21"/>
<connect gate="G$3" pin="NO3B" pad="9"/>
<connect gate="G$3" pin="NO4A" pad="22"/>
<connect gate="G$3" pin="NO4B" pad="8"/>
<connect gate="G$3" pin="NO5A" pad="23"/>
<connect gate="G$3" pin="NO5B" pad="7"/>
<connect gate="G$3" pin="NO6A" pad="24"/>
<connect gate="G$3" pin="NO6B" pad="6"/>
<connect gate="G$3" pin="NO7A" pad="25"/>
<connect gate="G$3" pin="NO7B" pad="5"/>
<connect gate="G$3" pin="NO8A" pad="26"/>
<connect gate="G$3" pin="NO8B" pad="4"/>
<connect gate="G$3" pin="V+" pad="1"/>
<connect gate="G$3" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX308CSE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="MAX308"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$4" pin="A0" pad="1"/>
<connect gate="G$4" pin="A1" pad="16"/>
<connect gate="G$4" pin="A2" pad="15"/>
<connect gate="G$4" pin="COM" pad="8"/>
<connect gate="G$4" pin="EN" pad="2"/>
<connect gate="G$4" pin="GND" pad="14"/>
<connect gate="G$4" pin="NO1" pad="4"/>
<connect gate="G$4" pin="NO2" pad="5"/>
<connect gate="G$4" pin="NO3" pad="6"/>
<connect gate="G$4" pin="NO4" pad="7"/>
<connect gate="G$4" pin="NO5" pad="12"/>
<connect gate="G$4" pin="NO6" pad="11"/>
<connect gate="G$4" pin="NO7" pad="10"/>
<connect gate="G$4" pin="NO8" pad="9"/>
<connect gate="G$4" pin="V+" pad="13"/>
<connect gate="G$4" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX309CSE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX309"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="COMA" pad="8"/>
<connect gate="G$1" pin="COMB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="NO1A" pad="4"/>
<connect gate="G$1" pin="NO1B" pad="13"/>
<connect gate="G$1" pin="NO2A" pad="5"/>
<connect gate="G$1" pin="NO2B" pad="12"/>
<connect gate="G$1" pin="NO3A" pad="6"/>
<connect gate="G$1" pin="NO3B" pad="11"/>
<connect gate="G$1" pin="NO4A" pad="7"/>
<connect gate="G$1" pin="NO4B" pad="10"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX333ACWP" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX333"/>
</gates>
<devices>
<device name="" package="SO20L">
<connects>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="8"/>
<connect gate="G$1" pin="COM3" pad="13"/>
<connect gate="G$1" pin="COM4" pad="18"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="IN3" pad="11"/>
<connect gate="G$1" pin="IN4" pad="20"/>
<connect gate="G$1" pin="NC" pad="15"/>
<connect gate="G$1" pin="NC1" pad="4"/>
<connect gate="G$1" pin="NC2" pad="7"/>
<connect gate="G$1" pin="NC3" pad="14"/>
<connect gate="G$1" pin="NC4" pad="17"/>
<connect gate="G$1" pin="NO1" pad="2"/>
<connect gate="G$1" pin="NO2" pad="9"/>
<connect gate="G$1" pin="NO3" pad="12"/>
<connect gate="G$1" pin="NO4" pad="19"/>
<connect gate="G$1" pin="V+" pad="16"/>
<connect gate="G$1" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX335CNG" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX335"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="COM0" pad="6"/>
<connect gate="G$1" pin="COM1" pad="8"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="COM3" pad="12"/>
<connect gate="G$1" pin="COM4" pad="13"/>
<connect gate="G$1" pin="COM5" pad="15"/>
<connect gate="G$1" pin="COM6" pad="17"/>
<connect gate="G$1" pin="COM7" pad="19"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="22"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NO0" pad="5"/>
<connect gate="G$1" pin="NO1" pad="7"/>
<connect gate="G$1" pin="NO2" pad="9"/>
<connect gate="G$1" pin="NO3" pad="11"/>
<connect gate="G$1" pin="NO4" pad="14"/>
<connect gate="G$1" pin="NO5" pad="16"/>
<connect gate="G$1" pin="NO6" pad="18"/>
<connect gate="G$1" pin="NO7" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="21"/>
<connect gate="G$1" pin="VL" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX335CWG" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX335"/>
</gates>
<devices>
<device name="" package="SO24L">
<connects>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="COM0" pad="6"/>
<connect gate="G$1" pin="COM1" pad="8"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="COM3" pad="12"/>
<connect gate="G$1" pin="COM4" pad="13"/>
<connect gate="G$1" pin="COM5" pad="15"/>
<connect gate="G$1" pin="COM6" pad="17"/>
<connect gate="G$1" pin="COM7" pad="19"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="22"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NO0" pad="5"/>
<connect gate="G$1" pin="NO1" pad="7"/>
<connect gate="G$1" pin="NO2" pad="9"/>
<connect gate="G$1" pin="NO3" pad="11"/>
<connect gate="G$1" pin="NO4" pad="14"/>
<connect gate="G$1" pin="NO5" pad="16"/>
<connect gate="G$1" pin="NO6" pad="18"/>
<connect gate="G$1" pin="NO7" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="21"/>
<connect gate="G$1" pin="VL" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX338CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX338"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="COM" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="NO1" pad="4"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="NO3" pad="6"/>
<connect gate="G$1" pin="NO4" pad="7"/>
<connect gate="G$1" pin="NO5" pad="12"/>
<connect gate="G$1" pin="NO6" pad="11"/>
<connect gate="G$1" pin="NO7" pad="10"/>
<connect gate="G$1" pin="NO8" pad="9"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX338CSE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX338"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="A0" pad="1"/>
<connect gate="G$2" pin="A1" pad="16"/>
<connect gate="G$2" pin="A2" pad="15"/>
<connect gate="G$2" pin="COM" pad="8"/>
<connect gate="G$2" pin="EN" pad="2"/>
<connect gate="G$2" pin="GND" pad="14"/>
<connect gate="G$2" pin="NO1" pad="4"/>
<connect gate="G$2" pin="NO2" pad="5"/>
<connect gate="G$2" pin="NO3" pad="6"/>
<connect gate="G$2" pin="NO4" pad="7"/>
<connect gate="G$2" pin="NO5" pad="12"/>
<connect gate="G$2" pin="NO6" pad="11"/>
<connect gate="G$2" pin="NO7" pad="10"/>
<connect gate="G$2" pin="NO8" pad="9"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX339CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="MAX339"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$3" pin="A0" pad="1"/>
<connect gate="G$3" pin="A1" pad="16"/>
<connect gate="G$3" pin="COMA" pad="8"/>
<connect gate="G$3" pin="COMB" pad="9"/>
<connect gate="G$3" pin="EN" pad="2"/>
<connect gate="G$3" pin="GND" pad="15"/>
<connect gate="G$3" pin="NO1A" pad="4"/>
<connect gate="G$3" pin="NO1B" pad="13"/>
<connect gate="G$3" pin="NO2A" pad="5"/>
<connect gate="G$3" pin="NO2B" pad="12"/>
<connect gate="G$3" pin="NO3A" pad="6"/>
<connect gate="G$3" pin="NO3B" pad="11"/>
<connect gate="G$3" pin="NO4A" pad="7"/>
<connect gate="G$3" pin="NO4B" pad="10"/>
<connect gate="G$3" pin="V+" pad="14"/>
<connect gate="G$3" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX339CSE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="MAX339"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$4" pin="A0" pad="1"/>
<connect gate="G$4" pin="A1" pad="16"/>
<connect gate="G$4" pin="COMA" pad="8"/>
<connect gate="G$4" pin="COMB" pad="9"/>
<connect gate="G$4" pin="EN" pad="2"/>
<connect gate="G$4" pin="GND" pad="15"/>
<connect gate="G$4" pin="NO1A" pad="4"/>
<connect gate="G$4" pin="NO1B" pad="13"/>
<connect gate="G$4" pin="NO2A" pad="5"/>
<connect gate="G$4" pin="NO2B" pad="12"/>
<connect gate="G$4" pin="NO3A" pad="6"/>
<connect gate="G$4" pin="NO3B" pad="11"/>
<connect gate="G$4" pin="NO4A" pad="7"/>
<connect gate="G$4" pin="NO4B" pad="10"/>
<connect gate="G$4" pin="V+" pad="14"/>
<connect gate="G$4" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX351CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX351"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX351CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX351"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="COM1" pad="2"/>
<connect gate="G$2" pin="COM2" pad="15"/>
<connect gate="G$2" pin="COM3" pad="10"/>
<connect gate="G$2" pin="COM4" pad="7"/>
<connect gate="G$2" pin="GND" pad="5"/>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="16"/>
<connect gate="G$2" pin="IN3" pad="9"/>
<connect gate="G$2" pin="IN4" pad="8"/>
<connect gate="G$2" pin="NC1" pad="3"/>
<connect gate="G$2" pin="NC2" pad="14"/>
<connect gate="G$2" pin="NC3" pad="11"/>
<connect gate="G$2" pin="NC4" pad="6"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="4"/>
<connect gate="G$2" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX352CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="MAX352"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$3" pin="COM1" pad="2"/>
<connect gate="G$3" pin="COM2" pad="15"/>
<connect gate="G$3" pin="COM3" pad="10"/>
<connect gate="G$3" pin="COM4" pad="7"/>
<connect gate="G$3" pin="GND" pad="5"/>
<connect gate="G$3" pin="IN1" pad="1"/>
<connect gate="G$3" pin="IN2" pad="16"/>
<connect gate="G$3" pin="IN3" pad="9"/>
<connect gate="G$3" pin="IN4" pad="8"/>
<connect gate="G$3" pin="NO1" pad="3"/>
<connect gate="G$3" pin="NO2" pad="14"/>
<connect gate="G$3" pin="NO3" pad="11"/>
<connect gate="G$3" pin="NO4" pad="6"/>
<connect gate="G$3" pin="V+" pad="13"/>
<connect gate="G$3" pin="V-" pad="4"/>
<connect gate="G$3" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX352CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="MAX352"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$4" pin="COM1" pad="2"/>
<connect gate="G$4" pin="COM2" pad="15"/>
<connect gate="G$4" pin="COM3" pad="10"/>
<connect gate="G$4" pin="COM4" pad="7"/>
<connect gate="G$4" pin="GND" pad="5"/>
<connect gate="G$4" pin="IN1" pad="1"/>
<connect gate="G$4" pin="IN2" pad="16"/>
<connect gate="G$4" pin="IN3" pad="9"/>
<connect gate="G$4" pin="IN4" pad="8"/>
<connect gate="G$4" pin="NO1" pad="3"/>
<connect gate="G$4" pin="NO2" pad="14"/>
<connect gate="G$4" pin="NO3" pad="11"/>
<connect gate="G$4" pin="NO4" pad="6"/>
<connect gate="G$4" pin="V+" pad="13"/>
<connect gate="G$4" pin="V-" pad="4"/>
<connect gate="G$4" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX353CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$5" symbol="MAX353"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$5" pin="COM1" pad="2"/>
<connect gate="G$5" pin="COM2" pad="15"/>
<connect gate="G$5" pin="COM3" pad="10"/>
<connect gate="G$5" pin="COM4" pad="7"/>
<connect gate="G$5" pin="GND" pad="5"/>
<connect gate="G$5" pin="IN1" pad="1"/>
<connect gate="G$5" pin="IN2" pad="16"/>
<connect gate="G$5" pin="IN3" pad="9"/>
<connect gate="G$5" pin="IN4" pad="8"/>
<connect gate="G$5" pin="NC2" pad="14"/>
<connect gate="G$5" pin="NC3" pad="11"/>
<connect gate="G$5" pin="NO1" pad="3"/>
<connect gate="G$5" pin="NO4" pad="6"/>
<connect gate="G$5" pin="V+" pad="13"/>
<connect gate="G$5" pin="V-" pad="4"/>
<connect gate="G$5" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX353CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$6" symbol="MAX353"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$6" pin="COM1" pad="2"/>
<connect gate="G$6" pin="COM2" pad="15"/>
<connect gate="G$6" pin="COM3" pad="10"/>
<connect gate="G$6" pin="COM4" pad="7"/>
<connect gate="G$6" pin="GND" pad="5"/>
<connect gate="G$6" pin="IN1" pad="1"/>
<connect gate="G$6" pin="IN2" pad="16"/>
<connect gate="G$6" pin="IN3" pad="9"/>
<connect gate="G$6" pin="IN4" pad="8"/>
<connect gate="G$6" pin="NC2" pad="14"/>
<connect gate="G$6" pin="NC3" pad="11"/>
<connect gate="G$6" pin="NO1" pad="3"/>
<connect gate="G$6" pin="NO4" pad="6"/>
<connect gate="G$6" pin="V+" pad="13"/>
<connect gate="G$6" pin="V-" pad="4"/>
<connect gate="G$6" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX361CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX361"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX361CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX361"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="COM1" pad="2"/>
<connect gate="G$2" pin="COM2" pad="15"/>
<connect gate="G$2" pin="COM3" pad="10"/>
<connect gate="G$2" pin="COM4" pad="7"/>
<connect gate="G$2" pin="GND" pad="5"/>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="16"/>
<connect gate="G$2" pin="IN3" pad="9"/>
<connect gate="G$2" pin="IN4" pad="8"/>
<connect gate="G$2" pin="NC" pad="12"/>
<connect gate="G$2" pin="NC1" pad="3"/>
<connect gate="G$2" pin="NC2" pad="14"/>
<connect gate="G$2" pin="NC3" pad="11"/>
<connect gate="G$2" pin="NC4" pad="6"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX362CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX362"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NO1" pad="3"/>
<connect gate="G$1" pin="NO2" pad="14"/>
<connect gate="G$1" pin="NO3" pad="11"/>
<connect gate="G$1" pin="NO4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX362CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX362"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="COM1" pad="2"/>
<connect gate="G$2" pin="COM2" pad="15"/>
<connect gate="G$2" pin="COM3" pad="10"/>
<connect gate="G$2" pin="COM4" pad="7"/>
<connect gate="G$2" pin="GND" pad="5"/>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="16"/>
<connect gate="G$2" pin="IN3" pad="9"/>
<connect gate="G$2" pin="IN4" pad="8"/>
<connect gate="G$2" pin="NC" pad="12"/>
<connect gate="G$2" pin="NO1" pad="3"/>
<connect gate="G$2" pin="NO2" pad="14"/>
<connect gate="G$2" pin="NO3" pad="11"/>
<connect gate="G$2" pin="NO4" pad="6"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX364CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX351"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX364CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX351"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="COM1" pad="2"/>
<connect gate="G$2" pin="COM2" pad="15"/>
<connect gate="G$2" pin="COM3" pad="10"/>
<connect gate="G$2" pin="COM4" pad="7"/>
<connect gate="G$2" pin="GND" pad="5"/>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="16"/>
<connect gate="G$2" pin="IN3" pad="9"/>
<connect gate="G$2" pin="IN4" pad="8"/>
<connect gate="G$2" pin="NC1" pad="3"/>
<connect gate="G$2" pin="NC2" pad="14"/>
<connect gate="G$2" pin="NC3" pad="11"/>
<connect gate="G$2" pin="NC4" pad="6"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="4"/>
<connect gate="G$2" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX365CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="MAX352"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$3" pin="COM1" pad="2"/>
<connect gate="G$3" pin="COM2" pad="15"/>
<connect gate="G$3" pin="COM3" pad="10"/>
<connect gate="G$3" pin="COM4" pad="7"/>
<connect gate="G$3" pin="GND" pad="5"/>
<connect gate="G$3" pin="IN1" pad="1"/>
<connect gate="G$3" pin="IN2" pad="16"/>
<connect gate="G$3" pin="IN3" pad="9"/>
<connect gate="G$3" pin="IN4" pad="8"/>
<connect gate="G$3" pin="NO1" pad="3"/>
<connect gate="G$3" pin="NO2" pad="14"/>
<connect gate="G$3" pin="NO3" pad="11"/>
<connect gate="G$3" pin="NO4" pad="6"/>
<connect gate="G$3" pin="V+" pad="13"/>
<connect gate="G$3" pin="V-" pad="4"/>
<connect gate="G$3" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX365CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="MAX352"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$4" pin="COM1" pad="2"/>
<connect gate="G$4" pin="COM2" pad="15"/>
<connect gate="G$4" pin="COM3" pad="10"/>
<connect gate="G$4" pin="COM4" pad="7"/>
<connect gate="G$4" pin="GND" pad="5"/>
<connect gate="G$4" pin="IN1" pad="1"/>
<connect gate="G$4" pin="IN2" pad="16"/>
<connect gate="G$4" pin="IN3" pad="9"/>
<connect gate="G$4" pin="IN4" pad="8"/>
<connect gate="G$4" pin="NO1" pad="3"/>
<connect gate="G$4" pin="NO2" pad="14"/>
<connect gate="G$4" pin="NO3" pad="11"/>
<connect gate="G$4" pin="NO4" pad="6"/>
<connect gate="G$4" pin="V+" pad="13"/>
<connect gate="G$4" pin="V-" pad="4"/>
<connect gate="G$4" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX366CPA" prefix="IC">
<description>Signal-line &lt;b&gt;CIRCUIT PROTECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX366"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="IN3" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="OUT3" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX366CSA" prefix="IC">
<description>Signal-line &lt;b&gt;CIRCUIT PROTECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX366"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="2"/>
<connect gate="G$2" pin="IN3" pad="3"/>
<connect gate="G$2" pin="OUT1" pad="7"/>
<connect gate="G$2" pin="OUT2" pad="6"/>
<connect gate="G$2" pin="OUT3" pad="5"/>
<connect gate="G$2" pin="V+" pad="8"/>
<connect gate="G$2" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX367CPN" prefix="IC">
<description>Signal-line &lt;b&gt;CIRCUIT PROTECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX367"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="IN3" pad="3"/>
<connect gate="G$1" pin="IN4" pad="4"/>
<connect gate="G$1" pin="IN5" pad="5"/>
<connect gate="G$1" pin="IN6" pad="6"/>
<connect gate="G$1" pin="IN7" pad="7"/>
<connect gate="G$1" pin="IN8" pad="8"/>
<connect gate="G$1" pin="OUT1" pad="17"/>
<connect gate="G$1" pin="OUT2" pad="16"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="OUT5" pad="13"/>
<connect gate="G$1" pin="OUT6" pad="12"/>
<connect gate="G$1" pin="OUT7" pad="11"/>
<connect gate="G$1" pin="OUT8" pad="10"/>
<connect gate="G$1" pin="V+" pad="18"/>
<connect gate="G$1" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX367CWN" prefix="IC">
<description>Signal-line &lt;b&gt;CIRCUIT PROTECTOR&lt;/b&gt;r</description>
<gates>
<gate name="G$2" symbol="MAX367"/>
</gates>
<devices>
<device name="" package="SO18L">
<connects>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="2"/>
<connect gate="G$2" pin="IN3" pad="3"/>
<connect gate="G$2" pin="IN4" pad="4"/>
<connect gate="G$2" pin="IN5" pad="5"/>
<connect gate="G$2" pin="IN6" pad="6"/>
<connect gate="G$2" pin="IN7" pad="7"/>
<connect gate="G$2" pin="IN8" pad="8"/>
<connect gate="G$2" pin="OUT1" pad="17"/>
<connect gate="G$2" pin="OUT2" pad="16"/>
<connect gate="G$2" pin="OUT3" pad="15"/>
<connect gate="G$2" pin="OUT4" pad="14"/>
<connect gate="G$2" pin="OUT5" pad="13"/>
<connect gate="G$2" pin="OUT6" pad="12"/>
<connect gate="G$2" pin="OUT7" pad="11"/>
<connect gate="G$2" pin="OUT8" pad="10"/>
<connect gate="G$2" pin="V+" pad="18"/>
<connect gate="G$2" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX381CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX381"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="1"/>
<connect gate="G$1" pin="COM2" pad="8"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="IN1" pad="15"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="4"/>
<connect gate="G$1" pin="NC@3" pad="5"/>
<connect gate="G$1" pin="NC@4" pad="6"/>
<connect gate="G$1" pin="NC@5" pad="7"/>
<connect gate="G$1" pin="NC@6" pad="12"/>
<connect gate="G$1" pin="NO1" pad="16"/>
<connect gate="G$1" pin="NO2" pad="9"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX381CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX381"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="COM1" pad="1"/>
<connect gate="G$2" pin="COM2" pad="8"/>
<connect gate="G$2" pin="GND" pad="13"/>
<connect gate="G$2" pin="IN1" pad="15"/>
<connect gate="G$2" pin="IN2" pad="10"/>
<connect gate="G$2" pin="NC" pad="2"/>
<connect gate="G$2" pin="NC@1" pad="3"/>
<connect gate="G$2" pin="NC@2" pad="4"/>
<connect gate="G$2" pin="NC@3" pad="5"/>
<connect gate="G$2" pin="NC@4" pad="6"/>
<connect gate="G$2" pin="NC@5" pad="7"/>
<connect gate="G$2" pin="NC@6" pad="12"/>
<connect gate="G$2" pin="NO1" pad="16"/>
<connect gate="G$2" pin="NO2" pad="9"/>
<connect gate="G$2" pin="V+" pad="11"/>
<connect gate="G$2" pin="V-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX383CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="MAX383"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$3" pin="COM1" pad="1"/>
<connect gate="G$3" pin="COM2" pad="8"/>
<connect gate="G$3" pin="COM3" pad="3"/>
<connect gate="G$3" pin="COM4" pad="6"/>
<connect gate="G$3" pin="GND" pad="13"/>
<connect gate="G$3" pin="IN1" pad="15"/>
<connect gate="G$3" pin="IN2" pad="10"/>
<connect gate="G$3" pin="NC" pad="2"/>
<connect gate="G$3" pin="NC3" pad="4"/>
<connect gate="G$3" pin="NC4" pad="5"/>
<connect gate="G$3" pin="NC@1" pad="7"/>
<connect gate="G$3" pin="NC@2" pad="12"/>
<connect gate="G$3" pin="NO1" pad="16"/>
<connect gate="G$3" pin="NO2" pad="9"/>
<connect gate="G$3" pin="V+" pad="11"/>
<connect gate="G$3" pin="V-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX383CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="MAX383"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$4" pin="COM1" pad="1"/>
<connect gate="G$4" pin="COM2" pad="8"/>
<connect gate="G$4" pin="COM3" pad="3"/>
<connect gate="G$4" pin="COM4" pad="6"/>
<connect gate="G$4" pin="GND" pad="13"/>
<connect gate="G$4" pin="IN1" pad="15"/>
<connect gate="G$4" pin="IN2" pad="10"/>
<connect gate="G$4" pin="NC" pad="2"/>
<connect gate="G$4" pin="NC3" pad="4"/>
<connect gate="G$4" pin="NC4" pad="5"/>
<connect gate="G$4" pin="NC@1" pad="7"/>
<connect gate="G$4" pin="NC@2" pad="12"/>
<connect gate="G$4" pin="NO1" pad="16"/>
<connect gate="G$4" pin="NO2" pad="9"/>
<connect gate="G$4" pin="V+" pad="11"/>
<connect gate="G$4" pin="V-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX385CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$6" symbol="MAX385"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$6" pin="COM1" pad="1"/>
<connect gate="G$6" pin="COM2" pad="8"/>
<connect gate="G$6" pin="COM3" pad="3"/>
<connect gate="G$6" pin="COM4" pad="6"/>
<connect gate="G$6" pin="GND" pad="13"/>
<connect gate="G$6" pin="IN1" pad="15"/>
<connect gate="G$6" pin="IN2" pad="10"/>
<connect gate="G$6" pin="NC" pad="2"/>
<connect gate="G$6" pin="NC@1" pad="7"/>
<connect gate="G$6" pin="NC@2" pad="12"/>
<connect gate="G$6" pin="NO1" pad="16"/>
<connect gate="G$6" pin="NO2" pad="9"/>
<connect gate="G$6" pin="NO3" pad="4"/>
<connect gate="G$6" pin="NO4" pad="5"/>
<connect gate="G$6" pin="V+" pad="11"/>
<connect gate="G$6" pin="V-" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX391CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX391"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX391CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX391"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="COM1" pad="2"/>
<connect gate="G$2" pin="COM2" pad="15"/>
<connect gate="G$2" pin="COM3" pad="10"/>
<connect gate="G$2" pin="COM4" pad="7"/>
<connect gate="G$2" pin="GND" pad="5"/>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="16"/>
<connect gate="G$2" pin="IN3" pad="9"/>
<connect gate="G$2" pin="IN4" pad="8"/>
<connect gate="G$2" pin="NC" pad="12"/>
<connect gate="G$2" pin="NC1" pad="3"/>
<connect gate="G$2" pin="NC2" pad="14"/>
<connect gate="G$2" pin="NC3" pad="11"/>
<connect gate="G$2" pin="NC4" pad="6"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX392CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="MAX392"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$3" pin="COM1" pad="2"/>
<connect gate="G$3" pin="COM2" pad="15"/>
<connect gate="G$3" pin="COM3" pad="10"/>
<connect gate="G$3" pin="COM4" pad="7"/>
<connect gate="G$3" pin="GND" pad="5"/>
<connect gate="G$3" pin="IN1" pad="1"/>
<connect gate="G$3" pin="IN2" pad="16"/>
<connect gate="G$3" pin="IN3" pad="9"/>
<connect gate="G$3" pin="IN4" pad="8"/>
<connect gate="G$3" pin="NC" pad="12"/>
<connect gate="G$3" pin="NO1" pad="3"/>
<connect gate="G$3" pin="NO2" pad="14"/>
<connect gate="G$3" pin="NO3" pad="11"/>
<connect gate="G$3" pin="NO4" pad="6"/>
<connect gate="G$3" pin="V+" pad="13"/>
<connect gate="G$3" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX392CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="MAX392"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$4" pin="COM1" pad="2"/>
<connect gate="G$4" pin="COM2" pad="15"/>
<connect gate="G$4" pin="COM3" pad="10"/>
<connect gate="G$4" pin="COM4" pad="7"/>
<connect gate="G$4" pin="GND" pad="5"/>
<connect gate="G$4" pin="IN1" pad="1"/>
<connect gate="G$4" pin="IN2" pad="16"/>
<connect gate="G$4" pin="IN3" pad="9"/>
<connect gate="G$4" pin="IN4" pad="8"/>
<connect gate="G$4" pin="NC" pad="12"/>
<connect gate="G$4" pin="NO1" pad="3"/>
<connect gate="G$4" pin="NO2" pad="14"/>
<connect gate="G$4" pin="NO3" pad="11"/>
<connect gate="G$4" pin="NO4" pad="6"/>
<connect gate="G$4" pin="V+" pad="13"/>
<connect gate="G$4" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX393CPE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$5" symbol="MAX393"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$5" pin="COM1" pad="2"/>
<connect gate="G$5" pin="COM2" pad="15"/>
<connect gate="G$5" pin="COM3" pad="10"/>
<connect gate="G$5" pin="COM4" pad="7"/>
<connect gate="G$5" pin="GND" pad="5"/>
<connect gate="G$5" pin="IN1" pad="1"/>
<connect gate="G$5" pin="IN2" pad="16"/>
<connect gate="G$5" pin="IN3" pad="9"/>
<connect gate="G$5" pin="IN4" pad="8"/>
<connect gate="G$5" pin="NC" pad="12"/>
<connect gate="G$5" pin="NC2" pad="14"/>
<connect gate="G$5" pin="NC3" pad="11"/>
<connect gate="G$5" pin="NO1" pad="3"/>
<connect gate="G$5" pin="NO4" pad="6"/>
<connect gate="G$5" pin="V+" pad="13"/>
<connect gate="G$5" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX393CSE" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$6" symbol="MAX393"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$6" pin="COM1" pad="2"/>
<connect gate="G$6" pin="COM2" pad="15"/>
<connect gate="G$6" pin="COM3" pad="10"/>
<connect gate="G$6" pin="COM4" pad="7"/>
<connect gate="G$6" pin="GND" pad="5"/>
<connect gate="G$6" pin="IN1" pad="1"/>
<connect gate="G$6" pin="IN2" pad="16"/>
<connect gate="G$6" pin="IN3" pad="9"/>
<connect gate="G$6" pin="IN4" pad="8"/>
<connect gate="G$6" pin="NC" pad="12"/>
<connect gate="G$6" pin="NC2" pad="14"/>
<connect gate="G$6" pin="NC3" pad="11"/>
<connect gate="G$6" pin="NO1" pad="3"/>
<connect gate="G$6" pin="NO4" pad="6"/>
<connect gate="G$6" pin="V+" pad="13"/>
<connect gate="G$6" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX389CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX398"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="COM" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="NO1" pad="4"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="NO3" pad="6"/>
<connect gate="G$1" pin="NO4" pad="7"/>
<connect gate="G$1" pin="NO5" pad="12"/>
<connect gate="G$1" pin="NO6" pad="11"/>
<connect gate="G$1" pin="NO7" pad="10"/>
<connect gate="G$1" pin="NO8" pad="9"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX398CSE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="MAX398"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="A0" pad="1"/>
<connect gate="G$2" pin="A1" pad="16"/>
<connect gate="G$2" pin="A2" pad="15"/>
<connect gate="G$2" pin="COM" pad="8"/>
<connect gate="G$2" pin="EN" pad="2"/>
<connect gate="G$2" pin="GND" pad="14"/>
<connect gate="G$2" pin="NO1" pad="4"/>
<connect gate="G$2" pin="NO2" pad="5"/>
<connect gate="G$2" pin="NO3" pad="6"/>
<connect gate="G$2" pin="NO4" pad="7"/>
<connect gate="G$2" pin="NO5" pad="12"/>
<connect gate="G$2" pin="NO6" pad="11"/>
<connect gate="G$2" pin="NO7" pad="10"/>
<connect gate="G$2" pin="NO8" pad="9"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX399CPE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="MAX399"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$3" pin="A0" pad="1"/>
<connect gate="G$3" pin="A1" pad="16"/>
<connect gate="G$3" pin="COMA" pad="8"/>
<connect gate="G$3" pin="COMB" pad="9"/>
<connect gate="G$3" pin="EN" pad="2"/>
<connect gate="G$3" pin="GND" pad="15"/>
<connect gate="G$3" pin="NO1A" pad="4"/>
<connect gate="G$3" pin="NO1B" pad="13"/>
<connect gate="G$3" pin="NO2A" pad="5"/>
<connect gate="G$3" pin="NO2B" pad="12"/>
<connect gate="G$3" pin="NO3A" pad="6"/>
<connect gate="G$3" pin="NO3B" pad="11"/>
<connect gate="G$3" pin="NO4A" pad="7"/>
<connect gate="G$3" pin="NO4B" pad="10"/>
<connect gate="G$3" pin="V+" pad="14"/>
<connect gate="G$3" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX399CSE" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="MAX399"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$4" pin="A0" pad="1"/>
<connect gate="G$4" pin="A1" pad="16"/>
<connect gate="G$4" pin="COMA" pad="8"/>
<connect gate="G$4" pin="COMB" pad="9"/>
<connect gate="G$4" pin="EN" pad="2"/>
<connect gate="G$4" pin="GND" pad="15"/>
<connect gate="G$4" pin="NO1A" pad="4"/>
<connect gate="G$4" pin="NO1B" pad="13"/>
<connect gate="G$4" pin="NO2A" pad="5"/>
<connect gate="G$4" pin="NO2B" pad="12"/>
<connect gate="G$4" pin="NO3A" pad="6"/>
<connect gate="G$4" pin="NO3B" pad="11"/>
<connect gate="G$4" pin="NO4A" pad="7"/>
<connect gate="G$4" pin="NO4B" pad="10"/>
<connect gate="G$4" pin="V+" pad="14"/>
<connect gate="G$4" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG401CY" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG401"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="8"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="IN1" pad="15"/>
<connect gate="G$1" pin="IN2" pad="10"/>
<connect gate="G$1" pin="S1" pad="16"/>
<connect gate="G$1" pin="S2" pad="9"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="14"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG403CJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="DG403"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$2" pin="D1" pad="1"/>
<connect gate="G$2" pin="D2" pad="8"/>
<connect gate="G$2" pin="D3" pad="3"/>
<connect gate="G$2" pin="D4" pad="6"/>
<connect gate="G$2" pin="GND" pad="13"/>
<connect gate="G$2" pin="IN1" pad="15"/>
<connect gate="G$2" pin="IN2" pad="10"/>
<connect gate="G$2" pin="S1" pad="16"/>
<connect gate="G$2" pin="S2" pad="9"/>
<connect gate="G$2" pin="S3" pad="4"/>
<connect gate="G$2" pin="S4" pad="5"/>
<connect gate="G$2" pin="V+" pad="11"/>
<connect gate="G$2" pin="V-" pad="14"/>
<connect gate="G$2" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG403CY" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$3" symbol="DG403"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$3" pin="D1" pad="1"/>
<connect gate="G$3" pin="D2" pad="8"/>
<connect gate="G$3" pin="D3" pad="3"/>
<connect gate="G$3" pin="D4" pad="6"/>
<connect gate="G$3" pin="GND" pad="13"/>
<connect gate="G$3" pin="IN1" pad="15"/>
<connect gate="G$3" pin="IN2" pad="10"/>
<connect gate="G$3" pin="S1" pad="16"/>
<connect gate="G$3" pin="S2" pad="9"/>
<connect gate="G$3" pin="S3" pad="4"/>
<connect gate="G$3" pin="S4" pad="5"/>
<connect gate="G$3" pin="V+" pad="11"/>
<connect gate="G$3" pin="V-" pad="14"/>
<connect gate="G$3" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG405CJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$4" symbol="DG403"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$4" pin="D1" pad="1"/>
<connect gate="G$4" pin="D2" pad="8"/>
<connect gate="G$4" pin="D3" pad="3"/>
<connect gate="G$4" pin="D4" pad="6"/>
<connect gate="G$4" pin="GND" pad="13"/>
<connect gate="G$4" pin="IN1" pad="15"/>
<connect gate="G$4" pin="IN2" pad="10"/>
<connect gate="G$4" pin="S1" pad="16"/>
<connect gate="G$4" pin="S2" pad="9"/>
<connect gate="G$4" pin="S3" pad="4"/>
<connect gate="G$4" pin="S4" pad="5"/>
<connect gate="G$4" pin="V+" pad="11"/>
<connect gate="G$4" pin="V-" pad="14"/>
<connect gate="G$4" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG405CY" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$5" symbol="DG403"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$5" pin="D1" pad="1"/>
<connect gate="G$5" pin="D2" pad="8"/>
<connect gate="G$5" pin="D3" pad="3"/>
<connect gate="G$5" pin="D4" pad="6"/>
<connect gate="G$5" pin="GND" pad="13"/>
<connect gate="G$5" pin="IN1" pad="15"/>
<connect gate="G$5" pin="IN2" pad="10"/>
<connect gate="G$5" pin="S1" pad="16"/>
<connect gate="G$5" pin="S2" pad="9"/>
<connect gate="G$5" pin="S3" pad="4"/>
<connect gate="G$5" pin="S4" pad="5"/>
<connect gate="G$5" pin="V+" pad="11"/>
<connect gate="G$5" pin="V-" pad="14"/>
<connect gate="G$5" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG406CWI" prefix="IC">
<description>&lt;b&gt;ANALOG MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG406"/>
</gates>
<devices>
<device name="" package="SO28L">
<connects>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="D" pad="28"/>
<connect gate="G$1" pin="EN" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="S1" pad="19"/>
<connect gate="G$1" pin="S10" pad="10"/>
<connect gate="G$1" pin="S11" pad="9"/>
<connect gate="G$1" pin="S12" pad="8"/>
<connect gate="G$1" pin="S13" pad="7"/>
<connect gate="G$1" pin="S14" pad="6"/>
<connect gate="G$1" pin="S15" pad="5"/>
<connect gate="G$1" pin="S16" pad="4"/>
<connect gate="G$1" pin="S2" pad="20"/>
<connect gate="G$1" pin="S3" pad="21"/>
<connect gate="G$1" pin="S4" pad="22"/>
<connect gate="G$1" pin="S5" pad="23"/>
<connect gate="G$1" pin="S6" pad="24"/>
<connect gate="G$1" pin="S7" pad="25"/>
<connect gate="G$1" pin="S8" pad="26"/>
<connect gate="G$1" pin="S9" pad="11"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG408DY" prefix="IC">
<description>&lt;b&gt;ANALOG MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="DG408"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="A0" pad="1"/>
<connect gate="G$2" pin="A1" pad="16"/>
<connect gate="G$2" pin="A2" pad="15"/>
<connect gate="G$2" pin="D" pad="8"/>
<connect gate="G$2" pin="EN" pad="2"/>
<connect gate="G$2" pin="GND" pad="14"/>
<connect gate="G$2" pin="S1" pad="4"/>
<connect gate="G$2" pin="S2" pad="5"/>
<connect gate="G$2" pin="S3" pad="6"/>
<connect gate="G$2" pin="S4" pad="7"/>
<connect gate="G$2" pin="S5" pad="12"/>
<connect gate="G$2" pin="S6" pad="11"/>
<connect gate="G$2" pin="S7" pad="10"/>
<connect gate="G$2" pin="S8" pad="9"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG411CJ" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DG411"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="D1" pad="2"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="S1" pad="3"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="11"/>
<connect gate="G$1" pin="S4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG409DY" prefix="IC">
<description>&lt;b&gt;ANALOG MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="DG409"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="A0" pad="1"/>
<connect gate="G$2" pin="A1" pad="16"/>
<connect gate="G$2" pin="DA" pad="8"/>
<connect gate="G$2" pin="DB" pad="9"/>
<connect gate="G$2" pin="EN" pad="2"/>
<connect gate="G$2" pin="GND" pad="15"/>
<connect gate="G$2" pin="S1A" pad="4"/>
<connect gate="G$2" pin="S1B" pad="13"/>
<connect gate="G$2" pin="S2A" pad="5"/>
<connect gate="G$2" pin="S2B" pad="12"/>
<connect gate="G$2" pin="S3A" pad="6"/>
<connect gate="G$2" pin="S3B" pad="11"/>
<connect gate="G$2" pin="S4A" pad="7"/>
<connect gate="G$2" pin="S4B" pad="10"/>
<connect gate="G$2" pin="V+" pad="14"/>
<connect gate="G$2" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG411CY" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$2" symbol="DG411"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$2" pin="D1" pad="2"/>
<connect gate="G$2" pin="D2" pad="15"/>
<connect gate="G$2" pin="D3" pad="10"/>
<connect gate="G$2" pin="D4" pad="7"/>
<connect gate="G$2" pin="GND" pad="5"/>
<connect gate="G$2" pin="IN1" pad="1"/>
<connect gate="G$2" pin="IN2" pad="16"/>
<connect gate="G$2" pin="IN3" pad="9"/>
<connect gate="G$2" pin="IN4" pad="8"/>
<connect gate="G$2" pin="S1" pad="3"/>
<connect gate="G$2" pin="S2" pad="14"/>
<connect gate="G$2" pin="S3" pad="11"/>
<connect gate="G$2" pin="S4" pad="6"/>
<connect gate="G$2" pin="V+" pad="13"/>
<connect gate="G$2" pin="V-" pad="4"/>
<connect gate="G$2" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX388CPN" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX388"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!RS" pad="18"/>
<connect gate="G$1" pin="!WR" pad="1"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="17"/>
<connect gate="G$1" pin="A2" pad="16"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="6"/>
<connect gate="G$1" pin="IN3" pad="7"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="IN5" pad="13"/>
<connect gate="G$1" pin="IN6" pad="12"/>
<connect gate="G$1" pin="IN7" pad="11"/>
<connect gate="G$1" pin="IN8" pad="10"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX389CPN" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX389"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!RS" pad="18"/>
<connect gate="G$1" pin="!WR" pad="1"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="17"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="IN1A" pad="5"/>
<connect gate="G$1" pin="IN1B" pad="14"/>
<connect gate="G$1" pin="IN2A" pad="6"/>
<connect gate="G$1" pin="IN2B" pad="13"/>
<connect gate="G$1" pin="IN3A" pad="7"/>
<connect gate="G$1" pin="IN3B" pad="12"/>
<connect gate="G$1" pin="IN4A" pad="8"/>
<connect gate="G$1" pin="IN4B" pad="11"/>
<connect gate="G$1" pin="OUTA" pad="9"/>
<connect gate="G$1" pin="OUTB" pad="10"/>
<connect gate="G$1" pin="V+" pad="15"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX516CNG" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX516"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="AIN0" pad="5"/>
<connect gate="G$1" pin="AIN1" pad="4"/>
<connect gate="G$1" pin="AIN2" pad="21"/>
<connect gate="G$1" pin="AIN3" pad="20"/>
<connect gate="G$1" pin="C0" pad="2"/>
<connect gate="G$1" pin="C1" pad="1"/>
<connect gate="G$1" pin="C2" pad="24"/>
<connect gate="G$1" pin="C3" pad="23"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="14"/>
<connect gate="G$1" pin="D5" pad="13"/>
<connect gate="G$1" pin="D6" pad="12"/>
<connect gate="G$1" pin="D7" pad="11"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="REF" pad="19"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VDD" pad="22"/>
<connect gate="G$1" pin="WR" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX752CPA" prefix="IC">
<description>&lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX752"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="!SHDN" pad="1"/>
<connect gate="G$1" pin="CC" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LX" pad="6"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="SS" pad="3"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX76*" prefix="IC">
<description>&lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX765"/>
</gates>
<devices>
<device name="PA" package="DIL08">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="REF" pad="4"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V+@0" pad="7"/>
</connects>
<technologies>
<technology name="4C"/>
<technology name="4E"/>
<technology name="5C"/>
<technology name="5E"/>
<technology name="6C"/>
<technology name="6E"/>
</technologies>
</device>
<device name="SA" package="SO08">
<connects>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="REF" pad="4"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V+@0" pad="7"/>
</connects>
<technologies>
<technology name="4C"/>
<technology name="4E"/>
<technology name="5C"/>
<technology name="5E"/>
<technology name="6C"/>
<technology name="6E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MXD1000" prefix="IC">
<description>&lt;b&gt;DELAY LINE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MXD1000"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="TAP1" pad="7"/>
<connect gate="G$1" pin="TAP2" pad="2"/>
<connect gate="G$1" pin="TAP3" pad="6"/>
<connect gate="G$1" pin="TAP4" pad="3"/>
<connect gate="G$1" pin="TAP5" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MXD1000S" prefix="IC">
<description>&lt;b&gt;DELAY LINE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MXD1000"/>
<gate name="G$2" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="TAP1" pad="7"/>
<connect gate="G$1" pin="TAP2" pad="2"/>
<connect gate="G$1" pin="TAP3" pad="6"/>
<connect gate="G$1" pin="TAP4" pad="3"/>
<connect gate="G$1" pin="TAP5" pad="5"/>
<connect gate="G$2" pin="GND" pad="4"/>
<connect gate="G$2" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MXD1000P" prefix="IC">
<description>&lt;b&gt;DELAY LINE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MXD1000"/>
<gate name="P" symbol="VCC-GND"/>
<gate name="2" symbol="NC"/>
<gate name="3" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="9" symbol="NC"/>
<gate name="11" symbol="NC"/>
<gate name="13" symbol="NC"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="11" pin="NC" pad="11"/>
<connect gate="13" pin="NC" pad="13"/>
<connect gate="2" pin="NC" pad="2"/>
<connect gate="3" pin="NC" pad="3"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="9" pin="NC" pad="9"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="TAP1" pad="12"/>
<connect gate="G$1" pin="TAP2" pad="4"/>
<connect gate="G$1" pin="TAP3" pad="10"/>
<connect gate="G$1" pin="TAP4" pad="6"/>
<connect gate="G$1" pin="TAP5" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MXD1000W" prefix="IC">
<description>&lt;b&gt;DELAY LINE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MXD1000"/>
<gate name="P" symbol="VCC-GND"/>
<gate name="2" symbol="NC"/>
<gate name="3" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="7" symbol="NC"/>
<gate name="10" symbol="NC"/>
<gate name="12" symbol="NC"/>
<gate name="14" symbol="NC"/>
<gate name="15" symbol="NC"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="10" pin="NC" pad="10"/>
<connect gate="12" pin="NC" pad="12"/>
<connect gate="14" pin="NC" pad="14"/>
<connect gate="15" pin="NC" pad="15"/>
<connect gate="2" pin="NC" pad="2"/>
<connect gate="3" pin="NC" pad="3"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="7" pin="NC" pad="7"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="TAP1" pad="13"/>
<connect gate="G$1" pin="TAP2" pad="4"/>
<connect gate="G$1" pin="TAP3" pad="11"/>
<connect gate="G$1" pin="TAP4" pad="6"/>
<connect gate="G$1" pin="TAP5" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3237" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX3237"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="C1+" pad="28"/>
<connect gate="G$1" pin="C1-" pad="25"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="3"/>
<connect gate="G$1" pin="EN/" pad="13"/>
<connect gate="G$1" pin="MBOUD" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="8"/>
<connect gate="G$1" pin="R1OUT" pad="21"/>
<connect gate="G$1" pin="R1OUTB" pad="16"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2OUT" pad="20"/>
<connect gate="G$1" pin="R3IN" pad="11"/>
<connect gate="G$1" pin="R3OUT" pad="18"/>
<connect gate="G$1" pin="SHDN/" pad="14"/>
<connect gate="G$1" pin="T1IN" pad="24"/>
<connect gate="G$1" pin="T1OUT" pad="5"/>
<connect gate="G$1" pin="T2IN" pad="23"/>
<connect gate="G$1" pin="T2OUT" pad="6"/>
<connect gate="G$1" pin="T3IN" pad="22"/>
<connect gate="G$1" pin="T3OUT" pad="7"/>
<connect gate="G$1" pin="T4IN" pad="19"/>
<connect gate="G$1" pin="T4OUT" pad="10"/>
<connect gate="G$1" pin="T5IN" pad="17"/>
<connect gate="G$1" pin="T5OUT" pad="12"/>
<connect gate="G$1" pin="V+" pad="27"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3241" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX3241"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="C1+" pad="28"/>
<connect gate="G$1" pin="C1-" pad="24"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="EN/" pad="23"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="19"/>
<connect gate="G$1" pin="R1OUTB" pad="21"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="18"/>
<connect gate="G$1" pin="R2OUTB" pad="20"/>
<connect gate="G$1" pin="R3IN" pad="6"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="R4IN" pad="7"/>
<connect gate="G$1" pin="R4OUT" pad="16"/>
<connect gate="G$1" pin="R5IN" pad="8"/>
<connect gate="G$1" pin="R5OUT" pad="15"/>
<connect gate="G$1" pin="SHDN/" pad="22"/>
<connect gate="G$1" pin="T1IN" pad="14"/>
<connect gate="G$1" pin="T1OUT" pad="9"/>
<connect gate="G$1" pin="T2IN" pad="13"/>
<connect gate="G$1" pin="T2OUT" pad="10"/>
<connect gate="G$1" pin="T3IN" pad="12"/>
<connect gate="G$1" pin="T3OUT" pad="11"/>
<connect gate="G$1" pin="V+" pad="27"/>
<connect gate="G$1" pin="V-" pad="3"/>
<connect gate="P" pin="GND" pad="25"/>
<connect gate="P" pin="VCC" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3222" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX3222"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="EN/" pad="1"/>
<connect gate="G$1" pin="R1IN" pad="14"/>
<connect gate="G$1" pin="R1OUT" pad="13"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="SHDN/" pad="18"/>
<connect gate="G$1" pin="T1IN" pad="12"/>
<connect gate="G$1" pin="T1OUT" pad="15"/>
<connect gate="G$1" pin="T2IN" pad="11"/>
<connect gate="G$1" pin="T2OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX410CPA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="PWR+-"/>
<gate name="NC" symbol="NC"/>
<gate name="G$1" symbol="OPOFF"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OFF1" pad="1"/>
<connect gate="G$1" pin="OFF2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="NC" pin="NC" pad="5"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX481CSA" prefix="IC">
<description>&lt;b&gt;RS485 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX481"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="RE/" pad="2"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX481CUA" prefix="IC">
<description>&lt;b&gt;RS485 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX481"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="UMAX8">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="DE" pad="5"/>
<connect gate="G$1" pin="DI" pad="6"/>
<connect gate="G$1" pin="RE/" pad="4"/>
<connect gate="G$1" pin="RO" pad="3"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX488" prefix="IC">
<description>&lt;b&gt;RS485 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX488"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="CSA" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Z" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CPD" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Z" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CUA" package="UMAX8">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="RO" pad="4"/>
<connect gate="G$1" pin="Y" pad="7"/>
<connect gate="G$1" pin="Z" pad="8"/>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX489CSD" prefix="IC">
<description>&lt;b&gt;RS485 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX489"/>
<gate name="1" symbol="NC"/>
<gate name="8" symbol="NC"/>
<gate name="13" symbol="NC"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="13" pin="NC" pad="13"/>
<connect gate="8" pin="NC" pad="8"/>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="RE/" pad="3"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1674" prefix="IC">
<description>&lt;b&gt;DC/DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX1674"/>
</gates>
<devices>
<device name="" package="UMAX8">
<connects>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LBI" pad="2"/>
<connect gate="G$1" pin="LBO/" pad="3"/>
<connect gate="G$1" pin="LX" pad="7"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="REF" pad="4"/>
<connect gate="G$1" pin="SHDN/" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1676" prefix="IC">
<description>&lt;b&gt;DC/DC CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX1676"/>
</gates>
<devices>
<device name="" package="UMAX10">
<connects>
<connect gate="G$1" pin="BATT" pad="7"/>
<connect gate="G$1" pin="CSEL" pad="4"/>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LBI" pad="2"/>
<connect gate="G$1" pin="LBO/" pad="3"/>
<connect gate="G$1" pin="LX" pad="9"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="SHDN/" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX813L" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX705"/>
</gates>
<devices>
<device name="CSA" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="WDI" pad="6"/>
<connect gate="G$1" pin="WDO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CUA" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="WDI" pad="6"/>
<connect gate="G$1" pin="WDO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX705CUA" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX705"/>
</gates>
<devices>
<device name="" package="UMAX8">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="WDI" pad="6"/>
<connect gate="G$1" pin="WDO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX705CSA" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX705"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="MR" pad="1"/>
<connect gate="G$1" pin="PFI" pad="4"/>
<connect gate="G$1" pin="PFO" pad="5"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="WDI" pad="6"/>
<connect gate="G$1" pin="WDO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX481CPA" prefix="IC">
<description>&lt;b&gt;RS485 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX481"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="RE/" pad="2"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX489CPD" prefix="IC">
<description>&lt;b&gt;RS485 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX489"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="RE/" pad="3"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC2" pin="NC" pad="8"/>
<connect gate="NC3" pin="NC" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4105ESA" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OP"/>
<gate name="P" symbol="VCC-VEE"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC2" pin="NC" pad="5"/>
<connect gate="NC3" pin="NC" pad="8"/>
<connect gate="P" pin="VCC" pad="7"/>
<connect gate="P" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4105EUK" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OP"/>
<gate name="P" symbol="VCC-VEE"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="P" pin="VCC" pad="5"/>
<connect gate="P" pin="VEE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX413*EWG" prefix="IC">
<description>&lt;b&gt;1-Input/4-Output Video Distribution Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX4137-MAX4138.pdf</description>
<gates>
<gate name="G$1" symbol="MAX4137"/>
</gates>
<devices>
<device name="" package="SO24L">
<connects>
<connect gate="G$1" pin="/SEL1" pad="23"/>
<connect gate="G$1" pin="/SEL2" pad="22"/>
<connect gate="G$1" pin="/SEL3" pad="15"/>
<connect gate="G$1" pin="/SEL4" pad="14"/>
<connect gate="G$1" pin="AGND@3" pad="18"/>
<connect gate="G$1" pin="AGND@4" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="IN+" pad="20"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC12" pad="12"/>
<connect gate="G$1" pin="NC13" pad="13"/>
<connect gate="G$1" pin="NC17" pad="17"/>
<connect gate="G$1" pin="NC24" pad="24"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="10"/>
<connect gate="G$1" pin="VCCI" pad="16"/>
<connect gate="G$1" pin="VCCO@1" pad="2"/>
<connect gate="G$1" pin="VCCO@2" pad="11"/>
<connect gate="G$1" pin="VEEI" pad="19"/>
<connect gate="G$1" pin="VEEO@1" pad="6"/>
<connect gate="G$1" pin="VEEO@2" pad="7"/>
</connects>
<technologies>
<technology name="7"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4137" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="NC1" symbol="MAX4137"/>
</gates>
<devices>
<device name="" package="SO24L">
<connects>
<connect gate="NC1" pin="/SEL1" pad="23"/>
<connect gate="NC1" pin="/SEL2" pad="22"/>
<connect gate="NC1" pin="/SEL3" pad="15"/>
<connect gate="NC1" pin="/SEL4" pad="14"/>
<connect gate="NC1" pin="AGND@3" pad="18"/>
<connect gate="NC1" pin="AGND@4" pad="21"/>
<connect gate="NC1" pin="GND@1" pad="4"/>
<connect gate="NC1" pin="GND@2" pad="9"/>
<connect gate="NC1" pin="IN+" pad="20"/>
<connect gate="NC1" pin="NC1" pad="1"/>
<connect gate="NC1" pin="NC12" pad="12"/>
<connect gate="NC1" pin="NC13" pad="13"/>
<connect gate="NC1" pin="NC17" pad="17"/>
<connect gate="NC1" pin="NC24" pad="24"/>
<connect gate="NC1" pin="OUT1" pad="3"/>
<connect gate="NC1" pin="OUT2" pad="5"/>
<connect gate="NC1" pin="OUT3" pad="8"/>
<connect gate="NC1" pin="OUT4" pad="10"/>
<connect gate="NC1" pin="VCCI" pad="16"/>
<connect gate="NC1" pin="VCCO@1" pad="2"/>
<connect gate="NC1" pin="VCCO@2" pad="11"/>
<connect gate="NC1" pin="VEEI" pad="19"/>
<connect gate="NC1" pin="VEEO@1" pad="6"/>
<connect gate="NC1" pin="VEEO@2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4138" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="NC1" symbol="MAX4138"/>
</gates>
<devices>
<device name="" package="SO24L">
<connects>
<connect gate="NC1" pin="/SEL1" pad="23"/>
<connect gate="NC1" pin="/SEL2" pad="22"/>
<connect gate="NC1" pin="/SEL3" pad="15"/>
<connect gate="NC1" pin="/SEL4" pad="14"/>
<connect gate="NC1" pin="AGND@1" pad="4"/>
<connect gate="NC1" pin="AGND@2" pad="9"/>
<connect gate="NC1" pin="AGND@4" pad="21"/>
<connect gate="NC1" pin="IN+" pad="20"/>
<connect gate="NC1" pin="NC1" pad="1"/>
<connect gate="NC1" pin="NC12" pad="12"/>
<connect gate="NC1" pin="NC13" pad="13"/>
<connect gate="NC1" pin="NC24" pad="24"/>
<connect gate="NC1" pin="OUT1" pad="3"/>
<connect gate="NC1" pin="OUT2" pad="5"/>
<connect gate="NC1" pin="OUT3" pad="8"/>
<connect gate="NC1" pin="OUT4" pad="10"/>
<connect gate="NC1" pin="RF" pad="17"/>
<connect gate="NC1" pin="RG" pad="18"/>
<connect gate="NC1" pin="VCCI" pad="16"/>
<connect gate="NC1" pin="VCCO@1" pad="2"/>
<connect gate="NC1" pin="VCCO@2" pad="11"/>
<connect gate="NC1" pin="VEEI" pad="19"/>
<connect gate="NC1" pin="VEEO@1" pad="6"/>
<connect gate="NC1" pin="VEEO@2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX232ECWE" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX232"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX202ECWE" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX232"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX203ECWP" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX203E"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="SO20L">
<connects>
<connect gate="G$1" pin="C1+" pad="13"/>
<connect gate="G$1" pin="C1-" pad="14"/>
<connect gate="G$1" pin="C2+/1" pad="12"/>
<connect gate="G$1" pin="C2+/2" pad="15"/>
<connect gate="G$1" pin="C2-/1" pad="11"/>
<connect gate="G$1" pin="C2-/2" pad="16"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="3"/>
<connect gate="G$1" pin="R2IN" pad="19"/>
<connect gate="G$1" pin="R2OUT" pad="20"/>
<connect gate="G$1" pin="T1IN" pad="2"/>
<connect gate="G$1" pin="T1OUT" pad="5"/>
<connect gate="G$1" pin="T2IN" pad="1"/>
<connect gate="G$1" pin="T2OUT" pad="18"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-/1" pad="10"/>
<connect gate="G$1" pin="V-/2" pad="17"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="9"/>
<connect gate="P" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX206ECWG" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="VCC-GND"/>
<gate name="G$1" symbol="MAX236"/>
</gates>
<devices>
<device name="" package="SO24L">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="12"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="14"/>
<connect gate="G$1" pin="EN" pad="20"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="5"/>
<connect gate="G$1" pin="R2IN" pad="23"/>
<connect gate="G$1" pin="R2OUT" pad="22"/>
<connect gate="G$1" pin="R3IN" pad="16"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="SHDN" pad="21"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="6"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="18"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="19"/>
<connect gate="G$1" pin="T4OUT" pad="24"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX205ECPG" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX235"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="EN" pad="20"/>
<connect gate="G$1" pin="R1IN" pad="10"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="6"/>
<connect gate="G$1" pin="R3IN" pad="24"/>
<connect gate="G$1" pin="R3OUT" pad="23"/>
<connect gate="G$1" pin="R4IN" pad="18"/>
<connect gate="G$1" pin="R4OUT" pad="17"/>
<connect gate="G$1" pin="R5IN" pad="13"/>
<connect gate="G$1" pin="R5OUT" pad="14"/>
<connect gate="G$1" pin="SHDN" pad="21"/>
<connect gate="G$1" pin="T1IN" pad="8"/>
<connect gate="G$1" pin="T1OUT" pad="3"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T2OUT" pad="4"/>
<connect gate="G$1" pin="T3IN" pad="15"/>
<connect gate="G$1" pin="T3OUT" pad="2"/>
<connect gate="G$1" pin="T4IN" pad="16"/>
<connect gate="G$1" pin="T4OUT" pad="1"/>
<connect gate="G$1" pin="T5IN" pad="22"/>
<connect gate="G$1" pin="T5OUT" pad="19"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX207ECWG" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX237"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO24L">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="12"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="5"/>
<connect gate="G$1" pin="R2IN" pad="23"/>
<connect gate="G$1" pin="R2OUT" pad="22"/>
<connect gate="G$1" pin="R3IN" pad="16"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="6"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="18"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="19"/>
<connect gate="G$1" pin="T4OUT" pad="24"/>
<connect gate="G$1" pin="T5IN" pad="21"/>
<connect gate="G$1" pin="T5OUT" pad="20"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX208ECWG" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX238"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO24L">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="12"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="7"/>
<connect gate="G$1" pin="R1OUT" pad="6"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R2OUT" pad="4"/>
<connect gate="G$1" pin="R3IN" pad="23"/>
<connect gate="G$1" pin="R3OUT" pad="22"/>
<connect gate="G$1" pin="R4IN" pad="16"/>
<connect gate="G$1" pin="R4OUT" pad="17"/>
<connect gate="G$1" pin="T1IN" pad="5"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="18"/>
<connect gate="G$1" pin="T2OUT" pad="1"/>
<connect gate="G$1" pin="T3IN" pad="19"/>
<connect gate="G$1" pin="T3OUT" pad="24"/>
<connect gate="G$1" pin="T4IN" pad="21"/>
<connect gate="G$1" pin="T4OUT" pad="20"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX241ECWI" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX211E"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO28L">
<connects>
<connect gate="G$1" pin="C1+" pad="12"/>
<connect gate="G$1" pin="C1-" pad="14"/>
<connect gate="G$1" pin="C2+" pad="15"/>
<connect gate="G$1" pin="C2-" pad="16"/>
<connect gate="G$1" pin="EN" pad="24"/>
<connect gate="G$1" pin="R1IN" pad="9"/>
<connect gate="G$1" pin="R1OUT" pad="8"/>
<connect gate="G$1" pin="R2IN" pad="4"/>
<connect gate="G$1" pin="R2OUT" pad="5"/>
<connect gate="G$1" pin="R3IN" pad="27"/>
<connect gate="G$1" pin="R3OUT" pad="26"/>
<connect gate="G$1" pin="R4IN" pad="23"/>
<connect gate="G$1" pin="R4OUT" pad="22"/>
<connect gate="G$1" pin="R5IN" pad="18"/>
<connect gate="G$1" pin="R5OUT" pad="19"/>
<connect gate="G$1" pin="SHDN" pad="25"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="6"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="20"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="21"/>
<connect gate="G$1" pin="T4OUT" pad="28"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX211ECWI" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX211E"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO28L">
<connects>
<connect gate="G$1" pin="C1+" pad="12"/>
<connect gate="G$1" pin="C1-" pad="14"/>
<connect gate="G$1" pin="C2+" pad="15"/>
<connect gate="G$1" pin="C2-" pad="16"/>
<connect gate="G$1" pin="EN" pad="24"/>
<connect gate="G$1" pin="R1IN" pad="9"/>
<connect gate="G$1" pin="R1OUT" pad="8"/>
<connect gate="G$1" pin="R2IN" pad="4"/>
<connect gate="G$1" pin="R2OUT" pad="5"/>
<connect gate="G$1" pin="R3IN" pad="27"/>
<connect gate="G$1" pin="R3OUT" pad="26"/>
<connect gate="G$1" pin="R4IN" pad="23"/>
<connect gate="G$1" pin="R4OUT" pad="22"/>
<connect gate="G$1" pin="R5IN" pad="18"/>
<connect gate="G$1" pin="R5OUT" pad="19"/>
<connect gate="G$1" pin="SHDN" pad="25"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="6"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="20"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="21"/>
<connect gate="G$1" pin="T4OUT" pad="28"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX213ECWI" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX213E"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO28L">
<connects>
<connect gate="G$1" pin="C1+" pad="12"/>
<connect gate="G$1" pin="C1-" pad="14"/>
<connect gate="G$1" pin="C2+" pad="15"/>
<connect gate="G$1" pin="C2-" pad="16"/>
<connect gate="G$1" pin="EN" pad="24"/>
<connect gate="G$1" pin="R1IN" pad="9"/>
<connect gate="G$1" pin="R1OUT" pad="8"/>
<connect gate="G$1" pin="R2IN" pad="4"/>
<connect gate="G$1" pin="R2OUT" pad="5"/>
<connect gate="G$1" pin="R3IN" pad="27"/>
<connect gate="G$1" pin="R3OUT" pad="26"/>
<connect gate="G$1" pin="R4IN" pad="23"/>
<connect gate="G$1" pin="R4OUT" pad="22"/>
<connect gate="G$1" pin="R5IN" pad="18"/>
<connect gate="G$1" pin="R5OUT" pad="19"/>
<connect gate="G$1" pin="SHDN" pad="25"/>
<connect gate="G$1" pin="T1IN" pad="7"/>
<connect gate="G$1" pin="T1OUT" pad="2"/>
<connect gate="G$1" pin="T2IN" pad="6"/>
<connect gate="G$1" pin="T2OUT" pad="3"/>
<connect gate="G$1" pin="T3IN" pad="20"/>
<connect gate="G$1" pin="T3OUT" pad="1"/>
<connect gate="G$1" pin="T4IN" pad="21"/>
<connect gate="G$1" pin="T4OUT" pad="28"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4278ESA" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="8" symbol="NC"/>
<gate name="2" symbol="BUFF3P"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="2" pin="GND" pad="2"/>
<connect gate="2" pin="IN" pad="3"/>
<connect gate="2" pin="OUT" pad="6"/>
<connect gate="2" pin="VCC" pad="7"/>
<connect gate="2" pin="VEE" pad="4"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="8" pin="NC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4278EUA" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BUFF3P"/>
<gate name="1" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="8" symbol="NC"/>
</gates>
<devices>
<device name="" package="UMAX8">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="8" pin="NC" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4278EUK" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="BUFF3P"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="1" pin="GND" pad="4"/>
<connect gate="1" pin="IN" pad="3"/>
<connect gate="1" pin="OUT" pad="1"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="1" pin="VEE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4178ESA" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BUFF3P"/>
<gate name="1" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="8" symbol="NC"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="8" pin="NC" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4178EUA" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BUFF3P"/>
<gate name="1" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="8" symbol="NC"/>
</gates>
<devices>
<device name="" package="UMAX8">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="8" pin="NC" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VEE" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4178EUK" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BUFF3P"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VEE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX807LSO" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX807"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="!CEIN" pad="12"/>
<connect gate="G$1" pin="!CEOUT" pad="11"/>
<connect gate="G$1" pin="!LOWLINE" pad="7"/>
<connect gate="G$1" pin="!MR" pad="6"/>
<connect gate="G$1" pin="!PFO" pad="2"/>
<connect gate="G$1" pin="!RESET" pad="9"/>
<connect gate="G$1" pin="!WDO" pad="10"/>
<connect gate="G$1" pin="BATT" pad="14"/>
<connect gate="G$1" pin="BATT_OK" pad="15"/>
<connect gate="G$1" pin="BATT_ON" pad="13"/>
<connect gate="G$1" pin="OUT" pad="16"/>
<connect gate="G$1" pin="PFI" pad="1"/>
<connect gate="G$1" pin="RESET" pad="8"/>
<connect gate="G$1" pin="WDI" pad="4"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX233AEWP" prefix="IC">
<description>&lt;b&gt;RS232 TRANSEIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX233"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="SO20L">
<connects>
<connect gate="G$1" pin="C1+" pad="13"/>
<connect gate="G$1" pin="C1-" pad="14"/>
<connect gate="G$1" pin="C2+@1" pad="12"/>
<connect gate="G$1" pin="C2+@2" pad="15"/>
<connect gate="G$1" pin="C2-@1" pad="11"/>
<connect gate="G$1" pin="C2-@2" pad="16"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="3"/>
<connect gate="G$1" pin="R2IN" pad="19"/>
<connect gate="G$1" pin="R2OUT" pad="20"/>
<connect gate="G$1" pin="T1IN" pad="2"/>
<connect gate="G$1" pin="T1OUT" pad="5"/>
<connect gate="G$1" pin="T2IN" pad="1"/>
<connect gate="G$1" pin="T2OUT" pad="18"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-@1" pad="10"/>
<connect gate="G$1" pin="V-@2" pad="17"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="9"/>
<connect gate="P" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX691CWE" prefix="IC">
<description>&lt;b&gt;WATCHDOG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX691"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="BATT-ON" pad="5"/>
<connect gate="G$1" pin="CE-IN" pad="13"/>
<connect gate="G$1" pin="CE-OUT" pad="12"/>
<connect gate="G$1" pin="LOW-LINE" pad="6"/>
<connect gate="G$1" pin="OSC-IN" pad="7"/>
<connect gate="G$1" pin="OSC-SEL" pad="8"/>
<connect gate="G$1" pin="PFI" pad="9"/>
<connect gate="G$1" pin="PFO" pad="10"/>
<connect gate="G$1" pin="RESET" pad="16"/>
<connect gate="G$1" pin="RESET@" pad="15"/>
<connect gate="G$1" pin="VBATT" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
<connect gate="G$1" pin="WDI" pad="11"/>
<connect gate="G$1" pin="WDO" pad="14"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX038*" prefix="IC">
<description>&lt;b&gt;HIGH FREQUENCY WAVEFORM GENERATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX038"/>
</gates>
<devices>
<device name="WP" package="SO20L">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="COSC" pad="5"/>
<connect gate="G$1" pin="DADJ" pad="7"/>
<connect gate="G$1" pin="DGND" pad="15"/>
<connect gate="G$1" pin="DV+" pad="16"/>
<connect gate="G$1" pin="FADJ" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="11"/>
<connect gate="G$1" pin="GND@4" pad="18"/>
<connect gate="G$1" pin="IIN" pad="10"/>
<connect gate="G$1" pin="OUT" pad="19"/>
<connect gate="G$1" pin="PDI" pad="13"/>
<connect gate="G$1" pin="PDO" pad="12"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SYNC" pad="14"/>
<connect gate="G$1" pin="V+" pad="17"/>
<connect gate="G$1" pin="V-" pad="20"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="PP" package="DIL20">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="COSC" pad="5"/>
<connect gate="G$1" pin="DADJ" pad="7"/>
<connect gate="G$1" pin="DGND" pad="15"/>
<connect gate="G$1" pin="DV+" pad="16"/>
<connect gate="G$1" pin="FADJ" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="11"/>
<connect gate="G$1" pin="GND@4" pad="18"/>
<connect gate="G$1" pin="IIN" pad="10"/>
<connect gate="G$1" pin="OUT" pad="19"/>
<connect gate="G$1" pin="PDI" pad="13"/>
<connect gate="G$1" pin="PDO" pad="12"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SYNC" pad="14"/>
<connect gate="G$1" pin="V+" pad="17"/>
<connect gate="G$1" pin="V-" pad="20"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3965CEP" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX3965"/>
</gates>
<devices>
<device name="" package="QSOP20">
<connects>
<connect gate="G$1" pin="CZN" pad="12"/>
<connect gate="G$1" pin="CZP" pad="11"/>
<connect gate="G$1" pin="FILTER" pad="4"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GNDO" pad="18"/>
<connect gate="G$1" pin="IN+" pad="7"/>
<connect gate="G$1" pin="IN-" pad="6"/>
<connect gate="G$1" pin="INV" pad="3"/>
<connect gate="G$1" pin="LOS+" pad="17"/>
<connect gate="G$1" pin="LOS-" pad="16"/>
<connect gate="G$1" pin="OUT+" pad="14"/>
<connect gate="G$1" pin="OUT-" pad="15"/>
<connect gate="G$1" pin="RSSI" pad="5"/>
<connect gate="G$1" pin="SQUELCH" pad="1"/>
<connect gate="G$1" pin="SUB" pad="8"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VCC@1" pad="20"/>
<connect gate="G$1" pin="VCCO" pad="13"/>
<connect gate="G$1" pin="VTH" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6342" prefix="IC">
<description>&lt;b&gt;RESET CIRCUIT&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6342"/>
</gates>
<devices>
<device name="" package="SOT23-6L">
<connects>
<connect gate="G$1" pin="!MR" pad="5"/>
<connect gate="G$1" pin="!PFO" pad="4"/>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PFI" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX71*?" prefix="IC">
<description>NiCd/NiMH Battery Fast-Charge Controller</description>
<gates>
<gate name="G$1" symbol="MAX712"/>
</gates>
<devices>
<device name="PE" package="DIL16">
<connects>
<connect gate="G$1" pin="!FASTCHG" pad="8"/>
<connect gate="G$1" pin="BATT+" pad="2"/>
<connect gate="G$1" pin="BATT-" pad="12"/>
<connect gate="G$1" pin="CC" pad="11"/>
<connect gate="G$1" pin="DRV" pad="14"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="PGM0" pad="3"/>
<connect gate="G$1" pin="PGM1" pad="4"/>
<connect gate="G$1" pin="PGM2" pad="9"/>
<connect gate="G$1" pin="PGM3" pad="10"/>
<connect gate="G$1" pin="REF" pad="16"/>
<connect gate="G$1" pin="TEMP" pad="7"/>
<connect gate="G$1" pin="THI" pad="5"/>
<connect gate="G$1" pin="TLO" pad="6"/>
<connect gate="G$1" pin="V+" pad="15"/>
<connect gate="G$1" pin="VLIMIT" pad="1"/>
</connects>
<technologies>
<technology name="2C"/>
<technology name="2E"/>
<technology name="3C"/>
<technology name="3E"/>
</technologies>
</device>
<device name="SE" package="SO16">
<connects>
<connect gate="G$1" pin="!FASTCHG" pad="8"/>
<connect gate="G$1" pin="BATT+" pad="2"/>
<connect gate="G$1" pin="BATT-" pad="12"/>
<connect gate="G$1" pin="CC" pad="11"/>
<connect gate="G$1" pin="DRV" pad="14"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="PGM0" pad="3"/>
<connect gate="G$1" pin="PGM1" pad="4"/>
<connect gate="G$1" pin="PGM2" pad="9"/>
<connect gate="G$1" pin="PGM3" pad="10"/>
<connect gate="G$1" pin="REF" pad="16"/>
<connect gate="G$1" pin="TEMP" pad="7"/>
<connect gate="G$1" pin="THI" pad="5"/>
<connect gate="G$1" pin="TLO" pad="6"/>
<connect gate="G$1" pin="V+" pad="15"/>
<connect gate="G$1" pin="VLIMIT" pad="1"/>
</connects>
<technologies>
<technology name="2C"/>
<technology name="2E"/>
<technology name="3C"/>
<technology name="3E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS2890" prefix="IC">
<description>&lt;b&gt;1-Wire Digital Potentiometer&lt;/b&gt;&lt;p&gt;
DALLAS Semiconductor; &lt;p&gt;
http://www.maxim-ic.com/</description>
<gates>
<gate name="G$1" symbol="DS2890"/>
</gates>
<devices>
<device name="P" package="TSOC6">
<connects>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RH" pad="4"/>
<connect gate="G$1" pin="RL" pad="6"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="WIPER" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS2405" prefix="IC">
<description>&lt;b&gt;Addressable Switch&lt;/b&gt;&lt;p&gt;
DALLAS Semiconductor</description>
<gates>
<gate name="G$1" symbol="DS2405"/>
</gates>
<devices>
<device name="" package="TO92-">
<connects>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="PIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Z" package="SOT223">
<connects>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="PIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="TSOC6">
<connects>
<connect gate="G$1" pin="DATA" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="PIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4355" prefix="IC">
<description>&lt;b&gt;16x16 Nonblocking Video Crosspoint Switch&lt;/b&gt;&lt;p&gt;
with I/O Buffers</description>
<gates>
<gate name="G$1" symbol="MAX4355"/>
<gate name="G1" symbol="AGND"/>
<gate name="G2" symbol="AGND"/>
<gate name="G3" symbol="AGND"/>
<gate name="G4" symbol="AGND"/>
<gate name="G5" symbol="AGND"/>
<gate name="G6" symbol="AGND"/>
<gate name="G7" symbol="AGND"/>
<gate name="G8" symbol="AGND"/>
<gate name="G9" symbol="AGND"/>
<gate name="G10" symbol="AGND"/>
<gate name="G11" symbol="AGND"/>
<gate name="G12" symbol="AGND"/>
<gate name="G13" symbol="AGND"/>
<gate name="G14" symbol="AGND"/>
<gate name="G15" symbol="AGND"/>
<gate name="G16" symbol="AGND"/>
<gate name="G17" symbol="AGND"/>
<gate name="G18" symbol="DGND"/>
<gate name="G19" symbol="VCC"/>
<gate name="G20" symbol="VCC"/>
<gate name="G21" symbol="VCC"/>
<gate name="G22" symbol="VCC"/>
<gate name="G23" symbol="VCC"/>
<gate name="G24" symbol="VCC"/>
<gate name="G25" symbol="VCC"/>
<gate name="G26" symbol="VCC"/>
<gate name="G27" symbol="VCC"/>
<gate name="G28" symbol="VCC"/>
<gate name="V1" symbol="VEE"/>
<gate name="V2" symbol="VEE"/>
<gate name="V3" symbol="VEE"/>
<gate name="V4" symbol="VEE"/>
<gate name="V5" symbol="VEE"/>
<gate name="V6" symbol="VEE"/>
<gate name="V7" symbol="VEE"/>
<gate name="V8" symbol="VEE"/>
<gate name="N1" symbol="NC"/>
<gate name="N2" symbol="NC"/>
<gate name="N3" symbol="NC"/>
<gate name="N4" symbol="NC"/>
<gate name="N5" symbol="NC"/>
<gate name="N6" symbol="NC"/>
<gate name="N7" symbol="NC"/>
<gate name="N8" symbol="NC"/>
<gate name="N9" symbol="NC"/>
<gate name="N10" symbol="NC"/>
<gate name="N11" symbol="NC"/>
<gate name="N12" symbol="NC"/>
<gate name="N13" symbol="NC"/>
<gate name="N14" symbol="NC"/>
<gate name="N15" symbol="NC"/>
<gate name="N16" symbol="NC"/>
<gate name="N17" symbol="NC"/>
<gate name="N18" symbol="NC"/>
<gate name="V9" symbol="VEE"/>
<gate name="N19" symbol="VDD"/>
</gates>
<devices>
<device name="ECQ" package="TQFP100">
<connects>
<connect gate="G$1" pin="!AOUT" pad="30"/>
<connect gate="G$1" pin="!CE" pad="32"/>
<connect gate="G$1" pin="!RESET" pad="34"/>
<connect gate="G$1" pin="!UPDATE" pad="35"/>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="22"/>
<connect gate="G$1" pin="A2" pad="20"/>
<connect gate="G$1" pin="A3" pad="18"/>
<connect gate="G$1" pin="DIN" pad="36"/>
<connect gate="G$1" pin="DOUT" pad="28"/>
<connect gate="G$1" pin="IN0" pad="90"/>
<connect gate="G$1" pin="IN1" pad="92"/>
<connect gate="G$1" pin="IN10" pad="13"/>
<connect gate="G$1" pin="IN11" pad="15"/>
<connect gate="G$1" pin="IN12" pad="17"/>
<connect gate="G$1" pin="IN13" pad="19"/>
<connect gate="G$1" pin="IN14" pad="21"/>
<connect gate="G$1" pin="IN15" pad="23"/>
<connect gate="G$1" pin="IN2" pad="94"/>
<connect gate="G$1" pin="IN3" pad="96"/>
<connect gate="G$1" pin="IN4" pad="1"/>
<connect gate="G$1" pin="IN5" pad="3"/>
<connect gate="G$1" pin="IN6" pad="5"/>
<connect gate="G$1" pin="IN7" pad="7"/>
<connect gate="G$1" pin="IN8" pad="9"/>
<connect gate="G$1" pin="IN9" pad="11"/>
<connect gate="G$1" pin="MODE" pad="33"/>
<connect gate="G$1" pin="OUT0" pad="80"/>
<connect gate="G$1" pin="OUT1" pad="78"/>
<connect gate="G$1" pin="OUT10" pad="58"/>
<connect gate="G$1" pin="OUT11" pad="56"/>
<connect gate="G$1" pin="OUT12" pad="54"/>
<connect gate="G$1" pin="OUT13" pad="52"/>
<connect gate="G$1" pin="OUT14" pad="50"/>
<connect gate="G$1" pin="OUT15" pad="48"/>
<connect gate="G$1" pin="OUT2" pad="74"/>
<connect gate="G$1" pin="OUT3" pad="72"/>
<connect gate="G$1" pin="OUT4" pad="70"/>
<connect gate="G$1" pin="OUT5" pad="68"/>
<connect gate="G$1" pin="OUT6" pad="66"/>
<connect gate="G$1" pin="OUT7" pad="64"/>
<connect gate="G$1" pin="OUT8" pad="62"/>
<connect gate="G$1" pin="OUT9" pad="60"/>
<connect gate="G$1" pin="SCLK" pad="31"/>
<connect gate="G1" pin="AGND" pad="2"/>
<connect gate="G10" pin="AGND" pad="46"/>
<connect gate="G11" pin="AGND" pad="82"/>
<connect gate="G12" pin="AGND" pad="83"/>
<connect gate="G13" pin="AGND" pad="84"/>
<connect gate="G14" pin="AGND" pad="91"/>
<connect gate="G15" pin="AGND" pad="93"/>
<connect gate="G16" pin="AGND" pad="95"/>
<connect gate="G17" pin="AGND" pad="97"/>
<connect gate="G18" pin="DGND" pad="29"/>
<connect gate="G19" pin="VCC" pad="25"/>
<connect gate="G2" pin="AGND" pad="4"/>
<connect gate="G20" pin="VCC" pad="47"/>
<connect gate="G21" pin="VCC" pad="51"/>
<connect gate="G22" pin="VCC" pad="55"/>
<connect gate="G23" pin="VCC" pad="59"/>
<connect gate="G24" pin="VCC" pad="63"/>
<connect gate="G25" pin="VCC" pad="67"/>
<connect gate="G26" pin="VCC" pad="71"/>
<connect gate="G27" pin="VCC" pad="75"/>
<connect gate="G28" pin="VCC" pad="81"/>
<connect gate="G3" pin="AGND" pad="6"/>
<connect gate="G4" pin="AGND" pad="8"/>
<connect gate="G5" pin="AGND" pad="10"/>
<connect gate="G6" pin="AGND" pad="12"/>
<connect gate="G7" pin="AGND" pad="14"/>
<connect gate="G8" pin="AGND" pad="16"/>
<connect gate="G9" pin="AGND" pad="45"/>
<connect gate="N1" pin="NC" pad="26"/>
<connect gate="N10" pin="NC" pad="76"/>
<connect gate="N11" pin="NC" pad="77"/>
<connect gate="N12" pin="NC" pad="85"/>
<connect gate="N13" pin="NC" pad="86"/>
<connect gate="N14" pin="NC" pad="87"/>
<connect gate="N15" pin="NC" pad="88"/>
<connect gate="N16" pin="NC" pad="89"/>
<connect gate="N17" pin="NC" pad="99"/>
<connect gate="N18" pin="NC" pad="100"/>
<connect gate="N19" pin="VDD" pad="37"/>
<connect gate="N2" pin="NC" pad="27"/>
<connect gate="N3" pin="NC" pad="38"/>
<connect gate="N4" pin="NC" pad="39"/>
<connect gate="N5" pin="NC" pad="40"/>
<connect gate="N6" pin="NC" pad="41"/>
<connect gate="N7" pin="NC" pad="42"/>
<connect gate="N8" pin="NC" pad="43"/>
<connect gate="N9" pin="NC" pad="44"/>
<connect gate="V1" pin="VEE" pad="49"/>
<connect gate="V2" pin="VEE" pad="53"/>
<connect gate="V3" pin="VEE" pad="57"/>
<connect gate="V4" pin="VEE" pad="61"/>
<connect gate="V5" pin="VEE" pad="65"/>
<connect gate="V6" pin="VEE" pad="69"/>
<connect gate="V7" pin="VEE" pad="73"/>
<connect gate="V8" pin="VEE" pad="79"/>
<connect gate="V9" pin="VEE" pad="98"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4313" prefix="IC">
<description>&lt;b&gt;Video Multiplexer-Amplifier&lt;/b&gt;&lt;p&gt;
High-Speed, Low-Power, Single-Supply, Multichannel</description>
<gates>
<gate name="N1" symbol="MAX4313"/>
</gates>
<devices>
<device name="EUA" package="UMAX8">
<connects>
<connect gate="N1" pin="!SHDN" pad="2"/>
<connect gate="N1" pin="A0" pad="1"/>
<connect gate="N1" pin="GND" pad="7"/>
<connect gate="N1" pin="IN0" pad="4"/>
<connect gate="N1" pin="IN1" pad="5"/>
<connect gate="N1" pin="OUT" pad="8"/>
<connect gate="N1" pin="V+" pad="3"/>
<connect gate="N1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ESA" package="SO08">
<connects>
<connect gate="N1" pin="!SHDN" pad="2"/>
<connect gate="N1" pin="A0" pad="1"/>
<connect gate="N1" pin="GND" pad="7"/>
<connect gate="N1" pin="IN0" pad="4"/>
<connect gate="N1" pin="IN1" pad="5"/>
<connect gate="N1" pin="OUT" pad="8"/>
<connect gate="N1" pin="V+" pad="3"/>
<connect gate="N1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4310" prefix="IC">
<description>&lt;b&gt;Video Multiplexer-Amplifier&lt;/b&gt;&lt;p&gt;
High-Speed, Low-Power, Single-Supply, Multichannel</description>
<gates>
<gate name="N1" symbol="MAX4310"/>
</gates>
<devices>
<device name="ESA" package="UMAX8">
<connects>
<connect gate="N1" pin="!SHDN" pad="2"/>
<connect gate="N1" pin="A0" pad="1"/>
<connect gate="N1" pin="FB" pad="7"/>
<connect gate="N1" pin="IN0" pad="4"/>
<connect gate="N1" pin="IN1" pad="5"/>
<connect gate="N1" pin="OUT" pad="8"/>
<connect gate="N1" pin="V+" pad="3"/>
<connect gate="N1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EUA" package="SO08">
<connects>
<connect gate="N1" pin="!SHDN" pad="2"/>
<connect gate="N1" pin="A0" pad="1"/>
<connect gate="N1" pin="FB" pad="7"/>
<connect gate="N1" pin="IN0" pad="4"/>
<connect gate="N1" pin="IN1" pad="5"/>
<connect gate="N1" pin="OUT" pad="8"/>
<connect gate="N1" pin="V+" pad="3"/>
<connect gate="N1" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4311" prefix="IC">
<description>&lt;b&gt;Video Multiplexer-Amplifier&lt;/b&gt;&lt;p&gt;
High-Speed, Low-Power, Single-Supply, Multichannel</description>
<gates>
<gate name="N1" symbol="MAX4311"/>
</gates>
<devices>
<device name="ESD" package="SO14">
<connects>
<connect gate="N1" pin="!SHDN" pad="12"/>
<connect gate="N1" pin="A0" pad="2"/>
<connect gate="N1" pin="A1" pad="1"/>
<connect gate="N1" pin="FB" pad="13"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="7"/>
<connect gate="N1" pin="IN2" pad="8"/>
<connect gate="N1" pin="IN3" pad="10"/>
<connect gate="N1" pin="OUT" pad="14"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EEE" package="QSOP16">
<connects>
<connect gate="N1" pin="!SHDN" pad="14"/>
<connect gate="N1" pin="A0" pad="2"/>
<connect gate="N1" pin="A1" pad="1"/>
<connect gate="N1" pin="FB" pad="15"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="7"/>
<connect gate="N1" pin="IN2" pad="10"/>
<connect gate="N1" pin="IN3" pad="12"/>
<connect gate="N1" pin="OUT" pad="16"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4312" prefix="IC">
<description>&lt;b&gt;Video Multiplexer-Amplifier&lt;/b&gt;&lt;p&gt;
High-Speed, Low-Power, Single-Supply, Multichannel</description>
<gates>
<gate name="N1" symbol="MAX4312"/>
</gates>
<devices>
<device name="ESE" package="SO16">
<connects>
<connect gate="N1" pin="!SHDN" pad="14"/>
<connect gate="N1" pin="A0" pad="3"/>
<connect gate="N1" pin="A1" pad="2"/>
<connect gate="N1" pin="A2" pad="1"/>
<connect gate="N1" pin="FB" pad="15"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="6"/>
<connect gate="N1" pin="IN2" pad="7"/>
<connect gate="N1" pin="IN3" pad="8"/>
<connect gate="N1" pin="IN4" pad="9"/>
<connect gate="N1" pin="IN5" pad="10"/>
<connect gate="N1" pin="IN6" pad="11"/>
<connect gate="N1" pin="IN7" pad="12"/>
<connect gate="N1" pin="OUT" pad="16"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EEE" package="QSOP16">
<connects>
<connect gate="N1" pin="!SHDN" pad="14"/>
<connect gate="N1" pin="A0" pad="3"/>
<connect gate="N1" pin="A1" pad="2"/>
<connect gate="N1" pin="A2" pad="1"/>
<connect gate="N1" pin="FB" pad="15"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="6"/>
<connect gate="N1" pin="IN2" pad="7"/>
<connect gate="N1" pin="IN3" pad="8"/>
<connect gate="N1" pin="IN4" pad="9"/>
<connect gate="N1" pin="IN5" pad="10"/>
<connect gate="N1" pin="IN6" pad="11"/>
<connect gate="N1" pin="IN7" pad="12"/>
<connect gate="N1" pin="OUT" pad="16"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4314" prefix="IC">
<description>&lt;b&gt;Video Multiplexer-Amplifier&lt;/b&gt;&lt;p&gt;
High-Speed, Low-Power, Single-Supply, Multichannel</description>
<gates>
<gate name="N1" symbol="MAX4314"/>
</gates>
<devices>
<device name="ESD" package="SO14">
<connects>
<connect gate="N1" pin="!SHDN" pad="12"/>
<connect gate="N1" pin="A0" pad="3"/>
<connect gate="N1" pin="A1" pad="2"/>
<connect gate="N1" pin="A2" pad="1"/>
<connect gate="N1" pin="GND" pad="13"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="7"/>
<connect gate="N1" pin="IN2" pad="8"/>
<connect gate="N1" pin="IN3" pad="10"/>
<connect gate="N1" pin="OUT" pad="14"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EEE" package="QSOP16">
<connects>
<connect gate="N1" pin="!SHDN" pad="14"/>
<connect gate="N1" pin="A0" pad="3"/>
<connect gate="N1" pin="A1" pad="2"/>
<connect gate="N1" pin="A2" pad="1"/>
<connect gate="N1" pin="GND" pad="15"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="7"/>
<connect gate="N1" pin="IN2" pad="10"/>
<connect gate="N1" pin="IN3" pad="12"/>
<connect gate="N1" pin="OUT" pad="16"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4315" prefix="IC">
<description>&lt;b&gt;Video Multiplexer-Amplifier&lt;/b&gt;&lt;p&gt;
High-Speed, Low-Power, Single-Supply, Multichannel</description>
<gates>
<gate name="N1" symbol="MAX4315"/>
</gates>
<devices>
<device name="ESE" package="SO16">
<connects>
<connect gate="N1" pin="!SHDN" pad="14"/>
<connect gate="N1" pin="A0" pad="3"/>
<connect gate="N1" pin="A1" pad="2"/>
<connect gate="N1" pin="A2" pad="1"/>
<connect gate="N1" pin="GND" pad="15"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="6"/>
<connect gate="N1" pin="IN2" pad="7"/>
<connect gate="N1" pin="IN3" pad="8"/>
<connect gate="N1" pin="IN4" pad="9"/>
<connect gate="N1" pin="IN5" pad="10"/>
<connect gate="N1" pin="IN6" pad="11"/>
<connect gate="N1" pin="IN7" pad="12"/>
<connect gate="N1" pin="OUT" pad="16"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EEE" package="QSOP16">
<connects>
<connect gate="N1" pin="!SHDN" pad="14"/>
<connect gate="N1" pin="A0" pad="3"/>
<connect gate="N1" pin="A1" pad="2"/>
<connect gate="N1" pin="A2" pad="1"/>
<connect gate="N1" pin="GND" pad="15"/>
<connect gate="N1" pin="IN0" pad="5"/>
<connect gate="N1" pin="IN1" pad="6"/>
<connect gate="N1" pin="IN2" pad="7"/>
<connect gate="N1" pin="IN3" pad="8"/>
<connect gate="N1" pin="IN4" pad="9"/>
<connect gate="N1" pin="IN5" pad="10"/>
<connect gate="N1" pin="IN6" pad="11"/>
<connect gate="N1" pin="IN7" pad="12"/>
<connect gate="N1" pin="OUT" pad="16"/>
<connect gate="N1" pin="V+" pad="4"/>
<connect gate="N1" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3221*" prefix="IC">
<description>&lt;b&gt;RS-232 Transceivers with AutoShutdown&lt;/b&gt;&lt;p&gt;
1µA Supply-Current, True +3V to +5.5V &lt;br&gt;
http://dbserv.maxim-ic.com/</description>
<gates>
<gate name="G$1" symbol="MAX3221"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="AE" package="SSOP16">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="!FORCEOFF" pad="16"/>
<connect gate="G$1" pin="!INVALID" pad="10"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="FORCEON" pad="12"/>
<connect gate="G$1" pin="R1IN" pad="8"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="13"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="UE" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="!FORCEOFF" pad="16"/>
<connect gate="G$1" pin="!INVALID" pad="10"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="FORCEON" pad="12"/>
<connect gate="G$1" pin="R1IN" pad="8"/>
<connect gate="G$1" pin="R1OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="13"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3223*" prefix="IC">
<description>&lt;b&gt;RS-232 Transceivers with AutoShutdown&lt;/b&gt;&lt;p&gt;
1µA Supply-Current, True +3V to +5.5V&lt;br&gt;
http://dbserv.maxim-ic.com/</description>
<gates>
<gate name="G$1" symbol="MAX3223"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="PP" package="DIL20">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="!FORCEOFF" pad="20"/>
<connect gate="G$1" pin="!INVALID" pad="11"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="FORCEON" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="16"/>
<connect gate="G$1" pin="R1OUT" pad="15"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="13"/>
<connect gate="G$1" pin="T1OUT" pad="17"/>
<connect gate="G$1" pin="T2IN" pad="12"/>
<connect gate="G$1" pin="T2OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="P" pin="GND" pad="18"/>
<connect gate="P" pin="VCC" pad="19"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="AP" package="SSOP20">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="!FORCEOFF" pad="20"/>
<connect gate="G$1" pin="!INVALID" pad="11"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="FORCEON" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="16"/>
<connect gate="G$1" pin="R1OUT" pad="15"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="13"/>
<connect gate="G$1" pin="T1OUT" pad="17"/>
<connect gate="G$1" pin="T2IN" pad="12"/>
<connect gate="G$1" pin="T2OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="P" pin="GND" pad="18"/>
<connect gate="P" pin="VCC" pad="19"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="UP" package="TSSOP20">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="!FORCEOFF" pad="20"/>
<connect gate="G$1" pin="!INVALID" pad="11"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="FORCEON" pad="14"/>
<connect gate="G$1" pin="R1IN" pad="16"/>
<connect gate="G$1" pin="R1OUT" pad="15"/>
<connect gate="G$1" pin="R2IN" pad="9"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="13"/>
<connect gate="G$1" pin="T1OUT" pad="17"/>
<connect gate="G$1" pin="T2IN" pad="12"/>
<connect gate="G$1" pin="T2OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="P" pin="GND" pad="18"/>
<connect gate="P" pin="VCC" pad="19"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3243*" prefix="IC">
<description>&lt;b&gt;RS-232 Transceivers with AutoShutdown&lt;/b&gt;&lt;p&gt;
1µA Supply-Current, True +3V to +5.5V&lt;br&gt;
http://dbserv.maxim-ic.com/</description>
<gates>
<gate name="G$1" symbol="MAX3243"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="AI" package="SSOP28">
<connects>
<connect gate="G$1" pin="!FORCEOFF" pad="22"/>
<connect gate="G$1" pin="!INVALID" pad="21"/>
<connect gate="G$1" pin="C1+" pad="28"/>
<connect gate="G$1" pin="C1-" pad="24"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="FORCEON" pad="23"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="19"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="18"/>
<connect gate="G$1" pin="R2OUTB" pad="20"/>
<connect gate="G$1" pin="R3IN" pad="6"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="R4IN" pad="7"/>
<connect gate="G$1" pin="R4OUT" pad="16"/>
<connect gate="G$1" pin="R5IN" pad="8"/>
<connect gate="G$1" pin="R5OUT" pad="15"/>
<connect gate="G$1" pin="T1IN" pad="14"/>
<connect gate="G$1" pin="T1OUT" pad="9"/>
<connect gate="G$1" pin="T2IN" pad="13"/>
<connect gate="G$1" pin="T2OUT" pad="10"/>
<connect gate="G$1" pin="T3IN" pad="12"/>
<connect gate="G$1" pin="T3OUT" pad="11"/>
<connect gate="G$1" pin="V+" pad="27"/>
<connect gate="G$1" pin="V-" pad="3"/>
<connect gate="P" pin="GND" pad="25"/>
<connect gate="P" pin="VCC" pad="26"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="UI" package="TSSOP28">
<connects>
<connect gate="G$1" pin="!FORCEOFF" pad="22"/>
<connect gate="G$1" pin="!INVALID" pad="21"/>
<connect gate="G$1" pin="C1+" pad="28"/>
<connect gate="G$1" pin="C1-" pad="24"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="FORCEON" pad="23"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="19"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="18"/>
<connect gate="G$1" pin="R2OUTB" pad="20"/>
<connect gate="G$1" pin="R3IN" pad="6"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="R4IN" pad="7"/>
<connect gate="G$1" pin="R4OUT" pad="16"/>
<connect gate="G$1" pin="R5IN" pad="8"/>
<connect gate="G$1" pin="R5OUT" pad="15"/>
<connect gate="G$1" pin="T1IN" pad="14"/>
<connect gate="G$1" pin="T1OUT" pad="9"/>
<connect gate="G$1" pin="T2IN" pad="13"/>
<connect gate="G$1" pin="T2OUT" pad="10"/>
<connect gate="G$1" pin="T3IN" pad="12"/>
<connect gate="G$1" pin="T3OUT" pad="11"/>
<connect gate="G$1" pin="V+" pad="27"/>
<connect gate="G$1" pin="V-" pad="3"/>
<connect gate="P" pin="GND" pad="25"/>
<connect gate="P" pin="VCC" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WI" package="SO28L">
<connects>
<connect gate="G$1" pin="!FORCEOFF" pad="22"/>
<connect gate="G$1" pin="!INVALID" pad="21"/>
<connect gate="G$1" pin="C1+" pad="28"/>
<connect gate="G$1" pin="C1-" pad="24"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="FORCEON" pad="23"/>
<connect gate="G$1" pin="R1IN" pad="4"/>
<connect gate="G$1" pin="R1OUT" pad="19"/>
<connect gate="G$1" pin="R2IN" pad="5"/>
<connect gate="G$1" pin="R2OUT" pad="18"/>
<connect gate="G$1" pin="R2OUTB" pad="20"/>
<connect gate="G$1" pin="R3IN" pad="6"/>
<connect gate="G$1" pin="R3OUT" pad="17"/>
<connect gate="G$1" pin="R4IN" pad="7"/>
<connect gate="G$1" pin="R4OUT" pad="16"/>
<connect gate="G$1" pin="R5IN" pad="8"/>
<connect gate="G$1" pin="R5OUT" pad="15"/>
<connect gate="G$1" pin="T1IN" pad="14"/>
<connect gate="G$1" pin="T1OUT" pad="9"/>
<connect gate="G$1" pin="T2IN" pad="13"/>
<connect gate="G$1" pin="T2OUT" pad="10"/>
<connect gate="G$1" pin="T3IN" pad="12"/>
<connect gate="G$1" pin="T3OUT" pad="11"/>
<connect gate="G$1" pin="V+" pad="27"/>
<connect gate="G$1" pin="V-" pad="3"/>
<connect gate="P" pin="GND" pad="25"/>
<connect gate="P" pin="VCC" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3232*" prefix="IC">
<description>&lt;b&gt;True RS-232 Transceivers&lt;/b&gt; 3.0V to 5.5V, Low-Power&lt;p&gt;
up to 1Mbps,  Using Four 0.1µF External Capacitors&lt;br&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX3222-MAX3241.pdf</description>
<gates>
<gate name="G$1" symbol="MAX232"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="PE" package="DIL16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="UE" package="TSSOP16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="WE" package="SO16L">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="SE" package="SO16">
<connects>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="R1IN" pad="13"/>
<connect gate="G$1" pin="R1OUT" pad="12"/>
<connect gate="G$1" pin="R2IN" pad="8"/>
<connect gate="G$1" pin="R2OUT" pad="9"/>
<connect gate="G$1" pin="T1IN" pad="11"/>
<connect gate="G$1" pin="T1OUT" pad="14"/>
<connect gate="G$1" pin="T2IN" pad="10"/>
<connect gate="G$1" pin="T2OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1150*" prefix="IC">
<description>&lt;b&gt;8-Bit, 500Msps Flash ADC&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX1150.pdf</description>
<gates>
<gate name="G$1" symbol="MAX1150"/>
<gate name="P" symbol="MAX1150-P"/>
</gates>
<devices>
<device name="" package="MQFP80-2">
<connects>
<connect gate="G$1" pin="AGND" pad="15"/>
<connect gate="G$1" pin="CLK" pad="48"/>
<connect gate="G$1" pin="D0A" pad="57"/>
<connect gate="G$1" pin="D0B" pad="78"/>
<connect gate="G$1" pin="D1A" pad="59"/>
<connect gate="G$1" pin="D1B" pad="80"/>
<connect gate="G$1" pin="D2A" pad="61"/>
<connect gate="G$1" pin="D2B" pad="1"/>
<connect gate="G$1" pin="D3A" pad="62"/>
<connect gate="G$1" pin="D3B" pad="2"/>
<connect gate="G$1" pin="D4A" pad="65"/>
<connect gate="G$1" pin="D4B" pad="3"/>
<connect gate="G$1" pin="D5A" pad="66"/>
<connect gate="G$1" pin="D5B" pad="6"/>
<connect gate="G$1" pin="D6A" pad="68"/>
<connect gate="G$1" pin="D6B" pad="8"/>
<connect gate="G$1" pin="D7A" pad="70"/>
<connect gate="G$1" pin="D7B" pad="10"/>
<connect gate="G$1" pin="D8A" pad="72"/>
<connect gate="G$1" pin="D8B" pad="12"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DRA" pad="53"/>
<connect gate="G$1" pin="DRB" pad="76"/>
<connect gate="G$1" pin="NCLK" pad="50"/>
<connect gate="G$1" pin="NDRA" pad="55"/>
<connect gate="G$1" pin="NDRB" pad="74"/>
<connect gate="G$1" pin="VEE" pad="4"/>
<connect gate="G$1" pin="VIN" pad="32"/>
<connect gate="G$1" pin="VIN@1" pad="33"/>
<connect gate="G$1" pin="VRBF" pad="21"/>
<connect gate="G$1" pin="VRBS" pad="24"/>
<connect gate="G$1" pin="VRM" pad="35"/>
<connect gate="G$1" pin="VRTF" pad="42"/>
<connect gate="G$1" pin="VRTS" pad="43"/>
<connect gate="P" pin="AGND@1" pad="16"/>
<connect gate="P" pin="AGND@10" pad="44"/>
<connect gate="P" pin="AGND@11" pad="45"/>
<connect gate="P" pin="AGND@12" pad="51"/>
<connect gate="P" pin="AGND@13" pad="52"/>
<connect gate="P" pin="AGND@2" pad="17"/>
<connect gate="P" pin="AGND@3" pad="18"/>
<connect gate="P" pin="AGND@4" pad="25"/>
<connect gate="P" pin="AGND@5" pad="26"/>
<connect gate="P" pin="AGND@6" pad="29"/>
<connect gate="P" pin="AGND@7" pad="30"/>
<connect gate="P" pin="AGND@8" pad="36"/>
<connect gate="P" pin="AGND@9" pad="37"/>
<connect gate="P" pin="DGND@1" pad="9"/>
<connect gate="P" pin="DGND@10" pad="77"/>
<connect gate="P" pin="DGND@2" pad="11"/>
<connect gate="P" pin="DGND@3" pad="54"/>
<connect gate="P" pin="DGND@4" pad="56"/>
<connect gate="P" pin="DGND@5" pad="69"/>
<connect gate="P" pin="DGND@6" pad="71"/>
<connect gate="P" pin="DGND@7" pad="58"/>
<connect gate="P" pin="DGND@8" pad="73"/>
<connect gate="P" pin="DGND@9" pad="75"/>
<connect gate="P" pin="NC@1" pad="13"/>
<connect gate="P" pin="NC@2" pad="14"/>
<connect gate="P" pin="NC@3" pad="31"/>
<connect gate="P" pin="NC@4" pad="34"/>
<connect gate="P" pin="NC@5" pad="41"/>
<connect gate="P" pin="NC@6" pad="63"/>
<connect gate="P" pin="NC@7" pad="64"/>
<connect gate="P" pin="VEE@1" pad="5"/>
<connect gate="P" pin="VEE@10" pad="40"/>
<connect gate="P" pin="VEE@11" pad="46"/>
<connect gate="P" pin="VEE@12" pad="47"/>
<connect gate="P" pin="VEE@13" pad="49"/>
<connect gate="P" pin="VEE@14" pad="60"/>
<connect gate="P" pin="VEE@15" pad="67"/>
<connect gate="P" pin="VEE@16" pad="79"/>
<connect gate="P" pin="VEE@2" pad="19"/>
<connect gate="P" pin="VEE@3" pad="20"/>
<connect gate="P" pin="VEE@4" pad="22"/>
<connect gate="P" pin="VEE@5" pad="23"/>
<connect gate="P" pin="VEE@6" pad="27"/>
<connect gate="P" pin="VEE@7" pad="28"/>
<connect gate="P" pin="VEE@8" pad="38"/>
<connect gate="P" pin="VEE@9" pad="39"/>
</connects>
<technologies>
<technology name="AIZS"/>
<technology name="BIZS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX346*" prefix="IC">
<description>&lt;b&gt;+5V, Fail-Safe, 40Mbps, Profibus RS-485/RS-422 Transceivers&lt;/b&gt;&lt;p&gt;
Source: MAX3465-MAX3469.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3465"/>
</gates>
<devices>
<device name="PD" package="DIL14">
<connects>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="RE/" pad="3"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="RXP" pad="13"/>
<connect gate="G$1" pin="SHDN" pad="1"/>
<connect gate="G$1" pin="TXP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name="5C"/>
<technology name="5E"/>
<technology name="6C"/>
<technology name="6E"/>
</technologies>
</device>
<device name="SD" package="SO14">
<connects>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="DE" pad="4"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="RE/" pad="3"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="RXP" pad="13"/>
<connect gate="G$1" pin="SHDN" pad="1"/>
<connect gate="G$1" pin="TXP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="Y" pad="9"/>
<connect gate="G$1" pin="Z" pad="10"/>
</connects>
<technologies>
<technology name="5C"/>
<technology name="5E"/>
<technology name="6C"/>
<technology name="6E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3467*" prefix="IC">
<description>&lt;b&gt;+5V, Fail-Safe, 40Mbps, Profibus RS-485/RS-422 Transceivers&lt;/b&gt;&lt;p&gt;
Source: MAX3465-MAX3469.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3467"/>
</gates>
<devices>
<device name="SA" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Z" pad="6"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="PA" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="8"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Z" pad="6"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX34*" prefix="IC">
<description>&lt;b&gt;+5V, Fail-Safe, 40Mbps, Profibus RS-485/RS-422 Transceivers&lt;/b&gt;&lt;p&gt;
Source: MAX3465-MAX3469.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3468"/>
</gates>
<devices>
<device name="PA" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RE/" pad="2"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="68C"/>
<technology name="68E"/>
<technology name="69C"/>
<technology name="69E"/>
</technologies>
</device>
<device name="SA" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RE/" pad="2"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="68C"/>
<technology name="68E"/>
<technology name="69C"/>
<technology name="69E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX304*" prefix="IC">
<description>&lt;b&gt;±10kV ESD-Protected, Quad 5V RS-485/422 Transmitters&lt;/b&gt;&lt;p&gt;
Source: MAX3040-MAX3045.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3043"/>
</gates>
<devices>
<device name="SE" package="SO16">
<connects>
<connect gate="G$1" pin="!EB" pad="12"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="T1IN" pad="1"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="G$1" pin="Y3" pad="10"/>
<connect gate="G$1" pin="Y4" pad="14"/>
<connect gate="G$1" pin="Z1" pad="3"/>
<connect gate="G$1" pin="Z2" pad="5"/>
<connect gate="G$1" pin="Z3" pad="11"/>
<connect gate="G$1" pin="Z4" pad="13"/>
</connects>
<technologies>
<technology name="3C"/>
<technology name="3E"/>
<technology name="4C"/>
<technology name="4E"/>
<technology name="5BC"/>
<technology name="5BE"/>
</technologies>
</device>
<device name="WE" package="SO16L">
<connects>
<connect gate="G$1" pin="!EB" pad="12"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="T1IN" pad="1"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="G$1" pin="Y3" pad="10"/>
<connect gate="G$1" pin="Y4" pad="14"/>
<connect gate="G$1" pin="Z1" pad="3"/>
<connect gate="G$1" pin="Z2" pad="5"/>
<connect gate="G$1" pin="Z3" pad="11"/>
<connect gate="G$1" pin="Z4" pad="13"/>
</connects>
<technologies>
<technology name="3C"/>
<technology name="3E"/>
<technology name="4C"/>
<technology name="4E"/>
<technology name="5BC"/>
<technology name="5BE"/>
</technologies>
</device>
<device name="UE" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!EB" pad="12"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="T1IN" pad="1"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="G$1" pin="Y3" pad="10"/>
<connect gate="G$1" pin="Y4" pad="14"/>
<connect gate="G$1" pin="Z1" pad="3"/>
<connect gate="G$1" pin="Z2" pad="5"/>
<connect gate="G$1" pin="Z3" pad="11"/>
<connect gate="G$1" pin="Z4" pad="13"/>
</connects>
<technologies>
<technology name="3C"/>
<technology name="3E"/>
<technology name="4C"/>
<technology name="4E"/>
<technology name="5BC"/>
<technology name="5BE"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX30*" prefix="IC">
<description>&lt;b&gt;±10kV ESD-Protected, Quad 5V RS-485/RS-422 Transmitters&lt;/b&gt;&lt;p&gt;
Source: www.maxim-ic.com .. MAX3040-MAX3045.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3040"/>
</gates>
<devices>
<device name="UE" package="TSSOP16">
<connects>
<connect gate="G$1" pin="EN12" pad="4"/>
<connect gate="G$1" pin="EN34" pad="12"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="T1IN" pad="1"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="G$1" pin="Y3" pad="10"/>
<connect gate="G$1" pin="Y4" pad="14"/>
<connect gate="G$1" pin="Z1" pad="3"/>
<connect gate="G$1" pin="Z2" pad="5"/>
<connect gate="G$1" pin="Z3" pad="11"/>
<connect gate="G$1" pin="Z4" pad="13"/>
</connects>
<technologies>
<technology name="40C"/>
<technology name="40E"/>
<technology name="41C"/>
<technology name="41E"/>
<technology name="42BC"/>
<technology name="42BE"/>
</technologies>
</device>
<device name="SE" package="SO16">
<connects>
<connect gate="G$1" pin="EN12" pad="4"/>
<connect gate="G$1" pin="EN34" pad="12"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="T1IN" pad="1"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="G$1" pin="Y3" pad="10"/>
<connect gate="G$1" pin="Y4" pad="14"/>
<connect gate="G$1" pin="Z1" pad="3"/>
<connect gate="G$1" pin="Z2" pad="5"/>
<connect gate="G$1" pin="Z3" pad="11"/>
<connect gate="G$1" pin="Z4" pad="13"/>
</connects>
<technologies>
<technology name="40C"/>
<technology name="40E"/>
<technology name="41C"/>
<technology name="41E"/>
<technology name="42BC"/>
<technology name="42BE"/>
</technologies>
</device>
<device name="WE" package="SO16L">
<connects>
<connect gate="G$1" pin="EN12" pad="4"/>
<connect gate="G$1" pin="EN34" pad="12"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="T1IN" pad="1"/>
<connect gate="G$1" pin="T2IN" pad="7"/>
<connect gate="G$1" pin="T3IN" pad="9"/>
<connect gate="G$1" pin="T4IN" pad="15"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="2"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="G$1" pin="Y3" pad="10"/>
<connect gate="G$1" pin="Y4" pad="14"/>
<connect gate="G$1" pin="Z1" pad="3"/>
<connect gate="G$1" pin="Z2" pad="5"/>
<connect gate="G$1" pin="Z3" pad="11"/>
<connect gate="G$1" pin="Z4" pad="13"/>
</connects>
<technologies>
<technology name="40C"/>
<technology name="40E"/>
<technology name="41C"/>
<technology name="41E"/>
<technology name="42BC"/>
<technology name="42BE"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX309*" prefix="IC">
<description>&lt;b&gt;±15kV ESD-Protected, 10Mbps, 3V/5V, Quad RS-422/RS-485 Receivers&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX3095-MAX3096.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3095"/>
</gates>
<devices>
<device name="PE" package="DIL16">
<connects>
<connect gate="G$1" pin="!G" pad="12"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="A4" pad="14"/>
<connect gate="G$1" pin="B1" pad="1"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="B4" pad="15"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="3"/>
<connect gate="G$1" pin="Y2" pad="5"/>
<connect gate="G$1" pin="Y3" pad="11"/>
<connect gate="G$1" pin="Y4" pad="13"/>
</connects>
<technologies>
<technology name="5C"/>
<technology name="5E"/>
<technology name="6C"/>
<technology name="6E"/>
</technologies>
</device>
<device name="SE" package="SO16">
<connects>
<connect gate="G$1" pin="!G" pad="12"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="A4" pad="14"/>
<connect gate="G$1" pin="B1" pad="1"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="B4" pad="15"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="3"/>
<connect gate="G$1" pin="Y2" pad="5"/>
<connect gate="G$1" pin="Y3" pad="11"/>
<connect gate="G$1" pin="Y4" pad="13"/>
</connects>
<technologies>
<technology name="5C"/>
<technology name="5E"/>
<technology name="6C"/>
<technology name="6E"/>
</technologies>
</device>
<device name="EE" package="QSOP16">
<connects>
<connect gate="G$1" pin="!G" pad="12"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="A4" pad="14"/>
<connect gate="G$1" pin="B1" pad="1"/>
<connect gate="G$1" pin="B2" pad="7"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="B4" pad="15"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y1" pad="3"/>
<connect gate="G$1" pin="Y2" pad="5"/>
<connect gate="G$1" pin="Y3" pad="11"/>
<connect gate="G$1" pin="Y4" pad="13"/>
</connects>
<technologies>
<technology name="5C"/>
<technology name="5E"/>
<technology name="6C"/>
<technology name="6E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX12527" prefix="IC">
<description>&lt;b&gt;Dual, 65Msps, 12-Bit, IF/Baseband ADC&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX12527.pdf</description>
<gates>
<gate name="G$1" symbol="MAX12527"/>
</gates>
<devices>
<device name="" package="68LQFN">
<connects>
<connect gate="G$1" pin="CLKN" pad="19"/>
<connect gate="G$1" pin="CLKP" pad="20"/>
<connect gate="G$1" pin="COMA" pad="6"/>
<connect gate="G$1" pin="COMB" pad="12"/>
<connect gate="G$1" pin="D0A" pad="47"/>
<connect gate="G$1" pin="D0B" pad="30"/>
<connect gate="G$1" pin="D10A" pad="57"/>
<connect gate="G$1" pin="D10B" pad="40"/>
<connect gate="G$1" pin="D11A" pad="58"/>
<connect gate="G$1" pin="D11B" pad="41"/>
<connect gate="G$1" pin="D1A" pad="48"/>
<connect gate="G$1" pin="D1B" pad="31"/>
<connect gate="G$1" pin="D2A" pad="49"/>
<connect gate="G$1" pin="D2B" pad="32"/>
<connect gate="G$1" pin="D3A" pad="50"/>
<connect gate="G$1" pin="D3B" pad="33"/>
<connect gate="G$1" pin="D4A" pad="51"/>
<connect gate="G$1" pin="D4B" pad="34"/>
<connect gate="G$1" pin="D5A" pad="52"/>
<connect gate="G$1" pin="D5B" pad="35"/>
<connect gate="G$1" pin="D6A" pad="53"/>
<connect gate="G$1" pin="D6B" pad="36"/>
<connect gate="G$1" pin="D7A" pad="54"/>
<connect gate="G$1" pin="D7B" pad="37"/>
<connect gate="G$1" pin="D8A" pad="55"/>
<connect gate="G$1" pin="D8B" pad="38"/>
<connect gate="G$1" pin="D9A" pad="56"/>
<connect gate="G$1" pin="D9B" pad="39"/>
<connect gate="G$1" pin="DAV" pad="44"/>
<connect gate="G$1" pin="DIFFCLK/!SECLK" pad="18"/>
<connect gate="G$1" pin="DIV2" pad="21"/>
<connect gate="G$1" pin="DIV4" pad="22"/>
<connect gate="G$1" pin="DORA" pad="59"/>
<connect gate="G$1" pin="DORB" pad="42"/>
<connect gate="G$1" pin="G/!T" pad="64"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="13"/>
<connect gate="G$1" pin="GND@5" pad="14"/>
<connect gate="G$1" pin="GND@6" pad="17"/>
<connect gate="G$1" pin="INAN" pad="3"/>
<connect gate="G$1" pin="INAP" pad="2"/>
<connect gate="G$1" pin="INBN" pad="15"/>
<connect gate="G$1" pin="INBP" pad="16"/>
<connect gate="G$1" pin="OVDD" pad="27"/>
<connect gate="G$1" pin="OVDD@1" pad="43"/>
<connect gate="G$1" pin="OVDD@2" pad="60"/>
<connect gate="G$1" pin="PD" pad="65"/>
<connect gate="G$1" pin="REFAN" pad="8"/>
<connect gate="G$1" pin="REFAP" pad="7"/>
<connect gate="G$1" pin="REFBN" pad="10"/>
<connect gate="G$1" pin="REFBP" pad="11"/>
<connect gate="G$1" pin="REFIN" pad="68"/>
<connect gate="G$1" pin="REFOUT" pad="67"/>
<connect gate="G$1" pin="SHREF" pad="66"/>
<connect gate="G$1" pin="THPAD" pad="TH"/>
<connect gate="G$1" pin="VDD" pad="23"/>
<connect gate="G$1" pin="VDD@1" pad="24"/>
<connect gate="G$1" pin="VDD@2" pad="25"/>
<connect gate="G$1" pin="VDD@3" pad="26"/>
<connect gate="G$1" pin="VDD@4" pad="61"/>
<connect gate="G$1" pin="VDD@5" pad="62"/>
<connect gate="G$1" pin="VDD@6" pad="63"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3766*" prefix="IC">
<description>&lt;b&gt;622Mbps LAN/WAN Laser Driver with Automatic Power Control and Safety Shutdown&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX3766.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3766"/>
</gates>
<devices>
<device name="" package="QSOP20">
<connects>
<connect gate="G$1" pin="!FAIL" pad="12"/>
<connect gate="G$1" pin="BIAS" pad="16"/>
<connect gate="G$1" pin="BIASMAX" pad="1"/>
<connect gate="G$1" pin="ENABLE" pad="10"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GNDOUT" pad="17"/>
<connect gate="G$1" pin="IN+" pad="7"/>
<connect gate="G$1" pin="IN-" pad="6"/>
<connect gate="G$1" pin="MD" pad="18"/>
<connect gate="G$1" pin="MOD" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="15"/>
<connect gate="G$1" pin="OUT-" pad="14"/>
<connect gate="G$1" pin="POWERSET" pad="19"/>
<connect gate="G$1" pin="REF1" pad="20"/>
<connect gate="G$1" pin="REF2" pad="3"/>
<connect gate="G$1" pin="SAFETY" pad="11"/>
<connect gate="G$1" pin="TC" pad="2"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCCOUT" pad="13"/>
</connects>
<technologies>
<technology name="EEP"/>
<technology name="EEP+"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX98*" prefix="IC">
<description>&lt;b&gt;Micropower, Low-Voltage Rail-to-Rail I/O Comparators&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX985-MAX994.pdf</description>
<gates>
<gate name="P" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="EBT-T" package="UCSP6">
<connects>
<connect gate="P" pin="+IN" pad="B1"/>
<connect gate="P" pin="-IN" pad="B2"/>
<connect gate="P" pin="OUT" pad="A2"/>
<connect gate="P" pin="V+" pad="A3"/>
<connect gate="P" pin="V-" pad="A1"/>
</connects>
<technologies>
<technology name="6"/>
</technologies>
</device>
<device name="EXK-T" package="SC70-5L">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
<connect gate="P" pin="V+" pad="2"/>
<connect gate="P" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="6"/>
</technologies>
</device>
<device name="EUK-T" package="SOT23-5L">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
<connect gate="P" pin="V+" pad="2"/>
<connect gate="P" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="5"/>
</technologies>
</device>
<device name="ESA" package="SO08">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="5"/>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX9*" prefix="IC">
<description>&lt;b&gt;Micropower, Low-Voltage Rail-to-Rail I/O Comparators&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX985-MAX994.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="ESA" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="89"/>
<technology name="90"/>
</technologies>
</device>
<device name="EUA" package="UMAX8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="89"/>
<technology name="90"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX99*" prefix="IC">
<description>&lt;b&gt;Micropower, Low-Voltage Rail-to-Rail I/O Comparators&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/MAX985-MAX994.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="ESD" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EUD" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3233E" prefix="IC">
<description>&lt;b&gt;Dual RS-232 Transceivers with Internal Capacitors&lt;/b&gt;&lt;p&gt;
±15kV ESD-Protected, 1µA, 250kbps, 3.3V/5V &lt;br&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX3233E-MAX3235E.pdf</description>
<gates>
<gate name="P" symbol="VCC-GND"/>
<gate name="Q" symbol="MAX3233"/>
</gates>
<devices>
<device name="WP" package="SO20L">
<connects>
<connect gate="P" pin="GND" pad="18"/>
<connect gate="P" pin="VCC" pad="9"/>
<connect gate="Q" pin="!FORCEOFF" pad="10"/>
<connect gate="Q" pin="!INVALID" pad="2"/>
<connect gate="Q" pin="C1+" pad="13"/>
<connect gate="Q" pin="C1-" pad="14"/>
<connect gate="Q" pin="C2+" pad="15"/>
<connect gate="Q" pin="C2-" pad="16"/>
<connect gate="Q" pin="FORCEON" pad="5"/>
<connect gate="Q" pin="R1IN" pad="8"/>
<connect gate="Q" pin="R1OUT" pad="6"/>
<connect gate="Q" pin="R2IN" pad="20"/>
<connect gate="Q" pin="R2OUT" pad="1"/>
<connect gate="Q" pin="T1IN" pad="4"/>
<connect gate="Q" pin="T1OUT" pad="7"/>
<connect gate="Q" pin="T2IN" pad="3"/>
<connect gate="Q" pin="T2OUT" pad="19"/>
<connect gate="Q" pin="V+@1" pad="11"/>
<connect gate="Q" pin="V+@2" pad="12"/>
<connect gate="Q" pin="V-" pad="17"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="PP" package="DIL20">
<connects>
<connect gate="P" pin="GND" pad="18"/>
<connect gate="P" pin="VCC" pad="9"/>
<connect gate="Q" pin="!FORCEOFF" pad="10"/>
<connect gate="Q" pin="!INVALID" pad="2"/>
<connect gate="Q" pin="C1+" pad="13"/>
<connect gate="Q" pin="C1-" pad="14"/>
<connect gate="Q" pin="C2+" pad="15"/>
<connect gate="Q" pin="C2-" pad="16"/>
<connect gate="Q" pin="FORCEON" pad="5"/>
<connect gate="Q" pin="R1IN" pad="8"/>
<connect gate="Q" pin="R1OUT" pad="6"/>
<connect gate="Q" pin="R2IN" pad="20"/>
<connect gate="Q" pin="R2OUT" pad="1"/>
<connect gate="Q" pin="T1IN" pad="4"/>
<connect gate="Q" pin="T1OUT" pad="7"/>
<connect gate="Q" pin="T2IN" pad="3"/>
<connect gate="Q" pin="T2OUT" pad="19"/>
<connect gate="Q" pin="V+@1" pad="11"/>
<connect gate="Q" pin="V+@2" pad="12"/>
<connect gate="Q" pin="V-" pad="17"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX338*" prefix="IC">
<description>&lt;b&gt;RS-232 Transceivers with ±15kV ESD-Protected I/O and Logic Pins&lt;/b&gt;&lt;p&gt;
+2.35V to +5.5V, 1µA, 2Tx/2Rx &lt;br&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX3380E-MAX3381E.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3380"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="UP" package="TSSOP20">
<connects>
<connect gate="G$1" pin="!FORCEOFF" pad="19"/>
<connect gate="G$1" pin="!INVALID" pad="7"/>
<connect gate="G$1" pin="C1+" pad="1"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="4"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="FORCEON" pad="12"/>
<connect gate="G$1" pin="R1IN" pad="15"/>
<connect gate="G$1" pin="R1OUT" pad="11"/>
<connect gate="G$1" pin="R2IN" pad="14"/>
<connect gate="G$1" pin="R2OUT" pad="10"/>
<connect gate="G$1" pin="T1IN" pad="8"/>
<connect gate="G$1" pin="T1OUT" pad="17"/>
<connect gate="G$1" pin="T2IN" pad="9"/>
<connect gate="G$1" pin="T2OUT" pad="16"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VL" pad="13"/>
<connect gate="P" pin="GND" pad="18"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="0EC"/>
<technology name="0EE"/>
<technology name="1EC"/>
<technology name="1EE"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7611" prefix="IC">
<description>&lt;b&gt;Single Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/ICL7612-ICL764X.pdf</description>
<gates>
<gate name="A" symbol="ICL76XX"/>
</gates>
<devices>
<device name="TV" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="IOSET" pad="8"/>
<connect gate="A" pin="OFF1" pad="1"/>
<connect gate="A" pin="OFF2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="AM"/>
<technology name="BC"/>
<technology name="BM"/>
<technology name="DC"/>
</technologies>
</device>
<device name="PA" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="IOSET" pad="8"/>
<connect gate="A" pin="OFF1" pad="1"/>
<connect gate="A" pin="OFF2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="BC"/>
<technology name="DC"/>
</technologies>
</device>
<device name="SA" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="IOSET" pad="8"/>
<connect gate="A" pin="OFF1" pad="1"/>
<connect gate="A" pin="OFF2" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="AC"/>
<technology name="BC"/>
<technology name="BE"/>
<technology name="DC"/>
<technology name="DE"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL762*" prefix="IC">
<description>&lt;b&gt;Dual Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/ICL7612-ICL764X.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="TV" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PD" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JD" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL763*" prefix="IC">
<description>&lt;b&gt;Triple Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/ICL7612-ICL764X.pdf</description>
<gates>
<gate name="P" symbol="PWR2+-"/>
<gate name="A" symbol="ICL763XX"/>
<gate name="B" symbol="ICL763XX"/>
<gate name="C" symbol="ICL763XX"/>
</gates>
<devices>
<device name="PD" package="DIL16">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="IOSET" pad="16"/>
<connect gate="A" pin="OUT" pad="14"/>
<connect gate="B" pin="+IN" pad="13"/>
<connect gate="B" pin="-IN" pad="12"/>
<connect gate="B" pin="IOSET" pad="11"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="8"/>
<connect gate="C" pin="-IN" pad="7"/>
<connect gate="C" pin="IOSET" pad="6"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="P" pin="V+@1" pad="5"/>
<connect gate="P" pin="V+@2" pad="15"/>
<connect gate="P" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL764*" prefix="IC">
<description>&lt;b&gt;Quad Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/ICL7612-ICL764X.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="DP" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
<device name="DPW" package="DIL16">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="14"/>
<connect gate="D" pin="-IN" pad="15"/>
<connect gate="D" pin="OUT" pad="16"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4337" prefix="IC">
<description>&lt;b&gt;50mA IOUT, Rail-to-Rail I/O Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4335-MAX4338.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="EKA-T" package="SOT23-8L">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EUA" package="UMAX8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4336" prefix="IC">
<description>&lt;b&gt;50mA IOUT, Rail-to-Rail I/O Op Amp with Shutdown/Mute&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4335-MAX4338.pdf</description>
<gates>
<gate name="A" symbol="OP-SHDOWN"/>
<gate name="P" symbol="PWR+-GATE"/>
</gates>
<devices>
<device name="EXT-T" package="SOT23-6L">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="SHUTDOWN" pad="5"/>
<connect gate="P" pin="V+" pad="6"/>
<connect gate="P" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4335" prefix="IC">
<description>&lt;b&gt;50mA IOUT, Rail-to-Rail I/O Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4335-MAX4338.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="P" symbol="PWR+-GATE"/>
</gates>
<devices>
<device name="EXT-T" package="SOT23-6L">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="P" pin="V+" pad="6"/>
<connect gate="P" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4338" prefix="IC">
<description>&lt;b&gt;50mA IOUT, Rail-to-Rail I/O Op Amp with Shutdown/Mute&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4335-MAX4338.pdf</description>
<gates>
<gate name="A" symbol="OP-SHDOWN"/>
<gate name="B" symbol="OP-SHDOWN"/>
<gate name="P" symbol="PWR+-GATE"/>
</gates>
<devices>
<device name="EUB" package="UMAX10">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="SHUTDOWN" pad="5"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="8"/>
<connect gate="B" pin="OUT" pad="9"/>
<connect gate="B" pin="SHUTDOWN" pad="6"/>
<connect gate="P" pin="V+" pad="10"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7042" prefix="IC">
<description>&lt;b&gt;308MHz/315MHz/418MHz/433.92MHz Low-Power, FSK Superheterodyne Receiver&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7042.pdf</description>
<gates>
<gate name="G$1" symbol="MAX7042"/>
</gates>
<devices>
<device name="ATJ" package="QFN32">
<connects>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="AVDD" pad="7"/>
<connect gate="G$1" pin="DATA" pad="30"/>
<connect gate="G$1" pin="DF" pad="22"/>
<connect gate="G$1" pin="DGND" pad="23"/>
<connect gate="G$1" pin="DS+" pad="20"/>
<connect gate="G$1" pin="DS-" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="24"/>
<connect gate="G$1" pin="EN" pad="26"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="FIN+" pad="16"/>
<connect gate="G$1" pin="FIN-" pad="15"/>
<connect gate="G$1" pin="FSEL1" pad="27"/>
<connect gate="G$1" pin="FSEL2" pad="28"/>
<connect gate="G$1" pin="HVIN" pad="29"/>
<connect gate="G$1" pin="LNAIN" pad="8"/>
<connect gate="G$1" pin="LNAOUT" pad="10"/>
<connect gate="G$1" pin="LNASEL" pad="31"/>
<connect gate="G$1" pin="LNASRC" pad="9"/>
<connect gate="G$1" pin="MIXIN+" pad="11"/>
<connect gate="G$1" pin="MIXIN-" pad="12"/>
<connect gate="G$1" pin="MIXOUT" pad="13"/>
<connect gate="G$1" pin="OP+" pad="21"/>
<connect gate="G$1" pin="PDMAX" pad="18"/>
<connect gate="G$1" pin="PDMIN" pad="17"/>
<connect gate="G$1" pin="RSSI" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="6"/>
<connect gate="G$1" pin="XTAL2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1621" prefix="IC">
<description>&lt;b&gt;Digital Thermometer and Thermostat&lt;/b&gt;&lt;p&gt;
Source: http://pdfserv.maxim-ic.com/en/ds/DS1621.pdf</description>
<gates>
<gate name="G$1" symbol="DS1621"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="TOUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="TOUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VT" package="SO08-208">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="TOUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4948ETG" prefix="IC">
<description>&lt;b&gt;Hex SPDT Data Switch&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4947-MAX4948.pdf</description>
<gates>
<gate name="G$1" symbol="MAX4948"/>
<gate name="P1" symbol="GND"/>
<gate name="EP" symbol="EXPOSED"/>
</gates>
<devices>
<device name="" package="TQFN24-EP">
<connects>
<connect gate="EP" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="!EN" pad="5"/>
<connect gate="G$1" pin="CB" pad="14"/>
<connect gate="G$1" pin="COM1" pad="20"/>
<connect gate="G$1" pin="COM2" pad="16"/>
<connect gate="G$1" pin="COM3" pad="11"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="COM5" pad="3"/>
<connect gate="G$1" pin="COM6" pad="23"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC1" pad="18"/>
<connect gate="G$1" pin="NC2" pad="15"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="9"/>
<connect gate="G$1" pin="NC5" pad="4"/>
<connect gate="G$1" pin="NC6" pad="1"/>
<connect gate="G$1" pin="NO1" pad="19"/>
<connect gate="G$1" pin="NO2" pad="17"/>
<connect gate="G$1" pin="NO3" pad="10"/>
<connect gate="G$1" pin="NO4" pad="8"/>
<connect gate="G$1" pin="NO5" pad="2"/>
<connect gate="G$1" pin="NO6" pad="24"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="P1" pin="GND" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4947EBA" prefix="IC">
<description>&lt;b&gt;Hex SPDT Data Switch&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4947-MAX4948.pdf</description>
<gates>
<gate name="A" symbol="MAX4947"/>
<gate name="B" symbol="MAX4947"/>
<gate name="C" symbol="MAX4947"/>
<gate name="P" symbol="VCC-GND"/>
<gate name="P1" symbol="GND"/>
<gate name="P2" symbol="GND"/>
</gates>
<devices>
<device name="" package="UCSP25">
<connects>
<connect gate="A" pin="CB" pad="B5"/>
<connect gate="A" pin="COM1" pad="E4"/>
<connect gate="A" pin="COM2" pad="C5"/>
<connect gate="A" pin="NC1" pad="D4"/>
<connect gate="A" pin="NC2" pad="C4"/>
<connect gate="A" pin="NO1" pad="E5"/>
<connect gate="A" pin="NO2" pad="D5"/>
<connect gate="B" pin="CB" pad="A5"/>
<connect gate="B" pin="COM1" pad="A4"/>
<connect gate="B" pin="COM2" pad="B2"/>
<connect gate="B" pin="NC1" pad="B4"/>
<connect gate="B" pin="NC2" pad="B3"/>
<connect gate="B" pin="NO1" pad="A3"/>
<connect gate="B" pin="NO2" pad="A2"/>
<connect gate="C" pin="CB" pad="B1"/>
<connect gate="C" pin="COM1" pad="C1"/>
<connect gate="C" pin="COM2" pad="E2"/>
<connect gate="C" pin="NC1" pad="C2"/>
<connect gate="C" pin="NC2" pad="D2"/>
<connect gate="C" pin="NO1" pad="D1"/>
<connect gate="C" pin="NO2" pad="E1"/>
<connect gate="P" pin="GND" pad="A1"/>
<connect gate="P" pin="VCC" pad="E3"/>
<connect gate="P1" pin="GND" pad="C3"/>
<connect gate="P2" pin="GND" pad="D3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4947ETG" prefix="IC">
<description>&lt;b&gt;Hex SPDT Data Switch&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4947-MAX4948.pdf</description>
<gates>
<gate name="A" symbol="MAX4947"/>
<gate name="B" symbol="MAX4947"/>
<gate name="C" symbol="MAX4947"/>
<gate name="P" symbol="VCC-GND"/>
<gate name="P1" symbol="GND"/>
<gate name="EXP" symbol="EXPOSED"/>
</gates>
<devices>
<device name="" package="TQFN24-EP">
<connects>
<connect gate="A" pin="CB" pad="14"/>
<connect gate="A" pin="COM1" pad="20"/>
<connect gate="A" pin="COM2" pad="16"/>
<connect gate="A" pin="NC1" pad="18"/>
<connect gate="A" pin="NC2" pad="15"/>
<connect gate="A" pin="NO1" pad="19"/>
<connect gate="A" pin="NO2" pad="17"/>
<connect gate="B" pin="CB" pad="13"/>
<connect gate="B" pin="COM1" pad="11"/>
<connect gate="B" pin="COM2" pad="7"/>
<connect gate="B" pin="NC1" pad="12"/>
<connect gate="B" pin="NC2" pad="9"/>
<connect gate="B" pin="NO1" pad="10"/>
<connect gate="B" pin="NO2" pad="8"/>
<connect gate="C" pin="CB" pad="5"/>
<connect gate="C" pin="COM1" pad="3"/>
<connect gate="C" pin="COM2" pad="23"/>
<connect gate="C" pin="NC1" pad="4"/>
<connect gate="C" pin="NC2" pad="1"/>
<connect gate="C" pin="NO1" pad="2"/>
<connect gate="C" pin="NO2" pad="24"/>
<connect gate="EXP" pin="EXP" pad="EXP"/>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="VCC" pad="22"/>
<connect gate="P1" pin="GND" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4948EBA" prefix="IC">
<description>&lt;b&gt;Hex SPDT Data Switch&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4947-MAX4948.pdf</description>
<gates>
<gate name="G$1" symbol="MAX4948"/>
<gate name="P1" symbol="GND"/>
<gate name="P2" symbol="GND"/>
</gates>
<devices>
<device name="" package="UCSP25">
<connects>
<connect gate="G$1" pin="!EN" pad="B1"/>
<connect gate="G$1" pin="CB" pad="B5"/>
<connect gate="G$1" pin="COM1" pad="E4"/>
<connect gate="G$1" pin="COM2" pad="C5"/>
<connect gate="G$1" pin="COM3" pad="A4"/>
<connect gate="G$1" pin="COM4" pad="B2"/>
<connect gate="G$1" pin="COM5" pad="C1"/>
<connect gate="G$1" pin="COM6" pad="E2"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="NC1" pad="D4"/>
<connect gate="G$1" pin="NC2" pad="C4"/>
<connect gate="G$1" pin="NC3" pad="B4"/>
<connect gate="G$1" pin="NC4" pad="B3"/>
<connect gate="G$1" pin="NC5" pad="C2"/>
<connect gate="G$1" pin="NC6" pad="D2"/>
<connect gate="G$1" pin="NO1" pad="E5"/>
<connect gate="G$1" pin="NO2" pad="D5"/>
<connect gate="G$1" pin="NO3" pad="A3"/>
<connect gate="G$1" pin="NO4" pad="A2"/>
<connect gate="G$1" pin="NO5" pad="D1"/>
<connect gate="G$1" pin="NO6" pad="E1"/>
<connect gate="G$1" pin="VCC" pad="E3"/>
<connect gate="P1" pin="GND" pad="C3"/>
<connect gate="P2" pin="GND" pad="D3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4906" prefix="IC">
<description>&lt;b&gt;High-/Full-Speed USB 2.0 Switches&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4906-MAX4907F.pdf</description>
<gates>
<gate name="G$1" symbol="MAX4906"/>
</gates>
<devices>
<device name="ELA" package="UDFN10">
<connects>
<connect gate="G$1" pin="COM1" pad="4"/>
<connect gate="G$1" pin="COM2" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NC1" pad="9"/>
<connect gate="G$1" pin="NC2" pad="8"/>
<connect gate="G$1" pin="NO1" pad="7"/>
<connect gate="G$1" pin="NO2" pad="6"/>
<connect gate="G$1" pin="SHDN/!EN" pad="2"/>
<connect gate="G$1" pin="V+" pad="10"/>
</connects>
<technologies>
<technology name=""/>
<technology name="F"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX4907" prefix="IC">
<description>&lt;b&gt;High-/Full-Speed USB 2.0 Switches&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX4906-MAX4907F.pdf</description>
<gates>
<gate name="G$1" symbol="MAX4907"/>
</gates>
<devices>
<device name="ELB" package="UDFN8">
<connects>
<connect gate="G$1" pin="COM1" pad="3"/>
<connect gate="G$1" pin="COM2" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="NO1" pad="6"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="SHDN/!EN" pad="1"/>
<connect gate="G$1" pin="V+" pad="7"/>
</connects>
<technologies>
<technology name=""/>
<technology name="F"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX617*ASA" prefix="IC">
<description>&lt;b&gt;High-Precision Voltage References with Temperature Sensor&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX6173-MAX6177.pdf</description>
<gates>
<gate name="G$1" symbol="MAX6173"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TEMP" pad="3"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
</connects>
<technologies>
<technology name="3A"/>
<technology name="3B"/>
<technology name="4A"/>
<technology name="4B"/>
<technology name="5A"/>
<technology name="5B"/>
<technology name="6A"/>
<technology name="6B"/>
<technology name="7A"/>
<technology name="7B"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1792EUA" prefix="IC">
<description>&lt;b&gt;500mA Low-Dropout Linear Regulator in µMAX&lt;/b&gt;&lt;p&gt;
Source: http://www.maxim-ic.com .. MAX1792-1.pdf</description>
<gates>
<gate name="G$1" symbol="MAX1792"/>
</gates>
<devices>
<device name="T" package="UMAX8-THERMAL">
<connects>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="!SHDN" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN@1" pad="1"/>
<connect gate="G$1" pin="IN@2" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="7"/>
<connect gate="G$1" pin="OUT@2" pad="8"/>
<connect gate="G$1" pin="SET" pad="6"/>
<connect gate="G$1" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1759" prefix="IC">
<description>&lt;b&gt;Buck/Boost Regulating Charge Pump in µMAX&lt;/b&gt;&lt;p&gt;
Source: http://www.maxim-ic.com .. MAX1759.pdf</description>
<gates>
<gate name="G$1" symbol="MAX1759"/>
</gates>
<devices>
<device name="" package="UMAX10">
<connects>
<connect gate="G$1" pin="!SHDN" pad="2"/>
<connect gate="G$1" pin="CXN" pad="7"/>
<connect gate="G$1" pin="CXP" pad="8"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN@1" pad="3"/>
<connect gate="G$1" pin="IN@2" pad="4"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="PGND" pad="6"/>
<connect gate="G$1" pin="POK" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1555" prefix="IC">
<description>&lt;b&gt;Dual-Input USB/AC Adapter 1-Cell Li+ Battery Chargers&lt;/b&gt;&lt;p&gt;
Source: http://www.maxim-ic.com .. MAX1551-MAX1555.pdf</description>
<gates>
<gate name="G$1" symbol="MAX1555"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="!CHG" pad="3"/>
<connect gate="G$1" pin="BAT" pad="5"/>
<connect gate="G$1" pin="DC" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="USB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1551" prefix="IC">
<description>&lt;b&gt;Dual-Input USB/AC Adapter 1-Cell Li+ Battery Chargers&lt;/b&gt;&lt;p&gt;
Source: http://www.maxim-ic.com .. MAX1551-MAX1555.pdf</description>
<gates>
<gate name="G$1" symbol="MAX1551"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="!POK" pad="3"/>
<connect gate="G$1" pin="BAT" pad="5"/>
<connect gate="G$1" pin="DC" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="USB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS275" prefix="IC">
<description>&lt;b&gt;Line-Powered RS-232 Transceiver Chip&lt;/b&gt;&lt;p&gt;
Source: http://www.maxim-ic.com .. DS275.pdf</description>
<gates>
<gate name="G$1" symbol="DS275"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RXIN" pad="7"/>
<connect gate="G$1" pin="RXOUT" pad="1"/>
<connect gate="G$1" pin="TXIN" pad="3"/>
<connect gate="G$1" pin="TXOUT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VDRV" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RXIN" pad="7"/>
<connect gate="G$1" pin="RXOUT" pad="1"/>
<connect gate="G$1" pin="TXIN" pad="3"/>
<connect gate="G$1" pin="TXOUT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VDRV" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="TSSOP14">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RXIN" pad="11"/>
<connect gate="G$1" pin="RXOUT" pad="1"/>
<connect gate="G$1" pin="TXIN" pad="5"/>
<connect gate="G$1" pin="TXOUT" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VDRV" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3311" prefix="IC">
<description>&lt;b&gt;460kbps, 1µA Supply Current, RS-232-Compatible Transceivers in µMAX&lt;/b&gt;&lt;p&gt;
Source: http://www.maxim-ic.com .. MAX3311-MAX3313.pdf</description>
<gates>
<gate name="G$1" symbol="MAX3311"/>
</gates>
<devices>
<device name="" package="UMAX10">
<connects>
<connect gate="G$1" pin="!SHDN" pad="3"/>
<connect gate="G$1" pin="C1+" pad="9"/>
<connect gate="G$1" pin="C1-" pad="2"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RIN" pad="6"/>
<connect gate="G$1" pin="ROUT" pad="5"/>
<connect gate="G$1" pin="TIN" pad="4"/>
<connect gate="G$1" pin="TOUT" pad="7"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7313AEG" prefix="IC">
<description>&lt;b&gt;16-Port I/O Expander with LED Intensity Control, Interrupt, and Hot-Insertion Protection&lt;/p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7313.pdf</description>
<gates>
<gate name="G$1" symbol="MAX7313AEG"/>
</gates>
<devices>
<device name="" package="QSOP24">
<connects>
<connect gate="G$1" pin="!INT!/O16" pad="1"/>
<connect gate="G$1" pin="AD0" pad="21"/>
<connect gate="G$1" pin="AD1" pad="2"/>
<connect gate="G$1" pin="AD2" pad="3"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="P0" pad="4"/>
<connect gate="G$1" pin="P1" pad="5"/>
<connect gate="G$1" pin="P10" pad="15"/>
<connect gate="G$1" pin="P11" pad="16"/>
<connect gate="G$1" pin="P12" pad="17"/>
<connect gate="G$1" pin="P13" pad="18"/>
<connect gate="G$1" pin="P14" pad="19"/>
<connect gate="G$1" pin="P15" pad="20"/>
<connect gate="G$1" pin="P2" pad="6"/>
<connect gate="G$1" pin="P3" pad="7"/>
<connect gate="G$1" pin="P4" pad="8"/>
<connect gate="G$1" pin="P5" pad="9"/>
<connect gate="G$1" pin="P6" pad="10"/>
<connect gate="G$1" pin="P7" pad="11"/>
<connect gate="G$1" pin="P8" pad="13"/>
<connect gate="G$1" pin="P9" pad="14"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="SLC" pad="22"/>
<connect gate="G$1" pin="V+" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7313ATG" prefix="IC">
<description>&lt;b&gt;16-Port I/O Expander with LED Intensity Control, Interrupt, and Hot-Insertion Protection&lt;/p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7313.pdf</description>
<gates>
<gate name="G$1" symbol="MAX7313"/>
</gates>
<devices>
<device name="" package="TQFN24-EP">
<connects>
<connect gate="G$1" pin="!INT!/O16" pad="22"/>
<connect gate="G$1" pin="AD0" pad="18"/>
<connect gate="G$1" pin="AD1" pad="23"/>
<connect gate="G$1" pin="AD2" pad="24"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="EXP"/>
<connect gate="G$1" pin="P0" pad="1"/>
<connect gate="G$1" pin="P1" pad="2"/>
<connect gate="G$1" pin="P10" pad="12"/>
<connect gate="G$1" pin="P11" pad="13"/>
<connect gate="G$1" pin="P12" pad="14"/>
<connect gate="G$1" pin="P13" pad="15"/>
<connect gate="G$1" pin="P14" pad="16"/>
<connect gate="G$1" pin="P15" pad="17"/>
<connect gate="G$1" pin="P2" pad="3"/>
<connect gate="G$1" pin="P3" pad="4"/>
<connect gate="G$1" pin="P4" pad="5"/>
<connect gate="G$1" pin="P5" pad="6"/>
<connect gate="G$1" pin="P6" pad="7"/>
<connect gate="G$1" pin="P7" pad="8"/>
<connect gate="G$1" pin="P8" pad="10"/>
<connect gate="G$1" pin="P9" pad="11"/>
<connect gate="G$1" pin="SDA" pad="20"/>
<connect gate="G$1" pin="SLC" pad="19"/>
<connect gate="G$1" pin="V+" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6520" prefix="IC">
<description>&lt;b&gt; 1.2V Voltage Reference&lt;/b&gt; 50ppm/°C, SOT23, 3-Terminal&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX6520.pdf</description>
<gates>
<gate name="-1" symbol="MAX6520"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="-1" pin="GND" pad="3"/>
<connect gate="-1" pin="IN" pad="1"/>
<connect gate="-1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX103*" prefix="IC">
<description>&lt;b&gt;2.7V to 5.5V, Low-Power, 4-/12-Channel 2-Wire Serial 8-Bit ADCs&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX1036-MAX1039M.pdf</description>
<gates>
<gate name="G$1" symbol="MAX1036"/>
</gates>
<devices>
<device name="" package="SOT23-8L">
<connects>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3/REF" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="6"/>
<technology name="7"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX10*" prefix="IC">
<description>&lt;b&gt;2.7V to 5.5V, Low-Power, 4-/12-Channel 2-Wire Serial 8-Bit ADCs&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX1036-MAX1039M.pdf</description>
<gates>
<gate name="G$1" symbol="MAX1038"/>
</gates>
<devices>
<device name="" package="QSOP16">
<connects>
<connect gate="G$1" pin="AIN0" pad="8"/>
<connect gate="G$1" pin="AIN1" pad="7"/>
<connect gate="G$1" pin="AIN10" pad="14"/>
<connect gate="G$1" pin="AIN11/REF" pad="13"/>
<connect gate="G$1" pin="AIN2" pad="6"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="AIN4" pad="4"/>
<connect gate="G$1" pin="AIN5" pad="3"/>
<connect gate="G$1" pin="AIN6" pad="2"/>
<connect gate="G$1" pin="AIN7" pad="1"/>
<connect gate="G$1" pin="AIN8" pad="16"/>
<connect gate="G$1" pin="AIN9" pad="15"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="VDD" pad="12"/>
</connects>
<technologies>
<technology name="38"/>
<technology name="39"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX313" prefix="IC">
<description>&lt;b&gt;10?, Quad, SPST, CMOS Analog Switches&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX312-MAX314.pdf</description>
<gates>
<gate name="G$1" symbol="MAX313"/>
</gates>
<devices>
<device name="PE" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NO1" pad="3"/>
<connect gate="G$1" pin="NO2" pad="14"/>
<connect gate="G$1" pin="NO3" pad="11"/>
<connect gate="G$1" pin="NO4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="SE" package="SO16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NO1" pad="3"/>
<connect gate="G$1" pin="NO2" pad="14"/>
<connect gate="G$1" pin="NO3" pad="11"/>
<connect gate="G$1" pin="NO4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="UE" package="TSSOP16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NO1" pad="3"/>
<connect gate="G$1" pin="NO2" pad="14"/>
<connect gate="G$1" pin="NO3" pad="11"/>
<connect gate="G$1" pin="NO4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX312" prefix="IC">
<description>&lt;b&gt;10?, Quad, SPST, CMOS Analog Switches&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX312-MAX314.pdf</description>
<gates>
<gate name="G$1" symbol="MAX312"/>
</gates>
<devices>
<device name="PE" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SE" package="SSOP16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UE" package="TSSOP16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX314" prefix="IC">
<description>&lt;b&gt;10?, Quad, SPST, CMOS Analog Switches&lt;/b&gt;&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX312-MAX314.pdf</description>
<gates>
<gate name="G$1" symbol="MAX314"/>
</gates>
<devices>
<device name="PE" package="DIL16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NO1" pad="3"/>
<connect gate="G$1" pin="NO4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="SE" package="SO16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NO1" pad="3"/>
<connect gate="G$1" pin="NO4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
<device name="UE" package="TSSOP16">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="15"/>
<connect gate="G$1" pin="COM3" pad="10"/>
<connect gate="G$1" pin="COM4" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="16"/>
<connect gate="G$1" pin="IN3" pad="9"/>
<connect gate="G$1" pin="IN4" pad="8"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NO1" pad="3"/>
<connect gate="G$1" pin="NO4" pad="6"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$1" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS2726" prefix="IC">
<description>&lt;b&gt;5-Cell to 10-Cell Li+ Protector with Cell Balancing&lt;/b&gt;&lt;p&gt;
Source: www.maxim-ic.com .. DS2726.pdf</description>
<gates>
<gate name="G$1" symbol="DS2726"/>
</gates>
<devices>
<device name="" package="TQFN32">
<connects>
<connect gate="G$1" pin="CBCFG" pad="9"/>
<connect gate="G$1" pin="CBS0" pad="10"/>
<connect gate="G$1" pin="CBS1" pad="11"/>
<connect gate="G$1" pin="CC" pad="31"/>
<connect gate="G$1" pin="CSCD" pad="8"/>
<connect gate="G$1" pin="DC" pad="28"/>
<connect gate="G$1" pin="DCOCD" pad="6"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="OVS0" pad="12"/>
<connect gate="G$1" pin="OVS1" pad="13"/>
<connect gate="G$1" pin="PKP" pad="32"/>
<connect gate="G$1" pin="RDOC" pad="2"/>
<connect gate="G$1" pin="RSC" pad="1"/>
<connect gate="G$1" pin="SEL0" pad="4"/>
<connect gate="G$1" pin="SEL1" pad="5"/>
<connect gate="G$1" pin="SLEEP" pad="7"/>
<connect gate="G$1" pin="SNS" pad="29"/>
<connect gate="G$1" pin="V00" pad="16"/>
<connect gate="G$1" pin="V01" pad="17"/>
<connect gate="G$1" pin="V02" pad="18"/>
<connect gate="G$1" pin="V03" pad="19"/>
<connect gate="G$1" pin="V04" pad="20"/>
<connect gate="G$1" pin="V05" pad="21"/>
<connect gate="G$1" pin="V06" pad="22"/>
<connect gate="G$1" pin="V07" pad="23"/>
<connect gate="G$1" pin="V08" pad="24"/>
<connect gate="G$1" pin="V09" pad="25"/>
<connect gate="G$1" pin="V10" pad="26"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS8500" prefix="IC">
<description>&lt;b&gt;HART Modem&lt;/b&gt; Single-Chip, Half-Duplex, 1200bps FSK Modulation and Demodulation&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/DS8500.pdf</description>
<gates>
<gate name="G$1" symbol="DS8500"/>
</gates>
<devices>
<device name="" package="TQFN20-5X5">
<connects>
<connect gate="G$1" pin="!RST" pad="4"/>
<connect gate="G$1" pin="AGND" pad="15"/>
<connect gate="G$1" pin="AVDD" pad="11"/>
<connect gate="G$1" pin="DGND@1" pad="3"/>
<connect gate="G$1" pin="DGND@2" pad="9"/>
<connect gate="G$1" pin="DGND@3" pad="16"/>
<connect gate="G$1" pin="DGND@4" pad="17"/>
<connect gate="G$1" pin="DGND@5" pad="18"/>
<connect gate="G$1" pin="DVDD@1" pad="1"/>
<connect gate="G$1" pin="DVDD@2" pad="2"/>
<connect gate="G$1" pin="D_IN" pad="20"/>
<connect gate="G$1" pin="D_OUT" pad="19"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="FSK_IN" pad="14"/>
<connect gate="G$1" pin="FSK_OUT" pad="12"/>
<connect gate="G$1" pin="OCD" pad="5"/>
<connect gate="G$1" pin="REF" pad="13"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="XCEN" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX31855" prefix="U">
<gates>
<gate name="G$1" symbol="MAX31855"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SO" pad="7"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
