<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="DO-1N4148">
</package>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
<package name="0805">
<description>0805 (2012 Metric)</description>
</package>
<package name="EIA3216-18/A-R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="EIA3216-18/A-W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="EIA3528-21/B-R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="EIA3528-21/B-W">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="1206">
<description>1206 (3216 Metric)</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="0603">
<description>0603 (1608 Metric)</description>
</package>
<package name="PUSHBUTTON_SMD_SJ">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="HEADER_1X05">
</package>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED 1206&lt;/b&gt;</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED 0805&lt;/b&gt;</description>
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="EIA7343-31/D-R">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Reflow solder</description>
</package>
<package name="EIA7343-31/D-W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="EIA6032-28/C-R">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="EIA6032-28/C-W">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="JTAG-ARM">
<description>20 Pin JTAG Connector (ARM7, ARM9)</description>
</package>
<package name="LQFP64">
</package>
<package name="LQFP48">
</package>
<package name="SOT223-R">
<description>&lt;b&gt;SOT223&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="SOT223-W">
<description>&lt;b&gt;SOT223&lt;/b&gt; - Wave soldering</description>
</package>
<package name="SOT323-R">
<description>&lt;b&gt;SOT323&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="SOT323-W">
<description>&lt;b&gt;SOT323&lt;/b&gt; - Wave soldering&lt;/b&gt;</description>
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
<package name="SOLDERJUMPER_REFLOW">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt; - Reflow</description>
</package>
<package name="SOLDERJUMPER_WAVE">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt; - Wave</description>
</package>
<package name="JUMPER2">
<description>&lt;b&gt;JUMPER&lt;/b&gt; - 2 Pins</description>
</package>
<package name="JUMPER3">
<description>&lt;b&gt;JUMPER&lt;/b&gt; - 3 Pins</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 6 Pin</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;SMD CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HEADER_1X02">
</package>
<package name="JSTPH2">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="LFCSP16-W">
<description>&lt;b&gt;16-Terminal Leadless Frame Chip Scale Package [LFCSP] (CP) - Wave Footprint&lt;/b&gt;&lt;p&gt;
Source: Analog Devices .. 780914713ADD8704_0.pdf</description>
</package>
<package name="MOUNTINGHOLE_2.8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
<package name="MOUNTINGHOLE_3.0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
<package name="MOUNTINGHOLE_3.2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
<package name="1X01_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="LFCSP16-R">
<description>&lt;b&gt;16-Terminal Leadless Frame Chip Scale Package [LFCSP] (CP) - Reflow Footprint&lt;/b&gt;&lt;p&gt;
Source: Analog Devices .. 780914713ADD8704_0.pdf</description>
</package>
<package name="FPC4PIN">
<description>4 Pin 0.5mm FPC Connector</description>
</package>
<package name="1X10_OVAL">
<description>&lt;b&gt;1x10 PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X16_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09_OVAL">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="TO92-LINE">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="SSOP24">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;&lt;p&gt;
SOT340-1 / JEDEC MO-150AG</description>
</package>
<package name="SOIC8_150MIL">
<description>&lt;b&gt;Small Outline IC - 150mil Wide&lt;/b&gt;</description>
</package>
<package name="SOIC16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="MSOP10">
<description>10-Lead Mini Small Outline Package [MSOP]</description>
</package>
<package name="SOIC24WIDE">
<description>&lt;b&gt;Small Outline Package 24&lt;/b&gt; wide</description>
</package>
<package name="DIPSWITCH_2PIN">
<description>Two button DIP switch</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="TRIMPOT_BOURNS3MM">
<description>&lt;p&gt;Bourns 3303W 3MM SMT Trimpot&lt;/p&gt;</description>
</package>
<package name="TESTPOINT_SMT">
<description>Surface Mount Test Point - Compact SMT</description>
</package>
<package name="PSP_TSCON">
<description>Sharp LQ043xxx Touch Screen Connector</description>
</package>
<package name="PSP_BACKLIGHTCON">
<description>&lt;p&gt;Sharp LQ043xxx Backlight Connector&lt;/p&gt;
FPC 0.5mm 4 Pin Upper Contacts</description>
</package>
<package name="FPC40PIN">
<description>&lt;p&gt;Sharp LQ043xxx LCD Connector&lt;/p&gt;
FPC 0.5mm 40 Pin Bottom</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="TESTPOINT_PAD_2MM">
<description>Testpoint - Pad</description>
</package>
<package name="TESTPOINT_ROUND_2MM">
<description>Testpoint - Round 2mm</description>
</package>
<package name="1X01_ROUND">
</package>
<package name="1X05_ROUND">
</package>
<package name="TCS3414_CS6">
<description>&lt;p&gt;6 Lead Chipscale&lt;br/&gt;
0.30mm pads, 0.61mm pitch&lt;/p&gt;
&lt;b&gt;Source&lt;/b&gt;: http://www.taosinc.com/getfile.aspx?type=press&amp;file=tcs3404cs-e46.pdf</description>
</package>
<package name="JSTPH4">
<description>4 Pin JST PH Series Female Connector&lt;br/&gt;
Righ-Angle SMT</description>
</package>
<package name="CRYSTAL_CYL_2X6MM_SMT">
<description>32.768KHz Crystal - SMT Cylinder</description>
</package>
<package name="1X06_ROUND">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="STANDARDCONNECTOR">
</package>
<package name="TSL2561_CS6">
<description>&lt;p&gt;6 Lead Chipscale&lt;br/&gt;
0.21mm pads, 0.5mm pitch&lt;/p&gt;</description>
</package>
<package name="TPS851">
<description>Toshiba TPS851 Luminance Sensor</description>
</package>
<package name="1X02_ROUND">
</package>
<package name="1X03_ROUND">
</package>
<package name="1X04_ROUND">
</package>
<package name="TSSOP8">
<description>&lt;p&gt;&lt;b&gt;Thin Shrink Small Outline Package&lt;/b&gt;&lt;br/&gt;
0.65mm Pitch, 3.0mm x 3.0mm
&lt;/p&gt;</description>
</package>
<package name="LQFP100">
<description>&lt;b&gt;LQFP100 &lt;/b&gt;&lt;p&gt;Low Profile Quad Flat Package 14x14x1.4 mm&lt;p&gt;</description>
</package>
<package name="LQFP80">
<description>&lt;b&gt;LQFP80 &lt;/b&gt;&lt;p&gt;Low profile Quad Flat Package 12x12x1.4 mm&lt;p&gt;</description>
</package>
<package name="1X02_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
2 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X03_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
2 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X04_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
4 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X05_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
5 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X06_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
6 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="1X10_SMT">
<description>&lt;p&gt;&lt;b&gt;Pin Headers&lt;/b&gt;&lt;br/&gt;
10 Pin, 0.1"/2.54mm pitch, SMT&lt;/p&gt;</description>
</package>
<package name="MOLEX20_RIGHTANGLE">
<description>&lt;p&gt;&lt;b&gt;Molex 20 Pin Header&lt;/b&gt;&lt;/p&gt; 
Footprint designed to mount connector on edge of board, one row on top layer, one row on bottom layer</description>
</package>
<package name="1X08_ROUND">
</package>
<package name="RGBLED_PLCC6">
<description>&lt;b&gt;RGB LED PLCC-6&lt;/b&gt;&lt;p&gt;
5.0mm x 5.0mm 1.5mm Pitch</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED 0603&lt;/b&gt;</description>
</package>
<package name="HVQFN33-7X7">
<description>&lt;b&gt;HVQFN33 &lt;/b&gt;&lt;p&gt;Plastic thermal enhanced very thin quad flat package; 33 terminals; body 7x7x0.85 mm;
&lt;p&gt;Thermal pad intentionally smaller than actual pad size to avoid bridges&lt;/p&gt;</description>
</package>
<package name="CORTEXM3_SWD10_MOLEX">
<description>10 Pin SWD Connector (Cortex M3)
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
<package name="1X16_ROUND">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X05_1.27MM_SMT">
<description>&lt;p&gt;2x05 1.27mm Headers SMT (2.0mm Height)&lt;/p&gt;
4UConnector: 16846</description>
</package>
<package name="XBEE">
<description>&lt;b&gt;XBEE&lt;/b&gt;&lt;p&gt;
Source: http://www.maxstream.net/products/xbee/datasheet_XBee_OEM_RF-Modules.pdf</description>
</package>
<package name="XBEE-PRO">
<description>&lt;b&gt;XBEE Pro&lt;/b&gt;&lt;p&gt;
Source: http://www.maxstream.net/products/xbee/datasheet_XBee_OEM_RF-Modules.pdf</description>
</package>
<package name="ENCLOSURE_TB59">
<description>&lt;b&gt;&lt;p&gt;TB-59 ABS Plastic Enclosure&lt;/p&gt;&lt;/b&gt;
Exterior Dimensions: 100L x 65W x 25H&lt;br/&gt;
Interior Dimensions: 95L x 60W x 20H</description>
</package>
<package name="ENCLOSURE_TB55">
<description>&lt;b&gt;&lt;p&gt;TB-55 ABS Plastic Enclosure&lt;/p&gt;&lt;/b&gt;
Exterior Dimensions: 80L x 50W x 20H&lt;br/&gt;
Interior Dimensions: 75L x 45W x 15H</description>
</package>
<package name="ENCLOSURE_TB56">
<description>&lt;b&gt;&lt;p&gt;TB-56 ABS Plastic Enclosure&lt;/p&gt;&lt;/b&gt;
Exterior Dimensions: 95L x 65W x 20H&lt;br/&gt;
Interior Dimensions: 90L x 60W x 15H</description>
</package>
<package name="ENCLOSURE_WINDOW_82X60X20">
<description>&lt;b&gt;&lt;p&gt;82x60x20mm Plastic Enclosure w/Window&lt;/p&gt;&lt;/b&gt;
Exterior Dimensions: 82L x 60W x 20H&lt;br/&gt;
Interior Dimensions: 75L x 54W x 12H</description>
</package>
<package name="ENCLOSURE_SS125">
<description>&lt;b&gt;&lt;p&gt;SS-125 ABS Plastic Enclosure - Takachi&lt;/p&gt;&lt;/b&gt;
Exterior Dimensions: 125L x 80W x 32H (mm)&lt;br/&gt;
Interior Dimensions: 118L x 69W x 27H (mm)
&lt;p&gt;Source: http://www.takachi-el.co.jp/data/pdf/05-13.pdf&lt;/p&gt;</description>
</package>
<package name="CRYSTAL_3.2X2.5">
<description>3.2mm x 2.5mm Thin SMT Crystal</description>
</package>
<package name="CRYSTAL_4.9X1.8">
<description>&lt;p&gt;4.9mm x 1.8mm Thin SMT Crystal&lt;/p&gt;
Epson Toyocom FCC-255</description>
</package>
<package name="CR2032">
<description>CR2032 Battery Holder</description>
</package>
<package name="SDCARD_SMT_4U06132">
<description>SD Card Holder - 90° SMT
&lt;p&gt;4UConnector: 06132&lt;/p&gt;</description>
</package>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
<package name="INDUCTOR_1007">
<description>Inductor - 1007 (2518 Metric)
&lt;p&gt;L: 2.5mm x W: 1.8mm x H: 1.8mm&lt;/p&gt;</description>
</package>
<package name="1X10_ROUND">
</package>
<package name="PTC1210">
<description>PTC 1210 (3225 Metric)

Source: http://www.bourns.com/data/global/PDFs/mfusmf.pdf</description>
</package>
<package name="PTC1812">
<description>PTC 1812 (4532 Metric)

Source: http://www.bourns.com/data/global/PDFs/MFMSMF.pdf</description>
</package>
<package name="1X07_ROUND">
</package>
<package name="1X20_ROUND">
</package>
<package name="TSOP54-400">
<description>&lt;b&gt;54-Pin Plastic TSOP&lt;/b&gt; (400 mil)&lt;p&gt;
Source: http://download.micron.com/pdf/datasheets/dram/sdram/256MSDRAM.pdf</description>
</package>
<package name="UMAX10">
<description>&lt;b&gt;micro MAX Package&lt;/b&gt;</description>
</package>
<package name="RJ45SMT">
<description>&lt;p&gt;RJ45 Connector SMT w/LEDs&lt;/p&gt;
&lt;p&gt;4UConnector: 15820&lt;/p&gt;</description>
</package>
<package name="RJ45PTH">
<description>RJ45 Connector PTH W/LEDs
&lt;p&gt;4UConnector: 17893&lt;/p&gt;</description>
</package>
<package name="RJ45_PULSEJACK">
<description>RJ45 (Ethernet) Connector with LEDs and Built-In Transformer 
&lt;p&gt;Model: J0026D21BNL&lt;br/&gt;
Digikey: 553-1349-ND&lt;/p&gt;</description>
</package>
<package name="PSP_LCDOUTLINE">
<description>Physical dimensions for the Sharp LQ043xxx (PSP1000) LCD Screen</description>
</package>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
<package name="1X11_ROUND">
</package>
<package name="1X12_ROUND">
</package>
<package name="EVQ-Q2">
</package>
<package name="SMA90_DIP">
<description>SMA DIP Connector 90° 50 Ohm</description>
</package>
<package name="32QN2">
<description>32QN2, 32-lead 5.0 x 5.0mm Body, 0.50mm Pitch, Quad Flat No Lead Package (QFN) Sawn</description>
</package>
<package name="BALUN1206">
</package>
<package name="LOWPASSFILTER0603">
</package>
<package name="869MHZANTENNA">
</package>
<package name="BALUN0805">
</package>
<package name="TSSOP8-4.4MM">
<description>&lt;b&gt;Thin Shrink Small Outline Package&lt;/b&gt;&lt;br&gt;
0.65mm Pitch, 4.4mm x 3.0mm Body</description>
</package>
<package name="HVQFN40-6X6">
<description>&lt;b&gt;HVQFN40 &lt;/b&gt;&lt;p&gt;Plastic thermal enhanced very thin quad flat package; 40 terminals; body 6x6x0.85 mm;</description>
</package>
<package name="SOIC-4">
<description>&lt;b&gt;SOIC-4 Package&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/products/discrete/pdf/soic4_dim.pdf</description>
</package>
<package name="GM862">
</package>
<package name="GM862_CONNECTOR">
</package>
<package name="1X10_ROUND_2MM">
<description>1x10 2.0mm Header Pins</description>
</package>
<package name="SOD-123">
<description>&lt;b&gt;SOD-123&lt;/b&gt;
&lt;p&gt;Source: http://www.diodes.com/datasheets/ds30139.pdf&lt;/p&gt;</description>
</package>
<package name="RGBLED_PLCC4">
<description>&lt;b&gt;RGB LED PLCC4&lt;/b&gt;</description>
</package>
<package name="0805-THM">
</package>
<package name="FIDUCIAL-1.5X3">
</package>
<package name="FIDUCIAL-1X2">
</package>
<package name="FIDUCIAL-1X2.5">
</package>
<package name="PASS-ROUND">
<description>&lt;b&gt;FIDUCIAL MARKER&lt;/b&gt;&lt;p&gt;
round, layers 1 + 16 + 21 + 39 + 49</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="1X12_OVAL">
</package>
<package name="0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1X12_ROUND_80MIL">
</package>
<package name="1X16_2MM">
</package>
<package name="1X01_2MM">
</package>
<package name="2X08">
</package>
<package name="LLP40">
<description>40-LLP Package
&lt;p&gt;Source: http://cache.national.com/ds/DP/DP83848J.pdf&lt;/p&gt;</description>
</package>
<package name="OSC_7X5MM">
</package>
<package name="CFAF240320K-T-TS">
</package>
<package name="MICROSD">
<description>Courtesy: Adafruit Industries</description>
</package>
<package name="ILI9325_28INCH_TS">
<description>1.0mm-Pitch 37 Pin LCD Connector</description>
</package>
<package name="JSTPH6">
</package>
<package name="JSTPH3">
</package>
<package name="1X16_2MM_OVAL">
</package>
<package name="1X01_2MM_OVAL">
</package>
<package name="LQFP144">
<description>&lt;b&gt;Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="1X28_OVAL">
</package>
<package name="ARDUINO">
<description>&lt;b&gt;Arduino Diecimila/Duemilanove&lt;/b&gt;
&lt;p&gt;
Make a shield with ease, this package has all the named pins as well as the two mounting drill holes and an outline of the USB and DC power connector. The outline is on the DIMENSION layer, so if your board house uses it they will cut the outline to match.</description>
</package>
<package name="ARDUINO-NOHOLE">
</package>
<package name="ARDUINO-NODIM">
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL40_0.9">
</package>
<package name="OSC_3.2X2.5MM">
</package>
<package name="TFBGA180_0.8">
<description>&lt;b&gt;TFBGA180 (12.0x12.0mm, 0.8mm pitch, 0.45mm balls)&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Source&lt;/b&gt;: http://ics.nxp.com/products/lpc3000/datasheet/lpc3130.lpc3131.pdf&lt;/p&gt;
&lt;p&gt;Pad size is 0.34mm copper and ~0.5mm total with the solder mask (which should allow 6mil traces) as per the TFBGA180 recommendations in:&lt;/p&gt;
http://www.nxp.com/documents/application_note/AN10778.pdf</description>
</package>
<package name="TFBGA208_0.65">
<description>TFBGA180 (12.0x12.0mm, 0.65mm pitch, 0.4mm balls)
&lt;p&gt;Source: http://ics.nxp.com/products/lpc3000/datasheet/lpc3152.lpc3154.pdf&lt;/p&gt;
&lt;p&gt;Pad size is 0.25mm copper and ~0.37mm total with the solder mask as per the TFBGA208 recommendations in:&lt;/p&gt;
http://www.nxp.com/documents/application_note/AN10778.pdf</description>
</package>
<package name="VFBGA54">
<description>vFBGA180 (8mm x 9mm, 0.8mm pitch, 0.45mm balls)
&lt;p&gt;Source: http://download.micron.com/pdf/datasheets/dram/mobile/512mb_mobile_sdram_y47m.pdf&lt;/p&gt;
&lt;p&gt;Pad size is 0.34mm copper and ~0.5mm total with the solder mask (which should allow 6mil traces)&lt;/p&gt;</description>
</package>
<package name="QFN20_3MM">
<description>20-Lead Plastic QFN (3mm x 3mm, 20-pin 0.4mm pitch)
&lt;p&gt;Source: http://cds.linear.com/docs/Datasheet/3554fa.pdf&lt;/p&gt;</description>
</package>
<package name="TMLF-6">
<description>6-Pin 1.6mm x 1.6mm Thin MLF
&lt;p&gt;Source: http://www.micrel.com/_PDF/mic5387.pdf&lt;/p&gt;</description>
</package>
<package name="TSSOP5">
</package>
<package name="QFN24_4MM">
</package>
<package name="1X27_OVAL">
</package>
<package name="SOIC14">
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="1X27_ROUND">
</package>
<package name="MOUNTINGHOLE_3.0_PLATED">
</package>
<package name="JSTPH8">
</package>
<package name="0603-MINI">
<description>0603-Mini
&lt;p&gt;Mini footprint for dense boards&lt;/p&gt;</description>
</package>
<package name="PAD-1.5X2.0">
<description>1.5 x 2.0mm SMT pad (no solder paste)</description>
</package>
<package name="STX3100">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
KS-S stereo microphone/headphone jack&lt;p&gt;
 PG203JN (Schukat)</description>
</package>
<package name="USB-MINIB_LARGER">
</package>
<package name="ILI9325_28INCH_TS_OUTLINE">
</package>
<package name="SOIC20WIDE">
</package>
<package name="JSTSH2">
</package>
<package name="GE865">
</package>
<package name="GE864">
</package>
<package name="UG-9664HDDAG01">
<description>96x64 RGB OLED Display - 0.95" (25.7x22.2mm)</description>
</package>
<package name="HVQFN32-5X5">
<description>HVQFN32 5x5x0.85mm (0.5mm pitch)
&lt;p&gt;Reference: http://ics.nxp.com/support/design/microcontrollers/smart.metering/pdf/ol2381.datasheet.pdf&lt;/p&gt;</description>
</package>
<package name="MINIMOLD6">
<description>6-Pin MINIMOLD Leadless Part

&lt;p&gt;Reference: http://www.cel.com/pdf/datasheets/upd5713tk.pdf&lt;/p&gt;</description>
</package>
<package name="MOUNTINGHOLE_1.0_PLATED">
</package>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
<package name="ANT_868MHZ_SPLATCH">
</package>
<package name="USB_A-SMT">
<description>4UConnector: 10017</description>
</package>
<package name="BTN_KMR2_4.6X2.8">
</package>
<package name="2X15">
</package>
<package name="1X03_1.0MM">
</package>
<package name="1X04_1.0MM">
</package>
<package name="U.FL">
</package>
<package name="ILI9481_35INCH_OUTLINE">
</package>
<package name="TFBGA208_0.8">
<description>TFBGA208 (15.0x15.0mm, 0.8mm pitch, 0.45mm balls)
&lt;p&gt;Source: http://ics.nxp.com/packaging/package.outlines/pdf/sot950-1.pdf&lt;/p&gt;
&lt;p&gt;Pad size is 0.34mm copper and ~0.5mm total with the solder mask (which should allow 6mil traces) as per the recommendations in:&lt;/p&gt;
http://www.nxp.com/documents/application_note/AN10778.pdf</description>
</package>
<package name="1X05_1.27MM">
</package>
<package name="SOLDERJUMPER_CLOSEDWIRE">
</package>
<package name="TO263-5">
<description>Warning: Part outline is approximative</description>
</package>
<package name="SOLDERJUMPER_REFLOW_NOPASTE">
</package>
<package name="LGA14">
</package>
<package name="TSL2561_FN">
<description>2.0x2.0mm DFN (0.65mm pitch)</description>
</package>
<package name="QFN20_4MM">
<description>20-Lead QFN 4x4mm Body, 0.5mm pitch
&lt;p&gt;Source: http://ww1.microchip.com/downloads/en/DeviceDoc/22090b.pdf&lt;/p&gt;</description>
</package>
<package name="TSSOP20">
</package>
<package name="DCJACK_1.3MM_PTH">
</package>
<package name="DFN10_3X3MM">
<description>&lt;b&gt;10-Lead 3.3mm DFN&lt;/b&gt;
&lt;p&gt;Source: http://ww1.microchip.com/downloads/en/DeviceDoc/22005b.pdf&lt;/p&gt;</description>
</package>
<package name="BTN_EVQPQ_4.5MM">
</package>
<package name="SPDT_SMT_SSSS811101">
</package>
<package name="UG-9616GLBBG02">
<description>96x16 OLED Display - 0.84"/29.1x9.2mm</description>
</package>
<package name="UG-2832HSWEG04">
<description>128x32 OLED Display - 0.91" (30x11.5mm)</description>
</package>
<package name="UG-2832HSWEG04_WRAPAROUND">
</package>
<package name="MOUNTINGHOLE_3.0_PLATEDTHIN">
</package>
<package name="1X07_ROUND_76">
</package>
<package name="1X10_ROUND_76">
</package>
<package name="UG-9664HDDAG01_WRAPAROUND">
</package>
<package name="HVQFN32-5X5_3MMTHERMAL">
</package>
<package name="DFN14_4X3MM">
<description>&lt;b&gt;14-lead DFN (4.0x3.0mm)&lt;/b&gt;
&lt;p&gt;Source: http://cds.linear.com/docs/Datasheet/3581f.pdf&lt;/p&gt;</description>
</package>
<package name="UG-9616GLBBG02_WRAPAROUND">
</package>
<package name="1X05_ROUND_76">
</package>
<package name="1X11_ROUND_76">
</package>
<package name="UG-9664HDDAG01_WRAPAROUND_NOHOLES">
</package>
<package name="1X06_ROUND_76">
</package>
<package name="BMP085">
</package>
<package name="1X08_ROUND_76">
</package>
<package name="HMC5883L">
</package>
<package name="ITG3200_QFN24">
</package>
<package name="UG-9616GLBBG02_0.65MM_WRAPAROUND">
</package>
<package name="VCNL4000">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.vishay.com/docs/83798/vcnl4000.pdf</description>
</package>
<package name="1X04_ROUND_76">
</package>
<package name="1X09_ROUND_76">
</package>
<package name="HMC5883L_EXTENDED">
</package>
<package name="QFN28_5MM">
<description>&lt;p&gt;28-Pin 0.5mm pitch QFN (5.0x5.0mm)&lt;/p&gt;
&lt;b&gt;Source: &lt;/b&gt;http://www.allegromicro.com/en/Products/Part_Numbers/4983/4983.pdf</description>
</package>
<package name="TPS61029">
</package>
<package name="INDUCTOR_6X6MM_TDK_VLC6045">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.tdk.co.jp/tefe02/e531_vlc6045.pdf</description>
</package>
<package name="SPST_SMT_19192">
<description>&lt;b&gt;4UCON:&lt;/b&gt; 19192</description>
</package>
<package name="USB_HOST-PTH">
</package>
<package name="VFSOP-8">
<description>&lt;b&gt;VFSOP8&lt;/b&gt; - 0.5mm pitch, 2.0x2.3mm
&lt;p&gt;Source: http://focus.ti.com/lit/ds/symlink/txs0102.pdf&lt;/p&gt;</description>
</package>
<package name="BATTOUTLINE_LIPO2700MAH">
</package>
<package name="BATTOUTLINE_LIPO1300MAH">
</package>
<package name="ALTOIDSMINTS">
</package>
<package name="DPDT_SMT_JS202011SCQN">
</package>
<package name="2012">
</package>
<package name="FPC_XF2M-3015-1A">
<description>&lt;b&gt;30-Pin 0.5mm FPC&lt;/b&gt; Top+Bottom - OMRON - XF2M-3015-1A</description>
</package>
<package name="WLCSP16">
<description>&lt;h2&gt;WLCSP-16&lt;/h2&gt;2.17x3.32x0.6mm
&lt;br&gt;Wafer Level chip-size package</description>
</package>
<package name="1X03_ROUND_76">
</package>
<package name="FPC45PIN">
<description>&lt;b&gt;45-Pin 0.5mm Pitch Bottom Contacts&lt;/b&gt;&lt;br/&gt;
Digikey: 609-1196-1-ND</description>
</package>
<package name="EINK_10BAR">
</package>
<package name="SIM900_SMT">
</package>
<package name="CR1220">
</package>
<package name="C707_10M006_512_2">
<description>&lt;b&gt;C707A SIMLOCK® 2.5 mm with wide solder tails&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.amphenol.info/downloads/C707_10M006_512_2.pdf"&gt;Data sheet&lt;/a&gt;</description>
</package>
<package name="SOT363">
<description>&lt;b&gt;Source:&lt;/b&gt; http://www.nxp.com/documents/data_sheet/2N7002PS.pdf</description>
</package>
<package name="RESPACK_4X0603">
</package>
<package name="SC70-6L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="4UCONN_19269">
<description>&lt;br&gt;
4UCONN: 19269
&lt;br&gt;
4UCONN: 19268
&lt;br&gt;
4UCONN: 19267
&lt;br&gt;
http://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19267&amp;seriesno_a=18</description>
</package>
<package name="SIM_5002">
<description>6 Contacts (3+3), low profile &lt;br&gt;
drawn by  DeSIG &lt;br&gt; desig@radikaldesig.com</description>
</package>
<package name="1X12_ROUND_76MIL">
</package>
<package name="SIM900B_SMT">
<description>SIM900B - 60 Pin B2B Connector</description>
</package>
<package name="4UCONN_19621_SPARK">
</package>
<package name="4UCONN_19621">
</package>
<package name="SOLDERJUMPER_CLOSEDPERM">
</package>
<package name="4UCONN_05550">
</package>
<package name="FPC_10PIN_52892-1095">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.molex.com/pdm_docs/sd/528921095_sd.pdf</description>
</package>
<package name="1X09_ROUND_70">
</package>
<package name="SOIC8_208MIL">
<description>&lt;b&gt;Small Outline IC - 208mil Wide&lt;/b&gt;</description>
</package>
<package name="INDUCTOR_6X6MM_TDK_SLF6045">
<description>&lt;b&gt;Source: &lt;/b&gt; http://www.tdk.co.jp/tefe02/e531_slf6045.pdf</description>
</package>
<package name="INDUCTOR_5X5MM_TDK_VLC5045">
<description>&lt;b&gt;Source: http://www.tdk.co.jp/tefe02/e531_vlc5045.pdf&lt;/b&gt;</description>
</package>
<package name="SOCKET_LBGA256_8117-256-4E-01">
<description>&lt;p&gt;&lt;b&gt;Wells 8117-256-4E-01 LBGA 256 socket&lt;/b&gt;&lt;/p&gt;
LBGA256 ... pitch is 1 mm / diameter pin = 0.43 mm</description>
</package>
<package name="LBGA256_1.0MM">
<description>&lt;b&gt;LBGA256 - SOT740-2 &lt;/b&gt;&lt;p&gt;
LBGA256: plastic low profile ball grid array package; 256 balls; body 17 x 17 x 1 mm</description>
</package>
<package name="LQFP208">
</package>
<package name="SEGMENT_BICOL_BL-M12A883XX">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.betlux.com/product/led_dot_matrix/BL-M12A883xx.PDF</description>
</package>
<package name="SEGMENT_BL-M07C881UR">
</package>
<package name="SEGMENT_BL-M12A881UR">
<description>&lt;b&gt;Source:&lt;/b&gt; http://www.betlux.com/product/LED_dot_matrix/BL-M12A881.PDF</description>
</package>
<package name="SEGMENT_BL-M12A883">
<description>&lt;b&gt;Source:&lt;/b&gt; http://www.betlux.com/product/LED_dot_matrix/BL-M12A883.PDF</description>
</package>
<package name="SEGMENT_BICOL_BL-AR12Z3010">
<description>&lt;b&gt;Souce: &lt;/b&gt;http://www.betlux.com/product/LED_light_bar/BL-AR12B3010xx.PDF</description>
</package>
<package name="SEGMENT_STARBURST_BL-S80A-13">
</package>
<package name="SEGMENT_STARBURST_BL-S230B-12">
</package>
<package name="BEAGLEBONE_SHIELD">
</package>
<package name="2X23">
</package>
<package name="1X06_ROUND_70">
</package>
<package name="1X08_ROUND_70">
</package>
<package name="1X07_ROUND_70">
</package>
<package name="1X23_ROUND_70MIL">
</package>
<package name="BREAKOUT_SOIC24">
</package>
<package name="BREAKOUT_SOT23-6">
</package>
<package name="BREAKOUT_SOIC8">
</package>
<package name="MSOP8_0.65MM">
<description>&lt;b&gt;Source: http://www.intersil.com/data/fn/fn7833.pdf&lt;/b&gt;</description>
</package>
<package name="TFBGA100_0.8">
<description>&lt;b&gt;TFBGA100 (9.0x9.0mm, 0.8mm pitch, 0.45mm balls)&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Source&lt;/b&gt;: http://www.nxp.com/documents/data_sheet/LPC1850_30_20_10.pdf&lt;/p&gt;
&lt;p&gt;Pad size is 0.34mm copper and ~0.5mm total with the solder mask (which should allow 6mil traces) as per the TFBGA100 recommendations in:&lt;/p&gt;
http://www.nxp.com/documents/application_note/AN10778.pdf</description>
</package>
<package name="HVQFN64">
</package>
<package name="HDMI_MOLEX_47151-0001">
</package>
<package name="HVQFN32">
<description>&lt;b&gt;HVQFN32&lt;/b&gt;&lt;br&gt;
SOT617-1&lt;br&gt;
JEDEC MO-220</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="ARDUINOR3">
<description>The new Arduino R3 'classic' adds duplicate I2C pins and an IORef pin (and an unused pin</description>
</package>
<package name="ARDUINOR3-BPLACE">
</package>
<package name="ARDUINOR3-NODIM">
</package>
<package name="1X10_ROUND70">
</package>
<package name="FGPMMOPA6B">
</package>
<package name="SIM908">
</package>
<package name="ADAFRUIT_16MM">
</package>
<package name="ADAFRUIT_30MM">
</package>
<package name="ADAFRUIT_9MM">
</package>
<package name="ADAFRUIT_5MM">
</package>
<package name="ADAFRUIT_2.5MM">
</package>
<package name="ADAFRUIT_TEXT_30MM">
</package>
<package name="ADAFRUIT_TEXT_20MM">
</package>
<package name="BUS_I2C_5MM">
</package>
<package name="BUS_SPI_5MM">
</package>
<package name="BUS_ADC_5MM">
</package>
<package name="LOGIC_5V_5MM">
</package>
<package name="LOGIC_3.3V_5MM">
</package>
<package name="POWER_3.3-5.0V_5MM">
</package>
<package name="2X03_ROUND_70MIL">
</package>
<package name="BTL221722-276L">
</package>
<package name="BLUETOOTH_MODULE">
</package>
<package name="1X17_ROUND70">
</package>
<package name="SOT23-WIDE">
</package>
<package name="ADAFRUIT_3.5MM">
</package>
<package name="UG-2832HSWEG02_WRAPUNDER">
</package>
<package name="TSSOP28">
</package>
<package name="3X08">
</package>
<package name="TERMBLOCK_1X2-3.5MM">
</package>
<package name="TSL13T">
</package>
<package name="1X05_ROUND_70">
</package>
<package name="QSOP24_0.635MM">
</package>
<package name="DIL28_600MIL">
<description>&lt;B&gt;28-Pin Dual In Line (600 mil)&lt;/B&gt;</description>
</package>
<package name="FGPMMOPA6C">
</package>
<package name="SEGMENT_BL-Q39A-42">
</package>
<package name="INDUCTOR_5X5MM_TDK_VLC5045_NOTHERMALS">
</package>
<package name="JSTPH2_NOTHERMALS">
</package>
<package name="0805_NOTHERMALS">
</package>
<package name="L3G4200D_LGA16L">
</package>
<package name="JD-T1800">
</package>
<package name="LOGIC_5VREADY_5MM">
</package>
<package name="3X04">
</package>
<package name="MOUNTINGHOLE_2.5_PLATED">
</package>
<package name="RASBERRYPI_SHIELD">
</package>
<package name="2X13">
</package>
<package name="UG-2864HSWEG01_1.3_WRAPAROUND">
</package>
<package name="SWITCH_4WAY_TPA511GLFS">
</package>
<package name="SOP20_300MIL">
</package>
<package name="SOP24_300MIL">
</package>
<package name="SOP28_300MIL">
</package>
<package name="TO263-5_NOPASTE">
</package>
<package name="INDUCTOR_5X5MM_NR5040_NOTHERMALS">
</package>
<package name="SEGMENT-BL-Q56C43">
</package>
<package name="TEA5767MODULE">
</package>
<package name="HB100">
</package>
<package name="SOT23-8">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.ti.com/lit/ml/mpds099c/mpds099c.pdf</description>
</package>
<package name="FGPMMOPA6H">
</package>
<package name="UG-2864HSWEG01_0.96IN_WRAPAROUND">
</package>
<package name="FH26-17S-0.3SHW">
<description>Source: http://www.hirose.co.jp/cataloge_hp/e58302093.pdf</description>
</package>
<package name="ADBM-A350">
<description>ADBM-A350 - Outline Only</description>
</package>
<package name="SOLDERJUMPER_2WAY_OPEN_NOPASTE">
</package>
<package name="SOLDERJUMPER_2WAY_OPEN_0603">
</package>
<package name="SOLDERJUMPER_2WAY_OPEN_0805">
</package>
<package name="TESTPOINT_ROUND_1MM">
</package>
<package name="WQFN16">
<description>&lt;p&gt;16-PWQFN 3.0x3.0mm&lt;/p&gt;
&lt;b&gt;Source&lt;/b&gt;: http://www.ti.com/lit/ds/symlink/ads7924.pdf</description>
</package>
<package name="2512">
<description>&lt;b&gt;RESISTOR 2512 (Metric 6432)&lt;/b&gt;</description>
</package>
<package name="S6B33B6_1.5IN_LCD">
<description>&lt;p&gt;Mystery 1.5" S6B33B6X TFT LCD&lt;/p&gt;
&lt;p&gt;BAsed on manual measurements with a caliper since no mechanical diagram was available, but should be relatively close.&lt;/p&gt;</description>
</package>
<package name="WQFN20">
<description>&lt;p&gt;20-PWQFN 4.0x4.0mm 0.5mm pitch&lt;/p&gt;
&lt;b&gt;Source&lt;/b&gt;: http://www.ti.com/lit/ds/symlink/tpa2012d2.pdf</description>
</package>
<package name="SI473X_SSOP">
<description>&lt;b&gt;Source:&lt;/b&gt;  http://www.silabs.com/Support%20Documents/TechnicalDocs/Si4730-31-34-35-D60.pdf</description>
</package>
<package name="HTSSOP16">
<description>&lt;p&gt;HTSSOP 16 (5x4.4mm 0.65mm Pitch)&lt;/p&gt;
&lt;p&gt;Source: http://www.ti.com/lit/ds/slvsar1b/slvsar1b.pdf&lt;/p&gt;</description>
</package>
<package name="SOLDERJUMPER_ARROW_NOPASTE">
</package>
<package name="WFDFN-14">
<description>&lt;p&gt;14-WFDFN 3x3mm 0.4mm Pitch&lt;/p&gt;
&lt;b&gt;Source: &lt;/b&gt; http://datasheets.maxim-ic.com/en/ds/MAX9814.pdf</description>
</package>
<package name="TESTPOINT_ROUND_0.5MM">
</package>
<package name="SMB_DIP">
</package>
<package name="1X13_ROUND_70">
</package>
<package name="CELEC_3.5MM_8MM">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="CELEC_3.5MM_10MM">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="TERMBLOCK_1X3-3.5MM">
</package>
<package name="LGA8">
<description>&lt;b&gt;LGA8 3x5mm 1.25mm Pitch&lt;/b&gt;
&lt;p&gt;Source: http://www.freescale.com/files/sensors/doc/data_sheet/MPL115A2.pdf&lt;/p&gt;</description>
</package>
<package name="SDCARD_SMT_4U19646">
<description>&lt;b&gt;Push/Pull SD Connector - 4U 19646&lt;/b&gt;</description>
</package>
<package name="RASBERRYPI_IDC">
</package>
<package name="TDFN14_3X3MM">
<description>&lt;b&gt;TDFN 14 3x3x0.75mm&lt;/b&gt;
&lt;p&gt;Source: http://datasheets.maxim-ic.com/en/ds/MAX98306.pdf&lt;/p&gt;
&lt;p&gt;Based on recommendtions in: http://www.freescale.com/files/sensors/doc/data_sheet/MAG3110.pdf&lt;/p&gt;</description>
</package>
<package name="CRYSTAL_8X3.8">
<description>&lt;p&gt;8.0x3.8x2.5mm SMT Crystal&lt;/p&gt;
&lt;p&gt;Source: http://www.abracon.com/Resonators/abs25.pdf&lt;/p&gt;</description>
</package>
<package name="1X15_ROUND_70">
</package>
<package name="BMI-S-209-F">
<description>&lt;b&gt;SURFACE MOUNT SHIELD FRAME&lt;/b&gt;&lt;p&gt;
Mates with cover part# BMI-S-209-C</description>
</package>
<package name="_0402">
<description>&lt;b&gt; 0402&lt;/b&gt;</description>
</package>
<package name="_0402MP">
<description>&lt;b&gt;0402 MicroPitch&lt;p&gt;</description>
</package>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
<package name="_0603MP">
<description>&lt;b&gt;0603 MicroPitch&lt;/b&gt;</description>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
<package name="_0805MP">
<description>&lt;b&gt;0805 MicroPitch&lt;/b&gt;</description>
</package>
<package name="SOT886">
<description>SOT-886&lt;br&gt;&lt;br&gt;
Source: PRTR5V0U2F</description>
</package>
<package name="SOT833-1">
<description>Source: http://ics.nxp.com/packaging/package.outlines/pdf/sot833-1.pdf</description>
</package>
<package name="QFN32_5MM">
<description>&lt;p&gt;QFN32 5x5mm 0.5mm pitch&lt;/p&gt;
&lt;b&gt;Source:&lt;/b&gt; Nordic nRF8001 Product Specification</description>
</package>
<package name="BALUN0603">
</package>
<package name="CRYSTAL_2.5X2">
</package>
<package name="BMC050">
</package>
<package name="BMC050_EXTENDED">
</package>
<package name="DIRECTION_BIDIR">
</package>
<package name="DIRECTION_IN">
</package>
<package name="DIRECTION_OUT">
</package>
<package name="BMI-S-202-F">
<description>&lt;b&gt;SURFACE MOUNT SHIELD FRAME&lt;/b&gt;&lt;p&gt;
Mates with cover part# BMI-S-202-C</description>
</package>
<package name="SOP8-1351">
<description>&lt;b&gt;SOP 8  (CASE 1351-01)&lt;/b&gt;
&lt;p&gt;Footprint: Bob Starr&lt;/p&gt;</description>
</package>
<package name="SOP8-1369">
<description>&lt;b&gt;SOP 8  (CASE 1369-01)&lt;/b&gt;
&lt;p&gt;Footprint: Bob Starr&lt;/p&gt;</description>
</package>
<package name="LGA16_5X5MM">
<description>&lt;b&gt;LGA-16&lt;p&gt;&lt;/b&gt;
body 5x5x1.5mm</description>
</package>
<package name="LGA16_3X3MM">
</package>
<package name="QFN16_3MM">
</package>
<package name="SDCARD_PCBCARRIER_DIM">
<description>&lt;p&gt;SD Card outline using the dimension layer&lt;/p&gt;
&lt;p&gt;Source: SD Card Standard v1.9&lt;/p&gt;</description>
</package>
<package name="SDCARD_PCBCARRIER_DOCU">
</package>
<package name="MOUNTINGHOLE_2.5_PLATED_THICK">
</package>
<package name="CHIPLED_0805_NOOUTLINE">
</package>
<package name="CHIPLED_0603_NOOUTLINE">
</package>
<package name="SYMBOL_GYROXYZ_10MM">
</package>
</packages>
<symbols>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="CAPACITOR">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="CAPACITOR_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="3.3V">
<pin name="3.3V" direction="sup"/>
</symbol>
<symbol name="5.0V">
<pin name="5.0V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="LM1117">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="PUSHBUTTON">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="FT232RL">
<pin name="USB+"/>
<pin name="USB-"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="DTR"/>
<pin name="VCC" direction="pwr"/>
<pin name="3V3OUT" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="TXLED"/>
<pin name="RXLED"/>
<pin name="TEST" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
</symbol>
<symbol name="GPS_LS20031">
<pin name="VCC" direction="pwr"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
</symbol>
<symbol name="LED">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ID"/>
</symbol>
<symbol name="DCBARREL">
<pin name="PWR" direction="pwr"/>
<pin name="GNDBREAK" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="JTAG-ARM">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="LPC2144/2146/2148">
<pin name="P0.0/TXD0/PWM1"/>
<pin name="P0.1/RXD0/PWM3/EINT0"/>
<pin name="P0.2/SCL0/CAP0.0"/>
<pin name="P0.4/SCK0/CAP0.1/AD0.6"/>
<pin name="P0.5/MISO0/MAT0.1/AD0.7"/>
<pin name="P0.6/MOSI0/CAP0.2/AD1.0"/>
<pin name="P0.7/SSEL0/PWM2/EINT2"/>
<pin name="P0.3/SDA0/MAT0.0/EINT1"/>
<pin name="P0.8/TXD1/PWM4/AD1.1"/>
<pin name="P0.9/RXD1/PWM6/EINT3"/>
<pin name="P0.10/RTS1/CAP1.0/AD1.2"/>
<pin name="P0.12/DSR1/MAT1.0/AD1.3"/>
<pin name="P0.11/CTS1/CAP1.1/SCL1"/>
<pin name="P0.13/DTR1/MAT1.1/AD1.4"/>
<pin name="P0.14/DCD1/EINT1/SDA1"/>
<pin name="P0.15/RI1/EINT2/AD1.5"/>
<pin name="P0.16/EINT0/MAT0.2/CAP0.2"/>
<pin name="P0.17/CAP1.2/SCK1/MAT1.2"/>
<pin name="P0.18/CAP1.3/MISO1/MAT1.3"/>
<pin name="P0.19/MAT1.2/MOSI1/CAP1.2"/>
<pin name="P0.20/MAT1.3/SSEL1/EINT3"/>
<pin name="P0.22/AD1.7/CAP0.0/MAT0.0"/>
<pin name="P0.21/PWM5/AD1.6/CAP1.3"/>
<pin name="P0.23/VBUS"/>
<pin name="!RESET" direction="in"/>
<pin name="P0.25/AD0.4/AOUT"/>
<pin name="D+"/>
<pin name="P0.28/AD0.1/CAP0.2/MAT0.2"/>
<pin name="D-"/>
<pin name="P0.29/AD0.2/CAP0.3/MAT0.3"/>
<pin name="P0.30/AD0.3/EINT3/CAP0.0"/>
<pin name="P0.31/UP_LED/CONNECT"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="RTXC1" direction="in"/>
<pin name="RTXC2" direction="out"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="P1.16/TRACEPKT0"/>
<pin name="P1.17/TRACEPKT1"/>
<pin name="P1.18/TRACEPKT2"/>
<pin name="P1.19/TRACEPKT3"/>
<pin name="P1.20/TRACESYNC"/>
<pin name="P1.21/PIPESTAT0"/>
<pin name="P1.22/PIPESTAT1"/>
<pin name="P1.23/PIPESTAT2"/>
<pin name="P1.24/TRACECLK"/>
<pin name="P1.25/EXTIN0"/>
<pin name="P1.26/RTCK"/>
<pin name="P1.27/TDO"/>
<pin name="P1.28/TDI"/>
<pin name="P1.29/TCK"/>
<pin name="P1.30/TMS"/>
<pin name="P1.31/!TRST"/>
</symbol>
<symbol name="LPC2103">
<pin name="P0.19/MAT1.2/MISO1"/>
<pin name="P0.20/MAT1.3/MOSI1"/>
<pin name="P0.21/SSEL1/P0.21"/>
<pin name="VBAT"/>
<pin name="VDD1.8(CORE)"/>
<pin name="RST" function="dot"/>
<pin name="VSS1"/>
<pin name="P0.27/CAP2.0/TRST"/>
<pin name="P0.28/CAP2.1/TMS"/>
<pin name="P0.29/CAP2.2/TCK"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="P0.0/MAT3.1/TXD0"/>
<pin name="P0.1/MAT3.2/RXD0"/>
<pin name="P0.30/MAT3.3/TDI"/>
<pin name="P0.31/TDO"/>
<pin name="VDD3-2(I/O)"/>
<pin name="P0.2/SCL/CAP0.0"/>
<pin name="VSS2"/>
<pin name="RTXC1"/>
<pin name="P0.3/SDA/MAT0.0"/>
<pin name="P0.4/SCK/CAP0.1"/>
<pin name="P0.5/MISO/MAT0.1"/>
<pin name="P0.6/MOSI/CAP0.2"/>
<pin name="RTXC2"/>
<pin name="RTCK"/>
<pin name="DBGSEL"/>
<pin name="P0.7/SSEL/MAT2.0"/>
<pin name="P0.8/TXD1/MAT2.1"/>
<pin name="P0.9/RXD1/MAT2.2"/>
<pin name="VSSA"/>
<pin name="P0.22/AIN0"/>
<pin name="P0.23/AIN1"/>
<pin name="P0.24/AIN2"/>
<pin name="P0.10/CAP1.0/AIN3/RTS1"/>
<pin name="P0.11/CAP1.1/AIN4/CTS1"/>
<pin name="P0.12/MAT1.0/AIN5/DSR1"/>
<pin name="P0.25/AIN6"/>
<pin name="P0.26/AIN7"/>
<pin name="VDD3-1(I/O)"/>
<pin name="P0.13/MAT1.1/DTR1"/>
<pin name="VDDA"/>
<pin name="VSS4"/>
<pin name="P0.14/EINT1/SCK1/DCD1"/>
<pin name="P0.15/EINT2/RI1"/>
<pin name="P0.16/EINT0/MAT0.2"/>
<pin name="PO0.17/CAP1.2/SCL1"/>
<pin name="P0.18/CAP1.3/SDA1"/>
</symbol>
<symbol name="SOLDERJUMPER">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="JUMPER2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JUMPER3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="FRAME_A4">
</symbol>
<symbol name="HEADER_1X02">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="ADXL335">
<pin name="VS1"/>
<pin name="VS2"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="X"/>
<pin name="Y"/>
<pin name="Z"/>
<pin name="TEST"/>
</symbol>
<symbol name="POTENTIOMETER">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="DSTOUCHCON">
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="ENC28J60">
<pin name="RESET"/>
<pin name="CS"/>
<pin name="VDD_OSC"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="VSS_OSC"/>
<pin name="VDD"/>
<pin name="VDD_PLL"/>
<pin name="VDD_RX"/>
<pin name="VDD_TX"/>
<pin name="RBIAS"/>
<pin name="VCAP"/>
<pin name="VSS"/>
<pin name="VSS_PLL"/>
<pin name="VSS_RX"/>
<pin name="VSS_TX"/>
<pin name="LEDA"/>
<pin name="LEDB"/>
<pin name="TPIN+"/>
<pin name="TPIN-"/>
<pin name="TPOUT+"/>
<pin name="TPOUT-"/>
<pin name="SCK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="WOL"/>
<pin name="INT"/>
<pin name="CLKOUT"/>
</symbol>
<symbol name="PINHD10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X16">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD16">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
<symbol name="MOSFET-N">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="CD74HC4067">
<pin name="CH0"/>
<pin name="CH1"/>
<pin name="CH2"/>
<pin name="CH3"/>
<pin name="CH4"/>
<pin name="CH5"/>
<pin name="CH6"/>
<pin name="CH7"/>
<pin name="CH8"/>
<pin name="CH9"/>
<pin name="CH10"/>
<pin name="CH11"/>
<pin name="CH12"/>
<pin name="CH13"/>
<pin name="CH14"/>
<pin name="CH15"/>
<pin name="COM"/>
<pin name="SEL0"/>
<pin name="SEL1"/>
<pin name="SEL2"/>
<pin name="SEL3"/>
<pin name="EN" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="MC34063ADR">
<pin name="S_COL"/>
<pin name="S_EMIT"/>
<pin name="TCAP"/>
<pin name="GND"/>
<pin name="CII"/>
<pin name="VCC"/>
<pin name="IPK"/>
<pin name="D_COL"/>
</symbol>
<symbol name="CD74HC4052">
<pin name="CH-A0"/>
<pin name="CH-A1"/>
<pin name="CH-A2"/>
<pin name="CH-A3"/>
<pin name="CH-B0"/>
<pin name="CH-B1"/>
<pin name="CH-B2"/>
<pin name="CH-B3"/>
<pin name="SEL0"/>
<pin name="SEL1"/>
<pin name="EN" function="dot"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="COM-A"/>
<pin name="COM-B"/>
<pin name="VEE"/>
</symbol>
<symbol name="MCP73833">
<pin name="VDD2"/>
<pin name="STAT1"/>
<pin name="STAT2"/>
<pin name="PG"/>
<pin name="GND"/>
<pin name="PROG"/>
<pin name="THERM"/>
<pin name="VBAT1"/>
<pin name="VDD1"/>
<pin name="VBAT2"/>
</symbol>
<symbol name="ALLEGRO3967">
<pin name="REF" direction="in"/>
<pin name="RC1" direction="in"/>
<pin name="RC2" direction="in"/>
<pin name="PFD" direction="in"/>
<pin name="!SLEEP" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="SENSE1" direction="in"/>
<pin name="SENSE2" direction="in"/>
<pin name="STEP" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="!ENABLE" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="LOAD-SUPPLY1" direction="in"/>
<pin name="LOAD-SUPPLY2" direction="in"/>
<pin name="OUT1A" direction="out"/>
<pin name="OUT1B" direction="out"/>
<pin name="OUT2A" direction="out"/>
<pin name="OUT2B" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="DIPSWITCH_2">
<pin name="1A"/>
<pin name="2A"/>
<pin name="1B"/>
<pin name="2B"/>
</symbol>
<symbol name="TESTPOINT">
<pin name="P$1"/>
</symbol>
<symbol name="PSP_TOUCHCON">
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="PSP_BACKLIGHTCON">
<pin name="VLED-" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="VLED+" direction="pwr"/>
</symbol>
<symbol name="PSP_LCDCON">
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="VCC1(2.5V)" direction="pwr"/>
<pin name="VCC2(2.5V)" direction="pwr"/>
<pin name="R0(LSB)" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="R3" direction="in"/>
<pin name="R4" direction="in"/>
<pin name="R5" direction="in"/>
<pin name="R6" direction="in"/>
<pin name="R7(MSB)" direction="in"/>
<pin name="G0(LSB)" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="G2" direction="in"/>
<pin name="G3" direction="in"/>
<pin name="G4" direction="in"/>
<pin name="G5" direction="in"/>
<pin name="G6" direction="in"/>
<pin name="G7(MSB)" direction="in"/>
<pin name="B0(LSB)" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B7(MSB)" direction="in"/>
<pin name="GND3" direction="pwr"/>
<pin name="CK"/>
<pin name="DISP"/>
<pin name="HSYNC"/>
<pin name="VSYNC"/>
<pin name="NC1" direction="nc"/>
<pin name="AVDD1(5V)"/>
<pin name="AVVD2(5V)"/>
<pin name="NC2" direction="nc"/>
<pin name="TEST1(OPEN)"/>
<pin name="TEST2(GND)"/>
<pin name="TEST3(GND)"/>
</symbol>
<symbol name="2.5V">
<pin name="2.5V" direction="sup"/>
</symbol>
<symbol name="1.8V">
<pin name="1.8V" direction="sup"/>
</symbol>
<symbol name="TCS3414">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SYNC"/>
<pin name="VDD"/>
<pin name="INT"/>
<pin name="GND"/>
</symbol>
<symbol name="TSL2561">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="INT"/>
<pin name="ADDRSEL"/>
<pin name="3.3V"/>
<pin name="GND"/>
</symbol>
<symbol name="STANDARDCONNECTOR">
<pin name="SPI_CS"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="I2C_SCL"/>
<pin name="I2C_SDA"/>
<pin name="INT1"/>
<pin name="INT2"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="ADC1"/>
<pin name="ADC2"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="VCC3.3V"/>
<pin name="VCC5.0V"/>
</symbol>
<symbol name="ADP1712">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="ADJ"/>
<pin name="EN"/>
<pin name="GND"/>
</symbol>
<symbol name="ADP121">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="EN"/>
<pin name="GND"/>
</symbol>
<symbol name="TPS851">
<pin name="VCC"/>
<pin name="AOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="LM75B">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OS"/>
</symbol>
<symbol name="LPC175X">
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="VDD(3V3)3" direction="pwr"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)2" direction="pwr"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREFP" direction="in"/>
<pin name="RSTOUT" direction="out"/>
<pin name="VREFN" direction="in"/>
<pin name="RTCX1" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="RTCX2" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="P0[30]/USB_DMIN"/>
<pin name="VSS1" direction="pwr"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MCOA0/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCI0/PWM1[2]/SCK0"/>
<pin name="P1[22]/MCOB0/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCI1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCI2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MCOA1/MAT1[1]"/>
<pin name="P1[26]/MCOB1/PWM1[6]/CAP0[0]"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD(REG)(3V3)1" direction="pwr"/>
<pin name="P1[28]/MCOA2/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MCOB2/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="VSS3" direction="pwr"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2/ENET_MDIO"/>
<pin name="P2[8]/TD2/TXD2/ENET_MDC"/>
<pin name="P2[7]/RD2/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="VDDA" direction="pwr"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="VSS4" direction="pwr"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
<pin name="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
<pin name="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
<pin name="VSS5" direction="pwr"/>
<pin name="VDD(REG)(3V3)2" direction="pwr"/>
<pin name="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
<pin name="P1[15]/ENET_REF_CLK"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[8]/ENET_CRS"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="VDD(3V3)4" direction="pwr"/>
<pin name="VSS6" direction="pwr"/>
<pin name="TDO/SWO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDD(3V3)1" direction="pwr"/>
<pin name="P0[29]/USB_DPLUS"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="TCK/SWDCLK"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
<pin name="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
</symbol>
<symbol name="MCP130T">
<pin name="RST"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LEDRGB_PLCC6">
<pin name="RED"/>
<pin name="GRN"/>
<pin name="BLUE"/>
<pin name="RGND" direction="pwr"/>
<pin name="GGND" direction="pwr"/>
<pin name="BGND" direction="pwr"/>
</symbol>
<symbol name="LPC1313FBD48">
<pin name="PIO2_6"/>
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_1/DSR"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO3_4"/>
<pin name="PIO2_4"/>
<pin name="PIO2_5"/>
<pin name="PIO3_5"/>
<pin name="PIO0_6/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_2/DCD"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO2_11/SCK"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="PIO3_0"/>
<pin name="PIO3_1"/>
<pin name="PIO2_3/RI"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO3_3"/>
</symbol>
<symbol name="LPC1313FHN33">
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO3_4"/>
<pin name="PIO3_5"/>
<pin name="PIO0_6/SCK"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LPC1343FHN33">
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO0_6/USB_CONNECT/SCK"/>
<pin name="PIO0_7(20MA)/CTS"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="LPC1343FBD48">
<pin name="PIO2_6"/>
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE"/>
<pin name="VSSIO" direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_1/DSR"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO2_4"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO2_5"/>
<pin name="PIO0_6/USB_CONNECT/SCK"/>
<pin name="PIO0_7(20MA)/CTS"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_2/DCD"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO2_11/SCK"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="PIO3_0"/>
<pin name="PIO3_1"/>
<pin name="PIO2_3/RI"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO3_3"/>
</symbol>
<symbol name="JTAG-CORTEXM3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="XBEE">
<pin name="VCC" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN/!CONFIG" direction="in"/>
<pin name="CD/DOUT_EN/DO8" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="PWM0/RSSI" direction="out"/>
<pin name="!DTR!/SLEEP_RQ/DI8"/>
<pin name="GND" direction="pwr"/>
<pin name="RF_TX/AD4/DIO4"/>
<pin name="!CTS!/DIO7"/>
<pin name="ON/!SLEEP" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="ASSOC/AD5/DIO5"/>
<pin name="!RTS!/AD6/DIO6"/>
<pin name="COORD_SEL/AD3/DIO3"/>
<pin name="AD2/DIO2"/>
<pin name="AD1/DIO1"/>
<pin name="AD0/DIO0"/>
</symbol>
<symbol name="MAX6364">
<pin name="VCC" direction="pwr"/>
<pin name="RSTIN"/>
<pin name="BATT"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET"/>
<pin name="OUT"/>
</symbol>
<symbol name="BATTERY">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="SDCARD">
<pin name="DATA3/CS"/>
<pin name="CMD/MOSI"/>
<pin name="VSS1"/>
<pin name="VDD"/>
<pin name="CLK/SCK"/>
<pin name="VSS2"/>
<pin name="DATA0/MISO"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="CARDDETECT"/>
<pin name="WRITEPROTECT"/>
<pin name="GND"/>
</symbol>
<symbol name="FRAME_A3">
</symbol>
<symbol name="NCP1400A">
<pin name="CE"/>
<pin name="OUT"/>
<pin name="NC"/>
<pin name="LX"/>
<pin name="GND"/>
</symbol>
<symbol name="MIC5320">
<pin name="VIN"/>
<pin name="EN1"/>
<pin name="EN2"/>
<pin name="VOUT1"/>
<pin name="VOUT2"/>
<pin name="GND"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="BAT54C">
<pin name="A1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="LPC1114_QFP">
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="VSS(IO)" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD(3.3V)" direction="pwr"/>
<pin name="RESET/PIO0_0"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="PIO0_3"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO2_0/DTR/SSEL1"/>
<pin name="PIO2_1/DSR/SCK1"/>
<pin name="PIO2_2/DCD/MISO1"/>
<pin name="PIO2_3/RI/MOSI1"/>
<pin name="PIO2_4"/>
<pin name="PIO2_5"/>
<pin name="PIO2_6"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_11/SCK0"/>
<pin name="PIO3_0/DTR"/>
<pin name="PIO3_1/DSR"/>
<pin name="PIO3_2/DCD"/>
<pin name="PIO3_3/RI"/>
<pin name="PIO3_4"/>
<pin name="PIO3_5"/>
</symbol>
<symbol name="PTC">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="2.8V">
<pin name="2.8V" direction="sup"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="sup"/>
</symbol>
<symbol name="PINHD20">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="MT48LC4M16A2P">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="BA0"/>
<pin name="BA1"/>
<pin name="DQML"/>
<pin name="DQMH"/>
<pin name="CS" function="dot"/>
<pin name="WE" function="dot"/>
<pin name="CAS" function="dot"/>
<pin name="RAS" function="dot"/>
<pin name="CLK" function="clk"/>
<pin name="CKE"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="DQ9"/>
<pin name="DQ10"/>
<pin name="DQ11"/>
<pin name="DQ12"/>
<pin name="DQ13"/>
<pin name="DQ14"/>
<pin name="DQ15"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDD3"/>
<pin name="VDDQ1"/>
<pin name="VDDQ2"/>
<pin name="VDDQ3"/>
<pin name="VDDQ4"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSSQ1"/>
<pin name="VSSQ2"/>
<pin name="VSSQ3"/>
<pin name="VSSQ4"/>
<pin name="NC2"/>
<pin name="NC1"/>
</symbol>
<symbol name="LPC2478">
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="P0[2]/TXD0"/>
<pin name="P0[3]/RXD0"/>
<pin name="P0[4]/I2SRX_CLK/LCDVD[0]/RD2/CAP2[0]"/>
<pin name="P0[5]/I2SRX_WS/LCDVD[1]/TD2/CAP2[1]"/>
<pin name="P0[6]/I2SRX_SDA/LCDVD[8]/SSEL1/MAT2[0]"/>
<pin name="P0[7]/I2STX_CLK/LCDVD[9]/SCK1/MAT2[1]"/>
<pin name="P0[8]/I2STX_WS/LCDVD[16]/MISO1/MAT2[2]"/>
<pin name="P0[9]/I2STX_SDA/LCDVD[17]/MOSI1/MAT2[3]"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P0[12]/USB_PPWR2/MISO1/AD0[6]"/>
<pin name="P0[13]/USB_UP_LED2/MOSI1/AD0[7]"/>
<pin name="P0[14]/USB_HSTEN2/USB_CONNECT2/SSEL1"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[19]/DSR1/MCICLK/SDA1"/>
<pin name="P0[20]/DTR1/MCICMD/SCL1"/>
<pin name="P0[21]/RI1/MCIPWR/RD1"/>
<pin name="P0[22]/RTS1/MCIDAT0/TD1"/>
<pin name="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]"/>
<pin name="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="P0[27]/SDA0"/>
<pin name="P0[28]/SCL0"/>
<pin name="P0[29]/USB_D+1"/>
<pin name="P0[30]/USB_D-1"/>
<pin name="P0[31]/USB_D+2"/>
<pin name="USB_D-2"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[2]/ENET_TXD2/MCICLK/PWM0[1]"/>
<pin name="P1[3]/ENET_TXD3/MCICMD/PWM0[2]"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[5]/ENET_TX_ER/MCIPWR/PWM0[3]"/>
<pin name="P1[6]/ENET_TX_CLK/MCIDAT0/PWM0[4]"/>
<pin name="P1[7]/ENET_COL/MCIDAT1/PWM0[5]"/>
<pin name="P1[8]/ENET_CRS_DV/ENET_CRS"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[11]/ENET_RXD2/MCIDAT2/PWM0[6]"/>
<pin name="P1[12]/ENET_RXD3/MCIDAT3/PCAP0[0]"/>
<pin name="P1[13]/ENET_RX_DV"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[15]/ENET_REF_CLK/ENET_RX_CLK"/>
<pin name="P1[16]/ENET_MDC"/>
<pin name="P1[17]/ENET_MDIO"/>
<pin name="P1[18]/USB_UP_LED1/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/USB_TX_E1/USB_PPWR1/CAP1[1]"/>
<pin name="P1[20]/USB_TX_DP1/LCDVD[6]/LCDVD[10]/PWM1[2]/SCK0"/>
<pin name="P1[21]/USB_TX_DM1/LCDVD[7]/LCDVD[11]/PWM1[3]/SSEL0"/>
<pin name="P1[22]/USB_RCV1/LCDVD[8]/LCDVD[12]/USB_PWRD1/MAT1[0]"/>
<pin name="P1[23]/USB_RX_DP1/LCDVD[9]/LCDVD[13]/PWM1[4]/MISO0"/>
<pin name="P1[24]/USB_RX_DM1/LCDVD[10]/LCDVD[14]/PWM1[5]/MOSI0"/>
<pin name="P1[25]/USB_LS1/LCDVD[11]/LCDVD[15]/USB_HSTEN1/MAT1[1]"/>
<pin name="P1[26]/USB_SSPND1/LCDVD[12]/LCDVD[20]/PWM1[6]/CAP0[0]"/>
<pin name="P1[27]/USB_INT1/LCDVD[13]/LCDVD[21]/USB_OVRCR1/CAP0[1]"/>
<pin name="P1[28]/USB_SCL1/LCDVD[14]/LCDVD[22]/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/USB_SDA1/LCDVD[15]/LCDVD[23]/PCAP1[1]/MAT0[1]"/>
<pin name="P1[30]/USB_PWRD2/VBUS/AD0[4]"/>
<pin name="P1[31]/USB_OVRCR2/SCK1/AD0[5]"/>
<pin name="P2[0]/PWM1[1]/TXD1/TRACECLK/LCDPWR"/>
<pin name="P2[1]/PWM1[2]/RXD1/PIPESTAT0/LCDLE"/>
<pin name="P2[2]/PWM1[3]/CTS1/PIPESTAT1/LCDDCLK"/>
<pin name="P2[3]/PWM1[4]/DCD1/PIPESTAT2/LCDFP"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACESYNC/LCDENAB/LCDM"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEPKT0/LCDLP"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACEPKT1/LCDVD[0]/LCDVD[4]"/>
<pin name="P2[7]/RD2/RTS1/TRACEPKT2/LCDVD[1]/LCDVD[5]"/>
<pin name="P2[8]/TD2/TXD2/TRACEPKT3/LCDVD[2]/LCDVD[6]"/>
<pin name="P2[9]/USB_CONNECT1/RXD2/EXTIN0/LCDVD[3]/LCDVD[7]"/>
<pin name="P2[10]/EINT0"/>
<pin name="P2[11]/EINT1/LCDCLKIN/MCIDAT1/I2STX_CLK"/>
<pin name="P2[12]/EINT2/LCDVD[4]/LCDVD[3]/LCDVD[8]/LCDVD[18]/MCIDAT2/I2STX_WS"/>
<pin name="P2[13]/EINT3/LCDVD[5]/LCDVD[9]/LCDVD[19]/MCIDAT3/I2STX_SDA"/>
<pin name="P2[14]/CS2/CAP2[0]/SDA1"/>
<pin name="P2[15]/CS3/CAP2[1]/SCL1"/>
<pin name="P2[16]/CAS"/>
<pin name="P2[17]/RAS"/>
<pin name="P2[18]/CLKOUT0"/>
<pin name="P2[19]/CLKOUT1"/>
<pin name="P2[20]/DYCS0"/>
<pin name="P2[21]/DYCS1"/>
<pin name="P2[22]/DYCS2/CAP3[0]/SCK0"/>
<pin name="P2[23]/DYCS3/CAP3[1]/SSEL0"/>
<pin name="P2[24]/CKEOUT0"/>
<pin name="P2[25]/CKEOUT1"/>
<pin name="P2[26]/CKEOUT2/MAT3[0]/MISO0"/>
<pin name="P2[27]/CKEOUT3/MAT3[1]/MOSI0"/>
<pin name="P2[28]/DQMOUT0"/>
<pin name="P2[29]/DQMOUT1"/>
<pin name="P2[30]/DQMOUT2/MAT3[2]/SDA2"/>
<pin name="P2[31]/DQMOUT3/MAT3[3]/SCL2"/>
<pin name="P3[0]/D0"/>
<pin name="P3[1]/D1"/>
<pin name="P3[2]/D2"/>
<pin name="P3[3]/D3"/>
<pin name="P3[4]/D4"/>
<pin name="P3[5]/D5"/>
<pin name="P3[6]/D6"/>
<pin name="P3[7]/D7"/>
<pin name="P3[8]/D8"/>
<pin name="P3[9]/D9"/>
<pin name="P3[10]/D10"/>
<pin name="P3[11]/D11"/>
<pin name="P3[12]/D12"/>
<pin name="P3[13]/D13"/>
<pin name="P3[14]/D14"/>
<pin name="P3[15]/D15"/>
<pin name="P3[16]/D16/PWM0[1]/TXD1"/>
<pin name="P3[17]/D17/PWM0[2]/RXD1"/>
<pin name="P3[18]/D18/PWM0[3]/CTS1"/>
<pin name="P3[19]/D19/PWM0[4]/DCD1"/>
<pin name="P3[20]/D20/PWM0[5]/DSR1"/>
<pin name="P3[21]/D21/PWM0[6]/DTR1"/>
<pin name="P3[22]/D22/PCAP0[0]/RI1"/>
<pin name="P3[23]/D23/CAP0[0]/PCAP1[0]"/>
<pin name="P3[24]/D24/CAP0[1]/PWM1[1]"/>
<pin name="P3[25]/D25/MAT0[0]/PWM1[2]"/>
<pin name="P3[26]/D26/MAT0[1]/PWM1[3]"/>
<pin name="P3[27]/D27/CAP1[0]/PWM1[4]"/>
<pin name="P3[28]/D28/CAP1[1]/PWM1[5]"/>
<pin name="P3[29]/D29/MAT1[0]/PWM1[6]"/>
<pin name="P3[30]/D30/MAT1[1]/RTS1"/>
<pin name="P3[31]/D31/MAT1[2]"/>
<pin name="P4[0]/A0"/>
<pin name="P4[1]/A1"/>
<pin name="P4[2]/A2"/>
<pin name="P4[3]/A3"/>
<pin name="P4[4]/A4"/>
<pin name="P4[5]/A5"/>
<pin name="P4[6]/A6"/>
<pin name="P4[7]/A7"/>
<pin name="P4[8]/A8"/>
<pin name="P4[9]/A9"/>
<pin name="P4[10]/A10"/>
<pin name="P4[11]/A11"/>
<pin name="P4[12]/A12"/>
<pin name="P4[13]/A13"/>
<pin name="P4[14]/A14"/>
<pin name="P4[15]/A15"/>
<pin name="P4[16]/A16"/>
<pin name="P4[17]/A17"/>
<pin name="P4[18]/A18"/>
<pin name="P4[19]/A19"/>
<pin name="P4[20]/A20/SDA2/SCK1"/>
<pin name="P4[21]/A21/SCL2/SSEL1"/>
<pin name="P4[22]/A22/TXD2/MISO1"/>
<pin name="P4[23]/A23/RXD2/MOSI1"/>
<pin name="P4[24]/OE"/>
<pin name="P4[25]/WE"/>
<pin name="P4[26]/BLS0"/>
<pin name="P4[27]/BLS1"/>
<pin name="P4[28]/BLS2/MAT2[0]/LCDVD[6]/LCDVD[10]/LCDVD[2]/TXD3"/>
<pin name="P4[29]/BLS3/MAT2[1]LCDVD[7]/LCDVD[11]/LCDVD[3]/RXD3"/>
<pin name="P4[30]/CS0"/>
<pin name="P4[31]/CS1"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RTCX1"/>
<pin name="RTCX2"/>
<pin name="ALARM"/>
<pin name="VREF"/>
<pin name="VBAT"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDD3"/>
<pin name="VDD4"/>
<pin name="VDD5"/>
<pin name="VDD6"/>
<pin name="VDD7"/>
<pin name="VDD8"/>
<pin name="VDD9"/>
<pin name="VDD10"/>
<pin name="VSS(IO)1"/>
<pin name="VSS(IO)2"/>
<pin name="VSS(IO)3"/>
<pin name="VSS(IO)4"/>
<pin name="VSS(IO)5"/>
<pin name="VSS(IO)6"/>
<pin name="VSS(IO)7"/>
<pin name="VSS(IO)8"/>
<pin name="VSS(IO)9"/>
<pin name="VSS(IO)10"/>
<pin name="VDD(DCDC)1"/>
<pin name="VDD(DCDC)2"/>
<pin name="VDD(DCDC)3"/>
<pin name="VSS(CORE)1"/>
<pin name="VSS(CORE)2"/>
<pin name="VSS(CORE)3"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="DBGEN"/>
<pin name="TDO"/>
<pin name="TDI"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="TCK"/>
<pin name="RTCK"/>
<pin name="RESET"/>
<pin name="RSTOUT"/>
</symbol>
<symbol name="FRAME_A3P">
</symbol>
<symbol name="MAX1698">
<pin name="VCC"/>
<pin name="SHDN"/>
<pin name="REF"/>
<pin name="ADJ"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="PGND"/>
<pin name="FB"/>
<pin name="CS"/>
<pin name="EXT"/>
</symbol>
<symbol name="RJ45_LEDS">
<pin name="LED1_A"/>
<pin name="LED1_K"/>
<pin name="LED2_A"/>
<pin name="LED2_K"/>
<pin name="TX+"/>
<pin name="TCT"/>
<pin name="TX-"/>
<pin name="RX+"/>
<pin name="RCT"/>
<pin name="RX-"/>
<pin name="GND1"/>
<pin name="GND2"/>
</symbol>
<symbol name="FERRITE">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="PINHD11">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="BUTTON_4PIN">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="SMACONNECTOR">
<pin name="ANT"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
</symbol>
<symbol name="AT86RF212">
<pin name="DIG3"/>
<pin name="DIG4"/>
<pin name="AVSS1"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="AVSS2"/>
<pin name="DVSS1"/>
<pin name="/RST"/>
<pin name="DIG1"/>
<pin name="DIG2"/>
<pin name="SLP_TR"/>
<pin name="DVSS2"/>
<pin name="DVDD1"/>
<pin name="DVDD2"/>
<pin name="DEVDD"/>
<pin name="DVSS3"/>
<pin name="CLKM"/>
<pin name="DVSS4"/>
<pin name="SCLK"/>
<pin name="MISO"/>
<pin name="DVSS5"/>
<pin name="MOSI"/>
<pin name="/SEL"/>
<pin name="IRQ"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="AVSS3"/>
<pin name="EVDD"/>
<pin name="AVDD"/>
<pin name="AVSS4"/>
<pin name="AVSS5"/>
<pin name="AVSS6"/>
<pin name="DIE"/>
</symbol>
<symbol name="BALUN">
<pin name="GND1"/>
<pin name="UNBAL"/>
<pin name="GND2"/>
<pin name="BALP1"/>
<pin name="NC"/>
<pin name="BALP2"/>
</symbol>
<symbol name="LOWPASSFILTER">
<pin name="GND1"/>
<pin name="NC"/>
<pin name="GND2"/>
<pin name="OUT"/>
<pin name="GND3"/>
<pin name="IN"/>
</symbol>
<symbol name="ANTENNA_CHIP">
<pin name="ANT"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
</symbol>
<symbol name="BALUN+LP_AT86RF">
<pin name="GND1"/>
<pin name="UNBAL"/>
<pin name="GND2"/>
<pin name="BALP1"/>
<pin name="GND3"/>
<pin name="BALP2"/>
</symbol>
<symbol name="AGND">
<pin name="AGND" direction="sup"/>
</symbol>
<symbol name="AVCC">
<pin name="AVCC" direction="sup"/>
</symbol>
<symbol name="FTDIUSBCABLE">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="AT25040A">
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="CS"/>
<pin name="WP"/>
<pin name="HOLD"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PN532">
<pin name="DGND"/>
<pin name="LOADMOD"/>
<pin name="TGND1"/>
<pin name="TX1"/>
<pin name="TVDD"/>
<pin name="TX2"/>
<pin name="TGND2"/>
<pin name="AVDD"/>
<pin name="VMID"/>
<pin name="RX"/>
<pin name="AGND"/>
<pin name="AUX1"/>
<pin name="AUX2"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="I0"/>
<pin name="I1"/>
<pin name="TESTEN"/>
<pin name="P35"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="PVDD"/>
<pin name="P30/UART_RX"/>
<pin name="IRQ"/>
<pin name="RSTOUT_N"/>
<pin name="NSS/P50_SCL/HSU_RX"/>
<pin name="MOSI/SDA/HSU_TX"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="P31"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34/SIC_CLK"/>
<pin name="SIGOUT"/>
<pin name="SIGIN"/>
<pin name="SVDD"/>
<pin name="RSTPD_N"/>
<pin name="DVDD"/>
<pin name="VBAT"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="BRIDGERECTIFIER">
<pin name="AC1" direction="pas"/>
<pin name="+" direction="pas"/>
<pin name="AC2" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="GM862">
<pin name="VBATT@0" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="VBATT@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VBATT@2" direction="pwr"/>
<pin name="GND/ADC" direction="pwr"/>
<pin name="VBATT@3" direction="pwr"/>
<pin name="CHARGE" direction="in"/>
<pin name="EAR_HF+" direction="out"/>
<pin name="EAR_MT-" direction="out"/>
<pin name="EAR_HF-" direction="out"/>
<pin name="EAR_MT+" direction="out"/>
<pin name="MIC_HF-" direction="in"/>
<pin name="MIC_MT+" direction="in"/>
<pin name="MIC_HF+" direction="in"/>
<pin name="MIC_MT-" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="AXE" direction="in"/>
<pin name="SIMIO"/>
<pin name="C103/TXD" direction="in"/>
<pin name="PWRMON" direction="out"/>
<pin name="SIMVCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="SIMRST" direction="out"/>
<pin name="RES@25"/>
<pin name="SIMCLK" direction="out"/>
<pin name="CCIN/SIMIN"/>
<pin name="GPO2/JDR" direction="out"/>
<pin name="C106/CTS"/>
<pin name="C125/RING" direction="out"/>
<pin name="GPI1" direction="in"/>
<pin name="GPIO8/PD[0]/CAM_ON"/>
<pin name="C107/DSR" direction="out"/>
<pin name="GPIO9/PD[1]/CAM_RST"/>
<pin name="EMMI_TX/TX_GPS" direction="out"/>
<pin name="C109/DCD" direction="out"/>
<pin name="C104/RXD" direction="out"/>
<pin name="GPIO10/PD[2]"/>
<pin name="STAT_LED" direction="out"/>
<pin name="GPIO11/PD[3]"/>
<pin name="EMMI_RX/RX_GPS" direction="in"/>
<pin name="GPIO12/PD[4]"/>
<pin name="C108/DTR" direction="in"/>
<pin name="GPIO13/PD[5]"/>
<pin name="C105/RTS" direction="in"/>
<pin name="GPIO3/PD[6]/CAM_SCL"/>
<pin name="GPIO4/IICSDA/CAM_SDA"/>
<pin name="GPIO5/CAM_RDY/RFTXMON"/>
<pin name="GPIO6/ALARM/PD[7]"/>
<pin name="GPIO7/BUZZER/CAM_PWR_ON"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
</symbol>
<symbol name="LD39015XX">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="EN"/>
<pin name="GND"/>
</symbol>
<symbol name="LPC1114_QFN33">
<pin name="PIO2_0/DTR"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL/CT16B0_CAP0"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO3_4"/>
<pin name="PIO3_5"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO3_2"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="AVDD">
<pin name="AVDD" direction="sup"/>
</symbol>
<symbol name="MCP24AA32">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="WP"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="DIODE-ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="LEDRGB_PLCC4">
<pin name="RED"/>
<pin name="GRN"/>
<pin name="BLUE"/>
<pin name="ANODE" direction="pwr"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="LM2671">
<pin name="VIN"/>
<pin name="ON/OFF"/>
<pin name="GND"/>
<pin name="SS"/>
<pin name="SYNC"/>
<pin name="FB"/>
<pin name="CB"/>
<pin name="VSW"/>
</symbol>
<symbol name="VREG_SOT23-5">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="P4"/>
</symbol>
<symbol name="LPC1114_QFP_SQUARE">
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="pwr"/>
<pin name="VSS(IO)" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD(3.3V)" direction="pwr"/>
<pin name="RESET/PIO0_0"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="PIO0_3"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO2_0/DTR/SSEL1"/>
<pin name="PIO2_1/DSR/SCK1"/>
<pin name="PIO2_2/DCD/MISO1"/>
<pin name="PIO2_3/RI/MOSI1"/>
<pin name="PIO2_4"/>
<pin name="PIO2_5"/>
<pin name="PIO2_6"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_11/SCK0"/>
<pin name="PIO3_0/DTR"/>
<pin name="PIO3_1/DSR"/>
<pin name="PIO3_2/DCD"/>
<pin name="PIO3_3/RI"/>
<pin name="PIO3_4"/>
<pin name="PIO3_5"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="FIDUCIAL">
</symbol>
<symbol name="MOSFET-P">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="ADT7410">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CT"/>
<pin name="INT"/>
</symbol>
<symbol name="ADM1191">
<pin name="VCC"/>
<pin name="SENSE"/>
<pin name="CONV"/>
<pin name="GND"/>
<pin name="SETV"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="ALERTB"/>
</symbol>
<symbol name="PINH2X8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
<symbol name="LPC1768_QFPSQ">
<pin name="TDO/SWO"/>
<pin name="TDI"/>
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="TCK/SWDCLK"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]"/>
<pin name="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="VREFP"/>
<pin name="N.C."/>
<pin name="RSTOUT"/>
<pin name="VREFN"/>
<pin name="RTCX1"/>
<pin name="RESET"/>
<pin name="RTCX2"/>
<pin name="VBAT"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0[28]/SCL0/USB_SCL"/>
<pin name="P0[27]/SDA0/USB_SDA"/>
<pin name="P3[26]/STCLK/MAT0[1]/PWM1[3]"/>
<pin name="P3[25]/MAT0[0]/PWM1[2]"/>
<pin name="VDD(3V3)1"/>
<pin name="P0[29]/USB_D+"/>
<pin name="P0[30]/USB_D-"/>
<pin name="VSS1"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MC0A/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCFB0/PWM1[2]/SCK0"/>
<pin name="P1[21]/MCABORT/PWM1[3]/SSEL0"/>
<pin name="P1[22]/MC0B/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCFB1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCFB2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MC1A/MAT1[1]"/>
<pin name="P1[26]/MC1B/PWM1[6]/CAP0[0]"/>
<pin name="VSS2"/>
<pin name="VDD(REG)(3V3)1"/>
<pin name="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]"/>
<pin name="P1[28]/MC2A/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MC2B/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P2[13]/EINT3/I2STX_SDA"/>
<pin name="P2[12]/EINT2/I2STX_WS"/>
<pin name="P2[11]/EINT1/I2STX_CLK"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VDD(3V3)2"/>
<pin name="VSS3"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[21]/RI1/RD1"/>
<pin name="P0[20]/DTR1/SCL1"/>
<pin name="P0[19]/DSR1/SDA1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2"/>
<pin name="P2[8]/TD2/TXD2"/>
<pin name="P2[7]/RD2/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)3"/>
<pin name="VSS4"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
<pin name="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
<pin name="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
<pin name="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
<pin name="P0[5]/I2SRX_WS/TD2/CAP2[1]"/>
<pin name="P0[4]/I2SRX_CLK/RD2/CAP2[0]"/>
<pin name="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
<pin name="VSS6"/>
<pin name="VDD(REG)(3V3)2"/>
<pin name="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
<pin name="P1[17]/ENET_MDIO"/>
<pin name="P1[16]/ENET_MDC"/>
<pin name="P1[15]/ENET_REF_CLK"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[8]/ENET_CRS"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="VDD(3V3)4"/>
<pin name="VSS5"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
<pin name="RTCK"/>
</symbol>
<symbol name="LPC1768_QFP">
<pin name="TDO/SWO"/>
<pin name="TDI"/>
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="TCK/SWDCLK"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="P0[25]/AD0[2]/I2SRX_SDA/TXD3"/>
<pin name="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]"/>
<pin name="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREFP" direction="pwr"/>
<pin name="N.C." direction="nc"/>
<pin name="RSTOUT"/>
<pin name="VREFN" direction="pwr"/>
<pin name="RTCX1"/>
<pin name="RESET"/>
<pin name="RTCX2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0[28]/SCL0/USB_SCL"/>
<pin name="P0[27]/SDA0/USB_SDA"/>
<pin name="P3[26]/STCLK/MAT0[1]/PWM1[3]"/>
<pin name="P3[25]/MAT0[0]/PWM1[2]"/>
<pin name="VDD(3V3)1" direction="pwr"/>
<pin name="P0[29]/USB_D+"/>
<pin name="P0[30]/USB_D-"/>
<pin name="VSS1" direction="pwr"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MC0A/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCFB0/PWM1[2]/SCK0"/>
<pin name="P1[21]/MCABORT/PWM1[3]/SSEL0"/>
<pin name="P1[22]/MC0B/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCFB1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCFB2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MC1A/MAT1[1]"/>
<pin name="P1[26]/MC1B/PWM1[6]/CAP0[0]"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD(REG)(3V3)1" direction="pwr"/>
<pin name="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]"/>
<pin name="P1[28]/MC2A/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MC2B/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P2[13]/EINT3/I2STX_SDA"/>
<pin name="P2[12]/EINT2/I2STX_WS"/>
<pin name="P2[11]/EINT1/I2STX_CLK"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VDD(3V3)2" direction="pwr"/>
<pin name="VSS3" direction="pwr"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[21]/RI1/RD1"/>
<pin name="P0[20]/DTR1/SCL1"/>
<pin name="P0[19]/DSR1/SDA1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2"/>
<pin name="P2[8]/TD2/TXD2"/>
<pin name="P2[7]/RD2/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)3" direction="pwr"/>
<pin name="VSS4" direction="pwr"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/I2STX_SDA/MOSI1/MAT2[3]"/>
<pin name="P0[8]/I2STX_WS/MISO1/MAT2[2]"/>
<pin name="P0[7]/I2STX_CLK/SCK1/MAT2[1]"/>
<pin name="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]"/>
<pin name="P0[5]/I2SRX_WS/TD2/CAP2[1]"/>
<pin name="P0[4]/I2SRX_CLK/RD2/CAP2[0]"/>
<pin name="P4[28]/RX_MCLK/MAT2[0]/TXD3"/>
<pin name="VSS6" direction="pwr"/>
<pin name="VDD(REG)(3V3)2" direction="pwr"/>
<pin name="P4[29]/TX_MCLK/MAT2[1]/RXD3"/>
<pin name="P1[17]/ENET_MDIO"/>
<pin name="P1[16]/ENET_MDC"/>
<pin name="P1[15]/ENET_REF_CLK"/>
<pin name="P1[14]/ENET_RX_ER"/>
<pin name="P1[10]/ENET_RXD1"/>
<pin name="P1[9]/ENET_RXD0"/>
<pin name="P1[8]/ENET_CRS"/>
<pin name="P1[4]/ENET_TX_EN"/>
<pin name="P1[1]/ENET_TXD1"/>
<pin name="P1[0]/ENET_TXD0"/>
<pin name="VDD(3V3)4" direction="pwr"/>
<pin name="VSS5" direction="pwr"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
<pin name="RTCK"/>
</symbol>
<symbol name="VIN">
<pin name="VIN" direction="sup"/>
</symbol>
<symbol name="DP83848">
<pin name="TX_CLK"/>
<pin name="TX_EN"/>
<pin name="TXD_0"/>
<pin name="TXD_1"/>
<pin name="TXD_2"/>
<pin name="TXD_3"/>
<pin name="RESERVED1"/>
<pin name="RESERVED2"/>
<pin name="RESERVED3"/>
<pin name="GNDPAD"/>
<pin name="RD-"/>
<pin name="RD+"/>
<pin name="AGND1"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="PFBIN1"/>
<pin name="AGND2"/>
<pin name="AVDD33"/>
<pin name="PFBOUT"/>
<pin name="RBIAS"/>
<pin name="LED_SPEED/AN1"/>
<pin name="LED_LINK/AN0"/>
<pin name="RESET_N"/>
<pin name="MDIO"/>
<pin name="MDC"/>
<pin name="IOVDD33(1)"/>
<pin name="X2"/>
<pin name="X1"/>
<pin name="DGND"/>
<pin name="PFBIN2"/>
<pin name="RX_CLK"/>
<pin name="RX_DV/MII_MODE"/>
<pin name="CRS/CRS_DV/LED_CFG"/>
<pin name="RX_ER/MDIX_EN"/>
<pin name="COL/PHYAD0"/>
<pin name="RXD_0/PHYAD1"/>
<pin name="RXD_1/PHYAD1"/>
<pin name="RXD_2/PHYAD2"/>
<pin name="RXD_3/PHYAD3"/>
<pin name="IOGND"/>
<pin name="IOVDD33(2)"/>
</symbol>
<symbol name="OSCILLATOR">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="INH"/>
</symbol>
<symbol name="CFAF240320K-T-TS">
<pin name="DB0" direction="pas"/>
<pin name="DB1" direction="pas"/>
<pin name="DB2" direction="pas"/>
<pin name="DB3" direction="pas"/>
<pin name="GND1" direction="pwr"/>
<pin name="IOVCC1" direction="pwr"/>
<pin name="!CS" direction="pas"/>
<pin name="RS" direction="pas"/>
<pin name="!WR" direction="pas"/>
<pin name="!RD" direction="pas"/>
<pin name="IMO" direction="pas"/>
<pin name="X+" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="X-" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="LED-A" direction="pas"/>
<pin name="LED-K1" direction="pas"/>
<pin name="LED-K2" direction="pas"/>
<pin name="LED-K3" direction="pas"/>
<pin name="LED-K4" direction="pas"/>
<pin name="IM3" direction="pas"/>
<pin name="DB4" direction="pas"/>
<pin name="DB10" direction="pas"/>
<pin name="DB11" direction="pas"/>
<pin name="DB12" direction="pas"/>
<pin name="DB13" direction="pas"/>
<pin name="DB14" direction="pas"/>
<pin name="DB15" direction="pas"/>
<pin name="DB16" direction="pas"/>
<pin name="DB17" direction="pas"/>
<pin name="!RESET" direction="pas"/>
<pin name="VCI" direction="pwr"/>
<pin name="IOVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DB5" direction="pas"/>
<pin name="DB6" direction="pas"/>
<pin name="DB7" direction="pas"/>
</symbol>
<symbol name="TRANSFLASH">
<pin name="CS" direction="in"/>
<pin name="DATA_IN" direction="in"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SD_VDD" direction="pwr"/>
<pin name="SCLK" direction="in"/>
<pin name="DATA_OUT" direction="out"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="CARD_DETECT" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="CARD_DETECT1" direction="pas"/>
</symbol>
<symbol name="ILI9325_LCD">
<pin name="DB0" direction="pas"/>
<pin name="DB1" direction="pas"/>
<pin name="DB2" direction="pas"/>
<pin name="DB3" direction="pas"/>
<pin name="GND1" direction="pwr"/>
<pin name="IOVCC1" direction="pwr"/>
<pin name="!CS" direction="pas"/>
<pin name="RS" direction="pas"/>
<pin name="!WR" direction="pas"/>
<pin name="!RD" direction="pas"/>
<pin name="IMO" direction="pas"/>
<pin name="X+" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="X-" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="LED-A" direction="pas"/>
<pin name="LED-K1" direction="pas"/>
<pin name="LED-K2" direction="pas"/>
<pin name="LED-K3" direction="pas"/>
<pin name="LED-K4" direction="pas"/>
<pin name="IM3" direction="pas"/>
<pin name="DB4" direction="pas"/>
<pin name="DB10/DB8" direction="pas"/>
<pin name="DB11/DB9" direction="pas"/>
<pin name="DB12/DB10" direction="pas"/>
<pin name="DB13/DB11" direction="pas"/>
<pin name="DB14/DB12" direction="pas"/>
<pin name="DB15/DB13" direction="pas"/>
<pin name="DB16/DB14" direction="pas"/>
<pin name="DB17/DB15" direction="pas"/>
<pin name="!RESET" direction="pas"/>
<pin name="VCI" direction="pwr"/>
<pin name="IOVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DB5" direction="pas"/>
<pin name="DB6" direction="pas"/>
<pin name="DB7" direction="pas"/>
</symbol>
<symbol name="VBAT">
<pin name="VBAT" direction="sup"/>
</symbol>
<symbol name="S1D13743_SQUARE">
<pin name="PIOVDD1"/>
<pin name="VSS1"/>
<pin name="DE"/>
<pin name="HS"/>
<pin name="VS"/>
<pin name="COREVDD1"/>
<pin name="VSS2"/>
<pin name="PCLK"/>
<pin name="PIOVDD2"/>
<pin name="VSS3"/>
<pin name="NC1"/>
<pin name="VD23"/>
<pin name="VD22"/>
<pin name="VD15"/>
<pin name="VD14"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="PIOVDD3"/>
<pin name="VSS4"/>
<pin name="VD16"/>
<pin name="VD7"/>
<pin name="NC4"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="NC7"/>
<pin name="COREVDD2"/>
<pin name="VSS5"/>
<pin name="PIOVDD4"/>
<pin name="NC8"/>
<pin name="NC9"/>
<pin name="NC10"/>
<pin name="NC11"/>
<pin name="NC12"/>
<pin name="NC13"/>
<pin name="NC14"/>
<pin name="NC15"/>
<pin name="NC16"/>
<pin name="VD8"/>
<pin name="VD0"/>
<pin name="VD17"/>
<pin name="COREVDD3"/>
<pin name="VSS6"/>
<pin name="VD1"/>
<pin name="VD9"/>
<pin name="VD18"/>
<pin name="PIOVDD5"/>
<pin name="VSS7"/>
<pin name="VD10"/>
<pin name="VD2"/>
<pin name="VD19"/>
<pin name="VD11"/>
<pin name="COREVDD4"/>
<pin name="VSS8"/>
<pin name="VD3"/>
<pin name="VD20"/>
<pin name="VD12"/>
<pin name="VD4"/>
<pin name="PIOVDD6"/>
<pin name="VSS9"/>
<pin name="VD21"/>
<pin name="VD13"/>
<pin name="VD5"/>
<pin name="VD6"/>
<pin name="COREVDD5"/>
<pin name="VSS10"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="IOVDD1"/>
<pin name="VSS11"/>
<pin name="PWRSAVE"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="NC17"/>
<pin name="COREVDD6"/>
<pin name="VSS12"/>
<pin name="CNF2"/>
<pin name="CNF1"/>
<pin name="CNF0"/>
<pin name="IOVDD2"/>
<pin name="VSS13"/>
<pin name="GPIO3"/>
<pin name="GPIO2"/>
<pin name="GPIO1"/>
<pin name="GPIO0"/>
<pin name="IOVDD3"/>
<pin name="VSS14"/>
<pin name="SCANEN"/>
<pin name="NC18"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="IOVDD4"/>
<pin name="VSS15"/>
<pin name="TEST0"/>
<pin name="TESTEN"/>
<pin name="COREVDD7"/>
<pin name="VSS16"/>
<pin name="RESET#"/>
<pin name="TE"/>
<pin name="VSS17"/>
<pin name="IOVDD5"/>
<pin name="GPIO_INT"/>
<pin name="MD12"/>
<pin name="MD11"/>
<pin name="VSS18"/>
<pin name="IOVDD6"/>
<pin name="MD0"/>
<pin name="MD2"/>
<pin name="MD1"/>
<pin name="NC19"/>
<pin name="CLKOUT"/>
<pin name="NC20"/>
<pin name="CLKOUTEN"/>
<pin name="VSS19"/>
<pin name="COREVDD8"/>
<pin name="CLKI"/>
<pin name="VSS"/>
<pin name="NC21"/>
<pin name="NC22"/>
<pin name="IOVDD7"/>
<pin name="PLLVDD"/>
<pin name="VCP"/>
<pin name="PLLVSS"/>
<pin name="NC23"/>
<pin name="MD13"/>
<pin name="MD3"/>
<pin name="MD14"/>
<pin name="MD4"/>
<pin name="IOVDD8"/>
<pin name="VSS20"/>
<pin name="CS#"/>
<pin name="MD15"/>
<pin name="MD5"/>
<pin name="COREVDD9"/>
<pin name="VSS21"/>
<pin name="MD6"/>
<pin name="MD8"/>
<pin name="WE#"/>
<pin name="MD7"/>
<pin name="IOVDD9"/>
<pin name="VSS22"/>
<pin name="MD9"/>
<pin name="RD#"/>
<pin name="MD10"/>
<pin name="D/C#"/>
</symbol>
<symbol name="S1D13743">
<pin name="PIOVDD1"/>
<pin name="VSS1"/>
<pin name="DE"/>
<pin name="HS"/>
<pin name="VS"/>
<pin name="COREVDD1"/>
<pin name="VSS2"/>
<pin name="PCLK"/>
<pin name="PIOVDD2"/>
<pin name="VSS3"/>
<pin name="NC1"/>
<pin name="VD23"/>
<pin name="VD22"/>
<pin name="VD15"/>
<pin name="VD14"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="PIOVDD3"/>
<pin name="VSS4"/>
<pin name="VD16"/>
<pin name="VD7"/>
<pin name="NC4"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="NC7"/>
<pin name="COREVDD2"/>
<pin name="VSS5"/>
<pin name="PIOVDD4"/>
<pin name="NC8"/>
<pin name="NC9"/>
<pin name="NC10"/>
<pin name="NC11"/>
<pin name="NC12"/>
<pin name="NC13"/>
<pin name="NC14"/>
<pin name="NC15"/>
<pin name="NC16"/>
<pin name="VD8"/>
<pin name="VD0"/>
<pin name="VD17"/>
<pin name="COREVDD3"/>
<pin name="VSS6"/>
<pin name="VD1"/>
<pin name="VD9"/>
<pin name="VD18"/>
<pin name="PIOVDD5"/>
<pin name="VSS7"/>
<pin name="VD10"/>
<pin name="VD2"/>
<pin name="VD19"/>
<pin name="VD11"/>
<pin name="COREVDD4"/>
<pin name="VSS8"/>
<pin name="VD3"/>
<pin name="VD20"/>
<pin name="VD12"/>
<pin name="VD4"/>
<pin name="PIOVDD6"/>
<pin name="VSS9"/>
<pin name="VD21"/>
<pin name="VD13"/>
<pin name="VD5"/>
<pin name="VD6"/>
<pin name="COREVDD5"/>
<pin name="VSS10"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="IOVDD1"/>
<pin name="VSS11"/>
<pin name="PWRSAVE"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="NC17"/>
<pin name="COREVDD6"/>
<pin name="VSS12"/>
<pin name="CNF2"/>
<pin name="CNF1"/>
<pin name="CNF0"/>
<pin name="IOVDD2"/>
<pin name="VSS13"/>
<pin name="GPIO3"/>
<pin name="GPIO2"/>
<pin name="GPIO1"/>
<pin name="GPIO0"/>
<pin name="IOVDD3"/>
<pin name="VSS14"/>
<pin name="SCANEN"/>
<pin name="NC18"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="IOVDD4"/>
<pin name="VSS15"/>
<pin name="TEST0"/>
<pin name="TESTEN"/>
<pin name="COREVDD7"/>
<pin name="VSS16"/>
<pin name="RESET#"/>
<pin name="TE"/>
<pin name="VSS17"/>
<pin name="IOVDD5"/>
<pin name="GPIO_INT"/>
<pin name="MD12"/>
<pin name="MD11"/>
<pin name="VSS18"/>
<pin name="IOVDD6"/>
<pin name="MD0"/>
<pin name="MD2"/>
<pin name="MD1"/>
<pin name="NC19"/>
<pin name="CLKOUT"/>
<pin name="NC20"/>
<pin name="CLKOUTEN"/>
<pin name="VSS19"/>
<pin name="COREVDD8"/>
<pin name="CLKI"/>
<pin name="VSS20"/>
<pin name="NC21"/>
<pin name="NC22"/>
<pin name="IOVDD7"/>
<pin name="PLLVDD"/>
<pin name="VCP"/>
<pin name="PLLVSS"/>
<pin name="NC23"/>
<pin name="MD13"/>
<pin name="MD3"/>
<pin name="MD14"/>
<pin name="MD4"/>
<pin name="IOVDD8"/>
<pin name="VSS21"/>
<pin name="CS#"/>
<pin name="MD15"/>
<pin name="MD5"/>
<pin name="COREVDD9"/>
<pin name="VSS22"/>
<pin name="MD6"/>
<pin name="MD8"/>
<pin name="WE#"/>
<pin name="MD7"/>
<pin name="IOVDD9"/>
<pin name="VSS23"/>
<pin name="MD9"/>
<pin name="RD#"/>
<pin name="MD10"/>
<pin name="D/C#"/>
</symbol>
<symbol name="PINHD28">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
</symbol>
<symbol name="1.5V">
<pin name="1.5V" direction="sup"/>
</symbol>
<symbol name="ARDUINO">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="/RESET"/>
</symbol>
<symbol name="FT232R">
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="DSR" direction="in" function="dot"/>
<pin name="DCD" direction="in" function="dot"/>
<pin name="RI" direction="in" function="dot"/>
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND7" direction="pwr"/>
<pin name="GND18" direction="pwr"/>
<pin name="GND21" direction="pwr"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="TXLED/CBUS0" direction="in" function="dot"/>
<pin name="RXLED/CBUS1" direction="in" function="dot"/>
<pin name="RTS" direction="out" function="dot"/>
<pin name="CTS" direction="in" function="dot"/>
<pin name="DTR" direction="out" function="dot"/>
<pin name="PWREN/CBUS3" direction="in" function="dot"/>
<pin name="TXDEN/CBUS2" direction="in"/>
<pin name="SLEEP/CBUS4" direction="in" function="dot"/>
</symbol>
<symbol name="MBED40">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
</symbol>
<symbol name="LPC313X/314X_0">
<pin name="VDDI_0" direction="pwr"/>
<pin name="VDDI_1" direction="pwr"/>
<pin name="VDDI_2" direction="pwr"/>
<pin name="VDDI_3" direction="pwr"/>
<pin name="VDDI_4" direction="pwr"/>
<pin name="VDDE_IOA_0" direction="pwr"/>
<pin name="VDDE_IOA_1" direction="pwr"/>
<pin name="VDDE_IOA_2" direction="pwr"/>
<pin name="VDDE_IOA_3" direction="pwr"/>
<pin name="VDDE_IOA_4" direction="pwr"/>
<pin name="VDDE_IOB_0" direction="pwr"/>
<pin name="VDDE_IOB_1" direction="pwr"/>
<pin name="VDDE_IOB_2" direction="pwr"/>
<pin name="VDDE_IOB_3" direction="pwr"/>
<pin name="VDDE_IOC_1" direction="pwr"/>
<pin name="VDDE_IOC_2" direction="pwr"/>
<pin name="VDDE_IOC_3" direction="pwr"/>
<pin name="VDDE_IOC_4" direction="pwr"/>
<pin name="VDDE_IOC_5" direction="pwr"/>
<pin name="VDDE_IOC_6" direction="pwr"/>
<pin name="VDDE_IOC_7" direction="pwr"/>
<pin name="VPP_0" direction="pwr"/>
<pin name="VPP_1" direction="pwr"/>
<pin name="VDDA12_0" direction="pwr"/>
<pin name="VDDA12_1" direction="pwr"/>
<pin name="ADC10B_VDDA33" direction="pwr"/>
<pin name="VSSI_0" direction="pwr"/>
<pin name="VSSI_1" direction="pwr"/>
<pin name="VSSI_2" direction="pwr"/>
<pin name="VSSI_3" direction="pwr"/>
<pin name="VSSI_4" direction="pwr"/>
<pin name="VSSI_5" direction="pwr"/>
<pin name="VSSE_IOA_0" direction="pwr"/>
<pin name="VSSE_IOA_1" direction="pwr"/>
<pin name="VSSE_IOA_2" direction="pwr"/>
<pin name="VSSE_IOA_3" direction="pwr"/>
<pin name="VSSE_IOA_4" direction="pwr"/>
<pin name="VSSE_IOA_5" direction="pwr"/>
<pin name="VSSE_IOB_0" direction="pwr"/>
<pin name="VSSE_IOB_1" direction="pwr"/>
<pin name="VSSE_IOB_2" direction="pwr"/>
<pin name="VSSE_IOB_3" direction="pwr"/>
<pin name="VSSE_IOC_0" direction="pwr"/>
<pin name="VSSE_IOC_1" direction="pwr"/>
<pin name="VSSE_IOC_2" direction="pwr"/>
<pin name="VSSE_IOC_3" direction="pwr"/>
<pin name="VSSE_IOC_4" direction="pwr"/>
<pin name="VSSE_IOC_5" direction="pwr"/>
<pin name="VSSE_IOC_6" direction="pwr"/>
<pin name="VSSA12" direction="pwr"/>
<pin name="ADC10B_GNDA" direction="pwr"/>
</symbol>
<symbol name="LPC313X/314X_2">
<pin name="EBI_D0"/>
<pin name="EBI_D1"/>
<pin name="EBI_D2"/>
<pin name="EBI_D3"/>
<pin name="EBI_D4"/>
<pin name="EBI_D5"/>
<pin name="EBI_D6"/>
<pin name="EBI_D7"/>
<pin name="EBI_D8"/>
<pin name="EBI_D9"/>
<pin name="EBI_D10"/>
<pin name="EBI_D11"/>
<pin name="EBI_D12"/>
<pin name="EBI_D13"/>
<pin name="EBI_D14"/>
<pin name="EBI_D15"/>
<pin name="EBI_DQM0/NOE"/>
<pin name="EBI_NWE"/>
<pin name="NAND_NCS0"/>
<pin name="NAND_NCS1"/>
<pin name="NAND_NCS2"/>
<pin name="NAND_NCS3"/>
<pin name="MNAND_RYBN0/MCI_DAT4"/>
<pin name="MNAND_RYBN1/MCI_DAT5"/>
<pin name="MNAND_RYBN2/MCI_DAT6"/>
<pin name="MNAND_RYBN3/MCI_DAT7"/>
<pin name="MLCD_DB0/EBI_CLKOUT"/>
<pin name="MLCD_DB1/EBI_NSTCS1"/>
<pin name="MLCD_DB2/EBI_A2"/>
<pin name="MLCD_DB3/EBI_A3"/>
<pin name="MLCD_DB4/EBI_A4"/>
<pin name="MLCD_DB5/EBI_A5"/>
<pin name="MLCD_DB6/EBI_A6"/>
<pin name="MLCD_DB7/EBI_A7"/>
<pin name="MLCD_DB8(8B0)/EBI_A8"/>
<pin name="MLCD_DB9(8B1)/EBI_A9"/>
<pin name="MLCD_DB10(8B2)/EBI_A10"/>
<pin name="MLCD_DB11(8B3)/EBI_A11"/>
<pin name="MLCD_DB12(8B4)/EBI_A12"/>
<pin name="MLCD_DB13(8B5)/EBI_A13"/>
<pin name="MLCD_DB14(8B6)/EBI_A14"/>
<pin name="MLCD_DB15(8B7)/EBI_A15"/>
<pin name="EBI_A0/ALE"/>
<pin name="EBI_A1/CLE"/>
<pin name="MLCD_RS/EBI_NDYCS"/>
<pin name="MLCD_RW_WR/EBI_DQM1"/>
<pin name="MLCD_E_RD/EBI_CKE"/>
<pin name="MLCD_CSB/EBI_NSTCS0"/>
<pin name="EBI_NCAS/BLOUT0"/>
<pin name="EBI_NRAS/BLOUT1"/>
</symbol>
<symbol name="LPC313X/314X_1">
<pin name="USB_VDDA33"/>
<pin name="USB_VDDA33_DRV"/>
<pin name="USB_VDDA12_PLL"/>
<pin name="USB_VBUS"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="USB_ID"/>
<pin name="USB_RREF"/>
<pin name="TRST_N"/>
<pin name="TDI"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="ARM_TDO"/>
<pin name="SCAN_TDO"/>
<pin name="BUF_TRST_N"/>
<pin name="BUF_TCK"/>
<pin name="BUF_TMS"/>
<pin name="JTAGSEL"/>
<pin name="FFAST_IN"/>
<pin name="FFAST_OUT"/>
<pin name="CLK_256FS_O"/>
<pin name="CLOCK_OUT"/>
<pin name="SYSCLK_O"/>
<pin name="RSTIN_N"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="MGPIO5/MCI_CLK"/>
<pin name="MGPIO6/MCI_CMD"/>
<pin name="MGPIO7/MCI_DAT0"/>
<pin name="MGPIO8/MCI_DAT1"/>
<pin name="MGPIO9/MCI_DAT2"/>
<pin name="MGPIO10/MCI_DAT3"/>
<pin name="GPIO11"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="GPIO15"/>
<pin name="GPIO16"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO19"/>
<pin name="GPIO20"/>
<pin name="PWM_DATA"/>
<pin name="ADC10B_GPA0"/>
<pin name="ADC10B_GPA1"/>
<pin name="ADC10B_GPA2"/>
<pin name="ADC10B_GPA3"/>
<pin name="USB_VSSA_REF"/>
<pin name="USB_VSSA_TERM"/>
<pin name="USB_GNDA"/>
<pin name="I2C_SDA0"/>
<pin name="I2C_SCL0"/>
<pin name="I2C_SDA1"/>
<pin name="I2C_SCL1"/>
<pin name="SPI_CS_OUT0"/>
<pin name="SPI_SCK"/>
<pin name="SPI_MISO"/>
<pin name="SPI_CS_IN"/>
<pin name="SPI_MOSI"/>
<pin name="UART_RXD"/>
<pin name="UART_TXD"/>
<pin name="MUART_CTS_N/SPI_CS_OUT1"/>
<pin name="MUART_RTS_N/SPI_CS_OUT2"/>
<pin name="I2SRX_DATA1"/>
<pin name="I2SRX_BCK1"/>
<pin name="I2SRX_WS1"/>
<pin name="I2SRX_DATA0"/>
<pin name="I2SRX_BCK0"/>
<pin name="I2SRX_WS0"/>
<pin name="I2STX_DATA0/IPINT_DA"/>
<pin name="I2STX_BCK0/IPINT_FSC"/>
<pin name="I2STX_WS0/IPINT_DCK"/>
<pin name="I2STX_CLK0/IPINT_DB"/>
<pin name="I2STX_DATA1"/>
<pin name="I2STX_BCK1"/>
<pin name="I2STX_WS1"/>
</symbol>
<symbol name="MT48H32M16LF">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="BA0"/>
<pin name="BA1"/>
<pin name="CS" function="dot"/>
<pin name="WE" function="dot"/>
<pin name="CAS" function="dot"/>
<pin name="RAS" function="dot"/>
<pin name="DQML"/>
<pin name="DQMH"/>
<pin name="NC"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDD3"/>
<pin name="VDDQ1"/>
<pin name="VDDQ2"/>
<pin name="VDDQ3"/>
<pin name="VDDQ4"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSSQ1"/>
<pin name="VSSQ2"/>
<pin name="VSSQ3"/>
<pin name="VSSQ4"/>
<pin name="CLK" function="clk"/>
<pin name="CKE"/>
<pin name="D15"/>
</symbol>
<symbol name="LTC3554">
<pin name="VBUS"/>
<pin name="NTC"/>
<pin name="PROG"/>
<pin name="HPWR"/>
<pin name="SUSP"/>
<pin name="PWR_ON1"/>
<pin name="FSEL"/>
<pin name="STBY"/>
<pin name="PGOOD"/>
<pin name="PWR_ON2"/>
<pin name="PBSTAT"/>
<pin name="/ON"/>
<pin name="FB2"/>
<pin name="SW2"/>
<pin name="FB1"/>
<pin name="SW1"/>
<pin name="BVIN"/>
<pin name="BAT"/>
<pin name="/CHRG"/>
<pin name="VOUT"/>
<pin name="THERM_GND"/>
</symbol>
<symbol name="1.2V">
<pin name="1.2V" direction="sup"/>
</symbol>
<symbol name="MIC5387">
<pin name="IN"/>
<pin name="EN2/3"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="GND"/>
<pin name="THERM"/>
</symbol>
<symbol name="FT2232D">
<pin name="3V3OUT" direction="pwr"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="BDBUS0" direction="out"/>
<pin name="BDBUS1" direction="in"/>
<pin name="BDBUS2" direction="out"/>
<pin name="BDBUS3" direction="in"/>
<pin name="BDBUS4" direction="out"/>
<pin name="BDBUS5" direction="in"/>
<pin name="BDBUS6" direction="in"/>
<pin name="BDBUS7" direction="in"/>
<pin name="PWEN#"/>
<pin name="VCCIOA" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="RSTOUT#"/>
<pin name="RESET#"/>
<pin name="XTIN"/>
<pin name="XTOUT"/>
<pin name="EECS"/>
<pin name="EESK"/>
<pin name="EEDATA"/>
<pin name="GND@4" direction="pwr"/>
<pin name="SI/WUB"/>
<pin name="BCBUS3"/>
<pin name="BCBUS2"/>
<pin name="BCBUS1"/>
<pin name="BCBUS0"/>
<pin name="ACBUS2"/>
<pin name="ACBUS1"/>
<pin name="ACBUS0"/>
<pin name="ADBUS7"/>
<pin name="ADBUS6"/>
<pin name="ADBUS5"/>
<pin name="SI/WUA"/>
<pin name="ACBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS3"/>
<pin name="ADBUS2"/>
<pin name="ADBUS1"/>
<pin name="ADBUS0"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="VCCIOB" direction="pwr"/>
</symbol>
<symbol name="BUFFER">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="LAN8720">
<pin name="MDIO"/>
<pin name="MDC"/>
<pin name="NINT/REFCLKO"/>
<pin name="TXD0"/>
<pin name="TXD1"/>
<pin name="TXEN"/>
<pin name="RXD0"/>
<pin name="RXD1"/>
<pin name="RXER"/>
<pin name="LED1/REGOFF"/>
<pin name="LED2/NINTSEL"/>
<pin name="NRST"/>
<pin name="TX+"/>
<pin name="TX-"/>
<pin name="RX+"/>
<pin name="RX-"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="CRS_DV"/>
<pin name="RBIAS"/>
<pin name="GND"/>
<pin name="VDD1A"/>
<pin name="VDD2A"/>
<pin name="VDDIO"/>
<pin name="VDDCR"/>
</symbol>
<symbol name="FT2232H">
<pin name="ADBUS0/TXD"/>
<pin name="ADBUS1/RXD"/>
<pin name="ADBUS2/RTS#"/>
<pin name="ADBUS3/CTS#"/>
<pin name="ADBUS4/DTR#"/>
<pin name="ADBUS5/DSR#"/>
<pin name="ADBUS6/DCD#"/>
<pin name="ADBUS7/RI#"/>
<pin name="ACBUS0/TXDEN"/>
<pin name="ACBUS1"/>
<pin name="ACBUS2"/>
<pin name="ACBUS3/RXLED#"/>
<pin name="ACBUS4/TXLED#"/>
<pin name="ACBUS5"/>
<pin name="ACBUS6"/>
<pin name="ACBUS7"/>
<pin name="BDBUS0/TXD"/>
<pin name="BDBUS1/RXD"/>
<pin name="BDBUS2/RTS#"/>
<pin name="BDBUS3/CTS#"/>
<pin name="BDBUS4/DTR#"/>
<pin name="BDBUS5/DSR#"/>
<pin name="BDBUS6/DCD#"/>
<pin name="BDBUS7/RI#"/>
<pin name="BCBUS0/TXDEN"/>
<pin name="BCBUS1"/>
<pin name="BCBUS2"/>
<pin name="BCBUS3/RXLED#"/>
<pin name="BCBUS4/TXLED#"/>
<pin name="BCBUS5"/>
<pin name="BCBUS6"/>
<pin name="BCBUS7"/>
<pin name="PWREN#"/>
<pin name="SUSPEND#"/>
<pin name="VREGIN"/>
<pin name="VREGOUT"/>
<pin name="USBD-"/>
<pin name="USBD+"/>
<pin name="REF"/>
<pin name="RESET#"/>
<pin name="GND@8"/>
<pin name="GND@7"/>
<pin name="GND@6"/>
<pin name="GND@5"/>
<pin name="GND@4"/>
<pin name="GND@3"/>
<pin name="GND@2"/>
<pin name="GND@1"/>
<pin name="AGND"/>
<pin name="EECS"/>
<pin name="EECLK"/>
<pin name="EEDATA"/>
<pin name="OSCIN"/>
<pin name="OSCOUT"/>
<pin name="TEST"/>
<pin name="VCCIO@4"/>
<pin name="VCCIO@3"/>
<pin name="VCCIO@2"/>
<pin name="VCCIO@1"/>
<pin name="VCORE@3"/>
<pin name="VCORE@2"/>
<pin name="VCORE@1"/>
<pin name="VPLL"/>
<pin name="VPHY"/>
</symbol>
<symbol name="PINHD27">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
</symbol>
<symbol name="93LC46B">
<pin name="CS" direction="in"/>
<pin name="ORG"/>
<pin name="D" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="Q" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74LVC1G04">
<pin name="NC" direction="nc"/>
<pin name="A"/>
<pin name="GND" direction="pwr"/>
<pin name="Y"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="BUFFER_PWR">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LOADCELL">
<pin name="OUT-"/>
<pin name="EXC+"/>
<pin name="OUT+"/>
<pin name="EXC-"/>
</symbol>
<symbol name="AD7780">
<pin name="VREF+"/>
<pin name="VREF-"/>
<pin name="AIN+"/>
<pin name="AIN-"/>
<pin name="BPDSW"/>
<pin name="AVDD"/>
<pin name="DVDD"/>
<pin name="SCLK"/>
<pin name="DOUT/RDY"/>
<pin name="PDRST"/>
<pin name="FILTER"/>
<pin name="GAIN"/>
<pin name="GND"/>
</symbol>
<symbol name="ADP3303">
<pin name="VIN1"/>
<pin name="VIN2"/>
<pin name="SD"/>
<pin name="GND"/>
<pin name="NR"/>
<pin name="OUT1"/>
<pin name="ERR"/>
<pin name="OUT2"/>
</symbol>
<symbol name="POWER">
<pin name="+" direction="pas" function="dot"/>
<pin name="-" direction="pas" function="dot"/>
</symbol>
<symbol name="LM4811">
<pin name="VIN1"/>
<pin name="VIN2"/>
<pin name="CLK"/>
<pin name="UP/DN"/>
<pin name="SHTDN"/>
<pin name="VDD"/>
<pin name="VOUT1"/>
<pin name="VOUT2"/>
<pin name="BYPASS"/>
<pin name="GND"/>
</symbol>
<symbol name="KS-S">
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MOUNTINGHOLE">
</symbol>
<symbol name="LPC1754">
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
<pin name="VDD(3V3)3" direction="pwr"/>
<pin name="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]"/>
<pin name="VDD(3V3)2" direction="pwr"/>
<pin name="P2[10]/EINT0/NMI"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VREFP" direction="in"/>
<pin name="RSTOUT" direction="out"/>
<pin name="VREFN" direction="in"/>
<pin name="RTCX1" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="RTCX2" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="P1[31]/SCK1/AD0[5]"/>
<pin name="P1[30]/VBUS/AD0[4]"/>
<pin name="P0[30]/USB_DMIN"/>
<pin name="VSS1" direction="pwr"/>
<pin name="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]"/>
<pin name="P1[19]/MCOA0/USB_PPWR/CAP1[1]"/>
<pin name="P1[20]/MCI0/PWM1[2]/SCK0"/>
<pin name="P1[22]/MCOB0/USB_PWRD/MAT1[0]"/>
<pin name="P1[23]/MCI1/PWM1[4]/MISO0"/>
<pin name="P1[24]/MCI2/PWM1[5]/MOSI0"/>
<pin name="P1[25]/MCOA1/MAT1[1]"/>
<pin name="P1[26]/MCOB1/PWM1[6]/CAP0[0]"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VDD(REG)(3V3)1" direction="pwr"/>
<pin name="P1[28]/MCOA2/PCAP1[0]/MAT0[0]"/>
<pin name="P1[29]/MCOB2/PCAP1[1]/MAT0[1]"/>
<pin name="P0[0]/RD1/TXD3/SDA1"/>
<pin name="P0[1]/TD1/RXD3/SCL1"/>
<pin name="VSS3" direction="pwr"/>
<pin name="P0[22]/RTS1/TD1"/>
<pin name="P0[18]/DCD1/MOSI0/MOSI"/>
<pin name="P0[17]/CTS1/MISO0/MISO"/>
<pin name="P0[15]/TXD1/SCK0/SCK"/>
<pin name="P0[16]/RXD1/SSEL0/SSEL"/>
<pin name="P2[9]/USB_CONNECT/RXD2"/>
<pin name="P2[8]/TXD2"/>
<pin name="P2[7]/RTS1"/>
<pin name="P2[6]/PCAP1[0]/RI1/TRACECLK"/>
<pin name="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]"/>
<pin name="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]"/>
<pin name="VDDA" direction="pwr"/>
<pin name="P0[25]/AD0[2]/TXD3"/>
<pin name="VSS4" direction="pwr"/>
<pin name="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]"/>
<pin name="P0[7]/SCK1/MAT2[1]"/>
<pin name="P0[6]/SSEL1/MAT2[0]"/>
<pin name="P4[28]/MAT2[0]/TXD3"/>
<pin name="VSS5" direction="pwr"/>
<pin name="VDD(REG)(3V3)2" direction="pwr"/>
<pin name="P4[29]/MAT2[1]/RXD3"/>
<pin name="P1[15]"/>
<pin name="P1[9]"/>
<pin name="P1[14]"/>
<pin name="P1[10]"/>
<pin name="P1[8]"/>
<pin name="P1[4]"/>
<pin name="P1[1]"/>
<pin name="P1[0]"/>
<pin name="VDD(3V3)4" direction="pwr"/>
<pin name="VSS6" direction="pwr"/>
<pin name="TDO/SWO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDD(3V3)1" direction="pwr"/>
<pin name="P0[29]/USB_DPLUS"/>
<pin name="P0[10]/TXD2/SDA2/MAT3[0]"/>
<pin name="P0[11]/RXD2/SCL2/MAT3[1]"/>
<pin name="P0[26]/AD0[3]/AOUT/RXD3"/>
<pin name="TCK/SWDCLK"/>
<pin name="P2[1]/PWM1[2]/RXD1"/>
<pin name="P2[0]/PWM1[1]/TXD1"/>
<pin name="P0[9]/MOSI1/MAT2[3]"/>
<pin name="P0[8]/MISO1/MAT2[2]"/>
<pin name="P0[2]/TXD0/AD0[7]"/>
<pin name="P0[3]/RXD0/AD0[6]"/>
</symbol>
<symbol name="PCF2129A">
<pin name="SCL"/>
<pin name="SDI"/>
<pin name="SDO"/>
<pin name="SDA/#CE"/>
<pin name="IFS"/>
<pin name="#TS"/>
<pin name="CLKOUT"/>
<pin name="VSS"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="NC7"/>
<pin name="NC8"/>
<pin name="#INT"/>
<pin name="BBS"/>
<pin name="VBAT"/>
<pin name="VDD"/>
</symbol>
<symbol name="LPC1227/6/5/4_QFP64">
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
<pin name="VREF_CMP"/>
<pin name="PIO0_19/ACMP0_I0/CT32B0_CAP1/CT32B0_MAT1"/>
<pin name="PIO0_20/ACMP0_I1/CT32B0_CAP2/CT32B0_MAT2"/>
<pin name="PIO0_21/ACMP0_I2/CT32B0_CAP3/CT32B0_MAT3"/>
<pin name="PIO0_22/ACMP0_I3"/>
<pin name="PIO0_23/ACMP1_I0/CT32B1_CAP0/CT32B1_MAT0"/>
<pin name="PIO0_24/ACMP1_I1/CT32B1_CAP1/CT32B1_MAT1"/>
<pin name="SWDIO/ACMP1_I2/CT32B1_CAP2/CT32B1_MAT2/PIO0_25"/>
<pin name="SWCLK/ACMP1_I3/CT32B1_CAP3/CT32B1_MAT3/PIO0_26"/>
<pin name="PIO0_27/ACMP0_O-(20MA)"/>
<pin name="PIO2_12/RXD1"/>
<pin name="PIO2_13/TXD1"/>
<pin name="PIO2_14"/>
<pin name="PIO2_15"/>
<pin name="PIO0_28/ACMP1_O/CT16B0_CAP0/CT16B0_MAT0-(20MA)"/>
<pin name="PIO0_29/ROSC/CT16B0_CAP1/CT16B0_MAT1-(20MA)"/>
<pin name="PIO0_0/RTS0"/>
<pin name="PIO0_1/RXD0/CT32B0_CAP0/CT32B0_MAT0"/>
<pin name="PIO0_2/TXD0/CT32B0_CAP1/CT32B0_MAT1"/>
<pin name="PIO0_3/DTR0/CT32B0_CAP2/CT32B0_MAT2"/>
<pin name="PIO0_4/DSR0/CT32B0_CAP3/CT32B0_MAT3"/>
<pin name="PIO0_5/DCD0"/>
<pin name="PIO0_6/RI0/CT32B1_CAP0/CT32B1_MAT0"/>
<pin name="PIO0_7/CTS0/CT32B1_CAP1/CT32B1_MAT1"/>
<pin name="PIO0_8/RXD1/CT32B1_CAP2/CT32B1_MAT2"/>
<pin name="PIO0_9/TXD1/CT32B1_CAP3/CT32B1_MAT3"/>
<pin name="PIO2_0/CT16B0_CAP0/CT16B0_MAT0/RTS0"/>
<pin name="PIO2_1/CT16B0_CAP1/CT16B0_MAT1/RXD0"/>
<pin name="PIO2_2/CT16B1_CAP0/CT16B1_MAT0/TXD0"/>
<pin name="PIO2_3/CT16B1_CAP1/CT16B1_MAT1/DTR0"/>
<pin name="PIO2_4/CT32B0_CAP0/CT32B0_MAT0/CTS0"/>
<pin name="PIO2_5/CT32B0_CAP1/CT32B0_MAT1/RI0"/>
<pin name="PIO2_6/CT32B0_CAP2/CT32B0_MAT2/DCD0"/>
<pin name="PIO2_7/CT32B0_CAP3/CT32B0_MAT3/DSR0"/>
<pin name="PIO0_10/SCL"/>
<pin name="PIO0_11/SDA/CT16B0_CAP0/CT16B0_MAT0"/>
<pin name="PIO0_12/CLKOUT/CT16B0_CAP1/CT16B0_MAT1_ISP-(20MA)"/>
<pin name="#RESET/PIO0_13"/>
<pin name="PIO0_14/SCK"/>
<pin name="PIO0_15/SSEL/CT16B1_CAP0/CT16B1_MAT0"/>
<pin name="PIO0_16/MISO/CT16B1_CAP1/CT16B1_MAT1"/>
<pin name="PIO0_17/MOSI"/>
<pin name="PIO0_18/SWCLK/CT32B0_CAP0/CT32B0_MAT0"/>
<pin name="R/PIO0_30/AD0"/>
<pin name="R/PIO0_31/AD1"/>
<pin name="R/PIO1_0/AD2"/>
<pin name="R/PIO1_1/AD3"/>
<pin name="PIO1_2/SWDIO/AD4"/>
<pin name="PIO1_3/AD5/WAKEUP"/>
<pin name="PIO1_4/AD6"/>
<pin name="PIO1_5/AD7/CT16B1_CAP0/CT16B1_MAT0"/>
<pin name="PIO1_6/CT16B1_CAP1/CT16B1_MAT1"/>
<pin name="VSS"/>
<pin name="VDD(3.3V)"/>
<pin name="RTCXIN"/>
<pin name="RTCXOUT"/>
<pin name="PIO2_8/CT32B1_CAP0/CT32B1_MAT0"/>
<pin name="PIO2_9/CT32B1_CAP1/CT32B1_MAT1"/>
<pin name="PIO2_10/CT32B1_CAP2/CT32B1_MAT2/TXD1"/>
<pin name="PIO2_11/CT32B1_CAP3/CT32B1_MAT3/RXD1"/>
<pin name="VDD(IO)"/>
<pin name="VSSIO"/>
</symbol>
<symbol name="GE865_2">
<pin name="EAR-"/>
<pin name="EAR+"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TXD_AUX"/>
<pin name="RXD_AUX"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="ON_OFF"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="GPIO_03"/>
<pin name="GPIO_04/TX_DISAB"/>
<pin name="GPIO_01"/>
<pin name="GPIO_08"/>
<pin name="GPIO_06/ALARM"/>
<pin name="GPIO_09"/>
<pin name="GPIO_02/JDR"/>
<pin name="GPIO_07/BUZZER"/>
<pin name="GPIO_05/RFTXMON"/>
<pin name="GPIO_10"/>
<pin name="VBATT@F1"/>
<pin name="VBATT@F2"/>
<pin name="VBATT@F3"/>
<pin name="GND@G1"/>
<pin name="GND@C2"/>
<pin name="GND@C7"/>
<pin name="GND@E5"/>
<pin name="GND@E7"/>
<pin name="GND@G5"/>
<pin name="GND@G4"/>
<pin name="GND@G3"/>
<pin name="GND@H3"/>
<pin name="GND@H6"/>
<pin name="SERVICE"/>
</symbol>
<symbol name="GE864">
<pin name="EAR_MT-"/>
<pin name="EAR_MT+"/>
<pin name="EAR_HF+"/>
<pin name="EAR_HF-"/>
<pin name="MIC_MT+"/>
<pin name="MIC_MT-"/>
<pin name="MIC_HF+"/>
<pin name="MIC_HF-"/>
<pin name="AXE"/>
<pin name="SIMCLK"/>
<pin name="SIMRST"/>
<pin name="SIMIO"/>
<pin name="SIMIN"/>
<pin name="SIMVCC"/>
<pin name="TX_TRACE"/>
<pin name="RX_TRACE"/>
<pin name="C103/TXD"/>
<pin name="C104/RXD"/>
<pin name="C108/DTR"/>
<pin name="C105/RTS"/>
<pin name="C106/CTS"/>
<pin name="C109/DCD"/>
<pin name="C107/DSR"/>
<pin name="C125/RING"/>
<pin name="DAC_OUT"/>
<pin name="ACD_IN1"/>
<pin name="ADC_IN2"/>
<pin name="ADC_IN3"/>
<pin name="RESET"/>
<pin name="VRTC"/>
<pin name="STAT_LED"/>
<pin name="CHARGE@G1"/>
<pin name="CHARGE@G2"/>
<pin name="ON_OFF"/>
<pin name="VAUX1"/>
<pin name="PWRMON"/>
<pin name="ANTENNA"/>
<pin name="DV12_CLK"/>
<pin name="TGPIO_12"/>
<pin name="TGPIO_03"/>
<pin name="TGPIO_04"/>
<pin name="TGPIO_20"/>
<pin name="TGPIO_14"/>
<pin name="TGPIO_11"/>
<pin name="TGPIO_19"/>
<pin name="TGPIO_01"/>
<pin name="TGPIO_18"/>
<pin name="TGPIO_17"/>
<pin name="TGPIO_15"/>
<pin name="TGPIO_08"/>
<pin name="TGPIO_06/ALARM"/>
<pin name="TGPIO_09"/>
<pin name="TGPIO_02/JDR"/>
<pin name="TGPIO_07/BUZZER"/>
<pin name="TGPIO_16"/>
<pin name="TGPIO_13"/>
<pin name="TGPIO_05/RFTXMON"/>
<pin name="TGPIO_21"/>
<pin name="TGPIO_22"/>
<pin name="TGPIO_10"/>
<pin name="VBATT@J1"/>
<pin name="VBATT@K1"/>
<pin name="VBATT@J2"/>
<pin name="VBATT@K2"/>
<pin name="GND@A1"/>
<pin name="GND@F1"/>
<pin name="GND@H1"/>
<pin name="GND@L1"/>
<pin name="GND@H2"/>
<pin name="GND@L2"/>
<pin name="GND@J3"/>
<pin name="GND@K3"/>
<pin name="GND@L3"/>
<pin name="GND@K4"/>
<pin name="GND@K5"/>
<pin name="GND@D6"/>
<pin name="GND@K6"/>
<pin name="GND@L6"/>
<pin name="GND@A11"/>
<pin name="GND@F11"/>
<pin name="GND@L11"/>
</symbol>
<symbol name="OLED_96X64_UNIVISION">
<pin name="NC1" direction="nc"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="VDDIO"/>
<pin name="BS1"/>
<pin name="BS2"/>
<pin name="IREF"/>
<pin name="CS#"/>
<pin name="RES#"/>
<pin name="D/C#"/>
<pin name="R/W#"/>
<pin name="E"/>
<pin name="D0/SCLK"/>
<pin name="D1/SDIN"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="VCOMH"/>
<pin name="VCC"/>
<pin name="NC2" direction="nc"/>
</symbol>
<symbol name="OL2381">
<pin name="VCCREG"/>
<pin name="VCCDIG"/>
<pin name="VCCXO"/>
<pin name="VCCRF"/>
<pin name="VCCIF"/>
<pin name="VCCPA"/>
<pin name="RSTDIS"/>
<pin name="SEN"/>
<pin name="SDIO"/>
<pin name="SCLK"/>
<pin name="P10/DATA"/>
<pin name="P11/INT"/>
<pin name="P12/CLOCK"/>
<pin name="P13/SDO"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="TEN"/>
<pin name="TEST1"/>
<pin name="TEST2"/>
<pin name="TEST3"/>
<pin name="VREGDIG"/>
<pin name="VREGVCO"/>
<pin name="VREGPLL"/>
<pin name="VREGPA"/>
<pin name="RF_OUT"/>
<pin name="RF_IN"/>
<pin name="P14/PIND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
</symbol>
<symbol name="UPD5713">
<pin name="NC"/>
<pin name="GND"/>
<pin name="NO"/>
<pin name="VDD"/>
<pin name="P"/>
<pin name="VCONT"/>
</symbol>
<symbol name="USB_NOID">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PINH2X15">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
</symbol>
<symbol name="U.FL">
<pin name="GND@0" direction="pas"/>
<pin name="SIGNAL" direction="pas"/>
<pin name="GND@1" direction="pas"/>
</symbol>
<symbol name="ILI9481_LCD">
<pin name="GND1" direction="pas"/>
<pin name="VDD1" direction="pas"/>
<pin name="VDD2" direction="pas"/>
<pin name="!CS" direction="pas"/>
<pin name="RS" direction="pwr"/>
<pin name="!WR" direction="pwr"/>
<pin name="!RD" direction="pas"/>
<pin name="!RESET" direction="pas"/>
<pin name="DB0" direction="pas"/>
<pin name="DB1" direction="pas"/>
<pin name="DB2" direction="pas"/>
<pin name="DB3" direction="pas"/>
<pin name="DB4" direction="pas"/>
<pin name="DB5" direction="pas"/>
<pin name="DB6" direction="pas"/>
<pin name="DB7" direction="pas"/>
<pin name="DB8" direction="pas"/>
<pin name="DB9" direction="pas"/>
<pin name="DB10" direction="pas"/>
<pin name="DB11" direction="pas"/>
<pin name="DB12" direction="pas"/>
<pin name="DB13" direction="pas"/>
<pin name="DB14" direction="pas"/>
<pin name="DB15" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="X-" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="X+" direction="pas"/>
<pin name="LED-K1" direction="pas"/>
<pin name="LED-K2" direction="pas"/>
<pin name="LED-K3" direction="pwr"/>
<pin name="LED-K4" direction="pwr"/>
<pin name="LED-K5" direction="pwr"/>
<pin name="LED-K6" direction="pas"/>
<pin name="LED-A" direction="pas"/>
<pin name="GND3" direction="pas"/>
</symbol>
<symbol name="SPX29300">
<pin name="ENABLE"/>
<pin name="VIN"/>
<pin name="GND1"/>
<pin name="VOUT"/>
<pin name="ADJUST"/>
<pin name="GND0"/>
</symbol>
<symbol name="ADXL345">
<pin name="VDD(I/O)"/>
<pin name="GND@1"/>
<pin name="RSV@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="VS"/>
<pin name="CS"/>
<pin name="INT1"/>
<pin name="INT2"/>
<pin name="NC"/>
<pin name="RSV@2"/>
<pin name="ADDR/SDO"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="MCP73871">
<pin name="VIN2"/>
<pin name="VPCC"/>
<pin name="/PG"/>
<pin name="STAT2"/>
<pin name="STAT1/LBO"/>
<pin name="SEL"/>
<pin name="PROG2"/>
<pin name="/TE"/>
<pin name="CE"/>
<pin name="VSS2"/>
<pin name="PROG3"/>
<pin name="PROG1"/>
<pin name="THERM"/>
<pin name="VBATSENS"/>
<pin name="VOUT2"/>
<pin name="VIN1"/>
<pin name="VOUT1"/>
<pin name="VSS1"/>
<pin name="VBAT1"/>
<pin name="VBAT2"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="74HC4050D">
<pin name="VCC"/>
<pin name="1A"/>
<pin name="2A"/>
<pin name="3A"/>
<pin name="4A"/>
<pin name="5A"/>
<pin name="6A"/>
<pin name="GND"/>
<pin name="1Y"/>
<pin name="2Y"/>
<pin name="3Y"/>
<pin name="4Y"/>
<pin name="5Y"/>
<pin name="6Y"/>
</symbol>
<symbol name="74LCX245MTC">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="T/R"/>
<pin name="/OE"/>
</symbol>
<symbol name="SWITCH_SPDT">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="UG-2832HSWEG04">
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="VBAT"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="CS#"/>
<pin name="RES#"/>
<pin name="D/C#"/>
<pin name="SCLK"/>
<pin name="SDIN"/>
<pin name="IREF"/>
<pin name="VCOMH"/>
<pin name="VCC"/>
</symbol>
<symbol name="UG-9616GLBBG02">
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="VBAT"/>
<pin name="VBREF"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="RES#"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="IREF"/>
<pin name="VCOMH"/>
<pin name="VCC"/>
</symbol>
<symbol name="FAN5331">
<pin name="VIN"/>
<pin name="SHDN"/>
<pin name="SW"/>
<pin name="FB"/>
<pin name="GND"/>
</symbol>
<symbol name="ISL12022M">
<pin name="VDD" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="#IRQ/FOUT"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="MAX3421E">
<pin name="GPIN0" direction="in"/>
<pin name="GPIN1" direction="in"/>
<pin name="GPIN2" direction="in"/>
<pin name="GPIN3" direction="in"/>
<pin name="GPIN4" direction="in"/>
<pin name="GPIN5" direction="in"/>
<pin name="GPIN6" direction="in"/>
<pin name="GPIN7" direction="in"/>
<pin name="GPOUT0" direction="out"/>
<pin name="GPOUT1" direction="out"/>
<pin name="GPOUT2" direction="out"/>
<pin name="GPOUT3" direction="out"/>
<pin name="GPOUT4" direction="out"/>
<pin name="GPOUT5" direction="out"/>
<pin name="GPOUT6" direction="out"/>
<pin name="GPOUT7" direction="out"/>
<pin name="INT"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="XO"/>
<pin name="XI"/>
<pin name="#RES"/>
<pin name="SCK"/>
<pin name="#SS"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="GPX"/>
<pin name="VBCOMP"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="GND3(THERMAL)" direction="pwr"/>
</symbol>
<symbol name="LT3581">
<pin name="VIN" direction="pwr"/>
<pin name="#FAULT"/>
<pin name="#SHDN"/>
<pin name="RT"/>
<pin name="SYNC"/>
<pin name="GND" direction="pwr"/>
<pin name="SW1B" direction="pwr"/>
<pin name="SW2A" direction="pwr"/>
<pin name="FB"/>
<pin name="GATE"/>
<pin name="CLKOUT" direction="out"/>
<pin name="VC"/>
<pin name="SS"/>
<pin name="SW1A" direction="pwr"/>
<pin name="SW2B" direction="pwr"/>
</symbol>
<symbol name="TXB0108PWR">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="OE"/>
</symbol>
<symbol name="TXB0104PWR">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="OE"/>
</symbol>
<symbol name="VCCIO">
<pin name="VCCIO" direction="sup"/>
</symbol>
<symbol name="BMP085">
<pin name="GND"/>
<pin name="EOC"/>
<pin name="AVDD"/>
<pin name="VDD"/>
<pin name="NC"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="XCLR"/>
</symbol>
<symbol name="HMC5883L">
<pin name="VDD"/>
<pin name="VDDIO"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="NC5"/>
<pin name="C1"/>
<pin name="SETC"/>
<pin name="S1"/>
<pin name="GND2"/>
<pin name="SETP"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="DRDY"/>
<pin name="GND1"/>
</symbol>
<symbol name="ITG3200">
<pin name="CLKIN"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="NC3"/>
<pin name="NC4"/>
<pin name="RESV1"/>
<pin name="RESV2"/>
<pin name="VLOGIC"/>
<pin name="AD0"/>
<pin name="REGOUT"/>
<pin name="RESV-G"/>
<pin name="INT"/>
<pin name="VDD"/>
<pin name="NC5"/>
<pin name="NC6"/>
<pin name="NC7"/>
<pin name="NC8"/>
<pin name="GND"/>
<pin name="RESV3"/>
<pin name="CPOUT"/>
<pin name="RESV4"/>
<pin name="RESV5"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="VCNL4000">
<pin name="IR_A"/>
<pin name="IR_K1"/>
<pin name="IR_K2"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GND2"/>
<pin name="GND1"/>
<pin name="VDD"/>
</symbol>
<symbol name="M25P16">
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SSEL"/>
<pin name="#WP/IO2"/>
<pin name="#HOLD/IO3"/>
<pin name="VCC"/>
<pin name="VSS"/>
</symbol>
<symbol name="A4983_LITERAL">
<pin name="OUT2B"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND1" direction="pwr"/>
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="VCP"/>
<pin name="NC1" direction="nc"/>
<pin name="VREG"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="MS3" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="ROSC"/>
<pin name="SLEEP"/>
<pin name="VDD" direction="pwr"/>
<pin name="STEP" direction="in"/>
<pin name="REF"/>
<pin name="GND2" direction="pwr"/>
<pin name="DIR" direction="in"/>
<pin name="NC2" direction="nc"/>
<pin name="OUT1B"/>
<pin name="VBB1"/>
<pin name="SENSE1"/>
<pin name="OUT1A"/>
<pin name="NC3" direction="nc"/>
<pin name="OUT2A"/>
<pin name="SENSE2"/>
<pin name="VBB2"/>
<pin name="GND3" direction="pwr"/>
</symbol>
<symbol name="TPS61029">
<pin name="PWRPAD1"/>
<pin name="PWRPAD2"/>
<pin name="PWRPAD3"/>
<pin name="PWRPAD4"/>
<pin name="PWRPAD5"/>
<pin name="SW"/>
<pin name="VBAT"/>
<pin name="EN"/>
<pin name="LBI"/>
<pin name="PS"/>
<pin name="VOUT"/>
<pin name="FB"/>
<pin name="LBO"/>
<pin name="PGND"/>
<pin name="GND"/>
</symbol>
<symbol name="SWITCH_SPST">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="A4983_LOGICAL">
<pin name="OUT2B"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND1" direction="pwr"/>
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="VCP"/>
<pin name="NC1" direction="nc"/>
<pin name="VREG"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="MS3" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="ROSC"/>
<pin name="SLEEP"/>
<pin name="VDD" direction="pwr"/>
<pin name="STEP" direction="in"/>
<pin name="REF"/>
<pin name="GND2" direction="pwr"/>
<pin name="DIR" direction="in"/>
<pin name="NC2" direction="nc"/>
<pin name="OUT1B"/>
<pin name="VBB1"/>
<pin name="SENSE1"/>
<pin name="OUT1A"/>
<pin name="NC3" direction="nc"/>
<pin name="OUT2A"/>
<pin name="SENSE2"/>
<pin name="VBB2"/>
<pin name="GND3" direction="pwr"/>
</symbol>
<symbol name="TXS0102">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="OE"/>
</symbol>
<symbol name="SWITCH_DPDT">
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="O1" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="O2" direction="pas"/>
</symbol>
<symbol name="UG-2828GDEDF11">
<pin name="NC(GND)@1" direction="nc"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCOMH" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="VSL"/>
<pin name="NC@1" direction="nc"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1/SDIN"/>
<pin name="D0/SCK"/>
<pin name="E/RD#"/>
<pin name="R/W#"/>
<pin name="BS0"/>
<pin name="BS1"/>
<pin name="CS#"/>
<pin name="D/C#"/>
<pin name="RES#"/>
<pin name="IREF"/>
<pin name="GPIO1"/>
<pin name="GPIO0"/>
<pin name="NC@2" direction="nc"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCI" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC(GND)@2" direction="nc"/>
</symbol>
<symbol name="12V">
<pin name="12V" direction="sup"/>
</symbol>
<symbol name="13V">
<pin name="13V" direction="sup"/>
</symbol>
<symbol name="LPC1102-16">
<pin name="!RESET!/PIO0_0"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="R/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="R/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="R/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="R/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="XTALIN" direction="pas"/>
<pin name="VSS2" direction="pwr"/>
</symbol>
<symbol name="FPC45">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
<pin name="P$41"/>
<pin name="P$42"/>
<pin name="P$43"/>
<pin name="P$44"/>
<pin name="P$45"/>
</symbol>
<symbol name="EINK_10BAR">
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="FIELD"/>
<pin name="TPLANE"/>
<pin name="1"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
</symbol>
<symbol name="SIM900_LITERAL">
<pin name="PWRKEY" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="DTR" direction="in"/>
<pin name="RI" direction="out"/>
<pin name="DCD" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="CTS" direction="out"/>
<pin name="RTS" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="DISP_CLK"/>
<pin name="DISP_DATA"/>
<pin name="DISP_DC"/>
<pin name="DISP_CS"/>
<pin name="VDD_EXT"/>
<pin name="NRESET"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="MIC_P"/>
<pin name="MIC_N"/>
<pin name="SPK_P"/>
<pin name="SPK_N"/>
<pin name="LINEIN_R"/>
<pin name="LINEIN_L"/>
<pin name="ADC"/>
<pin name="VRTC" direction="pwr"/>
<pin name="DBG_TXD" direction="out"/>
<pin name="DBG_RXD" direction="in"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SIM_VDD" direction="pwr"/>
<pin name="SIM_DATA"/>
<pin name="SIM_CLK"/>
<pin name="SIM_RST"/>
<pin name="SIM_PRESENCE"/>
<pin name="PWM1"/>
<pin name="PWM2"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GPIO1/KBR4"/>
<pin name="GPIO2/KBR3"/>
<pin name="GPIO3/KBR2"/>
<pin name="GPIO4/KBR1"/>
<pin name="GPIO5/KBR0"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GPIO6/KBC4"/>
<pin name="GPIO7/KBC3"/>
<pin name="GPIO8/KBC2"/>
<pin name="GPIO9/KBC1"/>
<pin name="GPIO10"/>
<pin name="NETLIGHT"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="VBAT1" direction="pwr"/>
<pin name="VBAT2" direction="pwr"/>
<pin name="VBAT3" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="RF_ANT"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="STATUS"/>
<pin name="GPIO11" direction="pwr"/>
<pin name="GPIO12" direction="pwr"/>
</symbol>
<symbol name="SIMLOCK-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="VREG_SOT23">
<pin name="VIN" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TVSARRAY_5LANE">
<pin name="A" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="C5" direction="pas"/>
</symbol>
<symbol name="3.5MMAUDIO_5PIN">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
</symbol>
<symbol name="VRTC">
<pin name="VRTC" direction="sup"/>
</symbol>
<symbol name="SIM900B_LITERAL">
<pin name="VBAT1" direction="pwr"/>
<pin name="VBAT2" direction="pwr"/>
<pin name="VBAT3" direction="pwr"/>
<pin name="VBAT4" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="VRTC" direction="pwr"/>
<pin name="VDD_EXT" direction="pwr"/>
<pin name="SIM_VDD" direction="pwr"/>
<pin name="SIM_DATA"/>
<pin name="SIM_CLK" direction="out"/>
<pin name="SIM_RST" direction="out"/>
<pin name="GPIO5/KBC0" direction="out"/>
<pin name="GPIO4/KBC1"/>
<pin name="GPIO3/KBC2"/>
<pin name="GPIO2/KBC3"/>
<pin name="GPIO1/KBC4"/>
<pin name="GPIO10/KBR0" direction="in"/>
<pin name="GPIO9/KBR1"/>
<pin name="GPIO8/KBR2"/>
<pin name="GPIO7/KBR3"/>
<pin name="GPIO6/KBR4"/>
<pin name="DBG_RXD" direction="in"/>
<pin name="DBG_TXD" direction="out"/>
<pin name="AGND1" direction="pwr"/>
<pin name="MIC1+" direction="in"/>
<pin name="MIC1-" direction="in"/>
<pin name="MIC2+" direction="in"/>
<pin name="MIC2-" direction="in"/>
<pin name="VBAT5" direction="pwr"/>
<pin name="VBAT6" direction="pwr"/>
<pin name="VBAT7" direction="pwr"/>
<pin name="VBAT8" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
<pin name="SIM_PRESENCE" direction="in"/>
<pin name="DISP_DATA"/>
<pin name="DISP_CLK" direction="out"/>
<pin name="DISP_CS" direction="out"/>
<pin name="DISP_D/C" direction="out"/>
<pin name="DISP_RST" direction="out"/>
<pin name="DCD" direction="out"/>
<pin name="NETLIGHT" direction="out"/>
<pin name="GPIO0"/>
<pin name="PWRKEY" direction="in"/>
<pin name="BUZZER" direction="out"/>
<pin name="DTR" direction="in"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RTS" direction="in"/>
<pin name="CTS" direction="out"/>
<pin name="RI" direction="out"/>
<pin name="AGND2" direction="pwr"/>
<pin name="ADC0" direction="in"/>
<pin name="SPK1+" direction="out"/>
<pin name="SPK1-" direction="out"/>
<pin name="SPK2+" direction="out"/>
<pin name="SPK2-" direction="out"/>
</symbol>
<symbol name="JACK_4POL">
<pin name="GND" direction="pas"/>
<pin name="SLEEVE_INNER" direction="pas"/>
<pin name="SLEEVE_OUTER" direction="pas"/>
<pin name="TIP" direction="pas"/>
</symbol>
<symbol name="VLIPO">
<pin name="VLIPO" direction="sup"/>
</symbol>
<symbol name="4.5V">
<pin name="4.5V" direction="sup"/>
</symbol>
<symbol name="SOLDERJUMPER_CLOSED">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SHARP_LS013B4DN02">
<pin name="SCLK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SCS" direction="in"/>
<pin name="EXTCOMIN" direction="in"/>
<pin name="DISP" direction="in"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EXTMODE" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="LBGA256">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="B9"/>
<pin name="B10"/>
<pin name="B11"/>
<pin name="B12"/>
<pin name="B13"/>
<pin name="B14"/>
<pin name="B15"/>
<pin name="B16"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="C5"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="C8"/>
<pin name="C9"/>
<pin name="C10"/>
<pin name="C11"/>
<pin name="C12"/>
<pin name="C13"/>
<pin name="C14"/>
<pin name="C15"/>
<pin name="C16"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="E1"/>
<pin name="E2"/>
<pin name="E3"/>
<pin name="E4"/>
<pin name="E5"/>
<pin name="E6"/>
<pin name="E7"/>
<pin name="E8"/>
<pin name="E9"/>
<pin name="E10"/>
<pin name="E11"/>
<pin name="E12"/>
<pin name="E13"/>
<pin name="E14"/>
<pin name="E15"/>
<pin name="E16"/>
<pin name="F1"/>
<pin name="F2"/>
<pin name="F3"/>
<pin name="F4"/>
<pin name="F5"/>
<pin name="F6"/>
<pin name="F7"/>
<pin name="F8"/>
<pin name="F9"/>
<pin name="F10"/>
<pin name="F11"/>
<pin name="F12"/>
<pin name="F13"/>
<pin name="F14"/>
<pin name="F15"/>
<pin name="F16"/>
<pin name="G1"/>
<pin name="G2"/>
<pin name="G3"/>
<pin name="G4"/>
<pin name="G5"/>
<pin name="G6"/>
<pin name="G7"/>
<pin name="G8"/>
<pin name="G9"/>
<pin name="G10"/>
<pin name="G11"/>
<pin name="G12"/>
<pin name="G13"/>
<pin name="G14"/>
<pin name="G15"/>
<pin name="G16"/>
<pin name="H1"/>
<pin name="H2"/>
<pin name="H3"/>
<pin name="H4"/>
<pin name="H5"/>
<pin name="H6"/>
<pin name="H7"/>
<pin name="H8"/>
<pin name="H9"/>
<pin name="H10"/>
<pin name="H11"/>
<pin name="H12"/>
<pin name="H13"/>
<pin name="H14"/>
<pin name="H15"/>
<pin name="H16"/>
<pin name="J1"/>
<pin name="J2"/>
<pin name="J3"/>
<pin name="J4"/>
<pin name="J5"/>
<pin name="J6"/>
<pin name="J7"/>
<pin name="J8"/>
<pin name="J9"/>
<pin name="J10"/>
<pin name="J11"/>
<pin name="J12"/>
<pin name="J13"/>
<pin name="J14"/>
<pin name="J15"/>
<pin name="J16"/>
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
<pin name="K9"/>
<pin name="K10"/>
<pin name="K11"/>
<pin name="K12"/>
<pin name="K13"/>
<pin name="K14"/>
<pin name="K15"/>
<pin name="K16"/>
<pin name="L1"/>
<pin name="L2"/>
<pin name="L3"/>
<pin name="L4"/>
<pin name="L5"/>
<pin name="L6"/>
<pin name="L7"/>
<pin name="L8"/>
<pin name="L9"/>
<pin name="L10"/>
<pin name="L11"/>
<pin name="L12"/>
<pin name="L13"/>
<pin name="L14"/>
<pin name="L15"/>
<pin name="L16"/>
<pin name="M1"/>
<pin name="M2"/>
<pin name="M3"/>
<pin name="M4"/>
<pin name="M5"/>
<pin name="M6"/>
<pin name="M7"/>
<pin name="M8"/>
<pin name="M9"/>
<pin name="M10"/>
<pin name="M11"/>
<pin name="M12"/>
<pin name="M13"/>
<pin name="M14"/>
<pin name="M15"/>
<pin name="M16"/>
<pin name="N1"/>
<pin name="N2"/>
<pin name="N3"/>
<pin name="N4"/>
<pin name="N5"/>
<pin name="N6"/>
<pin name="N7"/>
<pin name="N8"/>
<pin name="N9"/>
<pin name="N10"/>
<pin name="N11"/>
<pin name="N12"/>
<pin name="N13"/>
<pin name="N14"/>
<pin name="N15"/>
<pin name="N16"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="R1"/>
<pin name="R2"/>
<pin name="R3"/>
<pin name="R4"/>
<pin name="R5"/>
<pin name="R6"/>
<pin name="R7"/>
<pin name="R8"/>
<pin name="R9"/>
<pin name="R10"/>
<pin name="R11"/>
<pin name="R12"/>
<pin name="R13"/>
<pin name="R14"/>
<pin name="R15"/>
<pin name="R16"/>
<pin name="T1"/>
<pin name="T2"/>
<pin name="T3"/>
<pin name="T4"/>
<pin name="T5"/>
<pin name="T6"/>
<pin name="T7"/>
<pin name="T8"/>
<pin name="T9"/>
<pin name="T10"/>
<pin name="T11"/>
<pin name="T12"/>
<pin name="T13"/>
<pin name="T14"/>
<pin name="T15"/>
<pin name="T16"/>
</symbol>
<symbol name="LPC4300_PORT0">
<pin name="PORT0_0"/>
<pin name="PORT0_1"/>
</symbol>
<symbol name="LPC4300_PORT1">
<pin name="PORT1_0"/>
<pin name="PORT1_1"/>
<pin name="PORT1_2"/>
<pin name="PORT1_3"/>
<pin name="PORT1_4"/>
<pin name="PORT1_5"/>
<pin name="PORT1_6"/>
<pin name="PORT1_7"/>
<pin name="PORT1_8"/>
<pin name="PORT1_9"/>
<pin name="PORT1_10"/>
<pin name="PORT1_11"/>
<pin name="PORT1_12"/>
<pin name="PORT1_13"/>
<pin name="PORT1_14"/>
<pin name="PORT1_15"/>
<pin name="PORT1_16"/>
<pin name="PORT1_17"/>
<pin name="PORT1_18"/>
<pin name="PORT1_19"/>
<pin name="PORT1_20"/>
</symbol>
<symbol name="LPC4300_PORT2">
<pin name="PORT2_0"/>
<pin name="PORT2_1"/>
<pin name="PORT2_2"/>
<pin name="PORT2_3"/>
<pin name="PORT2_4"/>
<pin name="PORT2_5"/>
<pin name="PORT2_6"/>
<pin name="PORT2_7"/>
<pin name="PORT2_8"/>
<pin name="PORT2_9"/>
<pin name="PORT2_10"/>
<pin name="PORT2_11"/>
<pin name="PORT2_12"/>
<pin name="PORT2_13"/>
</symbol>
<symbol name="LPC4300_PORT3">
<pin name="PORT3_0"/>
<pin name="PORT3_1"/>
<pin name="PORT3_2"/>
<pin name="PORT3_3"/>
<pin name="PORT3_4"/>
<pin name="PORT3_5"/>
<pin name="PORT3_6"/>
<pin name="PORT3_7"/>
<pin name="PORT3_8"/>
</symbol>
<symbol name="LPC4300_PORT4">
<pin name="PORT4_0"/>
<pin name="PORT4_1"/>
<pin name="PORT4_2"/>
<pin name="PORT4_3"/>
<pin name="PORT4_4"/>
<pin name="PORT4_5"/>
<pin name="PORT4_6"/>
<pin name="PORT4_7"/>
<pin name="PORT4_8"/>
<pin name="PORT4_9"/>
<pin name="PORT4_10"/>
</symbol>
<symbol name="LPC4300_PORT5">
<pin name="PORT5_0"/>
<pin name="PORT5_1"/>
<pin name="PORT5_2"/>
<pin name="PORT5_3"/>
<pin name="PORT5_4"/>
<pin name="PORT5_5"/>
<pin name="PORT5_6"/>
<pin name="PORT5_7"/>
</symbol>
<symbol name="LPC4300_PORT6">
<pin name="PORT6_0"/>
<pin name="PORT6_1"/>
<pin name="PORT6_2"/>
<pin name="PORT6_3"/>
<pin name="PORT6_4"/>
<pin name="PORT6_5"/>
<pin name="PORT6_6"/>
<pin name="PORT6_7"/>
<pin name="PORT6_8"/>
<pin name="PORT6_9"/>
<pin name="PORT6_10"/>
<pin name="PORT6_11"/>
<pin name="PORT6_12"/>
</symbol>
<symbol name="LPC4300_PORT7">
<pin name="PORT7_0"/>
<pin name="PORT7_1"/>
<pin name="PORT7_2"/>
<pin name="PORT7_3"/>
<pin name="PORT7_4"/>
<pin name="PORT7_5"/>
<pin name="PORT7_6"/>
<pin name="PORT7_7"/>
</symbol>
<symbol name="LPC4300_PORT8">
<pin name="PORT8_0"/>
<pin name="PORT8_1"/>
<pin name="PORT8_2"/>
<pin name="PORT8_3"/>
<pin name="PORT8_4"/>
<pin name="PORT8_5"/>
<pin name="PORT8_6"/>
<pin name="PORT8_7"/>
<pin name="PORT8_8" direction="sup"/>
</symbol>
<symbol name="LPC4300_PORT9">
<pin name="PORT9_0"/>
<pin name="PORT9_1"/>
<pin name="PORT9_2"/>
<pin name="PORT9_3"/>
<pin name="PORT9_4"/>
<pin name="PORT9_5"/>
<pin name="PORT9_6"/>
</symbol>
<symbol name="LPC4300_PORTA">
<pin name="PORTA_0"/>
<pin name="PORTA_1"/>
<pin name="PORTA_2"/>
<pin name="PORTA_3"/>
<pin name="PORTA_4"/>
</symbol>
<symbol name="LPC4300_PORTB">
<pin name="PORTB_0"/>
<pin name="PORTB_1"/>
<pin name="PORTB_2"/>
<pin name="PORTB_3"/>
<pin name="PORTB_4"/>
<pin name="PORTB_5"/>
<pin name="PORTB_6"/>
</symbol>
<symbol name="LPC4300_PORTC">
<pin name="PORTC_0"/>
<pin name="PORTC_1"/>
<pin name="PORTC_2"/>
<pin name="PORTC_3"/>
<pin name="PORTC_4"/>
<pin name="PORTC_5"/>
<pin name="PORTC_6"/>
<pin name="PORTC_7"/>
<pin name="PORTC_8"/>
<pin name="PORTC_9"/>
<pin name="PORTC_10"/>
<pin name="PORTC_11"/>
<pin name="PORTC_12"/>
<pin name="PORTC_13"/>
<pin name="PORTC_14"/>
</symbol>
<symbol name="LPC4300_PORTD">
<pin name="PORTD_0"/>
<pin name="PORTD_1"/>
<pin name="PORTD_2"/>
<pin name="PORTD_3"/>
<pin name="PORTD_4"/>
<pin name="PORTD_5"/>
<pin name="PORTD_6"/>
<pin name="PORTD_7"/>
<pin name="PORTD_8"/>
<pin name="PORTD_9"/>
<pin name="PORTD_10"/>
<pin name="PORTD_11"/>
<pin name="PORTD_12"/>
<pin name="PORTD_13"/>
<pin name="PORTD_14"/>
<pin name="PORTD_15"/>
<pin name="PORTD_16"/>
</symbol>
<symbol name="LPC4300_PORTE">
<pin name="PORTE_0"/>
<pin name="PORTE_1"/>
<pin name="PORTE_2"/>
<pin name="PORTE_3"/>
<pin name="PORTE_4"/>
<pin name="PORTE_5"/>
<pin name="PORTE_6"/>
<pin name="PORTE_7"/>
<pin name="PORTE_8"/>
<pin name="PORTE_9"/>
<pin name="PORTE_10"/>
<pin name="PORTE_11"/>
<pin name="PORTE_12"/>
<pin name="PORTE_13"/>
<pin name="PORTE_14"/>
<pin name="PORTE_15"/>
</symbol>
<symbol name="LPC4300_PORTF">
<pin name="PORTF_0"/>
<pin name="PORTF_1"/>
<pin name="PORTF_2"/>
<pin name="PORTF_3"/>
<pin name="PORTF_4"/>
<pin name="PORTF_5"/>
<pin name="PORTF_6"/>
<pin name="PORTF_7"/>
<pin name="PORTF_8"/>
<pin name="PORTF_9"/>
<pin name="PORTF_10"/>
<pin name="PORTF_11"/>
</symbol>
<symbol name="LPC4300_ANA">
<pin name="VSSA" direction="sup"/>
<pin name="ADC0"/>
<pin name="ADC1"/>
<pin name="ADC2"/>
<pin name="ADC3"/>
<pin name="ADC4"/>
<pin name="ADC5"/>
<pin name="ADC6"/>
<pin name="ADC7"/>
<pin name="VDDA" direction="sup"/>
</symbol>
<symbol name="LPC4300_AO">
<pin name="ALARM"/>
<pin name="RESET" function="dot"/>
<pin name="RTCX1"/>
<pin name="RTXC2"/>
<pin name="SAMPLE_N"/>
<pin name="VBAT"/>
<pin name="WAKEUP0"/>
<pin name="WAKEUP1"/>
<pin name="WAKEUP2"/>
<pin name="WAKEUP3"/>
</symbol>
<symbol name="LPC4300_CLK">
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="CLK3"/>
<pin name="CLK2"/>
<pin name="CLK1"/>
<pin name="CLK0"/>
</symbol>
<symbol name="LPC4300_DBUG">
<pin name="DBGEN"/>
<pin name="TDI"/>
<pin name="TCK"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST" function="dot"/>
</symbol>
<symbol name="LPC4300_SUP">
<pin name="VDDE@1" direction="sup"/>
<pin name="VDDE@2" direction="sup"/>
<pin name="VDDE@3" direction="sup"/>
<pin name="VDDE@4" direction="sup"/>
<pin name="VDDE@5" direction="sup"/>
<pin name="VDDE@6" direction="sup"/>
<pin name="VDDE@7" direction="sup"/>
<pin name="VDDE@8" direction="sup"/>
<pin name="VDDE@9" direction="sup"/>
<pin name="VDDE@10" direction="sup"/>
<pin name="VDDE@11" direction="sup"/>
<pin name="VDDE@12" direction="sup"/>
<pin name="VDDE@13" direction="sup"/>
<pin name="VDDC@2" direction="sup"/>
<pin name="VDDC@1" direction="sup"/>
<pin name="VDDC@3" direction="sup"/>
<pin name="VDDC@4" direction="sup"/>
<pin name="VPP" direction="sup"/>
<pin name="VSS@1" direction="sup"/>
<pin name="VSS@2" direction="sup"/>
<pin name="VSS@3" direction="sup"/>
<pin name="VSS@4" direction="sup"/>
<pin name="VSS@5" direction="sup"/>
<pin name="VSS@6" direction="sup"/>
<pin name="VSS@7" direction="sup"/>
<pin name="VSS@8" direction="sup"/>
<pin name="VSS@9" direction="sup"/>
<pin name="VSS@10" direction="sup"/>
<pin name="VSS@11" direction="sup"/>
<pin name="VSS@12" direction="sup"/>
<pin name="VSS@13" direction="sup"/>
<pin name="VSS@14" direction="sup"/>
<pin name="VSS@15" direction="sup"/>
<pin name="VSS@16" direction="sup"/>
<pin name="VSS@17" direction="sup"/>
<pin name="VSS@18" direction="sup"/>
<pin name="VSS@19" direction="sup"/>
</symbol>
<symbol name="LPC4300_USB">
<pin name="USB_DM1"/>
<pin name="USB_DP1"/>
<pin name="USB_DM0"/>
<pin name="USB_DP0"/>
<pin name="USB_ID"/>
<pin name="USB_RREF"/>
<pin name="USB_VBUS"/>
<pin name="USB_VDDA3V3"/>
<pin name="USB_VDDA3V3_DRIVER"/>
<pin name="USB_VSSA_REF"/>
<pin name="USB_VSSA_TERM"/>
</symbol>
<symbol name="LPC4300_I2C">
<pin name="SDA" direction="sup"/>
<pin name="SCL" direction="sup"/>
</symbol>
<symbol name="LPC1800_PORT0">
<pin name="PORT0_0"/>
<pin name="PORT0_1"/>
</symbol>
<symbol name="LPC1800_PORT1">
<pin name="PORT1_0"/>
<pin name="PORT1_1"/>
<pin name="PORT1_2"/>
<pin name="PORT1_3"/>
<pin name="PORT1_4"/>
<pin name="PORT1_5"/>
<pin name="PORT1_6"/>
<pin name="PORT1_7"/>
<pin name="PORT1_8"/>
<pin name="PORT1_9"/>
<pin name="PORT1_10"/>
<pin name="PORT1_11"/>
<pin name="PORT1_12"/>
<pin name="PORT1_13"/>
<pin name="PORT1_14"/>
<pin name="PORT1_15"/>
<pin name="PORT1_16"/>
<pin name="PORT1_17"/>
<pin name="PORT1_18"/>
<pin name="PORT1_19"/>
<pin name="PORT1_20"/>
</symbol>
<symbol name="LPC1800_PORT2">
<pin name="PORT2_0"/>
<pin name="PORT2_1"/>
<pin name="PORT2_2"/>
<pin name="PORT2_3"/>
<pin name="PORT2_4"/>
<pin name="PORT2_5"/>
<pin name="PORT2_6"/>
<pin name="PORT2_7"/>
<pin name="PORT2_8"/>
<pin name="PORT2_9"/>
<pin name="PORT2_10"/>
<pin name="PORT2_11"/>
<pin name="PORT2_12"/>
<pin name="PORT2_13"/>
</symbol>
<symbol name="LPC1800_PORT3">
<pin name="PORT3_0"/>
<pin name="PORT3_1"/>
<pin name="PORT3_2"/>
<pin name="PORT3_3"/>
<pin name="PORT3_4"/>
<pin name="PORT3_5"/>
<pin name="PORT3_6"/>
<pin name="PORT3_7"/>
<pin name="PORT3_8"/>
</symbol>
<symbol name="LPC1800_PORT4">
<pin name="PORT4_0"/>
<pin name="PORT4_1"/>
<pin name="PORT4_2"/>
<pin name="PORT4_3"/>
<pin name="PORT4_4"/>
<pin name="PORT4_5"/>
<pin name="PORT4_6"/>
<pin name="PORT4_7"/>
<pin name="PORT4_8"/>
<pin name="PORT4_9"/>
<pin name="PORT4_10"/>
</symbol>
<symbol name="LPC1800_PORT5">
<pin name="PORT5_0"/>
<pin name="PORT5_1"/>
<pin name="PORT5_2"/>
<pin name="PORT5_3"/>
<pin name="PORT5_4"/>
<pin name="PORT5_5"/>
<pin name="PORT5_6"/>
<pin name="PORT5_7"/>
</symbol>
<symbol name="LPC1800_PORT6">
<pin name="PORT6_0"/>
<pin name="PORT6_1"/>
<pin name="PORT6_2"/>
<pin name="PORT6_3"/>
<pin name="PORT6_4"/>
<pin name="PORT6_5"/>
<pin name="PORT6_6"/>
<pin name="PORT6_7"/>
<pin name="PORT6_8"/>
<pin name="PORT6_9"/>
<pin name="PORT6_10"/>
<pin name="PORT6_11"/>
<pin name="PORT6_12"/>
</symbol>
<symbol name="LPC1800_PORT7">
<pin name="PORT7_0"/>
<pin name="PORT7_1"/>
<pin name="PORT7_2"/>
<pin name="PORT7_3"/>
<pin name="PORT7_4"/>
<pin name="PORT7_5"/>
<pin name="PORT7_6"/>
<pin name="PORT7_7"/>
</symbol>
<symbol name="LPC1800_PORT8">
<pin name="PORT8_0"/>
<pin name="PORT8_1"/>
<pin name="PORT8_2"/>
<pin name="PORT8_3"/>
<pin name="PORT8_4"/>
<pin name="PORT8_5"/>
<pin name="PORT8_6"/>
<pin name="PORT8_7"/>
<pin name="PORT8_8" direction="sup"/>
</symbol>
<symbol name="LPC1800_PORT9">
<pin name="PORT9_0"/>
<pin name="PORT9_1"/>
<pin name="PORT9_2"/>
<pin name="PORT9_3"/>
<pin name="PORT9_4"/>
<pin name="PORT9_5"/>
<pin name="PORT9_6"/>
</symbol>
<symbol name="LPC1800_PORTA">
<pin name="PORTA_0"/>
<pin name="PORTA_1"/>
<pin name="PORTA_2"/>
<pin name="PORTA_3"/>
<pin name="PORTA_4"/>
</symbol>
<symbol name="LPC1800_PORTB">
<pin name="PORTB_0"/>
<pin name="PORTB_1"/>
<pin name="PORTB_2"/>
<pin name="PORTB_3"/>
<pin name="PORTB_4"/>
<pin name="PORTB_5"/>
<pin name="PORTB_6"/>
</symbol>
<symbol name="LPC1800_PORTC">
<pin name="PORTC_0"/>
<pin name="PORTC_1"/>
<pin name="PORTC_2"/>
<pin name="PORTC_3"/>
<pin name="PORTC_4"/>
<pin name="PORTC_5"/>
<pin name="PORTC_6"/>
<pin name="PORTC_7"/>
<pin name="PORTC_8"/>
<pin name="PORTC_9"/>
<pin name="PORTC_10"/>
<pin name="PORTC_11"/>
<pin name="PORTC_12"/>
<pin name="PORTC_13"/>
<pin name="PORTC_14"/>
</symbol>
<symbol name="LPC1800_PORTD">
<pin name="PORTD_0"/>
<pin name="PORTD_1"/>
<pin name="PORTD_2"/>
<pin name="PORTD_3"/>
<pin name="PORTD_4"/>
<pin name="PORTD_5"/>
<pin name="PORTD_6"/>
<pin name="PORTD_7"/>
<pin name="PORTD_8"/>
<pin name="PORTD_9"/>
<pin name="PORTD_10"/>
<pin name="PORTD_11"/>
<pin name="PORTD_12"/>
<pin name="PORTD_13"/>
<pin name="PORTD_14"/>
<pin name="PORTD_15"/>
<pin name="PORTD_16"/>
</symbol>
<symbol name="LPC1800_PORTE">
<pin name="PORTE_0"/>
<pin name="PORTE_1"/>
<pin name="PORTE_2"/>
<pin name="PORTE_3"/>
<pin name="PORTE_4"/>
<pin name="PORTE_5"/>
<pin name="PORTE_6"/>
<pin name="PORTE_7"/>
<pin name="PORTE_8"/>
<pin name="PORTE_9"/>
<pin name="PORTE_10"/>
<pin name="PORTE_11"/>
<pin name="PORTE_12"/>
<pin name="PORTE_13"/>
<pin name="PORTE_14"/>
<pin name="PORTE_15"/>
</symbol>
<symbol name="LPC1800_PORTF">
<pin name="PORTF_0"/>
<pin name="PORTF_1"/>
<pin name="PORTF_2"/>
<pin name="PORTF_3"/>
<pin name="PORTF_4"/>
<pin name="PORTF_5"/>
<pin name="PORTF_6"/>
<pin name="PORTF_7"/>
<pin name="PORTF_8"/>
<pin name="PORTF_9"/>
<pin name="PORTF_10"/>
<pin name="PORTF_11"/>
</symbol>
<symbol name="LPC1800_ANA">
<pin name="VSSA" direction="sup"/>
<pin name="ADC0"/>
<pin name="ADC1"/>
<pin name="ADC2"/>
<pin name="ADC3"/>
<pin name="ADC4"/>
<pin name="ADC5"/>
<pin name="ADC6"/>
<pin name="ADC7"/>
<pin name="VDDA" direction="sup"/>
</symbol>
<symbol name="LPC1800_AO">
<pin name="ALARM"/>
<pin name="RESET" function="dot"/>
<pin name="RTCX1"/>
<pin name="RTXC2"/>
<pin name="SAMPLE_N"/>
<pin name="VBAT"/>
<pin name="WAKEUP0"/>
<pin name="WAKEUP1"/>
<pin name="WAKEUP2"/>
<pin name="WAKEUP3"/>
</symbol>
<symbol name="LPC1800_CLK">
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="CLK3"/>
<pin name="CLK2"/>
<pin name="CLK1"/>
<pin name="CLK0"/>
</symbol>
<symbol name="LPC1800_DBUG">
<pin name="DBGEN"/>
<pin name="TDI"/>
<pin name="TCK"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST" function="dot"/>
</symbol>
<symbol name="LPC1800_SUP">
<pin name="VDDE@1" direction="sup"/>
<pin name="VDDE@2" direction="sup"/>
<pin name="VDDE@3" direction="sup"/>
<pin name="VDDE@4" direction="sup"/>
<pin name="VDDE@5" direction="sup"/>
<pin name="VDDE@6" direction="sup"/>
<pin name="VDDE@7" direction="sup"/>
<pin name="VDDE@8" direction="sup"/>
<pin name="VDDE@9" direction="sup"/>
<pin name="VDDE@10" direction="sup"/>
<pin name="VDDE@11" direction="sup"/>
<pin name="VDDE@12" direction="sup"/>
<pin name="VDDE@13" direction="sup"/>
<pin name="VDDC@2" direction="sup"/>
<pin name="VDDC@1" direction="sup"/>
<pin name="VDDC@3" direction="sup"/>
<pin name="VDDC@4" direction="sup"/>
<pin name="VPP" direction="sup"/>
<pin name="VSS@1" direction="sup"/>
<pin name="VSS@2" direction="sup"/>
<pin name="VSS@3" direction="sup"/>
<pin name="VSS@4" direction="sup"/>
<pin name="VSS@5" direction="sup"/>
<pin name="VSS@6" direction="sup"/>
<pin name="VSS@7" direction="sup"/>
<pin name="VSS@8" direction="sup"/>
<pin name="VSS@9" direction="sup"/>
<pin name="VSS@10" direction="sup"/>
<pin name="VSS@11" direction="sup"/>
<pin name="VSS@12" direction="sup"/>
<pin name="VSS@13" direction="sup"/>
<pin name="VSS@14" direction="sup"/>
<pin name="VSS@15" direction="sup"/>
<pin name="VSS@16" direction="sup"/>
<pin name="VSS@17" direction="sup"/>
<pin name="VSS@18" direction="sup"/>
<pin name="VSS@19" direction="sup"/>
</symbol>
<symbol name="LPC1800_USB">
<pin name="USB_DM1"/>
<pin name="USB_DP1"/>
<pin name="USB_DM0"/>
<pin name="USB_DP0"/>
<pin name="USB_ID"/>
<pin name="USB_RREF"/>
<pin name="USB_VBUS"/>
<pin name="USB_VDDA3V3"/>
<pin name="USB_VDDA3V3_DRIVER"/>
<pin name="USB_VSSA_REF"/>
<pin name="USB_VSSA_TERM"/>
</symbol>
<symbol name="LPC1800_I2C">
<pin name="SDA" direction="sup"/>
<pin name="SCL" direction="sup"/>
</symbol>
<symbol name="LPC1788_PWR-208">
<pin name="JTAG_TDO(SWO)"/>
<pin name="JTAG_TDI"/>
<pin name="JTAG_TMS(SWDIO)"/>
<pin name="!JTAG_TRST!"/>
<pin name="JTAG_TCK(SWDCLK)"/>
<pin name="!RESET!"/>
<pin name="!RSTOUT!"/>
<pin name="RTC_ALARM"/>
<pin name="RTCX1"/>
<pin name="RTCX2"/>
<pin name="VBAT"/>
<pin name="VDDA"/>
<pin name="VREFP"/>
<pin name="VSSA"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VDD(REG)(3V3)1"/>
<pin name="VDD(REG)(3V3)2"/>
<pin name="VDD(REG)(3V3)3"/>
<pin name="VDD(3V3)1"/>
<pin name="VDD(3V3)2"/>
<pin name="VDD(3V3)3"/>
<pin name="VDD(3V3)4"/>
<pin name="VDD(3V3)5"/>
<pin name="VDD(3V3)6"/>
<pin name="VDD(3V3)7"/>
<pin name="VDD(3V3)8"/>
<pin name="VDD(3V3)9"/>
<pin name="VDD(3V3)10"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSS4"/>
<pin name="VSS5"/>
<pin name="VSS6"/>
<pin name="VSS7"/>
<pin name="VSS8"/>
<pin name="VSS9"/>
<pin name="VSS10"/>
<pin name="VSS(REG)1"/>
<pin name="VSS(REG)2"/>
<pin name="VSS(REG)3"/>
</symbol>
<symbol name="LPC1788_PORT0-208">
<pin name="P0[0]/CAN_RD1/U3_TXD/I2C1_SDA/U0_TXD"/>
<pin name="P0[1]/CAN_TD1/U3_RXD/I2C1_SCL/U0_RXD"/>
<pin name="P0[2]/U0_TXD/U3_TXD"/>
<pin name="P0[3]/U0_RXD/U3_RXD"/>
<pin name="P0[4]/I2S_RX_SCK/CAN_RD_2/T2_CAP0/LCD_VD[0]"/>
<pin name="P0[5]/I2S_RX_WS/CAN_TD_2/T2_CAP1/LCD_VD[1]"/>
<pin name="P0[6]/I2S_RX_SDA/SSP1_SSEL/T2_MAT0/U1_RTS/LCD_VD[8]"/>
<pin name="P0[7]/I2S_TX_SCK/SSP1_SCK/T2_MAT1/LCD_VD[9]"/>
<pin name="P0[8]/I2S_TX_WS/SSP1_MISO/T2_MAT2/LCD_VD[16]"/>
<pin name="P0[9]/I2S_TX_SDA/SSP1_MOSI/T2_MAT3/LCD_VD[17]"/>
<pin name="P0[10]/U2_TXD/I2C2_SDA/T3_MAT0"/>
<pin name="P0[11]/U2_RXD/I2C2_SCL/T3_MAT1"/>
<pin name="P0[12]/!USB_PPWR2!/SSP1_MISO/ADC0_IN[6]"/>
<pin name="P0[13]/USB_UP_LED2/SSP1_MOSI/ADC0_IN[7]"/>
<pin name="P0[14]/!USB_HSTEN2!/SSP1_SSEL/USB_CONNECT2"/>
<pin name="P0[15]/U1_TXD/SSP0_SCK"/>
<pin name="P0[16]/U1_RXD/SSP0_SSEL"/>
<pin name="P0[17]/U1_CTS/SSP0_MISO"/>
<pin name="P0[18]/U1_DCD/SSP0_MOSI"/>
<pin name="P0[19]/U1_DSR/SD_CLK/I2C1_SDA"/>
<pin name="P0[20]/U1_DTR/SD_CMD/I2C1_SCL"/>
<pin name="P0[21]/U1_RI/SD_PWR/U4_OE/CAN_RD1"/>
<pin name="P0[22]/U1_RTS/SD_DAT[0]/U4_TXD/CAN_TD1"/>
<pin name="P0[23]/ADC0_IN[0]/I2S_RX_SCK/T3_CAP0"/>
<pin name="P0[24]/ADC0_IN[1]/I2S_RX_WS/T3_CAP1"/>
<pin name="P0[25]/ADC0_IN[2]/I2S_RX_SDA/U3_TXD"/>
<pin name="P0[26]/ADC0_IN[3]/DAC_OUT/U3_RXD"/>
<pin name="P0[27]/I2C0_SDA/USB_SDA1"/>
<pin name="P0[28]/I2C0_SCL/USB_SCL1"/>
<pin name="P0[29]/USB_D+1/EINT_0"/>
<pin name="P0[30]/USB_D?1/EINT_1"/>
<pin name="P0[31]/USB_D+2"/>
<pin name="USB_D-2"/>
</symbol>
<symbol name="LPC1788_PORT1-208">
<pin name="P1[0]/ENET_TXD0/T3_CAP1/SSP2_SCK"/>
<pin name="P1[1]/ENET_TXD1/T3_MAT3/SSP2_MOSI"/>
<pin name="P1[2]/ENET_TXD2/SD_CLK/PWM0_1"/>
<pin name="P1[3]/ENET_TXD3/SD_CMD/PWM0_2"/>
<pin name="P1[4]/ENET_TX_EN/T3_MAT2/SSP2_MISO"/>
<pin name="P1[5]/ENET_TX_ER/SD_PWR/PWM0_3"/>
<pin name="P1[6]/ENET_TX_CLK/SD_DAT[0]/PWM0_4"/>
<pin name="P1[7]/ENET_COL/SD_DAT[1]/PWM0_5"/>
<pin name="P1[8]/ENET_CRS/T3_MAT1/SSP2_SSEL"/>
<pin name="P1[9]/ENET_RXD0/T3_MAT0"/>
<pin name="P1[10]/ENET_RXD1/T3_CAP0"/>
<pin name="P1[11]/ENET_RXD2/SD_DAT[2]/PWM0_6"/>
<pin name="P1[12]/ENET_RXD3/SD_DAT[3]/PWM0_CAP0"/>
<pin name="P1[13]/ENET_RX_DV"/>
<pin name="P1[14]/ENET_RX_ER/T2_CAP0"/>
<pin name="P1[15]/ENET_RX_CLK/I2C2_SDA"/>
<pin name="P1[16]/ENET_MDC/I2S_TX_MCLK"/>
<pin name="P1[17]/ENET_MDIO/I2S_RX_MCLK"/>
<pin name="P1[18]/USB_UP_LED1/PWM1_1/T1_CAP0/SSP1_MISO"/>
<pin name="P1[19]/!USB_TX_E1!/!USB_PPWR1!/T1_CAP1/MC_0A/SSP1_SCK/U2_OE"/>
<pin name="P1[20]/USB_TX_DP1/PWM1_2/QEI_PHA/MC_FB0/SSP0_SCK/LCD_VD[6]/LCD_VD[10]"/>
<pin name="P1[21]/USB_TX_DM1/PWM1_3/SSP0_SSEL/!MC_ABORT!/LCD_VD[7]/LCD_VD[11]"/>
<pin name="P1[22]/USB_RCV1/USB_PWRD1/T1_MAT0/MC_0B/SSP1_MOSI/LCD_VD[8]/LCD_VD[12]"/>
<pin name="P1[23]/USB_RX_DP1/PWM1_4/QEI_PHB/MC_FB1/SSP0_MISO/LCD_VD[9]/LCD_VD[13]"/>
<pin name="P1[24]/USB_RX_DM1/PWM1_5/QEI_IDX/MC_FB2/SSP0_MOSI/LCD_VD[10]/LCD_VD[14]"/>
<pin name="P1[25]/!USB_LS1!/!USB_HSTEN1!/T1_MAT1/MC_1A/CLKOUT/LCD_VD[11]/LCD_VD[15]"/>
<pin name="P1[26]/!USB_SSPND1!/PWM1_6/T0_CAP0/MC_1B/SSP1_SSEL/LCD_VD[12]/LCD_VD[20]"/>
<pin name="P1[27]/!USB_INT1!/!USB_OVRCR1!/T0_CAP1/CLKOUT/LCD_VD[13]/LCD_VD[21]"/>
<pin name="P1[28]/USB_SCL1/PWM1_CAP0/T0_MAT0/MC_2A/SSP0_SSEL/LCD_VD[14]/LCD_VD[22]"/>
<pin name="P1[29]/USB_SDA1/PWM1_CAP1/T0_MAT1/MC_2B/U4_TXD/LCD_VD[15]/LCD_VD[23]"/>
<pin name="P1[30]/USB_PWRD2/USB_VBUS/ADC0_IN[4]/I2C0_SDA/U3_OE"/>
<pin name="P1[31]/USB_OVRCR2/SSP1_SCK/ADC0_IN[5]/I2C0_SCL"/>
</symbol>
<symbol name="LPC1788_PORT2-208">
<pin name="P2[0]/PWM1[1]/U1_TXD/LCD_PWR"/>
<pin name="P2[1]/PWM1[2]/U1_RXD/LCD_LE"/>
<pin name="P2[2]/PWM1[3]/U1_CTS/T2_MAT3/TRACEDATA[3]/LCD_DCLK"/>
<pin name="P2[3]/PWM1[4]/U1_DCD/T2_MAT2/TRACEDATA[2]/LCD_FP"/>
<pin name="P2[4]/PWM1[5]/U1_DSR/T2_MAT1/TRACEDATA[1]/LCD_ENAB_M"/>
<pin name="P2[5]/PWM1[6]/U1_DTR/T2_MAT0/TRACEDATA[0]/LCD_LP"/>
<pin name="P2[6]/PWM1_CAP0/U1_RI/T2_CAP0/U2_OE/TRACECLK/LCD_VD[0]/LCD_VD[4]"/>
<pin name="P2[7]/CAN_RD2/U1_RTS/LCD_VD[1]/LCD_VD[5]"/>
<pin name="P2[8]/CAN_TD2/U2_TXD/U1_CTS/ENET_MDC/LCD_VD[2]/LCD_VD[6]"/>
<pin name="P2[9]/USB_CONNECT1/U2_RXD/U4_RXD/ENET_MDIO/LCD_VD[3]/LCD_VD[7]"/>
<pin name="P2[10]/EINT_0/NMI"/>
<pin name="P2[11]/EINT1/SD_DAT[1]/I2S_TX_SCK/LCD_CLKIN"/>
<pin name="P2[12]/EINT2/SD_DAT[2]/I2S_TX_WS/LCD_VD[4]/LCD_VD[3]/LCD_VD[8]/LCD_VD[18]"/>
<pin name="P2[13]/EINT3/SD_DAT[3]/I2S_TX_SDA/LCD_VD[5]/LCD_VD[9]/LCD_VD[19]"/>
<pin name="P2[14]/!EMC_CS2!/I2C1_SDA/T2_CAP0"/>
<pin name="P2[15/!EMC_CS3!/I2C1_SCL/T2_CAP1"/>
<pin name="P2[16]/!EMC_CAS!"/>
<pin name="P2[17]/!EMC_RAS!"/>
<pin name="P2[18]/EMC_CLK[0]"/>
<pin name="P2[19]/EMC_CLK[1]"/>
<pin name="P2[20]/!EMC_DYCS0!"/>
<pin name="P2[21]/!EMC_DYCS1!"/>
<pin name="P2[22]/!EMC_DYCS2!/SSP0_SCK/T3_CAP0"/>
<pin name="P2[23]/!EMC_DYCS3!/SSP0_SSEL/T3_CAP1"/>
<pin name="P2[24]/EMC_CKE0"/>
<pin name="P2[25]/EMC_CKE1"/>
<pin name="P2[26]/EMC_CKE2/SSP0_MISO/T3_MAT0"/>
<pin name="P2[27]/EMC_CKE3/SSP0_MOSI/T3_MAT1"/>
<pin name="P2[28]/EMC_DQM0"/>
<pin name="P2[29]/EMC_DQM1"/>
<pin name="P2[30]/EMC_DQM2/I2C2_SDA/T3_MAT2"/>
<pin name="P2[31]/EMC_DQM3/I2C2_SCL/T3_MAT3"/>
</symbol>
<symbol name="LPC1788_PORT3-208">
<pin name="P3[0]/EMC_D[0]"/>
<pin name="P3[1]/EMC_D[1]"/>
<pin name="P3[2]/EMC_D[2]"/>
<pin name="P3[3]/EMC_D[3]"/>
<pin name="P3[4]/EMC_D[4]"/>
<pin name="P3[5]/EMC_D[5]"/>
<pin name="P3[6]/EMC_D[6]"/>
<pin name="P3[7]/EMC_D[7]"/>
<pin name="P3[8]/EMC_D[8]"/>
<pin name="P3[9]/EMC_D[9]"/>
<pin name="P3[10]/EMC_D[10]"/>
<pin name="P3[11]/EMC_D[11]"/>
<pin name="P3[12]/EMC_D[12]"/>
<pin name="P3[13]/EMC_D[13]"/>
<pin name="P3[14]/EMC_D[14]"/>
<pin name="P3[15]/EMC_D[15]"/>
<pin name="P3[16]/EMC_D[16]/PWM0_1/U1_TXD"/>
<pin name="P3[17]/EMC_D[17]/PWM0_2/U1_RXD"/>
<pin name="P3[18]/EMC_D[18]/PWM0_3/U1_CTS"/>
<pin name="P3[19]/EMC_D[19]/PWM0_4/U1_DCD"/>
<pin name="P3[20]/EMC_D[20]/PWM0_5/U1_DSR"/>
<pin name="P3[21]/EMC_D[21]/PWM0_6/U1_DTR"/>
<pin name="P3[22]/EMC_D[22]/PWM0_CAP0/U1_RI"/>
<pin name="P3[23]/EMC_D[23]/PWM1_CAP0/T0_CAP0"/>
<pin name="P3[24]/EMC_D[24]/PWM1[1]/T0_CAP1"/>
<pin name="P3[25]/EMC_D[25]/PWM1[2]/T0_MAT0"/>
<pin name="P3[26]/EMC_D[26]/PWM1[3]/T0_MAT1/STCLK"/>
<pin name="P3[27]/EMC_D[27]/PWM1[4]/T1_CAP0"/>
<pin name="P3[28]/EMC_D[28]/PWM1[5]/T1_CAP1"/>
<pin name="P3[29]/EMC_D[29]/PWM1[6]/T1_MAT0"/>
<pin name="P3[30]/EMC_D[30]/U1_RTS/T1_MAT1"/>
<pin name="P3[31]/EMC_D[31]/T1_MAT2"/>
</symbol>
<symbol name="LPC1788_PORT4-208">
<pin name="P4[0]/EMC_A[0]"/>
<pin name="P4[1]/EMC_A[1]"/>
<pin name="P4[2]/EMC_A[2]"/>
<pin name="P4[3]/EMC_A[3]"/>
<pin name="P4[4]/EMC_A[4]"/>
<pin name="P4[5]/EMC_A[5]"/>
<pin name="P4[6]/EMC_A[6]"/>
<pin name="P4[7]/EMC_A[7]"/>
<pin name="P4[8]/EMC_A[8]"/>
<pin name="P4[9]/EMC_A[9]"/>
<pin name="P4[10]/EMC_A[10]"/>
<pin name="P4[11]/EMC_A[11]"/>
<pin name="P4[12]/EMC_A[12]"/>
<pin name="P4[13]/EMC_A[13]"/>
<pin name="P4[14]/EMC_A[14]"/>
<pin name="P4[15]/EMC_A[15]"/>
<pin name="P4[16]/EMC_A[16]"/>
<pin name="P4[17]/EMC_A[17]"/>
<pin name="P4[18]/EMC_A[18]"/>
<pin name="P4[19]/EMC_A[19]"/>
<pin name="P4[20]/EMC_A[20]/I2C2_SDA/SSP1_SCK"/>
<pin name="P4[21]/EMC_A[21]/I2C2_SCL/SSP1_SSEL"/>
<pin name="P4[22]/EMC_A[22]/U2_TXD/SSP1_MISO"/>
<pin name="P4[23]/EMC_A[23]/U2_RXD/SSP1_MOSI"/>
<pin name="P4[24]/!EMC_OE!"/>
<pin name="P4[25]/!EMC_WE!"/>
<pin name="P4[26]/!EMC_BLS0!"/>
<pin name="P4[27]/!EMC_BLS1!"/>
<pin name="P4[28]/!EMC_BLS2!/U3_TXD/T2_MAT0/LCD_VD[6]/LCD_VD[10]/LCD_VD[2]"/>
<pin name="P4[29]/!EMC_BLS3!/U3_RXD/T2_MAT1/I2C2_SCL/LCD_VD[7]/LCD_VD[11]/LCD_VD[3]"/>
<pin name="P4[30]/!EMC_CS0!"/>
<pin name="P4[31]/!EMC_CS1!"/>
</symbol>
<symbol name="LPC1788_PORT5-208">
<pin name="P5[0]/EMC_A[24]/T2_MAT2"/>
<pin name="P5[1]/EMC_A[25]/T2_MAT3"/>
<pin name="P5[2]/T3_MAT2/I2C0_SDA"/>
<pin name="P5[3]/U4_RXD/I2C0_SCL"/>
<pin name="P5[4]/U0_OE/T3_MAT3/U4_TXD"/>
</symbol>
<symbol name="FRAME_A4_ADAFRUIT">
</symbol>
<symbol name="FRAME_A3_ADAFRUIT">
</symbol>
<symbol name="SEGMENT_8X8_BICOLOR_CATHODEROW">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
</symbol>
<symbol name="SEGMENT_8X8_CATHODEROW">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
</symbol>
<symbol name="SEGMENT_12BAR_BICOLOR_CATHODEROW">
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
</symbol>
<symbol name="SEGMENT_STARBURST_COMMONCATHODE">
<pin name="VCC" direction="pwr"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G1"/>
<pin name="G2"/>
<pin name="H"/>
<pin name="J"/>
<pin name="K"/>
<pin name="L"/>
<pin name="M"/>
<pin name="N"/>
<pin name="DP"/>
</symbol>
<symbol name="SEGMENT_STARBURST_COMMONCATHODE_2VCC">
<pin name="VCC1" direction="pwr"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G1"/>
<pin name="G2"/>
<pin name="H"/>
<pin name="J"/>
<pin name="K"/>
<pin name="L"/>
<pin name="M"/>
<pin name="N"/>
<pin name="DP"/>
<pin name="VCC2" direction="pwr"/>
</symbol>
<symbol name="DS1302">
<pin name="CE"/>
<pin name="IO"/>
<pin name="SCLK"/>
<pin name="GND"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="X1"/>
<pin name="X2"/>
</symbol>
<symbol name="PINH2X23">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
<pin name="41" direction="pas" function="dot"/>
<pin name="42" direction="pas" function="dot"/>
<pin name="43" direction="pas" function="dot"/>
<pin name="44" direction="pas" function="dot"/>
<pin name="45" direction="pas" function="dot"/>
<pin name="46" direction="pas" function="dot"/>
</symbol>
<symbol name="BEAGLEBONE">
<pin name="GND@1" direction="pwr" function="dot"/>
<pin name="GND@2" direction="pwr" function="dot"/>
<pin name="VDD_3V3EXP@1" direction="pwr" function="dot"/>
<pin name="VDD_3V3EXP@2" direction="pwr" function="dot"/>
<pin name="VDD_5V@1" direction="pwr" function="dot"/>
<pin name="VDD_5V@2" direction="pwr" function="dot"/>
<pin name="SYS_5V@1" direction="pwr" function="dot"/>
<pin name="SYS_5V@2" direction="pwr" function="dot"/>
<pin name="PWR_BUT" function="dot"/>
<pin name="SYS_RESETN" direction="in" function="dot"/>
<pin name="UART4_RXD" direction="in" function="dot"/>
<pin name="GPIO1_28" function="dot"/>
<pin name="UART4_TXD" direction="out" function="dot"/>
<pin name="EHRPWM1A" function="dot"/>
<pin name="GPIO1_16" function="dot"/>
<pin name="EHRPWM1B" function="dot"/>
<pin name="I2C1_SCL" function="dot"/>
<pin name="I2C1_SDA" function="dot"/>
<pin name="I2C2_SCL" function="dot"/>
<pin name="I2C2_SDA" function="dot"/>
<pin name="UART2_TXD" direction="out" function="dot"/>
<pin name="UART2_RXD" direction="in" function="dot"/>
<pin name="GPIO1_17" function="dot"/>
<pin name="UART1_TXD" direction="out" function="dot"/>
<pin name="GPIO3_21" function="dot"/>
<pin name="UART1_RXD" direction="in" function="dot"/>
<pin name="GPIO3_19" function="dot"/>
<pin name="SPI1_CS0" function="dot"/>
<pin name="SPI1_DO" function="dot"/>
<pin name="SPI1_DI" function="dot"/>
<pin name="SPI1_SCLK" function="dot"/>
<pin name="VDD_ADC" direction="pwr" function="dot"/>
<pin name="AIN4" direction="in" function="dot"/>
<pin name="GNDA_ADC" direction="pwr" function="dot"/>
<pin name="AIN6" direction="in" function="dot"/>
<pin name="AIN5" direction="in" function="dot"/>
<pin name="AIN2" direction="in" function="dot"/>
<pin name="AIN3" direction="in" function="dot"/>
<pin name="AIN0" direction="in" function="dot"/>
<pin name="AIN1" direction="in" function="dot"/>
<pin name="CLKOUT2" direction="out" function="dot"/>
<pin name="GPIO0_7" function="dot"/>
<pin name="GND@3" direction="pwr" function="dot"/>
<pin name="GND@5" direction="pwr" function="dot"/>
<pin name="GND@4" direction="pwr" function="dot"/>
<pin name="GND@6" direction="pwr" function="dot"/>
<pin name="GND@7" direction="pwr" function="dot"/>
<pin name="GND@8" direction="pwr" function="dot"/>
<pin name="GPIO1_6" function="dot"/>
<pin name="GPIO1_7" function="dot"/>
<pin name="GPIO1_2" function="dot"/>
<pin name="GPIO1_3" function="dot"/>
<pin name="TIMER4" function="dot"/>
<pin name="TIMER7" function="dot"/>
<pin name="TIMER5" function="dot"/>
<pin name="TIMER6" function="dot"/>
<pin name="GPIO1_13" function="dot"/>
<pin name="GPIO1_12" function="dot"/>
<pin name="EHRPWM2B" function="dot"/>
<pin name="GPIO0_26" function="dot"/>
<pin name="GPIO1_15" function="dot"/>
<pin name="GPIO1_14" function="dot"/>
<pin name="GPIO0_27" function="dot"/>
<pin name="GPIO2_1" function="dot"/>
<pin name="EHRPWM2A" function="dot"/>
<pin name="GPIO1_31" function="dot"/>
<pin name="GPIO1_30" function="dot"/>
<pin name="GPIO1_5" function="dot"/>
<pin name="GPIO1_4" function="dot"/>
<pin name="GPIO1_1" function="dot"/>
<pin name="GPIO1_0" function="dot"/>
<pin name="GPIO1_29" function="dot"/>
<pin name="GPIO2_22" function="dot"/>
<pin name="GPIO2_24" function="dot"/>
<pin name="GPIO2_23" function="dot"/>
<pin name="GPIO2_25" function="dot"/>
<pin name="UART5_CTSN" function="dot"/>
<pin name="UART5_RTSN" function="dot"/>
<pin name="UART4_RTSN" function="dot"/>
<pin name="UART3_RTSN" function="dot"/>
<pin name="UART4_CTSN" function="dot"/>
<pin name="UART3_CTSN" function="dot"/>
<pin name="UART5_TXD" direction="out" function="dot"/>
<pin name="UART5_RXD" direction="in" function="dot"/>
<pin name="GPIO2_12" function="dot"/>
<pin name="GPIO2_13" function="dot"/>
<pin name="GPIO2_10" function="dot"/>
<pin name="GPIO2_11" function="dot"/>
<pin name="GPIO2_8" function="dot"/>
<pin name="GPIO2_9" function="dot"/>
<pin name="GPIO2_6" function="dot"/>
<pin name="GPIO2_7" function="dot"/>
</symbol>
<symbol name="PINHD23">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
</symbol>
<symbol name="BREAKOUT_SOIC24">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
</symbol>
<symbol name="BREAKOUT_SOT23-6">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="BREAKOUT_SOIC8">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="SHUNT-VREF">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="VREF" direction="pas"/>
</symbol>
<symbol name="LPC1850_EMC">
<pin name="EMC_A0"/>
<pin name="EMC_A1"/>
<pin name="EMC_A2"/>
<pin name="EMC_A3"/>
<pin name="EMC_A4"/>
<pin name="EMC_A5"/>
<pin name="EMC_A6"/>
<pin name="EMC_A7"/>
<pin name="EMC_A8"/>
<pin name="EMC_A9"/>
<pin name="EMC_A10"/>
<pin name="EMC_A11"/>
<pin name="EMC_A12"/>
<pin name="EMC_A13"/>
<pin name="EMC_A14"/>
<pin name="EMC_A15"/>
<pin name="EMC_A16"/>
<pin name="EMC_A17"/>
<pin name="EMC_A18"/>
<pin name="EMC_A19"/>
<pin name="EMC_A20"/>
<pin name="EMC_A21"/>
<pin name="EMC_A22"/>
<pin name="EMC_A23"/>
<pin name="EMC_BLS0"/>
<pin name="EMC_CAS"/>
<pin name="EMC_CKEOUT0"/>
<pin name="EMC_CLK01"/>
<pin name="EMC_CS0"/>
<pin name="EMC_D0"/>
<pin name="EMC_D1"/>
<pin name="EMC_D2"/>
<pin name="EMC_D3"/>
<pin name="EMC_D4"/>
<pin name="EMC_D5"/>
<pin name="EMC_D6"/>
<pin name="EMC_D7"/>
<pin name="EMC_D8"/>
<pin name="EMC_D9"/>
<pin name="EMC_D10"/>
<pin name="EMC_D11"/>
<pin name="EMC_D12"/>
<pin name="EMC_D13"/>
<pin name="EMC_D14"/>
<pin name="EMC_D15"/>
<pin name="EMC_DQMOUT0"/>
<pin name="EMC_DYCS0"/>
<pin name="EMC_OE"/>
<pin name="EMC_RAS"/>
<pin name="EMC_WE"/>
<pin name="EMC_DQMOUT1"/>
<pin name="EMC_CLK23"/>
<pin name="EMC_BLS1"/>
</symbol>
<symbol name="LPC1850_ADC">
<pin name="ADC1_0"/>
<pin name="ADC1_1"/>
<pin name="ADC1_2"/>
<pin name="ADC1_3"/>
<pin name="ADC1_4"/>
<pin name="ADC1_5"/>
<pin name="ADC1_6"/>
<pin name="ADC1_7"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="DAC"/>
</symbol>
<symbol name="LPC1850_LCD">
<pin name="LCD_VD0_[4.1]"/>
<pin name="LCD_VD1_[4.4]"/>
<pin name="LCD_VD2_[4.3]"/>
<pin name="LCD_VD3_[4.2]"/>
<pin name="LCD_VD4_[8.7]"/>
<pin name="LCD_VD5_[8.6]"/>
<pin name="LCD_VD6_[8.5]"/>
<pin name="LCD_VD7_[8.4]"/>
<pin name="LCD_VD8_[7.5]"/>
<pin name="LCD_VD9_[4.8]"/>
<pin name="LCD_VD10_[4.10]"/>
<pin name="LCD_VD11_[4.9]"/>
<pin name="LCD_VD12_[8.3]"/>
<pin name="LCD_VD13_[B.6]"/>
<pin name="LCD_VD14_[B.5]"/>
<pin name="LCD_VD15_[B.4]"/>
<pin name="LCD_VD16_[7.4]"/>
<pin name="LCD_VD17_[7.3]"/>
<pin name="LCD_VD18_[7.2]"/>
<pin name="LCD_VD19_[7.1]"/>
<pin name="LCD_VD20_[B.3]"/>
<pin name="LCD_VD21_[B.2]"/>
<pin name="LCD_VD22_[B.1]"/>
<pin name="LCD_VD23_[B.0]"/>
<pin name="LCD_DCLK_[4.7]"/>
<pin name="LCD_ENBL_[4.6]"/>
<pin name="LCD_FP_[4.5]"/>
<pin name="LCD_LE_[7.0]"/>
<pin name="LCD_LP_[7.6]"/>
<pin name="LCD_PWR_[7.7]"/>
</symbol>
<symbol name="LPC1850_RTC">
<pin name="VBAT"/>
<pin name="RTCX1"/>
<pin name="RTCX2"/>
<pin name="RTC_ALARM"/>
</symbol>
<symbol name="LPC1850_CGU">
<pin name="CGU_OUT0"/>
<pin name="CGU_OUT1"/>
</symbol>
<symbol name="LPC1850_ETHERNET">
<pin name="ENET_COL"/>
<pin name="ENET_CRS"/>
<pin name="ENET_MDC"/>
<pin name="ENET_MDIO"/>
<pin name="ENET_RX_CLK"/>
<pin name="ENET_RXD0"/>
<pin name="ENET_RXD1"/>
<pin name="ENET_RXD2"/>
<pin name="ENET_RXD3"/>
<pin name="ENET_RX_DV"/>
<pin name="ENET_RX_ER"/>
<pin name="ENET_TX_CLK"/>
<pin name="ENET_TXD0"/>
<pin name="ENET_TXD1"/>
<pin name="ENET_TXD2"/>
<pin name="ENET_TXD3"/>
<pin name="ENET_TX_EN"/>
<pin name="ENET_TX_ER"/>
</symbol>
<symbol name="LPC1850_CLOCK">
<pin name="CLKOUT"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
</symbol>
<symbol name="LPC1850_I2C">
<pin name="I2C0_SCL"/>
<pin name="I2C0_SDA"/>
<pin name="I2C1_SCL"/>
<pin name="I2C1_SDA"/>
</symbol>
<symbol name="LPC1850_I2S">
<pin name="I2S0_RX_SCK"/>
<pin name="I2S0_RX_SDA"/>
<pin name="I2S0_RX_WS"/>
<pin name="I2S0_TX_SCK"/>
<pin name="I2S0_TX_SDA"/>
<pin name="I2S0_TX_WS"/>
</symbol>
<symbol name="LPC1850_JTAG">
<pin name="DBGEN"/>
<pin name="TCK/SWDCLK"/>
<pin name="TDI"/>
<pin name="TDO/SWO"/>
<pin name="TMS/SWDIO"/>
<pin name="TRST"/>
</symbol>
<symbol name="LPC1850_NMI_WAKEUP">
<pin name="WAKEUP0"/>
<pin name="WAKEUP2"/>
<pin name="WAKEUP1"/>
<pin name="WAKEUP3"/>
<pin name="NMI_EXT"/>
</symbol>
<symbol name="LPC1850_QEI">
<pin name="QEI_IDX"/>
<pin name="QEI_PHA"/>
<pin name="QEI_PHB"/>
</symbol>
<symbol name="LPC1850_SPIFI">
<pin name="SPIFI_CS"/>
<pin name="SPIFI_MISO"/>
<pin name="SPIFI_MOSI"/>
<pin name="SPIFI_SCK"/>
<pin name="SPIFI_SIO2"/>
<pin name="SPIFI_SIO3"/>
</symbol>
<symbol name="LPC1850_SSP">
<pin name="SSP0_MISO"/>
<pin name="SSP0_MOSI"/>
<pin name="SSP0_SCK"/>
<pin name="SSP0_SSEL"/>
</symbol>
<symbol name="LPC1850_TIMERS">
<pin name="TO_MAT0"/>
<pin name="T2_CAP2"/>
<pin name="T2_CAP1"/>
</symbol>
<symbol name="LPC1850_UART0">
<pin name="U0_DIR_[F.9]"/>
<pin name="U0_RXD_[F.11]"/>
<pin name="U0_TXD_[F.10]"/>
</symbol>
<symbol name="LPC1850_UART1">
<pin name="U1_CTS"/>
<pin name="U1_DCD"/>
<pin name="U1_DSR"/>
<pin name="U1_DTR"/>
<pin name="U1_RI"/>
<pin name="U1_RTS"/>
<pin name="U1_RXD"/>
<pin name="U1_TXD"/>
</symbol>
<symbol name="LPC1850_USB0">
<pin name="USB0_VBUS"/>
<pin name="USB0_DM"/>
<pin name="USB0_DP"/>
<pin name="USB0_ID"/>
<pin name="USB0_RREF"/>
<pin name="USB0_VDDA3V3_DRIVER"/>
<pin name="USB0_VDDA3V3"/>
<pin name="USB0_VSSA_TERM"/>
<pin name="USB0_VSSA_REF"/>
<pin name="USB0_PWR_FAULT"/>
<pin name="USB0_PWR_EN"/>
<pin name="USB0_IND0"/>
<pin name="USB0_IND1"/>
</symbol>
<symbol name="LPC1850_USB1">
<pin name="USB1_VBUS"/>
<pin name="USB1_DP"/>
<pin name="USB1_DM"/>
</symbol>
<symbol name="LPC1850_GPIO">
<pin name="GPIO4[11]"/>
<pin name="GPIO4[12]"/>
<pin name="GPIO5[24]"/>
<pin name="GPIO7[14]"/>
<pin name="GPIO7[19]"/>
<pin name="GPIO7[20]"/>
<pin name="GPIO7[21]"/>
<pin name="GPIO7[22]"/>
</symbol>
<symbol name="LPC1850_GPIO6">
<pin name="GPIO6[1]"/>
<pin name="GPIO6[5]"/>
<pin name="GPIO6[6]"/>
<pin name="GPIO6[8]"/>
<pin name="GPIO6[9]"/>
<pin name="GPIO6[10]"/>
<pin name="GPIO6[13]"/>
<pin name="GPIO6[14]"/>
<pin name="GPIO6[15]"/>
<pin name="GPIO6[16]"/>
<pin name="GPIO6[17]"/>
<pin name="GPIO6[18]"/>
<pin name="GPIO6[19]"/>
<pin name="GPIO6[20]"/>
<pin name="GPIO6[21]"/>
<pin name="GPIO6[22]"/>
<pin name="GPIO6[23]"/>
<pin name="GPIO6[24]"/>
<pin name="GPIO6[25]"/>
<pin name="GPIO6[26]"/>
<pin name="GPIO6[27]"/>
<pin name="GPIO6[28]"/>
</symbol>
<symbol name="LPC1850_POWER">
<pin name="VDDREG@0" direction="pwr"/>
<pin name="VDDREG@1" direction="pwr"/>
<pin name="VDDREG@2" direction="pwr"/>
<pin name="VDDREG@3" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VPP" direction="pwr"/>
<pin name="VSSIO@0" direction="pwr"/>
<pin name="VSSIO@1" direction="pwr"/>
<pin name="VSSIO@2" direction="pwr"/>
<pin name="VSSIO@3" direction="pwr"/>
<pin name="VSSIO@4" direction="pwr"/>
<pin name="VSSIO@5" direction="pwr"/>
<pin name="VSSIO@6" direction="pwr"/>
<pin name="VSSIO@7" direction="pwr"/>
<pin name="VSSIO@8" direction="pwr"/>
<pin name="VSSIO@9" direction="pwr"/>
<pin name="VSSIO@10" direction="pwr"/>
<pin name="VSSIO@11" direction="pwr"/>
<pin name="VSSIO@12" direction="pwr"/>
<pin name="VSSIO@13" direction="pwr"/>
<pin name="VDDIO@0" direction="pwr"/>
<pin name="VDDIO@1" direction="pwr"/>
<pin name="VDDIO@2" direction="pwr"/>
<pin name="VDDIO@3" direction="pwr"/>
<pin name="VDDIO@4" direction="pwr"/>
<pin name="VDDIO@5" direction="pwr"/>
<pin name="VDDIO@6" direction="pwr"/>
<pin name="VDDIO@7" direction="pwr"/>
<pin name="VDDIO@8" direction="pwr"/>
<pin name="VDDIO@9" direction="pwr"/>
<pin name="VDDIO@10" direction="pwr"/>
<pin name="VDDIO@11" direction="pwr"/>
<pin name="VDDIO@12" direction="pwr"/>
</symbol>
<symbol name="LPC1850_RESET">
<pin name="RESET"/>
</symbol>
<symbol name="FRAME_A3_ADAFRUIT_FULL">
</symbol>
<symbol name="TDA19988_AUDIO">
<pin name="ACLK" direction="in" function="clk"/>
<pin name="AP1" direction="in"/>
<pin name="AP2" direction="in"/>
<pin name="AP3" direction="in"/>
<pin name="AP4" direction="in"/>
<pin name="WS" direction="in"/>
</symbol>
<symbol name="TDA19988_CTRL">
<pin name="A0"/>
<pin name="A1"/>
<pin name="CDSA"/>
<pin name="CEC"/>
<pin name="CSCL"/>
<pin name="DSCL"/>
<pin name="DSDA"/>
<pin name="HPD"/>
<pin name="INT"/>
<pin name="TEST"/>
<pin name="VPP"/>
</symbol>
<symbol name="TDA19988_PWR">
<pin name="GND" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDA_PLL@1" direction="pwr"/>
<pin name="VDDA_PLL@2" direction="pwr"/>
<pin name="VDDA_TMDS@1" direction="pwr"/>
<pin name="VDDA_TMDS@2" direction="pwr"/>
<pin name="VDDA_TMDS@3" direction="pwr"/>
<pin name="VDDC@1" direction="pwr"/>
<pin name="VDDC@2" direction="pwr"/>
<pin name="VDDIO@1" direction="pwr"/>
<pin name="VDDIO@2" direction="pwr"/>
</symbol>
<symbol name="TDA19988_VIDEO">
<pin name="DE/FREF" direction="in"/>
<pin name="EXT_SWING" direction="out"/>
<pin name="HSYNC/HREF" direction="in"/>
<pin name="PCLK" direction="in" function="clk"/>
<pin name="TX0+" direction="out"/>
<pin name="TX0-" direction="out"/>
<pin name="TX1+" direction="out"/>
<pin name="TX1-" direction="out"/>
<pin name="TX2+" direction="out"/>
<pin name="TX2-" direction="out"/>
<pin name="TXC+" direction="out"/>
<pin name="TXC-" direction="out"/>
<pin name="VPA0" direction="in"/>
<pin name="VPA1" direction="in"/>
<pin name="VPA2" direction="in"/>
<pin name="VPA3" direction="in"/>
<pin name="VPA4" direction="in"/>
<pin name="VPA5" direction="in"/>
<pin name="VPA6" direction="in"/>
<pin name="VPA7" direction="in"/>
<pin name="VPB0" direction="in"/>
<pin name="VPB1" direction="in"/>
<pin name="VPB2" direction="in"/>
<pin name="VPB3" direction="in"/>
<pin name="VPB4" direction="in"/>
<pin name="VPB5" direction="in"/>
<pin name="VPB6" direction="in"/>
<pin name="VPB7" direction="in"/>
<pin name="VPC0" direction="in"/>
<pin name="VPC1" direction="in"/>
<pin name="VPC2" direction="in"/>
<pin name="VPC3" direction="in"/>
<pin name="VPC4" direction="in"/>
<pin name="VPC5" direction="in"/>
<pin name="VPC6" direction="in"/>
<pin name="VPC7" direction="in"/>
<pin name="VSYNC/VREF" direction="in"/>
</symbol>
<symbol name="HDMI_CONN">
<pin name="+5V" direction="pwr"/>
<pin name="CEC"/>
<pin name="DCLK"/>
<pin name="DDAT"/>
<pin name="GND" direction="pwr"/>
<pin name="HOTPLUG"/>
<pin name="TX0+"/>
<pin name="TX0-"/>
<pin name="TX0_SHIELD" direction="pwr"/>
<pin name="TX1+"/>
<pin name="TX1-"/>
<pin name="TX1_SHIELD" direction="pwr"/>
<pin name="TX2+"/>
<pin name="TX2-"/>
<pin name="TX2_SHIELD" direction="pwr"/>
<pin name="TXC+"/>
<pin name="TXC-"/>
<pin name="TXC_SHIELD" direction="pwr"/>
<pin name="UTILITY"/>
</symbol>
<symbol name="HDMI_SHELL">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="UDA1380_POWER">
<pin name="VADCN" direction="pwr"/>
<pin name="VADCP" direction="pwr"/>
<pin name="VDDA(AD)" direction="pwr"/>
<pin name="VDDA(DA)" direction="pwr"/>
<pin name="VDDA(HP)" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VREF" direction="pwr"/>
<pin name="VSSA(AD)" direction="pwr"/>
<pin name="VSSA(DA)" direction="pwr"/>
<pin name="VSSA(HP)" direction="pwr"/>
<pin name="VSSD" direction="pwr"/>
</symbol>
<symbol name="UDA1380">
<pin name="BCKI" direction="in"/>
<pin name="BCKO"/>
<pin name="DATAI" direction="in"/>
<pin name="DATAO" direction="out"/>
<pin name="L3CLOCK/SCL" direction="in"/>
<pin name="L3DATA/SDA"/>
<pin name="L3MODE/A1" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="RTCB" direction="in"/>
<pin name="SEL_L3_IIC" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="VINL" direction="in"/>
<pin name="VINM" direction="in"/>
<pin name="VINR" direction="in"/>
<pin name="VOUTL" direction="out"/>
<pin name="VOUTLHP" direction="out"/>
<pin name="VOUTR" direction="out"/>
<pin name="VOUTRHP" direction="out"/>
<pin name="VREF(HP)"/>
<pin name="WSI" direction="in"/>
<pin name="WSO"/>
</symbol>
<symbol name="IP4786CZ32">
<pin name="CEC_CON"/>
<pin name="CEC_STDBY"/>
<pin name="CEC_SYS"/>
<pin name="DCLK_CON"/>
<pin name="DCLK_SYS"/>
<pin name="DDAT_CON"/>
<pin name="DDAT_SYS"/>
<pin name="ESD_BYPASS"/>
<pin name="GND"/>
<pin name="HOTPLUG_CON"/>
<pin name="HOTPLUG_SYS"/>
<pin name="TX0+_CON"/>
<pin name="TX0+_SYS"/>
<pin name="TX0-_CON"/>
<pin name="TX0-_SYS"/>
<pin name="TX1+_CON"/>
<pin name="TX1+_SYS"/>
<pin name="TX1-_CON"/>
<pin name="TX1-_SYS"/>
<pin name="TX2+_CON"/>
<pin name="TX2+_SYS"/>
<pin name="TX2-_CON"/>
<pin name="TX2-_SYS"/>
<pin name="TXC+_CON"/>
<pin name="TXC+_SYS"/>
<pin name="TXC-_CON"/>
<pin name="TXC-_SYS"/>
<pin name="UTILITY"/>
<pin name="VCC(4.5-6.5V)"/>
<pin name="VCCO_5V"/>
<pin name="VCC_SYS(1.62-5.5V)"/>
</symbol>
<symbol name="LM3407">
<pin name="ISNS"/>
<pin name="DIM"/>
<pin name="EN"/>
<pin name="FS"/>
<pin name="LX"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="VIN"/>
</symbol>
<symbol name="ARDUINOR3">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF"/>
<pin name="A5/SCL"/>
<pin name="A4/SDA"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="/RESET"/>
<pin name="IOREF" direction="out"/>
<pin name="RESERVED" direction="nc"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="FGPMMOPA6B">
<pin name="VCC"/>
<pin name="ENABLE"/>
<pin name="GND@1"/>
<pin name="VBACKUP"/>
<pin name="3D-FIX"/>
<pin name="DPLUS"/>
<pin name="DMINUS"/>
<pin name="GND@2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
</symbol>
<symbol name="SIM908_LITERAL">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="PWRKEY" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="GND@3" direction="pwr"/>
<pin name="DISP-CLK" direction="out"/>
<pin name="DISP-DATA"/>
<pin name="DISP-D/C" direction="out"/>
<pin name="DISP-CS" direction="out"/>
<pin name="GND@4" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GPS/DBG-TXD" direction="out"/>
<pin name="GPS/DBG-RXD" direction="in"/>
<pin name="SIM-DATA"/>
<pin name="SIM-RST" direction="out"/>
<pin name="SIM-CLK" direction="out"/>
<pin name="SIM-VDD" direction="pwr"/>
<pin name="SPK1N" direction="out"/>
<pin name="SPK1P" direction="out"/>
<pin name="MIC1P" direction="in"/>
<pin name="MIC1N" direction="in"/>
<pin name="SPK2N" direction="out"/>
<pin name="SPK2P" direction="out"/>
<pin name="MIC2P" direction="in"/>
<pin name="MIC2N" direction="in"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="GPIO1/KBR0"/>
<pin name="GPIO2/KBR1"/>
<pin name="GPIO3/KBR2"/>
<pin name="GPIO4/KBC0"/>
<pin name="GPIO5/KBC1"/>
<pin name="GPIO6/KBC2"/>
<pin name="GND@6" direction="pwr"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="VRTC" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="VDD-EXT" direction="pwr"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="ADC" direction="in"/>
<pin name="PWM1" direction="out"/>
<pin name="PWM2" direction="out"/>
<pin name="PWM3" direction="out"/>
<pin name="NETLIGHT" direction="out"/>
<pin name="STATUS" direction="out"/>
<pin name="NC@11" direction="nc"/>
<pin name="NC@12" direction="nc"/>
<pin name="I2C-SCL"/>
<pin name="I2C-SDA" direction="out"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GSM-ANT"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="VBAT@1" direction="pwr"/>
<pin name="VBAT@2" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="RXD" direction="in"/>
<pin name="RI" direction="out"/>
<pin name="DCD" direction="out"/>
<pin name="TXD" direction="out"/>
<pin name="DTR" direction="in"/>
<pin name="TEMP-BAT" direction="in"/>
<pin name="VCHG" direction="pwr"/>
<pin name="GPS-VANT-OUT" direction="pwr"/>
<pin name="GPS-VANT-IN" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GPS-ANT" direction="in"/>
<pin name="GND@18" direction="pwr"/>
</symbol>
<symbol name="ADAFRUIT_TEXT">
</symbol>
<symbol name="LPC11U24_QFP48">
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_19/DTR/SSEL1"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)"/>
<pin name="VSS@1"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
<pin name="VDD@1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_20/DSR/SCK1"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL-(20MA_SINK)"/>
<pin name="PIO0_5/SDA-(20MA_SINK)"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO0_6/USB_CONNECT/SCK0"/>
<pin name="PIO0_7/CTS-(20MA_SOURCE)"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_31"/>
<pin name="PIO1_21/DCD/MISO1"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO1_13/DTR/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/DSR/CT16B0_MAT1/RXD"/>
<pin name="PIO1_22/RI/MOSI1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS@2"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_15/DCD/CT16B0_MAT2/SCK1"/>
<pin name="VDD@2"/>
<pin name="PIO0_17/RTS/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO1_16/RI/CT16B0_CAP0"/>
</symbol>
<symbol name="LPC11U24_QFP64">
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_19/DTR/SSEL1"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)"/>
<pin name="VSS@1"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
<pin name="VDD@1"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_20/DSR/SCK1"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL-(20MA_SINK)"/>
<pin name="PIO0_5/SDA-(20MA_SINK)"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO0_6/USB_CONNECT/SCK0"/>
<pin name="PIO0_7/CTS-(20MA_SOURCE)"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_21/DCD/MISO1"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO1_13/DTR/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/DSR/CT16B0_MAT1/RXD"/>
<pin name="PIO1_22/RI/MOSI1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS@2"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_15/DCD/CT16B0_MAT2/SCK1"/>
<pin name="VDD@2"/>
<pin name="PIO0_17/RTS/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO1_16/RI/CT16B0_CAP0"/>
<pin name="VDD@3"/>
<pin name="VDD@4"/>
<pin name="PIO1_18/CT16B1_CAP1/TXD"/>
<pin name="PIO1_17/CT16B0_CAP1/RXD"/>
<pin name="PIO1_12"/>
<pin name="PIO1_11"/>
<pin name="PIO1_10"/>
<pin name="PIO1_9"/>
<pin name="PIO1_8"/>
<pin name="PIO1_7"/>
<pin name="PIO1_6"/>
<pin name="PIO1_5/CT32B1_CAP1"/>
<pin name="PIO1_4/CT32B1_CAP0"/>
<pin name="PIO1_3/CT32B1_MAT3"/>
<pin name="PIO1_2/CT32B1_MAT2"/>
<pin name="PIO1_1/CT32B1_MAT1"/>
<pin name="PIO1_0/CT32B1_MAT0"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="BTL221722-276L">
<pin name="VSS@1" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="LED+" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="CS"/>
<pin name="SDI"/>
<pin name="SCL"/>
<pin name="RS"/>
<pin name="RESET"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="LED_K1" direction="pwr"/>
<pin name="LED_K2" direction="pwr"/>
<pin name="LED_K3" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="BLUETOOTH_MODULE">
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="PCM_CLK"/>
<pin name="PCM_OUT"/>
<pin name="PCM_IN"/>
<pin name="PCM_SYNC"/>
<pin name="AIO_0"/>
<pin name="AIO_1"/>
<pin name="RESET"/>
<pin name="3.3V" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="USB_D-"/>
<pin name="SPI_CS"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="SPI_CLK"/>
<pin name="USB_D+"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="PIO_0"/>
<pin name="PIO_1"/>
<pin name="PIO_2"/>
<pin name="PIO_3"/>
<pin name="PIO_4"/>
<pin name="PIO_5"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="PIO_8"/>
<pin name="PIO_9"/>
<pin name="PIO_10"/>
<pin name="PIO_11"/>
</symbol>
<symbol name="PINHD17">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
</symbol>
<symbol name="UG-2832HSWEG02">
<pin name="C2+"/>
<pin name="C2-"/>
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VBREF" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RES#"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="IREF"/>
<pin name="VCOMH" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PCA9865">
<pin name="PWM0" direction="out"/>
<pin name="PWM1" direction="out"/>
<pin name="PWM2" direction="out"/>
<pin name="PWM3" direction="out"/>
<pin name="PWM4" direction="out"/>
<pin name="PWM5" direction="out"/>
<pin name="PWM6" direction="out"/>
<pin name="PWM7" direction="out"/>
<pin name="PWM8" direction="out"/>
<pin name="PWM9" direction="out"/>
<pin name="PWM10" direction="out"/>
<pin name="PWM11" direction="out"/>
<pin name="PWM12" direction="out"/>
<pin name="PWM13" direction="out"/>
<pin name="PWM14" direction="out"/>
<pin name="PWM15" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="#OE" direction="in"/>
<pin name="EXTCLK" direction="in"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PINHD3X08">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
</symbol>
<symbol name="1X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TSL13T">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="AS1115">
<pin name="SEGA"/>
<pin name="SEGB"/>
<pin name="SEGC"/>
<pin name="SEGD"/>
<pin name="SEGE"/>
<pin name="SEGF"/>
<pin name="SEGG"/>
<pin name="SEGDP"/>
<pin name="DIG0"/>
<pin name="DIG1"/>
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG4"/>
<pin name="DIG5"/>
<pin name="DIG6"/>
<pin name="DIG7"/>
<pin name="SDA"/>
<pin name="GND"/>
<pin name="KEYA"/>
<pin name="KEYB"/>
<pin name="ISET"/>
<pin name="SCL"/>
<pin name="VDD"/>
<pin name="IRQ"/>
</symbol>
<symbol name="LPC1114_DIP28">
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="R/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/SCK0"/>
<pin name="VDDA"/>
<pin name="VSSA"/>
<pin name="R/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="R/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="R/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_5/#RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO1_9/CT16B1_MAT0"/>
<pin name="XTALOUT"/>
<pin name="XTALIN"/>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="#RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_3"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_7/#CTS"/>
</symbol>
<symbol name="FGPMMOPA6C">
<pin name="VCC"/>
<pin name="NC@1"/>
<pin name="GND@1"/>
<pin name="VBACKUP"/>
<pin name="3D-FIX"/>
<pin name="1PPS"/>
<pin name="NC@2"/>
<pin name="GND@2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="NC@5"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
</symbol>
<symbol name="SEGMENT_4DIGIT_COMMONCATHODE_TIME">
<pin name="SEG1_K"/>
<pin name="SEG2_K"/>
<pin name="COLON_K"/>
<pin name="DOT_K"/>
<pin name="SEG3_K"/>
<pin name="SEG4_K"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="COLON"/>
<pin name="DOT"/>
</symbol>
<symbol name="L3G4200D">
<pin name="VDDIO" direction="pwr"/>
<pin name="SCL/SPC"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SAO"/>
<pin name="CS"/>
<pin name="DRDY/INT2"/>
<pin name="INT1"/>
<pin name="RSVRD1(GND)"/>
<pin name="RSVRD2(GND)"/>
<pin name="RSVRD3(GND)"/>
<pin name="RSVRD4(GND)"/>
<pin name="RSVRD5(GND)"/>
<pin name="GND"/>
<pin name="PLLFILT"/>
<pin name="RSVRD6(VDD)"/>
<pin name="VDD"/>
</symbol>
<symbol name="JD-T1800">
<pin name="GND" direction="pwr"/>
<pin name="LEDK" direction="in"/>
<pin name="LEDA" direction="in"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="RS/DC" direction="in"/>
<pin name="DATA"/>
<pin name="CLOCK" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="GND1" direction="pwr"/>
</symbol>
<symbol name="LPC1347_QFP48">
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_19/DTR/SSEL1"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_20/DSR/SCK1"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL-(20MA_SINK)"/>
<pin name="PIO0_5/SDA-(20MA_SINK)"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO0_6/USB_CONNECT/SCK0"/>
<pin name="PIO0_7/CTS-(20MA_SOURCE)"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_31"/>
<pin name="PIO1_21/DCD/MISO1"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO1_13/DTR/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/DSR/CT16B0_MAT1/RXD"/>
<pin name="PIO1_22/RI/MOSI1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_15/DCD/CT16B0_MAT2/SCK1"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="PIO0_17/RTS/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO1_16/RI/CT16B0_CAP0"/>
</symbol>
<symbol name="LPC1347_QFP64">
<pin name="PIO1_25/CT32B0_MAT1"/>
<pin name="PIO1_19/DTR/SSEL1"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="XTALIN"/>
<pin name="XTALOUT"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="PIO0_20/CT16B1_CAP0"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO1_26/CT32B0_MAT2/RXD"/>
<pin name="PIO1_27/CT32B0_MAT3/TXD"/>
<pin name="PIO1_20/DSR/SCK1"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4/SCL-(20MA_SINK)"/>
<pin name="PIO0_5/SDA-(20MA_SINK)"/>
<pin name="PIO0_21/CT16B1_MAT0/MOSI1"/>
<pin name="PIO1_23/CT16B1_MAT1/SSEL1"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO1_24/CT32B0_MAT0"/>
<pin name="PIO0_6/USB_CONNECT/SCK0"/>
<pin name="PIO0_7/CTS-(20MA_SOURCE)"/>
<pin name="PIO1_28/CT32B0_CAP0/SCLK"/>
<pin name="PIO1_21/DCD/MISO1"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1/SWO"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="PIO0_22/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO1_29/SCK0/CT32B0_CAP1"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO0_12/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO0_13/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO0_14/AD3/CT32B1_MAT1"/>
<pin name="PIO1_13/DTR/CT16B0_MAT0/TXD"/>
<pin name="PIO1_14/DSR/CT16B0_MAT1/RXD"/>
<pin name="PIO1_22/RI/MOSI1"/>
<pin name="SWDIO/PIO0_15/AD4/CT32B1_MAT2"/>
<pin name="PIO0_16/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="PIO0_23/AD7"/>
<pin name="PIO1_15/DCD/CT16B0_MAT2/SCK1"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="PIO0_17/RTS/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_18/RXD/CT32B0_MAT0"/>
<pin name="PIO0_19/TXD/CT32B0_MAT1"/>
<pin name="PIO1_16/RI/CT16B0_CAP0"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VREFN"/>
<pin name="PIO1_18/CT16B1_CAP1/TXD"/>
<pin name="PIO1_17/CT16B0_CAP1/RXD"/>
<pin name="VREFP"/>
<pin name="PIO1_11"/>
<pin name="PIO1_10"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PIO1_8"/>
<pin name="PIO1_7"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PIO1_5/CT32B1_CAP1"/>
<pin name="PIO1_4/CT32B1_CAP0"/>
<pin name="PIO1_3/CT32B1_MAT3"/>
<pin name="PIO1_2/CT32B1_MAT2"/>
<pin name="PIO1_1/CT32B1_MAT1"/>
<pin name="PIO1_0/CT32B1_MAT0"/>
</symbol>
<symbol name="PINHD3X04">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X13">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
</symbol>
<symbol name="UG-2864HSWEG01">
<pin name="NC(GND)@1" direction="in"/>
<pin name="C2P" direction="in"/>
<pin name="C2N" direction="in"/>
<pin name="C1P" direction="in"/>
<pin name="C1N" direction="in"/>
<pin name="VBAT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="BS0" direction="in"/>
<pin name="BS1" direction="in"/>
<pin name="BS2" direction="in"/>
<pin name="/CS" direction="in"/>
<pin name="/RES" direction="in"/>
<pin name="DC/I2C_SA0" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="E/RD" direction="in"/>
<pin name="D0/SPI_SCLK/I2C_SCK"/>
<pin name="D1/SPI_SDIN/I2C_SDA"/>
<pin name="D2/I2C_SDA"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="IREF" direction="in"/>
<pin name="VCOMH" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VLSS" direction="pwr"/>
<pin name="NC(GND)@2" direction="in"/>
</symbol>
<symbol name="SWITCH_4WAY_TPA511GLFS">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="7"/>
</symbol>
<symbol name="HT16K33_20PIN">
<pin name="VSS"/>
<pin name="COM0/AD"/>
<pin name="COM1/KS0"/>
<pin name="COM2/KS1"/>
<pin name="COM3/KS2"/>
<pin name="COM4"/>
<pin name="COM5"/>
<pin name="COM6"/>
<pin name="COM7"/>
<pin name="ROW7/K8/INT"/>
<pin name="ROW6/K7"/>
<pin name="ROW5/K6"/>
<pin name="ROW4/K5"/>
<pin name="ROW3/K4"/>
<pin name="ROW2/K3"/>
<pin name="ROW1/K2"/>
<pin name="ROW0/K1"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
</symbol>
<symbol name="HT16K33_24PIN">
<pin name="VSS"/>
<pin name="COM0/AD"/>
<pin name="COM1/KS0"/>
<pin name="COM2/KS1"/>
<pin name="COM3/KS2"/>
<pin name="COM4"/>
<pin name="COM5"/>
<pin name="COM6"/>
<pin name="COM7"/>
<pin name="ROW11/K10/INT"/>
<pin name="ROW6/K5"/>
<pin name="ROW5/K4"/>
<pin name="ROW4/K3"/>
<pin name="ROW3/K2"/>
<pin name="ROW2/K1"/>
<pin name="ROW1/A0"/>
<pin name="ROW0/A1"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
<pin name="ROW10/K9"/>
<pin name="ROW9/K8"/>
<pin name="ROW8/K7"/>
<pin name="ROW7/K6"/>
</symbol>
<symbol name="HT16K33_28PIN">
<pin name="VSS"/>
<pin name="COM0/AD"/>
<pin name="COM1/KS0"/>
<pin name="COM2/KS1"/>
<pin name="COM3/KS2"/>
<pin name="COM4"/>
<pin name="COM5"/>
<pin name="COM6"/>
<pin name="COM7"/>
<pin name="ROW15/K13/INT"/>
<pin name="ROW6/K4"/>
<pin name="ROW5/K3"/>
<pin name="ROW4/K2"/>
<pin name="ROW3/K1"/>
<pin name="ROW2/A0"/>
<pin name="ROW1/A1"/>
<pin name="ROW0/A2"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
<pin name="ROW14/K12"/>
<pin name="ROW13/K11"/>
<pin name="ROW8/K6"/>
<pin name="ROW7/K5"/>
<pin name="ROW12/K10"/>
<pin name="ROW11/K9"/>
<pin name="ROW10/K8"/>
<pin name="ROW9/K7"/>
</symbol>
<symbol name="SEGMENT_4DIGIT_COMMONCATHODE_TIME_14PIN">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$15"/>
</symbol>
<symbol name="TEA5767MODULE">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="BUSMODE"/>
<pin name="W/R"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="R-OUT"/>
<pin name="L-OUT"/>
<pin name="MPXO"/>
<pin name="ANT"/>
</symbol>
<symbol name="NCP2811">
<pin name="NC@3"/>
<pin name="AVCC"/>
<pin name="CP+"/>
<pin name="GND"/>
<pin name="CP-"/>
<pin name="PVM"/>
<pin name="/SD"/>
<pin name="NC@1"/>
<pin name="IN_LEFT"/>
<pin name="AGND"/>
<pin name="IN_RIGHT"/>
<pin name="NC@2"/>
<pin name="OUT_RIGHT"/>
<pin name="OUT_LEFT"/>
</symbol>
<symbol name="HB100">
<pin name="5V@1"/>
<pin name="5V@2"/>
<pin name="IF@1"/>
<pin name="IF@2"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
</symbol>
<symbol name="INA219">
<pin name="VIN+"/>
<pin name="VIN-"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="A0"/>
<pin name="A1"/>
</symbol>
<symbol name="FGPMMOPA6H">
<pin name="VCC"/>
<pin name="NRESET"/>
<pin name="GND@1"/>
<pin name="VBACKUP"/>
<pin name="3D-FIX"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="GND@2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="EX_ANT"/>
<pin name="GND@3"/>
<pin name="1PPS"/>
<pin name="RTCM"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
<pin name="NC@5"/>
<pin name="NC@6"/>
<pin name="GND@4"/>
<pin name="NC@7"/>
</symbol>
<symbol name="RASPBERRYPI_REV_B">
<pin name="3.3V@1" direction="sup"/>
<pin name="SDA0"/>
<pin name="SCL0" direction="out"/>
<pin name="GPIO7"/>
<pin name="DNC@2" direction="nc"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="DNC@4" direction="nc"/>
<pin name="SPI_MOSI" direction="out"/>
<pin name="SPI_MISO" direction="in"/>
<pin name="SPI_SCLK" direction="out"/>
<pin name="DNC@6" direction="nc"/>
<pin name="#SPI_CE1" direction="out"/>
<pin name="#SPI_CE0" direction="out"/>
<pin name="GPIO6"/>
<pin name="DNC@5" direction="nc"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="DNC@3" direction="nc"/>
<pin name="GPIO1"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="GND" direction="sup"/>
<pin name="DNC@1" direction="nc"/>
<pin name="5.0V@1" direction="sup"/>
</symbol>
<symbol name="ADBM-A350">
<pin name="VDD" direction="pwr"/>
<pin name="VDDIO" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="MISO_SDA" direction="in"/>
<pin name="MOSI_A0" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="NCS_A1" direction="in"/>
<pin name="EVENT_INT" direction="in"/>
<pin name="SHTDWN" direction="in"/>
<pin name="GPIO" direction="in"/>
<pin name="NRST" direction="in"/>
<pin name="IO_SELECT" direction="in"/>
<pin name="DOME-" direction="in"/>
<pin name="DOME+" direction="in"/>
</symbol>
<symbol name="LPC1113/4/5_FBD48/XL">
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS(IO)" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RESET/PIO0_0"/>
<pin name="SWCLK/PIO0_10/SCK0/CT16B0_MAT2"/>
<pin name="TDI/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="TMS/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="TDO/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="TRST/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
<pin name="PIO0_1/CLKOUT/CT32B0_MAT2"/>
<pin name="PIO0_2/SSEL0/CT16B0_CAP0"/>
<pin name="PIO0_4/SCL"/>
<pin name="PIO0_5/SDA"/>
<pin name="PIO0_6/SCK0"/>
<pin name="PIO0_7/CTS"/>
<pin name="PIO0_8/MISO0/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI0/CT16B0_MAT1"/>
<pin name="PIO0_3"/>
<pin name="PIO1_8/CT16B1_CAP0"/>
<pin name="PIO1_9/CT16B1_MAT0/MOSI1"/>
<pin name="PIO1_10/AD6/CT16B1_MAT1/MISO1"/>
<pin name="PIO1_4/AD5/CT32B1_MAT3/WAKEUP"/>
<pin name="PIO1_11/AD7/CT32B1_CAP1"/>
<pin name="PIO1_5/RTS/CT32B0_CAP0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="PIO2_0/DTR/SSEL1"/>
<pin name="PIO2_1/DSR/SCK1"/>
<pin name="PIO2_2/DCD/MISO1"/>
<pin name="PIO2_3/RI/MOSI1"/>
<pin name="PIO2_4/CT16B1_MAT1/SSEL1"/>
<pin name="PIO2_5/CT32B0_MAT0"/>
<pin name="PIO2_6/CT32B0_MAT1"/>
<pin name="PIO2_7/CT32B0_MAT2/RXD"/>
<pin name="PIO2_8/CT32B0_MAT3/TXD"/>
<pin name="PIO2_9/CT32B0_CAP0"/>
<pin name="PIO2_10"/>
<pin name="PIO2_11/SCK0/CT32B0_CAP1"/>
<pin name="PIO3_0/DTR/CT16B0_MAT0/TXD"/>
<pin name="PIO3_1/DSR/CT16B0_MAT1/RXD"/>
<pin name="PIO3_2/DCD/CT16B0_MAT2/SCK1"/>
<pin name="PIO3_3/RI/CT16B0_CAP0"/>
<pin name="PIO3_4/CT16B0_CAP1/RXD"/>
<pin name="PIO3_5/CT16B1_CAP1/TXD"/>
</symbol>
<symbol name="SOLDERJUMPER_2WAY">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MCP4725">
<pin name="VOUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="A0" direction="in"/>
</symbol>
<symbol name="ADS1015">
<pin name="AIN0"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="AIN3"/>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="ADDR"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="ALERT"/>
</symbol>
<symbol name="ADS7924">
<pin name="AIN0"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="AIN3"/>
<pin name="RESET"/>
<pin name="INT"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A0"/>
<pin name="DGND"/>
<pin name="PWRCON"/>
<pin name="AGND"/>
<pin name="MUXOUT"/>
<pin name="ADCIN"/>
<pin name="AVDD"/>
<pin name="DVDD"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="74AUP2G126">
<pin name="1A" direction="in"/>
<pin name="1OE" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2OE" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="S6B33B6_1.5IN_LCD">
<pin name="NC@1" direction="nc"/>
<pin name="LED_K"/>
<pin name="LED_A"/>
<pin name="VRP" direction="out"/>
<pin name="VEE" direction="in"/>
<pin name="VDD(3V3)" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="DB15"/>
<pin name="DB14"/>
<pin name="DB13"/>
<pin name="DB12"/>
<pin name="DB11"/>
<pin name="DB10"/>
<pin name="DB9"/>
<pin name="DB8"/>
<pin name="DB7/SDI"/>
<pin name="DB6/SCL"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="RD" direction="in"/>
<pin name="WR" direction="in"/>
<pin name="RS/DATA_INSTR" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="MPU" direction="in"/>
<pin name="PS" direction="in"/>
<pin name="OTPG(NC)" direction="nc"/>
<pin name="OTPD(NC)" direction="nc"/>
</symbol>
<symbol name="TPA2012D2">
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="G1" direction="in"/>
<pin name="OUTL+" direction="out"/>
<pin name="PVDD@1" direction="pwr"/>
<pin name="PGND@1" direction="pwr"/>
<pin name="OUTL-" direction="out"/>
<pin name="SHUTDOWN_L" direction="in"/>
<pin name="SHUTDOWN_R" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="OUTR-" direction="out"/>
<pin name="PGND@2" direction="pwr"/>
<pin name="PVDD@2" direction="pwr"/>
<pin name="OUTR+" direction="out"/>
<pin name="G0" direction="in"/>
<pin name="INR+" direction="in"/>
<pin name="INR-" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="INL-" direction="in"/>
<pin name="INL+" direction="in"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="SI4731-D60-GU">
<pin name="DOUT/LIN"/>
<pin name="DFS/RIN"/>
<pin name="GPO3/DCLK"/>
<pin name="GPO2/INT"/>
<pin name="GPO1"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="FMI"/>
<pin name="RFGND"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
<pin name="AMI"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="RSTB"/>
<pin name="SENB"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="RCLK"/>
<pin name="VCCD"/>
<pin name="VCCA"/>
<pin name="DBYP"/>
<pin name="ROUT"/>
<pin name="LOUT"/>
</symbol>
<symbol name="DRV8833">
<pin name="A_IN1" direction="in"/>
<pin name="A_IN2" direction="in"/>
<pin name="B_IN1" direction="in"/>
<pin name="B_IN2" direction="in"/>
<pin name="NSLEEP" direction="in"/>
<pin name="VM" direction="pwr"/>
<pin name="VCP"/>
<pin name="A_OUT1" direction="out"/>
<pin name="A_OUT2" direction="out"/>
<pin name="B_OUT1" direction="out"/>
<pin name="B_OUT2" direction="out"/>
<pin name="NFAULT"/>
<pin name="VINT" direction="pwr"/>
<pin name="A_ISENSE"/>
<pin name="B_ISENSE"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND(THRML)" direction="pwr"/>
</symbol>
<symbol name="TB6612FNG">
<pin name="VCC" direction="pwr"/>
<pin name="STBY" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="PWMA" direction="in"/>
<pin name="BIN1" direction="in"/>
<pin name="BIN2" direction="in"/>
<pin name="PWMB" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VM@1" direction="pwr"/>
<pin name="AOUT1@1" direction="out"/>
<pin name="AOUT1@2" direction="out"/>
<pin name="AOUT2@1" direction="out"/>
<pin name="AOUT2@2" direction="out"/>
<pin name="PGND1@1" direction="pwr"/>
<pin name="PGND1@2" direction="pwr"/>
<pin name="VM@2" direction="pwr"/>
<pin name="VM@3" direction="pwr"/>
<pin name="BOUT1@1" direction="out"/>
<pin name="BOUT1@2" direction="out"/>
<pin name="BOUT2@1" direction="out"/>
<pin name="BOUT2@2" direction="out"/>
<pin name="PGND2@1" direction="pwr"/>
<pin name="PGND2@2" direction="pwr"/>
</symbol>
<symbol name="MAX9814">
<pin name="BIAS"/>
<pin name="MICBIAS"/>
<pin name="MICIN"/>
<pin name="CT"/>
<pin name="CG"/>
<pin name="VDD"/>
<pin name="SHUTDOWN"/>
<pin name="GND"/>
<pin name="A/R"/>
<pin name="TH"/>
<pin name="GAIN"/>
<pin name="MICOUT"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="THERMAL"/>
</symbol>
<symbol name="SMBCONNECTOR">
<pin name="ANT"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
</symbol>
<symbol name="PINHD13">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
</symbol>
<symbol name="ESDDIODEARRAY_SINGLE_UNIDIR">
<pin name="GNDPIN" direction="pwr"/>
<pin name="SUPPLYPIN" direction="pwr"/>
<pin name="IO" direction="pas"/>
</symbol>
<symbol name="VMOTOR">
<pin name="VMOTOR" direction="sup"/>
</symbol>
<symbol name="1X3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="MPL115A2">
<pin name="VDD" direction="pwr"/>
<pin name="CAP"/>
<pin name="GND" direction="pwr"/>
<pin name="SHDN"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="NC" direction="nc"/>
<pin name="RST"/>
</symbol>
<symbol name="MAX98306">
<pin name="PGND@1" direction="pwr"/>
<pin name="SHDN" direction="in"/>
<pin name="INL+" direction="in"/>
<pin name="INL-" direction="in"/>
<pin name="GAIN" direction="in"/>
<pin name="INR-" direction="in"/>
<pin name="INR+" direction="in"/>
<pin name="PGND@2" direction="pwr"/>
<pin name="OUTR-" direction="out"/>
<pin name="OUTR+" direction="out"/>
<pin name="PVDD@1" direction="pwr"/>
<pin name="PVDD@2" direction="pwr"/>
<pin name="OUTL+" direction="out"/>
<pin name="OUTL-" direction="out"/>
<pin name="THERMAL" direction="pwr"/>
</symbol>
<symbol name="DS1307">
<pin name="X1"/>
<pin name="X2"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND"/>
<pin name="VBAT"/>
<pin name="VCC"/>
<pin name="SQW/OUT"/>
</symbol>
<symbol name="EEPROM_SOIC8_24C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LPC11A14_QFN33_LITERAL">
<pin name="PIO0_26/TXD/MISO1/CT16B1_CAP1/CT32B0_CAP2"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/RXD/CLKOUT/CT32B0_MAT2/SSEL0/CLKIN"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD(IO)" direction="sup"/>
<pin name="PIO0_24/SCL/CLKIN/CT16B1_CAP0"/>
<pin name="PIO0_18/R/SSEL0/CT16B0_CAP0/CT16B1_CAP1"/>
<pin name="PIO0_19/CLKIN/CLKOUT/MOSI0/CT16B1_MAT0"/>
<pin name="PIO0_2/SCL/ACMP_O/TCK/SWCLK/CT16B0_CAP0"/>
<pin name="PIO0_3/SDA/ACMP_O/SWDIO/CT16B1_CAP0"/>
<pin name="PIO0_25/SDA/SSEL1/CT16B1_MAT0"/>
<pin name="PIO0_16/ATRG0/ACMP_I3/CT16B0_CAP1/SCL"/>
<pin name="PIO0_17/ATRG1/ACMP_I4/CT16B0_CAP2/CT16B0_MAT0"/>
<pin name="PIO0_20/R/SCK0/CT32B1_CAP0/CT16B1_MAT2"/>
<pin name="PIO0_21/CTS/ACMP_O/CT32B1_CAP1/SCLK"/>
<pin name="PIO0_22/MISO0/ACMP_I5/CT32B1_MAT2/CT32B1_CAP2"/>
<pin name="PIO0_4/R/AOUT/CT16B0_MAT1/MOSI0"/>
<pin name="TCK/SWCLK/PIO0_5/R/CT16B0_MAT2/SCK0"/>
<pin name="PIO0_14/MISO1/AD6/CT32B0_CAP1/CT16B1_MAT1/VDDCMP"/>
<pin name="TDI/PIO0_6/AD0/CT32B0_MAT3/MISO0"/>
<pin name="TMS/PIO0_7/AD1/CT32B1_CAP0/CT16B0_MAT0"/>
<pin name="TDO/PIO0_8/AD2/CT32B1_MAT0/SCK1"/>
<pin name="TRST/PIO0_9/AD3/CT32B1_MAT1/CT16B0_MAT1/CTS"/>
<pin name="SWDIO/PIO0_10/AD4/CT32B1_MAT2/CT16B0_MAT2/RTS"/>
<pin name="PIO0_11/SCLK/AD5/CT32B1_MAT3/CT32B0_CAP0"/>
<pin name="PIO0_15/TXD/AD7/CT32B0_CAP2/SDA"/>
<pin name="PIO0_27/MOSI1/ACMP_I1/CT32B1_MAT1/CT16B1_CAP2"/>
<pin name="VDD(3V3)" direction="sup"/>
<pin name="PIO0_23/RTS/ACMP_O/CT32B0_CAP0/SCLK"/>
<pin name="PIO0_12/RXD/ACMP_O/CT32B0_MAT0/SCL/CLKIN"/>
<pin name="PIO0_13/TXD/ACMP_I2/CT32B0_MAT1/SDA"/>
<pin name="VSS" direction="sup"/>
</symbol>
<symbol name="VS1053B">
<pin name="MIC_P/LINEIN"/>
<pin name="MIC_N"/>
<pin name="XRESET"/>
<pin name="DGND@0" direction="sup"/>
<pin name="CVDD@0" direction="sup"/>
<pin name="IOVDD@0" direction="sup"/>
<pin name="CVDD@1" direction="sup"/>
<pin name="DREQ"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="GPIO6/I2S_SCLK"/>
<pin name="GPIO7/I2S_SDATA"/>
<pin name="XDCS/BSYNC"/>
<pin name="IOVDD@1" direction="sup"/>
<pin name="VCO"/>
<pin name="DGND@1" direction="sup"/>
<pin name="XTALOUT" direction="out"/>
<pin name="XTALIN" direction="in"/>
<pin name="IOVDD@2" direction="sup"/>
<pin name="DGND@2" direction="sup"/>
<pin name="DGND@3" direction="sup"/>
<pin name="DGND@4" direction="sup"/>
<pin name="XCS"/>
<pin name="CVDD@2" direction="sup"/>
<pin name="GPIO5/I2S_MCLK"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="CVDD@3" direction="sup"/>
<pin name="XTEST"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GND" direction="sup"/>
<pin name="GPIO4/I2S_LROUT"/>
<pin name="AGND@0" direction="sup"/>
<pin name="AVDD@0" direction="sup"/>
<pin name="RIGHT"/>
<pin name="AGND@1" direction="sup"/>
<pin name="AGND@2" direction="sup"/>
<pin name="GBUF"/>
<pin name="AVDD@1" direction="sup"/>
<pin name="RCAP"/>
<pin name="AVDD@2" direction="sup"/>
<pin name="LEFT"/>
<pin name="AGND@3" direction="sup"/>
<pin name="LINE2"/>
</symbol>
<symbol name="BATTERY_SINGLECELL">
<pin name="-" direction="sup"/>
<pin name="+" direction="sup"/>
</symbol>
<symbol name="PINHD15">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
</symbol>
<symbol name="SHIELD">
</symbol>
<symbol name="LPC18XX-LIB_USBLC6-2">
<pin name="GND" direction="pas"/>
<pin name="I/O1_1" direction="pas"/>
<pin name="I/O1_2" direction="pas"/>
<pin name="I/O2_1" direction="pas"/>
<pin name="I/O2_2" direction="pas"/>
<pin name="VBUS" direction="pas"/>
</symbol>
<symbol name="NTS0102">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="OE"/>
</symbol>
<symbol name="NRF8001">
<pin name="VDD@1" direction="pwr"/>
<pin name="DEC1"/>
<pin name="DEC2"/>
<pin name="XL2" direction="out"/>
<pin name="XL1" direction="in"/>
<pin name="ACTIVE" direction="out"/>
<pin name="TXD" direction="out"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="RXD" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="REQN" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="RDYN" direction="out"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="VDD_PA"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="IREF" direction="out"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="XC2" direction="out"/>
<pin name="XC1" direction="in"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="DCC"/>
</symbol>
<symbol name="BALUN+LP_NORDIC">
<pin name="BAL1"/>
<pin name="GND" direction="sup"/>
<pin name="UNBAL"/>
<pin name="BAL2"/>
<pin name="DC"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="BMC050">
<pin name="INT2" direction="out"/>
<pin name="PS1" direction="in"/>
<pin name="PS2" direction="in"/>
<pin name="INT3" direction="out"/>
<pin name="CSB1" direction="in"/>
<pin name="CSB2" direction="in"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="DRDY" direction="out"/>
<pin name="SDO/ADDR" direction="out"/>
<pin name="SDI/SDA"/>
<pin name="GND@3" direction="sup"/>
<pin name="VDD" direction="sup"/>
<pin name="VDDIO" direction="sup"/>
<pin name="SCK/SCL" direction="in"/>
<pin name="INT1" direction="out"/>
</symbol>
<symbol name="VDDIO">
<pin name="VDDIO" direction="sup"/>
</symbol>
<symbol name="PSENSE-DPD">
<pin name="VS" direction="pwr"/>
<pin name="+VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PSENSE-SP">
<pin name="VS" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LIS3DHTR">
<pin name="VDDIO" direction="sup"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="SCL"/>
<pin name="GND@1" direction="sup"/>
<pin name="SDA"/>
<pin name="SDO"/>
<pin name="CS" direction="in"/>
<pin name="INT2" direction="out"/>
<pin name="RES(GND)"/>
<pin name="INT1" direction="out"/>
<pin name="GND@2" direction="sup"/>
<pin name="ADC3" direction="in"/>
<pin name="VDD" direction="sup"/>
<pin name="ADC2" direction="in"/>
<pin name="ADC1" direction="in"/>
</symbol>
<symbol name="THERMAL-SLUG">
<pin name="TP" direction="pwr"/>
</symbol>
<symbol name="STMPE610">
<pin name="Y-" direction="in"/>
<pin name="INT" direction="out"/>
<pin name="A0/MISO"/>
<pin name="SCLK"/>
<pin name="SDA/CS"/>
<pin name="VCC" direction="pwr"/>
<pin name="MOSI" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="MODE" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="IN2/GPIO2"/>
<pin name="IN3/GPIO3"/>
<pin name="X+" direction="in"/>
<pin name="VIO" direction="pwr"/>
<pin name="Y+" direction="in"/>
<pin name="X-" direction="in"/>
</symbol>
<symbol name="SDCARD_PCBCARRIER">
<pin name="DAT1"/>
<pin name="DAT0"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="CLK"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="CMD"/>
<pin name="CD/DAT3"/>
<pin name="DAT2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;b&gt;Diode&lt;/b&gt;
&lt;p&gt;
&lt;h3&gt;SMA&lt;/h3&gt;
&lt;table cellpadding="5" width="600"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
  &lt;td&gt;&lt;b&gt;Model&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Volts&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Amps&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Type&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vf&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vr&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Digikey #&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Notes&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;SSA34-E3&lt;/td&gt;
  &lt;td&gt;40V&lt;/td&gt;
  &lt;td&gt;3A&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;480mV @ 3A&lt;/td&gt;
  &lt;td&gt;200uA @ 40V&lt;/td&gt;
  &lt;td&gt;SSA34-E3/61TGITR-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;CDBA120-G&lt;/td&gt;
  &lt;td&gt;20V&lt;/td&gt;
  &lt;td&gt;1A&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;500mV @ 1A&lt;/td&gt;
  &lt;td&gt;500uA @ 20V&lt;/td&gt;
  &lt;td&gt;641-1014-6-ND&lt;/td&gt;
  &lt;td&gt;REEL&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MBRA210&lt;/td&gt;
  &lt;td&gt;10V&lt;/td&gt;
  &lt;td&gt;2A&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;350mV @ 2A&lt;/td&gt;
  &lt;td&gt;700uA @ 10V&lt;/td&gt;
  &lt;td&gt;MBRA210LT3&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;h3&gt;SOD-123&lt;/h3&gt;
&lt;table cellpadding="5" width="600"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
  &lt;td&gt;&lt;b&gt;Model&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Volts&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Amps&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Type&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vf&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vr&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Order #&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Notes&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;BAT54T1G&lt;/td&gt;
  &lt;td&gt;30V&lt;/td&gt;
  &lt;td&gt;200mA&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;800mV @ 200mA&lt;/td&gt;
  &lt;td&gt;2uA @ 25V&lt;/td&gt;
  &lt;td&gt;BAT54T1GOSTR-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;B0530W&lt;/td&gt;
  &lt;td&gt;30V&lt;/td&gt;
  &lt;td&gt;500mA&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;430mV @ 500mA&lt;/td&gt;
  &lt;td&gt;130uA @ 30V&lt;/td&gt;
  &lt;td&gt;B0530W-FDICT-ND&lt;/td&gt;
  &lt;td&gt;REEL&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MBR120&lt;/td&gt;
  &lt;td&gt;1A&lt;/td&gt;
  &lt;td&gt;20V&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;340mV @ 1A&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;MBR120VLSFT1GOSCT-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;h3&gt;SOD-323&lt;/h3&gt;
&lt;table cellpadding="5" width="600"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
  &lt;td&gt;&lt;b&gt;Model&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Volts&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Amps&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Type&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vf&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vr&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Order #&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Notes&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;PMEG2005EJ&lt;/td&gt;
  &lt;td&gt;20V&lt;/td&gt;
  &lt;td&gt;500mA&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;355mV @ 500mA&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;568-4110-1-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ZLLS410&lt;/td&gt;
  &lt;td&gt;10V&lt;/td&gt;
  &lt;td&gt;570mA&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;380mV @ 570mA&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;ZLLS410CT-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;1N4148WS&lt;/td&gt;
  &lt;td&gt;75V&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;Silicon/Simple&lt;/td&gt;
  &lt;td&gt;1V&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;1N4148WSFSCT-ND&lt;/td&gt;
  &lt;td&gt;REEL&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;h3&gt;SOD-523&lt;/h3&gt;
&lt;table cellpadding="5" width="600"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
  &lt;td&gt;&lt;b&gt;Model&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Volts&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Amps&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Type&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vf&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vr&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Order #&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Notes&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;BAT54XV2&lt;/td&gt;
  &lt;td&gt;30V&lt;/td&gt;
  &lt;td&gt;200mA&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;0.8V @ 100mA&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;BAT54XV2CT-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;TB751S&lt;/td&gt;
  &lt;td&gt;30V&lt;/td&gt;
  &lt;td&gt;30mA&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;RB751S-40TE61CT-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;h3&gt;SOT23-R/W&lt;/h3&gt;(R = Solder Paste/Reflow Ovens, W = Hand-Soldering)
&lt;br/&gt;
&lt;table cellpadding="5" width="600"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
  &lt;td&gt;&lt;b&gt;Model&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Volts&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Amps&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Type&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vf&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Vr&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Order #&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;Notes&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;BAT54FILM&lt;/td&gt;
  &lt;td&gt;40V&lt;/td&gt;
  &lt;td&gt;300mA&lt;/td&gt;
  &lt;td&gt;Schottky&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;497-7162-1-ND&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="SMA" package="SMADIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO-1N4148" package="DO-1N4148">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_REFLOW" package="SOT23-R">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-523" package="SOD-523">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-323" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-123" package="SOD-123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_CERAMIC" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Ceramic Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0402&lt;/b&gt; - 0402 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;16pF 50V 5% [Digikey: 445-4899-2-ND]&lt;/li&gt;
&lt;li&gt;18pF 50V 5% [Digikey: 490-1281-2-ND]&lt;/li&gt;
&lt;li&gt;22pF 50V 5% [Digikey: 490-1283-2-ND]&lt;/li&gt;
&lt;li&gt;68pF 50V 5% [Digikey: 490-1289-2-ND]&lt;/li&gt;
&lt;li&gt;0.1uF 10V 10% [Digikey: 490-1318-2-ND]&lt;/li&gt;
&lt;li&gt;1.0uF 6.3V 10% [Digikey: 490-1320-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;16 pF 50V 5% [Digikey: 445-5051-2-ND]&lt;/li&gt;
&lt;li&gt;22 pF 50V [Digikey: PCC220ACVTR-ND]&lt;/li&gt;
&lt;li&gt;33 pF 50V 5% [Digikey: 490-1415-1-ND]&lt;/li&gt;
&lt;li&gt;56pF 50V 5% [Digikey: 490-1421-1-ND]&lt;/li&gt;
&lt;li&gt;220pF 50V 5% [Digikey: 445-1285-1-ND]&lt;/li&gt;
&lt;li&gt;680 pF 50V &lt;/li&gt;
&lt;li&gt;2200 pF 50V 5% C0G [Digikey: 445-1297-1-ND]&lt;/li&gt;
&lt;li&gt;5600 pF 100V 5% X7R [Digikey: 478-3711-1-ND]&lt;/li&gt;
&lt;li&gt;0.1 µF 25V 10% [Digikey: PCC2277TR-ND]&lt;/li&gt;
&lt;li&gt;0.22 µF 16V 10% X7R [Digikey: 445-1318-1-ND]&lt;/li&gt;
&lt;li&gt;1.0 µF 25V 10% [Digikey: 445-5146-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - RF Specific
&lt;ul&gt;
&lt;li&gt;3pF 250V +/-0.1pF RF [Digikey: 712-1347-1-ND]&lt;/li&gt;
&lt;li&gt;18 pF 250V 5%  [Digikey: 478-3505-1-ND or 712-1322-1-ND]&lt;/li&gt;
&lt;li&gt;56 pF 250V 5% C0G RF [Digikey: 490-4867-1-ND]&lt;/li&gt;
&lt;li&gt;68 pF 250V RF [Digikey: 490-4868-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;220 pF 250V 2% &lt;strong&gt;RF&lt;/strong&gt; Ceramic Capacitor [Digikey: 712-1398-1-ND]&lt;/li&gt;
&lt;li&gt;1000 pF 50V 2% NP0 Ceramic Capacitor [Digikey: 478-3760-1-ND]&lt;/li&gt;
&lt;li&gt;0.1 µF 25V 10% Ceramic Capacitor [Digikey: PCC1828TR-ND]&lt;/li&gt;
&lt;li&gt;1.0 µF 16V 10% Ceramic Capacitor[Digikey: 490-1691-2-ND]&lt;/li&gt;
&lt;li&gt;10.0 µF 10V 10% Ceramic Capacitor[Digikey: 709-1228-1-ND]&lt;/li&gt;
&lt;li&gt;10.0 uF 16V 10% Ceramic Capacitor [Digikey: 478-5165-2-ND]&lt;/li&gt;
&lt;li&gt;47 uF 6.3V 20% Ceramic Capacitor [Digikey: 587-1779-1-ND or 399-5506-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;/ul&gt;&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Capacitors
&lt;ul&gt;
&lt;li&gt;47uF 10V 20% Ceramic Capacitor [Digikey: 490-5528-1-ND or 399-5508-1-ND or 445-6010-1-ND]&lt;/li&gt;
&lt;li&gt;100uF 6.3V -20%, +80% Y5V Ceramic Capacitor (Digikey: 490-4512-1-ND, Mouser: 81-GRM31CF50J107ZE1L)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CAPACITOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603MINI" package="0603-MINI">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805-NOTHERMALS" package="0805_NOTHERMALS">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402" package="_0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402MP" package="_0402MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603" package="_0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603MP" package="_0603MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="_0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805MP" package="_0805MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_TANTALUM" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Tantalum Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Wave&lt;/b&gt; footprints have larger pads and are meant to be used for hand soldering.&lt;br/&gt;
&lt;b&gt;Reflow&lt;/b&gt; footprints are optimised for solder paste and a reflow oven.&lt;/p&gt;
&lt;b&gt;EIA3216-18/A-[R/W]&lt;/b&gt; - Size A / 3216-18 / 1206 footprint
&lt;ul&gt;
&lt;li&gt;4.7µF 25V 10% Tantalum Capacitor&lt;/li&gt;
&lt;li&gt;10µF 16V 10% Tantalum Capacitor [Digikey: 495-2236-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;EIA3528-21/B-[R/W]&lt;/b&gt; - Size B / 3528-21
&lt;ul&gt;
&lt;li&gt;47µF 10V 10% Tantalum Capactior [Digikey: 495-2216-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;EIA6032-28/C-[R/W]&lt;/b&gt; - Size C / 6032-28
&lt;ul&gt;
&lt;li&gt;10µF 35V 20% Tantalum Capacitor [Digikey: 495-2285-1-ND]&lt;/li&gt;
&lt;li&gt;100µF 16V 10% Tantalum Capactior [Digikey: 399-5214-1-ND]&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CAPACITOR_POL"/>
</gates>
<devices>
<device name="A/3216_REFLOW" package="EIA3216-18/A-R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216_WAVE" package="EIA3216-18/A-W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528_REFLOW" package="EIA3528-21/B-R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528_WAVE" package="EIA3528-21/B-W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032_REFLOW" package="EIA6032-28/C-R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032_WAVE" package="EIA6032-28/C-W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343_REFLOW" package="EIA7343-31/D-R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343_WAVE" package="EIA7343-31/D-W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Resistors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0402&lt;/b&gt; - 0402 Surface Mount Package
&lt;ul&gt;
&lt;li&gt;22 Ohm 1% 1/16W [Digikey: 311-22.0LRTR-ND]&lt;/li&gt;
&lt;li&gt;33 Ohm 5% 1/16W&lt;/li&gt;
&lt;li&gt;1.0K 5% 1/16W&lt;/li&gt;
&lt;li&gt;1.5K 5% 1/16W&lt;/li&gt;
&lt;li&gt;2.0K 1% 1/16W&lt;/li&gt;
&lt;li&gt;10.0K 1% 1/16W [Digikey: 311-10.0KLRTR-ND]&lt;/li&gt;
&lt;li&gt;10.0K 5% 1/16W [Digikey: RMCF0402JT10K0TR-ND]&lt;/li&gt;
&lt;li&gt;12.1K 1% 1/16W [Digikey: 311-22.0LRTR-ND]&lt;/li&gt;
&lt;li&gt;100.0K 5% 1/16W&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Package&lt;br&gt;
&lt;ul&gt;
&lt;li&gt;0 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;15 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;49.9 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;150 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;240 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;390 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;560 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;680 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;750 Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.5K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.2K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;3.3K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;4.7K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;10.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;12.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;12.1K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;20.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100.0K Ohm 1/10 Watt 1% Resistor&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Package
&lt;ul&gt;
&lt;li&gt;0 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;150 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;200 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;240 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;330 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;390 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;470 Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;1.5K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;2.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;4.7K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;5.1K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;5.6K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;10.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;22.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;33.0K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;li&gt;100K Ohm 1/8 Watt 1% Resistor&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Package&lt;br/&gt;
&lt;br/&gt;
&lt;b&gt;2012&lt;/b&gt; - 2010 Surface Mount Package&lt;br/&gt;
&lt;ul&gt;&lt;li&gt;0.11 Ohm 1/2 Watt 1% Resistor - Digikey: RHM.11UCT-ND&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603MINI" package="0603-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2012" package="2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805_NOTHERMALS" package="0805_NOTHERMALS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402" package="_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402MP" package="_0402MP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603" package="_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603MP" package="_0603MP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805MP" package="_0805MP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3.3V">
<description>&lt;b&gt;3.3V Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="3.3V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5.0V">
<description>&lt;b&gt;5.0V Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="5.0V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND">
<description>&lt;b&gt;GND&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;VCC SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117" prefix="U" uservalue="yes">
<description>&lt;b&gt;LM1117 Voltage Regulator&lt;/b&gt;&lt;br&gt;
&lt;p&gt;LM1117 Adjustable Voltage regulator [Digikey: LM1117IMP-ADJDKR-ND]&lt;br&gt;
LM1117 3.3V Voltage regulator [AP1117E33GDIDKR-ND]&lt;br&gt;
LM1117 5.0V Voltage regulator [AP1117E50GDIDKR-ND]&lt;br&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SOT223-REFLOW&lt;/b&gt; - SOT223 package for solder paste/reflow ovens&lt;br/&gt;
&lt;b&gt;SOT223-WAVE&lt;/b&gt; - SOT223 package for hand-soldering (larger pads)&lt;/p&gt;
&lt;p&gt;Note: For the fixed-voltage regulators, simply set the ADJ pin to GND.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LM1117"/>
</gates>
<devices>
<device name="SOT223-REFLOW" package="SOT223-R">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT223-WAVE" package="SOT223-W">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_ELECTROLYTIC" prefix="C" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Electrolytic Capacitors&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SMT&lt;/b&gt;&lt;hr/&gt;&lt;/p&gt;
&lt;b&gt;PANASONIC_C&lt;/b&gt; - Size C Panasonic Electrolytic Aluminum Capacitor
&lt;ul&gt;
&lt;li&gt;47µF 16V 20% Electrolytic Capacitor [Digikey: PCE3890TR-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;PANASONIC_D&lt;/b&gt; - Size D Panasonic Electrolytic Aluminum Capacitor
&lt;ul&gt;
&lt;li&gt;100µF 25V 20% Electrolytic Capacitor [Digikey: PCE3898TR-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;PTH&lt;/b&gt;&lt;hr/&gt;&lt;/p&gt;
&lt;b&gt;3.5 mm grid, 8 mm diameter&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;...&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;3.5 mm grid, 10 mm diameter&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;...&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CAPACITOR_POL"/>
</gates>
<devices>
<device name="PANASONIC_C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PANASONIC_D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_3.5MMGRID_8MMDIA" package="CELEC_3.5MM_8MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_3.5MMGRID_10MMDIA" package="CELEC_3.5MM_10MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_PUSHBUTTON" prefix="SW" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Buttons&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;SOFTTOUCHSMD_SJ&lt;/b&gt; - Soft touch temporary push button (Super Junk Akihabara)
&lt;p&gt;Compatible with SKPMANE010 [Mouser: 688-SKPMAN]&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PUSHBUTTON"/>
</gates>
<devices>
<device name="SOFTTOUCHSMD_SJ" package="PUSHBUTTON_SMD_SJ">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RL" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;FTDI FT232RL&lt;/b&gt;&lt;/p&gt;
USB TO RS232 Converter
&lt;p&gt;Digikey: 768-1007-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232RL"/>
</gates>
<devices>
<device name="SSOP28" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="RXLED" pad="22"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXLED" pad="23"/>
<connect gate="G$1" pin="USB+" pad="15"/>
<connect gate="G$1" pin="USB-" pad="16"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS_LS20031" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;GPS Devices&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;LS20031&lt;/b&gt; - LS20031 10Hz UART GPS [Prod. ID] (Footprint for 0.1" header pins)</description>
<gates>
<gate name="G$1" symbol="GPS_LS20031"/>
</gates>
<devices>
<device name="" package="HEADER_1X05">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="RX" pad="2"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LED&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;0603&lt;/b&gt; - 0603 Surface Mount Package
&lt;hr&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;2mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Green LED - Low Power (3.9mcd, 2ma, 1.7Vf) - Digikey: 475-2709-2-ND&lt;/li&gt;
&lt;li&gt;Orange LED - Low Power (9.8mcd, 2ma, 1.8Vf) - Digikey: 475-1194-2-ND&lt;/li&gt;
&lt;li&gt;Red LED - Low Power (5mcd, 2ma, 1.8Vf) - Digikey: 475-1195-2-ND&lt;/li&gt;
&lt;li&gt;Yellow LED - Low Power (7mcd, 2ma, 1.8Vf) - Digikey: 475-1196-2-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;5mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Blue LED - Low Power (17mcd, 5ma, 2.9Vf) - Digikey: LNJ937W8CRACT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;0805&lt;/b&gt; - 0805 Surface Mount Package
&lt;hr&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;2mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Red LED (8.8mcd, 2mA, 1.8Vf, Clear) - Low Power [Digikey: 475-2510-1-ND]&lt;/li&gt;
&lt;li&gt;Green LED (5mcd, 2mA, 1.8Vf, Clear) - Low Power [Digikey: 475-2730-1-ND]&lt;/li&gt;
&lt;li&gt;Yellow LED (11.3mcd, 2mA, 1.8Vf, Clear) - Low Power [Digikey: 475-2555-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;&lt;u&gt;20mA:&lt;/u&gt;&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Red LED (104mcd, 20mA, Diffused) - LS R976 [Digikey: 475-1278-6-ND]&lt;/li&gt;
&lt;li&gt;Red LED (12mcd, 20mA, 2.0Vf, Clear) - APT2012EC [Digikey: 754-1128-1-ND]&lt;/li&gt;
&lt;li&gt;Green LED (15mcd, 20mA, 2.2Vf, Clear) - APT2012GC [Digikey: 754-1131-1-ND]&lt;/li&gt;
&lt;li&gt;Orange LED (160mcd, 20mA, 2.1Vf, Clear) - APT2012SECK [Digikey: 754-1130-1-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;1206&lt;/b&gt; - 1206 Surface Mount Package
&lt;hr&gt;
&lt;ul&gt;
&lt;li&gt;Green LED (26mcd, 20mA, Diffused) - LG N971  [Digikey: 475-1407-6-ND]&lt;/li&gt;
&lt;li&gt;Red LED (15mcd, 20mA, Diffused) - LH N974 [Digikey: 475-1416-6-ND]&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603_NOOUTLINE" package="CHIPLED_0603_NOOUTLINE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805_NOOUTLINE" package="CHIPLED_0805_NOOUTLINE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;USB Connectors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;USBMINIB&lt;/b&gt; - Surface Mount Female Mini-B USB Connector
&lt;p&gt;4UConnector: 06564&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="MINIB" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINIBLARGE" package="USB-MINIB_LARGER">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCBARREL" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;DC Barrel Jack&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;DCJACK_1.3MM_PTH&lt;/b&gt; - Through Hole 1.3mm Jack (4UConnector: 05536)&lt;/p&gt;
&lt;p&gt;&lt;b&gt;DCJACK_2MM_PTH&lt;/b&gt; - Through Hole 2.0/2.1 Jack (4UConnector: 05537)&lt;/p&gt;
&lt;p&gt;&lt;b&gt;DCJACK_2MM_SMT&lt;/b&gt; - SMT 2.0/2.1mm Jack(4UConnector: 03267)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DCBARREL"/>
</gates>
<devices>
<device name="PTH" package="DCJACK_2MM_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="DCJACK_2MM_SMT">
<connects>
<connect gate="G$1" pin="GND" pad="GNDBREAK"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.3MM" package="DCJACK_1.3MM_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT_CORRECT" package="DCJACK_2MM_SMT">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JTAG-ARM" prefix="JTAG">
<description>&lt;p&gt;&lt;b&gt;20 Pin JTAG Connector&lt;/b&gt;&lt;/p&gt;
For use with ARM7, and ARM9.  Supported by some Cortex M3 boards with SWJ-DP interfaces (dual SWP/JTAG support).
&lt;p&gt;4UConnector: 03556&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="JTAG-ARM"/>
</gates>
<devices>
<device name="" package="JTAG-ARM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EDGE" package="MOLEX20_RIGHTANGLE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2148" prefix="U" uservalue="yes">
<description>LPC2146/2148
&lt;p&gt;Digikey: LPC2148 - 568-1765-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC2144/2146/2148"/>
</gates>
<devices>
<device name="FBD64" package="LQFP64">
<connects>
<connect gate="G$1" pin="!RESET" pad="57"/>
<connect gate="G$1" pin="D+" pad="10"/>
<connect gate="G$1" pin="D-" pad="11"/>
<connect gate="G$1" pin="P0.0/TXD0/PWM1" pad="19"/>
<connect gate="G$1" pin="P0.1/RXD0/PWM3/EINT0" pad="21"/>
<connect gate="G$1" pin="P0.10/RTS1/CAP1.0/AD1.2" pad="35"/>
<connect gate="G$1" pin="P0.11/CTS1/CAP1.1/SCL1" pad="37"/>
<connect gate="G$1" pin="P0.12/DSR1/MAT1.0/AD1.3" pad="38"/>
<connect gate="G$1" pin="P0.13/DTR1/MAT1.1/AD1.4" pad="39"/>
<connect gate="G$1" pin="P0.14/DCD1/EINT1/SDA1" pad="41"/>
<connect gate="G$1" pin="P0.15/RI1/EINT2/AD1.5" pad="45"/>
<connect gate="G$1" pin="P0.16/EINT0/MAT0.2/CAP0.2" pad="46"/>
<connect gate="G$1" pin="P0.17/CAP1.2/SCK1/MAT1.2" pad="47"/>
<connect gate="G$1" pin="P0.18/CAP1.3/MISO1/MAT1.3" pad="53"/>
<connect gate="G$1" pin="P0.19/MAT1.2/MOSI1/CAP1.2" pad="54"/>
<connect gate="G$1" pin="P0.2/SCL0/CAP0.0" pad="22"/>
<connect gate="G$1" pin="P0.20/MAT1.3/SSEL1/EINT3" pad="55"/>
<connect gate="G$1" pin="P0.21/PWM5/AD1.6/CAP1.3" pad="1"/>
<connect gate="G$1" pin="P0.22/AD1.7/CAP0.0/MAT0.0" pad="2"/>
<connect gate="G$1" pin="P0.23/VBUS" pad="58"/>
<connect gate="G$1" pin="P0.25/AD0.4/AOUT" pad="9"/>
<connect gate="G$1" pin="P0.28/AD0.1/CAP0.2/MAT0.2" pad="13"/>
<connect gate="G$1" pin="P0.29/AD0.2/CAP0.3/MAT0.3" pad="14"/>
<connect gate="G$1" pin="P0.3/SDA0/MAT0.0/EINT1" pad="26"/>
<connect gate="G$1" pin="P0.30/AD0.3/EINT3/CAP0.0" pad="15"/>
<connect gate="G$1" pin="P0.31/UP_LED/CONNECT" pad="17"/>
<connect gate="G$1" pin="P0.4/SCK0/CAP0.1/AD0.6" pad="27"/>
<connect gate="G$1" pin="P0.5/MISO0/MAT0.1/AD0.7" pad="29"/>
<connect gate="G$1" pin="P0.6/MOSI0/CAP0.2/AD1.0" pad="30"/>
<connect gate="G$1" pin="P0.7/SSEL0/PWM2/EINT2" pad="31"/>
<connect gate="G$1" pin="P0.8/TXD1/PWM4/AD1.1" pad="33"/>
<connect gate="G$1" pin="P0.9/RXD1/PWM6/EINT3" pad="34"/>
<connect gate="G$1" pin="P1.16/TRACEPKT0" pad="16"/>
<connect gate="G$1" pin="P1.17/TRACEPKT1" pad="12"/>
<connect gate="G$1" pin="P1.18/TRACEPKT2" pad="8"/>
<connect gate="G$1" pin="P1.19/TRACEPKT3" pad="4"/>
<connect gate="G$1" pin="P1.20/TRACESYNC" pad="48"/>
<connect gate="G$1" pin="P1.21/PIPESTAT0" pad="44"/>
<connect gate="G$1" pin="P1.22/PIPESTAT1" pad="40"/>
<connect gate="G$1" pin="P1.23/PIPESTAT2" pad="36"/>
<connect gate="G$1" pin="P1.24/TRACECLK" pad="32"/>
<connect gate="G$1" pin="P1.25/EXTIN0" pad="28"/>
<connect gate="G$1" pin="P1.26/RTCK" pad="24"/>
<connect gate="G$1" pin="P1.27/TDO" pad="64"/>
<connect gate="G$1" pin="P1.28/TDI" pad="60"/>
<connect gate="G$1" pin="P1.29/TCK" pad="56"/>
<connect gate="G$1" pin="P1.30/TMS" pad="52"/>
<connect gate="G$1" pin="P1.31/!TRST" pad="20"/>
<connect gate="G$1" pin="RTXC1" pad="3"/>
<connect gate="G$1" pin="RTXC2" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="49"/>
<connect gate="G$1" pin="VDD@1" pad="23"/>
<connect gate="G$1" pin="VDD@2" pad="43"/>
<connect gate="G$1" pin="VDD@3" pad="51"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VREF" pad="63"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="18"/>
<connect gate="G$1" pin="VSS@3" pad="25"/>
<connect gate="G$1" pin="VSS@4" pad="42"/>
<connect gate="G$1" pin="VSS@5" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="59"/>
<connect gate="G$1" pin="XTAL1" pad="62"/>
<connect gate="G$1" pin="XTAL2" pad="61"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2103" prefix="U" uservalue="yes">
<description>LPC2101/2102/2103
&lt;p&gt;Digikey: LPC2103 LQFP - 568-2094-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC2103"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="DBGSEL" pad="27"/>
<connect gate="G$1" pin="P0.0/MAT3.1/TXD0" pad="13"/>
<connect gate="G$1" pin="P0.1/MAT3.2/RXD0" pad="14"/>
<connect gate="G$1" pin="P0.10/CAP1.0/AIN3/RTS1" pad="35"/>
<connect gate="G$1" pin="P0.11/CAP1.1/AIN4/CTS1" pad="36"/>
<connect gate="G$1" pin="P0.12/MAT1.0/AIN5/DSR1" pad="37"/>
<connect gate="G$1" pin="P0.13/MAT1.1/DTR1" pad="41"/>
<connect gate="G$1" pin="P0.14/EINT1/SCK1/DCD1" pad="44"/>
<connect gate="G$1" pin="P0.15/EINT2/RI1" pad="45"/>
<connect gate="G$1" pin="P0.16/EINT0/MAT0.2" pad="46"/>
<connect gate="G$1" pin="P0.18/CAP1.3/SDA1" pad="48"/>
<connect gate="G$1" pin="P0.19/MAT1.2/MISO1" pad="1"/>
<connect gate="G$1" pin="P0.2/SCL/CAP0.0" pad="18"/>
<connect gate="G$1" pin="P0.20/MAT1.3/MOSI1" pad="2"/>
<connect gate="G$1" pin="P0.21/SSEL1/P0.21" pad="3"/>
<connect gate="G$1" pin="P0.22/AIN0" pad="32"/>
<connect gate="G$1" pin="P0.23/AIN1" pad="33"/>
<connect gate="G$1" pin="P0.24/AIN2" pad="34"/>
<connect gate="G$1" pin="P0.25/AIN6" pad="38"/>
<connect gate="G$1" pin="P0.26/AIN7" pad="39"/>
<connect gate="G$1" pin="P0.27/CAP2.0/TRST" pad="8"/>
<connect gate="G$1" pin="P0.28/CAP2.1/TMS" pad="9"/>
<connect gate="G$1" pin="P0.29/CAP2.2/TCK" pad="10"/>
<connect gate="G$1" pin="P0.3/SDA/MAT0.0" pad="21"/>
<connect gate="G$1" pin="P0.30/MAT3.3/TDI" pad="15"/>
<connect gate="G$1" pin="P0.31/TDO" pad="16"/>
<connect gate="G$1" pin="P0.4/SCK/CAP0.1" pad="22"/>
<connect gate="G$1" pin="P0.5/MISO/MAT0.1" pad="23"/>
<connect gate="G$1" pin="P0.6/MOSI/CAP0.2" pad="24"/>
<connect gate="G$1" pin="P0.7/SSEL/MAT2.0" pad="28"/>
<connect gate="G$1" pin="P0.8/TXD1/MAT2.1" pad="29"/>
<connect gate="G$1" pin="P0.9/RXD1/MAT2.2" pad="30"/>
<connect gate="G$1" pin="PO0.17/CAP1.2/SCL1" pad="47"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="RTCK" pad="26"/>
<connect gate="G$1" pin="RTXC1" pad="20"/>
<connect gate="G$1" pin="RTXC2" pad="25"/>
<connect gate="G$1" pin="VBAT" pad="4"/>
<connect gate="G$1" pin="VDD1.8(CORE)" pad="5"/>
<connect gate="G$1" pin="VDD3-1(I/O)" pad="40"/>
<connect gate="G$1" pin="VDD3-2(I/O)" pad="17"/>
<connect gate="G$1" pin="VDDA" pad="42"/>
<connect gate="G$1" pin="VSS1" pad="7"/>
<connect gate="G$1" pin="VSS2" pad="19"/>
<connect gate="G$1" pin="VSS4" pad="43"/>
<connect gate="G$1" pin="VSSA" pad="31"/>
<connect gate="G$1" pin="X1" pad="11"/>
<connect gate="G$1" pin="X2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER" prefix="SJ" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;SMD Solder JUMPER&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Solder the two pads together to create a connection, or remove the solder to break it.&lt;/p&gt;
&lt;b&gt;REFLOW&lt;/b&gt; - Use this footprint for solder paste and reflow ovens.&lt;br/&gt;
&lt;b&gt;WAVE&lt;/b&gt; - Use this footprint for hand-soldering (larger pads).
&lt;p&gt;&lt;b&gt;CLOSED&lt;/b&gt; - Has a trace between the two pads to ensure it is closed by default.  The trace needs to be cut to disable the jumper, and can be closed again by creating a solder bridge between the two pads.&lt;/p&gt;</description>
<gates>
<gate name="1" symbol="SOLDERJUMPER"/>
</gates>
<devices>
<device name="REFLOW" package="SOLDERJUMPER_REFLOW">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WAVE" package="SOLDERJUMPER_WAVE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CLOSED" package="SOLDERJUMPER_CLOSEDWIRE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="REFLOW_NOPASTE" package="SOLDERJUMPER_REFLOW_NOPASTE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOLDERJUMPER_ARROW_NOPASTE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="EXCLUDE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;JUMPER&lt;/b&gt; - 2 Pins</description>
<gates>
<gate name="A" symbol="JUMPER2"/>
</gates>
<devices>
<device name="" package="JUMPER2">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;JUMPER&lt;/b&gt; - 3 Pins</description>
<gates>
<gate name="1" symbol="JUMPER3"/>
</gates>
<devices>
<device name="" package="JUMPER3">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Y" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Crystals&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;HC49UP&lt;/b&gt; - Surface Mount Crystal
&lt;ul&gt;
&lt;li&gt;4.0MHz 18pF +/-30ppm Surface Mount Crystal [Digikey: 535-9857-1-ND]&lt;/li&gt;
&lt;li&gt;12.0 MHz Surface Mount Crystal [Digikey: 535-9869-6-ND]&lt;/li&gt;
&lt;li&gt;25.0 MHz Surface Mount Crystal [Digikey: 535-9078-1-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;2.5 x 2.0mm&lt;/b&gt; - MEMs SMT Crystal
&lt;ul&gt;
&lt;li&gt;16.0 MHz 10pF 20ppm 2.5 x 2.0mm Crystal [Digikey -40-85°C: 535-10923-1-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;3.2 x 2.5mm&lt;/b&gt; - MEMs SMT Crystal
&lt;ul&gt;
&lt;li&gt;12.0 MHz 8pF 15ppm 3.2 x 2.5mm Crystal [Digikey: &lt;b&gt;-10-70°C&lt;/b&gt;: 644-1047-1-ND &lt;b&gt;-40-125°C&lt;/b&gt;: 644-1128-1-ND]&lt;/li&gt;
&lt;li&gt;16.0 MHz 8pF 15ppm 3.2 x 2.5mm Crystal [Digikey: &lt;b&gt;-10-70°C&lt;/b&gt;: 644-1049-1-ND &lt;b&gt;-40-125°C&lt;/b&gt;: 644-1129-2-ND]&lt;/li&gt;
&lt;li&gt;16.0 MHz 10pF 10ppm 3.2 x 2.5mm Crystal [Digikey: 644-1100-1-ND]&lt;/li&gt;
&lt;li&gt;27.12 MHz 18pF 30ppm 3.2 x 2.5mm Crystal [Digikey: 887-1424-1-ND]&lt;/li&gt;
&lt;li&gt;27.12MHz 10pF 10ppm 3.2 x 2.5mm Crystal [Digikey: 887-1329-1-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;4.9 x 1.8mm&lt;/b&gt; - MEMs SMT Crystal
&lt;ul&gt;
&lt;li&gt;32.768 KHz 12.5pF 20ppm 4.9 x 1.8mm Crystal [Digikey: SE2415CT-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;8.0 x 3.8mm&lt;/b&gt;&lt;/p&gt; - Surface Mount Crystal
&lt;ul&gt;
&lt;li&gt;32.768kHz 12.5pF 20ppm -40°C-85°C [Digikey: 535-9166-2-ND]&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;Cylinder&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;32.768KHz Cylinder Crystal (2x6mm body) [Ex. Digikey: 300-8341-2-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;

&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="SMD" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="32.768" package="CRYSTAL_CYL_2X6MM_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THIN" package="CRYSTAL_3.2X2.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THIN32K" package="CRYSTAL_4.9X1.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8X3.8SMT" package="CRYSTAL_8X3.8">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5X2.0MM" package="CRYSTAL_2.5X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_PNP" prefix="Q" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;PNP Transistor&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Transistor (PNP) 800mA 60V, 1.6V VCE @ 500mA [Digikey: MMBT2907AFSTR-ND]&lt;/li&gt;
&lt;li&gt;Transistor (PNP) Low Sat - 1.5A 20V, 260mV VCE @ 400mA [Digikey: ZXTP25020DFLTR-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;
&lt;b&gt;SOT23-R&lt;/b&gt; - SOT23 footprint optimised for use with solder paste and reflow ovens.&lt;br&gt;
&lt;b&gt;SOT23-W&lt;/b&gt; - SOT23 footprint optimised for hand-soldering (larger pads).
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="SOT23-REFLOW" package="SOT23-R">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23-WAVE" package="SOT23-W">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME_A4" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="FRAME_A4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_2PIN" prefix="CN" uservalue="yes">
<description>JST 2-Pin Right-Angle Connector
&lt;ul&gt;
&lt;li&gt;PH-Series - 4UConnector: 17311&lt;/li&gt;
&lt;li&gt;SH-Series - 4UConnector: 07278&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="JSTPH2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SH2" package="JSTSH2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PH2_NOTHERMALS" package="JSTPH2_NOTHERMALS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER_1X02" prefix="CN" uservalue="yes">
<description>2-Pin 0,254cm / 0.1" Header</description>
<gates>
<gate name="G$1" symbol="HEADER_1X02"/>
</gates>
<devices>
<device name="" package="HEADER_1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACCEL_ADXL335" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;ADXL335 Low-Power 3 Axis Accelerometer&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;LFCSP16-R&lt;/b&gt; - 16 Pin LFCSP Package (Reflow footprint)&lt;br&gt;
&lt;b&gt;LFSCP16-W&lt;/b&gt; - 16 Pin LFCSP Package (Wave footprint with extended pads for hand soldering)&lt;br&gt;
&lt;/p&gt;
&lt;p&gt;Digikey: ADXL335BCPZ-RL7CT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADXL335"/>
</gates>
<devices>
<device name="REFLOW" package="LFCSP16-R">
<connects>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="6"/>
<connect gate="G$1" pin="GND4" pad="7"/>
<connect gate="G$1" pin="TEST" pad="2"/>
<connect gate="G$1" pin="VS1" pad="14"/>
<connect gate="G$1" pin="VS2" pad="15"/>
<connect gate="G$1" pin="X" pad="12"/>
<connect gate="G$1" pin="Y" pad="10"/>
<connect gate="G$1" pin="Z" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WAVE" package="LFCSP16-W">
<connects>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="6"/>
<connect gate="G$1" pin="GND4" pad="7"/>
<connect gate="G$1" pin="TEST" pad="2"/>
<connect gate="G$1" pin="VS1" pad="14"/>
<connect gate="G$1" pin="VS2" pad="15"/>
<connect gate="G$1" pin="X" pad="12"/>
<connect gate="G$1" pin="Y" pad="10"/>
<connect gate="G$1" pin="Z" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X01_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X01_2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM_OVAL" package="1X01_2MM_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="" package="1X02_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X02_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X02_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X03_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X03_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1MMPADS" package="1X03_1.0MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X03_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="1X04_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X04_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X04_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1MMPADS" package="1X04_1.0MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X04_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="1X05_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X05_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X05_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X05_1.27MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X05_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="70MIL" package="1X05_ROUND_70">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X06_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X06_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X06_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="70MIL" package="1X06_ROUND_70">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSTOUCHCON" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Nintendo DS Touch Screen Connector&lt;/b&gt; [Part No.]&lt;/p&gt;
4 pin 0.5mm Pitch ZIF Cable Connector

&lt;p&gt;Upper Contacts - 4UConnector: 08644&lt;br/&gt;Bottom Contacts - 4UConnector: 11793&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DSTOUCHCON"/>
</gates>
<devices>
<device name="" package="FPC4PIN">
<connects>
<connect gate="G$1" pin="X1" pad="4"/>
<connect gate="G$1" pin="X2" pad="2"/>
<connect gate="G$1" pin="Y1" pad="1"/>
<connect gate="G$1" pin="Y2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENC28J60" prefix="U" uservalue="yes">
<description>&lt;b&gt;ENC28J60 SPI Ethernet Controller&lt;/b&gt;
&lt;p&gt;Digikey: SSOP - ENC28J60/SS-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ENC28J60"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="CLKOUT" pad="3"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="INT" pad="4"/>
<connect gate="G$1" pin="LEDA" pad="27"/>
<connect gate="G$1" pin="LEDB" pad="26"/>
<connect gate="G$1" pin="OSC1" pad="23"/>
<connect gate="G$1" pin="OSC2" pad="24"/>
<connect gate="G$1" pin="RBIAS" pad="14"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SCK" pad="8"/>
<connect gate="G$1" pin="SI" pad="7"/>
<connect gate="G$1" pin="SO" pad="6"/>
<connect gate="G$1" pin="TPIN+" pad="13"/>
<connect gate="G$1" pin="TPIN-" pad="12"/>
<connect gate="G$1" pin="TPOUT+" pad="17"/>
<connect gate="G$1" pin="TPOUT-" pad="16"/>
<connect gate="G$1" pin="VCAP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VDD_OSC" pad="25"/>
<connect gate="G$1" pin="VDD_PLL" pad="20"/>
<connect gate="G$1" pin="VDD_RX" pad="19"/>
<connect gate="G$1" pin="VDD_TX" pad="15"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSS_OSC" pad="22"/>
<connect gate="G$1" pin="VSS_PLL" pad="21"/>
<connect gate="G$1" pin="VSS_RX" pad="11"/>
<connect gate="G$1" pin="VSS_TX" pad="18"/>
<connect gate="G$1" pin="WOL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD10"/>
</gates>
<devices>
<device name="" package="1X10_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X10_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X10_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X10_2MM" package="1X10_ROUND_2MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THICKER" package="1X10_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="70MIL" package="1X10_ROUND70">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X16" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X16"/>
</gates>
<devices>
<device name="" package="2X16">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X16" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD16"/>
</gates>
<devices>
<device name="" package="1X16_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X16_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X16_2MM">
<connects>
<connect gate="A" pin="1" pad="P$1"/>
<connect gate="A" pin="10" pad="P$10"/>
<connect gate="A" pin="11" pad="P$11"/>
<connect gate="A" pin="12" pad="P$12"/>
<connect gate="A" pin="13" pad="P$13"/>
<connect gate="A" pin="14" pad="P$14"/>
<connect gate="A" pin="15" pad="P$15"/>
<connect gate="A" pin="16" pad="P$16"/>
<connect gate="A" pin="2" pad="P$2"/>
<connect gate="A" pin="3" pad="P$3"/>
<connect gate="A" pin="4" pad="P$4"/>
<connect gate="A" pin="5" pad="P$5"/>
<connect gate="A" pin="6" pad="P$6"/>
<connect gate="A" pin="7" pad="P$7"/>
<connect gate="A" pin="8" pad="P$8"/>
<connect gate="A" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM_OVAL" package="1X16_2MM_OVAL">
<connects>
<connect gate="A" pin="1" pad="P$1"/>
<connect gate="A" pin="10" pad="P$10"/>
<connect gate="A" pin="11" pad="P$11"/>
<connect gate="A" pin="12" pad="P$12"/>
<connect gate="A" pin="13" pad="P$13"/>
<connect gate="A" pin="14" pad="P$14"/>
<connect gate="A" pin="15" pad="P$15"/>
<connect gate="A" pin="16" pad="P$16"/>
<connect gate="A" pin="2" pad="P$2"/>
<connect gate="A" pin="3" pad="P$3"/>
<connect gate="A" pin="4" pad="P$4"/>
<connect gate="A" pin="5" pad="P$5"/>
<connect gate="A" pin="6" pad="P$6"/>
<connect gate="A" pin="7" pad="P$7"/>
<connect gate="A" pin="8" pad="P$8"/>
<connect gate="A" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="2X05_1.27MM_SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MOLEX20_SIDE" package="MOLEX20_RIGHTANGLE">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X7"/>
</gates>
<devices>
<device name="" package="2X07">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD7"/>
</gates>
<devices>
<device name="" package="1X07_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X07_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THICKER" package="1X07_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="70MIL" package="1X07_ROUND_70">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD8"/>
</gates>
<devices>
<device name="" package="1X08_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X08_ROUND">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X08_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="70MIL" package="1X08_ROUND_70">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09_OVAL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X09_ROUND_76">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="70MIL" package="1X09_ROUND_70">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-N" prefix="Q" uservalue="yes">
<description>&lt;b&gt;N-Channel Mosfet&lt;/b&gt;
&lt;p&gt;&lt;b&gt;LEGEND&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;VDS&lt;/b&gt;: Voltage Drain-Source&lt;br/&gt;
&lt;b&gt;ID&lt;/b&gt;: Drain Current&lt;br/&gt;
&lt;b&gt;RDS(ON)&lt;/b&gt;: Drain-Source On-State Resistance&lt;br/&gt;
&lt;b&gt;VGS(TH)&lt;/b&gt;: Gate-Source Threshold Voltage&lt;br/&gt;
&lt;b&gt;CISS&lt;/b&gt;: Drain-Source Input Capacitance
&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;SOT-23&lt;/b&gt;
&lt;table border="0" width="90%" cellspacing="0" cellpadding="5"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
&lt;td&gt;Name&lt;/td&gt;
&lt;td&gt;VDS&lt;/td&gt;
&lt;td&gt;ID&lt;/td&gt;
&lt;td&gt;RDS(ON)&lt;/td&gt;
&lt;td&gt;VGS(TH)&lt;/td&gt;
&lt;td&gt;CISS&lt;/td&gt;
&lt;td&gt;Order Number&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;2N7002E&lt;/td&gt;
&lt;td&gt;60V&lt;/td&gt;
&lt;td&gt;260mA&lt;/td&gt;
&lt;td&gt;2.5 Ohm&lt;/td&gt;
&lt;td&gt;2.5V @ 250uA&lt;/td&gt;
&lt;td&gt;26.7pF @ 25V&lt;/td&gt;
&lt;td&gt;2N7002ET1GOSTR-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;BSH103&lt;/td&gt;
&lt;td&gt;30V&lt;/td&gt;
&lt;td&gt;850mA&lt;/td&gt;
&lt;td&gt;400 mOhm&lt;/td&gt;
&lt;td&gt;400mV @ 1mA&lt;/td&gt;
&lt;td&gt;83pF @ 24V&lt;/td&gt;
&lt;td&gt;BSH103,235-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;BSS138&lt;/td&gt;
&lt;td&gt;60V&lt;/td&gt;
&lt;td&gt;320mA&lt;/td&gt;
&lt;td&gt;1.6 Ohm&lt;/td&gt;
&lt;td&gt;1.5V @ 250uA&lt;/td&gt;
&lt;td&gt;50pF @ 10V&lt;/td&gt;
&lt;td&gt;Mouser: 771-BSS138PW115&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;DMN2075U-7&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;4.2A&lt;/td&gt;
&lt;td&gt;38 mOhm&lt;/td&gt;
&lt;td&gt;1V @ 250 uA&lt;/td&gt;
&lt;td&gt;594.3pF @ 10V&lt;/td&gt;
&lt;td&gt;DMN2075U-7DICT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;/table&gt; 
&lt;/p&gt;

&lt;p&gt;* BSS138 good choice for I2C level-shifting&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="REFLOW" package="SOT23-R">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WAVE" package="SOT23-W">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MUX-1X16" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;1x16 Channel Analog Multiplexer/Demultiplexer&lt;/b&gt; [Part No.]&lt;/p&gt;
Texas Instruments CD74HC4067
&lt;p&gt;Digikey: 296-9226-6-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CD74HC4067"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="CH0" pad="9"/>
<connect gate="G$1" pin="CH1" pad="8"/>
<connect gate="G$1" pin="CH10" pad="21"/>
<connect gate="G$1" pin="CH11" pad="20"/>
<connect gate="G$1" pin="CH12" pad="19"/>
<connect gate="G$1" pin="CH13" pad="18"/>
<connect gate="G$1" pin="CH14" pad="17"/>
<connect gate="G$1" pin="CH15" pad="16"/>
<connect gate="G$1" pin="CH2" pad="7"/>
<connect gate="G$1" pin="CH3" pad="6"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="4"/>
<connect gate="G$1" pin="CH6" pad="3"/>
<connect gate="G$1" pin="CH7" pad="2"/>
<connect gate="G$1" pin="CH8" pad="23"/>
<connect gate="G$1" pin="CH9" pad="22"/>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="EN" pad="15"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="SEL0" pad="10"/>
<connect gate="G$1" pin="SEL1" pad="11"/>
<connect gate="G$1" pin="SEL2" pad="14"/>
<connect gate="G$1" pin="SEL3" pad="13"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34063A" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;MC34063A - 1.5A 3V-40V Boost/Buck/Inverting Voltage Regulator&lt;/b&gt; [Part No.]&lt;/p&gt;
&lt;p&gt;Allows you to 'boost', reduce or invert the voltage of your power supply to a more appropriate level.  Common voltage regulators like the LM1117 are easy to use, but they can only 'reduce' the voltage level and require more volts than they provide, making them useless for low voltage power supplies like batteries or solar panels. A 'Step-Up' regulator like the MC34063A solves this problem by also allowing you to increase the voltage to a pre-determined level, though you still need to pay attention to the minimum voltage level the converter can handle, keeping in mind that many 'step-up' converts are less efficient at the two extreme ends of their working range.&lt;/p&gt;
&lt;p&gt;Given that many step-up circuits introduce some ripple to the power supply, you can often get a much 'smoother' supply by boosting the voltage up to 5.0V and then using a standard fixed voltage regulator (such as the common LM1117, etc.) to drop the voltage back down to 3.3V.  This may not be necessary, and some step up regulators can provide a smooth supply on their own, but it's worth keeping in mind if you do encounter some ripple in the power supply using only a step-up IC for your power supply.&lt;/p&gt;
Texas Instruments MC34063A
&lt;p&gt;Digikey: 296-17765-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MC34063ADR"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="CII" pad="5"/>
<connect gate="G$1" pin="D_COL" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IPK" pad="7"/>
<connect gate="G$1" pin="S_COL" pad="1"/>
<connect gate="G$1" pin="S_EMIT" pad="2"/>
<connect gate="G$1" pin="TCAP" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MUX-2X4" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;2x4 Channel Analog Multiplexer/Demultiplexer&lt;/b&gt; [Part No.]&lt;/p&gt;
Texas Instruments CD74HC4052M
&lt;p&gt;Digikey: 296-9218-5-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CD74HC4052"/>
</gates>
<devices>
<device name="" package="SOIC16">
<connects>
<connect gate="G$1" pin="CH-A0" pad="12"/>
<connect gate="G$1" pin="CH-A1" pad="14"/>
<connect gate="G$1" pin="CH-A2" pad="15"/>
<connect gate="G$1" pin="CH-A3" pad="11"/>
<connect gate="G$1" pin="CH-B0" pad="1"/>
<connect gate="G$1" pin="CH-B1" pad="5"/>
<connect gate="G$1" pin="CH-B2" pad="2"/>
<connect gate="G$1" pin="CH-B3" pad="4"/>
<connect gate="G$1" pin="COM-A" pad="13"/>
<connect gate="G$1" pin="COM-B" pad="3"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="SEL0" pad="10"/>
<connect gate="G$1" pin="SEL1" pad="9"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="VEE" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73833" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Lithium-Polymer/Lithium-Ion Battery Charger&lt;/b&gt; [Part No.]&lt;/p&gt;
Microchip MCP73833
&lt;p&gt;&lt;b&gt;MSOP10&lt;/b&gt; (tube only):&lt;/p&gt;
&lt;p&gt;Digikey: MCP73833T-AMI/UN or MCP73833-FCI/UN-ND&lt;br/&gt;
Mouser: 579-MCP73833-AMI/UN&lt;/p&gt;
&lt;p&gt;&lt;b&gt;DFN10&lt;/b&gt; (tape):&lt;/p&gt;
&lt;p&gt;Digikey: &lt;/p&gt;
&lt;p&gt;Note Chips ending in 'AMI' have no timer, and chips ending in 'FCI' have a 6-hour timer that will end the charge sequence after 6 horus regqrdless of current charge level.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP73833"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PG" pad="7"/>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="THERM" pad="8"/>
<connect gate="G$1" pin="VBAT1" pad="10"/>
<connect gate="G$1" pin="VBAT2" pad="9"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DFN" package="DFN10_3X3MM">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PG" pad="7"/>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="THERM" pad="8"/>
<connect gate="G$1" pin="VBAT1" pad="9"/>
<connect gate="G$1" pin="VBAT2" pad="10"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A3967SLB" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Allegro 3967&lt;/b&gt; - MICROSTEPPING DRIVER WITH TRANSLATOR&lt;/p&gt;
Source: 3967.pdf
&lt;p&gt;Digikey: 620-1140-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ALLEGRO3967"/>
</gates>
<devices>
<device name="" package="SOIC24WIDE">
<connects>
<connect gate="G$1" pin="!ENABLE" pad="15"/>
<connect gate="G$1" pin="!RESET" pad="22"/>
<connect gate="G$1" pin="!SLEEP" pad="3"/>
<connect gate="G$1" pin="DIR" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="18"/>
<connect gate="G$1" pin="GND@4" pad="19"/>
<connect gate="G$1" pin="LOAD-SUPPLY1" pad="20"/>
<connect gate="G$1" pin="LOAD-SUPPLY2" pad="5"/>
<connect gate="G$1" pin="MS1" pad="12"/>
<connect gate="G$1" pin="MS2" pad="13"/>
<connect gate="G$1" pin="OUT1A" pad="16"/>
<connect gate="G$1" pin="OUT1B" pad="21"/>
<connect gate="G$1" pin="OUT2A" pad="9"/>
<connect gate="G$1" pin="OUT2B" pad="4"/>
<connect gate="G$1" pin="PFD" pad="24"/>
<connect gate="G$1" pin="RC1" pad="23"/>
<connect gate="G$1" pin="RC2" pad="2"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE1" pad="17"/>
<connect gate="G$1" pin="SENSE2" pad="8"/>
<connect gate="G$1" pin="STEP" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIPSWITCH_2PIN" prefix="SW" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;DIP Switch - 2 Pin&lt;/b&gt; - [4UConnector: 19493]&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIPSWITCH_2"/>
</gates>
<devices>
<device name="" package="DIPSWITCH_2PIN">
<connects>
<connect gate="G$1" pin="1A" pad="1A"/>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="2A" pad="2A"/>
<connect gate="G$1" pin="2B" pad="2B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TESTPOINT" prefix="TP" uservalue="yes">
<description>&lt;b&gt;Test Point&lt;/b&gt;
&lt;p&gt;Various test points for characterisation and PCB testing&lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;TESTPOINT_SMT&lt;/b&gt; - Compact Surface Mount Test Point [Digikey: 5016KTR-ND]&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TESTPOINT"/>
</gates>
<devices>
<device name="" package="TESTPOINT_SMT">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PAD" package="TESTPOINT_PAD_2MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND2MM" package="TESTPOINT_ROUND_2MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.1&quot;" package="1X01_ROUND">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="EXCLUDE"/>
</technology>
</technologies>
</device>
<device name="1.5X2.0MM_NOCREAM" package="PAD-1.5X2.0">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND1MM" package="TESTPOINT_ROUND_1MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND0.5MM" package="TESTPOINT_ROUND_0.5MM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT" prefix="VR" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Potentiometers&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt; 3mm 10K Single Turn - Digikey: 3303W-103ETR-ND&lt;/li&gt;
&lt;li&gt; 3mm 100K Single Turn - Digikey: 3303X-104ETR-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="POTENTIOMETER"/>
</gates>
<devices>
<device name="10K_BOURNS" package="TRIMPOT_BOURNS3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_PSP_TSCON" prefix="CN" uservalue="yes">
<description>Sharp LQ043xxx/PSP Touch Screen Connector</description>
<gates>
<gate name="G$1" symbol="PSP_TOUCHCON"/>
</gates>
<devices>
<device name="" package="PSP_TSCON">
<connects>
<connect gate="G$1" pin="X1" pad="X1"/>
<connect gate="G$1" pin="X2" pad="X2"/>
<connect gate="G$1" pin="Y1" pad="Y1"/>
<connect gate="G$1" pin="Y2" pad="Y2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_PSP_BACKLIGHTCON" prefix="CN" uservalue="yes">
<description>&lt;p&gt;Sharp LQ043xx/PSP Backlight Connector&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;FPC4_UPPER&lt;/b&gt; - FPC Connector w/Upper Contacts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;FPC4_BOTTOM&lt;/b&gt; - FPC Connector w/Bottom Contacts&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Use the &lt;b&gt;UPPER&lt;/b&gt; connector if the LCD connector is on one side of the board and the screen will be wrapped around the edge onto the other side of the board (which is what normally happens).&lt;/p&gt;
&lt;p&gt;Use the &lt;b&gt;BOTTOM&lt;/b&gt; connector if the LCD and the connector are on the same side of the board (the cable with be folded directly underneath the screen).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PSP_BACKLIGHTCON"/>
</gates>
<devices>
<device name="" package="PSP_BACKLIGHTCON">
<connects>
<connect gate="G$1" pin="NC1" pad="NC1"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="VLED+" pad="VLED+"/>
<connect gate="G$1" pin="VLED-" pad="VLED-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FPC4_UPPER" package="FPC4PIN">
<connects>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="VLED+" pad="4"/>
<connect gate="G$1" pin="VLED-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FPC4_BOTTOM" package="FPC4PIN">
<connects>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="VLED+" pad="1"/>
<connect gate="G$1" pin="VLED-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_PSP_LCDCON" prefix="CN" uservalue="yes">
<description>&lt;p&gt;Sharp LQ043xx/PSP 24-Bit LCD Display&lt;/p&gt;
&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;UPPER&lt;/b&gt; - FPC Connector w/Upper Contacts&lt;/li&gt;
&lt;li&gt;&lt;b&gt;BOTTOM&lt;/b&gt; - FPC Connector w/Bottom Contacts&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Use the &lt;b&gt;UPPER&lt;/b&gt; connector if the LCD connector is on one side of the board and the LCD will be wrapped around the edge onto the other side of the board (which is what normally happens).&lt;/p&gt;
&lt;p&gt;Use the &lt;b&gt;BOTTOM&lt;/b&gt; connector if the LCD and the connector are on the same side of the board (the cable with be folded directly underneath the LCD).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PSP_LCDCON"/>
</gates>
<devices>
<device name="BOTTOM" package="FPC40PIN">
<connects>
<connect gate="G$1" pin="AVDD1(5V)" pad="P$35"/>
<connect gate="G$1" pin="AVVD2(5V)" pad="P$36"/>
<connect gate="G$1" pin="B0(LSB)" pad="P$21"/>
<connect gate="G$1" pin="B1" pad="P$22"/>
<connect gate="G$1" pin="B2" pad="P$23"/>
<connect gate="G$1" pin="B3" pad="P$24"/>
<connect gate="G$1" pin="B4" pad="P$25"/>
<connect gate="G$1" pin="B5" pad="P$26"/>
<connect gate="G$1" pin="B6" pad="P$27"/>
<connect gate="G$1" pin="B7(MSB)" pad="P$28"/>
<connect gate="G$1" pin="CK" pad="P$30"/>
<connect gate="G$1" pin="DISP" pad="P$31"/>
<connect gate="G$1" pin="G0(LSB)" pad="P$13"/>
<connect gate="G$1" pin="G1" pad="P$14"/>
<connect gate="G$1" pin="G2" pad="P$15"/>
<connect gate="G$1" pin="G3" pad="P$16"/>
<connect gate="G$1" pin="G4" pad="P$17"/>
<connect gate="G$1" pin="G5" pad="P$18"/>
<connect gate="G$1" pin="G6" pad="P$19"/>
<connect gate="G$1" pin="G7(MSB)" pad="P$20"/>
<connect gate="G$1" pin="GND1" pad="P$1"/>
<connect gate="G$1" pin="GND2" pad="P$2"/>
<connect gate="G$1" pin="GND3" pad="P$29"/>
<connect gate="G$1" pin="HSYNC" pad="P$32"/>
<connect gate="G$1" pin="NC1" pad="P$34"/>
<connect gate="G$1" pin="NC2" pad="P$37"/>
<connect gate="G$1" pin="R0(LSB)" pad="P$5"/>
<connect gate="G$1" pin="R1" pad="P$6"/>
<connect gate="G$1" pin="R2" pad="P$7"/>
<connect gate="G$1" pin="R3" pad="P$8"/>
<connect gate="G$1" pin="R4" pad="P$9"/>
<connect gate="G$1" pin="R5" pad="P$10"/>
<connect gate="G$1" pin="R6" pad="P$11"/>
<connect gate="G$1" pin="R7(MSB)" pad="P$12"/>
<connect gate="G$1" pin="TEST1(OPEN)" pad="P$38"/>
<connect gate="G$1" pin="TEST2(GND)" pad="P$39"/>
<connect gate="G$1" pin="TEST3(GND)" pad="P$40"/>
<connect gate="G$1" pin="VCC1(2.5V)" pad="P$3"/>
<connect gate="G$1" pin="VCC2(2.5V)" pad="P$4"/>
<connect gate="G$1" pin="VSYNC" pad="P$33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UPPER" package="FPC40PIN">
<connects>
<connect gate="G$1" pin="AVDD1(5V)" pad="P$6"/>
<connect gate="G$1" pin="AVVD2(5V)" pad="P$5"/>
<connect gate="G$1" pin="B0(LSB)" pad="P$20"/>
<connect gate="G$1" pin="B1" pad="P$19"/>
<connect gate="G$1" pin="B2" pad="P$18"/>
<connect gate="G$1" pin="B3" pad="P$17"/>
<connect gate="G$1" pin="B4" pad="P$16"/>
<connect gate="G$1" pin="B5" pad="P$15"/>
<connect gate="G$1" pin="B6" pad="P$14"/>
<connect gate="G$1" pin="B7(MSB)" pad="P$13"/>
<connect gate="G$1" pin="CK" pad="P$11"/>
<connect gate="G$1" pin="DISP" pad="P$10"/>
<connect gate="G$1" pin="G0(LSB)" pad="P$28"/>
<connect gate="G$1" pin="G1" pad="P$27"/>
<connect gate="G$1" pin="G2" pad="P$26"/>
<connect gate="G$1" pin="G3" pad="P$25"/>
<connect gate="G$1" pin="G4" pad="P$24"/>
<connect gate="G$1" pin="G5" pad="P$23"/>
<connect gate="G$1" pin="G6" pad="P$22"/>
<connect gate="G$1" pin="G7(MSB)" pad="P$21"/>
<connect gate="G$1" pin="GND1" pad="P$40"/>
<connect gate="G$1" pin="GND2" pad="P$39"/>
<connect gate="G$1" pin="GND3" pad="P$12"/>
<connect gate="G$1" pin="HSYNC" pad="P$9"/>
<connect gate="G$1" pin="NC1" pad="P$7"/>
<connect gate="G$1" pin="NC2" pad="P$4"/>
<connect gate="G$1" pin="R0(LSB)" pad="P$36"/>
<connect gate="G$1" pin="R1" pad="P$35"/>
<connect gate="G$1" pin="R2" pad="P$34"/>
<connect gate="G$1" pin="R3" pad="P$33"/>
<connect gate="G$1" pin="R4" pad="P$32"/>
<connect gate="G$1" pin="R5" pad="P$31"/>
<connect gate="G$1" pin="R6" pad="P$30"/>
<connect gate="G$1" pin="R7(MSB)" pad="P$29"/>
<connect gate="G$1" pin="TEST1(OPEN)" pad="P$3"/>
<connect gate="G$1" pin="TEST2(GND)" pad="P$2"/>
<connect gate="G$1" pin="TEST3(GND)" pad="P$1"/>
<connect gate="G$1" pin="VCC1(2.5V)" pad="P$38"/>
<connect gate="G$1" pin="VCC2(2.5V)" pad="P$37"/>
<connect gate="G$1" pin="VSYNC" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.5V">
<gates>
<gate name="G$1" symbol="2.5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.8V">
<gates>
<gate name="G$1" symbol="1.8V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHT_TCS3414" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Taos TCS3414CS Digital Colour Light Sensor&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Mouser: 856-TCS3414CS &lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TCS3414"/>
</gates>
<devices>
<device name="" package="TCS3414_CS6">
<connects>
<connect gate="G$1" pin="GND" pad="A3"/>
<connect gate="G$1" pin="INT" pad="B3"/>
<connect gate="G$1" pin="SCL" pad="A1"/>
<connect gate="G$1" pin="SDA" pad="B1"/>
<connect gate="G$1" pin="SYNC" pad="A2"/>
<connect gate="G$1" pin="VDD" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_4PIN" prefix="CN" uservalue="yes">
<description>JST 4-Pin Right-Angle Connector
&lt;p&gt;4UConnector: 17312&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="JSTPH4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHT_TSL2561" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;TSL2561 Light-To-Digital Sensor&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Mouser Part Numbers: &lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;CS (obsolete): 856-TSL2561CS&lt;/li&gt;
&lt;li&gt;DFN (cheapest): 856-TSL2561FN &lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="TSL2561"/>
</gates>
<devices>
<device name="CS" package="TSL2561_CS6">
<connects>
<connect gate="G$1" pin="3.3V" pad="VDD"/>
<connect gate="G$1" pin="ADDRSEL" pad="ADDR"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TSL2561_FN">
<connects>
<connect gate="G$1" pin="3.3V" pad="VDD"/>
<connect gate="G$1" pin="ADDRSEL" pad="ADR"/>
<connect gate="G$1" pin="GND" pad="VSS"/>
<connect gate="G$1" pin="INT" pad="INT"/>
<connect gate="G$1" pin="SCL" pad="CLK"/>
<connect gate="G$1" pin="SDA" pad="DATA"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STANDARDCONNECTOR" prefix="CN" uservalue="yes">
<description>Standard 20-Pin MCU Connector</description>
<gates>
<gate name="G$1" symbol="STANDARDCONNECTOR"/>
</gates>
<devices>
<device name="" package="STANDARDCONNECTOR">
<connects>
<connect gate="G$1" pin="ADC1" pad="11"/>
<connect gate="G$1" pin="ADC2" pad="12"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GPIO1" pad="13"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="17"/>
<connect gate="G$1" pin="GPIO6" pad="18"/>
<connect gate="G$1" pin="I2C_SCL" pad="5"/>
<connect gate="G$1" pin="I2C_SDA" pad="6"/>
<connect gate="G$1" pin="INT1" pad="7"/>
<connect gate="G$1" pin="INT2" pad="8"/>
<connect gate="G$1" pin="SPI_CLK" pad="2"/>
<connect gate="G$1" pin="SPI_CS" pad="1"/>
<connect gate="G$1" pin="SPI_MISO" pad="4"/>
<connect gate="G$1" pin="SPI_MOSI" pad="3"/>
<connect gate="G$1" pin="VCC3.3V" pad="19"/>
<connect gate="G$1" pin="VCC5.0V" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADP1712" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LDO Adj. Voltage Regulator 300mA&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;The ADP1712 voltage regulator is ideal for regulating battery or solar power due to it's very low foreward voltage drop (maximum 170mV at 300mA).&lt;/p&gt;
Forward Voltage Dropout: 170mV at 300mA&lt;br/&gt;
Input Voltage Range: 2.5V-5.5V&lt;br/&gt;
Output Voltage Range: 0.8V-5.0V
&lt;ul&gt;
&lt;li&gt;1.2V - Digikey: ADP1712AUJZ-1.2-R7CT-ND&lt;/li&gt;
&lt;li&gt;1.8V - Digikey: ADP1712AUJZ-1.8-R7CT-ND&lt;/li&gt;
&lt;li&gt;3.3V - Digikey: ADP1712AUJZ-3.3-R7CT-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ADP1712"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADP121" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LDO Fixed Voltage Regulator 150mA&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;The ADP121 voltage regulator is ideal for regulating battery or solar power due to it's very low foreward voltage drop (maximum 90mV at 150mA).&lt;/p&gt;
Forward Voltage Dropout: 90mV at 150mA&lt;br/&gt;
Input Voltage Range: 2.3V-5.5V&lt;br/&gt;
Output Voltage Range: 1.2V-3.3V (depending on model)
&lt;ul&gt;
&lt;li&gt;Digikey: 3.3V - ADP121-AUJZ33R7CT-ND&lt;/li&gt;
&lt;li&gt;Digikey: 3.0V - ADP121-AUJZ30R7CT-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ADP121"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHT_TPS851" prefix="U" uservalue="yes">
<description>&lt;p&gt;Toshiba TPS851 Illuminance Sensor&lt;/p&gt;
Digikey: TPS851CT-ND</description>
<gates>
<gate name="G$1" symbol="TPS851"/>
</gates>
<devices>
<device name="" package="TPS851">
<connects>
<connect gate="G$1" pin="AOUT" pad="AOUT"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP_LM75B" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LM75B I2C Temperature Sensor&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;The I2C-based LM75B can measure temperature between -55 and 125°C in 0.125°C increments (11-bit resolution).&lt;/p&gt;
&lt;p&gt;Digikey: 568-4768-1-ND&lt;/p&gt;
&lt;p&gt;For a 1.8V compatible part, look at the following pin and SW compatible parts:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;DS75LV - Mouser: 700-DS75LVS, Digikey: (TSSOP8) DS75LVU+-ND  (SOIC8) DS75LVS+-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LM75B"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OS" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OS" pad="3"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1754" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1754 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 microcontroller - 128 kB Flash, 32 kB SRAM, USB Device/Host/OTG, CAN, DAC, RTC &lt;/p&gt;
&lt;p&gt;Digikey: 568-4790-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1754"/>
</gates>
<devices>
<device name="" package="LQFP80">
<connects>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="37"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="39"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="40"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="47"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="48"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="46"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="45"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="38"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="44"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[29]/USB_DPLUS" pad="22"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="79"/>
<connect gate="G$1" pin="P0[30]/USB_DMIN" pad="23"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="80"/>
<connect gate="G$1" pin="P0[6]/SSEL1/MAT2[0]" pad="64"/>
<connect gate="G$1" pin="P0[7]/SCK1/MAT2[1]" pad="63"/>
<connect gate="G$1" pin="P0[8]/MISO1/MAT2[2]" pad="62"/>
<connect gate="G$1" pin="P0[9]/MOSI1/MAT2[3]" pad="61"/>
<connect gate="G$1" pin="P1[0]" pad="76"/>
<connect gate="G$1" pin="P1[10]" pad="71"/>
<connect gate="G$1" pin="P1[14]" pad="70"/>
<connect gate="G$1" pin="P1[15]" pad="69"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="25"/>
<connect gate="G$1" pin="P1[19]/MCOA0/USB_PPWR/CAP1[1]" pad="26"/>
<connect gate="G$1" pin="P1[1]" pad="75"/>
<connect gate="G$1" pin="P1[20]/MCI0/PWM1[2]/SCK0" pad="27"/>
<connect gate="G$1" pin="P1[22]/MCOB0/USB_PWRD/MAT1[0]" pad="28"/>
<connect gate="G$1" pin="P1[23]/MCI1/PWM1[4]/MISO0" pad="29"/>
<connect gate="G$1" pin="P1[24]/MCI2/PWM1[5]/MOSI0" pad="30"/>
<connect gate="G$1" pin="P1[25]/MCOA1/MAT1[1]" pad="31"/>
<connect gate="G$1" pin="P1[26]/MCOB1/PWM1[6]/CAP0[0]" pad="32"/>
<connect gate="G$1" pin="P1[28]/MCOA2/PCAP1[0]/MAT0[0]" pad="35"/>
<connect gate="G$1" pin="P1[29]/MCOB2/PCAP1[1]/MAT0[1]" pad="36"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="18"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="17"/>
<connect gate="G$1" pin="P1[4]" pad="74"/>
<connect gate="G$1" pin="P1[8]" pad="73"/>
<connect gate="G$1" pin="P1[9]" pad="72"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="60"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="41"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="59"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="58"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="55"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="54"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="53"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="52"/>
<connect gate="G$1" pin="P2[7]/RTS1" pad="51"/>
<connect gate="G$1" pin="P2[8]/TXD2" pad="50"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2" pad="49"/>
<connect gate="G$1" pin="P4[28]/MAT2[0]/TXD3" pad="65"/>
<connect gate="G$1" pin="P4[29]/MAT2[1]/RXD3" pad="68"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="RSTOUT" pad="11"/>
<connect gate="G$1" pin="RTCX1" pad="13"/>
<connect gate="G$1" pin="RTCX2" pad="15"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="16"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="21"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="42"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="56"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="77"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="34"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="67"/>
<connect gate="G$1" pin="VDDA" pad="8"/>
<connect gate="G$1" pin="VREFN" pad="12"/>
<connect gate="G$1" pin="VREFP" pad="10"/>
<connect gate="G$1" pin="VSS1" pad="24"/>
<connect gate="G$1" pin="VSS2" pad="33"/>
<connect gate="G$1" pin="VSS3" pad="43"/>
<connect gate="G$1" pin="VSS4" pad="57"/>
<connect gate="G$1" pin="VSS5" pad="66"/>
<connect gate="G$1" pin="VSS6" pad="78"/>
<connect gate="G$1" pin="VSSA" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP130T" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;MCP130T Voltage Supervisor (Active Low)&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Voltage supervisors will put the MCU in a reset state if the voltage drops below a pre-determined level.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SOT23-R/SOT23-W:&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Voltage Supervisor - 3.15V Active Low&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Note: Use the "Reflow" footprint when working with solder paste, and the "Wave" footprint when soldering by hand with a soldering iron (the latter has larger pads that are easier to solder by hand).&lt;/p&gt;
&lt;p&gt;Digikey: MCP130T-315I/TTCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP130T"/>
</gates>
<devices>
<device name="REFLOW" package="SOT23-R">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WAVE" package="SOT23-W">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB_PLCC6" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;RGB LED&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Cree CLV6A-FKB - Digikey: CLV6A-FKB-CK1P1G1BB7R3R3TR-ND&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;DC Foreward Current: 20mA&lt;/li&gt;
&lt;li&gt;Foreward Voltage: R = 2.0, G = 3.2, B = 3.2&lt;/li&gt;
&lt;li&gt;Viewing Angle: 120°&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LEDRGB_PLCC6"/>
</gates>
<devices>
<device name="CREE-CLV6A" package="RGBLED_PLCC6">
<connects>
<connect gate="G$1" pin="BGND" pad="1"/>
<connect gate="G$1" pin="BLUE" pad="6"/>
<connect gate="G$1" pin="GGND" pad="2"/>
<connect gate="G$1" pin="GRN" pad="5"/>
<connect gate="G$1" pin="RED" pad="4"/>
<connect gate="G$1" pin="RGND" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1313_QFP" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1313 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;Digikey: 568-4914-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1313FBD48"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/SCK" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="19"/>
<connect gate="G$1" pin="PIO2_5" pad="20"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0" pad="36"/>
<connect gate="G$1" pin="PIO3_1" pad="37"/>
<connect gate="G$1" pin="PIO3_2" pad="43"/>
<connect gate="G$1" pin="PIO3_3" pad="48"/>
<connect gate="G$1" pin="PIO3_4" pad="18"/>
<connect gate="G$1" pin="PIO3_5" pad="21"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="VDD(3V3)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="8"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="VSSIO" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1313_QFN" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1313 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;
&lt;p&gt;Digikey: 568-4913-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1313FHN33"/>
</gates>
<devices>
<device name="" package="HVQFN33-7X7">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="P$3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="P$8"/>
<connect gate="G$1" pin="PIO0_3" pad="P$9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="P$10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="P$11"/>
<connect gate="G$1" pin="PIO0_6/SCK" pad="P$15"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="P$16"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="P$17"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="P$18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="P$20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="P$27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="P$26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="P$30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="P$31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="P$32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="P$7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="P$12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="P$1"/>
<connect gate="G$1" pin="PIO3_2" pad="P$28"/>
<connect gate="G$1" pin="PIO3_4" pad="P$13"/>
<connect gate="G$1" pin="PIO3_5" pad="P$14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="P$2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="P$19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="P$25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="P$21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="P$23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="P$22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="P$24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="P$29"/>
<connect gate="G$1" pin="VDD(IO)" pad="P$6"/>
<connect gate="G$1" pin="VSS" pad="P$33"/>
<connect gate="G$1" pin="XTALIN" pad="P$4"/>
<connect gate="G$1" pin="XTALOUT" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1343_QFN" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1343 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 32 kB Flash, 8 kB SRAM, USB Device &lt;/p&gt;&lt;author&gt;MarcVl - Datasheet available on www.nxp.com&lt;/author&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1343FHN33"/>
</gates>
<devices>
<device name="" package="HVQFN33-7X7">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="P$3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="P$8"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="P$9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="P$10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="P$11"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK" pad="P$15"/>
<connect gate="G$1" pin="PIO0_7(20MA)/CTS" pad="P$16"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="P$17"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="P$18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="P$20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="P$27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="P$26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="P$30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="P$31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="P$32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="P$7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="P$12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="P$1"/>
<connect gate="G$1" pin="PIO3_2" pad="P$28"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="P$2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="P$19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="P$25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="P$21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="P$23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="P$22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="P$24"/>
<connect gate="G$1" pin="USB_DM" pad="P$13"/>
<connect gate="G$1" pin="USB_DP" pad="P$14"/>
<connect gate="G$1" pin="VDD(3V3)" pad="P$29"/>
<connect gate="G$1" pin="VDD(IO)" pad="P$6"/>
<connect gate="G$1" pin="VSS" pad="P$33"/>
<connect gate="G$1" pin="XTALIN" pad="P$4"/>
<connect gate="G$1" pin="XTALOUT" pad="P$5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY#" value="568-4944-ND"/>
<attribute name="MANF" value="NXP"/>
<attribute name="MANF#" value="LPC1343FHN33,551"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1343_QFP" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1343 &lt;/b&gt;&lt;p&gt;72 MHz 32-bit ARM Cortex-M3 microcontroller. 32 kB Flash, 8 kB SRAM, USB Device &lt;/p&gt;

&lt;p&gt;Mouser: 771-LPC1343FBD48151 &lt;br/&gt;
Digikey: 568-4945-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1343FBD48"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK" pad="22"/>
<connect gate="G$1" pin="PIO0_7(20MA)/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="18"/>
<connect gate="G$1" pin="PIO2_5" pad="21"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0" pad="36"/>
<connect gate="G$1" pin="PIO3_1" pad="37"/>
<connect gate="G$1" pin="PIO3_2" pad="43"/>
<connect gate="G$1" pin="PIO3_3" pad="48"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD(3V3)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="8"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="VSSIO" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY#" value="568-4945-ND"/>
<attribute name="MANF" value="NXP"/>
<attribute name="MANF#" value="LPC1343FBD48,151"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JTAG-CORTEXM3" prefix="JTAG" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Serial Wire (SW-DP) Connector&lt;/b&gt;&lt;/p&gt;
This standard 0.05" 10-pin connector is for use with the Cortex M0/M3's native SWD (serial wire debugger) interface (SW-DP).  Some boards support a 20-pin combined JTAG+SWD connector (SWJ-DP), such as the LPC1700 family, but many smaller devices only work with SWD which typically use the smaller 10-pin SW-DP connecter (the LPC1300 family, for example, only supports SWD).
&lt;p&gt;&lt;b&gt;2x05 1.27mm/0.05" Connector:&lt;/b&gt; This is the standard SMT connector defined by ARM for all Cortex devices, and should be used in most situations and for forward-compatibility since any new devices coming to market will likely use this connector.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;MOLEX 10 Pin 0.1" Connector:&lt;/b&gt; This 0.1" 10 pin connector has the same pin layout as the standard 0.05" connector, but is easier to work with if you are using standard jumper wires or custom cables to connect your SWD hardware.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;MOLEX 20 Pin 0.1" Connector:&lt;/b&gt; This 0.1" 20 pin connector is the same model used for ARM7/ARM9 JTAG debuggers, but is connected to match the pins on the Segger J-Link for ARM (which supports both JTAG and SWD debugging).&lt;/p&gt;
&lt;p&gt;See the following document from ARM for more information on Cortex M3 Debug Connectors: http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf&lt;br/&gt;And the following page for an overview with images of the different connector types: http://www.keil.com/peripherals/coresight/connectors.asp&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="JTAG-CORTEXM3"/>
</gates>
<devices>
<device name="" package="2X05_1.27MM_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MOLEX" package="CORTEXM3_SWD10_MOLEX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MOLEX20" package="JTAG-ARM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="15"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="9"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="13"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="17"/>
<connect gate="G$1" pin="9" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE" prefix="XB">
<description>&lt;b&gt;XBee (TM) /XBee-PRO(TM) OEM RF Modules&lt;/b&gt;&lt;p&gt;
Source: MaxStream, Inc. xbee_productmanual.pdf</description>
<gates>
<gate name="G$1" symbol="XBEE"/>
</gates>
<devices>
<device name="" package="XBEE">
<connects>
<connect gate="G$1" pin="!CTS!/DIO7" pad="12"/>
<connect gate="G$1" pin="!DTR!/SLEEP_RQ/DI8" pad="9"/>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!RTS!/AD6/DIO6" pad="16"/>
<connect gate="G$1" pin="AD0/DIO0" pad="20"/>
<connect gate="G$1" pin="AD1/DIO1" pad="19"/>
<connect gate="G$1" pin="AD2/DIO2" pad="18"/>
<connect gate="G$1" pin="ASSOC/AD5/DIO5" pad="15"/>
<connect gate="G$1" pin="CD/DOUT_EN/DO8" pad="4"/>
<connect gate="G$1" pin="COORD_SEL/AD3/DIO3" pad="17"/>
<connect gate="G$1" pin="DIN/!CONFIG" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="ON/!SLEEP" pad="13"/>
<connect gate="G$1" pin="PWM0/RSSI" pad="6"/>
<connect gate="G$1" pin="RF_TX/AD4/DIO4" pad="11"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PRO" package="XBEE-PRO">
<connects>
<connect gate="G$1" pin="!CTS!/DIO7" pad="12"/>
<connect gate="G$1" pin="!DTR!/SLEEP_RQ/DI8" pad="9"/>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!RTS!/AD6/DIO6" pad="16"/>
<connect gate="G$1" pin="AD0/DIO0" pad="20"/>
<connect gate="G$1" pin="AD1/DIO1" pad="19"/>
<connect gate="G$1" pin="AD2/DIO2" pad="18"/>
<connect gate="G$1" pin="ASSOC/AD5/DIO5" pad="15"/>
<connect gate="G$1" pin="CD/DOUT_EN/DO8" pad="4"/>
<connect gate="G$1" pin="COORD_SEL/AD3/DIO3" pad="17"/>
<connect gate="G$1" pin="DIN/!CONFIG" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="ON/!SLEEP" pad="13"/>
<connect gate="G$1" pin="PWM0/RSSI" pad="6"/>
<connect gate="G$1" pin="RF_TX/AD4/DIO4" pad="11"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6364" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;MAX6364 - Low Power Voltage Supervisor (3.08V) with Battery Backup&lt;/&lt;b&gt;&lt;/p&gt;
&lt;p&gt;This 'battery backup supervisor' will supply up to 150mA of current from VCC.  If VCC ever drops below the 3.08V threshold, the supervisor will automatically switch the power supply to battery power, allowing you to safely 'fall-back' on a secondary power source for critical applications, or where you know that the main power suppy is inherently volatile (solar panels, etc.)&lt;/p&gt;
&lt;p&gt;Digikey: MAX6364LUT31+TCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX6364"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="BATT" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="RSTIN" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY" prefix="B" uservalue="yes">
<description>&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;CR1220 SMT&lt;/b&gt; - Digikey: 3001K-ND&lt;/li&gt;
&lt;/ul&gt;

&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="" package="JSTPH2">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR2032" package="CR2032">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SH2" package="JSTSH2">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR1220_SMT" package="CR1220">
<connects>
<connect gate="G$1" pin="+" pad="+$1"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PH2_NOTHERMALS" package="JSTPH2_NOTHERMALS">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDCARD" prefix="CN" uservalue="yes">
<description>&lt;b&gt;SD Card Reader&lt;/b&gt;
&lt;p&gt;06132 = Inexpensive SMT&lt;/p&gt;
&lt;p&gt;19646 = Push/Pull SMT&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SDCARD"/>
</gates>
<devices>
<device name="" package="SDCARD_SMT_4U06132">
<connects>
<connect gate="G$1" pin="CARDDETECT" pad="CD"/>
<connect gate="G$1" pin="CLK/SCK" pad="5"/>
<connect gate="G$1" pin="CMD/MOSI" pad="2"/>
<connect gate="G$1" pin="DATA0/MISO" pad="7"/>
<connect gate="G$1" pin="DATA1" pad="8"/>
<connect gate="G$1" pin="DATA2" pad="9"/>
<connect gate="G$1" pin="DATA3/CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WRITEPROTECT" pad="WP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="19646" package="SDCARD_SMT_4U19646">
<connects>
<connect gate="G$1" pin="CARDDETECT" pad="CD"/>
<connect gate="G$1" pin="CLK/SCK" pad="P$5"/>
<connect gate="G$1" pin="CMD/MOSI" pad="P$2"/>
<connect gate="G$1" pin="DATA0/MISO" pad="P$7"/>
<connect gate="G$1" pin="DATA1" pad="P$8"/>
<connect gate="G$1" pin="DATA2" pad="P$9"/>
<connect gate="G$1" pin="DATA3/CS" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="GND@2"/>
<connect gate="G$1" pin="VDD" pad="P$4"/>
<connect gate="G$1" pin="VSS1" pad="P$3"/>
<connect gate="G$1" pin="VSS2" pad="P$6"/>
<connect gate="G$1" pin="WRITEPROTECT" pad="WP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME_A3" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A3, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="FRAME_A3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP1400A_STEPUP" prefix="U" uservalue="yes">
<description>&lt;b&gt;NCP1400A - 100mA PWM Step-Up Regulator&lt;/b&gt;
&lt;p&gt;100mA step-up DC-to-DC converter with low 0.8V startup.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;3.3V Version (SOT23-5) - Digikey: NCP1400ASN33T1GOSCT-ND&lt;/li&gt;
&lt;li&gt;5.0V Version (SOT23-5) - Digikey: NCP1400ASN50T1GOSCT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;NCP1402 - 200mA PWM Step-Up Regulator&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;200mA step-up DC-to-DC converter with low 0.8V startup&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;3.3V Version (SOT23-5) - Digikey: NCP1402SN33T1GOSCT-ND&lt;/li&gt;
&lt;li&gt;5.0V Version (SOT23-5) - Digikey: NCP1402SN50T1GOSCT-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="NCP1400A"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_SOT23-6_DUAL" prefix="U" uservalue="yes">
<description>&lt;b&gt;Dual Output SOT23-6 Linear Regulators&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;Diodes Inc. AP7312 - Dual 150mA LDO Linear Regulator&lt;/b&gt;
&lt;p&gt;0.2V dropout, 150mA output, 2-6V Input&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;AP7312-1833W6-7&lt;/b&gt; - 1.8V/3.3V SOT23-6 (Digikey: AP7312-1833W6-7DICT-ND)&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;

&lt;p&gt;
&lt;b&gt;MIC5320 - Dual 150mA ULDO Linear Regulator&lt;/b&gt;
&lt;p&gt;Ultra-low 35mV dropout at 150mA, 2.3-5.5V Input&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;3.3V/1.8V SOT23-6 (Digikey: 576-1658-1-ND)&lt;/li&gt;
&lt;li&gt;3.3V/1.5V SOT23-6 (Digikey: 576-3483-1-ND)&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MIC5320"/>
</gates>
<devices>
<device name="MIC5320" package="SOT23-6">
<connects>
<connect gate="G$1" pin="EN1" pad="6"/>
<connect gate="G$1" pin="EN2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT1" pad="4"/>
<connect gate="G$1" pin="VOUT2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AP7312" package="SOT23-6">
<connects>
<connect gate="G$1" pin="EN1" pad="4"/>
<connect gate="G$1" pin="EN2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VOUT1" pad="6"/>
<connect gate="G$1" pin="VOUT2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>&lt;b&gt;Inductors&lt;/b&gt;
&lt;p&gt;0603:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;10nH Ceramic Inductor - microwire antenna/RF (Digikey: 712-1434-2-ND)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;0805:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;560nH Ceramic Inductor - RF (Digikey: 553-1047-1-ND)&lt;/li&gt;
&lt;li&gt;270nH Ceramic Inductor - Q = 40@250MHz, +-5%, 1 Ohm DC Resistance (Digikey: 535-10506-2-ND)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;1007 (2518 Metric) SMT:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;10µH 10% 250mOhm 820mA 1007 Inductor (Digikey: 587-2189-1-ND)&lt;/li&gt;
&lt;li&gt;22µH 10% 500mOhm 580mA 1007 Inductor (Digikey: 587-2190-1-ND)&lt;/li&gt;
&lt;li&gt;47µH 10% 950mOhm 420mA 1007 Inductor (Digikey: 587-2191-1-ND)&lt;/li&gt;
&lt;li&gt;47µH 5% 100mOhm 1A 1008 Inductor (Digikey: 732-1816-1-ND)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;5.0x5.0mm (Taiyo Yuden NR5040 Series)&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;6.8µH 20% 2.3A 64mOhm Inductor (Digikey: 587-2374-2-ND)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;5.0x5.0mm (TDK VLC5045 Series)&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;4.7µH 20% 3.3A 34mOhm Inductor (Digikey: 445-6526-1-ND)&lt;/li&gt;
&lt;li&gt;6.8µH 20% 2.7A 46mOhm Inductor (Digikey: 445-6527-1-ND)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;6.0x6.0mm (TDK VLC6045 Series)&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;4.7µH 20% 3.8A 27mOhm Inductor (Digikey: 445-6538-2-ND)&lt;/li&gt;
&lt;li&gt;6.8µH 20% 3A 41mOhm Inductor (Digikey: 445-6540-1-ND)&lt;/li&gt;
&lt;li&gt;6.2µH 30% 2.2A 45mOhm Inductor (Digikey: SRR5028-6R2YCT-ND) - Not TDK VLC6045 but footprint should match&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;6.0x6.0mm (TDK SLF6045 Series)&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;6.8uH 30% 2A 33mOhm Inductor (Digikey: 445-4572-1-ND, Mouser: 810-SLF645T6R8N2R0PF)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="INDUCTOR_1007">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TDK_VLC6045" package="INDUCTOR_6X6MM_TDK_VLC6045">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TDK_SLF6045" package="INDUCTOR_6X6MM_TDK_SLF6045">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TDK_VLC5045" package="INDUCTOR_5X5MM_TDK_VLC5045">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TDK_VLC5045_NOTHERM" package="INDUCTOR_5X5MM_TDK_VLC5045_NOTHERMALS">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NR5040" package="INDUCTOR_5X5MM_NR5040_NOTHERMALS">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402" package="_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402MP" package="_0402MP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603" package="_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603MP" package="_0603MP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805MP" package="_0805MP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BAT54C" prefix="D" uservalue="yes">
<description>&lt;p&gt;BAT54C Schottky Diodes (Common Cathode)&lt;/p&gt;
&lt;p&gt;Vf: 800mV, 30V 200mA&lt;br/&gt;
Digikey: BAT54CFSCT-ND&lt;/p&gt;
&lt;p&gt;For 300mA see BAT54CFILM:&lt;br/&gt;
Vf: 900mV, 40V 300mA&lt;br/&gt;
Digkey: 497-3786-2-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BAT54C"/>
</gates>
<devices>
<device name="" package="SOT23-R">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1113/4" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LPC1113/4 MCU&lt;/b&gt;&lt;br/&gt; QFP48 Package&lt;/p&gt;
&lt;p&gt;ARM Cortex M0, 50MHz Operation, 8 Channel 10-Bit ADC, 1²C, 2xSPI, UART, 2x16 Bit and 2x32 Bit Timers, Internal 12MHz Oscillator, 1.8-3.6V operation.&lt;/p&gt;
&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;
&lt;td width="50"&gt;&lt;b&gt;Model&lt;/b&gt;&lt;/td&gt;
&lt;td width="40"&gt;&lt;b&gt;Flash&lt;/b&gt;&lt;/td&gt;
&lt;td width="40"&gt;&lt;b&gt;SRAM&lt;/b&gt;&lt;/td&gt;
&lt;td width="100"&gt;&lt;b&gt;Part N°:&lt;/b&gt;&lt;/td&gt;
&lt;td width="100"&gt;&lt;b&gt;Digikey&lt;/b&gt;&lt;/td&gt;
&lt;td width="125"&gt;&lt;b&gt;Mouser&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td&gt;LPC1113&lt;/td&gt;
&lt;td&gt;24KB&lt;/td&gt;
&lt;td&gt;8KB&lt;/td&gt;
&lt;td&gt;LPC1113FBD48/301&lt;/td&gt;
&lt;td&gt;TBD&lt;/td&gt;
&lt;td&gt;TBD&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td&gt;LPC1114&lt;/td&gt;
&lt;td&gt;32KB&lt;/td&gt;
&lt;td&gt;8KB&lt;/td&gt;
&lt;td&gt;LPC1114FBD48/301&lt;/td&gt;
&lt;td&gt;568-4950-ND&lt;/td&gt;
&lt;td&gt;771-LPC1114FBD483011 &lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114_QFP"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK0" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="19"/>
<connect gate="G$1" pin="PIO2_5" pad="20"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0/DTR" pad="36"/>
<connect gate="G$1" pin="PIO3_1/DSR" pad="37"/>
<connect gate="G$1" pin="PIO3_2/DCD" pad="43"/>
<connect gate="G$1" pin="PIO3_3/RI" pad="48"/>
<connect gate="G$1" pin="PIO3_4" pad="18"/>
<connect gate="G$1" pin="PIO3_5" pad="21"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="VDD(3.3V)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="8"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="VSS(IO)" pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY#" value="568-4950-ND"/>
<attribute name="MANF" value="NXP"/>
<attribute name="MANF#" value="LPC1114FBD48/301,1"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTC" prefix="PTC" uservalue="yes">
<description>&lt;b&gt;PTC (Resettable Fuse)&lt;/b&gt;
&lt;p&gt;&lt;b&gt;1206 Package&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;250mA PTC (16V Max, Time-to-Trip: 0.08s) - Digikey: F2110CT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;1210 Package&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;100mA PTC (30V Max, Time-to-Trip: 0.6s) - Digikey: MF-USMF010-2CT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;1812 Package&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;750mA PTC (24V Max, Time-to-Trip: 0.2s) - Digikey: MF-MSMF075/24-2CT-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PTC"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="PTC1210">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1812" package="PTC1812">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.8V">
<description>&lt;b&gt;2.8V Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="2.8V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VDD">
<description>&lt;b&gt;VDD Supply Symbol&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="VDD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X20" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD20"/>
</gates>
<devices>
<device name="ROUND" package="1X20_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDRAM_54TSOP" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;64Mb SDRAM (4Mb x 16)&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;Micron:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;MT48LC4M16A2P-7E:G TR - 133 MHz, 3V-3.6V, 0-70C - Digikey: 557-1089-1-ND&lt;/li&gt;
&lt;li&gt;MT48LC4M16A2P-75 IT:G TR - 133 MHz, 3V-3.6V, -40-85C - Digikey: 557-1087-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;ISSI (cheaper):&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;IS42S16400F-7TL - 143 MHz, 3V-3.6V, 0-70C - Digikey: 706-1077-ND&lt;/li&gt;
&lt;li&gt;IS42S16400J-7TLI - 143 MHz, 3V-3.6V, -40-85C - Digikey: 706-1132-ND&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;b&gt;256Mb SDRAM (16Mb x 16)&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;MT48LC16M16A2TG-7E IT:D TR - 133MHz, 3V-3.6V, -40-85C - Digikey: 557-1064-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MT48LC4M16A2P"/>
</gates>
<devices>
<device name="" package="TSOP54-400">
<connects>
<connect gate="G$1" pin="A0" pad="23"/>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="A10" pad="22"/>
<connect gate="G$1" pin="A11" pad="35"/>
<connect gate="G$1" pin="A2" pad="25"/>
<connect gate="G$1" pin="A3" pad="26"/>
<connect gate="G$1" pin="A4" pad="29"/>
<connect gate="G$1" pin="A5" pad="30"/>
<connect gate="G$1" pin="A6" pad="31"/>
<connect gate="G$1" pin="A7" pad="32"/>
<connect gate="G$1" pin="A8" pad="33"/>
<connect gate="G$1" pin="A9" pad="34"/>
<connect gate="G$1" pin="BA0" pad="20"/>
<connect gate="G$1" pin="BA1" pad="21"/>
<connect gate="G$1" pin="CAS" pad="17"/>
<connect gate="G$1" pin="CKE" pad="37"/>
<connect gate="G$1" pin="CLK" pad="38"/>
<connect gate="G$1" pin="CS" pad="19"/>
<connect gate="G$1" pin="DQ0" pad="2"/>
<connect gate="G$1" pin="DQ1" pad="4"/>
<connect gate="G$1" pin="DQ10" pad="45"/>
<connect gate="G$1" pin="DQ11" pad="47"/>
<connect gate="G$1" pin="DQ12" pad="48"/>
<connect gate="G$1" pin="DQ13" pad="50"/>
<connect gate="G$1" pin="DQ14" pad="51"/>
<connect gate="G$1" pin="DQ15" pad="53"/>
<connect gate="G$1" pin="DQ2" pad="5"/>
<connect gate="G$1" pin="DQ3" pad="7"/>
<connect gate="G$1" pin="DQ4" pad="8"/>
<connect gate="G$1" pin="DQ5" pad="10"/>
<connect gate="G$1" pin="DQ6" pad="11"/>
<connect gate="G$1" pin="DQ7" pad="13"/>
<connect gate="G$1" pin="DQ8" pad="42"/>
<connect gate="G$1" pin="DQ9" pad="44"/>
<connect gate="G$1" pin="DQMH" pad="39"/>
<connect gate="G$1" pin="DQML" pad="15"/>
<connect gate="G$1" pin="NC1" pad="36"/>
<connect gate="G$1" pin="NC2" pad="40"/>
<connect gate="G$1" pin="RAS" pad="18"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="14"/>
<connect gate="G$1" pin="VDD3" pad="27"/>
<connect gate="G$1" pin="VDDQ1" pad="3"/>
<connect gate="G$1" pin="VDDQ2" pad="9"/>
<connect gate="G$1" pin="VDDQ3" pad="43"/>
<connect gate="G$1" pin="VDDQ4" pad="49"/>
<connect gate="G$1" pin="VSS1" pad="28"/>
<connect gate="G$1" pin="VSS2" pad="41"/>
<connect gate="G$1" pin="VSS3" pad="54"/>
<connect gate="G$1" pin="VSSQ1" pad="6"/>
<connect gate="G$1" pin="VSSQ2" pad="12"/>
<connect gate="G$1" pin="VSSQ3" pad="46"/>
<connect gate="G$1" pin="VSSQ4" pad="52"/>
<connect gate="G$1" pin="WE" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2478" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LPC2470/2478&lt;/b&gt; - ARM7TDMI-S 72MHz MCU&lt;/p&gt;
&lt;p&gt;Single-chip 16-bit/32-bit micro; 512 kB flash, Ethernet, CAN,
LCD, USB 2.0 device/host/OTG, external memory interface&lt;/p&gt;
&lt;p&gt;Digikey: 568-4363-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC2478"/>
</gates>
<devices>
<device name="" package="LQFP208">
<connects>
<connect gate="G$1" pin="ALARM" pad="37"/>
<connect gate="G$1" pin="DBGEN" pad="9"/>
<connect gate="G$1" pin="NC1" pad="30"/>
<connect gate="G$1" pin="NC2" pad="117"/>
<connect gate="G$1" pin="NC3" pad="141"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="94"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="98"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="100"/>
<connect gate="G$1" pin="P0[12]/USB_PPWR2/MISO1/AD0[6]" pad="41"/>
<connect gate="G$1" pin="P0[13]/USB_UP_LED2/MOSI1/AD0[7]" pad="45"/>
<connect gate="G$1" pin="P0[14]/USB_HSTEN2/USB_CONNECT2/SSEL1" pad="69"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="128"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="130"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="126"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="124"/>
<connect gate="G$1" pin="P0[19]/DSR1/MCICLK/SDA1" pad="122"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="96"/>
<connect gate="G$1" pin="P0[20]/DTR1/MCICMD/SCL1" pad="120"/>
<connect gate="G$1" pin="P0[21]/RI1/MCIPWR/RD1" pad="118"/>
<connect gate="G$1" pin="P0[22]/RTS1/MCIDAT0/TD1" pad="116"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="18"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="16"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="14"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="12"/>
<connect gate="G$1" pin="P0[27]/SDA0" pad="50"/>
<connect gate="G$1" pin="P0[28]/SCL0" pad="48"/>
<connect gate="G$1" pin="P0[29]/USB_D+1" pad="61"/>
<connect gate="G$1" pin="P0[2]/TXD0" pad="202"/>
<connect gate="G$1" pin="P0[30]/USB_D-1" pad="62"/>
<connect gate="G$1" pin="P0[31]/USB_D+2" pad="51"/>
<connect gate="G$1" pin="P0[3]/RXD0" pad="204"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/LCDVD[0]/RD2/CAP2[0]" pad="168"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/LCDVD[1]/TD2/CAP2[1]" pad="166"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/LCDVD[8]/SSEL1/MAT2[0]" pad="164"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/LCDVD[9]/SCK1/MAT2[1]" pad="162"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/LCDVD[16]/MISO1/MAT2[2]" pad="160"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/LCDVD[17]/MOSI1/MAT2[3]" pad="158"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="196"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="186"/>
<connect gate="G$1" pin="P1[11]/ENET_RXD2/MCIDAT2/PWM0[6]" pad="163"/>
<connect gate="G$1" pin="P1[12]/ENET_RXD3/MCIDAT3/PCAP0[0]" pad="157"/>
<connect gate="G$1" pin="P1[13]/ENET_RX_DV" pad="147"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="184"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK/ENET_RX_CLK" pad="182"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="180"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="178"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED1/PWM1[1]/CAP1[0]" pad="66"/>
<connect gate="G$1" pin="P1[19]/USB_TX_E1/USB_PPWR1/CAP1[1]" pad="68"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="194"/>
<connect gate="G$1" pin="P1[20]/USB_TX_DP1/LCDVD[6]/LCDVD[10]/PWM1[2]/SCK0" pad="70"/>
<connect gate="G$1" pin="P1[21]/USB_TX_DM1/LCDVD[7]/LCDVD[11]/PWM1[3]/SSEL0" pad="72"/>
<connect gate="G$1" pin="P1[22]/USB_RCV1/LCDVD[8]/LCDVD[12]/USB_PWRD1/MAT1[0]" pad="74"/>
<connect gate="G$1" pin="P1[23]/USB_RX_DP1/LCDVD[9]/LCDVD[13]/PWM1[4]/MISO0" pad="76"/>
<connect gate="G$1" pin="P1[24]/USB_RX_DM1/LCDVD[10]/LCDVD[14]/PWM1[5]/MOSI0" pad="78"/>
<connect gate="G$1" pin="P1[25]/USB_LS1/LCDVD[11]/LCDVD[15]/USB_HSTEN1/MAT1[1]" pad="80"/>
<connect gate="G$1" pin="P1[26]/USB_SSPND1/LCDVD[12]/LCDVD[20]/PWM1[6]/CAP0[0]" pad="82"/>
<connect gate="G$1" pin="P1[27]/USB_INT1/LCDVD[13]/LCDVD[21]/USB_OVRCR1/CAP0[1]" pad="88"/>
<connect gate="G$1" pin="P1[28]/USB_SCL1/LCDVD[14]/LCDVD[22]/PCAP1[0]/MAT0[0]" pad="90"/>
<connect gate="G$1" pin="P1[29]/USB_SDA1/LCDVD[15]/LCDVD[23]/PCAP1[1]/MAT0[1]" pad="92"/>
<connect gate="G$1" pin="P1[2]/ENET_TXD2/MCICLK/PWM0[1]" pad="185"/>
<connect gate="G$1" pin="P1[30]/USB_PWRD2/VBUS/AD0[4]" pad="42"/>
<connect gate="G$1" pin="P1[31]/USB_OVRCR2/SCK1/AD0[5]" pad="40"/>
<connect gate="G$1" pin="P1[3]/ENET_TXD3/MCICMD/PWM0[2]" pad="177"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="192"/>
<connect gate="G$1" pin="P1[5]/ENET_TX_ER/MCIPWR/PWM0[3]" pad="156"/>
<connect gate="G$1" pin="P1[6]/ENET_TX_CLK/MCIDAT0/PWM0[4]" pad="171"/>
<connect gate="G$1" pin="P1[7]/ENET_COL/MCIDAT1/PWM0[5]" pad="153"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS_DV/ENET_CRS" pad="190"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="188"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1/TRACECLK/LCDPWR" pad="154"/>
<connect gate="G$1" pin="P2[10]/EINT0" pad="110"/>
<connect gate="G$1" pin="P2[11]/EINT1/LCDCLKIN/MCIDAT1/I2STX_CLK" pad="108"/>
<connect gate="G$1" pin="P2[12]/EINT2/LCDVD[4]/LCDVD[3]/LCDVD[8]/LCDVD[18]/MCIDAT2/I2STX_WS" pad="106"/>
<connect gate="G$1" pin="P2[13]/EINT3/LCDVD[5]/LCDVD[9]/LCDVD[19]/MCIDAT3/I2STX_SDA" pad="102"/>
<connect gate="G$1" pin="P2[14]/CS2/CAP2[0]/SDA1" pad="91"/>
<connect gate="G$1" pin="P2[15]/CS3/CAP2[1]/SCL1" pad="99"/>
<connect gate="G$1" pin="P2[16]/CAS" pad="87"/>
<connect gate="G$1" pin="P2[17]/RAS" pad="95"/>
<connect gate="G$1" pin="P2[18]/CLKOUT0" pad="59"/>
<connect gate="G$1" pin="P2[19]/CLKOUT1" pad="67"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1/PIPESTAT0/LCDLE" pad="152"/>
<connect gate="G$1" pin="P2[20]/DYCS0" pad="73"/>
<connect gate="G$1" pin="P2[21]/DYCS1" pad="81"/>
<connect gate="G$1" pin="P2[22]/DYCS2/CAP3[0]/SCK0" pad="85"/>
<connect gate="G$1" pin="P2[23]/DYCS3/CAP3[1]/SSEL0" pad="64"/>
<connect gate="G$1" pin="P2[24]/CKEOUT0" pad="53"/>
<connect gate="G$1" pin="P2[25]/CKEOUT1" pad="54"/>
<connect gate="G$1" pin="P2[26]/CKEOUT2/MAT3[0]/MISO0" pad="57"/>
<connect gate="G$1" pin="P2[27]/CKEOUT3/MAT3[1]/MOSI0" pad="47"/>
<connect gate="G$1" pin="P2[28]/DQMOUT0" pad="49"/>
<connect gate="G$1" pin="P2[29]/DQMOUT1" pad="43"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/PIPESTAT1/LCDDCLK" pad="150"/>
<connect gate="G$1" pin="P2[30]/DQMOUT2/MAT3[2]/SDA2" pad="31"/>
<connect gate="G$1" pin="P2[31]/DQMOUT3/MAT3[3]/SCL2" pad="39"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/PIPESTAT2/LCDFP" pad="144"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACESYNC/LCDENAB/LCDM" pad="142"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEPKT0/LCDLP" pad="140"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACEPKT1/LCDVD[0]/LCDVD[4]" pad="138"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1/TRACEPKT2/LCDVD[1]/LCDVD[5]" pad="136"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2/TRACEPKT3/LCDVD[2]/LCDVD[6]" pad="134"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT1/RXD2/EXTIN0/LCDVD[3]/LCDVD[7]" pad="132"/>
<connect gate="G$1" pin="P3[0]/D0" pad="197"/>
<connect gate="G$1" pin="P3[10]/D10" pad="205"/>
<connect gate="G$1" pin="P3[11]/D11" pad="208"/>
<connect gate="G$1" pin="P3[12]/D12" pad="1"/>
<connect gate="G$1" pin="P3[13]/D13" pad="7"/>
<connect gate="G$1" pin="P3[14]/D14" pad="21"/>
<connect gate="G$1" pin="P3[15]/D15" pad="28"/>
<connect gate="G$1" pin="P3[16]/D16/PWM0[1]/TXD1" pad="137"/>
<connect gate="G$1" pin="P3[17]/D17/PWM0[2]/RXD1" pad="143"/>
<connect gate="G$1" pin="P3[18]/D18/PWM0[3]/CTS1" pad="151"/>
<connect gate="G$1" pin="P3[19]/D19/PWM0[4]/DCD1" pad="161"/>
<connect gate="G$1" pin="P3[1]/D1" pad="201"/>
<connect gate="G$1" pin="P3[20]/D20/PWM0[5]/DSR1" pad="167"/>
<connect gate="G$1" pin="P3[21]/D21/PWM0[6]/DTR1" pad="175"/>
<connect gate="G$1" pin="P3[22]/D22/PCAP0[0]/RI1" pad="195"/>
<connect gate="G$1" pin="P3[23]/D23/CAP0[0]/PCAP1[0]" pad="65"/>
<connect gate="G$1" pin="P3[24]/D24/CAP0[1]/PWM1[1]" pad="58"/>
<connect gate="G$1" pin="P3[25]/D25/MAT0[0]/PWM1[2]" pad="56"/>
<connect gate="G$1" pin="P3[26]/D26/MAT0[1]/PWM1[3]" pad="55"/>
<connect gate="G$1" pin="P3[27]/D27/CAP1[0]/PWM1[4]" pad="203"/>
<connect gate="G$1" pin="P3[28]/D28/CAP1[1]/PWM1[5]" pad="5"/>
<connect gate="G$1" pin="P3[29]/D29/MAT1[0]/PWM1[6]" pad="11"/>
<connect gate="G$1" pin="P3[2]/D2" pad="207"/>
<connect gate="G$1" pin="P3[30]/D30/MAT1[1]/RTS1" pad="19"/>
<connect gate="G$1" pin="P3[31]/D31/MAT1[2]" pad="25"/>
<connect gate="G$1" pin="P3[3]/D3" pad="3"/>
<connect gate="G$1" pin="P3[4]/D4" pad="13"/>
<connect gate="G$1" pin="P3[5]/D5" pad="17"/>
<connect gate="G$1" pin="P3[6]/D6" pad="23"/>
<connect gate="G$1" pin="P3[7]/D7" pad="27"/>
<connect gate="G$1" pin="P3[8]/D8" pad="191"/>
<connect gate="G$1" pin="P3[9]/D9" pad="199"/>
<connect gate="G$1" pin="P4[0]/A0" pad="75"/>
<connect gate="G$1" pin="P4[10]/A10" pad="135"/>
<connect gate="G$1" pin="P4[11]/A11" pad="145"/>
<connect gate="G$1" pin="P4[12]/A12" pad="149"/>
<connect gate="G$1" pin="P4[13]/A13" pad="155"/>
<connect gate="G$1" pin="P4[14]/A14" pad="159"/>
<connect gate="G$1" pin="P4[15]/A15" pad="173"/>
<connect gate="G$1" pin="P4[16]/A16" pad="101"/>
<connect gate="G$1" pin="P4[17]/A17" pad="104"/>
<connect gate="G$1" pin="P4[18]/A18" pad="105"/>
<connect gate="G$1" pin="P4[19]/A19" pad="111"/>
<connect gate="G$1" pin="P4[1]/A1" pad="79"/>
<connect gate="G$1" pin="P4[20]/A20/SDA2/SCK1" pad="109"/>
<connect gate="G$1" pin="P4[21]/A21/SCL2/SSEL1" pad="115"/>
<connect gate="G$1" pin="P4[22]/A22/TXD2/MISO1" pad="123"/>
<connect gate="G$1" pin="P4[23]/A23/RXD2/MOSI1" pad="129"/>
<connect gate="G$1" pin="P4[24]/OE" pad="183"/>
<connect gate="G$1" pin="P4[25]/WE" pad="179"/>
<connect gate="G$1" pin="P4[26]/BLS0" pad="119"/>
<connect gate="G$1" pin="P4[27]/BLS1" pad="139"/>
<connect gate="G$1" pin="P4[28]/BLS2/MAT2[0]/LCDVD[6]/LCDVD[10]/LCDVD[2]/TXD3" pad="170"/>
<connect gate="G$1" pin="P4[29]/BLS3/MAT2[1]LCDVD[7]/LCDVD[11]/LCDVD[3]/RXD3" pad="176"/>
<connect gate="G$1" pin="P4[2]/A2" pad="83"/>
<connect gate="G$1" pin="P4[30]/CS0" pad="187"/>
<connect gate="G$1" pin="P4[31]/CS1" pad="193"/>
<connect gate="G$1" pin="P4[3]/A3" pad="97"/>
<connect gate="G$1" pin="P4[4]/A4" pad="103"/>
<connect gate="G$1" pin="P4[5]/A5" pad="107"/>
<connect gate="G$1" pin="P4[6]/A6" pad="113"/>
<connect gate="G$1" pin="P4[7]/A7" pad="121"/>
<connect gate="G$1" pin="P4[8]/A8" pad="127"/>
<connect gate="G$1" pin="P4[9]/A9" pad="131"/>
<connect gate="G$1" pin="RESET" pad="35"/>
<connect gate="G$1" pin="RSTOUT" pad="29"/>
<connect gate="G$1" pin="RTCK" pad="206"/>
<connect gate="G$1" pin="RTCX1" pad="34"/>
<connect gate="G$1" pin="RTCX2" pad="36"/>
<connect gate="G$1" pin="TCK" pad="10"/>
<connect gate="G$1" pin="TDI" pad="4"/>
<connect gate="G$1" pin="TDO" pad="2"/>
<connect gate="G$1" pin="TMS" pad="6"/>
<connect gate="G$1" pin="TRST" pad="8"/>
<connect gate="G$1" pin="USB_D-2" pad="52"/>
<connect gate="G$1" pin="VBAT" pad="38"/>
<connect gate="G$1" pin="VDD(DCDC)1" pad="26"/>
<connect gate="G$1" pin="VDD(DCDC)2" pad="86"/>
<connect gate="G$1" pin="VDD(DCDC)3" pad="174"/>
<connect gate="G$1" pin="VDD1" pad="15"/>
<connect gate="G$1" pin="VDD10" pad="198"/>
<connect gate="G$1" pin="VDD2" pad="60"/>
<connect gate="G$1" pin="VDD3" pad="71"/>
<connect gate="G$1" pin="VDD4" pad="89"/>
<connect gate="G$1" pin="VDD5" pad="112"/>
<connect gate="G$1" pin="VDD6" pad="125"/>
<connect gate="G$1" pin="VDD7" pad="146"/>
<connect gate="G$1" pin="VDD8" pad="165"/>
<connect gate="G$1" pin="VDD9" pad="181"/>
<connect gate="G$1" pin="VDDA" pad="20"/>
<connect gate="G$1" pin="VREF" pad="24"/>
<connect gate="G$1" pin="VSS(CORE)1" pad="32"/>
<connect gate="G$1" pin="VSS(CORE)2" pad="84"/>
<connect gate="G$1" pin="VSS(CORE)3" pad="172"/>
<connect gate="G$1" pin="VSS(IO)1" pad="33"/>
<connect gate="G$1" pin="VSS(IO)10" pad="200"/>
<connect gate="G$1" pin="VSS(IO)2" pad="63"/>
<connect gate="G$1" pin="VSS(IO)3" pad="77"/>
<connect gate="G$1" pin="VSS(IO)4" pad="93"/>
<connect gate="G$1" pin="VSS(IO)5" pad="114"/>
<connect gate="G$1" pin="VSS(IO)6" pad="133"/>
<connect gate="G$1" pin="VSS(IO)7" pad="148"/>
<connect gate="G$1" pin="VSS(IO)8" pad="169"/>
<connect gate="G$1" pin="VSS(IO)9" pad="189"/>
<connect gate="G$1" pin="VSSA" pad="22"/>
<connect gate="G$1" pin="XTAL1" pad="44"/>
<connect gate="G$1" pin="XTAL2" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME_A3P" prefix="FRAME" uservalue="yes">
<description>A3 Portrait</description>
<gates>
<gate name="G$1" symbol="FRAME_A3P"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1698" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;MX1698/MAX1698A&lt;/b&gt; - Step-Up Current Regulator for LEDs&lt;/p&gt;
&lt;p&gt;Digikey: MAX1698EUB+-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX1698"/>
</gates>
<devices>
<device name="" package="UMAX10">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="EXT" pad="10"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="SHDN" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;RJ45 (Ethernet) Connectors&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;J0026D21BNL&lt;/b&gt; - RJ45 Connector with internal transformer and 2 LEDs (Yellow/Green).  LEDs have max foreward-voltage of 2.5V.  LEDs require an external resistor.  Digikey: 553-1349-ND&lt;/p&gt;
&lt;p&gt;&lt;b&gt;J00-0065NL&lt;/b&gt; - RJ45 Connector with internal transformer and 2 LEDs (Yellow/Green).  LEDs have max foreward-voltage of 2.5V.  LEDs require an external resistor.  Digikey: 553-1345-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RJ45_LEDS"/>
</gates>
<devices>
<device name="J0026D21BNL" package="RJ45_PULSEJACK">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="LED1_A" pad="9"/>
<connect gate="G$1" pin="LED1_K" pad="10"/>
<connect gate="G$1" pin="LED2_A" pad="12"/>
<connect gate="G$1" pin="LED2_K" pad="11"/>
<connect gate="G$1" pin="RCT" pad="6"/>
<connect gate="G$1" pin="RX+" pad="7"/>
<connect gate="G$1" pin="RX-" pad="8"/>
<connect gate="G$1" pin="TCT" pad="3"/>
<connect gate="G$1" pin="TX+" pad="1"/>
<connect gate="G$1" pin="TX-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J000065NL" package="RJ45_PULSEJACK">
<connects>
<connect gate="G$1" pin="GND1" pad="8"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="LED1_A" pad="9"/>
<connect gate="G$1" pin="LED1_K" pad="10"/>
<connect gate="G$1" pin="LED2_A" pad="12"/>
<connect gate="G$1" pin="LED2_K" pad="11"/>
<connect gate="G$1" pin="RCT" pad="5"/>
<connect gate="G$1" pin="RX+" pad="3"/>
<connect gate="G$1" pin="RX-" pad="6"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TX+" pad="1"/>
<connect gate="G$1" pin="TX-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITE" prefix="FB" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Ferrite Bead&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0603&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;MMZ1608B121C - 120 Ohm @ 100MHz, 600mA, 0.15 Ohm DC Resistance - Digikey: 445-2164-1-ND&lt;/li&gt;
&lt;li&gt;BK1608HW121-T - 120 Ohm, 600mA Ferrite Chip - Digikey: 587-1876-2-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;0805&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;HZ0805B272R-10 - 2.7K Ohm @ 100MHz, 200mA, 0.8 Ohm DC Resistance - Digikey: 240-2504-1-ND (see also Murata BLM21BD272SN1L)&lt;/li&gt;
&lt;li&gt;MMZ2012Y152B - 1.5K Ohm @ 100MHz, 500mA, 0.4 Ohm DC Resistance - Digikey: 445-1560-1-ND - Mainly for high frequency (80-400MHz)&lt;/li&gt;
&lt;li&gt;MMZ2012R102A - 1K Ohm @ 100MHz, 500mA, 0.3 Ohm DC Resistance - Digikey: 445-1555-2-ND - More general purpose (10-200MHz)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="FERRITE"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402" package="_0402">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402MP" package="_0402MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603" package="_0603">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603MP" package="_0603MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="_0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805MP" package="_0805MP">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X11" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD11"/>
</gates>
<devices>
<device name="" package="1X11_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X11_ROUND_76">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X12" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD12"/>
</gates>
<devices>
<device name="" package="1X12_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OVAL" package="1X12_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="80MIL" package="1X12_ROUND_80MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="76MIL" package="1X12_ROUND_76MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_TACT_SMT" prefix="B" uservalue="yes">
<description>&lt;p&gt;SMT Tact Switches&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;6x6mm - Digikey: P12940SCT-ND&lt;/li&gt;
&lt;li&gt;KMR2 (4.6x2.8mm) - Digikey: 401-1426-1-ND&lt;/li&gt;
&lt;li&gt;EVQ-PQHB55 - Light Touch, 160GF (4.5x4.5mm) - Digikey: P8090SCT-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="BUTTON_4PIN"/>
</gates>
<devices>
<device name="" package="EVQ-Q2">
<connects>
<connect gate="G$1" pin="P" pad="A"/>
<connect gate="G$1" pin="P1" pad="A'"/>
<connect gate="G$1" pin="S" pad="B"/>
<connect gate="G$1" pin="S1" pad="B'"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.6X2.8" package="BTN_KMR2_4.6X2.8">
<connects>
<connect gate="G$1" pin="P" pad="A"/>
<connect gate="G$1" pin="P1" pad="A'"/>
<connect gate="G$1" pin="S" pad="B"/>
<connect gate="G$1" pin="S1" pad="B'"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EVQPQ" package="BTN_EVQPQ_4.5MM">
<connects>
<connect gate="G$1" pin="P" pad="A"/>
<connect gate="G$1" pin="P1" pad="C"/>
<connect gate="G$1" pin="S" pad="B"/>
<connect gate="G$1" pin="S1" pad="D"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMACONNECTOR" prefix="X" uservalue="yes">
<description>&lt;b&gt;SMA Connector&lt;/b&gt;
&lt;p&gt;90° DIP SMA Connector, 50 Ohm (4UConnector: 07259)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMACONNECTOR"/>
</gates>
<devices>
<device name="" package="SMA90_DIP">
<connects>
<connect gate="G$1" pin="ANT" pad="ANTENNA"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT86RF212" prefix="U" uservalue="yes">
<description>&lt;b&gt;AT86RF212&lt;/b&gt; - Low-Power SPI-based 700/800/900 MHz Transceiver
&lt;p&gt;Digikey: AT86RF212-ZU-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AT86RF212"/>
</gates>
<devices>
<device name="" package="32QN2">
<connects>
<connect gate="G$1" pin="/RST" pad="8"/>
<connect gate="G$1" pin="/SEL" pad="23"/>
<connect gate="G$1" pin="AVDD" pad="29"/>
<connect gate="G$1" pin="AVSS1" pad="3"/>
<connect gate="G$1" pin="AVSS2" pad="6"/>
<connect gate="G$1" pin="AVSS3" pad="27"/>
<connect gate="G$1" pin="AVSS4" pad="30"/>
<connect gate="G$1" pin="AVSS5" pad="31"/>
<connect gate="G$1" pin="AVSS6" pad="32"/>
<connect gate="G$1" pin="CLKM" pad="17"/>
<connect gate="G$1" pin="DEVDD" pad="15"/>
<connect gate="G$1" pin="DIE" pad="33"/>
<connect gate="G$1" pin="DIG1" pad="9"/>
<connect gate="G$1" pin="DIG2" pad="10"/>
<connect gate="G$1" pin="DIG3" pad="1"/>
<connect gate="G$1" pin="DIG4" pad="2"/>
<connect gate="G$1" pin="DVDD1" pad="13"/>
<connect gate="G$1" pin="DVDD2" pad="14"/>
<connect gate="G$1" pin="DVSS1" pad="7"/>
<connect gate="G$1" pin="DVSS2" pad="12"/>
<connect gate="G$1" pin="DVSS3" pad="16"/>
<connect gate="G$1" pin="DVSS4" pad="18"/>
<connect gate="G$1" pin="DVSS5" pad="21"/>
<connect gate="G$1" pin="EVDD" pad="28"/>
<connect gate="G$1" pin="IRQ" pad="24"/>
<connect gate="G$1" pin="MISO" pad="20"/>
<connect gate="G$1" pin="MOSI" pad="22"/>
<connect gate="G$1" pin="RFN" pad="5"/>
<connect gate="G$1" pin="RFP" pad="4"/>
<connect gate="G$1" pin="SCLK" pad="19"/>
<connect gate="G$1" pin="SLP_TR" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="26"/>
<connect gate="G$1" pin="XTAL2" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="PARTNO" value="AT86RF212-ZU"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BALUN" prefix="U" uservalue="yes">
<description>&lt;b&gt;BALUN&lt;/b&gt; - Baluns for RF

&lt;p&gt;
&lt;b&gt;1206&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;800-1000MHz Balun (1206) - Digikey: 712-1023-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BALUN"/>
</gates>
<devices>
<device name="" package="BALUN1206">
<connects>
<connect gate="G$1" pin="BALP1" pad="P$4"/>
<connect gate="G$1" pin="BALP2" pad="P$6"/>
<connect gate="G$1" pin="GND1" pad="P$1"/>
<connect gate="G$1" pin="GND2" pad="P$3"/>
<connect gate="G$1" pin="NC" pad="P$5"/>
<connect gate="G$1" pin="UNBAL" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOWPASSFILTER" prefix="U" uservalue="yes">
<description>&lt;b&gt;Low Pass Filter&lt;/b&gt; - RF Signal Filter
&lt;p&gt;
&lt;b&gt;0603&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;869MHz Low Pass Filter - Digikey: 712-1118-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LOWPASSFILTER"/>
</gates>
<devices>
<device name="" package="LOWPASSFILTER0603">
<connects>
<connect gate="G$1" pin="GND1" pad="P$1"/>
<connect gate="G$1" pin="GND2" pad="P$3"/>
<connect gate="G$1" pin="GND3" pad="P$5"/>
<connect gate="G$1" pin="IN" pad="P$6"/>
<connect gate="G$1" pin="NC" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA868MHZ" prefix="X" uservalue="yes">
<description>&lt;b&gt;868MHz Surface-Mount Antenna&lt;/b&gt;
&lt;p&gt;Digikey: ANT-868-SP_-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ANTENNA_CHIP"/>
</gates>
<devices>
<device name="" package="869MHZANTENNA">
<connects>
<connect gate="G$1" pin="ANT" pad="P$1"/>
<connect gate="G$1" pin="GND1" pad="P$2"/>
<connect gate="G$1" pin="GND2" pad="P$3"/>
<connect gate="G$1" pin="GND3" pad="P$4"/>
<connect gate="G$1" pin="GND4" pad="P$5"/>
<connect gate="G$1" pin="GND5" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BALUN+LP_AT86RF" prefix="B" uservalue="yes">
<description>&lt;b&gt;Balun + Low Pass Filter&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;0805&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Johanson 0896FB15A0100 (AT86RF212) - 863-928 MHz Balun + Filter - Digikey: 712-1473-1-ND&lt;/li&gt;
&lt;li&gt;Johanson 2450FB15L0001 (AR86RF230/231) - 2400-2500 MHz Balun + Filter - Digikey: 712-1538-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BALUN+LP_AT86RF"/>
</gates>
<devices>
<device name="" package="BALUN0805">
<connects>
<connect gate="G$1" pin="BALP1" pad="3"/>
<connect gate="G$1" pin="BALP2" pad="4"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="6"/>
<connect gate="G$1" pin="UNBAL" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AGND">
<description>&lt;b&gt;Analog GND&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AGND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVCC">
<description>&lt;b&gt;Analog VCC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AVCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDIUSBCABLE" prefix="CN" uservalue="yes">
<description>&lt;strong&gt;FTDI TTL-232R USB Cable&lt;/strong&gt;
&lt;p&gt;Connector for FTDI's USB-&gt;RS232 Cable&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FTDIUSBCABLE"/>
</gates>
<devices>
<device name="" package="1X06_ROUND">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM_SPI_AT25040A" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;AT25010a/40a EEPROM&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;SOIC8&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;AT25010a, 1K (128 x 8 bit) - Digikey: AT25010AN-10SU2.7-ND&lt;/li&gt;
&lt;li&gt;AT25040a, 4K (256 x 8 bit) - Digikey: AT25040AN-10SU1.8-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;TSSOP8&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;AT25010a, 1K (128 x 8 bit) - Digikey: AT25010A-10TU-1.8-ND&lt;/li&gt;
&lt;li&gt;AT25040a, 4K (256 x 8 bit) - Digikey: AT25040A-10TU-1.8-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="AT25040A"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TSSOP" package="TSSOP8-4.4MM">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PN532" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;PN532&lt;/b&gt; - Near Field Communication (NFC) controller&lt;/p&gt;
&lt;p&gt;Highly integrated transceiver module for contactless communication at 13.56 MHz (14443A/MIFARE, FeliCa, I4443B)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PN532"/>
</gates>
<devices>
<device name="" package="HVQFN40-6X6">
<connects>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="AUX1" pad="12"/>
<connect gate="G$1" pin="AUX2" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="8"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="DVDD" pad="39"/>
<connect gate="G$1" pin="I0" pad="16"/>
<connect gate="G$1" pin="I1" pad="17"/>
<connect gate="G$1" pin="IRQ" pad="25"/>
<connect gate="G$1" pin="LOADMOD" pad="2"/>
<connect gate="G$1" pin="MISO" pad="29"/>
<connect gate="G$1" pin="MOSI/SDA/HSU_TX" pad="28"/>
<connect gate="G$1" pin="NC1" pad="20"/>
<connect gate="G$1" pin="NC2" pad="21"/>
<connect gate="G$1" pin="NC3" pad="22"/>
<connect gate="G$1" pin="NSS/P50_SCL/HSU_RX" pad="27"/>
<connect gate="G$1" pin="P30/UART_RX" pad="24"/>
<connect gate="G$1" pin="P31" pad="31"/>
<connect gate="G$1" pin="P32" pad="32"/>
<connect gate="G$1" pin="P33" pad="33"/>
<connect gate="G$1" pin="P34/SIC_CLK" pad="34"/>
<connect gate="G$1" pin="P35" pad="19"/>
<connect gate="G$1" pin="PVDD" pad="23"/>
<connect gate="G$1" pin="RSTOUT_N" pad="26"/>
<connect gate="G$1" pin="RSTPD_N" pad="38"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="SCK" pad="30"/>
<connect gate="G$1" pin="SIGIN" pad="36"/>
<connect gate="G$1" pin="SIGOUT" pad="35"/>
<connect gate="G$1" pin="SVDD" pad="37"/>
<connect gate="G$1" pin="TESTEN" pad="18"/>
<connect gate="G$1" pin="TGND1" pad="3"/>
<connect gate="G$1" pin="TGND2" pad="7"/>
<connect gate="G$1" pin="THERMAL" pad="TP"/>
<connect gate="G$1" pin="TVDD" pad="5"/>
<connect gate="G$1" pin="TX1" pad="4"/>
<connect gate="G$1" pin="TX2" pad="6"/>
<connect gate="G$1" pin="VBAT" pad="40"/>
<connect gate="G$1" pin="VMID" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BRIDGERECTIFIER" prefix="G" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Bridge Rectifier&lt;/b&gt;&lt;/p&gt;
SOIC-4:
&lt;ul&gt;
&lt;li&gt;Comchip B4S-G - 400V 800mA, Peak Vf 1.1V (Digikey: 641-1334-1-ND)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="BRIDGERECTIFIER"/>
</gates>
<devices>
<device name="" package="SOIC-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="AC1" pad="~1"/>
<connect gate="G$1" pin="AC2" pad="~2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_GM862" prefix="U" uservalue="yes">
<description>&lt;b&gt;GM862 Cellular Module with GPS&lt;/b&gt;
Proven layout and schematic for GM862 cellular module with SiRF III GPS. Spark Fun Electronics SKU : CEL-07917
&lt;p&gt;Footprint taken from the Sparkfun Eagle library (CC-SA license).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="GM862"/>
</gates>
<devices>
<device name="GND" package="GM862">
<connects>
<connect gate="G$1" pin="AXE" pad="18"/>
<connect gate="G$1" pin="C103/TXD" pad="20"/>
<connect gate="G$1" pin="C104/RXD" pad="37"/>
<connect gate="G$1" pin="C105/RTS" pad="45"/>
<connect gate="G$1" pin="C106/CTS" pad="29"/>
<connect gate="G$1" pin="C107/DSR" pad="33"/>
<connect gate="G$1" pin="C108/DTR" pad="43"/>
<connect gate="G$1" pin="C109/DCD" pad="36"/>
<connect gate="G$1" pin="C125/RING" pad="30"/>
<connect gate="G$1" pin="CCIN/SIMIN" pad="27"/>
<connect gate="G$1" pin="CHARGE" pad="8"/>
<connect gate="G$1" pin="EAR_HF+" pad="9"/>
<connect gate="G$1" pin="EAR_HF-" pad="11"/>
<connect gate="G$1" pin="EAR_MT+" pad="12"/>
<connect gate="G$1" pin="EAR_MT-" pad="10"/>
<connect gate="G$1" pin="EMMI_RX/RX_GPS" pad="41"/>
<connect gate="G$1" pin="EMMI_TX/TX_GPS" pad="35"/>
<connect gate="G$1" pin="GND/ADC" pad="6"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="G1"/>
<connect gate="G$1" pin="GND@3" pad="G2"/>
<connect gate="G$1" pin="GND@4" pad="G3"/>
<connect gate="G$1" pin="GND@5" pad="G8"/>
<connect gate="G$1" pin="GND@6" pad="G4"/>
<connect gate="G$1" pin="GND@7" pad="G5"/>
<connect gate="G$1" pin="GND@8" pad="G6"/>
<connect gate="G$1" pin="GND@9" pad="G7"/>
<connect gate="G$1" pin="GPI1" pad="31"/>
<connect gate="G$1" pin="GPIO10/PD[2]" pad="38"/>
<connect gate="G$1" pin="GPIO11/PD[3]" pad="40"/>
<connect gate="G$1" pin="GPIO12/PD[4]" pad="42"/>
<connect gate="G$1" pin="GPIO13/PD[5]" pad="44"/>
<connect gate="G$1" pin="GPIO3/PD[6]/CAM_SCL" pad="46"/>
<connect gate="G$1" pin="GPIO4/IICSDA/CAM_SDA" pad="47"/>
<connect gate="G$1" pin="GPIO5/CAM_RDY/RFTXMON" pad="48"/>
<connect gate="G$1" pin="GPIO6/ALARM/PD[7]" pad="49"/>
<connect gate="G$1" pin="GPIO7/BUZZER/CAM_PWR_ON" pad="50"/>
<connect gate="G$1" pin="GPIO8/PD[0]/CAM_ON" pad="32"/>
<connect gate="G$1" pin="GPIO9/PD[1]/CAM_RST" pad="34"/>
<connect gate="G$1" pin="GPO2/JDR" pad="28"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="13"/>
<connect gate="G$1" pin="MIC_MT+" pad="14"/>
<connect gate="G$1" pin="MIC_MT-" pad="16"/>
<connect gate="G$1" pin="ON/OFF" pad="17"/>
<connect gate="G$1" pin="PWRMON" pad="21"/>
<connect gate="G$1" pin="RES@25" pad="25"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="SIMCLK" pad="26"/>
<connect gate="G$1" pin="SIMIO" pad="19"/>
<connect gate="G$1" pin="SIMRST" pad="24"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="39"/>
<connect gate="G$1" pin="VBATT@0" pad="1"/>
<connect gate="G$1" pin="VBATT@1" pad="3"/>
<connect gate="G$1" pin="VBATT@2" pad="5"/>
<connect gate="G$1" pin="VBATT@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GM862_CONNECTOR" package="GM862_CONNECTOR">
<connects>
<connect gate="G$1" pin="AXE" pad="18"/>
<connect gate="G$1" pin="C103/TXD" pad="20"/>
<connect gate="G$1" pin="C104/RXD" pad="37"/>
<connect gate="G$1" pin="C105/RTS" pad="45"/>
<connect gate="G$1" pin="C106/CTS" pad="29"/>
<connect gate="G$1" pin="C107/DSR" pad="33"/>
<connect gate="G$1" pin="C108/DTR" pad="43"/>
<connect gate="G$1" pin="C109/DCD" pad="36"/>
<connect gate="G$1" pin="C125/RING" pad="30"/>
<connect gate="G$1" pin="CCIN/SIMIN" pad="27"/>
<connect gate="G$1" pin="CHARGE" pad="8"/>
<connect gate="G$1" pin="EAR_HF+" pad="9"/>
<connect gate="G$1" pin="EAR_HF-" pad="11"/>
<connect gate="G$1" pin="EAR_MT+" pad="12"/>
<connect gate="G$1" pin="EAR_MT-" pad="10"/>
<connect gate="G$1" pin="EMMI_RX/RX_GPS" pad="41"/>
<connect gate="G$1" pin="EMMI_TX/TX_GPS" pad="35"/>
<connect gate="G$1" pin="GND/ADC" pad="6"/>
<connect gate="G$1" pin="GND@0" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="G1"/>
<connect gate="G$1" pin="GND@3" pad="G2"/>
<connect gate="G$1" pin="GND@4" pad="G3"/>
<connect gate="G$1" pin="GND@5" pad="G8"/>
<connect gate="G$1" pin="GND@6" pad="G4"/>
<connect gate="G$1" pin="GND@7" pad="G5"/>
<connect gate="G$1" pin="GND@8" pad="G6"/>
<connect gate="G$1" pin="GND@9" pad="G7"/>
<connect gate="G$1" pin="GPI1" pad="31"/>
<connect gate="G$1" pin="GPIO10/PD[2]" pad="38"/>
<connect gate="G$1" pin="GPIO11/PD[3]" pad="40"/>
<connect gate="G$1" pin="GPIO12/PD[4]" pad="42"/>
<connect gate="G$1" pin="GPIO13/PD[5]" pad="44"/>
<connect gate="G$1" pin="GPIO3/PD[6]/CAM_SCL" pad="46"/>
<connect gate="G$1" pin="GPIO4/IICSDA/CAM_SDA" pad="47"/>
<connect gate="G$1" pin="GPIO5/CAM_RDY/RFTXMON" pad="48"/>
<connect gate="G$1" pin="GPIO6/ALARM/PD[7]" pad="49"/>
<connect gate="G$1" pin="GPIO7/BUZZER/CAM_PWR_ON" pad="50"/>
<connect gate="G$1" pin="GPIO8/PD[0]/CAM_ON" pad="32"/>
<connect gate="G$1" pin="GPIO9/PD[1]/CAM_RST" pad="34"/>
<connect gate="G$1" pin="GPO2/JDR" pad="28"/>
<connect gate="G$1" pin="MIC_HF+" pad="15"/>
<connect gate="G$1" pin="MIC_HF-" pad="13"/>
<connect gate="G$1" pin="MIC_MT+" pad="14"/>
<connect gate="G$1" pin="MIC_MT-" pad="16"/>
<connect gate="G$1" pin="ON/OFF" pad="17"/>
<connect gate="G$1" pin="PWRMON" pad="21"/>
<connect gate="G$1" pin="RES@25" pad="25"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="SIMCLK" pad="26"/>
<connect gate="G$1" pin="SIMIO" pad="19"/>
<connect gate="G$1" pin="SIMRST" pad="24"/>
<connect gate="G$1" pin="SIMVCC" pad="22"/>
<connect gate="G$1" pin="STAT_LED" pad="39"/>
<connect gate="G$1" pin="VBATT@0" pad="1"/>
<connect gate="G$1" pin="VBATT@1" pad="3"/>
<connect gate="G$1" pin="VBATT@2" pad="5"/>
<connect gate="G$1" pin="VBATT@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD39015XX" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LDO Fixed Voltage Regulator 150mA&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;The LD39015xx voltage regulator is ideal for regulating battery or solar power due to it's very low foreward voltage drop (~100mV at 150mA).&lt;/p&gt;
Forward Voltage Dropout: 100mV at 150mA, 80mV at 100mA&lt;br/&gt;
Input Voltage Range: 1.5V-5.5V&lt;br/&gt;
Output Voltage Range: 0.8V-3.3V (depending on model)
&lt;p&gt;Digikey: 1.8V - 497-6977-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LD39015XX"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1113/4_QFN" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LPC1113/4&lt;/b&gt; ARM Cortex-M0 processor, running at frequencies of up to 50 MHz.&lt;/p&gt;
QFN 33 Pin Package</description>
<gates>
<gate name="G$1" symbol="LPC1114_QFN33"/>
</gates>
<devices>
<device name="" package="HVQFN33-7X7">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="P$3"/>
<connect gate="G$1" pin="PIO0_2/SSEL/CT16B0_CAP0" pad="P$8"/>
<connect gate="G$1" pin="PIO0_3" pad="P$9"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="P$10"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="P$11"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="P$15"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="P$16"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="P$17"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="P$18"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="P$20"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="P$27"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="P$26"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="P$30"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="P$31"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="P$32"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="P$7"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="P$12"/>
<connect gate="G$1" pin="PIO2_0/DTR" pad="P$1"/>
<connect gate="G$1" pin="PIO3_2" pad="P$28"/>
<connect gate="G$1" pin="PIO3_4" pad="P$13"/>
<connect gate="G$1" pin="PIO3_5" pad="P$14"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="P$2"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="P$19"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="P$25"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="P$21"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="P$23"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="P$22"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="P$24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="P$29"/>
<connect gate="G$1" pin="VDD(IO)" pad="P$6"/>
<connect gate="G$1" pin="VSS" pad="P$33"/>
<connect gate="G$1" pin="XTALIN" pad="P$4"/>
<connect gate="G$1" pin="XTALOUT" pad="P$5"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY#" value="568-4948-ND"/>
<attribute name="MANF" value="NXP"/>
<attribute name="MANF#" value="LPC1114FHN33/301,5"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVDD">
<description>&lt;b&gt;Analog VDD&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AVDD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM_I2C_MCP24AA32" prefix="U" uservalue="yes">
<description>&lt;b&gt;Microchip 32K (4K x 8) 1.8V I2C EEPROM&lt;/b&gt;
&lt;p&gt;SOT23-5 [Digikey: 24AA32AFT-I/OTCT-ND]&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP24AA32"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-ZENER" prefix="D" uservalue="yes">
<description>&lt;b&gt;Zener Diode&lt;/b&gt;
&lt;p&gt;&lt;b&gt;SMA:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;30V 1W Zener Diode, 1.2Vf - Digikey: SMAZ30-FDICT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE-ZENER"/>
</gates>
<devices>
<device name="" package="SMADIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB_PLCC4" prefix="LED" uservalue="yes">
<description>&lt;b&gt;RGB LED - PLCC4&lt;/b&gt;
&lt;p&gt;Cree 20mA Common Anode&lt;br/&gt;
Digikey: CLV1A-FKB-CJ1M1F1BB7R4S3CT-ND&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Red&lt;/b&gt;: 2.6V Vf, 550mcd&lt;br/&gt;
&lt;b&gt;Green&lt;/b&gt;: 3.2V Vf, 850mcd&lt;br/&gt;
&lt;b&gt;Blue&lt;/b&gt;: 3.2V Vf, 320mcd&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LEDRGB_PLCC4"/>
</gates>
<devices>
<device name="" package="RGBLED_PLCC4">
<connects>
<connect gate="G$1" pin="ANODE" pad="2"/>
<connect gate="G$1" pin="BLUE" pad="3"/>
<connect gate="G$1" pin="GRN" pad="4"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_NPN" prefix="Q" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;NPN Transistor&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Transistor (NPN) 500mA 45V - BC817 [Digikey: 568-1631-1-ND]&lt;/li&gt;
&lt;li&gt;Transistor (NPN) 500mA 45V - BC817,215 [Mouser: 771-BC817-T/R]&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;
&lt;b&gt;SOT23-R&lt;/b&gt; - SOT23 footprint optimised for use with solder paste and reflow ovens.&lt;br&gt;
&lt;b&gt;SOT23-W&lt;/b&gt; - SOT23 footprint optimised for hand-soldering (larger pads).
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT23-R">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WAVE" package="SOT23-W">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2671" prefix="U" uservalue="yes">
<description>&lt;b&gt;LM2671&lt;/b&gt;
&lt;p&gt;High Efficiency 500mA Switching Step-Down Voltage Regulator.  6.5-40V Input.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;3.3V SOIC-8&lt;/b&gt;: Digikey LM2671M-3.3-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LM2671"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="CB" pad="1"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="ON/OFF" pad="5"/>
<connect gate="G$1" pin="SS" pad="2"/>
<connect gate="G$1" pin="SYNC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_SOT23-5" prefix="U" uservalue="yes">
<description>&lt;b&gt;SOT23-5 Fixed Voltage Regulators&lt;/b&gt;
&lt;p&gt;To better organise some of the SOT23-5 fixed voltage regulators in this library, this new part was created.&lt;br/&gt;&lt;/p&gt;
&lt;table width="550"&gt;
&lt;tr bgcolor="#EEEEEE" &gt;
&lt;td&gt;&lt;b&gt;Part&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Current Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V In&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Dropout&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Digikey Part No.&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP121&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.4-5.5V&lt;/td&gt;
  &lt;td&gt;0.09V @ 150mA&lt;/td&gt;
  &lt;td&gt;ADP121-AUJZ33R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP121&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.0V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.1-5.5V&lt;/td&gt;
  &lt;td&gt;0.09V @ 150mA&lt;/td&gt;
  &lt;td&gt;ADP121-AUJZ30R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP122&lt;/td&gt;
  &lt;td&gt;&lt;strong&gt;300mA&lt;/strong&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.4-5.5V&lt;/td&gt;
  &lt;td&gt;0.085V @ 300mA&lt;/td&gt;
  &lt;td&gt;ADP122AUJZ-3.3-R7CT-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;ADP1712&lt;/td&gt;
  &lt;td&gt;&lt;strong&gt;300mA&lt;/strong&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-5.5V&lt;/td&gt;
  &lt;td&gt;0.17V @ 300mA&lt;/td&gt;
  &lt;td&gt;ADP1712AUJZ-3.3-R7TR-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;AP7311 (&lt;b&gt;Low Cost&lt;/b&gt;)&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-6V&lt;/td&gt;
  &lt;td&gt;0.15V @ 150mA&lt;/td&gt;
  &lt;td&gt;AP7311-33WG-7DICT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;LD39015M18R&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;1.8V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;1.9V-5.5V&lt;/td&gt;
  &lt;td&gt;0.08V @ 100mA&lt;/td&gt;
  &lt;td&gt;497-6977-1-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;MCP1824T-3302E/OT&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;300mA&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5V-6V&lt;/td&gt;
  &lt;td&gt;0.2V @ 300mA&lt;/td&gt;
  &lt;td&gt;MCP1824T-3302E/OTCT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;MIC5205-2.5YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;2.5V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;2.7-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;576-1257-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MIC5205-3.0YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.0V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.2V-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;576-1258-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MIC5205-3.3YM5 TR&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5V-16V&lt;/td&gt;
  &lt;td&gt;0.165V @ 150mA&lt;/td&gt;
  &lt;td&gt;576-1259-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;TPS780330220&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V+2.2V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.6-5.5V&lt;/td&gt;
  &lt;td&gt;250mV Max&lt;/td&gt;
  &lt;td&gt;296-23332-1-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;TDA3663/N1,135&lt;/td&gt;
  &lt;td&gt;100mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-&lt;b&gt;45V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;0.18V @ 50mA&lt;/td&gt;
  &lt;td&gt;568-5343-1-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;/table&gt;</description>
<gates>
<gate name="G$1" symbol="VREG_SOT23-5"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="P4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1113/4_QFP_SQUARE" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1113/4 QFP&lt;/b&gt;
&lt;p&gt;This is the same chip used in the LPC1113/4 footprint, but the schematic symbol is a square corresponding to the same pinout used on the LQFP48 IC.  This alternate layout can be useful when designing space-constrained devices, and to minimise the number of vias on a board.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114_QFP_SQUARE"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK0" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="19"/>
<connect gate="G$1" pin="PIO2_5" pad="20"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0/DTR" pad="36"/>
<connect gate="G$1" pin="PIO3_1/DSR" pad="37"/>
<connect gate="G$1" pin="PIO3_2/DCD" pad="43"/>
<connect gate="G$1" pin="PIO3_3/RI" pad="48"/>
<connect gate="G$1" pin="PIO3_4" pad="18"/>
<connect gate="G$1" pin="PIO3_5" pad="21"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="VDD(3.3V)" pad="44"/>
<connect gate="G$1" pin="VDD(IO)" pad="8"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS(IO)" pad="41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR_DUAL" prefix="R" uservalue="yes">
<description>&lt;B&gt;Flip Flop resistor&lt;/b&gt;
&lt;p&gt;
An 0805 resistor inside a standard 1/4W 5% resistor. Makes for easy mods
&lt;p&gt;Footprint taken from the Adafruit Industries Eagle Library.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="" package="0805-THM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL" prefix="FID">
<description>&lt;b&gt;Fiducial Alignment Points&lt;/b&gt;
&lt;p&gt;Various fiducial points for machine vision alignment.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FIDUCIAL"/>
</gates>
<devices>
<device name="1X2.5" package="FIDUCIAL-1X2.5">
<technologies>
<technology name="">
<attribute name="BOM" value="EXCLUDE"/>
</technology>
</technologies>
</device>
<device name="ROUND" package="PASS-ROUND">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="&quot;&quot;" package="FIDUCIAL_1MM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-P" prefix="Q" uservalue="yes">
<description>&lt;b&gt;P-Channel Mosfet&lt;/b&gt;
&lt;p&gt;&lt;b&gt;LEGEND&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;VDS&lt;/b&gt;: Voltage Drain-Source&lt;br/&gt;
&lt;b&gt;ID&lt;/b&gt;: Drain Current&lt;br/&gt;
&lt;b&gt;RDS(ON)&lt;/b&gt;: Drain-Source On-State Resistance&lt;br/&gt;
&lt;b&gt;VGS(TH)&lt;/b&gt;: Gate-Source Threshold Voltage&lt;br/&gt;
&lt;b&gt;CISS&lt;/b&gt;: Drain-Source Input Capacitance
&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;SOT-23&lt;/b&gt;
&lt;table border="0" width="90%" cellspacing="0" cellpadding="5"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
&lt;td&gt;Name&lt;/td&gt;
&lt;td&gt;VDS&lt;/td&gt;
&lt;td&gt;ID&lt;/td&gt;
&lt;td&gt;RDS(ON)&lt;/td&gt;
&lt;td&gt;VGS(TH)&lt;/td&gt;
&lt;td&gt;CISS&lt;/td&gt;
&lt;td&gt;Order Number&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;IRLML5103&lt;/td&gt;
&lt;td&gt;30V&lt;/td&gt;
&lt;td&gt;760mA&lt;/td&gt;
&lt;td&gt;600 mOhm&lt;/td&gt;
&lt;td&gt;--&lt;/td&gt;
&lt;td&gt;75pF @ 25V&lt;/td&gt;
&lt;td&gt;Digikey: IRLML5103PBFCT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;IRLML6401&lt;/td&gt;
&lt;td&gt;12V&lt;/td&gt;
&lt;td&gt;4.3A&lt;/td&gt;
&lt;td&gt;50 mOhm&lt;/td&gt;
&lt;td&gt;950mV @ 250µA&lt;/td&gt;
&lt;td&gt;830pF @ 10V&lt;/td&gt;
&lt;td&gt;Digikey: IRLML6401PBFTR-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;NTR0202PL&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;400mA&lt;/td&gt;
&lt;td&gt;800 mOhm&lt;/td&gt;
&lt;td&gt;2.3V @ 250uA&lt;/td&gt;
&lt;td&gt;70pF @ 5V&lt;/td&gt;
&lt;td&gt;Digikey: NTR0202PLT1GOSTR-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;NTR4101PT1G&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;1.8A&lt;/td&gt;
&lt;td&gt;85 mOhm&lt;/td&gt;
&lt;td&gt;1.2V @ 250uA&lt;/td&gt;
&lt;td&gt;675pF @ 10V&lt;/td&gt;
&lt;td&gt;Digikey: NTR4101PT1GOSCT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;DMP2004K&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;600mA&lt;/td&gt;
&lt;td&gt;900 mOhm&lt;/td&gt;
&lt;td&gt;1V @ 250uA&lt;/td&gt;
&lt;td&gt;175pF @ 16V&lt;/td&gt;
&lt;td&gt;Digikey: DMP2004KDICT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;PMV65XP&lt;/td&gt;
&lt;td&gt;20V&lt;/td&gt;
&lt;td&gt;3.9A&lt;/td&gt;
&lt;td&gt;76 mOhm&lt;/td&gt;
&lt;td&gt;950mV @ 1mA&lt;/td&gt;
&lt;td&gt;725pF @ 20V&lt;/td&gt;
&lt;td&gt;Digikey: 568-2358-2-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt; 
&lt;b&gt;TO-252&lt;/b&gt;
&lt;table border="0" width="90%" cellspacing="0" cellpadding="5"&gt;
&lt;tr bgcolor="#DDDDDD"&gt;
&lt;td&gt;Name&lt;/td&gt;
&lt;td&gt;VDS&lt;/td&gt;
&lt;td&gt;ID&lt;/td&gt;
&lt;td&gt;RDS(ON)&lt;/td&gt;
&lt;td&gt;VGS(TH)&lt;/td&gt;
&lt;td&gt;CISS&lt;/td&gt;
&lt;td&gt;Order Number&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;AOD417&lt;/td&gt;
&lt;td&gt;30V&lt;/td&gt;
&lt;td&gt;25A&lt;/td&gt;
&lt;td&gt;34 mOhm&lt;/td&gt;
&lt;td&gt;3V @ 250µA&lt;/td&gt;
&lt;td&gt;920pF @ 15V&lt;/td&gt;
&lt;td&gt;Digikey: 785-1106-2-ND&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOSFET-P"/>
</gates>
<devices>
<device name="" package="SOT23-R">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358" prefix="U" uservalue="yes">
<description>&lt;b&gt;LM358 Dual Operational Amplifier&lt;/b&gt;
&lt;p&gt;Digikey: LM358AMXFSCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
<gate name="G$2" symbol="OPAMP"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP_ADT7410" prefix="U" uservalue="yes">
<description>&lt;b&gt;ADT7410&lt;/b&gt; - 13-bit 0.5°C I2C Temperature Sensor
&lt;ul&gt;
&lt;li&gt;Operating Voltage: 2.7-5.5V&lt;/li&gt;
&lt;li&gt;Temperature Range: -55°C-150°C&lt;/li&gt;
&lt;li&gt;Accuracy: 0.5°C from -40°C-105°C&lt;/li&gt;
&lt;li&gt;Shutdown Current: 2uA (3.3V)&lt;/li&gt;
&lt;li&gt;Typical Operating Current (1 Sample/s): 46uA (3.3V)&lt;/li&gt;
&lt;/ul&gt;
Digikey: ADT7410TRZ-ND</description>
<gates>
<gate name="G$1" symbol="ADT7410"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="CT" pad="6"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="INT" pad="5"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADM1191" prefix="U" uservalue="yes">
<description>&lt;b&gt;ADM1191&lt;/b&gt; - I2C Digital Power Monitor
&lt;ul&gt;
&lt;li&gt;3.15V to 26V Operation&lt;/li&gt;
&lt;li&gt;12-bit ADC&lt;/li&gt;
&lt;li&gt;Precision Current Sense Amplifier&lt;/li&gt;
&lt;li&gt;Precision Voltage Input&lt;/li&gt;
&lt;/ul&gt;
Digikey: ADM1191-2ARMZ-R7TR-ND</description>
<gates>
<gate name="G$1" symbol="ADM1191"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="ALERTB" pad="10"/>
<connect gate="G$1" pin="CONV" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SETV" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X8" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINH2X8"/>
</gates>
<devices>
<device name="" package="2X08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1768" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1768 &lt;/b&gt;&lt;p&gt;100 MHz 32-bit ARM Cortex-M3 based microcontroller featuring a high level of integration and low power consumption. 512 kB Flash, 64 kB SRAM, USB Device/Host/OTG, Ethernet, CAN, I2S, 10-bit DAC &lt;/p&gt;
&lt;p&gt;Digikey: 568-4796-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1768_QFP"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="G$1" pin="N.C." pad="13"/>
<connect gate="G$1" pin="P0[0]/RD1/TXD3/SDA1" pad="46"/>
<connect gate="G$1" pin="P0[10]/TXD2/SDA2/MAT3[0]" pad="48"/>
<connect gate="G$1" pin="P0[11]/RXD2/SCL2/MAT3[1]" pad="49"/>
<connect gate="G$1" pin="P0[15]/TXD1/SCK0/SCK" pad="62"/>
<connect gate="G$1" pin="P0[16]/RXD1/SSEL0/SSEL" pad="63"/>
<connect gate="G$1" pin="P0[17]/CTS1/MISO0/MISO" pad="61"/>
<connect gate="G$1" pin="P0[18]/DCD1/MOSI0/MOSI" pad="60"/>
<connect gate="G$1" pin="P0[19]/DSR1/SDA1" pad="59"/>
<connect gate="G$1" pin="P0[1]/TD1/RXD3/SCL1" pad="47"/>
<connect gate="G$1" pin="P0[20]/DTR1/SCL1" pad="58"/>
<connect gate="G$1" pin="P0[21]/RI1/RD1" pad="57"/>
<connect gate="G$1" pin="P0[22]/RTS1/TD1" pad="56"/>
<connect gate="G$1" pin="P0[23]/AD0[0]/I2SRX_CLK/CAP3[0]" pad="9"/>
<connect gate="G$1" pin="P0[24]/AD0[1]/I2SRX_WS/CAP3[1]" pad="8"/>
<connect gate="G$1" pin="P0[25]/AD0[2]/I2SRX_SDA/TXD3" pad="7"/>
<connect gate="G$1" pin="P0[26]/AD0[3]/AOUT/RXD3" pad="6"/>
<connect gate="G$1" pin="P0[27]/SDA0/USB_SDA" pad="25"/>
<connect gate="G$1" pin="P0[28]/SCL0/USB_SCL" pad="24"/>
<connect gate="G$1" pin="P0[29]/USB_D+" pad="29"/>
<connect gate="G$1" pin="P0[2]/TXD0/AD0[7]" pad="98"/>
<connect gate="G$1" pin="P0[30]/USB_D-" pad="30"/>
<connect gate="G$1" pin="P0[3]/RXD0/AD0[6]" pad="99"/>
<connect gate="G$1" pin="P0[4]/I2SRX_CLK/RD2/CAP2[0]" pad="81"/>
<connect gate="G$1" pin="P0[5]/I2SRX_WS/TD2/CAP2[1]" pad="80"/>
<connect gate="G$1" pin="P0[6]/I2SRX_SDA/SSEL1/MAT2[0]" pad="79"/>
<connect gate="G$1" pin="P0[7]/I2STX_CLK/SCK1/MAT2[1]" pad="78"/>
<connect gate="G$1" pin="P0[8]/I2STX_WS/MISO1/MAT2[2]" pad="77"/>
<connect gate="G$1" pin="P0[9]/I2STX_SDA/MOSI1/MAT2[3]" pad="76"/>
<connect gate="G$1" pin="P1[0]/ENET_TXD0" pad="95"/>
<connect gate="G$1" pin="P1[10]/ENET_RXD1" pad="90"/>
<connect gate="G$1" pin="P1[14]/ENET_RX_ER" pad="89"/>
<connect gate="G$1" pin="P1[15]/ENET_REF_CLK" pad="88"/>
<connect gate="G$1" pin="P1[16]/ENET_MDC" pad="87"/>
<connect gate="G$1" pin="P1[17]/ENET_MDIO" pad="86"/>
<connect gate="G$1" pin="P1[18]/USB_UP_LED/PWM1[1]/CAP1[0]" pad="32"/>
<connect gate="G$1" pin="P1[19]/MC0A/USB_PPWR/CAP1[1]" pad="33"/>
<connect gate="G$1" pin="P1[1]/ENET_TXD1" pad="94"/>
<connect gate="G$1" pin="P1[20]/MCFB0/PWM1[2]/SCK0" pad="34"/>
<connect gate="G$1" pin="P1[21]/MCABORT/PWM1[3]/SSEL0" pad="35"/>
<connect gate="G$1" pin="P1[22]/MC0B/USB_PWRD/MAT1[0]" pad="36"/>
<connect gate="G$1" pin="P1[23]/MCFB1/PWM1[4]/MISO0" pad="37"/>
<connect gate="G$1" pin="P1[24]/MCFB2/PWM1[5]/MOSI0" pad="38"/>
<connect gate="G$1" pin="P1[25]/MC1A/MAT1[1]" pad="39"/>
<connect gate="G$1" pin="P1[26]/MC1B/PWM1[6]/CAP0[0]" pad="40"/>
<connect gate="G$1" pin="P1[27]/CLKOUT/USB_OVRCR/CAP0[1]" pad="43"/>
<connect gate="G$1" pin="P1[28]/MC2A/PCAP1[0]/MAT0[0]" pad="44"/>
<connect gate="G$1" pin="P1[29]/MC2B/PCAP1[1]/MAT0[1]" pad="45"/>
<connect gate="G$1" pin="P1[30]/VBUS/AD0[4]" pad="21"/>
<connect gate="G$1" pin="P1[31]/SCK1/AD0[5]" pad="20"/>
<connect gate="G$1" pin="P1[4]/ENET_TX_EN" pad="93"/>
<connect gate="G$1" pin="P1[8]/ENET_CRS" pad="92"/>
<connect gate="G$1" pin="P1[9]/ENET_RXD0" pad="91"/>
<connect gate="G$1" pin="P2[0]/PWM1[1]/TXD1" pad="75"/>
<connect gate="G$1" pin="P2[10]/EINT0/NMI" pad="53"/>
<connect gate="G$1" pin="P2[11]/EINT1/I2STX_CLK" pad="52"/>
<connect gate="G$1" pin="P2[12]/EINT2/I2STX_WS" pad="51"/>
<connect gate="G$1" pin="P2[13]/EINT3/I2STX_SDA" pad="50"/>
<connect gate="G$1" pin="P2[1]/PWM1[2]/RXD1" pad="74"/>
<connect gate="G$1" pin="P2[2]/PWM1[3]/CTS1/TRACEDATA[3]" pad="73"/>
<connect gate="G$1" pin="P2[3]/PWM1[4]/DCD1/TRACEDATA[2]" pad="70"/>
<connect gate="G$1" pin="P2[4]/PWM1[5]/DSR1/TRACEDATA[1]" pad="69"/>
<connect gate="G$1" pin="P2[5]/PWM1[6]/DTR1/TRACEDATA[0]" pad="68"/>
<connect gate="G$1" pin="P2[6]/PCAP1[0]/RI1/TRACECLK" pad="67"/>
<connect gate="G$1" pin="P2[7]/RD2/RTS1" pad="66"/>
<connect gate="G$1" pin="P2[8]/TD2/TXD2" pad="65"/>
<connect gate="G$1" pin="P2[9]/USB_CONNECT/RXD2" pad="64"/>
<connect gate="G$1" pin="P3[25]/MAT0[0]/PWM1[2]" pad="27"/>
<connect gate="G$1" pin="P3[26]/STCLK/MAT0[1]/PWM1[3]" pad="26"/>
<connect gate="G$1" pin="P4[28]/RX_MCLK/MAT2[0]/TXD3" pad="82"/>
<connect gate="G$1" pin="P4[29]/TX_MCLK/MAT2[1]/RXD3" pad="85"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="RSTOUT" pad="14"/>
<connect gate="G$1" pin="RTCK" pad="100"/>
<connect gate="G$1" pin="RTCX1" pad="16"/>
<connect gate="G$1" pin="RTCX2" pad="18"/>
<connect gate="G$1" pin="TCK/SWDCLK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="2"/>
<connect gate="G$1" pin="TDO/SWO" pad="1"/>
<connect gate="G$1" pin="TMS/SWDIO" pad="3"/>
<connect gate="G$1" pin="TRST" pad="4"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD(3V3)1" pad="28"/>
<connect gate="G$1" pin="VDD(3V3)2" pad="54"/>
<connect gate="G$1" pin="VDD(3V3)3" pad="71"/>
<connect gate="G$1" pin="VDD(3V3)4" pad="96"/>
<connect gate="G$1" pin="VDD(REG)(3V3)1" pad="42"/>
<connect gate="G$1" pin="VDD(REG)(3V3)2" pad="84"/>
<connect gate="G$1" pin="VDDA" pad="10"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="31"/>
<connect gate="G$1" pin="VSS2" pad="41"/>
<connect gate="G$1" pin="VSS3" pad="55"/>
<connect gate="G$1" pin="VSS4" pad="72"/>
<connect gate="G$1" pin="VSS5" pad="97"/>
<connect gate="G$1" pin="VSS6" pad="83"/>
<connect gate="G$1" pin="VSSA" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="22"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VIN">
<description>VIN Supply Symbol</description>
<gates>
<gate name="G$1" symbol="VIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848" prefix="U" uservalue="yes">
<description>&lt;b&gt;DP83848 (40-LLP)&lt;/b&gt; - Single Port 10/100 Ethernet Transceiver
&lt;p&gt;Digikey: DP83848JSQCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DP83848"/>
</gates>
<devices>
<device name="" package="LLP40">
<connects>
<connect gate="G$1" pin="AGND1" pad="13"/>
<connect gate="G$1" pin="AGND2" pad="17"/>
<connect gate="G$1" pin="AVDD33" pad="18"/>
<connect gate="G$1" pin="COL/PHYAD0" pad="35"/>
<connect gate="G$1" pin="CRS/CRS_DV/LED_CFG" pad="33"/>
<connect gate="G$1" pin="DGND" pad="29"/>
<connect gate="G$1" pin="GNDPAD" pad="41"/>
<connect gate="G$1" pin="IOGND" pad="40"/>
<connect gate="G$1" pin="IOVDD33(1)" pad="1"/>
<connect gate="G$1" pin="IOVDD33(2)" pad="26"/>
<connect gate="G$1" pin="LED_LINK/AN0" pad="22"/>
<connect gate="G$1" pin="LED_SPEED/AN1" pad="21"/>
<connect gate="G$1" pin="MDC" pad="25"/>
<connect gate="G$1" pin="MDIO" pad="24"/>
<connect gate="G$1" pin="PFBIN1" pad="16"/>
<connect gate="G$1" pin="PFBIN2" pad="30"/>
<connect gate="G$1" pin="PFBOUT" pad="19"/>
<connect gate="G$1" pin="RBIAS" pad="20"/>
<connect gate="G$1" pin="RD+" pad="12"/>
<connect gate="G$1" pin="RD-" pad="11"/>
<connect gate="G$1" pin="RESERVED1" pad="8"/>
<connect gate="G$1" pin="RESERVED2" pad="9"/>
<connect gate="G$1" pin="RESERVED3" pad="10"/>
<connect gate="G$1" pin="RESET_N" pad="23"/>
<connect gate="G$1" pin="RXD_0/PHYAD1" pad="36"/>
<connect gate="G$1" pin="RXD_1/PHYAD1" pad="37"/>
<connect gate="G$1" pin="RXD_2/PHYAD2" pad="38"/>
<connect gate="G$1" pin="RXD_3/PHYAD3" pad="39"/>
<connect gate="G$1" pin="RX_CLK" pad="31"/>
<connect gate="G$1" pin="RX_DV/MII_MODE" pad="32"/>
<connect gate="G$1" pin="RX_ER/MDIX_EN" pad="34"/>
<connect gate="G$1" pin="TD+" pad="15"/>
<connect gate="G$1" pin="TD-" pad="14"/>
<connect gate="G$1" pin="TXD_0" pad="4"/>
<connect gate="G$1" pin="TXD_1" pad="5"/>
<connect gate="G$1" pin="TXD_2" pad="6"/>
<connect gate="G$1" pin="TXD_3" pad="7"/>
<connect gate="G$1" pin="TX_CLK" pad="2"/>
<connect gate="G$1" pin="TX_EN" pad="3"/>
<connect gate="G$1" pin="X1" pad="28"/>
<connect gate="G$1" pin="X2" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSCILLATOR" prefix="OSC" uservalue="yes">
<description>&lt;b&gt;Oscillators&lt;/b&gt;
&lt;p&gt;&lt;b&gt;3.2x2.5mm SMT&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;4.0MHz +/- 50ppm, 3.3V, 9mA, -40/+85°C - Digikey: 535-9752-1-ND&lt;/li&gt;
&lt;li&gt;50MHz +/- 50ppm, 3.3V, 8mA, -10/+70°C - Digikey: 478-4792-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;b&gt;5x7mm SMT&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;4.0MHz +/-20ppm 3.3V, 20mA, -20/+70°C - Digikey: 535-9329-2-ND&lt;/li&gt;
&lt;li&gt;50MHz +/- 25ppm 3.3V, 35mA, -40/+85°C - Digikey: 631-1197-1-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="OSCILLATOR"/>
</gates>
<devices>
<device name="" package="OSC_7X5MM">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="INH" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.2X2.5" package="OSC_3.2X2.5MM">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="INH" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_CFAF240320K-T-TS" prefix="DISPLAY" uservalue="yes">
<description>Footprint courtesy Morten Hjerde</description>
<gates>
<gate name="G$1" symbol="CFAF240320K-T-TS"/>
</gates>
<devices>
<device name="" package="CFAF240320K-T-TS">
<connects>
<connect gate="G$1" pin="!CS" pad="P$7"/>
<connect gate="G$1" pin="!RD" pad="P$10"/>
<connect gate="G$1" pin="!RESET" pad="P$31"/>
<connect gate="G$1" pin="!WR" pad="P$9"/>
<connect gate="G$1" pin="DB0" pad="P$1"/>
<connect gate="G$1" pin="DB1" pad="P$2"/>
<connect gate="G$1" pin="DB10" pad="P$23"/>
<connect gate="G$1" pin="DB11" pad="P$24"/>
<connect gate="G$1" pin="DB12" pad="P$25"/>
<connect gate="G$1" pin="DB13" pad="P$26"/>
<connect gate="G$1" pin="DB14" pad="P$27"/>
<connect gate="G$1" pin="DB15" pad="P$28"/>
<connect gate="G$1" pin="DB16" pad="P$29"/>
<connect gate="G$1" pin="DB17" pad="P$30"/>
<connect gate="G$1" pin="DB2" pad="P$3"/>
<connect gate="G$1" pin="DB3" pad="P$4"/>
<connect gate="G$1" pin="DB4" pad="P$22"/>
<connect gate="G$1" pin="DB5" pad="P$35"/>
<connect gate="G$1" pin="DB6" pad="P$36"/>
<connect gate="G$1" pin="DB7" pad="P$37"/>
<connect gate="G$1" pin="GND" pad="P$34"/>
<connect gate="G$1" pin="GND1" pad="P$5"/>
<connect gate="G$1" pin="IM3" pad="P$21"/>
<connect gate="G$1" pin="IMO" pad="P$11"/>
<connect gate="G$1" pin="IOVCC" pad="P$33"/>
<connect gate="G$1" pin="IOVCC1" pad="P$6"/>
<connect gate="G$1" pin="LED-A" pad="P$16"/>
<connect gate="G$1" pin="LED-K1" pad="P$17"/>
<connect gate="G$1" pin="LED-K2" pad="P$18"/>
<connect gate="G$1" pin="LED-K3" pad="P$19"/>
<connect gate="G$1" pin="LED-K4" pad="P$20"/>
<connect gate="G$1" pin="RS" pad="P$8"/>
<connect gate="G$1" pin="VCI" pad="P$32"/>
<connect gate="G$1" pin="X+" pad="P$12"/>
<connect gate="G$1" pin="X-" pad="P$14"/>
<connect gate="G$1" pin="Y+" pad="P$13"/>
<connect gate="G$1" pin="Y-" pad="P$15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROSD" prefix="CN" uservalue="yes">
<description>&lt;b&gt;MicroSD/Transflash Card Holder with SPI pinout&lt;/b&gt;
&lt;p&gt;3M: 2908-05WB-MG&lt;br/&gt;4UConnector: 19656&lt;/p&gt;
&lt;p&gt;Footprint courtesy: Adafruit Industries&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TRANSFLASH"/>
</gates>
<devices>
<device name="" package="MICROSD">
<connects>
<connect gate="G$1" pin="CARD_DETECT" pad="CD1"/>
<connect gate="G$1" pin="CARD_DETECT1" pad="CD2"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="DATA_IN" pad="3"/>
<connect gate="G$1" pin="DATA_OUT" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="MT2"/>
<connect gate="G$1" pin="GND@2" pad="MT1"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="SD_VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_ILI932X/HX8347_37PIN" prefix="CN" uservalue="yes">
<description>&lt;p&gt;37-pin 2.8" 240x320 Displays based on ILI9325/ILI9328/HX8347 Controllers&lt;/p&gt;
&lt;p&gt;Make sure to double-check the footprint against any LCD since there are dozens of varieties, but this footprint uses a relatively common 37-pin layout for ILI9325, ILI9328 or HX9347 240x320 LCD displays.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ILI9325_LCD"/>
</gates>
<devices>
<device name="OUTLINE" package="ILI9325_28INCH_TS_OUTLINE">
<connects>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="!RD" pad="10"/>
<connect gate="G$1" pin="!RESET" pad="31"/>
<connect gate="G$1" pin="!WR" pad="9"/>
<connect gate="G$1" pin="DB0" pad="1"/>
<connect gate="G$1" pin="DB1" pad="2"/>
<connect gate="G$1" pin="DB10/DB8" pad="23"/>
<connect gate="G$1" pin="DB11/DB9" pad="24"/>
<connect gate="G$1" pin="DB12/DB10" pad="25"/>
<connect gate="G$1" pin="DB13/DB11" pad="26"/>
<connect gate="G$1" pin="DB14/DB12" pad="27"/>
<connect gate="G$1" pin="DB15/DB13" pad="28"/>
<connect gate="G$1" pin="DB16/DB14" pad="29"/>
<connect gate="G$1" pin="DB17/DB15" pad="30"/>
<connect gate="G$1" pin="DB2" pad="3"/>
<connect gate="G$1" pin="DB3" pad="4"/>
<connect gate="G$1" pin="DB4" pad="22"/>
<connect gate="G$1" pin="DB5" pad="35"/>
<connect gate="G$1" pin="DB6" pad="36"/>
<connect gate="G$1" pin="DB7" pad="37"/>
<connect gate="G$1" pin="GND" pad="34"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="IM3" pad="21"/>
<connect gate="G$1" pin="IMO" pad="11"/>
<connect gate="G$1" pin="IOVCC" pad="33"/>
<connect gate="G$1" pin="IOVCC1" pad="6"/>
<connect gate="G$1" pin="LED-A" pad="16"/>
<connect gate="G$1" pin="LED-K1" pad="17"/>
<connect gate="G$1" pin="LED-K2" pad="18"/>
<connect gate="G$1" pin="LED-K3" pad="19"/>
<connect gate="G$1" pin="LED-K4" pad="20"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="VCI" pad="32"/>
<connect gate="G$1" pin="X+" pad="12"/>
<connect gate="G$1" pin="X-" pad="14"/>
<connect gate="G$1" pin="Y+" pad="13"/>
<connect gate="G$1" pin="Y-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VBAT">
<description>VBAT Supply Sumbol</description>
<gates>
<gate name="G$1" symbol="VBAT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_6PIN" prefix="CN" uservalue="yes">
<description>JST 6-Pin Right-Angle Connector</description>
<gates>
<gate name="G$1" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="JSTPH6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_3PIN" prefix="CN" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="JSTPH3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="S1D13743" prefix="U" uservalue="yes">
<description>Epson S1D13743 Mobile Graphics Engine with 464K Internal SRAM</description>
<gates>
<gate name="G$1" symbol="S1D13743"/>
</gates>
<devices>
<device name="" package="LQFP144">
<connects>
<connect gate="G$1" pin="CLKI" pad="115"/>
<connect gate="G$1" pin="CLKOUT" pad="110"/>
<connect gate="G$1" pin="CLKOUTEN" pad="112"/>
<connect gate="G$1" pin="CNF0" pad="78"/>
<connect gate="G$1" pin="CNF1" pad="77"/>
<connect gate="G$1" pin="CNF2" pad="76"/>
<connect gate="G$1" pin="COREVDD1" pad="6"/>
<connect gate="G$1" pin="COREVDD2" pad="26"/>
<connect gate="G$1" pin="COREVDD3" pad="41"/>
<connect gate="G$1" pin="COREVDD4" pad="52"/>
<connect gate="G$1" pin="COREVDD5" pad="64"/>
<connect gate="G$1" pin="COREVDD6" pad="74"/>
<connect gate="G$1" pin="COREVDD7" pad="95"/>
<connect gate="G$1" pin="COREVDD8" pad="114"/>
<connect gate="G$1" pin="COREVDD9" pad="133"/>
<connect gate="G$1" pin="CS#" pad="130"/>
<connect gate="G$1" pin="D/C#" pad="144"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="GPIO0" pad="84"/>
<connect gate="G$1" pin="GPIO1" pad="83"/>
<connect gate="G$1" pin="GPIO2" pad="82"/>
<connect gate="G$1" pin="GPIO3" pad="81"/>
<connect gate="G$1" pin="GPIO4" pad="72"/>
<connect gate="G$1" pin="GPIO5" pad="71"/>
<connect gate="G$1" pin="GPIO6" pad="67"/>
<connect gate="G$1" pin="GPIO7" pad="66"/>
<connect gate="G$1" pin="GPIO_INT" pad="101"/>
<connect gate="G$1" pin="HS" pad="4"/>
<connect gate="G$1" pin="IOVDD1" pad="68"/>
<connect gate="G$1" pin="IOVDD2" pad="79"/>
<connect gate="G$1" pin="IOVDD3" pad="85"/>
<connect gate="G$1" pin="IOVDD4" pad="91"/>
<connect gate="G$1" pin="IOVDD5" pad="100"/>
<connect gate="G$1" pin="IOVDD6" pad="105"/>
<connect gate="G$1" pin="IOVDD7" pad="128"/>
<connect gate="G$1" pin="IOVDD8" pad="119"/>
<connect gate="G$1" pin="IOVDD9" pad="139"/>
<connect gate="G$1" pin="MD0" pad="106"/>
<connect gate="G$1" pin="MD1" pad="108"/>
<connect gate="G$1" pin="MD10" pad="143"/>
<connect gate="G$1" pin="MD11" pad="103"/>
<connect gate="G$1" pin="MD12" pad="102"/>
<connect gate="G$1" pin="MD13" pad="124"/>
<connect gate="G$1" pin="MD14" pad="126"/>
<connect gate="G$1" pin="MD15" pad="131"/>
<connect gate="G$1" pin="MD2" pad="107"/>
<connect gate="G$1" pin="MD3" pad="125"/>
<connect gate="G$1" pin="MD4" pad="127"/>
<connect gate="G$1" pin="MD5" pad="132"/>
<connect gate="G$1" pin="MD6" pad="135"/>
<connect gate="G$1" pin="MD7" pad="138"/>
<connect gate="G$1" pin="MD8" pad="136"/>
<connect gate="G$1" pin="MD9" pad="141"/>
<connect gate="G$1" pin="NC1" pad="11"/>
<connect gate="G$1" pin="NC10" pad="31"/>
<connect gate="G$1" pin="NC11" pad="32"/>
<connect gate="G$1" pin="NC12" pad="33"/>
<connect gate="G$1" pin="NC13" pad="34"/>
<connect gate="G$1" pin="NC14" pad="35"/>
<connect gate="G$1" pin="NC15" pad="36"/>
<connect gate="G$1" pin="NC16" pad="37"/>
<connect gate="G$1" pin="NC17" pad="73"/>
<connect gate="G$1" pin="NC18" pad="88"/>
<connect gate="G$1" pin="NC19" pad="109"/>
<connect gate="G$1" pin="NC2" pad="16"/>
<connect gate="G$1" pin="NC20" pad="111"/>
<connect gate="G$1" pin="NC21" pad="117"/>
<connect gate="G$1" pin="NC22" pad="118"/>
<connect gate="G$1" pin="NC23" pad="123"/>
<connect gate="G$1" pin="NC3" pad="17"/>
<connect gate="G$1" pin="NC4" pad="22"/>
<connect gate="G$1" pin="NC5" pad="23"/>
<connect gate="G$1" pin="NC6" pad="24"/>
<connect gate="G$1" pin="NC7" pad="25"/>
<connect gate="G$1" pin="NC8" pad="29"/>
<connect gate="G$1" pin="NC9" pad="30"/>
<connect gate="G$1" pin="PCLK" pad="8"/>
<connect gate="G$1" pin="PIOVDD1" pad="1"/>
<connect gate="G$1" pin="PIOVDD2" pad="9"/>
<connect gate="G$1" pin="PIOVDD3" pad="18"/>
<connect gate="G$1" pin="PIOVDD4" pad="28"/>
<connect gate="G$1" pin="PIOVDD5" pad="46"/>
<connect gate="G$1" pin="PIOVDD6" pad="58"/>
<connect gate="G$1" pin="PLLVDD" pad="120"/>
<connect gate="G$1" pin="PLLVSS" pad="122"/>
<connect gate="G$1" pin="PWRSAVE" pad="70"/>
<connect gate="G$1" pin="RD#" pad="142"/>
<connect gate="G$1" pin="RESET#" pad="97"/>
<connect gate="G$1" pin="SCANEN" pad="87"/>
<connect gate="G$1" pin="TE" pad="98"/>
<connect gate="G$1" pin="TEST0" pad="93"/>
<connect gate="G$1" pin="TEST1" pad="90"/>
<connect gate="G$1" pin="TEST2" pad="89"/>
<connect gate="G$1" pin="TESTEN" pad="94"/>
<connect gate="G$1" pin="VCP" pad="121"/>
<connect gate="G$1" pin="VD0" pad="39"/>
<connect gate="G$1" pin="VD1" pad="43"/>
<connect gate="G$1" pin="VD10" pad="48"/>
<connect gate="G$1" pin="VD11" pad="51"/>
<connect gate="G$1" pin="VD12" pad="56"/>
<connect gate="G$1" pin="VD13" pad="61"/>
<connect gate="G$1" pin="VD14" pad="15"/>
<connect gate="G$1" pin="VD15" pad="14"/>
<connect gate="G$1" pin="VD16" pad="20"/>
<connect gate="G$1" pin="VD17" pad="40"/>
<connect gate="G$1" pin="VD18" pad="45"/>
<connect gate="G$1" pin="VD19" pad="50"/>
<connect gate="G$1" pin="VD2" pad="49"/>
<connect gate="G$1" pin="VD20" pad="55"/>
<connect gate="G$1" pin="VD21" pad="60"/>
<connect gate="G$1" pin="VD22" pad="13"/>
<connect gate="G$1" pin="VD23" pad="12"/>
<connect gate="G$1" pin="VD3" pad="54"/>
<connect gate="G$1" pin="VD4" pad="57"/>
<connect gate="G$1" pin="VD5" pad="62"/>
<connect gate="G$1" pin="VD6" pad="63"/>
<connect gate="G$1" pin="VD7" pad="21"/>
<connect gate="G$1" pin="VD8" pad="38"/>
<connect gate="G$1" pin="VD9" pad="44"/>
<connect gate="G$1" pin="VS" pad="5"/>
<connect gate="G$1" pin="VSS1" pad="2"/>
<connect gate="G$1" pin="VSS10" pad="10"/>
<connect gate="G$1" pin="VSS11" pad="27"/>
<connect gate="G$1" pin="VSS12" pad="75"/>
<connect gate="G$1" pin="VSS13" pad="80"/>
<connect gate="G$1" pin="VSS14" pad="86"/>
<connect gate="G$1" pin="VSS15" pad="92"/>
<connect gate="G$1" pin="VSS16" pad="96"/>
<connect gate="G$1" pin="VSS17" pad="99"/>
<connect gate="G$1" pin="VSS18" pad="104"/>
<connect gate="G$1" pin="VSS19" pad="113"/>
<connect gate="G$1" pin="VSS2" pad="7"/>
<connect gate="G$1" pin="VSS20" pad="116"/>
<connect gate="G$1" pin="VSS21" pad="129"/>
<connect gate="G$1" pin="VSS22" pad="134"/>
<connect gate="G$1" pin="VSS23" pad="140"/>
<connect gate="G$1" pin="VSS3" pad="19"/>
<connect gate="G$1" pin="VSS4" pad="42"/>
<connect gate="G$1" pin="VSS5" pad="47"/>
<connect gate="G$1" pin="VSS6" pad="53"/>
<connect gate="G$1" pin="VSS7" pad="59"/>
<connect gate="G$1" pin="VSS8" pad="65"/>
<connect gate="G$1" pin="VSS9" pad="69"/>
<connect gate="G$1" pin="WE#" pad="137"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X28" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD28"/>
</gates>
<devices>
<device name="" package="1X28_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.5V">
<gates>
<gate name="G$1" symbol="1.5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO">
<description>&lt;b&gt;Arduino Diecimila/Duemilanove&lt;/b&gt;
&lt;p&gt;
Make a shield with ease, this package has all the named pins as well as the two mounting drill holes and an outline of the USB and DC power connector. The outline is on the DIMENSION layer, so if your board house uses it they will cut the outline to match.
&lt;p&gt;
http://www.ladyada.net/library/pcb/eaglelibrary.html</description>
<gates>
<gate name="G$1" symbol="ARDUINO"/>
</gates>
<devices>
<device name="DUEMILANOVE" package="ARDUINO">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DUEMILANOVE-NOHOLES" package="ARDUINO-NOHOLE">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DUEMILANOVE-NODIM" package="ARDUINO-NODIM">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT232RL-FULL" prefix="IC">
<description>&lt;b&gt;USB UART&lt;/b&gt;
FT232RL 4 - Complete Pinout 

&lt;p&gt;Footprint courtesy Spark Fun Electronics&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FT232R"/>
</gates>
<devices>
<device name="SSOP" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CTS" pad="11"/>
<connect gate="G$1" pin="DCD" pad="10"/>
<connect gate="G$1" pin="DSR" pad="9"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND18" pad="18"/>
<connect gate="G$1" pin="GND21" pad="21"/>
<connect gate="G$1" pin="GND7" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWREN/CBUS3" pad="14"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="RXLED/CBUS1" pad="22"/>
<connect gate="G$1" pin="SLEEP/CBUS4" pad="12"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXDEN/CBUS2" pad="13"/>
<connect gate="G$1" pin="TXLED/CBUS0" pad="23"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBED" prefix="IC">
<description>mbed Microcontroller, DIP40, 0.9"</description>
<gates>
<gate name="G$1" symbol="MBED40"/>
</gates>
<devices>
<device name="" package="DIL40_0.9">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC3130/1_LPC3141/3" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC3130/LPC3131&lt;/b&gt; - 180MHz ARM926EJ-S CPU with 96KB (LPC3130) or 192KB (LPC3131) SRAM&lt;br/&gt;
&lt;b&gt;LPC3141&lt;/b&gt; - 270MHz ARM926EJ-S CPU with 192KB SRAM&lt;br/&gt; 
&lt;b&gt;LPC3143&lt;/b&gt; - 270MHz ARM926EJ-S CPU with 192KB SRAM and AES decryption engine/128-bit unique ID (LPC3143 only)</description>
<gates>
<gate name="G$1" symbol="LPC313X/314X_0"/>
<gate name="G$2" symbol="LPC313X/314X_1"/>
<gate name="G$3" symbol="LPC313X/314X_2"/>
</gates>
<devices>
<device name="" package="TFBGA180_0.8">
<connects>
<connect gate="G$1" pin="ADC10B_GNDA" pad="A12"/>
<connect gate="G$1" pin="ADC10B_VDDA33" pad="A13"/>
<connect gate="G$1" pin="VDDA12_0" pad="D11"/>
<connect gate="G$1" pin="VDDA12_1" pad="E10"/>
<connect gate="G$1" pin="VDDE_IOA_0" pad="B2"/>
<connect gate="G$1" pin="VDDE_IOA_1" pad="E5"/>
<connect gate="G$1" pin="VDDE_IOA_2" pad="F5"/>
<connect gate="G$1" pin="VDDE_IOA_3" pad="G5"/>
<connect gate="G$1" pin="VDDE_IOA_4" pad="H5"/>
<connect gate="G$1" pin="VDDE_IOB_0" pad="L4"/>
<connect gate="G$1" pin="VDDE_IOB_1" pad="M5"/>
<connect gate="G$1" pin="VDDE_IOB_2" pad="M7"/>
<connect gate="G$1" pin="VDDE_IOB_3" pad="M9"/>
<connect gate="G$1" pin="VDDE_IOC_1" pad="C13"/>
<connect gate="G$1" pin="VDDE_IOC_2" pad="D5"/>
<connect gate="G$1" pin="VDDE_IOC_3" pad="D7"/>
<connect gate="G$1" pin="VDDE_IOC_4" pad="E8"/>
<connect gate="G$1" pin="VDDE_IOC_5" pad="G12"/>
<connect gate="G$1" pin="VDDE_IOC_6" pad="L10"/>
<connect gate="G$1" pin="VDDE_IOC_7" pad="K11"/>
<connect gate="G$1" pin="VDDI_0" pad="H3"/>
<connect gate="G$1" pin="VDDI_1" pad="L7"/>
<connect gate="G$1" pin="VDDI_2" pad="L12"/>
<connect gate="G$1" pin="VDDI_3" pad="C6"/>
<connect gate="G$1" pin="VDDI_4" pad="C12"/>
<connect gate="G$1" pin="VPP_0" pad="A9"/>
<connect gate="G$1" pin="VPP_1" pad="C9"/>
<connect gate="G$1" pin="VSSA12" pad="E9"/>
<connect gate="G$1" pin="VSSE_IOA_0" pad="C3"/>
<connect gate="G$1" pin="VSSE_IOA_1" pad="C4"/>
<connect gate="G$1" pin="VSSE_IOA_2" pad="E4"/>
<connect gate="G$1" pin="VSSE_IOA_3" pad="F4"/>
<connect gate="G$1" pin="VSSE_IOA_4" pad="H4"/>
<connect gate="G$1" pin="VSSE_IOA_5" pad="K3"/>
<connect gate="G$1" pin="VSSE_IOB_0" pad="M3"/>
<connect gate="G$1" pin="VSSE_IOB_1" pad="M4"/>
<connect gate="G$1" pin="VSSE_IOB_2" pad="M6"/>
<connect gate="G$1" pin="VSSE_IOB_3" pad="M8"/>
<connect gate="G$1" pin="VSSE_IOC_0" pad="B12"/>
<connect gate="G$1" pin="VSSE_IOC_1" pad="D6"/>
<connect gate="G$1" pin="VSSE_IOC_2" pad="D8"/>
<connect gate="G$1" pin="VSSE_IOC_3" pad="D9"/>
<connect gate="G$1" pin="VSSE_IOC_4" pad="G11"/>
<connect gate="G$1" pin="VSSE_IOC_5" pad="L9"/>
<connect gate="G$1" pin="VSSE_IOC_6" pad="L13"/>
<connect gate="G$1" pin="VSSI_0" pad="A11"/>
<connect gate="G$1" pin="VSSI_1" pad="C7"/>
<connect gate="G$1" pin="VSSI_2" pad="D12"/>
<connect gate="G$1" pin="VSSI_3" pad="G4"/>
<connect gate="G$1" pin="VSSI_4" pad="L6"/>
<connect gate="G$1" pin="VSSI_5" pad="L11"/>
<connect gate="G$2" pin="ADC10B_GPA0" pad="B14"/>
<connect gate="G$2" pin="ADC10B_GPA1" pad="A14"/>
<connect gate="G$2" pin="ADC10B_GPA2" pad="B13"/>
<connect gate="G$2" pin="ADC10B_GPA3" pad="C14"/>
<connect gate="G$2" pin="ARM_TDO" pad="E11"/>
<connect gate="G$2" pin="BUF_TCK" pad="D13"/>
<connect gate="G$2" pin="BUF_TMS" pad="D14"/>
<connect gate="G$2" pin="BUF_TRST_N" pad="F11"/>
<connect gate="G$2" pin="CLK_256FS_O" pad="H12"/>
<connect gate="G$2" pin="CLOCK_OUT" pad="J4"/>
<connect gate="G$2" pin="FFAST_IN" pad="A10"/>
<connect gate="G$2" pin="FFAST_OUT" pad="B10"/>
<connect gate="G$2" pin="GPIO0" pad="K10"/>
<connect gate="G$2" pin="GPIO1" pad="J10"/>
<connect gate="G$2" pin="GPIO11" pad="H13"/>
<connect gate="G$2" pin="GPIO12" pad="H10"/>
<connect gate="G$2" pin="GPIO13" pad="J12"/>
<connect gate="G$2" pin="GPIO14" pad="J14"/>
<connect gate="G$2" pin="GPIO15" pad="J13"/>
<connect gate="G$2" pin="GPIO16" pad="J11"/>
<connect gate="G$2" pin="GPIO17" pad="K12"/>
<connect gate="G$2" pin="GPIO18" pad="K14"/>
<connect gate="G$2" pin="GPIO19" pad="H11"/>
<connect gate="G$2" pin="GPIO2" pad="L14"/>
<connect gate="G$2" pin="GPIO20" pad="K13"/>
<connect gate="G$2" pin="GPIO3" pad="B11"/>
<connect gate="G$2" pin="GPIO4" pad="C11"/>
<connect gate="G$2" pin="I2C_SCL0" pad="D10"/>
<connect gate="G$2" pin="I2C_SCL1" pad="E13"/>
<connect gate="G$2" pin="I2C_SDA0" pad="C10"/>
<connect gate="G$2" pin="I2C_SDA1" pad="E12"/>
<connect gate="G$2" pin="I2SRX_BCK0" pad="N10"/>
<connect gate="G$2" pin="I2SRX_BCK1" pad="F14"/>
<connect gate="G$2" pin="I2SRX_DATA0" pad="M10"/>
<connect gate="G$2" pin="I2SRX_DATA1" pad="G14"/>
<connect gate="G$2" pin="I2SRX_WS0" pad="P11"/>
<connect gate="G$2" pin="I2SRX_WS1" pad="F13"/>
<connect gate="G$2" pin="I2STX_BCK0/IPINT_FSC" pad="M12"/>
<connect gate="G$2" pin="I2STX_BCK1" pad="E14"/>
<connect gate="G$2" pin="I2STX_CLK0/IPINT_DB" pad="N14"/>
<connect gate="G$2" pin="I2STX_DATA0/IPINT_DA" pad="M13"/>
<connect gate="G$2" pin="I2STX_DATA1" pad="F12"/>
<connect gate="G$2" pin="I2STX_WS0/IPINT_DCK" pad="M11"/>
<connect gate="G$2" pin="I2STX_WS1" pad="G10"/>
<connect gate="G$2" pin="JTAGSEL" pad="N11"/>
<connect gate="G$2" pin="MGPIO10/MCI_DAT3" pad="A4"/>
<connect gate="G$2" pin="MGPIO5/MCI_CLK" pad="B6"/>
<connect gate="G$2" pin="MGPIO6/MCI_CMD" pad="A6"/>
<connect gate="G$2" pin="MGPIO7/MCI_DAT0" pad="A5"/>
<connect gate="G$2" pin="MGPIO8/MCI_DAT1" pad="B5"/>
<connect gate="G$2" pin="MGPIO9/MCI_DAT2" pad="C5"/>
<connect gate="G$2" pin="MUART_CTS_N/SPI_CS_OUT1" pad="N13"/>
<connect gate="G$2" pin="MUART_RTS_N/SPI_CS_OUT2" pad="P14"/>
<connect gate="G$2" pin="PWM_DATA" pad="B9"/>
<connect gate="G$2" pin="RSTIN_N" pad="H14"/>
<connect gate="G$2" pin="SCAN_TDO" pad="F10"/>
<connect gate="G$2" pin="SPI_CS_IN" pad="B8"/>
<connect gate="G$2" pin="SPI_CS_OUT0" pad="A7"/>
<connect gate="G$2" pin="SPI_MISO" pad="C8"/>
<connect gate="G$2" pin="SPI_MOSI" pad="B7"/>
<connect gate="G$2" pin="SPI_SCK" pad="A8"/>
<connect gate="G$2" pin="SYSCLK_O" pad="G13"/>
<connect gate="G$2" pin="TCK" pad="M14"/>
<connect gate="G$2" pin="TDI" pad="K9"/>
<connect gate="G$2" pin="TMS" pad="P10"/>
<connect gate="G$2" pin="TRST_N" pad="P13"/>
<connect gate="G$2" pin="UART_RXD" pad="P12"/>
<connect gate="G$2" pin="UART_TXD" pad="N12"/>
<connect gate="G$2" pin="USB_DM" pad="N2"/>
<connect gate="G$2" pin="USB_DP" pad="P2"/>
<connect gate="G$2" pin="USB_GNDA" pad="N1"/>
<connect gate="G$2" pin="USB_ID" pad="M1"/>
<connect gate="G$2" pin="USB_RREF" pad="J5"/>
<connect gate="G$2" pin="USB_VBUS" pad="L2"/>
<connect gate="G$2" pin="USB_VDDA12_PLL" pad="L1"/>
<connect gate="G$2" pin="USB_VDDA33" pad="P1"/>
<connect gate="G$2" pin="USB_VDDA33_DRV" pad="M2"/>
<connect gate="G$2" pin="USB_VSSA_REF" pad="K4"/>
<connect gate="G$2" pin="USB_VSSA_TERM" pad="L3"/>
<connect gate="G$3" pin="EBI_A0/ALE" pad="B3"/>
<connect gate="G$3" pin="EBI_A1/CLE" pad="A2"/>
<connect gate="G$3" pin="EBI_D0" pad="G2"/>
<connect gate="G$3" pin="EBI_D1" pad="F2"/>
<connect gate="G$3" pin="EBI_D10" pad="A1"/>
<connect gate="G$3" pin="EBI_D11" pad="C2"/>
<connect gate="G$3" pin="EBI_D12" pad="G3"/>
<connect gate="G$3" pin="EBI_D13" pad="D3"/>
<connect gate="G$3" pin="EBI_D14" pad="E3"/>
<connect gate="G$3" pin="EBI_D15" pad="F3"/>
<connect gate="G$3" pin="EBI_D2" pad="F1"/>
<connect gate="G$3" pin="EBI_D3" pad="E1"/>
<connect gate="G$3" pin="EBI_D4" pad="E2"/>
<connect gate="G$3" pin="EBI_D5" pad="D1"/>
<connect gate="G$3" pin="EBI_D6" pad="D2"/>
<connect gate="G$3" pin="EBI_D7" pad="C1"/>
<connect gate="G$3" pin="EBI_D8" pad="B1"/>
<connect gate="G$3" pin="EBI_D9" pad="A3"/>
<connect gate="G$3" pin="EBI_DQM0/NOE" pad="H1"/>
<connect gate="G$3" pin="EBI_NCAS/BLOUT0" pad="G1"/>
<connect gate="G$3" pin="EBI_NRAS/BLOUT1" pad="H2"/>
<connect gate="G$3" pin="EBI_NWE" pad="J2"/>
<connect gate="G$3" pin="MLCD_CSB/EBI_NSTCS0" pad="K8"/>
<connect gate="G$3" pin="MLCD_DB0/EBI_CLKOUT" pad="N8"/>
<connect gate="G$3" pin="MLCD_DB1/EBI_NSTCS1" pad="P9"/>
<connect gate="G$3" pin="MLCD_DB10(8B2)/EBI_A10" pad="K7"/>
<connect gate="G$3" pin="MLCD_DB11(8B3)/EBI_A11" pad="N4"/>
<connect gate="G$3" pin="MLCD_DB12(8B4)/EBI_A12" pad="K5"/>
<connect gate="G$3" pin="MLCD_DB13(8B5)/EBI_A13" pad="P4"/>
<connect gate="G$3" pin="MLCD_DB14(8B6)/EBI_A14" pad="P3"/>
<connect gate="G$3" pin="MLCD_DB15(8B7)/EBI_A15" pad="N3"/>
<connect gate="G$3" pin="MLCD_DB2/EBI_A2" pad="N6"/>
<connect gate="G$3" pin="MLCD_DB3/EBI_A3" pad="P6"/>
<connect gate="G$3" pin="MLCD_DB4/EBI_A4" pad="N7"/>
<connect gate="G$3" pin="MLCD_DB5/EBI_A5" pad="P7"/>
<connect gate="G$3" pin="MLCD_DB6/EBI_A6" pad="K6"/>
<connect gate="G$3" pin="MLCD_DB7/EBI_A7" pad="P5"/>
<connect gate="G$3" pin="MLCD_DB8(8B0)/EBI_A8" pad="N5"/>
<connect gate="G$3" pin="MLCD_DB9(8B1)/EBI_A9" pad="L5"/>
<connect gate="G$3" pin="MLCD_E_RD/EBI_CKE" pad="L8"/>
<connect gate="G$3" pin="MLCD_RS/EBI_NDYCS" pad="P8"/>
<connect gate="G$3" pin="MLCD_RW_WR/EBI_DQM1" pad="N9"/>
<connect gate="G$3" pin="MNAND_RYBN0/MCI_DAT4" pad="E6"/>
<connect gate="G$3" pin="MNAND_RYBN1/MCI_DAT5" pad="E7"/>
<connect gate="G$3" pin="MNAND_RYBN2/MCI_DAT6" pad="B4"/>
<connect gate="G$3" pin="MNAND_RYBN3/MCI_DAT7" pad="D4"/>
<connect gate="G$3" pin="NAND_NCS0" pad="J1"/>
<connect gate="G$3" pin="NAND_NCS1" pad="J3"/>
<connect gate="G$3" pin="NAND_NCS2" pad="K1"/>
<connect gate="G$3" pin="NAND_NCS3" pad="K2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDRAM_MT48H32M16LF" prefix="U" uservalue="yes">
<description>&lt;b&gt;MT48H32M16LF&lt;/b&gt; - Mobile Low-Power SDR SDRAM
&lt;p&gt;512MBits (8 Meg x 16 x 4 banks)&lt;br/&gt;
1.8V, 133MHz, -40°C-85°C&lt;/p&gt;
&lt;p&gt;Digikey: 557-1389-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MT48H32M16LF"/>
</gates>
<devices>
<device name="" package="VFBGA54">
<connects>
<connect gate="G$1" pin="A0" pad="H7"/>
<connect gate="G$1" pin="A1" pad="H8"/>
<connect gate="G$1" pin="A10" pad="H9"/>
<connect gate="G$1" pin="A11" pad="G2"/>
<connect gate="G$1" pin="A12" pad="G1"/>
<connect gate="G$1" pin="A2" pad="J8"/>
<connect gate="G$1" pin="A3" pad="J7"/>
<connect gate="G$1" pin="A4" pad="J3"/>
<connect gate="G$1" pin="A5" pad="J2"/>
<connect gate="G$1" pin="A6" pad="H3"/>
<connect gate="G$1" pin="A7" pad="H2"/>
<connect gate="G$1" pin="A8" pad="H1"/>
<connect gate="G$1" pin="A9" pad="G3"/>
<connect gate="G$1" pin="BA0" pad="G7"/>
<connect gate="G$1" pin="BA1" pad="G8"/>
<connect gate="G$1" pin="CAS" pad="F7"/>
<connect gate="G$1" pin="CKE" pad="F3"/>
<connect gate="G$1" pin="CLK" pad="F2"/>
<connect gate="G$1" pin="CS" pad="G9"/>
<connect gate="G$1" pin="D0" pad="A8"/>
<connect gate="G$1" pin="D1" pad="B9"/>
<connect gate="G$1" pin="D10" pad="D1"/>
<connect gate="G$1" pin="D11" pad="C2"/>
<connect gate="G$1" pin="D12" pad="C1"/>
<connect gate="G$1" pin="D13" pad="B2"/>
<connect gate="G$1" pin="D14" pad="B1"/>
<connect gate="G$1" pin="D15" pad="A2"/>
<connect gate="G$1" pin="D2" pad="B8"/>
<connect gate="G$1" pin="D3" pad="C9"/>
<connect gate="G$1" pin="D4" pad="C8"/>
<connect gate="G$1" pin="D5" pad="D9"/>
<connect gate="G$1" pin="D6" pad="D8"/>
<connect gate="G$1" pin="D7" pad="E9"/>
<connect gate="G$1" pin="D8" pad="E1"/>
<connect gate="G$1" pin="D9" pad="D2"/>
<connect gate="G$1" pin="DQMH" pad="F1"/>
<connect gate="G$1" pin="DQML" pad="E8"/>
<connect gate="G$1" pin="NC" pad="E2"/>
<connect gate="G$1" pin="RAS" pad="F8"/>
<connect gate="G$1" pin="VDD1" pad="J9"/>
<connect gate="G$1" pin="VDD2" pad="E7"/>
<connect gate="G$1" pin="VDD3" pad="A9"/>
<connect gate="G$1" pin="VDDQ1" pad="A7"/>
<connect gate="G$1" pin="VDDQ2" pad="B3"/>
<connect gate="G$1" pin="VDDQ3" pad="C7"/>
<connect gate="G$1" pin="VDDQ4" pad="D3"/>
<connect gate="G$1" pin="VSS1" pad="J1"/>
<connect gate="G$1" pin="VSS2" pad="E3"/>
<connect gate="G$1" pin="VSS3" pad="A1"/>
<connect gate="G$1" pin="VSSQ1" pad="A3"/>
<connect gate="G$1" pin="VSSQ2" pad="B7"/>
<connect gate="G$1" pin="VSSQ3" pad="C3"/>
<connect gate="G$1" pin="VSSQ4" pad="D7"/>
<connect gate="G$1" pin="WE" pad="F9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC3554" prefix="U" uservalue="yes">
<description>&lt;b&gt;LTC3554&lt;/b&gt; - USB Power Manager with Li-Ion Charger and Two Step-Down Regulators
&lt;p&gt;The LTC3554 is a micropower, highly integrated power management and battery charger IC for single-cell Li-Ion/Polymer battery applications.  The LTC3554 also includes two synchronous step-down switching regulators as well as a pushbutton controller.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LTC3554"/>
</gates>
<devices>
<device name="" package="QFN20_3MM">
<connects>
<connect gate="G$1" pin="/CHRG" pad="14"/>
<connect gate="G$1" pin="/ON" pad="5"/>
<connect gate="G$1" pin="BAT" pad="17"/>
<connect gate="G$1" pin="BVIN" pad="12"/>
<connect gate="G$1" pin="FB1" pad="6"/>
<connect gate="G$1" pin="FB2" pad="7"/>
<connect gate="G$1" pin="FSEL" pad="2"/>
<connect gate="G$1" pin="HPWR" pad="1"/>
<connect gate="G$1" pin="NTC" pad="15"/>
<connect gate="G$1" pin="PBSTAT" pad="3"/>
<connect gate="G$1" pin="PGOOD" pad="4"/>
<connect gate="G$1" pin="PROG" pad="16"/>
<connect gate="G$1" pin="PWR_ON1" pad="9"/>
<connect gate="G$1" pin="PWR_ON2" pad="8"/>
<connect gate="G$1" pin="STBY" pad="10"/>
<connect gate="G$1" pin="SUSP" pad="19"/>
<connect gate="G$1" pin="SW1" pad="13"/>
<connect gate="G$1" pin="SW2" pad="11"/>
<connect gate="G$1" pin="THERM_GND" pad="21"/>
<connect gate="G$1" pin="VBUS" pad="20"/>
<connect gate="G$1" pin="VOUT" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.2V">
<gates>
<gate name="G$1" symbol="1.2V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_MIC5387" prefix="U" uservalue="yes">
<description>&lt;b&gt;MIC5387&lt;/b&gt; - Triple Output Linear LDO Regulator
&lt;p&gt;150ma Output on each LDO, 180mV Vf, 2.5-5.5V Input&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;3.3V, 1.8V, 1.2V - Digikey: 576-3689-1-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MIC5387"/>
</gates>
<devices>
<device name="" package="TMLF-6">
<connects>
<connect gate="G$1" pin="EN2/3" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="OUT3" pad="4"/>
<connect gate="G$1" pin="THERM" pad="THERM"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT2232D">
<gates>
<gate name="G$1" symbol="FT2232D"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="ACBUS0" pad="15"/>
<connect gate="G$1" pin="ACBUS1" pad="13"/>
<connect gate="G$1" pin="ACBUS2" pad="12"/>
<connect gate="G$1" pin="ACBUS3" pad="11"/>
<connect gate="G$1" pin="ADBUS0" pad="24"/>
<connect gate="G$1" pin="ADBUS1" pad="23"/>
<connect gate="G$1" pin="ADBUS2" pad="22"/>
<connect gate="G$1" pin="ADBUS3" pad="21"/>
<connect gate="G$1" pin="ADBUS4" pad="20"/>
<connect gate="G$1" pin="ADBUS5" pad="19"/>
<connect gate="G$1" pin="ADBUS6" pad="17"/>
<connect gate="G$1" pin="ADBUS7" pad="16"/>
<connect gate="G$1" pin="AGND" pad="45"/>
<connect gate="G$1" pin="AVCC" pad="46"/>
<connect gate="G$1" pin="BCBUS0" pad="30"/>
<connect gate="G$1" pin="BCBUS1" pad="29"/>
<connect gate="G$1" pin="BCBUS2" pad="28"/>
<connect gate="G$1" pin="BCBUS3" pad="27"/>
<connect gate="G$1" pin="BDBUS0" pad="40"/>
<connect gate="G$1" pin="BDBUS1" pad="39"/>
<connect gate="G$1" pin="BDBUS2" pad="38"/>
<connect gate="G$1" pin="BDBUS3" pad="37"/>
<connect gate="G$1" pin="BDBUS4" pad="36"/>
<connect gate="G$1" pin="BDBUS5" pad="35"/>
<connect gate="G$1" pin="BDBUS6" pad="33"/>
<connect gate="G$1" pin="BDBUS7" pad="32"/>
<connect gate="G$1" pin="EECS" pad="48"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="34"/>
<connect gate="G$1" pin="GND@4" pad="9"/>
<connect gate="G$1" pin="PWEN#" pad="41"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="SI/WUA" pad="10"/>
<connect gate="G$1" pin="SI/WUB" pad="26"/>
<connect gate="G$1" pin="TEST" pad="47"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC@1" pad="3"/>
<connect gate="G$1" pin="VCC@2" pad="42"/>
<connect gate="G$1" pin="VCCIOA" pad="14"/>
<connect gate="G$1" pin="VCCIOB" pad="31"/>
<connect gate="G$1" pin="XTIN" pad="43"/>
<connect gate="G$1" pin="XTOUT" pad="44"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74AUP" prefix="U" uservalue="yes">
<description>&lt;b&gt;SN74AUP Tri-State Buffer&lt;/b&gt;

&lt;p&gt;SN74AUP (0.8-3.6V) - Digikey: 296-21012-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BUFFER_PWR"/>
</gates>
<devices>
<device name="" package="TSSOP5">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="G$1" pin="OE" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LAN8720" prefix="U" uservalue="yes">
<description>&lt;b&gt;LAN8720A 10/100 Ethernet PHY&lt;/b&gt;
&lt;p&gt;Mouser: 886-LAN8720AI-CP&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LAN8720"/>
</gates>
<devices>
<device name="" package="QFN24_4MM">
<connects>
<connect gate="G$1" pin="CRS_DV" pad="11"/>
<connect gate="G$1" pin="GND" pad="THERM"/>
<connect gate="G$1" pin="LED1/REGOFF" pad="3"/>
<connect gate="G$1" pin="LED2/NINTSEL" pad="2"/>
<connect gate="G$1" pin="MDC" pad="13"/>
<connect gate="G$1" pin="MDIO" pad="12"/>
<connect gate="G$1" pin="NINT/REFCLKO" pad="14"/>
<connect gate="G$1" pin="NRST" pad="15"/>
<connect gate="G$1" pin="RBIAS" pad="24"/>
<connect gate="G$1" pin="RX+" pad="23"/>
<connect gate="G$1" pin="RX-" pad="22"/>
<connect gate="G$1" pin="RXD0" pad="8"/>
<connect gate="G$1" pin="RXD1" pad="7"/>
<connect gate="G$1" pin="RXER" pad="10"/>
<connect gate="G$1" pin="TX+" pad="21"/>
<connect gate="G$1" pin="TX-" pad="20"/>
<connect gate="G$1" pin="TXD0" pad="17"/>
<connect gate="G$1" pin="TXD1" pad="18"/>
<connect gate="G$1" pin="TXEN" pad="16"/>
<connect gate="G$1" pin="VDD1A" pad="19"/>
<connect gate="G$1" pin="VDD2A" pad="1"/>
<connect gate="G$1" pin="VDDCR" pad="6"/>
<connect gate="G$1" pin="VDDIO" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT2232H" prefix="U" uservalue="yes">
<description>&lt;b&gt;FTDI 2232H&lt;/b&gt; - Dual High-Speed USB to UART/FIFO</description>
<gates>
<gate name="G$1" symbol="FT2232H"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="ACBUS0/TXDEN" pad="26"/>
<connect gate="G$1" pin="ACBUS1" pad="27"/>
<connect gate="G$1" pin="ACBUS2" pad="28"/>
<connect gate="G$1" pin="ACBUS3/RXLED#" pad="29"/>
<connect gate="G$1" pin="ACBUS4/TXLED#" pad="30"/>
<connect gate="G$1" pin="ACBUS5" pad="32"/>
<connect gate="G$1" pin="ACBUS6" pad="33"/>
<connect gate="G$1" pin="ACBUS7" pad="34"/>
<connect gate="G$1" pin="ADBUS0/TXD" pad="16"/>
<connect gate="G$1" pin="ADBUS1/RXD" pad="17"/>
<connect gate="G$1" pin="ADBUS2/RTS#" pad="18"/>
<connect gate="G$1" pin="ADBUS3/CTS#" pad="19"/>
<connect gate="G$1" pin="ADBUS4/DTR#" pad="21"/>
<connect gate="G$1" pin="ADBUS5/DSR#" pad="22"/>
<connect gate="G$1" pin="ADBUS6/DCD#" pad="23"/>
<connect gate="G$1" pin="ADBUS7/RI#" pad="24"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCBUS0/TXDEN" pad="48"/>
<connect gate="G$1" pin="BCBUS1" pad="52"/>
<connect gate="G$1" pin="BCBUS2" pad="53"/>
<connect gate="G$1" pin="BCBUS3/RXLED#" pad="54"/>
<connect gate="G$1" pin="BCBUS4/TXLED#" pad="55"/>
<connect gate="G$1" pin="BCBUS5" pad="57"/>
<connect gate="G$1" pin="BCBUS6" pad="58"/>
<connect gate="G$1" pin="BCBUS7" pad="59"/>
<connect gate="G$1" pin="BDBUS0/TXD" pad="38"/>
<connect gate="G$1" pin="BDBUS1/RXD" pad="39"/>
<connect gate="G$1" pin="BDBUS2/RTS#" pad="40"/>
<connect gate="G$1" pin="BDBUS3/CTS#" pad="41"/>
<connect gate="G$1" pin="BDBUS4/DTR#" pad="43"/>
<connect gate="G$1" pin="BDBUS5/DSR#" pad="44"/>
<connect gate="G$1" pin="BDBUS6/DCD#" pad="45"/>
<connect gate="G$1" pin="BDBUS7/RI#" pad="46"/>
<connect gate="G$1" pin="EECLK" pad="62"/>
<connect gate="G$1" pin="EECS" pad="63"/>
<connect gate="G$1" pin="EEDATA" pad="61"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="11"/>
<connect gate="G$1" pin="GND@4" pad="15"/>
<connect gate="G$1" pin="GND@5" pad="25"/>
<connect gate="G$1" pin="GND@6" pad="35"/>
<connect gate="G$1" pin="GND@7" pad="47"/>
<connect gate="G$1" pin="GND@8" pad="51"/>
<connect gate="G$1" pin="OSCIN" pad="2"/>
<connect gate="G$1" pin="OSCOUT" pad="3"/>
<connect gate="G$1" pin="PWREN#" pad="60"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="RESET#" pad="14"/>
<connect gate="G$1" pin="SUSPEND#" pad="36"/>
<connect gate="G$1" pin="TEST" pad="13"/>
<connect gate="G$1" pin="USBD+" pad="8"/>
<connect gate="G$1" pin="USBD-" pad="7"/>
<connect gate="G$1" pin="VCCIO@1" pad="20"/>
<connect gate="G$1" pin="VCCIO@2" pad="31"/>
<connect gate="G$1" pin="VCCIO@3" pad="42"/>
<connect gate="G$1" pin="VCCIO@4" pad="56"/>
<connect gate="G$1" pin="VCORE@1" pad="12"/>
<connect gate="G$1" pin="VCORE@2" pad="37"/>
<connect gate="G$1" pin="VCORE@3" pad="64"/>
<connect gate="G$1" pin="VPHY" pad="4"/>
<connect gate="G$1" pin="VPLL" pad="9"/>
<connect gate="G$1" pin="VREGIN" pad="50"/>
<connect gate="G$1" pin="VREGOUT" pad="49"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X27" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD27"/>
</gates>
<devices>
<device name="" package="1X27_OVAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="1X27_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM_93LC46B" prefix="U" uservalue="yes">
<description>1K 16-Bit EEPROM (Compatible with FT2232H)
&lt;p&gt;SOIC8 - Digikey: 93LC46BT-I/SNCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="93LC46B"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="Q" pad="4"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC1G04" prefix="U" uservalue="yes">
<description>&lt;b&gt;74LVC1G04&lt;/b&gt; - Single Inverter Gate
&lt;p&gt;&lt;b&gt;SOT23-5&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;SN74LVC1G04DBVR - Digikey: 296-11599-1-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="74LVC1G04"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOADCELL" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Load Cell&lt;/b&gt;&lt;/p&gt;
Connector for use with four-wire load cells for precisely measuring weight or pressure</description>
<gates>
<gate name="G$1" symbol="LOADCELL"/>
</gates>
<devices>
<device name="" package="JSTPH4">
<connects>
<connect gate="G$1" pin="EXC+" pad="1"/>
<connect gate="G$1" pin="EXC-" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="3"/>
<connect gate="G$1" pin="OUT-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.1&quot;" package="1X04_OVAL">
<connects>
<connect gate="G$1" pin="EXC+" pad="1"/>
<connect gate="G$1" pin="EXC-" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="3"/>
<connect gate="G$1" pin="OUT-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC_AD7780" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;AD7780&lt;/b&gt; - Low-Power 24-Bit Signma-Delta ADC Converter with 128x PGA&lt;/p&gt;
&lt;p&gt;For use with load cells&lt;/p&gt;
&lt;p&gt;TSSOP16 = 5.0x4.4mm package - Digikey: AD7780BRUZ-ND&lt;/p&gt;
&lt;p&gt;SOIC14 = 8.70x3.9mm package - Digikey: AD7780BRZ-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AD7780"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="AIN+" pad="6"/>
<connect gate="G$1" pin="AIN-" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="12"/>
<connect gate="G$1" pin="BPDSW" pad="10"/>
<connect gate="G$1" pin="DOUT/RDY" pad="3"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="FILTER" pad="15"/>
<connect gate="G$1" pin="GAIN" pad="5"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PDRST" pad="14"/>
<connect gate="G$1" pin="SCLK" pad="2"/>
<connect gate="G$1" pin="VREF+" pad="8"/>
<connect gate="G$1" pin="VREF-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SOIC14">
<connects>
<connect gate="G$1" pin="AIN+" pad="5"/>
<connect gate="G$1" pin="AIN-" pad="6"/>
<connect gate="G$1" pin="AVDD" pad="11"/>
<connect gate="G$1" pin="BPDSW" pad="9"/>
<connect gate="G$1" pin="DOUT/RDY" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="12"/>
<connect gate="G$1" pin="FILTER" pad="14"/>
<connect gate="G$1" pin="GAIN" pad="4"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PDRST" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="VREF+" pad="7"/>
<connect gate="G$1" pin="VREF-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADP3303" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;ADP3303&lt;/b&gt; - High Accuracy 200 mA LDO&lt;/p&gt;
&lt;p&gt;Digikey: 3.3V - ADP3303ARZ-3.3-ND&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Input: 3.5-12V&lt;/li&gt;
&lt;li&gt;Vf: 180mV @ 200mA&lt;/li&gt;
&lt;li&gt;Temp: -20°C-85°C&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;Digikey: 5.0V - ADP3303ARZ-5-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADP3303"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="ERR" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NR" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="SD" pad="5"/>
<connect gate="G$1" pin="VIN1" pad="7"/>
<connect gate="G$1" pin="VIN2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_8PIN" prefix="CN" uservalue="yes">
<description>JST 8-Pin Right-Angle Connector</description>
<gates>
<gate name="G$1" symbol="PINHD8"/>
</gates>
<devices>
<device name="" package="JSTPH8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6022" prefix="U" uservalue="yes">
<description>&lt;b&gt;MCP6022&lt;/b&gt; - Dual Rail-to-Rail 10MHz Op-Amp

&lt;p&gt;Digikey: SOIC8 - MCP6022-I/SN-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP"/>
<gate name="G$2" symbol="OPAMP"/>
<gate name="G$3" symbol="POWER"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="+" pad="8"/>
<connect gate="G$3" pin="-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIOAMP_LM4811" prefix="U" uservalue="yes">
<description>&lt;b&gt;LM4811&lt;/b&gt; - Dual 105mW Headphone Amplifier with Digital Volume
Control

&lt;p&gt;Digikey: MSOP-10 - LM4811MMCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LM4811"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="BYPASS" pad="3"/>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SHTDN" pad="7"/>
<connect gate="G$1" pin="UP/DN" pad="6"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VIN1" pad="2"/>
<connect gate="G$1" pin="VIN2" pad="8"/>
<connect gate="G$1" pin="VOUT1" pad="1"/>
<connect gate="G$1" pin="VOUT2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_STEREOJACK" prefix="CN" uservalue="yes">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
Stereo jack with two switches. Kycon STX3100, CUI SJ1-3555NG and/or 4UCon 05544

&lt;p&gt;Digikey: CP1-3555NG-ND&lt;/p&gt;

&lt;p&gt;Shamelessly taken from the Adafruit Eagle library (public domain) ... thanks!&lt;/p&gt;

&lt;p&gt;These are normally connected as follows, from right-to-left on the schematic symbol above:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Tip: Left Audio&lt;/li&gt;
&lt;li&gt;Inner Ring: Right Audio&lt;/li&gt;
&lt;li&gt;Shell: Common/GND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="1" symbol="KS-S"/>
</gates>
<devices>
<device name="" package="STX3100">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOUNTINGHOLE">
<description>&lt;b&gt;Mounting Hole&lt;/b&gt;
&lt;p&gt;For #2 screws (0.086"/2.18mm width, 0.094"/2.4mm hole) use 2.5mm&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOUNTINGHOLE"/>
</gates>
<devices>
<device name="" package="MOUNTINGHOLE_3.0_PLATED">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.0" package="MOUNTINGHOLE_1.0_PLATED">
<technologies>
<technology name="">
<attribute name="BOM" value="EXCLUDE"/>
</technology>
</technologies>
</device>
<device name="2.0" package="MOUNTINGHOLE_2.0_PLATED">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.0THIN" package="MOUNTINGHOLE_3.0_PLATEDTHIN">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5" package="MOUNTINGHOLE_2.5_PLATED">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5_THICK" package="MOUNTINGHOLE_2.5_PLATED_THICK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTC_PCF2129A" prefix="U" uservalue="yes">
<description>&lt;b&gt;PCF2120A&lt;/b&gt; - High Accuracy, Temp Compensated RTC with Integrated Crystal

&lt;p&gt;Digikey: 568-4960-5-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PCF2129A"/>
</gates>
<devices>
<device name="" package="SOIC20WIDE">
<connects>
<connect gate="G$1" pin="#INT" pad="17"/>
<connect gate="G$1" pin="#TS" pad="6"/>
<connect gate="G$1" pin="BBS" pad="18"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="IFS" pad="5"/>
<connect gate="G$1" pin="NC1" pad="9"/>
<connect gate="G$1" pin="NC2" pad="10"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="NC4" pad="12"/>
<connect gate="G$1" pin="NC5" pad="13"/>
<connect gate="G$1" pin="NC6" pad="14"/>
<connect gate="G$1" pin="NC7" pad="15"/>
<connect gate="G$1" pin="NC8" pad="16"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA/#CE" pad="4"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="3"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PARTNO" value="PCF2129AT/1,512"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1227/6/5/4_QFP64" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1227/6/5/4 - 32-bit ARM Cortex-M0 microcontroller&lt;/b&gt; - LQFP64 Package
&lt;ul&gt;
&lt;li&gt;Low-Power ARM Cortex-M0 up to 33MHz&lt;/li&gt;
&lt;li&gt;Up to 8KB SRAM / 128KB Flash&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Digital Peripherals&lt;/b&gt;: Micro DMA Controller, CRC  Engine, 2xUART, SSP/SPI, I2C, 2x 32-bit Timers, 2x16-bit Timers&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Analog Periherals&lt;/b&gt;: 8-Channel 10-bit ADC, 2 Analog Comparators&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1227/6/5/4_QFP64"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="#RESET/PIO0_13" pad="40"/>
<connect gate="G$1" pin="PIO0_0/RTS0" pad="19"/>
<connect gate="G$1" pin="PIO0_1/RXD0/CT32B0_CAP0/CT32B0_MAT0" pad="20"/>
<connect gate="G$1" pin="PIO0_10/SCL" pad="37"/>
<connect gate="G$1" pin="PIO0_11/SDA/CT16B0_CAP0/CT16B0_MAT0" pad="38"/>
<connect gate="G$1" pin="PIO0_12/CLKOUT/CT16B0_CAP1/CT16B0_MAT1_ISP-(20MA)" pad="39"/>
<connect gate="G$1" pin="PIO0_14/SCK" pad="41"/>
<connect gate="G$1" pin="PIO0_15/SSEL/CT16B1_CAP0/CT16B1_MAT0" pad="42"/>
<connect gate="G$1" pin="PIO0_16/MISO/CT16B1_CAP1/CT16B1_MAT1" pad="43"/>
<connect gate="G$1" pin="PIO0_17/MOSI" pad="44"/>
<connect gate="G$1" pin="PIO0_18/SWCLK/CT32B0_CAP0/CT32B0_MAT0" pad="45"/>
<connect gate="G$1" pin="PIO0_19/ACMP0_I0/CT32B0_CAP1/CT32B0_MAT1" pad="4"/>
<connect gate="G$1" pin="PIO0_2/TXD0/CT32B0_CAP1/CT32B0_MAT1" pad="21"/>
<connect gate="G$1" pin="PIO0_20/ACMP0_I1/CT32B0_CAP2/CT32B0_MAT2" pad="5"/>
<connect gate="G$1" pin="PIO0_21/ACMP0_I2/CT32B0_CAP3/CT32B0_MAT3" pad="6"/>
<connect gate="G$1" pin="PIO0_22/ACMP0_I3" pad="7"/>
<connect gate="G$1" pin="PIO0_23/ACMP1_I0/CT32B1_CAP0/CT32B1_MAT0" pad="8"/>
<connect gate="G$1" pin="PIO0_24/ACMP1_I1/CT32B1_CAP1/CT32B1_MAT1" pad="9"/>
<connect gate="G$1" pin="PIO0_27/ACMP0_O-(20MA)" pad="12"/>
<connect gate="G$1" pin="PIO0_28/ACMP1_O/CT16B0_CAP0/CT16B0_MAT0-(20MA)" pad="17"/>
<connect gate="G$1" pin="PIO0_29/ROSC/CT16B0_CAP1/CT16B0_MAT1-(20MA)" pad="18"/>
<connect gate="G$1" pin="PIO0_3/DTR0/CT32B0_CAP2/CT32B0_MAT2" pad="22"/>
<connect gate="G$1" pin="PIO0_4/DSR0/CT32B0_CAP3/CT32B0_MAT3" pad="23"/>
<connect gate="G$1" pin="PIO0_5/DCD0" pad="24"/>
<connect gate="G$1" pin="PIO0_6/RI0/CT32B1_CAP0/CT32B1_MAT0" pad="25"/>
<connect gate="G$1" pin="PIO0_7/CTS0/CT32B1_CAP1/CT32B1_MAT1" pad="26"/>
<connect gate="G$1" pin="PIO0_8/RXD1/CT32B1_CAP2/CT32B1_MAT2" pad="27"/>
<connect gate="G$1" pin="PIO0_9/TXD1/CT32B1_CAP3/CT32B1_MAT3" pad="28"/>
<connect gate="G$1" pin="PIO1_2/SWDIO/AD4" pad="50"/>
<connect gate="G$1" pin="PIO1_3/AD5/WAKEUP" pad="51"/>
<connect gate="G$1" pin="PIO1_4/AD6" pad="52"/>
<connect gate="G$1" pin="PIO1_5/AD7/CT16B1_CAP0/CT16B1_MAT0" pad="53"/>
<connect gate="G$1" pin="PIO1_6/CT16B1_CAP1/CT16B1_MAT1" pad="54"/>
<connect gate="G$1" pin="PIO2_0/CT16B0_CAP0/CT16B0_MAT0/RTS0" pad="29"/>
<connect gate="G$1" pin="PIO2_1/CT16B0_CAP1/CT16B0_MAT1/RXD0" pad="30"/>
<connect gate="G$1" pin="PIO2_10/CT32B1_CAP2/CT32B1_MAT2/TXD1" pad="61"/>
<connect gate="G$1" pin="PIO2_11/CT32B1_CAP3/CT32B1_MAT3/RXD1" pad="62"/>
<connect gate="G$1" pin="PIO2_12/RXD1" pad="13"/>
<connect gate="G$1" pin="PIO2_13/TXD1" pad="14"/>
<connect gate="G$1" pin="PIO2_14" pad="15"/>
<connect gate="G$1" pin="PIO2_15" pad="16"/>
<connect gate="G$1" pin="PIO2_2/CT16B1_CAP0/CT16B1_MAT0/TXD0" pad="31"/>
<connect gate="G$1" pin="PIO2_3/CT16B1_CAP1/CT16B1_MAT1/DTR0" pad="32"/>
<connect gate="G$1" pin="PIO2_4/CT32B0_CAP0/CT32B0_MAT0/CTS0" pad="33"/>
<connect gate="G$1" pin="PIO2_5/CT32B0_CAP1/CT32B0_MAT1/RI0" pad="34"/>
<connect gate="G$1" pin="PIO2_6/CT32B0_CAP2/CT32B0_MAT2/DCD0" pad="35"/>
<connect gate="G$1" pin="PIO2_7/CT32B0_CAP3/CT32B0_MAT3/DSR0" pad="36"/>
<connect gate="G$1" pin="PIO2_8/CT32B1_CAP0/CT32B1_MAT0" pad="59"/>
<connect gate="G$1" pin="PIO2_9/CT32B1_CAP1/CT32B1_MAT1" pad="60"/>
<connect gate="G$1" pin="R/PIO0_30/AD0" pad="46"/>
<connect gate="G$1" pin="R/PIO0_31/AD1" pad="47"/>
<connect gate="G$1" pin="R/PIO1_0/AD2" pad="48"/>
<connect gate="G$1" pin="R/PIO1_1/AD3" pad="49"/>
<connect gate="G$1" pin="RTCXIN" pad="57"/>
<connect gate="G$1" pin="RTCXOUT" pad="58"/>
<connect gate="G$1" pin="SWCLK/ACMP1_I3/CT32B1_CAP3/CT32B1_MAT3/PIO0_26" pad="11"/>
<connect gate="G$1" pin="SWDIO/ACMP1_I2/CT32B1_CAP2/CT32B1_MAT2/PIO0_25" pad="10"/>
<connect gate="G$1" pin="VDD(3.3V)" pad="56"/>
<connect gate="G$1" pin="VDD(IO)" pad="63"/>
<connect gate="G$1" pin="VREF_CMP" pad="3"/>
<connect gate="G$1" pin="VSS" pad="55"/>
<connect gate="G$1" pin="VSSIO" pad="64"/>
<connect gate="G$1" pin="XTALIN" pad="1"/>
<connect gate="G$1" pin="XTALOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_GE865" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="GE865_2"/>
</gates>
<devices>
<device name="" package="GE865">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="F5"/>
<connect gate="G$1" pin="ADC_IN2" pad="F6"/>
<connect gate="G$1" pin="ANTENNA" pad="H5"/>
<connect gate="G$1" pin="C103/TXD" pad="A3"/>
<connect gate="G$1" pin="C104/RXD" pad="A4"/>
<connect gate="G$1" pin="C105/RTS" pad="A1"/>
<connect gate="G$1" pin="C106/CTS" pad="A2"/>
<connect gate="G$1" pin="C107/DSR" pad="B2"/>
<connect gate="G$1" pin="C108/DTR" pad="B3"/>
<connect gate="G$1" pin="C109/DCD" pad="B5"/>
<connect gate="G$1" pin="C125/RING" pad="B4"/>
<connect gate="G$1" pin="DAC_OUT" pad="G7"/>
<connect gate="G$1" pin="EAR+" pad="D8"/>
<connect gate="G$1" pin="EAR-" pad="E8"/>
<connect gate="G$1" pin="GND@C2" pad="C2"/>
<connect gate="G$1" pin="GND@C7" pad="C7"/>
<connect gate="G$1" pin="GND@E5" pad="E5"/>
<connect gate="G$1" pin="GND@E7" pad="E7"/>
<connect gate="G$1" pin="GND@G1" pad="G1"/>
<connect gate="G$1" pin="GND@G3" pad="G3"/>
<connect gate="G$1" pin="GND@G4" pad="G4"/>
<connect gate="G$1" pin="GND@G5" pad="G5"/>
<connect gate="G$1" pin="GND@H3" pad="H3"/>
<connect gate="G$1" pin="GND@H6" pad="H6"/>
<connect gate="G$1" pin="GPIO_01" pad="D3"/>
<connect gate="G$1" pin="GPIO_02/JDR" pad="D2"/>
<connect gate="G$1" pin="GPIO_03" pad="E4"/>
<connect gate="G$1" pin="GPIO_04/TX_DISAB" pad="H7"/>
<connect gate="G$1" pin="GPIO_05/RFTXMON" pad="G2"/>
<connect gate="G$1" pin="GPIO_06/ALARM" pad="H8"/>
<connect gate="G$1" pin="GPIO_07/BUZZER" pad="G6"/>
<connect gate="G$1" pin="GPIO_08" pad="D4"/>
<connect gate="G$1" pin="GPIO_09" pad="F4"/>
<connect gate="G$1" pin="GPIO_10" pad="E3"/>
<connect gate="G$1" pin="MIC+" pad="B8"/>
<connect gate="G$1" pin="MIC-" pad="C8"/>
<connect gate="G$1" pin="ON_OFF" pad="B1"/>
<connect gate="G$1" pin="PWRMON" pad="E2"/>
<connect gate="G$1" pin="RESET" pad="C1"/>
<connect gate="G$1" pin="RXD_AUX" pad="E1"/>
<connect gate="G$1" pin="SERVICE" pad="H1"/>
<connect gate="G$1" pin="SIMCLK" pad="A5"/>
<connect gate="G$1" pin="SIMIN" pad="B7"/>
<connect gate="G$1" pin="SIMIO" pad="A6"/>
<connect gate="G$1" pin="SIMRST" pad="A8"/>
<connect gate="G$1" pin="SIMVCC" pad="A7"/>
<connect gate="G$1" pin="STAT_LED" pad="G8"/>
<connect gate="G$1" pin="TXD_AUX" pad="D1"/>
<connect gate="G$1" pin="VBATT@F1" pad="F1"/>
<connect gate="G$1" pin="VBATT@F2" pad="F2"/>
<connect gate="G$1" pin="VBATT@F3" pad="F3"/>
<connect gate="G$1" pin="VRTC" pad="H2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_GE864" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="GE864"/>
</gates>
<devices>
<device name="" package="GE864">
<connects>
<connect gate="G$1" pin="ACD_IN1" pad="J11"/>
<connect gate="G$1" pin="ADC_IN2" pad="H11"/>
<connect gate="G$1" pin="ADC_IN3" pad="G11"/>
<connect gate="G$1" pin="ANTENNA" pad="L4"/>
<connect gate="G$1" pin="AXE" pad="F9"/>
<connect gate="G$1" pin="C103/TXD" pad="E7"/>
<connect gate="G$1" pin="C104/RXD" pad="H8"/>
<connect gate="G$1" pin="C105/RTS" pad="F7"/>
<connect gate="G$1" pin="C106/CTS" pad="F6"/>
<connect gate="G$1" pin="C107/DSR" pad="E11"/>
<connect gate="G$1" pin="C108/DTR" pad="B7"/>
<connect gate="G$1" pin="C109/DCD" pad="D9"/>
<connect gate="G$1" pin="C125/RING" pad="B6"/>
<connect gate="G$1" pin="CHARGE@G1" pad="G1"/>
<connect gate="G$1" pin="CHARGE@G2" pad="G2"/>
<connect gate="G$1" pin="DAC_OUT" pad="C7"/>
<connect gate="G$1" pin="DV12_CLK" pad="D7"/>
<connect gate="G$1" pin="EAR_HF+" pad="H10"/>
<connect gate="G$1" pin="EAR_HF-" pad="J10"/>
<connect gate="G$1" pin="EAR_MT+" pad="G10"/>
<connect gate="G$1" pin="EAR_MT-" pad="H9"/>
<connect gate="G$1" pin="GND@A1" pad="A1"/>
<connect gate="G$1" pin="GND@A11" pad="A11"/>
<connect gate="G$1" pin="GND@D6" pad="D6"/>
<connect gate="G$1" pin="GND@F1" pad="F1"/>
<connect gate="G$1" pin="GND@F11" pad="F11"/>
<connect gate="G$1" pin="GND@H1" pad="H1"/>
<connect gate="G$1" pin="GND@H2" pad="H2"/>
<connect gate="G$1" pin="GND@J3" pad="J3"/>
<connect gate="G$1" pin="GND@K3" pad="K3"/>
<connect gate="G$1" pin="GND@K4" pad="K4"/>
<connect gate="G$1" pin="GND@K5" pad="K5"/>
<connect gate="G$1" pin="GND@K6" pad="K6"/>
<connect gate="G$1" pin="GND@L1" pad="L1"/>
<connect gate="G$1" pin="GND@L11" pad="L11"/>
<connect gate="G$1" pin="GND@L2" pad="L2"/>
<connect gate="G$1" pin="GND@L3" pad="L3"/>
<connect gate="G$1" pin="GND@L6" pad="L6"/>
<connect gate="G$1" pin="MIC_HF+" pad="G8"/>
<connect gate="G$1" pin="MIC_HF-" pad="J9"/>
<connect gate="G$1" pin="MIC_MT+" pad="J8"/>
<connect gate="G$1" pin="MIC_MT-" pad="G9"/>
<connect gate="G$1" pin="ON_OFF" pad="J5"/>
<connect gate="G$1" pin="PWRMON" pad="L8"/>
<connect gate="G$1" pin="RESET" pad="A2"/>
<connect gate="G$1" pin="RX_TRACE" pad="F10"/>
<connect gate="G$1" pin="SIMCLK" pad="C10"/>
<connect gate="G$1" pin="SIMIN" pad="C11"/>
<connect gate="G$1" pin="SIMIO" pad="D10"/>
<connect gate="G$1" pin="SIMRST" pad="E9"/>
<connect gate="G$1" pin="SIMVCC" pad="D4"/>
<connect gate="G$1" pin="STAT_LED" pad="D8"/>
<connect gate="G$1" pin="TGPIO_01" pad="C1"/>
<connect gate="G$1" pin="TGPIO_02/JDR" pad="E6"/>
<connect gate="G$1" pin="TGPIO_03" pad="C2"/>
<connect gate="G$1" pin="TGPIO_04" pad="B3"/>
<connect gate="G$1" pin="TGPIO_05/RFTXMON" pad="K8"/>
<connect gate="G$1" pin="TGPIO_06/ALARM" pad="B5"/>
<connect gate="G$1" pin="TGPIO_07/BUZZER" pad="L9"/>
<connect gate="G$1" pin="TGPIO_08" pad="K11"/>
<connect gate="G$1" pin="TGPIO_09" pad="C9"/>
<connect gate="G$1" pin="TGPIO_10" pad="H3"/>
<connect gate="G$1" pin="TGPIO_11" pad="D1"/>
<connect gate="G$1" pin="TGPIO_12" pad="G4"/>
<connect gate="G$1" pin="TGPIO_13" pad="K10"/>
<connect gate="G$1" pin="TGPIO_14" pad="B4"/>
<connect gate="G$1" pin="TGPIO_15" pad="F5"/>
<connect gate="G$1" pin="TGPIO_16" pad="H6"/>
<connect gate="G$1" pin="TGPIO_17" pad="H5"/>
<connect gate="G$1" pin="TGPIO_18" pad="K7"/>
<connect gate="G$1" pin="TGPIO_19" pad="B1"/>
<connect gate="G$1" pin="TGPIO_20" pad="C3"/>
<connect gate="G$1" pin="TGPIO_21" pad="L10"/>
<connect gate="G$1" pin="TGPIO_22" pad="E8"/>
<connect gate="G$1" pin="TX_TRACE" pad="D11"/>
<connect gate="G$1" pin="VAUX1" pad="D5"/>
<connect gate="G$1" pin="VBATT@J1" pad="J1"/>
<connect gate="G$1" pin="VBATT@J2" pad="J2"/>
<connect gate="G$1" pin="VBATT@K1" pad="K1"/>
<connect gate="G$1" pin="VBATT@K2" pad="K2"/>
<connect gate="G$1" pin="VRTC" pad="E2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_OLED_UG-9664HDDAG01" prefix="LCD" uservalue="yes">
<description>OLED 96x64 Pixel, 0.95" 65K Color</description>
<gates>
<gate name="G$1" symbol="OLED_96X64_UNIVISION"/>
</gates>
<devices>
<device name="" package="UG-9664HDDAG01">
<connects>
<connect gate="G$1" pin="BS1" pad="5"/>
<connect gate="G$1" pin="BS2" pad="6"/>
<connect gate="G$1" pin="CS#" pad="8"/>
<connect gate="G$1" pin="D/C#" pad="10"/>
<connect gate="G$1" pin="D0/SCLK" pad="13"/>
<connect gate="G$1" pin="D1/SDIN" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="18"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="D7" pad="20"/>
<connect gate="G$1" pin="E" pad="12"/>
<connect gate="G$1" pin="IREF" pad="7"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="R/W#" pad="11"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="VCOMH" pad="21"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VDDIO" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WRAPAROUND" package="UG-9664HDDAG01_WRAPAROUND">
<connects>
<connect gate="G$1" pin="BS1" pad="5"/>
<connect gate="G$1" pin="BS2" pad="6"/>
<connect gate="G$1" pin="CS#" pad="8"/>
<connect gate="G$1" pin="D/C#" pad="10"/>
<connect gate="G$1" pin="D0/SCLK" pad="13"/>
<connect gate="G$1" pin="D1/SDIN" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="18"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="D7" pad="20"/>
<connect gate="G$1" pin="E" pad="12"/>
<connect gate="G$1" pin="IREF" pad="7"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="R/W#" pad="11"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="VCOMH" pad="21"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VDDIO" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WA_NOHOLES" package="UG-9664HDDAG01_WRAPAROUND_NOHOLES">
<connects>
<connect gate="G$1" pin="BS1" pad="5"/>
<connect gate="G$1" pin="BS2" pad="6"/>
<connect gate="G$1" pin="CS#" pad="8"/>
<connect gate="G$1" pin="D/C#" pad="10"/>
<connect gate="G$1" pin="D0/SCLK" pad="13"/>
<connect gate="G$1" pin="D1/SDIN" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="18"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="D7" pad="20"/>
<connect gate="G$1" pin="E" pad="12"/>
<connect gate="G$1" pin="IREF" pad="7"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="R/W#" pad="11"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="VCOMH" pad="21"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VDDIO" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OL2381" prefix="U" uservalue="yes">
<description>&lt;b&gt;OL2381 - Integrated UHF Transceiver (315/434/868/915 MHz)&lt;/b&gt;
&lt;p&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OL2381"/>
</gates>
<devices>
<device name="" package="HVQFN32-5X5">
<connects>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="8"/>
<connect gate="G$1" pin="GND3" pad="9"/>
<connect gate="G$1" pin="GND4" pad="16"/>
<connect gate="G$1" pin="GND5" pad="32"/>
<connect gate="G$1" pin="P10/DATA" pad="20"/>
<connect gate="G$1" pin="P11/INT" pad="21"/>
<connect gate="G$1" pin="P12/CLOCK" pad="22"/>
<connect gate="G$1" pin="P13/SDO" pad="23"/>
<connect gate="G$1" pin="P14/PIND" pad="15"/>
<connect gate="G$1" pin="RF_IN" pad="7"/>
<connect gate="G$1" pin="RF_OUT" pad="10"/>
<connect gate="G$1" pin="RSTDIS" pad="27"/>
<connect gate="G$1" pin="SCLK" pad="19"/>
<connect gate="G$1" pin="SDIO" pad="18"/>
<connect gate="G$1" pin="SEN" pad="17"/>
<connect gate="G$1" pin="TEN" pad="28"/>
<connect gate="G$1" pin="TEST1" pad="4"/>
<connect gate="G$1" pin="TEST2" pad="5"/>
<connect gate="G$1" pin="TEST3" pad="29"/>
<connect gate="G$1" pin="VCCDIG" pad="14"/>
<connect gate="G$1" pin="VCCIF" pad="3"/>
<connect gate="G$1" pin="VCCPA" pad="12"/>
<connect gate="G$1" pin="VCCREG" pad="31"/>
<connect gate="G$1" pin="VCCRF" pad="6"/>
<connect gate="G$1" pin="VCCXO" pad="26"/>
<connect gate="G$1" pin="VREGDIG" pad="13"/>
<connect gate="G$1" pin="VREGPA" pad="11"/>
<connect gate="G$1" pin="VREGPLL" pad="30"/>
<connect gate="G$1" pin="VREGVCO" pad="2"/>
<connect gate="G$1" pin="XTAL1" pad="25"/>
<connect gate="G$1" pin="XTAL2" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UPD5713" prefix="U" uservalue="yes">
<description>&lt;b&gt;UPD5713TK - Wide Band SPDT Switch (50MHz-2.5GHz)&lt;/b&gt;
&lt;p&gt;Digikey: UPD5713TK-E2-ACT-ND&lt;br/&gt;
Mouser: 551-UPD5713TK-A&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="UPD5713"/>
</gates>
<devices>
<device name="" package="MINIMOLD6">
<connects>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="NC" pad="P$1"/>
<connect gate="G$1" pin="NO" pad="P$3"/>
<connect gate="G$1" pin="P" pad="P$5"/>
<connect gate="G$1" pin="VCONT" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANT-868-SP" prefix="ANT" uservalue="yes">
<description>SMT Antenna
&lt;ul&gt;
&lt;li&gt;Antenna Factor 868MHz (1.10"x0.54") - Digikey: ANT-868-SP_-ND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ANTENNA_CHIP"/>
</gates>
<devices>
<device name="" package="ANT_868MHZ_SPLATCH">
<connects>
<connect gate="G$1" pin="ANT" pad="MICROSTRIP"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="GND5" pad="GND5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_TYPEA" prefix="CN" uservalue="yes">
<description>&lt;b&gt;USB - Type A Connectors&lt;/b&gt;
&lt;p&gt;Male types stick out and are inserted into a PC or matching females parts (these are the connectors used on USB Memory Sticks, etc.).  Female parts are generally used for USB Host and accept a male-type connector.&lt;/p&gt;
&lt;p&gt;SMT Male - 4UCON: 10017&lt;/p&gt;
&lt;p&gt;PTH Female - Digikey: 609-1045-ND, 4UCon: 05241&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB_NOID"/>
</gates>
<devices>
<device name="" package="USB_A-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTHFML" package="USB_HOST-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X15" prefix="CN" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINH2X15"/>
</gates>
<devices>
<device name="" package="2X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U.FL">
<description>&lt;p&gt;U.FL Antenna Connector&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="U.FL"/>
</gates>
<devices>
<device name="" package="U.FL">
<connects>
<connect gate="G$1" pin="GND@0" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="SIGNAL" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_ILI9481" prefix="LCD" uservalue="yes">
<gates>
<gate name="G$1" symbol="ILI9481_LCD"/>
</gates>
<devices>
<device name="" package="ILI9481_35INCH_OUTLINE">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RD" pad="7"/>
<connect gate="G$1" pin="!RESET" pad="8"/>
<connect gate="G$1" pin="!WR" pad="6"/>
<connect gate="G$1" pin="DB0" pad="9"/>
<connect gate="G$1" pin="DB1" pad="10"/>
<connect gate="G$1" pin="DB10" pad="19"/>
<connect gate="G$1" pin="DB11" pad="20"/>
<connect gate="G$1" pin="DB12" pad="21"/>
<connect gate="G$1" pin="DB13" pad="22"/>
<connect gate="G$1" pin="DB14" pad="23"/>
<connect gate="G$1" pin="DB15" pad="24"/>
<connect gate="G$1" pin="DB2" pad="11"/>
<connect gate="G$1" pin="DB3" pad="12"/>
<connect gate="G$1" pin="DB4" pad="13"/>
<connect gate="G$1" pin="DB5" pad="14"/>
<connect gate="G$1" pin="DB6" pad="15"/>
<connect gate="G$1" pin="DB7" pad="16"/>
<connect gate="G$1" pin="DB8" pad="17"/>
<connect gate="G$1" pin="DB9" pad="18"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="GND3" pad="37"/>
<connect gate="G$1" pin="LED-A" pad="36"/>
<connect gate="G$1" pin="LED-K1" pad="30"/>
<connect gate="G$1" pin="LED-K2" pad="31"/>
<connect gate="G$1" pin="LED-K3" pad="32"/>
<connect gate="G$1" pin="LED-K4" pad="33"/>
<connect gate="G$1" pin="LED-K5" pad="34"/>
<connect gate="G$1" pin="LED-K6" pad="35"/>
<connect gate="G$1" pin="RS" pad="5"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="3"/>
<connect gate="G$1" pin="X+" pad="29"/>
<connect gate="G$1" pin="X-" pad="27"/>
<connect gate="G$1" pin="Y+" pad="28"/>
<connect gate="G$1" pin="Y-" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_TO263-5" prefix="U" uservalue="yes">
<description>&lt;b&gt;TO263-5 Linear Voltage Regulators&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;LD29300xx&lt;/b&gt; - 3A LDO (Vf: 0.4V@3A, 0.2V@1A) - Digikey: &lt;b&gt;3.3V&lt;/b&gt; - 497-3475-1-ND&lt;/li&gt;
&lt;li&gt;&lt;b&gt;LD29300P2MTR&lt;/b&gt; - 3A LDO Adjustable - Digikey: 497-7780-1-ND, Mouser: 511-LD29300P2MTR&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPX29300"/>
</gates>
<devices>
<device name="" package="TO263-5">
<connects>
<connect gate="G$1" pin="ADJUST" pad="5"/>
<connect gate="G$1" pin="ENABLE" pad="1"/>
<connect gate="G$1" pin="GND0" pad="6"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOPASTE" package="TO263-5_NOPASTE">
<connects>
<connect gate="G$1" pin="ADJUST" pad="5"/>
<connect gate="G$1" pin="ENABLE" pad="1"/>
<connect gate="G$1" pin="GND0" pad="6"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACCEL_ADXL345" prefix="U" uservalue="yes">
<description>&lt;b&gt;ADXL345&lt;/b&gt; - Digital 3-Axis Accelerometer (I2C/SPI)</description>
<gates>
<gate name="G$1" symbol="ADXL345"/>
</gates>
<devices>
<device name="" package="LGA14">
<connects>
<connect gate="G$1" pin="ADDR/SDO" pad="12"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="GND@3" pad="5"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC" pad="10"/>
<connect gate="G$1" pin="RSV@1" pad="3"/>
<connect gate="G$1" pin="RSV@2" pad="11"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD(I/O)" pad="1"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73871" prefix="U" uservalue="yes">
<description>&lt;b&gt;MCP73871 Lithium Polymer Battery Charger&lt;/b&gt;
&lt;p&gt;Digikey: MCP73871-2CCI/ML-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP73871"/>
</gates>
<devices>
<device name="" package="QFN20_4MM">
<connects>
<connect gate="G$1" pin="/PG" pad="P$6"/>
<connect gate="G$1" pin="/TE" pad="P$9"/>
<connect gate="G$1" pin="CE" pad="P$17"/>
<connect gate="G$1" pin="PROG1" pad="P$13"/>
<connect gate="G$1" pin="PROG2" pad="P$4"/>
<connect gate="G$1" pin="PROG3" pad="P$12"/>
<connect gate="G$1" pin="SEL" pad="P$3"/>
<connect gate="G$1" pin="STAT1/LBO" pad="P$8"/>
<connect gate="G$1" pin="STAT2" pad="P$7"/>
<connect gate="G$1" pin="THERM" pad="P$5"/>
<connect gate="G$1" pin="THERMAL" pad="P$21"/>
<connect gate="G$1" pin="VBAT1" pad="P$14"/>
<connect gate="G$1" pin="VBAT2" pad="P$15"/>
<connect gate="G$1" pin="VBATSENS" pad="P$16"/>
<connect gate="G$1" pin="VIN1" pad="P$18"/>
<connect gate="G$1" pin="VIN2" pad="P$19"/>
<connect gate="G$1" pin="VOUT1" pad="P$1"/>
<connect gate="G$1" pin="VOUT2" pad="P$20"/>
<connect gate="G$1" pin="VPCC" pad="P$2"/>
<connect gate="G$1" pin="VSS1" pad="P$10"/>
<connect gate="G$1" pin="VSS2" pad="P$11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC4050D" prefix="U" uservalue="yes">
<description>&lt;p&gt;6-channel level shifter
&lt;p&gt;74HC4050D - 2V-6V Supply&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Digikey: 74HC4050D,653-ND&lt;/li&gt;
&lt;li&gt;Mouser: 771-74HC4050D-T &lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="74HC4050D"/>
</gates>
<devices>
<device name="" package="SOIC16">
<connects>
<connect gate="G$1" pin="1A" pad="3"/>
<connect gate="G$1" pin="1Y" pad="2"/>
<connect gate="G$1" pin="2A" pad="5"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="3A" pad="7"/>
<connect gate="G$1" pin="3Y" pad="6"/>
<connect gate="G$1" pin="4A" pad="9"/>
<connect gate="G$1" pin="4Y" pad="10"/>
<connect gate="G$1" pin="5A" pad="11"/>
<connect gate="G$1" pin="5Y" pad="12"/>
<connect gate="G$1" pin="6A" pad="14"/>
<connect gate="G$1" pin="6Y" pad="15"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LCX245" prefix="U" uservalue="yes">
<description>&lt;p&gt;74LCX245MTC - 5.0V Tolerant Bi-Directional Buffer
&lt;p&gt;Can be used to interface 5.0V logic to 2.5 or 3.3V devices&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Digikey: 74LCX245MTCXTR-ND&lt;/li&gt;
&lt;li&gt;Mouser: 512-74LCX245MTCX&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="74LCX245MTC"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="/OE" pad="19"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="B1" pad="18"/>
<connect gate="G$1" pin="B2" pad="17"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="B4" pad="15"/>
<connect gate="G$1" pin="B5" pad="14"/>
<connect gate="G$1" pin="B6" pad="13"/>
<connect gate="G$1" pin="B7" pad="12"/>
<connect gate="G$1" pin="B8" pad="11"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="T/R" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_SPDT" prefix="SW" uservalue="yes">
<description>&lt;p&gt;&lt;strong&gt;Switch - SPDT&lt;/strong&gt;&lt;/p&gt;
&lt;ul&gt;&lt;li&gt;&lt;strong&gt;SSSS811101&lt;/strong&gt; - Horizontal Two Position SMT, 0.3A 4V [Mouser: 688-SSSS811101]&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH_SPDT"/>
</gates>
<devices>
<device name="" package="SPDT_SMT_SSSS811101">
<connects>
<connect gate="G$1" pin="O" pad="A"/>
<connect gate="G$1" pin="P" pad="B"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_OLED_UG-2832HSWEG04" prefix="LCD" uservalue="yes">
<description>128x32 SPI 0.91" Monochrome OLED Display</description>
<gates>
<gate name="G$1" symbol="UG-2832HSWEG04"/>
</gates>
<devices>
<device name="" package="UG-2832HSWEG04">
<connects>
<connect gate="G$1" pin="C1+" pad="3"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="CS#" pad="8"/>
<connect gate="G$1" pin="D/C#" pad="10"/>
<connect gate="G$1" pin="IREF" pad="13"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIN" pad="12"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="G$1" pin="VCOMH" pad="14"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WRAPAROUND" package="UG-2832HSWEG04_WRAPAROUND">
<connects>
<connect gate="G$1" pin="C1+" pad="3"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="CS#" pad="8"/>
<connect gate="G$1" pin="D/C#" pad="10"/>
<connect gate="G$1" pin="IREF" pad="13"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIN" pad="12"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="G$1" pin="VCOMH" pad="14"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_OLED_UG-9616GLBBG02" prefix="LCD" uservalue="yes">
<description>96x16 0.84" I2C Mono OLED Display</description>
<gates>
<gate name="G$1" symbol="UG-9616GLBBG02"/>
</gates>
<devices>
<device name="0.5MMFLAT" package="UG-9616GLBBG02">
<connects>
<connect gate="G$1" pin="C1+" pad="3"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="IREF" pad="12"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VBREF" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VCOMH" pad="13"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.5MMWRAPUNDER" package="UG-9616GLBBG02_WRAPAROUND">
<connects>
<connect gate="G$1" pin="C1+" pad="3"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="IREF" pad="12"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VBREF" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VCOMH" pad="13"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="UG-9616GLBBG02_0.65MM_WRAPAROUND">
<connects>
<connect gate="G$1" pin="C1+" pad="3"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="IREF" pad="12"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VBREF" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VCOMH" pad="13"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FAN5331" prefix="U" uservalue="yes">
<description>&lt;b&gt;FAN5331 - LED/OLED 20V Boost Converter&lt;/b&gt;
&lt;p&gt;Digikey: FAN5331SXCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FAN5331"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTC_ISL12022M" prefix="U" uservalue="yes">
<description>&lt;b&gt;Temp. Compensated +/-5ppm RTC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ISL12022M"/>
</gates>
<devices>
<device name="" package="SOIC20WIDE">
<connects>
<connect gate="G$1" pin="#IRQ/FOUT" pad="13"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="GND2" pad="8"/>
<connect gate="G$1" pin="GND3" pad="15"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="7"/>
<connect gate="G$1" pin="VDD" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX3421E" prefix="U" uservalue="yes">
<description>&lt;b&gt;MAX3421E&lt;/b&gt; SPI-Interface USB Device/Host Controller
&lt;p&gt;Digikey: MAX3421EETJ+-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX3421E"/>
</gates>
<devices>
<device name="" package="HVQFN32-5X5_3MMTHERMAL">
<connects>
<connect gate="G$1" pin="#RES" pad="12"/>
<connect gate="G$1" pin="#SS" pad="14"/>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="20"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="19"/>
<connect gate="G$1" pin="GND3(THERMAL)" pad="THERMAL"/>
<connect gate="G$1" pin="GPIN0" pad="26"/>
<connect gate="G$1" pin="GPIN1" pad="27"/>
<connect gate="G$1" pin="GPIN2" pad="28"/>
<connect gate="G$1" pin="GPIN3" pad="29"/>
<connect gate="G$1" pin="GPIN4" pad="30"/>
<connect gate="G$1" pin="GPIN5" pad="31"/>
<connect gate="G$1" pin="GPIN6" pad="32"/>
<connect gate="G$1" pin="GPIN7" pad="1"/>
<connect gate="G$1" pin="GPOUT0" pad="4"/>
<connect gate="G$1" pin="GPOUT1" pad="5"/>
<connect gate="G$1" pin="GPOUT2" pad="6"/>
<connect gate="G$1" pin="GPOUT3" pad="7"/>
<connect gate="G$1" pin="GPOUT4" pad="8"/>
<connect gate="G$1" pin="GPOUT5" pad="9"/>
<connect gate="G$1" pin="GPOUT6" pad="10"/>
<connect gate="G$1" pin="GPOUT7" pad="11"/>
<connect gate="G$1" pin="GPX" pad="17"/>
<connect gate="G$1" pin="INT" pad="18"/>
<connect gate="G$1" pin="MISO" pad="15"/>
<connect gate="G$1" pin="MOSI" pad="16"/>
<connect gate="G$1" pin="SCK" pad="13"/>
<connect gate="G$1" pin="VBCOMP" pad="22"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VL" pad="2"/>
<connect gate="G$1" pin="XI" pad="24"/>
<connect gate="G$1" pin="XO" pad="25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3581" prefix="U" uservalue="yes">
<description>&lt;b&gt;LTC3581 - 3.3A Boost/Inverting DC/DC Converter (Boost/SEPIC/Inverting or Flyback)&lt;/b&gt;
&lt;p&gt;Digikey: LT3581EDE#PBF-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LT3581"/>
</gates>
<devices>
<device name="" package="DFN14_4X3MM">
<connects>
<connect gate="G$1" pin="#FAULT" pad="4"/>
<connect gate="G$1" pin="#SHDN" pad="11"/>
<connect gate="G$1" pin="CLKOUT" pad="10"/>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="GATE" pad="3"/>
<connect gate="G$1" pin="GND" pad="THERM"/>
<connect gate="G$1" pin="RT" pad="12"/>
<connect gate="G$1" pin="SS" pad="13"/>
<connect gate="G$1" pin="SW1A" pad="6"/>
<connect gate="G$1" pin="SW1B" pad="7"/>
<connect gate="G$1" pin="SW2A" pad="8"/>
<connect gate="G$1" pin="SW2B" pad="9"/>
<connect gate="G$1" pin="SYNC" pad="14"/>
<connect gate="G$1" pin="VC" pad="2"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0108PWR" prefix="U" uservalue="yes">
<description>&lt;b&gt;8-Bit Bi-Directional Level Shifter&lt;/b&gt;
&lt;ul&gt;
  &lt;li&gt;1.2V-3.6V (VCCA) to 1.65V-5.5V (VCCB) bi-directional level shifter with auto direction sensing.&lt;/li&gt;
  &lt;li&gt;Max data rate - VCCA 1.8V:  20Mbps (50ns), VCCA 3.3V: 100Mbps (10ns)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey: 296-21527-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TXB0108PWR"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="18"/>
<connect gate="G$1" pin="B3" pad="17"/>
<connect gate="G$1" pin="B4" pad="16"/>
<connect gate="G$1" pin="B5" pad="15"/>
<connect gate="G$1" pin="B6" pad="14"/>
<connect gate="G$1" pin="B7" pad="13"/>
<connect gate="G$1" pin="B8" pad="12"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OE" pad="10"/>
<connect gate="G$1" pin="VCCA" pad="2"/>
<connect gate="G$1" pin="VCCB" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0104PWR" prefix="U" uservalue="yes">
<description>&lt;b&gt;4-Bit Bi-Directional Level Shifter&lt;/b&gt;
&lt;ul&gt;
  &lt;li&gt;1.2V-3.6V (VCCA) to 1.65V-5.5V (VCCB) bi-directional level shifter with auto direction sensing.&lt;/li&gt;
  &lt;li&gt;Max data rate - VCCA 1.8V:  20Mbps (50ns), VCCA 3.3V: 100Mbps (10ns)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey: 296-21929-1-ND&lt;/p&gt;
&lt;p&gt;&lt;b&gt;NOTE:&lt;/b&gt; For cheaper alternative see NXP's NTB0104 (Digikey: 568-8404-1-ND)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TXB0104PWR"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="B1" pad="13"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="11"/>
<connect gate="G$1" pin="B4" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OE" pad="8"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCCIO">
<gates>
<gate name="G$1" symbol="VCCIO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMP085" prefix="U" uservalue="yes">
<description>&lt;b&gt;BMP085 Digital Pressure Sensor&lt;/b&gt;
&lt;p&gt;1.8-3.6V Supply, I2C Interface&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BMP085"/>
</gates>
<devices>
<device name="" package="BMP085">
<connects>
<connect gate="G$1" pin="AVDD" pad="P$3"/>
<connect gate="G$1" pin="EOC" pad="P$2"/>
<connect gate="G$1" pin="GND" pad="P$1"/>
<connect gate="G$1" pin="NC" pad="P$5"/>
<connect gate="G$1" pin="SCL" pad="P$6"/>
<connect gate="G$1" pin="SDA" pad="P$7"/>
<connect gate="G$1" pin="VDD" pad="P$4"/>
<connect gate="G$1" pin="XCLR" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HMC5883L" prefix="U" uservalue="yes">
<description>&lt;b&gt;HMC5883L 3-Axis Digital Compass&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="HMC5883L"/>
</gates>
<devices>
<device name="" package="HMC5883L">
<connects>
<connect gate="G$1" pin="C1" pad="10"/>
<connect gate="G$1" pin="DRDY" pad="15"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="5"/>
<connect gate="G$1" pin="NC3" pad="6"/>
<connect gate="G$1" pin="NC4" pad="7"/>
<connect gate="G$1" pin="NC5" pad="14"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="SETC" pad="12"/>
<connect gate="G$1" pin="SETP" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EXT" package="HMC5883L_EXTENDED">
<connects>
<connect gate="G$1" pin="C1" pad="10"/>
<connect gate="G$1" pin="DRDY" pad="15"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="5"/>
<connect gate="G$1" pin="NC3" pad="6"/>
<connect gate="G$1" pin="NC4" pad="7"/>
<connect gate="G$1" pin="NC5" pad="14"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="SETC" pad="12"/>
<connect gate="G$1" pin="SETP" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDIO" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GYRO_ITG3200" prefix="U" uservalue="yes">
<description>&lt;b&gt;ITG3200 3-Axis Digital Gyroscope&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;VDD: 2.1-3.6V&lt;/li&gt;
&lt;li&gt;VLOGIC: 1.71V-VDD&lt;/li&gt;
&lt;li&gt;I2C Speed: 400kHz&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ITG3200"/>
</gates>
<devices>
<device name="" package="ITG3200_QFN24">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="CLKIN" pad="1"/>
<connect gate="G$1" pin="CPOUT" pad="20"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="INT" pad="12"/>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="NC3" pad="4"/>
<connect gate="G$1" pin="NC4" pad="5"/>
<connect gate="G$1" pin="NC5" pad="14"/>
<connect gate="G$1" pin="NC6" pad="15"/>
<connect gate="G$1" pin="NC7" pad="16"/>
<connect gate="G$1" pin="NC8" pad="17"/>
<connect gate="G$1" pin="REGOUT" pad="10"/>
<connect gate="G$1" pin="RESV-G" pad="11"/>
<connect gate="G$1" pin="RESV1" pad="6"/>
<connect gate="G$1" pin="RESV2" pad="7"/>
<connect gate="G$1" pin="RESV3" pad="19"/>
<connect gate="G$1" pin="RESV4" pad="21"/>
<connect gate="G$1" pin="RESV5" pad="22"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VLOGIC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCNL4000" prefix="U" uservalue="yes">
<description>&lt;b&gt;VCNL4000&lt;/b&gt; - I²C Proximity and Light Sensor
&lt;p&gt;Supply: 2.5-3.6V&lt;br/&gt;
Proximity: up to 200mm&lt;br/&gt;
Luminosity: 0.25 to 16,000 lux (16-bit values)&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Digikey: &lt;/b&gt;751-1505-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VCNL4000"/>
</gates>
<devices>
<device name="" package="VCNL4000">
<connects>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="IR_A" pad="1"/>
<connect gate="G$1" pin="IR_K1" pad="2"/>
<connect gate="G$1" pin="IR_K2" pad="3"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPIFLASH_SOIC8" prefix="U" uservalue="yes">
<description>&lt;b&gt;SOIC8 SPI Flash&lt;/b&gt;
&lt;p&gt;Be careful with the size since SOIC8 flash comes in several 'widths'&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SOIC8 150 mil&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;M25P16&lt;/b&gt; - 16Mbit (2Mbit x 8) Serial Flash (75MHz SPI Bus), Supply: 2.7-3.6V &lt;br/&gt;&lt;b&gt;Digikey: &lt;/b&gt; SOIC8 - M25P16-VMN6P-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SOIC8 208 mil&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;W25Q16BVSSIG&lt;/b&gt; - 16Mbit (2Mbit x 8) Serial Flash (104MHz SPI Bus), Supply: 2.7-3.6V &lt;br/&gt;&lt;b&gt;Digikey: &lt;/b&gt; SOIC8 - W25Q16BVSSIG-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="M25P16"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="#HOLD/IO3" pad="7"/>
<connect gate="G$1" pin="#WP/IO2" pad="3"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="208MIL" package="SOIC8_208MIL">
<connects>
<connect gate="G$1" pin="#HOLD/IO3" pad="7"/>
<connect gate="G$1" pin="#WP/IO2" pad="3"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SSEL" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4983_LITERAL" prefix="U" uservalue="yes">
<description>&lt;b&gt;A4983 2A Micro-Stepping Stepper Motor Driver&lt;/b&gt;
&lt;p&gt;Logic: 3.0-5.5V&lt;br/&gt;
Load Supply: 8.0-35V&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="A4983_LITERAL"/>
</gates>
<devices>
<device name="" package="QFN28_5MM">
<connects>
<connect gate="G$1" pin="CP1" pad="4"/>
<connect gate="G$1" pin="CP2" pad="5"/>
<connect gate="G$1" pin="DIR" pad="19"/>
<connect gate="G$1" pin="ENABLE" pad="2"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="THERMAL"/>
<connect gate="G$1" pin="MS1" pad="9"/>
<connect gate="G$1" pin="MS2" pad="10"/>
<connect gate="G$1" pin="MS3" pad="11"/>
<connect gate="G$1" pin="NC1" pad="7"/>
<connect gate="G$1" pin="NC2" pad="20"/>
<connect gate="G$1" pin="NC3" pad="25"/>
<connect gate="G$1" pin="OUT1A" pad="24"/>
<connect gate="G$1" pin="OUT1B" pad="21"/>
<connect gate="G$1" pin="OUT2A" pad="26"/>
<connect gate="G$1" pin="OUT2B" pad="1"/>
<connect gate="G$1" pin="REF" pad="17"/>
<connect gate="G$1" pin="RESET" pad="12"/>
<connect gate="G$1" pin="ROSC" pad="13"/>
<connect gate="G$1" pin="SENSE1" pad="23"/>
<connect gate="G$1" pin="SENSE2" pad="27"/>
<connect gate="G$1" pin="SLEEP" pad="14"/>
<connect gate="G$1" pin="STEP" pad="16"/>
<connect gate="G$1" pin="VBB1" pad="22"/>
<connect gate="G$1" pin="VBB2" pad="28"/>
<connect gate="G$1" pin="VCP" pad="6"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VREG" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS61029" prefix="U" uservalue="yes">
<description>&lt;b&gt;TPS61029 - Boost Converter&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;Input: 0.9-6.5V&lt;/li&gt;
&lt;li&gt;Quiescent Current: 25uA (Typ.)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;TPS61029DRCT = 1.8-5.5V Output&lt;br/&gt;
TPS61027DRCR = 5.0V Output&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TPS61029"/>
</gates>
<devices>
<device name="" package="TPS61029">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LBI" pad="7"/>
<connect gate="G$1" pin="LBO" pad="4"/>
<connect gate="G$1" pin="PGND" pad="10"/>
<connect gate="G$1" pin="PS" pad="8"/>
<connect gate="G$1" pin="PWRPAD1" pad="GND1"/>
<connect gate="G$1" pin="PWRPAD2" pad="GND2"/>
<connect gate="G$1" pin="PWRPAD3" pad="GND3"/>
<connect gate="G$1" pin="PWRPAD4" pad="GND4"/>
<connect gate="G$1" pin="PWRPAD5" pad="GND5"/>
<connect gate="G$1" pin="SW" pad="9"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_SPST" prefix="SW" uservalue="yes">
<description>&lt;b&gt;Switch - SPST&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;4UCon 19192 (6.7x2.6mm SMT)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH_SPST"/>
</gates>
<devices>
<device name="" package="SPST_SMT_19192">
<connects>
<connect gate="G$1" pin="P" pad="B"/>
<connect gate="G$1" pin="S" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4983_LOGICAL" prefix="U" uservalue="yes">
<description>&lt;b&gt;A4983 2A Micro-Stepping Stepper Motor Driver&lt;/b&gt;
&lt;p&gt;Logic: 3.0-5.5V&lt;br/&gt;
Load Supply: 8.0-35V&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="A4983_LOGICAL"/>
</gates>
<devices>
<device name="" package="QFN28_5MM">
<connects>
<connect gate="G$1" pin="CP1" pad="4"/>
<connect gate="G$1" pin="CP2" pad="5"/>
<connect gate="G$1" pin="DIR" pad="19"/>
<connect gate="G$1" pin="ENABLE" pad="2"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="THERMAL"/>
<connect gate="G$1" pin="MS1" pad="9"/>
<connect gate="G$1" pin="MS2" pad="10"/>
<connect gate="G$1" pin="MS3" pad="11"/>
<connect gate="G$1" pin="NC1" pad="7"/>
<connect gate="G$1" pin="NC2" pad="20"/>
<connect gate="G$1" pin="NC3" pad="25"/>
<connect gate="G$1" pin="OUT1A" pad="24"/>
<connect gate="G$1" pin="OUT1B" pad="21"/>
<connect gate="G$1" pin="OUT2A" pad="26"/>
<connect gate="G$1" pin="OUT2B" pad="1"/>
<connect gate="G$1" pin="REF" pad="17"/>
<connect gate="G$1" pin="RESET" pad="12"/>
<connect gate="G$1" pin="ROSC" pad="13"/>
<connect gate="G$1" pin="SENSE1" pad="23"/>
<connect gate="G$1" pin="SENSE2" pad="27"/>
<connect gate="G$1" pin="SLEEP" pad="14"/>
<connect gate="G$1" pin="STEP" pad="16"/>
<connect gate="G$1" pin="VBB1" pad="22"/>
<connect gate="G$1" pin="VBB2" pad="28"/>
<connect gate="G$1" pin="VCP" pad="6"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VREG" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXS0102" prefix="U" uservalue="yes">
<description>&lt;b&gt;2-Bit Bi-Directional Level Shifter (I2C, etc.)&lt;/b&gt;
&lt;p&gt;Designed for I2C/1-Wire devices and has internal pullups.  Not to be confused with TX&lt;b&gt;B&lt;/b&gt;010x series.&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;1.2V-3.6V (VCCA) to 1.65V-5.5V (VCCB) bi-directional level shifter with auto direction sensing.&lt;/li&gt;
  &lt;li&gt;Max data rate - 24Mbps (Push Pull), 2Mbps (Open Drain)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey: 296-21931-1-ND&lt;/p&gt;
&lt;p&gt;&lt;b&gt;NOTE:&lt;/b&gt; For cheaper alternative see NXP's NTS0102 (Mouser: 771-NTS0102GT115)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TXS0102"/>
</gates>
<devices>
<device name="" package="VFSOP-8">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="6"/>
<connect gate="G$1" pin="VCCA" pad="3"/>
<connect gate="G$1" pin="VCCB" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_DPDT" prefix="SW" uservalue="yes">
<description>&lt;b&gt;Switch - DPDT&lt;/b&gt;
&lt;p&gt;A DPDT Switch acts like an SPDT switch, but has a pair of switches instead of just one.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Vertical - 0.3A @ 6V SMT - Digikey: JS202011SCQN&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH_DPDT"/>
</gates>
<devices>
<device name="" package="DPDT_SMT_JS202011SCQN">
<connects>
<connect gate="G$1" pin="O1" pad="P$1"/>
<connect gate="G$1" pin="O2" pad="P$6"/>
<connect gate="G$1" pin="P1" pad="P$2"/>
<connect gate="G$1" pin="P2" pad="P$5"/>
<connect gate="G$1" pin="S1" pad="P$3"/>
<connect gate="G$1" pin="S2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_OLED_UG-2828GDEDF11" prefix="U" uservalue="yes">
<description>&lt;b&gt;128x128 1.5" RGB OLED&lt;/b&gt; - UG-2828GDEDF11
&lt;p&gt;30-Pin 0.5mm Pitch FPC Cable (Top+Bottom Contacts) - OMRON XF2M-3015-1A (Digikey: OR723TR-ND)&lt;/p&gt;
&lt;p&gt;This FPC connector has contacts on the top and bottom, but the appropriate pin needs to be selected depending on whether the OLED will be inserted right-side up (use the TOP pinout) or upside-down (use the BOTTOM pinout).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="UG-2828GDEDF11"/>
</gates>
<devices>
<device name="TOP" package="FPC_XF2M-3015-1A">
<connects>
<connect gate="G$1" pin="BS0" pad="P$14"/>
<connect gate="G$1" pin="BS1" pad="P$13"/>
<connect gate="G$1" pin="CS#" pad="P$12"/>
<connect gate="G$1" pin="D/C#" pad="P$11"/>
<connect gate="G$1" pin="D0/SCK" pad="P$17"/>
<connect gate="G$1" pin="D1/SDIN" pad="P$18"/>
<connect gate="G$1" pin="D2" pad="P$19"/>
<connect gate="G$1" pin="D3" pad="P$20"/>
<connect gate="G$1" pin="D4" pad="P$21"/>
<connect gate="G$1" pin="D5" pad="P$22"/>
<connect gate="G$1" pin="D6" pad="P$23"/>
<connect gate="G$1" pin="D7" pad="P$24"/>
<connect gate="G$1" pin="E/RD#" pad="P$16"/>
<connect gate="G$1" pin="GPIO0" pad="P$7"/>
<connect gate="G$1" pin="GPIO1" pad="P$8"/>
<connect gate="G$1" pin="IREF" pad="P$9"/>
<connect gate="G$1" pin="NC(GND)@1" pad="P$30"/>
<connect gate="G$1" pin="NC(GND)@2" pad="P$1"/>
<connect gate="G$1" pin="NC@1" pad="P$25"/>
<connect gate="G$1" pin="NC@2" pad="P$6"/>
<connect gate="G$1" pin="NC@3" pad="P$2"/>
<connect gate="G$1" pin="R/W#" pad="P$15"/>
<connect gate="G$1" pin="RES#" pad="P$10"/>
<connect gate="G$1" pin="VCC" pad="P$29"/>
<connect gate="G$1" pin="VCI" pad="P$4"/>
<connect gate="G$1" pin="VCOMH" pad="P$28"/>
<connect gate="G$1" pin="VDD" pad="P$5"/>
<connect gate="G$1" pin="VDDIO" pad="P$27"/>
<connect gate="G$1" pin="VSL" pad="P$26"/>
<connect gate="G$1" pin="VSS" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BOTTOM" package="FPC_XF2M-3015-1A">
<connects>
<connect gate="G$1" pin="BS0" pad="P$17"/>
<connect gate="G$1" pin="BS1" pad="P$18"/>
<connect gate="G$1" pin="CS#" pad="P$19"/>
<connect gate="G$1" pin="D/C#" pad="P$20"/>
<connect gate="G$1" pin="D0/SCK" pad="P$14"/>
<connect gate="G$1" pin="D1/SDIN" pad="P$13"/>
<connect gate="G$1" pin="D2" pad="P$12"/>
<connect gate="G$1" pin="D3" pad="P$11"/>
<connect gate="G$1" pin="D4" pad="P$10"/>
<connect gate="G$1" pin="D5" pad="P$9"/>
<connect gate="G$1" pin="D6" pad="P$8"/>
<connect gate="G$1" pin="D7" pad="P$7"/>
<connect gate="G$1" pin="E/RD#" pad="P$15"/>
<connect gate="G$1" pin="GPIO0" pad="P$24"/>
<connect gate="G$1" pin="GPIO1" pad="P$23"/>
<connect gate="G$1" pin="IREF" pad="P$22"/>
<connect gate="G$1" pin="NC(GND)@1" pad="P$1"/>
<connect gate="G$1" pin="NC(GND)@2" pad="P$30"/>
<connect gate="G$1" pin="NC@1" pad="P$6"/>
<connect gate="G$1" pin="NC@2" pad="P$25"/>
<connect gate="G$1" pin="NC@3" pad="P$29"/>
<connect gate="G$1" pin="R/W#" pad="P$16"/>
<connect gate="G$1" pin="RES#" pad="P$21"/>
<connect gate="G$1" pin="VCC" pad="P$2"/>
<connect gate="G$1" pin="VCI" pad="P$27"/>
<connect gate="G$1" pin="VCOMH" pad="P$3"/>
<connect gate="G$1" pin="VDD" pad="P$26"/>
<connect gate="G$1" pin="VDDIO" pad="P$4"/>
<connect gate="G$1" pin="VSL" pad="P$5"/>
<connect gate="G$1" pin="VSS" pad="P$28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12V">
<description>&lt;b&gt;12V Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="12V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="13V">
<description>&lt;b&gt;13V Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="13V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1102-WLCSP16">
<description>&lt;h3&gt;NXP Semiconductors&lt;/h3&gt;
&lt;a href="http://ics.nxp.com/products/lpc1000/lpc11xx/lpc1102/"&gt;&lt;b&gt;LPC1102&lt;/b&gt; microcontroller&lt;/a&gt;
&lt;ul&gt;
&lt;li&gt;ARM 32-bit Cortex-M0 Microcontroller with MPU&lt;/li&gt;
&lt;li&gt;CPU clock up to 50MHz&lt;/li&gt;
&lt;li&gt;32KByte on-chip Flash ROM with In-System Programming (ISP) and In-Application Programming (IAP) via On-Chip Bootloader&lt;/li&gt;
&lt;li&gt;8KByte SRAM&lt;/li&gt;
&lt;li&gt;Nested Vectored Interrupt Controller&lt;/li&gt;
&lt;li&gt;SPI controller&lt;/li&gt;
&lt;li&gt;UART with full Modem Interface and RS485 Support&lt;/li&gt;
&lt;li&gt;4 Timers with 4 capture channels and 13 output channels&lt;/li&gt;
&lt;li&gt;Watchdog (WDT)&lt;/li&gt;
&lt;li&gt;Sytem tick timer&lt;/li&gt;
&lt;li&gt;10-bit ADC with 5 channels&lt;/li&gt;
&lt;li&gt;Power Management Unit (PMU)&lt;/li&gt;
&lt;li&gt;Brownout detection&lt;/li&gt;
&lt;li&gt;12MHz internal RC oscillator&lt;/li&gt;
&lt;li&gt;Serial Wire Debug/Trace port&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="LPC" symbol="LPC1102-16"/>
</gates>
<devices>
<device name="" package="WLCSP16">
<connects>
<connect gate="LPC" pin="!RESET!/PIO0_0" pad="C1"/>
<connect gate="LPC" pin="PIO0_8/MISO/CT16B0_MAT0" pad="A2"/>
<connect gate="LPC" pin="PIO0_9/MOSI/CT16B0_MAT1" pad="A3"/>
<connect gate="LPC" pin="PIO1_6/RXD/CT32B0_MAT0" pad="C2"/>
<connect gate="LPC" pin="PIO1_7/TXD/CT32B0_MAT1" pad="D1"/>
<connect gate="LPC" pin="R/PIO0_11/AD0/CT32B0_MAT3" pad="B4"/>
<connect gate="LPC" pin="R/PIO1_0/AD1/CT32B1_CAP0" pad="B3"/>
<connect gate="LPC" pin="R/PIO1_1/AD2/CT32B1_MAT0" pad="C4"/>
<connect gate="LPC" pin="R/PIO1_2/AD3/CT32B1_MAT1" pad="C3"/>
<connect gate="LPC" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="A4"/>
<connect gate="LPC" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="D4"/>
<connect gate="LPC" pin="VDD1" pad="A1"/>
<connect gate="LPC" pin="VDD2" pad="D2"/>
<connect gate="LPC" pin="VSS1" pad="B1"/>
<connect gate="LPC" pin="VSS2" pad="D3"/>
<connect gate="LPC" pin="XTALIN" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FPC45" prefix="CON" uservalue="yes">
<description>&lt;b&gt;FPC Connector - 45 Pin 0.5mm Bottom Contacts&lt;/b&gt;
&lt;p&gt;Digikey: 609-1196-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FPC45"/>
</gates>
<devices>
<device name="" package="FPC45PIN">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$10" pad="P$10"/>
<connect gate="G$1" pin="P$11" pad="P$11"/>
<connect gate="G$1" pin="P$12" pad="P$12"/>
<connect gate="G$1" pin="P$13" pad="P$13"/>
<connect gate="G$1" pin="P$14" pad="P$14"/>
<connect gate="G$1" pin="P$15" pad="P$15"/>
<connect gate="G$1" pin="P$16" pad="P$16"/>
<connect gate="G$1" pin="P$17" pad="P$17"/>
<connect gate="G$1" pin="P$18" pad="P$18"/>
<connect gate="G$1" pin="P$19" pad="P$19"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$20" pad="P$20"/>
<connect gate="G$1" pin="P$21" pad="P$21"/>
<connect gate="G$1" pin="P$22" pad="P$22"/>
<connect gate="G$1" pin="P$23" pad="P$23"/>
<connect gate="G$1" pin="P$24" pad="P$24"/>
<connect gate="G$1" pin="P$25" pad="P$25"/>
<connect gate="G$1" pin="P$26" pad="P$26"/>
<connect gate="G$1" pin="P$27" pad="P$27"/>
<connect gate="G$1" pin="P$28" pad="P$28"/>
<connect gate="G$1" pin="P$29" pad="P$29"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$30" pad="P$30"/>
<connect gate="G$1" pin="P$31" pad="P$31"/>
<connect gate="G$1" pin="P$32" pad="P$32"/>
<connect gate="G$1" pin="P$33" pad="P$33"/>
<connect gate="G$1" pin="P$34" pad="P$34"/>
<connect gate="G$1" pin="P$35" pad="P$35"/>
<connect gate="G$1" pin="P$36" pad="P$36"/>
<connect gate="G$1" pin="P$37" pad="P$37"/>
<connect gate="G$1" pin="P$38" pad="P$38"/>
<connect gate="G$1" pin="P$39" pad="P$39"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$40" pad="P$40"/>
<connect gate="G$1" pin="P$41" pad="P$41"/>
<connect gate="G$1" pin="P$42" pad="P$42"/>
<connect gate="G$1" pin="P$43" pad="P$43"/>
<connect gate="G$1" pin="P$44" pad="P$44"/>
<connect gate="G$1" pin="P$45" pad="P$45"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
<connect gate="G$1" pin="P$7" pad="P$7"/>
<connect gate="G$1" pin="P$8" pad="P$8"/>
<connect gate="G$1" pin="P$9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_EINK_10BAR" prefix="LCD" uservalue="yes">
<description>&lt;b&gt;eInk 10-Bar Display&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="EINK_10BAR"/>
</gates>
<devices>
<device name="" package="EINK_10BAR">
<connects>
<connect gate="G$1" pin="1" pad="P$6"/>
<connect gate="G$1" pin="10" pad="P$12"/>
<connect gate="G$1" pin="2" pad="P$3"/>
<connect gate="G$1" pin="3" pad="P$2"/>
<connect gate="G$1" pin="4" pad="P$1"/>
<connect gate="G$1" pin="5" pad="P$7"/>
<connect gate="G$1" pin="6" pad="P$8"/>
<connect gate="G$1" pin="7" pad="P$9"/>
<connect gate="G$1" pin="8" pad="P$10"/>
<connect gate="G$1" pin="9" pad="P$11"/>
<connect gate="G$1" pin="FIELD" pad="P$4"/>
<connect gate="G$1" pin="TPLANE" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_SIM900_LITERAL" prefix="IC" uservalue="yes">
<description>&lt;b&gt;SIM900 Quad-Band GSM/GPRS Module&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;Power Supply: 3.2-4.8V&lt;/li&gt;
&lt;li&gt;Temperature Range: -30°C-+80°C&lt;/li&gt;
&lt;li&gt;Bands: GSM 850, EGSM 900, DCS 1800, PCS 1900&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SIM900_LITERAL"/>
</gates>
<devices>
<device name="" package="SIM900_SMT">
<connects>
<connect gate="G$1" pin="ADC" pad="P$25"/>
<connect gate="G$1" pin="CTS" pad="P$7"/>
<connect gate="G$1" pin="DBG_RXD" pad="P$28"/>
<connect gate="G$1" pin="DBG_TXD" pad="P$27"/>
<connect gate="G$1" pin="DCD" pad="P$5"/>
<connect gate="G$1" pin="DISP_CLK" pad="P$11"/>
<connect gate="G$1" pin="DISP_CS" pad="P$14"/>
<connect gate="G$1" pin="DISP_DATA" pad="P$12"/>
<connect gate="G$1" pin="DISP_DC" pad="P$13"/>
<connect gate="G$1" pin="DTR" pad="P$3"/>
<connect gate="G$1" pin="GND@1" pad="P$17"/>
<connect gate="G$1" pin="GND@10" pad="P$59"/>
<connect gate="G$1" pin="GND@11" pad="P$61"/>
<connect gate="G$1" pin="GND@12" pad="P$62"/>
<connect gate="G$1" pin="GND@13" pad="P$63"/>
<connect gate="G$1" pin="GND@14" pad="P$64"/>
<connect gate="G$1" pin="GND@15" pad="P$65"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND@3" pad="P$29"/>
<connect gate="G$1" pin="GND@4" pad="P$39"/>
<connect gate="G$1" pin="GND@5" pad="P$45"/>
<connect gate="G$1" pin="GND@6" pad="P$46"/>
<connect gate="G$1" pin="GND@7" pad="P$53"/>
<connect gate="G$1" pin="GND@8" pad="P$54"/>
<connect gate="G$1" pin="GND@9" pad="P$58"/>
<connect gate="G$1" pin="GPIO1/KBR4" pad="P$40"/>
<connect gate="G$1" pin="GPIO10" pad="P$51"/>
<connect gate="G$1" pin="GPIO11" pad="P$67"/>
<connect gate="G$1" pin="GPIO12" pad="P$68"/>
<connect gate="G$1" pin="GPIO2/KBR3" pad="P$41"/>
<connect gate="G$1" pin="GPIO3/KBR2" pad="P$42"/>
<connect gate="G$1" pin="GPIO4/KBR1" pad="P$43"/>
<connect gate="G$1" pin="GPIO5/KBR0" pad="P$44"/>
<connect gate="G$1" pin="GPIO6/KBC4" pad="P$47"/>
<connect gate="G$1" pin="GPIO7/KBC3" pad="P$48"/>
<connect gate="G$1" pin="GPIO8/KBC2" pad="P$49"/>
<connect gate="G$1" pin="GPIO9/KBC1" pad="P$50"/>
<connect gate="G$1" pin="LINEIN_L" pad="P$24"/>
<connect gate="G$1" pin="LINEIN_R" pad="P$23"/>
<connect gate="G$1" pin="MIC_N" pad="P$20"/>
<connect gate="G$1" pin="MIC_P" pad="P$19"/>
<connect gate="G$1" pin="NC@1" pad="P$2"/>
<connect gate="G$1" pin="NC@2" pad="P$6"/>
<connect gate="G$1" pin="NETLIGHT" pad="P$52"/>
<connect gate="G$1" pin="NRESET" pad="P$16"/>
<connect gate="G$1" pin="PWM1" pad="P$35"/>
<connect gate="G$1" pin="PWM2" pad="P$36"/>
<connect gate="G$1" pin="PWRKEY" pad="P$1"/>
<connect gate="G$1" pin="RF_ANT" pad="P$60"/>
<connect gate="G$1" pin="RI" pad="P$4"/>
<connect gate="G$1" pin="RTS" pad="P$8"/>
<connect gate="G$1" pin="RXD" pad="P$10"/>
<connect gate="G$1" pin="SCL" pad="P$38"/>
<connect gate="G$1" pin="SDA" pad="P$37"/>
<connect gate="G$1" pin="SIM_CLK" pad="P$32"/>
<connect gate="G$1" pin="SIM_DATA" pad="P$31"/>
<connect gate="G$1" pin="SIM_PRESENCE" pad="P$34"/>
<connect gate="G$1" pin="SIM_RST" pad="P$33"/>
<connect gate="G$1" pin="SIM_VDD" pad="P$30"/>
<connect gate="G$1" pin="SPK_N" pad="P$22"/>
<connect gate="G$1" pin="SPK_P" pad="P$21"/>
<connect gate="G$1" pin="STATUS" pad="P$66"/>
<connect gate="G$1" pin="TXD" pad="P$9"/>
<connect gate="G$1" pin="VBAT1" pad="P$55"/>
<connect gate="G$1" pin="VBAT2" pad="P$56"/>
<connect gate="G$1" pin="VBAT3" pad="P$57"/>
<connect gate="G$1" pin="VDD_EXT" pad="P$15"/>
<connect gate="G$1" pin="VRTC" pad="P$26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIM_LOCK" prefix="X">
<description>&lt;b&gt;C707A SIMLOCK® 2.5 mm with wide solder tails&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.amphenol.info/downloads/C707_10M006_512_2.pdf"&gt;Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="SIMLOCK-6"/>
</gates>
<devices>
<device name="AMPHENOL" package="C707_10M006_512_2">
<connects>
<connect gate="G$1" pin="1" pad="C1"/>
<connect gate="G$1" pin="2" pad="C2"/>
<connect gate="G$1" pin="3" pad="C3"/>
<connect gate="G$1" pin="4" pad="C5"/>
<connect gate="G$1" pin="5" pad="C6"/>
<connect gate="G$1" pin="6" pad="C7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="" package="SIM_5002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-N_DUAL" prefix="Q" uservalue="yes">
<description>&lt;b&gt;Dual N-Channel MOSFET&lt;/b&gt;
&lt;p&gt;&lt;b&gt;SOT363&lt;/b&gt; (2.0x1.25mm)&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;2N7002PS - 60V, 320mA [Digikey: 568-5984-1-ND]&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
<gate name="G$2" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="D" pad="6"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="S" pad="1"/>
<connect gate="G$2" pin="D" pad="3"/>
<connect gate="G$2" pin="G" pad="5"/>
<connect gate="G$2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_SOT23" prefix="U" uservalue="yes">
<description>&lt;b&gt;SOT23 Fixed Voltage Regulators&lt;/b&gt;
&lt;br/&gt;
&lt;table width="550"&gt;
&lt;tr bgcolor="#EEEEEE" &gt;
&lt;td&gt;&lt;b&gt;Part&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Current Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Out&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V In&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;V Dropout&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Digikey Part No.&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;AP7313&lt;/td&gt;
  &lt;td&gt;150mA&lt;/td&gt;
  &lt;td&gt;&lt;b&gt;3.3V&lt;/b&gt;&lt;/td&gt;
  &lt;td&gt;3.5-6V&lt;/td&gt;
  &lt;td&gt;0.15V @ 150mA&lt;/td&gt;
  &lt;td&gt;AP7313-33SAG-7DICT-ND&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
  &lt;td&gt;&lt;/td&gt;
&lt;/tr&gt;

&lt;/table&gt;</description>
<gates>
<gate name="G$1" symbol="VREG_SOT23"/>
</gates>
<devices>
<device name="" package="SOT23-R">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_WIDE" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR_4PACK" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor Packs (4 resistors)&lt;/b&gt;
&lt;p&gt;&lt;b&gt;4 x 0603&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;&lt;li&gt;10K 1/16W - Digikey: YC164J-10KCT-ND&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
<gate name="G$2" symbol="RESISTOR"/>
<gate name="G$3" symbol="RESISTOR"/>
<gate name="G$4" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="RESPACK_4X0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$2" pin="1" pad="2"/>
<connect gate="G$2" pin="2" pad="7"/>
<connect gate="G$3" pin="1" pad="3"/>
<connect gate="G$3" pin="2" pad="6"/>
<connect gate="G$4" pin="1" pad="4"/>
<connect gate="G$4" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR_4PACK_US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor Packs (4 resistors)&lt;/b&gt;
&lt;p&gt;&lt;b&gt;4 x 0603&lt;/b&gt;&lt;/p&gt;
&lt;ul&gt;&lt;li&gt;10K 1/16W - Digikey: YC164J-10KCT-ND&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="R-US"/>
<gate name="G$2" symbol="R-US"/>
<gate name="G$3" symbol="R-US"/>
<gate name="G$4" symbol="R-US"/>
</gates>
<devices>
<device name="" package="RESPACK_4X0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="8"/>
<connect gate="G$2" pin="1" pad="2"/>
<connect gate="G$2" pin="2" pad="7"/>
<connect gate="G$3" pin="1" pad="3"/>
<connect gate="G$3" pin="2" pad="6"/>
<connect gate="G$4" pin="1" pad="4"/>
<connect gate="G$4" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVSARRAY_5LANE" prefix="D" uservalue="yes">
<description>&lt;b&gt;Voltage Transient Suppressor Array&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;SOT363&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;SMF05C - 100W 5V: Digikey - SMF05CT1GOSCT-ND&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TVSARRAY_5LANE"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C1" pad="1"/>
<connect gate="G$1" pin="C2" pad="3"/>
<connect gate="G$1" pin="C3" pad="4"/>
<connect gate="G$1" pin="C4" pad="5"/>
<connect gate="G$1" pin="C5" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_3.5MMJACK" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;3.5MM Audio Jack&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;These are normally connected as follows, from left-to right on the schematic symbol above:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Tip: Left Audio&lt;/li&gt;
&lt;li&gt;Inner Ring: Right Audio&lt;/li&gt;
&lt;li&gt;Shell: Common/GND&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="3.5MMAUDIO_5PIN"/>
</gates>
<devices>
<device name="" package="4UCONN_19269">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="3"/>
<connect gate="G$1" pin="P$3" pad="5"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="4UCONN_05550">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="3"/>
<connect gate="G$1" pin="P$3" pad="2"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VRTC">
<description>VRTC Power Supply</description>
<gates>
<gate name="G$1" symbol="VRTC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_SIM900B_LITERAL" prefix="U" uservalue="yes">
<description>&lt;b&gt;SIM900B GSM/GPRS Module&lt;/b&gt;
&lt;p&gt;Supply: 3.1-4.8V
&lt;br/&gt;Quad-Band: GSM 850, EGSM 900, DCS 1800, PCS 1900&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SIM900B_LITERAL"/>
</gates>
<devices>
<device name="" package="SIM900B_SMT">
<connects>
<connect gate="G$1" pin="ADC0" pad="52"/>
<connect gate="G$1" pin="AGND1" pad="51"/>
<connect gate="G$1" pin="AGND2" pad="50"/>
<connect gate="G$1" pin="BUZZER" pad="36"/>
<connect gate="G$1" pin="CTS" pad="46"/>
<connect gate="G$1" pin="DBG_RXD" pad="47"/>
<connect gate="G$1" pin="DBG_TXD" pad="49"/>
<connect gate="G$1" pin="DCD" pad="28"/>
<connect gate="G$1" pin="DISP_CLK" pad="20"/>
<connect gate="G$1" pin="DISP_CS" pad="22"/>
<connect gate="G$1" pin="DISP_D/C" pad="24"/>
<connect gate="G$1" pin="DISP_DATA" pad="18"/>
<connect gate="G$1" pin="DISP_RST" pad="26"/>
<connect gate="G$1" pin="DTR" pad="38"/>
<connect gate="G$1" pin="GND1" pad="9"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="GND4" pad="10"/>
<connect gate="G$1" pin="GND5" pad="12"/>
<connect gate="G$1" pin="GND6" pad="14"/>
<connect gate="G$1" pin="GPIO0" pad="32"/>
<connect gate="G$1" pin="GPIO1/KBC4" pad="35"/>
<connect gate="G$1" pin="GPIO10/KBR0" pad="37"/>
<connect gate="G$1" pin="GPIO2/KBC3" pad="33"/>
<connect gate="G$1" pin="GPIO3/KBC2" pad="31"/>
<connect gate="G$1" pin="GPIO4/KBC1" pad="29"/>
<connect gate="G$1" pin="GPIO5/KBC0" pad="27"/>
<connect gate="G$1" pin="GPIO6/KBR4" pad="45"/>
<connect gate="G$1" pin="GPIO7/KBR3" pad="43"/>
<connect gate="G$1" pin="GPIO8/KBR2" pad="41"/>
<connect gate="G$1" pin="GPIO9/KBR1" pad="39"/>
<connect gate="G$1" pin="MIC1+" pad="53"/>
<connect gate="G$1" pin="MIC1-" pad="55"/>
<connect gate="G$1" pin="MIC2+" pad="57"/>
<connect gate="G$1" pin="MIC2-" pad="59"/>
<connect gate="G$1" pin="NETLIGHT" pad="30"/>
<connect gate="G$1" pin="PWRKEY" pad="34"/>
<connect gate="G$1" pin="RI" pad="48"/>
<connect gate="G$1" pin="RTS" pad="44"/>
<connect gate="G$1" pin="RXD" pad="40"/>
<connect gate="G$1" pin="SIM_CLK" pad="23"/>
<connect gate="G$1" pin="SIM_DATA" pad="21"/>
<connect gate="G$1" pin="SIM_PRESENCE" pad="16"/>
<connect gate="G$1" pin="SIM_RST" pad="25"/>
<connect gate="G$1" pin="SIM_VDD" pad="19"/>
<connect gate="G$1" pin="SPK1+" pad="54"/>
<connect gate="G$1" pin="SPK1-" pad="56"/>
<connect gate="G$1" pin="SPK2+" pad="58"/>
<connect gate="G$1" pin="SPK2-" pad="60"/>
<connect gate="G$1" pin="TXD" pad="42"/>
<connect gate="G$1" pin="VBAT1" pad="1"/>
<connect gate="G$1" pin="VBAT2" pad="3"/>
<connect gate="G$1" pin="VBAT3" pad="5"/>
<connect gate="G$1" pin="VBAT4" pad="7"/>
<connect gate="G$1" pin="VBAT5" pad="2"/>
<connect gate="G$1" pin="VBAT6" pad="4"/>
<connect gate="G$1" pin="VBAT7" pad="6"/>
<connect gate="G$1" pin="VBAT8" pad="8"/>
<connect gate="G$1" pin="VDD_EXT" pad="17"/>
<connect gate="G$1" pin="VRTC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_3.5MMJACK_4POL" prefix="CN" uservalue="yes">
<description>&lt;p&gt;Footprint courtesy Morten Hjerde (Riftlabs.com)&lt;/p&gt;
&lt;p&gt;These are normally connected as follows (4-pin 3.5mm 'TRRS'), from left-to right on the schematic symbol above:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Tip: Left Audio&lt;/li&gt;
&lt;li&gt;Outermost Ring: Right Audio&lt;/li&gt;
&lt;li&gt;Innermost Ring: Common/GND&lt;/li&gt;
&lt;li&gt;Shell: Mic+&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="JACK_4POL"/>
</gates>
<devices>
<device name="1" package="4UCONN_19621_SPARK">
<connects>
<connect gate="G$1" pin="GND" pad="1-GND"/>
<connect gate="G$1" pin="SLEEVE_INNER" pad="4-INNER_SLEEVE"/>
<connect gate="G$1" pin="SLEEVE_OUTER" pad="3-OUTER_SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="2-TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="4UCONN_19621">
<connects>
<connect gate="G$1" pin="GND" pad="1-GND"/>
<connect gate="G$1" pin="SLEEVE_INNER" pad="4-INNER_SLEEVE"/>
<connect gate="G$1" pin="SLEEVE_OUTER" pad="3-OUTER_SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="2-TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VLIPO">
<description>&lt;b&gt;VLIPO&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="VLIPO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4.5V">
<description>&lt;b&gt;4.5V Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="4.5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_CLOSED" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper - Closed&lt;/b&gt;
&lt;p&gt;These solder jumpers are closed by default&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;CLOSEDWIRE&lt;/b&gt; - 10 mil trace between pads that can be cut and resoldered later&lt;/li&gt;
&lt;li&gt;&lt;b&gt;CLOSEDPERM&lt;/b&gt; - 63 mil trace between pads for a permanent connection (used to 'bridge' two signals, a shameless hack for Eagle).  Can double as a test point as well (no cream layer)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SOLDERJUMPER_CLOSED"/>
</gates>
<devices>
<device name="" package="SOLDERJUMPER_CLOSEDWIRE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PERM" package="SOLDERJUMPER_CLOSEDPERM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_EINK_SHARPMEMORYLCD_10PIN" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Sharp Mono Memory LCD&lt;/b&gt;
&lt;p&gt;&lt;b&gt;LS013B4DN02&lt;/b&gt; - 1.35" 96x96 Pixels&lt;/p&gt;
&lt;p&gt;&lt;b&gt;LS027B7DH01&lt;/b&gt; - 2.7" 400x240 Pixels&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SHARP_LS013B4DN02"/>
</gates>
<devices>
<device name="" package="FPC_10PIN_52892-1095">
<connects>
<connect gate="G$1" pin="DISP" pad="P$5"/>
<connect gate="G$1" pin="EXTCOMIN" pad="P$4"/>
<connect gate="G$1" pin="EXTMODE" pad="P$8"/>
<connect gate="G$1" pin="SCLK" pad="P$1"/>
<connect gate="G$1" pin="SCS" pad="P$3"/>
<connect gate="G$1" pin="SI" pad="P$2"/>
<connect gate="G$1" pin="VDD" pad="P$7"/>
<connect gate="G$1" pin="VDDA" pad="P$6"/>
<connect gate="G$1" pin="VSS" pad="P$9"/>
<connect gate="G$1" pin="VSSA" pad="P$10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOCKET_LBGA256" prefix="IC">
<description>LBGA256 socket ... pitch is 1 mm</description>
<gates>
<gate name="G$1" symbol="LBGA256"/>
</gates>
<devices>
<device name="" package="SOCKET_LBGA256_8117-256-4E-01">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A16" pad="A16"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B13" pad="B13"/>
<connect gate="G$1" pin="B14" pad="B14"/>
<connect gate="G$1" pin="B15" pad="B15"/>
<connect gate="G$1" pin="B16" pad="B16"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B9" pad="B9"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C10" pad="C10"/>
<connect gate="G$1" pin="C11" pad="C11"/>
<connect gate="G$1" pin="C12" pad="C12"/>
<connect gate="G$1" pin="C13" pad="C13"/>
<connect gate="G$1" pin="C14" pad="C14"/>
<connect gate="G$1" pin="C15" pad="C15"/>
<connect gate="G$1" pin="C16" pad="C16"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="C3" pad="C3"/>
<connect gate="G$1" pin="C4" pad="C4"/>
<connect gate="G$1" pin="C5" pad="C5"/>
<connect gate="G$1" pin="C6" pad="C6"/>
<connect gate="G$1" pin="C7" pad="C7"/>
<connect gate="G$1" pin="C8" pad="C8"/>
<connect gate="G$1" pin="C9" pad="C9"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D14" pad="D14"/>
<connect gate="G$1" pin="D15" pad="D15"/>
<connect gate="G$1" pin="D16" pad="D16"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E10" pad="E10"/>
<connect gate="G$1" pin="E11" pad="E11"/>
<connect gate="G$1" pin="E12" pad="E12"/>
<connect gate="G$1" pin="E13" pad="E13"/>
<connect gate="G$1" pin="E14" pad="E14"/>
<connect gate="G$1" pin="E15" pad="E15"/>
<connect gate="G$1" pin="E16" pad="E16"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="E3" pad="E3"/>
<connect gate="G$1" pin="E4" pad="E4"/>
<connect gate="G$1" pin="E5" pad="E5"/>
<connect gate="G$1" pin="E6" pad="E6"/>
<connect gate="G$1" pin="E7" pad="E7"/>
<connect gate="G$1" pin="E8" pad="E8"/>
<connect gate="G$1" pin="E9" pad="E9"/>
<connect gate="G$1" pin="F1" pad="F1"/>
<connect gate="G$1" pin="F10" pad="F10"/>
<connect gate="G$1" pin="F11" pad="F11"/>
<connect gate="G$1" pin="F12" pad="F12"/>
<connect gate="G$1" pin="F13" pad="F13"/>
<connect gate="G$1" pin="F14" pad="F14"/>
<connect gate="G$1" pin="F15" pad="F15"/>
<connect gate="G$1" pin="F16" pad="F16"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="F3" pad="F3"/>
<connect gate="G$1" pin="F4" pad="F4"/>
<connect gate="G$1" pin="F5" pad="F5"/>
<connect gate="G$1" pin="F6" pad="F6"/>
<connect gate="G$1" pin="F7" pad="F7"/>
<connect gate="G$1" pin="F8" pad="F8"/>
<connect gate="G$1" pin="F9" pad="F9"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G10" pad="G10"/>
<connect gate="G$1" pin="G11" pad="G11"/>
<connect gate="G$1" pin="G12" pad="G12"/>
<connect gate="G$1" pin="G13" pad="G13"/>
<connect gate="G$1" pin="G14" pad="G14"/>
<connect gate="G$1" pin="G15" pad="G15"/>
<connect gate="G$1" pin="G16" pad="G16"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="G3" pad="G3"/>
<connect gate="G$1" pin="G4" pad="G4"/>
<connect gate="G$1" pin="G5" pad="G5"/>
<connect gate="G$1" pin="G6" pad="G6"/>
<connect gate="G$1" pin="G7" pad="G7"/>
<connect gate="G$1" pin="G8" pad="G8"/>
<connect gate="G$1" pin="G9" pad="G9"/>
<connect gate="G$1" pin="H1" pad="H1"/>
<connect gate="G$1" pin="H10" pad="H10"/>
<connect gate="G$1" pin="H11" pad="H11"/>
<connect gate="G$1" pin="H12" pad="H12"/>
<connect gate="G$1" pin="H13" pad="H13"/>
<connect gate="G$1" pin="H14" pad="H14"/>
<connect gate="G$1" pin="H15" pad="H15"/>
<connect gate="G$1" pin="H16" pad="H16"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="H3" pad="H3"/>
<connect gate="G$1" pin="H4" pad="H4"/>
<connect gate="G$1" pin="H5" pad="H5"/>
<connect gate="G$1" pin="H6" pad="H6"/>
<connect gate="G$1" pin="H7" pad="H7"/>
<connect gate="G$1" pin="H8" pad="H8"/>
<connect gate="G$1" pin="H9" pad="H9"/>
<connect gate="G$1" pin="J1" pad="J1"/>
<connect gate="G$1" pin="J10" pad="J10"/>
<connect gate="G$1" pin="J11" pad="J11"/>
<connect gate="G$1" pin="J12" pad="J12"/>
<connect gate="G$1" pin="J13" pad="J13"/>
<connect gate="G$1" pin="J14" pad="J14"/>
<connect gate="G$1" pin="J15" pad="J15"/>
<connect gate="G$1" pin="J16" pad="J16"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="J3" pad="J3"/>
<connect gate="G$1" pin="J4" pad="J4"/>
<connect gate="G$1" pin="J5" pad="J5"/>
<connect gate="G$1" pin="J6" pad="J6"/>
<connect gate="G$1" pin="J7" pad="J7"/>
<connect gate="G$1" pin="J8" pad="J8"/>
<connect gate="G$1" pin="J9" pad="J9"/>
<connect gate="G$1" pin="K1" pad="K1"/>
<connect gate="G$1" pin="K10" pad="K10"/>
<connect gate="G$1" pin="K11" pad="K11"/>
<connect gate="G$1" pin="K12" pad="K12"/>
<connect gate="G$1" pin="K13" pad="K13"/>
<connect gate="G$1" pin="K14" pad="K14"/>
<connect gate="G$1" pin="K15" pad="K15"/>
<connect gate="G$1" pin="K16" pad="K16"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="K3" pad="K3"/>
<connect gate="G$1" pin="K4" pad="K4"/>
<connect gate="G$1" pin="K5" pad="K5"/>
<connect gate="G$1" pin="K6" pad="K6"/>
<connect gate="G$1" pin="K7" pad="K7"/>
<connect gate="G$1" pin="K8" pad="K8"/>
<connect gate="G$1" pin="K9" pad="K9"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="L10" pad="L10"/>
<connect gate="G$1" pin="L11" pad="L11"/>
<connect gate="G$1" pin="L12" pad="L12"/>
<connect gate="G$1" pin="L13" pad="L13"/>
<connect gate="G$1" pin="L14" pad="L14"/>
<connect gate="G$1" pin="L15" pad="L15"/>
<connect gate="G$1" pin="L16" pad="L16"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="L3" pad="L3"/>
<connect gate="G$1" pin="L4" pad="L4"/>
<connect gate="G$1" pin="L5" pad="L5"/>
<connect gate="G$1" pin="L6" pad="L6"/>
<connect gate="G$1" pin="L7" pad="L7"/>
<connect gate="G$1" pin="L8" pad="L8"/>
<connect gate="G$1" pin="L9" pad="L9"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="M10" pad="M10"/>
<connect gate="G$1" pin="M11" pad="M11"/>
<connect gate="G$1" pin="M12" pad="M12"/>
<connect gate="G$1" pin="M13" pad="M13"/>
<connect gate="G$1" pin="M14" pad="M14"/>
<connect gate="G$1" pin="M15" pad="M15"/>
<connect gate="G$1" pin="M16" pad="M16"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="M3" pad="M3"/>
<connect gate="G$1" pin="M4" pad="M4"/>
<connect gate="G$1" pin="M5" pad="M5"/>
<connect gate="G$1" pin="M6" pad="M6"/>
<connect gate="G$1" pin="M7" pad="M7"/>
<connect gate="G$1" pin="M8" pad="M8"/>
<connect gate="G$1" pin="M9" pad="M9"/>
<connect gate="G$1" pin="N1" pad="N1"/>
<connect gate="G$1" pin="N10" pad="N10"/>
<connect gate="G$1" pin="N11" pad="N11"/>
<connect gate="G$1" pin="N12" pad="N12"/>
<connect gate="G$1" pin="N13" pad="N13"/>
<connect gate="G$1" pin="N14" pad="N14"/>
<connect gate="G$1" pin="N15" pad="N15"/>
<connect gate="G$1" pin="N16" pad="N16"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="N3" pad="N3"/>
<connect gate="G$1" pin="N4" pad="N4"/>
<connect gate="G$1" pin="N5" pad="N5"/>
<connect gate="G$1" pin="N6" pad="N6"/>
<connect gate="G$1" pin="N7" pad="N7"/>
<connect gate="G$1" pin="N8" pad="N8"/>
<connect gate="G$1" pin="N9" pad="N9"/>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P10" pad="P10"/>
<connect gate="G$1" pin="P11" pad="P11"/>
<connect gate="G$1" pin="P12" pad="P12"/>
<connect gate="G$1" pin="P13" pad="P13"/>
<connect gate="G$1" pin="P14" pad="P14"/>
<connect gate="G$1" pin="P15" pad="P15"/>
<connect gate="G$1" pin="P16" pad="P16"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="P3" pad="P3"/>
<connect gate="G$1" pin="P4" pad="P4"/>
<connect gate="G$1" pin="P5" pad="P5"/>
<connect gate="G$1" pin="P6" pad="P6"/>
<connect gate="G$1" pin="P7" pad="P7"/>
<connect gate="G$1" pin="P8" pad="P8"/>
<connect gate="G$1" pin="P9" pad="P9"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R10" pad="R10"/>
<connect gate="G$1" pin="R11" pad="R11"/>
<connect gate="G$1" pin="R12" pad="R12"/>
<connect gate="G$1" pin="R13" pad="R13"/>
<connect gate="G$1" pin="R14" pad="R14"/>
<connect gate="G$1" pin="R15" pad="R15"/>
<connect gate="G$1" pin="R16" pad="R16"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="R3" pad="R3"/>
<connect gate="G$1" pin="R4" pad="R4"/>
<connect gate="G$1" pin="R5" pad="R5"/>
<connect gate="G$1" pin="R6" pad="R6"/>
<connect gate="G$1" pin="R7" pad="R7"/>
<connect gate="G$1" pin="R8" pad="R8"/>
<connect gate="G$1" pin="R9" pad="R9"/>
<connect gate="G$1" pin="T1" pad="T1"/>
<connect gate="G$1" pin="T10" pad="T10"/>
<connect gate="G$1" pin="T11" pad="T11"/>
<connect gate="G$1" pin="T12" pad="T12"/>
<connect gate="G$1" pin="T13" pad="T13"/>
<connect gate="G$1" pin="T14" pad="T14"/>
<connect gate="G$1" pin="T15" pad="T15"/>
<connect gate="G$1" pin="T16" pad="T16"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="T3" pad="T3"/>
<connect gate="G$1" pin="T4" pad="T4"/>
<connect gate="G$1" pin="T5" pad="T5"/>
<connect gate="G$1" pin="T6" pad="T6"/>
<connect gate="G$1" pin="T7" pad="T7"/>
<connect gate="G$1" pin="T8" pad="T8"/>
<connect gate="G$1" pin="T9" pad="T9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC4300_LBGA256" prefix="U" uservalue="yes">
<description>&lt;b&gt;Generic LPC4300 LBGA256 Package&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LPC4300_PORT0"/>
<gate name="G$2" symbol="LPC4300_PORT1"/>
<gate name="G$3" symbol="LPC4300_PORT2"/>
<gate name="G$4" symbol="LPC4300_PORT3"/>
<gate name="G$5" symbol="LPC4300_PORT4"/>
<gate name="G$6" symbol="LPC4300_PORT5"/>
<gate name="G$7" symbol="LPC4300_PORT6"/>
<gate name="G$8" symbol="LPC4300_PORT7"/>
<gate name="G$9" symbol="LPC4300_PORT8"/>
<gate name="G$10" symbol="LPC4300_PORT9"/>
<gate name="G$11" symbol="LPC4300_PORTA"/>
<gate name="G$12" symbol="LPC4300_PORTB"/>
<gate name="G$13" symbol="LPC4300_PORTC"/>
<gate name="G$14" symbol="LPC4300_PORTD"/>
<gate name="G$15" symbol="LPC4300_PORTE"/>
<gate name="G$16" symbol="LPC4300_PORTF"/>
<gate name="G$17" symbol="LPC4300_ANA"/>
<gate name="G$18" symbol="LPC4300_AO"/>
<gate name="G$19" symbol="LPC4300_CLK"/>
<gate name="G$20" symbol="LPC4300_DBUG"/>
<gate name="G$21" symbol="LPC4300_SUP"/>
<gate name="G$22" symbol="LPC4300_USB"/>
<gate name="G$23" symbol="LPC4300_I2C"/>
</gates>
<devices>
<device name="" package="LBGA256_1.0MM">
<connects>
<connect gate="G$1" pin="PORT0_0" pad="L3"/>
<connect gate="G$1" pin="PORT0_1" pad="M2"/>
<connect gate="G$10" pin="PORT9_0" pad="T1"/>
<connect gate="G$10" pin="PORT9_1" pad="N6"/>
<connect gate="G$10" pin="PORT9_2" pad="N8"/>
<connect gate="G$10" pin="PORT9_3" pad="M6"/>
<connect gate="G$10" pin="PORT9_4" pad="N10"/>
<connect gate="G$10" pin="PORT9_5" pad="M9"/>
<connect gate="G$10" pin="PORT9_6" pad="L11"/>
<connect gate="G$11" pin="PORTA_0" pad="L12"/>
<connect gate="G$11" pin="PORTA_1" pad="J14"/>
<connect gate="G$11" pin="PORTA_2" pad="K15"/>
<connect gate="G$11" pin="PORTA_3" pad="H11"/>
<connect gate="G$11" pin="PORTA_4" pad="G13"/>
<connect gate="G$12" pin="PORTB_0" pad="B15"/>
<connect gate="G$12" pin="PORTB_1" pad="A14"/>
<connect gate="G$12" pin="PORTB_2" pad="B12"/>
<connect gate="G$12" pin="PORTB_3" pad="A13"/>
<connect gate="G$12" pin="PORTB_4" pad="B11"/>
<connect gate="G$12" pin="PORTB_5" pad="A12"/>
<connect gate="G$12" pin="PORTB_6" pad="A6"/>
<connect gate="G$13" pin="PORTC_0" pad="D4"/>
<connect gate="G$13" pin="PORTC_1" pad="E4"/>
<connect gate="G$13" pin="PORTC_10" pad="M5"/>
<connect gate="G$13" pin="PORTC_11" pad="L5"/>
<connect gate="G$13" pin="PORTC_12" pad="L6"/>
<connect gate="G$13" pin="PORTC_13" pad="M1"/>
<connect gate="G$13" pin="PORTC_14" pad="N1"/>
<connect gate="G$13" pin="PORTC_2" pad="F6"/>
<connect gate="G$13" pin="PORTC_3" pad="F5"/>
<connect gate="G$13" pin="PORTC_4" pad="F4"/>
<connect gate="G$13" pin="PORTC_5" pad="G4"/>
<connect gate="G$13" pin="PORTC_6" pad="H6"/>
<connect gate="G$13" pin="PORTC_7" pad="G5"/>
<connect gate="G$13" pin="PORTC_8" pad="N4"/>
<connect gate="G$13" pin="PORTC_9" pad="K2"/>
<connect gate="G$14" pin="PORTD_0" pad="N2"/>
<connect gate="G$14" pin="PORTD_1" pad="P1"/>
<connect gate="G$14" pin="PORTD_10" pad="P11"/>
<connect gate="G$14" pin="PORTD_11" pad="N9"/>
<connect gate="G$14" pin="PORTD_12" pad="N11"/>
<connect gate="G$14" pin="PORTD_13" pad="T14"/>
<connect gate="G$14" pin="PORTD_14" pad="R13"/>
<connect gate="G$14" pin="PORTD_15" pad="T15"/>
<connect gate="G$14" pin="PORTD_16" pad="R14"/>
<connect gate="G$14" pin="PORTD_2" pad="R1"/>
<connect gate="G$14" pin="PORTD_3" pad="P4"/>
<connect gate="G$14" pin="PORTD_4" pad="T2"/>
<connect gate="G$14" pin="PORTD_5" pad="P6"/>
<connect gate="G$14" pin="PORTD_6" pad="R6"/>
<connect gate="G$14" pin="PORTD_7" pad="T6"/>
<connect gate="G$14" pin="PORTD_8" pad="P8"/>
<connect gate="G$14" pin="PORTD_9" pad="T11"/>
<connect gate="G$15" pin="PORTE_0" pad="P14"/>
<connect gate="G$15" pin="PORTE_1" pad="N14"/>
<connect gate="G$15" pin="PORTE_10" pad="E14"/>
<connect gate="G$15" pin="PORTE_11" pad="D16"/>
<connect gate="G$15" pin="PORTE_12" pad="D15"/>
<connect gate="G$15" pin="PORTE_13" pad="G14"/>
<connect gate="G$15" pin="PORTE_14" pad="C15"/>
<connect gate="G$15" pin="PORTE_15" pad="E13"/>
<connect gate="G$15" pin="PORTE_2" pad="M14"/>
<connect gate="G$15" pin="PORTE_3" pad="K12"/>
<connect gate="G$15" pin="PORTE_4" pad="K13"/>
<connect gate="G$15" pin="PORTE_5" pad="N16"/>
<connect gate="G$15" pin="PORTE_6" pad="M16"/>
<connect gate="G$15" pin="PORTE_7" pad="F15"/>
<connect gate="G$15" pin="PORTE_8" pad="F14"/>
<connect gate="G$15" pin="PORTE_9" pad="E16"/>
<connect gate="G$16" pin="PORTF_0" pad="D12"/>
<connect gate="G$16" pin="PORTF_1" pad="E11"/>
<connect gate="G$16" pin="PORTF_10" pad="A3"/>
<connect gate="G$16" pin="PORTF_11" pad="A2"/>
<connect gate="G$16" pin="PORTF_2" pad="D11"/>
<connect gate="G$16" pin="PORTF_3" pad="E10"/>
<connect gate="G$16" pin="PORTF_4" pad="D10"/>
<connect gate="G$16" pin="PORTF_5" pad="E9"/>
<connect gate="G$16" pin="PORTF_6" pad="E7"/>
<connect gate="G$16" pin="PORTF_7" pad="B7"/>
<connect gate="G$16" pin="PORTF_8" pad="E6"/>
<connect gate="G$16" pin="PORTF_9" pad="D6"/>
<connect gate="G$17" pin="ADC0" pad="E3"/>
<connect gate="G$17" pin="ADC1" pad="C3"/>
<connect gate="G$17" pin="ADC2" pad="A4"/>
<connect gate="G$17" pin="ADC3" pad="B5"/>
<connect gate="G$17" pin="ADC4" pad="C6"/>
<connect gate="G$17" pin="ADC5" pad="B3"/>
<connect gate="G$17" pin="ADC6" pad="A5"/>
<connect gate="G$17" pin="ADC7" pad="C5"/>
<connect gate="G$17" pin="VDDA" pad="B4"/>
<connect gate="G$17" pin="VSSA" pad="B2"/>
<connect gate="G$18" pin="ALARM" pad="A11"/>
<connect gate="G$18" pin="RESET" pad="D9"/>
<connect gate="G$18" pin="RTCX1" pad="A8"/>
<connect gate="G$18" pin="RTXC2" pad="B8"/>
<connect gate="G$18" pin="SAMPLE_N" pad="B9"/>
<connect gate="G$18" pin="VBAT" pad="B10"/>
<connect gate="G$18" pin="WAKEUP0" pad="A9"/>
<connect gate="G$18" pin="WAKEUP1" pad="A10"/>
<connect gate="G$18" pin="WAKEUP2" pad="C9"/>
<connect gate="G$18" pin="WAKEUP3" pad="D8"/>
<connect gate="G$19" pin="CLK0" pad="N5"/>
<connect gate="G$19" pin="CLK1" pad="T10"/>
<connect gate="G$19" pin="CLK2" pad="D14"/>
<connect gate="G$19" pin="CLK3" pad="P12"/>
<connect gate="G$19" pin="XTAL1" pad="D1"/>
<connect gate="G$19" pin="XTAL2" pad="E1"/>
<connect gate="G$2" pin="PORT1_0" pad="P2"/>
<connect gate="G$2" pin="PORT1_1" pad="R2"/>
<connect gate="G$2" pin="PORT1_10" pad="R8"/>
<connect gate="G$2" pin="PORT1_11" pad="T9"/>
<connect gate="G$2" pin="PORT1_12" pad="R9"/>
<connect gate="G$2" pin="PORT1_13" pad="R10"/>
<connect gate="G$2" pin="PORT1_14" pad="R11"/>
<connect gate="G$2" pin="PORT1_15" pad="T12"/>
<connect gate="G$2" pin="PORT1_16" pad="M7"/>
<connect gate="G$2" pin="PORT1_17" pad="M8"/>
<connect gate="G$2" pin="PORT1_18" pad="N12"/>
<connect gate="G$2" pin="PORT1_19" pad="M11"/>
<connect gate="G$2" pin="PORT1_2" pad="R3"/>
<connect gate="G$2" pin="PORT1_20" pad="M10"/>
<connect gate="G$2" pin="PORT1_3" pad="P5"/>
<connect gate="G$2" pin="PORT1_4" pad="T3"/>
<connect gate="G$2" pin="PORT1_5" pad="R5"/>
<connect gate="G$2" pin="PORT1_6" pad="T4"/>
<connect gate="G$2" pin="PORT1_7" pad="T5"/>
<connect gate="G$2" pin="PORT1_8" pad="R7"/>
<connect gate="G$2" pin="PORT1_9" pad="T7"/>
<connect gate="G$20" pin="DBGEN" pad="L4"/>
<connect gate="G$20" pin="TCK" pad="J5"/>
<connect gate="G$20" pin="TDI" pad="J4"/>
<connect gate="G$20" pin="TDO" pad="K5"/>
<connect gate="G$20" pin="TMS" pad="K6"/>
<connect gate="G$20" pin="TRST" pad="M4"/>
<connect gate="G$21" pin="VDDC@1" pad="F9"/>
<connect gate="G$21" pin="VDDC@2" pad="F10"/>
<connect gate="G$21" pin="VDDC@3" pad="L8"/>
<connect gate="G$21" pin="VDDC@4" pad="L7"/>
<connect gate="G$21" pin="VDDE@1" pad="D7"/>
<connect gate="G$21" pin="VDDE@10" pad="L9"/>
<connect gate="G$21" pin="VDDE@11" pad="L10"/>
<connect gate="G$21" pin="VDDE@12" pad="N7"/>
<connect gate="G$21" pin="VDDE@13" pad="N13"/>
<connect gate="G$21" pin="VDDE@2" pad="E12"/>
<connect gate="G$21" pin="VDDE@3" pad="F7"/>
<connect gate="G$21" pin="VDDE@4" pad="F8"/>
<connect gate="G$21" pin="VDDE@5" pad="G10"/>
<connect gate="G$21" pin="VDDE@6" pad="H10"/>
<connect gate="G$21" pin="VDDE@7" pad="J6"/>
<connect gate="G$21" pin="VDDE@8" pad="J7"/>
<connect gate="G$21" pin="VDDE@9" pad="K7"/>
<connect gate="G$21" pin="VPP" pad="E8"/>
<connect gate="G$21" pin="VSS@1" pad="C4"/>
<connect gate="G$21" pin="VSS@10" pad="K9"/>
<connect gate="G$21" pin="VSS@11" pad="K10"/>
<connect gate="G$21" pin="VSS@12" pad="M13"/>
<connect gate="G$21" pin="VSS@13" pad="P7"/>
<connect gate="G$21" pin="VSS@14" pad="P13"/>
<connect gate="G$21" pin="VSS@15" pad="G9"/>
<connect gate="G$21" pin="VSS@16" pad="H7"/>
<connect gate="G$21" pin="VSS@17" pad="J10"/>
<connect gate="G$21" pin="VSS@18" pad="J11"/>
<connect gate="G$21" pin="VSS@19" pad="K8"/>
<connect gate="G$21" pin="VSS@2" pad="D13"/>
<connect gate="G$21" pin="VSS@3" pad="G6"/>
<connect gate="G$21" pin="VSS@4" pad="G7"/>
<connect gate="G$21" pin="VSS@5" pad="G8"/>
<connect gate="G$21" pin="VSS@6" pad="H8"/>
<connect gate="G$21" pin="VSS@7" pad="H9"/>
<connect gate="G$21" pin="VSS@8" pad="J8"/>
<connect gate="G$21" pin="VSS@9" pad="J9"/>
<connect gate="G$22" pin="USB_DM0" pad="G2"/>
<connect gate="G$22" pin="USB_DM1" pad="G12"/>
<connect gate="G$22" pin="USB_DP0" pad="F2"/>
<connect gate="G$22" pin="USB_DP1" pad="F12"/>
<connect gate="G$22" pin="USB_ID" pad="H2"/>
<connect gate="G$22" pin="USB_RREF" pad="H1"/>
<connect gate="G$22" pin="USB_VBUS" pad="F1"/>
<connect gate="G$22" pin="USB_VDDA3V3" pad="G3"/>
<connect gate="G$22" pin="USB_VDDA3V3_DRIVER" pad="F3"/>
<connect gate="G$22" pin="USB_VSSA_REF" pad="G1"/>
<connect gate="G$22" pin="USB_VSSA_TERM" pad="H3"/>
<connect gate="G$23" pin="SCL" pad="L15"/>
<connect gate="G$23" pin="SDA" pad="L16"/>
<connect gate="G$3" pin="PORT2_0" pad="T16"/>
<connect gate="G$3" pin="PORT2_1" pad="N15"/>
<connect gate="G$3" pin="PORT2_10" pad="G16"/>
<connect gate="G$3" pin="PORT2_11" pad="F16"/>
<connect gate="G$3" pin="PORT2_12" pad="E15"/>
<connect gate="G$3" pin="PORT2_13" pad="C16"/>
<connect gate="G$3" pin="PORT2_2" pad="M15"/>
<connect gate="G$3" pin="PORT2_3" pad="J12"/>
<connect gate="G$3" pin="PORT2_4" pad="K11"/>
<connect gate="G$3" pin="PORT2_5" pad="K14"/>
<connect gate="G$3" pin="PORT2_6" pad="K16"/>
<connect gate="G$3" pin="PORT2_7" pad="H14"/>
<connect gate="G$3" pin="PORT2_8" pad="J16"/>
<connect gate="G$3" pin="PORT2_9" pad="H16"/>
<connect gate="G$4" pin="PORT3_0" pad="F13"/>
<connect gate="G$4" pin="PORT3_1" pad="G11"/>
<connect gate="G$4" pin="PORT3_2" pad="F11"/>
<connect gate="G$4" pin="PORT3_3" pad="B14"/>
<connect gate="G$4" pin="PORT3_4" pad="A15"/>
<connect gate="G$4" pin="PORT3_5" pad="C12"/>
<connect gate="G$4" pin="PORT3_6" pad="B13"/>
<connect gate="G$4" pin="PORT3_7" pad="C11"/>
<connect gate="G$4" pin="PORT3_8" pad="C10"/>
<connect gate="G$5" pin="PORT4_0" pad="D5"/>
<connect gate="G$5" pin="PORT4_1" pad="A1"/>
<connect gate="G$5" pin="PORT4_10" pad="M3"/>
<connect gate="G$5" pin="PORT4_2" pad="D3"/>
<connect gate="G$5" pin="PORT4_3" pad="C2"/>
<connect gate="G$5" pin="PORT4_4" pad="B1"/>
<connect gate="G$5" pin="PORT4_5" pad="D2"/>
<connect gate="G$5" pin="PORT4_6" pad="C1"/>
<connect gate="G$5" pin="PORT4_7" pad="H4"/>
<connect gate="G$5" pin="PORT4_8" pad="E2"/>
<connect gate="G$5" pin="PORT4_9" pad="L2"/>
<connect gate="G$6" pin="PORT5_0" pad="N3"/>
<connect gate="G$6" pin="PORT5_1" pad="P3"/>
<connect gate="G$6" pin="PORT5_2" pad="R4"/>
<connect gate="G$6" pin="PORT5_3" pad="T8"/>
<connect gate="G$6" pin="PORT5_4" pad="P9"/>
<connect gate="G$6" pin="PORT5_5" pad="P10"/>
<connect gate="G$6" pin="PORT5_6" pad="T13"/>
<connect gate="G$6" pin="PORT5_7" pad="R12"/>
<connect gate="G$7" pin="PORT6_0" pad="M12"/>
<connect gate="G$7" pin="PORT6_1" pad="R15"/>
<connect gate="G$7" pin="PORT6_10" pad="H15"/>
<connect gate="G$7" pin="PORT6_11" pad="H12"/>
<connect gate="G$7" pin="PORT6_12" pad="G15"/>
<connect gate="G$7" pin="PORT6_2" pad="L13"/>
<connect gate="G$7" pin="PORT6_3" pad="P15"/>
<connect gate="G$7" pin="PORT6_4" pad="R16"/>
<connect gate="G$7" pin="PORT6_5" pad="P16"/>
<connect gate="G$7" pin="PORT6_6" pad="L14"/>
<connect gate="G$7" pin="PORT6_7" pad="J13"/>
<connect gate="G$7" pin="PORT6_8" pad="H13"/>
<connect gate="G$7" pin="PORT6_9" pad="J15"/>
<connect gate="G$8" pin="PORT7_0" pad="B16"/>
<connect gate="G$8" pin="PORT7_1" pad="C14"/>
<connect gate="G$8" pin="PORT7_2" pad="A16"/>
<connect gate="G$8" pin="PORT7_3" pad="C13"/>
<connect gate="G$8" pin="PORT7_4" pad="C8"/>
<connect gate="G$8" pin="PORT7_5" pad="A7"/>
<connect gate="G$8" pin="PORT7_6" pad="C7"/>
<connect gate="G$8" pin="PORT7_7" pad="B6"/>
<connect gate="G$9" pin="PORT8_0" pad="E5"/>
<connect gate="G$9" pin="PORT8_1" pad="H5"/>
<connect gate="G$9" pin="PORT8_2" pad="K4"/>
<connect gate="G$9" pin="PORT8_3" pad="J3"/>
<connect gate="G$9" pin="PORT8_4" pad="J2"/>
<connect gate="G$9" pin="PORT8_5" pad="J1"/>
<connect gate="G$9" pin="PORT8_6" pad="K3"/>
<connect gate="G$9" pin="PORT8_7" pad="K1"/>
<connect gate="G$9" pin="PORT8_8" pad="L1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1800_LBGA256" prefix="U" uservalue="yes">
<description>&lt;b&gt;Generic LPC1800 LBGA256 Package&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1800_PORT0"/>
<gate name="G$2" symbol="LPC1800_PORT1"/>
<gate name="G$3" symbol="LPC1800_PORT2"/>
<gate name="G$4" symbol="LPC1800_PORT3"/>
<gate name="G$5" symbol="LPC1800_PORT4"/>
<gate name="G$6" symbol="LPC1800_PORT5"/>
<gate name="G$7" symbol="LPC1800_PORT6"/>
<gate name="G$8" symbol="LPC1800_PORT7"/>
<gate name="G$9" symbol="LPC1800_PORT8"/>
<gate name="G$10" symbol="LPC1800_PORT9"/>
<gate name="G$11" symbol="LPC1800_PORTA"/>
<gate name="G$12" symbol="LPC1800_PORTB"/>
<gate name="G$13" symbol="LPC1800_PORTC"/>
<gate name="G$14" symbol="LPC1800_PORTD"/>
<gate name="G$15" symbol="LPC1800_PORTE"/>
<gate name="G$16" symbol="LPC1800_PORTF"/>
<gate name="G$17" symbol="LPC1800_ANA"/>
<gate name="G$18" symbol="LPC1800_AO"/>
<gate name="G$19" symbol="LPC1800_CLK"/>
<gate name="G$20" symbol="LPC1800_DBUG"/>
<gate name="G$21" symbol="LPC1800_SUP"/>
<gate name="G$22" symbol="LPC1800_USB"/>
<gate name="G$23" symbol="LPC1800_I2C"/>
</gates>
<devices>
<device name="" package="LBGA256_1.0MM">
<connects>
<connect gate="G$1" pin="PORT0_0" pad="L3"/>
<connect gate="G$1" pin="PORT0_1" pad="M2"/>
<connect gate="G$10" pin="PORT9_0" pad="T1"/>
<connect gate="G$10" pin="PORT9_1" pad="N6"/>
<connect gate="G$10" pin="PORT9_2" pad="N8"/>
<connect gate="G$10" pin="PORT9_3" pad="M6"/>
<connect gate="G$10" pin="PORT9_4" pad="N10"/>
<connect gate="G$10" pin="PORT9_5" pad="M9"/>
<connect gate="G$10" pin="PORT9_6" pad="L11"/>
<connect gate="G$11" pin="PORTA_0" pad="L12"/>
<connect gate="G$11" pin="PORTA_1" pad="J14"/>
<connect gate="G$11" pin="PORTA_2" pad="K15"/>
<connect gate="G$11" pin="PORTA_3" pad="H11"/>
<connect gate="G$11" pin="PORTA_4" pad="G13"/>
<connect gate="G$12" pin="PORTB_0" pad="B15"/>
<connect gate="G$12" pin="PORTB_1" pad="A14"/>
<connect gate="G$12" pin="PORTB_2" pad="B12"/>
<connect gate="G$12" pin="PORTB_3" pad="A13"/>
<connect gate="G$12" pin="PORTB_4" pad="B11"/>
<connect gate="G$12" pin="PORTB_5" pad="A12"/>
<connect gate="G$12" pin="PORTB_6" pad="A6"/>
<connect gate="G$13" pin="PORTC_0" pad="D4"/>
<connect gate="G$13" pin="PORTC_1" pad="E4"/>
<connect gate="G$13" pin="PORTC_10" pad="M5"/>
<connect gate="G$13" pin="PORTC_11" pad="L5"/>
<connect gate="G$13" pin="PORTC_12" pad="L6"/>
<connect gate="G$13" pin="PORTC_13" pad="M1"/>
<connect gate="G$13" pin="PORTC_14" pad="N1"/>
<connect gate="G$13" pin="PORTC_2" pad="F6"/>
<connect gate="G$13" pin="PORTC_3" pad="F5"/>
<connect gate="G$13" pin="PORTC_4" pad="F4"/>
<connect gate="G$13" pin="PORTC_5" pad="G4"/>
<connect gate="G$13" pin="PORTC_6" pad="H6"/>
<connect gate="G$13" pin="PORTC_7" pad="G5"/>
<connect gate="G$13" pin="PORTC_8" pad="N4"/>
<connect gate="G$13" pin="PORTC_9" pad="K2"/>
<connect gate="G$14" pin="PORTD_0" pad="N2"/>
<connect gate="G$14" pin="PORTD_1" pad="P1"/>
<connect gate="G$14" pin="PORTD_10" pad="P11"/>
<connect gate="G$14" pin="PORTD_11" pad="N9"/>
<connect gate="G$14" pin="PORTD_12" pad="N11"/>
<connect gate="G$14" pin="PORTD_13" pad="T14"/>
<connect gate="G$14" pin="PORTD_14" pad="R13"/>
<connect gate="G$14" pin="PORTD_15" pad="T15"/>
<connect gate="G$14" pin="PORTD_16" pad="R14"/>
<connect gate="G$14" pin="PORTD_2" pad="R1"/>
<connect gate="G$14" pin="PORTD_3" pad="P4"/>
<connect gate="G$14" pin="PORTD_4" pad="T2"/>
<connect gate="G$14" pin="PORTD_5" pad="P6"/>
<connect gate="G$14" pin="PORTD_6" pad="R6"/>
<connect gate="G$14" pin="PORTD_7" pad="T6"/>
<connect gate="G$14" pin="PORTD_8" pad="P8"/>
<connect gate="G$14" pin="PORTD_9" pad="T11"/>
<connect gate="G$15" pin="PORTE_0" pad="P14"/>
<connect gate="G$15" pin="PORTE_1" pad="N14"/>
<connect gate="G$15" pin="PORTE_10" pad="E14"/>
<connect gate="G$15" pin="PORTE_11" pad="D16"/>
<connect gate="G$15" pin="PORTE_12" pad="D15"/>
<connect gate="G$15" pin="PORTE_13" pad="G14"/>
<connect gate="G$15" pin="PORTE_14" pad="C15"/>
<connect gate="G$15" pin="PORTE_15" pad="E13"/>
<connect gate="G$15" pin="PORTE_2" pad="M14"/>
<connect gate="G$15" pin="PORTE_3" pad="K12"/>
<connect gate="G$15" pin="PORTE_4" pad="K13"/>
<connect gate="G$15" pin="PORTE_5" pad="N16"/>
<connect gate="G$15" pin="PORTE_6" pad="M16"/>
<connect gate="G$15" pin="PORTE_7" pad="F15"/>
<connect gate="G$15" pin="PORTE_8" pad="F14"/>
<connect gate="G$15" pin="PORTE_9" pad="E16"/>
<connect gate="G$16" pin="PORTF_0" pad="D12"/>
<connect gate="G$16" pin="PORTF_1" pad="E11"/>
<connect gate="G$16" pin="PORTF_10" pad="A3"/>
<connect gate="G$16" pin="PORTF_11" pad="A2"/>
<connect gate="G$16" pin="PORTF_2" pad="D11"/>
<connect gate="G$16" pin="PORTF_3" pad="E10"/>
<connect gate="G$16" pin="PORTF_4" pad="D10"/>
<connect gate="G$16" pin="PORTF_5" pad="E9"/>
<connect gate="G$16" pin="PORTF_6" pad="E7"/>
<connect gate="G$16" pin="PORTF_7" pad="B7"/>
<connect gate="G$16" pin="PORTF_8" pad="E6"/>
<connect gate="G$16" pin="PORTF_9" pad="D6"/>
<connect gate="G$17" pin="ADC0" pad="E3"/>
<connect gate="G$17" pin="ADC1" pad="C3"/>
<connect gate="G$17" pin="ADC2" pad="A4"/>
<connect gate="G$17" pin="ADC3" pad="B5"/>
<connect gate="G$17" pin="ADC4" pad="C6"/>
<connect gate="G$17" pin="ADC5" pad="B3"/>
<connect gate="G$17" pin="ADC6" pad="A5"/>
<connect gate="G$17" pin="ADC7" pad="C5"/>
<connect gate="G$17" pin="VDDA" pad="B4"/>
<connect gate="G$17" pin="VSSA" pad="B2"/>
<connect gate="G$18" pin="ALARM" pad="A11"/>
<connect gate="G$18" pin="RESET" pad="D9"/>
<connect gate="G$18" pin="RTCX1" pad="A8"/>
<connect gate="G$18" pin="RTXC2" pad="B8"/>
<connect gate="G$18" pin="SAMPLE_N" pad="B9"/>
<connect gate="G$18" pin="VBAT" pad="B10"/>
<connect gate="G$18" pin="WAKEUP0" pad="A9"/>
<connect gate="G$18" pin="WAKEUP1" pad="A10"/>
<connect gate="G$18" pin="WAKEUP2" pad="C9"/>
<connect gate="G$18" pin="WAKEUP3" pad="D8"/>
<connect gate="G$19" pin="CLK0" pad="N5"/>
<connect gate="G$19" pin="CLK1" pad="T10"/>
<connect gate="G$19" pin="CLK2" pad="D14"/>
<connect gate="G$19" pin="CLK3" pad="P12"/>
<connect gate="G$19" pin="XTAL1" pad="D1"/>
<connect gate="G$19" pin="XTAL2" pad="E1"/>
<connect gate="G$2" pin="PORT1_0" pad="P2"/>
<connect gate="G$2" pin="PORT1_1" pad="R2"/>
<connect gate="G$2" pin="PORT1_10" pad="R8"/>
<connect gate="G$2" pin="PORT1_11" pad="T9"/>
<connect gate="G$2" pin="PORT1_12" pad="R9"/>
<connect gate="G$2" pin="PORT1_13" pad="R10"/>
<connect gate="G$2" pin="PORT1_14" pad="R11"/>
<connect gate="G$2" pin="PORT1_15" pad="T12"/>
<connect gate="G$2" pin="PORT1_16" pad="M7"/>
<connect gate="G$2" pin="PORT1_17" pad="M8"/>
<connect gate="G$2" pin="PORT1_18" pad="N12"/>
<connect gate="G$2" pin="PORT1_19" pad="M11"/>
<connect gate="G$2" pin="PORT1_2" pad="R3"/>
<connect gate="G$2" pin="PORT1_20" pad="M10"/>
<connect gate="G$2" pin="PORT1_3" pad="P5"/>
<connect gate="G$2" pin="PORT1_4" pad="T3"/>
<connect gate="G$2" pin="PORT1_5" pad="R5"/>
<connect gate="G$2" pin="PORT1_6" pad="T4"/>
<connect gate="G$2" pin="PORT1_7" pad="T5"/>
<connect gate="G$2" pin="PORT1_8" pad="R7"/>
<connect gate="G$2" pin="PORT1_9" pad="T7"/>
<connect gate="G$20" pin="DBGEN" pad="L4"/>
<connect gate="G$20" pin="TCK" pad="J5"/>
<connect gate="G$20" pin="TDI" pad="J4"/>
<connect gate="G$20" pin="TDO" pad="K5"/>
<connect gate="G$20" pin="TMS" pad="K6"/>
<connect gate="G$20" pin="TRST" pad="M4"/>
<connect gate="G$21" pin="VDDC@1" pad="F9"/>
<connect gate="G$21" pin="VDDC@2" pad="F10"/>
<connect gate="G$21" pin="VDDC@3" pad="L8"/>
<connect gate="G$21" pin="VDDC@4" pad="L7"/>
<connect gate="G$21" pin="VDDE@1" pad="D7"/>
<connect gate="G$21" pin="VDDE@10" pad="L9"/>
<connect gate="G$21" pin="VDDE@11" pad="L10"/>
<connect gate="G$21" pin="VDDE@12" pad="N7"/>
<connect gate="G$21" pin="VDDE@13" pad="N13"/>
<connect gate="G$21" pin="VDDE@2" pad="E12"/>
<connect gate="G$21" pin="VDDE@3" pad="F7"/>
<connect gate="G$21" pin="VDDE@4" pad="F8"/>
<connect gate="G$21" pin="VDDE@5" pad="G10"/>
<connect gate="G$21" pin="VDDE@6" pad="H10"/>
<connect gate="G$21" pin="VDDE@7" pad="J6"/>
<connect gate="G$21" pin="VDDE@8" pad="J7"/>
<connect gate="G$21" pin="VDDE@9" pad="K7"/>
<connect gate="G$21" pin="VPP" pad="E8"/>
<connect gate="G$21" pin="VSS@1" pad="C4"/>
<connect gate="G$21" pin="VSS@10" pad="K9"/>
<connect gate="G$21" pin="VSS@11" pad="K10"/>
<connect gate="G$21" pin="VSS@12" pad="M13"/>
<connect gate="G$21" pin="VSS@13" pad="P7"/>
<connect gate="G$21" pin="VSS@14" pad="P13"/>
<connect gate="G$21" pin="VSS@15" pad="G9"/>
<connect gate="G$21" pin="VSS@16" pad="H7"/>
<connect gate="G$21" pin="VSS@17" pad="J10"/>
<connect gate="G$21" pin="VSS@18" pad="J11"/>
<connect gate="G$21" pin="VSS@19" pad="K8"/>
<connect gate="G$21" pin="VSS@2" pad="D13"/>
<connect gate="G$21" pin="VSS@3" pad="G6"/>
<connect gate="G$21" pin="VSS@4" pad="G7"/>
<connect gate="G$21" pin="VSS@5" pad="G8"/>
<connect gate="G$21" pin="VSS@6" pad="H8"/>
<connect gate="G$21" pin="VSS@7" pad="H9"/>
<connect gate="G$21" pin="VSS@8" pad="J8"/>
<connect gate="G$21" pin="VSS@9" pad="J9"/>
<connect gate="G$22" pin="USB_DM0" pad="G2"/>
<connect gate="G$22" pin="USB_DM1" pad="G12"/>
<connect gate="G$22" pin="USB_DP0" pad="F2"/>
<connect gate="G$22" pin="USB_DP1" pad="F12"/>
<connect gate="G$22" pin="USB_ID" pad="H2"/>
<connect gate="G$22" pin="USB_RREF" pad="H1"/>
<connect gate="G$22" pin="USB_VBUS" pad="F1"/>
<connect gate="G$22" pin="USB_VDDA3V3" pad="G3"/>
<connect gate="G$22" pin="USB_VDDA3V3_DRIVER" pad="F3"/>
<connect gate="G$22" pin="USB_VSSA_REF" pad="G1"/>
<connect gate="G$22" pin="USB_VSSA_TERM" pad="H3"/>
<connect gate="G$23" pin="SCL" pad="L15"/>
<connect gate="G$23" pin="SDA" pad="L16"/>
<connect gate="G$3" pin="PORT2_0" pad="T16"/>
<connect gate="G$3" pin="PORT2_1" pad="N15"/>
<connect gate="G$3" pin="PORT2_10" pad="G16"/>
<connect gate="G$3" pin="PORT2_11" pad="F16"/>
<connect gate="G$3" pin="PORT2_12" pad="E15"/>
<connect gate="G$3" pin="PORT2_13" pad="C16"/>
<connect gate="G$3" pin="PORT2_2" pad="M15"/>
<connect gate="G$3" pin="PORT2_3" pad="J12"/>
<connect gate="G$3" pin="PORT2_4" pad="K11"/>
<connect gate="G$3" pin="PORT2_5" pad="K14"/>
<connect gate="G$3" pin="PORT2_6" pad="K16"/>
<connect gate="G$3" pin="PORT2_7" pad="H14"/>
<connect gate="G$3" pin="PORT2_8" pad="J16"/>
<connect gate="G$3" pin="PORT2_9" pad="H16"/>
<connect gate="G$4" pin="PORT3_0" pad="F13"/>
<connect gate="G$4" pin="PORT3_1" pad="G11"/>
<connect gate="G$4" pin="PORT3_2" pad="F11"/>
<connect gate="G$4" pin="PORT3_3" pad="B14"/>
<connect gate="G$4" pin="PORT3_4" pad="A15"/>
<connect gate="G$4" pin="PORT3_5" pad="C12"/>
<connect gate="G$4" pin="PORT3_6" pad="B13"/>
<connect gate="G$4" pin="PORT3_7" pad="C11"/>
<connect gate="G$4" pin="PORT3_8" pad="C10"/>
<connect gate="G$5" pin="PORT4_0" pad="D5"/>
<connect gate="G$5" pin="PORT4_1" pad="A1"/>
<connect gate="G$5" pin="PORT4_10" pad="M3"/>
<connect gate="G$5" pin="PORT4_2" pad="D3"/>
<connect gate="G$5" pin="PORT4_3" pad="C2"/>
<connect gate="G$5" pin="PORT4_4" pad="B1"/>
<connect gate="G$5" pin="PORT4_5" pad="D2"/>
<connect gate="G$5" pin="PORT4_6" pad="C1"/>
<connect gate="G$5" pin="PORT4_7" pad="H4"/>
<connect gate="G$5" pin="PORT4_8" pad="E2"/>
<connect gate="G$5" pin="PORT4_9" pad="L2"/>
<connect gate="G$6" pin="PORT5_0" pad="N3"/>
<connect gate="G$6" pin="PORT5_1" pad="P3"/>
<connect gate="G$6" pin="PORT5_2" pad="R4"/>
<connect gate="G$6" pin="PORT5_3" pad="T8"/>
<connect gate="G$6" pin="PORT5_4" pad="P9"/>
<connect gate="G$6" pin="PORT5_5" pad="P10"/>
<connect gate="G$6" pin="PORT5_6" pad="T13"/>
<connect gate="G$6" pin="PORT5_7" pad="R12"/>
<connect gate="G$7" pin="PORT6_0" pad="M12"/>
<connect gate="G$7" pin="PORT6_1" pad="R15"/>
<connect gate="G$7" pin="PORT6_10" pad="H15"/>
<connect gate="G$7" pin="PORT6_11" pad="H12"/>
<connect gate="G$7" pin="PORT6_12" pad="G15"/>
<connect gate="G$7" pin="PORT6_2" pad="L13"/>
<connect gate="G$7" pin="PORT6_3" pad="P15"/>
<connect gate="G$7" pin="PORT6_4" pad="R16"/>
<connect gate="G$7" pin="PORT6_5" pad="P16"/>
<connect gate="G$7" pin="PORT6_6" pad="L14"/>
<connect gate="G$7" pin="PORT6_7" pad="J13"/>
<connect gate="G$7" pin="PORT6_8" pad="H13"/>
<connect gate="G$7" pin="PORT6_9" pad="J15"/>
<connect gate="G$8" pin="PORT7_0" pad="B16"/>
<connect gate="G$8" pin="PORT7_1" pad="C14"/>
<connect gate="G$8" pin="PORT7_2" pad="A16"/>
<connect gate="G$8" pin="PORT7_3" pad="C13"/>
<connect gate="G$8" pin="PORT7_4" pad="C8"/>
<connect gate="G$8" pin="PORT7_5" pad="A7"/>
<connect gate="G$8" pin="PORT7_6" pad="C7"/>
<connect gate="G$8" pin="PORT7_7" pad="B6"/>
<connect gate="G$9" pin="PORT8_0" pad="E5"/>
<connect gate="G$9" pin="PORT8_1" pad="H5"/>
<connect gate="G$9" pin="PORT8_2" pad="K4"/>
<connect gate="G$9" pin="PORT8_3" pad="J3"/>
<connect gate="G$9" pin="PORT8_4" pad="J2"/>
<connect gate="G$9" pin="PORT8_5" pad="J1"/>
<connect gate="G$9" pin="PORT8_6" pad="K3"/>
<connect gate="G$9" pin="PORT8_7" pad="K1"/>
<connect gate="G$9" pin="PORT8_8" pad="L1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1778/88-LQFP208" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1778/88 - ARM Cortex M3 - 120MHz, 512KB Flash, 96KB SRAM, 4KB EEPROM&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;External Memory Controller&lt;/li&gt;
&lt;li&gt;LCD Controller&lt;/li&gt;
&lt;li&gt;10/100 Ethernet&lt;/li&gt;
&lt;li&gt;USB 2.0 Host/Device/OTG&lt;/li&gt;
&lt;li&gt;2 CAN&lt;/li&gt;
&lt;li&gt;12-bit ADC&lt;/li&gt;
&lt;li&gt;10-bit DAC&lt;/li&gt;
&lt;li&gt;SD/MMC&lt;/li&gt;
&lt;li&gt;I2S&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="_MAIN" symbol="LPC1788_PWR-208"/>
<gate name="_PORT0" symbol="LPC1788_PORT0-208"/>
<gate name="_PORT1" symbol="LPC1788_PORT1-208"/>
<gate name="_PORT2" symbol="LPC1788_PORT2-208"/>
<gate name="_PORT3" symbol="LPC1788_PORT3-208"/>
<gate name="_PORT4" symbol="LPC1788_PORT4-208"/>
<gate name="_PORT5" symbol="LPC1788_PORT5-208"/>
</gates>
<devices>
<device name="" package="LQFP208">
<connects>
<connect gate="_MAIN" pin="!JTAG_TRST!" pad="8"/>
<connect gate="_MAIN" pin="!RESET!" pad="35"/>
<connect gate="_MAIN" pin="!RSTOUT!" pad="29"/>
<connect gate="_MAIN" pin="JTAG_TCK(SWDCLK)" pad="10"/>
<connect gate="_MAIN" pin="JTAG_TDI" pad="4"/>
<connect gate="_MAIN" pin="JTAG_TDO(SWO)" pad="2"/>
<connect gate="_MAIN" pin="JTAG_TMS(SWDIO)" pad="6"/>
<connect gate="_MAIN" pin="RTCX1" pad="34"/>
<connect gate="_MAIN" pin="RTCX2" pad="36"/>
<connect gate="_MAIN" pin="RTC_ALARM" pad="37"/>
<connect gate="_MAIN" pin="VBAT" pad="38"/>
<connect gate="_MAIN" pin="VDD(3V3)1" pad="15"/>
<connect gate="_MAIN" pin="VDD(3V3)10" pad="198"/>
<connect gate="_MAIN" pin="VDD(3V3)2" pad="60"/>
<connect gate="_MAIN" pin="VDD(3V3)3" pad="71"/>
<connect gate="_MAIN" pin="VDD(3V3)4" pad="89"/>
<connect gate="_MAIN" pin="VDD(3V3)5" pad="112"/>
<connect gate="_MAIN" pin="VDD(3V3)6" pad="125"/>
<connect gate="_MAIN" pin="VDD(3V3)7" pad="146"/>
<connect gate="_MAIN" pin="VDD(3V3)8" pad="165"/>
<connect gate="_MAIN" pin="VDD(3V3)9" pad="181"/>
<connect gate="_MAIN" pin="VDD(REG)(3V3)1" pad="26"/>
<connect gate="_MAIN" pin="VDD(REG)(3V3)2" pad="86"/>
<connect gate="_MAIN" pin="VDD(REG)(3V3)3" pad="174"/>
<connect gate="_MAIN" pin="VDDA" pad="20"/>
<connect gate="_MAIN" pin="VREFP" pad="24"/>
<connect gate="_MAIN" pin="VSS(REG)1" pad="32"/>
<connect gate="_MAIN" pin="VSS(REG)2" pad="84"/>
<connect gate="_MAIN" pin="VSS(REG)3" pad="172"/>
<connect gate="_MAIN" pin="VSS1" pad="33"/>
<connect gate="_MAIN" pin="VSS10" pad="200"/>
<connect gate="_MAIN" pin="VSS2" pad="63"/>
<connect gate="_MAIN" pin="VSS3" pad="77"/>
<connect gate="_MAIN" pin="VSS4" pad="93"/>
<connect gate="_MAIN" pin="VSS5" pad="114"/>
<connect gate="_MAIN" pin="VSS6" pad="133"/>
<connect gate="_MAIN" pin="VSS7" pad="148"/>
<connect gate="_MAIN" pin="VSS8" pad="169"/>
<connect gate="_MAIN" pin="VSS9" pad="189"/>
<connect gate="_MAIN" pin="VSSA" pad="22"/>
<connect gate="_MAIN" pin="XTAL1" pad="44"/>
<connect gate="_MAIN" pin="XTAL2" pad="46"/>
<connect gate="_PORT0" pin="P0[0]/CAN_RD1/U3_TXD/I2C1_SDA/U0_TXD" pad="94"/>
<connect gate="_PORT0" pin="P0[10]/U2_TXD/I2C2_SDA/T3_MAT0" pad="98"/>
<connect gate="_PORT0" pin="P0[11]/U2_RXD/I2C2_SCL/T3_MAT1" pad="100"/>
<connect gate="_PORT0" pin="P0[12]/!USB_PPWR2!/SSP1_MISO/ADC0_IN[6]" pad="41"/>
<connect gate="_PORT0" pin="P0[13]/USB_UP_LED2/SSP1_MOSI/ADC0_IN[7]" pad="45"/>
<connect gate="_PORT0" pin="P0[14]/!USB_HSTEN2!/SSP1_SSEL/USB_CONNECT2" pad="69"/>
<connect gate="_PORT0" pin="P0[15]/U1_TXD/SSP0_SCK" pad="128"/>
<connect gate="_PORT0" pin="P0[16]/U1_RXD/SSP0_SSEL" pad="130"/>
<connect gate="_PORT0" pin="P0[17]/U1_CTS/SSP0_MISO" pad="126"/>
<connect gate="_PORT0" pin="P0[18]/U1_DCD/SSP0_MOSI" pad="124"/>
<connect gate="_PORT0" pin="P0[19]/U1_DSR/SD_CLK/I2C1_SDA" pad="122"/>
<connect gate="_PORT0" pin="P0[1]/CAN_TD1/U3_RXD/I2C1_SCL/U0_RXD" pad="96"/>
<connect gate="_PORT0" pin="P0[20]/U1_DTR/SD_CMD/I2C1_SCL" pad="120"/>
<connect gate="_PORT0" pin="P0[21]/U1_RI/SD_PWR/U4_OE/CAN_RD1" pad="118"/>
<connect gate="_PORT0" pin="P0[22]/U1_RTS/SD_DAT[0]/U4_TXD/CAN_TD1" pad="116"/>
<connect gate="_PORT0" pin="P0[23]/ADC0_IN[0]/I2S_RX_SCK/T3_CAP0" pad="18"/>
<connect gate="_PORT0" pin="P0[24]/ADC0_IN[1]/I2S_RX_WS/T3_CAP1" pad="16"/>
<connect gate="_PORT0" pin="P0[25]/ADC0_IN[2]/I2S_RX_SDA/U3_TXD" pad="14"/>
<connect gate="_PORT0" pin="P0[26]/ADC0_IN[3]/DAC_OUT/U3_RXD" pad="12"/>
<connect gate="_PORT0" pin="P0[27]/I2C0_SDA/USB_SDA1" pad="50"/>
<connect gate="_PORT0" pin="P0[28]/I2C0_SCL/USB_SCL1" pad="48"/>
<connect gate="_PORT0" pin="P0[29]/USB_D+1/EINT_0" pad="61"/>
<connect gate="_PORT0" pin="P0[2]/U0_TXD/U3_TXD" pad="202"/>
<connect gate="_PORT0" pin="P0[30]/USB_D?1/EINT_1" pad="62"/>
<connect gate="_PORT0" pin="P0[31]/USB_D+2" pad="51"/>
<connect gate="_PORT0" pin="P0[3]/U0_RXD/U3_RXD" pad="204"/>
<connect gate="_PORT0" pin="P0[4]/I2S_RX_SCK/CAN_RD_2/T2_CAP0/LCD_VD[0]" pad="168"/>
<connect gate="_PORT0" pin="P0[5]/I2S_RX_WS/CAN_TD_2/T2_CAP1/LCD_VD[1]" pad="166"/>
<connect gate="_PORT0" pin="P0[6]/I2S_RX_SDA/SSP1_SSEL/T2_MAT0/U1_RTS/LCD_VD[8]" pad="164"/>
<connect gate="_PORT0" pin="P0[7]/I2S_TX_SCK/SSP1_SCK/T2_MAT1/LCD_VD[9]" pad="162"/>
<connect gate="_PORT0" pin="P0[8]/I2S_TX_WS/SSP1_MISO/T2_MAT2/LCD_VD[16]" pad="160"/>
<connect gate="_PORT0" pin="P0[9]/I2S_TX_SDA/SSP1_MOSI/T2_MAT3/LCD_VD[17]" pad="158"/>
<connect gate="_PORT0" pin="USB_D-2" pad="52"/>
<connect gate="_PORT1" pin="P1[0]/ENET_TXD0/T3_CAP1/SSP2_SCK" pad="196"/>
<connect gate="_PORT1" pin="P1[10]/ENET_RXD1/T3_CAP0" pad="186"/>
<connect gate="_PORT1" pin="P1[11]/ENET_RXD2/SD_DAT[2]/PWM0_6" pad="163"/>
<connect gate="_PORT1" pin="P1[12]/ENET_RXD3/SD_DAT[3]/PWM0_CAP0" pad="157"/>
<connect gate="_PORT1" pin="P1[13]/ENET_RX_DV" pad="147"/>
<connect gate="_PORT1" pin="P1[14]/ENET_RX_ER/T2_CAP0" pad="184"/>
<connect gate="_PORT1" pin="P1[15]/ENET_RX_CLK/I2C2_SDA" pad="182"/>
<connect gate="_PORT1" pin="P1[16]/ENET_MDC/I2S_TX_MCLK" pad="180"/>
<connect gate="_PORT1" pin="P1[17]/ENET_MDIO/I2S_RX_MCLK" pad="178"/>
<connect gate="_PORT1" pin="P1[18]/USB_UP_LED1/PWM1_1/T1_CAP0/SSP1_MISO" pad="66"/>
<connect gate="_PORT1" pin="P1[19]/!USB_TX_E1!/!USB_PPWR1!/T1_CAP1/MC_0A/SSP1_SCK/U2_OE" pad="68"/>
<connect gate="_PORT1" pin="P1[1]/ENET_TXD1/T3_MAT3/SSP2_MOSI" pad="194"/>
<connect gate="_PORT1" pin="P1[20]/USB_TX_DP1/PWM1_2/QEI_PHA/MC_FB0/SSP0_SCK/LCD_VD[6]/LCD_VD[10]" pad="70"/>
<connect gate="_PORT1" pin="P1[21]/USB_TX_DM1/PWM1_3/SSP0_SSEL/!MC_ABORT!/LCD_VD[7]/LCD_VD[11]" pad="72"/>
<connect gate="_PORT1" pin="P1[22]/USB_RCV1/USB_PWRD1/T1_MAT0/MC_0B/SSP1_MOSI/LCD_VD[8]/LCD_VD[12]" pad="74"/>
<connect gate="_PORT1" pin="P1[23]/USB_RX_DP1/PWM1_4/QEI_PHB/MC_FB1/SSP0_MISO/LCD_VD[9]/LCD_VD[13]" pad="76"/>
<connect gate="_PORT1" pin="P1[24]/USB_RX_DM1/PWM1_5/QEI_IDX/MC_FB2/SSP0_MOSI/LCD_VD[10]/LCD_VD[14]" pad="78"/>
<connect gate="_PORT1" pin="P1[25]/!USB_LS1!/!USB_HSTEN1!/T1_MAT1/MC_1A/CLKOUT/LCD_VD[11]/LCD_VD[15]" pad="80"/>
<connect gate="_PORT1" pin="P1[26]/!USB_SSPND1!/PWM1_6/T0_CAP0/MC_1B/SSP1_SSEL/LCD_VD[12]/LCD_VD[20]" pad="82"/>
<connect gate="_PORT1" pin="P1[27]/!USB_INT1!/!USB_OVRCR1!/T0_CAP1/CLKOUT/LCD_VD[13]/LCD_VD[21]" pad="88"/>
<connect gate="_PORT1" pin="P1[28]/USB_SCL1/PWM1_CAP0/T0_MAT0/MC_2A/SSP0_SSEL/LCD_VD[14]/LCD_VD[22]" pad="90"/>
<connect gate="_PORT1" pin="P1[29]/USB_SDA1/PWM1_CAP1/T0_MAT1/MC_2B/U4_TXD/LCD_VD[15]/LCD_VD[23]" pad="92"/>
<connect gate="_PORT1" pin="P1[2]/ENET_TXD2/SD_CLK/PWM0_1" pad="185"/>
<connect gate="_PORT1" pin="P1[30]/USB_PWRD2/USB_VBUS/ADC0_IN[4]/I2C0_SDA/U3_OE" pad="42"/>
<connect gate="_PORT1" pin="P1[31]/USB_OVRCR2/SSP1_SCK/ADC0_IN[5]/I2C0_SCL" pad="40"/>
<connect gate="_PORT1" pin="P1[3]/ENET_TXD3/SD_CMD/PWM0_2" pad="177"/>
<connect gate="_PORT1" pin="P1[4]/ENET_TX_EN/T3_MAT2/SSP2_MISO" pad="192"/>
<connect gate="_PORT1" pin="P1[5]/ENET_TX_ER/SD_PWR/PWM0_3" pad="156"/>
<connect gate="_PORT1" pin="P1[6]/ENET_TX_CLK/SD_DAT[0]/PWM0_4" pad="171"/>
<connect gate="_PORT1" pin="P1[7]/ENET_COL/SD_DAT[1]/PWM0_5" pad="153"/>
<connect gate="_PORT1" pin="P1[8]/ENET_CRS/T3_MAT1/SSP2_SSEL" pad="190"/>
<connect gate="_PORT1" pin="P1[9]/ENET_RXD0/T3_MAT0" pad="188"/>
<connect gate="_PORT2" pin="P2[0]/PWM1[1]/U1_TXD/LCD_PWR" pad="154"/>
<connect gate="_PORT2" pin="P2[10]/EINT_0/NMI" pad="110"/>
<connect gate="_PORT2" pin="P2[11]/EINT1/SD_DAT[1]/I2S_TX_SCK/LCD_CLKIN" pad="108"/>
<connect gate="_PORT2" pin="P2[12]/EINT2/SD_DAT[2]/I2S_TX_WS/LCD_VD[4]/LCD_VD[3]/LCD_VD[8]/LCD_VD[18]" pad="106"/>
<connect gate="_PORT2" pin="P2[13]/EINT3/SD_DAT[3]/I2S_TX_SDA/LCD_VD[5]/LCD_VD[9]/LCD_VD[19]" pad="102"/>
<connect gate="_PORT2" pin="P2[14]/!EMC_CS2!/I2C1_SDA/T2_CAP0" pad="91"/>
<connect gate="_PORT2" pin="P2[15/!EMC_CS3!/I2C1_SCL/T2_CAP1" pad="99"/>
<connect gate="_PORT2" pin="P2[16]/!EMC_CAS!" pad="87"/>
<connect gate="_PORT2" pin="P2[17]/!EMC_RAS!" pad="95"/>
<connect gate="_PORT2" pin="P2[18]/EMC_CLK[0]" pad="59"/>
<connect gate="_PORT2" pin="P2[19]/EMC_CLK[1]" pad="67"/>
<connect gate="_PORT2" pin="P2[1]/PWM1[2]/U1_RXD/LCD_LE" pad="152"/>
<connect gate="_PORT2" pin="P2[20]/!EMC_DYCS0!" pad="73"/>
<connect gate="_PORT2" pin="P2[21]/!EMC_DYCS1!" pad="81"/>
<connect gate="_PORT2" pin="P2[22]/!EMC_DYCS2!/SSP0_SCK/T3_CAP0" pad="85"/>
<connect gate="_PORT2" pin="P2[23]/!EMC_DYCS3!/SSP0_SSEL/T3_CAP1" pad="64"/>
<connect gate="_PORT2" pin="P2[24]/EMC_CKE0" pad="53"/>
<connect gate="_PORT2" pin="P2[25]/EMC_CKE1" pad="54"/>
<connect gate="_PORT2" pin="P2[26]/EMC_CKE2/SSP0_MISO/T3_MAT0" pad="57"/>
<connect gate="_PORT2" pin="P2[27]/EMC_CKE3/SSP0_MOSI/T3_MAT1" pad="47"/>
<connect gate="_PORT2" pin="P2[28]/EMC_DQM0" pad="49"/>
<connect gate="_PORT2" pin="P2[29]/EMC_DQM1" pad="43"/>
<connect gate="_PORT2" pin="P2[2]/PWM1[3]/U1_CTS/T2_MAT3/TRACEDATA[3]/LCD_DCLK" pad="150"/>
<connect gate="_PORT2" pin="P2[30]/EMC_DQM2/I2C2_SDA/T3_MAT2" pad="31"/>
<connect gate="_PORT2" pin="P2[31]/EMC_DQM3/I2C2_SCL/T3_MAT3" pad="39"/>
<connect gate="_PORT2" pin="P2[3]/PWM1[4]/U1_DCD/T2_MAT2/TRACEDATA[2]/LCD_FP" pad="144"/>
<connect gate="_PORT2" pin="P2[4]/PWM1[5]/U1_DSR/T2_MAT1/TRACEDATA[1]/LCD_ENAB_M" pad="142"/>
<connect gate="_PORT2" pin="P2[5]/PWM1[6]/U1_DTR/T2_MAT0/TRACEDATA[0]/LCD_LP" pad="140"/>
<connect gate="_PORT2" pin="P2[6]/PWM1_CAP0/U1_RI/T2_CAP0/U2_OE/TRACECLK/LCD_VD[0]/LCD_VD[4]" pad="138"/>
<connect gate="_PORT2" pin="P2[7]/CAN_RD2/U1_RTS/LCD_VD[1]/LCD_VD[5]" pad="136"/>
<connect gate="_PORT2" pin="P2[8]/CAN_TD2/U2_TXD/U1_CTS/ENET_MDC/LCD_VD[2]/LCD_VD[6]" pad="134"/>
<connect gate="_PORT2" pin="P2[9]/USB_CONNECT1/U2_RXD/U4_RXD/ENET_MDIO/LCD_VD[3]/LCD_VD[7]" pad="132"/>
<connect gate="_PORT3" pin="P3[0]/EMC_D[0]" pad="197"/>
<connect gate="_PORT3" pin="P3[10]/EMC_D[10]" pad="205"/>
<connect gate="_PORT3" pin="P3[11]/EMC_D[11]" pad="208"/>
<connect gate="_PORT3" pin="P3[12]/EMC_D[12]" pad="1"/>
<connect gate="_PORT3" pin="P3[13]/EMC_D[13]" pad="7"/>
<connect gate="_PORT3" pin="P3[14]/EMC_D[14]" pad="21"/>
<connect gate="_PORT3" pin="P3[15]/EMC_D[15]" pad="28"/>
<connect gate="_PORT3" pin="P3[16]/EMC_D[16]/PWM0_1/U1_TXD" pad="137"/>
<connect gate="_PORT3" pin="P3[17]/EMC_D[17]/PWM0_2/U1_RXD" pad="143"/>
<connect gate="_PORT3" pin="P3[18]/EMC_D[18]/PWM0_3/U1_CTS" pad="151"/>
<connect gate="_PORT3" pin="P3[19]/EMC_D[19]/PWM0_4/U1_DCD" pad="161"/>
<connect gate="_PORT3" pin="P3[1]/EMC_D[1]" pad="201"/>
<connect gate="_PORT3" pin="P3[20]/EMC_D[20]/PWM0_5/U1_DSR" pad="167"/>
<connect gate="_PORT3" pin="P3[21]/EMC_D[21]/PWM0_6/U1_DTR" pad="175"/>
<connect gate="_PORT3" pin="P3[22]/EMC_D[22]/PWM0_CAP0/U1_RI" pad="195"/>
<connect gate="_PORT3" pin="P3[23]/EMC_D[23]/PWM1_CAP0/T0_CAP0" pad="65"/>
<connect gate="_PORT3" pin="P3[24]/EMC_D[24]/PWM1[1]/T0_CAP1" pad="58"/>
<connect gate="_PORT3" pin="P3[25]/EMC_D[25]/PWM1[2]/T0_MAT0" pad="56"/>
<connect gate="_PORT3" pin="P3[26]/EMC_D[26]/PWM1[3]/T0_MAT1/STCLK" pad="55"/>
<connect gate="_PORT3" pin="P3[27]/EMC_D[27]/PWM1[4]/T1_CAP0" pad="203"/>
<connect gate="_PORT3" pin="P3[28]/EMC_D[28]/PWM1[5]/T1_CAP1" pad="5"/>
<connect gate="_PORT3" pin="P3[29]/EMC_D[29]/PWM1[6]/T1_MAT0" pad="11"/>
<connect gate="_PORT3" pin="P3[2]/EMC_D[2]" pad="207"/>
<connect gate="_PORT3" pin="P3[30]/EMC_D[30]/U1_RTS/T1_MAT1" pad="19"/>
<connect gate="_PORT3" pin="P3[31]/EMC_D[31]/T1_MAT2" pad="25"/>
<connect gate="_PORT3" pin="P3[3]/EMC_D[3]" pad="3"/>
<connect gate="_PORT3" pin="P3[4]/EMC_D[4]" pad="13"/>
<connect gate="_PORT3" pin="P3[5]/EMC_D[5]" pad="17"/>
<connect gate="_PORT3" pin="P3[6]/EMC_D[6]" pad="23"/>
<connect gate="_PORT3" pin="P3[7]/EMC_D[7]" pad="27"/>
<connect gate="_PORT3" pin="P3[8]/EMC_D[8]" pad="191"/>
<connect gate="_PORT3" pin="P3[9]/EMC_D[9]" pad="199"/>
<connect gate="_PORT4" pin="P4[0]/EMC_A[0]" pad="75"/>
<connect gate="_PORT4" pin="P4[10]/EMC_A[10]" pad="135"/>
<connect gate="_PORT4" pin="P4[11]/EMC_A[11]" pad="145"/>
<connect gate="_PORT4" pin="P4[12]/EMC_A[12]" pad="149"/>
<connect gate="_PORT4" pin="P4[13]/EMC_A[13]" pad="155"/>
<connect gate="_PORT4" pin="P4[14]/EMC_A[14]" pad="159"/>
<connect gate="_PORT4" pin="P4[15]/EMC_A[15]" pad="173"/>
<connect gate="_PORT4" pin="P4[16]/EMC_A[16]" pad="101"/>
<connect gate="_PORT4" pin="P4[17]/EMC_A[17]" pad="104"/>
<connect gate="_PORT4" pin="P4[18]/EMC_A[18]" pad="105"/>
<connect gate="_PORT4" pin="P4[19]/EMC_A[19]" pad="111"/>
<connect gate="_PORT4" pin="P4[1]/EMC_A[1]" pad="79"/>
<connect gate="_PORT4" pin="P4[20]/EMC_A[20]/I2C2_SDA/SSP1_SCK" pad="109"/>
<connect gate="_PORT4" pin="P4[21]/EMC_A[21]/I2C2_SCL/SSP1_SSEL" pad="115"/>
<connect gate="_PORT4" pin="P4[22]/EMC_A[22]/U2_TXD/SSP1_MISO" pad="123"/>
<connect gate="_PORT4" pin="P4[23]/EMC_A[23]/U2_RXD/SSP1_MOSI" pad="129"/>
<connect gate="_PORT4" pin="P4[24]/!EMC_OE!" pad="183"/>
<connect gate="_PORT4" pin="P4[25]/!EMC_WE!" pad="179"/>
<connect gate="_PORT4" pin="P4[26]/!EMC_BLS0!" pad="119"/>
<connect gate="_PORT4" pin="P4[27]/!EMC_BLS1!" pad="139"/>
<connect gate="_PORT4" pin="P4[28]/!EMC_BLS2!/U3_TXD/T2_MAT0/LCD_VD[6]/LCD_VD[10]/LCD_VD[2]" pad="170"/>
<connect gate="_PORT4" pin="P4[29]/!EMC_BLS3!/U3_RXD/T2_MAT1/I2C2_SCL/LCD_VD[7]/LCD_VD[11]/LCD_VD[3]" pad="176"/>
<connect gate="_PORT4" pin="P4[2]/EMC_A[2]" pad="83"/>
<connect gate="_PORT4" pin="P4[30]/!EMC_CS0!" pad="187"/>
<connect gate="_PORT4" pin="P4[31]/!EMC_CS1!" pad="193"/>
<connect gate="_PORT4" pin="P4[3]/EMC_A[3]" pad="97"/>
<connect gate="_PORT4" pin="P4[4]/EMC_A[4]" pad="103"/>
<connect gate="_PORT4" pin="P4[5]/EMC_A[5]" pad="107"/>
<connect gate="_PORT4" pin="P4[6]/EMC_A[6]" pad="113"/>
<connect gate="_PORT4" pin="P4[7]/EMC_A[7]" pad="121"/>
<connect gate="_PORT4" pin="P4[8]/EMC_A[8]" pad="127"/>
<connect gate="_PORT4" pin="P4[9]/EMC_A[9]" pad="131"/>
<connect gate="_PORT5" pin="P5[0]/EMC_A[24]/T2_MAT2" pad="9"/>
<connect gate="_PORT5" pin="P5[1]/EMC_A[25]/T2_MAT3" pad="30"/>
<connect gate="_PORT5" pin="P5[2]/T3_MAT2/I2C0_SDA" pad="117"/>
<connect gate="_PORT5" pin="P5[3]/U4_RXD/I2C0_SCL" pad="141"/>
<connect gate="_PORT5" pin="P5[4]/U0_OE/T3_MAT3/U4_TXD" pad="206"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME_A3_ADAFRUIT">
<description>Frame - A3</description>
<gates>
<gate name="G$1" symbol="FRAME_A3_ADAFRUIT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME_A4_ADAFRUIT">
<description>Frame A4</description>
<gates>
<gate name="G$1" symbol="FRAME_A4_ADAFRUIT"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_SEGMENT_8X8_BICOLOR_ROWCATHODE" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;8x8 Bi-Color LED Segment Displays: Row = Cathode&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;1.2" Bi-Color 8x8 Matrix, 3.0mm Square LEDs - BL-M12A883XX&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_8X8_BICOLOR_CATHODEROW"/>
</gates>
<devices>
<device name="MI2A883XX" package="SEGMENT_BICOL_BL-M12A883XX">
<connects>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="A10" pad="2"/>
<connect gate="G$1" pin="A11" pad="4"/>
<connect gate="G$1" pin="A12" pad="5"/>
<connect gate="G$1" pin="A13" pad="7"/>
<connect gate="G$1" pin="A14" pad="8"/>
<connect gate="G$1" pin="A15" pad="10"/>
<connect gate="G$1" pin="A16" pad="11"/>
<connect gate="G$1" pin="A2" pad="23"/>
<connect gate="G$1" pin="A3" pad="21"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="A5" pad="18"/>
<connect gate="G$1" pin="A6" pad="17"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="14"/>
<connect gate="G$1" pin="A9" pad="1"/>
<connect gate="G$1" pin="K1" pad="22"/>
<connect gate="G$1" pin="K2" pad="19"/>
<connect gate="G$1" pin="K3" pad="16"/>
<connect gate="G$1" pin="K4" pad="13"/>
<connect gate="G$1" pin="K5" pad="3"/>
<connect gate="G$1" pin="K6" pad="6"/>
<connect gate="G$1" pin="K7" pad="9"/>
<connect gate="G$1" pin="K8" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_SEGMENT_8X8_ROWCATHODE" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;8x8 LED Segment Displays: Row = Cathode&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.7" Red 8X8 Matrix, 1.9mm Round LEDs - BL-M07C881UR&lt;/p&gt;
&lt;p&gt;1.2" Red 8x8 Matrix, 3.0mm Round LEDs - BL-M12A881UR&lt;/p&gt;
&lt;p&gt;1.2" Red 8x8 Matrix, 3.0mm Square LEDs - BL-M12A883&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_8X8_CATHODEROW"/>
</gates>
<devices>
<device name="" package="SEGMENT_BL-M07C881UR">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="16"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="14"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
<connect gate="G$1" pin="K3" pad="3"/>
<connect gate="G$1" pin="K4" pad="4"/>
<connect gate="G$1" pin="K5" pad="12"/>
<connect gate="G$1" pin="K6" pad="11"/>
<connect gate="G$1" pin="K7" pad="10"/>
<connect gate="G$1" pin="K8" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M12A881UR" package="SEGMENT_BL-M12A881UR">
<connects>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="10"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="16"/>
<connect gate="G$1" pin="K1" pad="9"/>
<connect gate="G$1" pin="K2" pad="14"/>
<connect gate="G$1" pin="K3" pad="8"/>
<connect gate="G$1" pin="K4" pad="12"/>
<connect gate="G$1" pin="K5" pad="1"/>
<connect gate="G$1" pin="K6" pad="7"/>
<connect gate="G$1" pin="K7" pad="2"/>
<connect gate="G$1" pin="K8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BL-M12A883" package="SEGMENT_BL-M12A883">
<connects>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="10"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="16"/>
<connect gate="G$1" pin="K1" pad="9"/>
<connect gate="G$1" pin="K2" pad="14"/>
<connect gate="G$1" pin="K3" pad="8"/>
<connect gate="G$1" pin="K4" pad="12"/>
<connect gate="G$1" pin="K5" pad="1"/>
<connect gate="G$1" pin="K6" pad="7"/>
<connect gate="G$1" pin="K7" pad="2"/>
<connect gate="G$1" pin="K8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_SEGMENT_12BAR_BICOLOR" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;12-Bar Bi-Color LED Segment Displays: Row = Cathode&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;30.2 x 10.1mm Bi-Color 12 LED Bar Graph, 5.0 x 1.74mm Square LEDs - BL-AR12Z3010&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_12BAR_BICOLOR_CATHODEROW"/>
</gates>
<devices>
<device name="AR12Z3010" package="SEGMENT_BICOL_BL-AR12Z3010">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="14"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="9"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="K1" pad="2"/>
<connect gate="G$1" pin="K2" pad="13"/>
<connect gate="G$1" pin="K3" pad="3"/>
<connect gate="G$1" pin="K4" pad="12"/>
<connect gate="G$1" pin="K5" pad="4"/>
<connect gate="G$1" pin="K6" pad="11"/>
<connect gate="G$1" pin="K7" pad="5"/>
<connect gate="G$1" pin="K8" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_SEGMENT_STARBURST_COMMONCATHODE" prefix="LED" uservalue="yes">
<description>&lt;b&gt;Starburst Segment Display - Common Cathode&lt;/b&gt;
&lt;p&gt;0.8" Red Alphanumeric LED Display - BL-S80A-13UHR-11&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_STARBURST_COMMONCATHODE"/>
</gates>
<devices>
<device name="BLS80A13" package="SEGMENT_STARBURST_BL-S80A-13">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="18"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="D1" pad="9"/>
<connect gate="G$1" pin="D2" pad="10"/>
<connect gate="G$1" pin="DP" pad="12"/>
<connect gate="G$1" pin="E" pad="8"/>
<connect gate="G$1" pin="F" pad="4"/>
<connect gate="G$1" pin="G1" pad="5"/>
<connect gate="G$1" pin="G2" pad="15"/>
<connect gate="G$1" pin="H" pad="3"/>
<connect gate="G$1" pin="J" pad="2"/>
<connect gate="G$1" pin="K" pad="17"/>
<connect gate="G$1" pin="L" pad="14"/>
<connect gate="G$1" pin="M" pad="6"/>
<connect gate="G$1" pin="N" pad="7"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_SEGMENT_STARBURST_COMMONCATHODE_2VCC" prefix="LED" uservalue="yes">
<description>&lt;b&gt;Starburst Segment Display - Common Cathode&lt;/b&gt;
&lt;p&gt;2.3" Red Alphanumeric LED Display - BL-S230B-12&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_STARBURST_COMMONCATHODE_2VCC"/>
</gates>
<devices>
<device name="BLS230B12" package="SEGMENT_STARBURST_BL-S230B-12">
<connects>
<connect gate="G$1" pin="A1" pad="17"/>
<connect gate="G$1" pin="A2" pad="14"/>
<connect gate="G$1" pin="B" pad="13"/>
<connect gate="G$1" pin="C" pad="9"/>
<connect gate="G$1" pin="D1" pad="4"/>
<connect gate="G$1" pin="D2" pad="7"/>
<connect gate="G$1" pin="DP" pad="10"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="F" pad="19"/>
<connect gate="G$1" pin="G1" pad="2"/>
<connect gate="G$1" pin="G2" pad="12"/>
<connect gate="G$1" pin="H" pad="18"/>
<connect gate="G$1" pin="J" pad="16"/>
<connect gate="G$1" pin="K" pad="15"/>
<connect gate="G$1" pin="L" pad="8"/>
<connect gate="G$1" pin="M" pad="6"/>
<connect gate="G$1" pin="N" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTC_DS1302" prefix="U" uservalue="yes">
<description>&lt;b&gt;DS1302 Trickle-Charge Timekeeping Chip&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DS1302"/>
</gates>
<devices>
<device name="150" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IO" pad="6"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="8"/>
<connect gate="G$1" pin="VCC2" pad="1"/>
<connect gate="G$1" pin="X1" pad="2"/>
<connect gate="G$1" pin="X2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="208" package="SOIC8_208MIL">
<connects>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IO" pad="6"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="8"/>
<connect gate="G$1" pin="VCC2" pad="1"/>
<connect gate="G$1" pin="X1" pad="2"/>
<connect gate="G$1" pin="X2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X23" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Pin Header&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINH2X23"/>
</gates>
<devices>
<device name="" package="2X23">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BEAGLEBONE_OUTLINE">
<gates>
<gate name="G$1" symbol="BEAGLEBONE"/>
</gates>
<devices>
<device name="" package="BEAGLEBONE_SHIELD">
<connects>
<connect gate="G$1" pin="AIN0" pad="85"/>
<connect gate="G$1" pin="AIN1" pad="86"/>
<connect gate="G$1" pin="AIN2" pad="83"/>
<connect gate="G$1" pin="AIN3" pad="84"/>
<connect gate="G$1" pin="AIN4" pad="79"/>
<connect gate="G$1" pin="AIN5" pad="82"/>
<connect gate="G$1" pin="AIN6" pad="81"/>
<connect gate="G$1" pin="CLKOUT2" pad="87"/>
<connect gate="G$1" pin="EHRPWM1A" pad="60"/>
<connect gate="G$1" pin="EHRPWM1B" pad="62"/>
<connect gate="G$1" pin="EHRPWM2A" pad="19"/>
<connect gate="G$1" pin="EHRPWM2B" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="47"/>
<connect gate="G$1" pin="GND@2" pad="48"/>
<connect gate="G$1" pin="GND@3" pad="89"/>
<connect gate="G$1" pin="GND@4" pad="91"/>
<connect gate="G$1" pin="GND@5" pad="90"/>
<connect gate="G$1" pin="GND@6" pad="92"/>
<connect gate="G$1" pin="GND@7" pad="1"/>
<connect gate="G$1" pin="GND@8" pad="2"/>
<connect gate="G$1" pin="GNDA_ADC" pad="80"/>
<connect gate="G$1" pin="GPIO0_26" pad="14"/>
<connect gate="G$1" pin="GPIO0_27" pad="17"/>
<connect gate="G$1" pin="GPIO0_7" pad="88"/>
<connect gate="G$1" pin="GPIO1_0" pad="25"/>
<connect gate="G$1" pin="GPIO1_1" pad="24"/>
<connect gate="G$1" pin="GPIO1_12" pad="12"/>
<connect gate="G$1" pin="GPIO1_13" pad="11"/>
<connect gate="G$1" pin="GPIO1_14" pad="16"/>
<connect gate="G$1" pin="GPIO1_15" pad="15"/>
<connect gate="G$1" pin="GPIO1_16" pad="61"/>
<connect gate="G$1" pin="GPIO1_17" pad="69"/>
<connect gate="G$1" pin="GPIO1_2" pad="5"/>
<connect gate="G$1" pin="GPIO1_28" pad="58"/>
<connect gate="G$1" pin="GPIO1_29" pad="26"/>
<connect gate="G$1" pin="GPIO1_3" pad="6"/>
<connect gate="G$1" pin="GPIO1_30" pad="21"/>
<connect gate="G$1" pin="GPIO1_31" pad="20"/>
<connect gate="G$1" pin="GPIO1_4" pad="23"/>
<connect gate="G$1" pin="GPIO1_5" pad="22"/>
<connect gate="G$1" pin="GPIO1_6" pad="3"/>
<connect gate="G$1" pin="GPIO1_7" pad="4"/>
<connect gate="G$1" pin="GPIO2_1" pad="18"/>
<connect gate="G$1" pin="GPIO2_10" pad="41"/>
<connect gate="G$1" pin="GPIO2_11" pad="42"/>
<connect gate="G$1" pin="GPIO2_12" pad="39"/>
<connect gate="G$1" pin="GPIO2_13" pad="40"/>
<connect gate="G$1" pin="GPIO2_22" pad="27"/>
<connect gate="G$1" pin="GPIO2_23" pad="29"/>
<connect gate="G$1" pin="GPIO2_24" pad="28"/>
<connect gate="G$1" pin="GPIO2_25" pad="30"/>
<connect gate="G$1" pin="GPIO2_6" pad="45"/>
<connect gate="G$1" pin="GPIO2_7" pad="46"/>
<connect gate="G$1" pin="GPIO2_8" pad="43"/>
<connect gate="G$1" pin="GPIO2_9" pad="44"/>
<connect gate="G$1" pin="GPIO3_19" pad="73"/>
<connect gate="G$1" pin="GPIO3_21" pad="71"/>
<connect gate="G$1" pin="I2C1_SCL" pad="63"/>
<connect gate="G$1" pin="I2C1_SDA" pad="64"/>
<connect gate="G$1" pin="I2C2_SCL" pad="65"/>
<connect gate="G$1" pin="I2C2_SDA" pad="66"/>
<connect gate="G$1" pin="PWR_BUT" pad="55"/>
<connect gate="G$1" pin="SPI1_CS0" pad="74"/>
<connect gate="G$1" pin="SPI1_DI" pad="76"/>
<connect gate="G$1" pin="SPI1_DO" pad="75"/>
<connect gate="G$1" pin="SPI1_SCLK" pad="77"/>
<connect gate="G$1" pin="SYS_5V@1" pad="53"/>
<connect gate="G$1" pin="SYS_5V@2" pad="54"/>
<connect gate="G$1" pin="SYS_RESETN" pad="56"/>
<connect gate="G$1" pin="TIMER4" pad="7"/>
<connect gate="G$1" pin="TIMER5" pad="9"/>
<connect gate="G$1" pin="TIMER6" pad="10"/>
<connect gate="G$1" pin="TIMER7" pad="8"/>
<connect gate="G$1" pin="UART1_RXD" pad="72"/>
<connect gate="G$1" pin="UART1_TXD" pad="70"/>
<connect gate="G$1" pin="UART2_RXD" pad="68"/>
<connect gate="G$1" pin="UART2_TXD" pad="67"/>
<connect gate="G$1" pin="UART3_CTSN" pad="36"/>
<connect gate="G$1" pin="UART3_RTSN" pad="34"/>
<connect gate="G$1" pin="UART4_CTSN" pad="35"/>
<connect gate="G$1" pin="UART4_RTSN" pad="33"/>
<connect gate="G$1" pin="UART4_RXD" pad="57"/>
<connect gate="G$1" pin="UART4_TXD" pad="59"/>
<connect gate="G$1" pin="UART5_CTSN" pad="31"/>
<connect gate="G$1" pin="UART5_RTSN" pad="32"/>
<connect gate="G$1" pin="UART5_RXD" pad="38"/>
<connect gate="G$1" pin="UART5_TXD" pad="37"/>
<connect gate="G$1" pin="VDD_3V3EXP@1" pad="49"/>
<connect gate="G$1" pin="VDD_3V3EXP@2" pad="50"/>
<connect gate="G$1" pin="VDD_5V@1" pad="51"/>
<connect gate="G$1" pin="VDD_5V@2" pad="52"/>
<connect gate="G$1" pin="VDD_ADC" pad="78"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X23" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD23"/>
</gates>
<devices>
<device name="" package="1X23_ROUND_70MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREAKOUT_SOIC24" prefix="U" uservalue="yes">
<description>&lt;b&gt;Chip Breakout - SOIC24 (Dual-Width)&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BREAKOUT_SOIC24"/>
</gates>
<devices>
<device name="" package="BREAKOUT_SOIC24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREAKOUT_SOT23-6" prefix="U" uservalue="yes">
<description>&lt;b&gt;IC Breakout SOT23-6&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BREAKOUT_SOT23-6"/>
</gates>
<devices>
<device name="" package="BREAKOUT_SOT23-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREAKOUT_SOIC8" prefix="U" uservalue="yes">
<description>&lt;b&gt;SOIC8 IC Breakout&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BREAKOUT_SOIC8"/>
</gates>
<devices>
<device name="" package="BREAKOUT_SOIC8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SHUNT-VREF" prefix="D" uservalue="yes">
<description>&lt;b&gt;Shunt Voltage Reference&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;TS3431 - 1.24V Programmable Shunt Voltage Ref. - 1.24-24V, up to 0.25% accuracy, SOT23 (&lt;b&gt;0.25%&lt;/b&gt; = Digikey: 497-4637-1-ND)&lt;/li&gt;
&lt;li&gt;TLVH431 - 1.24V Programmable Shunt Voltage Ref - 1.24-18V, up to 0.50% accuracy, SOT23 (&lt;b&gt;0.50%&lt;/b&gt; = Digikey: 296-17687-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;See: http://www.ti.com/lit/an/slva445/slva445.pdf&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SHUNT-VREF"/>
</gates>
<devices>
<device name="" package="SOT23-R">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP_DUAL" prefix="U" uservalue="yes">
<description>&lt;b&gt;Dual Op-Amp&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;MSOP8 - 0.65mm Pitch&lt;/b&gt;
&lt;/p&gt;
&lt;p&gt;
&lt;table cellpadding="2"&gt;
&lt;tr bgcolor="#EEEEEE"&gt;
&lt;td&gt;Manuf. ID&lt;/td&gt;
&lt;td&gt;Slew Rate&lt;/td&gt;
&lt;td&gt;Gain Bandwidth Prod.&lt;/td&gt;
&lt;td&gt;-3dB Bandwidth&lt;/td&gt;
&lt;td&gt;Current Input Bias&lt;/td&gt;
&lt;td&gt;Voltage Input Offset&lt;/td&gt;
&lt;td&gt;Supply - Single&lt;/td&gt;
&lt;td&gt;Supply - Dual&lt;/td&gt;
&lt;td&gt;Digikey&lt;/td&gt;
&lt;td&gt;Mouser&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
&lt;td&gt;&lt;b&gt;EL5236IYZ-T7&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;128V/µs &lt;/td&gt;
&lt;td&gt;300MHz&lt;/td&gt;
&lt;td&gt;250MHz&lt;/td&gt;
&lt;td&gt;6.5µA&lt;/td&gt;
&lt;td&gt;100µV&lt;/td&gt;
&lt;td&gt;5-12V&lt;/td&gt;
&lt;td&gt;+/-2.5-6V&lt;/td&gt;
&lt;td&gt;EL5236IYZ-T7TR-ND&lt;/td&gt;
&lt;td&gt;--&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
<gate name="G$2" symbol="OPAMP"/>
</gates>
<devices>
<device name="MSOP8_65" package="MSOP8_0.65MM">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$2" pin="+IN" pad="5"/>
<connect gate="G$2" pin="-IN" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP_SINGLE" prefix="U" uservalue="yes">
<description>&lt;b&gt;Single-Output Op-Amp&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;SOT363 (6-TSSOP)&lt;/b&gt;
&lt;/p&gt;
&lt;p&gt;
&lt;table cellpadding="2"&gt;
&lt;tr bgcolor="#EEEEEE"&gt;
&lt;td&gt;Manuf. ID&lt;/td&gt;
&lt;td&gt;Slew Rate&lt;/td&gt;
&lt;td&gt;Gain Bandwidth Prod.&lt;/td&gt;
&lt;td&gt;-3dB Bandwidth&lt;/td&gt;
&lt;td&gt;Current Input Bias&lt;/td&gt;
&lt;td&gt;Voltage Input Offset&lt;/td&gt;
&lt;td&gt;Supply - Single&lt;/td&gt;
&lt;td&gt;Supply - Dual&lt;/td&gt;
&lt;td&gt;Digikey&lt;/td&gt;
&lt;td&gt;Mouser&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;&lt;b&gt;LMV341MG/NOPB&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;1V/µs &lt;/td&gt;
&lt;td&gt;1MHz&lt;/td&gt;
&lt;td&gt;--&lt;/td&gt;
&lt;td&gt;0.02pA&lt;/td&gt;
&lt;td&gt;25µV&lt;/td&gt;
&lt;td&gt;2.4-5.5V&lt;/td&gt;
&lt;td&gt;&lt;/td&gt;
&lt;td&gt;LMV341MGTR-ND&lt;/td&gt;
&lt;td&gt;926-LMV341MG/NOPB&lt;/td&gt;
&lt;/tr&gt;

&lt;tr&gt;
&lt;td&gt;&lt;b&gt;LMH6601MG/NOPB&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;275V/µs &lt;/td&gt;
&lt;td&gt;155MHz&lt;/td&gt;
&lt;td&gt;250MHz&lt;/td&gt;
&lt;td&gt;5pA&lt;/td&gt;
&lt;td&gt;1000µV&lt;/td&gt;
&lt;td&gt;2.4-5.5V&lt;/td&gt;
&lt;td&gt;+/-1.2-2.75V&lt;/td&gt;
&lt;td&gt;LMH6601MGCT-ND&lt;/td&gt;
&lt;td&gt;926-LMH6601MG/NOPB&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="SOT363" package="SOT363">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1850_BGA256" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1850/LPC4350 - LBGA256&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This footprint was designed for a specific application, and numerous choices have been made concering the PINMUX to make certain peripherals available at the expense of others.  These pin choices may not be appropriate in your own situation (for example, only one set of selection pins is broken out for the EMC rather than all four, although some pins on GPIO6 can be sacrificed to enable another memory device on the EMC using CS2).&lt;/p&gt;</description>
<gates>
<gate name="_ANALOG" symbol="LPC1850_ADC"/>
<gate name="_EMC" symbol="LPC1850_EMC"/>
<gate name="_LCD" symbol="LPC1850_LCD"/>
<gate name="_RTC" symbol="LPC1850_RTC"/>
<gate name="_CGU" symbol="LPC1850_CGU"/>
<gate name="_ENET" symbol="LPC1850_ETHERNET"/>
<gate name="_CLOCK" symbol="LPC1850_CLOCK"/>
<gate name="_I2C" symbol="LPC1850_I2C"/>
<gate name="_I2S" symbol="LPC1850_I2S"/>
<gate name="_DEBUG" symbol="LPC1850_JTAG"/>
<gate name="_WAKEUP" symbol="LPC1850_NMI_WAKEUP"/>
<gate name="_QEI" symbol="LPC1850_QEI"/>
<gate name="_SPIFI" symbol="LPC1850_SPIFI"/>
<gate name="_SSP" symbol="LPC1850_SSP"/>
<gate name="_TIMERS" symbol="LPC1850_TIMERS"/>
<gate name="_UART0" symbol="LPC1850_UART0"/>
<gate name="_UART1" symbol="LPC1850_UART1"/>
<gate name="_USB0_HS" symbol="LPC1850_USB0"/>
<gate name="_USB1" symbol="LPC1850_USB1"/>
<gate name="_GPIO" symbol="LPC1850_GPIO"/>
<gate name="_GPIO6" symbol="LPC1850_GPIO6"/>
<gate name="_POWER" symbol="LPC1850_POWER"/>
<gate name="_RESET" symbol="LPC1850_RESET"/>
</gates>
<devices>
<device name="" package="LBGA256_1.0MM">
<connects>
<connect gate="_ANALOG" pin="ADC1_0" pad="F5"/>
<connect gate="_ANALOG" pin="ADC1_1" pad="C3"/>
<connect gate="_ANALOG" pin="ADC1_2" pad="A4"/>
<connect gate="_ANALOG" pin="ADC1_3" pad="B5"/>
<connect gate="_ANALOG" pin="ADC1_4" pad="C6"/>
<connect gate="_ANALOG" pin="ADC1_5" pad="B3"/>
<connect gate="_ANALOG" pin="ADC1_6" pad="A5"/>
<connect gate="_ANALOG" pin="ADC1_7" pad="C5"/>
<connect gate="_ANALOG" pin="DAC" pad="E3"/>
<connect gate="_ANALOG" pin="VDDA" pad="B4"/>
<connect gate="_ANALOG" pin="VSSA" pad="B2"/>
<connect gate="_CGU" pin="CGU_OUT0" pad="L1"/>
<connect gate="_CGU" pin="CGU_OUT1" pad="L12"/>
<connect gate="_CLOCK" pin="CLKOUT" pad="T10"/>
<connect gate="_CLOCK" pin="XTAL1" pad="D1"/>
<connect gate="_CLOCK" pin="XTAL2" pad="E1"/>
<connect gate="_DEBUG" pin="DBGEN" pad="L4"/>
<connect gate="_DEBUG" pin="TCK/SWDCLK" pad="J5"/>
<connect gate="_DEBUG" pin="TDI" pad="J4"/>
<connect gate="_DEBUG" pin="TDO/SWO" pad="K5"/>
<connect gate="_DEBUG" pin="TMS/SWDIO" pad="K6"/>
<connect gate="_DEBUG" pin="TRST" pad="M4"/>
<connect gate="_EMC" pin="EMC_A0" pad="H16"/>
<connect gate="_EMC" pin="EMC_A1" pad="G16"/>
<connect gate="_EMC" pin="EMC_A10" pad="K16"/>
<connect gate="_EMC" pin="EMC_A11" pad="M15"/>
<connect gate="_EMC" pin="EMC_A12" pad="N15"/>
<connect gate="_EMC" pin="EMC_A13" pad="T16"/>
<connect gate="_EMC" pin="EMC_A14" pad="H13"/>
<connect gate="_EMC" pin="EMC_A15" pad="J13"/>
<connect gate="_EMC" pin="EMC_A16" pad="R14"/>
<connect gate="_EMC" pin="EMC_A17" pad="T15"/>
<connect gate="_EMC" pin="EMC_A18" pad="P14"/>
<connect gate="_EMC" pin="EMC_A19" pad="N14"/>
<connect gate="_EMC" pin="EMC_A2" pad="F16"/>
<connect gate="_EMC" pin="EMC_A20" pad="M14"/>
<connect gate="_EMC" pin="EMC_A21" pad="K12"/>
<connect gate="_EMC" pin="EMC_A22" pad="K13"/>
<connect gate="_EMC" pin="EMC_A23" pad="G13"/>
<connect gate="_EMC" pin="EMC_A3" pad="E15"/>
<connect gate="_EMC" pin="EMC_A4" pad="C16"/>
<connect gate="_EMC" pin="EMC_A5" pad="P2"/>
<connect gate="_EMC" pin="EMC_A6" pad="R2"/>
<connect gate="_EMC" pin="EMC_A7" pad="R3"/>
<connect gate="_EMC" pin="EMC_A8" pad="J16"/>
<connect gate="_EMC" pin="EMC_A9" pad="H14"/>
<connect gate="_EMC" pin="EMC_BLS0" pad="T3"/>
<connect gate="_EMC" pin="EMC_BLS1" pad="L14"/>
<connect gate="_EMC" pin="EMC_CAS" pad="R16"/>
<connect gate="_EMC" pin="EMC_CKEOUT0" pad="H12"/>
<connect gate="_EMC" pin="EMC_CLK01" pad="N5"/>
<connect gate="_EMC" pin="EMC_CLK23" pad="D14"/>
<connect gate="_EMC" pin="EMC_CS0" pad="R5"/>
<connect gate="_EMC" pin="EMC_D0" pad="T5"/>
<connect gate="_EMC" pin="EMC_D1" pad="R7"/>
<connect gate="_EMC" pin="EMC_D10" pad="T13"/>
<connect gate="_EMC" pin="EMC_D11" pad="R12"/>
<connect gate="_EMC" pin="EMC_D12" pad="N3"/>
<connect gate="_EMC" pin="EMC_D13" pad="P3"/>
<connect gate="_EMC" pin="EMC_D14" pad="R4"/>
<connect gate="_EMC" pin="EMC_D15" pad="T8"/>
<connect gate="_EMC" pin="EMC_D2" pad="T7"/>
<connect gate="_EMC" pin="EMC_D3" pad="R8"/>
<connect gate="_EMC" pin="EMC_D4" pad="T9"/>
<connect gate="_EMC" pin="EMC_D5" pad="R9"/>
<connect gate="_EMC" pin="EMC_D6" pad="R10"/>
<connect gate="_EMC" pin="EMC_D7" pad="R11"/>
<connect gate="_EMC" pin="EMC_D8" pad="P9"/>
<connect gate="_EMC" pin="EMC_D9" pad="P10"/>
<connect gate="_EMC" pin="EMC_DQMOUT0" pad="G15"/>
<connect gate="_EMC" pin="EMC_DQMOUT1" pad="H15"/>
<connect gate="_EMC" pin="EMC_DYCS0" pad="J15"/>
<connect gate="_EMC" pin="EMC_OE" pad="P5"/>
<connect gate="_EMC" pin="EMC_RAS" pad="P16"/>
<connect gate="_EMC" pin="EMC_WE" pad="T4"/>
<connect gate="_ENET" pin="ENET_COL" pad="M2"/>
<connect gate="_ENET" pin="ENET_CRS" pad="M7"/>
<connect gate="_ENET" pin="ENET_MDC" pad="E4"/>
<connect gate="_ENET" pin="ENET_MDIO" pad="M8"/>
<connect gate="_ENET" pin="ENET_RXD0" pad="T12"/>
<connect gate="_ENET" pin="ENET_RXD1" pad="L3"/>
<connect gate="_ENET" pin="ENET_RXD2" pad="M6"/>
<connect gate="_ENET" pin="ENET_RXD3" pad="N8"/>
<connect gate="_ENET" pin="ENET_RX_CLK" pad="D4"/>
<connect gate="_ENET" pin="ENET_RX_DV" pad="N4"/>
<connect gate="_ENET" pin="ENET_RX_ER" pad="N6"/>
<connect gate="_ENET" pin="ENET_TXD0" pad="N12"/>
<connect gate="_ENET" pin="ENET_TXD1" pad="M10"/>
<connect gate="_ENET" pin="ENET_TXD2" pad="N10"/>
<connect gate="_ENET" pin="ENET_TXD3" pad="M9"/>
<connect gate="_ENET" pin="ENET_TX_CLK" pad="M11"/>
<connect gate="_ENET" pin="ENET_TX_EN" pad="F4"/>
<connect gate="_ENET" pin="ENET_TX_ER" pad="G4"/>
<connect gate="_GPIO" pin="GPIO4[11]" pad="L11"/>
<connect gate="_GPIO" pin="GPIO4[12]" pad="T1"/>
<connect gate="_GPIO" pin="GPIO5[24]" pad="B11"/>
<connect gate="_GPIO" pin="GPIO7[14]" pad="C15"/>
<connect gate="_GPIO" pin="GPIO7[19]" pad="E9"/>
<connect gate="_GPIO" pin="GPIO7[20]" pad="E7"/>
<connect gate="_GPIO" pin="GPIO7[21]" pad="B7"/>
<connect gate="_GPIO" pin="GPIO7[22]" pad="E6"/>
<connect gate="_GPIO6" pin="GPIO6[10]" pad="L5"/>
<connect gate="_GPIO6" pin="GPIO6[13]" pad="N1"/>
<connect gate="_GPIO6" pin="GPIO6[14]" pad="N2"/>
<connect gate="_GPIO6" pin="GPIO6[15]" pad="P1"/>
<connect gate="_GPIO6" pin="GPIO6[16]" pad="R1"/>
<connect gate="_GPIO6" pin="GPIO6[17]" pad="P4"/>
<connect gate="_GPIO6" pin="GPIO6[18]" pad="T2"/>
<connect gate="_GPIO6" pin="GPIO6[19]" pad="P6"/>
<connect gate="_GPIO6" pin="GPIO6[1]" pad="F6"/>
<connect gate="_GPIO6" pin="GPIO6[20]" pad="R6"/>
<connect gate="_GPIO6" pin="GPIO6[21]" pad="T6"/>
<connect gate="_GPIO6" pin="GPIO6[22]" pad="P8"/>
<connect gate="_GPIO6" pin="GPIO6[23]" pad="T11"/>
<connect gate="_GPIO6" pin="GPIO6[24]" pad="P11"/>
<connect gate="_GPIO6" pin="GPIO6[25]" pad="N9"/>
<connect gate="_GPIO6" pin="GPIO6[26]" pad="N11"/>
<connect gate="_GPIO6" pin="GPIO6[27]" pad="T14"/>
<connect gate="_GPIO6" pin="GPIO6[28]" pad="R13"/>
<connect gate="_GPIO6" pin="GPIO6[5]" pad="H6"/>
<connect gate="_GPIO6" pin="GPIO6[6]" pad="G5"/>
<connect gate="_GPIO6" pin="GPIO6[8]" pad="K2"/>
<connect gate="_GPIO6" pin="GPIO6[9]" pad="M5"/>
<connect gate="_I2C" pin="I2C0_SCL" pad="L15"/>
<connect gate="_I2C" pin="I2C0_SDA" pad="L16"/>
<connect gate="_I2C" pin="I2C1_SCL" pad="E13"/>
<connect gate="_I2C" pin="I2C1_SDA" pad="G14"/>
<connect gate="_I2S" pin="I2S0_RX_SCK" pad="D10"/>
<connect gate="_I2S" pin="I2S0_RX_SDA" pad="F11"/>
<connect gate="_I2S" pin="I2S0_RX_WS" pad="R15"/>
<connect gate="_I2S" pin="I2S0_TX_SCK" pad="F13"/>
<connect gate="_I2S" pin="I2S0_TX_SDA" pad="L6"/>
<connect gate="_I2S" pin="I2S0_TX_WS" pad="M1"/>
<connect gate="_LCD" pin="LCD_DCLK_[4.7]" pad="H4"/>
<connect gate="_LCD" pin="LCD_ENBL_[4.6]" pad="C1"/>
<connect gate="_LCD" pin="LCD_FP_[4.5]" pad="D2"/>
<connect gate="_LCD" pin="LCD_LE_[7.0]" pad="B16"/>
<connect gate="_LCD" pin="LCD_LP_[7.6]" pad="C7"/>
<connect gate="_LCD" pin="LCD_PWR_[7.7]" pad="B6"/>
<connect gate="_LCD" pin="LCD_VD0_[4.1]" pad="A1"/>
<connect gate="_LCD" pin="LCD_VD10_[4.10]" pad="M3"/>
<connect gate="_LCD" pin="LCD_VD11_[4.9]" pad="L2"/>
<connect gate="_LCD" pin="LCD_VD12_[8.3]" pad="J3"/>
<connect gate="_LCD" pin="LCD_VD13_[B.6]" pad="A6"/>
<connect gate="_LCD" pin="LCD_VD14_[B.5]" pad="A12"/>
<connect gate="_LCD" pin="LCD_VD15_[B.4]" pad="G11"/>
<connect gate="_LCD" pin="LCD_VD16_[7.4]" pad="C8"/>
<connect gate="_LCD" pin="LCD_VD17_[7.3]" pad="C13"/>
<connect gate="_LCD" pin="LCD_VD18_[7.2]" pad="A16"/>
<connect gate="_LCD" pin="LCD_VD19_[7.1]" pad="C14"/>
<connect gate="_LCD" pin="LCD_VD1_[4.4]" pad="B1"/>
<connect gate="_LCD" pin="LCD_VD20_[B.3]" pad="A13"/>
<connect gate="_LCD" pin="LCD_VD21_[B.2]" pad="B12"/>
<connect gate="_LCD" pin="LCD_VD22_[B.1]" pad="A14"/>
<connect gate="_LCD" pin="LCD_VD23_[B.0]" pad="B15"/>
<connect gate="_LCD" pin="LCD_VD2_[4.3]" pad="C2"/>
<connect gate="_LCD" pin="LCD_VD3_[4.2]" pad="D3"/>
<connect gate="_LCD" pin="LCD_VD4_[8.7]" pad="K1"/>
<connect gate="_LCD" pin="LCD_VD5_[8.6]" pad="K3"/>
<connect gate="_LCD" pin="LCD_VD6_[8.5]" pad="J1"/>
<connect gate="_LCD" pin="LCD_VD7_[8.4]" pad="J2"/>
<connect gate="_LCD" pin="LCD_VD8_[7.5]" pad="A7"/>
<connect gate="_LCD" pin="LCD_VD9_[4.8]" pad="E2"/>
<connect gate="_POWER" pin="VDDIO@0" pad="F7"/>
<connect gate="_POWER" pin="VDDIO@1" pad="J7"/>
<connect gate="_POWER" pin="VDDIO@10" pad="J6"/>
<connect gate="_POWER" pin="VDDIO@11" pad="F8"/>
<connect gate="_POWER" pin="VDDIO@12" pad="K7"/>
<connect gate="_POWER" pin="VDDIO@2" pad="N7"/>
<connect gate="_POWER" pin="VDDIO@3" pad="L10"/>
<connect gate="_POWER" pin="VDDIO@4" pad="E12"/>
<connect gate="_POWER" pin="VDDIO@5" pad="N13"/>
<connect gate="_POWER" pin="VDDIO@6" pad="L9"/>
<connect gate="_POWER" pin="VDDIO@7" pad="H10"/>
<connect gate="_POWER" pin="VDDIO@8" pad="G10"/>
<connect gate="_POWER" pin="VDDIO@9" pad="D7"/>
<connect gate="_POWER" pin="VDDREG@0" pad="F10"/>
<connect gate="_POWER" pin="VDDREG@1" pad="F9"/>
<connect gate="_POWER" pin="VDDREG@2" pad="L8"/>
<connect gate="_POWER" pin="VDDREG@3" pad="L7"/>
<connect gate="_POWER" pin="VPP" pad="E8"/>
<connect gate="_POWER" pin="VSS@0" pad="H7"/>
<connect gate="_POWER" pin="VSS@1" pad="K8"/>
<connect gate="_POWER" pin="VSS@2" pad="G9"/>
<connect gate="_POWER" pin="VSS@3" pad="J11"/>
<connect gate="_POWER" pin="VSS@4" pad="J10"/>
<connect gate="_POWER" pin="VSSIO@0" pad="G6"/>
<connect gate="_POWER" pin="VSSIO@1" pad="J8"/>
<connect gate="_POWER" pin="VSSIO@10" pad="H8"/>
<connect gate="_POWER" pin="VSSIO@11" pad="G7"/>
<connect gate="_POWER" pin="VSSIO@12" pad="C4"/>
<connect gate="_POWER" pin="VSSIO@13" pad="H9"/>
<connect gate="_POWER" pin="VSSIO@2" pad="J9"/>
<connect gate="_POWER" pin="VSSIO@3" pad="K9"/>
<connect gate="_POWER" pin="VSSIO@4" pad="K10"/>
<connect gate="_POWER" pin="VSSIO@5" pad="P7"/>
<connect gate="_POWER" pin="VSSIO@6" pad="M13"/>
<connect gate="_POWER" pin="VSSIO@7" pad="P13"/>
<connect gate="_POWER" pin="VSSIO@8" pad="D13"/>
<connect gate="_POWER" pin="VSSIO@9" pad="G8"/>
<connect gate="_QEI" pin="QEI_IDX" pad="J14"/>
<connect gate="_QEI" pin="QEI_PHA" pad="H11"/>
<connect gate="_QEI" pin="QEI_PHB" pad="K15"/>
<connect gate="_RESET" pin="RESET" pad="D9"/>
<connect gate="_RTC" pin="RTCX1" pad="A8"/>
<connect gate="_RTC" pin="RTCX2" pad="B8"/>
<connect gate="_RTC" pin="RTC_ALARM" pad="A11"/>
<connect gate="_RTC" pin="VBAT" pad="B10"/>
<connect gate="_SPIFI" pin="SPIFI_CS" pad="C10"/>
<connect gate="_SPIFI" pin="SPIFI_MISO" pad="B13"/>
<connect gate="_SPIFI" pin="SPIFI_MOSI" pad="C11"/>
<connect gate="_SPIFI" pin="SPIFI_SCK" pad="B14"/>
<connect gate="_SPIFI" pin="SPIFI_SIO2" pad="C12"/>
<connect gate="_SPIFI" pin="SPIFI_SIO3" pad="A15"/>
<connect gate="_SSP" pin="SSP0_MISO" pad="D11"/>
<connect gate="_SSP" pin="SSP0_MOSI" pad="E10"/>
<connect gate="_SSP" pin="SSP0_SCK" pad="D12"/>
<connect gate="_SSP" pin="SSP0_SSEL" pad="E11"/>
<connect gate="_TIMERS" pin="T2_CAP1" pad="L13"/>
<connect gate="_TIMERS" pin="T2_CAP2" pad="P15"/>
<connect gate="_TIMERS" pin="TO_MAT0" pad="E5"/>
<connect gate="_UART0" pin="U0_DIR_[F.9]" pad="D6"/>
<connect gate="_UART0" pin="U0_RXD_[F.11]" pad="A2"/>
<connect gate="_UART0" pin="U0_TXD_[F.10]" pad="A3"/>
<connect gate="_UART1" pin="U1_CTS" pad="F15"/>
<connect gate="_UART1" pin="U1_DCD" pad="E16"/>
<connect gate="_UART1" pin="U1_DSR" pad="F14"/>
<connect gate="_UART1" pin="U1_DTR" pad="E14"/>
<connect gate="_UART1" pin="U1_RI" pad="M16"/>
<connect gate="_UART1" pin="U1_RTS" pad="N16"/>
<connect gate="_UART1" pin="U1_RXD" pad="D15"/>
<connect gate="_UART1" pin="U1_TXD" pad="D16"/>
<connect gate="_USB0_HS" pin="USB0_DM" pad="G2"/>
<connect gate="_USB0_HS" pin="USB0_DP" pad="F2"/>
<connect gate="_USB0_HS" pin="USB0_ID" pad="H2"/>
<connect gate="_USB0_HS" pin="USB0_IND0" pad="K4"/>
<connect gate="_USB0_HS" pin="USB0_IND1" pad="H5"/>
<connect gate="_USB0_HS" pin="USB0_PWR_EN" pad="J12"/>
<connect gate="_USB0_HS" pin="USB0_PWR_FAULT" pad="K11"/>
<connect gate="_USB0_HS" pin="USB0_RREF" pad="H1"/>
<connect gate="_USB0_HS" pin="USB0_VBUS" pad="F1"/>
<connect gate="_USB0_HS" pin="USB0_VDDA3V3" pad="G3"/>
<connect gate="_USB0_HS" pin="USB0_VDDA3V3_DRIVER" pad="F3"/>
<connect gate="_USB0_HS" pin="USB0_VSSA_REF" pad="G1"/>
<connect gate="_USB0_HS" pin="USB0_VSSA_TERM" pad="H3"/>
<connect gate="_USB1" pin="USB1_DM" pad="G12"/>
<connect gate="_USB1" pin="USB1_DP" pad="F12"/>
<connect gate="_USB1" pin="USB1_VBUS" pad="K14"/>
<connect gate="_WAKEUP" pin="NMI_EXT" pad="D5"/>
<connect gate="_WAKEUP" pin="WAKEUP0" pad="A9"/>
<connect gate="_WAKEUP" pin="WAKEUP1" pad="A10"/>
<connect gate="_WAKEUP" pin="WAKEUP2" pad="C9"/>
<connect gate="_WAKEUP" pin="WAKEUP3" pad="D8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME_A3_ADAFRUIT_FULL">
<description>FRame - A3 - BOM</description>
<gates>
<gate name="G$1" symbol="FRAME_A3_ADAFRUIT_FULL"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA19988" prefix="U" uservalue="yes">
<gates>
<gate name="_AUDIO" symbol="TDA19988_AUDIO"/>
<gate name="_CONTROL" symbol="TDA19988_CTRL"/>
<gate name="_POWER" symbol="TDA19988_PWR"/>
<gate name="_VIDEO" symbol="TDA19988_VIDEO"/>
</gates>
<devices>
<device name="" package="HVQFN64">
<connects>
<connect gate="_AUDIO" pin="ACLK" pad="23"/>
<connect gate="_AUDIO" pin="AP1" pad="25"/>
<connect gate="_AUDIO" pin="AP2" pad="26"/>
<connect gate="_AUDIO" pin="AP3" pad="27"/>
<connect gate="_AUDIO" pin="AP4" pad="28"/>
<connect gate="_AUDIO" pin="WS" pad="24"/>
<connect gate="_CONTROL" pin="A0" pad="53"/>
<connect gate="_CONTROL" pin="A1" pad="54"/>
<connect gate="_CONTROL" pin="CDSA" pad="51"/>
<connect gate="_CONTROL" pin="CEC" pad="30"/>
<connect gate="_CONTROL" pin="CSCL" pad="52"/>
<connect gate="_CONTROL" pin="DSCL" pad="33"/>
<connect gate="_CONTROL" pin="DSDA" pad="32"/>
<connect gate="_CONTROL" pin="HPD" pad="31"/>
<connect gate="_CONTROL" pin="INT" pad="50"/>
<connect gate="_CONTROL" pin="TEST" pad="49"/>
<connect gate="_CONTROL" pin="VPP" pad="19"/>
<connect gate="_POWER" pin="GND" pad="PAD"/>
<connect gate="_POWER" pin="VDDA" pad="35"/>
<connect gate="_POWER" pin="VDDA_PLL@1" pad="47"/>
<connect gate="_POWER" pin="VDDA_PLL@2" pad="48"/>
<connect gate="_POWER" pin="VDDA_TMDS@1" pad="36"/>
<connect gate="_POWER" pin="VDDA_TMDS@2" pad="41"/>
<connect gate="_POWER" pin="VDDA_TMDS@3" pad="46"/>
<connect gate="_POWER" pin="VDDC@1" pad="5"/>
<connect gate="_POWER" pin="VDDC@2" pad="29"/>
<connect gate="_POWER" pin="VDDIO@1" pad="14"/>
<connect gate="_POWER" pin="VDDIO@2" pad="55"/>
<connect gate="_VIDEO" pin="DE/FREF" pad="20"/>
<connect gate="_VIDEO" pin="EXT_SWING" pad="34"/>
<connect gate="_VIDEO" pin="HSYNC/HREF" pad="22"/>
<connect gate="_VIDEO" pin="PCLK" pad="4"/>
<connect gate="_VIDEO" pin="TX0+" pad="40"/>
<connect gate="_VIDEO" pin="TX0-" pad="39"/>
<connect gate="_VIDEO" pin="TX1+" pad="43"/>
<connect gate="_VIDEO" pin="TX1-" pad="42"/>
<connect gate="_VIDEO" pin="TX2+" pad="45"/>
<connect gate="_VIDEO" pin="TX2-" pad="44"/>
<connect gate="_VIDEO" pin="TXC+" pad="38"/>
<connect gate="_VIDEO" pin="TXC-" pad="37"/>
<connect gate="_VIDEO" pin="VPA0" pad="63"/>
<connect gate="_VIDEO" pin="VPA1" pad="62"/>
<connect gate="_VIDEO" pin="VPA2" pad="61"/>
<connect gate="_VIDEO" pin="VPA3" pad="60"/>
<connect gate="_VIDEO" pin="VPA4" pad="59"/>
<connect gate="_VIDEO" pin="VPA5" pad="58"/>
<connect gate="_VIDEO" pin="VPA6" pad="57"/>
<connect gate="_VIDEO" pin="VPA7" pad="56"/>
<connect gate="_VIDEO" pin="VPB0" pad="9"/>
<connect gate="_VIDEO" pin="VPB1" pad="8"/>
<connect gate="_VIDEO" pin="VPB2" pad="7"/>
<connect gate="_VIDEO" pin="VPB3" pad="6"/>
<connect gate="_VIDEO" pin="VPB4" pad="3"/>
<connect gate="_VIDEO" pin="VPB5" pad="2"/>
<connect gate="_VIDEO" pin="VPB6" pad="1"/>
<connect gate="_VIDEO" pin="VPB7" pad="64"/>
<connect gate="_VIDEO" pin="VPC0" pad="18"/>
<connect gate="_VIDEO" pin="VPC1" pad="17"/>
<connect gate="_VIDEO" pin="VPC2" pad="16"/>
<connect gate="_VIDEO" pin="VPC3" pad="15"/>
<connect gate="_VIDEO" pin="VPC4" pad="13"/>
<connect gate="_VIDEO" pin="VPC5" pad="12"/>
<connect gate="_VIDEO" pin="VPC6" pad="11"/>
<connect gate="_VIDEO" pin="VPC7" pad="10"/>
<connect gate="_VIDEO" pin="VSYNC/VREF" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HDMI_MOLEX_47151-0001" prefix="CN" uservalue="yes">
<gates>
<gate name="G$1" symbol="HDMI_CONN"/>
<gate name="SHELL" symbol="HDMI_SHELL"/>
</gates>
<devices>
<device name="" package="HDMI_MOLEX_47151-0001">
<connects>
<connect gate="G$1" pin="+5V" pad="18"/>
<connect gate="G$1" pin="CEC" pad="13"/>
<connect gate="G$1" pin="DCLK" pad="15"/>
<connect gate="G$1" pin="DDAT" pad="16"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="HOTPLUG" pad="19"/>
<connect gate="G$1" pin="TX0+" pad="7"/>
<connect gate="G$1" pin="TX0-" pad="9"/>
<connect gate="G$1" pin="TX0_SHIELD" pad="8"/>
<connect gate="G$1" pin="TX1+" pad="4"/>
<connect gate="G$1" pin="TX1-" pad="6"/>
<connect gate="G$1" pin="TX1_SHIELD" pad="5"/>
<connect gate="G$1" pin="TX2+" pad="1"/>
<connect gate="G$1" pin="TX2-" pad="3"/>
<connect gate="G$1" pin="TX2_SHIELD" pad="2"/>
<connect gate="G$1" pin="TXC+" pad="10"/>
<connect gate="G$1" pin="TXC-" pad="12"/>
<connect gate="G$1" pin="TXC_SHIELD" pad="11"/>
<connect gate="G$1" pin="UTILITY" pad="14"/>
<connect gate="SHELL" pin="GND@1" pad="P$1"/>
<connect gate="SHELL" pin="GND@2" pad="P$2"/>
<connect gate="SHELL" pin="GND@3" pad="P$3"/>
<connect gate="SHELL" pin="GND@4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UDA1380HN" prefix="U">
<gates>
<gate name="_PWR" symbol="UDA1380_POWER"/>
<gate name="_SYS" symbol="UDA1380"/>
</gates>
<devices>
<device name="" package="HVQFN32">
<connects>
<connect gate="_PWR" pin="VADCN" pad="30"/>
<connect gate="_PWR" pin="VADCP" pad="32"/>
<connect gate="_PWR" pin="VDDA(AD)" pad="28"/>
<connect gate="_PWR" pin="VDDA(DA)" pad="22"/>
<connect gate="_PWR" pin="VDDA(HP)" pad="20"/>
<connect gate="_PWR" pin="VDDD" pad="2"/>
<connect gate="_PWR" pin="VREF" pad="25"/>
<connect gate="_PWR" pin="VSSA(AD)" pad="26"/>
<connect gate="_PWR" pin="VSSA(DA)" pad="24"/>
<connect gate="_PWR" pin="VSSA(HP)" pad="16"/>
<connect gate="_PWR" pin="VSSD" pad="10"/>
<connect gate="_SYS" pin="BCKI" pad="6"/>
<connect gate="_SYS" pin="BCKO" pad="3"/>
<connect gate="_SYS" pin="DATAI" pad="8"/>
<connect gate="_SYS" pin="DATAO" pad="5"/>
<connect gate="_SYS" pin="L3CLOCK/SCL" pad="13"/>
<connect gate="_SYS" pin="L3DATA/SDA" pad="14"/>
<connect gate="_SYS" pin="L3MODE/A1" pad="12"/>
<connect gate="_SYS" pin="RESET" pad="1"/>
<connect gate="_SYS" pin="RTCB" pad="11"/>
<connect gate="_SYS" pin="SEL_L3_IIC" pad="15"/>
<connect gate="_SYS" pin="SYSCLK" pad="9"/>
<connect gate="_SYS" pin="VINL" pad="27"/>
<connect gate="_SYS" pin="VINM" pad="31"/>
<connect gate="_SYS" pin="VINR" pad="29"/>
<connect gate="_SYS" pin="VOUTL" pad="23"/>
<connect gate="_SYS" pin="VOUTLHP" pad="19"/>
<connect gate="_SYS" pin="VOUTR" pad="21"/>
<connect gate="_SYS" pin="VOUTRHP" pad="17"/>
<connect gate="_SYS" pin="VREF(HP)" pad="18"/>
<connect gate="_SYS" pin="WSI" pad="7"/>
<connect gate="_SYS" pin="WSO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IP4786CZ32" prefix="U" uservalue="yes">
<description>&lt;b&gt;IP4786CZ32&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="IP4786CZ32"/>
</gates>
<devices>
<device name="" package="HVQFN32">
<connects>
<connect gate="G$1" pin="CEC_CON" pad="25"/>
<connect gate="G$1" pin="CEC_STDBY" pad="28"/>
<connect gate="G$1" pin="CEC_SYS" pad="29"/>
<connect gate="G$1" pin="DCLK_CON" pad="15"/>
<connect gate="G$1" pin="DCLK_SYS" pad="9"/>
<connect gate="G$1" pin="DDAT_CON" pad="14"/>
<connect gate="G$1" pin="DDAT_SYS" pad="10"/>
<connect gate="G$1" pin="ESD_BYPASS" pad="26"/>
<connect gate="G$1" pin="GND" pad="PAD"/>
<connect gate="G$1" pin="HOTPLUG_CON" pad="12"/>
<connect gate="G$1" pin="HOTPLUG_SYS" pad="32"/>
<connect gate="G$1" pin="TX0+_CON" pad="20"/>
<connect gate="G$1" pin="TX0+_SYS" pad="5"/>
<connect gate="G$1" pin="TX0-_CON" pad="19"/>
<connect gate="G$1" pin="TX0-_SYS" pad="6"/>
<connect gate="G$1" pin="TX1+_CON" pad="22"/>
<connect gate="G$1" pin="TX1+_SYS" pad="3"/>
<connect gate="G$1" pin="TX1-_CON" pad="21"/>
<connect gate="G$1" pin="TX1-_SYS" pad="4"/>
<connect gate="G$1" pin="TX2+_CON" pad="24"/>
<connect gate="G$1" pin="TX2+_SYS" pad="1"/>
<connect gate="G$1" pin="TX2-_CON" pad="23"/>
<connect gate="G$1" pin="TX2-_SYS" pad="2"/>
<connect gate="G$1" pin="TXC+_CON" pad="18"/>
<connect gate="G$1" pin="TXC+_SYS" pad="7"/>
<connect gate="G$1" pin="TXC-_CON" pad="17"/>
<connect gate="G$1" pin="TXC-_SYS" pad="8"/>
<connect gate="G$1" pin="UTILITY" pad="16"/>
<connect gate="G$1" pin="VCC(4.5-6.5V)" pad="11"/>
<connect gate="G$1" pin="VCCO_5V" pad="13"/>
<connect gate="G$1" pin="VCC_SYS(1.62-5.5V)" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3407" prefix="U" uservalue="yes">
<description>&lt;b&gt;LM3407&lt;/b&gt; - 350 mA, Constant Current Output Floating Buck Switching Converter for High Power LEDs</description>
<gates>
<gate name="G$1" symbol="LM3407"/>
</gates>
<devices>
<device name="" package="MSOP8_0.65MM">
<connects>
<connect gate="G$1" pin="DIM" pad="2"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="ISNS" pad="1"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINOR3" prefix="U">
<description>This is a new object for the new Arduino R3 - with extra pins that you may want to use (such as IOref, and duplicated A4/A5</description>
<gates>
<gate name="G$1" symbol="ARDUINOR3"/>
</gates>
<devices>
<device name="-DIMENSION" package="ARDUINOR3">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BPLACE" package="ARDUINOR3-BPLACE">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NODIM" package="ARDUINOR3-NODIM">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS_FGPMMOPA6B" prefix="U" uservalue="yes">
<description>&lt;b&gt;FGPMMOPA6B&lt;/b&gt; 16x16x0.6mm GPS Module
&lt;p&gt;&lt;b&gt;NMEA Sentences&lt;/b&gt;: GGA, GSA, GSV, RMC, VTG&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;General Specifications&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;Chipset&lt;/b&gt;: MTK MT3329&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Baud Rate&lt;/b&gt;: 9600bps (default)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Update Rate&lt;/b&gt;: 1Hz (default)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Cold Start&lt;/b&gt;: ~35s&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Operating Temp&lt;/b&gt;: -40 to 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;DC Characteristics&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;Supply Voltage&lt;/b&gt;: 3.2-5.0V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Backup Battery Voltage&lt;/b&gt;: 2.0-4.3V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Digital Logic (UART)&lt;/b&gt;: 3.3V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;I(Tracking)&lt;/b&gt;: 42mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;I(Acquisition)&lt;/b&gt;: 53mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;I(BackupBattery)&lt;/b&gt;: 10uA&lt;/li&gt;

&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FGPMMOPA6B"/>
</gates>
<devices>
<device name="" package="FGPMMOPA6B">
<connects>
<connect gate="G$1" pin="3D-FIX" pad="P$5"/>
<connect gate="G$1" pin="DMINUS" pad="P$7"/>
<connect gate="G$1" pin="DPLUS" pad="P$6"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$8"/>
<connect gate="G$1" pin="NC@1" pad="P$11"/>
<connect gate="G$1" pin="NC@2" pad="P$12"/>
<connect gate="G$1" pin="RX" pad="P$10"/>
<connect gate="G$1" pin="TX" pad="P$9"/>
<connect gate="G$1" pin="VBACKUP" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_SIM908" prefix="U" uservalue="yes">
<description>&lt;b&gt;SIM908 GSM + GPS Module&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SIM908_LITERAL"/>
</gates>
<devices>
<device name="" package="SIM908">
<connects>
<connect gate="G$1" pin="ADC" pad="P$47"/>
<connect gate="G$1" pin="CTS" pad="P$67"/>
<connect gate="G$1" pin="DCD" pad="P$70"/>
<connect gate="G$1" pin="DISP-CLK" pad="P$6"/>
<connect gate="G$1" pin="DISP-CS" pad="P$9"/>
<connect gate="G$1" pin="DISP-D/C" pad="P$8"/>
<connect gate="G$1" pin="DISP-DATA" pad="P$7"/>
<connect gate="G$1" pin="DTR" pad="P$72"/>
<connect gate="G$1" pin="GND@1" pad="P$1"/>
<connect gate="G$1" pin="GND@10" pad="P$57"/>
<connect gate="G$1" pin="GND@11" pad="P$58"/>
<connect gate="G$1" pin="GND@12" pad="P$60"/>
<connect gate="G$1" pin="GND@13" pad="P$61"/>
<connect gate="G$1" pin="GND@14" pad="P$64"/>
<connect gate="G$1" pin="GND@15" pad="P$65"/>
<connect gate="G$1" pin="GND@16" pad="P$77"/>
<connect gate="G$1" pin="GND@17" pad="P$78"/>
<connect gate="G$1" pin="GND@18" pad="P$80"/>
<connect gate="G$1" pin="GND@2" pad="P$2"/>
<connect gate="G$1" pin="GND@3" pad="P$5"/>
<connect gate="G$1" pin="GND@4" pad="P$10"/>
<connect gate="G$1" pin="GND@5" pad="P$14"/>
<connect gate="G$1" pin="GND@6" pad="P$37"/>
<connect gate="G$1" pin="GND@7" pad="P$40"/>
<connect gate="G$1" pin="GND@8" pad="P$41"/>
<connect gate="G$1" pin="GND@9" pad="P$43"/>
<connect gate="G$1" pin="GPIO1/KBR0" pad="P$31"/>
<connect gate="G$1" pin="GPIO2/KBR1" pad="P$32"/>
<connect gate="G$1" pin="GPIO3/KBR2" pad="P$33"/>
<connect gate="G$1" pin="GPIO4/KBC0" pad="P$34"/>
<connect gate="G$1" pin="GPIO5/KBC1" pad="P$35"/>
<connect gate="G$1" pin="GPIO6/KBC2" pad="P$36"/>
<connect gate="G$1" pin="GPS-ANT" pad="P$79"/>
<connect gate="G$1" pin="GPS-VANT-IN" pad="P$76"/>
<connect gate="G$1" pin="GPS-VANT-OUT" pad="P$75"/>
<connect gate="G$1" pin="GPS/DBG-RXD" pad="P$16"/>
<connect gate="G$1" pin="GPS/DBG-TXD" pad="P$15"/>
<connect gate="G$1" pin="GSM-ANT" pad="P$59"/>
<connect gate="G$1" pin="I2C-SCL" pad="P$55"/>
<connect gate="G$1" pin="I2C-SDA" pad="P$56"/>
<connect gate="G$1" pin="MIC1N" pad="P$24"/>
<connect gate="G$1" pin="MIC1P" pad="P$23"/>
<connect gate="G$1" pin="MIC2N" pad="P$28"/>
<connect gate="G$1" pin="MIC2P" pad="P$27"/>
<connect gate="G$1" pin="NC@1" pad="P$4"/>
<connect gate="G$1" pin="NC@10" pad="P$46"/>
<connect gate="G$1" pin="NC@11" pad="P$53"/>
<connect gate="G$1" pin="NC@12" pad="P$54"/>
<connect gate="G$1" pin="NC@2" pad="P$11"/>
<connect gate="G$1" pin="NC@3" pad="P$12"/>
<connect gate="G$1" pin="NC@4" pad="P$13"/>
<connect gate="G$1" pin="NC@5" pad="P$29"/>
<connect gate="G$1" pin="NC@6" pad="P$30"/>
<connect gate="G$1" pin="NC@7" pad="P$38"/>
<connect gate="G$1" pin="NC@8" pad="P$39"/>
<connect gate="G$1" pin="NC@9" pad="P$45"/>
<connect gate="G$1" pin="NETLIGHT" pad="P$51"/>
<connect gate="G$1" pin="PWM1" pad="P$48"/>
<connect gate="G$1" pin="PWM2" pad="P$49"/>
<connect gate="G$1" pin="PWM3" pad="P$50"/>
<connect gate="G$1" pin="PWRKEY" pad="P$3"/>
<connect gate="G$1" pin="RI" pad="P$69"/>
<connect gate="G$1" pin="RTS" pad="P$66"/>
<connect gate="G$1" pin="RXD" pad="P$68"/>
<connect gate="G$1" pin="SIM-CLK" pad="P$19"/>
<connect gate="G$1" pin="SIM-DATA" pad="P$17"/>
<connect gate="G$1" pin="SIM-RST" pad="P$18"/>
<connect gate="G$1" pin="SIM-VDD" pad="P$20"/>
<connect gate="G$1" pin="SPK1N" pad="P$21"/>
<connect gate="G$1" pin="SPK1P" pad="P$22"/>
<connect gate="G$1" pin="SPK2N" pad="P$25"/>
<connect gate="G$1" pin="SPK2P" pad="P$26"/>
<connect gate="G$1" pin="STATUS" pad="P$52"/>
<connect gate="G$1" pin="TEMP-BAT" pad="P$73"/>
<connect gate="G$1" pin="TXD" pad="P$71"/>
<connect gate="G$1" pin="VBAT@1" pad="P$62"/>
<connect gate="G$1" pin="VBAT@2" pad="P$63"/>
<connect gate="G$1" pin="VCHG" pad="P$74"/>
<connect gate="G$1" pin="VDD-EXT" pad="P$44"/>
<connect gate="G$1" pin="VRTC" pad="P$42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U24_QFP48" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC11U24 - ARM Cortex M0 50MHz MCU&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Supply: 1.8-3.6V&lt;/li&gt;
&lt;li&gt;Flash: 32KB&lt;/li&gt;
&lt;li&gt;EEPROM: 4KB&lt;/li&gt;
&lt;li&gt;SRAM: 8KB + 2KB USB&lt;/li&gt;
&lt;li&gt;Temp: -40°C - 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U24_QFP48"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)" pad="4"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO0_17/RTS/CT32B0_CAP0/SCLK" pad="45"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="42"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL-(20MA_SINK)" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA-(20MA_SINK)" pad="16"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS-(20MA_SOURCE)" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_13/DTR/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="G$1" pin="PIO1_14/DSR/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="G$1" pin="PIO1_15/DCD/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="G$1" pin="PIO1_16/RI/CT16B0_CAP0" pad="48"/>
<connect gate="G$1" pin="PIO1_19/DTR/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO1_20/DSR/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO1_21/DCD/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO1_22/RI/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="18"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="21"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="1"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="24"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="G$1" pin="PIO1_31" pad="25"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO0_14/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="8"/>
<connect gate="G$1" pin="VDD@2" pad="44"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11U24_QFP64" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC11U24 - ARM Cortex M0 50MHz MCU&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Supply: 1.8-3.6V&lt;/li&gt;
&lt;li&gt;Flash: 32KB&lt;/li&gt;
&lt;li&gt;EEPROM: 4KB&lt;/li&gt;
&lt;li&gt;SRAM: 8KB + 2KB USB&lt;/li&gt;
&lt;li&gt;Temp: -40°C - 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11U24_QFP64"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)" pad="5"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="53"/>
<connect gate="G$1" pin="PIO0_17/RTS/CT32B0_CAP0/SCLK" pad="60"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="61"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="62"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="13"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="11"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="22"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="40"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="56"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL-(20MA_SINK)" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA-(20MA_SINK)" pad="21"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK0" pad="29"/>
<connect gate="G$1" pin="PIO0_7/CTS-(20MA_SOURCE)" pad="30"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="36"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="37"/>
<connect gate="G$1" pin="PIO1_0/CT32B1_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO1_1/CT32B1_MAT1" pad="17"/>
<connect gate="G$1" pin="PIO1_10" pad="12"/>
<connect gate="G$1" pin="PIO1_11" pad="43"/>
<connect gate="G$1" pin="PIO1_12" pad="59"/>
<connect gate="G$1" pin="PIO1_13/DTR/CT16B0_MAT0/TXD" pad="47"/>
<connect gate="G$1" pin="PIO1_14/DSR/CT16B0_MAT1/RXD" pad="49"/>
<connect gate="G$1" pin="PIO1_15/DCD/CT16B0_MAT2/SCK1" pad="57"/>
<connect gate="G$1" pin="PIO1_16/RI/CT16B0_CAP0" pad="63"/>
<connect gate="G$1" pin="PIO1_17/CT16B0_CAP1/RXD" pad="23"/>
<connect gate="G$1" pin="PIO1_18/CT16B1_CAP1/TXD" pad="28"/>
<connect gate="G$1" pin="PIO1_19/DTR/SSEL1" pad="3"/>
<connect gate="G$1" pin="PIO1_2/CT32B1_MAT2" pad="34"/>
<connect gate="G$1" pin="PIO1_20/DSR/SCK1" pad="18"/>
<connect gate="G$1" pin="PIO1_21/DCD/MISO1" pad="35"/>
<connect gate="G$1" pin="PIO1_22/RI/MOSI1" pad="51"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="24"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="14"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="15"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="31"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="41"/>
<connect gate="G$1" pin="PIO1_3/CT32B1_MAT3" pad="50"/>
<connect gate="G$1" pin="PIO1_4/CT32B1_CAP0" pad="16"/>
<connect gate="G$1" pin="PIO1_5/CT32B1_CAP1" pad="32"/>
<connect gate="G$1" pin="PIO1_6" pad="64"/>
<connect gate="G$1" pin="PIO1_7" pad="6"/>
<connect gate="G$1" pin="PIO1_8" pad="39"/>
<connect gate="G$1" pin="PIO1_9" pad="55"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="4"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="38"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="52"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="42"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="45"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="44"/>
<connect gate="G$1" pin="TRST/PIO0_14/AD3/CT32B1_MAT1" pad="46"/>
<connect gate="G$1" pin="USB_DM" pad="25"/>
<connect gate="G$1" pin="USB_DP" pad="26"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="33"/>
<connect gate="G$1" pin="VDD@3" pad="48"/>
<connect gate="G$1" pin="VDD@4" pad="58"/>
<connect gate="G$1" pin="VSS@1" pad="7"/>
<connect gate="G$1" pin="VSS@2" pad="54"/>
<connect gate="G$1" pin="XTALIN" pad="8"/>
<connect gate="G$1" pin="XTALOUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03_ROUND_70MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_BTL221722-276L" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;BTL221722-276L&lt;/b&gt; - 2.2" 176x220 LCD Display - SPI Interface&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;Dimensions&lt;/b&gt;: W: 40.3mm, L: 55mm, H: 2.35mm&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Logic&lt;/b&gt;: 1.8-3.3V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;VDD&lt;/b&gt;: 2.8-3.3V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;LEDs&lt;/b&gt;: 3*20mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;LED Vf&lt;/b&gt;: ~3.3V&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="BTL221722-276L"/>
</gates>
<devices>
<device name="" package="BTL221722-276L">
<connects>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="LED+" pad="3"/>
<connect gate="G$1" pin="LED_K1" pad="11"/>
<connect gate="G$1" pin="LED_K2" pad="12"/>
<connect gate="G$1" pin="LED_K3" pad="13"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="SCL" pad="7"/>
<connect gate="G$1" pin="SDI" pad="6"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="4"/>
<connect gate="G$1" pin="VSS@1" pad="1"/>
<connect gate="G$1" pin="VSS@2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUETOOTH_MODULE" prefix="U" uservalue="yes">
<description>&lt;b&gt;BLUETOOTH MODULE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BLUETOOTH_MODULE"/>
</gates>
<devices>
<device name="" package="BLUETOOTH_MODULE">
<connects>
<connect gate="G$1" pin="3.3V" pad="12"/>
<connect gate="G$1" pin="AIO_0" pad="9"/>
<connect gate="G$1" pin="AIO_1" pad="10"/>
<connect gate="G$1" pin="CTS" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="GND@3" pad="21"/>
<connect gate="G$1" pin="GND@4" pad="22"/>
<connect gate="G$1" pin="PCM_CLK" pad="5"/>
<connect gate="G$1" pin="PCM_IN" pad="7"/>
<connect gate="G$1" pin="PCM_OUT" pad="6"/>
<connect gate="G$1" pin="PCM_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO_0" pad="23"/>
<connect gate="G$1" pin="PIO_1" pad="24"/>
<connect gate="G$1" pin="PIO_10" pad="33"/>
<connect gate="G$1" pin="PIO_11" pad="34"/>
<connect gate="G$1" pin="PIO_2" pad="25"/>
<connect gate="G$1" pin="PIO_3" pad="26"/>
<connect gate="G$1" pin="PIO_4" pad="27"/>
<connect gate="G$1" pin="PIO_5" pad="28"/>
<connect gate="G$1" pin="PIO_6" pad="29"/>
<connect gate="G$1" pin="PIO_7" pad="30"/>
<connect gate="G$1" pin="PIO_8" pad="31"/>
<connect gate="G$1" pin="PIO_9" pad="32"/>
<connect gate="G$1" pin="RESET" pad="11"/>
<connect gate="G$1" pin="RTS" pad="4"/>
<connect gate="G$1" pin="RXD" pad="2"/>
<connect gate="G$1" pin="SPI_CLK" pad="19"/>
<connect gate="G$1" pin="SPI_CS" pad="16"/>
<connect gate="G$1" pin="SPI_MISO" pad="18"/>
<connect gate="G$1" pin="SPI_MOSI" pad="17"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="USB_D+" pad="20"/>
<connect gate="G$1" pin="USB_D-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X17" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 1x17&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD17"/>
</gates>
<devices>
<device name="" package="1X17_ROUND70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_OLED_UG-2832HSWEG02" prefix="LCD" uservalue="yes">
<description>128x32 I2C 0.91" Monochrome OLED Display</description>
<gates>
<gate name="G$1" symbol="UG-2832HSWEG02"/>
</gates>
<devices>
<device name="" package="UG-2832HSWEG02_WRAPUNDER">
<connects>
<connect gate="G$1" pin="C1+" pad="3"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="2"/>
<connect gate="G$1" pin="IREF" pad="12"/>
<connect gate="G$1" pin="RES#" pad="9"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="5"/>
<connect gate="G$1" pin="VBREF" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VCOMH" pad="13"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9685" prefix="U" uservalue="yes">
<description>&lt;b&gt;PCA9685&lt;/b&gt; - 16 Channel 12-Bit I2C PWM Controller
&lt;p&gt;5.0V tolerant 16 channel, 12-bit I2C PWM controller with 25mA per output (max. 400mA total)&lt;/p&gt;
&lt;p&gt;Digikey: 568-5931-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PCA9865"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="G$1" pin="#OE" pad="23"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="24"/>
<connect gate="G$1" pin="EXTCLK" pad="25"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="PWM0" pad="6"/>
<connect gate="G$1" pin="PWM1" pad="7"/>
<connect gate="G$1" pin="PWM10" pad="17"/>
<connect gate="G$1" pin="PWM11" pad="18"/>
<connect gate="G$1" pin="PWM12" pad="19"/>
<connect gate="G$1" pin="PWM13" pad="20"/>
<connect gate="G$1" pin="PWM14" pad="21"/>
<connect gate="G$1" pin="PWM15" pad="22"/>
<connect gate="G$1" pin="PWM2" pad="8"/>
<connect gate="G$1" pin="PWM3" pad="9"/>
<connect gate="G$1" pin="PWM4" pad="10"/>
<connect gate="G$1" pin="PWM5" pad="11"/>
<connect gate="G$1" pin="PWM6" pad="12"/>
<connect gate="G$1" pin="PWM7" pad="13"/>
<connect gate="G$1" pin="PWM8" pad="15"/>
<connect gate="G$1" pin="PWM9" pad="16"/>
<connect gate="G$1" pin="SCL" pad="26"/>
<connect gate="G$1" pin="SDA" pad="27"/>
<connect gate="G$1" pin="VDD" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-3X08" prefix="JP" uservalue="yes">
<description>&lt;b&gt;3x8 0.1" Headers&lt;/b&gt;
&lt;p&gt;Male - 4UCON: 01058&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD3X08"/>
</gates>
<devices>
<device name="" package="3X08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERMBLOCK_1X2" prefix="J" uservalue="yes">
<description>3.5mm Terminal block
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="1X2"/>
</gates>
<devices>
<device name="" package="TERMBLOCK_1X2-3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHT_TSL13T" prefix="U" uservalue="yes">
<description>&lt;b&gt;TSL13T Analog Luminosity Sensor&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;VDD: 2.7-5.5V&lt;/li&gt;
&lt;li&gt;Range: 320-1050 nm&lt;/li&gt;
&lt;li&gt;Responsivity: 24mV/(µW/cm²)&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;b&gt;Mouser:&lt;/b&gt; 856-TSL13T</description>
<gates>
<gate name="G$1" symbol="TSL13T"/>
</gates>
<devices>
<device name="" package="TSL13T">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AS1115" prefix="U" uservalue="yes">
<description>&lt;b&gt;AS1115&lt;/b&gt; - 64 LED (8 * 7-Segment) LED Driver
&lt;p&gt;&lt;b&gt;VDD: &lt;/b&gt;2.7-5.5V&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Digikey:&lt;/b&gt; AS1115-BSSTCT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AS1115"/>
</gates>
<devices>
<device name="" package="QSOP24_0.635MM">
<connects>
<connect gate="G$1" pin="DIG0" pad="2"/>
<connect gate="G$1" pin="DIG1" pad="3"/>
<connect gate="G$1" pin="DIG2" pad="4"/>
<connect gate="G$1" pin="DIG3" pad="5"/>
<connect gate="G$1" pin="DIG4" pad="7"/>
<connect gate="G$1" pin="DIG5" pad="8"/>
<connect gate="G$1" pin="DIG6" pad="9"/>
<connect gate="G$1" pin="DIG7" pad="10"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IRQ" pad="24"/>
<connect gate="G$1" pin="ISET" pad="13"/>
<connect gate="G$1" pin="KEYA" pad="11"/>
<connect gate="G$1" pin="KEYB" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="SEGA" pad="15"/>
<connect gate="G$1" pin="SEGB" pad="17"/>
<connect gate="G$1" pin="SEGC" pad="20"/>
<connect gate="G$1" pin="SEGD" pad="23"/>
<connect gate="G$1" pin="SEGDP" pad="22"/>
<connect gate="G$1" pin="SEGE" pad="21"/>
<connect gate="G$1" pin="SEGF" pad="16"/>
<connect gate="G$1" pin="SEGG" pad="18"/>
<connect gate="G$1" pin="VDD" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1114/DIP28" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;LPC1114 MCU&lt;/b&gt;&lt;br/&gt; DIP28 Package&lt;/p&gt;
&lt;p&gt;ARM Cortex M0, 50MHz Operation, 6 Channel 10-Bit ADC, 1²C, SPI, UART, 2x16 Bit and 2x32 Bit Timers, Internal 12MHz Oscillator, 1.8-3.6V operation.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1114_DIP28"/>
</gates>
<devices>
<device name="" package="DIL28_600MIL">
<connects>
<connect gate="G$1" pin="#RESET/PIO0_0" pad="23"/>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="24"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="25"/>
<connect gate="G$1" pin="PIO0_3" pad="26"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="27"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="5"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="6"/>
<connect gate="G$1" pin="PIO0_7/#CTS" pad="28"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="13"/>
<connect gate="G$1" pin="PIO1_5/#RTS/CT32B0_CAP0" pad="14"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="15"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="16"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="17"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0" pad="18"/>
<connect gate="G$1" pin="R/PIO0_11/AD0/CT32B0_MAT3" pad="4"/>
<connect gate="G$1" pin="R/PIO1_0/AD1/CT32B1_CAP0" pad="9"/>
<connect gate="G$1" pin="R/PIO1_1/AD2/CT32B1_MAT0" pad="10"/>
<connect gate="G$1" pin="R/PIO1_2/AD3/CT32B1_MAT1" pad="11"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="3"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="12"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="XTALIN" pad="20"/>
<connect gate="G$1" pin="XTALOUT" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS_FGPMMOPA6C" prefix="U" uservalue="yes">
<description>&lt;b&gt;FGPMMOPA6C&lt;/b&gt; 16x16 GPS Module
&lt;p&gt;&lt;b&gt;NMEA Sentences&lt;/b&gt;: GGA, GSA, GSV, RMC, VTG&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FGPMMOPA6C"/>
</gates>
<devices>
<device name="" package="FGPMMOPA6C">
<connects>
<connect gate="G$1" pin="1PPS" pad="P$6"/>
<connect gate="G$1" pin="3D-FIX" pad="P$5"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$8"/>
<connect gate="G$1" pin="NC@1" pad="P$2"/>
<connect gate="G$1" pin="NC@2" pad="P$7"/>
<connect gate="G$1" pin="NC@3" pad="P$11"/>
<connect gate="G$1" pin="NC@4" pad="P$13"/>
<connect gate="G$1" pin="NC@5" pad="P$12"/>
<connect gate="G$1" pin="RX" pad="P$10"/>
<connect gate="G$1" pin="TX" pad="P$9"/>
<connect gate="G$1" pin="VBACKUP" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_SEGMENT_4DIGIT_TIME" prefix="LED" uservalue="yes">
<description>&lt;b&gt;4-Digit 7-Segment Display with colon and AM/PM dots&lt;/b&gt; - Common Cathode</description>
<gates>
<gate name="G$1" symbol="SEGMENT_4DIGIT_COMMONCATHODE_TIME"/>
</gates>
<devices>
<device name="" package="SEGMENT_BL-Q39A-42">
<connects>
<connect gate="G$1" pin="A" pad="P$14"/>
<connect gate="G$1" pin="B" pad="P$16"/>
<connect gate="G$1" pin="C" pad="P$13"/>
<connect gate="G$1" pin="COLON" pad="P$12"/>
<connect gate="G$1" pin="COLON_K" pad="P$4"/>
<connect gate="G$1" pin="D" pad="P$3"/>
<connect gate="G$1" pin="DOT" pad="P$9"/>
<connect gate="G$1" pin="DOT_K" pad="P$10"/>
<connect gate="G$1" pin="DP" pad="P$7"/>
<connect gate="G$1" pin="E" pad="P$5"/>
<connect gate="G$1" pin="F" pad="P$11"/>
<connect gate="G$1" pin="G" pad="P$15"/>
<connect gate="G$1" pin="SEG1_K" pad="P$1"/>
<connect gate="G$1" pin="SEG2_K" pad="P$2"/>
<connect gate="G$1" pin="SEG3_K" pad="P$6"/>
<connect gate="G$1" pin="SEG4_K" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GYRO_L3G2400D" prefix="U" uservalue="yes">
<description>&lt;b&gt;L3G4200D&lt;/b&gt; - 3-Axis MEMS gyroscope/motion sensor
&lt;ul&gt;
&lt;li&gt;Three selectable scales: 250/500/2000 dps&lt;/li&gt;
&lt;li&gt;1²C/SPI Interface&lt;/li&gt;
&lt;li&gt;16-bit data&lt;/li&gt;
&lt;li&gt;8-bit temperature&lt;/li&gt;
&lt;li&gt;VDD: 2.4-3.6V (IO 1.8V compatible)&lt;/li&gt;
&lt;li&gt;-40°C-85°C&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="L3G4200D"/>
</gates>
<devices>
<device name="" package="L3G4200D_LGA16L">
<connects>
<connect gate="G$1" pin="CS" pad="P$5"/>
<connect gate="G$1" pin="DRDY/INT2" pad="P$6"/>
<connect gate="G$1" pin="GND" pad="P$13"/>
<connect gate="G$1" pin="INT1" pad="P$7"/>
<connect gate="G$1" pin="PLLFILT" pad="P$14"/>
<connect gate="G$1" pin="RSVRD1(GND)" pad="P$8"/>
<connect gate="G$1" pin="RSVRD2(GND)" pad="P$9"/>
<connect gate="G$1" pin="RSVRD3(GND)" pad="P$10"/>
<connect gate="G$1" pin="RSVRD4(GND)" pad="P$11"/>
<connect gate="G$1" pin="RSVRD5(GND)" pad="P$12"/>
<connect gate="G$1" pin="RSVRD6(VDD)" pad="P$15"/>
<connect gate="G$1" pin="SCL/SPC" pad="P$2"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="P$3"/>
<connect gate="G$1" pin="SDO/SAO" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$16"/>
<connect gate="G$1" pin="VDDIO" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_JDT1800" prefix="LCD">
<gates>
<gate name="G$1" symbol="JD-T1800"/>
</gates>
<devices>
<device name="" package="JD-T1800">
<connects>
<connect gate="G$1" pin="CLOCK" pad="9"/>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="13"/>
<connect gate="G$1" pin="LEDA" pad="4"/>
<connect gate="G$1" pin="LEDK" pad="3"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="RS/DC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1347_QFP48" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1347 - ARM Cortex M3 72MHz MCU&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Supply: 2.0-3.6V&lt;/li&gt;
&lt;li&gt;12-bit 500kHz ADC&lt;/li&gt;
&lt;li&gt;Flash: 64KB&lt;/li&gt;
&lt;li&gt;EEPROM: 4KB&lt;/li&gt;
&lt;li&gt;SRAM: 8KB SRAM0 + 2KB SRAM1 + 2KB USB&lt;/li&gt;
&lt;li&gt;Temp: -40°C - 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1347_QFP48"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)" pad="4"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO0_17/RTS/CT32B0_CAP0/SCLK" pad="45"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="42"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL-(20MA_SINK)" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA-(20MA_SINK)" pad="16"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS-(20MA_SOURCE)" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1/SWO" pad="28"/>
<connect gate="G$1" pin="PIO1_13/DTR/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="G$1" pin="PIO1_14/DSR/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="G$1" pin="PIO1_15/DCD/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="G$1" pin="PIO1_16/RI/CT16B0_CAP0" pad="48"/>
<connect gate="G$1" pin="PIO1_19/DTR/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO1_20/DSR/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO1_21/DCD/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO1_22/RI/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="18"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="21"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="1"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="24"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="G$1" pin="PIO1_31" pad="25"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO0_14/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="8"/>
<connect gate="G$1" pin="VDD@2" pad="44"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1347_QFP64" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1347 - ARM Cortex M3 72MHz MCU&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Supply: 2.0-3.6V&lt;/li&gt;
&lt;li&gt;12-bit 500kHz ADC&lt;/li&gt;
&lt;li&gt;Flash: 64KB&lt;/li&gt;
&lt;li&gt;EEPROM: 4KB&lt;/li&gt;
&lt;li&gt;SRAM: 8KB SRAM0 + 2KB SRAM1 + 2KB USB&lt;/li&gt;
&lt;li&gt;Temp: -40°C - 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1347_QFP64"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2/USB_FTOGGLE-(ISP)" pad="5"/>
<connect gate="G$1" pin="PIO0_16/AD5/CT32B1_MAT3/WAKEUP" pad="53"/>
<connect gate="G$1" pin="PIO0_17/RTS/CT32B0_CAP0/SCLK" pad="60"/>
<connect gate="G$1" pin="PIO0_18/RXD/CT32B0_MAT0" pad="61"/>
<connect gate="G$1" pin="PIO0_19/TXD/CT32B0_MAT1" pad="62"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="13"/>
<connect gate="G$1" pin="PIO0_20/CT16B1_CAP0" pad="11"/>
<connect gate="G$1" pin="PIO0_21/CT16B1_MAT0/MOSI1" pad="22"/>
<connect gate="G$1" pin="PIO0_22/AD6/CT16B1_MAT1/MISO1" pad="40"/>
<connect gate="G$1" pin="PIO0_23/AD7" pad="56"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="19"/>
<connect gate="G$1" pin="PIO0_4/SCL-(20MA_SINK)" pad="20"/>
<connect gate="G$1" pin="PIO0_5/SDA-(20MA_SINK)" pad="21"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT/SCK0" pad="29"/>
<connect gate="G$1" pin="PIO0_7/CTS-(20MA_SOURCE)" pad="30"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="36"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1/SWO" pad="37"/>
<connect gate="G$1" pin="PIO1_0/CT32B1_MAT0" pad="1"/>
<connect gate="G$1" pin="PIO1_1/CT32B1_MAT1" pad="17"/>
<connect gate="G$1" pin="PIO1_10" pad="12"/>
<connect gate="G$1" pin="PIO1_11" pad="43"/>
<connect gate="G$1" pin="PIO1_13/DTR/CT16B0_MAT0/TXD" pad="47"/>
<connect gate="G$1" pin="PIO1_14/DSR/CT16B0_MAT1/RXD" pad="49"/>
<connect gate="G$1" pin="PIO1_15/DCD/CT16B0_MAT2/SCK1" pad="57"/>
<connect gate="G$1" pin="PIO1_16/RI/CT16B0_CAP0" pad="63"/>
<connect gate="G$1" pin="PIO1_17/CT16B0_CAP1/RXD" pad="23"/>
<connect gate="G$1" pin="PIO1_18/CT16B1_CAP1/TXD" pad="28"/>
<connect gate="G$1" pin="PIO1_19/DTR/SSEL1" pad="3"/>
<connect gate="G$1" pin="PIO1_2/CT32B1_MAT2" pad="34"/>
<connect gate="G$1" pin="PIO1_20/DSR/SCK1" pad="18"/>
<connect gate="G$1" pin="PIO1_21/DCD/MISO1" pad="35"/>
<connect gate="G$1" pin="PIO1_22/RI/MOSI1" pad="51"/>
<connect gate="G$1" pin="PIO1_23/CT16B1_MAT1/SSEL1" pad="24"/>
<connect gate="G$1" pin="PIO1_24/CT32B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO1_25/CT32B0_MAT1" pad="2"/>
<connect gate="G$1" pin="PIO1_26/CT32B0_MAT2/RXD" pad="14"/>
<connect gate="G$1" pin="PIO1_27/CT32B0_MAT3/TXD" pad="15"/>
<connect gate="G$1" pin="PIO1_28/CT32B0_CAP0/SCLK" pad="31"/>
<connect gate="G$1" pin="PIO1_29/SCK0/CT32B0_CAP1" pad="41"/>
<connect gate="G$1" pin="PIO1_3/CT32B1_MAT3" pad="50"/>
<connect gate="G$1" pin="PIO1_4/CT32B1_CAP0" pad="16"/>
<connect gate="G$1" pin="PIO1_5/CT32B1_CAP1" pad="32"/>
<connect gate="G$1" pin="PIO1_7" pad="6"/>
<connect gate="G$1" pin="PIO1_8" pad="39"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="4"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="38"/>
<connect gate="G$1" pin="SWDIO/PIO0_15/AD4/CT32B1_MAT2" pad="52"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="42"/>
<connect gate="G$1" pin="TDO/PIO0_13/AD2/CT32B1_MAT0" pad="45"/>
<connect gate="G$1" pin="TMS/PIO0_12/AD1/CT32B1_CAP0" pad="44"/>
<connect gate="G$1" pin="TRST/PIO0_14/AD3/CT32B1_MAT1" pad="46"/>
<connect gate="G$1" pin="USB_DM" pad="25"/>
<connect gate="G$1" pin="USB_DP" pad="26"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="33"/>
<connect gate="G$1" pin="VDD@3" pad="58"/>
<connect gate="G$1" pin="VDDA" pad="59"/>
<connect gate="G$1" pin="VREFN" pad="48"/>
<connect gate="G$1" pin="VREFP" pad="64"/>
<connect gate="G$1" pin="VSS@1" pad="7"/>
<connect gate="G$1" pin="VSS@2" pad="54"/>
<connect gate="G$1" pin="VSSA" pad="55"/>
<connect gate="G$1" pin="XTALIN" pad="8"/>
<connect gate="G$1" pin="XTALOUT" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-3X04" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD3X04"/>
</gates>
<devices>
<device name="" package="3X04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-2X13" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINH2X13"/>
</gates>
<devices>
<device name="" package="2X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_OLED_UG-2864HSWEG01" prefix="U" uservalue="yes">
<description>UG-2864HSWEG01 OLED display
&lt;p&gt;Both 1.3" and 0.96" models share the same FPC tab footprint, only the screen dimensions vary.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="UG-2864HSWEG01"/>
</gates>
<devices>
<device name="" package="UG-2864HSWEG01_1.3_WRAPAROUND">
<connects>
<connect gate="G$1" pin="/CS" pad="13"/>
<connect gate="G$1" pin="/RES" pad="14"/>
<connect gate="G$1" pin="BS0" pad="10"/>
<connect gate="G$1" pin="BS1" pad="11"/>
<connect gate="G$1" pin="BS2" pad="12"/>
<connect gate="G$1" pin="C1N" pad="5"/>
<connect gate="G$1" pin="C1P" pad="4"/>
<connect gate="G$1" pin="C2N" pad="3"/>
<connect gate="G$1" pin="C2P" pad="2"/>
<connect gate="G$1" pin="D0/SPI_SCLK/I2C_SCK" pad="18"/>
<connect gate="G$1" pin="D1/SPI_SDIN/I2C_SDA" pad="19"/>
<connect gate="G$1" pin="D2/I2C_SDA" pad="20"/>
<connect gate="G$1" pin="D3" pad="21"/>
<connect gate="G$1" pin="D4" pad="22"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="24"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="DC/I2C_SA0" pad="15"/>
<connect gate="G$1" pin="E/RD" pad="17"/>
<connect gate="G$1" pin="IREF" pad="26"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC(GND)@1" pad="1"/>
<connect gate="G$1" pin="NC(GND)@2" pad="30"/>
<connect gate="G$1" pin="R/W" pad="16"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VCOMH" pad="27"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VLSS" pad="29"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.96&quot;" package="UG-2864HSWEG01_0.96IN_WRAPAROUND">
<connects>
<connect gate="G$1" pin="/CS" pad="13"/>
<connect gate="G$1" pin="/RES" pad="14"/>
<connect gate="G$1" pin="BS0" pad="10"/>
<connect gate="G$1" pin="BS1" pad="11"/>
<connect gate="G$1" pin="BS2" pad="12"/>
<connect gate="G$1" pin="C1N" pad="5"/>
<connect gate="G$1" pin="C1P" pad="4"/>
<connect gate="G$1" pin="C2N" pad="3"/>
<connect gate="G$1" pin="C2P" pad="2"/>
<connect gate="G$1" pin="D0/SPI_SCLK/I2C_SCK" pad="18"/>
<connect gate="G$1" pin="D1/SPI_SDIN/I2C_SDA" pad="19"/>
<connect gate="G$1" pin="D2/I2C_SDA" pad="20"/>
<connect gate="G$1" pin="D3" pad="21"/>
<connect gate="G$1" pin="D4" pad="22"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="24"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="DC/I2C_SA0" pad="15"/>
<connect gate="G$1" pin="E/RD" pad="17"/>
<connect gate="G$1" pin="IREF" pad="26"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC(GND)@1" pad="1"/>
<connect gate="G$1" pin="NC(GND)@2" pad="30"/>
<connect gate="G$1" pin="R/W" pad="16"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VCOMH" pad="27"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VLSS" pad="29"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_4WAY_TPA511GLFS" prefix="BTN" uservalue="yes">
<gates>
<gate name="G$1" symbol="SWITCH_4WAY_TPA511GLFS"/>
</gates>
<devices>
<device name="" package="SWITCH_4WAY_TPA511GLFS">
<connects>
<connect gate="G$1" pin="1" pad="COMMON1"/>
<connect gate="G$1" pin="2" pad="COMMON2"/>
<connect gate="G$1" pin="3" pad="UP/3"/>
<connect gate="G$1" pin="4" pad="DOWN/4"/>
<connect gate="G$1" pin="5" pad="SELECT/5"/>
<connect gate="G$1" pin="6" pad="RIGHT/6"/>
<connect gate="G$1" pin="7" pad="LEFT/7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HT16K33_SOP20" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="HT16K33_20PIN"/>
</gates>
<devices>
<device name="" package="SOP20_300MIL">
<connects>
<connect gate="G$1" pin="COM0/AD" pad="P$2"/>
<connect gate="G$1" pin="COM1/KS0" pad="P$3"/>
<connect gate="G$1" pin="COM2/KS1" pad="P$4"/>
<connect gate="G$1" pin="COM3/KS2" pad="P$5"/>
<connect gate="G$1" pin="COM4" pad="P$6"/>
<connect gate="G$1" pin="COM5" pad="P$7"/>
<connect gate="G$1" pin="COM6" pad="P$8"/>
<connect gate="G$1" pin="COM7" pad="P$9"/>
<connect gate="G$1" pin="ROW0/K1" pad="P$17"/>
<connect gate="G$1" pin="ROW1/K2" pad="P$16"/>
<connect gate="G$1" pin="ROW2/K3" pad="P$15"/>
<connect gate="G$1" pin="ROW3/K4" pad="P$14"/>
<connect gate="G$1" pin="ROW4/K5" pad="P$13"/>
<connect gate="G$1" pin="ROW5/K6" pad="P$12"/>
<connect gate="G$1" pin="ROW6/K7" pad="P$11"/>
<connect gate="G$1" pin="ROW7/K8/INT" pad="P$10"/>
<connect gate="G$1" pin="SCL" pad="P$18"/>
<connect gate="G$1" pin="SDA" pad="P$19"/>
<connect gate="G$1" pin="VDD" pad="P$20"/>
<connect gate="G$1" pin="VSS" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HT16K33_SOP24" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="HT16K33_24PIN"/>
</gates>
<devices>
<device name="" package="SOP24_300MIL">
<connects>
<connect gate="G$1" pin="COM0/AD" pad="P$2"/>
<connect gate="G$1" pin="COM1/KS0" pad="P$3"/>
<connect gate="G$1" pin="COM2/KS1" pad="P$4"/>
<connect gate="G$1" pin="COM3/KS2" pad="P$5"/>
<connect gate="G$1" pin="COM4" pad="P$6"/>
<connect gate="G$1" pin="COM5" pad="P$7"/>
<connect gate="G$1" pin="COM6" pad="P$8"/>
<connect gate="G$1" pin="COM7" pad="P$9"/>
<connect gate="G$1" pin="ROW0/A1" pad="P$21"/>
<connect gate="G$1" pin="ROW1/A0" pad="P$20"/>
<connect gate="G$1" pin="ROW10/K9" pad="P$11"/>
<connect gate="G$1" pin="ROW11/K10/INT" pad="P$10"/>
<connect gate="G$1" pin="ROW2/K1" pad="P$19"/>
<connect gate="G$1" pin="ROW3/K2" pad="P$18"/>
<connect gate="G$1" pin="ROW4/K3" pad="P$17"/>
<connect gate="G$1" pin="ROW5/K4" pad="P$16"/>
<connect gate="G$1" pin="ROW6/K5" pad="P$15"/>
<connect gate="G$1" pin="ROW7/K6" pad="P$14"/>
<connect gate="G$1" pin="ROW8/K7" pad="P$13"/>
<connect gate="G$1" pin="ROW9/K8" pad="P$12"/>
<connect gate="G$1" pin="SCL" pad="P$22"/>
<connect gate="G$1" pin="SDA" pad="P$23"/>
<connect gate="G$1" pin="VDD" pad="P$24"/>
<connect gate="G$1" pin="VSS" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HT16K33_SOP28" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="HT16K33_28PIN"/>
</gates>
<devices>
<device name="" package="SOP28_300MIL">
<connects>
<connect gate="G$1" pin="COM0/AD" pad="P$2"/>
<connect gate="G$1" pin="COM1/KS0" pad="P$3"/>
<connect gate="G$1" pin="COM2/KS1" pad="P$4"/>
<connect gate="G$1" pin="COM3/KS2" pad="P$5"/>
<connect gate="G$1" pin="COM4" pad="P$6"/>
<connect gate="G$1" pin="COM5" pad="P$7"/>
<connect gate="G$1" pin="COM6" pad="P$8"/>
<connect gate="G$1" pin="COM7" pad="P$9"/>
<connect gate="G$1" pin="ROW0/A2" pad="P$25"/>
<connect gate="G$1" pin="ROW1/A1" pad="P$24"/>
<connect gate="G$1" pin="ROW10/K8" pad="P$15"/>
<connect gate="G$1" pin="ROW11/K9" pad="P$14"/>
<connect gate="G$1" pin="ROW12/K10" pad="P$13"/>
<connect gate="G$1" pin="ROW13/K11" pad="P$12"/>
<connect gate="G$1" pin="ROW14/K12" pad="P$11"/>
<connect gate="G$1" pin="ROW15/K13/INT" pad="P$10"/>
<connect gate="G$1" pin="ROW2/A0" pad="P$23"/>
<connect gate="G$1" pin="ROW3/K1" pad="P$22"/>
<connect gate="G$1" pin="ROW4/K2" pad="P$21"/>
<connect gate="G$1" pin="ROW5/K3" pad="P$20"/>
<connect gate="G$1" pin="ROW6/K4" pad="P$19"/>
<connect gate="G$1" pin="ROW7/K5" pad="P$18"/>
<connect gate="G$1" pin="ROW8/K6" pad="P$17"/>
<connect gate="G$1" pin="ROW9/K7" pad="P$16"/>
<connect gate="G$1" pin="SCL" pad="P$26"/>
<connect gate="G$1" pin="SDA" pad="P$27"/>
<connect gate="G$1" pin="VDD" pad="P$28"/>
<connect gate="G$1" pin="VSS" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_SEGMENT_4DIGIT_BL-Q56C43" prefix="LED" uservalue="yes">
<gates>
<gate name="G$1" symbol="SEGMENT_4DIGIT_COMMONCATHODE_TIME_14PIN"/>
</gates>
<devices>
<device name="" package="SEGMENT-BL-Q56C43">
<connects>
<connect gate="G$1" pin="P$1" pad="P$14"/>
<connect gate="G$1" pin="P$10" pad="P$1"/>
<connect gate="G$1" pin="P$11" pad="P$12"/>
<connect gate="G$1" pin="P$12" pad="P$5"/>
<connect gate="G$1" pin="P$13" pad="P$3"/>
<connect gate="G$1" pin="P$15" pad="P$8"/>
<connect gate="G$1" pin="P$2" pad="P$11"/>
<connect gate="G$1" pin="P$3" pad="P$7"/>
<connect gate="G$1" pin="P$4" pad="P$10"/>
<connect gate="G$1" pin="P$5" pad="P$6"/>
<connect gate="G$1" pin="P$6" pad="P$13"/>
<connect gate="G$1" pin="P$7" pad="P$9"/>
<connect gate="G$1" pin="P$8" pad="P$4"/>
<connect gate="G$1" pin="P$9" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA5767MODULE" prefix="U" uservalue="yes">
<description>&lt;b&gt;TEA5767 FM-Receiver Module&lt;/b&gt; - 87.5-108MHz</description>
<gates>
<gate name="G$1" symbol="TEA5767MODULE"/>
</gates>
<devices>
<device name="" package="TEA5767MODULE">
<connects>
<connect gate="G$1" pin="ANT" pad="10"/>
<connect gate="G$1" pin="BUSMODE" pad="3"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="L-OUT" pad="8"/>
<connect gate="G$1" pin="MPXO" pad="9"/>
<connect gate="G$1" pin="R-OUT" pad="7"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="W/R" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIOAMP_NCP2811" prefix="U" uservalue="yes">
<description>&lt;b&gt;NCP2811 Stereo Headphone Amplifier&lt;/b&gt;
&lt;p&gt;TSSOP-14 - Mouser: 863-NCP2811ADTBR2G&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NCP2811"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="/SD" pad="7"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="AVCC" pad="2"/>
<connect gate="G$1" pin="CP+" pad="3"/>
<connect gate="G$1" pin="CP-" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN_LEFT" pad="9"/>
<connect gate="G$1" pin="IN_RIGHT" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="8"/>
<connect gate="G$1" pin="NC@3" pad="1"/>
<connect gate="G$1" pin="OUT_LEFT" pad="14"/>
<connect gate="G$1" pin="OUT_RIGHT" pad="13"/>
<connect gate="G$1" pin="PVM" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HB100" prefix="U" uservalue="yes">
<description>&lt;b&gt;HB100 Miniature Microwave Motion Sensor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="HB100"/>
</gates>
<devices>
<device name="" package="HB100">
<connects>
<connect gate="G$1" pin="5V@1" pad="5V@1"/>
<connect gate="G$1" pin="5V@2" pad="5V@2"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="GND@4" pad="GND@4"/>
<connect gate="G$1" pin="IF@1" pad="IF@1"/>
<connect gate="G$1" pin="IF@2" pad="IF@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA219" prefix="U" uservalue="yes">
<description>&lt;b&gt;INA219 - I2C Current/Power Monitor&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Voltage Range: 0-26V&lt;/li&gt;
&lt;li&gt;Accuracy: 0.5%&lt;/li&gt;
&lt;li&gt;Temperature: -40°C - 125°C&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="INA219"/>
</gates>
<devices>
<device name="" package="SOT23-8">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="8"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VIN+" pad="1"/>
<connect gate="G$1" pin="VIN-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS_FGPMMOPA6H" prefix="U" uservalue="yes">
<description>&lt;b&gt;GPS Module&lt;/b&gt; - MTK MT3339 Chipset, -165dBm sensitivity, 22 channels, 10Hz, auto-select external antenna options</description>
<gates>
<gate name="G$1" symbol="FGPMMOPA6H"/>
</gates>
<devices>
<device name="" package="FGPMMOPA6H">
<connects>
<connect gate="G$1" pin="1PPS" pad="P$13"/>
<connect gate="G$1" pin="3D-FIX" pad="P$5"/>
<connect gate="G$1" pin="EX_ANT" pad="P$11"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$8"/>
<connect gate="G$1" pin="GND@3" pad="P$12"/>
<connect gate="G$1" pin="GND@4" pad="P$19"/>
<connect gate="G$1" pin="NC@1" pad="P$6"/>
<connect gate="G$1" pin="NC@2" pad="P$7"/>
<connect gate="G$1" pin="NC@3" pad="P$15"/>
<connect gate="G$1" pin="NC@4" pad="P$16"/>
<connect gate="G$1" pin="NC@5" pad="P$17"/>
<connect gate="G$1" pin="NC@6" pad="P$18"/>
<connect gate="G$1" pin="NC@7" pad="P$20"/>
<connect gate="G$1" pin="NRESET" pad="P$2"/>
<connect gate="G$1" pin="RTCM" pad="P$14"/>
<connect gate="G$1" pin="RX" pad="P$10"/>
<connect gate="G$1" pin="TX" pad="P$9"/>
<connect gate="G$1" pin="VBACKUP" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRYPI_B">
<gates>
<gate name="G$1" symbol="RASPBERRYPI_REV_B"/>
</gates>
<devices>
<device name="B" package="RASBERRYPI_SHIELD">
<connects>
<connect gate="G$1" pin="#SPI_CE0" pad="24"/>
<connect gate="G$1" pin="#SPI_CE1" pad="26"/>
<connect gate="G$1" pin="3.3V@1" pad="1"/>
<connect gate="G$1" pin="5.0V@1" pad="2"/>
<connect gate="G$1" pin="DNC@1" pad="4"/>
<connect gate="G$1" pin="DNC@2" pad="9"/>
<connect gate="G$1" pin="DNC@3" pad="14"/>
<connect gate="G$1" pin="DNC@4" pad="17"/>
<connect gate="G$1" pin="DNC@5" pad="20"/>
<connect gate="G$1" pin="DNC@6" pad="25"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL0" pad="5"/>
<connect gate="G$1" pin="SDA0" pad="3"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADBM-A350" prefix="U" uservalue="yes">
<description>&lt;b&gt;ADBM-A350&lt;/b&gt; - Optical Finger Navigation Sensor
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;VDD: 1.7-2.1V (1.8V Typical)&lt;/li&gt;
&lt;li&gt;VDDIO: 1.65-3.6V (1.8V or 2.8V Typical)&lt;/li&gt;
&lt;li&gt;Operating Temp: -20-70°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;FPC Connector&lt;/b&gt;: Hirose FH26-17S-0.3SHW(05)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADBM-A350"/>
</gates>
<devices>
<device name="" package="ADBM-A350">
<connects>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="DOME+" pad="14"/>
<connect gate="G$1" pin="DOME-" pad="9"/>
<connect gate="G$1" pin="EVENT_INT" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="GPIO" pad="2"/>
<connect gate="G$1" pin="IO_SELECT" pad="15"/>
<connect gate="G$1" pin="MISO_SDA" pad="5"/>
<connect gate="G$1" pin="MOSI_A0" pad="6"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="17"/>
<connect gate="G$1" pin="NCS_A1" pad="4"/>
<connect gate="G$1" pin="NRST" pad="8"/>
<connect gate="G$1" pin="SHTDWN" pad="11"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VDDIO" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1113/4/5_QFP48_XLSERIES" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC1113/4/5 ARM Cortex M0 MCU (50MHz)&lt;/b&gt; - XL Series (FBD48/3x3)
&lt;p&gt;
LPC1115FBD48/303:
&lt;ul&gt;
&lt;li&gt;Max Frequency: 50MHz&lt;/li&gt;
&lt;li&gt;Flash: 64kB&lt;/li&gt;
&lt;li&gt;SRAM: 8kB&lt;/li&gt;
&lt;li&gt;ADC: 10-bit&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1113/4/5_FBD48/XL"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/CLKOUT/CT32B0_MAT2" pad="4"/>
<connect gate="G$1" pin="PIO0_2/SSEL0/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_3" pad="14"/>
<connect gate="G$1" pin="PIO0_4/SCL" pad="15"/>
<connect gate="G$1" pin="PIO0_5/SDA" pad="16"/>
<connect gate="G$1" pin="PIO0_6/SCK0" pad="22"/>
<connect gate="G$1" pin="PIO0_7/CTS" pad="23"/>
<connect gate="G$1" pin="PIO0_8/MISO0/CT16B0_MAT0" pad="27"/>
<connect gate="G$1" pin="PIO0_9/MOSI0/CT16B0_MAT1" pad="28"/>
<connect gate="G$1" pin="PIO1_10/AD6/CT16B1_MAT1/MISO1" pad="30"/>
<connect gate="G$1" pin="PIO1_11/AD7/CT32B1_CAP1" pad="42"/>
<connect gate="G$1" pin="PIO1_4/AD5/CT32B1_MAT3/WAKEUP" pad="40"/>
<connect gate="G$1" pin="PIO1_5/RTS/CT32B0_CAP0" pad="45"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="46"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="47"/>
<connect gate="G$1" pin="PIO1_8/CT16B1_CAP0" pad="9"/>
<connect gate="G$1" pin="PIO1_9/CT16B1_MAT0/MOSI1" pad="17"/>
<connect gate="G$1" pin="PIO2_0/DTR/SSEL1" pad="2"/>
<connect gate="G$1" pin="PIO2_1/DSR/SCK1" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11/SCK0/CT32B0_CAP1" pad="31"/>
<connect gate="G$1" pin="PIO2_2/DCD/MISO1" pad="26"/>
<connect gate="G$1" pin="PIO2_3/RI/MOSI1" pad="38"/>
<connect gate="G$1" pin="PIO2_4/CT16B1_MAT1/SSEL1" pad="19"/>
<connect gate="G$1" pin="PIO2_5/CT32B0_MAT0" pad="20"/>
<connect gate="G$1" pin="PIO2_6/CT32B0_MAT1" pad="1"/>
<connect gate="G$1" pin="PIO2_7/CT32B0_MAT2/RXD" pad="11"/>
<connect gate="G$1" pin="PIO2_8/CT32B0_MAT3/TXD" pad="12"/>
<connect gate="G$1" pin="PIO2_9/CT32B0_CAP0" pad="24"/>
<connect gate="G$1" pin="PIO3_0/DTR/CT16B0_MAT0/TXD" pad="36"/>
<connect gate="G$1" pin="PIO3_1/DSR/CT16B0_MAT1/RXD" pad="37"/>
<connect gate="G$1" pin="PIO3_2/DCD/CT16B0_MAT2/SCK1" pad="43"/>
<connect gate="G$1" pin="PIO3_3/RI/CT16B0_CAP0" pad="48"/>
<connect gate="G$1" pin="PIO3_4/CT16B0_CAP1/RXD" pad="18"/>
<connect gate="G$1" pin="PIO3_5/CT16B1_CAP1/TXD" pad="21"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK0/CT16B0_MAT2" pad="29"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="39"/>
<connect gate="G$1" pin="TDI/PIO0_11/AD0/CT32B0_MAT3" pad="32"/>
<connect gate="G$1" pin="TDO/PIO1_1/AD2/CT32B1_MAT0" pad="34"/>
<connect gate="G$1" pin="TMS/PIO1_0/AD1/CT32B1_CAP0" pad="33"/>
<connect gate="G$1" pin="TRST/PIO1_2/AD3/CT32B1_MAT1" pad="35"/>
<connect gate="G$1" pin="VDD@1" pad="8"/>
<connect gate="G$1" pin="VDD@2" pad="44"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="G$1" pin="VSS(IO)" pad="41"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;2-Way Solder Jumper&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SOLDERJUMPER_2WAY"/>
</gates>
<devices>
<device name="" package="SOLDERJUMPER_2WAY_OPEN_NOPASTE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="SOLDERJUMPER_2WAY_OPEN_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="SOLDERJUMPER_2WAY_OPEN_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC_MCP4725" prefix="U" uservalue="yes">
<description>&lt;b&gt;MCP4725 - 12-Bit I2C DAC with on-board EEPROM&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Settling Time: 6 µs&lt;/li&gt;
&lt;li&gt;2.7-5.5V Supply&lt;/li&gt;
&lt;li&gt;100kHz, 400kHz, 3.4 Mbps I²C&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;EEPROM can be used to store a specific output voltage which will be set coming out of reset&lt;/p&gt;
&lt;p&gt;&lt;b&gt;I²C Address&lt;/b&gt;: 1100 A2 A1 A0&lt;/p&gt;
&lt;p&gt;A0 is set via the A0 pin, A2 and A1 are hard-wired on the chip depending on the model chosen:&lt;/p&gt;
&lt;p&gt;
&lt;table cellpadding="5" border="1" cellspacing="5"&gt;
&lt;tr&gt;
&lt;td&gt;&lt;b&gt;Part Number&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;A2 A1&lt;/b&gt;&lt;/td&gt;
&lt;td&gt;&lt;b&gt;Code&lt;/b&gt;&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MCP4725A0T-E/CH&lt;/td&gt;
  &lt;td&gt;0 0&lt;/td&gt;
  &lt;td&gt;AJNN&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MCP4725A1T-E/CH&lt;/td&gt;
  &lt;td&gt;0 1&lt;/td&gt;
  &lt;td&gt;APNN&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MCP4725A2T-E/CH&lt;/td&gt;
  &lt;td&gt;1 0&lt;/td&gt;
  &lt;td&gt;AQNN&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;MCP4725A3T-E/CH&lt;/td&gt;
  &lt;td&gt;1 1&lt;/td&gt;
  &lt;td&gt;ARNN&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MCP4725"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC_ADS1015" prefix="U" uservalue="yes">
<description>&lt;b&gt;ADS1015 - 12-bit 4-Channel I2C ADC with Internal PGA&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;VDD: 2.0-5.5V&lt;/li&gt;
&lt;li&gt;Sampling Rate: 3.3ksps&lt;/li&gt;
&lt;li&gt;Gain Settings: 2/3, 1, 2, 4, 8, 16&lt;/li&gt;
&lt;li&gt;I2C Address: ADDR low = 1001000x, ADDR high = 1001001x&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Internal Comparator&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;The ADS1015 includes an internal comparator that can be set to output a high-level on ALERT when the conversion results exceeeds a pre-defined upper level, and will deassert itself when the level falls below a pre-defined lower threshold level. It can also be set to windowed mode where the ALERT pin will be asserted if the data exceeds the upper threshold or falls below the lower threshold.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADS1015"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="ADDR" pad="1"/>
<connect gate="G$1" pin="AIN0" pad="4"/>
<connect gate="G$1" pin="AIN1" pad="5"/>
<connect gate="G$1" pin="AIN2" pad="6"/>
<connect gate="G$1" pin="AIN3" pad="7"/>
<connect gate="G$1" pin="ALERT" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC_ADS7924" prefix="U" uservalue="yes">
<description>&lt;b&gt;ADS7924 - 12-bit 4-Channel I2C ADC&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;AVDD: 2.2-5.5V&lt;/li&gt;
&lt;li&gt;DVDD: 1.65V-5.5V&lt;/li&gt;
&lt;li&gt;Sampling Rate: 100ksps&lt;/li&gt;
&lt;li&gt;I2C Address: ADDR low = 1001000x, ADDR DVDD = 1001001x&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Digital Threshold Comparators&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;The ADS794 is a relatively low-power device and can be useful in certain low-power scenarios since it can be configured to regularly check the voltage on the analog input pins, and throw an interrupt or pull an MCU out of reset when a specific condition is met.  Each of the four inputs has it's own programmable threshold level.  It could be used to monitor the input level of solar or other ambient energy sources, and when the level is sufficiently high, wakeup the MCU to perform read some sensor data, etc., or wait until a supercap is charged to a sufficiently high level before waking the MCU.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7924"/>
</gates>
<devices>
<device name="" package="WQFN16">
<connects>
<connect gate="G$1" pin="A0" pad="P$5"/>
<connect gate="G$1" pin="ADCIN" pad="P$14"/>
<connect gate="G$1" pin="AGND" pad="P$8"/>
<connect gate="G$1" pin="AIN0" pad="P$12"/>
<connect gate="G$1" pin="AIN1" pad="P$11"/>
<connect gate="G$1" pin="AIN2" pad="P$10"/>
<connect gate="G$1" pin="AIN3" pad="P$9"/>
<connect gate="G$1" pin="AVDD" pad="P$15"/>
<connect gate="G$1" pin="DGND" pad="P$6"/>
<connect gate="G$1" pin="DVDD" pad="P$16"/>
<connect gate="G$1" pin="INT" pad="P$2"/>
<connect gate="G$1" pin="MUXOUT" pad="P$13"/>
<connect gate="G$1" pin="PWRCON" pad="P$7"/>
<connect gate="G$1" pin="RESET" pad="P$1"/>
<connect gate="G$1" pin="SCL" pad="P$3"/>
<connect gate="G$1" pin="SDA" pad="P$4"/>
<connect gate="G$1" pin="THERMAL" pad="P$17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AUP2G126" prefix="U" uservalue="yes">
<description>&lt;b&gt;74AUP2G126&lt;/b&gt; - Low-Power Dual Tri-State Buffer
&lt;p&gt;OE high enables output.  For OE Low enabled output use 74AUP2G125.&lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;VCC: 0.8-3.6V&lt;/li&gt;
&lt;li&gt;Temp: -40°C - 125°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;Package Variant: 8-VSSOP (SOT765-1)&lt;/p&gt;
&lt;p&gt;Manuf. ID: 74AUP2G126DC,125&lt;/p&gt;
&lt;p&gt;Digikey: 568-4987-1-ND&lt;/p&gt;
&lt;p&gt;&lt;b&gt;NOTE: &lt;/b&gt;Make sure to check the propogation delay to see if it's short enough for your timing since it's largely dependant on the line capacitance and supply voltage!&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="74AUP2G126"/>
</gates>
<devices>
<device name="" package="VFSOP-8">
<connects>
<connect gate="G$1" pin="1A" pad="2"/>
<connect gate="G$1" pin="1OE" pad="1"/>
<connect gate="G$1" pin="1Y" pad="6"/>
<connect gate="G$1" pin="2A" pad="5"/>
<connect gate="G$1" pin="2OE" pad="7"/>
<connect gate="G$1" pin="2Y" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_S6B33B6_15IN33PIN" prefix="U" uservalue="yes">
<description>&lt;b&gt;1.5" 128x128 Pixel 65K CSTN LCD with S6B33B6 Controller&lt;/b&gt;
&lt;p&gt;33-Pins&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="S6B33B6_1.5IN_LCD"/>
</gates>
<devices>
<device name="" package="S6B33B6_1.5IN_LCD">
<connects>
<connect gate="G$1" pin="CS1" pad="P$28"/>
<connect gate="G$1" pin="DB0" pad="P$23"/>
<connect gate="G$1" pin="DB1" pad="P$22"/>
<connect gate="G$1" pin="DB10" pad="P$13"/>
<connect gate="G$1" pin="DB11" pad="P$12"/>
<connect gate="G$1" pin="DB12" pad="P$11"/>
<connect gate="G$1" pin="DB13" pad="P$10"/>
<connect gate="G$1" pin="DB14" pad="P$9"/>
<connect gate="G$1" pin="DB15" pad="P$8"/>
<connect gate="G$1" pin="DB2" pad="P$21"/>
<connect gate="G$1" pin="DB3" pad="P$20"/>
<connect gate="G$1" pin="DB4" pad="P$19"/>
<connect gate="G$1" pin="DB5" pad="P$18"/>
<connect gate="G$1" pin="DB6/SCL" pad="P$17"/>
<connect gate="G$1" pin="DB7/SDI" pad="P$16"/>
<connect gate="G$1" pin="DB8" pad="P$15"/>
<connect gate="G$1" pin="DB9" pad="P$14"/>
<connect gate="G$1" pin="GND@1" pad="P$7"/>
<connect gate="G$1" pin="GND@2" pad="P$29"/>
<connect gate="G$1" pin="LED_A" pad="P$3"/>
<connect gate="G$1" pin="LED_K" pad="P$2"/>
<connect gate="G$1" pin="MPU" pad="P$30"/>
<connect gate="G$1" pin="NC@1" pad="P$1"/>
<connect gate="G$1" pin="OTPD(NC)" pad="P$33"/>
<connect gate="G$1" pin="OTPG(NC)" pad="P$32"/>
<connect gate="G$1" pin="PS" pad="P$31"/>
<connect gate="G$1" pin="RD" pad="P$24"/>
<connect gate="G$1" pin="RESET" pad="P$27"/>
<connect gate="G$1" pin="RS/DATA_INSTR" pad="P$26"/>
<connect gate="G$1" pin="VDD(3V3)" pad="P$6"/>
<connect gate="G$1" pin="VEE" pad="P$5"/>
<connect gate="G$1" pin="VRP" pad="P$4"/>
<connect gate="G$1" pin="WR" pad="P$25"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIOAMP_TPA2012D2" prefix="U" uservalue="yes">
<description>&lt;b&gt;TPA2012D2 2.1W/CH Stereo Class-D Audio Amp&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;2.1W/Ch into 4 Ohm at 5V&lt;/li&gt;
&lt;li&gt;1.4W/Ch into 8 Ohm at 5V&lt;/li&gt;
&lt;li&gt;720mW/Ch into 8 ohm at 3.6V&lt;/li&gt;
&lt;li&gt;Selectable Gain: 6, 12, 18 or 24 dB&lt;/li&gt;
&lt;li&gt;Power Supply (PVDD and AVDD): 2.5-5.5V&lt;/li&gt;
&lt;li&gt;Operating Temperature: -40 to 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey (QFN20): 296-17692-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TPA2012D2"/>
</gates>
<devices>
<device name="" package="WQFN20">
<connects>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="AVDD" pad="9"/>
<connect gate="G$1" pin="G0" pad="15"/>
<connect gate="G$1" pin="G1" pad="1"/>
<connect gate="G$1" pin="INL+" pad="20"/>
<connect gate="G$1" pin="INL-" pad="19"/>
<connect gate="G$1" pin="INR+" pad="16"/>
<connect gate="G$1" pin="INR-" pad="17"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="10"/>
<connect gate="G$1" pin="OUTL+" pad="2"/>
<connect gate="G$1" pin="OUTL-" pad="5"/>
<connect gate="G$1" pin="OUTR+" pad="14"/>
<connect gate="G$1" pin="OUTR-" pad="11"/>
<connect gate="G$1" pin="PGND@1" pad="4"/>
<connect gate="G$1" pin="PGND@2" pad="12"/>
<connect gate="G$1" pin="PVDD@1" pad="3"/>
<connect gate="G$1" pin="PVDD@2" pad="13"/>
<connect gate="G$1" pin="SHUTDOWN_L" pad="7"/>
<connect gate="G$1" pin="SHUTDOWN_R" pad="8"/>
<connect gate="G$1" pin="THERMAL" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI4731-D60-GU" prefix="U" uservalue="yes">
<description>&lt;b&gt;Silicon Labs Si4731 AM/FM/SW/LW Radio Receiver&lt;/b&gt; -- SSOP Package</description>
<gates>
<gate name="G$1" symbol="SI4731-D60-GU"/>
</gates>
<devices>
<device name="" package="SI473X_SSOP">
<connects>
<connect gate="G$1" pin="AMI" pad="P$12"/>
<connect gate="G$1" pin="DBYP" pad="P$22"/>
<connect gate="G$1" pin="DFS/RIN" pad="P$2"/>
<connect gate="G$1" pin="DOUT/LIN" pad="P$1"/>
<connect gate="G$1" pin="FMI" pad="P$8"/>
<connect gate="G$1" pin="GND@1" pad="P$13"/>
<connect gate="G$1" pin="GND@2" pad="P$14"/>
<connect gate="G$1" pin="GPO1" pad="P$5"/>
<connect gate="G$1" pin="GPO2/INT" pad="P$4"/>
<connect gate="G$1" pin="GPO3/DCLK" pad="P$3"/>
<connect gate="G$1" pin="LOUT" pad="P$24"/>
<connect gate="G$1" pin="NC@1" pad="P$6"/>
<connect gate="G$1" pin="NC@2" pad="P$7"/>
<connect gate="G$1" pin="NC@3" pad="P$10"/>
<connect gate="G$1" pin="NC@4" pad="P$11"/>
<connect gate="G$1" pin="RCLK" pad="P$19"/>
<connect gate="G$1" pin="RFGND" pad="P$9"/>
<connect gate="G$1" pin="ROUT" pad="P$23"/>
<connect gate="G$1" pin="RSTB" pad="P$15"/>
<connect gate="G$1" pin="SCLK" pad="P$17"/>
<connect gate="G$1" pin="SDIO" pad="P$18"/>
<connect gate="G$1" pin="SENB" pad="P$16"/>
<connect gate="G$1" pin="VCCA" pad="P$21"/>
<connect gate="G$1" pin="VCCD" pad="P$20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRV8833" prefix="U" uservalue="yes">
<description>&lt;b&gt;DRV8833 Dual H-Bridge Motor Driver&lt;/b&gt; -- HTSSOP Package</description>
<gates>
<gate name="G$1" symbol="DRV8833"/>
</gates>
<devices>
<device name="" package="HTSSOP16">
<connects>
<connect gate="G$1" pin="A_IN1" pad="P$16"/>
<connect gate="G$1" pin="A_IN2" pad="P$15"/>
<connect gate="G$1" pin="A_ISENSE" pad="P$3"/>
<connect gate="G$1" pin="A_OUT1" pad="P$2"/>
<connect gate="G$1" pin="A_OUT2" pad="P$4"/>
<connect gate="G$1" pin="B_IN1" pad="P$9"/>
<connect gate="G$1" pin="B_IN2" pad="P$10"/>
<connect gate="G$1" pin="B_ISENSE" pad="P$6"/>
<connect gate="G$1" pin="B_OUT1" pad="P$7"/>
<connect gate="G$1" pin="B_OUT2" pad="P$5"/>
<connect gate="G$1" pin="GND(THRML)" pad="P$17"/>
<connect gate="G$1" pin="GND@1" pad="P$13"/>
<connect gate="G$1" pin="NFAULT" pad="P$8"/>
<connect gate="G$1" pin="NSLEEP" pad="P$1"/>
<connect gate="G$1" pin="VCP" pad="P$11"/>
<connect gate="G$1" pin="VINT" pad="P$14"/>
<connect gate="G$1" pin="VM" pad="P$12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TB6612FNG" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;TB6612FNG Dual H-Bridge Motor Driver&lt;/b&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TB6612FNG"/>
</gates>
<devices>
<device name="SSOP" package="SSOP24">
<connects>
<connect gate="G$1" pin="AIN1" pad="21"/>
<connect gate="G$1" pin="AIN2" pad="22"/>
<connect gate="G$1" pin="AOUT1@1" pad="1"/>
<connect gate="G$1" pin="AOUT1@2" pad="2"/>
<connect gate="G$1" pin="AOUT2@1" pad="5"/>
<connect gate="G$1" pin="AOUT2@2" pad="6"/>
<connect gate="G$1" pin="BIN1" pad="17"/>
<connect gate="G$1" pin="BIN2" pad="16"/>
<connect gate="G$1" pin="BOUT1@1" pad="11"/>
<connect gate="G$1" pin="BOUT1@2" pad="12"/>
<connect gate="G$1" pin="BOUT2@1" pad="7"/>
<connect gate="G$1" pin="BOUT2@2" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="PGND1@1" pad="3"/>
<connect gate="G$1" pin="PGND1@2" pad="4"/>
<connect gate="G$1" pin="PGND2@1" pad="9"/>
<connect gate="G$1" pin="PGND2@2" pad="10"/>
<connect gate="G$1" pin="PWMA" pad="23"/>
<connect gate="G$1" pin="PWMB" pad="15"/>
<connect gate="G$1" pin="STBY" pad="19"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VM@1" pad="24"/>
<connect gate="G$1" pin="VM@2" pad="13"/>
<connect gate="G$1" pin="VM@3" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIOAMP_MAX9814" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;MAX9814&lt;/b&gt; - Mono Microphone Amplifier with AGC&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX9814"/>
</gates>
<devices>
<device name="" package="WFDFN-14">
<connects>
<connect gate="G$1" pin="A/R" pad="P$9"/>
<connect gate="G$1" pin="BIAS" pad="P$12"/>
<connect gate="G$1" pin="CG" pad="P$3"/>
<connect gate="G$1" pin="CT" pad="P$1"/>
<connect gate="G$1" pin="GAIN" pad="P$10"/>
<connect gate="G$1" pin="GND" pad="P$7"/>
<connect gate="G$1" pin="MICBIAS" pad="P$13"/>
<connect gate="G$1" pin="MICIN" pad="P$8"/>
<connect gate="G$1" pin="MICOUT" pad="P$6"/>
<connect gate="G$1" pin="NC@1" pad="P$4"/>
<connect gate="G$1" pin="NC@2" pad="P$11"/>
<connect gate="G$1" pin="SHUTDOWN" pad="P$2"/>
<connect gate="G$1" pin="TH" pad="P$14"/>
<connect gate="G$1" pin="THERMAL" pad="P$THERM"/>
<connect gate="G$1" pin="VDD" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMBCONNECTOR" prefix="X" uservalue="yes">
<description>&lt;b&gt;SMB Connector&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SMBCONNECTOR"/>
</gates>
<devices>
<device name="" package="SMB_DIP">
<connects>
<connect gate="G$1" pin="ANT" pad="ANTENNA"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X13" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD13"/>
</gates>
<devices>
<device name="" package="1X13_ROUND_70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESDDIODEARRAY_SINGLE_UNIDIR" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;ESD Protection Diode Array - Single Channel Unidirectional&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;SOT23-3&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;NUP1301,215 - Ultra low capacitance (0.6pF), Rev Voltage 80V, Forward Current: 215mA - Digikey: 568-6351-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ESDDIODEARRAY_SINGLE_UNIDIR"/>
</gates>
<devices>
<device name="" package="SOT23-WIDE">
<connects>
<connect gate="G$1" pin="GNDPIN" pad="1"/>
<connect gate="G$1" pin="IO" pad="3"/>
<connect gate="G$1" pin="SUPPLYPIN" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VMOTOR">
<description>&lt;b&gt;VMOTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="VMOTOR"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERMBLOCK_1X3" prefix="J" uservalue="yes">
<description>3.5mm Terminal block
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="1X3"/>
</gates>
<devices>
<device name="" package="TERMBLOCK_1X3-3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPL115A2" prefix="U" uservalue="yes">
<description>&lt;b&gt;MPL115A2 I2C Barometric Pressure Sensor (50-115 kPa/7.25-16.68 PSI)&lt;/b&gt; - LGA8 Package
&lt;p&gt;Digikey: MPL115A2T1CT-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MPL115A2"/>
</gates>
<devices>
<device name="" package="LGA8">
<connects>
<connect gate="G$1" pin="CAP" pad="P$2"/>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="NC" pad="P$6"/>
<connect gate="G$1" pin="RST" pad="P$5"/>
<connect gate="G$1" pin="SCL" pad="P$8"/>
<connect gate="G$1" pin="SDA" pad="P$7"/>
<connect gate="G$1" pin="SHDN" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASBERRYPI_IDC" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Rasberry PI IDC Header&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="RASPBERRYPI_REV_B"/>
</gates>
<devices>
<device name="" package="RASBERRYPI_IDC">
<connects>
<connect gate="G$1" pin="#SPI_CE0" pad="24"/>
<connect gate="G$1" pin="#SPI_CE1" pad="26"/>
<connect gate="G$1" pin="3.3V@1" pad="1"/>
<connect gate="G$1" pin="5.0V@1" pad="2"/>
<connect gate="G$1" pin="DNC@1" pad="4"/>
<connect gate="G$1" pin="DNC@2" pad="9"/>
<connect gate="G$1" pin="DNC@3" pad="14"/>
<connect gate="G$1" pin="DNC@4" pad="17"/>
<connect gate="G$1" pin="DNC@5" pad="20"/>
<connect gate="G$1" pin="DNC@6" pad="25"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO0" pad="11"/>
<connect gate="G$1" pin="GPIO1" pad="12"/>
<connect gate="G$1" pin="GPIO2" pad="13"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="18"/>
<connect gate="G$1" pin="GPIO6" pad="22"/>
<connect gate="G$1" pin="GPIO7" pad="7"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL0" pad="5"/>
<connect gate="G$1" pin="SDA0" pad="3"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIOAMP_MAX98306" prefix="U" uservalue="yes">
<description>&lt;b&gt;MAX98306 3.7W Stereo Audio Amp&lt;/b&gt; - TDFN14
&lt;p&gt;3.7W @ 3 ohm, 2.6-5.5V supply, 6-18dB selectable gain&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX98306"/>
</gates>
<devices>
<device name="" package="TDFN14_3X3MM">
<connects>
<connect gate="G$1" pin="GAIN" pad="P$5"/>
<connect gate="G$1" pin="INL+" pad="P$3"/>
<connect gate="G$1" pin="INL-" pad="P$4"/>
<connect gate="G$1" pin="INR+" pad="P$7"/>
<connect gate="G$1" pin="INR-" pad="P$6"/>
<connect gate="G$1" pin="OUTL+" pad="P$13"/>
<connect gate="G$1" pin="OUTL-" pad="P$14"/>
<connect gate="G$1" pin="OUTR+" pad="P$10"/>
<connect gate="G$1" pin="OUTR-" pad="P$9"/>
<connect gate="G$1" pin="PGND@1" pad="P$1"/>
<connect gate="G$1" pin="PGND@2" pad="P$8"/>
<connect gate="G$1" pin="PVDD@1" pad="P$11"/>
<connect gate="G$1" pin="PVDD@2" pad="P$12"/>
<connect gate="G$1" pin="SHDN" pad="P$2"/>
<connect gate="G$1" pin="THERMAL" pad="P$THERMAL"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTC_DS1307" prefix="U" uservalue="yes">
<description>&lt;b&gt;DS1307 I2C RTC with 56-Bytes RAM&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DS1307"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW/OUT" pad="7"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EEPROM_I2C_SOIC8_GENERIC" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Note&lt;/b&gt;: The same pinout is used for many I2C EEPROMs in SOIC8(150mil) from a variety of manufacturers and in various sizes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Examples:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;16K (2K x 8 Bit) I2C EEPROM&lt;br/&gt;
1.7-5.5V, 400KHz, -40°C-85°C&lt;br/&gt;
Digikey: CAT24C16WI-GT3CT-ND&lt;/p&gt;

&lt;p&gt;256K (32K x 8 Bit) I2C EEPROM&lt;br/&gt;
1.7-5.5V, 400KHz, -40°C-85°C&lt;br/&gt;
Digikey: 24AA256-I/SN-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="EEPROM_SOIC8_24C"/>
</gates>
<devices>
<device name="" package="SOIC8_150MIL">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC11A14/QFN_LITERAL" prefix="U" uservalue="yes">
<description>&lt;b&gt;LPC11A14/QFN33&lt;/b&gt; - 50MHz ARM Cortex M0 with 32kb Flash, 8kb SRAM, 10-bit ADC and DAC, Temperature Sensor, Analog Comparator, and 4kb EEPROM
&lt;p&gt;Temp Range: -40°C - 85°C&lt;br/&gt;VDD: 2.6-3.6V&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LPC11A14_QFN33_LITERAL"/>
</gates>
<devices>
<device name="" package="HVQFN32">
<connects>
<connect gate="G$1" pin="PIO0_1/RXD/CLKOUT/CT32B0_MAT2/SSEL0/CLKIN" pad="3"/>
<connect gate="G$1" pin="PIO0_11/SCLK/AD5/CT32B1_MAT3/CT32B0_CAP0" pad="26"/>
<connect gate="G$1" pin="PIO0_12/RXD/ACMP_O/CT32B0_MAT0/SCL/CLKIN" pad="31"/>
<connect gate="G$1" pin="PIO0_13/TXD/ACMP_I2/CT32B0_MAT1/SDA" pad="32"/>
<connect gate="G$1" pin="PIO0_14/MISO1/AD6/CT32B0_CAP1/CT16B1_MAT1/VDDCMP" pad="20"/>
<connect gate="G$1" pin="PIO0_15/TXD/AD7/CT32B0_CAP2/SDA" pad="27"/>
<connect gate="G$1" pin="PIO0_16/ATRG0/ACMP_I3/CT16B0_CAP1/SCL" pad="13"/>
<connect gate="G$1" pin="PIO0_17/ATRG1/ACMP_I4/CT16B0_CAP2/CT16B0_MAT0" pad="14"/>
<connect gate="G$1" pin="PIO0_18/R/SSEL0/CT16B0_CAP0/CT16B1_CAP1" pad="8"/>
<connect gate="G$1" pin="PIO0_19/CLKIN/CLKOUT/MOSI0/CT16B1_MAT0" pad="9"/>
<connect gate="G$1" pin="PIO0_2/SCL/ACMP_O/TCK/SWCLK/CT16B0_CAP0" pad="10"/>
<connect gate="G$1" pin="PIO0_20/R/SCK0/CT32B1_CAP0/CT16B1_MAT2" pad="15"/>
<connect gate="G$1" pin="PIO0_21/CTS/ACMP_O/CT32B1_CAP1/SCLK" pad="16"/>
<connect gate="G$1" pin="PIO0_22/MISO0/ACMP_I5/CT32B1_MAT2/CT32B1_CAP2" pad="17"/>
<connect gate="G$1" pin="PIO0_23/RTS/ACMP_O/CT32B0_CAP0/SCLK" pad="30"/>
<connect gate="G$1" pin="PIO0_24/SCL/CLKIN/CT16B1_CAP0" pad="7"/>
<connect gate="G$1" pin="PIO0_25/SDA/SSEL1/CT16B1_MAT0" pad="12"/>
<connect gate="G$1" pin="PIO0_26/TXD/MISO1/CT16B1_CAP1/CT32B0_CAP2" pad="1"/>
<connect gate="G$1" pin="PIO0_27/MOSI1/ACMP_I1/CT32B1_MAT1/CT16B1_CAP2" pad="28"/>
<connect gate="G$1" pin="PIO0_3/SDA/ACMP_O/SWDIO/CT16B1_CAP0" pad="11"/>
<connect gate="G$1" pin="PIO0_4/R/AOUT/CT16B0_MAT1/MOSI0" pad="18"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="2"/>
<connect gate="G$1" pin="SWDIO/PIO0_10/AD4/CT32B1_MAT2/CT16B0_MAT2/RTS" pad="25"/>
<connect gate="G$1" pin="TCK/SWCLK/PIO0_5/R/CT16B0_MAT2/SCK0" pad="19"/>
<connect gate="G$1" pin="TDI/PIO0_6/AD0/CT32B0_MAT3/MISO0" pad="21"/>
<connect gate="G$1" pin="TDO/PIO0_8/AD2/CT32B1_MAT0/SCK1" pad="23"/>
<connect gate="G$1" pin="TMS/PIO0_7/AD1/CT32B1_CAP0/CT16B0_MAT0" pad="22"/>
<connect gate="G$1" pin="TRST/PIO0_9/AD3/CT32B1_MAT1/CT16B0_MAT1/CTS" pad="24"/>
<connect gate="G$1" pin="VDD(3V3)" pad="29"/>
<connect gate="G$1" pin="VDD(IO)" pad="6"/>
<connect gate="G$1" pin="VSS" pad="PAD"/>
<connect gate="G$1" pin="XTALIN" pad="4"/>
<connect gate="G$1" pin="XTALOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1053B" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;VS1053b Audio Codec - Ogg Vorbis/MP3/AAC/WMA/FLAC/MIDI&lt;/b&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VS1053B"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="AGND@0" pad="37"/>
<connect gate="G$1" pin="AGND@1" pad="40"/>
<connect gate="G$1" pin="AGND@2" pad="41"/>
<connect gate="G$1" pin="AGND@3" pad="47"/>
<connect gate="G$1" pin="AVDD@0" pad="38"/>
<connect gate="G$1" pin="AVDD@1" pad="43"/>
<connect gate="G$1" pin="AVDD@2" pad="45"/>
<connect gate="G$1" pin="CVDD@0" pad="5"/>
<connect gate="G$1" pin="CVDD@1" pad="7"/>
<connect gate="G$1" pin="CVDD@2" pad="24"/>
<connect gate="G$1" pin="CVDD@3" pad="31"/>
<connect gate="G$1" pin="DGND@0" pad="4"/>
<connect gate="G$1" pin="DGND@1" pad="16"/>
<connect gate="G$1" pin="DGND@2" pad="20"/>
<connect gate="G$1" pin="DGND@3" pad="21"/>
<connect gate="G$1" pin="DGND@4" pad="22"/>
<connect gate="G$1" pin="DREQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GND" pad="35"/>
<connect gate="G$1" pin="GPIO0" pad="33"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="GPIO4/I2S_LROUT" pad="36"/>
<connect gate="G$1" pin="GPIO5/I2S_MCLK" pad="25"/>
<connect gate="G$1" pin="GPIO6/I2S_SCLK" pad="11"/>
<connect gate="G$1" pin="GPIO7/I2S_SDATA" pad="12"/>
<connect gate="G$1" pin="IOVDD@0" pad="6"/>
<connect gate="G$1" pin="IOVDD@1" pad="14"/>
<connect gate="G$1" pin="IOVDD@2" pad="19"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="LINE2" pad="48"/>
<connect gate="G$1" pin="MIC_N" pad="2"/>
<connect gate="G$1" pin="MIC_P/LINEIN" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="VCO" pad="15"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTALIN" pad="18"/>
<connect gate="G$1" pin="XTALOUT" pad="17"/>
<connect gate="G$1" pin="XTEST" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER-1X15" prefix="JP" uservalue="yes">
<description>&lt;b&gt;1x15 Header&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD15"/>
</gates>
<devices>
<device name="" package="1X15_ROUND_70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMI-S-209-F" prefix="SHIELD">
<description>&lt;b&gt;SHIELD&lt;/b&gt;&lt;p&gt;
Surface Mount</description>
<gates>
<gate name="G$1" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="BMI-S-209-F">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESDDIODEARRAY_PRTR5V0U2F" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="LPC18XX-LIB_USBLC6-2"/>
</gates>
<devices>
<device name="" package="SOT886">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1_1" pad="1"/>
<connect gate="G$1" pin="I/O1_2" pad="6"/>
<connect gate="G$1" pin="I/O2_1" pad="3"/>
<connect gate="G$1" pin="I/O2_2" pad="4"/>
<connect gate="G$1" pin="VBUS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NTS0102" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;NTS0102&lt;/b&gt; - I2C Level Shifter&lt;/p&gt;
&lt;p&gt;The NTS0102 is a 2-bit, open-drain, dual supply translating transceiver with auto direction sensing, that enables bidirectional voltage level translation.&lt;/p&gt;

&lt;ul&gt;
&lt;li&gt;VCCA: 1.65-3.6V&lt;/li&gt;
&lt;li&gt;VCCB: 2.3V-5.5V&lt;/li&gt;
&lt;li&gt;Max Data Rate: 50 Mbps&lt;/li&gt;
&lt;li&gt;Temperature: -40°C - 125°C&lt;/li&gt;
&lt;/ul&gt;

&lt;ul&gt;
&lt;li&gt;XSON8 Package (NTS0102GT) - Mouser: 771-NTS0102GT115&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="NTS0102"/>
</gates>
<devices>
<device name="XSON8" package="SOT833-1">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="B1" pad="8"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OE" pad="6"/>
<connect gate="G$1" pin="VCCA" pad="3"/>
<connect gate="G$1" pin="VCCB" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF8001" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;nRF8001&lt;/b&gt; - Bluetooth Low-Energy Transceiver&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;VDD: 1.9-3.6V&lt;/li&gt;
&lt;li&gt;Temp: -40°C - 85°C&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="A" symbol="NRF8001"/>
<gate name="-SLUG" symbol="THERMAL-SLUG"/>
</gates>
<devices>
<device name="" package="QFN32_5MM">
<connects>
<connect gate="-SLUG" pin="TP" pad="33"/>
<connect gate="A" pin="ACTIVE" pad="6"/>
<connect gate="A" pin="ANT1" pad="21"/>
<connect gate="A" pin="ANT2" pad="22"/>
<connect gate="A" pin="AVDD@1" pad="24"/>
<connect gate="A" pin="AVDD@2" pad="26"/>
<connect gate="A" pin="AVDD@3" pad="29"/>
<connect gate="A" pin="DCC" pad="32"/>
<connect gate="A" pin="DEC1" pad="2"/>
<connect gate="A" pin="DEC2" pad="3"/>
<connect gate="A" pin="IREF" pad="25"/>
<connect gate="A" pin="MISO" pad="14"/>
<connect gate="A" pin="MOSI" pad="13"/>
<connect gate="A" pin="NC" pad="15"/>
<connect gate="A" pin="RDYN" pad="16"/>
<connect gate="A" pin="REQN" pad="12"/>
<connect gate="A" pin="RESET" pad="19"/>
<connect gate="A" pin="RXD" pad="10"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="TXD" pad="7"/>
<connect gate="A" pin="VDD@1" pad="1"/>
<connect gate="A" pin="VDD@2" pad="9"/>
<connect gate="A" pin="VDD_PA" pad="20"/>
<connect gate="A" pin="VSS@1" pad="8"/>
<connect gate="A" pin="VSS@2" pad="17"/>
<connect gate="A" pin="VSS@3" pad="18"/>
<connect gate="A" pin="VSS@4" pad="23"/>
<connect gate="A" pin="VSS@5" pad="30"/>
<connect gate="A" pin="VSS@6" pad="31"/>
<connect gate="A" pin="XC1" pad="28"/>
<connect gate="A" pin="XC2" pad="27"/>
<connect gate="A" pin="XL1" pad="5"/>
<connect gate="A" pin="XL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BALUN+LP_NORDIC" prefix="B" uservalue="yes">
<description>&lt;b&gt;Balun + Low Pass Filter&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;0603&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Johanson 2450BM14A0002 (nRF8001) - 2400-2500 MHz Balun + Filter&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="BALUN+LP_NORDIC"/>
</gates>
<devices>
<device name="" package="BALUN0603">
<connects>
<connect gate="G$1" pin="BAL1" pad="3"/>
<connect gate="G$1" pin="BAL2" pad="4"/>
<connect gate="G$1" pin="DC" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="UNBAL" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMC050" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;BMC050 - Electronic Compass (Three Axis Magnetic Field Sensor and Accelerometer)&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Support SPI and I2C interfaces&lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Acceleration Range: +/-2g,+/-4g, +/-8g, +/-16g,  &lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BMC050"/>
</gates>
<devices>
<device name="" package="BMC050">
<connects>
<connect gate="G$1" pin="CSB1" pad="5"/>
<connect gate="G$1" pin="CSB2" pad="6"/>
<connect gate="G$1" pin="DRDY" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="GND@3" pad="12"/>
<connect gate="G$1" pin="INT1" pad="16"/>
<connect gate="G$1" pin="INT2" pad="1"/>
<connect gate="G$1" pin="INT3" pad="4"/>
<connect gate="G$1" pin="PS1" pad="2"/>
<connect gate="G$1" pin="PS2" pad="3"/>
<connect gate="G$1" pin="SCK/SCL" pad="15"/>
<connect gate="G$1" pin="SDI/SDA" pad="11"/>
<connect gate="G$1" pin="SDO/ADDR" pad="10"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VDDIO" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EXT" package="BMC050_EXTENDED">
<connects>
<connect gate="G$1" pin="CSB1" pad="5"/>
<connect gate="G$1" pin="CSB2" pad="6"/>
<connect gate="G$1" pin="DRDY" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="GND@3" pad="12"/>
<connect gate="G$1" pin="INT1" pad="16"/>
<connect gate="G$1" pin="INT2" pad="1"/>
<connect gate="G$1" pin="INT3" pad="4"/>
<connect gate="G$1" pin="PS1" pad="2"/>
<connect gate="G$1" pin="PS2" pad="3"/>
<connect gate="G$1" pin="SCK/SCL" pad="15"/>
<connect gate="G$1" pin="SDI/SDA" pad="11"/>
<connect gate="G$1" pin="SDO/ADDR" pad="10"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VDDIO" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VDDIO">
<gates>
<gate name="G$1" symbol="VDDIO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMI-S-202-F" prefix="SHIELD">
<description>&lt;b&gt;SHIELD&lt;/b&gt;&lt;p&gt;
Surface Mount</description>
<gates>
<gate name="G$1" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="BMI-S-202-F">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPXV7025DP" prefix="U" uservalue="yes">
<description>&lt;b&gt;PRESSURE SENSOR&lt;/b&gt; - Differential Input, Single-Ended Output</description>
<gates>
<gate name="G$1" symbol="PSENSE-DPD"/>
</gates>
<devices>
<device name="" package="SOP8-1351">
<connects>
<connect gate="G$1" pin="+VOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPXV7025GP" prefix="U" uservalue="yes">
<description>&lt;b&gt;PRESSURE SENSOR&lt;/b&gt; -Single Port</description>
<gates>
<gate name="G$1" symbol="PSENSE-SP"/>
</gates>
<devices>
<device name="" package="SOP8-1369">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACCEL_LIS3DHTR" prefix="U" uservalue="yes">
<description>&lt;b&gt;LIS3DHTR 3-Axis Accelerometer with I2C/SPI Interface&lt;/b&gt;

&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;VDD&lt;/b&gt;: 1.71-3.6V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;VDDIO&lt;/b&gt;: 1.71-VDD+0.1V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Scale&lt;/b&gt;: +/-2g, 4g, 8g, 16g with 16--bit data output&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Temp:&lt;/b&gt;: -40°C - 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;Mouser: 511-LIS3DHTR&lt;br/&gt;Digikey: 497-10613-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LIS3DHTR"/>
</gates>
<devices>
<device name="" package="LGA16_3X3MM">
<connects>
<connect gate="G$1" pin="ADC1" pad="16"/>
<connect gate="G$1" pin="ADC2" pad="15"/>
<connect gate="G$1" pin="ADC3" pad="13"/>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="RES(GND)" pad="10"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="SDO" pad="7"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STMPE610" prefix="U" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;STMPE610 - 12-Bit Touch Screen Controller&lt;/b&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="STMPE610"/>
</gates>
<devices>
<device name="" package="QFN16_3MM">
<connects>
<connect gate="G$1" pin="A0/MISO" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$10"/>
<connect gate="G$1" pin="IN2/GPIO2" pad="P$11"/>
<connect gate="G$1" pin="IN3/GPIO3" pad="P$12"/>
<connect gate="G$1" pin="INT" pad="P$2"/>
<connect gate="G$1" pin="MODE" pad="P$9"/>
<connect gate="G$1" pin="MOSI" pad="P$7"/>
<connect gate="G$1" pin="NC" pad="P$8"/>
<connect gate="G$1" pin="SCLK" pad="P$4"/>
<connect gate="G$1" pin="SDA/CS" pad="P$5"/>
<connect gate="G$1" pin="VCC" pad="P$6"/>
<connect gate="G$1" pin="VIO" pad="P$14"/>
<connect gate="G$1" pin="X+" pad="P$13"/>
<connect gate="G$1" pin="X-" pad="P$16"/>
<connect gate="G$1" pin="Y+" pad="P$15"/>
<connect gate="G$1" pin="Y-" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDCARD_PCBCARRIER">
<description>&lt;p&gt;Physical PCB representing an SD Card&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SDCARD_PCBCARRIER"/>
</gates>
<devices>
<device name="DIMEN" package="SDCARD_PCBCARRIER_DIM">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="P$1"/>
<connect gate="G$1" pin="CLK" pad="P$5"/>
<connect gate="G$1" pin="CMD" pad="P$2"/>
<connect gate="G$1" pin="DAT0" pad="P$7"/>
<connect gate="G$1" pin="DAT1" pad="P$8"/>
<connect gate="G$1" pin="DAT2" pad="P$9"/>
<connect gate="G$1" pin="VDD" pad="P$4"/>
<connect gate="G$1" pin="VSS@1" pad="P$3"/>
<connect gate="G$1" pin="VSS@2" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TDOCU" package="SDCARD_PCBCARRIER_DOCU">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="P$1"/>
<connect gate="G$1" pin="CLK" pad="P$5"/>
<connect gate="G$1" pin="CMD" pad="P$2"/>
<connect gate="G$1" pin="DAT0" pad="P$7"/>
<connect gate="G$1" pin="DAT1" pad="P$8"/>
<connect gate="G$1" pin="DAT2" pad="P$9"/>
<connect gate="G$1" pin="VDD" pad="P$4"/>
<connect gate="G$1" pin="VSS@1" pad="P$3"/>
<connect gate="G$1" pin="VSS@2" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
