<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;b&gt;National Semiconductor&lt;/b&gt;&lt;p&gt;
http://www.national.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MSO28W">
<description>&lt;B&gt;Molded SO Wide Body Package (WM)&lt;/b&gt;&lt;p&gt;
See NS Package Number M28B&lt;br&gt;
Source: http://www.national.com .. USBN9603.pdf</description>
</package>
<package name="LSB28">
<description>&lt;b&gt;Laminate Substrate Based Package&lt;/b&gt;&lt;p&gt;
See NS Package Number SLB28AA&lt;br&gt;
Source: http://www.national.com .. USBN9603.pdf</description>
</package>
<package name="TO-220-11">
<description>&lt;b&gt;11-Lead TO-220 Power Package (T)&lt;/b&gt; NS Package Number TA11B&lt;p&gt;
Source: http://cache.national.com/ds/LM/LMD18200.pdf</description>
</package>
<package name="LQA036D">
<description>&lt;b&gt;NS LLP Package Number LQA036D&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LMX2531LQ1515E.pdf?</description>
</package>
<package name="LQA036A">
<description>&lt;b&gt;NS Package Number LQA036A&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LMX2531LQ1515E.pdf?</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;14-Lead Exposed Pad Package&lt;/b&gt; NS Package Number MXA14A&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM5015.pdf</description>
</package>
<package name="LQFP48">
<description>&lt;b&gt;LQFP48&lt;/b&gt; VXH48A&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: http://www.national.com/ds/DP/DP83848VYB.pdf</description>
</package>
<package name="T05A">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
5 lead, National Semiconductor T05A&lt;br&gt;
Motorola 314D-01</description>
</package>
<package name="T05D">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
5 lead, National Semiconductor T05D</description>
</package>
<package name="TO263-5">
<description>&lt;b&gt;TO-263&lt;/b&gt;</description>
</package>
<package name="WG10A">
<description>&lt;b&gt;NS Package Number WG10A&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/ds/LP/LP2950.pdf</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="H08C">
<description>&lt;b&gt;TO-99&lt;/b&gt;&lt;p&gt;
National Semiconductor H08C&lt;br&gt;
Motorola MOT 601-04</description>
</package>
<package name="LLP8">
<description>&lt;b&gt;LLP Package NS Package Number SDC08A&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LP/LP2950.pdf</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="LLP6">
</package>
</packages>
<symbols>
<symbol name="USBN9603">
<pin name="!CS" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="A0/ALE" direction="in"/>
<pin name="D0/AD0" direction="in"/>
<pin name="D1/AD1" direction="in"/>
<pin name="D2/AD2" direction="in"/>
<pin name="D3/AD3" direction="in"/>
<pin name="D4/AD4" direction="in"/>
<pin name="D5/AD5" direction="in"/>
<pin name="D6/AD6" direction="in"/>
<pin name="D7/AD7" direction="in"/>
<pin name="INTR" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="CLKOUT" direction="out"/>
<pin name="V3.3" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="MODE1" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="DRQ" direction="in"/>
<pin name="!DACK" direction="in"/>
</symbol>
<symbol name="LM18200">
<pin name="BOOTSTRAP1" direction="in"/>
<pin name="BOOTSTRAP2" direction="in"/>
<pin name="OUTPUT1" direction="out"/>
<pin name="OUTPUT2" direction="out"/>
<pin name="DIRECTION" direction="in"/>
<pin name="BREAK" direction="in"/>
<pin name="PWM" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SENSE" direction="out"/>
<pin name="THERMAL" direction="out"/>
</symbol>
<symbol name="LMX2531LQ-D">
<pin name="VCCDIG" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="VREGBUF" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="VCCVCO" direction="in"/>
<pin name="VREGVCO" direction="pas"/>
<pin name="VREFVCO" direction="pas"/>
<pin name="FOUT" direction="out"/>
<pin name="VCCBUF" direction="in"/>
<pin name="VTUNE" direction="in"/>
<pin name="CPOUT" direction="out"/>
<pin name="FLOUT" direction="out"/>
<pin name="VREGPLL1" direction="pas"/>
<pin name="VCCPLL" direction="in"/>
<pin name="VREGPLL2" direction="pas"/>
<pin name="FTEST/LD" direction="out"/>
<pin name="OSCIN" direction="in"/>
<pin name="OSCIN*" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="VREGDIG" direction="in"/>
<pin name="NC@11" direction="nc"/>
<pin name="GND@5" direction="pwr"/>
</symbol>
<symbol name="LMX2531LQ-A">
<pin name="VCCDIG" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="VREGBUF" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="VCCVCO" direction="in"/>
<pin name="VREGVCO" direction="pas"/>
<pin name="VREFVCO" direction="pas"/>
<pin name="FOUT" direction="out"/>
<pin name="VCCBUF" direction="in"/>
<pin name="VTUNE" direction="in"/>
<pin name="CPOUT" direction="out"/>
<pin name="FLOUT" direction="out"/>
<pin name="VREGPLL1" direction="pas"/>
<pin name="VCCPLL" direction="in"/>
<pin name="VREGPLL2" direction="pas"/>
<pin name="FTEST/LD" direction="out"/>
<pin name="OSCIN" direction="in"/>
<pin name="OSCIN*" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="VREGDIG" direction="in"/>
<pin name="NC@11" direction="nc"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
</symbol>
<symbol name="LM5015">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="CFB" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="RT" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="PVIN" direction="in"/>
<pin name="HO" direction="out"/>
<pin name="BST" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="COMP" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="DP83848">
<pin name="CLK2MAC"/>
<pin name="LED_ACTCOL"/>
<pin name="LED_SPD"/>
<pin name="LED_LNK"/>
<pin name="RESET_N" direction="in"/>
<pin name="MDIO"/>
<pin name="MDC" direction="in"/>
<pin name="IO_VDD2" direction="pwr"/>
<pin name="X2" direction="out"/>
<pin name="X1" direction="in"/>
<pin name="IO_VSS2" direction="pwr"/>
<pin name="CORE_VSS" direction="pwr"/>
<pin name="CORE_VDD" direction="pwr"/>
<pin name="RX_CLK"/>
<pin name="RX_DV"/>
<pin name="CRS"/>
<pin name="RX_ER"/>
<pin name="COL"/>
<pin name="RXD_0"/>
<pin name="RXD_1"/>
<pin name="RXD_2"/>
<pin name="RXD_3"/>
<pin name="IO_VSS1" direction="pwr"/>
<pin name="IO_VDD1" direction="pwr"/>
<pin name="TX_CLK"/>
<pin name="TX_EN"/>
<pin name="TXD_0"/>
<pin name="TXD_1"/>
<pin name="TXD_2"/>
<pin name="TXD_3"/>
<pin name="PWRDN_INTN"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRST_N" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TPRDM"/>
<pin name="TPRDP"/>
<pin name="CDVSS" direction="pwr"/>
<pin name="TPTDM"/>
<pin name="TPTDP"/>
<pin name="ANA18VDD" direction="pwr"/>
<pin name="ANA18VSS" direction="pwr"/>
<pin name="IP_PH_M" direction="in"/>
<pin name="IP_PH_P" direction="in"/>
<pin name="ANA33VDD" direction="pwr"/>
<pin name="REG_OUT" direction="out"/>
<pin name="VREF"/>
</symbol>
<symbol name="LM2596">
<pin name="VIN" direction="in"/>
<pin name="!ON!/OFF" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="FB" direction="in"/>
</symbol>
<symbol name="LP2950">
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="LP2951WG">
<pin name="VIN" direction="in"/>
<pin name="SHDWN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="!ERROR" direction="out"/>
<pin name="VTAB" direction="in"/>
</symbol>
<symbol name="LMX2322">
<pin name="OSCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VP" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CPO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="XFIN" direction="in"/>
<pin name="FIN" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="LM2735">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="SW"/>
<pin name="FB"/>
</symbol>
<symbol name="LP38692">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="VOUT"/>
<pin name="SNS"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="USBN960*" prefix="IC">
<description>&lt;b&gt;USBN9603/USBN9604 Universal Serial Bus&lt;/b&gt; Full Speed Node Controller with Enhanced DMA Support&lt;p&gt;
Source: http://www.national.com .. USBN9603.pdf</description>
<gates>
<gate name="G$1" symbol="USBN9603"/>
</gates>
<devices>
<device name="-28M" package="MSO28W">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!DACK" pad="6"/>
<connect gate="G$1" pin="!RD" pad="2"/>
<connect gate="G$1" pin="!RESET" pad="16"/>
<connect gate="G$1" pin="!WR" pad="3"/>
<connect gate="G$1" pin="A0/ALE" pad="7"/>
<connect gate="G$1" pin="AGND" pad="17"/>
<connect gate="G$1" pin="CLKOUT" pad="28"/>
<connect gate="G$1" pin="D+" pad="19"/>
<connect gate="G$1" pin="D-" pad="20"/>
<connect gate="G$1" pin="D0/AD0" pad="8"/>
<connect gate="G$1" pin="D1/AD1" pad="9"/>
<connect gate="G$1" pin="D2/AD2" pad="10"/>
<connect gate="G$1" pin="D3/AD3" pad="11"/>
<connect gate="G$1" pin="D4/AD4" pad="12"/>
<connect gate="G$1" pin="D5/AD5" pad="13"/>
<connect gate="G$1" pin="D6/AD6" pad="14"/>
<connect gate="G$1" pin="D7/AD7" pad="15"/>
<connect gate="G$1" pin="DRQ" pad="5"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="23"/>
<connect gate="G$1" pin="INTR" pad="4"/>
<connect gate="G$1" pin="MODE0" pad="25"/>
<connect gate="G$1" pin="MODE1" pad="24"/>
<connect gate="G$1" pin="V3.3" pad="18"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="XIN" pad="26"/>
<connect gate="G$1" pin="XOUT" pad="27"/>
</connects>
<technologies>
<technology name="3"/>
<technology name="4"/>
</technologies>
</device>
<device name="SLB" package="LSB28">
<connects>
<connect gate="G$1" pin="!CS" pad="19"/>
<connect gate="G$1" pin="!DACK" pad="24"/>
<connect gate="G$1" pin="!RD" pad="20"/>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="!WR" pad="21"/>
<connect gate="G$1" pin="A0/ALE" pad="25"/>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="CLKOUT" pad="18"/>
<connect gate="G$1" pin="D+" pad="9"/>
<connect gate="G$1" pin="D-" pad="10"/>
<connect gate="G$1" pin="D0/AD0" pad="26"/>
<connect gate="G$1" pin="D1/AD1" pad="27"/>
<connect gate="G$1" pin="D2/AD2" pad="28"/>
<connect gate="G$1" pin="D3/AD3" pad="1"/>
<connect gate="G$1" pin="D4/AD4" pad="2"/>
<connect gate="G$1" pin="D5/AD5" pad="3"/>
<connect gate="G$1" pin="D6/AD6" pad="4"/>
<connect gate="G$1" pin="D7/AD7" pad="5"/>
<connect gate="G$1" pin="DRQ" pad="23"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="INTR" pad="22"/>
<connect gate="G$1" pin="MODE0" pad="15"/>
<connect gate="G$1" pin="MODE1" pad="14"/>
<connect gate="G$1" pin="V3.3" pad="8"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="XIN" pad="16"/>
<connect gate="G$1" pin="XOUT" pad="17"/>
</connects>
<technologies>
<technology name="3"/>
<technology name="4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM18200T" prefix="IC">
<description>&lt;b&gt;3A, 55V H-Bridge Motor Control&lt;/b&gt;&lt;p&gt;
SourcE: http://cache.national.com/ds/LM/LMD18200.pdf</description>
<gates>
<gate name="G$1" symbol="LM18200"/>
</gates>
<devices>
<device name="" package="TO-220-11">
<connects>
<connect gate="G$1" pin="BOOTSTRAP1" pad="1"/>
<connect gate="G$1" pin="BOOTSTRAP2" pad="11"/>
<connect gate="G$1" pin="BREAK" pad="4"/>
<connect gate="G$1" pin="DIRECTION" pad="3"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUTPUT1" pad="2"/>
<connect gate="G$1" pin="OUTPUT2" pad="10"/>
<connect gate="G$1" pin="PWM" pad="5"/>
<connect gate="G$1" pin="SENSE" pad="8"/>
<connect gate="G$1" pin="THERMAL" pad="9"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMX2531LQ-D" prefix="IC">
<description>&lt;b&gt;High Performance Frequency Synthesizer System with Integrated VCO&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LMX2531LQ1515E.pdf?</description>
<gates>
<gate name="G$1" symbol="LMX2531LQ-D"/>
</gates>
<devices>
<device name="" package="LQA036D">
<connects>
<connect gate="G$1" pin="CE" pad="11"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="CPOUT" pad="24"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="FLOUT" pad="25"/>
<connect gate="G$1" pin="FOUT" pad="21"/>
<connect gate="G$1" pin="FTEST/LD" pad="30"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="GND@4" pad="34"/>
<connect gate="G$1" pin="GND@5" pad="38"/>
<connect gate="G$1" pin="LE" pad="10"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@10" pad="35"/>
<connect gate="G$1" pin="NC@11" pad="37"/>
<connect gate="G$1" pin="NC@2" pad="4"/>
<connect gate="G$1" pin="NC@3" pad="5"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="NC@5" pad="12"/>
<connect gate="G$1" pin="NC@6" pad="13"/>
<connect gate="G$1" pin="NC@7" pad="14"/>
<connect gate="G$1" pin="NC@8" pad="15"/>
<connect gate="G$1" pin="NC@9" pad="29"/>
<connect gate="G$1" pin="OSCIN" pad="31"/>
<connect gate="G$1" pin="OSCIN*" pad="32"/>
<connect gate="G$1" pin="TEST" pad="33"/>
<connect gate="G$1" pin="VCCBUF" pad="22"/>
<connect gate="G$1" pin="VCCDIG" pad="1"/>
<connect gate="G$1" pin="VCCPLL" pad="27"/>
<connect gate="G$1" pin="VCCVCO" pad="16"/>
<connect gate="G$1" pin="VREFVCO" pad="18"/>
<connect gate="G$1" pin="VREGBUF" pad="6"/>
<connect gate="G$1" pin="VREGDIG" pad="36"/>
<connect gate="G$1" pin="VREGPLL1" pad="26"/>
<connect gate="G$1" pin="VREGPLL2" pad="28"/>
<connect gate="G$1" pin="VREGVCO" pad="17"/>
<connect gate="G$1" pin="VTUNE" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMX2531LQ-A" prefix="IC">
<description>&lt;b&gt;High Performance Frequency Synthesizer System with Integrated VCO&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LMX2531LQ1515E.pdf?</description>
<gates>
<gate name="G$1" symbol="LMX2531LQ-A"/>
</gates>
<devices>
<device name="" package="LQA036A">
<connects>
<connect gate="G$1" pin="CE" pad="11"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="CPOUT" pad="24"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="FLOUT" pad="25"/>
<connect gate="G$1" pin="FOUT" pad="21"/>
<connect gate="G$1" pin="FTEST/LD" pad="30"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="GND@4" pad="34"/>
<connect gate="G$1" pin="GND@5" pad="38"/>
<connect gate="G$1" pin="GND@6" pad="39"/>
<connect gate="G$1" pin="LE" pad="10"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@10" pad="35"/>
<connect gate="G$1" pin="NC@11" pad="37"/>
<connect gate="G$1" pin="NC@2" pad="4"/>
<connect gate="G$1" pin="NC@3" pad="5"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="NC@5" pad="12"/>
<connect gate="G$1" pin="NC@6" pad="13"/>
<connect gate="G$1" pin="NC@7" pad="14"/>
<connect gate="G$1" pin="NC@8" pad="15"/>
<connect gate="G$1" pin="NC@9" pad="29"/>
<connect gate="G$1" pin="OSCIN" pad="31"/>
<connect gate="G$1" pin="OSCIN*" pad="32"/>
<connect gate="G$1" pin="TEST" pad="33"/>
<connect gate="G$1" pin="VCCBUF" pad="22"/>
<connect gate="G$1" pin="VCCDIG" pad="1"/>
<connect gate="G$1" pin="VCCPLL" pad="27"/>
<connect gate="G$1" pin="VCCVCO" pad="16"/>
<connect gate="G$1" pin="VREFVCO" pad="18"/>
<connect gate="G$1" pin="VREGBUF" pad="6"/>
<connect gate="G$1" pin="VREGDIG" pad="36"/>
<connect gate="G$1" pin="VREGPLL1" pad="26"/>
<connect gate="G$1" pin="VREGPLL2" pad="28"/>
<connect gate="G$1" pin="VREGVCO" pad="17"/>
<connect gate="G$1" pin="VTUNE" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5015" prefix="IC">
<description>&lt;b&gt;High Voltage Monolithic Two-Switch Forward DC-DC Regulator&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM5015.pdf</description>
<gates>
<gate name="G$1" symbol="LM5015"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="BST" pad="10"/>
<connect gate="G$1" pin="CFB" pad="5"/>
<connect gate="G$1" pin="COMP" pad="4"/>
<connect gate="G$1" pin="EN" pad="13"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="HO" pad="9"/>
<connect gate="G$1" pin="LO" pad="7"/>
<connect gate="G$1" pin="PGND" pad="6"/>
<connect gate="G$1" pin="PVIN" pad="8"/>
<connect gate="G$1" pin="RT" pad="2"/>
<connect gate="G$1" pin="SS" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VIN" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DP83848" prefix="IC">
<description>&lt;b&gt;PHYTER® - Extended Temperature Single Port 10/100 Mb/s Ethernet Physical Layer Transceiver&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: dp83848yb.bsdl&lt;br&gt;
http://www.national.com/ds/DP/DP83848VYB.pdf</description>
<gates>
<gate name="G$1" symbol="DP83848"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="ANA18VDD" pad="18"/>
<connect gate="G$1" pin="ANA18VSS" pad="19"/>
<connect gate="G$1" pin="ANA33VDD" pad="22"/>
<connect gate="G$1" pin="CDVSS" pad="15"/>
<connect gate="G$1" pin="CLK2MAC" pad="25"/>
<connect gate="G$1" pin="COL" pad="42"/>
<connect gate="G$1" pin="CORE_VDD" pad="37"/>
<connect gate="G$1" pin="CORE_VSS" pad="36"/>
<connect gate="G$1" pin="CRS" pad="40"/>
<connect gate="G$1" pin="IO_VDD1" pad="48"/>
<connect gate="G$1" pin="IO_VDD2" pad="32"/>
<connect gate="G$1" pin="IO_VSS1" pad="47"/>
<connect gate="G$1" pin="IO_VSS2" pad="35"/>
<connect gate="G$1" pin="IP_PH_M" pad="20"/>
<connect gate="G$1" pin="IP_PH_P" pad="21"/>
<connect gate="G$1" pin="LED_ACTCOL" pad="26"/>
<connect gate="G$1" pin="LED_LNK" pad="28"/>
<connect gate="G$1" pin="LED_SPD" pad="27"/>
<connect gate="G$1" pin="MDC" pad="31"/>
<connect gate="G$1" pin="MDIO" pad="30"/>
<connect gate="G$1" pin="PWRDN_INTN" pad="7"/>
<connect gate="G$1" pin="REG_OUT" pad="23"/>
<connect gate="G$1" pin="RESET_N" pad="29"/>
<connect gate="G$1" pin="RXD_0" pad="43"/>
<connect gate="G$1" pin="RXD_1" pad="44"/>
<connect gate="G$1" pin="RXD_2" pad="45"/>
<connect gate="G$1" pin="RXD_3" pad="46"/>
<connect gate="G$1" pin="RX_CLK" pad="38"/>
<connect gate="G$1" pin="RX_DV" pad="39"/>
<connect gate="G$1" pin="RX_ER" pad="41"/>
<connect gate="G$1" pin="TCK" pad="8"/>
<connect gate="G$1" pin="TDI" pad="12"/>
<connect gate="G$1" pin="TDO" pad="9"/>
<connect gate="G$1" pin="TMS" pad="10"/>
<connect gate="G$1" pin="TPRDM" pad="13"/>
<connect gate="G$1" pin="TPRDP" pad="14"/>
<connect gate="G$1" pin="TPTDM" pad="16"/>
<connect gate="G$1" pin="TPTDP" pad="17"/>
<connect gate="G$1" pin="TRST_N" pad="11"/>
<connect gate="G$1" pin="TXD_0" pad="3"/>
<connect gate="G$1" pin="TXD_1" pad="4"/>
<connect gate="G$1" pin="TXD_2" pad="5"/>
<connect gate="G$1" pin="TXD_3" pad="6"/>
<connect gate="G$1" pin="TX_CLK" pad="1"/>
<connect gate="G$1" pin="TX_EN" pad="2"/>
<connect gate="G$1" pin="VREF" pad="24"/>
<connect gate="G$1" pin="X1" pad="34"/>
<connect gate="G$1" pin="X2" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596" prefix="IC">
<description>&lt;b&gt;SIMPLE SWITCHER® Power Converter 150 kHz 3A Step-Down Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/ds/LM/LM2596.pdf</description>
<gates>
<gate name="G$1" symbol="LM2596"/>
</gates>
<devices>
<device name="T" package="T05D">
<connects>
<connect gate="G$1" pin="!ON!/OFF" pad="5"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="TO263-5">
<connects>
<connect gate="G$1" pin="!ON!/OFF" pad="5"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951" prefix="IC">
<description>&lt;b&gt;Adjustable Micropower Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/ds/LP/LP2950.pdf</description>
<gates>
<gate name="G$1" symbol="LP2951WG"/>
</gates>
<devices>
<device name="WG" package="WG10A">
<connects>
<connect gate="G$1" pin="!ERROR" pad="7"/>
<connect gate="G$1" pin="FB" pad="9"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDWN" pad="3"/>
<connect gate="G$1" pin="VIN" pad="10"/>
<connect gate="G$1" pin="VTAB" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SO08">
<connects>
<connect gate="G$1" pin="!ERROR" pad="5"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDWN" pad="3"/>
<connect gate="G$1" pin="VIN" pad="8"/>
<connect gate="G$1" pin="VTAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="!ERROR" pad="5"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDWN" pad="3"/>
<connect gate="G$1" pin="VIN" pad="8"/>
<connect gate="G$1" pin="VTAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="H08C">
<connects>
<connect gate="G$1" pin="!ERROR" pad="5"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDWN" pad="3"/>
<connect gate="G$1" pin="VIN" pad="8"/>
<connect gate="G$1" pin="VTAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="LLP8">
<connects>
<connect gate="G$1" pin="!ERROR" pad="5"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDWN" pad="3"/>
<connect gate="G$1" pin="VIN" pad="8"/>
<connect gate="G$1" pin="VTAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2950" prefix="IC">
<description>&lt;b&gt;Adjustable Micropower Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/ds/LP/LP2950.pdf</description>
<gates>
<gate name="G$1" symbol="LP2950"/>
</gates>
<devices>
<device name="Z" package="TO92">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="O" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="TO252">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="O" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMX2322" prefix="IC">
<description>&lt;b&gt;PLLatinumTM 2.0 GHz Frequency Synthesizer for RF Personal Communications&lt;/b&gt;&lt;p&gt;

Source: LMX2322.pdf</description>
<gates>
<gate name="G$1" symbol="LMX2322"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="CE" pad="12"/>
<connect gate="G$1" pin="CLOCK" pad="9"/>
<connect gate="G$1" pin="CPO" pad="5"/>
<connect gate="G$1" pin="DATA" pad="10"/>
<connect gate="G$1" pin="FIN" pad="8"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LE" pad="11"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="NC@3" pad="15"/>
<connect gate="G$1" pin="NC@4" pad="16"/>
<connect gate="G$1" pin="OSCIN" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VP" pad="3"/>
<connect gate="G$1" pin="XFIN" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2735" prefix="U">
<gates>
<gate name="G$1" symbol="LM2735"/>
</gates>
<devices>
<device name="" package="LLP6">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="1 5 PAD"/>
<connect gate="G$1" pin="SW" pad="6"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38692" prefix="U">
<gates>
<gate name="G$1" symbol="LP38692"/>
</gates>
<devices>
<device name="" package="LLP6">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2 PAD"/>
<connect gate="G$1" pin="SNS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1 6"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
