<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<library>
<description>&lt;b&gt;ON Semiconductor&lt;/b&gt;&lt;p&gt;
&lt;a href="http://onsemi.com"&gt; Home page &lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="MICRO8">
<description>&lt;b&gt;Micro8&lt;/b&gt; CASE 846A-02&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF</description>
</package>
<package name="SOIC8">
<description>&lt;b&gt;SOIC-8&lt;/b&gt; CASE 751-07&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF&lt;p&gt;
&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;PLATIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
<package name="TO263_5">
<description>&lt;b&gt;TO-263 5-LEAD (TV)&lt;/b&gt;&lt;p&gt;
Source: ON Semiconductor .. 4101.pdf</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23 (TO-236) CASE 318-08 ISSUE AN&lt;/b&gt;&lt;p&gt;
Source: U6 OnSemi Inductive Load Driver MDC3105-D.PDF</description>
</package>
<package name="SC-74">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt; SC-74 CASE 318F-05 ISSUE M&lt;p&gt;
Source: U6 OnSemi Inductive Load Driver MDC3105-D.PDF</description>
</package>
<package name="SOT-563">
<description>&lt;b&gt;SOT-563, 6 LEAD CASE 463A-01 ISSUE F&lt;/b&gt;&lt;p&gt;
Source: U6 OnSemi Inductive Load Driver MDC3105-D.PDF</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="LQFP32-7X7MM">
<description>&lt;b&gt;LQFP 32 7 x 7 mm&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source:OnSemi A5191HRT HART Modem Data Sheet.pdf</description>
</package>
<package name="UDFN8-EP">
</package>
<package name="A5191HRTI">
<description>&lt;b&gt;&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="FLIP-CHIP9">
<description>&lt;b&gt;9 PIN FLIP?CHIP&lt;/b&gt; CASE 499AL?01 ISSUE O&lt;p&gt;
BGA 9 pol.&lt;br&gt;
Source: &lt;a href = "http://www.farnell.com/datasheets/72510.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="UDFN8">
</package>
</packages>
<symbols>
<symbol name="MC34161">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT1" direction="oc"/>
<pin name="OUT2" direction="oc"/>
<pin name="VREF" direction="out"/>
<pin name="MODE" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
</symbol>
<symbol name="CAT4101">
<pin name="EN/PWM" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="LED" direction="pwr"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="MC12052A">
<pin name="IN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="SW" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="MC" direction="in"/>
<pin name="!IN" direction="in"/>
</symbol>
<symbol name="MC12080">
<pin name="IN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="SW1" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SW2" direction="in"/>
<pin name="!IN" direction="in"/>
<pin name="SW3" direction="in"/>
</symbol>
<symbol name="NPN-DRIVER">
<pin name="VIN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="pas"/>
</symbol>
<symbol name="NPN-DRIVER_4C">
<pin name="VIN" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="pas"/>
<pin name="VOUT1" direction="pas"/>
<pin name="VOUT2" direction="pas"/>
<pin name="VOUT3" direction="pas"/>
</symbol>
<symbol name="A5191HRT">
<pin name="TEST1" direction="in"/>
<pin name="TEST2" direction="nc"/>
<pin name="TEST3" direction="nc"/>
<pin name="TEST4" direction="nc"/>
<pin name="TEST5" direction="in"/>
<pin name="INRESET" direction="in"/>
<pin name="TEST7" direction="in"/>
<pin name="TEST8" direction="in"/>
<pin name="TEST9" direction="in"/>
<pin name="OTXA" direction="out"/>
<pin name="IAREF" direction="in"/>
<pin name="ICDREF" direction="in"/>
<pin name="OCBIAS" direction="out"/>
<pin name="TEST10" direction="in"/>
<pin name="VDDA" direction="pwr"/>
<pin name="IRXA" direction="in"/>
<pin name="ORXAF" direction="out"/>
<pin name="IRXAC" direction="in"/>
<pin name="OXTL" direction="out"/>
<pin name="IXTL" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INRTS" direction="in"/>
<pin name="ITXD" direction="in"/>
<pin name="TEST11" direction="nc"/>
<pin name="ORXD" direction="out"/>
<pin name="OCD" direction="out"/>
<pin name="TEST12" direction="nc"/>
</symbol>
<symbol name="A5191HRTI">
<pin name="TEST5" direction="in"/>
<pin name="INRESET" direction="in"/>
<pin name="TEST7" direction="in"/>
<pin name="TEST8" direction="in"/>
<pin name="TEST9" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="OTXA" direction="out"/>
<pin name="IAREF" direction="in"/>
<pin name="ICDREF" direction="in"/>
<pin name="OCBIAS" direction="out"/>
<pin name="TEST10" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="IRXA" direction="in"/>
<pin name="ORXAF" direction="out"/>
<pin name="IRXAC" direction="in"/>
<pin name="OXTL" direction="out"/>
<pin name="IXTL" direction="in"/>
<pin name="VSSA@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="INRTS" direction="in"/>
<pin name="ITXD" direction="in"/>
<pin name="TEST11" direction="nc"/>
<pin name="ORXD" direction="out"/>
<pin name="OCD" direction="out"/>
<pin name="TEST12" direction="nc"/>
<pin name="TEST1" direction="in"/>
<pin name="TEST2" direction="nc"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="TEST3" direction="nc"/>
<pin name="TEST4" direction="nc"/>
</symbol>
<symbol name="NCP2820">
<pin name="INP" direction="in"/>
<pin name="INM" direction="in"/>
<pin name="!SD" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="OUTM" direction="out"/>
<pin name="OUTP" direction="out"/>
<pin name="VP@1" direction="pwr"/>
<pin name="VP@2" direction="pwr"/>
</symbol>
<symbol name="CAT24CXX">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="WP"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="*161" prefix="IC">
<description>&lt;b&gt;Universal Voltage Monitor&lt;/b&gt;&lt;p&gt;
Source: www.onsemi.com/pub_link/Collateral/MC34161-D.PDF</description>
<gates>
<gate name="G$1" symbol="MC34161"/>
</gates>
<devices>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="MC33">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33161P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="07F4769"/>
</technology>
<technology name="MC34">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC34161P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="07F5035"/>
</technology>
</technologies>
</device>
<device name="D" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="MC33">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33161D"/>
<attribute name="OC_FARNELL" value="1192059"/>
<attribute name="OC_NEWARK" value="07F4768"/>
</technology>
<technology name="MC34">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC34161D"/>
<attribute name="OC_FARNELL" value="1652462"/>
<attribute name="OC_NEWARK" value="07F5034"/>
</technology>
<technology name="NCV33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NCV33161DR2G"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="27M2600"/>
</technology>
</technologies>
</device>
<device name="DM" package="MICRO8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="MC33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC33161DMR2G"/>
<attribute name="OC_FARNELL" value="1705447"/>
<attribute name="OC_NEWARK" value="04R7825"/>
</technology>
<technology name="MC34">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC34161DMR2G"/>
<attribute name="OC_FARNELL" value="1652462"/>
<attribute name="OC_NEWARK" value="42K0658"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT4101" prefix="IC">
<description>&lt;b&gt;1A Constant-Current LED Driver with PWM Dimming&lt;/b&gt;&lt;p&gt;
Source: ON Semiconductor .. 4101.pdf</description>
<gates>
<gate name="G$1" symbol="CAT4101"/>
</gates>
<devices>
<device name="" package="TO263_5">
<connects>
<connect gate="G$1" pin="EN/PWM" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LED" pad="5"/>
<connect gate="G$1" pin="RSET" pad="4"/>
<connect gate="G$1" pin="TAB" pad="TAB"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT4101TV-T75"/>
<attribute name="OC_FARNELL" value="1718452"/>
<attribute name="OC_NEWARK" value="08R5264"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC12052A" prefix="IC">
<description>&lt;b&gt;1.1 GHZ Suiper Low Power Dual Modulus Prescaler&lt;/b&gt;&lt;p&gt;
Source:http://motorola.com/sps .. MC12052A.pdf</description>
<gates>
<gate name="G$1" symbol="MC12052A"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="!IN" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="MC" pad="6"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SW" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC12080" prefix="IC">
<description>&lt;b&gt;1.1 GHz Prescaler&lt;/b&gt; MECL PLL COMPONENTS ÷10/20/40/80 PRESCALER&lt;p&gt;
Source: http://motorola.com/sps .. MC12080.pdf</description>
<gates>
<gate name="G$1" symbol="MC12080"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="!IN" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SW1" pad="3"/>
<connect gate="G$1" pin="SW2" pad="6"/>
<connect gate="G$1" pin="SW3" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC12080D"/>
<attribute name="OC_FARNELL" value="1607924"/>
<attribute name="OC_NEWARK" value="40C2542"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="!IN" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="SW1" pad="3"/>
<connect gate="G$1" pin="SW2" pad="6"/>
<connect gate="G$1" pin="SW3" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MDC3105LT1" prefix="IC">
<description>&lt;b&gt;Integrated Relay, Inductive Load Driver&lt;/b&gt;&lt;p&gt;
Sopurce: U6 OnSemi Inductive Load Driver MDC3105-D.PDF</description>
<gates>
<gate name="P" symbol="NPN-DRIVER"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VIN" pad="1"/>
<connect gate="P" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MDC3105LT1"/>
<attribute name="OC_FARNELL" value="1126459"/>
<attribute name="OC_NEWARK" value="16F6132"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MDC3105DMT1" prefix="IC">
<description>&lt;b&gt;Integrated Relay, Inductive Load Driver&lt;/b&gt;&lt;p&gt;
Sopurce: U6 OnSemi Inductive Load Driver MDC3105-D.PDF</description>
<gates>
<gate name="A" symbol="NPN-DRIVER"/>
<gate name="B" symbol="NPN-DRIVER"/>
</gates>
<devices>
<device name="" package="SC-74">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VIN" pad="5"/>
<connect gate="A" pin="VOUT" pad="6"/>
<connect gate="B" pin="GND" pad="4"/>
<connect gate="B" pin="VIN" pad="2"/>
<connect gate="B" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MDC3105DMT1G"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="04R7836"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MDC3105XV6T1" prefix="IC">
<description>&lt;b&gt;Integrated Relay, Inductive Load Driver&lt;/b&gt;&lt;p&gt;
Sopurce: U6 OnSemi Inductive Load Driver MDC3105-D.PDF</description>
<gates>
<gate name="A" symbol="NPN-DRIVER_4C"/>
</gates>
<devices>
<device name="" package="SOT-563">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VIN" pad="3"/>
<connect gate="A" pin="VOUT" pad="1"/>
<connect gate="A" pin="VOUT1" pad="2"/>
<connect gate="A" pin="VOUT2" pad="5"/>
<connect gate="A" pin="VOUT3" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A5191HRT" prefix="IC">
<description>&lt;b&gt;HART Modem&lt;/b&gt; Single-chip, half-duplex 1200 bits per second FSK modem&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source:OnSemi A5191HRT HART Modem Data Sheet.pdf</description>
<gates>
<gate name="G$1" symbol="A5191HRT"/>
</gates>
<devices>
<device name="" package="PLCC28">
<connects>
<connect gate="G$1" pin="IAREF" pad="11"/>
<connect gate="G$1" pin="ICDREF" pad="12"/>
<connect gate="G$1" pin="INRESET" pad="6"/>
<connect gate="G$1" pin="INRTS" pad="23"/>
<connect gate="G$1" pin="IRXA" pad="16"/>
<connect gate="G$1" pin="IRXAC" pad="18"/>
<connect gate="G$1" pin="ITXD" pad="24"/>
<connect gate="G$1" pin="IXTL" pad="20"/>
<connect gate="G$1" pin="OCBIAS" pad="13"/>
<connect gate="G$1" pin="OCD" pad="27"/>
<connect gate="G$1" pin="ORXAF" pad="17"/>
<connect gate="G$1" pin="ORXD" pad="26"/>
<connect gate="G$1" pin="OTXA" pad="10"/>
<connect gate="G$1" pin="OXTL" pad="19"/>
<connect gate="G$1" pin="TEST1" pad="1"/>
<connect gate="G$1" pin="TEST10" pad="14"/>
<connect gate="G$1" pin="TEST11" pad="25"/>
<connect gate="G$1" pin="TEST12" pad="28"/>
<connect gate="G$1" pin="TEST2" pad="2"/>
<connect gate="G$1" pin="TEST3" pad="3"/>
<connect gate="G$1" pin="TEST4" pad="4"/>
<connect gate="G$1" pin="TEST5" pad="5"/>
<connect gate="G$1" pin="TEST7" pad="7"/>
<connect gate="G$1" pin="TEST8" pad="8"/>
<connect gate="G$1" pin="TEST9" pad="9"/>
<connect gate="G$1" pin="VDD" pad="22"/>
<connect gate="G$1" pin="VDDA" pad="15"/>
<connect gate="G$1" pin="VSS" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="A5191HRTPG-XTD"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="03P1167"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A5191HRTI" prefix="IC">
<description>&lt;b&gt;HART Modem&lt;/b&gt; Single-chip, half-duplex 1200 bits per second FSK modem&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source:OnSemi A5191HRT HART Modem Data Sheet.pdf</description>
<gates>
<gate name="G$1" symbol="A5191HRTI"/>
</gates>
<devices>
<device name="" package="LQFP32-7X7MM">
<connects>
<connect gate="G$1" pin="IAREF" pad="8"/>
<connect gate="G$1" pin="ICDREF" pad="9"/>
<connect gate="G$1" pin="INRESET" pad="2"/>
<connect gate="G$1" pin="INRTS" pad="22"/>
<connect gate="G$1" pin="IRXA" pad="14"/>
<connect gate="G$1" pin="IRXAC" pad="16"/>
<connect gate="G$1" pin="ITXD" pad="23"/>
<connect gate="G$1" pin="IXTL" pad="18"/>
<connect gate="G$1" pin="OCBIAS" pad="10"/>
<connect gate="G$1" pin="OCD" pad="26"/>
<connect gate="G$1" pin="ORXAF" pad="15"/>
<connect gate="G$1" pin="ORXD" pad="25"/>
<connect gate="G$1" pin="OTXA" pad="7"/>
<connect gate="G$1" pin="OXTL" pad="17"/>
<connect gate="G$1" pin="TEST1" pad="28"/>
<connect gate="G$1" pin="TEST10" pad="11"/>
<connect gate="G$1" pin="TEST11" pad="24"/>
<connect gate="G$1" pin="TEST12" pad="27"/>
<connect gate="G$1" pin="TEST2" pad="29"/>
<connect gate="G$1" pin="TEST3" pad="31"/>
<connect gate="G$1" pin="TEST4" pad="32"/>
<connect gate="G$1" pin="TEST5" pad="1"/>
<connect gate="G$1" pin="TEST7" pad="3"/>
<connect gate="G$1" pin="TEST8" pad="4"/>
<connect gate="G$1" pin="TEST9" pad="5"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDD@1" pad="30"/>
<connect gate="G$1" pin="VDDA" pad="13"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="20"/>
<connect gate="G$1" pin="VSSA" pad="12"/>
<connect gate="G$1" pin="VSSA@1" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="A5191HRTLG-XTD"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="03P1166"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP2820" prefix="IC">
<description>&lt;b&gt;2.65 W Filterless Class-D Audio Power Amplifier&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.onsemi.com/pub_link/Collateral/NCP2820-D.PDF"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="NCP2820"/>
</gates>
<devices>
<device name="" package="FLIP-CHIP9">
<connects>
<connect gate="G$1" pin="!SD" pad="C2"/>
<connect gate="G$1" pin="GND@1" pad="A2"/>
<connect gate="G$1" pin="GND@2" pad="B3"/>
<connect gate="G$1" pin="INM" pad="C1"/>
<connect gate="G$1" pin="INP" pad="A1"/>
<connect gate="G$1" pin="OUTM" pad="A3"/>
<connect gate="G$1" pin="OUTP" pad="C3"/>
<connect gate="G$1" pin="VP@1" pad="B1"/>
<connect gate="G$1" pin="VP@2" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAT24CXX" prefix="U">
<gates>
<gate name="G$1" symbol="CAT24CXX"/>
</gates>
<devices>
<device name=".UDFN8-EP" package="UDFN8-EP">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 PAD"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".UDFN8" package="UDFN8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4 PAD"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
