<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="TDFN14">
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="CERM_OSC">
</package>
<package name="EG1213">
</package>
<package name="PJ-102A">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0504">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1310">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1608">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1825">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C2012">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C3225">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C4532">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C4564">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="C025-040X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 4 x 5 mm</description>
</package>
<package name="C025-050X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 5 x 5 mm</description>
</package>
<package name="C025-060X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 6 x 5 mm</description>
</package>
<package name="C025_050-024X070">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm + 5 mm, outline 2.4 x 7 mm</description>
</package>
<package name="C025_050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C025_050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C025_050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C025_050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="C050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="C050-050X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5 x 7.5 mm</description>
</package>
<package name="C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C050H075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Horizontal, grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="C075-032X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 3.2 x 10.3 mm</description>
</package>
<package name="C075-042X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 4.2 x 10.3 mm</description>
</package>
<package name="C075-052X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 5.2 x 10.6 mm</description>
</package>
<package name="C102-043X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 4.3 x 13.3 mm</description>
</package>
<package name="C102-054X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 5.4 x 13.3 mm</description>
</package>
<package name="C102-064X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 6.4 x 13.3 mm</description>
</package>
<package name="C102_152-062X184">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm + 15.2 mm, outline 6.2 x 18.4 mm</description>
</package>
<package name="C150-054X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 5.4 x 18.3 mm</description>
</package>
<package name="C150-064X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 6.4 x 18.3 mm</description>
</package>
<package name="C150-072X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 7.2 x 18.3 mm</description>
</package>
<package name="C150-084X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 8.4 x 18.3 mm</description>
</package>
<package name="C150-091X182">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 9.1 x 18.2 mm</description>
</package>
<package name="C225-062X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 6.2 x 26.8 mm</description>
</package>
<package name="C225-074X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 7.4 x 26.8 mm</description>
</package>
<package name="C225-087X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 8.7 x 26.8 mm</description>
</package>
<package name="C225-108X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 10.8 x 26.8 mm</description>
</package>
<package name="C225-113X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 11.3 x 26.8 mm</description>
</package>
<package name="C275-093X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 9.3 x 31.6 mm</description>
</package>
<package name="C275-113X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 11.3 x 31.6 mm</description>
</package>
<package name="C275-134X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 13.4 x 31.6 mm</description>
</package>
<package name="C275-205X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 20.5 x 31.6 mm</description>
</package>
<package name="C325-137X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 13.7 x 37.4 mm</description>
</package>
<package name="C325-162X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 16.2 x 37.4 mm</description>
</package>
<package name="C325-182X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 18.2 x 37.4 mm</description>
</package>
<package name="C375-192X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 19.2 x 41.8 mm</description>
</package>
<package name="C375-203X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 20.3 x 41.8 mm</description>
</package>
<package name="C050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="C375-155X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 15.5 x 41.8 mm</description>
</package>
<package name="C075-063X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 6.3 x 10.6 mm</description>
</package>
<package name="C275-154X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 15.4 x 31.6 mm</description>
</package>
<package name="C275-173X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 17.3 x 31.6 mm</description>
</package>
<package name="C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="C1812K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1812 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4532</description>
</package>
<package name="C1825K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1825 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4564</description>
</package>
<package name="C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 5650</description>
</package>
<package name="C2225K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2225 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 5664</description>
</package>
<package name="CT3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT3528">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT6032">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="CT7343">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip
tantalum</description>
</package>
<package name="B45181A">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 5 x 5 mm, rectangle, grid 2.54 mm</description>
</package>
<package name="B45181B">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 7.6 x 5 mm, rectangle, grid 5.08 mm</description>
</package>
<package name="B45181C">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.7 x 7.6 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="B45181D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
body 12.5 x 12.5 mm, rectangle, grid 10.16 mm</description>
</package>
<package name="TT2D4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D4L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4 mm, grid 2.54 mm</description>
</package>
<package name="TT2D5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT2D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 2.54 mm</description>
</package>
<package name="TT5D10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 10 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D11L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 11 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D6L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D7L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="TT5D9L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="ETR1">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 2.54 mm</description>
</package>
<package name="ETR2">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR3">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 5.08 mm</description>
</package>
<package name="ETR4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="ETR5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
rectangle, grid 10.16 mm</description>
</package>
<package name="P128-35">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-40">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="P128-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TAP5-45">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 4.5 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-50">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-70">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 7.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-60">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 6.0 mm, grid 5.08 mm</description>
</package>
<package name="TAP5-80">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 8.0 mm, grid 5.08 mm</description>
</package>
<package name="085CS_1R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AR">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="085CS_1AW">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Standard 085 CS&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-2W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3R">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; reflow soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="139CLL-3W">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt; wave soldering&lt;p&gt;
SMD (Chip) Long Life 139 CLL&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="140CLH-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, High temperature 140 CLH&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="150CLZ-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors SMD (Chip)&lt;/b&gt;&lt;p&gt;
Long life base plate, very low impedance 150 CLZ&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0505">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0807">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1010">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1012">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-1014">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0808">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="175TMP-0810">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
High Temperature solid electrolytic SMD 175 TMP&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="A/3216-18W">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="B/3528-21R">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="B/3528-21W">
<description>&lt;b&gt;Chip Capacitor Type KEMET B / EIA 3528-21 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
<package name="C/6032-28R">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="C/6032-28W">
<description>&lt;b&gt;Chip Capacitor Type KEMET C / EIA 6032-28 Wafe solder&lt;/b&gt;&lt;p&gt;
KEMET U / EIA 6032-15</description>
</package>
<package name="D/7343-31R">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Reflow solder</description>
</package>
<package name="D/7343-31W">
<description>&lt;b&gt;Chip Capacitor Type KEMET D / EIA 7343-21&lt;/b&gt;&lt;p&gt;
KEMET V / EIA 7343-20, KEMET X / EIA 7343-43 Wafe solder</description>
</package>
<package name="E/7260-38R">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Reflow solder&lt;/b&gt;</description>
</package>
<package name="E/7260-38W">
<description>&lt;b&gt;Chip Capacitor Type KEMET E / EIA 7260-38 Wafe solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12R">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Reflow solder&lt;/b&gt;</description>
</package>
<package name="R/2012-12W">
<description>&lt;b&gt;Chip Capacitor Type KEMET R/EIA 2012-12 Wafe solder&lt;/b&gt;</description>
</package>
<package name="PANASONIC_A">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package A&lt;/b&gt;</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="PANASONIC_E">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="E1,8-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 1.8 mm, diameter 4 mm</description>
</package>
<package name="EB20D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 20 mm</description>
</package>
<package name="EB22,5D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 22.5 mm</description>
</package>
<package name="EB25D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 25 mm</description>
</package>
<package name="EB30D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 30 mm</description>
</package>
<package name="EB35D">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.16 mm, diameter 35 mm</description>
</package>
<package name="E15-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 5 mm</description>
</package>
<package name="E15-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 6 mm</description>
</package>
<package name="E15-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15.24 mm, diameter 9 mm</description>
</package>
<package name="E2,5-6E">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="E2-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.032 mm, diameter 5 mm</description>
</package>
<package name="E2,5RE">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm,</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E2,5-4R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 4 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="E22-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 10 mm</description>
</package>
<package name="E22-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 6 mm</description>
</package>
<package name="E22-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="E25-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 10 mm</description>
</package>
<package name="E25-9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 25.4 mm, diameter 9 mm</description>
</package>
<package name="E3,5-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 10 mm</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
<package name="E30-10">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 10 mm</description>
</package>
<package name="E30-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 12 mm</description>
</package>
<package name="E30-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-12">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 35.56 mm, diameter 12 mm</description>
</package>
<package name="E35-14">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 14 mm</description>
</package>
<package name="E35-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 16 mm</description>
</package>
<package name="E35-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 30.48 mm, diameter 18 mm</description>
</package>
<package name="E45-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 16 mm</description>
</package>
<package name="E45-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 18 mm</description>
</package>
<package name="E45-21">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 21 mm</description>
</package>
<package name="E45-22">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 22 mm</description>
</package>
<package name="E45-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 45.72 mm, diameter 25 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="E5-13">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 13 mm</description>
</package>
<package name="E5-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.05 mm, diameter 4 mm</description>
</package>
<package name="E5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 5 mm</description>
</package>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="E5R">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 9 mm</description>
</package>
<package name="E50-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 25 mm</description>
</package>
<package name="E50-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 50 mm, diameter 30 mm</description>
</package>
<package name="E55-25">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 25 mm</description>
</package>
<package name="E55-30">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 55 mm, diameter 30 mm</description>
</package>
<package name="E7,5-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 16 mm</description>
</package>
<package name="E7,5-18">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 18 mm</description>
</package>
<package name="TT2D5L">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 5 mm, grid 2.54 mm</description>
</package>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
<package name="LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LSU260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
1 mm, round, Siemens</description>
</package>
<package name="LZR181">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
1 LED, Siemens</description>
</package>
<package name="Q62902-B152">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B153">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B155">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B156">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="SFH480">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="SFH482">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="U57X32">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
</package>
<package name="IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="P-LCC-2">
<description>&lt;b&gt;TOPLED® High-optical Power LED (HOP)&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... ls_t675.pdf</description>
</package>
<package name="OSRAM-MINI-TOP-LED">
<description>&lt;b&gt;BLUE LINETM Hyper Mini TOPLED® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LB M676.pdf</description>
</package>
<package name="OSRAM-SIDELED">
<description>&lt;b&gt;Super SIDELED® High-Current LED&lt;/b&gt;&lt;p&gt;
LG A672, LP A672 &lt;br&gt;
Source: http://www.osram.convergy.de/ ... LG_LP_A672.pdf (2004.05.13)</description>
</package>
<package name="SMART-LED">
<description>&lt;b&gt;SmartLEDTM Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY L896.pdf</description>
</package>
<package name="P-LCC-2-TOPLED-RG">
<description>&lt;b&gt;Hyper TOPLED® RG Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY T776.pdf</description>
</package>
<package name="MICRO-SIDELED">
<description>&lt;b&gt;Hyper Micro SIDELED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY Y876.pdf</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="MINI-TOPLED-SANTANA">
<description>&lt;b&gt;Mini TOPLED Santana®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG M470.pdf</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="SMARTLED-TTW">
<description>&lt;b&gt;SmartLED TTW&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R1005">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
<package name="0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
<package name="MSOP10">
<description>10-Lead Mini Small Outline Package [MSOP]</description>
</package>
<package name="1X2-3.5MM">
</package>
<package name="UMAX10">
</package>
<package name="CSTCR-G">
</package>
<package name="AWCSR">
</package>
<package name="TC33X">
</package>
<package name="NX8045">
</package>
<package name="NX5032">
</package>
<package name="OS102011MA1Q">
</package>
<package name="EVQ-Q2">
</package>
<package name="TQFP44">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)&lt;p&gt;
Source: http://www.atmel.com .. doc1477.pdf</description>
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
<package name="12BH412">
</package>
<package name="EG1218">
</package>
<package name="PS603">
</package>
<package name="DIL08-ROUND">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="LED5MMRGB">
</package>
<package name="FB">
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09-BIG">
</package>
<package name="1X10-BIG">
</package>
<package name="PNA460XM">
</package>
<package name="1X04-BIG">
</package>
<package name="PROPPLUG">
</package>
<package name="PROPCLIP">
</package>
<package name="AL60P">
<description>&lt;b&gt;SPEAKER&lt;/b&gt;</description>
</package>
<package name="AL11P">
<description>&lt;b&gt;SPEAKER&lt;/b&gt;</description>
</package>
<package name="PS12">
</package>
<package name="TS12864">
</package>
<package name="CR1220-SMD">
</package>
<package name="CR1220-THM">
</package>
<package name="IV18">
</package>
<package name="PLCC-S28">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt; Socked</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
<package name="TO39">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="SO08">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="2747">
</package>
<package name="1800R">
</package>
<package name="6000">
</package>
<package name="DO13M">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 6.35 mm metall, horizontal, grid 20.32 mm</description>
</package>
<package name="C4111-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.3 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="P6T15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 9 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="CB429-17">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5 mm, horizontal, grid 17 mm</description>
</package>
<package name="DO201T15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.6 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="F126Z12">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 3 mm, horizontal, grid 12.7 mm</description>
</package>
<package name="AG">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 9 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="TO92H">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
2-lead plastic, vertical</description>
</package>
<package name="CB417-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 3.5 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="CB429-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5 mm, horizontal, grid 15.24 mm</description>
</package>
<package name="TO237">
<description>&lt;b&gt;TO 273&lt;/b&gt;</description>
</package>
<package name="ALTOIDSTIN">
</package>
<package name="2XAA">
</package>
<package name="DIL14-LARDO">
</package>
<package name="ARDUINO">
<description>&lt;b&gt;Arduino Uno&lt;/b&gt;
&lt;p&gt;
Make a shield with ease, this package has all the named pins as well as the two mounting drill holes and an outline of the USB and DC power connector. The outline is on the DIMENSION layer, so if your board house uses it they will cut the outline to match.</description>
</package>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="JST-PH-2-THM">
<description>4UCon #01528
http://www.4uconnector.com/online/object/4udrawing/01528.pdf</description>
</package>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
<package name="USB-MINIB-THM">
<description>&lt;b&gt;Mini USB 5-pin thru-mount connector&lt;/b&gt;
&lt;p&gt;
4Ucon #18732</description>
</package>
<package name="ARDUINO-NOHOLE">
</package>
<package name="USB-MINIB-THM-MOLEX">
</package>
<package name="B3F-31XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="ARDUINO-NODIM">
</package>
<package name="SCDA">
</package>
<package name="SDCARD">
</package>
<package name="06132">
</package>
<package name="THUMBWHEEL">
</package>
<package name="THUMBWHEELV">
</package>
<package name="STX3100">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
KS-S stereo microphone/headphone jack&lt;p&gt;
 PG203JN (Schukat)</description>
</package>
<package name="1X03-CLEANBIG">
</package>
<package name="1X08-BIG">
</package>
<package name="1X08-CLEANBIG">
</package>
<package name="1X08-LOCK">
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06-CLEAN">
</package>
<package name="1X06-CLEANBIG">
</package>
<package name="1X06-BIG">
</package>
<package name="1X06-BIGLOCK">
</package>
<package name="TO92-INLINE">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="1035D">
</package>
<package name="JST-8POS">
</package>
<package name="JST-6POS">
</package>
<package name="TRIMBLE">
</package>
<package name="CP-2350">
<description>Female &lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
5 pins 90 deg. with shield, horizontal (DIN 41524)</description>
</package>
<package name="TEENSY">
</package>
<package name="MICROSD">
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
<package name="SO16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
<package name="0805-THM">
</package>
<package name="9.7ELECTRET">
</package>
<package name="2XAAA">
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
<package name="RK0971221">
</package>
<package name="2XAAA-SIDE">
</package>
<package name="USB-MINIB-THM-MOLEX-PWRONLY">
</package>
<package name="ADAFRUIT200MIL">
</package>
<package name="CQFP-44">
<description>&lt;b&gt;CERAMIC QUAD FLAT PACK&lt;/b&gt;</description>
</package>
<package name="SQFP-S-5X5-48">
<description>&lt;b&gt;QFP48&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="SQFP-S-7X7-48">
<description>&lt;b&gt;QFP48&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, horinzontal</description>
</package>
<package name="TO220-NOHOLE">
</package>
<package name="DO41-7">
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="USB-MINIB-THM-PWRONLY">
</package>
<package name="AVRISP">
</package>
<package name="SOT23-6">
</package>
<package name="LQH55">
</package>
<package name="SMADIODE">
<description>&lt;b&gt;SMA Surface Mount Diode&lt;/b&gt;</description>
</package>
<package name="DO-1N4148">
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
<package name="SOD-123">
</package>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
<package name="SO18W">
</package>
<package name="DIL18">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="SOP24">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt;</description>
</package>
<package name="SSOP24">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt; SSOP-24&lt;p&gt;</description>
</package>
<package name="1X05-3.5MM">
</package>
<package name="LCD1602">
</package>
<package name="SUN">
</package>
<package name="TO92-OVAL">
</package>
<package name="JST-PH-2-SMT">
</package>
<package name="2X22">
</package>
<package name="1X22">
</package>
<package name="2X09-BIG">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X09-CLEANBIG">
</package>
<package name="ILI9325_28INCH_TS">
<description>1.0mm-Pitch 37 Pin LCD Connector</description>
</package>
<package name="1812">
<description>Multilayer SMD</description>
</package>
<package name="1X14">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X14-CB">
</package>
<package name="1X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X12-CB">
</package>
<package name="1X40-1MM">
</package>
<package name="1X40-0.6MM">
</package>
<package name="1X40-0.7MM">
</package>
<package name="1X40-0.8MM">
</package>
<package name="1X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X20-BIG">
</package>
<package name="2X20-BIG">
</package>
<package name="1X40-0.5MM">
</package>
<package name="PIRANHA5MM">
</package>
<package name="DIL28-3-TI">
</package>
<package name="1X30-0.7MM">
</package>
<package name="2X14-CLEANBIG">
</package>
<package name="2X14">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X22-SMT">
</package>
<package name="XF2E-0515-1">
<description>&lt;b&gt;Non-ZIF Type (0.8 mm-pitch)&lt;/b&gt;&lt;p&gt;
Source : http://www.omron.com/ecb/products/pdf/fpc.pdf</description>
</package>
<package name="XF2L-0535-1">
<description>&lt;b&gt;ZIF Slide-locking Type (0.5 mm-pitch)&lt;/b&gt; Lower-contact Type&lt;p&gt;
Source : http://www.omron.com/ecb/products/pdf/fpc.pdf</description>
</package>
<package name="XF2H-4015-1LW">
<description>&lt;b&gt;Standard Rotary Backlock Type (0.5 mm-pitch)&lt;/b&gt;&lt;p&gt;
Source : http://www.omron.com/ecb/products/pdf/fpc.pdf</description>
</package>
<package name="4-1734839-0">
<description>&lt;b&gt;Reduced-area Rotary Backlock Type (0.5 mm-pitch)&lt;/b&gt;&lt;p&gt;
Source : http://www.omron.com/ecb/products/pdf/fpc.pdf</description>
</package>
<package name="XF2R-4015-4A">
<description>&lt;b&gt;Low-profile Rotary Backlock Type (0.5 mm-pitch)&lt;/b&gt;&lt;p&gt;Source : http://www.omron.com/ecb/products/pdf/fpc.pdf</description>
</package>
<package name="F15D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F15H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F15HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F15V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F15VP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="HDF15H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="HDF15V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F15VB">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="XF2M-4015-1F-REVERSE">
</package>
<package name="SFV4R-1STE1LF">
<description>&lt;b&gt;FPC Connector ZIF for SMT 0.5mm&lt;/b&gt;&lt;p&gt;

FCI SFV4R-1STE1LF</description>
</package>
<package name="2X14-SMT">
</package>
<package name="1X25-CB">
</package>
<package name="1X15">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X15-CB">
</package>
<package name="TSSOP-8">
</package>
<package name="XTAL3215">
</package>
<package name="NX3225">
</package>
<package name="SMT-0540-S-R">
</package>
<package name="MOLEX_480371000">
</package>
<package name="OSHWLOGO_0.3">
</package>
<package name="OSHWLOGO_TOP_0.2">
</package>
<package name="MOON">
</package>
<package name="FPC_0.5MM-4">
</package>
<package name="1X04-CLEANBIG">
</package>
<package name="1X08-3.5MM">
</package>
<package name="1X06-3.5MM">
</package>
<package name="1X04-3.5MM">
</package>
<package name="ARDUINO-BPLACE">
</package>
<package name="JUDCOSPST">
</package>
<package name="JD-T1800">
</package>
<package name="16LCSP">
</package>
<package name="EVQQ7GA50">
</package>
<package name="RN-171">
</package>
<package name="1X18">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X18-BIG">
</package>
<package name="RN-ANT">
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="SSOP20">
</package>
<package name="1X13">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X13-BIG">
</package>
<package name="QFN20">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="UDFN-8">
</package>
<package name="SMLK34">
</package>
<package name="OSHWLOGO_TOL_0.2">
</package>
<package name="XBEE">
</package>
<package name="1X01-CLEANBIG">
</package>
<package name="BMP085">
</package>
<package name="VFSOP-8">
<description>&lt;b&gt;VFSOP8&lt;/b&gt; - 0.5mm pitch, 2.0x2.3mm
&lt;p&gt;Source: http://focus.ti.com/lit/ds/symlink/txs0102.pdf&lt;/p&gt;</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="TSSOP20">
</package>
<package name="JOYSTICK">
</package>
<package name="CR2032-THRU">
</package>
<package name="CR2032-SMD">
</package>
<package name="SEGMENT_BICOL_BL-M12A883XX">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.betlux.com/product/led_dot_matrix/BL-M12A883xx.PDF</description>
</package>
<package name="SEGMENT_BL-M07C881UR">
</package>
<package name="SEGMENT_BL-M12A881UR">
<description>&lt;b&gt;Source:&lt;/b&gt; http://www.betlux.com/product/LED_dot_matrix/BL-M12A881.PDF</description>
</package>
<package name="SEGMENT_BL-M12A883">
<description>&lt;b&gt;Source:&lt;/b&gt; http://www.betlux.com/product/LED_dot_matrix/BL-M12A883.PDF</description>
</package>
<package name="SEGMENT_BICOL_BL-AR12Z3010">
<description>&lt;b&gt;Souce: &lt;/b&gt;http://www.betlux.com/product/LED_light_bar/BL-AR12B3010xx.PDF</description>
</package>
<package name="SEGMENT_BL-M15A881">
</package>
<package name="STRIP-3PIN">
</package>
<package name="3-STRIP">
</package>
<package name="5-STRIP">
</package>
<package name="8-STRIP">
</package>
<package name="12-STRIP">
</package>
<package name="ALTOIDSTIN-DIM">
</package>
<package name="DIL28-3-ROUND">
</package>
<package name="414-VA5R">
</package>
<package name="SO08-SKINNYPADS">
</package>
<package name="STRIP-5PINSS">
</package>
<package name="RGBLED5050">
</package>
<package name="SEWINGTAP_0.5">
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="SO28W">
<description>&lt;B&gt;28-Lead Plastic Small Outline (SO) &lt;/B&gt; Wide, 300 mil Body (SOIC)&lt;/B&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="QFN28-ML_6X6MM">
<description>&lt;b&gt;QFN28-ML_6X6MM&lt;/b&gt;&lt;p&gt;
Source: http://www.microchip.com .. 39637a.pdf</description>
</package>
<package name="DFN-6">
</package>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="SOD-323F">
</package>
<package name="SOIC8_208MIL">
<description>&lt;b&gt;Small Outline IC - 208mil Wide&lt;/b&gt;</description>
</package>
<package name="SEWINGTAP_0.4">
</package>
<package name="JSTPH3">
</package>
<package name="ARDUINOR3">
<description>The new Arduino R3 'classic' adds duplicate I2C pins and an IORef pin (and an unused pin</description>
</package>
<package name="LCD1602-RGB">
</package>
<package name="ARDUINOR3-BPLACE">
</package>
<package name="6MM">
</package>
<package name="2X08-IDC">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="SEWINGTAP_2.0">
</package>
<package name="EG1390">
</package>
<package name="KMR2">
</package>
<package name="BEAGLEBONE_SHIELD">
</package>
<package name="ADAFRUIT450MIL">
</package>
<package name="ARDUINOR3-NOTEXT-NOIOREF">
</package>
<package name="0805-THM-7">
</package>
<package name="INDUCTOR_5X5MM_TDK_VLC5045">
<description>&lt;b&gt;Source: http://www.tdk.co.jp/tefe02/e531_vlc5045.pdf&lt;/b&gt;</description>
</package>
<package name="FGPMMOPA6B">
</package>
<package name="FGPMMOPA6C">
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="ARDUINOMICRO">
</package>
<package name="SPRINGTERMINAL-17">
</package>
<package name="TSSOP28">
</package>
<package name="FGPMMOPA6H">
</package>
<package name="B3F-31XX-SKINNIER">
</package>
<package name="TDFN14_3X3MM">
<description>&lt;b&gt;TDFN 14 3x3x0.75mm&lt;/b&gt;
&lt;p&gt;Source: http://datasheets.maxim-ic.com/en/ds/MAX98306.pdf&lt;/p&gt;
&lt;p&gt;Based on recommendtions in: http://www.freescale.com/files/sensors/doc/data_sheet/MAG3110.pdf&lt;/p&gt;</description>
</package>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49GW">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49TL-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-LM">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U70">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC13U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC18U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC18U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC33U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC33U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="86SMX">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
<package name="MM20SS">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="MM39SL">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="ALTOIDSSMALLS">
</package>
<package name="SLIDEPOT-45">
</package>
<package name="ARDUINOR3_ICSP">
</package>
<package name="B3F-40XX-ROUND">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="B3F-40XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="MC14093B-TSSOP14">
<description>&lt;b&gt;plastic thin shrink small outline package; 14 leads; body width 4.4 mm &lt;/b&gt;&lt;p&gt;
SOT402-1&lt;br&gt;
Source: http://www.onsemi.com/pub_link/Collateral/MC14093B-D.PDF</description>
</package>
<package name="BLUEFRUITLOGO_150MM">
</package>
<package name="HTSSOP32DAP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DAP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds029b/mpds029b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP20DAP">
</package>
<package name="WS2812">
</package>
<package name="1X4-SMT">
</package>
<package name="TRIM-3386">
</package>
<package name="0207/9">
</package>
<package name="AVRISP-BOX">
</package>
<package name="SOD-123FL">
</package>
<package name="ARDUINOR3_ICSP_SMT">
</package>
<package name="1X08_SMT">
<description>&lt;p&gt;4UCON: 06678&lt;/p&gt;</description>
</package>
<package name="BIGTAP">
</package>
<package name="BLUEFRUITLOGO_100MM">
</package>
<package name="WS2812B">
</package>
<package name="U.FL">
</package>
<package name="ARDUINOR3_ICSP_NODIM">
</package>
<package name="SMA_EDGELAUNCH">
</package>
<package name="SMA90_DIP">
<description>SMA DIP Connector 90° 50 Ohm</description>
</package>
<package name="SMA_EDGELAUNCH_UFL">
</package>
<package name="TFT_2.83IN_240X320_50PIN">
</package>
<package name="TFT_CTP28">
</package>
<package name="PROTRINKET">
</package>
<package name="ESP-12">
</package>
<package name="TESTCLIP">
</package>
<package name="1X1-BIGPOGO">
</package>
<package name="SIM800L">
</package>
<package name="SIM900_SMT">
</package>
<package name="PUSHBUTTON_SMD_SJ">
</package>
<package name="TACT_PANA-EVQ">
</package>
<package name="BTN_CK_KSS">
</package>
<package name="FEATHERWING">
</package>
<package name="FEATHERWING_DIM">
</package>
<package name="WS2812B-NARROW">
</package>
<package name="LED3535">
</package>
<package name="ARDUINO_DUE_SHIELD">
<description>Arudiono Due Shield</description>
</package>
<package name="ARDUINO_DUE_OUTLINE">
<description>The board outline for an Arduino DUE.</description>
</package>
</packages>
<symbols>
<symbol name="POWERJACK">
<pin name="TIP"/>
<pin name="SLEEVE"/>
<pin name="SHUNT"/>
</symbol>
<symbol name="LM3622">
<pin name="VCC" direction="sup"/>
<pin name="EXT" direction="out"/>
<pin name="CEL" direction="pas"/>
<pin name="CS" direction="pas"/>
<pin name="LVSEL" direction="in"/>
<pin name="#LVEN" direction="in" function="dot"/>
<pin name="#LV" direction="out" function="dot"/>
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="LTC1730">
<pin name="/CHRG"/>
<pin name="VCC" direction="sup"/>
<pin name="SENSE"/>
<pin name="GATE" direction="out"/>
<pin name="BATT" direction="out"/>
<pin name="NTC/#SHDN" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="TIMER" direction="pas"/>
</symbol>
<symbol name="LTC1731">
<pin name="/CHRG"/>
<pin name="VCC" direction="sup"/>
<pin name="SENSE"/>
<pin name="DRV" direction="out"/>
<pin name="BATT" direction="out"/>
<pin name="PROG" direction="pas"/>
<pin name="GND" direction="sup"/>
<pin name="TIMER" direction="pas"/>
</symbol>
<symbol name="MAX1811">
<pin name="IN"/>
<pin name="SELV"/>
<pin name="EN"/>
<pin name="SELI"/>
<pin name="GND"/>
<pin name="/CHG"/>
<pin name="BATT"/>
<pin name="GND2"/>
</symbol>
<symbol name="MAX8601">
<pin name="BAT" direction="in"/>
<pin name="SETI" direction="pas"/>
<pin name="THM" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="CT" direction="pas"/>
<pin name="/POK" direction="out"/>
<pin name="/CHG" direction="out"/>
<pin name="DC2" direction="in"/>
<pin name="DC" direction="in"/>
<pin name="/FLT" direction="out"/>
<pin name="/EN" direction="in"/>
<pin name="BAT1" direction="in"/>
<pin name="USB" direction="in"/>
<pin name="USEL" direction="in"/>
</symbol>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="CAPOSC">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="TSU">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="MT">
<pin name="MT" direction="pas"/>
</symbol>
<symbol name="POWERJACK-1">
<pin name="TIP"/>
<pin name="RING"/>
<pin name="RING_SW"/>
</symbol>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CPOL-US">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ID"/>
</symbol>
<symbol name="MAX898">
<pin name="IN" direction="in"/>
<pin name="/CHG" direction="out"/>
<pin name="EN/OK" direction="in"/>
<pin name="I_SET" direction="pas"/>
<pin name="CT" direction="pas"/>
<pin name="RSTRT" direction="pas"/>
<pin name="BATT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="DRV" direction="out"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="1X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DOT">
</symbol>
<symbol name="CERMOSC">
<pin name="IN"/>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="TRIMPOT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="XTAL">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="ATMEGA32U4">
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="UVCC"/>
<pin name="UGND"/>
<pin name="D-"/>
<pin name="AVCC"/>
<pin name="PB3(PDO/MISO)"/>
<pin name="PB2(PDI/MOSI)"/>
<pin name="PB1(SCK)"/>
<pin name="PB0(SS)"/>
<pin name="PD7(OC4D/ADC10/T0)"/>
<pin name="PD6(T1/ADC9/!OC4D)"/>
<pin name="PD5(XCK/CTS)"/>
<pin name="PD4(ICP1/ADC8)"/>
<pin name="PD3(INT3/TXD1)"/>
<pin name="PD2(INT2/RXD1)"/>
<pin name="PD1(INT1/SDA)"/>
<pin name="PD0(INT0/OC0B/SCL)"/>
<pin name="PC7(ICP3/CLK0/OC4A)"/>
<pin name="PC6(OC3A/!OC4A)"/>
<pin name="PB4(ADC11)"/>
<pin name="PB6(OC1B/OC4B/ADC13)"/>
<pin name="PB5(OC1A/ADC12/!OC4B)"/>
<pin name="PB7(OC0A/OC1C/RTS)"/>
<pin name="/RESET" function="dot"/>
<pin name="D+"/>
<pin name="UCAP"/>
<pin name="PE2(!HWB)"/>
<pin name="PF0(ADC0)"/>
<pin name="PF1(ADC1)"/>
<pin name="PF4(ADC4/TCK)"/>
<pin name="PF5(ADC5/TMS)"/>
<pin name="PF6(ADC6/TDO)"/>
<pin name="PF7(ADC7(TDI)"/>
<pin name="PE6(INT.6/AIN0)"/>
<pin name="VBUS"/>
<pin name="GND1"/>
<pin name="AVCC1"/>
<pin name="VCC1"/>
<pin name="AREF"/>
<pin name="GND2"/>
<pin name="GND3"/>
</symbol>
<symbol name="AT90USB162">
<pin name="PC2"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="UVCC"/>
<pin name="UGND"/>
<pin name="D-"/>
<pin name="AVCC"/>
<pin name="PB3(PDO/MISO)"/>
<pin name="PB2(PDI/MISO)"/>
<pin name="PB1(SCK)"/>
<pin name="PB0(SS)"/>
<pin name="PD7(INT7/HWB/CTS/T0)"/>
<pin name="PD6(INT6/RTS)"/>
<pin name="PD5(XCK)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT3/TXD1)"/>
<pin name="PD2(INT2/AIN1/RXD1)"/>
<pin name="PD1(INT1/AIN0)"/>
<pin name="PD0(INT0/OC0B)"/>
<pin name="PC7(ICP1/INT4)"/>
<pin name="PC6(OC1A)"/>
<pin name="PC5(OC1B)"/>
<pin name="PC4"/>
<pin name="PB4(T1)"/>
<pin name="PB6"/>
<pin name="PB5"/>
<pin name="PB7(OC0A/OC1C)"/>
<pin name="PC1(/RESET)" function="dot"/>
<pin name="D+"/>
<pin name="UCAP"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="AAA">
<pin name="-"/>
<pin name="+"/>
</symbol>
<symbol name="SIS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SPK">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="555">
<pin name="TR" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="R" direction="in" function="dot"/>
<pin name="CV" direction="in"/>
<pin name="THR" direction="in"/>
<pin name="DIS" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="RGBLED_CC">
<pin name="BLUE"/>
<pin name="GREEN"/>
<pin name="GND"/>
<pin name="RED"/>
</symbol>
<symbol name="FB">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PINHD1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PNA460XM">
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PROPPLUG">
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="RST" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="RGBLED_CA">
<pin name="BLUE"/>
<pin name="GREEN"/>
<pin name="VCC"/>
<pin name="RED"/>
</symbol>
<symbol name="SP">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="GLCD">
<pin name="K" direction="in"/>
<pin name="A" direction="sup"/>
<pin name="VEE" direction="sup"/>
<pin name="/RST" direction="in"/>
<pin name="CS0" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="E" direction="in"/>
<pin name="RW" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VO" direction="in"/>
<pin name="VDD" direction="sup"/>
<pin name="VSS" direction="sup"/>
</symbol>
<symbol name="3V">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="+1" direction="pas"/>
</symbol>
<symbol name="LS026">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="GND" direction="sup"/>
<pin name="VBIAS" direction="sup"/>
</symbol>
<symbol name="MAX6921">
<pin name="OUT0" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="OUT9" direction="out"/>
<pin name="OUT10" direction="out"/>
<pin name="OUT11" direction="out"/>
<pin name="OUT12" direction="out"/>
<pin name="OUT13" direction="out"/>
<pin name="OUT14" direction="out"/>
<pin name="OUT15" direction="out"/>
<pin name="OUT16" direction="out"/>
<pin name="OUT17" direction="out"/>
<pin name="OUT18" direction="out"/>
<pin name="OUT19" direction="out"/>
<pin name="VBB" direction="sup"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="sup"/>
<pin name="BLANK" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="LOAD" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
</symbol>
<symbol name="DS1307">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="SQW/OUT"/>
<pin name="VCC" direction="pwr"/>
<pin name="X1" direction="pas"/>
<pin name="X2" direction="pas"/>
</symbol>
<symbol name="78XX">
<pin name="VI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
</symbol>
<symbol name="MC33340/2">
<pin name="VSEN" direction="in"/>
<pin name="GATE" direction="out"/>
<pin name="F/T" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="T3" direction="pas"/>
<pin name="T2" direction="pas"/>
<pin name="T1" direction="pas"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LT1173">
<pin name="ILIM" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="AO" direction="out"/>
<pin name="FB" direction="sup"/>
<pin name="SW2" direction="pas"/>
<pin name="SET" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SW1" direction="pas"/>
</symbol>
<symbol name="MAX756">
<pin name="LBI" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="REF" direction="pas"/>
<pin name="LBO" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="3/5"/>
<pin name="/SHDN" direction="in"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="MAX757">
<pin name="LBI" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="REF" direction="pas"/>
<pin name="LBO" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="FB"/>
<pin name="/SHDN" direction="in"/>
<pin name="LX" direction="out"/>
</symbol>
<symbol name="LT1302">
<pin name="VIN" direction="in"/>
<pin name="SW" direction="in"/>
<pin name="PGND" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="VC" direction="pas"/>
<pin name="SNS" direction="pas"/>
<pin name="SHDN" direction="in"/>
<pin name="IT" direction="in"/>
</symbol>
<symbol name="L">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="IGFET-EN-GDS">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="74125">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ARDUINO">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="/RESET"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="TS">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SD-MMC">
<pin name="CS" direction="in"/>
<pin name="DATA_IN" direction="in"/>
<pin name="VSS1" direction="sup"/>
<pin name="VDD" direction="sup"/>
<pin name="SCLK" direction="in"/>
<pin name="VSS2" direction="sup"/>
<pin name="DATA_OUT" direction="out"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="WRITE_PROTECT" direction="pas"/>
<pin name="CARD_DETECT" direction="pas"/>
<pin name="COMMON_SW" direction="pas"/>
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="SW">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="POT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="KS-S">
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MCP4921">
<pin name="VDD" direction="sup"/>
<pin name="#CS" direction="in" function="dot"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="DACA" direction="out"/>
<pin name="REFA" direction="in"/>
<pin name="AVSS" direction="sup"/>
</symbol>
<symbol name="MCP4922">
<pin name="VDD" direction="sup"/>
<pin name="#CS" direction="in" function="dot"/>
<pin name="SCK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="LDAC" direction="in" function="dot"/>
<pin name="#SHDN" direction="in" function="dot"/>
<pin name="DACB" direction="out"/>
<pin name="DACA" direction="out"/>
<pin name="REFA" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="AVSS" direction="sup"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="78XX-1">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="1035D">
<pin name="RX0" direction="in"/>
<pin name="TX0" direction="out"/>
<pin name="VBAK" direction="sup"/>
<pin name="GND1" direction="sup"/>
<pin name="VCC" direction="sup"/>
<pin name="PPS" direction="out"/>
<pin name="TX1" direction="out"/>
<pin name="RX1" direction="in"/>
<pin name="BOOTSEL" direction="in"/>
<pin name="ON_OFF" direction="in"/>
<pin name="#RST" direction="in"/>
<pin name="RFPWUP" direction="out"/>
</symbol>
<symbol name="EB-85A">
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="BAT" direction="sup"/>
<pin name="GND1" direction="sup"/>
<pin name="VCC" direction="sup"/>
<pin name="PPS" direction="out"/>
<pin name="TX2" direction="out"/>
<pin name="RX2" direction="in"/>
</symbol>
<symbol name="EM-406A">
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="GND" direction="sup"/>
<pin name="GND1" direction="sup"/>
<pin name="VCC" direction="sup"/>
<pin name="PPS" direction="out"/>
</symbol>
<symbol name="DIN-5">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="TEENSY">
<pin name="GND"/>
<pin name="B0/SS"/>
<pin name="B1/SCK"/>
<pin name="B2/MOSI"/>
<pin name="B3/MISO"/>
<pin name="B7"/>
<pin name="D0/SCL"/>
<pin name="D1/SDA"/>
<pin name="D2/RX"/>
<pin name="D3/TX"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="D5"/>
<pin name="VCC"/>
<pin name="GND1"/>
<pin name="RST"/>
<pin name="D4"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="F7"/>
<pin name="F6"/>
<pin name="F5"/>
<pin name="F4"/>
<pin name="F1"/>
<pin name="F0"/>
<pin name="VCC1"/>
</symbol>
<symbol name="TRANSFLASH">
<pin name="CS" direction="in"/>
<pin name="DATA_IN" direction="in"/>
<pin name="VSS" direction="sup"/>
<pin name="VDD" direction="sup"/>
<pin name="SCLK" direction="in"/>
<pin name="DATA_OUT" direction="out"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="CARD_DETECT" direction="pas"/>
<pin name="GND" direction="sup"/>
<pin name="GND1" direction="sup"/>
<pin name="CARD_DETECT1" direction="pas"/>
</symbol>
<symbol name="LP298X">
<pin name="VOUT"/>
<pin name="VIN"/>
<pin name="GND"/>
<pin name="EN"/>
<pin name="BYP"/>
</symbol>
<symbol name="MCP7386X">
<pin name="VDD" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="PROG" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="THREF" direction="pas"/>
<pin name="THERM" direction="pas"/>
<pin name="TIMER" direction="pas"/>
<pin name="STAT2" direction="out"/>
<pin name="STAT1" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VSET" direction="in"/>
<pin name="VBAT3" direction="in"/>
<pin name="VBAT2" direction="in"/>
<pin name="VBAT1" direction="in"/>
</symbol>
<symbol name="SSM2167">
<pin name="GND" direction="pwr"/>
<pin name="VCA_IN" direction="in"/>
<pin name="SHTDN" direction="in"/>
<pin name="BUFOUT" direction="out"/>
<pin name="INPUT" direction="in"/>
<pin name="AVGCAP" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUTPUT" direction="out"/>
<pin name="CMPRS" direction="pas"/>
<pin name="GATE" direction="pas"/>
</symbol>
<symbol name="ELECTRET">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DCBARREL">
<pin name="PWR" direction="pwr"/>
<pin name="GNDBREAK" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX6675">
<pin name="GND" direction="pwr"/>
<pin name="T-" direction="in"/>
<pin name="T+" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="/CS" direction="in"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="USB-PWR">
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MAX9814">
<pin name="CT"/>
<pin name="/SHDN"/>
<pin name="CG"/>
<pin name="VDD"/>
<pin name="MICOUT"/>
<pin name="GND"/>
<pin name="MICIN"/>
<pin name="A/R"/>
<pin name="GAIN"/>
<pin name="BIAS"/>
<pin name="MICBIAS"/>
<pin name="TH"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="EP"/>
</symbol>
<symbol name="VS1033">
<pin name="SO" direction="out"/>
<pin name="SI" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="/CS" direction="in"/>
<pin name="BSYNC" direction="in"/>
<pin name="/RESET" direction="in"/>
<pin name="DREQ" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND1" direction="pwr"/>
<pin name="DGND2" direction="pwr"/>
<pin name="DGND3" direction="pwr"/>
<pin name="DGND4" direction="pwr"/>
<pin name="DGND5" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="IOVDD1" direction="pwr"/>
<pin name="IOVDD2" direction="pwr"/>
<pin name="CVDD" direction="pwr"/>
<pin name="CVDD1" direction="pwr"/>
<pin name="CVDD2" direction="pwr"/>
<pin name="CVDD3" direction="pwr"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="out"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="LEFT" direction="out"/>
<pin name="RIGHT" direction="out"/>
<pin name="GBUF" direction="out"/>
<pin name="MIC+" direction="in"/>
<pin name="MIC-" direction="in"/>
<pin name="XT1" direction="pas"/>
<pin name="XT2" direction="pas"/>
<pin name="VCO" direction="out"/>
<pin name="GPIO1/I2C_DA"/>
<pin name="GPIO0/I2C_CLK"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="GPIO4/I2C_LROUT"/>
<pin name="GPIO5/I2C_MCLK"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="LINEIN" direction="in"/>
<pin name="RCAP" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="AGND3" direction="pwr"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MCP73833">
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="STAT1" direction="pas"/>
<pin name="STAT2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="PROG" direction="in"/>
<pin name="/PG" direction="pas"/>
<pin name="THERM"/>
<pin name="VBAT2" direction="out"/>
<pin name="VBAT1" direction="out"/>
</symbol>
<symbol name="AVRISP">
<pin name="MISO" direction="in"/>
<pin name="SCK" direction="out"/>
<pin name="RST" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="MOSI" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LT3426">
<pin name="VIN" direction="in"/>
<pin name="/SHDN" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="SW" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="FB" direction="in"/>
</symbol>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MCP2300X">
<pin name="GP0"/>
<pin name="GP1"/>
<pin name="GP2"/>
<pin name="GP3"/>
<pin name="GP4"/>
<pin name="GP5"/>
<pin name="GP6"/>
<pin name="GP7"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="/RST" direction="in"/>
<pin name="INT" direction="out"/>
</symbol>
<symbol name="TB6612FNG">
<pin name="AO1" direction="out"/>
<pin name="AO1'" direction="out"/>
<pin name="PGND1" direction="pwr"/>
<pin name="PGND1'" direction="pwr"/>
<pin name="AO2" direction="out"/>
<pin name="AO2'" direction="out"/>
<pin name="BO1" direction="out"/>
<pin name="BO1'" direction="out"/>
<pin name="PGND2" direction="pwr"/>
<pin name="PGND2'" direction="pwr"/>
<pin name="BO2" direction="out"/>
<pin name="BO2'" direction="out"/>
<pin name="VM2" direction="pwr"/>
<pin name="VM3" direction="pwr"/>
<pin name="PWMB" direction="in"/>
<pin name="BIN2" direction="in"/>
<pin name="BIN1" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="STBY" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="PWMA" direction="in"/>
<pin name="VM1" direction="pwr"/>
</symbol>
<symbol name="1X5">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="CLCD">
<pin name="K" direction="in"/>
<pin name="A" direction="in"/>
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="E" direction="in"/>
<pin name="RW" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VO" direction="in"/>
<pin name="VDD" direction="sup"/>
<pin name="VSS" direction="sup"/>
</symbol>
<symbol name="SUNLOGO">
</symbol>
<symbol name="IGFPA">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="2X22">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
</symbol>
<symbol name="CHUMBYVIDEO">
<pin name="LCD_YM"/>
<pin name="B0"/>
<pin name="LCD_XP"/>
<pin name="B1"/>
<pin name="LCD_YP"/>
<pin name="B2"/>
<pin name="LRADC0"/>
<pin name="B3"/>
<pin name="KRADC1"/>
<pin name="B4"/>
<pin name="LCD_XM"/>
<pin name="B5"/>
<pin name="R0"/>
<pin name="R1"/>
<pin name="R2"/>
<pin name="RS"/>
<pin name="R3"/>
<pin name="DET"/>
<pin name="R4"/>
<pin name="LINE1_INR"/>
<pin name="R5"/>
<pin name="LINE1_INL"/>
<pin name="G0"/>
<pin name="WE"/>
<pin name="G1"/>
<pin name="CS"/>
<pin name="G2"/>
<pin name="DOTCLK"/>
<pin name="G3"/>
<pin name="LED_A"/>
<pin name="G4"/>
<pin name="LED_K"/>
<pin name="G5"/>
<pin name="RST"/>
<pin name="VSYNC"/>
<pin name="HSYNC"/>
<pin name="3.3V"/>
<pin name="ENA"/>
<pin name="2.5V"/>
<pin name="GND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
</symbol>
<symbol name="1X22">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
</symbol>
<symbol name="PINH2X9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
</symbol>
<symbol name="ILI9325_LCD">
<pin name="DB0" direction="pas"/>
<pin name="DB1" direction="pas"/>
<pin name="DB2" direction="pas"/>
<pin name="DB3" direction="pas"/>
<pin name="GND1" direction="pwr"/>
<pin name="IOVCC1" direction="pwr"/>
<pin name="!CS" direction="pas"/>
<pin name="RS" direction="pas"/>
<pin name="!WR" direction="pas"/>
<pin name="!RD" direction="pas"/>
<pin name="IMO" direction="pas"/>
<pin name="X+" direction="pas"/>
<pin name="Y+" direction="pas"/>
<pin name="X-" direction="pas"/>
<pin name="Y-" direction="pas"/>
<pin name="LED-A" direction="pas"/>
<pin name="LED-K1" direction="pas"/>
<pin name="LED-K2" direction="pas"/>
<pin name="LED-K3" direction="pas"/>
<pin name="LED-K4" direction="pas"/>
<pin name="IM3" direction="pas"/>
<pin name="DB4" direction="pas"/>
<pin name="DB10/DB8" direction="pas"/>
<pin name="DB11/DB9" direction="pas"/>
<pin name="DB12/DB10" direction="pas"/>
<pin name="DB13/DB11" direction="pas"/>
<pin name="DB14/DB12" direction="pas"/>
<pin name="DB15/DB13" direction="pas"/>
<pin name="DB16/DB14" direction="pas"/>
<pin name="DB17/DB15" direction="pas"/>
<pin name="!RESET" direction="pas"/>
<pin name="VCI" direction="pwr"/>
<pin name="IOVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DB5" direction="pas"/>
<pin name="DB6" direction="pas"/>
<pin name="DB7" direction="pas"/>
</symbol>
<symbol name="FUSE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ATMEGA32U2">
<pin name="PC2(AIN2/PCIN11)"/>
<pin name="XTAL2/PC0"/>
<pin name="XTAL1"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="UVCC"/>
<pin name="UGND"/>
<pin name="D-"/>
<pin name="AVCC"/>
<pin name="PB3(PDO/MISO/PCINT3)"/>
<pin name="PB2(PDI/MOSI/PCINT2)"/>
<pin name="PB1(SCK/PCINT1)"/>
<pin name="PB0(SS/PCINT0)"/>
<pin name="PD7(INT7/HWB/AIN6/T0)"/>
<pin name="PD6(INT6/AIN5/RTS)"/>
<pin name="PD5(XCK/AIN4/PCINT12)"/>
<pin name="PD4(INT5/AIN3)"/>
<pin name="PD3(INT3/TXD1)"/>
<pin name="PD2(INT2/AIN1/RXD1)"/>
<pin name="PD1(INT1/AIN0)"/>
<pin name="PD0(INT0/OC0B)"/>
<pin name="PC7(ICP1/INT4/CLKO)"/>
<pin name="PC6(OC1A/PCINT8)"/>
<pin name="PC5(OC1B/PCINT9)"/>
<pin name="PC4(PCINT10)"/>
<pin name="PB4(T1/PCINT4)"/>
<pin name="PB6(PCINT6)"/>
<pin name="PB5(PCINT5)"/>
<pin name="PB7(OC0A/OC1C/PCINT7)"/>
<pin name="/RESET(PC1)" function="dot"/>
<pin name="D+"/>
<pin name="UCAP"/>
</symbol>
<symbol name="PINHD14">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD-1X40">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
</symbol>
<symbol name="PINHD20">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X20">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
</symbol>
<symbol name="TLC5941">
<pin name="OUT0" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="OUT9" direction="out"/>
<pin name="OUT10" direction="out"/>
<pin name="OUT11" direction="out"/>
<pin name="OUT12" direction="out"/>
<pin name="OUT13" direction="out"/>
<pin name="OUT14" direction="out"/>
<pin name="OUT15" direction="out"/>
<pin name="BLANK" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GSCLK" direction="in"/>
<pin name="IREF"/>
<pin name="SCLK" direction="in"/>
<pin name="SIN" direction="in"/>
<pin name="SOUT" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="XLAT" direction="in"/>
<pin name="XERR" direction="out"/>
</symbol>
<symbol name="UG-2864HSWEG01">
<pin name="MT" direction="in"/>
<pin name="C2P" direction="in"/>
<pin name="C2N" direction="in"/>
<pin name="C1P" direction="in"/>
<pin name="C1N" direction="in"/>
<pin name="VBAT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="BS0" direction="in"/>
<pin name="BS1" direction="in"/>
<pin name="BS2" direction="in"/>
<pin name="/CS" direction="in"/>
<pin name="/RES" direction="in"/>
<pin name="D/C" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="E/RD" direction="in"/>
<pin name="D0/DI"/>
<pin name="D1/SCLK"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="IREF" direction="in"/>
<pin name="VCOMH" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VLSS" direction="pwr"/>
<pin name="MT2" direction="in"/>
</symbol>
<symbol name="PINH2X14">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
</symbol>
<symbol name="PV">
<pin name="MSV" direction="pas"/>
</symbol>
<symbol name="P">
<pin name="MS" direction="pas"/>
</symbol>
<symbol name="F15">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="MV">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="MC33063">
<pin name="SWC" direction="in"/>
<pin name="SWE" direction="in"/>
<pin name="TC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="IPK"/>
<pin name="DC" direction="in"/>
</symbol>
<symbol name="PINHD15">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
</symbol>
<symbol name="MCP73811/2">
<pin name="CE" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VBAT"/>
<pin name="VDD" direction="pwr"/>
<pin name="PROG" direction="in"/>
</symbol>
<symbol name="MCP73831/2">
<pin name="STAT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VBAT"/>
<pin name="VDD" direction="pwr"/>
<pin name="PROG" direction="in"/>
</symbol>
<symbol name="S-35390A">
<pin name="/INT1" direction="out"/>
<pin name="XTALO" direction="out"/>
<pin name="XTALI" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="/INT2" direction="out"/>
</symbol>
<symbol name="ISL1209">
<pin name="XTALI" direction="in"/>
<pin name="XTALO" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="EVIN" direction="in"/>
<pin name="EVDET" direction="out"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="/IRQ" direction="out"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="XTAL-4">
<pin name="X1"/>
<pin name="X2"/>
<pin name="G1" direction="pwr"/>
<pin name="G2" direction="pwr"/>
</symbol>
<symbol name="USB-4">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="10F200T">
<pin name="GP0"/>
<pin name="VSS" direction="pwr"/>
<pin name="GP1"/>
<pin name="GP2"/>
<pin name="VDD" direction="pwr"/>
<pin name="GP3"/>
</symbol>
<symbol name="ATTINY10">
<pin name="PB0"/>
<pin name="GND" direction="pwr"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="VCC" direction="pwr"/>
<pin name="/RST"/>
</symbol>
<symbol name="1X4">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="HL1606">
<pin name="A3" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="SI" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="LI" direction="in"/>
<pin name="CI" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="CO" direction="out"/>
<pin name="DO" direction="out"/>
<pin name="SO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="B3" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B1" direction="out"/>
</symbol>
<symbol name="SPST">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="JD-T1800">
<pin name="GND" direction="pwr"/>
<pin name="LEDK" direction="in"/>
<pin name="LEDA" direction="in"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="RS/DC" direction="in"/>
<pin name="DATA"/>
<pin name="CLOCK" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="GND1" direction="pwr"/>
</symbol>
<symbol name="ADXL33X">
<pin name="ST" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="GND1" direction="sup"/>
<pin name="GND2" direction="sup"/>
<pin name="GND3" direction="sup"/>
<pin name="XOUT" direction="out"/>
<pin name="YOUT" direction="out"/>
<pin name="ZOUT" direction="out"/>
<pin name="VS" direction="sup"/>
<pin name="VS1" direction="sup"/>
</symbol>
<symbol name="NAVSWITCH">
<pin name="E"/>
<pin name="D"/>
<pin name="C"/>
<pin name="A"/>
<pin name="B"/>
<pin name="COM2"/>
<pin name="COM1"/>
<pin name="COM3"/>
</symbol>
<symbol name="RN-171">
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
<pin name="GND7" direction="pwr"/>
<pin name="GND8" direction="pwr"/>
<pin name="SENSOR0" direction="in"/>
<pin name="SENSOR1" direction="in"/>
<pin name="SENSOR2" direction="in"/>
<pin name="SENSOR3" direction="in"/>
<pin name="SENSOR4" direction="in"/>
<pin name="SENSOR5" direction="in"/>
<pin name="SENSOR6" direction="in"/>
<pin name="SENSOR7" direction="in"/>
<pin name="GND9" direction="pwr"/>
<pin name="SENSOR_PWR" direction="pwr"/>
<pin name="VDD_RF" direction="pwr"/>
<pin name="VDD_SW" direction="nc"/>
<pin name="MOSI" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="/FLASH_CS" direction="in"/>
<pin name="GND10" direction="pwr"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="GPIO8"/>
<pin name="GPIO9"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="GND11" direction="pwr"/>
<pin name="VBATT" direction="in"/>
<pin name="BOOST_CTRL" direction="out"/>
<pin name="GPIO10"/>
<pin name="GPIO11"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14" direction="nc"/>
<pin name="GND12" direction="pwr"/>
<pin name="FORCE_AWAKE" direction="in"/>
<pin name="/RESET" direction="in"/>
<pin name="VDD_3V3" direction="pwr"/>
<pin name="ANTENNA" direction="out"/>
</symbol>
<symbol name="PINHD18">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
</symbol>
<symbol name="ANT">
<pin name="FEED" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="ANTENNA">
</symbol>
<symbol name="74245">
<pin name="DIR" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="PINHD13">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
</symbol>
<symbol name="MCP73871">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="VPCC" direction="in"/>
<pin name="/PG" direction="out"/>
<pin name="STAT2" direction="out"/>
<pin name="STAT1/LBO" direction="out"/>
<pin name="SEL" direction="in"/>
<pin name="PROG2" direction="in"/>
<pin name="/TE" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="PROG3" direction="in"/>
<pin name="PROG1" direction="in"/>
<pin name="THERM" direction="in"/>
<pin name="VBAT3" direction="out"/>
<pin name="VBAT2" direction="out"/>
<pin name="VBAT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
</symbol>
<symbol name="RESET_SUPERVISOR">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="/RESET" direction="out"/>
</symbol>
<symbol name="XBEE">
<pin name="VCC" direction="sup"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="DO8" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="PWM0/RSSI" direction="out"/>
<pin name="PWM1" direction="out"/>
<pin name="RESERVED" direction="nc"/>
<pin name="DTR/DI8" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="AD4/DIO4"/>
<pin name="CTS/DIO7"/>
<pin name="ON/SLEEP" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="ASC/AD5/DIO5"/>
<pin name="RTS/AD6/DIO6"/>
<pin name="AD3/DIO3"/>
<pin name="AD2/DIO2"/>
<pin name="AD1/DIO1"/>
<pin name="AD0/DIO0"/>
</symbol>
<symbol name="TXS0102">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="OE"/>
</symbol>
<symbol name="TXB0104PWR">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="OE"/>
</symbol>
<symbol name="TXB0108PWR">
<pin name="VCCA"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GND"/>
<pin name="VCCB"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="OE"/>
</symbol>
<symbol name="JOYSTICK">
<pin name="V+"/>
<pin name="V"/>
<pin name="V-"/>
<pin name="H+"/>
<pin name="H"/>
<pin name="H-"/>
<pin name="SEL+"/>
<pin name="SEL-"/>
</symbol>
<symbol name="SEGMENT_8X8_BICOLOR_CATHODEROW">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
</symbol>
<symbol name="SEGMENT_8X8_CATHODEROW">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
</symbol>
<symbol name="SEGMENT_12BAR_BICOLOR_CATHODEROW">
<pin name="K1"/>
<pin name="K2"/>
<pin name="K3"/>
<pin name="K4"/>
<pin name="K5"/>
<pin name="K6"/>
<pin name="K7"/>
<pin name="K8"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
</symbol>
<symbol name="SEGMENT_8X8_15_CATHODEROW">
</symbol>
<symbol name="8-STRIP">
<pin name="P$1"/>
</symbol>
<symbol name="DS1337">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="#INTA" direction="out"/>
<pin name="SQW/#INTB" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="X1" direction="pas"/>
<pin name="X2" direction="pas"/>
</symbol>
<symbol name="MEGA168">
<pin name="(PCI5/SCK)PB5"/>
<pin name="PB7(XTAL2/TOSC2/PCI7)"/>
<pin name="PB6(XTAL1/TOSC1/PCI6)"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="(PCI4/MISO)PB4"/>
<pin name="(PCI3/MOSI/OC2A)PB3"/>
<pin name="(PCI2/SS/OC1B)PB2"/>
<pin name="(PCI1/OC1A/OC1S)PB1"/>
<pin name="(PCI0/ICP/CLKO)PB0"/>
<pin name="(PCI23/AIN1)PD7"/>
<pin name="(PCI22/AIN0OC0A)PD6"/>
<pin name="(PCI21/T1/OC0B)PD5"/>
<pin name="(PCI20/XCK/T0)PD4"/>
<pin name="(PCI19/INT1/OC2B)PD3"/>
<pin name="(PCI18/INT0)PD2"/>
<pin name="(PCI17/TXD)PD1"/>
<pin name="(PCI16/RXD)PD0"/>
<pin name="(PCI13/ADC5/SCL)PC5"/>
<pin name="(PCI12/ADC4/SDA)PC4"/>
<pin name="(PCI11/ADC3)PC3"/>
<pin name="(PCI10/ADC2)PC2"/>
<pin name="(PCI9/ADC1)PC1"/>
<pin name="(PCI8/ADC0)PC0"/>
<pin name="PC6(/RESET/PCI14)" function="dot"/>
</symbol>
<symbol name="DS1302">
<pin name="SCLK" direction="in"/>
<pin name="I/O"/>
<pin name="GND" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="X1" direction="pas"/>
<pin name="X2" direction="pas"/>
</symbol>
<symbol name="SUPERCAP">
</symbol>
<symbol name="TM1804">
<pin name="R" direction="out"/>
<pin name="G" direction="out"/>
<pin name="B" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SET" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="RGBLED">
<pin name="BLUE_C"/>
<pin name="GREEN_C"/>
<pin name="GREEN_A"/>
<pin name="RED_C"/>
<pin name="BLUE_A"/>
<pin name="RED_A"/>
</symbol>
<symbol name="SEWTAP">
<pin name="SEW"/>
</symbol>
<symbol name="MCP23017">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="INTA" direction="out"/>
<pin name="INTB" direction="out"/>
<pin name="GPB0"/>
<pin name="GPB1"/>
<pin name="GPB2"/>
<pin name="GPB3"/>
<pin name="GPB4"/>
<pin name="GPB5"/>
<pin name="GPB6"/>
<pin name="GPB7"/>
<pin name="GPA0"/>
<pin name="GPA1"/>
<pin name="GPA2"/>
<pin name="GPA3"/>
<pin name="GPA4"/>
<pin name="GPA5"/>
<pin name="GPA6"/>
<pin name="GPA7"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="WS2811">
<pin name="R" direction="oc"/>
<pin name="G" direction="oc"/>
<pin name="B" direction="oc"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DIN" direction="in"/>
<pin name="DO" direction="out"/>
<pin name="SET" direction="in"/>
</symbol>
<symbol name="BEAGLEBONE">
<pin name="DGND_1" direction="pwr" function="dot"/>
<pin name="DGND_2" direction="pwr" function="dot"/>
<pin name="VDD5V_1" direction="pwr" function="dot"/>
<pin name="VDD5V_2" direction="pwr" function="dot"/>
<pin name="SYS5V_1" direction="pwr" function="dot"/>
<pin name="SYS5V_2" direction="pwr" function="dot"/>
<pin name="SPIO_CLK" direction="pas" function="dot"/>
<pin name="MCASP0_AHCLKR" direction="pas" function="dot"/>
<pin name="MCASP0_ACLKX" direction="pas" function="dot"/>
<pin name="MCASP0_AXR0" direction="pas" function="dot"/>
<pin name="MCASP0_FSX" direction="pas" function="dot"/>
<pin name="MCASP0_AXR1" direction="pas" function="dot"/>
<pin name="MCASP0_AHCLKX" direction="pas" function="dot"/>
<pin name="GPMC_NCS0" direction="pas" function="dot"/>
<pin name="MCASP0_FSR" direction="pas" function="dot"/>
<pin name="GPIO1_4" direction="pas" function="dot"/>
<pin name="GPMC_NCS1" direction="pas" function="dot"/>
<pin name="GPIO1_2" direction="pas" function="dot"/>
<pin name="GPIO1_3" direction="pas" function="dot"/>
<pin name="GPIO1_0" direction="pas" function="dot"/>
<pin name="GPIO1_1" direction="pas" function="dot"/>
<pin name="UART4_RTSN" direction="pas" function="dot"/>
<pin name="GPMC_CLK" direction="pas" function="dot"/>
<pin name="UART3_RTSN" direction="pas" function="dot"/>
<pin name="ESCAP0_PWMOUT" direction="pas" function="dot"/>
<pin name="UART5_RXD" direction="pas" function="dot"/>
<pin name="UART4_CTSN" direction="pas" function="dot"/>
<pin name="GPIO2_13" direction="pas" function="dot"/>
<pin name="UART3_CTSN" direction="pas" function="dot"/>
<pin name="GPIO2_11" direction="pas" function="dot"/>
<pin name="UART5_TXD" direction="pas" function="dot"/>
<pin name="GPIO2_9" direction="pas" function="dot"/>
<pin name="GPIO_12" direction="pas" function="dot"/>
<pin name="GPIO2_7" direction="pas" function="dot"/>
<pin name="GPIO2_10" direction="pas" function="dot"/>
<pin name="GPIO2_6" direction="pas" function="dot"/>
<pin name="GPIO2_8" direction="pas" function="dot"/>
<pin name="GNDA" direction="pwr" function="dot"/>
<pin name="VDDA" direction="pwr" function="dot"/>
<pin name="AIN0" direction="in" function="dot"/>
<pin name="AIN1" direction="in" function="dot"/>
<pin name="AIN2" direction="in" function="dot"/>
<pin name="AIN3" direction="in" function="dot"/>
<pin name="AIN4" direction="in" function="dot"/>
<pin name="AIN5" direction="in" function="dot"/>
<pin name="AIN6" direction="in" function="dot"/>
<pin name="DGND_3" direction="pwr" function="dot"/>
<pin name="DGND_4" direction="pwr" function="dot"/>
<pin name="VDD3.3V_1" direction="pwr" function="dot"/>
<pin name="VDD3.3V_2" direction="pwr" function="dot"/>
<pin name="SYS_RESETN" direction="pas" function="dot"/>
<pin name="DCAN0_RX" direction="pas" function="dot"/>
<pin name="DCAN0_TX" direction="pas" function="dot"/>
<pin name="SPI0_D0" direction="pas" function="dot"/>
<pin name="EHRPWM1B" direction="pas" function="dot"/>
<pin name="EHRPWM1A" direction="pas" function="dot"/>
<pin name="GPMC_OEN" direction="pas" function="dot"/>
<pin name="GPMC_BE0N" direction="pas" function="dot"/>
<pin name="GPMC_WEN" direction="pas" function="dot"/>
<pin name="GPMC_ADVN_ALE" direction="pas" function="dot"/>
<pin name="GPIO1_5" direction="pas" function="dot"/>
<pin name="GPIO1_6" direction="pas" function="dot"/>
<pin name="GPIO1_7" direction="pas" function="dot"/>
<pin name="GPMC_WPN" direction="pas" function="dot"/>
<pin name="GPMC_WAIT0" direction="pas" function="dot"/>
<pin name="GPMC_NCS2" direction="pas" function="dot"/>
<pin name="GPMC_BE1N" direction="pas" function="dot"/>
<pin name="XDMA_EVENT_INTR1" direction="pas" function="dot"/>
<pin name="LCD_VSYNC" direction="pas" function="dot"/>
<pin name="LCD_PCLK" direction="pas" function="dot"/>
<pin name="LCD_AC_BIAS_EN" direction="pas" function="dot"/>
<pin name="LCD_HSYNC" direction="pas" function="dot"/>
<pin name="EHRPWM2B" direction="pas" function="dot"/>
<pin name="EHRPWM2A" direction="pas" function="dot"/>
<pin name="GPIO0_27" direction="pas" function="dot"/>
<pin name="GPIO0_26" direction="pas" function="dot"/>
<pin name="GPIO1_13" direction="pas" function="dot"/>
<pin name="GPIO1_12" direction="pas" function="dot"/>
<pin name="GPIO1_15" direction="pas" function="dot"/>
<pin name="GPIO1_14" direction="pas" function="dot"/>
<pin name="UART5_CTSN" direction="pas" function="dot"/>
<pin name="UART5_RTSN" direction="pas" function="dot"/>
<pin name="DCAN1_RX" direction="pas" function="dot"/>
<pin name="DCAN1_TX" direction="pas" function="dot"/>
<pin name="PWR_BUT" direction="pas" function="dot"/>
<pin name="I2C1_SDA" direction="pas" function="dot"/>
<pin name="I2C1_SCL" direction="pas" function="dot"/>
<pin name="DGND_5" direction="pwr" function="dot"/>
<pin name="DGND_6" direction="pwr" function="dot"/>
<pin name="DGND_7" direction="pwr" function="dot"/>
<pin name="DGND_8" direction="pwr" function="dot"/>
<pin name="DGND_9" direction="pwr" function="dot"/>
</symbol>
<symbol name="A1171">
<pin name="VOUTPS" direction="out"/>
<pin name="VOUTPN" direction="out"/>
<pin name="SELECT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="2N7002">
</symbol>
<symbol name="MOSFET-N">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="AT45DBXXX">
<pin name="SI" direction="in"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="/RST" direction="in" function="dot"/>
<pin name="/CS" direction="in" function="dot"/>
<pin name="/WP" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SO" direction="out"/>
</symbol>
<symbol name="ARDUINOR3">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF"/>
<pin name="A5/SCL"/>
<pin name="A4/SDA"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="/RESET"/>
<pin name="IOREF" direction="out"/>
<pin name="RESERVED" direction="nc"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="CHARLCD_RGB">
<pin name="RED" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="E" direction="in"/>
<pin name="RW" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="VO" direction="in"/>
<pin name="VDD" direction="sup"/>
<pin name="VSS" direction="sup"/>
<pin name="GREEN" direction="in"/>
<pin name="BLUE" direction="in"/>
</symbol>
<symbol name="TRIM">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="HUB75_IDC">
<pin name="RED1" direction="in"/>
<pin name="GREEN1" direction="in"/>
<pin name="GREEN2" direction="in"/>
<pin name="ADDR_B" direction="in"/>
<pin name="LATCH" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="BLUE1" direction="in"/>
<pin name="RED2" direction="in"/>
<pin name="BLUE2" direction="in"/>
<pin name="ADDR_A" direction="in"/>
<pin name="ADDR_C" direction="in"/>
<pin name="CLOCK" direction="in" function="clk"/>
<pin name="/ENABLE" direction="in" function="dot"/>
<pin name="GND1" direction="pwr"/>
</symbol>
<symbol name="DS3231">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="/RST" direction="pas" function="dot"/>
<pin name="VBAT" direction="pwr"/>
<pin name="32KHZ" direction="out"/>
<pin name="SQW/INT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC5" direction="nc"/>
<pin name="NC6" direction="nc"/>
<pin name="NC7" direction="nc"/>
</symbol>
<symbol name="HUB08_IDC">
<pin name="RED" direction="in"/>
<pin name="GREEN" direction="in"/>
<pin name="ADDR_B" direction="in"/>
<pin name="LATCH" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="BLUE" direction="in"/>
<pin name="ADDR_A" direction="in"/>
<pin name="ADDR_C" direction="in"/>
<pin name="CLOCK" direction="in" function="clk"/>
<pin name="/ENABLE" direction="in" function="dot"/>
<pin name="GND1" direction="pwr"/>
<pin name="ADDR_D" direction="in"/>
<pin name="GND4" direction="pwr"/>
<pin name="N/C" direction="nc"/>
</symbol>
<symbol name="MAX486X">
<pin name="IN" direction="in"/>
<pin name="GATEP" direction="out"/>
<pin name="GATEN" direction="out"/>
<pin name="/EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="FLAG" direction="out"/>
</symbol>
<symbol name="P-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="SEWTAP_2.0">
</symbol>
<symbol name="BEAGLEBONE-1">
<pin name="GND@1" direction="pwr" function="dot"/>
<pin name="GND@2" direction="pwr" function="dot"/>
<pin name="VDD_3V3EXP@1" direction="pwr" function="dot"/>
<pin name="VDD_3V3EXP@2" direction="pwr" function="dot"/>
<pin name="VDD_5V@1" direction="pwr" function="dot"/>
<pin name="VDD_5V@2" direction="pwr" function="dot"/>
<pin name="SYS_5V@1" direction="pwr" function="dot"/>
<pin name="SYS_5V@2" direction="pas" function="dot"/>
<pin name="PWR_BUT" direction="pas" function="dot"/>
<pin name="SYS_RESETN" direction="pas" function="dot"/>
<pin name="UART4_RXD" direction="pas" function="dot"/>
<pin name="GPIO1_28" direction="pas" function="dot"/>
<pin name="UART4_TXD" direction="pas" function="dot"/>
<pin name="EHRPWM1A" direction="pas" function="dot"/>
<pin name="GPIO1_16" direction="pas" function="dot"/>
<pin name="EHRPWM1B" direction="pas" function="dot"/>
<pin name="I2C1_SCL" direction="pas" function="dot"/>
<pin name="I2C1_SDA" direction="pas" function="dot"/>
<pin name="I2C2_SCL" direction="pas" function="dot"/>
<pin name="I2C2_SDA" direction="pas" function="dot"/>
<pin name="UART2_TXD" direction="pas" function="dot"/>
<pin name="UART2_RXD" direction="pas" function="dot"/>
<pin name="GPIO1_17" direction="pas" function="dot"/>
<pin name="UART1_TXD" direction="pas" function="dot"/>
<pin name="GPIO3_21" direction="pas" function="dot"/>
<pin name="UART1_RXD" direction="pas" function="dot"/>
<pin name="GPIO3_19" direction="pas" function="dot"/>
<pin name="SPI1_CS0" direction="pas" function="dot"/>
<pin name="SPI1_DO" direction="pas" function="dot"/>
<pin name="SPI1_DI" direction="pas" function="dot"/>
<pin name="SPI1_SCLK" direction="pas" function="dot"/>
<pin name="VDD_ADC" direction="pas" function="dot"/>
<pin name="AIN4" direction="pas" function="dot"/>
<pin name="GNDA_ADC" direction="pas" function="dot"/>
<pin name="AIN6" direction="pas" function="dot"/>
<pin name="AIN5" direction="pas" function="dot"/>
<pin name="AIN2" direction="pas" function="dot"/>
<pin name="AIN3" direction="pas" function="dot"/>
<pin name="AIN0" direction="pwr" function="dot"/>
<pin name="AIN1" direction="pas" function="dot"/>
<pin name="CLKOUT2" direction="in" function="dot"/>
<pin name="GPIO0_7" direction="pas" function="dot"/>
<pin name="GND@3" direction="pwr" function="dot"/>
<pin name="GND@5" direction="pwr" function="dot"/>
<pin name="GND@4" direction="pwr" function="dot"/>
<pin name="GND@6" direction="pwr" function="dot"/>
<pin name="GND@7" direction="pwr" function="dot"/>
<pin name="GND@8" direction="pwr" function="dot"/>
<pin name="GPIO1_6" direction="pas" function="dot"/>
<pin name="GPIO1_7" direction="pas" function="dot"/>
<pin name="GPIO1_2" direction="pas" function="dot"/>
<pin name="GPIO1_3" direction="pas" function="dot"/>
<pin name="TIMER4" direction="pas" function="dot"/>
<pin name="TIMER7" direction="pas" function="dot"/>
<pin name="TIMER5" direction="pas" function="dot"/>
<pin name="TIMER6" direction="pas" function="dot"/>
<pin name="GPIO1_13" direction="pas" function="dot"/>
<pin name="GPIO1_12" direction="pas" function="dot"/>
<pin name="EHRPWM2B" direction="pas" function="dot"/>
<pin name="GPIO0_26" direction="pas" function="dot"/>
<pin name="GPIO1_15" direction="pas" function="dot"/>
<pin name="GPIO1_14" direction="pas" function="dot"/>
<pin name="GPIO0_27" direction="pas" function="dot"/>
<pin name="GPIO2_1" direction="pas" function="dot"/>
<pin name="EHRPWM2A" direction="pas" function="dot"/>
<pin name="GPIO1_31" direction="pas" function="dot"/>
<pin name="GPIO1_30" direction="pas" function="dot"/>
<pin name="GPIO1_5" direction="pas" function="dot"/>
<pin name="GPIO1_4" direction="pas" function="dot"/>
<pin name="GPIO1_1" direction="pas" function="dot"/>
<pin name="GPIO1_0" direction="pas" function="dot"/>
<pin name="GPIO1_29" direction="pas" function="dot"/>
<pin name="GPIO2_22" direction="pas" function="dot"/>
<pin name="GPIO2_24" direction="pas" function="dot"/>
<pin name="GPIO2_23" direction="pas" function="dot"/>
<pin name="GPIO2_25" direction="pas" function="dot"/>
<pin name="UART5_CTSN" direction="pas" function="dot"/>
<pin name="UART5_RTSN" direction="pas" function="dot"/>
<pin name="UART4_RTSN" direction="pas" function="dot"/>
<pin name="UART3_RTSN" direction="pas" function="dot"/>
<pin name="UART4_CTSN" direction="pas" function="dot"/>
<pin name="UART3_CTSN" direction="pas" function="dot"/>
<pin name="UART5_TXD" direction="pas" function="dot"/>
<pin name="UART5_RXD" direction="pas" function="dot"/>
<pin name="GPIO2_12" direction="pas" function="dot"/>
<pin name="GPIO2_13" direction="pas" function="dot"/>
<pin name="GPIO2_10" direction="pas" function="dot"/>
<pin name="GPIO2_11" direction="pas" function="dot"/>
<pin name="GPIO2_8" direction="pas" function="dot"/>
<pin name="GPIO2_9" direction="pas" function="dot"/>
<pin name="GPIO2_6" direction="pas" function="dot"/>
<pin name="GPIO2_7" direction="pas" function="dot"/>
</symbol>
<symbol name="ARDUINOR3-NOIOREF">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF"/>
<pin name="A5/SCL"/>
<pin name="A4/SDA"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="/RESET"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="FGPMMOPA6B">
<pin name="VCC"/>
<pin name="ENABLE"/>
<pin name="GND@1"/>
<pin name="VBACKUP"/>
<pin name="3D-FIX"/>
<pin name="DPLUS"/>
<pin name="DMINUS"/>
<pin name="GND@2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
</symbol>
<symbol name="FGPMMOPA6C">
<pin name="VCC"/>
<pin name="NC@1"/>
<pin name="GND@1"/>
<pin name="VBACKUP"/>
<pin name="3D-FIX"/>
<pin name="1PPS"/>
<pin name="NC@2"/>
<pin name="GND@2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="NC@5"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
</symbol>
<symbol name="PINH2X4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="ARDUINOMICRO">
<pin name="12"/>
<pin name="11"/>
<pin name="10"/>
<pin name="9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="GND@1"/>
<pin name="R@2"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SS"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="9V"/>
<pin name="GND"/>
<pin name="R@1"/>
<pin name="5V"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="AREF"/>
<pin name="3V"/>
<pin name="13"/>
</symbol>
<symbol name="SPRINGTERMININAL-1X17">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="'1" direction="pas"/>
<pin name="'2" direction="pas"/>
<pin name="'3" direction="pas"/>
<pin name="'4" direction="pas"/>
<pin name="'5" direction="pas"/>
<pin name="'6" direction="pas"/>
<pin name="'7" direction="pas"/>
<pin name="'8" direction="pas"/>
<pin name="'9" direction="pas"/>
<pin name="'10" direction="pas"/>
<pin name="'11" direction="pas"/>
<pin name="'12" direction="pas"/>
<pin name="'13" direction="pas"/>
<pin name="'14" direction="pas"/>
<pin name="'15" direction="pas"/>
<pin name="'16" direction="pas"/>
<pin name="'17" direction="pas"/>
</symbol>
<symbol name="PCA9865">
<pin name="PWM0" direction="out"/>
<pin name="PWM1" direction="out"/>
<pin name="PWM2" direction="out"/>
<pin name="PWM3" direction="out"/>
<pin name="PWM4" direction="out"/>
<pin name="PWM5" direction="out"/>
<pin name="PWM6" direction="out"/>
<pin name="PWM7" direction="out"/>
<pin name="PWM8" direction="out"/>
<pin name="PWM9" direction="out"/>
<pin name="PWM10" direction="out"/>
<pin name="PWM11" direction="out"/>
<pin name="PWM12" direction="out"/>
<pin name="PWM13" direction="out"/>
<pin name="PWM14" direction="out"/>
<pin name="PWM15" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="#OE" direction="in"/>
<pin name="EXTCLK" direction="in"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="FGPMMOPA6H">
<pin name="VCC"/>
<pin name="NRESET"/>
<pin name="GND@1"/>
<pin name="VBACKUP"/>
<pin name="3D-FIX"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="GND@2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="EX_ANT"/>
<pin name="GND@3"/>
<pin name="1PPS"/>
<pin name="RTCM"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
<pin name="NC@5"/>
<pin name="NC@6"/>
<pin name="GND@4"/>
<pin name="NC@7"/>
</symbol>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MCP3008">
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="DOUT" direction="out"/>
<pin name="DIN" direction="in"/>
<pin name="/CS" direction="in" function="dot"/>
</symbol>
<symbol name="AT42QT1070">
<pin name="VDD" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="G_OUT" direction="oc"/>
<pin name="OUT1" direction="oc"/>
<pin name="OUT2" direction="oc"/>
<pin name="OUT3" direction="oc"/>
<pin name="OUT4" direction="oc"/>
<pin name="G_IN" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="ARDUINOR3-ICSP">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF"/>
<pin name="A5/SCL"/>
<pin name="A4/SDA"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="/RESET"/>
<pin name="IOREF" direction="out"/>
<pin name="RESERVED" direction="nc"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="MISO" direction="pas"/>
<pin name="5V@1" direction="pas"/>
<pin name="MOSI" direction="pas"/>
<pin name="GND@3" direction="pas"/>
<pin name="SCK" direction="pas"/>
<pin name="RST" direction="pas"/>
</symbol>
<symbol name="4093">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="PWRN-1">
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="TLC5947">
<pin name="OUT0" direction="oc"/>
<pin name="OUT1" direction="oc"/>
<pin name="OUT2" direction="oc"/>
<pin name="OUT3" direction="oc"/>
<pin name="OUT4" direction="oc"/>
<pin name="OUT5" direction="oc"/>
<pin name="OUT6" direction="oc"/>
<pin name="OUT7" direction="oc"/>
<pin name="OUT8" direction="oc"/>
<pin name="OUT9" direction="oc"/>
<pin name="OUT10" direction="oc"/>
<pin name="OUT11" direction="oc"/>
<pin name="OUT12" direction="oc"/>
<pin name="OUT13" direction="oc"/>
<pin name="OUT14" direction="oc"/>
<pin name="OUT15" direction="oc"/>
<pin name="BLANK" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="IREF"/>
<pin name="SCLK" direction="in"/>
<pin name="SIN" direction="in"/>
<pin name="SOUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="XLAT" direction="in"/>
<pin name="OUT16" direction="oc"/>
<pin name="OUT17" direction="oc"/>
<pin name="OUT18" direction="oc"/>
<pin name="OUT19" direction="oc"/>
<pin name="OUT20" direction="oc"/>
<pin name="OUT21" direction="oc"/>
<pin name="OUT22" direction="oc"/>
<pin name="OUT23" direction="oc"/>
</symbol>
<symbol name="THERMAL_PAD">
<pin name="PAD" direction="pas"/>
</symbol>
<symbol name="TLC59711">
<pin name="OUTR0" direction="oc"/>
<pin name="OUTG0" direction="oc"/>
<pin name="OUTB0" direction="oc"/>
<pin name="OUTR1" direction="oc"/>
<pin name="OUTG1" direction="oc"/>
<pin name="OUTB1" direction="oc"/>
<pin name="OUTR2" direction="oc"/>
<pin name="OUTG2" direction="oc"/>
<pin name="OUTB2" direction="oc"/>
<pin name="OUTR3" direction="oc"/>
<pin name="OUTG3" direction="oc"/>
<pin name="OUTB3" direction="oc"/>
<pin name="GND" direction="pwr"/>
<pin name="IREF"/>
<pin name="SCKI" direction="in"/>
<pin name="SDTI" direction="in"/>
<pin name="SDTO" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCKO" direction="out"/>
<pin name="VREG"/>
</symbol>
<symbol name="WS2812">
<pin name="VDD" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="out"/>
<pin name="LEDVDD" direction="pwr"/>
</symbol>
<symbol name="74AHC1G125">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="!OE" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="1SS309">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="C"/>
</symbol>
<symbol name="WS2812B">
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="VDD"/>
<pin name="GND"/>
</symbol>
<symbol name="U.FL">
<pin name="GND@0" direction="pas"/>
<pin name="SIGNAL" direction="pas"/>
<pin name="GND@1" direction="pas"/>
</symbol>
<symbol name="SMACONNECTOR">
<pin name="ANT"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
</symbol>
<symbol name="TFT_2.83IN_240X320_50PIN">
<pin name="LEDK"/>
<pin name="LEDA@1"/>
<pin name="LEDA@2"/>
<pin name="LEDA@3"/>
<pin name="LEDA@4"/>
<pin name="IM0"/>
<pin name="IM1"/>
<pin name="IM2"/>
<pin name="IM3"/>
<pin name="RESET"/>
<pin name="VSYNC"/>
<pin name="HSYNC"/>
<pin name="DOTCLK"/>
<pin name="DE"/>
<pin name="DB17"/>
<pin name="DB16"/>
<pin name="DB15"/>
<pin name="DB14"/>
<pin name="DB13"/>
<pin name="DB12"/>
<pin name="DB11"/>
<pin name="DB10"/>
<pin name="DB9"/>
<pin name="DB8"/>
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="#RD"/>
<pin name="#WR"/>
<pin name="RS"/>
<pin name="#CS"/>
<pin name="TE"/>
<pin name="IOVCC@1"/>
<pin name="IOVCC@2"/>
<pin name="VCI"/>
<pin name="GND@1"/>
<pin name="XR"/>
<pin name="YD"/>
<pin name="XL"/>
<pin name="YU"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
</symbol>
<symbol name="TFT_CTP28_240X320_50PIN">
<pin name="LEDK"/>
<pin name="LEDA@1"/>
<pin name="LEDA@2"/>
<pin name="LEDA@3"/>
<pin name="LEDA@4"/>
<pin name="IM0"/>
<pin name="IM1"/>
<pin name="IM2"/>
<pin name="IM3"/>
<pin name="/RESET"/>
<pin name="VSYNC"/>
<pin name="HSYNC"/>
<pin name="DOTCLK"/>
<pin name="DE"/>
<pin name="DB17"/>
<pin name="DB16"/>
<pin name="DB15"/>
<pin name="DB14"/>
<pin name="DB13"/>
<pin name="DB12"/>
<pin name="DB11"/>
<pin name="DB10"/>
<pin name="DB9"/>
<pin name="DB8"/>
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="SDO"/>
<pin name="SDI"/>
<pin name="/RD"/>
<pin name="/WR_RS"/>
<pin name="RS_SCL"/>
<pin name="/CS"/>
<pin name="TE"/>
<pin name="IOVCC@1"/>
<pin name="IOVCC@2"/>
<pin name="VCI"/>
<pin name="GND@1"/>
<pin name="TP_SCK"/>
<pin name="TP_SDA"/>
<pin name="TP_IRQ"/>
<pin name="TP_RES"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
</symbol>
<symbol name="PROTRINKET">
<pin name="BAT+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="USB" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D8"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="RST" direction="pas"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="AREF" direction="pas"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6" direction="pas"/>
<pin name="A7" direction="pas"/>
</symbol>
<symbol name="ESP8266-12">
<pin name="RESET" direction="in"/>
<pin name="ADC" direction="pas"/>
<pin name="CH_PD" direction="in"/>
<pin name="GPIO16"/>
<pin name="GPIO14"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO15"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
</symbol>
<symbol name="SIM800L">
<pin name="VBAT" direction="pwr"/>
<pin name="VRTC" direction="pwr"/>
<pin name="VEXT" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PWRKEY" direction="in"/>
<pin name="MIC1P" direction="in"/>
<pin name="MIC1N" direction="in"/>
<pin name="SPK1P" direction="out"/>
<pin name="SPK1N" direction="out"/>
<pin name="MIC2P" direction="in"/>
<pin name="MIC2N" direction="in"/>
<pin name="SPK2P/8Ω" direction="out"/>
<pin name="SPK2N" direction="out"/>
<pin name="PCMCLK" direction="out"/>
<pin name="PCMOUT" direction="out"/>
<pin name="PCMSYNC" direction="out"/>
<pin name="PCMIN" direction="in"/>
<pin name="COL4"/>
<pin name="COL1"/>
<pin name="COL2"/>
<pin name="COL3"/>
<pin name="COL0"/>
<pin name="ROW4"/>
<pin name="ROW3"/>
<pin name="ROW2"/>
<pin name="ROW1"/>
<pin name="ROW0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="NETLIGHT" direction="out"/>
<pin name="STATUS" direction="out"/>
<pin name="UART_DTR" direction="in"/>
<pin name="UART_RI" direction="out"/>
<pin name="UART_DCD" direction="in"/>
<pin name="UART_CTS" direction="out"/>
<pin name="UART_RTS" direction="in"/>
<pin name="UART_TXD" direction="out"/>
<pin name="UART_RXD" direction="in"/>
<pin name="VBUS" direction="pwr"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="ADC" direction="in"/>
<pin name="PWM" direction="out"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VSIM" direction="pwr"/>
<pin name="SIM_DATA"/>
<pin name="SIM_CLK" direction="out"/>
<pin name="SIM_RST" direction="out"/>
<pin name="SIMPRE" direction="in"/>
<pin name="ANT"/>
<pin name="FM_ANT_P"/>
<pin name="FM_ANT_N"/>
<pin name="BPI_BUS1" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="ISINK1" direction="in"/>
<pin name="ISINK0" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="SIM808_LITERAL">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VBAT@1" direction="pwr"/>
<pin name="VBAT@2" direction="pwr"/>
<pin name="VBAT@3" direction="pwr"/>
<pin name="VDD_EXT(2.8VOUT)" direction="pwr"/>
<pin name="PWRKEY" direction="in"/>
<pin name="DTR" direction="in"/>
<pin name="RI" direction="out"/>
<pin name="DCD" direction="out"/>
<pin name="CTS" direction="out"/>
<pin name="RTS" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VRTC" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="MIC1P" direction="in"/>
<pin name="MIC1N" direction="in"/>
<pin name="SPK1P" direction="out"/>
<pin name="SPK1N" direction="out"/>
<pin name="ADC1" direction="in"/>
<pin name="ADC2" direction="in"/>
<pin name="VBUS" direction="pwr"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="GND@5" direction="pwr"/>
<pin name="SIM_VDD" direction="pwr"/>
<pin name="SIM_DATA"/>
<pin name="SIM_CLK" direction="out"/>
<pin name="SIM_RST" direction="out"/>
<pin name="SIM_PRE" direction="in"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GPS_RF_IN"/>
<pin name="GND@7" direction="pwr"/>
<pin name="1PPS" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="out"/>
<pin name="GND@8" direction="pwr"/>
<pin name="PWM2" direction="out"/>
<pin name="PWM1" direction="out"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="PCM_SYNC" direction="out"/>
<pin name="PCM_CLK" direction="in"/>
<pin name="PCM_IN" direction="in"/>
<pin name="PCM_OUT" direction="out"/>
<pin name="STATUS" direction="out"/>
<pin name="NETLIGHT" direction="out"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="ANT_BT"/>
<pin name="GND@11" direction="pwr"/>
<pin name="ROW3" direction="out"/>
<pin name="ROW2" direction="out"/>
<pin name="ROW1" direction="out"/>
<pin name="ROW0" direction="out"/>
<pin name="COL3" direction="in"/>
<pin name="COL2" direction="in"/>
<pin name="COL1" direction="in"/>
<pin name="COL0" direction="in"/>
<pin name="RF_SYNC" direction="out"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GSM_RF_IN" direction="in"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
</symbol>
<symbol name="PUSHBUTTON">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="MICROSHIELD">
<pin name="!RESET" direction="in"/>
<pin name="3V" direction="sup"/>
<pin name="AREF" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIOA0"/>
<pin name="GPIOA1"/>
<pin name="GPIOA2"/>
<pin name="GPIOA3"/>
<pin name="GPIOA4"/>
<pin name="GPIOA5"/>
<pin name="GPIOSCK"/>
<pin name="GPIOMOSI"/>
<pin name="GPIOMISO"/>
<pin name="GPIORX"/>
<pin name="GPIOTX"/>
<pin name="NC" direction="pas"/>
<pin name="GPIOSDA"/>
<pin name="GPIOSCL"/>
<pin name="GPIO5"/>
<pin name="GPIO9"/>
<pin name="GPIO6"/>
<pin name="GPIO10"/>
<pin name="GPIO11"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="EN" direction="pas"/>
<pin name="USB" direction="sup"/>
<pin name="VBAT" direction="sup"/>
</symbol>
<symbol name="WS2812BLED">
<pin name="VDD" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="out"/>
</symbol>
<symbol name="OUTLINE">
<description>Board Outline</description>
</symbol>
<symbol name="ARDUINO-X">
<description>The extra pins of the lerger form factors.</description>
<pin name="SCL21"/>
<pin name="SDA20"/>
<pin name="RX119"/>
<pin name="TX118"/>
<pin name="RX217"/>
<pin name="TX216"/>
<pin name="RX315"/>
<pin name="TX314"/>
<pin name="CANTX"/>
<pin name="CANRX"/>
<pin name="A9"/>
<pin name="DAC1"/>
<pin name="DAC0"/>
<pin name="A11"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A10"/>
<pin name="GND1" direction="sup"/>
<pin name="53"/>
<pin name="51"/>
<pin name="49"/>
<pin name="47"/>
<pin name="45"/>
<pin name="39"/>
<pin name="37"/>
<pin name="35"/>
<pin name="33"/>
<pin name="31"/>
<pin name="43"/>
<pin name="41"/>
<pin name="29"/>
<pin name="27"/>
<pin name="25"/>
<pin name="23"/>
<pin name="+5V" direction="sup"/>
<pin name="+5V0" direction="sup"/>
<pin name="22"/>
<pin name="24"/>
<pin name="26"/>
<pin name="28"/>
<pin name="30"/>
<pin name="32"/>
<pin name="34"/>
<pin name="36"/>
<pin name="38"/>
<pin name="40"/>
<pin name="42"/>
<pin name="44"/>
<pin name="46"/>
<pin name="48"/>
<pin name="50"/>
<pin name="52"/>
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LM3622">
<description>National LM3622 li-ion charger
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LM3622"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="#LV" pad="3"/>
<connect gate="G$1" pin="#LVEN" pad="2"/>
<connect gate="G$1" pin="CEL" pad="6"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="EXT" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LVSEL" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1730">
<description>Linear Tech LTC1730 Lipoly charger
&lt;p&gt;By microbuilder.eu&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LTC1730"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="/CHRG" pad="3"/>
<connect gate="G$1" pin="BATT" pad="8"/>
<connect gate="G$1" pin="GATE" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NTC/#SHDN" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="1"/>
<connect gate="G$1" pin="TIMER" pad="5"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC1731" uservalue="yes">
<description>Linear Tech LTC1731 lipoly charger
&lt;p&gt;By microbuilder.eu&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LTC1731"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="/CHRG" pad="2"/>
<connect gate="G$1" pin="BATT" pad="1"/>
<connect gate="G$1" pin="DRV" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="SENSE" pad="8"/>
<connect gate="G$1" pin="TIMER" pad="3"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1811">
<description>Maxim MAX1811 USB li-ion battery charger
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX1811"/>
</gates>
<devices>
<device name="SO8" package="SO08">
<connects>
<connect gate="G$1" pin="/CHG" pad="8"/>
<connect gate="G$1" pin="BATT" pad="5"/>
<connect gate="G$1" pin="EN" pad="7"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND2" pad="6"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="SELI" pad="2"/>
<connect gate="G$1" pin="SELV" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX8601">
<description>Maxim MAX8601 dual USB/DC lipoly battery charger
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX8601"/>
</gates>
<devices>
<device name="" package="TDFN14">
<connects>
<connect gate="G$1" pin="/CHG" pad="11"/>
<connect gate="G$1" pin="/EN" pad="8"/>
<connect gate="G$1" pin="/FLT" pad="14"/>
<connect gate="G$1" pin="/POK" pad="10"/>
<connect gate="G$1" pin="BAT" pad="1"/>
<connect gate="G$1" pin="BAT1" pad="7"/>
<connect gate="G$1" pin="CT" pad="5"/>
<connect gate="G$1" pin="DC" pad="12"/>
<connect gate="G$1" pin="DC2" pad="13"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SETI" pad="2"/>
<connect gate="G$1" pin="THM" pad="3"/>
<connect gate="G$1" pin="USB" pad="9"/>
<connect gate="G$1" pin="USEL" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1N4004" prefix="D">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
General purpose 1N400x type rectifier
&lt;p&gt;(With bigger pads)&lt;/p&gt;
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="1" symbol="D"/>
</gates>
<devices>
<device name="" package="DO41-10">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERMOSCILL" uservalue="yes">
<description>Ceramic oscillator with built in capacitors such as ZTT-12MHz
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAPOSC"/>
</gates>
<devices>
<device name="-THM" package="CERM_OSC">
<connects>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="IN" pad="P$1"/>
<connect gate="G$1" pin="OUT" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CSTCRG" package="CSTCR-G">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AWCSR" package="AWCSR">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EG1213" prefix="S">
<description>&lt;b&gt;E-Switch right-angle slide SPDT&lt;/b&gt; Part #EG1213
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="1" symbol="TSU"/>
<gate name="G$1" symbol="MT"/>
<gate name="G$2" symbol="MT"/>
</gates>
<devices>
<device name="" package="EG1213">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
<connect gate="G$1" pin="MT" pad="MT1"/>
<connect gate="G$2" pin="MT" pad="MT2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.1MMJACK">
<description>2.1mm x 5.5mm THM DC jack with internal switch. Digikey part #PJ-102A, 4UCON part #05537 &lt;br&gt;
2.1mm x 5.5mm SMT DC jack with internal switch. Digikey part #PJ-002A-SMT, 4UCON part #03267
&lt;p&gt;By microbuilder.eu &amp; adafruit.com&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="POWERJACK-1"/>
</gates>
<devices>
<device name="THM" package="PJ-102A">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RING_SW" pad="RING_SW"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="DCJACK_2MM_SMT">
<connects>
<connect gate="G$1" pin="RING" pad="GND"/>
<connect gate="G$1" pin="RING_SW" pad="GNDBREAK"/>
<connect gate="G$1" pin="TIP" pad="PWR2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C-US" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="C0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0504" package="C0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1005" package="C1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210" package="C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1310" package="C1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1608" package="C1608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812" package="C1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825" package="C1825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2012" package="C2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3216" package="C3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3225" package="C3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4532" package="C4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4564" package="C4564">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-024X044" package="C025-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-025X050" package="C025-025X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-030X050" package="C025-030X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-040X050" package="C025-040X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-050X050" package="C025-050X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-060X050" package="C025-060X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C025_050-024X070" package="C025_050-024X070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-025X075" package="C025_050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-035X075" package="C025_050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-045X075" package="C025_050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-055X075" package="C025_050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-024X044" package="C050-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-025X075" package="C050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-045X075" package="C050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-030X075" package="C050-030X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-050X075" package="C050-050X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-055X075" package="C050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-075X075" package="C050-075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050H075X075" package="C050H075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-032X103" package="C075-032X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-042X103" package="C075-042X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-052X106" package="C075-052X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-043X133" package="C102-043X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-054X133" package="C102-054X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-064X133" package="C102-064X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102_152-062X184" package="C102_152-062X184">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-054X183" package="C150-054X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-064X183" package="C150-064X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-072X183" package="C150-072X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-084X183" package="C150-084X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-091X182" package="C150-091X182">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-062X268" package="C225-062X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-074X268" package="C225-074X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-087X268" package="C225-087X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-108X268" package="C225-108X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-113X268" package="C225-113X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-093X316" package="C275-093X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-113X316" package="C275-113X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-134X316" package="C275-134X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-205X316" package="C275-205X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-137X374" package="C325-137X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-162X374" package="C325-162X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-182X374" package="C325-182X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-192X418" package="C375-192X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-203X418" package="C375-203X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-035X075" package="C050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-155X418" package="C375-155X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-063X106" package="C075-063X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-154X316" package="C275-154X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-173X316" package="C275-173X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402K" package="C0402K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603K" package="C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805K" package="C0805K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210K" package="C1210K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812K" package="C1812K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825K" package="C1825K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2220K" package="C2220K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2225K" package="C2225K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CPOL-US" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="CPOL-US"/>
</gates>
<devices>
<device name="CT3216" package="CT3216">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT3528" package="CT3528">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT6032" package="CT6032">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CT7343" package="CT7343">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181A" package="B45181A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181B" package="B45181B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181C" package="B45181C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B45181D" package="B45181D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4" package="TT2D4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D4L" package="TT2D4L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5" package="TT2D5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6" package="TT2D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D6L" package="TT2D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7L" package="TT2D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D7" package="TT2D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D10" package="TT5D10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11" package="TT5D11">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D11L" package="TT5D11L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT6D6" package="TT5D6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D6L" package="TT5D6L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7" package="TT5D7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D7L" package="TT5D7L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9" package="TT5D9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT5D9L" package="TT5D9L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR1" package="ETR1">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR2" package="ETR2">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR3" package="ETR3">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR4" package="ETR4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ETR5" package="ETR5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-35" package="P128-35">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-40" package="P128-40">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-50" package="P128-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P128-60" package="P128-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-45" package="TAP5-45">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-50" package="TAP5-50">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-70" package="TAP5-70">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-60" package="TAP5-60">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TAP5-80" package="TAP5-80">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1R" package="085CS_1R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1W" package="085CS_1W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AR" package="085CS_1AR">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="085CS-1AW" package="085CS_1AW">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2R" package="139CLL-2R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-2W" package="139CLL-2W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3R" package="139CLL-3R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="139CLL-3W" package="139CLL-3W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-0810" package="140CLH-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1010" package="140CLH-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="140CLH-1014" package="140CLH-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-0810" package="150CLZ-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1010" package="150CLZ-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150CLZ-1014" package="150CLZ-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0405" package="153CLV-0405">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0505" package="153CLV-0505">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0605" package="153CLV-0605">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0807" package="153CLV-0807">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-0810" package="153CLV-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1010" package="153CLV-1010">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1012" package="153CLV-1012">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="153CLV-1014" package="153CLV-1014">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0808" package="175TMP-0808">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="175TMP-0810" package="175TMP-0810">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18R" package="A/3216-18R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A/3216-18W" package="A/3216-18W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21R" package="B/3528-21R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B/3528-21W" package="B/3528-21W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28R" package="C/6032-28R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C/6032-28W" package="C/6032-28W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31R" package="D/7343-31R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D/7343-31W" package="D/7343-31W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38R" package="E/7260-38R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E/7260-38W" package="E/7260-38W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12R" package="R/2012-12R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R/2012-12W" package="R/2012-12W">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="PANASONIC_A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B" package="PANASONIC_B">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="PANASONIC_E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F" package="PANASONIC_F">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E1.8-4" package="E1,8-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-20" package="EB20D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-22.5" package="EB22,5D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-25" package="EB25D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-30" package="EB30D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E10-35" package="EB35D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-5AXIAL" package="E15-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-6AXIAL" package="E15-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E15-9AXIAL" package="E15-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2,5-6E" package="E2,5-6E">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-4" package="E2-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2-5" package="E2-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-4V" package="E2,5RE">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5" package="E2,5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-5V" package="E2,5-4R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-6" package="E2,5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E2.5-7" package="E2,5-7">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-10AXIAL" package="E22-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-6AXIAL" package="E22-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E22-9AXIAL" package="E22-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-10AXIAL" package="E25-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E25-9AXIAL" package="E25-9">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-10" package="E3,5-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E3.5-8" package="E3,5-8">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-10AXIAL" package="E30-10">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-12AXIAL" package="E30-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E30-16AXIAL" package="E30-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-12AXIAL" package="E35-12">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-14AXIAL" package="E35-14">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-16AXIAL" package="E35-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E35-18AXIAL" package="E35-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-16AXIAL" package="E45-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-18AXIAL" package="E45-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-21AXIAL" package="E45-21">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-22AXIAL" package="E45-22">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E45-25AXIAL" package="E45-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-10.5" package="E5-10,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-13" package="E5-13">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-4" package="E5-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-5" package="E5-5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-6" package="E5-6">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-8.5" package="E5-8,5">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E5-9VAXIAL" package="E5R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-25AXIAL" package="E50-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E50-30AXIAL" package="E50-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-25AXIAL" package="E55-25">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E55-30AXIAL" package="E55-30">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-16" package="E7,5-16">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E7.5-18" package="E7,5-18">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TT2D5L" package="TT2D5L">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;


- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K&lt;br&gt;

&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="SMT1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD260" package="LD260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR2X5" package="LED2X5">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LSU260" package="LSU260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZR181" package="LZR181">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B152" package="Q62902-B152">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B153" package="Q62902-B153">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B155" package="Q62902-B155">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B156" package="Q62902-B156">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH480" package="SFH480">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH482" package="SFH482">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR5.7X3.2" package="U57X32">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRL80A" package="IRL80A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2" package="P-LCC-2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-TOP" package="OSRAM-MINI-TOP-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDELED" package="OSRAM-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMART-LED" package="SMART-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2-BACK" package="P-LCC-2-TOPLED-RG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICRO-SIDELED" package="MICRO-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0603" package="CHIP-LED0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0805" package="CHIP-LED0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOPLED-SANTANA" package="MINI-TOPLED-SANTANA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED-0603-TTW" package="CHIPLED-0603-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SMARTLED-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMLK34" package="SMLK34">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R-US_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="R0402" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0603" package="R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805W" package="R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1005" package="R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210" package="R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210W" package="R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010W" package="R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012" package="R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012W" package="R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512W" package="R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216" package="R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216W" package="R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225" package="R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225W" package="R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025" package="R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025W" package="R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332" package="R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332W" package="R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M0805" package="M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1206" package="M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1406" package="M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2012" package="M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2309" package="M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3216" package="M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3516" package="M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M5923" package="M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/10" package="0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/12" package="0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/12" package="0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/15" package="0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/3V" package="0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/15" package="0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/5V" package="0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/17" package="0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/22" package="0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/5V" package="0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922/22" package="0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/5V" package="P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/15" package="P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/22" package="P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/7V" package="P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V234/12" package="V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V235/17" package="V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V526-0" package="V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102AX" package="MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922V" package="0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102R" package="MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102W" package="MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204R" package="MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204W" package="MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207R" package="MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207W" package="MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RDH/15" package="RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/2V" package="0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/V" package="0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FLIPFLOP" package="0805-THM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FLIPFLOP7" package="0805-THM-7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/9" package="0207/9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL">
<description>For use by pick and place machines to calibrate the vision/machine, 1mm
&lt;p&gt;By microbuilder.eu&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DOT"/>
</gates>
<devices>
<device name="" package="FIDUCIAL_1MM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;USB Connectors&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;USBMINIB&lt;/b&gt; - Surface Mount Female Mini-B USB Connector 4UConnector: 06564&lt;/p&gt;
&lt;p&gt;By microbuilder.eu&lt;/p&gt;
Thru-hole RA Female Mini-B USB Connector 4UConnector: 18732&lt;/p&gt;
&lt;p&gt;By ladyada.net&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="MINIB" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THM" package="USB-MINIB-THM">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MOLEX" package="USB-MINIB-THM-MOLEX">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1898">
<description>Maxim MAX1898 li-poly battery charger
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX898"/>
</gates>
<devices>
<device name="U" package="UMAX10">
<connects>
<connect gate="G$1" pin="/CHG" pad="2"/>
<connect gate="G$1" pin="BATT" pad="7"/>
<connect gate="G$1" pin="CS" pad="10"/>
<connect gate="G$1" pin="CT" pad="5"/>
<connect gate="G$1" pin="DRV" pad="9"/>
<connect gate="G$1" pin="EN/OK" pad="3"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="I_SET" pad="4"/>
<connect gate="G$1" pin="RSTRT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1X2" prefix="J">
<description>3.5mm Terminal block
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="1X2"/>
</gates>
<devices>
<device name="-3.5MM" package="1X2-3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT" prefix="TM" uservalue="yes">
<description>SMT trimmer potentiometer part number TC33X
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TRIMPOT"/>
</gates>
<devices>
<device name="TC33X" package="TC33X">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3386" package="TRIM-3386">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTAL" prefix="X" uservalue="yes">
<description>Low cost SMT crystals, no capacitors included
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="XTAL"/>
</gates>
<devices>
<device name="NX8045" package="NX8045">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NX5032" package="NX5032">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.2X1.5" package="XTAL3215">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OS102011MA1Q" prefix="SW">
<description>OS10201MA1Q through-hole right angle switch
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TSU"/>
<gate name="G$2" symbol="MT"/>
<gate name="G$3" symbol="MT"/>
</gates>
<devices>
<device name="" package="OS102011MA1Q">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="2"/>
<connect gate="G$1" pin="S" pad="1"/>
<connect gate="G$2" pin="MT" pad="MT1"/>
<connect gate="G$3" pin="MT" pad="MT2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPST_TACT" prefix="SW">
<description>SMT 6mm switch, EVQQ2 series
&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TS2"/>
</gates>
<devices>
<device name="-EVQQ2" package="EVQ-Q2">
<connects>
<connect gate="G$1" pin="P" pad="A"/>
<connect gate="G$1" pin="P1" pad="A'"/>
<connect gate="G$1" pin="S" pad="B"/>
<connect gate="G$1" pin="S1" pad="B'"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-KMR2" package="KMR2">
<connects>
<connect gate="G$1" pin="P" pad="1"/>
<connect gate="G$1" pin="P1" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
<connect gate="G$1" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32U4">
<description>&lt;p&gt;http://www.ladyada.net/library/eagle&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ATMEGA32U4"/>
</gates>
<devices>
<device name="-AU" package="TQFP44">
<connects>
<connect gate="G$1" pin="/RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC" pad="24"/>
<connect gate="G$1" pin="AVCC1" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="GND1" pad="23"/>
<connect gate="G$1" pin="GND2" pad="35"/>
<connect gate="G$1" pin="GND3" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(PDI/MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(PDO/MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(OC1A/ADC12/!OC4B)" pad="29"/>
<connect gate="G$1" pin="PB6(OC1B/OC4B/ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7(OC0A/OC1C/RTS)" pad="12"/>
<connect gate="G$1" pin="PC6(OC3A/!OC4A)" pad="31"/>
<connect gate="G$1" pin="PC7(ICP3/CLK0/OC4A)" pad="32"/>
<connect gate="G$1" pin="PD0(INT0/OC0B/SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(INT1/SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(INT2/RXD1)" pad="20"/>
<connect gate="G$1" pin="PD3(INT3/TXD1)" pad="21"/>
<connect gate="G$1" pin="PD4(ICP1/ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5(XCK/CTS)" pad="22"/>
<connect gate="G$1" pin="PD6(T1/ADC9/!OC4D)" pad="26"/>
<connect gate="G$1" pin="PD7(OC4D/ADC10/T0)" pad="27"/>
<connect gate="G$1" pin="PE2(!HWB)" pad="33"/>
<connect gate="G$1" pin="PE6(INT.6/AIN0)" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7(TDI)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VCC1" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90USB162" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
6-channel 10 bit ADC&lt;p&gt;
2-channel 8 bit ADC</description>
<gates>
<gate name="G$1" symbol="AT90USB162"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PB0(SS)" pad="14"/>
<connect gate="G$1" pin="PB1(SCK)" pad="15"/>
<connect gate="G$1" pin="PB2(PDI/MISO)" pad="16"/>
<connect gate="G$1" pin="PB3(PDO/MISO)" pad="17"/>
<connect gate="G$1" pin="PB4(T1)" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="20"/>
<connect gate="G$1" pin="PB7(OC0A/OC1C)" pad="21"/>
<connect gate="G$1" pin="PC1(/RESET)" pad="24"/>
<connect gate="G$1" pin="PC2" pad="5"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5(OC1B)" pad="25"/>
<connect gate="G$1" pin="PC6(OC1A)" pad="23"/>
<connect gate="G$1" pin="PC7(ICP1/INT4)" pad="22"/>
<connect gate="G$1" pin="PD0(INT0/OC0B)" pad="6"/>
<connect gate="G$1" pin="PD1(INT1/AIN0)" pad="7"/>
<connect gate="G$1" pin="PD2(INT2/AIN1/RXD1)" pad="8"/>
<connect gate="G$1" pin="PD3(INT3/TXD1)" pad="9"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="10"/>
<connect gate="G$1" pin="PD5(XCK)" pad="11"/>
<connect gate="G$1" pin="PD6(INT6/RTS)" pad="12"/>
<connect gate="G$1" pin="PD7(INT7/HWB/CTS/T0)" pad="13"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
<connect gate="G$1" pin="XTAL2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN" package="MLF32">
<connects>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PB0(SS)" pad="14"/>
<connect gate="G$1" pin="PB1(SCK)" pad="15"/>
<connect gate="G$1" pin="PB2(PDI/MISO)" pad="16"/>
<connect gate="G$1" pin="PB3(PDO/MISO)" pad="17"/>
<connect gate="G$1" pin="PB4(T1)" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="20"/>
<connect gate="G$1" pin="PB7(OC0A/OC1C)" pad="21"/>
<connect gate="G$1" pin="PC1(/RESET)" pad="24"/>
<connect gate="G$1" pin="PC2" pad="5"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5(OC1B)" pad="25"/>
<connect gate="G$1" pin="PC6(OC1A)" pad="23"/>
<connect gate="G$1" pin="PC7(ICP1/INT4)" pad="22"/>
<connect gate="G$1" pin="PD0(INT0/OC0B)" pad="6"/>
<connect gate="G$1" pin="PD1(INT1/AIN0)" pad="7"/>
<connect gate="G$1" pin="PD2(INT2/AIN1/RXD1)" pad="8"/>
<connect gate="G$1" pin="PD3(INT3/TXD1)" pad="9"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="10"/>
<connect gate="G$1" pin="PD5(XCK)" pad="11"/>
<connect gate="G$1" pin="PD6(INT6/RTS)" pad="12"/>
<connect gate="G$1" pin="PD7(INT7/HWB/CTS/T0)" pad="13"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
<connect gate="G$1" pin="XTAL2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N2222" prefix="T">
<description>&lt;b&gt;NPN TRANSISTOR&lt;/b&gt;
Big oval pads</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="TO92-EBC-OVAL">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N2907*" prefix="Q">
<description>&lt;b&gt;PNP Transistor&lt;/b&gt;
Big Oval pads</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="TO92-EBC-OVAL">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AAA" prefix="BATT">
<description>&lt;b&gt;AAA PC pin holder&lt;/b&gt;
&lt;p&gt;
Mouser part #12BH412 - but pretty much any 1x AAA battery holder should be the same 
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AAA"/>
</gates>
<devices>
<device name="" package="12BH412">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EG1218" prefix="S" uservalue="yes">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
0.1" spacing through hole, vertical SPDT slide switch
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;/p&gt;</description>
<gates>
<gate name="1" symbol="SIS"/>
</gates>
<devices>
<device name="S" package="EG1218">
<connects>
<connect gate="1" pin="O" pad="O"/>
<connect gate="1" pin="P" pad="P"/>
<connect gate="1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PS603">
<description>&lt;b&gt;PS603&lt;/b&gt;
Small 8 ohm speaker, from Mouser. Can SMT solder to board

&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPK"/>
</gates>
<devices>
<device name="SPK" package="PS603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*555" prefix="IC">
<description>&lt;b&gt;TIMER&lt;/b&gt;
Changed DIP package to have round (not oval) pin pads
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="A" symbol="555"/>
</gates>
<devices>
<device name="N" package="DIL08-ROUND">
<connects>
<connect gate="A" pin="CV" pad="5"/>
<connect gate="A" pin="DIS" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="THR" pad="6"/>
<connect gate="A" pin="TR" pad="2"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
<technology name="SE"/>
<technology name="UA"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="CV" pad="5"/>
<connect gate="A" pin="DIS" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="THR" pad="6"/>
<connect gate="A" pin="TR" pad="2"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
<technology name="SE"/>
<technology name="UA"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5MMRGBLED">
<gates>
<gate name="G$1" symbol="RGBLED_CC"/>
</gates>
<devices>
<device name="" package="LED5MMRGB">
<connects>
<connect gate="G$1" pin="BLUE" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GREEN" pad="2"/>
<connect gate="G$1" pin="RED" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FB">
<description>&lt;b&gt;Ferrite bead&lt;/b&gt;
&lt;p&gt;
Digikey #P9821BK-ND</description>
<gates>
<gate name="G$1" symbol="FB"/>
</gates>
<devices>
<device name="" package="FB">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X1" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Pin header 1x1 for 0.1" spacing&lt;/b&gt;
&lt;p&gt;
With round pins</description>
<gates>
<gate name="G$1" symbol="PINHD1"/>
</gates>
<devices>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB" package="1X01-CLEANBIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BIGPOGO" package="1X1-BIGPOGO">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Pin header 1x10 0.1" spacing&lt;/b&gt;
&lt;p&gt;
With round pins</description>
<gates>
<gate name="G$1" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09-BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X10">
<description>&lt;b&gt;Pin header 1x10 0.1" spacing&lt;/b&gt;
&lt;p&gt;
With round pins</description>
<gates>
<gate name="G$1" symbol="PINHD10"/>
</gates>
<devices>
<device name="" package="1X10-BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PNA460XM">
<description>&lt;b&gt;IR 38KHz receiver&lt;/b&gt;
&lt;p&gt;
PNA4602 and related receivers
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="PNA460XM"/>
</gates>
<devices>
<device name="" package="PNA460XM">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RGBLED_CA" prefix="LED">
<description>&lt;b&gt;RGB LED, common-anode&lt;/b&gt;&lt;p&gt;5MM Staggered pins&lt;p&gt;5mm Piranha package
&lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="RGBLED_CA"/>
</gates>
<devices>
<device name="-5MM" package="LED5MMRGB">
<connects>
<connect gate="G$1" pin="BLUE" pad="4"/>
<connect gate="G$1" pin="GREEN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PIRANHA" package="PIRANHA5MM">
<connects>
<connect gate="G$1" pin="BLUE" pad="1"/>
<connect gate="G$1" pin="GREEN" pad="3"/>
<connect gate="G$1" pin="RED" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPEAKER" prefix="SP">
<description>&lt;b&gt;SPEAKER&lt;/b&gt;&lt;p&gt; Source: Buerklin&lt;p&gt;Added PS12 (for part # PS1240 piezo) &lt;p&gt;http://www.ladyada.net/library/pcb/eaglelibrary.html&lt;p&gt;</description>
<gates>
<gate name="S1" symbol="SP"/>
</gates>
<devices>
<device name="/AL60P" package="AL60P">
<connects>
<connect gate="S1" pin="+" pad="1"/>
<connect gate="S1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/AL11P" package="AL11P">
<connects>
<connect gate="S1" pin="+" pad="+"/>
<connect gate="S1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/PS12" package="PS12">
<connects>
<connect gate="S1" pin="+" pad="P$1"/>
<connect gate="S1" pin="-" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS12864A">
<description>KS0108 based display. Some have slightly different pinouts so double check!</description>
<gates>
<gate name="G$1" symbol="GLCD"/>
</gates>
<devices>
<device name="" package="TS12864">
<connects>
<connect gate="G$1" pin="/RST" pad="17"/>
<connect gate="G$1" pin="A" pad="19"/>
<connect gate="G$1" pin="CS0" pad="15"/>
<connect gate="G$1" pin="CS1" pad="16"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="20"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="RW" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VEE" pad="18"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CR1220" uservalue="yes">
<description>&lt;b&gt;CR1216/CR1220/CR1225 12mm 3V lithium coin cell &lt;/b&gt;
&lt;p&gt;
Great for battery packup. Both SMT and THM holders. 
&lt;br&gt;
Note the THM package has the ground pads on both sides of the PCB so that the masks are the same - this reduces the cost</description>
<gates>
<gate name="G$1" symbol="3V"/>
</gates>
<devices>
<device name="SMT" package="CR1220-SMD">
<connects>
<connect gate="G$1" pin="+" pad="+$1"/>
<connect gate="G$1" pin="+1" pad="+$2"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THM" package="CR1220-THM">
<connects>
<connect gate="G$1" pin="+" pad="+1"/>
<connect gate="G$1" pin="+1" pad="+2"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IV18" prefix="DIS">
<description>&lt;b&gt;LCD DISPLAY&lt;/b&gt;&lt;p&gt;
8-character 7 segment</description>
<gates>
<gate name="G$1" symbol="LS026"/>
</gates>
<devices>
<device name="" package="IV18">
<connects>
<connect gate="G$1" pin="1" pad="15"/>
<connect gate="G$1" pin="2" pad="22"/>
<connect gate="G$1" pin="3" pad="16"/>
<connect gate="G$1" pin="4" pad="21"/>
<connect gate="G$1" pin="5" pad="17"/>
<connect gate="G$1" pin="6" pad="20"/>
<connect gate="G$1" pin="7" pad="19"/>
<connect gate="G$1" pin="8" pad="18"/>
<connect gate="G$1" pin="9" pad="14"/>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="9"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="H" pad="2"/>
<connect gate="G$1" pin="VBIAS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6921">
<description>&lt;b&gt;MAX6921&lt;/b&gt;
&lt;p&gt;
76V VFD driver in TSSOP and PLCC. Can be cascaded, talk to it via SPI</description>
<gates>
<gate name="G$1" symbol="MAX6921"/>
</gates>
<devices>
<device name="" package="PLCC-S28">
<connects>
<connect gate="G$1" pin="BLANK" pad="13"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="DIN" pad="27"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="LOAD" pad="16"/>
<connect gate="G$1" pin="OUT0" pad="26"/>
<connect gate="G$1" pin="OUT1" pad="25"/>
<connect gate="G$1" pin="OUT10" pad="12"/>
<connect gate="G$1" pin="OUT11" pad="11"/>
<connect gate="G$1" pin="OUT12" pad="10"/>
<connect gate="G$1" pin="OUT13" pad="9"/>
<connect gate="G$1" pin="OUT14" pad="8"/>
<connect gate="G$1" pin="OUT15" pad="7"/>
<connect gate="G$1" pin="OUT16" pad="6"/>
<connect gate="G$1" pin="OUT17" pad="5"/>
<connect gate="G$1" pin="OUT18" pad="4"/>
<connect gate="G$1" pin="OUT19" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="24"/>
<connect gate="G$1" pin="OUT3" pad="23"/>
<connect gate="G$1" pin="OUT4" pad="22"/>
<connect gate="G$1" pin="OUT5" pad="21"/>
<connect gate="G$1" pin="OUT6" pad="20"/>
<connect gate="G$1" pin="OUT7" pad="19"/>
<connect gate="G$1" pin="OUT8" pad="18"/>
<connect gate="G$1" pin="OUT9" pad="17"/>
<connect gate="G$1" pin="VBB" pad="1"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1307" prefix="IC">
<description>&lt;b&gt;DS1307&lt;/b&gt;
&lt;p&gt;
Real time clock (RTC) with battery backup ability. Talk to it via i2c</description>
<gates>
<gate name="G$1" symbol="DS1307"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW/OUT" pad="7"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78*" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;
&lt;p&gt;
Added bigger pads to the TO-92 package</description>
<gates>
<gate name="A1" symbol="78XX"/>
</gates>
<devices>
<device name="Z" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="L05"/>
<technology name="L08"/>
<technology name="L12"/>
<technology name="L15"/>
<technology name="L18"/>
<technology name="L24"/>
</technologies>
</device>
<device name="T" package="TO220H">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="VI" pad="1"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="H" package="TO39">
<connects>
<connect gate="A1" pin="GND" pad="3"/>
<connect gate="A1" pin="VI" pad="1"/>
<connect gate="A1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="L" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="DT" package="TO252">
<connects>
<connect gate="A1" pin="GND" pad="3"/>
<connect gate="A1" pin="VI" pad="1"/>
<connect gate="A1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33340/2">
<description>&lt;b&gt;MC33340 or MC33342&lt;/b&gt;
&lt;p&gt;
NiMH/NiCad Battery fast charge controller</description>
<gates>
<gate name="G$1" symbol="MC33340/2"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="F/T" pad="3"/>
<connect gate="G$1" pin="GATE" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="T1" pad="7"/>
<connect gate="G$1" pin="T2" pad="6"/>
<connect gate="G$1" pin="T3" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSEN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1173">
<gates>
<gate name="G$1" symbol="LT1173"/>
</gates>
<devices>
<device name="CS" package="SO08">
<connects>
<connect gate="G$1" pin="AO" pad="6"/>
<connect gate="G$1" pin="FB" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ILIM" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="SET" pad="7"/>
<connect gate="G$1" pin="SW1" pad="3"/>
<connect gate="G$1" pin="SW2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CN" package="DIL08">
<connects>
<connect gate="G$1" pin="AO" pad="6"/>
<connect gate="G$1" pin="FB" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ILIM" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="SET" pad="7"/>
<connect gate="G$1" pin="SW1" pad="3"/>
<connect gate="G$1" pin="SW2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX756">
<gates>
<gate name="G$1" symbol="MAX756"/>
</gates>
<devices>
<device name="CSA" package="SO08">
<connects>
<connect gate="G$1" pin="/SHDN" pad="1"/>
<connect gate="G$1" pin="3/5" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="LBI" pad="5"/>
<connect gate="G$1" pin="LBO" pad="4"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CPA" package="DIL08">
<connects>
<connect gate="G$1" pin="/SHDN" pad="1"/>
<connect gate="G$1" pin="3/5" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="LBI" pad="5"/>
<connect gate="G$1" pin="LBO" pad="4"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX757">
<gates>
<gate name="G$1" symbol="MAX757"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="/SHDN" pad="1"/>
<connect gate="G$1" pin="FB" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="LBI" pad="5"/>
<connect gate="G$1" pin="LBO" pad="4"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1302">
<gates>
<gate name="G$1" symbol="LT1302"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IT" pad="5"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="SHDN" pad="3"/>
<connect gate="G$1" pin="SNS" pad="4"/>
<connect gate="G$1" pin="SW" pad="7"/>
<connect gate="G$1" pin="VC" pad="2"/>
<connect gate="G$1" pin="VIN" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L">
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="2474/10" package="2747">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1800R" package="1800R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="6000">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LQH55" package="LQH55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCHOTTKY-DIODE" prefix="D" uservalue="yes">
<description>Schottky Diode</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY"/>
</gates>
<devices>
<device name="DO13M" package="DO13M">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4111-15" package="C4111-15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P6T15" package="P6T15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB429-17" package="CB429-17">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO201T15" package="DO201T15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO35-7" package="DO35-7">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F126Z12" package="F126Z12">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AG" package="AG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92H" package="TO92H">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB417-15" package="CB417-15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB429-15" package="CB429-15">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO41" package="DO41-10">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO41-7" package="DO41-7">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FQN1N50C" prefix="Q">
<description>&lt;b&gt;N-Channel Enhancement MOSFET&lt;/B&gt; 500V, 0.4A, 6.0 Ohm</description>
<gates>
<gate name="G$1" symbol="IGFET-EN-GDS"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="I" package="TO92-INLINE">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*125" prefix="IC">
<description>Quad bus &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74125"/>
<gate name="B" symbol="74125"/>
<gate name="C" symbol="74125"/>
<gate name="D" symbol="74125"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="N-LARDO" package="DIL14-LARDO">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO">
<description>&lt;b&gt;Arduino Diecimila/Duemilanove&lt;/b&gt;
&lt;p&gt;
Make a shield with ease, this package has all the named pins as well as the two mounting drill holes and an outline of the USB and DC power connector. The outline is on the DIMENSION layer, so if your board house uses it they will cut the outline to match.
&lt;p&gt;
http://www.ladyada.net/library/pcb/eaglelibrary.html</description>
<gates>
<gate name="G$1" symbol="ARDUINO"/>
</gates>
<devices>
<device name="UNO" package="ARDUINO">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BPLACE" package="ARDUINO-BPLACE">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-NOHOLE" package="ARDUINO-NOHOLE">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-NODIM" package="ARDUINO-NODIM">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DUE" package="ARDUINO_DUE_SHIELD">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V3"/>
<connect gate="G$1" pin="5V" pad="5V0"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="0"/>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D10" pad="10"/>
<connect gate="G$1" pin="D11" pad="11"/>
<connect gate="G$1" pin="D12" pad="12"/>
<connect gate="G$1" pin="D13" pad="13"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="3"/>
<connect gate="G$1" pin="D4" pad="4"/>
<connect gate="G$1" pin="D5" pad="5"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D7" pad="7"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND_1"/>
<connect gate="G$1" pin="GND2" pad="GND_2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_2PIN" prefix="CN" uservalue="yes">
<description>&lt;b&gt;JST 2-Pin Connectors of various flavors&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;SMT-RA (S2B-PH-SM4) 4UConnector #17311&lt;/li&gt;
&lt;li&gt;SMT  (B2B-PH-SM4)&lt;/li&gt;
&lt;li&gt;THM-RA (S2B-PH)&lt;/li&gt;
&lt;li&gt;THM  (B2B-PH)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="-SMT-RA" package="JST-PH-2-SMT-RA">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-THM" package="JST-PH-2-THM">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-THM-RA" package="JST-PH-2-THM-RA">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT" package="JST-PH-2-SMT">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="31-XX" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;

Now with beefier pads!</description>
<gates>
<gate name="1" symbol="TS"/>
</gates>
<devices>
<device name="" package="B3F-31XX">
<connects>
<connect gate="1" pin="P" pad="1"/>
<connect gate="1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SKINNY" package="B3F-31XX-SKINNIER">
<connects>
<connect gate="1" pin="P" pad="1"/>
<connect gate="1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDMMC">
<description>&lt;b&gt;SD MMC Card holder&lt;/b&gt;
&lt;p&gt;
4UCON part #06132 - easy to solder</description>
<gates>
<gate name="G$1" symbol="SD-MMC"/>
</gates>
<devices>
<device name="SCDA" package="SCDA">
<connects>
<connect gate="G$1" pin="CARD_DETECT" pad="10"/>
<connect gate="G$1" pin="COMMON_SW" pad="11"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="DATA_IN" pad="2"/>
<connect gate="G$1" pin="DATA_OUT" pad="7"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WRITE_PROTECT" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="18650" package="SDCARD">
<connects>
<connect gate="G$1" pin="CARD_DETECT" pad="CD"/>
<connect gate="G$1" pin="COMMON_SW" pad="COM"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="DATA_IN" pad="2"/>
<connect gate="G$1" pin="DATA_OUT" pad="7"/>
<connect gate="G$1" pin="GND" pad="MT1"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WRITE_PROTECT" pad="WP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="06132" package="06132">
<connects>
<connect gate="G$1" pin="CARD_DETECT" pad="CD"/>
<connect gate="G$1" pin="COMMON_SW" pad="GP3"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="DATA_IN" pad="2"/>
<connect gate="G$1" pin="DATA_OUT" pad="7"/>
<connect gate="G$1" pin="GND" pad="GP"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WRITE_PROTECT" pad="WP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="THUMBPOT" prefix="POT">
<description>&lt;b&gt;Thumbwheel pot with switch&lt;/b&gt;
&lt;p&gt;
Available in horizontal (Alpha RV121SF) or vertical (Xicon 311-1701)</description>
<gates>
<gate name="SW" symbol="SW"/>
<gate name="POT" symbol="POT"/>
</gates>
<devices>
<device name="" package="THUMBWHEEL">
<connects>
<connect gate="POT" pin="A" pad="1"/>
<connect gate="POT" pin="E" pad="3"/>
<connect gate="POT" pin="S" pad="2"/>
<connect gate="SW" pin="P" pad="SW2"/>
<connect gate="SW" pin="S" pad="SW1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="THUMBWHEELV">
<connects>
<connect gate="POT" pin="A" pad="A"/>
<connect gate="POT" pin="E" pad="E"/>
<connect gate="POT" pin="S" pad="S"/>
<connect gate="SW" pin="P" pad="SW2"/>
<connect gate="SW" pin="S" pad="SW1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STEREOJACK" prefix="X">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
Stereo jack with two switches. Kycon STX3100, CUI SJ1-3555NG and/or 4UCon 05544</description>
<gates>
<gate name="1" symbol="KS-S"/>
</gates>
<devices>
<device name="" package="STX3100">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4921">
<gates>
<gate name="G$1" symbol="MCP4921"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="#CS" pad="2"/>
<connect gate="G$1" pin="AVSS" pad="7"/>
<connect gate="G$1" pin="DACA" pad="8"/>
<connect gate="G$1" pin="LDAC" pad="5"/>
<connect gate="G$1" pin="REFA" pad="6"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="SDI" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP9422" prefix="IC">
<gates>
<gate name="G$1" symbol="MCP4922"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="#CS" pad="3"/>
<connect gate="G$1" pin="#SHDN" pad="9"/>
<connect gate="G$1" pin="AVSS" pad="12"/>
<connect gate="G$1" pin="DACA" pad="14"/>
<connect gate="G$1" pin="DACB" pad="10"/>
<connect gate="G$1" pin="LDAC" pad="8"/>
<connect gate="G$1" pin="REFA" pad="13"/>
<connect gate="G$1" pin="REFB" pad="11"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SDI" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD8"/>
</gates>
<devices>
<device name="CLEANBIG" package="1X08-CLEANBIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BIG" package="1X08-BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X08-LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.5MM" package="1X08-3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB" package="1X03-CLEANBIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CLEAN" package="1X06-CLEAN">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB" package="1X06-CLEANBIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B" package="1X06-BIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X06-BIGLOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.5MM" package="1X06-3.5MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1700" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="78XX-1"/>
</gates>
<devices>
<device name="INLINE" package="TO92-INLINE">
<connects>
<connect gate="1" pin="GND" pad="1"/>
<connect gate="1" pin="IN" pad="2"/>
<connect gate="1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRI" package="TO92">
<connects>
<connect gate="1" pin="GND" pad="1"/>
<connect gate="1" pin="IN" pad="2"/>
<connect gate="1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1035D">
<gates>
<gate name="G$1" symbol="1035D"/>
</gates>
<devices>
<device name="" package="1035D">
<connects>
<connect gate="G$1" pin="#RST" pad="#RST"/>
<connect gate="G$1" pin="BOOTSEL" pad="BOOT"/>
<connect gate="G$1" pin="GND1" pad="GND"/>
<connect gate="G$1" pin="ON_OFF" pad="ON_OFF"/>
<connect gate="G$1" pin="PPS" pad="PPS"/>
<connect gate="G$1" pin="RFPWUP" pad="RFPWUP"/>
<connect gate="G$1" pin="RX0" pad="RX0"/>
<connect gate="G$1" pin="RX1" pad="RX1"/>
<connect gate="G$1" pin="TX0" pad="TX0"/>
<connect gate="G$1" pin="TX1" pad="TX1"/>
<connect gate="G$1" pin="VBAK" pad="VBAK"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EB-85A">
<gates>
<gate name="G$1" symbol="EB-85A"/>
</gates>
<devices>
<device name="" package="JST-8POS">
<connects>
<connect gate="G$1" pin="BAT" pad="8"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="PPS" pad="7"/>
<connect gate="G$1" pin="RX" pad="4"/>
<connect gate="G$1" pin="RX2" pad="6"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="TX2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM-406A">
<gates>
<gate name="G$1" symbol="EM-406A"/>
</gates>
<devices>
<device name="" package="JST-6POS">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="PPS" pad="1"/>
<connect gate="G$1" pin="RX" pad="4"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LASSENIQ">
<gates>
<gate name="G$1" symbol="EB-85A"/>
</gates>
<devices>
<device name="" package="TRIMBLE">
<connects>
<connect gate="G$1" pin="BAT" pad="8"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="PPS" pad="4"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="RX2" pad="6"/>
<connect gate="G$1" pin="TX" pad="1"/>
<connect gate="G$1" pin="TX2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIDIJACK">
<description>&lt;b&gt;DIN 5 jack also known as MIDI jack&lt;/b&gt;
A modification of conn-hirshman:MAB5SH with two options for the grounding 'teeth'</description>
<gates>
<gate name="G$2" symbol="MT"/>
<gate name="G$3" symbol="MT"/>
<gate name="G$1" symbol="DIN-5"/>
<gate name="G$4" symbol="MT"/>
<gate name="G$5" symbol="MT"/>
</gates>
<devices>
<device name="" package="CP-2350">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$2" pin="MT" pad="PE"/>
<connect gate="G$3" pin="MT" pad="PE@"/>
<connect gate="G$4" pin="MT" pad="PE1"/>
<connect gate="G$5" pin="MT" pad="PE2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROSD">
<description>&lt;b&gt;Micro-SD / Transflash card holder with SPI pinout&lt;/b&gt;
&lt;p&gt;
For the 3M # 2908-05WB-MG and/or 4UCON #19656&lt;br&gt;
push-push type</description>
<gates>
<gate name="G$1" symbol="TRANSFLASH"/>
</gates>
<devices>
<device name="" package="MICROSD">
<connects>
<connect gate="G$1" pin="CARD_DETECT" pad="CD1"/>
<connect gate="G$1" pin="CARD_DETECT1" pad="CD2"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="DATA_IN" pad="3"/>
<connect gate="G$1" pin="DATA_OUT" pad="7"/>
<connect gate="G$1" pin="GND" pad="MT1"/>
<connect gate="G$1" pin="GND1" pad="MT2"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP298X" prefix="IC">
<gates>
<gate name="G$1" symbol="LP298X"/>
</gates>
<devices>
<device name="S" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="BYP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP7386X" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MCP7386x&lt;/b&gt;
&lt;p&gt;

4.1, 4.2, 8.2, 8.4 LiPoly battery charger chip family, with wide DC input, thermal cutoff, adjustable curret, and indicator LEDs</description>
<gates>
<gate name="G$1" symbol="MCP7386X"/>
</gates>
<devices>
<device name="S" package="SO16">
<connects>
<connect gate="G$1" pin="EN" pad="16"/>
<connect gate="G$1" pin="PROG" pad="7"/>
<connect gate="G$1" pin="STAT1" pad="2"/>
<connect gate="G$1" pin="STAT2" pad="1"/>
<connect gate="G$1" pin="THERM" pad="9"/>
<connect gate="G$1" pin="THREF" pad="8"/>
<connect gate="G$1" pin="TIMER" pad="10"/>
<connect gate="G$1" pin="VBAT1" pad="12"/>
<connect gate="G$1" pin="VBAT2" pad="13"/>
<connect gate="G$1" pin="VBAT3" pad="14"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VDD1" pad="5"/>
<connect gate="G$1" pin="VSET" pad="3"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="15"/>
<connect gate="G$1" pin="VSS2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FLIPFLOP-RES" prefix="R" uservalue="yes">
<description>&lt;B&gt;Flip Flop resistor&lt;/b&gt;
&lt;p&gt;
An 0805 resistor inside a standard 1/4W 5% resistor. Makes for easy mods</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="" package="0805-THM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSM2167" prefix="IC">
<description>&lt;b&gt;SSM2167&lt;/b&gt;
&lt;p&gt;
Microphone conditioner chip</description>
<gates>
<gate name="G$1" symbol="SSM2167"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="AVGCAP" pad="6"/>
<connect gate="G$1" pin="BUFOUT" pad="4"/>
<connect gate="G$1" pin="CMPRS" pad="8"/>
<connect gate="G$1" pin="GATE" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="INPUT" pad="5"/>
<connect gate="G$1" pin="OUTPUT" pad="9"/>
<connect gate="G$1" pin="SHTDN" pad="3"/>
<connect gate="G$1" pin="VCA_IN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELECTRET" prefix="Q" uservalue="yes">
<description>&lt;b&gt;Electret microphone&lt;/b&gt;
&lt;p&gt;
Thru hole 2.54mm spacing with 9.7mm diameter</description>
<gates>
<gate name="G$1" symbol="ELECTRET"/>
</gates>
<devices>
<device name="" package="9.7ELECTRET">
<connects>
<connect gate="G$1" pin="1" pad="-"/>
<connect gate="G$1" pin="2" pad="+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCBARREL" prefix="CN" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;2.0mm DC Barrel Jack&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;DCJACK_2MM_PTH&lt;/b&gt; - Through Hole Jack (4UConnector: 05537)</description>
<gates>
<gate name="G$1" symbol="DCBARREL"/>
</gates>
<devices>
<device name="PTH" package="DCJACK_2MM_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="DCJACK_2MM_SMT">
<connects>
<connect gate="G$1" pin="GND" pad="GNDBREAK"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="PWR1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUALPOTSW" prefix="TM" uservalue="yes">
<gates>
<gate name="SW" symbol="SW"/>
<gate name="P2" symbol="POT"/>
<gate name="P1" symbol="POT"/>
</gates>
<devices>
<device name="" package="RK0971221">
<connects>
<connect gate="P1" pin="A" pad="B1"/>
<connect gate="P1" pin="E" pad="A1"/>
<connect gate="P1" pin="S" pad="W1"/>
<connect gate="P2" pin="A" pad="B2"/>
<connect gate="P2" pin="E" pad="A2"/>
<connect gate="P2" pin="S" pad="W2"/>
<connect gate="SW" pin="P" pad="SW1"/>
<connect gate="SW" pin="S" pad="SW2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6675" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX6675"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="/CS" pad="6"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-PWR">
<gates>
<gate name="G$1" symbol="USB-PWR"/>
</gates>
<devices>
<device name="" package="USB-MINIB-THM-MOLEX-PWRONLY">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="U4CON" package="USB-MINIB-THM-PWRONLY">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX9814">
<gates>
<gate name="G$1" symbol="MAX9814"/>
</gates>
<devices>
<device name="TDFN14" package="TDFN14_3X3MM">
<connects>
<connect gate="G$1" pin="/SHDN" pad="P$2"/>
<connect gate="G$1" pin="A/R" pad="P$9"/>
<connect gate="G$1" pin="BIAS" pad="P$12"/>
<connect gate="G$1" pin="CG" pad="P$3"/>
<connect gate="G$1" pin="CT" pad="P$1"/>
<connect gate="G$1" pin="EP" pad="P$THERMAL"/>
<connect gate="G$1" pin="GAIN" pad="P$10"/>
<connect gate="G$1" pin="GND" pad="P$7"/>
<connect gate="G$1" pin="MICBIAS" pad="P$13"/>
<connect gate="G$1" pin="MICIN" pad="P$8"/>
<connect gate="G$1" pin="MICOUT" pad="P$6"/>
<connect gate="G$1" pin="NC1" pad="P$4"/>
<connect gate="G$1" pin="NC2" pad="P$11"/>
<connect gate="G$1" pin="TH" pad="P$14"/>
<connect gate="G$1" pin="VDD" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1033" prefix="IC">
<gates>
<gate name="G$1" symbol="VS1033"/>
</gates>
<devices>
<device name="" package="SQFP-S-7X7-48">
<connects>
<connect gate="G$1" pin="/CS" pad="23"/>
<connect gate="G$1" pin="/RESET" pad="3"/>
<connect gate="G$1" pin="AGND" pad="37"/>
<connect gate="G$1" pin="AGND1" pad="40"/>
<connect gate="G$1" pin="AGND2" pad="41"/>
<connect gate="G$1" pin="AGND3" pad="47"/>
<connect gate="G$1" pin="AVDD" pad="38"/>
<connect gate="G$1" pin="AVDD1" pad="43"/>
<connect gate="G$1" pin="AVDD2" pad="45"/>
<connect gate="G$1" pin="BSYNC" pad="13"/>
<connect gate="G$1" pin="CVDD" pad="5"/>
<connect gate="G$1" pin="CVDD1" pad="7"/>
<connect gate="G$1" pin="CVDD2" pad="24"/>
<connect gate="G$1" pin="CVDD3" pad="31"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DGND1" pad="16"/>
<connect gate="G$1" pin="DGND2" pad="20"/>
<connect gate="G$1" pin="DGND3" pad="21"/>
<connect gate="G$1" pin="DGND4" pad="22"/>
<connect gate="G$1" pin="DGND5" pad="35"/>
<connect gate="G$1" pin="DREQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO0/I2C_CLK" pad="33"/>
<connect gate="G$1" pin="GPIO1/I2C_DA" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="GPIO4/I2C_LROUT" pad="36"/>
<connect gate="G$1" pin="GPIO5/I2C_MCLK" pad="25"/>
<connect gate="G$1" pin="GPIO6" pad="11"/>
<connect gate="G$1" pin="GPIO7" pad="12"/>
<connect gate="G$1" pin="IOVDD" pad="6"/>
<connect gate="G$1" pin="IOVDD1" pad="14"/>
<connect gate="G$1" pin="IOVDD2" pad="19"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="LINEIN" pad="48"/>
<connect gate="G$1" pin="MIC+" pad="1"/>
<connect gate="G$1" pin="MIC-" pad="2"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="VCO" pad="15"/>
<connect gate="G$1" pin="XT1" pad="18"/>
<connect gate="G$1" pin="XT2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TIP30" prefix="Q">
<description>&lt;b&gt;PNP Transistor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="TO220">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLE" package="TO220-NOHOLE">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUAD_OPAMP" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;
Standard quad package</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-TI" package="DIL14-LARDO">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73833" prefix="IC">
<gates>
<gate name="G$1" symbol="MCP73833"/>
</gates>
<devices>
<device name="-UN" package="MSOP10">
<connects>
<connect gate="G$1" pin="/PG" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="THERM" pad="8"/>
<connect gate="G$1" pin="VBAT1" pad="9"/>
<connect gate="G$1" pin="VBAT2" pad="10"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVRISP" prefix="ISP">
<description>&lt;b&gt;AVR ISP HEADER&lt;/b&gt;
&lt;br&gt;
Standard 6 pin header for AVR programming</description>
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="-6" package="AVRISP">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BOX" package="AVRISP-BOX">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT3426">
<description>&lt;B&gt;LT3426&lt;/B&gt;&lt;p&gt;
1.2MHz, 2A boost converter in SOT-23
&lt;p&gt;
http://www.linear.com/pc/productDetail.jsp?navId=H0,C1,C1003,C1042,C1031,C1061,P8430 (Linear website)</description>
<gates>
<gate name="G$1" symbol="LT3426"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="/SHDN" pad="4"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="6"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;b&gt;Diode&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;SMADIODE&lt;/b&gt; - SMA Surface Mount Package
&lt;ul&gt;
&lt;li&gt;20V 1A Schottky Diode Digikey: 641-1014-6-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;DO-1N4148&lt;/b&gt; - Through Hole Small Current Diode&lt;br&gt;
&lt;b&gt;SOD-123&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;20V 1 A (.5mV Vf) Schottky Diode - Digikey: MBRX120TPMSCT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;SOD-323&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;10V 570mA (.38mV Vf, 3ns) Schottky Diode - Digikey: ZLLS410CT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;SOD-523&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;30V 30mA Schottky Diode (RB751S-40TE61) - Digikey: RB751S-40TE61CT-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;b&gt;SOT23-R/W&lt;/b&gt; - SOT23 Package (R = Solder Paste/Reflow Ovens, W = Hand-Soldering)
&lt;ul&gt;
&lt;li&gt;BAT54Film 40V 300mA - Digikey: 497-7162-1-ND&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="SMA" package="SMADIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO-1N4148" package="DO-1N4148">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_REFLOW" package="SOT23-R">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23_WAVE" package="SOT23-W">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-523" package="SOD-523">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-123" package="SOD-123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-323F" package="SOD-323F">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SOD-123FL" package="SOD-123FL">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23008" prefix="IC">
<description>&lt;B&gt;MCP23008&lt;/B&gt;
&lt;p&gt;
Inexpensive i2c i/o expander - 8 general purpose i/o pins with optional pullups</description>
<gates>
<gate name="G$1" symbol="MCP2300X"/>
</gates>
<devices>
<device name="/SO" package="SO18W">
<connects>
<connect gate="G$1" pin="/RST" pad="6"/>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GP0" pad="10"/>
<connect gate="G$1" pin="GP1" pad="11"/>
<connect gate="G$1" pin="GP2" pad="12"/>
<connect gate="G$1" pin="GP3" pad="13"/>
<connect gate="G$1" pin="GP4" pad="14"/>
<connect gate="G$1" pin="GP5" pad="15"/>
<connect gate="G$1" pin="GP6" pad="16"/>
<connect gate="G$1" pin="GP7" pad="17"/>
<connect gate="G$1" pin="INT" pad="8"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VCC" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/P" package="DIL18">
<connects>
<connect gate="G$1" pin="/RST" pad="6"/>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GP0" pad="10"/>
<connect gate="G$1" pin="GP1" pad="11"/>
<connect gate="G$1" pin="GP2" pad="12"/>
<connect gate="G$1" pin="GP3" pad="13"/>
<connect gate="G$1" pin="GP4" pad="14"/>
<connect gate="G$1" pin="GP5" pad="15"/>
<connect gate="G$1" pin="GP6" pad="16"/>
<connect gate="G$1" pin="GP7" pad="17"/>
<connect gate="G$1" pin="INT" pad="8"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VCC" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TB6612FNG" prefix="IC">
<description>&lt;b&gt;TB6612FNG&lt;/b&gt;
&lt;p&gt;
MOS dual H-bridge motor driver, 1.2A current 3.2A peak
3 or 5v logic and 3-15v motor</description>
<gates>
<gate name="G$1" symbol="TB6612FNG"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="AIN1" pad="21"/>
<connect gate="G$1" pin="AIN2" pad="22"/>
<connect gate="G$1" pin="AO1" pad="1"/>
<connect gate="G$1" pin="AO1'" pad="2"/>
<connect gate="G$1" pin="AO2" pad="5"/>
<connect gate="G$1" pin="AO2'" pad="6"/>
<connect gate="G$1" pin="BIN1" pad="17"/>
<connect gate="G$1" pin="BIN2" pad="16"/>
<connect gate="G$1" pin="BO1" pad="11"/>
<connect gate="G$1" pin="BO1'" pad="12"/>
<connect gate="G$1" pin="BO2" pad="7"/>
<connect gate="G$1" pin="BO2'" pad="8"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="PGND1" pad="3"/>
<connect gate="G$1" pin="PGND1'" pad="4"/>
<connect gate="G$1" pin="PGND2" pad="9"/>
<connect gate="G$1" pin="PGND2'" pad="10"/>
<connect gate="G$1" pin="PWMA" pad="23"/>
<connect gate="G$1" pin="PWMB" pad="15"/>
<connect gate="G$1" pin="STBY" pad="19"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VM1" pad="24"/>
<connect gate="G$1" pin="VM2" pad="13"/>
<connect gate="G$1" pin="VM3" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1X5" prefix="J">
<gates>
<gate name="G$1" symbol="1X5"/>
</gates>
<devices>
<device name="" package="1X05-3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HD44780LCD" prefix="X">
<description>&lt;b&gt;HD44780 LCD&lt;/b&gt;
&lt;p&gt;
Standard character type LCDs, available in sizes from 8x1 to 40x4!</description>
<gates>
<gate name="G$1" symbol="CLCD"/>
</gates>
<devices>
<device name="-1602" package="LCD1602">
<connects>
<connect gate="G$1" pin="A" pad="15"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="RW" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUNLOGO">
<description>Just a SMT logo of a sun. cute!</description>
<gates>
<gate name="G$1" symbol="SUNLOGO"/>
</gates>
<devices>
<device name="" package="SUN">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PFET" prefix="Q">
<description>&lt;b&gt;P-CHANNEL MOS FET&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="IGFPA"/>
</gates>
<devices>
<device name="TP0610KL" package="TO92-OVAL">
<connects>
<connect gate="1" pin="D" pad="3"/>
<connect gate="1" pin="G" pad="2"/>
<connect gate="1" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ZVP3306" package="TO92-OVAL">
<connects>
<connect gate="1" pin="D" pad="3"/>
<connect gate="1" pin="G" pad="2"/>
<connect gate="1" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BS250" package="TO92-OVAL">
<connects>
<connect gate="1" pin="D" pad="1"/>
<connect gate="1" pin="G" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2X22">
<gates>
<gate name="G$1" symbol="2X22"/>
</gates>
<devices>
<device name="-2MM" package="2X22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT" package="2X22-SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHUMBYLCD">
<gates>
<gate name="G$1" symbol="CHUMBYVIDEO"/>
</gates>
<devices>
<device name="-THM" package="2X22">
<connects>
<connect gate="G$1" pin="2.5V" pad="38"/>
<connect gate="G$1" pin="3.3V" pad="22"/>
<connect gate="G$1" pin="B0" pad="2"/>
<connect gate="G$1" pin="B1" pad="3"/>
<connect gate="G$1" pin="B2" pad="4"/>
<connect gate="G$1" pin="B3" pad="5"/>
<connect gate="G$1" pin="B4" pad="6"/>
<connect gate="G$1" pin="B5" pad="7"/>
<connect gate="G$1" pin="CS" pad="33"/>
<connect gate="G$1" pin="DET" pad="34"/>
<connect gate="G$1" pin="DOTCLK" pad="25"/>
<connect gate="G$1" pin="ENA" pad="27"/>
<connect gate="G$1" pin="G0" pad="9"/>
<connect gate="G$1" pin="G1" pad="10"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="12"/>
<connect gate="G$1" pin="G4" pad="13"/>
<connect gate="G$1" pin="G5" pad="14"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="8"/>
<connect gate="G$1" pin="GND2" pad="15"/>
<connect gate="G$1" pin="GND3" pad="26"/>
<connect gate="G$1" pin="GND4" pad="37"/>
<connect gate="G$1" pin="HSYNC" pad="24"/>
<connect gate="G$1" pin="KRADC1" pad="39"/>
<connect gate="G$1" pin="LCD_XM" pad="43"/>
<connect gate="G$1" pin="LCD_XP" pad="41"/>
<connect gate="G$1" pin="LCD_YM" pad="44"/>
<connect gate="G$1" pin="LCD_YP" pad="42"/>
<connect gate="G$1" pin="LED_A" pad="29"/>
<connect gate="G$1" pin="LED_K" pad="30"/>
<connect gate="G$1" pin="LINE1_INL" pad="35"/>
<connect gate="G$1" pin="LINE1_INR" pad="36"/>
<connect gate="G$1" pin="LRADC0" pad="40"/>
<connect gate="G$1" pin="R0" pad="16"/>
<connect gate="G$1" pin="R1" pad="17"/>
<connect gate="G$1" pin="R2" pad="18"/>
<connect gate="G$1" pin="R3" pad="19"/>
<connect gate="G$1" pin="R4" pad="20"/>
<connect gate="G$1" pin="R5" pad="21"/>
<connect gate="G$1" pin="RS" pad="32"/>
<connect gate="G$1" pin="RST" pad="28"/>
<connect gate="G$1" pin="VSYNC" pad="23"/>
<connect gate="G$1" pin="WE" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT" package="2X22-SMT">
<connects>
<connect gate="G$1" pin="2.5V" pad="38"/>
<connect gate="G$1" pin="3.3V" pad="22"/>
<connect gate="G$1" pin="B0" pad="2"/>
<connect gate="G$1" pin="B1" pad="3"/>
<connect gate="G$1" pin="B2" pad="4"/>
<connect gate="G$1" pin="B3" pad="5"/>
<connect gate="G$1" pin="B4" pad="6"/>
<connect gate="G$1" pin="B5" pad="7"/>
<connect gate="G$1" pin="CS" pad="33"/>
<connect gate="G$1" pin="DET" pad="34"/>
<connect gate="G$1" pin="DOTCLK" pad="25"/>
<connect gate="G$1" pin="ENA" pad="27"/>
<connect gate="G$1" pin="G0" pad="9"/>
<connect gate="G$1" pin="G1" pad="10"/>
<connect gate="G$1" pin="G2" pad="11"/>
<connect gate="G$1" pin="G3" pad="12"/>
<connect gate="G$1" pin="G4" pad="13"/>
<connect gate="G$1" pin="G5" pad="14"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="8"/>
<connect gate="G$1" pin="GND2" pad="15"/>
<connect gate="G$1" pin="GND3" pad="26"/>
<connect gate="G$1" pin="GND4" pad="37"/>
<connect gate="G$1" pin="HSYNC" pad="24"/>
<connect gate="G$1" pin="KRADC1" pad="39"/>
<connect gate="G$1" pin="LCD_XM" pad="43"/>
<connect gate="G$1" pin="LCD_XP" pad="41"/>
<connect gate="G$1" pin="LCD_YM" pad="44"/>
<connect gate="G$1" pin="LCD_YP" pad="42"/>
<connect gate="G$1" pin="LED_A" pad="29"/>
<connect gate="G$1" pin="LED_K" pad="30"/>
<connect gate="G$1" pin="LINE1_INL" pad="35"/>
<connect gate="G$1" pin="LINE1_INR" pad="36"/>
<connect gate="G$1" pin="LRADC0" pad="40"/>
<connect gate="G$1" pin="R0" pad="16"/>
<connect gate="G$1" pin="R1" pad="17"/>
<connect gate="G$1" pin="R2" pad="18"/>
<connect gate="G$1" pin="R3" pad="19"/>
<connect gate="G$1" pin="R4" pad="20"/>
<connect gate="G$1" pin="R5" pad="21"/>
<connect gate="G$1" pin="RS" pad="32"/>
<connect gate="G$1" pin="RST" pad="28"/>
<connect gate="G$1" pin="VSYNC" pad="23"/>
<connect gate="G$1" pin="WE" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1X22">
<gates>
<gate name="G$1" symbol="1X22"/>
</gates>
<devices>
<device name="THM" package="1X22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;
&lt;p&gt;
With larger annulars</description>
<gates>
<gate name="A" symbol="PINH2X9"/>
</gates>
<devices>
<device name="-BIG" package="2X09-BIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CBIG" package="2X09-CLEANBIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ILI9325_LCD" prefix="CN" uservalue="yes">
<description>2.8" ILI9325-based TFT LCD w/Integrated Touch Screen</description>
<gates>
<gate name="G$1" symbol="ILI9325_LCD"/>
</gates>
<devices>
<device name="1.0MM" package="ILI9325_28INCH_TS">
<connects>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="!RD" pad="10"/>
<connect gate="G$1" pin="!RESET" pad="31"/>
<connect gate="G$1" pin="!WR" pad="9"/>
<connect gate="G$1" pin="DB0" pad="1"/>
<connect gate="G$1" pin="DB1" pad="2"/>
<connect gate="G$1" pin="DB10/DB8" pad="23"/>
<connect gate="G$1" pin="DB11/DB9" pad="24"/>
<connect gate="G$1" pin="DB12/DB10" pad="25"/>
<connect gate="G$1" pin="DB13/DB11" pad="26"/>
<connect gate="G$1" pin="DB14/DB12" pad="27"/>
<connect gate="G$1" pin="DB15/DB13" pad="28"/>
<connect gate="G$1" pin="DB16/DB14" pad="29"/>
<connect gate="G$1" pin="DB17/DB15" pad="30"/>
<connect gate="G$1" pin="DB2" pad="3"/>
<connect gate="G$1" pin="DB3" pad="4"/>
<connect gate="G$1" pin="DB4" pad="22"/>
<connect gate="G$1" pin="DB5" pad="35"/>
<connect gate="G$1" pin="DB6" pad="36"/>
<connect gate="G$1" pin="DB7" pad="37"/>
<connect gate="G$1" pin="GND" pad="34"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="IM3" pad="21"/>
<connect gate="G$1" pin="IMO" pad="11"/>
<connect gate="G$1" pin="IOVCC" pad="33"/>
<connect gate="G$1" pin="IOVCC1" pad="6"/>
<connect gate="G$1" pin="LED-A" pad="16"/>
<connect gate="G$1" pin="LED-K1" pad="17"/>
<connect gate="G$1" pin="LED-K2" pad="18"/>
<connect gate="G$1" pin="LED-K3" pad="19"/>
<connect gate="G$1" pin="LED-K4" pad="20"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="VCI" pad="32"/>
<connect gate="G$1" pin="X+" pad="12"/>
<connect gate="G$1" pin="X-" pad="14"/>
<connect gate="G$1" pin="Y+" pad="13"/>
<connect gate="G$1" pin="Y-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PTCFUSE" prefix="F" uservalue="yes">
<description>PTC fuses, resettable thermistors</description>
<gates>
<gate name="G$1" symbol="FUSE"/>
</gates>
<devices>
<device name="-1812" package="1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32U2" prefix="IC">
<description>&lt;B&gt;ATmega32u2&lt;/b&gt;
&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Pin compatible with the atmega8u2, atmega16u2 and atmega32u2&lt;/li&gt;
&lt;li&gt;8, 16 or 32 K flash, 1K RAM, 512b EEPROM&lt;/li&gt;
&lt;li&gt;8 bit and 16 bit timer (5 PWM total)&lt;/li&gt;
&lt;li&gt;UART, SPI (no I2C!)&lt;/li&gt;
&lt;li&gt;USB with 4 endpoints, LUFA compatible&lt;/li&gt;
&lt;li&gt;22 I/O lines, analog comparator (no ADC!)&lt;/li&gt;
&lt;li&gt;Comes with DFU bootloader burned in!&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ATMEGA32U2"/>
</gates>
<devices>
<device name="-TQFP" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="/RESET(PC1)" pad="24"/>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PB0(SS/PCINT0)" pad="14"/>
<connect gate="G$1" pin="PB1(SCK/PCINT1)" pad="15"/>
<connect gate="G$1" pin="PB2(PDI/MOSI/PCINT2)" pad="16"/>
<connect gate="G$1" pin="PB3(PDO/MISO/PCINT3)" pad="17"/>
<connect gate="G$1" pin="PB4(T1/PCINT4)" pad="18"/>
<connect gate="G$1" pin="PB5(PCINT5)" pad="19"/>
<connect gate="G$1" pin="PB6(PCINT6)" pad="20"/>
<connect gate="G$1" pin="PB7(OC0A/OC1C/PCINT7)" pad="21"/>
<connect gate="G$1" pin="PC2(AIN2/PCIN11)" pad="5"/>
<connect gate="G$1" pin="PC4(PCINT10)" pad="26"/>
<connect gate="G$1" pin="PC5(OC1B/PCINT9)" pad="25"/>
<connect gate="G$1" pin="PC6(OC1A/PCINT8)" pad="23"/>
<connect gate="G$1" pin="PC7(ICP1/INT4/CLKO)" pad="22"/>
<connect gate="G$1" pin="PD0(INT0/OC0B)" pad="6"/>
<connect gate="G$1" pin="PD1(INT1/AIN0)" pad="7"/>
<connect gate="G$1" pin="PD2(INT2/AIN1/RXD1)" pad="8"/>
<connect gate="G$1" pin="PD3(INT3/TXD1)" pad="9"/>
<connect gate="G$1" pin="PD4(INT5/AIN3)" pad="10"/>
<connect gate="G$1" pin="PD5(XCK/AIN4/PCINT12)" pad="11"/>
<connect gate="G$1" pin="PD6(INT6/AIN5/RTS)" pad="12"/>
<connect gate="G$1" pin="PD7(INT7/HWB/AIN6/T0)" pad="13"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
<connect gate="G$1" pin="XTAL2/PC0" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X14" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD14"/>
</gates>
<devices>
<device name="" package="1X14">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CB" package="1X14-CB">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X12" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD12"/>
</gates>
<devices>
<device name="" package="1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CB" package="1X12-CB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1X40">
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X40" prefix="CON">
<description>Pinouts for OLED/LCD displays with flex ribbons</description>
<gates>
<gate name="G$1" symbol="PINHD-1X40"/>
</gates>
<devices>
<device name="-1MM" package="1X40-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0.6MM" package="1X40-0.6MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0.7MM" package="1X40-0.7MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0.8MM" package="1X40-0.8MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0.5MM" package="1X40-0.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X20" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD20"/>
</gates>
<devices>
<device name="" package="1X20">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BIG" package="1X20-BIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X20" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X20"/>
</gates>
<devices>
<device name="" package="2X20">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BIG" package="2X20-BIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="29" pad="29"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="30" pad="30"/>
<connect gate="A" pin="31" pad="31"/>
<connect gate="A" pin="32" pad="32"/>
<connect gate="A" pin="33" pad="33"/>
<connect gate="A" pin="34" pad="34"/>
<connect gate="A" pin="35" pad="35"/>
<connect gate="A" pin="36" pad="36"/>
<connect gate="A" pin="37" pad="37"/>
<connect gate="A" pin="38" pad="38"/>
<connect gate="A" pin="39" pad="39"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="40" pad="40"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5941" prefix="IC">
<gates>
<gate name="G$1" symbol="TLC5941"/>
</gates>
<devices>
<device name="NT" package="DIL28-3">
<connects>
<connect gate="G$1" pin="BLANK" pad="23"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GSCLK" pad="18"/>
<connect gate="G$1" pin="IREF" pad="20"/>
<connect gate="G$1" pin="MODE" pad="27"/>
<connect gate="G$1" pin="OUT0" pad="28"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT10" pad="10"/>
<connect gate="G$1" pin="OUT11" pad="11"/>
<connect gate="G$1" pin="OUT12" pad="12"/>
<connect gate="G$1" pin="OUT13" pad="13"/>
<connect gate="G$1" pin="OUT14" pad="14"/>
<connect gate="G$1" pin="OUT15" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="3"/>
<connect gate="G$1" pin="OUT4" pad="4"/>
<connect gate="G$1" pin="OUT5" pad="5"/>
<connect gate="G$1" pin="OUT6" pad="6"/>
<connect gate="G$1" pin="OUT7" pad="7"/>
<connect gate="G$1" pin="OUT8" pad="8"/>
<connect gate="G$1" pin="OUT9" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="25"/>
<connect gate="G$1" pin="SIN" pad="26"/>
<connect gate="G$1" pin="SOUT" pad="17"/>
<connect gate="G$1" pin="TEST" pad="19"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="XERR" pad="16"/>
<connect gate="G$1" pin="XLAT" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UG-2864HSWEG01">
<description>UG-2864HSWEG01 OLED display</description>
<gates>
<gate name="G$1" symbol="UG-2864HSWEG01"/>
</gates>
<devices>
<device name="" package="1X30-0.7MM">
<connects>
<connect gate="G$1" pin="/CS" pad="13"/>
<connect gate="G$1" pin="/RES" pad="14"/>
<connect gate="G$1" pin="BS0" pad="10"/>
<connect gate="G$1" pin="BS1" pad="11"/>
<connect gate="G$1" pin="BS2" pad="12"/>
<connect gate="G$1" pin="C1N" pad="5"/>
<connect gate="G$1" pin="C1P" pad="4"/>
<connect gate="G$1" pin="C2N" pad="3"/>
<connect gate="G$1" pin="C2P" pad="2"/>
<connect gate="G$1" pin="D/C" pad="15"/>
<connect gate="G$1" pin="D0/DI" pad="18"/>
<connect gate="G$1" pin="D1/SCLK" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="21"/>
<connect gate="G$1" pin="D4" pad="22"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="24"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="E/RD" pad="17"/>
<connect gate="G$1" pin="IREF" pad="26"/>
<connect gate="G$1" pin="MT" pad="1"/>
<connect gate="G$1" pin="MT2" pad="30"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="R/W" pad="16"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VCOMH" pad="27"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VLSS" pad="29"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X14" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X14"/>
</gates>
<devices>
<device name="" package="2X14">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CB" package="2X14-CLEANBIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT" package="2X14-SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="25" pad="25"/>
<connect gate="A" pin="26" pad="26"/>
<connect gate="A" pin="27" pad="27"/>
<connect gate="A" pin="28" pad="28"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XF2*-05?" prefix="J">
<description>&lt;b&gt;OMRON FPC Connector&lt;/b&gt;&lt;p&gt;
Source : http://www.omron.com/ecb/products/pdf/fpc.pdf</description>
<gates>
<gate name="-1" symbol="PV"/>
<gate name="-2" symbol="P"/>
<gate name="-3" symbol="P"/>
<gate name="-4" symbol="P"/>
<gate name="-5" symbol="P"/>
</gates>
<devices>
<device name="15-1" package="XF2E-0515-1">
<connects>
<connect gate="-1" pin="MSV" pad="1"/>
<connect gate="-2" pin="MS" pad="2"/>
<connect gate="-3" pin="MS" pad="3"/>
<connect gate="-4" pin="MS" pad="4"/>
<connect gate="-5" pin="MS" pad="5"/>
</connects>
<technologies>
<technology name="E"/>
</technologies>
</device>
<device name="35-1" package="XF2L-0535-1">
<connects>
<connect gate="-1" pin="MSV" pad="1"/>
<connect gate="-2" pin="MS" pad="2"/>
<connect gate="-3" pin="MS" pad="3"/>
<connect gate="-4" pin="MS" pad="4"/>
<connect gate="-5" pin="MS" pad="5"/>
</connects>
<technologies>
<technology name="L"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="40PINFPC" prefix="J">
<description>&lt;b&gt;OMRON FPC Connector&lt;/b&gt;&lt;p&gt;
Source : http://www.omron.com/ecb/products/pdf/fpc.pdf

&lt;p&gt;
XF2M-4015-rev is good for connecting up 'PSP' SHARP LQ043 LCDs</description>
<gates>
<gate name="-1" symbol="PV"/>
<gate name="-2" symbol="P"/>
<gate name="-3" symbol="P"/>
<gate name="-4" symbol="P"/>
<gate name="-5" symbol="P"/>
<gate name="-6" symbol="P"/>
<gate name="-7" symbol="P"/>
<gate name="-8" symbol="P"/>
<gate name="-9" symbol="P"/>
<gate name="-10" symbol="P"/>
<gate name="-11" symbol="P"/>
<gate name="-12" symbol="P"/>
<gate name="-13" symbol="P"/>
<gate name="-14" symbol="P"/>
<gate name="-15" symbol="P"/>
<gate name="-16" symbol="P"/>
<gate name="-17" symbol="P"/>
<gate name="-18" symbol="P"/>
<gate name="-19" symbol="P"/>
<gate name="-20" symbol="P"/>
<gate name="-21" symbol="P"/>
<gate name="-22" symbol="P"/>
<gate name="-23" symbol="P"/>
<gate name="-24" symbol="P"/>
<gate name="-25" symbol="P"/>
<gate name="-26" symbol="P"/>
<gate name="-27" symbol="P"/>
<gate name="-28" symbol="P"/>
<gate name="-29" symbol="P"/>
<gate name="-30" symbol="P"/>
<gate name="-31" symbol="P"/>
<gate name="-32" symbol="P"/>
<gate name="-33" symbol="P"/>
<gate name="-34" symbol="P"/>
<gate name="-35" symbol="P"/>
<gate name="-36" symbol="P"/>
<gate name="-37" symbol="P"/>
<gate name="-38" symbol="P"/>
<gate name="-39" symbol="P"/>
<gate name="-40" symbol="P"/>
</gates>
<devices>
<device name="15-1LW" package="XF2H-4015-1LW">
<connects>
<connect gate="-1" pin="MSV" pad="1"/>
<connect gate="-10" pin="MS" pad="10"/>
<connect gate="-11" pin="MS" pad="11"/>
<connect gate="-12" pin="MS" pad="12"/>
<connect gate="-13" pin="MS" pad="13"/>
<connect gate="-14" pin="MS" pad="14"/>
<connect gate="-15" pin="MS" pad="15"/>
<connect gate="-16" pin="MS" pad="16"/>
<connect gate="-17" pin="MS" pad="17"/>
<connect gate="-18" pin="MS" pad="18"/>
<connect gate="-19" pin="MS" pad="19"/>
<connect gate="-2" pin="MS" pad="2"/>
<connect gate="-20" pin="MS" pad="20"/>
<connect gate="-21" pin="MS" pad="21"/>
<connect gate="-22" pin="MS" pad="22"/>
<connect gate="-23" pin="MS" pad="23"/>
<connect gate="-24" pin="MS" pad="24"/>
<connect gate="-25" pin="MS" pad="25"/>
<connect gate="-26" pin="MS" pad="26"/>
<connect gate="-27" pin="MS" pad="27"/>
<connect gate="-28" pin="MS" pad="28"/>
<connect gate="-29" pin="MS" pad="29"/>
<connect gate="-3" pin="MS" pad="3"/>
<connect gate="-30" pin="MS" pad="30"/>
<connect gate="-31" pin="MS" pad="31"/>
<connect gate="-32" pin="MS" pad="32"/>
<connect gate="-33" pin="MS" pad="33"/>
<connect gate="-34" pin="MS" pad="34"/>
<connect gate="-35" pin="MS" pad="35"/>
<connect gate="-36" pin="MS" pad="36"/>
<connect gate="-37" pin="MS" pad="37"/>
<connect gate="-38" pin="MS" pad="38"/>
<connect gate="-39" pin="MS" pad="39"/>
<connect gate="-4" pin="MS" pad="4"/>
<connect gate="-40" pin="MS" pad="40"/>
<connect gate="-5" pin="MS" pad="5"/>
<connect gate="-6" pin="MS" pad="6"/>
<connect gate="-7" pin="MS" pad="7"/>
<connect gate="-8" pin="MS" pad="8"/>
<connect gate="-9" pin="MS" pad="9"/>
</connects>
<technologies>
<technology name="H"/>
</technologies>
</device>
<device name="4-1734839-0" package="4-1734839-0">
<connects>
<connect gate="-1" pin="MSV" pad="1"/>
<connect gate="-10" pin="MS" pad="10"/>
<connect gate="-11" pin="MS" pad="11"/>
<connect gate="-12" pin="MS" pad="12"/>
<connect gate="-13" pin="MS" pad="13"/>
<connect gate="-14" pin="MS" pad="14"/>
<connect gate="-15" pin="MS" pad="15"/>
<connect gate="-16" pin="MS" pad="16"/>
<connect gate="-17" pin="MS" pad="17"/>
<connect gate="-18" pin="MS" pad="18"/>
<connect gate="-19" pin="MS" pad="19"/>
<connect gate="-2" pin="MS" pad="2"/>
<connect gate="-20" pin="MS" pad="20"/>
<connect gate="-21" pin="MS" pad="21"/>
<connect gate="-22" pin="MS" pad="22"/>
<connect gate="-23" pin="MS" pad="23"/>
<connect gate="-24" pin="MS" pad="24"/>
<connect gate="-25" pin="MS" pad="25"/>
<connect gate="-26" pin="MS" pad="26"/>
<connect gate="-27" pin="MS" pad="27"/>
<connect gate="-28" pin="MS" pad="28"/>
<connect gate="-29" pin="MS" pad="29"/>
<connect gate="-3" pin="MS" pad="3"/>
<connect gate="-30" pin="MS" pad="30"/>
<connect gate="-31" pin="MS" pad="31"/>
<connect gate="-32" pin="MS" pad="32"/>
<connect gate="-33" pin="MS" pad="33"/>
<connect gate="-34" pin="MS" pad="34"/>
<connect gate="-35" pin="MS" pad="35"/>
<connect gate="-36" pin="MS" pad="36"/>
<connect gate="-37" pin="MS" pad="37"/>
<connect gate="-38" pin="MS" pad="38"/>
<connect gate="-39" pin="MS" pad="39"/>
<connect gate="-4" pin="MS" pad="4"/>
<connect gate="-40" pin="MS" pad="40"/>
<connect gate="-5" pin="MS" pad="5"/>
<connect gate="-6" pin="MS" pad="6"/>
<connect gate="-7" pin="MS" pad="7"/>
<connect gate="-8" pin="MS" pad="8"/>
<connect gate="-9" pin="MS" pad="9"/>
</connects>
<technologies>
<technology name="M"/>
</technologies>
</device>
<device name="15-4A" package="XF2R-4015-4A">
<connects>
<connect gate="-1" pin="MSV" pad="1"/>
<connect gate="-10" pin="MS" pad="10"/>
<connect gate="-11" pin="MS" pad="11"/>
<connect gate="-12" pin="MS" pad="12"/>
<connect gate="-13" pin="MS" pad="13"/>
<connect gate="-14" pin="MS" pad="14"/>
<connect gate="-15" pin="MS" pad="15"/>
<connect gate="-16" pin="MS" pad="16"/>
<connect gate="-17" pin="MS" pad="17"/>
<connect gate="-18" pin="MS" pad="18"/>
<connect gate="-19" pin="MS" pad="19"/>
<connect gate="-2" pin="MS" pad="2"/>
<connect gate="-20" pin="MS" pad="20"/>
<connect gate="-21" pin="MS" pad="21"/>
<connect gate="-22" pin="MS" pad="22"/>
<connect gate="-23" pin="MS" pad="23"/>
<connect gate="-24" pin="MS" pad="24"/>
<connect gate="-25" pin="MS" pad="25"/>
<connect gate="-26" pin="MS" pad="26"/>
<connect gate="-27" pin="MS" pad="27"/>
<connect gate="-28" pin="MS" pad="28"/>
<connect gate="-29" pin="MS" pad="29"/>
<connect gate="-3" pin="MS" pad="3"/>
<connect gate="-30" pin="MS" pad="30"/>
<connect gate="-31" pin="MS" pad="31"/>
<connect gate="-32" pin="MS" pad="32"/>
<connect gate="-33" pin="MS" pad="33"/>
<connect gate="-34" pin="MS" pad="34"/>
<connect gate="-35" pin="MS" pad="35"/>
<connect gate="-36" pin="MS" pad="36"/>
<connect gate="-37" pin="MS" pad="37"/>
<connect gate="-38" pin="MS" pad="38"/>
<connect gate="-39" pin="MS" pad="39"/>
<connect gate="-4" pin="MS" pad="4"/>
<connect gate="-40" pin="MS" pad="40"/>
<connect gate="-5" pin="MS" pad="5"/>
<connect gate="-6" pin="MS" pad="6"/>
<connect gate="-7" pin="MS" pad="7"/>
<connect gate="-8" pin="MS" pad="8"/>
<connect gate="-9" pin="MS" pad="9"/>
</connects>
<technologies>
<technology name="R"/>
</technologies>
</device>
<device name="15-1F-REV" package="XF2M-4015-1F-REVERSE">
<connects>
<connect gate="-1" pin="MSV" pad="1"/>
<connect gate="-10" pin="MS" pad="10"/>
<connect gate="-11" pin="MS" pad="11"/>
<connect gate="-12" pin="MS" pad="12"/>
<connect gate="-13" pin="MS" pad="13"/>
<connect gate="-14" pin="MS" pad="14"/>
<connect gate="-15" pin="MS" pad="15"/>
<connect gate="-16" pin="MS" pad="16"/>
<connect gate="-17" pin="MS" pad="17"/>
<connect gate="-18" pin="MS" pad="18"/>
<connect gate="-19" pin="MS" pad="19"/>
<connect gate="-2" pin="MS" pad="2"/>
<connect gate="-20" pin="MS" pad="20"/>
<connect gate="-21" pin="MS" pad="21"/>
<connect gate="-22" pin="MS" pad="22"/>
<connect gate="-23" pin="MS" pad="23"/>
<connect gate="-24" pin="MS" pad="24"/>
<connect gate="-25" pin="MS" pad="25"/>
<connect gate="-26" pin="MS" pad="26"/>
<connect gate="-27" pin="MS" pad="27"/>
<connect gate="-28" pin="MS" pad="28"/>
<connect gate="-29" pin="MS" pad="29"/>
<connect gate="-3" pin="MS" pad="3"/>
<connect gate="-30" pin="MS" pad="30"/>
<connect gate="-31" pin="MS" pad="31"/>
<connect gate="-32" pin="MS" pad="32"/>
<connect gate="-33" pin="MS" pad="33"/>
<connect gate="-34" pin="MS" pad="34"/>
<connect gate="-35" pin="MS" pad="35"/>
<connect gate="-36" pin="MS" pad="36"/>
<connect gate="-37" pin="MS" pad="37"/>
<connect gate="-38" pin="MS" pad="38"/>
<connect gate="-39" pin="MS" pad="39"/>
<connect gate="-4" pin="MS" pad="4"/>
<connect gate="-40" pin="MS" pad="40"/>
<connect gate="-5" pin="MS" pad="5"/>
<connect gate="-6" pin="MS" pad="6"/>
<connect gate="-7" pin="MS" pad="7"/>
<connect gate="-8" pin="MS" pad="8"/>
<connect gate="-9" pin="MS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="F15" prefix="X" uservalue="yes">
<description>&lt;b&gt;SUB-D&lt;/b&gt;
&lt;p&gt;
&lt;b&gt;HDH is also known as a 'right angle VGA' connector</description>
<gates>
<gate name="-1" symbol="F15"/>
</gates>
<devices>
<device name="D" package="F15D">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="F15H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HP" package="F15HP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="F15V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VP" package="F15VP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HDV" package="HDF15V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VB" package="F15VB">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HDH" package="HDF15H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SFV4R-1STE1LF" prefix="X">
<description>&lt;b&gt;FPC Connector ZIF for SMT 0.5mm&lt;/b&gt;&lt;p&gt;

SFV4R-1STE1LF

Useful as the LED backlight connector for a PSP display</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
</gates>
<devices>
<device name="" package="SFV4R-1STE1LF">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33063/MC34063">
<description>&lt;b&gt;MC33063 and MC34063&lt;/b&gt;
&lt;p&gt;
Basic DC/DC converter with internal power-NPN transistor, 100KHz, 1.5A peak switch current. 3-40 input/output.</description>
<gates>
<gate name="G$1" symbol="MC33063"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="DC" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IPK" pad="7"/>
<connect gate="G$1" pin="SWC" pad="1"/>
<connect gate="G$1" pin="SWE" pad="2"/>
<connect gate="G$1" pin="TC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="DC" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IPK" pad="7"/>
<connect gate="G$1" pin="SWC" pad="1"/>
<connect gate="G$1" pin="SWE" pad="2"/>
<connect gate="G$1" pin="TC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X15" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD15"/>
</gates>
<devices>
<device name="" package="1X15">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CB" package="1X15-CB">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73811/2" prefix="IC">
<description>&lt;b&gt;MCP73811 and MCP73812&lt;/b&gt;
&lt;p&gt;
Simple, Miniature Single-Cell, Fully Integrated Li-Ion / Li-Polymer Charge Management Controllers
&lt;br&gt;
SOT-23-5 package, no indicator LED but with adjustable current, small and very inexpensive</description>
<gates>
<gate name="G$1" symbol="MCP73811/2"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73831" prefix="IC">
<description>&lt;b&gt;MCP73831/2&lt;/b&gt;
&lt;P&gt;
Miniature Single-Cell, Fully Integrated Li-Ion,
Li-Polymer Charge Management Controllers.
&lt;p&gt;
Nice and small simple lipoly charge controller, with adjustable current and status output (LED)
&lt;p&gt;
http://www.ladyada.net/library/pcb/eaglelibrary.html</description>
<gates>
<gate name="G$1" symbol="MCP73831/2"/>
</gates>
<devices>
<device name="/OT" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="STAT" pad="1"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="S-35390A" prefix="IC">
<description>&lt;b&gt;S-35390A  2-WIRE REAL-TIME CLOCK&lt;/b&gt;
&lt;p&gt;
The S-35390A is a CMOS 2-wire real-time clock IC which operates with the very low current consumption and in the wide
range of operation voltage. The operation voltage is 1.3 V to 5.5 V so that this IC can be used for various power supplies from
main supply to backup battery. Due to the 0.25 ?A current consumption and wide range of power supply voltage at time
keeping, this IC makes the battery life longer. In the system which operates with a backup battery, the included free registers
can be used as the function for user?s backup memory</description>
<gates>
<gate name="G$1" symbol="S-35390A"/>
</gates>
<devices>
<device name="-T" package="TSSOP-8">
<connects>
<connect gate="G$1" pin="/INT1" pad="1"/>
<connect gate="G$1" pin="/INT2" pad="5"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="XTALI" pad="3"/>
<connect gate="G$1" pin="XTALO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISL1209" prefix="IC">
<description>&lt;b&gt;ISL1209&lt;/b&gt;
&lt;p&gt;
Low Power RTC with Battery Backed
SRAM and Event Detection
&lt;p&gt;
The ISL1209 device is a low power real time clock with event
detect function, timing and crystal compensation,
clock/calendar, power fail indicator, periodic or polled alarm,
intelligent battery backup switching and battery-backed user
SRAM.</description>
<gates>
<gate name="G$1" symbol="ISL1209"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="/IRQ" pad="9"/>
<connect gate="G$1" pin="EVDET" pad="6"/>
<connect gate="G$1" pin="EVIN" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="XTALI" pad="1"/>
<connect gate="G$1" pin="XTALO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTAL-4" prefix="Q" uservalue="yes">
<description>Classic 4-pin 3.2 x 2.5mm crystal</description>
<gates>
<gate name="G$1" symbol="XTAL-4"/>
</gates>
<devices>
<device name="-3225" package="NX3225">
<connects>
<connect gate="G$1" pin="G1" pad="4"/>
<connect gate="G$1" pin="G2" pad="2"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMT-0540-S-R" prefix="SPK">
<description>&lt;b&gt;SMT-0549-S-R&lt;/b&gt;
&lt;P&gt;
Small surface-mount magnetic buzzer</description>
<gates>
<gate name="G$1" symbol="SP"/>
</gates>
<devices>
<device name="" package="SMT-0540-S-R">
<connects>
<connect gate="G$1" pin="+" pad="-"/>
<connect gate="G$1" pin="-" pad="+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-A" prefix="X">
<description>&lt;b&gt;USB type A 'plug'&lt;/b&gt;
&lt;p&gt;
Used for things that can directly connect to a USB port, say USB key</description>
<gates>
<gate name="G$1" symbol="USB-4"/>
</gates>
<devices>
<device name="" package="MOLEX_480371000">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10F200T">
<description>&lt;b&gt;PIC10F200/202/204/206&lt;/b&gt;&lt;p&gt;
Ultra-small 8-bit PIC micros in SOT-23-6 and SOIC</description>
<gates>
<gate name="G$1" symbol="10F200T"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="GP0" pad="1"/>
<connect gate="G$1" pin="GP1" pad="3"/>
<connect gate="G$1" pin="GP2" pad="4"/>
<connect gate="G$1" pin="GP3" pad="6"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY10" prefix="IC">
<description>&lt;b&gt;ATtiny4/5/9/10&lt;/b&gt;
8-bit Microcontroller with 512/1024 Bytes In-System Programmable Flash</description>
<gates>
<gate name="G$1" symbol="ATTINY10"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="/RST" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PB0" pad="1"/>
<connect gate="G$1" pin="PB1" pad="3"/>
<connect gate="G$1" pin="PB2" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MAHR" package="UDFN-8">
<connects>
<connect gate="G$1" pin="/RST" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="1"/>
<connect gate="G$1" pin="PB2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1X4" prefix="CN">
<description>4-pin connector</description>
<gates>
<gate name="G$1" symbol="1X4"/>
</gates>
<devices>
<device name="FPC0.5" package="FPC_0.5MM-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BIG" package="1X04-BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CLEANBIG" package="1X04-CLEANBIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.5MM" package="1X04-3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X4-SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HL1606">
<gates>
<gate name="G$1" symbol="HL1606"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="A3" pad="1"/>
<connect gate="G$1" pin="B1" pad="16"/>
<connect gate="G$1" pin="B2" pad="15"/>
<connect gate="G$1" pin="B3" pad="14"/>
<connect gate="G$1" pin="CI" pad="7"/>
<connect gate="G$1" pin="CO" pad="10"/>
<connect gate="G$1" pin="DI" pad="6"/>
<connect gate="G$1" pin="DO" pad="11"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="LI" pad="8"/>
<connect gate="G$1" pin="LO" pad="9"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="12"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPST" prefix="S">
<description>Judco 50-0015-00</description>
<gates>
<gate name="G$1" symbol="SPST"/>
</gates>
<devices>
<device name="" package="JUDCOSPST">
<connects>
<connect gate="G$1" pin="P" pad="P"/>
<connect gate="G$1" pin="S" pad="T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JD-T1800" prefix="LCD">
<gates>
<gate name="G$1" symbol="JD-T1800"/>
</gates>
<devices>
<device name="" package="JD-T1800">
<connects>
<connect gate="G$1" pin="CLOCK" pad="9"/>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="DATA" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="13"/>
<connect gate="G$1" pin="LEDA" pad="4"/>
<connect gate="G$1" pin="LEDK" pad="3"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="RS/DC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL33X">
<gates>
<gate name="G$1" symbol="ADXL33X"/>
</gates>
<devices>
<device name="" package="16LCSP">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="6"/>
<connect gate="G$1" pin="GND3" pad="7"/>
<connect gate="G$1" pin="ST" pad="2"/>
<connect gate="G$1" pin="VS" pad="15"/>
<connect gate="G$1" pin="VS1" pad="14"/>
<connect gate="G$1" pin="XOUT" pad="12"/>
<connect gate="G$1" pin="YOUT" pad="10"/>
<connect gate="G$1" pin="ZOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EVQQ7" prefix="SQ" uservalue="yes">
<gates>
<gate name="G$1" symbol="NAVSWITCH"/>
</gates>
<devices>
<device name="GA50" package="EVQQ7GA50">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="COM1" pad="COM1"/>
<connect gate="G$1" pin="COM2" pad="COM2"/>
<connect gate="G$1" pin="COM3" pad="COM3"/>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN-171" prefix="X">
<gates>
<gate name="G$1" symbol="RN-171"/>
</gates>
<devices>
<device name="" package="RN-171">
<connects>
<connect gate="G$1" pin="/FLASH_CS" pad="15"/>
<connect gate="G$1" pin="/RESET" pad="40"/>
<connect gate="G$1" pin="ANTENNA" pad="24"/>
<connect gate="G$1" pin="BOOST_CTRL" pad="48"/>
<connect gate="G$1" pin="FORCE_AWAKE" pad="41"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND10" pad="28"/>
<connect gate="G$1" pin="GND11" pad="39"/>
<connect gate="G$1" pin="GND12" pad="47"/>
<connect gate="G$1" pin="GND2" pad="14"/>
<connect gate="G$1" pin="GND3" pad="20"/>
<connect gate="G$1" pin="GND4" pad="21"/>
<connect gate="G$1" pin="GND5" pad="22"/>
<connect gate="G$1" pin="GND6" pad="23"/>
<connect gate="G$1" pin="GND7" pad="25"/>
<connect gate="G$1" pin="GND8" pad="26"/>
<connect gate="G$1" pin="GND9" pad="27"/>
<connect gate="G$1" pin="GPIO1" pad="13"/>
<connect gate="G$1" pin="GPIO10" pad="46"/>
<connect gate="G$1" pin="GPIO11" pad="45"/>
<connect gate="G$1" pin="GPIO12" pad="44"/>
<connect gate="G$1" pin="GPIO13" pad="43"/>
<connect gate="G$1" pin="GPIO14" pad="42"/>
<connect gate="G$1" pin="GPIO2" pad="12"/>
<connect gate="G$1" pin="GPIO3" pad="11"/>
<connect gate="G$1" pin="GPIO4" pad="9"/>
<connect gate="G$1" pin="GPIO5" pad="8"/>
<connect gate="G$1" pin="GPIO6" pad="7"/>
<connect gate="G$1" pin="GPIO7" pad="6"/>
<connect gate="G$1" pin="GPIO8" pad="5"/>
<connect gate="G$1" pin="GPIO9" pad="4"/>
<connect gate="G$1" pin="MISO" pad="16"/>
<connect gate="G$1" pin="MOSI" pad="18"/>
<connect gate="G$1" pin="SCK" pad="17"/>
<connect gate="G$1" pin="SENSOR0" pad="29"/>
<connect gate="G$1" pin="SENSOR1" pad="30"/>
<connect gate="G$1" pin="SENSOR2" pad="31"/>
<connect gate="G$1" pin="SENSOR3" pad="32"/>
<connect gate="G$1" pin="SENSOR4" pad="35"/>
<connect gate="G$1" pin="SENSOR5" pad="36"/>
<connect gate="G$1" pin="SENSOR6" pad="37"/>
<connect gate="G$1" pin="SENSOR7" pad="38"/>
<connect gate="G$1" pin="SENSOR_PWR" pad="33"/>
<connect gate="G$1" pin="UART_RX" pad="3"/>
<connect gate="G$1" pin="UART_TX" pad="2"/>
<connect gate="G$1" pin="VBATT" pad="49"/>
<connect gate="G$1" pin="VDD_3V3" pad="10"/>
<connect gate="G$1" pin="VDD_RF" pad="34"/>
<connect gate="G$1" pin="VDD_SW" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X18" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD18"/>
</gates>
<devices>
<device name="" package="1X18">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BIG" package="1X18-BIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA" prefix="ANT">
<gates>
<gate name="G$1" symbol="ANT"/>
</gates>
<devices>
<device name="" package="RN-ANT">
<connects>
<connect gate="G$1" pin="FEED" pad="FEED"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*245" prefix="IC">
<description>Octal &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74245"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="MTC" package="SSOP20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X13" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD13"/>
</gates>
<devices>
<device name="" package="1X13">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_BIG" package="1X13-BIG">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP73871" prefix="IC">
<gates>
<gate name="G$1" symbol="MCP73871"/>
</gates>
<devices>
<device name="" package="QFN20">
<connects>
<connect gate="G$1" pin="/PG" pad="6"/>
<connect gate="G$1" pin="/TE" pad="9"/>
<connect gate="G$1" pin="CE" pad="17"/>
<connect gate="G$1" pin="GND1" pad="10"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="IN1" pad="18"/>
<connect gate="G$1" pin="IN2" pad="19"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="20"/>
<connect gate="G$1" pin="PROG1" pad="13"/>
<connect gate="G$1" pin="PROG2" pad="4"/>
<connect gate="G$1" pin="PROG3" pad="12"/>
<connect gate="G$1" pin="SEL" pad="3"/>
<connect gate="G$1" pin="STAT1/LBO" pad="8"/>
<connect gate="G$1" pin="STAT2" pad="7"/>
<connect gate="G$1" pin="THERM" pad="5"/>
<connect gate="G$1" pin="VBAT1" pad="14"/>
<connect gate="G$1" pin="VBAT2" pad="15"/>
<connect gate="G$1" pin="VBAT3" pad="16"/>
<connect gate="G$1" pin="VPCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AXP083" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="RESET_SUPERVISOR"/>
</gates>
<devices>
<device name="-SAG" package="SOT23">
<connects>
<connect gate="G$1" pin="/RESET" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE">
<gates>
<gate name="G$1" symbol="XBEE"/>
</gates>
<devices>
<device name="" package="XBEE">
<connects>
<connect gate="G$1" pin="AD0/DIO0" pad="20"/>
<connect gate="G$1" pin="AD1/DIO1" pad="19"/>
<connect gate="G$1" pin="AD2/DIO2" pad="18"/>
<connect gate="G$1" pin="AD3/DIO3" pad="17"/>
<connect gate="G$1" pin="AD4/DIO4" pad="11"/>
<connect gate="G$1" pin="ASC/AD5/DIO5" pad="15"/>
<connect gate="G$1" pin="CTS/DIO7" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DO8" pad="4"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR/DI8" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="ON/SLEEP" pad="13"/>
<connect gate="G$1" pin="PWM0/RSSI" pad="6"/>
<connect gate="G$1" pin="PWM1" pad="7"/>
<connect gate="G$1" pin="RESERVED" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RTS/AD6/DIO6" pad="16"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXS0102" prefix="U" uservalue="yes">
<description>&lt;b&gt;2-Bit Bi-Directional Level Shifter (I2C, etc.)&lt;/b&gt;
&lt;p&gt;Designed for I2C devices and has internal pullups.  Not to be confused with TX&lt;b&gt;B&lt;/b&gt;010x series.&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;1.2V-3.6V (VCCA) to 1.65V-5.5V (VCCB) bi-directional level shifter with auto direction sensing.&lt;/li&gt;
  &lt;li&gt;Max data rate - 24Mbps (Push Pull), 2Mbps (Open Drain)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey: 296-21931-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TXS0102"/>
</gates>
<devices>
<device name="" package="VFSOP-8">
<connects>
<connect gate="G$1" pin="A1" pad="P$5"/>
<connect gate="G$1" pin="A2" pad="P$4"/>
<connect gate="G$1" pin="B1" pad="P$8"/>
<connect gate="G$1" pin="B2" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OE" pad="P$6"/>
<connect gate="G$1" pin="VCCA" pad="P$3"/>
<connect gate="G$1" pin="VCCB" pad="P$7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0104PWR" prefix="U" uservalue="yes">
<description>&lt;b&gt;4-Bit Bi-Directional Level Shifter&lt;/b&gt;
&lt;ul&gt;
  &lt;li&gt;1.2V-3.6V (VCCA) to 1.65V-5.5V (VCCB) bi-directional level shifter with auto direction sensing.&lt;/li&gt;
  &lt;li&gt;Max data rate - VCCA 1.8V:  20Mbps (50ns), VCCA 3.3V: 100Mbps (10ns)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey: 296-21929-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TXB0104PWR"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="B1" pad="13"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="11"/>
<connect gate="G$1" pin="B4" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OE" pad="8"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TXB0108PWR" prefix="U" uservalue="yes">
<description>&lt;b&gt;8-Bit Bi-Directional Level Shifter&lt;/b&gt;
&lt;ul&gt;
  &lt;li&gt;1.2V-3.6V (VCCA) to 1.65V-5.5V (VCCB) bi-directional level shifter with auto direction sensing.&lt;/li&gt;
  &lt;li&gt;Max data rate - VCCA 1.8V:  20Mbps (50ns), VCCA 3.3V: 100Mbps (10ns)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Digikey: 296-21527-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TXB0108PWR"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="18"/>
<connect gate="G$1" pin="B3" pad="17"/>
<connect gate="G$1" pin="B4" pad="16"/>
<connect gate="G$1" pin="B5" pad="15"/>
<connect gate="G$1" pin="B6" pad="14"/>
<connect gate="G$1" pin="B7" pad="13"/>
<connect gate="G$1" pin="B8" pad="12"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OE" pad="10"/>
<connect gate="G$1" pin="VCCA" pad="2"/>
<connect gate="G$1" pin="VCCB" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK" prefix="U">
<description>&lt;b&gt;Thumb Joystick&lt;/b&gt;
Joystick commonly found in PS2 controllers. Two pots and a select switch. Adapted from Sparkfun Library (but for more common 6mm switch sticks)</description>
<gates>
<gate name="G$1" symbol="JOYSTICK"/>
</gates>
<devices>
<device name="PTH" package="JOYSTICK">
<connects>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="H+" pad="H1"/>
<connect gate="G$1" pin="H-" pad="H3"/>
<connect gate="G$1" pin="SEL+" pad="B1A"/>
<connect gate="G$1" pin="SEL-" pad="B2A"/>
<connect gate="G$1" pin="V" pad="V2"/>
<connect gate="G$1" pin="V+" pad="V1"/>
<connect gate="G$1" pin="V-" pad="V3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CR2032" uservalue="yes">
<gates>
<gate name="G$1" symbol="3V"/>
</gates>
<devices>
<device name="SMT" package="CR2032-SMD">
<connects>
<connect gate="G$1" pin="+" pad="+$1"/>
<connect gate="G$1" pin="+1" pad="+$2"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="THM" package="CR2032-THRU">
<connects>
<connect gate="G$1" pin="+" pad="+1"/>
<connect gate="G$1" pin="+1" pad="+2"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEGMENT_8X8_BICOLOR_ROWCATHODE" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;8x8 Bi-Color LED Segment Displays: Row = Cathode&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;1.2" Bi-Color 8x8 Matrix, 3.0mm Square LEDs - BL-M12A883XX&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_8X8_BICOLOR_CATHODEROW"/>
</gates>
<devices>
<device name="MI2A883XX" package="SEGMENT_BICOL_BL-M12A883XX">
<connects>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="A10" pad="2"/>
<connect gate="G$1" pin="A11" pad="4"/>
<connect gate="G$1" pin="A12" pad="5"/>
<connect gate="G$1" pin="A13" pad="7"/>
<connect gate="G$1" pin="A14" pad="8"/>
<connect gate="G$1" pin="A15" pad="10"/>
<connect gate="G$1" pin="A16" pad="11"/>
<connect gate="G$1" pin="A2" pad="23"/>
<connect gate="G$1" pin="A3" pad="21"/>
<connect gate="G$1" pin="A4" pad="20"/>
<connect gate="G$1" pin="A5" pad="18"/>
<connect gate="G$1" pin="A6" pad="17"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="14"/>
<connect gate="G$1" pin="A9" pad="1"/>
<connect gate="G$1" pin="K1" pad="22"/>
<connect gate="G$1" pin="K2" pad="19"/>
<connect gate="G$1" pin="K3" pad="16"/>
<connect gate="G$1" pin="K4" pad="13"/>
<connect gate="G$1" pin="K5" pad="3"/>
<connect gate="G$1" pin="K6" pad="6"/>
<connect gate="G$1" pin="K7" pad="9"/>
<connect gate="G$1" pin="K8" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEGMENT_8X8_ROWCATHODE" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;8x8 LED Segment Displays: Row = Cathode&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.7" Red 8X8 Matrix, 1.9mm Round LEDs - BL-M07C881UR&lt;/p&gt;
&lt;p&gt;1.2" Red 8x8 Matrix, 3.0mm Round LEDs - BL-M12A881UR&lt;/p&gt;
&lt;p&gt;1.2" Red 8x8 Matrix, 3.0mm Square LEDs - BL-M12A883&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_8X8_CATHODEROW"/>
</gates>
<devices>
<device name="" package="SEGMENT_BL-M07C881UR">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="16"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="14"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="K1" pad="1"/>
<connect gate="G$1" pin="K2" pad="2"/>
<connect gate="G$1" pin="K3" pad="3"/>
<connect gate="G$1" pin="K4" pad="4"/>
<connect gate="G$1" pin="K5" pad="12"/>
<connect gate="G$1" pin="K6" pad="11"/>
<connect gate="G$1" pin="K7" pad="10"/>
<connect gate="G$1" pin="K8" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M12A881UR" package="SEGMENT_BL-M12A881UR">
<connects>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="10"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="16"/>
<connect gate="G$1" pin="K1" pad="9"/>
<connect gate="G$1" pin="K2" pad="14"/>
<connect gate="G$1" pin="K3" pad="8"/>
<connect gate="G$1" pin="K4" pad="12"/>
<connect gate="G$1" pin="K5" pad="1"/>
<connect gate="G$1" pin="K6" pad="7"/>
<connect gate="G$1" pin="K7" pad="2"/>
<connect gate="G$1" pin="K8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BL-M12A883" package="SEGMENT_BL-M12A883">
<connects>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="10"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="16"/>
<connect gate="G$1" pin="K1" pad="9"/>
<connect gate="G$1" pin="K2" pad="14"/>
<connect gate="G$1" pin="K3" pad="8"/>
<connect gate="G$1" pin="K4" pad="12"/>
<connect gate="G$1" pin="K5" pad="1"/>
<connect gate="G$1" pin="K6" pad="7"/>
<connect gate="G$1" pin="K7" pad="2"/>
<connect gate="G$1" pin="K8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BL-M15" package="SEGMENT_BL-M15A881">
<connects>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="10"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="16"/>
<connect gate="G$1" pin="K1" pad="9"/>
<connect gate="G$1" pin="K2" pad="14"/>
<connect gate="G$1" pin="K3" pad="8"/>
<connect gate="G$1" pin="K4" pad="12"/>
<connect gate="G$1" pin="K5" pad="1"/>
<connect gate="G$1" pin="K6" pad="7"/>
<connect gate="G$1" pin="K7" pad="2"/>
<connect gate="G$1" pin="K8" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEGMENT_12BAR_BICOLOR" prefix="LED" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;12-Bar Bi-Color LED Segment Displays: Row = Cathode&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;30.2 x 10.1mm Bi-Color 12 LED Bar Graph, 5.0 x 1.74mm Square LEDs - BL-AR12Z3010&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEGMENT_12BAR_BICOLOR_CATHODEROW"/>
</gates>
<devices>
<device name="AR12Z3010" package="SEGMENT_BICOL_BL-AR12Z3010">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="14"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="9"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="K1" pad="2"/>
<connect gate="G$1" pin="K2" pad="13"/>
<connect gate="G$1" pin="K3" pad="3"/>
<connect gate="G$1" pin="K4" pad="12"/>
<connect gate="G$1" pin="K5" pad="4"/>
<connect gate="G$1" pin="K6" pad="11"/>
<connect gate="G$1" pin="K7" pad="5"/>
<connect gate="G$1" pin="K8" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1337">
<description>DS1337 - Maxim RTC without battery backup</description>
<gates>
<gate name="G$1" symbol="DS1337"/>
</gates>
<devices>
<device name="" package="DIL08-ROUND">
<connects>
<connect gate="G$1" pin="#INTA" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW/#INTB" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA168*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 kBytes FLASH&lt;p&gt;
1 kBytes SRAM&lt;p&gt;
512 Bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA168"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="14"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="15"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="3"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="5"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="16"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="6"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="11"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="12"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="17"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="10"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="ROUND" package="DIL28-3-ROUND">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="14"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="15"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="3"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="5"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="16"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="6"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="11"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="12"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="17"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="10"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1302">
<description>DS1302 - Real time clock with supercap trickle charger</description>
<gates>
<gate name="G$1" symbol="DS1302"/>
</gates>
<devices>
<device name="" package="DIL08-ROUND">
<connects>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="I/O" pad="6"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="VBAT" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="X1" pad="2"/>
<connect gate="G$1" pin="X2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPERCAP" prefix="C" uservalue="yes">
<gates>
<gate name="G$1" symbol="CPOL-US"/>
</gates>
<devices>
<device name="" package="414-VA5R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TM1804" prefix="IC">
<description>TM1804 is a PWM LED driver chip with manchester code data transfer!</description>
<gates>
<gate name="G$1" symbol="TM1804"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="DO" pad="5"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="SET" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SKINNY" package="SO08-SKINNYPADS">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="DO" pad="5"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="SET" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RGBLED" prefix="LED">
<description>For 5050 RGB LEDs, the order of the LEDs may vary from one manufacturer to another!</description>
<gates>
<gate name="G$1" symbol="RGBLED"/>
</gates>
<devices>
<device name="5050" package="RGBLED5050">
<connects>
<connect gate="G$1" pin="BLUE_A" pad="3"/>
<connect gate="G$1" pin="BLUE_C" pad="4"/>
<connect gate="G$1" pin="GREEN_A" pad="1"/>
<connect gate="G$1" pin="GREEN_C" pad="6"/>
<connect gate="G$1" pin="RED_A" pad="2"/>
<connect gate="G$1" pin="RED_C" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEWTAP" prefix="TP">
<gates>
<gate name="G$1" symbol="SEWTAP"/>
</gates>
<devices>
<device name="0.5IN" package="SEWINGTAP_0.5">
<connects>
<connect gate="G$1" pin="SEW" pad="TAP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.4IN" package="SEWINGTAP_0.4">
<connects>
<connect gate="G$1" pin="SEW" pad="TAP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2.0IN" package="SEWINGTAP_2.0">
<connects>
<connect gate="G$1" pin="SEW" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BIG" package="BIGTAP">
<connects>
<connect gate="G$1" pin="SEW" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP23017" prefix="IC">
<description>&lt;b&gt;http://ww1.microchip.com/downloads/en/DeviceDoc/21952a.pdf&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21952a.pdf</description>
<gates>
<gate name="G$1" symbol="MCP23017"/>
</gates>
<devices>
<device name="SP" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SO28W">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SS" package="SSOP28">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ML" package="QFN28-ML_6X6MM">
<connects>
<connect gate="G$1" pin="!RESET" pad="14"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="12"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="GPA0" pad="17"/>
<connect gate="G$1" pin="GPA1" pad="18"/>
<connect gate="G$1" pin="GPA2" pad="19"/>
<connect gate="G$1" pin="GPA3" pad="20"/>
<connect gate="G$1" pin="GPA4" pad="21"/>
<connect gate="G$1" pin="GPA5" pad="22"/>
<connect gate="G$1" pin="GPA6" pad="23"/>
<connect gate="G$1" pin="GPA7" pad="24"/>
<connect gate="G$1" pin="GPB0" pad="25"/>
<connect gate="G$1" pin="GPB1" pad="26"/>
<connect gate="G$1" pin="GPB2" pad="27"/>
<connect gate="G$1" pin="GPB3" pad="28"/>
<connect gate="G$1" pin="GPB4" pad="1"/>
<connect gate="G$1" pin="GPB5" pad="2"/>
<connect gate="G$1" pin="GPB6" pad="3"/>
<connect gate="G$1" pin="GPB7" pad="4"/>
<connect gate="G$1" pin="INTA" pad="16"/>
<connect gate="G$1" pin="INTB" pad="15"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SP2" package="DIL28-3-ROUND">
<connects>
<connect gate="G$1" pin="!RESET" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="17"/>
<connect gate="G$1" pin="GPA0" pad="21"/>
<connect gate="G$1" pin="GPA1" pad="22"/>
<connect gate="G$1" pin="GPA2" pad="23"/>
<connect gate="G$1" pin="GPA3" pad="24"/>
<connect gate="G$1" pin="GPA4" pad="25"/>
<connect gate="G$1" pin="GPA5" pad="26"/>
<connect gate="G$1" pin="GPA6" pad="27"/>
<connect gate="G$1" pin="GPA7" pad="28"/>
<connect gate="G$1" pin="GPB0" pad="1"/>
<connect gate="G$1" pin="GPB1" pad="2"/>
<connect gate="G$1" pin="GPB2" pad="3"/>
<connect gate="G$1" pin="GPB3" pad="4"/>
<connect gate="G$1" pin="GPB4" pad="5"/>
<connect gate="G$1" pin="GPB5" pad="6"/>
<connect gate="G$1" pin="GPB6" pad="7"/>
<connect gate="G$1" pin="GPB7" pad="8"/>
<connect gate="G$1" pin="INTA" pad="20"/>
<connect gate="G$1" pin="INTB" pad="19"/>
<connect gate="G$1" pin="SCL" pad="12"/>
<connect gate="G$1" pin="SDA" pad="13"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2811" prefix="IC">
<gates>
<gate name="G$1" symbol="WS2811"/>
</gates>
<devices>
<device name="-SOP8" package="SO08-SKINNYPADS">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="DO" pad="5"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="SET" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A1171" prefix="IC">
<description>A1171 Allegro push-pull hall effect sensor</description>
<gates>
<gate name="G$1" symbol="A1171"/>
</gates>
<devices>
<device name="" package="DFN-6">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SELECT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VOUTPN" pad="2"/>
<connect gate="G$1" pin="VOUTPS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-N" prefix="Q" uservalue="yes">
<description>&lt;b&gt;N-Channel Mosfet&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;2N7002E - 60V 260mA SOT23 [Digikey: 2N7002ET1GOSTR-ND] - &lt;b&gt;REEL&lt;/b&gt;&lt;/li&gt;
&lt;li&gt;BSH103 - 30V 850mA SOT23 [Digikey: 568-5013-1-ND]&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MOSFET-N"/>
</gates>
<devices>
<device name="WAVE" package="SOT23-W">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="REFLOW" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GDS_TO220V" package="TO220V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB" prefix="IC">
<gates>
<gate name="G$1" symbol="AT45DBXXX"/>
</gates>
<devices>
<device name="-S" package="SOIC8_208MIL">
<connects>
<connect gate="G$1" pin="/CS" pad="4"/>
<connect gate="G$1" pin="/RST" pad="3"/>
<connect gate="G$1" pin="/WP" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_3PIN" prefix="CN" uservalue="yes">
<gates>
<gate name="G$1" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="JSTPH3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINOR3" prefix="U">
<description>This is a new object for the new Arduino R3 - with extra pins that you may want to use (such as IOref, and duplicated A4/A5</description>
<gates>
<gate name="G$1" symbol="ARDUINOR3"/>
</gates>
<devices>
<device name="-DIMENSION" package="ARDUINOR3">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BPLACE" package="ARDUINOR3-BPLACE">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HD44780LCD_RGB">
<gates>
<gate name="G$1" symbol="CHARLCD_RGB"/>
</gates>
<devices>
<device name="LONGPINS" package="LCD1602-RGB">
<connects>
<connect gate="G$1" pin="ANODE" pad="15"/>
<connect gate="G$1" pin="BLUE" pad="18"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="10"/>
<connect gate="G$1" pin="DB4" pad="11"/>
<connect gate="G$1" pin="DB5" pad="12"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="E" pad="6"/>
<connect gate="G$1" pin="GREEN" pad="17"/>
<connect gate="G$1" pin="RED" pad="16"/>
<connect gate="G$1" pin="RS" pad="4"/>
<connect gate="G$1" pin="RW" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIM" prefix="TM" uservalue="yes">
<gates>
<gate name="G$1" symbol="TRIM"/>
</gates>
<devices>
<device name="" package="6MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SLIDE45" package="SLIDEPOT-45">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="E" pad="C"/>
<connect gate="G$1" pin="S" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3386" package="TRIM-3386">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HUB75MATRIX" prefix="LED">
<gates>
<gate name="G$1" symbol="HUB75_IDC"/>
</gates>
<devices>
<device name="" package="2X08-IDC">
<connects>
<connect gate="G$1" pin="/ENABLE" pad="15"/>
<connect gate="G$1" pin="ADDR_A" pad="9"/>
<connect gate="G$1" pin="ADDR_B" pad="10"/>
<connect gate="G$1" pin="ADDR_C" pad="11"/>
<connect gate="G$1" pin="BLUE1" pad="3"/>
<connect gate="G$1" pin="BLUE2" pad="7"/>
<connect gate="G$1" pin="CLOCK" pad="13"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND1" pad="8"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="GND3" pad="16"/>
<connect gate="G$1" pin="GREEN1" pad="2"/>
<connect gate="G$1" pin="GREEN2" pad="6"/>
<connect gate="G$1" pin="LATCH" pad="14"/>
<connect gate="G$1" pin="RED1" pad="1"/>
<connect gate="G$1" pin="RED2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS3231" prefix="IC">
<gates>
<gate name="G$1" symbol="DS3231"/>
</gates>
<devices>
<device name="/SO" package="SO16W">
<connects>
<connect gate="G$1" pin="/RST" pad="4"/>
<connect gate="G$1" pin="32KHZ" pad="1"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="7"/>
<connect gate="G$1" pin="NC3" pad="8"/>
<connect gate="G$1" pin="NC4" pad="9"/>
<connect gate="G$1" pin="NC5" pad="10"/>
<connect gate="G$1" pin="NC6" pad="11"/>
<connect gate="G$1" pin="NC7" pad="12"/>
<connect gate="G$1" pin="SCL" pad="16"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="SQW/INT" pad="3"/>
<connect gate="G$1" pin="VBAT" pad="14"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HUB08MATRIX" prefix="LED">
<gates>
<gate name="G$1" symbol="HUB08_IDC"/>
</gates>
<devices>
<device name="" package="2X08-IDC">
<connects>
<connect gate="G$1" pin="/ENABLE" pad="7"/>
<connect gate="G$1" pin="ADDR_A" pad="2"/>
<connect gate="G$1" pin="ADDR_B" pad="4"/>
<connect gate="G$1" pin="ADDR_C" pad="6"/>
<connect gate="G$1" pin="ADDR_D" pad="8"/>
<connect gate="G$1" pin="BLUE" pad="11"/>
<connect gate="G$1" pin="CLOCK" pad="16"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="GND4" pad="15"/>
<connect gate="G$1" pin="GREEN" pad="10"/>
<connect gate="G$1" pin="LATCH" pad="14"/>
<connect gate="G$1" pin="N/C" pad="12"/>
<connect gate="G$1" pin="RED" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX486X" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX486X"/>
</gates>
<devices>
<device name="/SOT" package="SOT23-6">
<connects>
<connect gate="G$1" pin="/EN" pad="6"/>
<connect gate="G$1" pin="FLAG" pad="3"/>
<connect gate="G$1" pin="GATEN" pad="4"/>
<connect gate="G$1" pin="GATEP" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-P" prefix="Q">
<gates>
<gate name="G$1" symbol="P-MOSFET"/>
</gates>
<devices>
<device name="GDS_TO220V" package="TO220V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DPDT" prefix="SW" uservalue="yes">
<gates>
<gate name="1" symbol="TSU"/>
<gate name="2" symbol="TSU"/>
</gates>
<devices>
<device name="-EG1390" package="EG1390">
<connects>
<connect gate="1" pin="O" pad="O1"/>
<connect gate="1" pin="P" pad="P1"/>
<connect gate="1" pin="S" pad="S1"/>
<connect gate="2" pin="O" pad="O2"/>
<connect gate="2" pin="P" pad="P2"/>
<connect gate="2" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BEAGLEBONE_OUTLINE">
<description>Should match A3 pinout - but not completely tested</description>
<gates>
<gate name="G$1" symbol="BEAGLEBONE-1"/>
</gates>
<devices>
<device name="" package="BEAGLEBONE_SHIELD">
<connects>
<connect gate="G$1" pin="AIN0" pad="85"/>
<connect gate="G$1" pin="AIN1" pad="86"/>
<connect gate="G$1" pin="AIN2" pad="83"/>
<connect gate="G$1" pin="AIN3" pad="84"/>
<connect gate="G$1" pin="AIN4" pad="79"/>
<connect gate="G$1" pin="AIN5" pad="82"/>
<connect gate="G$1" pin="AIN6" pad="81"/>
<connect gate="G$1" pin="CLKOUT2" pad="87"/>
<connect gate="G$1" pin="EHRPWM1A" pad="60"/>
<connect gate="G$1" pin="EHRPWM1B" pad="62"/>
<connect gate="G$1" pin="EHRPWM2A" pad="19"/>
<connect gate="G$1" pin="EHRPWM2B" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="47"/>
<connect gate="G$1" pin="GND@2" pad="48"/>
<connect gate="G$1" pin="GND@3" pad="89"/>
<connect gate="G$1" pin="GND@4" pad="91"/>
<connect gate="G$1" pin="GND@5" pad="90"/>
<connect gate="G$1" pin="GND@6" pad="92"/>
<connect gate="G$1" pin="GND@7" pad="1"/>
<connect gate="G$1" pin="GND@8" pad="2"/>
<connect gate="G$1" pin="GNDA_ADC" pad="80"/>
<connect gate="G$1" pin="GPIO0_26" pad="14"/>
<connect gate="G$1" pin="GPIO0_27" pad="17"/>
<connect gate="G$1" pin="GPIO0_7" pad="88"/>
<connect gate="G$1" pin="GPIO1_0" pad="25"/>
<connect gate="G$1" pin="GPIO1_1" pad="24"/>
<connect gate="G$1" pin="GPIO1_12" pad="12"/>
<connect gate="G$1" pin="GPIO1_13" pad="11"/>
<connect gate="G$1" pin="GPIO1_14" pad="16"/>
<connect gate="G$1" pin="GPIO1_15" pad="15"/>
<connect gate="G$1" pin="GPIO1_16" pad="61"/>
<connect gate="G$1" pin="GPIO1_17" pad="69"/>
<connect gate="G$1" pin="GPIO1_2" pad="5"/>
<connect gate="G$1" pin="GPIO1_28" pad="58"/>
<connect gate="G$1" pin="GPIO1_29" pad="26"/>
<connect gate="G$1" pin="GPIO1_3" pad="6"/>
<connect gate="G$1" pin="GPIO1_30" pad="21"/>
<connect gate="G$1" pin="GPIO1_31" pad="20"/>
<connect gate="G$1" pin="GPIO1_4" pad="23"/>
<connect gate="G$1" pin="GPIO1_5" pad="22"/>
<connect gate="G$1" pin="GPIO1_6" pad="3"/>
<connect gate="G$1" pin="GPIO1_7" pad="4"/>
<connect gate="G$1" pin="GPIO2_1" pad="18"/>
<connect gate="G$1" pin="GPIO2_10" pad="41"/>
<connect gate="G$1" pin="GPIO2_11" pad="42"/>
<connect gate="G$1" pin="GPIO2_12" pad="39"/>
<connect gate="G$1" pin="GPIO2_13" pad="40"/>
<connect gate="G$1" pin="GPIO2_22" pad="27"/>
<connect gate="G$1" pin="GPIO2_23" pad="29"/>
<connect gate="G$1" pin="GPIO2_24" pad="28"/>
<connect gate="G$1" pin="GPIO2_25" pad="30"/>
<connect gate="G$1" pin="GPIO2_6" pad="45"/>
<connect gate="G$1" pin="GPIO2_7" pad="46"/>
<connect gate="G$1" pin="GPIO2_8" pad="43"/>
<connect gate="G$1" pin="GPIO2_9" pad="44"/>
<connect gate="G$1" pin="GPIO3_19" pad="73"/>
<connect gate="G$1" pin="GPIO3_21" pad="71"/>
<connect gate="G$1" pin="I2C1_SCL" pad="63"/>
<connect gate="G$1" pin="I2C1_SDA" pad="64"/>
<connect gate="G$1" pin="I2C2_SCL" pad="65"/>
<connect gate="G$1" pin="I2C2_SDA" pad="66"/>
<connect gate="G$1" pin="PWR_BUT" pad="55"/>
<connect gate="G$1" pin="SPI1_CS0" pad="74"/>
<connect gate="G$1" pin="SPI1_DI" pad="76"/>
<connect gate="G$1" pin="SPI1_DO" pad="75"/>
<connect gate="G$1" pin="SPI1_SCLK" pad="77"/>
<connect gate="G$1" pin="SYS_5V@1" pad="53"/>
<connect gate="G$1" pin="SYS_5V@2" pad="54"/>
<connect gate="G$1" pin="SYS_RESETN" pad="56"/>
<connect gate="G$1" pin="TIMER4" pad="7"/>
<connect gate="G$1" pin="TIMER5" pad="9"/>
<connect gate="G$1" pin="TIMER6" pad="10"/>
<connect gate="G$1" pin="TIMER7" pad="8"/>
<connect gate="G$1" pin="UART1_RXD" pad="72"/>
<connect gate="G$1" pin="UART1_TXD" pad="70"/>
<connect gate="G$1" pin="UART2_RXD" pad="68"/>
<connect gate="G$1" pin="UART2_TXD" pad="67"/>
<connect gate="G$1" pin="UART3_CTSN" pad="36"/>
<connect gate="G$1" pin="UART3_RTSN" pad="34"/>
<connect gate="G$1" pin="UART4_CTSN" pad="35"/>
<connect gate="G$1" pin="UART4_RTSN" pad="33"/>
<connect gate="G$1" pin="UART4_RXD" pad="57"/>
<connect gate="G$1" pin="UART4_TXD" pad="59"/>
<connect gate="G$1" pin="UART5_CTSN" pad="31"/>
<connect gate="G$1" pin="UART5_RTSN" pad="32"/>
<connect gate="G$1" pin="UART5_RXD" pad="38"/>
<connect gate="G$1" pin="UART5_TXD" pad="37"/>
<connect gate="G$1" pin="VDD_3V3EXP@1" pad="49"/>
<connect gate="G$1" pin="VDD_3V3EXP@2" pad="50"/>
<connect gate="G$1" pin="VDD_5V@1" pad="51"/>
<connect gate="G$1" pin="VDD_5V@2" pad="52"/>
<connect gate="G$1" pin="VDD_ADC" pad="78"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINOR3-NOIOREF" prefix="Q">
<gates>
<gate name="G$1" symbol="ARDUINOR3-NOIOREF"/>
</gates>
<devices>
<device name="-NOTEXT" package="ARDUINOR3-NOTEXT-NOIOREF">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS_FGPMMOPA6B" prefix="U" uservalue="yes">
<description>&lt;b&gt;FGPMMOPA6B&lt;/b&gt; 16x16x0.6mm GPS Module
&lt;p&gt;&lt;b&gt;NMEA Sentences&lt;/b&gt;: GGA, GSA, GSV, RMC, VTG&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;General Specifications&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;Chipset&lt;/b&gt;: MTK MT3329&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Baud Rate&lt;/b&gt;: 9600bps (default)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Update Rate&lt;/b&gt;: 1Hz (default)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Cold Start&lt;/b&gt;: ~35s&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Operating Temp&lt;/b&gt;: -40 to 85°C&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;
&lt;b&gt;DC Characteristics&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;Supply Voltage&lt;/b&gt;: 3.2-5.0V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Backup Battery Voltage&lt;/b&gt;: 2.0-4.3V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Digital Logic (UART)&lt;/b&gt;: 3.3V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;I(Tracking)&lt;/b&gt;: 42mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;I(Acquisition)&lt;/b&gt;: 53mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;I(BackupBattery)&lt;/b&gt;: 10uA&lt;/li&gt;

&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FGPMMOPA6B"/>
</gates>
<devices>
<device name="" package="FGPMMOPA6B">
<connects>
<connect gate="G$1" pin="3D-FIX" pad="P$5"/>
<connect gate="G$1" pin="DMINUS" pad="P$7"/>
<connect gate="G$1" pin="DPLUS" pad="P$6"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$8"/>
<connect gate="G$1" pin="NC@1" pad="P$11"/>
<connect gate="G$1" pin="NC@2" pad="P$12"/>
<connect gate="G$1" pin="RX" pad="P$10"/>
<connect gate="G$1" pin="TX" pad="P$9"/>
<connect gate="G$1" pin="VBACKUP" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS_FGPMMOPA6C" prefix="U" uservalue="yes">
<description>&lt;b&gt;FGPMMOPA6C&lt;/b&gt; 16x16 GPS Module
&lt;p&gt;&lt;b&gt;NMEA Sentences&lt;/b&gt;: GGA, GSA, GSV, RMC, VTG&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FGPMMOPA6C"/>
</gates>
<devices>
<device name="" package="FGPMMOPA6C">
<connects>
<connect gate="G$1" pin="1PPS" pad="P$6"/>
<connect gate="G$1" pin="3D-FIX" pad="P$5"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$8"/>
<connect gate="G$1" pin="NC@1" pad="P$2"/>
<connect gate="G$1" pin="NC@2" pad="P$7"/>
<connect gate="G$1" pin="NC@3" pad="P$11"/>
<connect gate="G$1" pin="NC@4" pad="P$13"/>
<connect gate="G$1" pin="NC@5" pad="P$12"/>
<connect gate="G$1" pin="RX" pad="P$10"/>
<connect gate="G$1" pin="TX" pad="P$9"/>
<connect gate="G$1" pin="VBACKUP" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X4"/>
</gates>
<devices>
<device name="" package="2X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINOMICRO">
<gates>
<gate name="G$1" symbol="ARDUINOMICRO"/>
</gates>
<devices>
<device name="" package="ARDUINOMICRO">
<connects>
<connect gate="G$1" pin="10" pad="P$3"/>
<connect gate="G$1" pin="11" pad="P$2"/>
<connect gate="G$1" pin="12" pad="P$1"/>
<connect gate="G$1" pin="13" pad="P$34"/>
<connect gate="G$1" pin="2" pad="P$11"/>
<connect gate="G$1" pin="3" pad="P$10"/>
<connect gate="G$1" pin="3V" pad="P$33"/>
<connect gate="G$1" pin="4" pad="P$9"/>
<connect gate="G$1" pin="5" pad="P$8"/>
<connect gate="G$1" pin="5V" pad="P$23"/>
<connect gate="G$1" pin="6" pad="P$7"/>
<connect gate="G$1" pin="7" pad="P$6"/>
<connect gate="G$1" pin="8" pad="P$5"/>
<connect gate="G$1" pin="9" pad="P$4"/>
<connect gate="G$1" pin="9V" pad="P$20"/>
<connect gate="G$1" pin="A0" pad="P$31"/>
<connect gate="G$1" pin="A1" pad="P$30"/>
<connect gate="G$1" pin="A2" pad="P$29"/>
<connect gate="G$1" pin="A3" pad="P$28"/>
<connect gate="G$1" pin="A4" pad="P$27"/>
<connect gate="G$1" pin="A5" pad="P$26"/>
<connect gate="G$1" pin="AREF" pad="P$32"/>
<connect gate="G$1" pin="GND" pad="P$12"/>
<connect gate="G$1" pin="GND@1" pad="P$21"/>
<connect gate="G$1" pin="MISO" pad="P$19"/>
<connect gate="G$1" pin="MOSI" pad="P$17"/>
<connect gate="G$1" pin="NC@1" pad="P$24"/>
<connect gate="G$1" pin="NC@2" pad="P$25"/>
<connect gate="G$1" pin="R@1" pad="P$13"/>
<connect gate="G$1" pin="R@2" pad="P$22"/>
<connect gate="G$1" pin="RX" pad="P$14"/>
<connect gate="G$1" pin="SCK" pad="P$18"/>
<connect gate="G$1" pin="SS" pad="P$16"/>
<connect gate="G$1" pin="TX" pad="P$15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1X17-SPRINGTERMINAL" prefix="Q">
<gates>
<gate name="G$1" symbol="SPRINGTERMININAL-1X17"/>
</gates>
<devices>
<device name="" package="SPRINGTERMINAL-17">
<connects>
<connect gate="G$1" pin="'1" pad="1'"/>
<connect gate="G$1" pin="'10" pad="10'"/>
<connect gate="G$1" pin="'11" pad="11'"/>
<connect gate="G$1" pin="'12" pad="12'"/>
<connect gate="G$1" pin="'13" pad="13'"/>
<connect gate="G$1" pin="'14" pad="14'"/>
<connect gate="G$1" pin="'15" pad="15'"/>
<connect gate="G$1" pin="'16" pad="16'"/>
<connect gate="G$1" pin="'17" pad="17'"/>
<connect gate="G$1" pin="'2" pad="2'"/>
<connect gate="G$1" pin="'3" pad="3'"/>
<connect gate="G$1" pin="'4" pad="4'"/>
<connect gate="G$1" pin="'5" pad="5'"/>
<connect gate="G$1" pin="'6" pad="6'"/>
<connect gate="G$1" pin="'7" pad="7'"/>
<connect gate="G$1" pin="'8" pad="8'"/>
<connect gate="G$1" pin="'9" pad="9'"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9685" prefix="U" uservalue="yes">
<description>&lt;b&gt;PCA9685&lt;/b&gt; - 16 Channel 12-Bit I2C PWM Controller
&lt;p&gt;5.0V tolerant 16 channel, 12-bit I2C PWM controller with 25mA per output (max. 400mA total)&lt;/p&gt;
&lt;p&gt;Digikey: 568-5931-1-ND&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PCA9865"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="G$1" pin="#OE" pad="23"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="24"/>
<connect gate="G$1" pin="EXTCLK" pad="25"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="PWM0" pad="6"/>
<connect gate="G$1" pin="PWM1" pad="7"/>
<connect gate="G$1" pin="PWM10" pad="17"/>
<connect gate="G$1" pin="PWM11" pad="18"/>
<connect gate="G$1" pin="PWM12" pad="19"/>
<connect gate="G$1" pin="PWM13" pad="20"/>
<connect gate="G$1" pin="PWM14" pad="21"/>
<connect gate="G$1" pin="PWM15" pad="22"/>
<connect gate="G$1" pin="PWM2" pad="8"/>
<connect gate="G$1" pin="PWM3" pad="9"/>
<connect gate="G$1" pin="PWM4" pad="10"/>
<connect gate="G$1" pin="PWM5" pad="11"/>
<connect gate="G$1" pin="PWM6" pad="12"/>
<connect gate="G$1" pin="PWM7" pad="13"/>
<connect gate="G$1" pin="PWM8" pad="15"/>
<connect gate="G$1" pin="PWM9" pad="16"/>
<connect gate="G$1" pin="SCL" pad="26"/>
<connect gate="G$1" pin="SDA" pad="27"/>
<connect gate="G$1" pin="VDD" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS_FGPMMOPA6H" prefix="U" uservalue="yes">
<description>&lt;b&gt;GPS Module&lt;/b&gt; - MTK MT3339 Chipset, -165dBm sensitivity, 22 channels, 10Hz, auto-select external antenna options</description>
<gates>
<gate name="G$1" symbol="FGPMMOPA6H"/>
</gates>
<devices>
<device name="" package="FGPMMOPA6H">
<connects>
<connect gate="G$1" pin="1PPS" pad="P$13"/>
<connect gate="G$1" pin="3D-FIX" pad="P$5"/>
<connect gate="G$1" pin="EX_ANT" pad="P$11"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$8"/>
<connect gate="G$1" pin="GND@3" pad="P$12"/>
<connect gate="G$1" pin="GND@4" pad="P$19"/>
<connect gate="G$1" pin="NC@1" pad="P$6"/>
<connect gate="G$1" pin="NC@2" pad="P$7"/>
<connect gate="G$1" pin="NC@3" pad="P$15"/>
<connect gate="G$1" pin="NC@4" pad="P$16"/>
<connect gate="G$1" pin="NC@5" pad="P$17"/>
<connect gate="G$1" pin="NC@6" pad="P$18"/>
<connect gate="G$1" pin="NC@7" pad="P$20"/>
<connect gate="G$1" pin="NRESET" pad="P$2"/>
<connect gate="G$1" pin="RTCM" pad="P$14"/>
<connect gate="G$1" pin="RX" pad="P$10"/>
<connect gate="G$1" pin="TX" pad="P$9"/>
<connect gate="G$1" pin="VBACKUP" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Q" uservalue="yes">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="HC49S" package="HC49/S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49GW" package="HC49GW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49TL-H" package="HC49TL-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U-H" package="HC49U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1666973"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U-LM" package="HC49U-LM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1666956"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U-V" package="HC49U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1666969"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U70" package="HC49U70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49UP" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC13U-H" package="HC13U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC18U-H" package="HC18U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC18U-V" package="HC18U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC33U-H" package="HC33U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC33U-V" package="HC33U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SM49" package="SM49">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TC26H" package="TC26H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TC26V" package="TC26V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TC38H" package="TC38H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="68SMX" package="86SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="6344860"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="MM20SS" package="MM20SS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="MM39SL" package="MM39SL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="CTS406" package="CTS406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP3008" prefix="IC">
<gates>
<gate name="G$1" symbol="MCP3008"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="/CS" pad="10"/>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="DIN" pad="11"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT42QT1070" prefix="IC">
<description>&lt;b&gt;QTouch 5-channel standalone sensor IC&lt;/b&gt;
&lt;br&gt;
AT42QT1070 in standalone mode has 5 inputs (guard + 4 key) and open drain outputs. 1.8V-5.5V power.</description>
<gates>
<gate name="G$1" symbol="AT42QT1070"/>
</gates>
<devices>
<device name="-SSU" package="SO14">
<connects>
<connect gate="G$1" pin="!RST" pad="4"/>
<connect gate="G$1" pin="G_IN" pad="13"/>
<connect gate="G$1" pin="G_OUT" pad="3"/>
<connect gate="G$1" pin="IN1" pad="12"/>
<connect gate="G$1" pin="IN2" pad="11"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="9"/>
<connect gate="G$1" pin="MODE" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="8"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="6"/>
<connect gate="G$1" pin="OUT4" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_R3_ICSP" prefix="M">
<gates>
<gate name="G$1" symbol="ARDUINOR3-ICSP"/>
</gates>
<devices>
<device name="" package="ARDUINOR3_ICSP">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="5V@1" pad="5V_ICSP"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@3"/>
<connect gate="G$1" pin="GND@2" pad="GND@1"/>
<connect gate="G$1" pin="GND@3" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="RST" pad="RESET_ICSP"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="ARDUINOR3_ICSP_SMT">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="5V@1" pad="5V_ICSP"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="RST" pad="RESET_ICSP"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NODIM" package="ARDUINOR3_ICSP_NODIM">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="5V@1" pad="5V_ICSP"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4/SDA" pad="A4"/>
<connect gate="G$1" pin="A5/SCL" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND@3"/>
<connect gate="G$1" pin="GND@2" pad="GND@1"/>
<connect gate="G$1" pin="GND@3" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED"/>
<connect gate="G$1" pin="RST" pad="RESET_ICSP"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="40-XX" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="TS2"/>
</gates>
<devices>
<device name="" package="B3F-40XX">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="B3F-4000"/>
<attribute name="OC_FARNELL" value="176434"/>
<attribute name="OC_NEWARK" value="36K3105"/>
</technology>
</technologies>
</device>
<device name="-ROUND" package="B3F-40XX-ROUND">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="1" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4093" prefix="IC">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; schmitt trigger</description>
<gates>
<gate name="A" symbol="4093"/>
<gate name="B" symbol="4093"/>
<gate name="C" symbol="4093"/>
<gate name="D" symbol="4093"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DT" package="MC14093B-TSSOP14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5947" prefix="IC">
<gates>
<gate name="G$1" symbol="TLC5947"/>
<gate name="G$2" symbol="THERMAL_PAD"/>
</gates>
<devices>
<device name="-DAP" package="HTSSOP32DAP">
<connects>
<connect gate="G$1" pin="BLANK" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IREF" pad="31"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="15"/>
<connect gate="G$1" pin="OUT11" pad="16"/>
<connect gate="G$1" pin="OUT12" pad="17"/>
<connect gate="G$1" pin="OUT13" pad="18"/>
<connect gate="G$1" pin="OUT14" pad="19"/>
<connect gate="G$1" pin="OUT15" pad="20"/>
<connect gate="G$1" pin="OUT16" pad="21"/>
<connect gate="G$1" pin="OUT17" pad="22"/>
<connect gate="G$1" pin="OUT18" pad="23"/>
<connect gate="G$1" pin="OUT19" pad="24"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT20" pad="25"/>
<connect gate="G$1" pin="OUT21" pad="26"/>
<connect gate="G$1" pin="OUT22" pad="27"/>
<connect gate="G$1" pin="OUT23" pad="28"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="13"/>
<connect gate="G$1" pin="OUT9" pad="14"/>
<connect gate="G$1" pin="SCLK" pad="3"/>
<connect gate="G$1" pin="SIN" pad="4"/>
<connect gate="G$1" pin="SOUT" pad="29"/>
<connect gate="G$1" pin="VCC" pad="32"/>
<connect gate="G$1" pin="XLAT" pad="30"/>
<connect gate="G$2" pin="PAD" pad="EXP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC59711" prefix="IC">
<gates>
<gate name="G$1" symbol="TLC59711"/>
<gate name="G$2" symbol="THERMAL_PAD"/>
</gates>
<devices>
<device name="" package="HTSSOP20DAP">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IREF" pad="1"/>
<connect gate="G$1" pin="OUTB0" pad="5"/>
<connect gate="G$1" pin="OUTB1" pad="8"/>
<connect gate="G$1" pin="OUTB2" pad="15"/>
<connect gate="G$1" pin="OUTB3" pad="18"/>
<connect gate="G$1" pin="OUTG0" pad="4"/>
<connect gate="G$1" pin="OUTG1" pad="7"/>
<connect gate="G$1" pin="OUTG2" pad="14"/>
<connect gate="G$1" pin="OUTG3" pad="17"/>
<connect gate="G$1" pin="OUTR0" pad="3"/>
<connect gate="G$1" pin="OUTR1" pad="6"/>
<connect gate="G$1" pin="OUTR2" pad="13"/>
<connect gate="G$1" pin="OUTR3" pad="16"/>
<connect gate="G$1" pin="SCKI" pad="10"/>
<connect gate="G$1" pin="SCKO" pad="11"/>
<connect gate="G$1" pin="SDTI" pad="9"/>
<connect gate="G$1" pin="SDTO" pad="12"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VREG" pad="20"/>
<connect gate="G$2" pin="PAD" pad="EXP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="40FPC">
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AHC1G125" prefix="IC">
<gates>
<gate name="G$1" symbol="74AHC1G125"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1SS309" prefix="D">
<gates>
<gate name="G$1" symbol="1SS309"/>
</gates>
<devices>
<device name="" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA_U.FL" prefix="X" uservalue="yes">
<description>&lt;p&gt;U.FL Antenna Connector&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="U.FL"/>
</gates>
<devices>
<device name="" package="U.FL">
<connects>
<connect gate="G$1" pin="GND@0" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="SIGNAL" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMACONNECTOR" prefix="X" uservalue="yes">
<description>&lt;b&gt;SMA Connector&lt;/b&gt;
&lt;p&gt;90° DIP SMA Connector, 50 Ohm (4UConnector: 07259)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMACONNECTOR"/>
</gates>
<devices>
<device name="" package="SMA90_DIP">
<connects>
<connect gate="G$1" pin="ANT" pad="ANTENNA"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_EDGE" package="SMA_EDGELAUNCH">
<connects>
<connect gate="G$1" pin="ANT" pad="P"/>
<connect gate="G$1" pin="GND1" pad="GND@4"/>
<connect gate="G$1" pin="GND2" pad="GND@3"/>
<connect gate="G$1" pin="GND3" pad="GND@2"/>
<connect gate="G$1" pin="GND4" pad="GND@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_EDGE_UFL" package="SMA_EDGELAUNCH_UFL">
<connects>
<connect gate="G$1" pin="ANT" pad="P"/>
<connect gate="G$1" pin="GND1" pad="GND@1"/>
<connect gate="G$1" pin="GND2" pad="GND@2"/>
<connect gate="G$1" pin="GND3" pad="GND@3"/>
<connect gate="G$1" pin="GND4" pad="GND@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_2.8IN_240X320_50PIN">
<gates>
<gate name="G$1" symbol="TFT_2.83IN_240X320_50PIN"/>
</gates>
<devices>
<device name="" package="TFT_2.83IN_240X320_50PIN">
<connects>
<connect gate="G$1" pin="#CS" pad="38"/>
<connect gate="G$1" pin="#RD" pad="35"/>
<connect gate="G$1" pin="#WR" pad="36"/>
<connect gate="G$1" pin="DB0" pad="32"/>
<connect gate="G$1" pin="DB1" pad="31"/>
<connect gate="G$1" pin="DB10" pad="22"/>
<connect gate="G$1" pin="DB11" pad="21"/>
<connect gate="G$1" pin="DB12" pad="20"/>
<connect gate="G$1" pin="DB13" pad="19"/>
<connect gate="G$1" pin="DB14" pad="18"/>
<connect gate="G$1" pin="DB15" pad="17"/>
<connect gate="G$1" pin="DB16" pad="16"/>
<connect gate="G$1" pin="DB17" pad="15"/>
<connect gate="G$1" pin="DB2" pad="30"/>
<connect gate="G$1" pin="DB3" pad="29"/>
<connect gate="G$1" pin="DB4" pad="28"/>
<connect gate="G$1" pin="DB5" pad="27"/>
<connect gate="G$1" pin="DB6" pad="26"/>
<connect gate="G$1" pin="DB7" pad="25"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="23"/>
<connect gate="G$1" pin="DE" pad="14"/>
<connect gate="G$1" pin="DOTCLK" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="43"/>
<connect gate="G$1" pin="GND@2" pad="48"/>
<connect gate="G$1" pin="GND@3" pad="49"/>
<connect gate="G$1" pin="GND@4" pad="50"/>
<connect gate="G$1" pin="HSYNC" pad="12"/>
<connect gate="G$1" pin="IM0" pad="6"/>
<connect gate="G$1" pin="IM1" pad="7"/>
<connect gate="G$1" pin="IM2" pad="8"/>
<connect gate="G$1" pin="IM3" pad="9"/>
<connect gate="G$1" pin="IOVCC@1" pad="40"/>
<connect gate="G$1" pin="IOVCC@2" pad="41"/>
<connect gate="G$1" pin="LEDA@1" pad="2"/>
<connect gate="G$1" pin="LEDA@2" pad="3"/>
<connect gate="G$1" pin="LEDA@3" pad="4"/>
<connect gate="G$1" pin="LEDA@4" pad="5"/>
<connect gate="G$1" pin="LEDK" pad="1"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="RS" pad="37"/>
<connect gate="G$1" pin="SDI" pad="34"/>
<connect gate="G$1" pin="SDO" pad="33"/>
<connect gate="G$1" pin="TE" pad="39"/>
<connect gate="G$1" pin="VCI" pad="42"/>
<connect gate="G$1" pin="VSYNC" pad="11"/>
<connect gate="G$1" pin="XL" pad="46"/>
<connect gate="G$1" pin="XR" pad="44"/>
<connect gate="G$1" pin="YD" pad="45"/>
<connect gate="G$1" pin="YU" pad="47"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD_CTP28" prefix="TFT" uservalue="yes">
<description>&lt;p&gt;2.83" 240x320 Pixel Capacitive Touch Display&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TFT_CTP28_240X320_50PIN"/>
</gates>
<devices>
<device name="_DATASHEET" package="TFT_CTP28">
<connects>
<connect gate="G$1" pin="/CS" pad="38"/>
<connect gate="G$1" pin="/RD" pad="35"/>
<connect gate="G$1" pin="/RESET" pad="10"/>
<connect gate="G$1" pin="/WR_RS" pad="36"/>
<connect gate="G$1" pin="DB0" pad="32"/>
<connect gate="G$1" pin="DB1" pad="31"/>
<connect gate="G$1" pin="DB10" pad="22"/>
<connect gate="G$1" pin="DB11" pad="21"/>
<connect gate="G$1" pin="DB12" pad="20"/>
<connect gate="G$1" pin="DB13" pad="19"/>
<connect gate="G$1" pin="DB14" pad="18"/>
<connect gate="G$1" pin="DB15" pad="17"/>
<connect gate="G$1" pin="DB16" pad="16"/>
<connect gate="G$1" pin="DB17" pad="15"/>
<connect gate="G$1" pin="DB2" pad="30"/>
<connect gate="G$1" pin="DB3" pad="29"/>
<connect gate="G$1" pin="DB4" pad="28"/>
<connect gate="G$1" pin="DB5" pad="27"/>
<connect gate="G$1" pin="DB6" pad="26"/>
<connect gate="G$1" pin="DB7" pad="25"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="23"/>
<connect gate="G$1" pin="DE" pad="14"/>
<connect gate="G$1" pin="DOTCLK" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="43"/>
<connect gate="G$1" pin="GND@2" pad="48"/>
<connect gate="G$1" pin="GND@3" pad="49"/>
<connect gate="G$1" pin="GND@4" pad="50"/>
<connect gate="G$1" pin="HSYNC" pad="12"/>
<connect gate="G$1" pin="IM0" pad="6"/>
<connect gate="G$1" pin="IM1" pad="7"/>
<connect gate="G$1" pin="IM2" pad="8"/>
<connect gate="G$1" pin="IM3" pad="9"/>
<connect gate="G$1" pin="IOVCC@1" pad="40"/>
<connect gate="G$1" pin="IOVCC@2" pad="41"/>
<connect gate="G$1" pin="LEDA@1" pad="2"/>
<connect gate="G$1" pin="LEDA@2" pad="3"/>
<connect gate="G$1" pin="LEDA@3" pad="4"/>
<connect gate="G$1" pin="LEDA@4" pad="5"/>
<connect gate="G$1" pin="LEDK" pad="1"/>
<connect gate="G$1" pin="RS_SCL" pad="37"/>
<connect gate="G$1" pin="SDI" pad="34"/>
<connect gate="G$1" pin="SDO" pad="33"/>
<connect gate="G$1" pin="TE" pad="39"/>
<connect gate="G$1" pin="TP_IRQ" pad="46"/>
<connect gate="G$1" pin="TP_RES" pad="47"/>
<connect gate="G$1" pin="TP_SCK" pad="44"/>
<connect gate="G$1" pin="TP_SDA" pad="45"/>
<connect gate="G$1" pin="VCI" pad="42"/>
<connect gate="G$1" pin="VSYNC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SAMPLE" package="TFT_2.83IN_240X320_50PIN">
<connects>
<connect gate="G$1" pin="/CS" pad="38"/>
<connect gate="G$1" pin="/RD" pad="35"/>
<connect gate="G$1" pin="/RESET" pad="10"/>
<connect gate="G$1" pin="/WR_RS" pad="36"/>
<connect gate="G$1" pin="DB0" pad="32"/>
<connect gate="G$1" pin="DB1" pad="31"/>
<connect gate="G$1" pin="DB10" pad="22"/>
<connect gate="G$1" pin="DB11" pad="21"/>
<connect gate="G$1" pin="DB12" pad="20"/>
<connect gate="G$1" pin="DB13" pad="19"/>
<connect gate="G$1" pin="DB14" pad="18"/>
<connect gate="G$1" pin="DB15" pad="17"/>
<connect gate="G$1" pin="DB16" pad="16"/>
<connect gate="G$1" pin="DB17" pad="15"/>
<connect gate="G$1" pin="DB2" pad="30"/>
<connect gate="G$1" pin="DB3" pad="29"/>
<connect gate="G$1" pin="DB4" pad="28"/>
<connect gate="G$1" pin="DB5" pad="27"/>
<connect gate="G$1" pin="DB6" pad="26"/>
<connect gate="G$1" pin="DB7" pad="25"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="23"/>
<connect gate="G$1" pin="DE" pad="14"/>
<connect gate="G$1" pin="DOTCLK" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="43"/>
<connect gate="G$1" pin="GND@2" pad="48"/>
<connect gate="G$1" pin="GND@3" pad="49"/>
<connect gate="G$1" pin="GND@4" pad="50"/>
<connect gate="G$1" pin="HSYNC" pad="12"/>
<connect gate="G$1" pin="IM0" pad="6"/>
<connect gate="G$1" pin="IM1" pad="7"/>
<connect gate="G$1" pin="IM2" pad="8"/>
<connect gate="G$1" pin="IM3" pad="9"/>
<connect gate="G$1" pin="IOVCC@1" pad="40"/>
<connect gate="G$1" pin="IOVCC@2" pad="41"/>
<connect gate="G$1" pin="LEDA@1" pad="2"/>
<connect gate="G$1" pin="LEDA@2" pad="3"/>
<connect gate="G$1" pin="LEDA@3" pad="4"/>
<connect gate="G$1" pin="LEDA@4" pad="5"/>
<connect gate="G$1" pin="LEDK" pad="1"/>
<connect gate="G$1" pin="RS_SCL" pad="37"/>
<connect gate="G$1" pin="SDI" pad="34"/>
<connect gate="G$1" pin="SDO" pad="33"/>
<connect gate="G$1" pin="TE" pad="39"/>
<connect gate="G$1" pin="TP_IRQ" pad="46"/>
<connect gate="G$1" pin="TP_RES" pad="47"/>
<connect gate="G$1" pin="TP_SCK" pad="44"/>
<connect gate="G$1" pin="TP_SDA" pad="45"/>
<connect gate="G$1" pin="VCI" pad="42"/>
<connect gate="G$1" pin="VSYNC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PRO_TRINKET">
<gates>
<gate name="G$1" symbol="PROTRINKET"/>
</gates>
<devices>
<device name="" package="PROTRINKET">
<connects>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="D10" pad="10"/>
<connect gate="G$1" pin="D11" pad="11"/>
<connect gate="G$1" pin="D12" pad="12"/>
<connect gate="G$1" pin="D13" pad="13"/>
<connect gate="G$1" pin="D3" pad="3"/>
<connect gate="G$1" pin="D4" pad="4"/>
<connect gate="G$1" pin="D5" pad="5"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="USB" pad="USB"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP-12" prefix="X" uservalue="yes">
<gates>
<gate name="G$1" symbol="ESP8266-12"/>
</gates>
<devices>
<device name="" package="ESP-12">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="CH_PD" pad="3"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GPIO0" pad="12"/>
<connect gate="G$1" pin="GPIO12" pad="6"/>
<connect gate="G$1" pin="GPIO13" pad="7"/>
<connect gate="G$1" pin="GPIO14" pad="5"/>
<connect gate="G$1" pin="GPIO15" pad="10"/>
<connect gate="G$1" pin="GPIO16" pad="4"/>
<connect gate="G$1" pin="GPIO2" pad="11"/>
<connect gate="G$1" pin="GPIO4" pad="14"/>
<connect gate="G$1" pin="GPIO5" pad="13"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="RXD" pad="15"/>
<connect gate="G$1" pin="TXD" pad="16"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_SIM800L" prefix="U" uservalue="yes">
<description>&lt;p&gt;SIM800K Quad-Band GSM/GPRS Module&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;850/900/1800/1900 MHz&lt;/li&gt;
&lt;li&gt;Bluetooth EDR (3.0)&lt;/li&gt;
&lt;li&gt;FM Band: 76-109MHz (50kHz steps)&lt;/li&gt;
&lt;li&gt;-40 - 85°C&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SIM800L"/>
</gates>
<devices>
<device name="" package="SIM800L">
<connects>
<connect gate="G$1" pin="ADC" pad="50"/>
<connect gate="G$1" pin="ANT" pad="40"/>
<connect gate="G$1" pin="BPI_BUS1" pad="5"/>
<connect gate="G$1" pin="COL0" pad="20"/>
<connect gate="G$1" pin="COL1" pad="25"/>
<connect gate="G$1" pin="COL2" pad="22"/>
<connect gate="G$1" pin="COL3" pad="21"/>
<connect gate="G$1" pin="COL4" pad="24"/>
<connect gate="G$1" pin="FM_ANT_N" pad="57"/>
<connect gate="G$1" pin="FM_ANT_P" pad="17"/>
<connect gate="G$1" pin="GND" pad="2 6 8 35 37 38 39 41 43 44 45 58 67 71 72 73 76 77 78 79 80 81 82 83 84 85 86 87 88"/>
<connect gate="G$1" pin="GPIO1" pad="3"/>
<connect gate="G$1" pin="GPIO2" pad="27"/>
<connect gate="G$1" pin="GPIO3" pad="28"/>
<connect gate="G$1" pin="ISINK0" pad="47"/>
<connect gate="G$1" pin="ISINK1" pad="46"/>
<connect gate="G$1" pin="MIC1N" pad="12"/>
<connect gate="G$1" pin="MIC1P" pad="52"/>
<connect gate="G$1" pin="MIC2N" pad="10"/>
<connect gate="G$1" pin="MIC2P" pad="9"/>
<connect gate="G$1" pin="NC" pad="36"/>
<connect gate="G$1" pin="NETLIGHT" pad="64"/>
<connect gate="G$1" pin="PCMCLK" pad="29"/>
<connect gate="G$1" pin="PCMIN" pad="66"/>
<connect gate="G$1" pin="PCMOUT" pad="30"/>
<connect gate="G$1" pin="PCMSYNC" pad="65"/>
<connect gate="G$1" pin="PWM" pad="26"/>
<connect gate="G$1" pin="PWRKEY" pad="48"/>
<connect gate="G$1" pin="RESET" pad="49"/>
<connect gate="G$1" pin="ROW0" pad="62"/>
<connect gate="G$1" pin="ROW1" pad="60"/>
<connect gate="G$1" pin="ROW2" pad="61"/>
<connect gate="G$1" pin="ROW3" pad="23"/>
<connect gate="G$1" pin="ROW4" pad="63"/>
<connect gate="G$1" pin="SCL" pad="74"/>
<connect gate="G$1" pin="SDA" pad="75"/>
<connect gate="G$1" pin="SIMPRE" pad="54"/>
<connect gate="G$1" pin="SIM_CLK" pad="55"/>
<connect gate="G$1" pin="SIM_DATA" pad="14"/>
<connect gate="G$1" pin="SIM_RST" pad="15"/>
<connect gate="G$1" pin="SPK1N" pad="13"/>
<connect gate="G$1" pin="SPK1P" pad="53"/>
<connect gate="G$1" pin="SPK2N" pad="11"/>
<connect gate="G$1" pin="SPK2P/8Ω" pad="51"/>
<connect gate="G$1" pin="STATUS" pad="4"/>
<connect gate="G$1" pin="UART_CTS" pad="34"/>
<connect gate="G$1" pin="UART_DCD" pad="70"/>
<connect gate="G$1" pin="UART_DTR" pad="69"/>
<connect gate="G$1" pin="UART_RI" pad="68"/>
<connect gate="G$1" pin="UART_RTS" pad="33"/>
<connect gate="G$1" pin="UART_RXD" pad="31"/>
<connect gate="G$1" pin="UART_TXD" pad="32"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="59"/>
<connect gate="G$1" pin="VBAT" pad="1 42"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VEXT" pad="18"/>
<connect gate="G$1" pin="VRTC" pad="56"/>
<connect gate="G$1" pin="VSIM" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM_SIM808_LITERAL" prefix="U" uservalue="yes">
<description>&lt;p&gt;SIM808 GSM Module&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SIM808_LITERAL"/>
</gates>
<devices>
<device name="" package="SIM900_SMT">
<connects>
<connect gate="G$1" pin="1PPS" pad="P$37"/>
<connect gate="G$1" pin="ADC1" pad="P$23"/>
<connect gate="G$1" pin="ADC2" pad="P$24"/>
<connect gate="G$1" pin="ANT_BT" pad="P$53"/>
<connect gate="G$1" pin="COL0" pad="P$62"/>
<connect gate="G$1" pin="COL1" pad="P$61"/>
<connect gate="G$1" pin="COL2" pad="P$60"/>
<connect gate="G$1" pin="COL3" pad="P$59"/>
<connect gate="G$1" pin="CTS" pad="P$12"/>
<connect gate="G$1" pin="DCD" pad="P$11"/>
<connect gate="G$1" pin="DTR" pad="P$9"/>
<connect gate="G$1" pin="GND@1" pad="P$1"/>
<connect gate="G$1" pin="GND@10" pad="P$52"/>
<connect gate="G$1" pin="GND@11" pad="P$54"/>
<connect gate="G$1" pin="GND@12" pad="P$64"/>
<connect gate="G$1" pin="GND@13" pad="P$65"/>
<connect gate="G$1" pin="GND@14" pad="P$67"/>
<connect gate="G$1" pin="GND@15" pad="P$68"/>
<connect gate="G$1" pin="GND@2" pad="P$2"/>
<connect gate="G$1" pin="GND@3" pad="P$3"/>
<connect gate="G$1" pin="GND@4" pad="P$18"/>
<connect gate="G$1" pin="GND@5" pad="P$28"/>
<connect gate="G$1" pin="GND@6" pad="P$34"/>
<connect gate="G$1" pin="GND@7" pad="P$36"/>
<connect gate="G$1" pin="GND@8" pad="P$40"/>
<connect gate="G$1" pin="GND@9" pad="P$51"/>
<connect gate="G$1" pin="GPIO5" pad="P$43"/>
<connect gate="G$1" pin="GPIO6" pad="P$44"/>
<connect gate="G$1" pin="GPS_RF_IN" pad="P$35"/>
<connect gate="G$1" pin="GSM_RF_IN" pad="P$66"/>
<connect gate="G$1" pin="MIC1N" pad="P$20"/>
<connect gate="G$1" pin="MIC1P" pad="P$19"/>
<connect gate="G$1" pin="NETLIGHT" pad="P$50"/>
<connect gate="G$1" pin="PCM_CLK" pad="P$46"/>
<connect gate="G$1" pin="PCM_IN" pad="P$47"/>
<connect gate="G$1" pin="PCM_OUT" pad="P$48"/>
<connect gate="G$1" pin="PCM_SYNC" pad="P$45"/>
<connect gate="G$1" pin="PWM1" pad="P$42"/>
<connect gate="G$1" pin="PWM2" pad="P$41"/>
<connect gate="G$1" pin="PWRKEY" pad="P$8"/>
<connect gate="G$1" pin="RESET" pad="P$16"/>
<connect gate="G$1" pin="RF_SYNC" pad="P$63"/>
<connect gate="G$1" pin="RI" pad="P$10"/>
<connect gate="G$1" pin="ROW0" pad="P$58"/>
<connect gate="G$1" pin="ROW1" pad="P$57"/>
<connect gate="G$1" pin="ROW2" pad="P$56"/>
<connect gate="G$1" pin="ROW3" pad="P$55"/>
<connect gate="G$1" pin="RTS" pad="P$13"/>
<connect gate="G$1" pin="RXD" pad="P$15"/>
<connect gate="G$1" pin="SCL" pad="P$39"/>
<connect gate="G$1" pin="SDA" pad="P$38"/>
<connect gate="G$1" pin="SIM_CLK" pad="P$31"/>
<connect gate="G$1" pin="SIM_DATA" pad="P$30"/>
<connect gate="G$1" pin="SIM_PRE" pad="P$33"/>
<connect gate="G$1" pin="SIM_RST" pad="P$32"/>
<connect gate="G$1" pin="SIM_VDD" pad="P$29"/>
<connect gate="G$1" pin="SPK1N" pad="P$22"/>
<connect gate="G$1" pin="SPK1P" pad="P$21"/>
<connect gate="G$1" pin="STATUS" pad="P$49"/>
<connect gate="G$1" pin="TXD" pad="P$14"/>
<connect gate="G$1" pin="USB_DM" pad="P$27"/>
<connect gate="G$1" pin="USB_DP" pad="P$26"/>
<connect gate="G$1" pin="VBAT@1" pad="P$4"/>
<connect gate="G$1" pin="VBAT@2" pad="P$5"/>
<connect gate="G$1" pin="VBAT@3" pad="P$6"/>
<connect gate="G$1" pin="VBUS" pad="P$25"/>
<connect gate="G$1" pin="VDD_EXT(2.8VOUT)" pad="P$7"/>
<connect gate="G$1" pin="VRTC" pad="P$17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_PUSHBUTTON" prefix="SW" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Buttons&lt;/b&gt;&lt;/p&gt;
&lt;b&gt;SOFTTOUCHSMD_SJ&lt;/b&gt; - Soft touch temporary push button (Super Junk Akihabara)
&lt;p&gt;Compatible with SKPMANE010 [Mouser: 688-SKPMAN]&lt;/p&gt;
&lt;p&gt;C&amp;K_KSS = Digikey: KSS221GLFS&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PUSHBUTTON"/>
</gates>
<devices>
<device name="SOFTTOUCHSMD_SJ" package="PUSHBUTTON_SMD_SJ">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EVQ-PE" package="TACT_PANA-EVQ">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C&amp;K_KSS" package="BTN_CK_KSS">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FEATHERWING" prefix="MS">
<gates>
<gate name="G$1" symbol="MICROSHIELD"/>
</gates>
<devices>
<device name="" package="FEATHERWING">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="3V" pad="2"/>
<connect gate="G$1" pin="AREF" pad="3"/>
<connect gate="G$1" pin="EN" pad="27"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GPIO10" pad="22"/>
<connect gate="G$1" pin="GPIO11" pad="23"/>
<connect gate="G$1" pin="GPIO12" pad="24"/>
<connect gate="G$1" pin="GPIO13" pad="25"/>
<connect gate="G$1" pin="GPIO5" pad="19"/>
<connect gate="G$1" pin="GPIO6" pad="20"/>
<connect gate="G$1" pin="GPIO9" pad="21"/>
<connect gate="G$1" pin="GPIOA0" pad="5"/>
<connect gate="G$1" pin="GPIOA1" pad="6"/>
<connect gate="G$1" pin="GPIOA2" pad="7"/>
<connect gate="G$1" pin="GPIOA3" pad="8"/>
<connect gate="G$1" pin="GPIOA4" pad="9"/>
<connect gate="G$1" pin="GPIOA5" pad="10"/>
<connect gate="G$1" pin="GPIOMISO" pad="13"/>
<connect gate="G$1" pin="GPIOMOSI" pad="12"/>
<connect gate="G$1" pin="GPIORX" pad="14"/>
<connect gate="G$1" pin="GPIOSCK" pad="11"/>
<connect gate="G$1" pin="GPIOSCL" pad="18"/>
<connect gate="G$1" pin="GPIOSDA" pad="17"/>
<connect gate="G$1" pin="GPIOTX" pad="15"/>
<connect gate="G$1" pin="NC" pad="16"/>
<connect gate="G$1" pin="USB" pad="26"/>
<connect gate="G$1" pin="VBAT" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NODIM" package="FEATHERWING_DIM">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="3V" pad="2"/>
<connect gate="G$1" pin="AREF" pad="3"/>
<connect gate="G$1" pin="EN" pad="27"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GPIO10" pad="22"/>
<connect gate="G$1" pin="GPIO11" pad="23"/>
<connect gate="G$1" pin="GPIO12" pad="24"/>
<connect gate="G$1" pin="GPIO13" pad="25"/>
<connect gate="G$1" pin="GPIO5" pad="19"/>
<connect gate="G$1" pin="GPIO6" pad="20"/>
<connect gate="G$1" pin="GPIO9" pad="21"/>
<connect gate="G$1" pin="GPIOA0" pad="5"/>
<connect gate="G$1" pin="GPIOA1" pad="6"/>
<connect gate="G$1" pin="GPIOA2" pad="7"/>
<connect gate="G$1" pin="GPIOA3" pad="8"/>
<connect gate="G$1" pin="GPIOA4" pad="9"/>
<connect gate="G$1" pin="GPIOA5" pad="10"/>
<connect gate="G$1" pin="GPIOMISO" pad="13"/>
<connect gate="G$1" pin="GPIOMOSI" pad="12"/>
<connect gate="G$1" pin="GPIORX" pad="14"/>
<connect gate="G$1" pin="GPIOSCK" pad="11"/>
<connect gate="G$1" pin="GPIOSCL" pad="18"/>
<connect gate="G$1" pin="GPIOSDA" pad="17"/>
<connect gate="G$1" pin="GPIOTX" pad="15"/>
<connect gate="G$1" pin="NC" pad="16"/>
<connect gate="G$1" pin="USB" pad="26"/>
<connect gate="G$1" pin="VBAT" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2812B" prefix="LED">
<gates>
<gate name="G$1" symbol="WS2812BLED"/>
</gates>
<devices>
<device name="5050" package="WS2812B">
<connects>
<connect gate="G$1" pin="DI" pad="4-DIN"/>
<connect gate="G$1" pin="DO" pad="2-DOUT"/>
<connect gate="G$1" pin="GND" pad="3-GND"/>
<connect gate="G$1" pin="VDD" pad="1-VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_5050N" package="WS2812B-NARROW">
<connects>
<connect gate="G$1" pin="DI" pad="4-DIN"/>
<connect gate="G$1" pin="DO" pad="2-DOUT"/>
<connect gate="G$1" pin="GND" pad="3-GND"/>
<connect gate="G$1" pin="VDD" pad="1-VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3535" package="LED3535">
<connects>
<connect gate="G$1" pin="DI" pad="1"/>
<connect gate="G$1" pin="DO" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_OUTLINE" prefix="ARD">
<description>Board Outlines for Arduino variants.</description>
<gates>
<gate name="G$1" symbol="OUTLINE"/>
</gates>
<devices>
<device name="-DUE" package="ARDUINO_DUE_OUTLINE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-X">
<description>Extended Body Arduino</description>
<gates>
<gate name="G$1" symbol="ARDUINO"/>
<gate name="G$2" symbol="ARDUINO-X"/>
</gates>
<devices>
<device name="" package="ARDUINO_DUE_SHIELD">
<connects>
<connect gate="G$1" pin="/RESET" pad="RESET"/>
<connect gate="G$1" pin="3V" pad="3V3"/>
<connect gate="G$1" pin="5V" pad="5V0"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="0"/>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D10" pad="10"/>
<connect gate="G$1" pin="D11" pad="11"/>
<connect gate="G$1" pin="D12" pad="12"/>
<connect gate="G$1" pin="D13" pad="13"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="3"/>
<connect gate="G$1" pin="D4" pad="4"/>
<connect gate="G$1" pin="D5" pad="5"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D7" pad="7"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND_1"/>
<connect gate="G$1" pin="GND2" pad="GND_2"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$2" pin="+5V" pad="5V0_1"/>
<connect gate="G$2" pin="+5V0" pad="5V0_2"/>
<connect gate="G$2" pin="22" pad="22"/>
<connect gate="G$2" pin="23" pad="23"/>
<connect gate="G$2" pin="24" pad="24"/>
<connect gate="G$2" pin="25" pad="25"/>
<connect gate="G$2" pin="26" pad="26"/>
<connect gate="G$2" pin="27" pad="27"/>
<connect gate="G$2" pin="28" pad="28"/>
<connect gate="G$2" pin="29" pad="29"/>
<connect gate="G$2" pin="30" pad="30"/>
<connect gate="G$2" pin="31" pad="31"/>
<connect gate="G$2" pin="32" pad="32"/>
<connect gate="G$2" pin="33" pad="33"/>
<connect gate="G$2" pin="34" pad="34"/>
<connect gate="G$2" pin="35" pad="35"/>
<connect gate="G$2" pin="36" pad="36"/>
<connect gate="G$2" pin="37" pad="37"/>
<connect gate="G$2" pin="38" pad="38"/>
<connect gate="G$2" pin="39" pad="39"/>
<connect gate="G$2" pin="40" pad="40"/>
<connect gate="G$2" pin="41" pad="41"/>
<connect gate="G$2" pin="42" pad="42"/>
<connect gate="G$2" pin="43" pad="43"/>
<connect gate="G$2" pin="44" pad="44"/>
<connect gate="G$2" pin="45" pad="45"/>
<connect gate="G$2" pin="46" pad="46"/>
<connect gate="G$2" pin="47" pad="47"/>
<connect gate="G$2" pin="48" pad="48"/>
<connect gate="G$2" pin="49" pad="49"/>
<connect gate="G$2" pin="50" pad="50"/>
<connect gate="G$2" pin="51" pad="51"/>
<connect gate="G$2" pin="52" pad="52"/>
<connect gate="G$2" pin="53" pad="53"/>
<connect gate="G$2" pin="A10" pad="A10"/>
<connect gate="G$2" pin="A11" pad="A11"/>
<connect gate="G$2" pin="A6" pad="A6"/>
<connect gate="G$2" pin="A7" pad="A7"/>
<connect gate="G$2" pin="A8" pad="A8"/>
<connect gate="G$2" pin="A9" pad="A9"/>
<connect gate="G$2" pin="CANRX" pad="CANRX"/>
<connect gate="G$2" pin="CANTX" pad="CANTX"/>
<connect gate="G$2" pin="DAC0" pad="DAC0"/>
<connect gate="G$2" pin="DAC1" pad="DAC1"/>
<connect gate="G$2" pin="GND" pad="GND_3"/>
<connect gate="G$2" pin="GND1" pad="GND_4"/>
<connect gate="G$2" pin="RX119" pad="19"/>
<connect gate="G$2" pin="RX217" pad="17"/>
<connect gate="G$2" pin="RX315" pad="15"/>
<connect gate="G$2" pin="SCL21" pad="21"/>
<connect gate="G$2" pin="SDA20" pad="20"/>
<connect gate="G$2" pin="TX118" pad="18"/>
<connect gate="G$2" pin="TX216" pad="16"/>
<connect gate="G$2" pin="TX314" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
