<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="ARDUINO_DUE_ALL">
</package>
<package name="ARDUINO_DUE_SHIELD">
</package>
</packages>
<symbols>
<symbol name="ARDUINO_DUE_ALL">
<pin name="NC" direction="nc"/>
<pin name="IOREF"/>
<pin name="RESET"/>
<pin name="3V3"/>
<pin name="5V"/>
<pin name="GND"/>
<pin name="GND@1"/>
<pin name="AN0"/>
<pin name="AN1"/>
<pin name="AN2"/>
<pin name="AN3"/>
<pin name="AN4"/>
<pin name="AN5"/>
<pin name="AN6"/>
<pin name="AN7"/>
<pin name="AN8"/>
<pin name="AN9"/>
<pin name="AN10"/>
<pin name="AN11"/>
<pin name="DAC0"/>
<pin name="DAC1"/>
<pin name="CANRX"/>
<pin name="CANTX"/>
<pin name="GND@2"/>
<pin name="52"/>
<pin name="50"/>
<pin name="48"/>
<pin name="46"/>
<pin name="44"/>
<pin name="42"/>
<pin name="40"/>
<pin name="38"/>
<pin name="36"/>
<pin name="34"/>
<pin name="32"/>
<pin name="30"/>
<pin name="28"/>
<pin name="26"/>
<pin name="24"/>
<pin name="22"/>
<pin name="5V@1"/>
<pin name="GND@3"/>
<pin name="53"/>
<pin name="51"/>
<pin name="49"/>
<pin name="47"/>
<pin name="45"/>
<pin name="43"/>
<pin name="41"/>
<pin name="39"/>
<pin name="37"/>
<pin name="35"/>
<pin name="33"/>
<pin name="31"/>
<pin name="29"/>
<pin name="27"/>
<pin name="25"/>
<pin name="23"/>
<pin name="5V@2"/>
<pin name="SCL_21"/>
<pin name="SDA_20"/>
<pin name="RX1_19"/>
<pin name="TX1_18"/>
<pin name="RX2_17"/>
<pin name="TX2_16"/>
<pin name="RX3_15"/>
<pin name="TX3_14"/>
<pin name="RX0&lt;0"/>
<pin name="TX0&gt;1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="GND@4"/>
<pin name="AREF"/>
<pin name="SDA1"/>
<pin name="SCL1"/>
<pin name="MASTER_R_JTAG"/>
<pin name="JTAG_TMS"/>
<pin name="JTAG_TCK"/>
<pin name="GND@7"/>
<pin name="GND_ICSP1"/>
<pin name="RESET2"/>
<pin name="MOSI2"/>
<pin name="SCK2"/>
<pin name="5V_ICSP1"/>
<pin name="MISO2"/>
<pin name="3V3_JTAG"/>
<pin name="JTAG_TMS_2"/>
<pin name="GND@8"/>
<pin name="JTAG_TCK_2"/>
<pin name="GND@9"/>
<pin name="JTAG_TDO"/>
<pin name="NC@5"/>
<pin name="JTAG_TDI"/>
<pin name="GND@10"/>
<pin name="JTAG_RESET"/>
<pin name="VIN"/>
<pin name="MISO"/>
<pin name="5V_SPI"/>
<pin name="SPCK"/>
<pin name="MOSI"/>
<pin name="MASTER_R_SPI"/>
<pin name="GND@5"/>
</symbol>
<symbol name="ARDUINO_DUE_SHIELD">
<pin name="NC" direction="nc"/>
<pin name="IOREF"/>
<pin name="RESET"/>
<pin name="3V3"/>
<pin name="5V"/>
<pin name="GND"/>
<pin name="GND@1"/>
<pin name="AN0"/>
<pin name="AN1"/>
<pin name="AN2"/>
<pin name="AN3"/>
<pin name="AN4"/>
<pin name="AN5"/>
<pin name="AN6"/>
<pin name="AN7"/>
<pin name="AN8"/>
<pin name="AN9"/>
<pin name="AN10"/>
<pin name="AN11"/>
<pin name="DAC0"/>
<pin name="DAC1"/>
<pin name="CANRX"/>
<pin name="CANTX"/>
<pin name="GND@2"/>
<pin name="52"/>
<pin name="50"/>
<pin name="48"/>
<pin name="46"/>
<pin name="44"/>
<pin name="42"/>
<pin name="40"/>
<pin name="38"/>
<pin name="36"/>
<pin name="34"/>
<pin name="32"/>
<pin name="30"/>
<pin name="28"/>
<pin name="26"/>
<pin name="24"/>
<pin name="22"/>
<pin name="5V@1"/>
<pin name="GND@3"/>
<pin name="53"/>
<pin name="51"/>
<pin name="49"/>
<pin name="47"/>
<pin name="45"/>
<pin name="43"/>
<pin name="41"/>
<pin name="39"/>
<pin name="37"/>
<pin name="35"/>
<pin name="33"/>
<pin name="31"/>
<pin name="29"/>
<pin name="27"/>
<pin name="25"/>
<pin name="23"/>
<pin name="5V@2"/>
<pin name="SCL_21"/>
<pin name="SDA_20"/>
<pin name="RX1_19"/>
<pin name="TX1_18"/>
<pin name="RX2_17"/>
<pin name="TX2_16"/>
<pin name="RX3_15"/>
<pin name="TX3_14"/>
<pin name="RX0&lt;0"/>
<pin name="TX0&gt;1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="GND@4"/>
<pin name="AREF"/>
<pin name="SDA1"/>
<pin name="SCL1"/>
<pin name="VIN"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO_DUE_ALL" prefix="ARDUINO_DUE" uservalue="yes">
<gates>
<gate name="G$1" symbol="ARDUINO_DUE_ALL"/>
</gates>
<devices>
<device name="" package="ARDUINO_DUE_ALL">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="3V3_JTAG" pad="3V3_JTAG"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V" pad="5V0"/>
<connect gate="G$1" pin="5V@1" pad="5V0_1"/>
<connect gate="G$1" pin="5V@2" pad="5V0_2"/>
<connect gate="G$1" pin="5V_ICSP1" pad="5V_ICSP1"/>
<connect gate="G$1" pin="5V_SPI" pad="5V_2"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="AN0" pad="A0"/>
<connect gate="G$1" pin="AN1" pad="A1"/>
<connect gate="G$1" pin="AN10" pad="A10"/>
<connect gate="G$1" pin="AN11" pad="A11"/>
<connect gate="G$1" pin="AN2" pad="A2"/>
<connect gate="G$1" pin="AN3" pad="A3"/>
<connect gate="G$1" pin="AN4" pad="A4"/>
<connect gate="G$1" pin="AN5" pad="A5"/>
<connect gate="G$1" pin="AN6" pad="A6"/>
<connect gate="G$1" pin="AN7" pad="A7"/>
<connect gate="G$1" pin="AN8" pad="A8"/>
<connect gate="G$1" pin="AN9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="CANRX" pad="CANRX"/>
<connect gate="G$1" pin="CANTX" pad="CANTX"/>
<connect gate="G$1" pin="DAC0" pad="DAC0"/>
<connect gate="G$1" pin="DAC1" pad="DAC1"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND_1"/>
<connect gate="G$1" pin="GND@10" pad="GND_10"/>
<connect gate="G$1" pin="GND@2" pad="GND_2"/>
<connect gate="G$1" pin="GND@3" pad="GND_3"/>
<connect gate="G$1" pin="GND@4" pad="GND_4"/>
<connect gate="G$1" pin="GND@5" pad="GND_5"/>
<connect gate="G$1" pin="GND@7" pad="GND_7"/>
<connect gate="G$1" pin="GND@8" pad="GND_8"/>
<connect gate="G$1" pin="GND@9" pad="GND_9"/>
<connect gate="G$1" pin="GND_ICSP1" pad="GND_ICSP1"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="JTAG_RESET" pad="JTAG_RESET"/>
<connect gate="G$1" pin="JTAG_TCK" pad="JTAG_TCK"/>
<connect gate="G$1" pin="JTAG_TCK_2" pad="JTAG_TCK_2"/>
<connect gate="G$1" pin="JTAG_TDI" pad="JTAG_TDI"/>
<connect gate="G$1" pin="JTAG_TDO" pad="JTAG_TDO"/>
<connect gate="G$1" pin="JTAG_TMS" pad="JTAG_TMS"/>
<connect gate="G$1" pin="JTAG_TMS_2" pad="JTAG_TMS_2"/>
<connect gate="G$1" pin="MASTER_R_JTAG" pad="MASTER_RESET_JTAG"/>
<connect gate="G$1" pin="MASTER_R_SPI" pad="MASTER_RESET_SPI"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MISO2" pad="MISO2"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="MOSI2" pad="MOSI2"/>
<connect gate="G$1" pin="NC" pad="NC_2"/>
<connect gate="G$1" pin="NC@5" pad="NC_5"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RX0&lt;0" pad="0"/>
<connect gate="G$1" pin="RX1_19" pad="19"/>
<connect gate="G$1" pin="RX2_17" pad="17"/>
<connect gate="G$1" pin="RX3_15" pad="15"/>
<connect gate="G$1" pin="SCK2" pad="SCK2"/>
<connect gate="G$1" pin="SCL1" pad="SCL1"/>
<connect gate="G$1" pin="SCL_21" pad="21"/>
<connect gate="G$1" pin="SDA1" pad="SDA1"/>
<connect gate="G$1" pin="SDA_20" pad="20"/>
<connect gate="G$1" pin="SPCK" pad="SPCK"/>
<connect gate="G$1" pin="TX0&gt;1" pad="1"/>
<connect gate="G$1" pin="TX1_18" pad="18"/>
<connect gate="G$1" pin="TX2_16" pad="16"/>
<connect gate="G$1" pin="TX3_14" pad="14"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_DUE_SHIELD" prefix="ARD">
<description>Shield suitable for Arduino Due</description>
<gates>
<gate name="G$1" symbol="ARDUINO_DUE_SHIELD"/>
</gates>
<devices>
<device name="" package="ARDUINO_DUE_SHIELD">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="5V" pad="5V0"/>
<connect gate="G$1" pin="5V@1" pad="5V0_1"/>
<connect gate="G$1" pin="5V@2" pad="5V0_2"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="AN0" pad="A0"/>
<connect gate="G$1" pin="AN1" pad="A1"/>
<connect gate="G$1" pin="AN10" pad="A10"/>
<connect gate="G$1" pin="AN11" pad="A11"/>
<connect gate="G$1" pin="AN2" pad="A2"/>
<connect gate="G$1" pin="AN3" pad="A3"/>
<connect gate="G$1" pin="AN4" pad="A4"/>
<connect gate="G$1" pin="AN5" pad="A5"/>
<connect gate="G$1" pin="AN6" pad="A6"/>
<connect gate="G$1" pin="AN7" pad="A7"/>
<connect gate="G$1" pin="AN8" pad="A8"/>
<connect gate="G$1" pin="AN9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="CANRX" pad="CANRX"/>
<connect gate="G$1" pin="CANTX" pad="CANTX"/>
<connect gate="G$1" pin="DAC0" pad="DAC0"/>
<connect gate="G$1" pin="DAC1" pad="DAC1"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="GND_1"/>
<connect gate="G$1" pin="GND@2" pad="GND_2"/>
<connect gate="G$1" pin="GND@3" pad="GND_3"/>
<connect gate="G$1" pin="GND@4" pad="GND_4"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="NC" pad="NC_2"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="RX0&lt;0" pad="0"/>
<connect gate="G$1" pin="RX1_19" pad="19"/>
<connect gate="G$1" pin="RX2_17" pad="17"/>
<connect gate="G$1" pin="RX3_15" pad="15"/>
<connect gate="G$1" pin="SCL1" pad="SCL1"/>
<connect gate="G$1" pin="SCL_21" pad="21"/>
<connect gate="G$1" pin="SDA1" pad="SDA1"/>
<connect gate="G$1" pin="SDA_20" pad="20"/>
<connect gate="G$1" pin="TX0&gt;1" pad="1"/>
<connect gate="G$1" pin="TX1_18" pad="18"/>
<connect gate="G$1" pin="TX2_16" pad="16"/>
<connect gate="G$1" pin="TX3_14" pad="14"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
