<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>DEC Flip-Chips
&lt;BR&gt;Vincent R. Slyngstad
&lt;BR&gt;vrs@msn.com</description>
<packages>
<package name="H807">
<description>One-wide female edge connector</description>
</package>
<package name="H807-2">
<description>Two-wide Female Edge Connector</description>
</package>
<package name="EMPTY">
<description>Empty package</description>
</package>
<package name="CBLOCK">
<description>Connector block outline with mounting holes.</description>
</package>
<package name="H807S">
<description>One-wide female edge connector, Side 2 only</description>
</package>
<package name="H807S-2">
<description>Two-wide Female Edge Connector, Side 2 only</description>
</package>
<package name="H800">
<description>One-wide female edge connector, 18 pin</description>
</package>
<package name="H800-2">
<description>Two-wide Female Edge Connector</description>
</package>
</packages>
<symbols>
<symbol name="NAND2">
<pin name="IN1" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN2" direction="in"/>
</symbol>
<symbol name="NAND1">
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="ENABLE">
<pin name="P$1" direction="in"/>
</symbol>
<symbol name="POWER">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="M101A">
<pin name="O1" direction="out" function="dot"/>
<pin name="IN1" direction="in"/>
<pin name="O2" direction="out" function="dot"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="O3" direction="out" function="dot"/>
<pin name="O4" direction="out" function="dot"/>
<pin name="O5" direction="out" function="dot"/>
<pin name="O6" direction="out" function="dot"/>
<pin name="O7" direction="out" function="dot"/>
<pin name="O8" direction="out" function="dot"/>
<pin name="O9" direction="out" function="dot"/>
<pin name="O10" direction="out" function="dot"/>
<pin name="O11" direction="out" function="dot"/>
<pin name="O12" direction="out" function="dot"/>
<pin name="O13" direction="out" function="dot"/>
<pin name="O14" direction="out" function="dot"/>
<pin name="O15" direction="out" function="dot"/>
<pin name="IN9" direction="in"/>
<pin name="IN10" direction="in"/>
<pin name="IN11" direction="in"/>
<pin name="IN12" direction="in"/>
<pin name="IN13" direction="in"/>
<pin name="IN14" direction="in"/>
<pin name="IN15" direction="in"/>
<pin name="ENABLE" direction="in"/>
</symbol>
<symbol name="NAND8">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
</symbol>
<symbol name="M103A">
<pin name="V2" direction="out"/>
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="H2" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="K2" direction="in"/>
<pin name="L2" direction="in"/>
<pin name="N2" direction="in"/>
<pin name="U2" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="A1" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="C1" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="F1" direction="out"/>
</symbol>
<symbol name="INVERTER-N">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="T1GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="NAND3">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
</symbol>
<symbol name="NAND4">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
</symbol>
<symbol name="AND-NOR">
<pin name="IN1A" direction="in"/>
<pin name="IN1B" direction="in"/>
<pin name="IN2A" direction="in"/>
<pin name="IN2B" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
</symbol>
<symbol name="M161">
<pin name="!O0" direction="out" function="dot"/>
<pin name="!O1" direction="out" function="dot"/>
<pin name="!O2" direction="out" function="dot"/>
<pin name="!O3" direction="out" function="dot"/>
<pin name="!O4" direction="out" function="dot"/>
<pin name="!O5" direction="out" function="dot"/>
<pin name="O0" direction="out"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
<pin name="O8" direction="out"/>
<pin name="!O6" direction="out" function="dot"/>
<pin name="!O7" direction="out" function="dot"/>
<pin name="!O8" direction="out" function="dot"/>
<pin name="O9" direction="out"/>
<pin name="!O9" direction="out" function="dot"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="EN3" direction="in"/>
<pin name="IN*" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN0" direction="in"/>
</symbol>
<symbol name="D-FLOP">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="1" direction="out"/>
<pin name="0" direction="out"/>
<pin name="S" direction="in" function="dot"/>
<pin name="R" direction="in" function="dot"/>
</symbol>
<symbol name="M206A">
<pin name="C1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="D1" direction="in" function="dot"/>
<pin name="E1" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="F2" direction="in" function="dot"/>
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="H2" direction="out"/>
<pin name="J2" direction="out"/>
<pin name="K1" direction="in" function="dot"/>
<pin name="M1" direction="out"/>
<pin name="L1" direction="out"/>
<pin name="J1" direction="in"/>
<pin name="H1" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="N2" direction="in" function="dot"/>
<pin name="M2" direction="in"/>
<pin name="P2" direction="out"/>
<pin name="L2" direction="in"/>
<pin name="R2" direction="out"/>
<pin name="R1" direction="in" function="dot"/>
<pin name="P1" direction="in"/>
<pin name="N1" direction="in"/>
<pin name="S1" direction="out"/>
<pin name="U1" direction="out"/>
<pin name="U2" direction="in" function="dot"/>
<pin name="V2" direction="out"/>
<pin name="V1" direction="out"/>
<pin name="T2" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="K2" direction="in"/>
</symbol>
<symbol name="JUMP-UP">
</symbol>
<symbol name="JUMP-DOWN">
</symbol>
<symbol name="M302A">
<pin name="D2" direction="pas"/>
<pin name="E2" direction="pas"/>
<pin name="F1" direction="pas"/>
<pin name="L2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="H1" direction="pas"/>
<pin name="J1" direction="pas"/>
<pin name="E1" direction="pas"/>
<pin name="F2" direction="out"/>
<pin name="H2" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="K2" direction="in"/>
</symbol>
<symbol name="M228A">
<pin name="BJ2" direction="out"/>
<pin name="BV2" direction="out"/>
<pin name="BE2" direction="out"/>
<pin name="AT2" direction="out"/>
<pin name="BU2" direction="out"/>
<pin name="AM2" direction="out"/>
<pin name="AK2" direction="out"/>
<pin name="AL1" direction="out"/>
<pin name="BF2" direction="out"/>
<pin name="BP2" direction="out"/>
<pin name="AU2" direction="out"/>
<pin name="AJ2" direction="out"/>
<pin name="AF1" direction="out"/>
<pin name="AH2" direction="out"/>
<pin name="AF2" direction="out"/>
<pin name="BV1" direction="out"/>
<pin name="BU1" direction="out"/>
<pin name="BM2" direction="out"/>
<pin name="BN2" direction="out"/>
<pin name="AE2" direction="out"/>
<pin name="AD2" direction="out"/>
<pin name="BS2" direction="out"/>
<pin name="BT2" direction="out"/>
<pin name="AH1" direction="out"/>
<pin name="AJ1" direction="out"/>
<pin name="AM1" direction="out"/>
<pin name="AN1" direction="in"/>
<pin name="AU1" direction="out"/>
<pin name="BR2" direction="in"/>
<pin name="BL2" direction="out"/>
<pin name="AP2" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="BC1" direction="in"/>
<pin name="AS2" direction="in"/>
<pin name="BF1" direction="in"/>
<pin name="BH2" direction="in"/>
<pin name="AV2" direction="in"/>
<pin name="AN2" direction="out"/>
<pin name="AR2" direction="out"/>
<pin name="BS1" direction="out"/>
<pin name="BK2" direction="out"/>
<pin name="BR1" direction="out"/>
<pin name="AK1" direction="out"/>
<pin name="BH1" direction="in"/>
</symbol>
<symbol name="M207A">
<pin name="S1" direction="out"/>
<pin name="U1" direction="out"/>
<pin name="V2" direction="out"/>
<pin name="V1" direction="out"/>
<pin name="P2" direction="out"/>
<pin name="R2" direction="out"/>
<pin name="M1" direction="out"/>
<pin name="L1" direction="out"/>
<pin name="J2" direction="out"/>
<pin name="H2" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="C1" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="K1" direction="in"/>
<pin name="H1" direction="in"/>
<pin name="J1" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="N1" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="U2" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="T2" direction="in"/>
<pin name="N2" direction="in"/>
<pin name="L2" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="K2" direction="in"/>
<pin name="A1" direction="in"/>
</symbol>
<symbol name="M307A">
<pin name="U1" direction="in" function="dot"/>
<pin name="S1" direction="in" function="dot"/>
<pin name="N1" direction="in"/>
<pin name="M2" direction="pas"/>
<pin name="U2" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="N2" direction="pas"/>
<pin name="V1" direction="pas"/>
<pin name="P1" direction="pas"/>
<pin name="H2" direction="out"/>
<pin name="F2" direction="out" function="dot"/>
<pin name="M1" direction="in" function="dot"/>
</symbol>
<symbol name="M401A">
<pin name="M2" direction="pas"/>
<pin name="N2" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="T2" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="K2" direction="in" function="dot"/>
<pin name="J2" direction="in" function="dot"/>
<pin name="E2" direction="out" function="dot"/>
<pin name="D2" direction="out"/>
</symbol>
<symbol name="M502A">
<pin name="D2" direction="out"/>
<pin name="H2" direction="in"/>
<pin name="E2" direction="pas"/>
</symbol>
<symbol name="-15V">
<pin name="-15V" direction="pwr"/>
</symbol>
<symbol name="M602A">
<pin name="H2" direction="in" function="dot"/>
<pin name="J2" direction="in" function="dot"/>
<pin name="K2" direction="in" function="dot"/>
<pin name="E2" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="F2" direction="out" function="dot"/>
</symbol>
<symbol name="M623A">
<pin name="D" direction="oc" function="dot"/>
<pin name="C" direction="in"/>
<pin name="A" direction="in"/>
<pin name="E" direction="oc" function="dot"/>
<pin name="B" direction="in"/>
</symbol>
<symbol name="M633A">
<pin name="A" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="D" direction="out" function="dot"/>
<pin name="E" direction="out" function="dot"/>
</symbol>
<symbol name="PIN">
<pin name="P$2"/>
</symbol>
<symbol name="W005A">
<pin name="P$1" direction="pas"/>
</symbol>
<symbol name="G888">
<pin name="N2" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="P2" direction="in" function="dot"/>
<pin name="L2" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="J2" direction="out"/>
<pin name="K2" direction="out"/>
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="H2" direction="in"/>
<pin name="V2" direction="out"/>
<pin name="U2" direction="out"/>
</symbol>
<symbol name="G821A">
<pin name="VCC@1" direction="sup"/>
<pin name="VCC@2" direction="sup"/>
<pin name="VCC@3" direction="sup"/>
<pin name="VCC@4" direction="sup"/>
<pin name="+11V" direction="pwr"/>
<pin name="BN1" direction="in"/>
<pin name="BP1" direction="in"/>
<pin name="BR1" direction="out"/>
<pin name="BM1" direction="out"/>
</symbol>
<symbol name="PULL-UP">
<pin name="P$1" direction="pas"/>
</symbol>
<symbol name="D-FLOP-K2">
<pin name="S" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="1" direction="out"/>
<pin name="0" direction="out"/>
</symbol>
<symbol name="D-FLOP-A1">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="1" direction="out"/>
<pin name="0" direction="out"/>
<pin name="S" direction="in" function="dot"/>
</symbol>
<symbol name="PART">
</symbol>
<symbol name="NC">
<pin name="NC" direction="sup"/>
</symbol>
<symbol name="+11V">
<pin name="+11V" direction="sup"/>
</symbol>
<symbol name="M651">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="SLOW" direction="pas"/>
</symbol>
<symbol name="M507">
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="DIODECLAMP">
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="G805">
<pin name="AV2" direction="in"/>
<pin name="-6V@BM2" direction="sup"/>
<pin name="GND@BC2" direction="sup"/>
<pin name="-30V@AE2" direction="sup"/>
</symbol>
<symbol name="G826">
<pin name="BR2" direction="pas"/>
<pin name="BS2" direction="pas"/>
<pin name="AH2" direction="in"/>
<pin name="AF2" direction="out"/>
<pin name="AJ2"/>
<pin name="BJ2" direction="out"/>
<pin name="BK2" direction="pas"/>
<pin name="-6V@BM2" direction="sup"/>
<pin name="-30V@BV2" direction="sup"/>
<pin name="AS2"/>
</symbol>
<symbol name="-6V">
<pin name="-6V" direction="pwr"/>
</symbol>
<symbol name="-30V">
<pin name="-30V" direction="pwr"/>
</symbol>
<symbol name="G624A">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="G624B">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
<pin name="P$3" direction="pas"/>
</symbol>
<symbol name="G624C">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="G624D">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="M310">
<pin name="H2" direction="in"/>
<pin name="J2" direction="out"/>
<pin name="K2" direction="out"/>
<pin name="L2" direction="out"/>
<pin name="M2" direction="out"/>
<pin name="N2" direction="out"/>
<pin name="P2" direction="out"/>
<pin name="R2" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="T2" direction="out"/>
<pin name="U2" direction="out"/>
<pin name="V2" direction="out"/>
</symbol>
<symbol name="BUFFER">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="G228A">
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="N2" direction="in"/>
<pin name="L1" direction="in"/>
<pin name="L2" direction="pas"/>
<pin name="F2" direction="pas"/>
<pin name="K1" direction="pas"/>
<pin name="E1" direction="pas"/>
<pin name="U2" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="M1" direction="pas"/>
<pin name="V2" direction="in"/>
</symbol>
<symbol name="AND-NOR4">
<pin name="IN1A" direction="in"/>
<pin name="IN1B" direction="in"/>
<pin name="IN2A" direction="in"/>
<pin name="IN2B" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN3A" direction="in"/>
<pin name="IN3B" direction="in"/>
<pin name="IN4A" direction="in"/>
<pin name="IN4B" direction="in"/>
<pin name="IN1C" direction="in"/>
<pin name="IN1D" direction="in"/>
<pin name="IN4C" direction="in"/>
<pin name="IN4D" direction="in"/>
</symbol>
<symbol name="AND-NOR5">
<pin name="IN1A" direction="in"/>
<pin name="IN1B" direction="in"/>
<pin name="IN2A" direction="in"/>
<pin name="IN2B" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN3A" direction="in"/>
<pin name="IN3B" direction="in"/>
<pin name="IN4A" direction="in"/>
<pin name="IN4B" direction="in"/>
<pin name="IN5A" direction="in"/>
<pin name="IN5B" direction="in"/>
<pin name="IN1D" direction="in"/>
<pin name="IN1C" direction="in"/>
<pin name="IN5C" direction="in"/>
</symbol>
<symbol name="M162">
<pin name="1B" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="8B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="8A" direction="in"/>
<pin name="ODD" direction="out"/>
<pin name="EVEN" direction="out" function="dot"/>
</symbol>
<symbol name="M506">
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN2" direction="pas"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="M660">
<pin name="IN1" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN2" direction="in"/>
</symbol>
<symbol name="M661">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="M516">
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN2"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="M220">
<pin name="BH2" direction="in"/>
<pin name="BJ2" direction="in"/>
<pin name="BF1" direction="in"/>
<pin name="BC1" direction="in"/>
<pin name="BF2" direction="in"/>
<pin name="BL1" direction="in"/>
<pin name="BL2" direction="in"/>
<pin name="BP1" direction="in"/>
<pin name="BS2" direction="in"/>
<pin name="BU2" direction="in"/>
<pin name="BT2" direction="in"/>
<pin name="BJ1" direction="out"/>
<pin name="BK2" direction="in"/>
<pin name="AA1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="AB1" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="AF2" direction="in"/>
<pin name="AH1" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AB2" direction="in"/>
<pin name="AC1" direction="in"/>
<pin name="AJ2" direction="in"/>
<pin name="AE2" direction="out"/>
<pin name="AF1" direction="out"/>
<pin name="AU1" direction="in"/>
<pin name="BA1" direction="out"/>
<pin name="BB1" direction="out"/>
<pin name="AR1" direction="in"/>
<pin name="AT2" direction="out"/>
<pin name="AU2" direction="out"/>
<pin name="AN2" direction="in"/>
<pin name="AP1" direction="out"/>
<pin name="AR2" direction="out"/>
<pin name="AK1" direction="in"/>
<pin name="AM2" direction="out"/>
<pin name="AM1" direction="out"/>
<pin name="AV1" direction="out"/>
<pin name="AV2" direction="out"/>
<pin name="AS2" direction="out"/>
<pin name="AS1" direction="out"/>
<pin name="AN1" direction="out"/>
<pin name="AP2" direction="out"/>
<pin name="AL2" direction="out"/>
<pin name="AL1" direction="out"/>
<pin name="AJ1" direction="out"/>
<pin name="AK2" direction="out"/>
<pin name="BB2" direction="in"/>
<pin name="BH1" direction="in"/>
<pin name="BE1" direction="in"/>
<pin name="BD1" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="BK1" direction="in"/>
<pin name="BR1" direction="in"/>
<pin name="BS1" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="BN2" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="BN1" direction="in"/>
<pin name="BP2" direction="in"/>
<pin name="BM1" direction="in"/>
<pin name="BR2" direction="in"/>
<pin name="BV2" direction="in"/>
<pin name="BV1" direction="in"/>
<pin name="BU1" direction="in"/>
</symbol>
<symbol name="G610A">
<pin name="L2" direction="pas"/>
<pin name="K2" direction="pas"/>
<pin name="J2" direction="pas"/>
<pin name="H2" direction="pas"/>
<pin name="F2" direction="pas"/>
<pin name="E2" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="U2" direction="pas"/>
<pin name="T2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="N2" direction="pas"/>
<pin name="M2" direction="pas"/>
</symbol>
<symbol name="CORE">
</symbol>
<symbol name="M921">
<pin name="L1"/>
<pin name="L2"/>
<pin name="L3"/>
<pin name="R1"/>
<pin name="R2"/>
</symbol>
<symbol name="M900">
<pin name="1" direction="in"/>
</symbol>
<symbol name="NAND1D">
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="OR2">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OR1C">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OR1D">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="ACTIVELOW">
</symbol>
<symbol name="ACTIVEHIGH">
</symbol>
<symbol name="R401">
<pin name="R" direction="pas"/>
<pin name="L" direction="pas"/>
<pin name="T" direction="pas"/>
<pin name="U" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="D" direction="out"/>
<pin name="S" direction="in"/>
<pin name="M" direction="pas"/>
<pin name="N" direction="pas"/>
<pin name="P" direction="pas"/>
</symbol>
<symbol name="R202A">
<pin name="PU1" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="PU0" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="SET" direction="pas"/>
<pin name="RESET" direction="in"/>
<pin name="1" direction="oc"/>
<pin name="0" direction="oc"/>
</symbol>
<symbol name="R202B">
<pin name="PU1" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="PU0" direction="in"/>
<pin name="EN0" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="1" direction="oc"/>
<pin name="0" direction="oc"/>
</symbol>
<symbol name="R113">
<pin name="I$1" direction="in"/>
<pin name="I$2" direction="in"/>
<pin name="O$1" direction="oc"/>
</symbol>
<symbol name="R107A">
<pin name="I$1" direction="in"/>
<pin name="O$1" direction="oc"/>
</symbol>
<symbol name="R107B">
<pin name="I$1" direction="in"/>
<pin name="I$2" direction="pas"/>
<pin name="O$1" direction="oc"/>
</symbol>
<symbol name="R111">
<pin name="I$1" direction="in"/>
<pin name="I$2" direction="in"/>
<pin name="O$1" direction="oc"/>
<pin name="I$3" direction="pas"/>
</symbol>
<symbol name="R603">
<pin name="PU0" direction="in"/>
<pin name="EN0" direction="pas"/>
<pin name="O" direction="oc"/>
<pin name="G" direction="in"/>
<pin name="I$1" direction="pas"/>
</symbol>
<symbol name="R602A">
<pin name="H" direction="in"/>
<pin name="J" direction="in"/>
<pin name="K" direction="oc"/>
<pin name="GND" direction="pwr"/>
<pin name="L" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="D" direction="pas"/>
<pin name="M" direction="pas"/>
</symbol>
<symbol name="R602B">
<pin name="H" direction="in"/>
<pin name="J" direction="in"/>
<pin name="K" direction="oc"/>
<pin name="C" direction="in"/>
<pin name="L" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="R302">
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="M" direction="out"/>
<pin name="H" direction="pas"/>
<pin name="J" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="L" direction="pas"/>
</symbol>
<symbol name="R151">
<pin name="E" direction="in"/>
<pin name="L" direction="in"/>
<pin name="K" direction="in"/>
<pin name="F" direction="in"/>
<pin name="J" direction="in"/>
<pin name="H" direction="in"/>
<pin name="M" direction="out"/>
<pin name="N" direction="out"/>
<pin name="P" direction="out"/>
<pin name="R" direction="out"/>
<pin name="S" direction="out"/>
<pin name="T" direction="out"/>
<pin name="U" direction="out"/>
<pin name="V" direction="out"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="R002">
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="oc"/>
</symbol>
<symbol name="R001">
<pin name="D" direction="in"/>
<pin name="E" direction="oc"/>
</symbol>
<symbol name="W050">
<pin name="I$1" direction="in"/>
<pin name="O$1" direction="out"/>
</symbol>
<symbol name="W506">
<pin name="K" direction="out"/>
<pin name="L" direction="out"/>
<pin name="M" direction="out"/>
<pin name="J" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="pas"/>
<pin name="H" direction="pas"/>
</symbol>
<symbol name="W501A">
<pin name="M" direction="in"/>
<pin name="L" direction="in"/>
<pin name="R" direction="in"/>
<pin name="F" direction="out"/>
<pin name="P" direction="in"/>
</symbol>
<symbol name="W501B">
<pin name="N" direction="out"/>
<pin name="K" direction="out"/>
</symbol>
<symbol name="M051">
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="M507-1">
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="W512">
<pin name="OUT" direction="out"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="R181">
<pin name="K" direction="in"/>
<pin name="F" direction="in"/>
<pin name="H" direction="in"/>
<pin name="E" direction="in"/>
<pin name="J" direction="in"/>
<pin name="D" direction="in"/>
<pin name="S" direction="out"/>
<pin name="R" direction="out"/>
<pin name="N" direction="out"/>
<pin name="P" direction="out"/>
<pin name="T" direction="out"/>
<pin name="U" direction="out"/>
<pin name="M" direction="in"/>
</symbol>
<symbol name="W640">
<pin name="H" direction="out"/>
<pin name="J" direction="in"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="R141">
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="H" direction="in"/>
<pin name="J" direction="in"/>
<pin name="K" direction="in"/>
<pin name="L" direction="in"/>
<pin name="M" direction="in"/>
<pin name="N" direction="in"/>
<pin name="P" direction="in"/>
<pin name="R" direction="in"/>
<pin name="S" direction="in"/>
<pin name="T" direction="in"/>
<pin name="U" direction="in"/>
<pin name="V" direction="in"/>
<pin name="D" direction="out"/>
</symbol>
<symbol name="W501C">
<pin name="S" direction="pas"/>
<pin name="T" direction="pas"/>
</symbol>
<symbol name="INVERTER-P">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
</symbol>
<symbol name="M700">
<pin name="CS2" direction="in"/>
<pin name="CN2" direction="out"/>
<pin name="CR2" direction="in"/>
<pin name="CP2" direction="in"/>
<pin name="CM2" direction="out"/>
<pin name="CT2" direction="out"/>
<pin name="CL2" direction="in"/>
<pin name="CK2" direction="out"/>
<pin name="CJ2" direction="out"/>
<pin name="CH2" direction="out"/>
<pin name="CF2" direction="out"/>
<pin name="CE2" direction="out"/>
<pin name="DD2" direction="out"/>
</symbol>
<symbol name="M220A">
<pin name="AJ1" direction="out"/>
<pin name="BA1" direction="out"/>
<pin name="BB1" direction="out"/>
<pin name="AK2" direction="out"/>
<pin name="AV1" direction="out"/>
<pin name="AV2" direction="out"/>
<pin name="AU1" direction="in"/>
<pin name="AT2" direction="out"/>
<pin name="AU2" direction="out"/>
<pin name="AS2" direction="out"/>
<pin name="AS1" direction="out"/>
<pin name="AR1" direction="in"/>
<pin name="AP1" direction="out"/>
<pin name="AR2" direction="out"/>
<pin name="AN1" direction="out"/>
<pin name="AP2" direction="out"/>
<pin name="AN2" direction="in"/>
<pin name="AM2" direction="out"/>
<pin name="AM1" direction="out"/>
<pin name="AL2" direction="out"/>
<pin name="AL1" direction="out"/>
<pin name="AK1" direction="in"/>
</symbol>
<symbol name="M220B">
<pin name="BH2" direction="in"/>
<pin name="BJ2" direction="in"/>
<pin name="BF1" direction="in"/>
<pin name="BC1" direction="in"/>
<pin name="BF2" direction="in"/>
<pin name="BL1" direction="in"/>
<pin name="BL2" direction="in"/>
<pin name="BP1" direction="in"/>
<pin name="BS2" direction="in"/>
<pin name="BU2" direction="in"/>
<pin name="BT2" direction="in"/>
<pin name="BK2" direction="out"/>
<pin name="AA1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="AB1" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="AF2" direction="in"/>
<pin name="AH1" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AB2" direction="in"/>
<pin name="AC1" direction="in"/>
<pin name="AJ2" direction="in"/>
<pin name="AE2" direction="out"/>
<pin name="AF1" direction="out"/>
<pin name="BB2" direction="in"/>
<pin name="BH1" direction="in"/>
<pin name="BE1" direction="in"/>
<pin name="BD1" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="BK1" direction="in"/>
<pin name="BR1" direction="in"/>
<pin name="BS1" direction="in"/>
</symbol>
<symbol name="M220C">
<pin name="BJ1" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="BN2" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="BN1" direction="in"/>
<pin name="BP2" direction="in"/>
<pin name="BM1" direction="in"/>
<pin name="BR2" direction="in"/>
<pin name="BV2" direction="in"/>
<pin name="BV1" direction="in"/>
<pin name="BU1" direction="in"/>
</symbol>
<symbol name="M706">
<pin name="BU1" direction="in"/>
<pin name="P$2" direction="in"/>
<pin name="AK2" direction="out" function="dot"/>
<pin name="AR2" direction="out" function="dot"/>
<pin name="AS2" direction="out" function="dot"/>
<pin name="AL1" direction="out" function="dot"/>
<pin name="AM1" direction="out" function="dot"/>
<pin name="AP2" direction="out" function="dot"/>
<pin name="AT2" direction="out" function="dot"/>
<pin name="AN2" direction="out" function="dot"/>
<pin name="BH2" direction="out" function="dot"/>
<pin name="BD2" direction="in"/>
<pin name="AS1" direction="out"/>
<pin name="BK2" direction="out"/>
<pin name="AS3" direction="out"/>
<pin name="AS4" direction="out"/>
</symbol>
<symbol name="M360">
<pin name="P" direction="in"/>
<pin name="S" direction="out"/>
<pin name="R" direction="in"/>
<pin name="T" direction="oc" function="dot"/>
</symbol>
<symbol name="G020">
<pin name="B1" direction="in"/>
<pin name="C1" direction="out"/>
<pin name="T2" direction="in"/>
<pin name="A1" direction="oc" function="dot"/>
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="E1" direction="out"/>
<pin name="S2" direction="pas"/>
<pin name="S1" direction="out"/>
<pin name="U2" direction="oc" function="dot"/>
<pin name="L1" direction="in"/>
<pin name="M1" direction="in"/>
<pin name="K2" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="R1" direction="in"/>
</symbol>
<symbol name="G228B">
<pin name="H" direction="in"/>
<pin name="J" direction="pas"/>
<pin name="K" direction="pas"/>
</symbol>
<symbol name="MEMSUP">
<pin name="MEM_SUPPLY+" direction="pwr"/>
<pin name="MEM_SUPPLY-" direction="pwr"/>
</symbol>
<symbol name="G221">
<pin name="E2" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="H2" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="T2" direction="in"/>
<pin name="R2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="N2" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="L2" direction="pas"/>
<pin name="M2" direction="pas"/>
<pin name="J2" direction="pas"/>
<pin name="K2" direction="pas"/>
<pin name="V2" direction="in"/>
</symbol>
<symbol name="NAND4OC">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="OUT" direction="oc" function="dot"/>
</symbol>
<symbol name="M710">
<pin name="BF2" direction="in"/>
<pin name="AK1" direction="out"/>
<pin name="AL1" direction="out"/>
<pin name="AM1" direction="out"/>
<pin name="AN1" direction="out"/>
<pin name="AK2" direction="out"/>
<pin name="AL2" direction="out"/>
<pin name="AM2" direction="out"/>
<pin name="AN2" direction="out"/>
<pin name="AH1" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AF1" direction="in"/>
<pin name="AF2" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="AE2" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="BD1" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="BE1" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="BF1" direction="in"/>
<pin name="AP2" direction="in"/>
<pin name="AR1" direction="in"/>
<pin name="AR2" direction="in"/>
<pin name="AJ2" direction="out"/>
<pin name="AS1" direction="out"/>
<pin name="AU2" direction="out"/>
<pin name="BN2" direction="oc" function="dot"/>
<pin name="BS2" direction="oc" function="dot"/>
<pin name="AS2" direction="in"/>
<pin name="AT2" direction="in"/>
<pin name="AJ1" direction="out"/>
<pin name="AV2" direction="in"/>
<pin name="BV1" direction="out"/>
<pin name="BH2" direction="out" function="dot"/>
<pin name="AU1" direction="in"/>
</symbol>
<symbol name="M715">
<pin name="AK" direction="in"/>
<pin name="BS" direction="in"/>
<pin name="AM" direction="out"/>
<pin name="BR" direction="out"/>
<pin name="AS" direction="out"/>
<pin name="AP" direction="out"/>
<pin name="AU" direction="out"/>
<pin name="AT" direction="out"/>
<pin name="BP" direction="in"/>
<pin name="BT" direction="in"/>
</symbol>
<symbol name="M705">
<pin name="BD2" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="BE1" direction="in"/>
<pin name="BF2" direction="in"/>
<pin name="BF1" direction="in"/>
<pin name="BH2" direction="in"/>
<pin name="AU2" direction="in"/>
<pin name="AV2" direction="in"/>
<pin name="BK1" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="BS2" direction="in"/>
<pin name="BP1" direction="in"/>
<pin name="BJ1" direction="in"/>
<pin name="BM1" direction="in"/>
<pin name="AJ1" direction="out"/>
<pin name="BN2" direction="in"/>
<pin name="BD1" direction="in"/>
<pin name="AF1" direction="in"/>
<pin name="AF2" direction="in"/>
<pin name="AH1" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="AE2" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="AJ2" direction="out"/>
<pin name="AM2" direction="out"/>
<pin name="AK2" direction="oc"/>
<pin name="AL2" direction="oc"/>
<pin name="BR2" direction="out"/>
<pin name="BK2" direction="out"/>
<pin name="BS1" direction="out"/>
<pin name="BP2" direction="out"/>
<pin name="BU2" direction="out"/>
<pin name="BR1" direction="out"/>
<pin name="AP2" direction="oc"/>
<pin name="AS2" direction="oc"/>
<pin name="AR1" direction="oc"/>
<pin name="AN2" direction="oc"/>
<pin name="AS1" direction="oc"/>
<pin name="AP1" direction="oc"/>
<pin name="AR2" direction="oc"/>
<pin name="AN1" direction="oc"/>
<pin name="AT2" direction="out"/>
<pin name="AK1" direction="out"/>
</symbol>
<symbol name="M306">
<pin name="H" direction="in"/>
<pin name="J" direction="in"/>
<pin name="E" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="L" direction="pas"/>
<pin name="M" direction="pas"/>
<pin name="T" direction="out"/>
<pin name="S" direction="out" function="dot"/>
</symbol>
<symbol name="M7102A">
<pin name="AK1" direction="in"/>
<pin name="AF1" direction="oc"/>
<pin name="BE2" direction="in"/>
<pin name="AL1" direction="in"/>
<pin name="BL2" direction="oc"/>
<pin name="BD2" direction="in"/>
<pin name="AM1" direction="in"/>
<pin name="BM2" direction="oc"/>
<pin name="BE1" direction="out"/>
<pin name="AF2" direction="oc"/>
<pin name="AJ1" direction="oc"/>
<pin name="AJ2" direction="oc"/>
<pin name="AH1" direction="oc"/>
<pin name="AH2" direction="oc"/>
<pin name="BK2" direction="oc"/>
</symbol>
<symbol name="M7102B">
<pin name="AN1" direction="in"/>
<pin name="AP1" direction="in"/>
<pin name="BH2" direction="oc"/>
<pin name="AR1" direction="in"/>
<pin name="BJ2" direction="oc"/>
<pin name="BF2" direction="oc"/>
</symbol>
<symbol name="M7102C">
<pin name="AK2" direction="in"/>
<pin name="AL2" direction="in"/>
<pin name="AM2" direction="out"/>
<pin name="AN2" direction="out"/>
</symbol>
<symbol name="M7102D">
<pin name="AP2" direction="in"/>
<pin name="AR2" direction="in"/>
<pin name="AS2" direction="out"/>
<pin name="BB1" direction="oc"/>
<pin name="AT2" direction="out"/>
<pin name="BA1" direction="oc"/>
</symbol>
<symbol name="M7102E">
<pin name="BN2" direction="in"/>
<pin name="BP2" direction="in"/>
<pin name="AE1" direction="oc"/>
<pin name="AD1" direction="oc"/>
<pin name="BR2" direction="in"/>
<pin name="BS2" direction="in"/>
<pin name="AE2" direction="oc"/>
<pin name="AD2" direction="oc"/>
</symbol>
<symbol name="NOR2">
<pin name="OUT" direction="out" function="dot"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
</symbol>
<symbol name="M7102F">
<pin name="BD1" direction="in"/>
<pin name="BC1" direction="out"/>
<pin name="BV2" direction="oc" function="dot"/>
<pin name="AV1" direction="in"/>
<pin name="AU1" direction="out"/>
</symbol>
<symbol name="M7102G">
<pin name="BU1" direction="in"/>
<pin name="BU2" direction="out" function="dot"/>
<pin name="AB1" direction="oc"/>
<pin name="BV1" direction="in"/>
<pin name="AA1" direction="oc" function="dot"/>
</symbol>
<symbol name="M7101">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="BR1" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="IN7" direction="in"/>
<pin name="J" direction="in"/>
<pin name="AS2" direction="out"/>
<pin name="AT2" direction="out" function="dot"/>
<pin name="IN9" direction="in"/>
<pin name="T1" direction="out"/>
<pin name="T2" direction="out"/>
<pin name="IN8" direction="in"/>
<pin name="T3" direction="out"/>
<pin name="J1" direction="in"/>
<pin name="OUT42" direction="out"/>
<pin name="IN2A" direction="in"/>
<pin name="IN2B" direction="in"/>
<pin name="OUT1" direction="out" function="dot"/>
<pin name="IN3A" direction="in"/>
<pin name="BD1" direction="in"/>
<pin name="BE1" direction="in"/>
<pin name="OUT3" direction="out" function="dot"/>
<pin name="BF1" direction="in"/>
<pin name="BK1" direction="in"/>
<pin name="AS1" direction="out"/>
<pin name="J2" direction="in"/>
<pin name="AU1" direction="in"/>
<pin name="J3" direction="in"/>
<pin name="AV2" direction="out"/>
<pin name="C" direction="in"/>
<pin name="0" direction="out"/>
<pin name="C1" direction="in"/>
<pin name="3" direction="out"/>
<pin name="C2" direction="in"/>
<pin name="5" direction="out"/>
<pin name="C3" direction="in"/>
<pin name="7" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="OUT9" direction="out"/>
<pin name="OUT10" direction="out"/>
<pin name="C4" direction="in"/>
<pin name="C5" direction="in"/>
<pin name="C6" direction="in"/>
<pin name="AP2" direction="in"/>
<pin name="AP1" direction="out"/>
<pin name="AV1" direction="in"/>
</symbol>
<symbol name="M650">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="SLOW" direction="pas"/>
</symbol>
<symbol name="G021">
<pin name="B1" direction="in"/>
<pin name="C1" direction="out"/>
<pin name="T2" direction="in"/>
<pin name="A1" direction="oc" function="dot"/>
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="E1" direction="out"/>
<pin name="S2" direction="pas"/>
<pin name="S1" direction="out"/>
<pin name="U2" direction="oc" function="dot"/>
<pin name="L1" direction="in"/>
<pin name="M1" direction="in"/>
<pin name="K2" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="H2" direction="in"/>
<pin name="J2" direction="out"/>
<pin name="N1" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="R2" direction="out"/>
</symbol>
<symbol name="M720">
<pin name="V2" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="E2" direction="oc" function="dot"/>
<pin name="D2" direction="oc" function="dot"/>
</symbol>
<symbol name="INVERTER-OC">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="oc" function="dot"/>
</symbol>
<symbol name="M040">
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="H" direction="in"/>
<pin name="R" direction="oc" function="dot"/>
</symbol>
<symbol name="M706X">
<pin name="BR1" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="BJ2" direction="in"/>
<pin name="AL2" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="AF1" direction="in"/>
<pin name="AH1" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AJ1" direction="in"/>
<pin name="BF2" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="BU1" direction="in"/>
<pin name="AV2" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="AR1" direction="in"/>
<pin name="BR2" direction="in"/>
<pin name="AK1" direction="in"/>
<pin name="AK2" direction="out"/>
<pin name="AR2" direction="out"/>
<pin name="AS2" direction="out"/>
<pin name="AL1" direction="out"/>
<pin name="AM1" direction="out"/>
<pin name="AP2" direction="out"/>
<pin name="AT2" direction="out"/>
<pin name="AN2" direction="out"/>
<pin name="BH2" direction="out"/>
<pin name="BE2" direction="out"/>
<pin name="AD1" direction="out"/>
<pin name="BN2" direction="out"/>
<pin name="BK2" direction="out"/>
<pin name="AF2" direction="out"/>
<pin name="BS2" direction="out"/>
<pin name="BS1" direction="out"/>
<pin name="BT2" direction="out"/>
<pin name="AE2" direction="out"/>
<pin name="AU2" direction="out"/>
<pin name="AM2" direction="out"/>
<pin name="AJ2" direction="out"/>
<pin name="BU2" direction="out"/>
<pin name="BV2" direction="out"/>
<pin name="BD1" direction="in"/>
<pin name="AS1" direction="out"/>
</symbol>
<symbol name="M501">
<pin name="K2" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="D2" direction="out"/>
<pin name="F2"/>
</symbol>
<symbol name="M452">
<pin name="R2" direction="out"/>
<pin name="J2" direction="out"/>
<pin name="M2" direction="out"/>
<pin name="N2" direction="out"/>
<pin name="L2" direction="out"/>
<pin name="K2" direction="out"/>
<pin name="P2" direction="in"/>
</symbol>
<symbol name="M707">
<pin name="AH1" direction="in"/>
<pin name="AK1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AP2" direction="in"/>
<pin name="AR2" direction="in"/>
<pin name="AL2" direction="in"/>
<pin name="AM2" direction="in"/>
<pin name="AU2" direction="in"/>
<pin name="AS2" direction="in"/>
<pin name="AT2" direction="in"/>
<pin name="AU1" direction="in"/>
<pin name="AE2" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="AF2" direction="in"/>
<pin name="AF1" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AJ2" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="BH2" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="AS1" direction="in"/>
<pin name="BF2" direction="in"/>
<pin name="BS2" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="BN2" direction="in"/>
<pin name="BP2" direction="in"/>
<pin name="AL1" direction="out"/>
<pin name="AK2" direction="out"/>
<pin name="AJ1" direction="out"/>
<pin name="AD2" direction="out"/>
<pin name="AV2" direction="out"/>
<pin name="AR1" direction="out"/>
<pin name="BR2" direction="out"/>
<pin name="BP1" direction="out"/>
<pin name="BN1" direction="out"/>
<pin name="AD1" direction="out"/>
<pin name="BK2" direction="out"/>
<pin name="BJ1" direction="out"/>
<pin name="BJ2" direction="out"/>
</symbol>
<symbol name="M703">
<pin name="L2" direction="out"/>
<pin name="R2" direction="out"/>
<pin name="T2" direction="out"/>
<pin name="P2" direction="out"/>
<pin name="N2" direction="out"/>
<pin name="U1" direction="out"/>
<pin name="D2" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="H2" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="K2" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="U2" direction="in"/>
<pin name="S2" direction="in"/>
</symbol>
<symbol name="M701">
<pin name="BF2" direction="in"/>
<pin name="BH2" direction="in"/>
<pin name="BK2" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="BN2" direction="in"/>
<pin name="BL2" direction="in"/>
<pin name="BJ2" direction="in"/>
<pin name="AK2" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AP1" direction="in"/>
<pin name="AK1" direction="in"/>
<pin name="AR1" direction="in"/>
<pin name="AJ2" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AP2" direction="out"/>
<pin name="AS1" direction="out"/>
<pin name="AR2" direction="out"/>
<pin name="AS2" direction="out"/>
<pin name="AE2" direction="out"/>
<pin name="AJ1" direction="out"/>
<pin name="BP2" direction="oc"/>
<pin name="BR2" direction="oc"/>
</symbol>
<symbol name="A607">
<pin name="AD2"/>
<pin name="AE2" direction="in"/>
<pin name="AF2" direction="in"/>
<pin name="AM2" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AS2" direction="in"/>
<pin name="AT2" direction="in"/>
<pin name="BD2" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="BH2" direction="in"/>
<pin name="BJ2" direction="in"/>
<pin name="AL2"/>
<pin name="BS2" direction="out"/>
</symbol>
<symbol name="M704">
<pin name="AF2" direction="in"/>
<pin name="AH2" direction="in"/>
<pin name="AE2" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="BU1" direction="in"/>
<pin name="AS2" direction="in"/>
<pin name="BV1" direction="in"/>
<pin name="AK2" direction="in"/>
<pin name="BH2" direction="in"/>
<pin name="BL2" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="BP2" direction="in"/>
<pin name="BT2" direction="in"/>
<pin name="BN2" direction="in"/>
<pin name="AJ2" direction="out"/>
<pin name="AL2" direction="out"/>
<pin name="AN2" direction="out"/>
<pin name="AR2" direction="out"/>
<pin name="AT2" direction="out"/>
<pin name="AV2" direction="out"/>
<pin name="BJ2" direction="out"/>
<pin name="BK2" direction="out"/>
<pin name="AP2" direction="out"/>
<pin name="BD2" direction="out"/>
<pin name="AU2" direction="out"/>
<pin name="AM2" direction="out"/>
<pin name="BS2" direction="out"/>
<pin name="BE2" direction="oc"/>
<pin name="BF2" direction="oc"/>
</symbol>
<symbol name="M708">
<pin name="D2" direction="in"/>
<pin name="T2" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="N2" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="N1" direction="in"/>
<pin name="U2" direction="in"/>
<pin name="L1" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="L2" direction="in"/>
<pin name="R1" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="H1" direction="oc"/>
<pin name="C1" direction="oc"/>
<pin name="J2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="E1" direction="out"/>
<pin name="K1" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="V2" direction="in"/>
<pin name="K2" direction="out"/>
<pin name="V1" direction="in"/>
</symbol>
<symbol name="M709">
<pin name="BJ2" direction="in"/>
<pin name="BP1" direction="in"/>
<pin name="BJ1" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="BA1" direction="in"/>
<pin name="AV1" direction="in"/>
<pin name="AH1" direction="in"/>
<pin name="AU2" direction="in"/>
<pin name="AK1" direction="in"/>
<pin name="AT2" direction="in"/>
<pin name="AL1" direction="in"/>
<pin name="AR1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AR2" direction="in"/>
<pin name="AP1" direction="in"/>
<pin name="BL1" direction="in"/>
<pin name="BK1" direction="in"/>
<pin name="BN1" direction="out"/>
<pin name="BS1" direction="out"/>
<pin name="AF2" direction="oc"/>
<pin name="BD1" direction="oc"/>
<pin name="AF1" direction="oc"/>
<pin name="BB1" direction="oc"/>
<pin name="AJ2" direction="oc"/>
<pin name="AU1" direction="oc"/>
<pin name="AJ1" direction="oc"/>
<pin name="AV2" direction="oc"/>
<pin name="AM1" direction="oc"/>
<pin name="AP2" direction="oc"/>
<pin name="AM2" direction="oc"/>
<pin name="AS1" direction="oc"/>
<pin name="BM2" direction="oc"/>
<pin name="BF1" direction="out"/>
<pin name="BH1" direction="out"/>
<pin name="AE2" direction="out"/>
<pin name="BR1" direction="out"/>
<pin name="BM1" direction="out"/>
<pin name="BH2" direction="out"/>
</symbol>
<symbol name="M714">
<pin name="C1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="E1" direction="in"/>
<pin name="F2" direction="in"/>
<pin name="H2" direction="in"/>
<pin name="F1" direction="in"/>
<pin name="N1" direction="in"/>
<pin name="U2" direction="in"/>
<pin name="R2" direction="in"/>
<pin name="J1" direction="in"/>
<pin name="K1" direction="in"/>
<pin name="M1" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="J2" direction="out"/>
<pin name="H1" direction="out"/>
<pin name="P1" direction="out"/>
<pin name="R1" direction="out"/>
<pin name="P2" direction="oc"/>
<pin name="N2" direction="oc"/>
<pin name="T2" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="U1" direction="out"/>
<pin name="L1" direction="out"/>
</symbol>
<symbol name="M716">
<pin name="AF1" direction="oc"/>
<pin name="AF2" direction="oc"/>
<pin name="AH2" direction="oc"/>
<pin name="AJ2" direction="oc"/>
<pin name="AN2" direction="oc"/>
<pin name="AM2" direction="oc"/>
<pin name="AU2" direction="oc"/>
<pin name="AV2" direction="oc"/>
<pin name="BP2" direction="oc"/>
<pin name="BN2" direction="oc"/>
<pin name="BJ2" direction="oc"/>
<pin name="BH2" direction="oc"/>
<pin name="BU1" direction="out"/>
<pin name="AE2" direction="in"/>
<pin name="AE1" direction="in"/>
<pin name="AL2" direction="in"/>
<pin name="AK2" direction="in"/>
<pin name="AR2" direction="in"/>
<pin name="AP2" direction="in"/>
<pin name="BE2" direction="in"/>
<pin name="AS2" direction="in"/>
<pin name="BS1" direction="in"/>
<pin name="BR1" direction="in"/>
<pin name="BK2" direction="in"/>
<pin name="BL2" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="AH1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="BS2" direction="in"/>
</symbol>
<symbol name="G610B">
<pin name="L2" direction="pas"/>
<pin name="K2" direction="pas"/>
<pin name="J2" direction="pas"/>
<pin name="H2" direction="pas"/>
<pin name="F2" direction="pas"/>
<pin name="E2" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="V2" direction="pas"/>
<pin name="U2" direction="pas"/>
<pin name="T2" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="P2" direction="pas"/>
<pin name="N2" direction="pas"/>
<pin name="M2" direction="pas"/>
</symbol>
<symbol name="PAS">
<pin name="P$2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M101" prefix="M101_">
<description>&lt;qt&gt;&lt;b&gt;Bus Data Interface&lt;/b&gt;
&lt;p&gt;
The M101 contains 15 two-input NAND gates.  One input of each gate is tied to a common line so that all data signals can be enabled simultaneously.  &lt;p&gt;Each data signal presents one TTL load.  The common input presents 15 loads. &lt;p&gt; Each output can drive 10 loads.&lt;p&gt;
Power: 5V@82ma (max.)
&lt;/qt&gt;</description>
<gates>
<gate name="E1" symbol="NAND1"/>
<gate name="H1" symbol="NAND1"/>
<gate name="K1" symbol="NAND1"/>
<gate name="M1" symbol="NAND1"/>
<gate name="P1" symbol="NAND1"/>
<gate name="S1" symbol="NAND1"/>
<gate name="U1" symbol="NAND1"/>
<gate name="F2" symbol="NAND1"/>
<gate name="J2" symbol="NAND1"/>
<gate name="L2" symbol="NAND1"/>
<gate name="N2" symbol="NAND1"/>
<gate name="R2" symbol="NAND1"/>
<gate name="T2" symbol="NAND1"/>
<gate name="V2" symbol="NAND1"/>
<gate name="G$16" symbol="POWER"/>
<gate name="B1" symbol="NAND2"/>
<gate name="G$1" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="B1" pin="IN1" pad="A1"/>
<connect gate="B1" pin="IN2" pad="C1"/>
<connect gate="B1" pin="OUT" pad="B1"/>
<connect gate="E1" pin="IN" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="F2" pin="IN" pad="E2"/>
<connect gate="F2" pin="OUT" pad="F2"/>
<connect gate="G$1" pin="GND" pad="T1"/>
<connect gate="G$16" pin="GND" pad="C2"/>
<connect gate="G$16" pin="VCC" pad="A2"/>
<connect gate="H1" pin="IN" pad="F1"/>
<connect gate="H1" pin="OUT" pad="H1"/>
<connect gate="J2" pin="IN" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="K1" pin="IN" pad="J1"/>
<connect gate="K1" pin="OUT" pad="K1"/>
<connect gate="L2" pin="IN" pad="K2"/>
<connect gate="L2" pin="OUT" pad="L2"/>
<connect gate="M1" pin="IN" pad="L1"/>
<connect gate="M1" pin="OUT" pad="M1"/>
<connect gate="N2" pin="IN" pad="M2"/>
<connect gate="N2" pin="OUT" pad="N2"/>
<connect gate="P1" pin="IN" pad="N1"/>
<connect gate="P1" pin="OUT" pad="P1"/>
<connect gate="R2" pin="IN" pad="P2"/>
<connect gate="R2" pin="OUT" pad="R2"/>
<connect gate="S1" pin="IN" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="T2" pin="IN" pad="S2"/>
<connect gate="T2" pin="OUT" pad="T2"/>
<connect gate="U1" pin="IN" pad="V1"/>
<connect gate="U1" pin="OUT" pad="U1"/>
<connect gate="V2" pin="IN" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M101-ARRAY" prefix="M101_">
<description>M101 Bus Data Interface</description>
<gates>
<gate name="G$1" symbol="M101A"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="ENABLE" pad="C1"/>
<connect gate="G$1" pin="IN1" pad="A1"/>
<connect gate="G$1" pin="IN10" pad="H2"/>
<connect gate="G$1" pin="IN11" pad="K2"/>
<connect gate="G$1" pin="IN12" pad="M2"/>
<connect gate="G$1" pin="IN13" pad="P2"/>
<connect gate="G$1" pin="IN14" pad="S2"/>
<connect gate="G$1" pin="IN15" pad="U2"/>
<connect gate="G$1" pin="IN2" pad="D1"/>
<connect gate="G$1" pin="IN3" pad="F1"/>
<connect gate="G$1" pin="IN4" pad="J1"/>
<connect gate="G$1" pin="IN5" pad="L1"/>
<connect gate="G$1" pin="IN6" pad="N1"/>
<connect gate="G$1" pin="IN7" pad="R1"/>
<connect gate="G$1" pin="IN8" pad="V1"/>
<connect gate="G$1" pin="IN9" pad="E2"/>
<connect gate="G$1" pin="O1" pad="B1"/>
<connect gate="G$1" pin="O10" pad="J2"/>
<connect gate="G$1" pin="O11" pad="L2"/>
<connect gate="G$1" pin="O12" pad="N2"/>
<connect gate="G$1" pin="O13" pad="R2"/>
<connect gate="G$1" pin="O14" pad="T2"/>
<connect gate="G$1" pin="O15" pad="V2"/>
<connect gate="G$1" pin="O2" pad="E1"/>
<connect gate="G$1" pin="O3" pad="H1"/>
<connect gate="G$1" pin="O4" pad="K1"/>
<connect gate="G$1" pin="O5" pad="M1"/>
<connect gate="G$1" pin="O6" pad="P1"/>
<connect gate="G$1" pin="O7" pad="S1"/>
<connect gate="G$1" pin="O8" pad="U1"/>
<connect gate="G$1" pin="O9" pad="F2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M103" prefix="M103_">
<description>M103 Device Selector
&lt;p&gt;Used to decode IOT requests.</description>
<gates>
<gate name="K1" symbol="NAND2"/>
<gate name="N1" symbol="NAND2"/>
<gate name="V2" symbol="M103A"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="V1" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
<connect gate="K1" pin="IN1" pad="H1"/>
<connect gate="K1" pin="IN2" pad="J1"/>
<connect gate="K1" pin="OUT" pad="K1"/>
<connect gate="N1" pin="IN1" pad="L1"/>
<connect gate="N1" pin="IN2" pad="M1"/>
<connect gate="N1" pin="OUT" pad="N1"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="A1" pad="A1"/>
<connect gate="V2" pin="B1" pad="B1"/>
<connect gate="V2" pin="C1" pad="C1"/>
<connect gate="V2" pin="D1" pad="D1"/>
<connect gate="V2" pin="D2" pad="D2"/>
<connect gate="V2" pin="E1" pad="E1"/>
<connect gate="V2" pin="E2" pad="E2"/>
<connect gate="V2" pin="F1" pad="F1"/>
<connect gate="V2" pin="F2" pad="F2"/>
<connect gate="V2" pin="H2" pad="H2"/>
<connect gate="V2" pin="J2" pad="J2"/>
<connect gate="V2" pin="K2" pad="K2"/>
<connect gate="V2" pin="L2" pad="L2"/>
<connect gate="V2" pin="N2" pad="N2"/>
<connect gate="V2" pin="P2" pad="P2"/>
<connect gate="V2" pin="R2" pad="R2"/>
<connect gate="V2" pin="S2" pad="S2"/>
<connect gate="V2" pin="U2" pad="U2"/>
<connect gate="V2" pin="V2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M111" prefix="M111_">
<description>Sixteen inverters.</description>
<gates>
<gate name="G$17" symbol="POWER"/>
<gate name="G$1" symbol="T1GND"/>
<gate name="B1" symbol="INVERTER-P"/>
<gate name="D2" symbol="INVERTER-P"/>
<gate name="E1" symbol="INVERTER-P"/>
<gate name="H1" symbol="INVERTER-P"/>
<gate name="F2" symbol="INVERTER-P"/>
<gate name="K1" symbol="INVERTER-P"/>
<gate name="J2" symbol="INVERTER-P"/>
<gate name="M1" symbol="INVERTER-P"/>
<gate name="L2" symbol="INVERTER-P"/>
<gate name="P1" symbol="INVERTER-P"/>
<gate name="N2" symbol="INVERTER-P"/>
<gate name="S1" symbol="INVERTER-P"/>
<gate name="R2" symbol="INVERTER-P"/>
<gate name="U1" symbol="INVERTER-P"/>
<gate name="T2" symbol="INVERTER-P"/>
<gate name="V2" symbol="INVERTER-P"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="B1" pin="IN" pad="A1"/>
<connect gate="B1" pin="OUT" pad="B1"/>
<connect gate="D2" pin="IN" pad="C1"/>
<connect gate="D2" pin="OUT" pad="D2"/>
<connect gate="E1" pin="IN" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="F2" pin="IN" pad="E2"/>
<connect gate="F2" pin="OUT" pad="F2"/>
<connect gate="G$1" pin="GND" pad="T1"/>
<connect gate="G$17" pin="GND" pad="C2"/>
<connect gate="G$17" pin="VCC" pad="A2"/>
<connect gate="H1" pin="IN" pad="F1"/>
<connect gate="H1" pin="OUT" pad="H1"/>
<connect gate="J2" pin="IN" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="K1" pin="IN" pad="J1"/>
<connect gate="K1" pin="OUT" pad="K1"/>
<connect gate="L2" pin="IN" pad="K2"/>
<connect gate="L2" pin="OUT" pad="L2"/>
<connect gate="M1" pin="IN" pad="L1"/>
<connect gate="M1" pin="OUT" pad="M1"/>
<connect gate="N2" pin="IN" pad="M2"/>
<connect gate="N2" pin="OUT" pad="N2"/>
<connect gate="P1" pin="IN" pad="N1"/>
<connect gate="P1" pin="OUT" pad="P1"/>
<connect gate="R2" pin="IN" pad="P2"/>
<connect gate="R2" pin="OUT" pad="R2"/>
<connect gate="S1" pin="IN" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="T2" pin="IN" pad="S2"/>
<connect gate="T2" pin="OUT" pad="T2"/>
<connect gate="U1" pin="IN" pad="V1"/>
<connect gate="U1" pin="OUT" pad="U1"/>
<connect gate="V2" pin="IN" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M113" prefix="M113_">
<description>10 2-input NAND Gates</description>
<gates>
<gate name="C1" symbol="NAND2"/>
<gate name="F1" symbol="NAND2"/>
<gate name="F2" symbol="NAND2"/>
<gate name="K1" symbol="NAND2"/>
<gate name="K2" symbol="NAND2"/>
<gate name="N1" symbol="NAND2"/>
<gate name="N2" symbol="NAND2"/>
<gate name="S1" symbol="NAND2"/>
<gate name="S2" symbol="NAND2"/>
<gate name="V2" symbol="NAND2"/>
<gate name="G$11" symbol="POWER"/>
<gate name="G$12" symbol="T1GND"/>
<gate name="U1" symbol="PULL-UP"/>
<gate name="V1" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="C1" pin="IN1" pad="A1"/>
<connect gate="C1" pin="IN2" pad="B1"/>
<connect gate="C1" pin="OUT" pad="C1"/>
<connect gate="F1" pin="IN1" pad="D1"/>
<connect gate="F1" pin="IN2" pad="E1"/>
<connect gate="F1" pin="OUT" pad="F1"/>
<connect gate="F2" pin="IN1" pad="D2"/>
<connect gate="F2" pin="IN2" pad="E2"/>
<connect gate="F2" pin="OUT" pad="F2"/>
<connect gate="G$11" pin="GND" pad="C2"/>
<connect gate="G$11" pin="VCC" pad="A2"/>
<connect gate="G$12" pin="GND" pad="T1"/>
<connect gate="K1" pin="IN1" pad="H1"/>
<connect gate="K1" pin="IN2" pad="J1"/>
<connect gate="K1" pin="OUT" pad="K1"/>
<connect gate="K2" pin="IN1" pad="H2"/>
<connect gate="K2" pin="IN2" pad="J2"/>
<connect gate="K2" pin="OUT" pad="K2"/>
<connect gate="N1" pin="IN1" pad="L1"/>
<connect gate="N1" pin="IN2" pad="M1"/>
<connect gate="N1" pin="OUT" pad="N1"/>
<connect gate="N2" pin="IN1" pad="L2"/>
<connect gate="N2" pin="IN2" pad="M2"/>
<connect gate="N2" pin="OUT" pad="N2"/>
<connect gate="S1" pin="IN1" pad="P1"/>
<connect gate="S1" pin="IN2" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="S2" pin="IN1" pad="P2"/>
<connect gate="S2" pin="IN2" pad="R2"/>
<connect gate="S2" pin="OUT" pad="S2"/>
<connect gate="U1" pin="P$1" pad="U1"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="IN1" pad="T2"/>
<connect gate="V2" pin="IN2" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M115" prefix="M115_">
<description>8 3-input NAND Gates</description>
<gates>
<gate name="D1" symbol="NAND3"/>
<gate name="J1" symbol="NAND3"/>
<gate name="N1" symbol="NAND3"/>
<gate name="U1" symbol="NAND3"/>
<gate name="H2" symbol="NAND3"/>
<gate name="M2" symbol="NAND3"/>
<gate name="S2" symbol="NAND3"/>
<gate name="V1" symbol="NAND3"/>
<gate name="G$9" symbol="POWER"/>
<gate name="G$10" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D1" pin="IN1" pad="A1"/>
<connect gate="D1" pin="IN2" pad="B1"/>
<connect gate="D1" pin="IN3" pad="C1"/>
<connect gate="D1" pin="OUT" pad="D1"/>
<connect gate="G$10" pin="GND" pad="T1"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="H2" pin="IN1" pad="D2"/>
<connect gate="H2" pin="IN2" pad="E2"/>
<connect gate="H2" pin="IN3" pad="F2"/>
<connect gate="H2" pin="OUT" pad="H2"/>
<connect gate="J1" pin="IN1" pad="E1"/>
<connect gate="J1" pin="IN2" pad="F1"/>
<connect gate="J1" pin="IN3" pad="H1"/>
<connect gate="J1" pin="OUT" pad="J1"/>
<connect gate="M2" pin="IN1" pad="J2"/>
<connect gate="M2" pin="IN2" pad="K2"/>
<connect gate="M2" pin="IN3" pad="L2"/>
<connect gate="M2" pin="OUT" pad="M2"/>
<connect gate="N1" pin="IN1" pad="K1"/>
<connect gate="N1" pin="IN2" pad="L1"/>
<connect gate="N1" pin="IN3" pad="M1"/>
<connect gate="N1" pin="OUT" pad="N1"/>
<connect gate="S2" pin="IN1" pad="N2"/>
<connect gate="S2" pin="IN2" pad="P2"/>
<connect gate="S2" pin="IN3" pad="R2"/>
<connect gate="S2" pin="OUT" pad="S2"/>
<connect gate="U1" pin="IN1" pad="P1"/>
<connect gate="U1" pin="IN2" pad="R1"/>
<connect gate="U1" pin="IN3" pad="S1"/>
<connect gate="U1" pin="OUT" pad="U1"/>
<connect gate="V1" pin="IN1" pad="T2"/>
<connect gate="V1" pin="IN2" pad="U2"/>
<connect gate="V1" pin="IN3" pad="V2"/>
<connect gate="V1" pin="OUT" pad="V1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M117" prefix="M117_">
<description>6 4-input NAND Gates</description>
<gates>
<gate name="E1" symbol="NAND4"/>
<gate name="L1" symbol="NAND4"/>
<gate name="S1" symbol="NAND4"/>
<gate name="J2" symbol="NAND4"/>
<gate name="P2" symbol="NAND4"/>
<gate name="V2" symbol="NAND4"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="U1" symbol="PULL-UP"/>
<gate name="V1" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="IN1" pad="A1"/>
<connect gate="E1" pin="IN2" pad="B1"/>
<connect gate="E1" pin="IN3" pad="C1"/>
<connect gate="E1" pin="IN4" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="J2" pin="IN1" pad="D2"/>
<connect gate="J2" pin="IN2" pad="E2"/>
<connect gate="J2" pin="IN3" pad="F2"/>
<connect gate="J2" pin="IN4" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="L1" pin="IN1" pad="F1"/>
<connect gate="L1" pin="IN2" pad="H1"/>
<connect gate="L1" pin="IN3" pad="J1"/>
<connect gate="L1" pin="IN4" pad="K1"/>
<connect gate="L1" pin="OUT" pad="L1"/>
<connect gate="P2" pin="IN1" pad="K2"/>
<connect gate="P2" pin="IN2" pad="L2"/>
<connect gate="P2" pin="IN3" pad="M2"/>
<connect gate="P2" pin="IN4" pad="N2"/>
<connect gate="P2" pin="OUT" pad="P2"/>
<connect gate="S1" pin="IN1" pad="M1"/>
<connect gate="S1" pin="IN2" pad="N1"/>
<connect gate="S1" pin="IN3" pad="P1"/>
<connect gate="S1" pin="IN4" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="U1" pin="P$1" pad="U1"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="IN1" pad="R2"/>
<connect gate="V2" pin="IN2" pad="S2"/>
<connect gate="V2" pin="IN3" pad="T2"/>
<connect gate="V2" pin="IN4" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M119" prefix="M119_">
<description>3 8-input NAND Gates</description>
<gates>
<gate name="J2" symbol="NAND8"/>
<gate name="P2" symbol="NAND8"/>
<gate name="V2" symbol="NAND8"/>
<gate name="G$4" symbol="POWER"/>
<gate name="G$5" symbol="T1GND"/>
<gate name="U1" symbol="PULL-UP"/>
<gate name="V1" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="GND" pad="T1"/>
<connect gate="J2" pin="IN1" pad="A1"/>
<connect gate="J2" pin="IN2" pad="B1"/>
<connect gate="J2" pin="IN3" pad="C1"/>
<connect gate="J2" pin="IN4" pad="D1"/>
<connect gate="J2" pin="IN5" pad="D2"/>
<connect gate="J2" pin="IN6" pad="E2"/>
<connect gate="J2" pin="IN7" pad="F2"/>
<connect gate="J2" pin="IN8" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="P2" pin="IN1" pad="F1"/>
<connect gate="P2" pin="IN2" pad="H1"/>
<connect gate="P2" pin="IN3" pad="J1"/>
<connect gate="P2" pin="IN4" pad="K1"/>
<connect gate="P2" pin="IN5" pad="K2"/>
<connect gate="P2" pin="IN6" pad="L2"/>
<connect gate="P2" pin="IN7" pad="M2"/>
<connect gate="P2" pin="IN8" pad="N2"/>
<connect gate="P2" pin="OUT" pad="P2"/>
<connect gate="U1" pin="P$1" pad="U1"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="IN1" pad="M1"/>
<connect gate="V2" pin="IN2" pad="N1"/>
<connect gate="V2" pin="IN3" pad="P1"/>
<connect gate="V2" pin="IN4" pad="R1"/>
<connect gate="V2" pin="IN5" pad="R2"/>
<connect gate="V2" pin="IN6" pad="S2"/>
<connect gate="V2" pin="IN7" pad="T2"/>
<connect gate="V2" pin="IN8" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M121" prefix="M121_">
<description>6 2-2 AND-NOR Gates</description>
<gates>
<gate name="E1" symbol="AND-NOR"/>
<gate name="L1" symbol="AND-NOR"/>
<gate name="S1" symbol="AND-NOR"/>
<gate name="J2" symbol="AND-NOR"/>
<gate name="P2" symbol="AND-NOR"/>
<gate name="V2" symbol="AND-NOR"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="U1" symbol="PULL-UP"/>
<gate name="V1" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="IN1A" pad="A1"/>
<connect gate="E1" pin="IN1B" pad="B1"/>
<connect gate="E1" pin="IN2A" pad="C1"/>
<connect gate="E1" pin="IN2B" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="J2" pin="IN1A" pad="D2"/>
<connect gate="J2" pin="IN1B" pad="E2"/>
<connect gate="J2" pin="IN2A" pad="F2"/>
<connect gate="J2" pin="IN2B" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="L1" pin="IN1A" pad="F1"/>
<connect gate="L1" pin="IN1B" pad="H1"/>
<connect gate="L1" pin="IN2A" pad="J1"/>
<connect gate="L1" pin="IN2B" pad="K1"/>
<connect gate="L1" pin="OUT" pad="L1"/>
<connect gate="P2" pin="IN1A" pad="K2"/>
<connect gate="P2" pin="IN1B" pad="L2"/>
<connect gate="P2" pin="IN2A" pad="M2"/>
<connect gate="P2" pin="IN2B" pad="N2"/>
<connect gate="P2" pin="OUT" pad="P2"/>
<connect gate="S1" pin="IN1A" pad="M1"/>
<connect gate="S1" pin="IN1B" pad="N1"/>
<connect gate="S1" pin="IN2A" pad="P1"/>
<connect gate="S1" pin="IN2B" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="U1" pin="P$1" pad="U1"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="IN1A" pad="R2"/>
<connect gate="V2" pin="IN1B" pad="S2"/>
<connect gate="V2" pin="IN2A" pad="T2"/>
<connect gate="V2" pin="IN2B" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M161" prefix="M161_">
<description>Octal or Decimal Decoder</description>
<gates>
<gate name="G$1" symbol="M161"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="!O0" pad="D1"/>
<connect gate="G$1" pin="!O1" pad="E1"/>
<connect gate="G$1" pin="!O2" pad="J1"/>
<connect gate="G$1" pin="!O3" pad="N1"/>
<connect gate="G$1" pin="!O4" pad="F1"/>
<connect gate="G$1" pin="!O5" pad="M1"/>
<connect gate="G$1" pin="!O6" pad="H1"/>
<connect gate="G$1" pin="!O7" pad="L1"/>
<connect gate="G$1" pin="!O8" pad="P1"/>
<connect gate="G$1" pin="!O9" pad="R1"/>
<connect gate="G$1" pin="EN1" pad="S2"/>
<connect gate="G$1" pin="EN2" pad="S1"/>
<connect gate="G$1" pin="EN3" pad="T2"/>
<connect gate="G$1" pin="IN*" pad="U1"/>
<connect gate="G$1" pin="IN0" pad="V1"/>
<connect gate="G$1" pin="IN1" pad="U2"/>
<connect gate="G$1" pin="IN2" pad="V2"/>
<connect gate="G$1" pin="O0" pad="D2"/>
<connect gate="G$1" pin="O1" pad="E2"/>
<connect gate="G$1" pin="O2" pad="J2"/>
<connect gate="G$1" pin="O3" pad="N2"/>
<connect gate="G$1" pin="O4" pad="F2"/>
<connect gate="G$1" pin="O5" pad="M2"/>
<connect gate="G$1" pin="O6" pad="H2"/>
<connect gate="G$1" pin="O7" pad="L2"/>
<connect gate="G$1" pin="O8" pad="P2"/>
<connect gate="G$1" pin="O9" pad="R2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M206" prefix="M206_">
<description>6 D flip-flops</description>
<gates>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="G$1" symbol="M206A"/>
<gate name="G$2" symbol="JUMP-DOWN"/>
<gate name="G$3" symbol="JUMP-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="F1" pad="F1"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="H1" pad="H1"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="J1" pad="J1"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K1" pad="K1"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N1" pad="N1"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="U1" pad="U1"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="G$1" pin="V1" pad="V1"/>
<connect gate="G$1" pin="V2" pad="V2"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M302" prefix="M302_">
<description>Dual one-shot</description>
<gates>
<gate name="F2" symbol="M302A"/>
<gate name="T2" symbol="M302A"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="F2" pin="D1" pad="D1"/>
<connect gate="F2" pin="D2" pad="D2"/>
<connect gate="F2" pin="E1" pad="E1"/>
<connect gate="F2" pin="E2" pad="E2"/>
<connect gate="F2" pin="F1" pad="F1"/>
<connect gate="F2" pin="F2" pad="F2"/>
<connect gate="F2" pin="H1" pad="H1"/>
<connect gate="F2" pin="H2" pad="H2"/>
<connect gate="F2" pin="J1" pad="J1"/>
<connect gate="F2" pin="J2" pad="J2"/>
<connect gate="F2" pin="K2" pad="K2"/>
<connect gate="F2" pin="L2" pad="L2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="GND" pad="T1"/>
<connect gate="T2" pin="D1" pad="N1"/>
<connect gate="T2" pin="D2" pad="V2"/>
<connect gate="T2" pin="E1" pad="P1"/>
<connect gate="T2" pin="E2" pad="R2"/>
<connect gate="T2" pin="F1" pad="R1"/>
<connect gate="T2" pin="F2" pad="T2"/>
<connect gate="T2" pin="H1" pad="S1"/>
<connect gate="T2" pin="H2" pad="M2"/>
<connect gate="T2" pin="J1" pad="U1"/>
<connect gate="T2" pin="J2" pad="N2"/>
<connect gate="T2" pin="K2" pad="P2"/>
<connect gate="T2" pin="L2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M228" prefix="M228_">
<description>Mark Track Decoder</description>
<gates>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="POWER"/>
<gate name="G$1" symbol="M228A"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF1" pad="AF1"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH1" pad="AH1"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AK2" pad="AK2"/>
<connect gate="G$1" pin="AL1" pad="AL1"/>
<connect gate="G$1" pin="AM1" pad="AM1"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN1" pad="AN1"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="AU1" pad="AU1"/>
<connect gate="G$1" pin="AU2" pad="AU2"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="BC1" pad="BC1"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BF1" pad="BF1"/>
<connect gate="G$1" pin="BF2" pad="BF2"/>
<connect gate="G$1" pin="BH1" pad="BH1"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BL2" pad="BL2"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$1" pin="BN2" pad="BN2"/>
<connect gate="G$1" pin="BP2" pad="BP2"/>
<connect gate="G$1" pin="BR1" pad="BR1"/>
<connect gate="G$1" pin="BR2" pad="BR2"/>
<connect gate="G$1" pin="BS1" pad="BS1"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$1" pin="BT2" pad="BT2"/>
<connect gate="G$1" pin="BU1" pad="BU1"/>
<connect gate="G$1" pin="BU2" pad="BU2"/>
<connect gate="G$1" pin="BV1" pad="BV1"/>
<connect gate="G$1" pin="BV2" pad="BV2"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="AT1"/>
<connect gate="G$4" pin="GND" pad="BT1"/>
<connect gate="G$5" pin="GND" pad="BC2"/>
<connect gate="G$5" pin="VCC" pad="BA2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M207" prefix="M207_">
<description>6 J-K flip-flops</description>
<gates>
<gate name="G$1" symbol="M207A"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="G$4" symbol="JUMP-DOWN"/>
<gate name="G$5" symbol="JUMP-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="F1" pad="F1"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="H1" pad="H1"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="J1" pad="J1"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K1" pad="K1"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N1" pad="N1"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="U1" pad="U1"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="G$1" pin="V1" pad="V1"/>
<connect gate="G$1" pin="V2" pad="V2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M307" prefix="M307_">
<description>Dual Integrating One-Shot</description>
<gates>
<gate name="H2" symbol="M307A"/>
<gate name="K1" symbol="M307A"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="-15V"/>
<gate name="R1" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="GND" pad="T1"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
<connect gate="H2" pin="F2" pad="F2"/>
<connect gate="H2" pin="H2" pad="H2"/>
<connect gate="H2" pin="M1" pad="M1"/>
<connect gate="H2" pin="M2" pad="M2"/>
<connect gate="H2" pin="N1" pad="N1"/>
<connect gate="H2" pin="N2" pad="N2"/>
<connect gate="H2" pin="P1" pad="P1"/>
<connect gate="H2" pin="P2" pad="P2"/>
<connect gate="H2" pin="R2" pad="R2"/>
<connect gate="H2" pin="S1" pad="S1"/>
<connect gate="H2" pin="S2" pad="S2"/>
<connect gate="H2" pin="U1" pad="U1"/>
<connect gate="H2" pin="U2" pad="U2"/>
<connect gate="H2" pin="V1" pad="V1"/>
<connect gate="H2" pin="V2" pad="V2"/>
<connect gate="K1" pin="F2" pad="E2"/>
<connect gate="K1" pin="H2" pad="K1"/>
<connect gate="K1" pin="M1" pad="L1"/>
<connect gate="K1" pin="M2" pad="D2"/>
<connect gate="K1" pin="N1" pad="J2"/>
<connect gate="K1" pin="N2" pad="J1"/>
<connect gate="K1" pin="P1" pad="C1"/>
<connect gate="K1" pin="P2" pad="H1"/>
<connect gate="K1" pin="R2" pad="F1"/>
<connect gate="K1" pin="S1" pad="L2"/>
<connect gate="K1" pin="S2" pad="E1"/>
<connect gate="K1" pin="U1" pad="K2"/>
<connect gate="K1" pin="U2" pad="D1"/>
<connect gate="K1" pin="V1" pad="A1"/>
<connect gate="K1" pin="V2" pad="B1"/>
<connect gate="R1" pin="P$1" pad="R1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M401" prefix="M401_">
<description>Variable Clock</description>
<gates>
<gate name="E2" symbol="M401A"/>
<gate name="G$2" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E2" pin="D2" pad="D2"/>
<connect gate="E2" pin="E2" pad="E2"/>
<connect gate="E2" pin="J2" pad="J2"/>
<connect gate="E2" pin="K2" pad="K2"/>
<connect gate="E2" pin="M2" pad="M2"/>
<connect gate="E2" pin="N2" pad="N2"/>
<connect gate="E2" pin="P2" pad="P2"/>
<connect gate="E2" pin="R2" pad="R2"/>
<connect gate="E2" pin="S2" pad="S2"/>
<connect gate="E2" pin="T2" pad="T2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="E2" pin="D2" pad="D2"/>
<connect gate="E2" pin="E2" pad="E2"/>
<connect gate="E2" pin="J2" pad="J2"/>
<connect gate="E2" pin="K2" pad="K2"/>
<connect gate="E2" pin="M2" pad="M2"/>
<connect gate="E2" pin="N2" pad="N2"/>
<connect gate="E2" pin="P2" pad="P2"/>
<connect gate="E2" pin="R2" pad="R2"/>
<connect gate="E2" pin="S2" pad="S2"/>
<connect gate="E2" pin="T2" pad="T2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="E2" pin="D2" pad="D2"/>
<connect gate="E2" pin="E2" pad="E2"/>
<connect gate="E2" pin="J2" pad="J2"/>
<connect gate="E2" pin="K2" pad="K2"/>
<connect gate="E2" pin="M2" pad="M2"/>
<connect gate="E2" pin="N2" pad="N2"/>
<connect gate="E2" pin="P2" pad="P2"/>
<connect gate="E2" pin="R2" pad="R2"/>
<connect gate="E2" pin="S2" pad="S2"/>
<connect gate="E2" pin="T2" pad="T2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M502" prefix="M502_">
<description>Dual Negative Input Converter</description>
<gates>
<gate name="D2" symbol="M502A"/>
<gate name="R2" symbol="M502A"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D2" pin="D2" pad="D2"/>
<connect gate="D2" pin="E2" pad="E2"/>
<connect gate="D2" pin="H2" pad="H2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="GND" pad="M2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
<connect gate="R2" pin="D2" pad="R2"/>
<connect gate="R2" pin="E2" pad="P2"/>
<connect gate="R2" pin="H2" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D2" pin="D2" pad="D2"/>
<connect gate="D2" pin="E2" pad="E2"/>
<connect gate="D2" pin="H2" pad="H2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="GND" pad="M2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
<connect gate="R2" pin="D2" pad="R2"/>
<connect gate="R2" pin="E2" pad="P2"/>
<connect gate="R2" pin="H2" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D2" pin="D2" pad="D2"/>
<connect gate="D2" pin="E2" pad="E2"/>
<connect gate="D2" pin="H2" pad="H2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="GND" pad="M2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
<connect gate="R2" pin="D2" pad="R2"/>
<connect gate="R2" pin="E2" pad="P2"/>
<connect gate="R2" pin="H2" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M602" prefix="M602_">
<description>Dual Pulse Amplifier</description>
<gates>
<gate name="F" symbol="M602A"/>
<gate name="L" symbol="M602A"/>
<gate name="G$3" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="F" pin="D2" pad="D2"/>
<connect gate="F" pin="E2" pad="E2"/>
<connect gate="F" pin="F2" pad="F2"/>
<connect gate="F" pin="H2" pad="H2"/>
<connect gate="F" pin="J2" pad="J2"/>
<connect gate="F" pin="K2" pad="K2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="L" pin="D2" pad="S2"/>
<connect gate="L" pin="E2" pad="R2"/>
<connect gate="L" pin="F2" pad="L2"/>
<connect gate="L" pin="H2" pad="P2"/>
<connect gate="L" pin="J2" pad="N2"/>
<connect gate="L" pin="K2" pad="M2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="F" pin="D2" pad="D2"/>
<connect gate="F" pin="E2" pad="E2"/>
<connect gate="F" pin="F2" pad="F2"/>
<connect gate="F" pin="H2" pad="H2"/>
<connect gate="F" pin="J2" pad="J2"/>
<connect gate="F" pin="K2" pad="K2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="L" pin="D2" pad="S2"/>
<connect gate="L" pin="E2" pad="R2"/>
<connect gate="L" pin="F2" pad="L2"/>
<connect gate="L" pin="H2" pad="P2"/>
<connect gate="L" pin="J2" pad="N2"/>
<connect gate="L" pin="K2" pad="M2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="F" pin="D2" pad="D2"/>
<connect gate="F" pin="E2" pad="E2"/>
<connect gate="F" pin="F2" pad="F2"/>
<connect gate="F" pin="H2" pad="H2"/>
<connect gate="F" pin="J2" pad="J2"/>
<connect gate="F" pin="K2" pad="K2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="L" pin="D2" pad="S2"/>
<connect gate="L" pin="E2" pad="R2"/>
<connect gate="L" pin="F2" pad="L2"/>
<connect gate="L" pin="H2" pad="P2"/>
<connect gate="L" pin="J2" pad="N2"/>
<connect gate="L" pin="K2" pad="M2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M627" prefix="M627_">
<description>6 4-input NAND Power Amplifier</description>
<gates>
<gate name="E1" symbol="NAND4"/>
<gate name="L1" symbol="NAND4"/>
<gate name="S1" symbol="NAND4"/>
<gate name="J2" symbol="NAND4"/>
<gate name="P2" symbol="NAND4"/>
<gate name="V2" symbol="NAND4"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="U1" symbol="PULL-UP"/>
<gate name="V1" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="IN1" pad="A1"/>
<connect gate="E1" pin="IN2" pad="B1"/>
<connect gate="E1" pin="IN3" pad="C1"/>
<connect gate="E1" pin="IN4" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="J2" pin="IN1" pad="D2"/>
<connect gate="J2" pin="IN2" pad="E2"/>
<connect gate="J2" pin="IN3" pad="F2"/>
<connect gate="J2" pin="IN4" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="L1" pin="IN1" pad="F1"/>
<connect gate="L1" pin="IN2" pad="H1"/>
<connect gate="L1" pin="IN3" pad="J1"/>
<connect gate="L1" pin="IN4" pad="K1"/>
<connect gate="L1" pin="OUT" pad="L1"/>
<connect gate="P2" pin="IN1" pad="K2"/>
<connect gate="P2" pin="IN2" pad="L2"/>
<connect gate="P2" pin="IN3" pad="M2"/>
<connect gate="P2" pin="IN4" pad="N2"/>
<connect gate="P2" pin="OUT" pad="P2"/>
<connect gate="S1" pin="IN1" pad="M1"/>
<connect gate="S1" pin="IN2" pad="N1"/>
<connect gate="S1" pin="IN3" pad="P1"/>
<connect gate="S1" pin="IN4" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="U1" pin="P$1" pad="U1"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="IN1" pad="R2"/>
<connect gate="V2" pin="IN2" pad="S2"/>
<connect gate="V2" pin="IN3" pad="T2"/>
<connect gate="V2" pin="IN4" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M623" prefix="M623_">
<description>6 Dual Bus Drivers</description>
<gates>
<gate name="D1" symbol="M623A"/>
<gate name="K1" symbol="M623A"/>
<gate name="R1" symbol="M623A"/>
<gate name="H2" symbol="M623A"/>
<gate name="N2" symbol="M623A"/>
<gate name="U2" symbol="M623A"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="G$9" symbol="T1GND"/>
<gate name="G$10" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D1" pin="A" pad="A1"/>
<connect gate="D1" pin="B" pad="B1"/>
<connect gate="D1" pin="C" pad="C1"/>
<connect gate="D1" pin="D" pad="D1"/>
<connect gate="D1" pin="E" pad="E1"/>
<connect gate="G$10" pin="GND" pad="V1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="G$9" pin="GND" pad="U1"/>
<connect gate="H2" pin="A" pad="D2"/>
<connect gate="H2" pin="B" pad="E2"/>
<connect gate="H2" pin="C" pad="F2"/>
<connect gate="H2" pin="D" pad="H2"/>
<connect gate="H2" pin="E" pad="J2"/>
<connect gate="K1" pin="A" pad="F1"/>
<connect gate="K1" pin="B" pad="H1"/>
<connect gate="K1" pin="C" pad="J1"/>
<connect gate="K1" pin="D" pad="K1"/>
<connect gate="K1" pin="E" pad="L1"/>
<connect gate="N2" pin="A" pad="K2"/>
<connect gate="N2" pin="B" pad="L2"/>
<connect gate="N2" pin="C" pad="M2"/>
<connect gate="N2" pin="D" pad="N2"/>
<connect gate="N2" pin="E" pad="P2"/>
<connect gate="R1" pin="A" pad="M1"/>
<connect gate="R1" pin="B" pad="N1"/>
<connect gate="R1" pin="C" pad="P1"/>
<connect gate="R1" pin="D" pad="R1"/>
<connect gate="R1" pin="E" pad="S1"/>
<connect gate="U2" pin="A" pad="R2"/>
<connect gate="U2" pin="B" pad="S2"/>
<connect gate="U2" pin="C" pad="T2"/>
<connect gate="U2" pin="D" pad="U2"/>
<connect gate="U2" pin="E" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M633" prefix="M633_">
<description>6 Dual Negative Bus Drivers</description>
<gates>
<gate name="D1" symbol="M633A"/>
<gate name="K1" symbol="M633A"/>
<gate name="R1" symbol="M633A"/>
<gate name="H2" symbol="M633A"/>
<gate name="N2" symbol="M633A"/>
<gate name="U2" symbol="M633A"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="-15V"/>
<gate name="G$9" symbol="T1GND"/>
<gate name="G$10" symbol="T1GND"/>
<gate name="G$11" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D1" pin="A" pad="A1"/>
<connect gate="D1" pin="B" pad="B1"/>
<connect gate="D1" pin="C" pad="C1"/>
<connect gate="D1" pin="D" pad="D1"/>
<connect gate="D1" pin="E" pad="E1"/>
<connect gate="G$10" pin="GND" pad="U1"/>
<connect gate="G$11" pin="GND" pad="V1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="T1"/>
<connect gate="H2" pin="A" pad="D2"/>
<connect gate="H2" pin="B" pad="E2"/>
<connect gate="H2" pin="C" pad="F2"/>
<connect gate="H2" pin="D" pad="H2"/>
<connect gate="H2" pin="E" pad="J2"/>
<connect gate="K1" pin="A" pad="F1"/>
<connect gate="K1" pin="B" pad="H1"/>
<connect gate="K1" pin="C" pad="J1"/>
<connect gate="K1" pin="D" pad="K1"/>
<connect gate="K1" pin="E" pad="L1"/>
<connect gate="N2" pin="A" pad="K2"/>
<connect gate="N2" pin="B" pad="L2"/>
<connect gate="N2" pin="C" pad="M2"/>
<connect gate="N2" pin="D" pad="N2"/>
<connect gate="N2" pin="E" pad="P2"/>
<connect gate="R1" pin="A" pad="M1"/>
<connect gate="R1" pin="B" pad="N1"/>
<connect gate="R1" pin="C" pad="P1"/>
<connect gate="R1" pin="D" pad="R1"/>
<connect gate="R1" pin="E" pad="S1"/>
<connect gate="U2" pin="A" pad="R2"/>
<connect gate="U2" pin="B" pad="S2"/>
<connect gate="U2" pin="C" pad="T2"/>
<connect gate="U2" pin="D" pad="U2"/>
<connect gate="U2" pin="E" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W032" prefix="W032_">
<description>Cable Connector (15 signals)</description>
<gates>
<gate name="AF" symbol="PIN"/>
<gate name="AH" symbol="PIN"/>
<gate name="AJ" symbol="PIN"/>
<gate name="AN" symbol="PIN"/>
<gate name="AP" symbol="PIN"/>
<gate name="AR" symbol="PIN"/>
<gate name="AU" symbol="PIN"/>
<gate name="AV" symbol="PIN"/>
<gate name="BD" symbol="PIN"/>
<gate name="BF" symbol="PIN"/>
<gate name="BH" symbol="PIN"/>
<gate name="BJ" symbol="PIN"/>
<gate name="BM" symbol="PIN"/>
<gate name="BN" symbol="PIN"/>
<gate name="BP" symbol="PIN"/>
<gate name="G$16" symbol="T1GND"/>
<gate name="G$17" symbol="T1GND"/>
<gate name="G$18" symbol="T1GND"/>
<gate name="G$19" symbol="T1GND"/>
<gate name="G$20" symbol="T1GND"/>
<gate name="G$21" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="G$16" pin="GND" pad="AC2"/>
<connect gate="G$17" pin="GND" pad="AK2"/>
<connect gate="G$18" pin="GND" pad="AS2"/>
<connect gate="G$19" pin="GND" pad="AT2"/>
<connect gate="G$20" pin="GND" pad="BE2"/>
<connect gate="G$21" pin="GND" pad="BL2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800-2">
<connects>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="G$16" pin="GND" pad="AC2"/>
<connect gate="G$17" pin="GND" pad="AK2"/>
<connect gate="G$18" pin="GND" pad="AS2"/>
<connect gate="G$19" pin="GND" pad="AT2"/>
<connect gate="G$20" pin="GND" pad="BE2"/>
<connect gate="G$21" pin="GND" pad="BL2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S-2">
<connects>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="G$16" pin="GND" pad="AC2"/>
<connect gate="G$17" pin="GND" pad="AK2"/>
<connect gate="G$18" pin="GND" pad="AS2"/>
<connect gate="G$19" pin="GND" pad="AT2"/>
<connect gate="G$20" pin="GND" pad="BE2"/>
<connect gate="G$21" pin="GND" pad="BL2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W005" prefix="W005_">
<description>15 Clamped Loads</description>
<gates>
<gate name="D" symbol="W005A"/>
<gate name="E" symbol="W005A"/>
<gate name="F" symbol="W005A"/>
<gate name="H" symbol="W005A"/>
<gate name="J" symbol="W005A"/>
<gate name="K" symbol="W005A"/>
<gate name="L" symbol="W005A"/>
<gate name="M" symbol="W005A"/>
<gate name="N" symbol="W005A"/>
<gate name="P" symbol="W005A"/>
<gate name="R" symbol="W005A"/>
<gate name="S" symbol="W005A"/>
<gate name="T" symbol="W005A"/>
<gate name="U" symbol="W005A"/>
<gate name="V" symbol="W005A"/>
<gate name="G$16" symbol="-15V"/>
<gate name="G$1" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="P$1" pad="D2"/>
<connect gate="E" pin="P$1" pad="E2"/>
<connect gate="F" pin="P$1" pad="F2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="A2"/>
<connect gate="G$16" pin="-15V" pad="B2"/>
<connect gate="H" pin="P$1" pad="H2"/>
<connect gate="J" pin="P$1" pad="J2"/>
<connect gate="K" pin="P$1" pad="K2"/>
<connect gate="L" pin="P$1" pad="L2"/>
<connect gate="M" pin="P$1" pad="M2"/>
<connect gate="N" pin="P$1" pad="N2"/>
<connect gate="P" pin="P$1" pad="P2"/>
<connect gate="R" pin="P$1" pad="R2"/>
<connect gate="S" pin="P$1" pad="S2"/>
<connect gate="T" pin="P$1" pad="T2"/>
<connect gate="U" pin="P$1" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="P$1" pad="D2"/>
<connect gate="E" pin="P$1" pad="E2"/>
<connect gate="F" pin="P$1" pad="F2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="A2"/>
<connect gate="G$16" pin="-15V" pad="B2"/>
<connect gate="H" pin="P$1" pad="H2"/>
<connect gate="J" pin="P$1" pad="J2"/>
<connect gate="K" pin="P$1" pad="K2"/>
<connect gate="L" pin="P$1" pad="L2"/>
<connect gate="M" pin="P$1" pad="M2"/>
<connect gate="N" pin="P$1" pad="N2"/>
<connect gate="P" pin="P$1" pad="P2"/>
<connect gate="R" pin="P$1" pad="R2"/>
<connect gate="S" pin="P$1" pad="S2"/>
<connect gate="T" pin="P$1" pad="T2"/>
<connect gate="U" pin="P$1" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="P$1" pad="D2"/>
<connect gate="E" pin="P$1" pad="E2"/>
<connect gate="F" pin="P$1" pad="F2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="A2"/>
<connect gate="G$16" pin="-15V" pad="B2"/>
<connect gate="H" pin="P$1" pad="H2"/>
<connect gate="J" pin="P$1" pad="J2"/>
<connect gate="K" pin="P$1" pad="K2"/>
<connect gate="L" pin="P$1" pad="L2"/>
<connect gate="M" pin="P$1" pad="M2"/>
<connect gate="N" pin="P$1" pad="N2"/>
<connect gate="P" pin="P$1" pad="P2"/>
<connect gate="R" pin="P$1" pad="R2"/>
<connect gate="S" pin="P$1" pad="S2"/>
<connect gate="T" pin="P$1" pad="T2"/>
<connect gate="U" pin="P$1" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G888" prefix="G888_">
<description>Manchester Reader/Writer</description>
<gates>
<gate name="G$1" symbol="G888"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="G$1" pin="V2" pad="V2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="-15V" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G821" prefix="G821_">
<description>+5V Regulator</description>
<gates>
<gate name="G$1" symbol="-15V"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="-15V"/>
<gate name="G$4" symbol="-15V"/>
<gate name="G$5" symbol="POWER"/>
<gate name="G$6" symbol="POWER"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="POWER"/>
<gate name="G$9" symbol="POWER"/>
<gate name="G$10" symbol="POWER"/>
<gate name="G$11" symbol="POWER"/>
<gate name="G$12" symbol="POWER"/>
<gate name="G$13" symbol="POWER"/>
<gate name="G$15" symbol="POWER"/>
<gate name="G$14" symbol="G821A"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="-15V" pad="AB2"/>
<connect gate="G$10" pin="GND" pad="BK2"/>
<connect gate="G$10" pin="VCC" pad="AB1"/>
<connect gate="G$11" pin="GND" pad="BL2"/>
<connect gate="G$11" pin="VCC" pad="AC1"/>
<connect gate="G$12" pin="GND" pad="BT1"/>
<connect gate="G$12" pin="VCC" pad="AD1"/>
<connect gate="G$13" pin="GND" pad="AH2"/>
<connect gate="G$13" pin="VCC" pad="AE1"/>
<connect gate="G$14" pin="+11V" pad="BM2"/>
<connect gate="G$14" pin="BM1" pad="BM1"/>
<connect gate="G$14" pin="BN1" pad="BN1"/>
<connect gate="G$14" pin="BP1" pad="BP1"/>
<connect gate="G$14" pin="BR1" pad="BR1"/>
<connect gate="G$14" pin="VCC@1" pad="AF1"/>
<connect gate="G$14" pin="VCC@2" pad="AH1"/>
<connect gate="G$14" pin="VCC@3" pad="AJ1"/>
<connect gate="G$14" pin="VCC@4" pad="AK1"/>
<connect gate="G$15" pin="GND" pad="AK2"/>
<connect gate="G$15" pin="VCC" pad="AL1"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="BB1"/>
<connect gate="G$3" pin="-15V" pad="AF2"/>
<connect gate="G$4" pin="-15V" pad="AE2"/>
<connect gate="G$5" pin="GND" pad="AL2"/>
<connect gate="G$5" pin="VCC" pad="BC1"/>
<connect gate="G$6" pin="GND" pad="AT1"/>
<connect gate="G$6" pin="VCC" pad="BD1"/>
<connect gate="G$7" pin="GND" pad="BC2"/>
<connect gate="G$7" pin="VCC" pad="BE1"/>
<connect gate="G$8" pin="GND" pad="BD2"/>
<connect gate="G$8" pin="VCC" pad="AA2"/>
<connect gate="G$9" pin="GND" pad="BH2"/>
<connect gate="G$9" pin="VCC" pad="BA2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G879" prefix="G879_">
<description>Transport Detector</description>
<gates>
<gate name="G$1" symbol="INVERTER-N"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="IN" pad="T2"/>
<connect gate="G$1" pin="OUT" pad="U2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="-15V" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M206X" prefix="M206_">
<description>Two sets of 3 D flip-flops</description>
<gates>
<gate name="P2" symbol="D-FLOP"/>
<gate name="E1" symbol="D-FLOP"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="S1" symbol="D-FLOP-K2"/>
<gate name="V2" symbol="D-FLOP-K2"/>
<gate name="H2" symbol="D-FLOP-A1"/>
<gate name="L1" symbol="D-FLOP-A1"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="0" pad="F1"/>
<connect gate="E1" pin="1" pad="E1"/>
<connect gate="E1" pin="C" pad="B1"/>
<connect gate="E1" pin="D" pad="C1"/>
<connect gate="E1" pin="R" pad="A1"/>
<connect gate="E1" pin="S" pad="D1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="H2" pin="0" pad="J2"/>
<connect gate="H2" pin="1" pad="H2"/>
<connect gate="H2" pin="C" pad="D2"/>
<connect gate="H2" pin="D" pad="E2"/>
<connect gate="H2" pin="S" pad="F2"/>
<connect gate="L1" pin="0" pad="M1"/>
<connect gate="L1" pin="1" pad="L1"/>
<connect gate="L1" pin="C" pad="H1"/>
<connect gate="L1" pin="D" pad="J1"/>
<connect gate="L1" pin="S" pad="K1"/>
<connect gate="P2" pin="0" pad="R2"/>
<connect gate="P2" pin="1" pad="P2"/>
<connect gate="P2" pin="C" pad="L2"/>
<connect gate="P2" pin="D" pad="M2"/>
<connect gate="P2" pin="R" pad="K2"/>
<connect gate="P2" pin="S" pad="N2"/>
<connect gate="S1" pin="0" pad="U1"/>
<connect gate="S1" pin="1" pad="S1"/>
<connect gate="S1" pin="C" pad="N1"/>
<connect gate="S1" pin="D" pad="P1"/>
<connect gate="S1" pin="S" pad="R1"/>
<connect gate="V2" pin="0" pad="V1"/>
<connect gate="V2" pin="1" pad="V2"/>
<connect gate="V2" pin="C" pad="S2"/>
<connect gate="V2" pin="D" pad="T2"/>
<connect gate="V2" pin="S" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M903" prefix="M903_">
<description>Two-sided Posibus cable/connector.</description>
<gates>
<gate name="B1" symbol="PIN"/>
<gate name="D1" symbol="PIN"/>
<gate name="E1" symbol="PIN"/>
<gate name="H1" symbol="PIN"/>
<gate name="J1" symbol="PIN"/>
<gate name="L1" symbol="PIN"/>
<gate name="M1" symbol="PIN"/>
<gate name="P1" symbol="PIN"/>
<gate name="S1" symbol="PIN"/>
<gate name="D2" symbol="PIN"/>
<gate name="E2" symbol="PIN"/>
<gate name="H2" symbol="PIN"/>
<gate name="K2" symbol="PIN"/>
<gate name="M2" symbol="PIN"/>
<gate name="P2" symbol="PIN"/>
<gate name="S2" symbol="PIN"/>
<gate name="T2" symbol="PIN"/>
<gate name="V2" symbol="PIN"/>
<gate name="A1" symbol="T1GND"/>
<gate name="C1" symbol="T1GND"/>
<gate name="F1" symbol="T1GND"/>
<gate name="K1" symbol="T1GND"/>
<gate name="N1" symbol="T1GND"/>
<gate name="R1" symbol="T1GND"/>
<gate name="T1" symbol="T1GND"/>
<gate name="C2" symbol="T1GND"/>
<gate name="F2" symbol="T1GND"/>
<gate name="J2" symbol="T1GND"/>
<gate name="L2" symbol="T1GND"/>
<gate name="N2" symbol="T1GND"/>
<gate name="R2" symbol="T1GND"/>
<gate name="U2" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="A1" pin="GND" pad="A1"/>
<connect gate="B1" pin="P$2" pad="B1"/>
<connect gate="C1" pin="GND" pad="C1"/>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="D1" pin="P$2" pad="D1"/>
<connect gate="D2" pin="P$2" pad="D2"/>
<connect gate="E1" pin="P$2" pad="E1"/>
<connect gate="E2" pin="P$2" pad="E2"/>
<connect gate="F1" pin="GND" pad="F1"/>
<connect gate="F2" pin="GND" pad="F2"/>
<connect gate="H1" pin="P$2" pad="H1"/>
<connect gate="H2" pin="P$2" pad="H2"/>
<connect gate="J1" pin="P$2" pad="J1"/>
<connect gate="J2" pin="GND" pad="J2"/>
<connect gate="K1" pin="GND" pad="K1"/>
<connect gate="K2" pin="P$2" pad="K2"/>
<connect gate="L1" pin="P$2" pad="L1"/>
<connect gate="L2" pin="GND" pad="L2"/>
<connect gate="M1" pin="P$2" pad="M1"/>
<connect gate="M2" pin="P$2" pad="M2"/>
<connect gate="N1" pin="GND" pad="N1"/>
<connect gate="N2" pin="GND" pad="N2"/>
<connect gate="P1" pin="P$2" pad="P1"/>
<connect gate="P2" pin="P$2" pad="P2"/>
<connect gate="R1" pin="GND" pad="R1"/>
<connect gate="R2" pin="GND" pad="R2"/>
<connect gate="S1" pin="P$2" pad="S1"/>
<connect gate="S2" pin="P$2" pad="S2"/>
<connect gate="T1" pin="GND" pad="T1"/>
<connect gate="T2" pin="P$2" pad="T2"/>
<connect gate="U2" pin="GND" pad="U2"/>
<connect gate="V2" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M916" prefix="M916_">
<description>Simple 36 pin connector/wire cable</description>
<gates>
<gate name="A1" symbol="PIN"/>
<gate name="A2" symbol="PIN"/>
<gate name="B1" symbol="PIN"/>
<gate name="B2" symbol="PIN"/>
<gate name="C1" symbol="PIN"/>
<gate name="C2" symbol="PIN"/>
<gate name="D1" symbol="PIN"/>
<gate name="D2" symbol="PIN"/>
<gate name="E1" symbol="PIN"/>
<gate name="E2" symbol="PIN"/>
<gate name="F1" symbol="PIN"/>
<gate name="F2" symbol="PIN"/>
<gate name="H1" symbol="PIN"/>
<gate name="H2" symbol="PIN"/>
<gate name="J1" symbol="PIN"/>
<gate name="J2" symbol="PIN"/>
<gate name="K1" symbol="PIN"/>
<gate name="K2" symbol="PIN"/>
<gate name="L1" symbol="PIN"/>
<gate name="L2" symbol="PIN"/>
<gate name="M1" symbol="PIN"/>
<gate name="M2" symbol="PIN"/>
<gate name="N1" symbol="PIN"/>
<gate name="N2" symbol="PIN"/>
<gate name="P1" symbol="PIN"/>
<gate name="P2" symbol="PIN"/>
<gate name="R1" symbol="PIN"/>
<gate name="R2" symbol="PIN"/>
<gate name="S1" symbol="PIN"/>
<gate name="S2" symbol="PIN"/>
<gate name="T1" symbol="PIN"/>
<gate name="T2" symbol="PIN"/>
<gate name="U1" symbol="PIN"/>
<gate name="U2" symbol="PIN"/>
<gate name="V1" symbol="PIN"/>
<gate name="V2" symbol="PIN"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="A1" pin="P$2" pad="A1"/>
<connect gate="A2" pin="P$2" pad="A2"/>
<connect gate="B1" pin="P$2" pad="B1"/>
<connect gate="B2" pin="P$2" pad="B2"/>
<connect gate="C1" pin="P$2" pad="C1"/>
<connect gate="C2" pin="P$2" pad="C2"/>
<connect gate="D1" pin="P$2" pad="D1"/>
<connect gate="D2" pin="P$2" pad="D2"/>
<connect gate="E1" pin="P$2" pad="E1"/>
<connect gate="E2" pin="P$2" pad="E2"/>
<connect gate="F1" pin="P$2" pad="F1"/>
<connect gate="F2" pin="P$2" pad="F2"/>
<connect gate="H1" pin="P$2" pad="H1"/>
<connect gate="H2" pin="P$2" pad="H2"/>
<connect gate="J1" pin="P$2" pad="J1"/>
<connect gate="J2" pin="P$2" pad="J2"/>
<connect gate="K1" pin="P$2" pad="K1"/>
<connect gate="K2" pin="P$2" pad="K2"/>
<connect gate="L1" pin="P$2" pad="L1"/>
<connect gate="L2" pin="P$2" pad="L2"/>
<connect gate="M1" pin="P$2" pad="M1"/>
<connect gate="M2" pin="P$2" pad="M2"/>
<connect gate="N1" pin="P$2" pad="N1"/>
<connect gate="N2" pin="P$2" pad="N2"/>
<connect gate="P1" pin="P$2" pad="P1"/>
<connect gate="P2" pin="P$2" pad="P2"/>
<connect gate="R1" pin="P$2" pad="R1"/>
<connect gate="R2" pin="P$2" pad="R2"/>
<connect gate="S1" pin="P$2" pad="S1"/>
<connect gate="S2" pin="P$2" pad="S2"/>
<connect gate="T1" pin="P$2" pad="T1"/>
<connect gate="T2" pin="P$2" pad="T2"/>
<connect gate="U1" pin="P$2" pad="U1"/>
<connect gate="U2" pin="P$2" pad="U2"/>
<connect gate="V1" pin="P$2" pad="V1"/>
<connect gate="V2" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W023" prefix="W023_">
<description>One-sided 18 pin connector/cable.</description>
<gates>
<gate name="A" symbol="PIN"/>
<gate name="B" symbol="PIN"/>
<gate name="C" symbol="PIN"/>
<gate name="D" symbol="PIN"/>
<gate name="E" symbol="PIN"/>
<gate name="F" symbol="PIN"/>
<gate name="H" symbol="PIN"/>
<gate name="J" symbol="PIN"/>
<gate name="K" symbol="PIN"/>
<gate name="L" symbol="PIN"/>
<gate name="M" symbol="PIN"/>
<gate name="N" symbol="PIN"/>
<gate name="P" symbol="PIN"/>
<gate name="R" symbol="PIN"/>
<gate name="S" symbol="PIN"/>
<gate name="T" symbol="PIN"/>
<gate name="U" symbol="PIN"/>
<gate name="V" symbol="PIN"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="A" pin="P$2" pad="A2"/>
<connect gate="B" pin="P$2" pad="B2"/>
<connect gate="C" pin="P$2" pad="C2"/>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="F" pin="P$2" pad="F2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="J" pin="P$2" pad="J2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="L" pin="P$2" pad="L2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="N" pin="P$2" pad="N2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="R" pin="P$2" pad="R2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="U" pin="P$2" pad="U2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="A" pin="P$2" pad="A2"/>
<connect gate="B" pin="P$2" pad="B2"/>
<connect gate="C" pin="P$2" pad="C2"/>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="F" pin="P$2" pad="F2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="J" pin="P$2" pad="J2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="L" pin="P$2" pad="L2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="N" pin="P$2" pad="N2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="R" pin="P$2" pad="R2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="U" pin="P$2" pad="U2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="A" pin="P$2" pad="A2"/>
<connect gate="B" pin="P$2" pad="B2"/>
<connect gate="C" pin="P$2" pad="C2"/>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="F" pin="P$2" pad="F2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="J" pin="P$2" pad="J2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="L" pin="P$2" pad="L2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="N" pin="P$2" pad="N2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="R" pin="P$2" pad="R2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="U" pin="P$2" pad="U2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="H807" prefix="H807_">
<description>Empty card slot</description>
<gates>
<gate name="G$1" symbol="PART"/>
</gates>
<devices>
<device name="" package="H807">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC">
<description>An unconnected pin</description>
<gates>
<gate name="NC" symbol="NC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+11V">
<description>11V Supply Connection</description>
<gates>
<gate name="G$1" symbol="+11V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M651" prefix="M651_">
<description>M651 - Negative Output Converter</description>
<gates>
<gate name="D" symbol="M651"/>
<gate name="K" symbol="M651"/>
<gate name="S" symbol="M651"/>
<gate name="G$4" symbol="-15V"/>
<gate name="G$5" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="IN1" pad="F2"/>
<connect gate="D" pin="IN2" pad="H2"/>
<connect gate="D" pin="IN3" pad="J2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="D" pin="SLOW" pad="E2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="K" pin="IN1" pad="M2"/>
<connect gate="K" pin="IN2" pad="N2"/>
<connect gate="K" pin="IN3" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="K" pin="SLOW" pad="L2"/>
<connect gate="S" pin="IN1" pad="T2"/>
<connect gate="S" pin="IN2" pad="U2"/>
<connect gate="S" pin="IN3" pad="V2"/>
<connect gate="S" pin="OUT" pad="S2"/>
<connect gate="S" pin="SLOW" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="IN1" pad="F2"/>
<connect gate="D" pin="IN2" pad="H2"/>
<connect gate="D" pin="IN3" pad="J2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="D" pin="SLOW" pad="E2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="K" pin="IN1" pad="M2"/>
<connect gate="K" pin="IN2" pad="N2"/>
<connect gate="K" pin="IN3" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="K" pin="SLOW" pad="L2"/>
<connect gate="S" pin="IN1" pad="T2"/>
<connect gate="S" pin="IN2" pad="U2"/>
<connect gate="S" pin="IN3" pad="V2"/>
<connect gate="S" pin="OUT" pad="S2"/>
<connect gate="S" pin="SLOW" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="IN1" pad="F2"/>
<connect gate="D" pin="IN2" pad="H2"/>
<connect gate="D" pin="IN3" pad="J2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="D" pin="SLOW" pad="E2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="K" pin="IN1" pad="M2"/>
<connect gate="K" pin="IN2" pad="N2"/>
<connect gate="K" pin="IN3" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="K" pin="SLOW" pad="L2"/>
<connect gate="S" pin="IN1" pad="T2"/>
<connect gate="S" pin="IN2" pad="U2"/>
<connect gate="S" pin="IN3" pad="V2"/>
<connect gate="S" pin="OUT" pad="S2"/>
<connect gate="S" pin="SLOW" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M507" prefix="M507_">
<description>M507 Negative Bus Converter</description>
<gates>
<gate name="D" symbol="M507"/>
<gate name="F" symbol="M507"/>
<gate name="J" symbol="M507"/>
<gate name="L" symbol="M507"/>
<gate name="N" symbol="M507"/>
<gate name="R" symbol="M507"/>
<gate name="G$7" symbol="-15V"/>
<gate name="G$8" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M517" prefix="M517_">
<description>M517 Negative Bus Converter</description>
<gates>
<gate name="D" symbol="M507"/>
<gate name="F" symbol="M507"/>
<gate name="J" symbol="M507"/>
<gate name="L" symbol="M507"/>
<gate name="N" symbol="M507"/>
<gate name="R" symbol="M507"/>
<gate name="B" symbol="-15V"/>
<gate name="C2" symbol="POWER"/>
<gate name="T" symbol="T1GND"/>
<gate name="U" symbol="T1GND"/>
<gate name="V" symbol="ENABLE"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="B" pin="-15V" pad="B2"/>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="C2" pin="VCC" pad="A2"/>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
<connect gate="T" pin="GND" pad="T2"/>
<connect gate="U" pin="GND" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="B" pin="-15V" pad="B2"/>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="C2" pin="VCC" pad="A2"/>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
<connect gate="T" pin="GND" pad="T2"/>
<connect gate="U" pin="GND" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="B" pin="-15V" pad="B2"/>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="C2" pin="VCC" pad="A2"/>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
<connect gate="T" pin="GND" pad="T2"/>
<connect gate="U" pin="GND" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M907" prefix="M907_">
<description>M907 Diode Clamp</description>
<gates>
<gate name="A1" symbol="T1GND"/>
<gate name="C1" symbol="T1GND"/>
<gate name="F1" symbol="T1GND"/>
<gate name="K1" symbol="T1GND"/>
<gate name="N1" symbol="T1GND"/>
<gate name="R1" symbol="T1GND"/>
<gate name="T1" symbol="T1GND"/>
<gate name="U1" symbol="PULL-UP"/>
<gate name="U2" symbol="T1GND"/>
<gate name="F2" symbol="T1GND"/>
<gate name="J2" symbol="T1GND"/>
<gate name="L2" symbol="T1GND"/>
<gate name="N2" symbol="T1GND"/>
<gate name="R2" symbol="T1GND"/>
<gate name="B1" symbol="DIODECLAMP"/>
<gate name="D1" symbol="DIODECLAMP"/>
<gate name="E1" symbol="DIODECLAMP"/>
<gate name="H1" symbol="DIODECLAMP"/>
<gate name="J1" symbol="DIODECLAMP"/>
<gate name="L1" symbol="DIODECLAMP"/>
<gate name="M1" symbol="DIODECLAMP"/>
<gate name="P1" symbol="DIODECLAMP"/>
<gate name="S1" symbol="DIODECLAMP"/>
<gate name="D2" symbol="DIODECLAMP"/>
<gate name="E2" symbol="DIODECLAMP"/>
<gate name="H2" symbol="DIODECLAMP"/>
<gate name="K2" symbol="DIODECLAMP"/>
<gate name="M2" symbol="DIODECLAMP"/>
<gate name="P2" symbol="DIODECLAMP"/>
<gate name="S2" symbol="DIODECLAMP"/>
<gate name="T2" symbol="DIODECLAMP"/>
<gate name="V2" symbol="DIODECLAMP"/>
<gate name="V1" symbol="PULL-UP"/>
<gate name="G$35" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="A1" pin="GND" pad="A1"/>
<connect gate="B1" pin="CATHODE" pad="B1"/>
<connect gate="C1" pin="GND" pad="C1"/>
<connect gate="D1" pin="CATHODE" pad="D1"/>
<connect gate="D2" pin="CATHODE" pad="D2"/>
<connect gate="E1" pin="CATHODE" pad="E1"/>
<connect gate="E2" pin="CATHODE" pad="E2"/>
<connect gate="F1" pin="GND" pad="F1"/>
<connect gate="F2" pin="GND" pad="F2"/>
<connect gate="G$35" pin="GND" pad="C2"/>
<connect gate="G$35" pin="VCC" pad="A2"/>
<connect gate="H1" pin="CATHODE" pad="H1"/>
<connect gate="H2" pin="CATHODE" pad="H2"/>
<connect gate="J1" pin="CATHODE" pad="J1"/>
<connect gate="J2" pin="GND" pad="J2"/>
<connect gate="K1" pin="GND" pad="K1"/>
<connect gate="K2" pin="CATHODE" pad="K2"/>
<connect gate="L1" pin="CATHODE" pad="L1"/>
<connect gate="L2" pin="GND" pad="L2"/>
<connect gate="M1" pin="CATHODE" pad="M1"/>
<connect gate="M2" pin="CATHODE" pad="M2"/>
<connect gate="N1" pin="GND" pad="N1"/>
<connect gate="N2" pin="GND" pad="N2"/>
<connect gate="P1" pin="CATHODE" pad="P1"/>
<connect gate="P2" pin="CATHODE" pad="P2"/>
<connect gate="R1" pin="GND" pad="R1"/>
<connect gate="R2" pin="GND" pad="R2"/>
<connect gate="S1" pin="CATHODE" pad="S1"/>
<connect gate="S2" pin="CATHODE" pad="S2"/>
<connect gate="T1" pin="GND" pad="T1"/>
<connect gate="T2" pin="CATHODE" pad="T2"/>
<connect gate="U1" pin="P$1" pad="U1"/>
<connect gate="U2" pin="GND" pad="U2"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="CATHODE" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W011" prefix="W011_">
<description>One-sided 9 pin connector/cable with grounds (Negibus).</description>
<gates>
<gate name="D" symbol="PIN"/>
<gate name="E" symbol="PIN"/>
<gate name="H" symbol="PIN"/>
<gate name="K" symbol="PIN"/>
<gate name="M" symbol="PIN"/>
<gate name="P" symbol="PIN"/>
<gate name="S" symbol="PIN"/>
<gate name="T" symbol="PIN"/>
<gate name="V" symbol="PIN"/>
<gate name="G$1" symbol="T1GND"/>
<gate name="G$2" symbol="T1GND"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="G$6" symbol="T1GND"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="G$10" symbol="T1GND"/>
<gate name="G$12" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G826" prefix="G826_">
<description>Regulator and Power Detector</description>
<gates>
<gate name="G$1" symbol="G826"/>
<gate name="G$2" symbol="-15V"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="-30V@BV2" pad="BV2"/>
<connect gate="G$1" pin="-6V@BM2" pad="BM2"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BR2" pad="BR2"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$2" pin="-15V" pad="AB2"/>
<connect gate="G$3" pin="GND" pad="AC2"/>
<connect gate="G$3" pin="VCC" pad="AA2"/>
<connect gate="G$4" pin="GND" pad="BC2"/>
<connect gate="G$4" pin="VCC" pad="BA2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G805" prefix="G805_">
<description>Negative Regulator</description>
<gates>
<gate name="G$1" symbol="G805"/>
<gate name="G$2" symbol="T1GND"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="T1GND"/>
<gate name="G$6" symbol="T1GND"/>
<gate name="G$7" symbol="T1GND"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="G$9" symbol="-30V"/>
<gate name="G$10" symbol="-30V"/>
<gate name="G$11" symbol="-30V"/>
<gate name="G$12" symbol="-30V"/>
<gate name="G$13" symbol="-30V"/>
<gate name="G$14" symbol="-30V"/>
<gate name="G$15" symbol="-30V"/>
<gate name="G$16" symbol="-6V"/>
<gate name="G$17" symbol="-6V"/>
<gate name="G$18" symbol="-6V"/>
<gate name="G$19" symbol="-6V"/>
<gate name="G$20" symbol="-6V"/>
<gate name="G$21" symbol="-6V"/>
<gate name="G$22" symbol="-6V"/>
<gate name="G$23" symbol="T1GND"/>
<gate name="G$24" symbol="T1GND"/>
<gate name="G$25" symbol="T1GND"/>
<gate name="G$26" symbol="T1GND"/>
<gate name="G$27" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="-30V@AE2" pad="AE2"/>
<connect gate="G$1" pin="-6V@BM2" pad="BM2"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="GND@BC2" pad="BC2"/>
<connect gate="G$10" pin="-30V" pad="AH2"/>
<connect gate="G$11" pin="-30V" pad="AJ2"/>
<connect gate="G$12" pin="-30V" pad="AK2"/>
<connect gate="G$13" pin="-30V" pad="AL2"/>
<connect gate="G$14" pin="-30V" pad="AM2"/>
<connect gate="G$15" pin="-30V" pad="AN2"/>
<connect gate="G$16" pin="-6V" pad="BN2"/>
<connect gate="G$17" pin="-6V" pad="BP2"/>
<connect gate="G$18" pin="-6V" pad="BR2"/>
<connect gate="G$19" pin="-6V" pad="BS2"/>
<connect gate="G$2" pin="GND" pad="BD2"/>
<connect gate="G$20" pin="-6V" pad="BT2"/>
<connect gate="G$21" pin="-6V" pad="BU2"/>
<connect gate="G$22" pin="-6V" pad="BV2"/>
<connect gate="G$23" pin="GND" pad="AP2"/>
<connect gate="G$24" pin="GND" pad="AR2"/>
<connect gate="G$25" pin="GND" pad="AS2"/>
<connect gate="G$26" pin="GND" pad="AT2"/>
<connect gate="G$27" pin="GND" pad="AU2"/>
<connect gate="G$3" pin="GND" pad="BE2"/>
<connect gate="G$4" pin="GND" pad="BF2"/>
<connect gate="G$5" pin="GND" pad="BH2"/>
<connect gate="G$6" pin="GND" pad="BJ2"/>
<connect gate="G$7" pin="GND" pad="BK2"/>
<connect gate="G$8" pin="GND" pad="BL2"/>
<connect gate="G$9" pin="-30V" pad="AF2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G624" prefix="G624_">
<description>Resistor Board</description>
<gates>
<gate name="P" symbol="G624A"/>
<gate name="R" symbol="G624A"/>
<gate name="S" symbol="G624A"/>
<gate name="T" symbol="G624A"/>
<gate name="U" symbol="G624B"/>
<gate name="E" symbol="G624C"/>
<gate name="C" symbol="G624C"/>
<gate name="D" symbol="G624D"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="C" pin="P$1" pad="V2"/>
<connect gate="C" pin="P$2" pad="C2"/>
<connect gate="D" pin="P$1" pad="B2"/>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$1" pad="H2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="P" pin="P$1" pad="N2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="R" pin="P$1" pad="M2"/>
<connect gate="R" pin="P$2" pad="R2"/>
<connect gate="S" pin="P$1" pad="L2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$1" pad="K2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="U" pin="P$1" pad="F2"/>
<connect gate="U" pin="P$2" pad="U2"/>
<connect gate="U" pin="P$3" pad="J2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M617" prefix="M617_">
<description>6 4-input NAND Buffers</description>
<gates>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="U1" symbol="PULL-UP"/>
<gate name="V1" symbol="PULL-UP"/>
<gate name="J2" symbol="NAND4OC"/>
<gate name="E1" symbol="NAND4OC"/>
<gate name="P2" symbol="NAND4OC"/>
<gate name="S1" symbol="NAND4OC"/>
<gate name="V2" symbol="NAND4OC"/>
<gate name="L1" symbol="NAND4OC"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="IN1" pad="A1"/>
<connect gate="E1" pin="IN2" pad="B1"/>
<connect gate="E1" pin="IN3" pad="C1"/>
<connect gate="E1" pin="IN4" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="J2" pin="IN1" pad="D2"/>
<connect gate="J2" pin="IN2" pad="E2"/>
<connect gate="J2" pin="IN3" pad="F2"/>
<connect gate="J2" pin="IN4" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="L1" pin="IN1" pad="F1"/>
<connect gate="L1" pin="IN2" pad="H1"/>
<connect gate="L1" pin="IN3" pad="J1"/>
<connect gate="L1" pin="IN4" pad="K1"/>
<connect gate="L1" pin="OUT" pad="L1"/>
<connect gate="P2" pin="IN1" pad="K2"/>
<connect gate="P2" pin="IN2" pad="L2"/>
<connect gate="P2" pin="IN3" pad="M2"/>
<connect gate="P2" pin="IN4" pad="N2"/>
<connect gate="P2" pin="OUT" pad="P2"/>
<connect gate="S1" pin="IN1" pad="M1"/>
<connect gate="S1" pin="IN2" pad="N1"/>
<connect gate="S1" pin="IN3" pad="P1"/>
<connect gate="S1" pin="IN4" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="U1" pin="P$1" pad="U1"/>
<connect gate="V1" pin="P$1" pad="V1"/>
<connect gate="V2" pin="IN1" pad="R2"/>
<connect gate="V2" pin="IN2" pad="S2"/>
<connect gate="V2" pin="IN3" pad="T2"/>
<connect gate="V2" pin="IN4" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M310" prefix="M310_">
<description>Tapped Delay Line</description>
<gates>
<gate name="H2" symbol="M310"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="F1" symbol="BUFFER"/>
<gate name="J1" symbol="BUFFER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="F1" pin="IN" pad="E1"/>
<connect gate="F1" pin="OUT" pad="F1"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
<connect gate="H2" pin="H2" pad="H2"/>
<connect gate="H2" pin="J2" pad="J2"/>
<connect gate="H2" pin="K2" pad="K2"/>
<connect gate="H2" pin="L2" pad="L2"/>
<connect gate="H2" pin="M2" pad="M2"/>
<connect gate="H2" pin="N2" pad="N2"/>
<connect gate="H2" pin="P2" pad="P2"/>
<connect gate="H2" pin="R2" pad="R2"/>
<connect gate="H2" pin="S2" pad="S2"/>
<connect gate="H2" pin="T2" pad="T2"/>
<connect gate="H2" pin="U2" pad="U2"/>
<connect gate="H2" pin="V2" pad="V2"/>
<connect gate="J1" pin="IN" pad="H1"/>
<connect gate="J1" pin="OUT" pad="J1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G228" prefix="G228_">
<description>Inhibit Driver</description>
<gates>
<gate name="G$1" symbol="G228A"/>
<gate name="C2" symbol="POWER"/>
<gate name="H2" symbol="G228B"/>
<gate name="F1" symbol="G228B"/>
<gate name="R2" symbol="G228B"/>
<gate name="N1" symbol="G228B"/>
<gate name="T1" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="C2" pin="VCC" pad="A2"/>
<connect gate="F1" pin="H" pad="F1"/>
<connect gate="F1" pin="J" pad="H1"/>
<connect gate="F1" pin="K" pad="J1"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="K1" pad="K1"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="G$1" pin="V2" pad="V2"/>
<connect gate="H2" pin="H" pad="H2"/>
<connect gate="H2" pin="J" pad="J2"/>
<connect gate="H2" pin="K" pad="K2"/>
<connect gate="N1" pin="H" pad="N1"/>
<connect gate="N1" pin="J" pad="P1"/>
<connect gate="N1" pin="K" pad="R1"/>
<connect gate="R2" pin="H" pad="R2"/>
<connect gate="R2" pin="J" pad="S2"/>
<connect gate="R2" pin="K" pad="T2"/>
<connect gate="T1" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M160" prefix="M160_">
<description>AND-NOR Gates</description>
<gates>
<gate name="V2" symbol="AND-NOR"/>
<gate name="G$4" symbol="POWER"/>
<gate name="G$5" symbol="T1GND"/>
<gate name="R1" symbol="AND-NOR5"/>
<gate name="T2" symbol="AND-NOR4"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="GND" pad="T1"/>
<connect gate="R1" pin="IN1A" pad="A1"/>
<connect gate="R1" pin="IN1B" pad="B1"/>
<connect gate="R1" pin="IN1C" pad="C1"/>
<connect gate="R1" pin="IN1D" pad="D1"/>
<connect gate="R1" pin="IN2A" pad="E1"/>
<connect gate="R1" pin="IN2B" pad="F1"/>
<connect gate="R1" pin="IN3A" pad="H1"/>
<connect gate="R1" pin="IN3B" pad="J1"/>
<connect gate="R1" pin="IN4A" pad="K1"/>
<connect gate="R1" pin="IN4B" pad="L1"/>
<connect gate="R1" pin="IN5A" pad="M1"/>
<connect gate="R1" pin="IN5B" pad="N1"/>
<connect gate="R1" pin="IN5C" pad="P1"/>
<connect gate="R1" pin="OUT" pad="R1"/>
<connect gate="T2" pin="IN1A" pad="D2"/>
<connect gate="T2" pin="IN1B" pad="E2"/>
<connect gate="T2" pin="IN1C" pad="F2"/>
<connect gate="T2" pin="IN1D" pad="H2"/>
<connect gate="T2" pin="IN2A" pad="J2"/>
<connect gate="T2" pin="IN2B" pad="K2"/>
<connect gate="T2" pin="IN3A" pad="L2"/>
<connect gate="T2" pin="IN3B" pad="M2"/>
<connect gate="T2" pin="IN4A" pad="N2"/>
<connect gate="T2" pin="IN4B" pad="P2"/>
<connect gate="T2" pin="IN4C" pad="R2"/>
<connect gate="T2" pin="IN4D" pad="S2"/>
<connect gate="T2" pin="OUT" pad="T2"/>
<connect gate="V2" pin="IN1A" pad="S1"/>
<connect gate="V2" pin="IN1B" pad="U1"/>
<connect gate="V2" pin="IN2A" pad="V1"/>
<connect gate="V2" pin="IN2B" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M162" prefix="M162_">
<description>Parity Circuit</description>
<gates>
<gate name="K1" symbol="M162"/>
<gate name="U2" symbol="M162"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="GND" pad="T1"/>
<connect gate="K1" pin="1A" pad="E1"/>
<connect gate="K1" pin="1B" pad="A1"/>
<connect gate="K1" pin="2A" pad="F1"/>
<connect gate="K1" pin="2B" pad="B1"/>
<connect gate="K1" pin="4A" pad="H1"/>
<connect gate="K1" pin="4B" pad="C1"/>
<connect gate="K1" pin="8A" pad="J1"/>
<connect gate="K1" pin="8B" pad="D1"/>
<connect gate="K1" pin="EVEN" pad="L1"/>
<connect gate="K1" pin="ODD" pad="K1"/>
<connect gate="U2" pin="1A" pad="P2"/>
<connect gate="U2" pin="1B" pad="K2"/>
<connect gate="U2" pin="2A" pad="R2"/>
<connect gate="U2" pin="2B" pad="L2"/>
<connect gate="U2" pin="4A" pad="S2"/>
<connect gate="U2" pin="4B" pad="M2"/>
<connect gate="U2" pin="8A" pad="T2"/>
<connect gate="U2" pin="8B" pad="N2"/>
<connect gate="U2" pin="EVEN" pad="V2"/>
<connect gate="U2" pin="ODD" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M506" prefix="M506_">
<description>Hex Negative Bus Receiver</description>
<gates>
<gate name="E1" symbol="M506"/>
<gate name="J2" symbol="M506"/>
<gate name="L1" symbol="M506"/>
<gate name="P2" symbol="M506"/>
<gate name="S1" symbol="M506"/>
<gate name="V2" symbol="M506"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="G$9" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="IN" pad="A1"/>
<connect gate="E1" pin="IN2" pad="B1"/>
<connect gate="E1" pin="IN3" pad="C1"/>
<connect gate="E1" pin="IN4" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="G$9" pin="-15V" pad="B2"/>
<connect gate="J2" pin="IN" pad="D2"/>
<connect gate="J2" pin="IN2" pad="E2"/>
<connect gate="J2" pin="IN3" pad="F2"/>
<connect gate="J2" pin="IN4" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="L1" pin="IN" pad="F1"/>
<connect gate="L1" pin="IN2" pad="H1"/>
<connect gate="L1" pin="IN3" pad="J1"/>
<connect gate="L1" pin="IN4" pad="K1"/>
<connect gate="L1" pin="OUT" pad="L1"/>
<connect gate="P2" pin="IN" pad="K2"/>
<connect gate="P2" pin="IN2" pad="L2"/>
<connect gate="P2" pin="IN3" pad="M2"/>
<connect gate="P2" pin="IN4" pad="N2"/>
<connect gate="P2" pin="OUT" pad="P2"/>
<connect gate="S1" pin="IN" pad="M1"/>
<connect gate="S1" pin="IN2" pad="N1"/>
<connect gate="S1" pin="IN3" pad="P1"/>
<connect gate="S1" pin="IN4" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="V2" pin="IN" pad="R2"/>
<connect gate="V2" pin="IN2" pad="S2"/>
<connect gate="V2" pin="IN3" pad="T2"/>
<connect gate="V2" pin="IN4" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M660" prefix="M660_">
<description>Positive Level Driver</description>
<gates>
<gate name="D" symbol="M660"/>
<gate name="K" symbol="M660"/>
<gate name="S" symbol="M660"/>
<gate name="G$4" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="IN1" pad="H2"/>
<connect gate="D" pin="IN2" pad="J2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="K" pin="IN1" pad="N2"/>
<connect gate="K" pin="IN2" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="S" pin="IN1" pad="U2"/>
<connect gate="S" pin="IN2" pad="V2"/>
<connect gate="S" pin="OUT" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="IN1" pad="H2"/>
<connect gate="D" pin="IN2" pad="J2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="K" pin="IN1" pad="N2"/>
<connect gate="K" pin="IN2" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="S" pin="IN1" pad="U2"/>
<connect gate="S" pin="IN2" pad="V2"/>
<connect gate="S" pin="OUT" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="IN1" pad="H2"/>
<connect gate="D" pin="IN2" pad="J2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="K" pin="IN1" pad="N2"/>
<connect gate="K" pin="IN2" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="S" pin="IN1" pad="U2"/>
<connect gate="S" pin="IN2" pad="V2"/>
<connect gate="S" pin="OUT" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M661" prefix="M661_">
<description>Positive Level Driver</description>
<gates>
<gate name="D" symbol="M661"/>
<gate name="K" symbol="M661"/>
<gate name="S" symbol="M661"/>
<gate name="G$4" symbol="POWER"/>
<gate name="G$5" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="IN1" pad="J2"/>
<connect gate="D" pin="IN2" pad="H2"/>
<connect gate="D" pin="IN3" pad="F2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
<connect gate="K" pin="IN1" pad="M2"/>
<connect gate="K" pin="IN2" pad="N2"/>
<connect gate="K" pin="IN3" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="S" pin="IN1" pad="V2"/>
<connect gate="S" pin="IN2" pad="U2"/>
<connect gate="S" pin="IN3" pad="T2"/>
<connect gate="S" pin="OUT" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="IN1" pad="J2"/>
<connect gate="D" pin="IN2" pad="H2"/>
<connect gate="D" pin="IN3" pad="F2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
<connect gate="K" pin="IN1" pad="M2"/>
<connect gate="K" pin="IN2" pad="N2"/>
<connect gate="K" pin="IN3" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="S" pin="IN1" pad="V2"/>
<connect gate="S" pin="IN2" pad="U2"/>
<connect gate="S" pin="IN3" pad="T2"/>
<connect gate="S" pin="OUT" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="IN1" pad="J2"/>
<connect gate="D" pin="IN2" pad="H2"/>
<connect gate="D" pin="IN3" pad="F2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
<connect gate="K" pin="IN1" pad="M2"/>
<connect gate="K" pin="IN2" pad="N2"/>
<connect gate="K" pin="IN3" pad="P2"/>
<connect gate="K" pin="OUT" pad="K2"/>
<connect gate="S" pin="IN1" pad="V2"/>
<connect gate="S" pin="IN2" pad="U2"/>
<connect gate="S" pin="IN3" pad="T2"/>
<connect gate="S" pin="OUT" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M516" prefix="M516_">
<description>Hex Positive Bus Receiver</description>
<gates>
<gate name="E1" symbol="M516"/>
<gate name="J2" symbol="M516"/>
<gate name="L1" symbol="M516"/>
<gate name="P2" symbol="M516"/>
<gate name="S1" symbol="M516"/>
<gate name="V2" symbol="M516"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="IN" pad="A1"/>
<connect gate="E1" pin="IN2" pad="B1"/>
<connect gate="E1" pin="IN3" pad="C1"/>
<connect gate="E1" pin="IN4" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="J2" pin="IN" pad="D2"/>
<connect gate="J2" pin="IN2" pad="E2"/>
<connect gate="J2" pin="IN3" pad="F2"/>
<connect gate="J2" pin="IN4" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="L1" pin="IN" pad="F1"/>
<connect gate="L1" pin="IN2" pad="H1"/>
<connect gate="L1" pin="IN3" pad="J1"/>
<connect gate="L1" pin="IN4" pad="K1"/>
<connect gate="L1" pin="OUT" pad="L1"/>
<connect gate="P2" pin="IN" pad="K2"/>
<connect gate="P2" pin="IN2" pad="L2"/>
<connect gate="P2" pin="IN3" pad="M2"/>
<connect gate="P2" pin="IN4" pad="N2"/>
<connect gate="P2" pin="OUT" pad="P2"/>
<connect gate="S1" pin="IN" pad="M1"/>
<connect gate="S1" pin="IN2" pad="N1"/>
<connect gate="S1" pin="IN3" pad="P1"/>
<connect gate="S1" pin="IN4" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="V2" pin="IN" pad="R2"/>
<connect gate="V2" pin="IN2" pad="S2"/>
<connect gate="V2" pin="IN3" pad="T2"/>
<connect gate="V2" pin="IN4" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M921" prefix="M921_">
<description>Device Code Select Jumper Board</description>
<gates>
<gate name="A" symbol="M921"/>
<gate name="B" symbol="M921"/>
<gate name="C" symbol="M921"/>
<gate name="D" symbol="M921"/>
<gate name="E" symbol="M921"/>
<gate name="F" symbol="M921"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="A" pin="L1" pad="A1"/>
<connect gate="A" pin="L2" pad="B1"/>
<connect gate="A" pin="L3" pad="C1"/>
<connect gate="A" pin="R1" pad="D2"/>
<connect gate="A" pin="R2" pad="E2"/>
<connect gate="B" pin="L1" pad="D1"/>
<connect gate="B" pin="L2" pad="E1"/>
<connect gate="B" pin="L3" pad="F1"/>
<connect gate="B" pin="R1" pad="F2"/>
<connect gate="B" pin="R2" pad="H2"/>
<connect gate="C" pin="L1" pad="H1"/>
<connect gate="C" pin="L2" pad="J1"/>
<connect gate="C" pin="L3" pad="K1"/>
<connect gate="C" pin="R1" pad="J2"/>
<connect gate="C" pin="R2" pad="K2"/>
<connect gate="D" pin="L1" pad="L1"/>
<connect gate="D" pin="L2" pad="M1"/>
<connect gate="D" pin="L3" pad="N1"/>
<connect gate="D" pin="R1" pad="L2"/>
<connect gate="D" pin="R2" pad="M2"/>
<connect gate="E" pin="L1" pad="P1"/>
<connect gate="E" pin="L2" pad="R1"/>
<connect gate="E" pin="L3" pad="S1"/>
<connect gate="E" pin="R1" pad="N2"/>
<connect gate="E" pin="R2" pad="P2"/>
<connect gate="F" pin="L1" pad="S2"/>
<connect gate="F" pin="L2" pad="U1"/>
<connect gate="F" pin="L3" pad="V1"/>
<connect gate="F" pin="R1" pad="T2"/>
<connect gate="F" pin="R2" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M900" prefix="M900_">
<description>PDP-8/i Console Connector</description>
<gates>
<gate name="G$31" symbol="T1GND"/>
<gate name="G$32" symbol="POWER"/>
<gate name="TOP1" symbol="M900"/>
<gate name="TOP2" symbol="M900"/>
<gate name="TOP3" symbol="M900"/>
<gate name="TOP4" symbol="M900"/>
<gate name="TOP5" symbol="M900"/>
<gate name="TOP6" symbol="M900"/>
<gate name="TOP7" symbol="M900"/>
<gate name="TOP8" symbol="M900"/>
<gate name="TOP12" symbol="M900"/>
<gate name="TOP13" symbol="M900"/>
<gate name="TOP14" symbol="M900"/>
<gate name="TOP15" symbol="M900"/>
<gate name="TOP16" symbol="M900"/>
<gate name="TOP17" symbol="M900"/>
<gate name="TOP18" symbol="M900"/>
<gate name="BOT1" symbol="M900"/>
<gate name="BOT2" symbol="M900"/>
<gate name="BOT3" symbol="M900"/>
<gate name="BOT4" symbol="M900"/>
<gate name="BOT5" symbol="M900"/>
<gate name="BOT6" symbol="M900"/>
<gate name="BOT9" symbol="M900"/>
<gate name="BOT11" symbol="M900"/>
<gate name="BOT12" symbol="M900"/>
<gate name="BOT14" symbol="M900"/>
<gate name="BOT15" symbol="M900"/>
<gate name="BOT16" symbol="M900"/>
<gate name="BOT17" symbol="M900"/>
<gate name="BOT18" symbol="M900"/>
<gate name="BOT19" symbol="M900"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="BOT1" pin="1" pad="M2"/>
<connect gate="BOT11" pin="1" pad="D2"/>
<connect gate="BOT12" pin="1" pad="E2"/>
<connect gate="BOT14" pin="1" pad="N1"/>
<connect gate="BOT15" pin="1" pad="H1"/>
<connect gate="BOT16" pin="1" pad="B1"/>
<connect gate="BOT17" pin="1" pad="A1"/>
<connect gate="BOT18" pin="1" pad="E1"/>
<connect gate="BOT19" pin="1" pad="D1"/>
<connect gate="BOT2" pin="1" pad="T2"/>
<connect gate="BOT3" pin="1" pad="P1"/>
<connect gate="BOT4" pin="1" pad="R2"/>
<connect gate="BOT5" pin="1" pad="S1"/>
<connect gate="BOT6" pin="1" pad="L2"/>
<connect gate="BOT9" pin="1" pad="H2"/>
<connect gate="G$31" pin="GND" pad="T1"/>
<connect gate="G$32" pin="GND" pad="C2"/>
<connect gate="G$32" pin="VCC" pad="A2"/>
<connect gate="TOP1" pin="1" pad="J2"/>
<connect gate="TOP12" pin="1" pad="J1"/>
<connect gate="TOP13" pin="1" pad="N2"/>
<connect gate="TOP14" pin="1" pad="C1"/>
<connect gate="TOP15" pin="1" pad="L1"/>
<connect gate="TOP16" pin="1" pad="K1"/>
<connect gate="TOP17" pin="1" pad="M1"/>
<connect gate="TOP18" pin="1" pad="F1"/>
<connect gate="TOP2" pin="1" pad="U2"/>
<connect gate="TOP3" pin="1" pad="R1"/>
<connect gate="TOP4" pin="1" pad="V2"/>
<connect gate="TOP5" pin="1" pad="S2"/>
<connect gate="TOP6" pin="1" pad="P2"/>
<connect gate="TOP7" pin="1" pad="K2"/>
<connect gate="TOP8" pin="1" pad="F2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M002.DEV" prefix="W005_" uservalue="yes">
<description>15 Clamped Loads</description>
<gates>
<gate name="G$1" symbol="W005A"/>
<gate name="G$2" symbol="W005A"/>
<gate name="G$3" symbol="W005A"/>
<gate name="G$4" symbol="W005A"/>
<gate name="G$5" symbol="W005A"/>
<gate name="G$6" symbol="W005A"/>
<gate name="G$7" symbol="W005A"/>
<gate name="G$8" symbol="W005A"/>
<gate name="G$9" symbol="W005A"/>
<gate name="G$10" symbol="W005A"/>
<gate name="G$11" symbol="W005A"/>
<gate name="G$12" symbol="W005A"/>
<gate name="G$13" symbol="W005A"/>
<gate name="G$14" symbol="W005A"/>
<gate name="G$15" symbol="W005A"/>
<gate name="G$16" symbol="-15V"/>
<gate name="G$17" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="P$1" pad="D2"/>
<connect gate="G$10" pin="P$1" pad="P2"/>
<connect gate="G$11" pin="P$1" pad="R2"/>
<connect gate="G$12" pin="P$1" pad="S2"/>
<connect gate="G$13" pin="P$1" pad="T2"/>
<connect gate="G$14" pin="P$1" pad="U2"/>
<connect gate="G$15" pin="P$1" pad="V2"/>
<connect gate="G$16" pin="-15V" pad="B2"/>
<connect gate="G$17" pin="GND" pad="C2"/>
<connect gate="G$2" pin="P$1" pad="E2"/>
<connect gate="G$3" pin="P$1" pad="F2"/>
<connect gate="G$4" pin="P$1" pad="H2"/>
<connect gate="G$5" pin="P$1" pad="J2"/>
<connect gate="G$6" pin="P$1" pad="K2"/>
<connect gate="G$7" pin="P$1" pad="L2"/>
<connect gate="G$8" pin="P$1" pad="M2"/>
<connect gate="G$9" pin="P$1" pad="N2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M002" prefix="M002_">
<description>15 Clamped Loads</description>
<gates>
<gate name="D2" symbol="W005A"/>
<gate name="E2" symbol="W005A"/>
<gate name="F2" symbol="W005A"/>
<gate name="H2" symbol="W005A"/>
<gate name="J2" symbol="W005A"/>
<gate name="K2" symbol="W005A"/>
<gate name="L2" symbol="W005A"/>
<gate name="M2" symbol="W005A"/>
<gate name="N2" symbol="W005A"/>
<gate name="P2" symbol="W005A"/>
<gate name="R2" symbol="W005A"/>
<gate name="S2" symbol="W005A"/>
<gate name="T2" symbol="W005A"/>
<gate name="U2" symbol="W005A"/>
<gate name="V2" symbol="W005A"/>
<gate name="G$17" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D2" pin="P$1" pad="D2"/>
<connect gate="E2" pin="P$1" pad="E2"/>
<connect gate="F2" pin="P$1" pad="F2"/>
<connect gate="G$17" pin="GND" pad="C2"/>
<connect gate="G$17" pin="VCC" pad="A2"/>
<connect gate="H2" pin="P$1" pad="H2"/>
<connect gate="J2" pin="P$1" pad="J2"/>
<connect gate="K2" pin="P$1" pad="K2"/>
<connect gate="L2" pin="P$1" pad="L2"/>
<connect gate="M2" pin="P$1" pad="M2"/>
<connect gate="N2" pin="P$1" pad="N2"/>
<connect gate="P2" pin="P$1" pad="P2"/>
<connect gate="R2" pin="P$1" pad="R2"/>
<connect gate="S2" pin="P$1" pad="S2"/>
<connect gate="T2" pin="P$1" pad="T2"/>
<connect gate="U2" pin="P$1" pad="U2"/>
<connect gate="V2" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M624" prefix="M624_">
<description>&lt;qt&gt;&lt;b&gt;Bus Data Interface&lt;/b&gt;
&lt;p&gt;
The M101 contains 15 two-input NAND gates.  One input of each gate is tied to a common line so that all data signals can be enabled simultaneously.  &lt;p&gt;Each data signal presents one TTL load.  The common input presents 15 loads. &lt;p&gt; Each output can drive 10 loads.&lt;p&gt;
Power: 5V@82ma (max.)
&lt;/qt&gt;</description>
<gates>
<gate name="G$16" symbol="POWER"/>
<gate name="G$1" symbol="T1GND"/>
<gate name="V2" symbol="BUFFER"/>
<gate name="B1" symbol="OR2"/>
<gate name="E1" symbol="OR1C"/>
<gate name="F2" symbol="OR1C"/>
<gate name="J2" symbol="OR1C"/>
<gate name="L2" symbol="OR1C"/>
<gate name="K1" symbol="OR1C"/>
<gate name="M1" symbol="OR1C"/>
<gate name="P1" symbol="OR1C"/>
<gate name="S1" symbol="OR1C"/>
<gate name="U1" symbol="OR1C"/>
<gate name="H1" symbol="OR1C"/>
<gate name="N2" symbol="OR1C"/>
<gate name="R2" symbol="OR2"/>
<gate name="T2" symbol="OR1D"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="B1" pin="IN1" pad="A1"/>
<connect gate="B1" pin="IN2" pad="C1"/>
<connect gate="B1" pin="OUT" pad="B1"/>
<connect gate="E1" pin="IN" pad="D1"/>
<connect gate="E1" pin="OUT" pad="E1"/>
<connect gate="F2" pin="IN" pad="E2"/>
<connect gate="F2" pin="OUT" pad="F2"/>
<connect gate="G$1" pin="GND" pad="T1"/>
<connect gate="G$16" pin="GND" pad="C2"/>
<connect gate="G$16" pin="VCC" pad="A2"/>
<connect gate="H1" pin="IN" pad="F1"/>
<connect gate="H1" pin="OUT" pad="H1"/>
<connect gate="J2" pin="IN" pad="H2"/>
<connect gate="J2" pin="OUT" pad="J2"/>
<connect gate="K1" pin="IN" pad="J1"/>
<connect gate="K1" pin="OUT" pad="K1"/>
<connect gate="L2" pin="IN" pad="K2"/>
<connect gate="L2" pin="OUT" pad="L2"/>
<connect gate="M1" pin="IN" pad="L1"/>
<connect gate="M1" pin="OUT" pad="M1"/>
<connect gate="N2" pin="IN" pad="M2"/>
<connect gate="N2" pin="OUT" pad="N2"/>
<connect gate="P1" pin="IN" pad="N1"/>
<connect gate="P1" pin="OUT" pad="P1"/>
<connect gate="R2" pin="IN1" pad="P2"/>
<connect gate="R2" pin="IN2" pad="D2"/>
<connect gate="R2" pin="OUT" pad="R2"/>
<connect gate="S1" pin="IN" pad="R1"/>
<connect gate="S1" pin="OUT" pad="S1"/>
<connect gate="T2" pin="IN" pad="S2"/>
<connect gate="T2" pin="OUT" pad="T2"/>
<connect gate="U1" pin="IN" pad="V1"/>
<connect gate="U1" pin="OUT" pad="U1"/>
<connect gate="V2" pin="IN" pad="U2"/>
<connect gate="V2" pin="OUT" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R401" prefix="R401_">
<description>Variable Frequency Clock</description>
<gates>
<gate name="D" symbol="R401"/>
<gate name="G$2" symbol="-15V"/>
<gate name="G$3" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="D" pad="D2"/>
<connect gate="D" pin="F" pad="F2"/>
<connect gate="D" pin="H" pad="H2"/>
<connect gate="D" pin="L" pad="L2"/>
<connect gate="D" pin="M" pad="M2"/>
<connect gate="D" pin="N" pad="N2"/>
<connect gate="D" pin="P" pad="P2"/>
<connect gate="D" pin="R" pad="R2"/>
<connect gate="D" pin="S" pad="S2"/>
<connect gate="D" pin="T" pad="T2"/>
<connect gate="D" pin="U" pad="U2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="D" pin="D" pad="D2"/>
<connect gate="D" pin="F" pad="F2"/>
<connect gate="D" pin="H" pad="H2"/>
<connect gate="D" pin="L" pad="L2"/>
<connect gate="D" pin="M" pad="M2"/>
<connect gate="D" pin="N" pad="N2"/>
<connect gate="D" pin="P" pad="P2"/>
<connect gate="D" pin="R" pad="R2"/>
<connect gate="D" pin="S" pad="S2"/>
<connect gate="D" pin="T" pad="T2"/>
<connect gate="D" pin="U" pad="U2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="D" pad="D2"/>
<connect gate="D" pin="F" pad="F2"/>
<connect gate="D" pin="H" pad="H2"/>
<connect gate="D" pin="L" pad="L2"/>
<connect gate="D" pin="M" pad="M2"/>
<connect gate="D" pin="N" pad="N2"/>
<connect gate="D" pin="P" pad="P2"/>
<connect gate="D" pin="R" pad="R2"/>
<connect gate="D" pin="S" pad="S2"/>
<connect gate="D" pin="T" pad="T2"/>
<connect gate="D" pin="U" pad="U2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R202" prefix="R202_">
<description>Dual Flip-Flop</description>
<gates>
<gate name="J" symbol="R202A"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="-15V"/>
<gate name="T" symbol="R202B"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="J" pin="0" pad="H2"/>
<connect gate="J" pin="1" pad="J2"/>
<connect gate="J" pin="EN0" pad="E2"/>
<connect gate="J" pin="EN1" pad="L2"/>
<connect gate="J" pin="PU0" pad="D2"/>
<connect gate="J" pin="PU1" pad="K2"/>
<connect gate="J" pin="RESET" pad="F2"/>
<connect gate="J" pin="SET" pad="M2"/>
<connect gate="T" pin="0" pad="S2"/>
<connect gate="T" pin="1" pad="T2"/>
<connect gate="T" pin="EN0" pad="P2"/>
<connect gate="T" pin="EN1" pad="V2"/>
<connect gate="T" pin="PU0" pad="N2"/>
<connect gate="T" pin="PU1" pad="U2"/>
<connect gate="T" pin="RESET" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="J" pin="0" pad="H2"/>
<connect gate="J" pin="1" pad="J2"/>
<connect gate="J" pin="EN0" pad="E2"/>
<connect gate="J" pin="EN1" pad="L2"/>
<connect gate="J" pin="PU0" pad="D2"/>
<connect gate="J" pin="PU1" pad="K2"/>
<connect gate="J" pin="RESET" pad="F2"/>
<connect gate="J" pin="SET" pad="M2"/>
<connect gate="T" pin="0" pad="S2"/>
<connect gate="T" pin="1" pad="T2"/>
<connect gate="T" pin="EN0" pad="P2"/>
<connect gate="T" pin="EN1" pad="V2"/>
<connect gate="T" pin="PU0" pad="N2"/>
<connect gate="T" pin="PU1" pad="U2"/>
<connect gate="T" pin="RESET" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="J" pin="0" pad="H2"/>
<connect gate="J" pin="1" pad="J2"/>
<connect gate="J" pin="EN0" pad="E2"/>
<connect gate="J" pin="EN1" pad="L2"/>
<connect gate="J" pin="PU0" pad="D2"/>
<connect gate="J" pin="PU1" pad="K2"/>
<connect gate="J" pin="RESET" pad="F2"/>
<connect gate="J" pin="SET" pad="M2"/>
<connect gate="T" pin="0" pad="S2"/>
<connect gate="T" pin="1" pad="T2"/>
<connect gate="T" pin="EN0" pad="P2"/>
<connect gate="T" pin="EN1" pad="V2"/>
<connect gate="T" pin="PU0" pad="N2"/>
<connect gate="T" pin="PU1" pad="U2"/>
<connect gate="T" pin="RESET" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R113" prefix="R113_">
<description>Diode Gate</description>
<gates>
<gate name="F" symbol="R113"/>
<gate name="K" symbol="R113"/>
<gate name="N" symbol="R113"/>
<gate name="S" symbol="R113"/>
<gate name="V" symbol="R113"/>
<gate name="G$7" symbol="-15V"/>
<gate name="G$8" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="F" pin="I$1" pad="D2"/>
<connect gate="F" pin="I$2" pad="E2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="K" pin="I$1" pad="H2"/>
<connect gate="K" pin="I$2" pad="J2"/>
<connect gate="K" pin="O$1" pad="K2"/>
<connect gate="N" pin="I$1" pad="L2"/>
<connect gate="N" pin="I$2" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="S" pin="I$1" pad="P2"/>
<connect gate="S" pin="I$2" pad="R2"/>
<connect gate="S" pin="O$1" pad="S2"/>
<connect gate="V" pin="I$1" pad="T2"/>
<connect gate="V" pin="I$2" pad="U2"/>
<connect gate="V" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="F" pin="I$1" pad="D2"/>
<connect gate="F" pin="I$2" pad="E2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="K" pin="I$1" pad="H2"/>
<connect gate="K" pin="I$2" pad="J2"/>
<connect gate="K" pin="O$1" pad="K2"/>
<connect gate="N" pin="I$1" pad="L2"/>
<connect gate="N" pin="I$2" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="S" pin="I$1" pad="P2"/>
<connect gate="S" pin="I$2" pad="R2"/>
<connect gate="S" pin="O$1" pad="S2"/>
<connect gate="V" pin="I$1" pad="T2"/>
<connect gate="V" pin="I$2" pad="U2"/>
<connect gate="V" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="F" pin="I$1" pad="D2"/>
<connect gate="F" pin="I$2" pad="E2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="K" pin="I$1" pad="H2"/>
<connect gate="K" pin="I$2" pad="J2"/>
<connect gate="K" pin="O$1" pad="K2"/>
<connect gate="N" pin="I$1" pad="L2"/>
<connect gate="N" pin="I$2" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="S" pin="I$1" pad="P2"/>
<connect gate="S" pin="I$2" pad="R2"/>
<connect gate="S" pin="O$1" pad="S2"/>
<connect gate="V" pin="I$1" pad="T2"/>
<connect gate="V" pin="I$2" pad="U2"/>
<connect gate="V" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R107" prefix="R107_">
<description>7 Inverters</description>
<gates>
<gate name="D" symbol="R107A"/>
<gate name="F" symbol="R107A"/>
<gate name="J" symbol="R107A"/>
<gate name="L" symbol="R107A"/>
<gate name="N" symbol="R107A"/>
<gate name="R" symbol="R107A"/>
<gate name="G$8" symbol="-15V"/>
<gate name="G$9" symbol="POWER"/>
<gate name="T" symbol="R107B"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="I$1" pad="E2"/>
<connect gate="D" pin="O$1" pad="D2"/>
<connect gate="F" pin="I$1" pad="H2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="J" pin="I$1" pad="K2"/>
<connect gate="J" pin="O$1" pad="J2"/>
<connect gate="L" pin="I$1" pad="M2"/>
<connect gate="L" pin="O$1" pad="L2"/>
<connect gate="N" pin="I$1" pad="P2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="R" pin="I$1" pad="S2"/>
<connect gate="R" pin="O$1" pad="R2"/>
<connect gate="T" pin="I$1" pad="U2"/>
<connect gate="T" pin="I$2" pad="V2"/>
<connect gate="T" pin="O$1" pad="T2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="D" pin="I$1" pad="E2"/>
<connect gate="D" pin="O$1" pad="D2"/>
<connect gate="F" pin="I$1" pad="H2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="J" pin="I$1" pad="K2"/>
<connect gate="J" pin="O$1" pad="J2"/>
<connect gate="L" pin="I$1" pad="M2"/>
<connect gate="L" pin="O$1" pad="L2"/>
<connect gate="N" pin="I$1" pad="P2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="R" pin="I$1" pad="S2"/>
<connect gate="R" pin="O$1" pad="R2"/>
<connect gate="T" pin="I$1" pad="U2"/>
<connect gate="T" pin="I$2" pad="V2"/>
<connect gate="T" pin="O$1" pad="T2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="I$1" pad="E2"/>
<connect gate="D" pin="O$1" pad="D2"/>
<connect gate="F" pin="I$1" pad="H2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="J" pin="I$1" pad="K2"/>
<connect gate="J" pin="O$1" pad="J2"/>
<connect gate="L" pin="I$1" pad="M2"/>
<connect gate="L" pin="O$1" pad="L2"/>
<connect gate="N" pin="I$1" pad="P2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="R" pin="I$1" pad="S2"/>
<connect gate="R" pin="O$1" pad="R2"/>
<connect gate="T" pin="I$1" pad="U2"/>
<connect gate="T" pin="I$2" pad="V2"/>
<connect gate="T" pin="O$1" pad="T2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R111" prefix="R111_">
<description>Diode Gate</description>
<gates>
<gate name="H" symbol="R111"/>
<gate name="N" symbol="R111"/>
<gate name="U" symbol="R111"/>
<gate name="J" symbol="W005A"/>
<gate name="P" symbol="W005A"/>
<gate name="V" symbol="W005A"/>
<gate name="G$7" symbol="-15V"/>
<gate name="G$8" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="H" pin="I$1" pad="D2"/>
<connect gate="H" pin="I$2" pad="E2"/>
<connect gate="H" pin="I$3" pad="F2"/>
<connect gate="H" pin="O$1" pad="H2"/>
<connect gate="J" pin="P$1" pad="J2"/>
<connect gate="N" pin="I$1" pad="K2"/>
<connect gate="N" pin="I$2" pad="L2"/>
<connect gate="N" pin="I$3" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="P" pin="P$1" pad="P2"/>
<connect gate="U" pin="I$1" pad="R2"/>
<connect gate="U" pin="I$2" pad="S2"/>
<connect gate="U" pin="I$3" pad="T2"/>
<connect gate="U" pin="O$1" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="H" pin="I$1" pad="D2"/>
<connect gate="H" pin="I$2" pad="E2"/>
<connect gate="H" pin="I$3" pad="F2"/>
<connect gate="H" pin="O$1" pad="H2"/>
<connect gate="J" pin="P$1" pad="J2"/>
<connect gate="N" pin="I$1" pad="K2"/>
<connect gate="N" pin="I$2" pad="L2"/>
<connect gate="N" pin="I$3" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="P" pin="P$1" pad="P2"/>
<connect gate="U" pin="I$1" pad="R2"/>
<connect gate="U" pin="I$2" pad="S2"/>
<connect gate="U" pin="I$3" pad="T2"/>
<connect gate="U" pin="O$1" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="H" pin="I$1" pad="D2"/>
<connect gate="H" pin="I$2" pad="E2"/>
<connect gate="H" pin="I$3" pad="F2"/>
<connect gate="H" pin="O$1" pad="H2"/>
<connect gate="J" pin="P$1" pad="J2"/>
<connect gate="N" pin="I$1" pad="K2"/>
<connect gate="N" pin="I$2" pad="L2"/>
<connect gate="N" pin="I$3" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="P" pin="P$1" pad="P2"/>
<connect gate="U" pin="I$1" pad="R2"/>
<connect gate="U" pin="I$2" pad="S2"/>
<connect gate="U" pin="I$3" pad="T2"/>
<connect gate="U" pin="O$1" pad="U2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R603" prefix="R603_">
<description>Triple Pulse Amplifier</description>
<gates>
<gate name="F" symbol="R603"/>
<gate name="M" symbol="R603"/>
<gate name="T" symbol="R603"/>
<gate name="G$4" symbol="-15V"/>
<gate name="G$5" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="F" pin="EN0" pad="E2"/>
<connect gate="F" pin="G" pad="H2"/>
<connect gate="F" pin="I$1" pad="J2"/>
<connect gate="F" pin="O" pad="F2"/>
<connect gate="F" pin="PU0" pad="D2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="M" pin="EN0" pad="L2"/>
<connect gate="M" pin="G" pad="N2"/>
<connect gate="M" pin="I$1" pad="P2"/>
<connect gate="M" pin="O" pad="M2"/>
<connect gate="M" pin="PU0" pad="K2"/>
<connect gate="T" pin="EN0" pad="S2"/>
<connect gate="T" pin="G" pad="U2"/>
<connect gate="T" pin="I$1" pad="V2"/>
<connect gate="T" pin="O" pad="T2"/>
<connect gate="T" pin="PU0" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="F" pin="EN0" pad="E2"/>
<connect gate="F" pin="G" pad="H2"/>
<connect gate="F" pin="I$1" pad="J2"/>
<connect gate="F" pin="O" pad="F2"/>
<connect gate="F" pin="PU0" pad="D2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="M" pin="EN0" pad="L2"/>
<connect gate="M" pin="G" pad="N2"/>
<connect gate="M" pin="I$1" pad="P2"/>
<connect gate="M" pin="O" pad="M2"/>
<connect gate="M" pin="PU0" pad="K2"/>
<connect gate="T" pin="EN0" pad="S2"/>
<connect gate="T" pin="G" pad="U2"/>
<connect gate="T" pin="I$1" pad="V2"/>
<connect gate="T" pin="O" pad="T2"/>
<connect gate="T" pin="PU0" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="F" pin="EN0" pad="E2"/>
<connect gate="F" pin="G" pad="H2"/>
<connect gate="F" pin="I$1" pad="J2"/>
<connect gate="F" pin="O" pad="F2"/>
<connect gate="F" pin="PU0" pad="D2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="M" pin="EN0" pad="L2"/>
<connect gate="M" pin="G" pad="N2"/>
<connect gate="M" pin="I$1" pad="P2"/>
<connect gate="M" pin="O" pad="M2"/>
<connect gate="M" pin="PU0" pad="K2"/>
<connect gate="T" pin="EN0" pad="S2"/>
<connect gate="T" pin="G" pad="U2"/>
<connect gate="T" pin="I$1" pad="V2"/>
<connect gate="T" pin="O" pad="T2"/>
<connect gate="T" pin="PU0" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R602" prefix="R602_">
<description>Dual Pulse Amplifier</description>
<gates>
<gate name="K" symbol="R602A"/>
<gate name="U" symbol="R602B"/>
<gate name="G$3" symbol="-15V"/>
<gate name="G$4" symbol="VCC"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="K" pin="D" pad="D2"/>
<connect gate="K" pin="E" pad="E2"/>
<connect gate="K" pin="F" pad="F2"/>
<connect gate="K" pin="GND" pad="C2"/>
<connect gate="K" pin="H" pad="H2"/>
<connect gate="K" pin="J" pad="J2"/>
<connect gate="K" pin="K" pad="K2"/>
<connect gate="K" pin="L" pad="L2"/>
<connect gate="K" pin="M" pad="M2"/>
<connect gate="U" pin="C" pad="N2"/>
<connect gate="U" pin="E" pad="P2"/>
<connect gate="U" pin="F" pad="R2"/>
<connect gate="U" pin="H" pad="S2"/>
<connect gate="U" pin="J" pad="T2"/>
<connect gate="U" pin="K" pad="U2"/>
<connect gate="U" pin="L" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="K" pin="D" pad="D2"/>
<connect gate="K" pin="E" pad="E2"/>
<connect gate="K" pin="F" pad="F2"/>
<connect gate="K" pin="GND" pad="C2"/>
<connect gate="K" pin="H" pad="H2"/>
<connect gate="K" pin="J" pad="J2"/>
<connect gate="K" pin="K" pad="K2"/>
<connect gate="K" pin="L" pad="L2"/>
<connect gate="K" pin="M" pad="M2"/>
<connect gate="U" pin="C" pad="N2"/>
<connect gate="U" pin="E" pad="P2"/>
<connect gate="U" pin="F" pad="R2"/>
<connect gate="U" pin="H" pad="S2"/>
<connect gate="U" pin="J" pad="T2"/>
<connect gate="U" pin="K" pad="U2"/>
<connect gate="U" pin="L" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="K" pin="D" pad="D2"/>
<connect gate="K" pin="E" pad="E2"/>
<connect gate="K" pin="F" pad="F2"/>
<connect gate="K" pin="GND" pad="C2"/>
<connect gate="K" pin="H" pad="H2"/>
<connect gate="K" pin="J" pad="J2"/>
<connect gate="K" pin="K" pad="K2"/>
<connect gate="K" pin="L" pad="L2"/>
<connect gate="K" pin="M" pad="M2"/>
<connect gate="U" pin="C" pad="N2"/>
<connect gate="U" pin="E" pad="P2"/>
<connect gate="U" pin="F" pad="R2"/>
<connect gate="U" pin="H" pad="S2"/>
<connect gate="U" pin="J" pad="T2"/>
<connect gate="U" pin="K" pad="U2"/>
<connect gate="U" pin="L" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R302" prefix="R302_">
<description>Dual Delay (One Shot)</description>
<gates>
<gate name="M" symbol="R302"/>
<gate name="V" symbol="R302"/>
<gate name="G$3" symbol="-15V"/>
<gate name="G$4" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="M" pin="E" pad="E2"/>
<connect gate="M" pin="F" pad="F2"/>
<connect gate="M" pin="H" pad="H2"/>
<connect gate="M" pin="J" pad="J2"/>
<connect gate="M" pin="K" pad="K2"/>
<connect gate="M" pin="L" pad="L2"/>
<connect gate="M" pin="M" pad="M2"/>
<connect gate="V" pin="E" pad="N2"/>
<connect gate="V" pin="F" pad="P2"/>
<connect gate="V" pin="H" pad="R2"/>
<connect gate="V" pin="J" pad="S2"/>
<connect gate="V" pin="K" pad="T2"/>
<connect gate="V" pin="L" pad="U2"/>
<connect gate="V" pin="M" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="M" pin="E" pad="E2"/>
<connect gate="M" pin="F" pad="F2"/>
<connect gate="M" pin="H" pad="H2"/>
<connect gate="M" pin="J" pad="J2"/>
<connect gate="M" pin="K" pad="K2"/>
<connect gate="M" pin="L" pad="L2"/>
<connect gate="M" pin="M" pad="M2"/>
<connect gate="V" pin="E" pad="N2"/>
<connect gate="V" pin="F" pad="P2"/>
<connect gate="V" pin="H" pad="R2"/>
<connect gate="V" pin="J" pad="S2"/>
<connect gate="V" pin="K" pad="T2"/>
<connect gate="V" pin="L" pad="U2"/>
<connect gate="V" pin="M" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="M" pin="E" pad="E2"/>
<connect gate="M" pin="F" pad="F2"/>
<connect gate="M" pin="H" pad="H2"/>
<connect gate="M" pin="J" pad="J2"/>
<connect gate="M" pin="K" pad="K2"/>
<connect gate="M" pin="L" pad="L2"/>
<connect gate="M" pin="M" pad="M2"/>
<connect gate="V" pin="E" pad="N2"/>
<connect gate="V" pin="F" pad="P2"/>
<connect gate="V" pin="H" pad="R2"/>
<connect gate="V" pin="J" pad="S2"/>
<connect gate="V" pin="K" pad="T2"/>
<connect gate="V" pin="L" pad="U2"/>
<connect gate="V" pin="M" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R151" prefix="R151_">
<description>Binary-to-Octal Decoder</description>
<gates>
<gate name="M" symbol="R151"/>
<gate name="G$2" symbol="-15V"/>
<gate name="G$3" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="M" pin="D" pad="D2"/>
<connect gate="M" pin="E" pad="E2"/>
<connect gate="M" pin="F" pad="F2"/>
<connect gate="M" pin="H" pad="H2"/>
<connect gate="M" pin="J" pad="J2"/>
<connect gate="M" pin="K" pad="K2"/>
<connect gate="M" pin="L" pad="L2"/>
<connect gate="M" pin="M" pad="M2"/>
<connect gate="M" pin="N" pad="N2"/>
<connect gate="M" pin="P" pad="P2"/>
<connect gate="M" pin="R" pad="R2"/>
<connect gate="M" pin="S" pad="S2"/>
<connect gate="M" pin="T" pad="T2"/>
<connect gate="M" pin="U" pad="U2"/>
<connect gate="M" pin="V" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="M" pin="D" pad="D2"/>
<connect gate="M" pin="E" pad="E2"/>
<connect gate="M" pin="F" pad="F2"/>
<connect gate="M" pin="H" pad="H2"/>
<connect gate="M" pin="J" pad="J2"/>
<connect gate="M" pin="K" pad="K2"/>
<connect gate="M" pin="L" pad="L2"/>
<connect gate="M" pin="M" pad="M2"/>
<connect gate="M" pin="N" pad="N2"/>
<connect gate="M" pin="P" pad="P2"/>
<connect gate="M" pin="R" pad="R2"/>
<connect gate="M" pin="S" pad="S2"/>
<connect gate="M" pin="T" pad="T2"/>
<connect gate="M" pin="U" pad="U2"/>
<connect gate="M" pin="V" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="M" pin="D" pad="D2"/>
<connect gate="M" pin="E" pad="E2"/>
<connect gate="M" pin="F" pad="F2"/>
<connect gate="M" pin="H" pad="H2"/>
<connect gate="M" pin="J" pad="J2"/>
<connect gate="M" pin="K" pad="K2"/>
<connect gate="M" pin="L" pad="L2"/>
<connect gate="M" pin="M" pad="M2"/>
<connect gate="M" pin="N" pad="N2"/>
<connect gate="M" pin="P" pad="P2"/>
<connect gate="M" pin="R" pad="R2"/>
<connect gate="M" pin="S" pad="S2"/>
<connect gate="M" pin="T" pad="T2"/>
<connect gate="M" pin="U" pad="U2"/>
<connect gate="M" pin="V" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R002" prefix="R002_">
<description>5 Diode Networks</description>
<gates>
<gate name="F" symbol="R002"/>
<gate name="K" symbol="R002"/>
<gate name="N" symbol="R002"/>
<gate name="S" symbol="R002"/>
<gate name="V" symbol="R002"/>
<gate name="G$6" symbol="-15V"/>
<gate name="G$7" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="F" pin="D" pad="D2"/>
<connect gate="F" pin="E" pad="E2"/>
<connect gate="F" pin="F" pad="F2"/>
<connect gate="G$6" pin="-15V" pad="B2"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="K" pin="D" pad="H2"/>
<connect gate="K" pin="E" pad="J2"/>
<connect gate="K" pin="F" pad="K2"/>
<connect gate="N" pin="D" pad="L2"/>
<connect gate="N" pin="E" pad="M2"/>
<connect gate="N" pin="F" pad="N2"/>
<connect gate="S" pin="D" pad="P2"/>
<connect gate="S" pin="E" pad="R2"/>
<connect gate="S" pin="F" pad="S2"/>
<connect gate="V" pin="D" pad="T2"/>
<connect gate="V" pin="E" pad="U2"/>
<connect gate="V" pin="F" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="F" pin="D" pad="D2"/>
<connect gate="F" pin="E" pad="E2"/>
<connect gate="F" pin="F" pad="F2"/>
<connect gate="G$6" pin="-15V" pad="B2"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="K" pin="D" pad="H2"/>
<connect gate="K" pin="E" pad="J2"/>
<connect gate="K" pin="F" pad="K2"/>
<connect gate="N" pin="D" pad="L2"/>
<connect gate="N" pin="E" pad="M2"/>
<connect gate="N" pin="F" pad="N2"/>
<connect gate="S" pin="D" pad="P2"/>
<connect gate="S" pin="E" pad="R2"/>
<connect gate="S" pin="F" pad="S2"/>
<connect gate="V" pin="D" pad="T2"/>
<connect gate="V" pin="E" pad="U2"/>
<connect gate="V" pin="F" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="F" pin="D" pad="D2"/>
<connect gate="F" pin="E" pad="E2"/>
<connect gate="F" pin="F" pad="F2"/>
<connect gate="G$6" pin="-15V" pad="B2"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="K" pin="D" pad="H2"/>
<connect gate="K" pin="E" pad="J2"/>
<connect gate="K" pin="F" pad="K2"/>
<connect gate="N" pin="D" pad="L2"/>
<connect gate="N" pin="E" pad="M2"/>
<connect gate="N" pin="F" pad="N2"/>
<connect gate="S" pin="D" pad="P2"/>
<connect gate="S" pin="E" pad="R2"/>
<connect gate="S" pin="F" pad="S2"/>
<connect gate="V" pin="D" pad="T2"/>
<connect gate="V" pin="E" pad="U2"/>
<connect gate="V" pin="F" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R001" prefix="R001_">
<description>7 Diodes</description>
<gates>
<gate name="E" symbol="R001"/>
<gate name="H" symbol="R001"/>
<gate name="K" symbol="R001"/>
<gate name="M" symbol="R001"/>
<gate name="P" symbol="R001"/>
<gate name="S" symbol="R001"/>
<gate name="U" symbol="R001"/>
<gate name="G$8" symbol="-15V"/>
<gate name="G$9" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="E" pin="D" pad="D2"/>
<connect gate="E" pin="E" pad="E2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="H" pin="D" pad="F2"/>
<connect gate="H" pin="E" pad="H2"/>
<connect gate="K" pin="D" pad="J2"/>
<connect gate="K" pin="E" pad="K2"/>
<connect gate="M" pin="D" pad="L2"/>
<connect gate="M" pin="E" pad="M2"/>
<connect gate="P" pin="D" pad="N2"/>
<connect gate="P" pin="E" pad="P2"/>
<connect gate="S" pin="D" pad="R2"/>
<connect gate="S" pin="E" pad="S2"/>
<connect gate="U" pin="D" pad="T2"/>
<connect gate="U" pin="E" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="E" pin="D" pad="D2"/>
<connect gate="E" pin="E" pad="E2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="H" pin="D" pad="F2"/>
<connect gate="H" pin="E" pad="H2"/>
<connect gate="K" pin="D" pad="J2"/>
<connect gate="K" pin="E" pad="K2"/>
<connect gate="M" pin="D" pad="L2"/>
<connect gate="M" pin="E" pad="M2"/>
<connect gate="P" pin="D" pad="N2"/>
<connect gate="P" pin="E" pad="P2"/>
<connect gate="S" pin="D" pad="R2"/>
<connect gate="S" pin="E" pad="S2"/>
<connect gate="U" pin="D" pad="T2"/>
<connect gate="U" pin="E" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="E" pin="D" pad="D2"/>
<connect gate="E" pin="E" pad="E2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="H" pin="D" pad="F2"/>
<connect gate="H" pin="E" pad="H2"/>
<connect gate="K" pin="D" pad="J2"/>
<connect gate="K" pin="E" pad="K2"/>
<connect gate="M" pin="D" pad="L2"/>
<connect gate="M" pin="E" pad="M2"/>
<connect gate="P" pin="D" pad="N2"/>
<connect gate="P" pin="E" pad="P2"/>
<connect gate="S" pin="D" pad="R2"/>
<connect gate="S" pin="E" pad="S2"/>
<connect gate="U" pin="D" pad="T2"/>
<connect gate="U" pin="E" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W050" prefix="W050_">
<description>Indicator Driver</description>
<gates>
<gate name="F" symbol="W050"/>
<gate name="J" symbol="W050"/>
<gate name="L" symbol="W050"/>
<gate name="N" symbol="W050"/>
<gate name="R" symbol="W050"/>
<gate name="T" symbol="W050"/>
<gate name="V" symbol="W050"/>
<gate name="G$8" symbol="-15V"/>
<gate name="G$9" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="F" pin="I$1" pad="E2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="J" pin="I$1" pad="H2"/>
<connect gate="J" pin="O$1" pad="J2"/>
<connect gate="L" pin="I$1" pad="K2"/>
<connect gate="L" pin="O$1" pad="L2"/>
<connect gate="N" pin="I$1" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="R" pin="I$1" pad="P2"/>
<connect gate="R" pin="O$1" pad="R2"/>
<connect gate="T" pin="I$1" pad="S2"/>
<connect gate="T" pin="O$1" pad="T2"/>
<connect gate="V" pin="I$1" pad="U2"/>
<connect gate="V" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="F" pin="I$1" pad="E2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="J" pin="I$1" pad="H2"/>
<connect gate="J" pin="O$1" pad="J2"/>
<connect gate="L" pin="I$1" pad="K2"/>
<connect gate="L" pin="O$1" pad="L2"/>
<connect gate="N" pin="I$1" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="R" pin="I$1" pad="P2"/>
<connect gate="R" pin="O$1" pad="R2"/>
<connect gate="T" pin="I$1" pad="S2"/>
<connect gate="T" pin="O$1" pad="T2"/>
<connect gate="V" pin="I$1" pad="U2"/>
<connect gate="V" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="F" pin="I$1" pad="E2"/>
<connect gate="F" pin="O$1" pad="F2"/>
<connect gate="G$8" pin="-15V" pad="B2"/>
<connect gate="G$9" pin="GND" pad="C2"/>
<connect gate="G$9" pin="VCC" pad="A2"/>
<connect gate="J" pin="I$1" pad="H2"/>
<connect gate="J" pin="O$1" pad="J2"/>
<connect gate="L" pin="I$1" pad="K2"/>
<connect gate="L" pin="O$1" pad="L2"/>
<connect gate="N" pin="I$1" pad="M2"/>
<connect gate="N" pin="O$1" pad="N2"/>
<connect gate="R" pin="I$1" pad="P2"/>
<connect gate="R" pin="O$1" pad="R2"/>
<connect gate="T" pin="I$1" pad="S2"/>
<connect gate="T" pin="O$1" pad="T2"/>
<connect gate="V" pin="I$1" pad="U2"/>
<connect gate="V" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W028" prefix="W028_">
<description>One-sided 9 pin connector/cable with grounds (Negibus).</description>
<gates>
<gate name="D" symbol="PIN"/>
<gate name="E" symbol="PIN"/>
<gate name="H" symbol="PIN"/>
<gate name="K" symbol="PIN"/>
<gate name="M" symbol="PIN"/>
<gate name="P" symbol="PIN"/>
<gate name="S" symbol="PIN"/>
<gate name="T" symbol="PIN"/>
<gate name="V" symbol="PIN"/>
<gate name="G$1" symbol="T1GND"/>
<gate name="G$2" symbol="T1GND"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="G$6" symbol="T1GND"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="G$10" symbol="T1GND"/>
<gate name="G$12" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W021" prefix="W021_">
<description>One-sided 9 pin connector/cable with grounds (Negibus).</description>
<gates>
<gate name="D" symbol="PIN"/>
<gate name="E" symbol="PIN"/>
<gate name="H" symbol="PIN"/>
<gate name="K" symbol="PIN"/>
<gate name="M" symbol="PIN"/>
<gate name="P" symbol="PIN"/>
<gate name="S" symbol="PIN"/>
<gate name="T" symbol="PIN"/>
<gate name="V" symbol="PIN"/>
<gate name="G$1" symbol="T1GND"/>
<gate name="G$2" symbol="T1GND"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="G$6" symbol="T1GND"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="G$10" symbol="T1GND"/>
<gate name="G$12" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="P$2" pad="D2"/>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$10" pin="GND" pad="R2"/>
<connect gate="G$12" pin="GND" pad="U2"/>
<connect gate="G$2" pin="GND" pad="F2"/>
<connect gate="G$3" pin="GND" pad="J2"/>
<connect gate="G$6" pin="GND" pad="L2"/>
<connect gate="G$8" pin="GND" pad="N2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="P" pin="P$2" pad="P2"/>
<connect gate="S" pin="P$2" pad="S2"/>
<connect gate="T" pin="P$2" pad="T2"/>
<connect gate="V" pin="P$2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W506" prefix="W506_">
<description>Power Monitor</description>
<gates>
<gate name="A" symbol="W506"/>
<gate name="G$2" symbol="-15V"/>
<gate name="G$3" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="A" pin="E" pad="E2"/>
<connect gate="A" pin="F" pad="F2"/>
<connect gate="A" pin="H" pad="H2"/>
<connect gate="A" pin="J" pad="J2"/>
<connect gate="A" pin="K" pad="K2"/>
<connect gate="A" pin="L" pad="L2"/>
<connect gate="A" pin="M" pad="M2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="A" pin="E" pad="E2"/>
<connect gate="A" pin="F" pad="F2"/>
<connect gate="A" pin="H" pad="H2"/>
<connect gate="A" pin="J" pad="J2"/>
<connect gate="A" pin="K" pad="K2"/>
<connect gate="A" pin="L" pad="L2"/>
<connect gate="A" pin="M" pad="M2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="A" pin="E" pad="E2"/>
<connect gate="A" pin="F" pad="F2"/>
<connect gate="A" pin="H" pad="H2"/>
<connect gate="A" pin="J" pad="J2"/>
<connect gate="A" pin="K" pad="K2"/>
<connect gate="A" pin="L" pad="L2"/>
<connect gate="A" pin="M" pad="M2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W501" prefix="W501_">
<description>Negative Input Converter and Schmidt Trigger</description>
<gates>
<gate name="F" symbol="W501A"/>
<gate name="K" symbol="W501B"/>
<gate name="E" symbol="W005A"/>
<gate name="D" symbol="W005A"/>
<gate name="G$4" symbol="-15V"/>
<gate name="G$5" symbol="POWER"/>
<gate name="V" symbol="T1GND"/>
<gate name="T" symbol="W501C"/>
<gate name="U" symbol="W005A"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="P$1" pad="D2"/>
<connect gate="E" pin="P$1" pad="E2"/>
<connect gate="F" pin="F" pad="F2"/>
<connect gate="F" pin="L" pad="L2"/>
<connect gate="F" pin="M" pad="M2"/>
<connect gate="F" pin="P" pad="P2"/>
<connect gate="F" pin="R" pad="R2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="K" pin="K" pad="K2"/>
<connect gate="K" pin="N" pad="N2"/>
<connect gate="T" pin="S" pad="S2"/>
<connect gate="T" pin="T" pad="T2"/>
<connect gate="U" pin="P$1" pad="U2"/>
<connect gate="V" pin="GND" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="D" pin="P$1" pad="D2"/>
<connect gate="E" pin="P$1" pad="E2"/>
<connect gate="F" pin="F" pad="F2"/>
<connect gate="F" pin="L" pad="L2"/>
<connect gate="F" pin="M" pad="M2"/>
<connect gate="F" pin="P" pad="P2"/>
<connect gate="F" pin="R" pad="R2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="K" pin="K" pad="K2"/>
<connect gate="K" pin="N" pad="N2"/>
<connect gate="T" pin="S" pad="S2"/>
<connect gate="T" pin="T" pad="T2"/>
<connect gate="U" pin="P$1" pad="U2"/>
<connect gate="V" pin="GND" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="P$1" pad="D2"/>
<connect gate="E" pin="P$1" pad="E2"/>
<connect gate="F" pin="F" pad="F2"/>
<connect gate="F" pin="L" pad="L2"/>
<connect gate="F" pin="M" pad="M2"/>
<connect gate="F" pin="P" pad="P2"/>
<connect gate="F" pin="R" pad="R2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
<connect gate="K" pin="K" pad="K2"/>
<connect gate="K" pin="N" pad="N2"/>
<connect gate="T" pin="S" pad="S2"/>
<connect gate="T" pin="T" pad="T2"/>
<connect gate="U" pin="P$1" pad="U2"/>
<connect gate="V" pin="GND" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EMPTY" prefix="EMPTY_">
<description>Empty Slot</description>
<gates>
<gate name="G$1" symbol="-15V"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="PART"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="-15V" pad="B2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="-15V" pad="B2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="-15V" pad="B2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M051" prefix="M051_">
<description>M051 Positive Bus Converter</description>
<gates>
<gate name="G$8" symbol="POWER"/>
<gate name="D1" symbol="M051"/>
<gate name="E`" symbol="M051"/>
<gate name="F1" symbol="M051"/>
<gate name="H1" symbol="M051"/>
<gate name="J1" symbol="M051"/>
<gate name="K1" symbol="M051"/>
<gate name="L1" symbol="M051"/>
<gate name="M1" symbol="M051"/>
<gate name="N1" symbol="M051"/>
<gate name="P1" symbol="M051"/>
<gate name="R1" symbol="M051"/>
<gate name="S1" symbol="M051"/>
<gate name="G$15" symbol="T1GND"/>
<gate name="G$7" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D1" pin="IN" pad="D2"/>
<connect gate="D1" pin="OUT" pad="D1"/>
<connect gate="E`" pin="IN" pad="E2"/>
<connect gate="E`" pin="OUT" pad="E1"/>
<connect gate="F1" pin="IN" pad="F2"/>
<connect gate="F1" pin="OUT" pad="F1"/>
<connect gate="G$15" pin="GND" pad="T1"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="H1" pin="IN" pad="H2"/>
<connect gate="H1" pin="OUT" pad="H1"/>
<connect gate="J1" pin="IN" pad="J2"/>
<connect gate="J1" pin="OUT" pad="J1"/>
<connect gate="K1" pin="IN" pad="K2"/>
<connect gate="K1" pin="OUT" pad="K1"/>
<connect gate="L1" pin="IN" pad="L2"/>
<connect gate="L1" pin="OUT" pad="L1"/>
<connect gate="M1" pin="IN" pad="M2"/>
<connect gate="M1" pin="OUT" pad="M1"/>
<connect gate="N1" pin="IN" pad="N2"/>
<connect gate="N1" pin="OUT" pad="N1"/>
<connect gate="P1" pin="IN" pad="P2"/>
<connect gate="P1" pin="OUT" pad="P1"/>
<connect gate="R1" pin="IN" pad="R2"/>
<connect gate="R1" pin="OUT" pad="R1"/>
<connect gate="S1" pin="IN" pad="S2"/>
<connect gate="S1" pin="OUT" pad="S1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M508" prefix="M508_">
<description>M508 Negative Bus Converter</description>
<gates>
<gate name="D" symbol="M507-1"/>
<gate name="F" symbol="M507-1"/>
<gate name="J" symbol="M507-1"/>
<gate name="L" symbol="M507-1"/>
<gate name="N" symbol="M507-1"/>
<gate name="R" symbol="M507-1"/>
<gate name="G$8" symbol="POWER"/>
<gate name="G$7" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$7" pin="-15V" pad="B2"/>
<connect gate="G$8" pin="GND" pad="C2"/>
<connect gate="G$8" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W512" prefix="R512_">
<description>Positive Level Converter</description>
<gates>
<gate name="G$1" symbol="-15V"/>
<gate name="G$2" symbol="POWER"/>
<gate name="V" symbol="ENABLE"/>
<gate name="D" symbol="W512"/>
<gate name="F" symbol="W512"/>
<gate name="J" symbol="W512"/>
<gate name="L" symbol="W512"/>
<gate name="N" symbol="W512"/>
<gate name="R" symbol="W512"/>
<gate name="T" symbol="W512"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$1" pin="-15V" pad="B2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
<connect gate="T" pin="IN" pad="U2"/>
<connect gate="T" pin="OUT" pad="T2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$1" pin="-15V" pad="B2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
<connect gate="T" pin="IN" pad="U2"/>
<connect gate="T" pin="OUT" pad="T2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="D" pin="IN" pad="E2"/>
<connect gate="D" pin="OUT" pad="D2"/>
<connect gate="F" pin="IN" pad="H2"/>
<connect gate="F" pin="OUT" pad="F2"/>
<connect gate="G$1" pin="-15V" pad="B2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="J" pin="IN" pad="K2"/>
<connect gate="J" pin="OUT" pad="J2"/>
<connect gate="L" pin="IN" pad="M2"/>
<connect gate="L" pin="OUT" pad="L2"/>
<connect gate="N" pin="IN" pad="P2"/>
<connect gate="N" pin="OUT" pad="N2"/>
<connect gate="R" pin="IN" pad="S2"/>
<connect gate="R" pin="OUT" pad="R2"/>
<connect gate="T" pin="IN" pad="U2"/>
<connect gate="T" pin="OUT" pad="T2"/>
<connect gate="V" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R181" prefix="R181_">
<description>Carry Chain/Priority Encoder</description>
<gates>
<gate name="G$1" symbol="R181"/>
<gate name="G$2" symbol="-15V"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="R107A"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="K" pad="K2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="N" pad="N2"/>
<connect gate="G$1" pin="P" pad="P2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$1" pin="U" pad="U2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="I$1" pad="L2"/>
<connect gate="G$4" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="K" pad="K2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="N" pad="N2"/>
<connect gate="G$1" pin="P" pad="P2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$1" pin="U" pad="U2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="I$1" pad="L2"/>
<connect gate="G$4" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="K" pad="K2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="N" pad="N2"/>
<connect gate="G$1" pin="P" pad="P2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$1" pin="U" pad="U2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
<connect gate="G$4" pin="I$1" pad="L2"/>
<connect gate="G$4" pin="O$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W640" prefix="W640_">
<description>Pulse Amplifiers</description>
<gates>
<gate name="G$1" symbol="W640"/>
<gate name="G$2" symbol="W640"/>
<gate name="G$3" symbol="W640"/>
<gate name="G$4" symbol="-15V"/>
<gate name="G$5" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$2" pin="D" pad="K2"/>
<connect gate="G$2" pin="E" pad="L2"/>
<connect gate="G$2" pin="F" pad="M2"/>
<connect gate="G$2" pin="H" pad="N2"/>
<connect gate="G$2" pin="J" pad="P2"/>
<connect gate="G$3" pin="D" pad="R2"/>
<connect gate="G$3" pin="E" pad="S2"/>
<connect gate="G$3" pin="F" pad="T2"/>
<connect gate="G$3" pin="H" pad="U2"/>
<connect gate="G$3" pin="J" pad="V2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$2" pin="D" pad="K2"/>
<connect gate="G$2" pin="E" pad="L2"/>
<connect gate="G$2" pin="F" pad="M2"/>
<connect gate="G$2" pin="H" pad="N2"/>
<connect gate="G$2" pin="J" pad="P2"/>
<connect gate="G$3" pin="D" pad="R2"/>
<connect gate="G$3" pin="E" pad="S2"/>
<connect gate="G$3" pin="F" pad="T2"/>
<connect gate="G$3" pin="H" pad="U2"/>
<connect gate="G$3" pin="J" pad="V2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$2" pin="D" pad="K2"/>
<connect gate="G$2" pin="E" pad="L2"/>
<connect gate="G$2" pin="F" pad="M2"/>
<connect gate="G$2" pin="H" pad="N2"/>
<connect gate="G$2" pin="J" pad="P2"/>
<connect gate="G$3" pin="D" pad="R2"/>
<connect gate="G$3" pin="E" pad="S2"/>
<connect gate="G$3" pin="F" pad="T2"/>
<connect gate="G$3" pin="H" pad="U2"/>
<connect gate="G$3" pin="J" pad="V2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="R141" prefix="R141_">
<description>AND/NOR Gate</description>
<gates>
<gate name="G$1" symbol="R141"/>
<gate name="G$2" symbol="-15V"/>
<gate name="G$3" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="K" pad="K2"/>
<connect gate="G$1" pin="L" pad="L2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="N" pad="N2"/>
<connect gate="G$1" pin="P" pad="P2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$1" pin="U" pad="U2"/>
<connect gate="G$1" pin="V" pad="V2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="K" pad="K2"/>
<connect gate="G$1" pin="L" pad="L2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="N" pad="N2"/>
<connect gate="G$1" pin="P" pad="P2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$1" pin="U" pad="U2"/>
<connect gate="G$1" pin="V" pad="V2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="K" pad="K2"/>
<connect gate="G$1" pin="L" pad="L2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="N" pad="N2"/>
<connect gate="G$1" pin="P" pad="P2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$1" pin="U" pad="U2"/>
<connect gate="G$1" pin="V" pad="V2"/>
<connect gate="G$2" pin="-15V" pad="B2"/>
<connect gate="G$3" pin="GND" pad="C2"/>
<connect gate="G$3" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M700" prefix="M700">
<description>Manual Function Timing and Run</description>
<gates>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="POWER"/>
<gate name="DE2" symbol="PULL-UP"/>
<gate name="DF2" symbol="PULL-UP"/>
<gate name="G$1" symbol="M700"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="DE2" pin="P$1" pad="BE2"/>
<connect gate="DF2" pin="P$1" pad="BF2"/>
<connect gate="G$1" pin="CE2" pad="AE2"/>
<connect gate="G$1" pin="CF2" pad="AF2"/>
<connect gate="G$1" pin="CH2" pad="AH2"/>
<connect gate="G$1" pin="CJ2" pad="AJ2"/>
<connect gate="G$1" pin="CK2" pad="AK2"/>
<connect gate="G$1" pin="CL2" pad="AL2"/>
<connect gate="G$1" pin="CM2" pad="AM2"/>
<connect gate="G$1" pin="CN2" pad="AN2"/>
<connect gate="G$1" pin="CP2" pad="AP2"/>
<connect gate="G$1" pin="CR2" pad="AR2"/>
<connect gate="G$1" pin="CS2" pad="AS2"/>
<connect gate="G$1" pin="CT2" pad="AT2"/>
<connect gate="G$1" pin="DD2" pad="BD2"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M220" prefix="M220_">
<description>PDP-8 Major Registers</description>
<gates>
<gate name="G$1" symbol="M220A"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="T1GND"/>
<gate name="B0" symbol="M220B"/>
<gate name="B1" symbol="M220C"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="B0" pin="AA1" pad="AA1"/>
<connect gate="B0" pin="AB1" pad="AB1"/>
<connect gate="B0" pin="AB2" pad="AB2"/>
<connect gate="B0" pin="AC1" pad="AC1"/>
<connect gate="B0" pin="AD1" pad="AD1"/>
<connect gate="B0" pin="AD2" pad="AD2"/>
<connect gate="B0" pin="AE1" pad="AE1"/>
<connect gate="B0" pin="AE2" pad="AE2"/>
<connect gate="B0" pin="AF1" pad="AF1"/>
<connect gate="B0" pin="AF2" pad="AF2"/>
<connect gate="B0" pin="AH1" pad="AH1"/>
<connect gate="B0" pin="AH2" pad="AH2"/>
<connect gate="B0" pin="AJ2" pad="AJ2"/>
<connect gate="B0" pin="BB2" pad="BB2"/>
<connect gate="B0" pin="BC1" pad="BC1"/>
<connect gate="B0" pin="BD1" pad="BD1"/>
<connect gate="B0" pin="BE1" pad="BE1"/>
<connect gate="B0" pin="BF1" pad="BF1"/>
<connect gate="B0" pin="BF2" pad="BF2"/>
<connect gate="B0" pin="BH1" pad="BH1"/>
<connect gate="B0" pin="BH2" pad="BH2"/>
<connect gate="B0" pin="BJ2" pad="BJ2"/>
<connect gate="B0" pin="BK1" pad="BK1"/>
<connect gate="B0" pin="BK2" pad="BK2"/>
<connect gate="B0" pin="BL1" pad="BL1"/>
<connect gate="B0" pin="BL2" pad="BL2"/>
<connect gate="B0" pin="BM2" pad="BM2"/>
<connect gate="B0" pin="BP1" pad="BP1"/>
<connect gate="B0" pin="BR1" pad="BR1"/>
<connect gate="B0" pin="BS1" pad="BS1"/>
<connect gate="B0" pin="BS2" pad="BS2"/>
<connect gate="B0" pin="BT2" pad="BT2"/>
<connect gate="B0" pin="BU2" pad="BU2"/>
<connect gate="B1" pin="BD2" pad="BD2"/>
<connect gate="B1" pin="BE2" pad="BE2"/>
<connect gate="B1" pin="BJ1" pad="BJ1"/>
<connect gate="B1" pin="BM1" pad="BM1"/>
<connect gate="B1" pin="BN1" pad="BN1"/>
<connect gate="B1" pin="BN2" pad="BN2"/>
<connect gate="B1" pin="BP2" pad="BP2"/>
<connect gate="B1" pin="BR2" pad="BR2"/>
<connect gate="B1" pin="BU1" pad="BU1"/>
<connect gate="B1" pin="BV1" pad="BV1"/>
<connect gate="B1" pin="BV2" pad="BV2"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AK2" pad="AK2"/>
<connect gate="G$1" pin="AL1" pad="AL1"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM1" pad="AM1"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN1" pad="AN1"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP1" pad="AP1"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR1" pad="AR1"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS1" pad="AS1"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="AU1" pad="AU1"/>
<connect gate="G$1" pin="AU2" pad="AU2"/>
<connect gate="G$1" pin="AV1" pad="AV1"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="BA1" pad="BA1"/>
<connect gate="G$1" pin="BB1" pad="BB1"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="GND" pad="AT1"/>
<connect gate="G$5" pin="GND" pad="BT1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M906" prefix="M906_">
<description>Cable Terminator</description>
<gates>
<gate name="G$1" symbol="POWER"/>
<gate name="A1" symbol="T1GND"/>
<gate name="B1" symbol="W005A"/>
<gate name="D1" symbol="W005A"/>
<gate name="E1" symbol="W005A"/>
<gate name="H1" symbol="W005A"/>
<gate name="J1" symbol="W005A"/>
<gate name="L1" symbol="W005A"/>
<gate name="M1" symbol="W005A"/>
<gate name="P1" symbol="W005A"/>
<gate name="C1" symbol="T1GND"/>
<gate name="F1" symbol="T1GND"/>
<gate name="K1" symbol="T1GND"/>
<gate name="R1" symbol="T1GND"/>
<gate name="T1" symbol="T1GND"/>
<gate name="F2" symbol="T1GND"/>
<gate name="J2" symbol="T1GND"/>
<gate name="L2" symbol="T1GND"/>
<gate name="N2" symbol="T1GND"/>
<gate name="R2" symbol="T1GND"/>
<gate name="U2" symbol="T1GND"/>
<gate name="S1" symbol="W005A"/>
<gate name="D2" symbol="W005A"/>
<gate name="E2" symbol="W005A"/>
<gate name="H2" symbol="W005A"/>
<gate name="K2" symbol="W005A"/>
<gate name="M2" symbol="W005A"/>
<gate name="P2" symbol="W005A"/>
<gate name="S2" symbol="W005A"/>
<gate name="T2" symbol="W005A"/>
<gate name="V2" symbol="W005A"/>
<gate name="N1" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="A1" pin="GND" pad="A1"/>
<connect gate="B1" pin="P$1" pad="B1"/>
<connect gate="C1" pin="GND" pad="C1"/>
<connect gate="D1" pin="P$1" pad="D1"/>
<connect gate="D2" pin="P$1" pad="D2"/>
<connect gate="E1" pin="P$1" pad="E1"/>
<connect gate="E2" pin="P$1" pad="E2"/>
<connect gate="F1" pin="GND" pad="F1"/>
<connect gate="F2" pin="GND" pad="F2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="A2"/>
<connect gate="H1" pin="P$1" pad="H1"/>
<connect gate="H2" pin="P$1" pad="H2"/>
<connect gate="J1" pin="P$1" pad="J1"/>
<connect gate="J2" pin="GND" pad="J2"/>
<connect gate="K1" pin="GND" pad="K1"/>
<connect gate="K2" pin="P$1" pad="K2"/>
<connect gate="L1" pin="P$1" pad="L1"/>
<connect gate="L2" pin="GND" pad="L2"/>
<connect gate="M1" pin="P$1" pad="M1"/>
<connect gate="M2" pin="P$1" pad="M2"/>
<connect gate="N1" pin="GND" pad="N1"/>
<connect gate="N2" pin="GND" pad="N2"/>
<connect gate="P1" pin="P$1" pad="P1"/>
<connect gate="P2" pin="P$1" pad="P2"/>
<connect gate="R1" pin="GND" pad="R1"/>
<connect gate="R2" pin="GND" pad="R2"/>
<connect gate="S1" pin="P$1" pad="S1"/>
<connect gate="S2" pin="P$1" pad="S2"/>
<connect gate="T1" pin="GND" pad="T1"/>
<connect gate="T2" pin="P$1" pad="T2"/>
<connect gate="U2" pin="GND" pad="U2"/>
<connect gate="V2" pin="P$1" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M360" prefix="M360_">
<description>Variable Delay</description>
<gates>
<gate name="T" symbol="M360"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$1" symbol="INVERTER-OC"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="IN" pad="U2"/>
<connect gate="G$1" pin="OUT" pad="V2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="T" pin="P" pad="P2"/>
<connect gate="T" pin="R" pad="R2"/>
<connect gate="T" pin="S" pad="S2"/>
<connect gate="T" pin="T" pad="T2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G020" prefix="G020_">
<description>Sense Amps</description>
<gates>
<gate name="G$1" symbol="G020"/>
<gate name="C2" symbol="POWER"/>
<gate name="T1" symbol="T1GND"/>
<gate name="B2" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="B2" pin="-15V" pad="B2"/>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="C2" pin="VCC" pad="A2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="T1" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G221" prefix="G221_">
<description>Memory Selector</description>
<gates>
<gate name="G$1" symbol="G221"/>
<gate name="C2" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="C2" pin="VCC" pad="A2"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="V2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M710" prefix="M710_">
<description>Punch Control</description>
<gates>
<gate name="G$1" symbol="POWER"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="M710"/>
<gate name="BU2" symbol="PULL-UP"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="BU2" pin="P$1" pad="BU2"/>
<connect gate="G$1" pin="GND" pad="AC2"/>
<connect gate="G$1" pin="VCC" pad="AA2"/>
<connect gate="G$2" pin="GND" pad="BC2"/>
<connect gate="G$2" pin="VCC" pad="BA2"/>
<connect gate="G$3" pin="GND" pad="AT1"/>
<connect gate="G$4" pin="GND" pad="BT1"/>
<connect gate="G$5" pin="AD1" pad="AD1"/>
<connect gate="G$5" pin="AD2" pad="AD2"/>
<connect gate="G$5" pin="AE1" pad="AE1"/>
<connect gate="G$5" pin="AE2" pad="AE2"/>
<connect gate="G$5" pin="AF1" pad="AF1"/>
<connect gate="G$5" pin="AF2" pad="AF2"/>
<connect gate="G$5" pin="AH1" pad="AH1"/>
<connect gate="G$5" pin="AH2" pad="AH2"/>
<connect gate="G$5" pin="AJ1" pad="AJ1"/>
<connect gate="G$5" pin="AJ2" pad="AJ2"/>
<connect gate="G$5" pin="AK1" pad="AK1"/>
<connect gate="G$5" pin="AK2" pad="AK2"/>
<connect gate="G$5" pin="AL1" pad="AL1"/>
<connect gate="G$5" pin="AL2" pad="AL2"/>
<connect gate="G$5" pin="AM1" pad="AM1"/>
<connect gate="G$5" pin="AM2" pad="AM2"/>
<connect gate="G$5" pin="AN1" pad="AN1"/>
<connect gate="G$5" pin="AN2" pad="AN2"/>
<connect gate="G$5" pin="AP2" pad="AP2"/>
<connect gate="G$5" pin="AR1" pad="AR1"/>
<connect gate="G$5" pin="AR2" pad="AR2"/>
<connect gate="G$5" pin="AS1" pad="AS1"/>
<connect gate="G$5" pin="AS2" pad="AS2"/>
<connect gate="G$5" pin="AT2" pad="AT2"/>
<connect gate="G$5" pin="AU1" pad="AU1"/>
<connect gate="G$5" pin="AU2" pad="AU2"/>
<connect gate="G$5" pin="AV2" pad="AV2"/>
<connect gate="G$5" pin="BD1" pad="BD1"/>
<connect gate="G$5" pin="BD2" pad="BD2"/>
<connect gate="G$5" pin="BE1" pad="BE1"/>
<connect gate="G$5" pin="BE2" pad="BE2"/>
<connect gate="G$5" pin="BF1" pad="BF1"/>
<connect gate="G$5" pin="BF2" pad="BF2"/>
<connect gate="G$5" pin="BH2" pad="BH2"/>
<connect gate="G$5" pin="BN2" pad="BN2"/>
<connect gate="G$5" pin="BS2" pad="BS2"/>
<connect gate="G$5" pin="BV1" pad="BV1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M715" prefix="M715_">
<description>Reader Clock</description>
<gates>
<gate name="AC" symbol="POWER"/>
<gate name="BC" symbol="POWER"/>
<gate name="AB2" symbol="-15V"/>
<gate name="BB2" symbol="-15V"/>
<gate name="G$1" symbol="M715"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="AB2" pin="-15V" pad="AB2"/>
<connect gate="AC" pin="GND" pad="AC2"/>
<connect gate="AC" pin="VCC" pad="AA2"/>
<connect gate="BB2" pin="-15V" pad="BB2"/>
<connect gate="BC" pin="GND" pad="BC2"/>
<connect gate="BC" pin="VCC" pad="BA2"/>
<connect gate="G$1" pin="AK" pad="AK2"/>
<connect gate="G$1" pin="AM" pad="AM2"/>
<connect gate="G$1" pin="AP" pad="AP2"/>
<connect gate="G$1" pin="AS" pad="AS2"/>
<connect gate="G$1" pin="AT" pad="AT2"/>
<connect gate="G$1" pin="AU" pad="AU2"/>
<connect gate="G$1" pin="BP" pad="BP2"/>
<connect gate="G$1" pin="BR" pad="BR2"/>
<connect gate="G$1" pin="BS" pad="BS2"/>
<connect gate="G$1" pin="BT" pad="BT2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S-2">
<connects>
<connect gate="AB2" pin="-15V" pad="AB2"/>
<connect gate="AC" pin="GND" pad="AC2"/>
<connect gate="AC" pin="VCC" pad="AA2"/>
<connect gate="BB2" pin="-15V" pad="BB2"/>
<connect gate="BC" pin="GND" pad="BC2"/>
<connect gate="BC" pin="VCC" pad="BA2"/>
<connect gate="G$1" pin="AK" pad="AK2"/>
<connect gate="G$1" pin="AM" pad="AM2"/>
<connect gate="G$1" pin="AP" pad="AP2"/>
<connect gate="G$1" pin="AS" pad="AS2"/>
<connect gate="G$1" pin="AT" pad="AT2"/>
<connect gate="G$1" pin="AU" pad="AU2"/>
<connect gate="G$1" pin="BP" pad="BP2"/>
<connect gate="G$1" pin="BR" pad="BR2"/>
<connect gate="G$1" pin="BS" pad="BS2"/>
<connect gate="G$1" pin="BT" pad="BT2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800-2">
<connects>
<connect gate="AB2" pin="-15V" pad="AB2"/>
<connect gate="AC" pin="GND" pad="AC2"/>
<connect gate="AC" pin="VCC" pad="AA2"/>
<connect gate="BB2" pin="-15V" pad="BB2"/>
<connect gate="BC" pin="GND" pad="BC2"/>
<connect gate="BC" pin="VCC" pad="BA2"/>
<connect gate="G$1" pin="AK" pad="AK2"/>
<connect gate="G$1" pin="AM" pad="AM2"/>
<connect gate="G$1" pin="AP" pad="AP2"/>
<connect gate="G$1" pin="AS" pad="AS2"/>
<connect gate="G$1" pin="AT" pad="AT2"/>
<connect gate="G$1" pin="AU" pad="AU2"/>
<connect gate="G$1" pin="BP" pad="BP2"/>
<connect gate="G$1" pin="BR" pad="BR2"/>
<connect gate="G$1" pin="BS" pad="BS2"/>
<connect gate="G$1" pin="BT" pad="BT2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M705" prefix="M705_">
<description>Reader Control</description>
<gates>
<gate name="AC2" symbol="POWER"/>
<gate name="BC2" symbol="POWER"/>
<gate name="AT1" symbol="T1GND"/>
<gate name="BT1" symbol="T1GND"/>
<gate name="G$1" symbol="M705"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="AC2" pin="GND" pad="AC2"/>
<connect gate="AC2" pin="VCC" pad="AA2"/>
<connect gate="AT1" pin="GND" pad="AT1"/>
<connect gate="BC2" pin="GND" pad="BC2"/>
<connect gate="BC2" pin="VCC" pad="BA2"/>
<connect gate="BT1" pin="GND" pad="BT1"/>
<connect gate="G$1" pin="AD1" pad="AD1"/>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE1" pad="AE1"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF1" pad="AF1"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH1" pad="AH1"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AK2" pad="AK2"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN1" pad="AN1"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP1" pad="AP1"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR1" pad="AR1"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS1" pad="AS1"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="AU2" pad="AU2"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="BD1" pad="BD1"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE1" pad="BE1"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BF1" pad="BF1"/>
<connect gate="G$1" pin="BF2" pad="BF2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ1" pad="BJ1"/>
<connect gate="G$1" pin="BK1" pad="BK1"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BM1" pad="BM1"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$1" pin="BN2" pad="BN2"/>
<connect gate="G$1" pin="BP1" pad="BP1"/>
<connect gate="G$1" pin="BP2" pad="BP2"/>
<connect gate="G$1" pin="BR1" pad="BR1"/>
<connect gate="G$1" pin="BR2" pad="BR2"/>
<connect gate="G$1" pin="BS1" pad="BS1"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$1" pin="BU2" pad="BU2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M306" prefix="M306_">
<description>M306 Integrating One-Shot</description>
<gates>
<gate name="G$1" symbol="M306"/>
<gate name="G$2" symbol="POWER"/>
<gate name="K2" symbol="PULL-UP"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="L" pad="L2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="K2" pin="P$1" pad="K2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="L" pad="L2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="K2" pin="P$1" pad="K2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="J" pad="J2"/>
<connect gate="G$1" pin="L" pad="L2"/>
<connect gate="G$1" pin="M" pad="M2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G$1" pin="T" pad="T2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="K2" pin="P$1" pad="K2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M7102" prefix="M7102_">
<description>Positive I/O Bus Converter</description>
<gates>
<gate name="G$1" symbol="M7102A"/>
<gate name="G$2" symbol="M7102B"/>
<gate name="G$3" symbol="M7102C"/>
<gate name="G$4" symbol="M7102D"/>
<gate name="G$6" symbol="-15V"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="POWER"/>
<gate name="G$9" symbol="-15V"/>
<gate name="G$10" symbol="T1GND"/>
<gate name="G$11" symbol="T1GND"/>
<gate name="NAND" symbol="NAND2"/>
<gate name="NOR1" symbol="NOR2"/>
<gate name="NOR2" symbol="NOR2"/>
<gate name="G$12" symbol="M7102F"/>
<gate name="G$5" symbol="M7102E"/>
<gate name="G$13" symbol="M7102G"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AF1" pad="AF1"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH1" pad="AH1"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AL1" pad="AL1"/>
<connect gate="G$1" pin="AM1" pad="AM1"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE1" pad="BE1"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BL2" pad="BL2"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$10" pin="GND" pad="AT1"/>
<connect gate="G$11" pin="GND" pad="BT1"/>
<connect gate="G$12" pin="AU1" pad="AU1"/>
<connect gate="G$12" pin="AV1" pad="AV1"/>
<connect gate="G$12" pin="BC1" pad="BC1"/>
<connect gate="G$12" pin="BD1" pad="BD1"/>
<connect gate="G$12" pin="BV2" pad="BV2"/>
<connect gate="G$13" pin="AA1" pad="AA1"/>
<connect gate="G$13" pin="AB1" pad="AB1"/>
<connect gate="G$13" pin="BU1" pad="BU1"/>
<connect gate="G$13" pin="BU2" pad="BU2"/>
<connect gate="G$13" pin="BV1" pad="BV1"/>
<connect gate="G$2" pin="AN1" pad="AN1"/>
<connect gate="G$2" pin="AP1" pad="AP1"/>
<connect gate="G$2" pin="AR1" pad="AR1"/>
<connect gate="G$2" pin="BF2" pad="BF2"/>
<connect gate="G$2" pin="BH2" pad="BH2"/>
<connect gate="G$2" pin="BJ2" pad="BJ2"/>
<connect gate="G$3" pin="AK2" pad="AK2"/>
<connect gate="G$3" pin="AL2" pad="AL2"/>
<connect gate="G$3" pin="AM2" pad="AM2"/>
<connect gate="G$3" pin="AN2" pad="AN2"/>
<connect gate="G$4" pin="AP2" pad="AP2"/>
<connect gate="G$4" pin="AR2" pad="AR2"/>
<connect gate="G$4" pin="AS2" pad="AS2"/>
<connect gate="G$4" pin="AT2" pad="AT2"/>
<connect gate="G$4" pin="BA1" pad="BA1"/>
<connect gate="G$4" pin="BB1" pad="BB1"/>
<connect gate="G$5" pin="AD1" pad="AD1"/>
<connect gate="G$5" pin="AD2" pad="AD2"/>
<connect gate="G$5" pin="AE1" pad="AE1"/>
<connect gate="G$5" pin="AE2" pad="AE2"/>
<connect gate="G$5" pin="BN2" pad="BN2"/>
<connect gate="G$5" pin="BP2" pad="BP2"/>
<connect gate="G$5" pin="BR2" pad="BR2"/>
<connect gate="G$5" pin="BS2" pad="BS2"/>
<connect gate="G$6" pin="-15V" pad="AB2"/>
<connect gate="G$7" pin="GND" pad="AC2"/>
<connect gate="G$7" pin="VCC" pad="AA2"/>
<connect gate="G$8" pin="GND" pad="BC2"/>
<connect gate="G$8" pin="VCC" pad="BA2"/>
<connect gate="G$9" pin="-15V" pad="BB2"/>
<connect gate="NAND" pin="IN1" pad="BR1"/>
<connect gate="NAND" pin="IN2" pad="BS1"/>
<connect gate="NAND" pin="OUT" pad="BP1"/>
<connect gate="NOR1" pin="IN1" pad="BK1"/>
<connect gate="NOR1" pin="IN2" pad="BL1"/>
<connect gate="NOR1" pin="OUT" pad="BM1"/>
<connect gate="NOR2" pin="IN1" pad="BH1"/>
<connect gate="NOR2" pin="IN2" pad="BJ1"/>
<connect gate="NOR2" pin="OUT" pad="BF1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M7103" prefix="M7103_">
<description>Negative I/O Bus Converter</description>
<gates>
<gate name="G$1" symbol="M7102A"/>
<gate name="G$2" symbol="M7102B"/>
<gate name="G$3" symbol="M7102C"/>
<gate name="G$4" symbol="M7102D"/>
<gate name="G$6" symbol="-15V"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="POWER"/>
<gate name="G$9" symbol="-15V"/>
<gate name="G$10" symbol="T1GND"/>
<gate name="G$11" symbol="T1GND"/>
<gate name="NAND" symbol="NAND2"/>
<gate name="NOR1" symbol="NOR2"/>
<gate name="NOR2" symbol="NOR2"/>
<gate name="G$12" symbol="INVERTER-P"/>
<gate name="G$5" symbol="M7102E"/>
<gate name="G$13" symbol="M7102G"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AF1" pad="AF1"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH1" pad="AH1"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AL1" pad="AL1"/>
<connect gate="G$1" pin="AM1" pad="AM1"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE1" pad="BE1"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BL2" pad="BL2"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$10" pin="GND" pad="AT1"/>
<connect gate="G$11" pin="GND" pad="BT1"/>
<connect gate="G$12" pin="IN" pad="AV1"/>
<connect gate="G$12" pin="OUT" pad="AU1"/>
<connect gate="G$13" pin="AA1" pad="AA1"/>
<connect gate="G$13" pin="AB1" pad="AB1"/>
<connect gate="G$13" pin="BU1" pad="BU1"/>
<connect gate="G$13" pin="BU2" pad="BU2"/>
<connect gate="G$13" pin="BV1" pad="BV1"/>
<connect gate="G$2" pin="AN1" pad="AN1"/>
<connect gate="G$2" pin="AP1" pad="AP1"/>
<connect gate="G$2" pin="AR1" pad="AR1"/>
<connect gate="G$2" pin="BF2" pad="BF2"/>
<connect gate="G$2" pin="BH2" pad="BH2"/>
<connect gate="G$2" pin="BJ2" pad="BJ2"/>
<connect gate="G$3" pin="AK2" pad="AK2"/>
<connect gate="G$3" pin="AL2" pad="AL2"/>
<connect gate="G$3" pin="AM2" pad="AM2"/>
<connect gate="G$3" pin="AN2" pad="AN2"/>
<connect gate="G$4" pin="AP2" pad="AP2"/>
<connect gate="G$4" pin="AR2" pad="AR2"/>
<connect gate="G$4" pin="AS2" pad="AS2"/>
<connect gate="G$4" pin="AT2" pad="AT2"/>
<connect gate="G$4" pin="BA1" pad="BA1"/>
<connect gate="G$4" pin="BB1" pad="BB1"/>
<connect gate="G$5" pin="AD1" pad="AD1"/>
<connect gate="G$5" pin="AD2" pad="AD2"/>
<connect gate="G$5" pin="AE1" pad="AE1"/>
<connect gate="G$5" pin="AE2" pad="AE2"/>
<connect gate="G$5" pin="BN2" pad="BN2"/>
<connect gate="G$5" pin="BP2" pad="BP2"/>
<connect gate="G$5" pin="BR2" pad="BR2"/>
<connect gate="G$5" pin="BS2" pad="BS2"/>
<connect gate="G$6" pin="-15V" pad="AB2"/>
<connect gate="G$7" pin="GND" pad="AC2"/>
<connect gate="G$7" pin="VCC" pad="AA2"/>
<connect gate="G$8" pin="GND" pad="BC2"/>
<connect gate="G$8" pin="VCC" pad="BA2"/>
<connect gate="G$9" pin="-15V" pad="BB2"/>
<connect gate="NAND" pin="IN1" pad="BR1"/>
<connect gate="NAND" pin="IN2" pad="BS1"/>
<connect gate="NAND" pin="OUT" pad="BP1"/>
<connect gate="NOR1" pin="IN1" pad="BK1"/>
<connect gate="NOR1" pin="IN2" pad="BL1"/>
<connect gate="NOR1" pin="OUT" pad="BM1"/>
<connect gate="NOR2" pin="IN1" pad="BH1"/>
<connect gate="NOR2" pin="IN2" pad="BJ1"/>
<connect gate="NOR2" pin="OUT" pad="BF1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M650" prefix="M650_">
<gates>
<gate name="G$1" symbol="M650"/>
<gate name="G$2" symbol="M650"/>
<gate name="G$3" symbol="M650"/>
<gate name="G$4" symbol="-15V"/>
<gate name="G$5" symbol="POWER"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="IN1" pad="F2"/>
<connect gate="G$1" pin="IN2" pad="H2"/>
<connect gate="G$1" pin="IN3" pad="J2"/>
<connect gate="G$1" pin="OUT" pad="D2"/>
<connect gate="G$1" pin="SLOW" pad="E2"/>
<connect gate="G$2" pin="IN1" pad="M2"/>
<connect gate="G$2" pin="IN2" pad="N2"/>
<connect gate="G$2" pin="IN3" pad="P2"/>
<connect gate="G$2" pin="OUT" pad="K2"/>
<connect gate="G$2" pin="SLOW" pad="L2"/>
<connect gate="G$3" pin="IN1" pad="T2"/>
<connect gate="G$3" pin="IN2" pad="U2"/>
<connect gate="G$3" pin="IN3" pad="V2"/>
<connect gate="G$3" pin="OUT" pad="S2"/>
<connect gate="G$3" pin="SLOW" pad="R2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="IN1" pad="F2"/>
<connect gate="G$1" pin="IN2" pad="H2"/>
<connect gate="G$1" pin="IN3" pad="J2"/>
<connect gate="G$1" pin="OUT" pad="D2"/>
<connect gate="G$1" pin="SLOW" pad="E2"/>
<connect gate="G$2" pin="IN1" pad="M2"/>
<connect gate="G$2" pin="IN2" pad="N2"/>
<connect gate="G$2" pin="IN3" pad="P2"/>
<connect gate="G$2" pin="OUT" pad="K2"/>
<connect gate="G$2" pin="SLOW" pad="L2"/>
<connect gate="G$3" pin="IN1" pad="T2"/>
<connect gate="G$3" pin="IN2" pad="U2"/>
<connect gate="G$3" pin="IN3" pad="V2"/>
<connect gate="G$3" pin="OUT" pad="S2"/>
<connect gate="G$3" pin="SLOW" pad="R2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="IN1" pad="F2"/>
<connect gate="G$1" pin="IN2" pad="H2"/>
<connect gate="G$1" pin="IN3" pad="J2"/>
<connect gate="G$1" pin="OUT" pad="D2"/>
<connect gate="G$1" pin="SLOW" pad="E2"/>
<connect gate="G$2" pin="IN1" pad="M2"/>
<connect gate="G$2" pin="IN2" pad="N2"/>
<connect gate="G$2" pin="IN3" pad="P2"/>
<connect gate="G$2" pin="OUT" pad="K2"/>
<connect gate="G$2" pin="SLOW" pad="L2"/>
<connect gate="G$3" pin="IN1" pad="T2"/>
<connect gate="G$3" pin="IN2" pad="U2"/>
<connect gate="G$3" pin="IN3" pad="V2"/>
<connect gate="G$3" pin="OUT" pad="S2"/>
<connect gate="G$3" pin="SLOW" pad="R2"/>
<connect gate="G$4" pin="-15V" pad="B2"/>
<connect gate="G$5" pin="GND" pad="C2"/>
<connect gate="G$5" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W025" prefix="W025_">
<description>Core memory cable.</description>
<gates>
<gate name="AA" symbol="PAS"/>
<gate name="AB" symbol="PAS"/>
<gate name="AC" symbol="PAS"/>
<gate name="AD" symbol="PAS"/>
<gate name="AE" symbol="PAS"/>
<gate name="AF" symbol="PAS"/>
<gate name="AH" symbol="PAS"/>
<gate name="AJ" symbol="PAS"/>
<gate name="AK" symbol="PAS"/>
<gate name="AL" symbol="PAS"/>
<gate name="AM" symbol="PAS"/>
<gate name="AN" symbol="PAS"/>
<gate name="AP" symbol="PAS"/>
<gate name="AR" symbol="PAS"/>
<gate name="AS" symbol="PAS"/>
<gate name="AT" symbol="PAS"/>
<gate name="AU" symbol="PAS"/>
<gate name="AV" symbol="PAS"/>
<gate name="BA" symbol="PAS"/>
<gate name="BB" symbol="PAS"/>
<gate name="BC" symbol="PAS"/>
<gate name="BD" symbol="PAS"/>
<gate name="BE" symbol="PAS"/>
<gate name="BF" symbol="PAS"/>
<gate name="BH" symbol="PAS"/>
<gate name="BJ" symbol="PAS"/>
<gate name="BK" symbol="PAS"/>
<gate name="BL" symbol="PAS"/>
<gate name="BM" symbol="PAS"/>
<gate name="BN" symbol="PAS"/>
<gate name="BP" symbol="PAS"/>
<gate name="BR" symbol="PAS"/>
<gate name="BS" symbol="PAS"/>
<gate name="BT" symbol="PAS"/>
<gate name="BU" symbol="PAS"/>
<gate name="BV" symbol="PAS"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="AA" pin="P$2" pad="AA2"/>
<connect gate="AB" pin="P$2" pad="AB2"/>
<connect gate="AC" pin="P$2" pad="AC2"/>
<connect gate="AD" pin="P$2" pad="AD2"/>
<connect gate="AE" pin="P$2" pad="AE2"/>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AK" pin="P$2" pad="AK2"/>
<connect gate="AL" pin="P$2" pad="AL2"/>
<connect gate="AM" pin="P$2" pad="AM2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AS" pin="P$2" pad="AS2"/>
<connect gate="AT" pin="P$2" pad="AT2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BA" pin="P$2" pad="BA2"/>
<connect gate="BB" pin="P$2" pad="BB2"/>
<connect gate="BC" pin="P$2" pad="BC2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BE" pin="P$2" pad="BE2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BK" pin="P$2" pad="BK2"/>
<connect gate="BL" pin="P$2" pad="BL2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="BR" pin="P$2" pad="BR2"/>
<connect gate="BS" pin="P$2" pad="BS2"/>
<connect gate="BT" pin="P$2" pad="BT2"/>
<connect gate="BU" pin="P$2" pad="BU2"/>
<connect gate="BV" pin="P$2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800-2">
<connects>
<connect gate="AA" pin="P$2" pad="AA2"/>
<connect gate="AB" pin="P$2" pad="AB2"/>
<connect gate="AC" pin="P$2" pad="AC2"/>
<connect gate="AD" pin="P$2" pad="AD2"/>
<connect gate="AE" pin="P$2" pad="AE2"/>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AK" pin="P$2" pad="AK2"/>
<connect gate="AL" pin="P$2" pad="AL2"/>
<connect gate="AM" pin="P$2" pad="AM2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AS" pin="P$2" pad="AS2"/>
<connect gate="AT" pin="P$2" pad="AT2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BA" pin="P$2" pad="BA2"/>
<connect gate="BB" pin="P$2" pad="BB2"/>
<connect gate="BC" pin="P$2" pad="BC2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BE" pin="P$2" pad="BE2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BK" pin="P$2" pad="BK2"/>
<connect gate="BL" pin="P$2" pad="BL2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="BR" pin="P$2" pad="BR2"/>
<connect gate="BS" pin="P$2" pad="BS2"/>
<connect gate="BT" pin="P$2" pad="BT2"/>
<connect gate="BU" pin="P$2" pad="BU2"/>
<connect gate="BV" pin="P$2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S-2">
<connects>
<connect gate="AA" pin="P$2" pad="AA2"/>
<connect gate="AB" pin="P$2" pad="AB2"/>
<connect gate="AC" pin="P$2" pad="AC2"/>
<connect gate="AD" pin="P$2" pad="AD2"/>
<connect gate="AE" pin="P$2" pad="AE2"/>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AK" pin="P$2" pad="AK2"/>
<connect gate="AL" pin="P$2" pad="AL2"/>
<connect gate="AM" pin="P$2" pad="AM2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AS" pin="P$2" pad="AS2"/>
<connect gate="AT" pin="P$2" pad="AT2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BA" pin="P$2" pad="BA2"/>
<connect gate="BB" pin="P$2" pad="BB2"/>
<connect gate="BC" pin="P$2" pad="BC2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BE" pin="P$2" pad="BE2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BK" pin="P$2" pad="BK2"/>
<connect gate="BL" pin="P$2" pad="BL2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="BR" pin="P$2" pad="BR2"/>
<connect gate="BS" pin="P$2" pad="BS2"/>
<connect gate="BT" pin="P$2" pad="BT2"/>
<connect gate="BU" pin="P$2" pad="BU2"/>
<connect gate="BV" pin="P$2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G021" prefix="G021_">
<description>Sense Amps</description>
<gates>
<gate name="C2" symbol="POWER"/>
<gate name="T1" symbol="T1GND"/>
<gate name="B2" symbol="-15V"/>
<gate name="G$1" symbol="G021"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="B2" pin="-15V" pad="B2"/>
<connect gate="C2" pin="GND" pad="C2"/>
<connect gate="C2" pin="VCC" pad="A2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="N1" pad="N1"/>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="T1" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M216" prefix="M216_">
<description>Two sets of 3 D flip-flops</description>
<gates>
<gate name="P2" symbol="D-FLOP"/>
<gate name="E1" symbol="D-FLOP"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="T1GND"/>
<gate name="S1" symbol="D-FLOP-K2"/>
<gate name="V2" symbol="D-FLOP-K2"/>
<gate name="H2" symbol="D-FLOP-A1"/>
<gate name="L1" symbol="D-FLOP-A1"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="E1" pin="0" pad="F1"/>
<connect gate="E1" pin="1" pad="E1"/>
<connect gate="E1" pin="C" pad="B1"/>
<connect gate="E1" pin="D" pad="C1"/>
<connect gate="E1" pin="R" pad="A1"/>
<connect gate="E1" pin="S" pad="D1"/>
<connect gate="G$7" pin="GND" pad="C2"/>
<connect gate="G$7" pin="VCC" pad="A2"/>
<connect gate="G$8" pin="GND" pad="T1"/>
<connect gate="H2" pin="0" pad="J2"/>
<connect gate="H2" pin="1" pad="H2"/>
<connect gate="H2" pin="C" pad="D2"/>
<connect gate="H2" pin="D" pad="E2"/>
<connect gate="H2" pin="S" pad="F2"/>
<connect gate="L1" pin="0" pad="M1"/>
<connect gate="L1" pin="1" pad="L1"/>
<connect gate="L1" pin="C" pad="H1"/>
<connect gate="L1" pin="D" pad="J1"/>
<connect gate="L1" pin="S" pad="K1"/>
<connect gate="P2" pin="0" pad="R2"/>
<connect gate="P2" pin="1" pad="P2"/>
<connect gate="P2" pin="C" pad="L2"/>
<connect gate="P2" pin="D" pad="M2"/>
<connect gate="P2" pin="R" pad="K2"/>
<connect gate="P2" pin="S" pad="N2"/>
<connect gate="S1" pin="0" pad="U1"/>
<connect gate="S1" pin="1" pad="S1"/>
<connect gate="S1" pin="C" pad="N1"/>
<connect gate="S1" pin="D" pad="P1"/>
<connect gate="S1" pin="S" pad="R1"/>
<connect gate="V2" pin="0" pad="V1"/>
<connect gate="V2" pin="1" pad="V2"/>
<connect gate="V2" pin="C" pad="S2"/>
<connect gate="V2" pin="D" pad="T2"/>
<connect gate="V2" pin="S" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M720" prefix="M720_">
<description>M720 Memory Detection</description>
<gates>
<gate name="G$1" symbol="M720"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="NAND2"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="V2" pad="V2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="IN1" pad="S2"/>
<connect gate="G$3" pin="IN2" pad="T2"/>
<connect gate="G$3" pin="OUT" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M040" prefix="M040_">
<description>M040 Solenoid Driver</description>
<gates>
<gate name="G$1" symbol="M040"/>
<gate name="G$2" symbol="M040"/>
<gate name="G$3" symbol="ENABLE"/>
<gate name="G$4" symbol="POWER"/>
<gate name="G$5" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$2" pin="D" pad="J2"/>
<connect gate="G$2" pin="E" pad="K2"/>
<connect gate="G$2" pin="F" pad="L2"/>
<connect gate="G$2" pin="H" pad="M2"/>
<connect gate="G$2" pin="R" pad="S2"/>
<connect gate="G$3" pin="P$1" pad="V2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$2" pin="D" pad="J2"/>
<connect gate="G$2" pin="E" pad="K2"/>
<connect gate="G$2" pin="F" pad="L2"/>
<connect gate="G$2" pin="H" pad="M2"/>
<connect gate="G$2" pin="R" pad="S2"/>
<connect gate="G$3" pin="P$1" pad="V2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="E" pad="E2"/>
<connect gate="G$1" pin="F" pad="F2"/>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="R" pad="R2"/>
<connect gate="G$2" pin="D" pad="J2"/>
<connect gate="G$2" pin="E" pad="K2"/>
<connect gate="G$2" pin="F" pad="L2"/>
<connect gate="G$2" pin="H" pad="M2"/>
<connect gate="G$2" pin="R" pad="S2"/>
<connect gate="G$3" pin="P$1" pad="V2"/>
<connect gate="G$4" pin="GND" pad="C2"/>
<connect gate="G$4" pin="VCC" pad="A2"/>
<connect gate="G$5" pin="-15V" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G792" prefix="G792_">
<description>Power Supply Connector</description>
<gates>
<gate name="G$1" symbol="-15V"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="PART"/>
<gate name="G$4" symbol="POWER"/>
<gate name="G$5" symbol="POWER"/>
<gate name="G$6" symbol="POWER"/>
<gate name="G$7" symbol="POWER"/>
<gate name="G$8" symbol="POWER"/>
<gate name="G$9" symbol="POWER"/>
<gate name="G$10" symbol="POWER"/>
<gate name="G$11" symbol="POWER"/>
<gate name="G$12" symbol="POWER"/>
<gate name="G$13" symbol="POWER"/>
<gate name="G$14" symbol="POWER"/>
<gate name="G$15" symbol="POWER"/>
<gate name="G$16" symbol="POWER"/>
<gate name="G$17" symbol="POWER"/>
<gate name="G$18" symbol="POWER"/>
<gate name="G$19" symbol="POWER"/>
<gate name="G$20" symbol="POWER"/>
<gate name="G$21" symbol="POWER"/>
<gate name="G$22" symbol="POWER"/>
<gate name="G$23" symbol="T1GND"/>
<gate name="G$24" symbol="T1GND"/>
<gate name="G$25" symbol="T1GND"/>
<gate name="G$26" symbol="T1GND"/>
<gate name="G$27" symbol="T1GND"/>
<gate name="G$28" symbol="T1GND"/>
<gate name="G$29" symbol="T1GND"/>
<gate name="G$30" symbol="T1GND"/>
<gate name="G$31" symbol="T1GND"/>
<gate name="G$32" symbol="T1GND"/>
<gate name="G$33" symbol="-15V"/>
<gate name="G$34" symbol="-15V"/>
<gate name="G$35" symbol="-15V"/>
<gate name="G$36" symbol="-15V"/>
<gate name="G$37" symbol="-15V"/>
<gate name="G$38" symbol="-15V"/>
<gate name="G$39" symbol="-15V"/>
<gate name="G$40" symbol="-15V"/>
<gate name="G$41" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="-15V" pad="BV2"/>
<connect gate="G$10" pin="GND" pad="AM1"/>
<connect gate="G$10" pin="VCC" pad="AF2"/>
<connect gate="G$11" pin="GND" pad="AN1"/>
<connect gate="G$11" pin="VCC" pad="AH2"/>
<connect gate="G$12" pin="GND" pad="AP1"/>
<connect gate="G$12" pin="VCC" pad="AJ2"/>
<connect gate="G$13" pin="GND" pad="AR1"/>
<connect gate="G$13" pin="VCC" pad="AK2"/>
<connect gate="G$14" pin="GND" pad="AS1"/>
<connect gate="G$14" pin="VCC" pad="AL2"/>
<connect gate="G$15" pin="GND" pad="AT1"/>
<connect gate="G$15" pin="VCC" pad="AM2"/>
<connect gate="G$16" pin="GND" pad="AU1"/>
<connect gate="G$16" pin="VCC" pad="AN2"/>
<connect gate="G$17" pin="GND" pad="AV1"/>
<connect gate="G$17" pin="VCC" pad="AP2"/>
<connect gate="G$18" pin="GND" pad="BD1"/>
<connect gate="G$18" pin="VCC" pad="AR2"/>
<connect gate="G$19" pin="GND" pad="BE1"/>
<connect gate="G$19" pin="VCC" pad="AS2"/>
<connect gate="G$2" pin="GND" pad="AD1"/>
<connect gate="G$2" pin="VCC" pad="BJ2"/>
<connect gate="G$20" pin="GND" pad="BF1"/>
<connect gate="G$20" pin="VCC" pad="AT2"/>
<connect gate="G$21" pin="GND" pad="BH1"/>
<connect gate="G$21" pin="VCC" pad="AU2"/>
<connect gate="G$22" pin="GND" pad="BJ1"/>
<connect gate="G$22" pin="VCC" pad="AV2"/>
<connect gate="G$23" pin="GND" pad="BK1"/>
<connect gate="G$24" pin="GND" pad="BL1"/>
<connect gate="G$25" pin="GND" pad="BM1"/>
<connect gate="G$26" pin="GND" pad="BN1"/>
<connect gate="G$27" pin="GND" pad="BP1"/>
<connect gate="G$28" pin="GND" pad="BR1"/>
<connect gate="G$29" pin="GND" pad="BS1"/>
<connect gate="G$30" pin="GND" pad="BT1"/>
<connect gate="G$31" pin="GND" pad="BU1"/>
<connect gate="G$32" pin="GND" pad="BV1"/>
<connect gate="G$33" pin="-15V" pad="BK2"/>
<connect gate="G$34" pin="-15V" pad="BL2"/>
<connect gate="G$35" pin="-15V" pad="BM2"/>
<connect gate="G$36" pin="-15V" pad="BN2"/>
<connect gate="G$37" pin="-15V" pad="BP2"/>
<connect gate="G$38" pin="-15V" pad="BR2"/>
<connect gate="G$39" pin="-15V" pad="BS2"/>
<connect gate="G$4" pin="GND" pad="AE1"/>
<connect gate="G$4" pin="VCC" pad="BH2"/>
<connect gate="G$40" pin="-15V" pad="BT2"/>
<connect gate="G$41" pin="-15V" pad="BU2"/>
<connect gate="G$5" pin="GND" pad="AF1"/>
<connect gate="G$5" pin="VCC" pad="BF2"/>
<connect gate="G$6" pin="GND" pad="AH1"/>
<connect gate="G$6" pin="VCC" pad="BE2"/>
<connect gate="G$7" pin="GND" pad="AJ1"/>
<connect gate="G$7" pin="VCC" pad="BD2"/>
<connect gate="G$8" pin="GND" pad="AK1"/>
<connect gate="G$8" pin="VCC" pad="AD2"/>
<connect gate="G$9" pin="GND" pad="AL1"/>
<connect gate="G$9" pin="VCC" pad="AE2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M706" prefix="M706_">
<description>M706 TTY Receiver</description>
<gates>
<gate name="G$1" symbol="POWER"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="M706X"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="GND" pad="AC2"/>
<connect gate="G$1" pin="VCC" pad="AA2"/>
<connect gate="G$2" pin="GND" pad="BC2"/>
<connect gate="G$2" pin="VCC" pad="BA2"/>
<connect gate="G$3" pin="AD1" pad="AD1"/>
<connect gate="G$3" pin="AD2" pad="AD2"/>
<connect gate="G$3" pin="AE1" pad="AE1"/>
<connect gate="G$3" pin="AE2" pad="AE2"/>
<connect gate="G$3" pin="AF1" pad="AF1"/>
<connect gate="G$3" pin="AF2" pad="AF2"/>
<connect gate="G$3" pin="AH1" pad="AH1"/>
<connect gate="G$3" pin="AH2" pad="AH2"/>
<connect gate="G$3" pin="AJ1" pad="AJ1"/>
<connect gate="G$3" pin="AJ2" pad="AJ2"/>
<connect gate="G$3" pin="AK1" pad="AK1"/>
<connect gate="G$3" pin="AK2" pad="AK2"/>
<connect gate="G$3" pin="AL1" pad="AL1"/>
<connect gate="G$3" pin="AL2" pad="AL2"/>
<connect gate="G$3" pin="AM1" pad="AM1"/>
<connect gate="G$3" pin="AM2" pad="AM2"/>
<connect gate="G$3" pin="AN1" pad="AN1"/>
<connect gate="G$3" pin="AN2" pad="AN2"/>
<connect gate="G$3" pin="AP2" pad="AP2"/>
<connect gate="G$3" pin="AR1" pad="AR1"/>
<connect gate="G$3" pin="AR2" pad="AR2"/>
<connect gate="G$3" pin="AS1" pad="AS1"/>
<connect gate="G$3" pin="AS2" pad="AS2"/>
<connect gate="G$3" pin="AT2" pad="AT2"/>
<connect gate="G$3" pin="AU2" pad="AU2"/>
<connect gate="G$3" pin="AV2" pad="AV2"/>
<connect gate="G$3" pin="BD1" pad="BD1"/>
<connect gate="G$3" pin="BD2" pad="BD2"/>
<connect gate="G$3" pin="BE2" pad="BE2"/>
<connect gate="G$3" pin="BF2" pad="BF2"/>
<connect gate="G$3" pin="BH2" pad="BH2"/>
<connect gate="G$3" pin="BJ2" pad="BJ2"/>
<connect gate="G$3" pin="BK2" pad="BK2"/>
<connect gate="G$3" pin="BM2" pad="BM2"/>
<connect gate="G$3" pin="BN2" pad="BN2"/>
<connect gate="G$3" pin="BR1" pad="BR1"/>
<connect gate="G$3" pin="BR2" pad="BR2"/>
<connect gate="G$3" pin="BS1" pad="BS1"/>
<connect gate="G$3" pin="BS2" pad="BS2"/>
<connect gate="G$3" pin="BT2" pad="BT2"/>
<connect gate="G$3" pin="BU1" pad="BU1"/>
<connect gate="G$3" pin="BU2" pad="BU2"/>
<connect gate="G$3" pin="BV2" pad="BV2"/>
<connect gate="G$4" pin="GND" pad="AT1"/>
<connect gate="G$5" pin="GND" pad="BT1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M452" prefix="M452_">
<description>M452 Baud Rate Clock</description>
<gates>
<gate name="G$1" symbol="M452"/>
<gate name="G$2" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M707" prefix="M707_">
<description>M707 TTY Transmitter</description>
<gates>
<gate name="G$1" symbol="M707"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AD1" pad="AD1"/>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE1" pad="AE1"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF1" pad="AF1"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH1" pad="AH1"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AK2" pad="AK2"/>
<connect gate="G$1" pin="AL1" pad="AL1"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN1" pad="AN1"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR1" pad="AR1"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS1" pad="AS1"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="AU1" pad="AU1"/>
<connect gate="G$1" pin="AU2" pad="AU2"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BF2" pad="BF2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ1" pad="BJ1"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BN1" pad="BN1"/>
<connect gate="G$1" pin="BN2" pad="BN2"/>
<connect gate="G$1" pin="BP1" pad="BP1"/>
<connect gate="G$1" pin="BP2" pad="BP2"/>
<connect gate="G$1" pin="BR2" pad="BR2"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="GND" pad="AT1"/>
<connect gate="G$5" pin="GND" pad="BT1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M703" prefix="M703_">
<description>M703 Power Fail and Restart</description>
<gates>
<gate name="G$1" symbol="M703"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="U1" pad="U1"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M701" prefix="M701_">
<description>M701 Display Control</description>
<gates>
<gate name="G$1" symbol="M701"/>
<gate name="G$2" symbol="-30V"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="POWER"/>
<gate name="G$5" symbol="T1GND"/>
<gate name="G$6" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AK2" pad="AK2"/>
<connect gate="G$1" pin="AN1" pad="AN1"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP1" pad="AP1"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR1" pad="AR1"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS1" pad="AS1"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BF2" pad="BF2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BL2" pad="BL2"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$1" pin="BN2" pad="BN2"/>
<connect gate="G$1" pin="BP2" pad="BP2"/>
<connect gate="G$1" pin="BR2" pad="BR2"/>
<connect gate="G$2" pin="-30V" pad="AV2"/>
<connect gate="G$3" pin="GND" pad="AC2"/>
<connect gate="G$3" pin="VCC" pad="AA2"/>
<connect gate="G$4" pin="GND" pad="BC2"/>
<connect gate="G$4" pin="VCC" pad="BA2"/>
<connect gate="G$5" pin="GND" pad="AT1"/>
<connect gate="G$6" pin="GND" pad="BT1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A607" prefix="A607_">
<description>A607 Digital to Analog Converter</description>
<gates>
<gate name="G$1" symbol="A607"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="-15V"/>
<gate name="G$5" symbol="-15V"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="-15V" pad="AB2"/>
<connect gate="G$5" pin="-15V" pad="BB2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800-2">
<connects>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="-15V" pad="AB2"/>
<connect gate="G$5" pin="-15V" pad="BB2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S-2">
<connects>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="-15V" pad="AB2"/>
<connect gate="G$5" pin="-15V" pad="BB2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M704" prefix="M704_">
<description>M704 Plotter Control</description>
<gates>
<gate name="G$1" symbol="M704"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK2" pad="AK2"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="AU2" pad="AU2"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="BD2" pad="BD2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BF2" pad="BF2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BL2" pad="BL2"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$1" pin="BN2" pad="BN2"/>
<connect gate="G$1" pin="BP2" pad="BP2"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$1" pin="BT2" pad="BT2"/>
<connect gate="G$1" pin="BU1" pad="BU1"/>
<connect gate="G$1" pin="BV1" pad="BV1"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="GND" pad="AT1"/>
<connect gate="G$5" pin="GND" pad="BT1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M501" prefix="M501_">
<description>M401/M405/M501 Frequency Source</description>
<gates>
<gate name="G$1" symbol="M501"/>
<gate name="G$2" symbol="POWER"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M708" prefix="M708_">
<description>M708 Clock Control</description>
<gates>
<gate name="G$1" symbol="M708"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="H1" pad="H1"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K1" pad="K1"/>
<connect gate="G$1" pin="K2" pad="K2"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="L2" pad="L2"/>
<connect gate="G$1" pin="M2" pad="M2"/>
<connect gate="G$1" pin="N1" pad="N1"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="G$1" pin="V1" pad="V1"/>
<connect gate="G$1" pin="V2" pad="V2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M709" prefix="M709_">
<description>M709 Clock Counter</description>
<gates>
<gate name="G$1" symbol="M709"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AE1" pad="AE1"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF1" pad="AF1"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH1" pad="AH1"/>
<connect gate="G$1" pin="AJ1" pad="AJ1"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK1" pad="AK1"/>
<connect gate="G$1" pin="AL1" pad="AL1"/>
<connect gate="G$1" pin="AM1" pad="AM1"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP1" pad="AP1"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR1" pad="AR1"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS1" pad="AS1"/>
<connect gate="G$1" pin="AT2" pad="AT2"/>
<connect gate="G$1" pin="AU1" pad="AU1"/>
<connect gate="G$1" pin="AU2" pad="AU2"/>
<connect gate="G$1" pin="AV1" pad="AV1"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="BA1" pad="BA1"/>
<connect gate="G$1" pin="BB1" pad="BB1"/>
<connect gate="G$1" pin="BD1" pad="BD1"/>
<connect gate="G$1" pin="BF1" pad="BF1"/>
<connect gate="G$1" pin="BH1" pad="BH1"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ1" pad="BJ1"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BK1" pad="BK1"/>
<connect gate="G$1" pin="BL1" pad="BL1"/>
<connect gate="G$1" pin="BM1" pad="BM1"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$1" pin="BN1" pad="BN1"/>
<connect gate="G$1" pin="BP1" pad="BP1"/>
<connect gate="G$1" pin="BR1" pad="BR1"/>
<connect gate="G$1" pin="BS1" pad="BS1"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="GND" pad="AT1"/>
<connect gate="G$5" pin="GND" pad="BT1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M714" prefix="M714_">
<description>M714 Card Reader Control</description>
<gates>
<gate name="G$1" symbol="M714"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="F1" pad="F1"/>
<connect gate="G$1" pin="F2" pad="F2"/>
<connect gate="G$1" pin="H1" pad="H1"/>
<connect gate="G$1" pin="H2" pad="H2"/>
<connect gate="G$1" pin="J1" pad="J1"/>
<connect gate="G$1" pin="J2" pad="J2"/>
<connect gate="G$1" pin="K1" pad="K1"/>
<connect gate="G$1" pin="L1" pad="L1"/>
<connect gate="G$1" pin="M1" pad="M1"/>
<connect gate="G$1" pin="N1" pad="N1"/>
<connect gate="G$1" pin="N2" pad="N2"/>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="T2" pad="T2"/>
<connect gate="G$1" pin="U1" pad="U1"/>
<connect gate="G$1" pin="U2" pad="U2"/>
<connect gate="G$2" pin="GND" pad="C2"/>
<connect gate="G$2" pin="VCC" pad="A2"/>
<connect gate="G$3" pin="GND" pad="T1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M716" prefix="M716_">
<description>M716 Card Reader Control</description>
<gates>
<gate name="G$1" symbol="M716"/>
<gate name="G$2" symbol="POWER"/>
<gate name="G$3" symbol="POWER"/>
<gate name="G$4" symbol="T1GND"/>
<gate name="G$5" symbol="T1GND"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="AD2" pad="AD2"/>
<connect gate="G$1" pin="AE1" pad="AE1"/>
<connect gate="G$1" pin="AE2" pad="AE2"/>
<connect gate="G$1" pin="AF1" pad="AF1"/>
<connect gate="G$1" pin="AF2" pad="AF2"/>
<connect gate="G$1" pin="AH1" pad="AH1"/>
<connect gate="G$1" pin="AH2" pad="AH2"/>
<connect gate="G$1" pin="AJ2" pad="AJ2"/>
<connect gate="G$1" pin="AK2" pad="AK2"/>
<connect gate="G$1" pin="AL2" pad="AL2"/>
<connect gate="G$1" pin="AM2" pad="AM2"/>
<connect gate="G$1" pin="AN2" pad="AN2"/>
<connect gate="G$1" pin="AP2" pad="AP2"/>
<connect gate="G$1" pin="AR2" pad="AR2"/>
<connect gate="G$1" pin="AS2" pad="AS2"/>
<connect gate="G$1" pin="AU2" pad="AU2"/>
<connect gate="G$1" pin="AV2" pad="AV2"/>
<connect gate="G$1" pin="BE2" pad="BE2"/>
<connect gate="G$1" pin="BH2" pad="BH2"/>
<connect gate="G$1" pin="BJ2" pad="BJ2"/>
<connect gate="G$1" pin="BK2" pad="BK2"/>
<connect gate="G$1" pin="BL2" pad="BL2"/>
<connect gate="G$1" pin="BM2" pad="BM2"/>
<connect gate="G$1" pin="BN2" pad="BN2"/>
<connect gate="G$1" pin="BP2" pad="BP2"/>
<connect gate="G$1" pin="BR1" pad="BR1"/>
<connect gate="G$1" pin="BS1" pad="BS1"/>
<connect gate="G$1" pin="BS2" pad="BS2"/>
<connect gate="G$1" pin="BU1" pad="BU1"/>
<connect gate="G$2" pin="GND" pad="AC2"/>
<connect gate="G$2" pin="VCC" pad="AA2"/>
<connect gate="G$3" pin="GND" pad="BC2"/>
<connect gate="G$3" pin="VCC" pad="BA2"/>
<connect gate="G$4" pin="GND" pad="AT1"/>
<connect gate="G$5" pin="GND" pad="BT1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G610" prefix="G610_">
<description>G610 Core Connector</description>
<gates>
<gate name="G$2" symbol="G610B"/>
<gate name="G$1" symbol="G610A"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="G$1" pin="C2" pad="AC2"/>
<connect gate="G$1" pin="D2" pad="AD2"/>
<connect gate="G$1" pin="E2" pad="AE2"/>
<connect gate="G$1" pin="F2" pad="AF2"/>
<connect gate="G$1" pin="H2" pad="AH2"/>
<connect gate="G$1" pin="J2" pad="AJ2"/>
<connect gate="G$1" pin="K2" pad="AK2"/>
<connect gate="G$1" pin="L2" pad="AL2"/>
<connect gate="G$1" pin="M2" pad="AM2"/>
<connect gate="G$1" pin="N2" pad="AN2"/>
<connect gate="G$1" pin="P2" pad="AP2"/>
<connect gate="G$1" pin="R2" pad="AR2"/>
<connect gate="G$1" pin="S2" pad="AS2"/>
<connect gate="G$1" pin="T2" pad="AT2"/>
<connect gate="G$1" pin="U2" pad="AU2"/>
<connect gate="G$1" pin="V2" pad="AV2"/>
<connect gate="G$2" pin="C2" pad="BC2"/>
<connect gate="G$2" pin="D2" pad="BD2"/>
<connect gate="G$2" pin="E2" pad="BE2"/>
<connect gate="G$2" pin="F2" pad="BF2"/>
<connect gate="G$2" pin="H2" pad="BH2"/>
<connect gate="G$2" pin="J2" pad="BJ2"/>
<connect gate="G$2" pin="K2" pad="BK2"/>
<connect gate="G$2" pin="L2" pad="BL2"/>
<connect gate="G$2" pin="M2" pad="BM2"/>
<connect gate="G$2" pin="N2" pad="BN2"/>
<connect gate="G$2" pin="P2" pad="BP2"/>
<connect gate="G$2" pin="R2" pad="BR2"/>
<connect gate="G$2" pin="S2" pad="BS2"/>
<connect gate="G$2" pin="T2" pad="BT2"/>
<connect gate="G$2" pin="U2" pad="BU2"/>
<connect gate="G$2" pin="V2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800-2">
<connects>
<connect gate="G$1" pin="C2" pad="AC2"/>
<connect gate="G$1" pin="D2" pad="AD2"/>
<connect gate="G$1" pin="E2" pad="AE2"/>
<connect gate="G$1" pin="F2" pad="AF2"/>
<connect gate="G$1" pin="H2" pad="AH2"/>
<connect gate="G$1" pin="J2" pad="AJ2"/>
<connect gate="G$1" pin="K2" pad="AK2"/>
<connect gate="G$1" pin="L2" pad="AL2"/>
<connect gate="G$1" pin="M2" pad="AM2"/>
<connect gate="G$1" pin="N2" pad="AN2"/>
<connect gate="G$1" pin="P2" pad="AP2"/>
<connect gate="G$1" pin="R2" pad="AR2"/>
<connect gate="G$1" pin="S2" pad="AS2"/>
<connect gate="G$1" pin="T2" pad="AT2"/>
<connect gate="G$1" pin="U2" pad="AU2"/>
<connect gate="G$1" pin="V2" pad="AV2"/>
<connect gate="G$2" pin="C2" pad="BC2"/>
<connect gate="G$2" pin="D2" pad="BD2"/>
<connect gate="G$2" pin="E2" pad="BE2"/>
<connect gate="G$2" pin="F2" pad="BF2"/>
<connect gate="G$2" pin="H2" pad="BH2"/>
<connect gate="G$2" pin="J2" pad="BJ2"/>
<connect gate="G$2" pin="K2" pad="BK2"/>
<connect gate="G$2" pin="L2" pad="BL2"/>
<connect gate="G$2" pin="M2" pad="BM2"/>
<connect gate="G$2" pin="N2" pad="BN2"/>
<connect gate="G$2" pin="P2" pad="BP2"/>
<connect gate="G$2" pin="R2" pad="BR2"/>
<connect gate="G$2" pin="S2" pad="BS2"/>
<connect gate="G$2" pin="T2" pad="BT2"/>
<connect gate="G$2" pin="U2" pad="BU2"/>
<connect gate="G$2" pin="V2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S-2">
<connects>
<connect gate="G$1" pin="C2" pad="AC2"/>
<connect gate="G$1" pin="D2" pad="AD2"/>
<connect gate="G$1" pin="E2" pad="AE2"/>
<connect gate="G$1" pin="F2" pad="AF2"/>
<connect gate="G$1" pin="H2" pad="AH2"/>
<connect gate="G$1" pin="J2" pad="AJ2"/>
<connect gate="G$1" pin="K2" pad="AK2"/>
<connect gate="G$1" pin="L2" pad="AL2"/>
<connect gate="G$1" pin="M2" pad="AM2"/>
<connect gate="G$1" pin="N2" pad="AN2"/>
<connect gate="G$1" pin="P2" pad="AP2"/>
<connect gate="G$1" pin="R2" pad="AR2"/>
<connect gate="G$1" pin="S2" pad="AS2"/>
<connect gate="G$1" pin="T2" pad="AT2"/>
<connect gate="G$1" pin="U2" pad="AU2"/>
<connect gate="G$1" pin="V2" pad="AV2"/>
<connect gate="G$2" pin="C2" pad="BC2"/>
<connect gate="G$2" pin="D2" pad="BD2"/>
<connect gate="G$2" pin="E2" pad="BE2"/>
<connect gate="G$2" pin="F2" pad="BF2"/>
<connect gate="G$2" pin="H2" pad="BH2"/>
<connect gate="G$2" pin="J2" pad="BJ2"/>
<connect gate="G$2" pin="K2" pad="BK2"/>
<connect gate="G$2" pin="L2" pad="BL2"/>
<connect gate="G$2" pin="M2" pad="BM2"/>
<connect gate="G$2" pin="N2" pad="BN2"/>
<connect gate="G$2" pin="P2" pad="BP2"/>
<connect gate="G$2" pin="R2" pad="BR2"/>
<connect gate="G$2" pin="S2" pad="BS2"/>
<connect gate="G$2" pin="T2" pad="BT2"/>
<connect gate="G$2" pin="U2" pad="BU2"/>
<connect gate="G$2" pin="V2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W991" prefix="W991_">
<description>One-sided 36 pin (double hight) connector/cable.</description>
<gates>
<gate name="AA" symbol="PIN"/>
<gate name="AB" symbol="PIN"/>
<gate name="AC" symbol="PIN"/>
<gate name="AD" symbol="PIN"/>
<gate name="AE" symbol="PIN"/>
<gate name="AF" symbol="PIN"/>
<gate name="AH" symbol="PIN"/>
<gate name="AJ" symbol="PIN"/>
<gate name="AK" symbol="PIN"/>
<gate name="AL" symbol="PIN"/>
<gate name="AM" symbol="PIN"/>
<gate name="AN" symbol="PIN"/>
<gate name="AP" symbol="PIN"/>
<gate name="AR" symbol="PIN"/>
<gate name="AS" symbol="PIN"/>
<gate name="AT" symbol="PIN"/>
<gate name="AU" symbol="PIN"/>
<gate name="AV" symbol="PIN"/>
<gate name="BA" symbol="PIN"/>
<gate name="BB" symbol="PIN"/>
<gate name="BC" symbol="PIN"/>
<gate name="BD" symbol="PIN"/>
<gate name="BE" symbol="PIN"/>
<gate name="BF" symbol="PIN"/>
<gate name="BH" symbol="PIN"/>
<gate name="BJ" symbol="PIN"/>
<gate name="BK" symbol="PIN"/>
<gate name="BL" symbol="PIN"/>
<gate name="BM" symbol="PIN"/>
<gate name="BN" symbol="PIN"/>
<gate name="BP" symbol="PIN"/>
<gate name="BR" symbol="PIN"/>
<gate name="BS" symbol="PIN"/>
<gate name="BT" symbol="PIN"/>
<gate name="BU" symbol="PIN"/>
<gate name="BV" symbol="PIN"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="AA" pin="P$2" pad="AA2"/>
<connect gate="AB" pin="P$2" pad="AB2"/>
<connect gate="AC" pin="P$2" pad="AC2"/>
<connect gate="AD" pin="P$2" pad="AD2"/>
<connect gate="AE" pin="P$2" pad="AE2"/>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AK" pin="P$2" pad="AK2"/>
<connect gate="AL" pin="P$2" pad="AL2"/>
<connect gate="AM" pin="P$2" pad="AM2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AS" pin="P$2" pad="AS2"/>
<connect gate="AT" pin="P$2" pad="AT2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BA" pin="P$2" pad="BA2"/>
<connect gate="BB" pin="P$2" pad="BB2"/>
<connect gate="BC" pin="P$2" pad="BC2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BE" pin="P$2" pad="BE2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BK" pin="P$2" pad="BK2"/>
<connect gate="BL" pin="P$2" pad="BL2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="BR" pin="P$2" pad="BR2"/>
<connect gate="BS" pin="P$2" pad="BS2"/>
<connect gate="BT" pin="P$2" pad="BT2"/>
<connect gate="BU" pin="P$2" pad="BU2"/>
<connect gate="BV" pin="P$2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="O" package="H800-2">
<connects>
<connect gate="AA" pin="P$2" pad="AA2"/>
<connect gate="AB" pin="P$2" pad="AB2"/>
<connect gate="AC" pin="P$2" pad="AC2"/>
<connect gate="AD" pin="P$2" pad="AD2"/>
<connect gate="AE" pin="P$2" pad="AE2"/>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AK" pin="P$2" pad="AK2"/>
<connect gate="AL" pin="P$2" pad="AL2"/>
<connect gate="AM" pin="P$2" pad="AM2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AS" pin="P$2" pad="AS2"/>
<connect gate="AT" pin="P$2" pad="AT2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BA" pin="P$2" pad="BA2"/>
<connect gate="BB" pin="P$2" pad="BB2"/>
<connect gate="BC" pin="P$2" pad="BC2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BE" pin="P$2" pad="BE2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BK" pin="P$2" pad="BK2"/>
<connect gate="BL" pin="P$2" pad="BL2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="BR" pin="P$2" pad="BR2"/>
<connect gate="BS" pin="P$2" pad="BS2"/>
<connect gate="BT" pin="P$2" pad="BT2"/>
<connect gate="BU" pin="P$2" pad="BU2"/>
<connect gate="BV" pin="P$2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S-2">
<connects>
<connect gate="AA" pin="P$2" pad="AA2"/>
<connect gate="AB" pin="P$2" pad="AB2"/>
<connect gate="AC" pin="P$2" pad="AC2"/>
<connect gate="AD" pin="P$2" pad="AD2"/>
<connect gate="AE" pin="P$2" pad="AE2"/>
<connect gate="AF" pin="P$2" pad="AF2"/>
<connect gate="AH" pin="P$2" pad="AH2"/>
<connect gate="AJ" pin="P$2" pad="AJ2"/>
<connect gate="AK" pin="P$2" pad="AK2"/>
<connect gate="AL" pin="P$2" pad="AL2"/>
<connect gate="AM" pin="P$2" pad="AM2"/>
<connect gate="AN" pin="P$2" pad="AN2"/>
<connect gate="AP" pin="P$2" pad="AP2"/>
<connect gate="AR" pin="P$2" pad="AR2"/>
<connect gate="AS" pin="P$2" pad="AS2"/>
<connect gate="AT" pin="P$2" pad="AT2"/>
<connect gate="AU" pin="P$2" pad="AU2"/>
<connect gate="AV" pin="P$2" pad="AV2"/>
<connect gate="BA" pin="P$2" pad="BA2"/>
<connect gate="BB" pin="P$2" pad="BB2"/>
<connect gate="BC" pin="P$2" pad="BC2"/>
<connect gate="BD" pin="P$2" pad="BD2"/>
<connect gate="BE" pin="P$2" pad="BE2"/>
<connect gate="BF" pin="P$2" pad="BF2"/>
<connect gate="BH" pin="P$2" pad="BH2"/>
<connect gate="BJ" pin="P$2" pad="BJ2"/>
<connect gate="BK" pin="P$2" pad="BK2"/>
<connect gate="BL" pin="P$2" pad="BL2"/>
<connect gate="BM" pin="P$2" pad="BM2"/>
<connect gate="BN" pin="P$2" pad="BN2"/>
<connect gate="BP" pin="P$2" pad="BP2"/>
<connect gate="BR" pin="P$2" pad="BR2"/>
<connect gate="BS" pin="P$2" pad="BS2"/>
<connect gate="BT" pin="P$2" pad="BT2"/>
<connect gate="BU" pin="P$2" pad="BU2"/>
<connect gate="BV" pin="P$2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W076" prefix="W076_">
<description>W076 Terminal Connector</description>
<gates>
<gate name="G$1" symbol="POWER"/>
<gate name="G$2" symbol="-30V"/>
<gate name="G$3" symbol="-15V"/>
<gate name="M" symbol="PIN"/>
<gate name="H" symbol="PIN"/>
<gate name="E" symbol="PIN"/>
<gate name="K" symbol="PIN"/>
<gate name="U" symbol="PIN"/>
</gates>
<devices>
<device name="O" package="H800">
<connects>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="A2"/>
<connect gate="G$2" pin="-30V" pad="V2"/>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="U" pin="P$2" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="H807">
<connects>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="A2"/>
<connect gate="G$2" pin="-30V" pad="V2"/>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="U" pin="P$2" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="H807S">
<connects>
<connect gate="E" pin="P$2" pad="E2"/>
<connect gate="G$1" pin="GND" pad="C2"/>
<connect gate="G$1" pin="VCC" pad="A2"/>
<connect gate="G$2" pin="-30V" pad="V2"/>
<connect gate="G$3" pin="-15V" pad="B2"/>
<connect gate="H" pin="P$2" pad="H2"/>
<connect gate="K" pin="P$2" pad="K2"/>
<connect gate="M" pin="P$2" pad="M2"/>
<connect gate="U" pin="P$2" pad="U2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W971" prefix="W971_">
<description>Double sided Double Height Connector, 72 pins</description>
<gates>
<gate name="AA1" symbol="PIN"/>
<gate name="AB1" symbol="PIN"/>
<gate name="AC1" symbol="PIN"/>
<gate name="AD1" symbol="PIN"/>
<gate name="AE1" symbol="PIN"/>
<gate name="AF1" symbol="PIN"/>
<gate name="AH1" symbol="PIN"/>
<gate name="AJ1" symbol="PIN"/>
<gate name="AK1" symbol="PIN"/>
<gate name="AL1" symbol="PIN"/>
<gate name="AM1" symbol="PIN"/>
<gate name="AN1" symbol="PIN"/>
<gate name="AP1" symbol="PIN"/>
<gate name="AR1" symbol="PIN"/>
<gate name="AS1" symbol="PIN"/>
<gate name="AT1" symbol="PIN"/>
<gate name="AU1" symbol="PIN"/>
<gate name="AV1" symbol="PIN"/>
<gate name="AA2" symbol="PIN"/>
<gate name="AB2" symbol="PIN"/>
<gate name="AC2" symbol="PIN"/>
<gate name="AD2" symbol="PIN"/>
<gate name="AE2" symbol="PIN"/>
<gate name="AF2" symbol="PIN"/>
<gate name="AH2" symbol="PIN"/>
<gate name="AJ2" symbol="PIN"/>
<gate name="AK2" symbol="PIN"/>
<gate name="AL2" symbol="PIN"/>
<gate name="AM2" symbol="PIN"/>
<gate name="AN2" symbol="PIN"/>
<gate name="AP2" symbol="PIN"/>
<gate name="AR2" symbol="PIN"/>
<gate name="AS2" symbol="PIN"/>
<gate name="AT2" symbol="PIN"/>
<gate name="AU2" symbol="PIN"/>
<gate name="AV2" symbol="PIN"/>
<gate name="BA1" symbol="PIN"/>
<gate name="BB1" symbol="PIN"/>
<gate name="BC1" symbol="PIN"/>
<gate name="BD1" symbol="PIN"/>
<gate name="BE1" symbol="PIN"/>
<gate name="BF1" symbol="PIN"/>
<gate name="BH1" symbol="PIN"/>
<gate name="BJ1" symbol="PIN"/>
<gate name="BK1" symbol="PIN"/>
<gate name="BL1" symbol="PIN"/>
<gate name="BM1" symbol="PIN"/>
<gate name="BN1" symbol="PIN"/>
<gate name="BP1" symbol="PIN"/>
<gate name="BR1" symbol="PIN"/>
<gate name="BS1" symbol="PIN"/>
<gate name="BT1" symbol="PIN"/>
<gate name="BU1" symbol="PIN"/>
<gate name="BV1" symbol="PIN"/>
<gate name="BA2" symbol="PIN"/>
<gate name="BB2" symbol="PIN"/>
<gate name="BC2" symbol="PIN"/>
<gate name="BD2" symbol="PIN"/>
<gate name="BE2" symbol="PIN"/>
<gate name="BF2" symbol="PIN"/>
<gate name="BH2" symbol="PIN"/>
<gate name="BJ2" symbol="PIN"/>
<gate name="BK2" symbol="PIN"/>
<gate name="BL2" symbol="PIN"/>
<gate name="BM2" symbol="PIN"/>
<gate name="BN2" symbol="PIN"/>
<gate name="BP2" symbol="PIN"/>
<gate name="BR2" symbol="PIN"/>
<gate name="BS2" symbol="PIN"/>
<gate name="BT2" symbol="PIN"/>
<gate name="BU2" symbol="PIN"/>
<gate name="BV2" symbol="PIN"/>
</gates>
<devices>
<device name="" package="H807-2">
<connects>
<connect gate="AA1" pin="P$2" pad="AA1"/>
<connect gate="AA2" pin="P$2" pad="AA2"/>
<connect gate="AB1" pin="P$2" pad="AB1"/>
<connect gate="AB2" pin="P$2" pad="AB2"/>
<connect gate="AC1" pin="P$2" pad="AC1"/>
<connect gate="AC2" pin="P$2" pad="AC2"/>
<connect gate="AD1" pin="P$2" pad="AD1"/>
<connect gate="AD2" pin="P$2" pad="AD2"/>
<connect gate="AE1" pin="P$2" pad="AE1"/>
<connect gate="AE2" pin="P$2" pad="AE2"/>
<connect gate="AF1" pin="P$2" pad="AF1"/>
<connect gate="AF2" pin="P$2" pad="AF2"/>
<connect gate="AH1" pin="P$2" pad="AH1"/>
<connect gate="AH2" pin="P$2" pad="AH2"/>
<connect gate="AJ1" pin="P$2" pad="AJ1"/>
<connect gate="AJ2" pin="P$2" pad="AJ2"/>
<connect gate="AK1" pin="P$2" pad="AK1"/>
<connect gate="AK2" pin="P$2" pad="AK2"/>
<connect gate="AL1" pin="P$2" pad="AL1"/>
<connect gate="AL2" pin="P$2" pad="AL2"/>
<connect gate="AM1" pin="P$2" pad="AM1"/>
<connect gate="AM2" pin="P$2" pad="AM2"/>
<connect gate="AN1" pin="P$2" pad="AN1"/>
<connect gate="AN2" pin="P$2" pad="AN2"/>
<connect gate="AP1" pin="P$2" pad="AP1"/>
<connect gate="AP2" pin="P$2" pad="AP2"/>
<connect gate="AR1" pin="P$2" pad="AR1"/>
<connect gate="AR2" pin="P$2" pad="AR2"/>
<connect gate="AS1" pin="P$2" pad="AS1"/>
<connect gate="AS2" pin="P$2" pad="AS2"/>
<connect gate="AT1" pin="P$2" pad="AT1"/>
<connect gate="AT2" pin="P$2" pad="AT2"/>
<connect gate="AU1" pin="P$2" pad="AU1"/>
<connect gate="AU2" pin="P$2" pad="AU2"/>
<connect gate="AV1" pin="P$2" pad="AV1"/>
<connect gate="AV2" pin="P$2" pad="AV2"/>
<connect gate="BA1" pin="P$2" pad="BA1"/>
<connect gate="BA2" pin="P$2" pad="BA2"/>
<connect gate="BB1" pin="P$2" pad="BB1"/>
<connect gate="BB2" pin="P$2" pad="BB2"/>
<connect gate="BC1" pin="P$2" pad="BC1"/>
<connect gate="BC2" pin="P$2" pad="BC2"/>
<connect gate="BD1" pin="P$2" pad="BD1"/>
<connect gate="BD2" pin="P$2" pad="BD2"/>
<connect gate="BE1" pin="P$2" pad="BE1"/>
<connect gate="BE2" pin="P$2" pad="BE2"/>
<connect gate="BF1" pin="P$2" pad="BF1"/>
<connect gate="BF2" pin="P$2" pad="BF2"/>
<connect gate="BH1" pin="P$2" pad="BH1"/>
<connect gate="BH2" pin="P$2" pad="BH2"/>
<connect gate="BJ1" pin="P$2" pad="BJ1"/>
<connect gate="BJ2" pin="P$2" pad="BJ2"/>
<connect gate="BK1" pin="P$2" pad="BK1"/>
<connect gate="BK2" pin="P$2" pad="BK2"/>
<connect gate="BL1" pin="P$2" pad="BL1"/>
<connect gate="BL2" pin="P$2" pad="BL2"/>
<connect gate="BM1" pin="P$2" pad="BM1"/>
<connect gate="BM2" pin="P$2" pad="BM2"/>
<connect gate="BN1" pin="P$2" pad="BN1"/>
<connect gate="BN2" pin="P$2" pad="BN2"/>
<connect gate="BP1" pin="P$2" pad="BP1"/>
<connect gate="BP2" pin="P$2" pad="BP2"/>
<connect gate="BR1" pin="P$2" pad="BR1"/>
<connect gate="BR2" pin="P$2" pad="BR2"/>
<connect gate="BS1" pin="P$2" pad="BS1"/>
<connect gate="BS2" pin="P$2" pad="BS2"/>
<connect gate="BT1" pin="P$2" pad="BT1"/>
<connect gate="BT2" pin="P$2" pad="BT2"/>
<connect gate="BU1" pin="P$2" pad="BU1"/>
<connect gate="BU2" pin="P$2" pad="BU2"/>
<connect gate="BV1" pin="P$2" pad="BV1"/>
<connect gate="BV2" pin="P$2" pad="BV2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
