<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="BATT2032">
</package>
<package name="C0.1PTH">
</package>
<package name="C1206">
</package>
<package name="C402">
</package>
<package name="C603">
</package>
<package name="C805">
</package>
<package name="CASE_A">
</package>
<package name="CASE_B">
</package>
<package name="CAT16-F8/CAT16-J8">
</package>
<package name="LOGO_CC-BY-SA">
</package>
<package name="CON_ARDUINO">
</package>
<package name="CON_ATX_PWR_90DEG">
<description>place with 9.7mm spacing from the edge of the board</description>
</package>
<package name="CONN_USB_A_MALE">
<description>SMD mount USB Type A Male</description>
</package>
<package name="CONN_USB_MINI-B">
<description>USB mini-b connector SMT 0.8 mm pitch
adjusted pad dimesion (0.5 x 3.3 mm) on pin 1 to 5</description>
</package>
<package name="D2PAK">
<description>D2PAK</description>
</package>
<package name="DBV-R-PDSO-G6">
</package>
<package name="DC_BARREL_JACK_SMD_2MM">
<description>DC barrel jack SMD 2.0mm pin, 6.5mm barrel</description>
</package>
<package name="DCK_R_PDSO_G6">
</package>
<package name="DCT_R_PDSO_G8">
</package>
<package name="DCU_R_PDSO_G8">
</package>
<package name="DFN6_3X3">
</package>
<package name="DFN8_3X2-EASY">
</package>
<package name="DFN8_3X2">
</package>
<package name="DFN8_3X3-EASY">
</package>
<package name="DGK_S_PDSO_G8">
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="DIL28-N">
</package>
<package name="DIP14">
</package>
<package name="DIP14W">
</package>
<package name="DIP18">
</package>
<package name="DIP20">
</package>
<package name="DIP8">
</package>
<package name="DISP_7SEG">
</package>
<package name="DO323">
</package>
<package name="DP10050_V1">
</package>
<package name="DP10062_V1">
</package>
<package name="DP10080_V1">
</package>
<package name="DP3030_V1">
</package>
<package name="DP4040_V1">
</package>
<package name="DP5031_V1">
</package>
<package name="DP5050_V1">
</package>
<package name="DP6037_V1">
</package>
<package name="DP6060_V1">
</package>
<package name="DP7043_V1">
</package>
<package name="DP7070_V1">
</package>
<package name="DP8049_V1">
</package>
<package name="DP8080_V1">
</package>
<package name="DP9056_V1">
</package>
<package name="DP_LOGO">
</package>
<package name="DP_LOGO_ART_0.5X0.5">
</package>
<package name="DP_LOGO_ART_1.5X1.5">
</package>
<package name="DP_LOGO_ART_1X1">
</package>
<package name="DP_LOGO_ART_2.5X2.5">
</package>
<package name="DP_LOGO_ART_2X2">
</package>
<package name="DP_LOGO_ART_3X3">
</package>
<package name="DPAK">
<description>DPAK</description>
</package>
<package name="DSBGA-8">
</package>
<package name="EDGE_CONNECTOR_6X2">
<description>0.100 x 0.200 inch pitch Edge Connector with no mounting ear</description>
</package>
<package name="EGDE2X10">
</package>
<package name="EGDE2X9">
</package>
<package name="FB1206">
</package>
<package name="FB402">
</package>
<package name="FB603">
</package>
<package name="FB805">
</package>
<package name="HC-49U">
</package>
<package name="HDR-BUSPIRATE">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="HEADER_PRG_1X04">
</package>
<package name="HEADER_PRG_1X05">
</package>
<package name="HEADER_PRG_1X05_ICSP_B">
<description>PIC ICSP Header with triangular marker above pin 1</description>
</package>
<package name="HEADER_PRG_1X06">
</package>
<package name="HEADER_PRG_2X03">
</package>
<package name="HR911105A">
</package>
<package name="JOYSTICK">
</package>
<package name="JP3_0805">
</package>
<package name="JUMP2_DESC">
</package>
<package name="JUMP2_DESC_OFF">
</package>
<package name="JUMP2_DESC_ON">
</package>
<package name="JUMP2X2_DESC">
</package>
<package name="JUMP3_DESC">
</package>
<package name="JUMP3_DESC_LEFT">
</package>
<package name="JUMP3_DESC_RIGHT">
</package>
<package name="JUMPER_SOLDER">
</package>
<package name="LED-3MM">
</package>
<package name="LED-5MM-90DEG">
</package>
<package name="LED-5MM">
</package>
<package name="LED-805">
</package>
<package name="LGA-14">
</package>
<package name="LOGO_CC-0">
</package>
<package name="LQFP48">
</package>
<package name="LQFP64">
<description>LQFP64 &lt;AUTHOR&gt;Richard Myrick T. Arellaga&lt;/author&gt; &lt;copyright&gt;March2010&lt;/copyright&gt;</description>
</package>
<package name="M1X1">
</package>
<package name="M1X2">
</package>
<package name="M1X3">
</package>
<package name="M1X4">
</package>
<package name="M1X5">
</package>
<package name="M1X6">
</package>
<package name="M1X8">
</package>
<package name="M2X10">
</package>
<package name="M2X2">
</package>
<package name="M2X3">
</package>
<package name="M2X4">
</package>
<package name="M2X5">
</package>
<package name="M2X6">
</package>
<package name="MRF24WBOMA">
</package>
<package name="MSOP8">
</package>
<package name="OLED96X16">
</package>
<package name="OSCILLATOR_7X5_SMD">
<description>Oscillator 7.0 x 5.0 mm SMD Ceramic Package</description>
</package>
<package name="PAD_ROUND_4.1MM">
<description>Round pad 4.1mm hole 8mm pad diameter</description>
</package>
<package name="PCB_EDGE_CONNECTOR_6X2">
</package>
<package name="PINSHRD_PTH_2X05">
</package>
<package name="PINSHRD_PTH_2X05B">
<description>2X5 Pin header with flipped shrouded case</description>
</package>
<package name="PINSHRD_PTH_2X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="PINSHRD_SMT_2X05">
<description>pitch = 0.100 [2.54], 2x5

source: http://www.mlelectronic.com/shrouded-headers/shrouded-headers-100.asp</description>
</package>
<package name="PINSHRD_SMT_2X06">
<description>pitch = 0.100 [2.54], 2x5

source: http://www.mlelectronic.com/shrouded-headers/shrouded-headers-100.asp</description>
</package>
<package name="PLCC4">
</package>
<package name="PROTO_VIAS_05X05">
<description>5x5 square pad 0.04 inch drill prototyping block</description>
</package>
<package name="PTC0805">
<description>0805 fuse</description>
</package>
<package name="PTC1812L">
<description>4.73mm x 3.41mm</description>
</package>
<package name="QFN-20">
</package>
<package name="QFN16_4X4">
</package>
<package name="QFN25_5X5">
</package>
<package name="QFN36_6X6">
</package>
<package name="QSE15X">
</package>
<package name="R1206">
</package>
<package name="R402">
</package>
<package name="R603">
</package>
<package name="R805">
</package>
<package name="RGBLED">
</package>
<package name="RGBLED1206">
</package>
<package name="RN8P-4R-CRA06S">
</package>
<package name="RTH025W">
</package>
<package name="SLIDE_SWITCH_SMD">
</package>
<package name="SMC_A">
</package>
<package name="SMC_B">
</package>
<package name="SMDPAD05X05">
</package>
<package name="SO-18">
</package>
<package name="SO-18L">
</package>
<package name="SO-8">
</package>
<package name="SOD-123">
<description>SOD-123 0.91x1.22 mm pad</description>
</package>
<package name="SOD-323F">
<description>SOD-323F 0.8x0.8 mm pad</description>
</package>
<package name="SOIC-16">
</package>
<package name="SOIC-16W">
</package>
<package name="SOIC-20">
</package>
<package name="SOIC-24">
</package>
<package name="SOIC-28W">
</package>
<package name="SOIC-8">
</package>
<package name="SOIC-8W">
</package>
<package name="SOT-223">
</package>
<package name="SOT-23-5">
</package>
<package name="SOT-23-5LT">
<description>5-Lead Small Outline Transistor (LT)</description>
</package>
<package name="SOT-23-6">
</package>
<package name="SOT-23-6L">
</package>
<package name="SOT-23">
</package>
<package name="SSOP-20-DBQ">
<description>SSOP20-DBQ package 0.025 inch pitch</description>
</package>
<package name="SSOP-20">
</package>
<package name="SSOP-28">
<description>SSOP28</description>
</package>
<package name="SSOP-48DL">
<description>&lt;B&gt;Shrink Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SW_MEMBRANE">
</package>
<package name="SW_PUSH_BUTTON_MINI">
</package>
<package name="SW_TACT_SMALL">
</package>
<package name="TC-26">
<description>2mm dia 6.0mm height</description>
</package>
<package name="TC-38">
<description>3mm dia 8.3mm height</description>
</package>
<package name="TO-220-2">
</package>
<package name="TO-220V">
<description>TO-220 Vertical mount, 0.1" (2.5mm) pitch</description>
</package>
<package name="TO-92">
</package>
<package name="TQFN-40-5X5">
</package>
<package name="TQFP-100-12X12">
<description>100-Lead Plastic Thin Quad Flatpack</description>
</package>
<package name="TQFP-100">
<description>100-Lead Plastic Thin Quad Flatpack</description>
</package>
<package name="TQFP-144">
</package>
<package name="TQFP-44">
</package>
<package name="TQFP-64-10X10">
</package>
<package name="TRIMMER_3362P">
<description>1/4 inch trimpot</description>
</package>
<package name="TSSOP-16">
</package>
<package name="TSSOP-28">
<description>Thin Shrink Small Outline Plastic 28 (TSSOP28)</description>
</package>
<package name="TSSOP-48">
</package>
<package name="VQ-100">
</package>
<package name="VQ-44">
</package>
<package name="XTAL_4X6">
<description>3.6mm * 6mm dimension &lt;br&gt;
12MHz available</description>
</package>
<package name="XTAL_5X8">
<description>4.5mm * 8mm dimension &lt;br&gt;
12MHz available</description>
</package>
<package name="DISP_LCD_4X20">
</package>
<package name="L1812">
</package>
<package name="HC-49U-PTH">
</package>
<package name="DC_BARREL_JACK_PTH_2MM">
<description>DC barrel jack PTH 2.1mm pin, 6.0mm barrel</description>
</package>
<package name="MSOP-10">
<description>Exposed Pad 0.5mm pitch</description>
</package>
<package name="CONN_USB_MICRO-B">
<description>USB micro-b connector SMT 0.65 mm pitch,
1.45mm from center to PCB edge,
Based on TE part number 1981568-1</description>
</package>
<package name="TRIMMER_3306F">
<description>3306F. 5mm x 2.5mm pitch, 1mm PTH dia</description>
</package>
<package name="PEC12_INCREMENTAL_ENCODER">
<description>Incremental Encoder with switch</description>
</package>
<package name="PINSHRD_PTH_2X07">
<description>Shrouded pin header, 0.1" pitch</description>
</package>
<package name="SSOP-16">
<description>0.4mm x 1.5mm pad dimention, 0.65mm pad pitch</description>
</package>
<package name="DO-214AC">
<description>1.27mm x 2.10mm pad dimention, 2.69mm pitch</description>
</package>
<package name="SSOP-16-FTDI">
<description>SSOP-16, 0.32 x 1.26 mm pad, 0.63mm pitch, 6.82mm Pad length</description>
</package>
<package name="DP8654_V1">
<description>&lt;B&gt;Credit Card sized PCB &lt;/B&gt; &lt;br&gt;
ISO/IEC 7810, ID-1 Standard size 85.60 x 53.98 mm</description>
</package>
<package name="QFN32_5X5">
</package>
<package name="QFN-10">
<description>&lt;b&gt;10 pins Quad Flat Leadless &lt;/b&gt;
&lt;br&gt;Size: 3 x 3 mm
&lt;br&gt;Pads: 0.85 x 0.28 mm pads
&lt;br&gt;Pin Pitch: 0.5mm pitch</description>
</package>
<package name="M2X8">
</package>
<package name="SW_TACT_3X6">
</package>
<package name="TFT18">
</package>
<package name="PINSHRD_PTH_2X10">
<description>Shrouded 2x10 pin header 0.1"/2.54mm pitch</description>
</package>
<package name="M1X2_08_17">
<description>square pad &lt;br&gt;
drill: 0.8 mm &lt;br&gt;
pad diameter: 1.7 mm</description>
</package>
<package name="M1X2_10_17">
<description>square pad &lt;br&gt;
drill: 1 mm &lt;br&gt;
pad diameter: 1.7 mm</description>
</package>
<package name="TERMINAL_BLOCK_2P_5">
<description>wire to board terminal block 2 pins 5mm pitch &lt;br&gt;
Mfr no: 1776244-2 &lt;br&gt;
&lt;a href="http://www.ebay.com/itm/10pcs-2-Pin-Screw-Terminal-Block-Connector-5mm-Pitch-B-/300625175136?pt=LH_DefaultDomain_0&amp;hash=item45fea82260#ht_1330wt_1396"&gt; Ebay &lt;/a&gt;
&lt;br&gt;
&lt;a href="http://www.digikey.com/product-detail/en/1776244-2/A97996-ND/1826859"&gt; Digikey &lt;/a&gt;</description>
</package>
<package name="TERMINAL_BLOCK_3P_5">
<description>wire to board terminal block 3 pins 5mm pitch &lt;br&gt;
Mfr no: 1776244-3 &lt;br&gt;
&lt;a href="http://www.digikey.com/product-detail/en/1776244-3/A97997-ND/1826860"&gt; Digikey &lt;/a&gt;</description>
</package>
<package name="CONN_USB_A_F">
<description>USB AF SMD &lt;br&gt;
Mfr no. AU-Y1006-2-R&lt;br&gt;
&lt;a href="http://www.digikey.com/product-detail/en/AU-Y1006-2-R/AE10332-ND/2077795"&gt; Digikey &lt;/a&gt;</description>
</package>
<package name="LQFP-32">
</package>
<package name="LOGO_FLAME">
<description>12x16 mm</description>
</package>
<package name="DIL16">
<description>DIL-16</description>
</package>
<package name="DISP_IN-12_SOCKET">
</package>
<package name="DISP_IN-12_SOCKET_CUTOUT">
<description>&lt;B&gt;IN-12 Socket &lt;/B&gt; &lt;br&gt;
Socket cutout: 22 x 28 cm &lt;br&gt;
Mounting drill hole dia: 3.3mm</description>
</package>
<package name="DISP_D8035E">
</package>
<package name="DC_BARREL_JACK_PTH_2MM_2">
</package>
<package name="JOYSTICK_SF303GJ26-3">
</package>
<package name="JUMPER_SOLDER_1X2">
<description>Solder jumper 6mil clearance</description>
</package>
<package name="CON_MICROSD_HINGED">
</package>
<package name="SOIC-14">
<description>SSOP-14, 0.6 x 1.5 mm pad, 1.27mm pad pitch</description>
</package>
<package name="M1X8_SMD">
<description>1x08 0.1" header SMD, 1.00 x 1.90 pad size
&lt;br&gt; Mfr no: NPTC081KFXC-RC
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/NPTC081KFXC-RC/S5600-ND/776058"&gt; NPTC081KFXC-RC&lt;/a&gt;</description>
</package>
<package name="M1X6_SMD">
<description>1x06 0.1" header SMD, 1.00 x 1.90 pad size
&lt;br&gt; Mfr no: NPTC061KFXC-RC
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/NPTC061KFXC-RC/S5598-ND/776056"&gt; NPTC061KFXC-RC&lt;/a&gt;</description>
</package>
<package name="DIL28-SMD">
<description>0.1" pitch 28 DIP socket to SMD
&lt;br&gt; Mfr no: SHD-028-3
&lt;br&gt; &lt;a href="http://oomlout.com/parts/SOCK-28-SMD-datasheet.pdf"&gt; SHD-028-3&lt;/a&gt;</description>
</package>
<package name="SW_TACT_STANDARD_RIGHT_ANGLE">
<description>Tactile switch standard right angled
&lt;br&gt; Mfr no: B3F-3100
&lt;br&gt; &lt;a href="http://www.digikey.com/scripts/dksearch/dksus.dll?vendor=0&amp;keywords=b3f-3100"&gt; B3F-3100&lt;/a&gt;</description>
</package>
<package name="TRIMMER_3314G">
<description>SMD Trimmer 4.5 x 4.5 mm
&lt;br&gt; Mfr no: 3314G
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/3314G-1-103E/3314G-103ETR-ND/87348"&gt; 3314G&lt;/a&gt;</description>
</package>
<package name="M1X6_MALE_RIGHT_ANGLED">
<description>1x06 Right angled male header PTH
&lt;br&gt; Mfr no: 22-28-8060
&lt;br&gt; &lt;a href="http://www.digikey.com/scripts/dksearch/dksus.dll?vendor=0&amp;keywords=22288060"&gt; 22-28-8060&lt;/a&gt;</description>
</package>
<package name="M2X3_SMD">
<description>2x03 Straight male header SMD
&lt;br&gt; Mfr no:5-146134-2
&lt;br&gt; &lt;a href="http://www.digikey.com/product-search/en?x=0&amp;y=0&amp;lang=en&amp;site=us&amp;KeyWords=5-146134-2"&gt; 5-146134-2&lt;/a&gt;</description>
</package>
<package name="M1X6_MALE_RIGHT_ANGLED_SMD">
<description>1x06 Right angled male header SMD
&lt;br&gt; Mfr no: 961106-5500
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/961106-5500-AR-PR/3M9501TR-ND/2071542"&gt; 961106-5500&lt;/a&gt;</description>
</package>
<package name="CON_POGO_ICSP_TARGET">
<description>&lt;B&gt;Pogo pin ICSP target side footprint &lt;/B&gt;
&lt;BR/&gt; pogo pin pad diameter 1.00mm
&lt;BR/&gt; pinout from top left: VCC, GND, MCLR
&lt;BR/&gt; pinout from bottom left:  PGC, PGD</description>
</package>
<package name="CON_POGO_ICSP_PROG">
<description>&lt;B&gt;Pogo pin ICSP programmer side footprint &lt;/B&gt;
&lt;BR/&gt; pogo pin diameter 0.65mm
&lt;BR/&gt; total pogo diameter 1.70mm
&lt;BR/&gt; pinout from top left: MCLR, GND, VCC
&lt;BR/&gt; pinout from bottom left: PGD, PGC, KEY(NC)</description>
</package>
<package name="BB_QFP_050">
<description>&lt;b&gt;QFP 0.5 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (5mm sq)
&lt;br/&gt;48p (7mm sq)
&lt;br/&gt;64p (10mm sq)
&lt;br/&gt;80p (12mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="BB_QFP_050_BREAKOUT_BOARD">
<description>&lt;b&gt;QFP 0.5 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (5mm sq)
&lt;br/&gt;48p (7mm sq)
&lt;br/&gt;64p (10mm sq)
&lt;br/&gt;80p (12mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="BB_QFP_065">
<description>&lt;b&gt;QFP 0.65 mm pitch&lt;/b&gt;
&lt;br/&gt;52p (10mm sq)
&lt;br/&gt;80p (14mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="BB_QFP_065_BREAKOUT_BOARD">
<description>&lt;b&gt;QFP 0.65 mm pitch&lt;/b&gt;
&lt;br/&gt;52p (10mm sq)
&lt;br/&gt;80p (14mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="BB_QFP_080">
<description>&lt;b&gt;QFP 0.8 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (7mm sq)
&lt;br/&gt;44p (10mm sq)
&lt;br/&gt;64p (14mm sq)
&lt;br/&gt;80p (16.5mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="BB_QFP_080_BREAKOUT_BOARD">
<description>&lt;b&gt;QFP 0.8 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (7mm sq)
&lt;br/&gt;44p (10mm sq)
&lt;br/&gt;64p (14mm sq)
&lt;br/&gt;80p (16.5mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="CON_SOLO_STACKER_6_FOOTPRINT">
<description>SOLO Staggard Stocker
&lt;br&gt; Mfr no: 009188006020062
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/009188006020062/478-5491-1-ND/2024954?cur=USD"&gt;  009188006020062&lt;/a&gt;</description>
</package>
<package name="CON_SOLO_STACKER_6_CONNECTOR">
<description>SOLO Staggard Stocker
&lt;br&gt; Mfr no: 009188006020062
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/009188006020062/478-5491-1-ND/2024954?cur=USD"&gt;  009188006020062&lt;/a&gt;</description>
</package>
<package name="BB_QFP_050_065_BREAKOUT_BOARD">
<description>&lt;b&gt;QFP 0.5 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (5mm sq)
&lt;br/&gt;48p (7mm sq)
&lt;br/&gt;64p (10mm sq)
&lt;br/&gt;80p (12mm sq)
&lt;br/&gt;
&lt;br/&gt;
&lt;b&gt;QFP 0.65 mm pitch&lt;/b&gt;
&lt;br/&gt;52p (10mm sq)
&lt;br/&gt;80p (14mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="BB_QFP_080_050_BREAKOUT_BOARD">
<description>&lt;b&gt;QFP 0.5 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (5mm sq)
&lt;br/&gt;48p (7mm sq)
&lt;br/&gt;64p (10mm sq)
&lt;br/&gt;80p (12mm sq)
&lt;br/&gt;
&lt;br/&gt;
&lt;b&gt;QFP 0.8 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (7mm sq)
&lt;br/&gt;44p (10mm sq)
&lt;br/&gt;64p (14mm sq)
&lt;br/&gt;80p (16.5mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="BB_QFP_080_065_BREAKOUT_BOARD">
<description>&lt;b&gt;QFP 0.65 mm pitch&lt;/b&gt;
&lt;br/&gt;52p (10mm sq)
&lt;br/&gt;80p (14mm sq)
&lt;br/&gt;
&lt;br/&gt;
&lt;b&gt;QFP 0.8 mm pitch&lt;/b&gt;
&lt;br/&gt;32p (7mm sq)
&lt;br/&gt;44p (10mm sq)
&lt;br/&gt;64p (14mm sq)
&lt;br/&gt;80p (16.5mm sq)
&lt;br/&gt;&lt;b&gt; CC-BY-SA</description>
</package>
<package name="TSSOP-20">
<description>Pad size: 0.35 x 1.43 mm
&lt;br/&gt;Pad pitch: 0.65 mm
&lt;br/&gt;Pad lateral pitch: 5.4 mm</description>
</package>
<package name="PROTO_VIAS_01X01">
<description>square pad 0.04 inch/1.016 mm drill prototyping block</description>
</package>
</packages>
<symbols>
<symbol name="2032">
<pin name="V1" direction="pwr" function="dotclk"/>
<pin name="V2" direction="pwr" function="dotclk"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="23AXX">
<pin name="+" direction="pwr"/>
<pin name="/CS"/>
<pin name="/HOLD"/>
<pin name="CLK"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="G" direction="pwr"/>
</symbol>
<symbol name="24AA">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="2801A">
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="O8" direction="oc"/>
<pin name="O1" direction="oc"/>
<pin name="O2" direction="oc"/>
<pin name="O3" direction="oc"/>
<pin name="O4" direction="oc"/>
<pin name="O5" direction="oc"/>
<pin name="O6" direction="oc"/>
<pin name="O7" direction="oc"/>
<pin name="CD+" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="2T45">
<pin name="VCCA"/>
<pin name="VCCB"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="DIR"/>
<pin name="GND"/>
</symbol>
<symbol name="3WIRE">
<pin name="CS"/>
<pin name="SK"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="VCC"/>
<pin name="DC"/>
<pin name="ORG"/>
<pin name="GND"/>
</symbol>
<symbol name="4PWR8GND">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
</symbol>
<symbol name="4T245">
<pin name="VCCA" direction="pwr"/>
<pin name="1DIR"/>
<pin name="2DIR"/>
<pin name="1A1"/>
<pin name="1A2"/>
<pin name="2A1"/>
<pin name="2A2"/>
<pin name="GNDB" direction="pwr"/>
<pin name="GNDA" direction="pwr"/>
<pin name="2B2"/>
<pin name="2B1"/>
<pin name="1B2"/>
<pin name="1B1"/>
<pin name="VCCB" direction="pwr"/>
<pin name="1OE" function="dot"/>
<pin name="2OE" function="dot"/>
</symbol>
<symbol name="7416245">
<pin name="1G" direction="in" function="dot"/>
<pin name="1DIR" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2DIR" direction="in" function="dot"/>
<pin name="1B1"/>
<pin name="1B2"/>
<pin name="1B3"/>
<pin name="1B4"/>
<pin name="1B5"/>
<pin name="1B6"/>
<pin name="1B7"/>
<pin name="1B8"/>
<pin name="2B1"/>
<pin name="2B2"/>
<pin name="2B3"/>
<pin name="2B4"/>
<pin name="2B5"/>
<pin name="2B6"/>
<pin name="2B7"/>
<pin name="2B8"/>
<pin name="1A1"/>
<pin name="1A2"/>
<pin name="1A3"/>
<pin name="1A4"/>
<pin name="1A5"/>
<pin name="1A6"/>
<pin name="1A7"/>
<pin name="1A8"/>
<pin name="2A1"/>
<pin name="2A2"/>
<pin name="2A3"/>
<pin name="2A4"/>
<pin name="2A5"/>
<pin name="2A6"/>
<pin name="2A7"/>
<pin name="2A8"/>
</symbol>
<symbol name="74LVC1G125">
<pin name="A" direction="in"/>
<pin name="OE" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="74LVC245A">
<pin name="!OE" direction="in" function="dot"/>
<pin name="DIR" direction="in"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
</symbol>
<symbol name="7SEGCC">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="C1"/>
<pin name="C2"/>
</symbol>
<symbol name="ADS831">
<pin name="CLK" direction="in" function="clk"/>
<pin name="BIT1"/>
<pin name="BIT2"/>
<pin name="BIT3"/>
<pin name="BIT4"/>
<pin name="BIT5"/>
<pin name="BIT6"/>
<pin name="BIT7"/>
<pin name="BIT8"/>
<pin name="RSEL"/>
<pin name="!INT!/EXT"/>
<pin name="!IN"/>
<pin name="IN"/>
<pin name="CM"/>
<pin name="REFB"/>
<pin name="REFT"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="+VS" direction="sup"/>
<pin name="VDRV" direction="pwr"/>
</symbol>
<symbol name="ARDUINO">
<pin name="DIG0_RX"/>
<pin name="DIG1_TX"/>
<pin name="DIG2"/>
<pin name="DIG3_PWM"/>
<pin name="DIG4"/>
<pin name="DIG5_PWM"/>
<pin name="DIG6_PWM"/>
<pin name="DIG7"/>
<pin name="DIG8"/>
<pin name="DIG9_PWM"/>
<pin name="DIG10_PWM"/>
<pin name="DIG11_PWM"/>
<pin name="DIG12"/>
<pin name="DIG13"/>
<pin name="GND0" direction="sup"/>
<pin name="AREF"/>
<pin name="AN5" direction="in"/>
<pin name="AN4" direction="in"/>
<pin name="AN3" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AN0" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND2" direction="sup"/>
<pin name="GND1" direction="sup"/>
<pin name="5V"/>
<pin name="3V3"/>
<pin name="RESET" direction="in"/>
</symbol>
<symbol name="ATMEGA328P">
<pin name="PC6/PCINT14/RESET"/>
<pin name="PD0/PCINT16/RXD"/>
<pin name="PD1/PCINT17/TXD"/>
<pin name="PD3/PCINT19/OC2B/INT1"/>
<pin name="PD2/PCINT18/INT0"/>
<pin name="PD4/PCINT20/XCK/T0"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="PB6/PCINT6/XTAL1/TOSC1"/>
<pin name="PB7/PCINT7/XTAL2/TOSC2"/>
<pin name="PD5/PCINT21/OCOB/T1"/>
<pin name="PD6/PCINT22/OC0A/AIN0"/>
<pin name="PD7/PCINT23/AIN1"/>
<pin name="PB0/PCINT0/CLKO/ICP1"/>
<pin name="PB1/OC1A/PCINT1"/>
<pin name="PB2/SS/OCIB/PCINT2"/>
<pin name="PB3/MOSI/OC2A/PCINT3"/>
<pin name="PB4/MISO/PCINT4"/>
<pin name="PB5/SCK/PCINT5"/>
<pin name="AREF"/>
<pin name="GND2"/>
<pin name="PC0/ADC0/PCINT8"/>
<pin name="PC1/ADC1/PCINT9"/>
<pin name="PC2/ADC2/PCINT10"/>
<pin name="PC3/ADC3/PCINT11"/>
<pin name="PC4/ADC4/SDA/PCINT12"/>
<pin name="PC5/ADC5/SCL/PCINT13"/>
<pin name="AVCC"/>
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP_POL">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="CONN_USB">
<pin name="GND"/>
<pin name="VUSB"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="USBID"/>
</symbol>
<symbol name="CONN_USB_4P">
<pin name="GND"/>
<pin name="VUSB"/>
<pin name="D-"/>
<pin name="D+"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="DC_JACK">
<pin name="P1" direction="pas"/>
<pin name="P3" direction="pas"/>
<pin name="P2" direction="pas"/>
</symbol>
<symbol name="DIL-14">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
</symbol>
<symbol name="DIL-18">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
</symbol>
<symbol name="DIL-20">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
</symbol>
<symbol name="DIL-5">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="DIL-6">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="DIL-8">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="DINA4_L">
</symbol>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DOCFIELD">
</symbol>
<symbol name="DP_LOGO">
</symbol>
<symbol name="DS1085">
<pin name="OUT1" direction="out"/>
<pin name="OUT0" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CTRL0" direction="in"/>
<pin name="CTRL1" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
</symbol>
<symbol name="DS1307">
<pin name="X1"/>
<pin name="X2"/>
<pin name="VBAT"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SQW/OUT"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="DUAL_SCHMITT">
<pin name="1A"/>
<pin name="GND"/>
<pin name="2A"/>
<pin name="2Y"/>
<pin name="VCC"/>
<pin name="1Y"/>
</symbol>
<symbol name="EDGE_CONNECTOR_6X2">
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="B6" direction="pas"/>
</symbol>
<symbol name="ENC424J600">
<pin name="VSSOSC" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="VDDOSC" direction="in"/>
<pin name="AD0"/>
<pin name="AD1" direction="in"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="SCK/AL" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SO/WR/EN"/>
<pin name="SI/RD/RW" direction="in"/>
<pin name="VSS2" direction="in"/>
<pin name="VCAP" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="LEDA" direction="out"/>
<pin name="LEDB" direction="out"/>
<pin name="RBIAS" direction="in"/>
<pin name="VSS1" direction="in"/>
<pin name="PSPCFG0" direction="in"/>
<pin name="INT/SPISEL"/>
<pin name="CLKOUT" direction="out" function="clk"/>
<pin name="VSSTX1" direction="in"/>
<pin name="TPOUT-" direction="out"/>
<pin name="TPOUT+" direction="out"/>
<pin name="VSSTX2" direction="in"/>
<pin name="VDDTX" direction="in"/>
<pin name="TPIN-" direction="in"/>
<pin name="TPIN+" direction="in"/>
<pin name="VDDRX" direction="in"/>
<pin name="VSSRX" direction="in"/>
<pin name="VSSPLL" direction="in"/>
<pin name="VDDPLL" direction="in"/>
</symbol>
<symbol name="EPM3064A">
<pin name="GNDIO@1" direction="sup"/>
<pin name="VCCINT@1" direction="sup"/>
<pin name="C-(7)I/O"/>
<pin name="I/GCLRN"/>
<pin name="I/OE2/GCLK2"/>
<pin name="VCCINT@2" direction="sup"/>
<pin name="A-(6)I/O"/>
<pin name="A-(7)I/O"/>
<pin name="A-(8)I/O"/>
<pin name="A-(1)I/O/TDI"/>
<pin name="A-(2)I/O"/>
<pin name="A-(3)I/O"/>
<pin name="VCCIO@2" direction="sup"/>
<pin name="GNDIO@4" direction="sup"/>
<pin name="D-(3)I/O"/>
<pin name="D-(4)I/O/TDO"/>
<pin name="D-(4)I/O"/>
<pin name="D-(5)I/O"/>
<pin name="GNDINT@2" direction="sup"/>
<pin name="I/GCLK1"/>
<pin name="I/OE1"/>
<pin name="A-(4)I/O"/>
<pin name="A-(5)I/O"/>
<pin name="B-(1)I/O/TMS"/>
<pin name="B-(2)I/O"/>
<pin name="B-(4)I/O"/>
<pin name="B-(5)I/O"/>
<pin name="B-(6)I/O"/>
<pin name="C-(1)I/O"/>
<pin name="GNDINT@1" direction="sup"/>
<pin name="C-(2)I/O"/>
<pin name="C-(3)I/O"/>
<pin name="C-(4)I/O"/>
<pin name="C-(5)I/O"/>
<pin name="C-(6)I/O"/>
<pin name="D-(1)I/O"/>
<pin name="D-(2)I/O"/>
<pin name="GNDIO@2" direction="sup"/>
<pin name="VCCIO@1" direction="sup"/>
<pin name="GNDIO@3" direction="sup"/>
<pin name="B-(3)I/O"/>
<pin name="B-(7)I/O"/>
<pin name="D-(6)I/O"/>
<pin name="C-(8)I/O/TCK"/>
</symbol>
<symbol name="FAN5331">
<pin name="SW"/>
<pin name="GND"/>
<pin name="FB"/>
<pin name="!SHDN"/>
<pin name="VIN"/>
</symbol>
<symbol name="FET">
<pin name="D"/>
<pin name="S"/>
<pin name="G"/>
</symbol>
<symbol name="FT-2232">
<pin name="GND0"/>
<pin name="OSCI"/>
<pin name="OSC0"/>
<pin name="VPHY"/>
<pin name="GND1"/>
<pin name="REF"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="VPLL"/>
<pin name="AGND"/>
<pin name="GND2"/>
<pin name="VCORE0"/>
<pin name="TEST"/>
<pin name="RESET#"/>
<pin name="GND3"/>
<pin name="ADBUS0/TXD/TCK/SK"/>
<pin name="ADBUS1/RXD/TDI/DO"/>
<pin name="ADBUS2/RTS#/TDO/DI"/>
<pin name="ADBUS3/CTS#/TMS/CS"/>
<pin name="VCCIO0"/>
<pin name="ADBUS4/DTR#/GPIOL0"/>
<pin name="ADBUS5/DSR#/GPIOL1"/>
<pin name="ADBUS6/DCD#/GPIOL2"/>
<pin name="ADBUS7/RI#/GPIOL3"/>
<pin name="GND4"/>
<pin name="ACBUS0/TXDEN/GPIOH0"/>
<pin name="ACBUS1/GPIOH1"/>
<pin name="ACBUS2/GPIOH2"/>
<pin name="ACBUS3/RXLED#/GPIOH3"/>
<pin name="ACBUS4/TXLED#/GPIOH4"/>
<pin name="VCCIO1"/>
<pin name="ACBUS5/GPIOH5"/>
<pin name="ACBUS6/GPIOH6"/>
<pin name="ACBUS7/GPIOH7"/>
<pin name="GND5"/>
<pin name="SUSPEND#"/>
<pin name="VCORE1"/>
<pin name="BDBUS0/TXD/TCK/SK"/>
<pin name="BDBUS1/RXD/TDI/DO"/>
<pin name="BDBUS2/RTS#/TDO/DI"/>
<pin name="BDBUS3/CTS#/TMS/CS"/>
<pin name="VCCIO2"/>
<pin name="BDBUS4/DTR#/GPIOL0"/>
<pin name="BDBUS5/DSR#/GPIOL1"/>
<pin name="BDBUS6/DCD#/GPIOL2"/>
<pin name="BDBUS7/RI#/GPIOL3"/>
<pin name="GND6"/>
<pin name="BCBUS0/GPIOH1"/>
<pin name="VREGOUT"/>
<pin name="VREGIN"/>
<pin name="GND7"/>
<pin name="BCBUS1/GPIOH2"/>
<pin name="BCBUS2"/>
<pin name="BCBUS3/RXLED#/GPIOH3"/>
<pin name="BCBUS4/TXLED#/GPIOH4"/>
<pin name="VCCIO3"/>
<pin name="BCBUS5/GPIOH5"/>
<pin name="BCBUS6/GPIOH6"/>
<pin name="BCBUS7/GPIOH7"/>
<pin name="PWREN#"/>
<pin name="EEDATA"/>
<pin name="EECLK"/>
<pin name="EECS"/>
<pin name="VCORE2"/>
</symbol>
<symbol name="FT232RL-VER2">
<pin name="VCCIO" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="NC1" direction="nc"/>
<pin name="RESET#" direction="in"/>
<pin name="NC2" direction="nc"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="3V3OUT" direction="out"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS#"/>
<pin name="CTS#"/>
<pin name="DTR#"/>
<pin name="DSR#"/>
<pin name="DCD#"/>
<pin name="RI#"/>
<pin name="CBUS0"/>
<pin name="CBUS1"/>
<pin name="CBUS2"/>
<pin name="CBUS3"/>
<pin name="CBUS4"/>
<pin name="AGND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="TEST" direction="in"/>
</symbol>
<symbol name="FT232RL">
<pin name="3V3OUT"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="!RESET" function="dot"/>
<pin name="OSCI"/>
<pin name="OSCO"/>
<pin name="TEST"/>
<pin name="AGND"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="VCC"/>
<pin name="VCCIO"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="!DTR" function="dot"/>
<pin name="!DSR" function="dot"/>
<pin name="!RTS" function="dot"/>
<pin name="!CTS" function="dot"/>
<pin name="!DCD" function="dot"/>
<pin name="!RI" function="dot"/>
<pin name="!TXLED" function="dot"/>
<pin name="!RXLED" function="dot"/>
<pin name="TXDEN"/>
<pin name="!PWREN" function="dot"/>
<pin name="!SLEEP" function="dot"/>
</symbol>
<symbol name="FUSE_PTC">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="HDR-BUSPIRATE">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER1X1">
<pin name="1" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER1X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER1X3">
<pin name="1" function="dot"/>
<pin name="2" function="dot"/>
<pin name="3" function="dot"/>
</symbol>
<symbol name="HEADER1X4">
<pin name="1" function="dot"/>
<pin name="2" function="dot"/>
<pin name="3" function="dot"/>
<pin name="4" function="dot"/>
</symbol>
<symbol name="HEADER1X5">
<pin name="1" function="dot"/>
<pin name="2" function="dot"/>
<pin name="3" function="dot"/>
<pin name="4" function="dot"/>
<pin name="5" function="dot"/>
</symbol>
<symbol name="HEADER1X6">
<pin name="1" function="dot"/>
<pin name="2" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER1X8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER2X4">
<pin name="P$1" direction="pas" function="dot"/>
<pin name="P$2" direction="pas" function="dot"/>
<pin name="P$3" direction="pas" function="dot"/>
<pin name="P$4" direction="pas" function="dot"/>
<pin name="P$5" direction="pas" function="dot"/>
<pin name="P$6" direction="pas" function="dot"/>
<pin name="P$7" direction="pas" function="dot"/>
<pin name="P$8" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="HEADER2X6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="HR911105A">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JOYSTICK">
<pin name="LEFT"/>
<pin name="DOWN"/>
<pin name="RIGHT"/>
<pin name="UP"/>
<pin name="COM"/>
<pin name="ACT"/>
</symbol>
<symbol name="JUMP2_DESC">
</symbol>
<symbol name="JUMP2X2_DESC">
</symbol>
<symbol name="JUMP3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="JUMP3_DESC">
</symbol>
<symbol name="LC4032V">
<pin name="A7"/>
<pin name="B-CLK2/I"/>
<pin name="B6"/>
<pin name="A-CLK/I"/>
<pin name="A-A0/GOE"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="TDI" direction="in"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="B8"/>
<pin name="B9"/>
<pin name="B10"/>
<pin name="TDO" direction="out"/>
<pin name="VCC@2"/>
<pin name="GND@2"/>
<pin name="B13"/>
<pin name="B14"/>
<pin name="B-B15/GOE"/>
<pin name="A-GND"/>
<pin name="A-VCCO"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="GND@1"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="B0"/>
<pin name="A15"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="TMS" direction="in"/>
<pin name="B-GND"/>
<pin name="B-VCCO"/>
<pin name="VCC@1"/>
<pin name="A10"/>
<pin name="B5"/>
<pin name="TCK" direction="in"/>
<pin name="A14"/>
<pin name="B12"/>
<pin name="B7"/>
</symbol>
<symbol name="LD-1117">
<pin name="GND"/>
<pin name="VIN"/>
<pin name="VOUT"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LM4910">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="!SHUTDOWN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
<pin name="VO3" direction="out"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="LOGO_CC-0">
</symbol>
<symbol name="LOGO_CC_BY_SA">
</symbol>
<symbol name="LPC1343">
<pin name="PIO2_6"/>
<pin name="PIO2_0"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO0_1/USB_FTOGGLE"/>
<pin name="VSS." direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="XTALOUT" direction="out"/>
<pin name="VDD." direction="pwr"/>
<pin name="PIO1_8"/>
<pin name="PIO0_2"/>
<pin name="PIO2_7"/>
<pin name="PIO2_8"/>
<pin name="PIO2_1"/>
<pin name="PIO0_3/USB_VBUS"/>
<pin name="PIO0_4"/>
<pin name="PIO0_5"/>
<pin name="PIO1_9"/>
<pin name="PIO2_4"/>
<pin name="USB_DM"/>
<pin name="USB_DP"/>
<pin name="PIO2_5"/>
<pin name="PIO0_6/USB_CONNECT"/>
<pin name="PIO0_7"/>
<pin name="PIO2_9"/>
<pin name="PIO2_10"/>
<pin name="PIO2_2"/>
<pin name="PIO0_8"/>
<pin name="PIO0_9"/>
<pin name="PIO0_10"/>
<pin name="PIO1_10"/>
<pin name="PIO2_11"/>
<pin name="PIO0_11"/>
<pin name="PIO1_0"/>
<pin name="PIO1_1"/>
<pin name="PIO1_2"/>
<pin name="PIO3_0"/>
<pin name="PIO3_1"/>
<pin name="PIO2_3"/>
<pin name="PIO1_3"/>
<pin name="PIO1_4"/>
<pin name="VSS" direction="pwr"/>
<pin name="PIO1_11"/>
<pin name="PIO3_2"/>
<pin name="VDD" direction="pwr"/>
<pin name="PIO1_5"/>
<pin name="PIO1_6"/>
<pin name="PIO1_7"/>
<pin name="PIO3_3"/>
</symbol>
<symbol name="MAX111**">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AIN" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="SCLK" direction="in"/>
</symbol>
<symbol name="MAX14500">
<pin name="CDAT1_3"/>
<pin name="CDAT1_2"/>
<pin name="CDAT1_1"/>
<pin name="CDAT1_0"/>
<pin name="CCMD1"/>
<pin name="CCLK1"/>
<pin name="CCPRS"/>
<pin name="HDAT1_3"/>
<pin name="HDAT1_2"/>
<pin name="HDAT1_1"/>
<pin name="HDAT1_0"/>
<pin name="HCMD1"/>
<pin name="HCKL1"/>
<pin name="HCPRS"/>
<pin name="CLDO"/>
<pin name="RREF"/>
<pin name="KVBUS"/>
<pin name="CD+"/>
<pin name="CD-"/>
<pin name="HD+"/>
<pin name="HD-"/>
<pin name="VSD"/>
<pin name="VCC"/>
<pin name="FREF"/>
<pin name="VTM"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="ADD"/>
<pin name="I2C_SEL"/>
<pin name="!BERR"/>
<pin name="!BUSY"/>
<pin name="MODE"/>
<pin name="VIO"/>
<pin name="GND2"/>
<pin name="NC2"/>
<pin name="GND1"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="NC1"/>
<pin name="EXPAD"/>
<pin name="!RST"/>
</symbol>
<symbol name="MAX1896">
<pin name="LX"/>
<pin name="GND"/>
<pin name="FB"/>
<pin name="!SHDN"/>
<pin name="SS"/>
<pin name="IN"/>
</symbol>
<symbol name="MAX31855">
<pin name="GND" direction="pwr"/>
<pin name="T-" direction="in"/>
<pin name="T+" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="DNC" direction="nc"/>
</symbol>
<symbol name="MCP2200">
<pin name="VDD"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="/RST"/>
<pin name="GP7"/>
<pin name="GP6"/>
<pin name="GP5"/>
<pin name="GP4"/>
<pin name="GP3"/>
<pin name="TXD"/>
<pin name="/RTS"/>
<pin name="RXD"/>
<pin name="/CTS"/>
<pin name="GP2"/>
<pin name="GP1"/>
<pin name="GP0"/>
<pin name="VUSB"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="VSS"/>
</symbol>
<symbol name="MCP3021">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="MCP4019">
<pin name="VDD" direction="sup"/>
<pin name="VSS/B" direction="sup"/>
<pin name="SCL" direction="in" function="clk"/>
<pin name="SDA"/>
<pin name="W"/>
</symbol>
<symbol name="MCP4725">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="MCP73831">
<pin name="VDD"/>
<pin name="STAT"/>
<pin name="VSS"/>
<pin name="PROG"/>
<pin name="BAT"/>
</symbol>
<symbol name="MIC5205">
<pin name="OUT"/>
<pin name="BYP"/>
<pin name="IN"/>
<pin name="GND"/>
<pin name="EN"/>
</symbol>
<symbol name="MMA7455L">
<pin name="DVDD_IO" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="IADDR0" direction="in"/>
<pin name="GND2" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!CS" direction="in"/>
<pin name="INT1/DRDY" direction="out"/>
<pin name="INT2" direction="out"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="SDO" direction="out"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SCL/SPC" direction="in"/>
</symbol>
<symbol name="MRF24WBOMA">
<pin name="JT_TDO"/>
<pin name="JT_TDI"/>
<pin name="JT_TCK"/>
<pin name="JT_TMS"/>
<pin name="JT_RST"/>
<pin name="JT_EN"/>
<pin name="RXD"/>
<pin name="TXD"/>
<pin name="SDI"/>
<pin name="SDO"/>
<pin name="SCK"/>
<pin name="!CS"/>
<pin name="!INT"/>
<pin name="!RESET"/>
<pin name="HBRNT"/>
<pin name="!WP"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
<pin name="GND7" direction="pwr"/>
<pin name="GND8" direction="pwr"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
</symbol>
<symbol name="MSP430F21X2">
<pin name="A7/TA1.1/P3.7"/>
<pin name="P2.0/ACLK/A0/CA2"/>
<pin name="CA1/VEREF+/VREF+/A4/TA0.2/P2.4" direction="pwr"/>
<pin name="CAOUT/ADC10CLK/TACLK/P1.0"/>
<pin name="TA1.0/TA0.0/P1.1"/>
<pin name="TA0.1/P1.2"/>
<pin name="TA0.2/P1.3"/>
<pin name="TCK/SMCLK/P1.4"/>
<pin name="TMS/TA0.0/P1.5"/>
<pin name="TCLK/TDI/TA0.1/P1.6"/>
<pin name="TDI/TDO/TA0.2/P1.7"/>
<pin name="TEST/SBWTCK" direction="in"/>
<pin name="DVCC" direction="pwr"/>
<pin name="P2.5/ROSC/CA5"/>
<pin name="DVSS" direction="pwr"/>
<pin name="XOUT/P2.7/CA7"/>
<pin name="XIN/P2.6/CA6"/>
<pin name="!RST!/NMI/SBWTDIO" direction="in"/>
<pin name="CA0/VEREF-/VREF-/A3/TA0.1/P2.3" direction="pwr"/>
<pin name="P2.1/TAINCLK/SMCLK/A1/CA3"/>
<pin name="P2.2/TA0.0/A2/CA4/CAOUT"/>
<pin name="P3.0/UCB0STE/UCA0CLK/A5"/>
<pin name="P3.1/UCB0SIMO/UCB0SDA"/>
<pin name="P3.2/UCB0SOMI/UCB0SCL"/>
<pin name="P3.3/UCB0CLK/UCA0STE"/>
<pin name="UCA0SIMO/UCA0TXD/P3.4"/>
<pin name="UCA0SOMI/UCA0RXD/P3.5"/>
<pin name="A6/TA1.0/P3.6"/>
</symbol>
<symbol name="MSP430G2XX1">
<pin name="P1.5/TA0.0/A5/SCLK/TMS"/>
<pin name="TCLK/TDI/SCL/SDO/A6/TA0.1/P1.6"/>
<pin name="TDI/TDO/SDA/SDI/A7/P1.7"/>
<pin name="SBWTDIO/NMI/!RST" direction="in"/>
<pin name="SBWTCK/TEST" direction="in"/>
<pin name="XOUT/P2.7"/>
<pin name="TA0.1/XIN/P2.6"/>
<pin name="P1.0/TA0CLK/ACLK/A0"/>
<pin name="DVCC" direction="pwr"/>
<pin name="P1.1/TA0.0/A1"/>
<pin name="DVSS" direction="pwr"/>
<pin name="P1.2/TA0.1/A2"/>
<pin name="P1.3/ADC10CLK/A3/VREF-/VEREF-"/>
<pin name="P1.4/SMCLK/A4/VREF+/VEREF+/TCK"/>
</symbol>
<symbol name="N-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="OLED96X16">
<pin name="VSS"/>
<pin name="RES#"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="IREF"/>
<pin name="VCOMH"/>
<pin name="VCC"/>
<pin name="VDD"/>
</symbol>
<symbol name="OPA2830">
<pin name="OUT1"/>
<pin name="INPUT1-"/>
<pin name="INPUT1+"/>
<pin name="VS-"/>
<pin name="INPUT2+"/>
<pin name="INPUT2-"/>
<pin name="OUT2"/>
<pin name="VS+"/>
</symbol>
<symbol name="OPAMP">
<pin name="+" direction="in"/>
<pin name="-" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OPAMP_V+-">
<pin name="+" direction="in"/>
<pin name="-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="V-" direction="sup"/>
</symbol>
<symbol name="OPAMP_V+GND">
<pin name="+" direction="in"/>
<pin name="-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="sup"/>
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="OSCILLATOR">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="P-MOSFET">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="PCB_STANDARD">
</symbol>
<symbol name="PCF8563">
<pin name="OSCI"/>
<pin name="OSCO"/>
<pin name="!INT"/>
<pin name="VSS"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="CLKOUT"/>
<pin name="VDD"/>
</symbol>
<symbol name="PIC10F22X">
<pin name="GP1"/>
<pin name="GP2"/>
<pin name="GP3"/>
<pin name="GP0"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PIC12F1822">
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RA5"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PIC12F508">
<pin name="GP0"/>
<pin name="GP1"/>
<pin name="GP2"/>
<pin name="GP3"/>
<pin name="GP4"/>
<pin name="GP5"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PIC16(L)F1829">
<pin name="VDD" direction="pwr"/>
<pin name="RA5"/>
<pin name="RA4"/>
<pin name="RA3/!MCLR" direction="in"/>
<pin name="RC5"/>
<pin name="RC4"/>
<pin name="RC3"/>
<pin name="RC6"/>
<pin name="RC7"/>
<pin name="RB7"/>
<pin name="RB6"/>
<pin name="RB5"/>
<pin name="RB4"/>
<pin name="RC2"/>
<pin name="RC1"/>
<pin name="RC0"/>
<pin name="RA2"/>
<pin name="RA1/PGC"/>
<pin name="RA0/PGD"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PIC16F1823">
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RA4"/>
<pin name="RA5"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="PIC18F44J50">
<pin name="RC7/RP18/5V/PMA4/RX1/DT1/SDO1"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="INT0/RP3/AN12/RB0"/>
<pin name="RTCC/PMBE/RP4/AN10/RB1"/>
<pin name="REFO/VMO/PMA3/CTEDG1/RP5/AN8/RB2"/>
<pin name="CTEDG2/PMA2/VPO/RP6/AN9/RB3"/>
<pin name="PMA1/KBI0/SCK1/SCL1/5V/RP7/RB4"/>
<pin name="PMA0/KBI1/SDI1/SDA1/5V/RP8/RB5"/>
<pin name="KBI2/PGC/5V/RP9/RB6"/>
<pin name="KBI3/PGD/5V/RP10/RB7"/>
<pin name="!MCLR!/5V" direction="in"/>
<pin name="RA0/AN0/RP0/C1INA/ULPWU/PMA6"/>
<pin name="RA1/AN1/RP1/C2INA/PMA7"/>
<pin name="RA2/AN2/C2INB/VREF-/CVREF"/>
<pin name="RA3/AN3/C1INB/VREF+"/>
<pin name="VDDCORE/VCAP" direction="in"/>
<pin name="RA5/AN4//RP2/!SS1!/HLVDIN/RCV"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA6/OSC2/CLKO"/>
<pin name="RC0/RP11/TIOSO/T1CKI"/>
<pin name="RC1/RP12/T1OSI/!UOE!"/>
<pin name="RC2/AN11/RP13/CTPLS"/>
<pin name="VUSB"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/RP17/5V/PMA5/TX1/CK1"/>
<pin name="RA7/OSC1/CLKI"/>
<pin name="PMD0/SCL2/5V/RD0"/>
<pin name="PMD1/SDA2/5V/RD1"/>
<pin name="PMD2/5V/RP19/RD2"/>
<pin name="PMD3/5V/RP20/RD3"/>
<pin name="PMD4/5V/RP21/RD4"/>
<pin name="PMD5/5V/RP22/RD5"/>
<pin name="PMD6/5V/RP23/RD6"/>
<pin name="PMD7/5V/RP24/RD7"/>
<pin name="PMRD/AN5/RE0"/>
<pin name="PMWR/AN6/RE1"/>
<pin name="PMCS/AN7/RE2"/>
<pin name="VDD@1" direction="pwr"/>
</symbol>
<symbol name="PIC18FJ2X50">
<pin name="RC7/RX1/DT1/SDO1/RP18/5V"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/INT0/RP3"/>
<pin name="RB1/AN10/RTCC/RP4"/>
<pin name="RB2/AN8/VMO/RP5"/>
<pin name="RB3/AN9/VPO/RP6"/>
<pin name="RB4/AN11/KBI0/SCK1/RP7/5V"/>
<pin name="RB5/KBI1/PGM/SDI1/RP8/5V"/>
<pin name="RB6/KBI2/PGC/PR9/5V"/>
<pin name="RB7/BKI3/PGD/RP10/5V"/>
<pin name="!MCLR!/VPP/RE3/5V" direction="in"/>
<pin name="RA0/AN0/RP0"/>
<pin name="RA1/AN1/RP1"/>
<pin name="RA2/AN2/VREF-/CVREF"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="VDDCORE/VCAP"/>
<pin name="RA5/AN4/!SS1!/HLVDIN/RP2"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/TIOSO/T1CKI/RP11"/>
<pin name="RC1/T1OSI/!UOE!/RP12"/>
<pin name="RC2/AN11/RP13"/>
<pin name="VUSB"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/TX1/CK1/RP17/5V"/>
</symbol>
<symbol name="PIC24FJ128GA">
<pin name="RB0/AN0/CN2/VR+/PGD1/RP0"/>
<pin name="RB1/AN1/CN3/VR-/PGC1/RP1"/>
<pin name="RB2/AN2/CN4/RP13"/>
<pin name="RB3/AN3/CN5"/>
<pin name="RB4/AN4/CN6/RP28"/>
<pin name="RB5/AN5/CN7/RP18"/>
<pin name="RB6/AN6/CN24/PGC2/RP6"/>
<pin name="RB7/AN7/CN25/PGD2/RP7"/>
<pin name="RB8/AN8/CN26/RP8"/>
<pin name="RB9/AN9/CN27/RP9"/>
<pin name="RB10/AN10/CN28/TMS"/>
<pin name="RB11/AN11/CN29/TDO"/>
<pin name="RB12/AN12/CN30/TCK"/>
<pin name="RB13/AN13/CN31/TDI"/>
<pin name="RB14/AN14/CN32/RP14"/>
<pin name="RB15/AN15/CN12/RP29"/>
<pin name="RD0/CN49/RP11"/>
<pin name="RD1/CN50/RP24"/>
<pin name="RD2/CN51/RP23"/>
<pin name="RD3/CN52/RP22"/>
<pin name="RD4/CN13/RP25"/>
<pin name="RD5/CN14/RP20"/>
<pin name="RD6/CN15"/>
<pin name="RD7/CN16"/>
<pin name="RD8/CN53/RP2"/>
<pin name="RD9/CN54/RP4"/>
<pin name="RD10/CN55/RP3"/>
<pin name="RD11/CN56/RP12"/>
<pin name="CLKO/OSC2/CN22/RC15"/>
<pin name="CLKI/OSC1/CN23/RC12"/>
<pin name="SCL3/CN64/RE6"/>
<pin name="SDA3/CN65/RE7"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="CN68/RF0"/>
<pin name="CN69/RF1"/>
<pin name="RP30/CN70/RF2"/>
<pin name="RP16/CN71/RF3"/>
<pin name="RP10/SDA2/CN17/RF4"/>
<pin name="RP17/SCL2/CN18/RF5"/>
<pin name="RPI45/CN72/RF6"/>
<pin name="CN58/RE0"/>
<pin name="CN59/RE1"/>
<pin name="SCL1/CN83/RG2"/>
<pin name="SDA1/CN84/RG3"/>
<pin name="RP21/CN8/RG6"/>
<pin name="RP26/CN9/RG7"/>
<pin name="RP19/CN10/RG8"/>
<pin name="RP27/CN11/RG9"/>
<pin name="CN60/RE2"/>
<pin name="CN61/RE3"/>
<pin name="CN62/RE4"/>
<pin name="CN63/RE5"/>
<pin name="MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VCEN" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDDC" direction="pwr"/>
</symbol>
<symbol name="PIC24FJ256GB106">
<pin name="!MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="ENVREG"/>
<pin name="RB0/CN2/PMA6/RP0/VREF+/AN0/PGED1"/>
<pin name="RB1/CN3/RP1/VREF-/AN1/PGEC1"/>
<pin name="RB2/CN4/RP13/VMIO/C2INB/AN2"/>
<pin name="RB3/CN5/VPIO/C2INA/AN3"/>
<pin name="RB4/CN6/RP28/USBOEN/C1INB/AN4/PGED3"/>
<pin name="RB5/CN7/RP18/VBUSON/C1INA/AN5/PGEC3"/>
<pin name="RB6/CN24/RP6/AN6/PGEC2"/>
<pin name="RB7/CN25/RCV/RP7/AN7/PGED2"/>
<pin name="RB8/CN26/RP8/AN8"/>
<pin name="RB9/CN27/PMA7/RP9/AN9"/>
<pin name="RB10/CN28/PMA13/AN10/CVREF/TMS"/>
<pin name="RB11/CN29/PMA12/AN11/TDO"/>
<pin name="RB12/CN30/CTED2/PMA11/AN12/TCK"/>
<pin name="RB13/CN31/CTED1/PMA10/AN13/TDI"/>
<pin name="RB14/CN32/PMA1/RP14/CTPLS/AN14"/>
<pin name="RB15/CN12/PMA0/REFO/RP29/AN15"/>
<pin name="RC12/CN23/CLKI/OSCI"/>
<pin name="RC13/CN1/C3IND/SOSCI"/>
<pin name="RC14/CN0/RPI37/C3INC/T1CK/SOSCO"/>
<pin name="RC15/CN22/CLKO/OSCO"/>
<pin name="RD0/CN49/INT0/RP11/DMH"/>
<pin name="RD1/CN50/RP24/VCPCON"/>
<pin name="RD2/CN51/RP23/DPH"/>
<pin name="RD3/CN52/PMBE/RP22"/>
<pin name="RD4/CN13/PMWR/RP25"/>
<pin name="RD5/CN14/PMRD/RP20"/>
<pin name="RD6/CN15/C3INB"/>
<pin name="RD7/CN16/C3INA"/>
<pin name="RD8/CN53/RP2/DMLN/RTCC"/>
<pin name="RD9/CN54/RP4/SDA1/DPLN"/>
<pin name="RD10/CN55/PMCS2/RP3/SCL1"/>
<pin name="RD11/CN56/PMCS1/RP12"/>
<pin name="RE0/CN58/PMD0"/>
<pin name="RE1/CN59/PMD1"/>
<pin name="RE2/CN60/PMD2"/>
<pin name="RE3/CN61/PMD3"/>
<pin name="RE4/CN62/PMD4"/>
<pin name="RE5/CN63/PMD5"/>
<pin name="RE6/CN64/PMD6/SCL3"/>
<pin name="RE7/CN65/PMD7/SDA3"/>
<pin name="RF0/CN68/VCMPST1/VBUSST"/>
<pin name="RF1/CN69/VCMPST2"/>
<pin name="RF3/CN71/USBID/RP16"/>
<pin name="RF4/CN17/PMA9/RP10/SDA2"/>
<pin name="RF5/CN18/PMA8/RP17/SCL2"/>
<pin name="RG2/D+"/>
<pin name="RG3/D-"/>
<pin name="RG6/CN8/PMA5/RP21/C1IND"/>
<pin name="RG7/CN9/PMA4/RP26/C1INC"/>
<pin name="RG8/CN10/PMA3/RP19/C2IND"/>
<pin name="RG9/CN11/C2INC/PMA2/RP27"/>
<pin name="VBUS"/>
<pin name="VCAP/VDDCORE"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VUSB"/>
</symbol>
<symbol name="PIC24FJ256GB110">
<pin name="RB0/AN0/CN2/PGED1/RP0"/>
<pin name="RB1/AN1/CN3/RP1/PGEC1"/>
<pin name="RB2/AN2/CN4/RP13/C2INB/VMIO"/>
<pin name="RB3/AN3/CN5/C2INA/VPIO"/>
<pin name="RB4/AN4/CN6/RP28/USBOEN/C1INB/PGED3"/>
<pin name="RB5/AN5/CN7/RP18/VBUSON/C1INA/PGEC3"/>
<pin name="RB6/AN6/CN24/PGEC2/RP6"/>
<pin name="RB7/AN7/CN25/PGED2/RCV/RP7"/>
<pin name="RB8/AN8/CN26/RP8"/>
<pin name="RB9/AN9/CN27/RP9"/>
<pin name="RB10/AN10/CN28/PMA13/CVREF"/>
<pin name="RB11/AN11/CN29/PMA12"/>
<pin name="RB12/AN12/CN30/CTED2/PMA11"/>
<pin name="RB13/AN13/CN31/CTED1/PMA10"/>
<pin name="RB14/AN14/CN32/PMA1/CTPLS/RP14"/>
<pin name="RB15/AN15/CN12/PMA0/REFO/RP29"/>
<pin name="RD0/5V/CN49/INT0/DMH/RP11"/>
<pin name="RD1/5V/CN50/VCPCON/RP24"/>
<pin name="RD2/5V/CN51/DPH/RP23"/>
<pin name="RD3/5V/CN52/PMBE/RP22"/>
<pin name="RD4/5V/CN13/PMWR/RP25"/>
<pin name="RD5/5V/CN14/PMRD/RP20"/>
<pin name="RD6/CN15/C3INB"/>
<pin name="RD7/CN16/C3INA"/>
<pin name="RD8/5V/CN53/DMLN/RTCC/RP2"/>
<pin name="RD9/5V/CN54/DPLN/RP4"/>
<pin name="RD10/5V/CN55/PMCS2/RP3"/>
<pin name="RD11/5V/CN56/PMCS1/RP12"/>
<pin name="CLKO/OSCO/CN22/RC15"/>
<pin name="CLKI/OSCI/CN23/RC12"/>
<pin name="SCL3/PMD6/CN64/5V/RE6"/>
<pin name="SDA3/PMD7/CN65/5V/RE7"/>
<pin name="SOSCI/C3IND/CN1/RC13"/>
<pin name="RPI37/SOSCO/C3INC/T1CK/CN0/RC14"/>
<pin name="VBUSST/VCMPST1/CN68/RF0"/>
<pin name="VCMPST2/CN69/5V/RF1"/>
<pin name="RP30/CN70/5V/RF2"/>
<pin name="RP16/USBID/CN71/5V/RF3"/>
<pin name="RP10/PMA9/CN17/5V/RF4"/>
<pin name="RP17/PMA8/CN18/5V/RF5"/>
<pin name="PMD0/CN58/5V/RE0"/>
<pin name="PMD1/CN59/5V/RE1"/>
<pin name="D+/RG2"/>
<pin name="D-/RG3"/>
<pin name="C1IND/RP21/PMA5/CN8/RG6"/>
<pin name="C1INC/RP26/PMA4/CN9/RG7"/>
<pin name="C2IND/RP19/PMA3/CN10/RG8"/>
<pin name="C2INC/RP27/PMA2/CN11/RG9"/>
<pin name="PMD2/CN60/5V/RE2"/>
<pin name="PMD3/CN61/5V/RE3"/>
<pin name="PMD4/CN62/5V/RE4"/>
<pin name="PMD5/CN63/5V/RE5"/>
<pin name="!MCLR" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="RA0/5V/CN33/TMS"/>
<pin name="CN82/5V/RG15"/>
<pin name="RPI38/CN45/5V/RC1"/>
<pin name="RPI39/CN46/5V/RC2"/>
<pin name="RPI40/CN47/5V/RC3"/>
<pin name="RPI41/CN48/5V/RC4"/>
<pin name="RPI33/CN66/5V/RE8"/>
<pin name="RPI34/CN67/5V/RE9"/>
<pin name="RA9/CN41/PMA7/VREF-"/>
<pin name="RA10/CN42/PMA6/VREF+"/>
<pin name="RA1/5V/CN34/TCK"/>
<pin name="RP31/CN76/5V/RF13"/>
<pin name="RPI32/CN75/5V/RF12"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="RD14/5V/CN20/RPI43"/>
<pin name="RD15/5V/CN21/RP5"/>
<pin name="RP15/CN74/5V/RF8"/>
<pin name="VBUS" direction="pwr"/>
<pin name="VUSB" direction="pwr"/>
<pin name="RA2/5V/CN35/SCL2"/>
<pin name="RA3/5V/CN36/SDA2"/>
<pin name="RA4/5V/CN37/TDI"/>
<pin name="RA5/5V/CN38/TDO"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="RA14/5V/CN43/SCL1/RPI36"/>
<pin name="RA15/5V/CN44/SDA1/RPI35"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="RD12/5V/CN57/RPI42"/>
<pin name="RD13/5V/CN19"/>
<pin name="VCAP/VDDCORE" direction="pwr"/>
<pin name="ENVREG" direction="in"/>
<pin name="CN78/5V/RG1"/>
<pin name="CN77/5V/RG0"/>
<pin name="RA6/CN39"/>
<pin name="RA7/5V/CN40"/>
<pin name="CN81/5V/RG14"/>
<pin name="CN79/5V/RG12"/>
<pin name="CN80/5V/RG13"/>
</symbol>
<symbol name="PIC24FJ64GA002">
<pin name="MCLR" direction="in"/>
<pin name="RA0/AN0/CN2/VREF+"/>
<pin name="RA1/AN1/CN3/VREF-"/>
<pin name="RB0/AN2/RP0/CN4/C2IN-/PGD1/EMUD1"/>
<pin name="RB1/AN3/RP1/CN5/C2IN+/PGC1/EMUC1"/>
<pin name="RB2/AN4/RP2/CN6/C1IN-/SDA2"/>
<pin name="RB3/AN5/RP3/CN7/C1IN+/SCL2"/>
<pin name="VSS@1" direction="sup"/>
<pin name="RA2/CN30/OSCI/CLKI"/>
<pin name="RA3/CN29/OSCO/CLKO/PMA0"/>
<pin name="RB4/RP4/CN1/SOSCI/PMBE"/>
<pin name="RA4/CN0/SOSCO/T1CK/PMA1"/>
<pin name="VDD@1" direction="sup"/>
<pin name="RB5/RP5/CN27/PGD3/EMUD3/ASDA1/PMD7"/>
<pin name="PMD6/ASCL1/EMUC3/PGC3/CN24/RP6/RB6"/>
<pin name="PMD5/INT0/CN23/RP7/RB7"/>
<pin name="PMD4/SCL1/TCK/CN22/RP8/RB8"/>
<pin name="PMD3/SDA1/TDO/CN21/RP9/RB9"/>
<pin name="DISVREG" direction="pwr"/>
<pin name="VCAP/VDDCORE" direction="pwr"/>
<pin name="PMD2/TDI/EMUD2/PGD2/CN16/RP10/RB10"/>
<pin name="PMD1/TMS/EMUC2/PGC2/CN15/RP11/RB11"/>
<pin name="PMD0/CN14/RP12/AN12/RB12"/>
<pin name="PMRD/CN13/RP13/AN11/RB13"/>
<pin name="PMWR/RTCC/CVREF/CN12/RP14/AN10/RB14"/>
<pin name="PMCS1/CN11/RP15/AN9/RB15"/>
<pin name="VSS@2" direction="sup"/>
<pin name="VDD@2" direction="sup"/>
</symbol>
<symbol name="PIC24FJ64GB002">
<pin name="!MCLR"/>
<pin name="RA0"/>
<pin name="RA1"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="RA2"/>
<pin name="RA3"/>
<pin name="RB4"/>
<pin name="RA4"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="RB5"/>
<pin name="VBUS" direction="pwr"/>
<pin name="RB7"/>
<pin name="RB8"/>
<pin name="RB9"/>
<pin name="DISVREG" direction="pas"/>
<pin name="VCAP/VDDCORE" direction="pwr"/>
<pin name="RB10/D+"/>
<pin name="RB11/D-"/>
<pin name="VUSB"/>
<pin name="RB13"/>
<pin name="RB14"/>
<pin name="RB15"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="POT">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="PRG_ICSP_AVR">
<pin name="+V" direction="pas" function="dot"/>
<pin name="MISO" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="PRG_ICSP_PIC">
<pin name="+V" direction="pas" function="dot"/>
<pin name="/MCLR" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="PGC" direction="pas" function="dot"/>
<pin name="PGD" direction="pas" function="dot"/>
</symbol>
<symbol name="PRG_SBW_MSP">
<pin name="SBWTCK" direction="pas" function="dot"/>
<pin name="SBWTDIO" direction="pas" function="dot"/>
<pin name="+V" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="QSE15X">
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="RGB">
<pin name="A1"/>
<pin name="A"/>
<pin name="A2"/>
<pin name="R"/>
<pin name="G"/>
<pin name="B"/>
</symbol>
<symbol name="RGB3">
<pin name="CB"/>
<pin name="CR"/>
<pin name="CG"/>
<pin name="AG"/>
<pin name="AR"/>
<pin name="AB"/>
</symbol>
<symbol name="RGBLED">
<pin name="A"/>
<pin name="R"/>
<pin name="G"/>
<pin name="B"/>
</symbol>
<symbol name="SI4707">
<pin name="NC1"/>
<pin name="FMI"/>
<pin name="RFGND"/>
<pin name="NP1"/>
<pin name="!RST"/>
<pin name="!SEN"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="RCLK"/>
<pin name="VIO"/>
<pin name="VDD"/>
<pin name="GND"/>
<pin name="ROUT"/>
<pin name="LOUT"/>
<pin name="NP2"/>
<pin name="NP3"/>
<pin name="GPO3"/>
<pin name="GPO2/!INT"/>
<pin name="GPO1"/>
<pin name="NC2"/>
<pin name="PAD"/>
</symbol>
<symbol name="SLIDE_SWITCH_SMD">
<pin name="COM" direction="pas"/>
<pin name="NC" direction="pas" function="dot"/>
<pin name="NO" direction="pas" function="dot"/>
</symbol>
<symbol name="SN74AVC4T245">
<pin name="VCCA" direction="pwr"/>
<pin name="1DIR"/>
<pin name="2DIR"/>
<pin name="1A1"/>
<pin name="1A2"/>
<pin name="2A1"/>
<pin name="2A2"/>
<pin name="GNDB" direction="pwr"/>
<pin name="GNDA" direction="pwr"/>
<pin name="2B2"/>
<pin name="2B1"/>
<pin name="1B2"/>
<pin name="1B1"/>
<pin name="VCCB" direction="pwr"/>
<pin name="1OE" function="dot"/>
<pin name="2OE" function="dot"/>
</symbol>
<symbol name="SN74LVC1T45">
<pin name="VCCA" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A"/>
<pin name="B"/>
<pin name="DIR" direction="in"/>
<pin name="VCCB" direction="pwr"/>
</symbol>
<symbol name="SN74LVC2T45">
<pin name="VCCA" direction="pwr"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="GND" direction="pwr"/>
<pin name="DIR" direction="in"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="VCCB" direction="pwr"/>
</symbol>
<symbol name="SN74LVC8T245">
<pin name="VCCA" direction="pwr"/>
<pin name="DIR" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="OE" direction="in"/>
<pin name="VCCB2" direction="pwr"/>
<pin name="VCCB1" direction="pwr"/>
</symbol>
<symbol name="SRAM">
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="!CS" direction="in" function="dot"/>
<pin name="!HOLD" direction="in" function="dot"/>
</symbol>
<symbol name="STM32-48">
<pin name="PA0-WKUP"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8/USART1_CK/MCO"/>
<pin name="PA9/USART1_TX"/>
<pin name="PA10.USART1_RX"/>
<pin name="PA11/USART1_CTS/USBDM"/>
<pin name="PA12/USART1_RTS/USBDP"/>
<pin name="PA13/JTMS-SWDIO"/>
<pin name="PA14/JTCK/SWCLK"/>
<pin name="PA15/JTDI"/>
<pin name="VBAT"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="sup"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VSS_3" direction="sup"/>
<pin name="VSS_2" direction="sup"/>
<pin name="VSS_1" direction="sup"/>
<pin name="NRST"/>
<pin name="PD1-OSC_OUT"/>
<pin name="PD0-OSC_IN"/>
<pin name="PC15-OSC32_OUT"/>
<pin name="PC14-0SC32_IN"/>
<pin name="PC13-TAMPER-RTC"/>
<pin name="BOOT0"/>
<pin name="PB15"/>
<pin name="PB14"/>
<pin name="PB13"/>
<pin name="PB12"/>
<pin name="PB11"/>
<pin name="PB10"/>
<pin name="PB9"/>
<pin name="PB8"/>
<pin name="PB7/I2C_SDA"/>
<pin name="PB6/I2C_SCL"/>
<pin name="PB5/I2C_SMBA"/>
<pin name="PB4/JNTRST"/>
<pin name="PB3/JTDO"/>
<pin name="PB2"/>
<pin name="PB1"/>
<pin name="PB0"/>
</symbol>
<symbol name="STM32F103RX">
<pin name="PA0/ADC0/USART2_CTS/TIM2_CH1_ETR/WKUP"/>
<pin name="PA1/ADC1/USART2_RTS/TIM2_CH2"/>
<pin name="PA2/ADC2/USART2_TX/TIM2_CH4"/>
<pin name="PA3/ADC3/USART2_RX/TIM2_CH4"/>
<pin name="PA4/ADC4/USART2_CK/SPI1_NSS"/>
<pin name="PA5/ADC5/SPI1_SCK"/>
<pin name="PA6/ADC6/SPI1_MISO/TIM3_CH1"/>
<pin name="PA7/ADC7/SPI1_MOSI/TIM3_CH2"/>
<pin name="PA8/5V/USART1_CK/TIM1_CH1/MCO"/>
<pin name="PA9/5V/USART1_TX/TIM1_CH2"/>
<pin name="PA10/5V/USART1_RX/TIM1_CH3"/>
<pin name="PA11/5V/USART1_CTS/TIM1_CH4/CAN_RX/USB_D-"/>
<pin name="PA12/5V/USART1_RTS/TIM1_ETR/CAN_TX/USB_D+"/>
<pin name="PA13/5V/JTMS/SWDIO"/>
<pin name="PA14/5V/JTCK/SWCLK"/>
<pin name="PA15/5V/JTDI"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="sup"/>
<pin name="VDD_1" direction="pwr"/>
<pin name="VDD_2" direction="pwr"/>
<pin name="VDD_3" direction="pwr"/>
<pin name="VSS_3" direction="sup"/>
<pin name="VSS_2" direction="sup"/>
<pin name="VSS_1" direction="sup"/>
<pin name="NRST"/>
<pin name="PD1/5V/OSC_OUT" direction="out"/>
<pin name="PD0/5V/OSC_IN" direction="in"/>
<pin name="OSC32_OUT/PC15"/>
<pin name="OSC32_IN/PC14"/>
<pin name="TAMPER-RTC/PC13"/>
<pin name="BOOT0" direction="in"/>
<pin name="SPI2_MOSI/TIM1_CH3N/5V/PB15"/>
<pin name="SPI2_MISO/USART3_RTS/TIM1_CH2N/5V/PB14"/>
<pin name="SPI2_SCK/USART3_CTS/TIM1_CH1N/5V/PB13"/>
<pin name="SPI2_NSS/I2C2_SMBAI/USART3_CK/TIM1_BKIN/5V/PB12"/>
<pin name="I2C2_SDA/USART3_RX/5V/PB11"/>
<pin name="I2C2_SCL/USART3_TX/5V/PB10"/>
<pin name="TIM4_CH4/5V/PB9"/>
<pin name="TIM4_CH3/5V/PB8"/>
<pin name="I2C1_SDA/TIM4_CH2/5V/PB7"/>
<pin name="I2C1_SCL/TIM4_CH1/5V/PB6"/>
<pin name="I2C1_SMBAI/PB5"/>
<pin name="JNTRST/5V/PB4"/>
<pin name="JTDO/5V/PB3"/>
<pin name="BOOT1/5V/PB2"/>
<pin name="TIM3_CH4/ADC9/PB1"/>
<pin name="TIM3_CH3/ADC8/PB0"/>
<pin name="ADC10/PC0"/>
<pin name="ADC11/PC1"/>
<pin name="ADC12/PC2"/>
<pin name="ADC13/PC3"/>
<pin name="VSS_4" direction="sup"/>
<pin name="VDD_4" direction="pwr"/>
<pin name="ADC14/PC4"/>
<pin name="ADC15/PC5"/>
<pin name="5V/PC6"/>
<pin name="5V/PC7"/>
<pin name="5V/PC8"/>
<pin name="5V/PC9"/>
<pin name="5V/PC10"/>
<pin name="5V/PC11"/>
<pin name="5V/PC12"/>
<pin name="PD2/5V/TIM3_ETR"/>
</symbol>
<symbol name="SUPPLY">
<pin name="V+" direction="sup"/>
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="SW_DPDT">
<pin name="COM1" direction="pas"/>
<pin name="NC1" direction="pas" function="dot"/>
<pin name="NO1" direction="pas" function="dot"/>
<pin name="COM2" direction="pas"/>
<pin name="NC2" direction="pas" function="dot"/>
<pin name="NO2" direction="pas" function="dot"/>
</symbol>
<symbol name="SW_MEMBRANE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SWITCH_2">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TC74">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="TERMINAL">
<pin name="P" direction="pas" function="dot"/>
</symbol>
<symbol name="TMP006">
<pin name="V+" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="ADR1" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="ADR0" direction="in"/>
<pin name="!DRDY" direction="out"/>
<pin name="SDA"/>
</symbol>
<symbol name="TPIC6B595">
<pin name="DRAIN7" direction="out"/>
<pin name="DRAIN6" direction="out"/>
<pin name="DRAIN5" direction="out"/>
<pin name="DRAIN4" direction="out"/>
<pin name="DRAIN3" direction="out"/>
<pin name="DRAIN2" direction="out"/>
<pin name="DRAIN1" direction="out"/>
<pin name="DRAIN0" direction="out"/>
<pin name="SEROUT" direction="out"/>
<pin name="SERIN" direction="in"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="!SCLR" direction="in" function="dot"/>
<pin name="SRCK" direction="in" function="clk"/>
<pin name="!G" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
</symbol>
<symbol name="TPS2041B">
<pin name="IN" direction="in"/>
<pin name="!OC" direction="out" function="dot"/>
<pin name="!EN" direction="in" function="dot"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TXB0108">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="GND"/>
<pin name="OE"/>
<pin name="VA"/>
<pin name="VB"/>
</symbol>
<symbol name="ULN2803">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
</symbol>
<symbol name="USB2514">
<pin name="USBDN_DP1"/>
<pin name="USBDN_DM1"/>
<pin name="USBDN_DP2"/>
<pin name="USBDN_DM2"/>
<pin name="USBDN_DP3"/>
<pin name="USBDN_DM3"/>
<pin name="USBDN_DP4"/>
<pin name="USBDN_DM4"/>
<pin name="USBUP_DP"/>
<pin name="USBUP_DM"/>
<pin name="VBUS"/>
<pin name="PRTPWR1"/>
<pin name="OCS1"/>
<pin name="PRTPWR2"/>
<pin name="OCS2"/>
<pin name="PRTPWR3"/>
<pin name="OCS3"/>
<pin name="PRTPWR4"/>
<pin name="OCS4"/>
<pin name="RBIAS"/>
<pin name="HS_IND/CFG_SEL1"/>
<pin name="SUSPEND/NON_REM0"/>
<pin name="SDA/NON_REM1"/>
<pin name="SCL/CFG_SEL0"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="!RESET"/>
<pin name="TEST"/>
<pin name="VSS"/>
<pin name="VDD18"/>
<pin name="VDD33PLL"/>
<pin name="VDD18PLL"/>
<pin name="VDDA33_1"/>
<pin name="VDDA33_2"/>
<pin name="VDDA33_3"/>
<pin name="VDD33CR_1"/>
<pin name="VDD33CR_2"/>
</symbol>
<symbol name="USB_BODY_PINS">
<pin name="BODY@4" direction="hiz"/>
<pin name="BODY@3" direction="hiz"/>
<pin name="BODY@1" direction="hiz"/>
<pin name="BODY@2" direction="hiz"/>
</symbol>
<symbol name="USB_BODY_PINS2">
<pin name="BODY@4" direction="hiz"/>
<pin name="BODY@3" direction="hiz"/>
<pin name="BODY@1" direction="hiz"/>
<pin name="BODY@2" direction="hiz"/>
</symbol>
<symbol name="USBLC">
<pin name="I/O_1"/>
<pin name="GND"/>
<pin name="I/O_2"/>
<pin name="I/O2"/>
<pin name="VBUS"/>
<pin name="I/O1"/>
</symbol>
<symbol name="W25X10">
<pin name="CS"/>
<pin name="DO"/>
<pin name="WP"/>
<pin name="GND" direction="pwr"/>
<pin name="DIO"/>
<pin name="CLK"/>
<pin name="HOLD"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="XC2C32A_VQ44-IAN">
<pin name="IO_22"/>
<pin name="IO_23"/>
<pin name="IO_24"/>
<pin name="GND@0" direction="pwr"/>
<pin name="IO_25"/>
<pin name="IO_26"/>
<pin name="VDDIO1" direction="pwr"/>
<pin name="IO_27"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="IO_28"/>
<pin name="IO_29"/>
<pin name="IO_30"/>
<pin name="VDDINT" direction="pwr"/>
<pin name="IO_31"/>
<pin name="GND@1" direction="pwr"/>
<pin name="IN_32" direction="in"/>
<pin name="IO_15"/>
<pin name="IO_14"/>
<pin name="IO_13"/>
<pin name="IO_12"/>
<pin name="IO_11"/>
<pin name="TDO" direction="out"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDDIO2" direction="pwr"/>
<pin name="IO_10"/>
<pin name="IO_9"/>
<pin name="IO_8"/>
<pin name="IO_7"/>
<pin name="IO_6"/>
<pin name="IO_5"/>
<pin name="IO_4"/>
<pin name="IO_3"/>
<pin name="VDDAUX" direction="pwr"/>
<pin name="IO_2"/>
<pin name="IO_1"/>
<pin name="IO_0"/>
<pin name="IO_16"/>
<pin name="IO_17"/>
<pin name="IO_18"/>
<pin name="IO_19"/>
<pin name="IO_20"/>
<pin name="IO_21"/>
</symbol>
<symbol name="XC3S100E">
<pin name="P$1_PROG_B"/>
<pin name="P$2_IO_L01P_3"/>
<pin name="P$3_IO_L01N_3"/>
<pin name="P$4_IO_L02P_3"/>
<pin name="P$5_IO_L02N_3"/>
<pin name="P$6_VCCINT"/>
<pin name="P$7_GND"/>
<pin name="P$8_VCCO_3"/>
<pin name="P$9_IO_L03P_3"/>
<pin name="P$10_IO_L03N_3"/>
<pin name="P$11_IO_L04P_3"/>
<pin name="P$12_IO_L04N_3"/>
<pin name="P$13_IP"/>
<pin name="P$14_GND"/>
<pin name="P$15_IO_L05P_3"/>
<pin name="P$16_IO_L05N_3"/>
<pin name="P$17_IO_L06P_3"/>
<pin name="P$18_IO_L06N_3"/>
<pin name="P$19_GND"/>
<pin name="P$20_VCCO_3"/>
<pin name="P$21_VCCAUX"/>
<pin name="P$22_IO_L07P_3"/>
<pin name="P$23_IO_L07N_3"/>
<pin name="P$24_IO_L01P_2"/>
<pin name="P$25_IO_L01N_2"/>
<pin name="P$26_IO_L02P_2"/>
<pin name="P$27_IO_L02N_2"/>
<pin name="P$28_VCCINT"/>
<pin name="P$29_GND"/>
<pin name="P$30_IP"/>
<pin name="P$31_VCCO_2"/>
<pin name="P$32_IO_L03P_2"/>
<pin name="P$33_IO_L03N_2"/>
<pin name="P$34_IO"/>
<pin name="P$35_IO_L04P_2"/>
<pin name="P$36_IO_L04N_2"/>
<pin name="P$37_GND"/>
<pin name="P$38_IP_L05P_2"/>
<pin name="P$39_IP_L05N_2"/>
<pin name="P$40_IO_L06P_2"/>
<pin name="P$41_IO_L06N_2"/>
<pin name="P$42_IO"/>
<pin name="P$43_IO_L07P_2"/>
<pin name="P$44_IO_L07N_2"/>
<pin name="P$45_VCCO_2"/>
<pin name="P$46_VCCAUX"/>
<pin name="P$47_IO_L08P_2"/>
<pin name="P$48_L08N_2"/>
<pin name="P$49_IO_L09P_2"/>
<pin name="P$50_IO_L09N_2"/>
<pin name="P$51_DONE"/>
<pin name="P$52_GND"/>
<pin name="P$53_IO_L01P_1"/>
<pin name="P$54_IO_L01N_1"/>
<pin name="P$55_VCCO_1"/>
<pin name="P$56_VCCINT"/>
<pin name="P$57_IO_L02P_1"/>
<pin name="P$58_IO_L02N_1"/>
<pin name="P$59_GND"/>
<pin name="P$60_IO_L03P_1"/>
<pin name="P$61_IO_L03N_1"/>
<pin name="P$62_IO_L04P_1"/>
<pin name="P$63_IO_L04N_1"/>
<pin name="P$64_GND"/>
<pin name="P$65_IO_L05P_1"/>
<pin name="P$66_IO_L05N_1"/>
<pin name="P$67_IO_L06P_1"/>
<pin name="P$68_IO_L06N_1"/>
<pin name="P$69_IP"/>
<pin name="P$70_IO_L07P_1"/>
<pin name="P$71_IO_L07N_1"/>
<pin name="P$72_GND"/>
<pin name="P$73_VCCO_1"/>
<pin name="P$74_VCCAUX"/>
<pin name="P$75_TMS"/>
<pin name="P$76_TDO"/>
<pin name="P$77_TCK"/>
<pin name="P$78_IO_L01P_0"/>
<pin name="P$79_IO_L01N_0"/>
<pin name="P$80_VCCINT"/>
<pin name="P$81_GND"/>
<pin name="P$82_VCCO_0"/>
<pin name="P$83_IO_L02P_0"/>
<pin name="P$84_IO_L02N_0"/>
<pin name="P$85_IO_L03P_0"/>
<pin name="P$86_IO_L03N_0"/>
<pin name="P$87_GND"/>
<pin name="P$88_IP_L04P_0"/>
<pin name="P$89_IP_L04N_0"/>
<pin name="P$90_IO_L05P_0"/>
<pin name="P$91_IO_L05N_0"/>
<pin name="P$92_IO"/>
<pin name="P$93_GND"/>
<pin name="P$94_IO_L06P_0"/>
<pin name="P$95_IO_L06N_0"/>
<pin name="P$96_VCCAUX"/>
<pin name="P$97_VCCO_0"/>
<pin name="P$98_IO_L07P_0"/>
<pin name="P$99_IO_L07N_0"/>
<pin name="P$100_TDI"/>
</symbol>
<symbol name="XC3S250E_VQ100">
<pin name="PROG_B" direction="in"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="VCCINT@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCCO_3@1" direction="pwr"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="IPAD152" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCCO_3@2" direction="pwr"/>
<pin name="VCCAUX@1" direction="pwr"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="VCCINT@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="IPAD114" direction="in"/>
<pin name="VCCO_2@1" direction="pwr"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="P36"/>
<pin name="GND@5" direction="pwr"/>
<pin name="IPAD108" direction="in"/>
<pin name="IPAD107" direction="in"/>
<pin name="P40"/>
<pin name="P41"/>
<pin name="P42"/>
<pin name="P43"/>
<pin name="P44"/>
<pin name="VCCO_2@2" direction="pwr"/>
<pin name="VCCAUX@2" direction="pwr"/>
<pin name="P47"/>
<pin name="P48"/>
<pin name="P49"/>
<pin name="P50"/>
<pin name="DONE"/>
<pin name="GND@6" direction="pwr"/>
<pin name="P53"/>
<pin name="P54"/>
<pin name="VCCO_1@1" direction="pwr"/>
<pin name="VCCINT@3" direction="pwr"/>
<pin name="P57"/>
<pin name="P58"/>
<pin name="GND@7" direction="pwr"/>
<pin name="P60"/>
<pin name="P61"/>
<pin name="P62"/>
<pin name="P63"/>
<pin name="GND@8" direction="pwr"/>
<pin name="P65"/>
<pin name="P66"/>
<pin name="P67"/>
<pin name="P68"/>
<pin name="IPAD61" direction="in"/>
<pin name="P70"/>
<pin name="P71"/>
<pin name="GND@9" direction="pwr"/>
<pin name="VCCO_1@2" direction="pwr"/>
<pin name="VCCAUX@3" direction="pwr"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="P78"/>
<pin name="P79"/>
<pin name="VCCINT@4" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="VCCO_0@1" direction="pwr"/>
<pin name="P83"/>
<pin name="P84"/>
<pin name="P85"/>
<pin name="P86"/>
<pin name="GND@11" direction="pwr"/>
<pin name="IPAD22" direction="in"/>
<pin name="IPAD21" direction="in"/>
<pin name="P90"/>
<pin name="P91"/>
<pin name="P92"/>
<pin name="GND@12" direction="pwr"/>
<pin name="P94"/>
<pin name="P95"/>
<pin name="VCCAUX@4" direction="pwr"/>
<pin name="VCCO_0@2" direction="pwr"/>
<pin name="P98"/>
<pin name="PUDC_B" direction="in"/>
<pin name="TDI" direction="in"/>
</symbol>
<symbol name="XC3S250E_VQ100_1532">
<pin name="DONE"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="IPAD107" direction="in"/>
<pin name="IPAD108" direction="in"/>
<pin name="IPAD114" direction="in"/>
<pin name="IPAD152" direction="in"/>
<pin name="IPAD21" direction="in"/>
<pin name="IPAD22" direction="in"/>
<pin name="IPAD61" direction="in"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P2"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P3"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="P36"/>
<pin name="P4"/>
<pin name="P40"/>
<pin name="P41"/>
<pin name="P42"/>
<pin name="P43"/>
<pin name="P44"/>
<pin name="P47"/>
<pin name="P48"/>
<pin name="P49"/>
<pin name="P5"/>
<pin name="P50"/>
<pin name="P53"/>
<pin name="P54"/>
<pin name="P57"/>
<pin name="P58"/>
<pin name="P60"/>
<pin name="P61"/>
<pin name="P62"/>
<pin name="P63"/>
<pin name="P65"/>
<pin name="P66"/>
<pin name="P67"/>
<pin name="P68"/>
<pin name="P70"/>
<pin name="P71"/>
<pin name="P78"/>
<pin name="P79"/>
<pin name="P83"/>
<pin name="P84"/>
<pin name="P85"/>
<pin name="P86"/>
<pin name="P9"/>
<pin name="P90"/>
<pin name="P91"/>
<pin name="P92"/>
<pin name="P94"/>
<pin name="P95"/>
<pin name="P98"/>
<pin name="PROG_B" direction="in"/>
<pin name="PUDC_B" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="VCCAUX@1" direction="pwr"/>
<pin name="VCCAUX@2" direction="pwr"/>
<pin name="VCCAUX@3" direction="pwr"/>
<pin name="VCCAUX@4" direction="pwr"/>
<pin name="VCCINT@1" direction="pwr"/>
<pin name="VCCINT@2" direction="pwr"/>
<pin name="VCCINT@3" direction="pwr"/>
<pin name="VCCINT@4" direction="pwr"/>
<pin name="VCCO_0@1" direction="pwr"/>
<pin name="VCCO_0@2" direction="pwr"/>
<pin name="VCCO_1@1" direction="pwr"/>
<pin name="VCCO_1@2" direction="pwr"/>
<pin name="VCCO_2@1" direction="pwr"/>
<pin name="VCCO_2@2" direction="pwr"/>
<pin name="VCCO_3@1" direction="pwr"/>
<pin name="VCCO_3@2" direction="pwr"/>
</symbol>
<symbol name="XC6SLX9-3TQG144C">
<pin name="IO_L83N_VREF_3"/>
<pin name="IO_L83P_3"/>
<pin name="GND_A" direction="pwr"/>
<pin name="VCCO_BANK3_A" direction="pwr"/>
<pin name="IO_L52N_3"/>
<pin name="IO_L52P_3"/>
<pin name="IO_L51N_3"/>
<pin name="IO_L51P_3"/>
<pin name="IO_L50N_3"/>
<pin name="IO_L50P_3"/>
<pin name="IO_L49N_3"/>
<pin name="IO_L49P_3"/>
<pin name="GND_B" direction="pwr"/>
<pin name="IO_L44N_GCLK20_3"/>
<pin name="IO_L44P_GCLK21_3"/>
<pin name="IO_L43N_GCLK22_IRDY2_3"/>
<pin name="IO_L43P_GCLK23_3"/>
<pin name="VCCO_BANK3_B" direction="pwr"/>
<pin name="VCCINT_A" direction="pwr"/>
<pin name="VCCAUX_A" direction="pwr"/>
<pin name="IO_L42N_GCLK24_3"/>
<pin name="IO_L42P_GCLK25_TRDY2_3"/>
<pin name="IO_L41N_GCLK26_3"/>
<pin name="IO_L41P_GCLK27_3"/>
<pin name="GND_C"/>
<pin name="IO_L37N_3"/>
<pin name="IO_L37P_3"/>
<pin name="VCCINT_B" direction="pwr"/>
<pin name="IO_L36N_3"/>
<pin name="IO_L36P_3"/>
<pin name="VCCO_BANK3_C" direction="pwr"/>
<pin name="IO_L2N_3"/>
<pin name="IO_L2P_3"/>
<pin name="IO_L1N_VREF_3"/>
<pin name="IO_L1P_3"/>
<pin name="VCCAUX_B" direction="pwr"/>
<pin name="PROGRAM_B_2"/>
<pin name="IO_L65N_CSO_B_2"/>
<pin name="IO_L65P_INIT_B_2"/>
<pin name="IO_L64N_D9_2"/>
<pin name="IO_L64P_D8_2"/>
<pin name="VCCO_BANK2_A" direction="pwr"/>
<pin name="IO_L62N_D6_2"/>
<pin name="IO_L62P_D5_2"/>
<pin name="IO_L49N_D4_2"/>
<pin name="IO_L49P_D3_2"/>
<pin name="IO_L48N_RDWR_B_VREF_2"/>
<pin name="IO_L48P_D7_2"/>
<pin name="GND_D" direction="pwr"/>
<pin name="IO_L31N_GCLK30_D15_2"/>
<pin name="IO_L31P_GCLK31_D14_2"/>
<pin name="VCCINT_C" direction="pwr"/>
<pin name="VCCAUX_C" direction="pwr"/>
<pin name="GND_E" direction="pwr"/>
<pin name="IO_L30N_GCLK0_USERCCLK_2"/>
<pin name="IO_L30P_GCLK1_D13_2"/>
<pin name="IO_L14N_D12_2"/>
<pin name="IO_L14P_D11_2"/>
<pin name="IO_L13N_D10_2"/>
<pin name="IO_L13P_M1_2"/>
<pin name="IO_L12N_D2_MISO3_2"/>
<pin name="IO_L12P_D1_MISO2_2"/>
<pin name="VCCO_BANK2_B" direction="pwr"/>
<pin name="IO_L3N_MOSI_CSI_B_MISO0_2"/>
<pin name="IO_L3P_D0_DIN_MISO_MISO1_2"/>
<pin name="IO_L2N_CMPMOSI_2"/>
<pin name="IO_L2P_CMPCLK_2"/>
<pin name="GND_F" direction="pwr"/>
<pin name="IO_L1N_M0_CMPMISO_2"/>
<pin name="IO_L1P_CCLK_2"/>
<pin name="DONE_2"/>
<pin name="CMPCS_B_2"/>
<pin name="SUSPEND"/>
<pin name="IO_L74N_DOUT_BUSY_1"/>
<pin name="IO_L74P_AWAKE_1"/>
<pin name="VCCO_BANK1_A" direction="pwr"/>
<pin name="GND_G" direction="pwr"/>
<pin name="IO_L47N_1"/>
<pin name="IO_L47P_1"/>
<pin name="IO_L46N_1"/>
<pin name="IO_L46P_1"/>
<pin name="IO_L45N_1"/>
<pin name="IO_L45P_1"/>
<pin name="IO_L43N_GCLK4_1"/>
<pin name="IO_L43P_GCLK5_1"/>
<pin name="VCCO_BANK1_B" direction="pwr"/>
<pin name="IO_L42N_GCLK6_TRDY1_1"/>
<pin name="IO_L42P_GCLK7_1"/>
<pin name="VCCINT_D" direction="pwr"/>
<pin name="VCCAUX_D" direction="pwr"/>
<pin name="GND_H" direction="pwr"/>
<pin name="IO_L41N_GCLK8_1"/>
<pin name="IO_L41P_GCLK9_IRDY1_1"/>
<pin name="IO_L40N_GCLK10_1"/>
<pin name="IO_L40P_GCLK11_1"/>
<pin name="GND_I" direction="pwr"/>
<pin name="IO_L34N_1"/>
<pin name="IO_L34P_1"/>
<pin name="IO_L33N_1"/>
<pin name="IO_L33P_1"/>
<pin name="IO_L32N_1"/>
<pin name="IO_L32P_1"/>
<pin name="VCCO_BANK1_C" direction="pwr"/>
<pin name="IO_L1N_VREF_1"/>
<pin name="IO_L1P_1"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="GND_J" direction="pwr"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="IO_L66N_SCP0_0"/>
<pin name="IO_L66P_SCP1_0"/>
<pin name="GND_K" direction="pwr"/>
<pin name="IO_L65N_SCP2_0"/>
<pin name="IO_L65P_SCP3_0"/>
<pin name="IO_L64N_SCP4_0"/>
<pin name="IO_L64P_SCP5_0"/>
<pin name="IO_L63N_SCP6_0"/>
<pin name="IO_L63P_SCP7_0"/>
<pin name="IO_L62N_VREF_0"/>
<pin name="IO_L62P_0"/>
<pin name="VCCO_BANK0_A" direction="pwr"/>
<pin name="IO_L37N_GCLK12_0"/>
<pin name="IO_L37P_GCLK13_0"/>
<pin name="VCCO_BANK0_B" direction="pwr"/>
<pin name="IO_L36N_GCLK14_0"/>
<pin name="IO_L36P_GCLK15_0"/>
<pin name="VCCINT_E" direction="pwr"/>
<pin name="VCCAUX_E" direction="pwr"/>
<pin name="GND_L" direction="pwr"/>
<pin name="IO_L35N_GCLK16_0"/>
<pin name="IO_L35P_GCLK17_0"/>
<pin name="IO_L34N_GCLK18_0"/>
<pin name="IO_L34P_GCLK19_0"/>
<pin name="VCCO_BANK0_C" direction="pwr"/>
<pin name="GND_M" direction="pwr"/>
<pin name="IO_L4N_0"/>
<pin name="IO_L4P_0"/>
<pin name="IO_L3N_0"/>
<pin name="IO_L3P_0"/>
<pin name="IO_L2N_0"/>
<pin name="IO_L2P_0"/>
<pin name="IO_L1N_VREF_0"/>
<pin name="IO_L1P_HSWAPEN_0"/>
</symbol>
<symbol name="XC9572XL">
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="IO1-2"/>
<pin name="IO1-5"/>
<pin name="IO1-6"/>
<pin name="IO1-8"/>
<pin name="IO1-9/GCK1"/>
<pin name="IO1-11/GCK2"/>
<pin name="IO1-14/GCK3"/>
<pin name="IO1-15"/>
<pin name="IO1-17"/>
<pin name="IO2-2"/>
<pin name="IO2-5"/>
<pin name="IO2-6"/>
<pin name="IO2-8"/>
<pin name="IO2-9/GSR"/>
<pin name="IO2-11/GTS2"/>
<pin name="IO2-14/GTS1"/>
<pin name="IO2-15"/>
<pin name="IO2-17"/>
<pin name="IO3-2"/>
<pin name="IO3-5"/>
<pin name="IO3-8"/>
<pin name="IO3-9"/>
<pin name="IO3-11"/>
<pin name="IO3-14"/>
<pin name="IO3-15"/>
<pin name="IO3-16"/>
<pin name="IO3-17"/>
<pin name="IO4-2"/>
<pin name="IO4-5"/>
<pin name="IO4-8"/>
<pin name="IO4-11"/>
<pin name="IO4-14"/>
<pin name="IO4-15"/>
<pin name="IO4-17"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="VCCINT1"/>
<pin name="VCCINT2"/>
<pin name="VCCIO"/>
</symbol>
<symbol name="XILINX_JTAG6">
<pin name="+V" direction="pas" function="dot"/>
<pin name="TCK" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
<pin name="TDI" direction="pas" function="dot"/>
<pin name="TDO" direction="pas" function="dot"/>
<pin name="TMS" direction="pas" function="dot"/>
</symbol>
<symbol name="ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DISP_LCD">
<pin name="GND" direction="sup"/>
<pin name="VCC" direction="sup"/>
<pin name="CONTR" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="R/W" direction="in"/>
<pin name="E" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="A" direction="sup"/>
<pin name="K" direction="sup"/>
</symbol>
<symbol name="DISP_VFD_IV-22">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="GRID" direction="in"/>
<pin name="FA" direction="pwr"/>
<pin name="FB" direction="pwr"/>
</symbol>
<symbol name="MAX6921">
<pin name="OUT0" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="OUT9" direction="out"/>
<pin name="OUT10" direction="out"/>
<pin name="OUT11" direction="out"/>
<pin name="OUT12" direction="out"/>
<pin name="OUT13" direction="out"/>
<pin name="OUT14" direction="out"/>
<pin name="OUT15" direction="out"/>
<pin name="OUT16" direction="out"/>
<pin name="OUT17" direction="out"/>
<pin name="OUT18" direction="out"/>
<pin name="OUT19" direction="out"/>
<pin name="VBB" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DIN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="LOAD" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="BLANK" direction="in"/>
</symbol>
<symbol name="ATMEGA32U4">
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PE2"/>
<pin name="PE6"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="!RESET" direction="in" function="dot"/>
<pin name="VBUS" direction="pwr"/>
<pin name="VCC@0" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="UVCC" direction="pwr"/>
<pin name="AVCC@0" direction="pwr"/>
<pin name="AVCC@1" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AREF" direction="pwr"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="UCAP" direction="pwr"/>
<pin name="UGND" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="COIL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="ENC28J60">
<pin name="VSSOSC" direction="sup"/>
<pin name="OSC2" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="VDDOSC" direction="sup"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="!CS" direction="in" function="dot"/>
<pin name="SO" direction="out"/>
<pin name="SI" direction="in"/>
<pin name="VCAP" direction="in"/>
<pin name="VDD" direction="sup"/>
<pin name="LEDA" direction="out"/>
<pin name="LEDB" direction="out"/>
<pin name="RBIAS" direction="in"/>
<pin name="VSS" direction="sup"/>
<pin name="!INT" direction="out" function="dot"/>
<pin name="CLKOUT" direction="out" function="clk"/>
<pin name="VSSTX" direction="sup"/>
<pin name="TPOUT-" direction="out"/>
<pin name="TPOUT+" direction="out"/>
<pin name="VDDTX" direction="sup"/>
<pin name="TPIN-" direction="in"/>
<pin name="TPIN+" direction="in"/>
<pin name="VDDRX" direction="sup"/>
<pin name="VSSRX" direction="sup"/>
<pin name="VSSPLL" direction="sup"/>
<pin name="VDDPLL" direction="sup"/>
<pin name="!RESET" direction="in" function="dot"/>
</symbol>
<symbol name="LTC4053">
<pin name="!CHRG" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="!FAULT" direction="pas"/>
<pin name="TIMER" direction="pas"/>
<pin name="GND@1" direction="pwr"/>
<pin name="NTC" direction="pas"/>
<pin name="PROG" direction="pas"/>
<pin name="!SHDN" direction="pas"/>
<pin name="BAT" direction="pas"/>
<pin name="!ACPR" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="ENCODER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="HEADER2X7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
</symbol>
<symbol name="FT230X">
<pin name="3V3OUT" direction="pwr"/>
<pin name="USB-" direction="in"/>
<pin name="USB+" direction="out"/>
<pin name="!RESET"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="CBUS3"/>
<pin name="CBUS2"/>
<pin name="CBUS1"/>
<pin name="CBUS0"/>
<pin name="!CTS"/>
<pin name="!RTS"/>
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="VCC" direction="sup"/>
<pin name="VCCIO" direction="pwr"/>
</symbol>
<symbol name="VREG-ADJ">
<pin name="ADJ" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VOUT" direction="pwr"/>
</symbol>
<symbol name="74595">
<pin name="SDA" direction="in"/>
<pin name="!OE" direction="in" function="dot"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q7S" direction="out"/>
<pin name="SCLK" direction="in"/>
<pin name="!RST" direction="in" function="dot"/>
<pin name="LATCH" direction="in"/>
</symbol>
<symbol name="ULN2003">
<pin name="1B"/>
<pin name="2B"/>
<pin name="3B"/>
<pin name="4B"/>
<pin name="5B"/>
<pin name="6B"/>
<pin name="7B"/>
<pin name="GND"/>
<pin name="COM"/>
<pin name="7C"/>
<pin name="6C"/>
<pin name="5C"/>
<pin name="4C"/>
<pin name="3C"/>
<pin name="2C"/>
<pin name="1C"/>
</symbol>
<symbol name="74HC4017">
<pin name="!CP1" direction="in" function="dotclk"/>
<pin name="CP0" direction="in" function="clk"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="!Q5-9" direction="out" function="dot"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="MR" direction="in"/>
</symbol>
<symbol name="555">
<pin name="VCC" direction="sup"/>
<pin name="DIS" direction="in"/>
<pin name="THR" direction="in"/>
<pin name="CTRL" direction="sup"/>
<pin name="GND" direction="sup"/>
<pin name="TRIG" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="RST" direction="in"/>
</symbol>
<symbol name="IC_KSZ8851SNL">
<pin name="LED0"/>
<pin name="PME"/>
<pin name="!INT"/>
<pin name="DGND@1" direction="sup"/>
<pin name="VDD_CO18"/>
<pin name="EDD_IO"/>
<pin name="EESK"/>
<pin name="AGND@1"/>
<pin name="VDD_A18"/>
<pin name="EECS"/>
<pin name="RXP"/>
<pin name="RXM"/>
<pin name="AGND@2"/>
<pin name="TXP"/>
<pin name="TXM"/>
<pin name="VDD_A33"/>
<pin name="ISET"/>
<pin name="AGND@3" direction="sup"/>
<pin name="!RST"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="DGND@2"/>
<pin name="VDD_D18" direction="sup"/>
<pin name="DGND@3"/>
<pin name="VDD_IO@1"/>
<pin name="!CS"/>
<pin name="SO"/>
<pin name="SCLK"/>
<pin name="DGND@4"/>
<pin name="VDD_IO@2"/>
<pin name="SI"/>
<pin name="LED1"/>
</symbol>
<symbol name="QFN25_GND">
<pin name="GND@0" direction="sup"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="GND@3" direction="sup"/>
<pin name="GND@4" direction="sup"/>
<pin name="GND@5" direction="sup"/>
<pin name="GND@6" direction="sup"/>
<pin name="GND@7" direction="sup"/>
<pin name="GND@8" direction="sup"/>
</symbol>
<symbol name="TPS6120X">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="PS" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="FB" direction="in"/>
<pin name="VAUX"/>
<pin name="VOUT" direction="out"/>
<pin name="L" direction="in"/>
<pin name="PGND" direction="sup"/>
</symbol>
<symbol name="QFN-10-GND">
<pin name="GND@0" direction="sup"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="GND@3" direction="sup"/>
<pin name="GND@4" direction="sup"/>
<pin name="GND@5" direction="sup"/>
<pin name="GND@6" direction="sup"/>
</symbol>
<symbol name="HEADER2X8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
<symbol name="SWITCH_1">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="LCD_SPI">
<pin name="CS"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="LEDA"/>
<pin name="LEDK"/>
<pin name="NC1"/>
<pin name="NC2"/>
<pin name="RS"/>
<pin name="RST"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
</symbol>
<symbol name="SUPPLY_+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="SUPPLY_+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="SUPPLY_GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="SUPPLY_VUSB">
<pin name="VUSB" direction="sup"/>
</symbol>
<symbol name="USB_BODY_PINS_2P">
<pin name="BODY@1" direction="hiz"/>
<pin name="BODY@2" direction="hiz"/>
</symbol>
<symbol name="74AC573">
<pin name="!OE" direction="in" function="dot"/>
<pin name="LE" direction="in"/>
<pin name="8Q"/>
<pin name="7Q"/>
<pin name="6Q"/>
<pin name="5Q"/>
<pin name="4Q"/>
<pin name="3Q"/>
<pin name="2Q"/>
<pin name="1Q"/>
<pin name="8D"/>
<pin name="7D"/>
<pin name="6D"/>
<pin name="5D"/>
<pin name="4D"/>
<pin name="3D"/>
<pin name="2D"/>
<pin name="1D"/>
</symbol>
<symbol name="FT311D">
<pin name="XTIN" direction="in"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@2" direction="sup"/>
<pin name="GND@1" direction="sup"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS1"/>
<pin name="IOBUS0"/>
<pin name="VCCIO@2" direction="sup"/>
<pin name="GND@3" direction="sup"/>
<pin name="USB-" direction="in"/>
<pin name="USB+" direction="out"/>
<pin name="VCC" direction="sup"/>
<pin name="VCCIO@1" direction="sup"/>
<pin name="XTOUT" direction="out"/>
<pin name="VREGOUT" direction="pwr"/>
<pin name="TEST1" direction="in"/>
<pin name="GND@4" direction="sup"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="!USB_ERROR" direction="out" function="dot"/>
<pin name="GND@5" direction="sup"/>
<pin name="CNFG1" direction="in"/>
<pin name="CNFG2" direction="in"/>
<pin name="CNFG0" direction="in"/>
<pin name="TEST0" direction="out"/>
<pin name="!RESET" direction="in" function="dot"/>
<pin name="TEST2" direction="in"/>
<pin name="VCCIO@3" direction="sup"/>
</symbol>
<symbol name="SRAM-23LCXXXX">
<pin name="SI/SIO0"/>
<pin name="SO/SIO1"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="!CS" direction="in" function="dot"/>
<pin name="!HOLD/SIO3" direction="in" function="dot"/>
<pin name="SIO2"/>
</symbol>
<symbol name="74141">
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="A" direction="in"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="SUPPLY_+12V">
<pin name="+12V" direction="sup"/>
</symbol>
<symbol name="SUPPLY_-12V">
<pin name="-12V" direction="sup"/>
</symbol>
<symbol name="SUPPLY_-5V">
<pin name="-5V" direction="sup"/>
</symbol>
<symbol name="DISP_IN-12">
<pin name="K0" direction="in"/>
<pin name="K1" direction="in"/>
<pin name="K2" direction="in"/>
<pin name="K3" direction="in"/>
<pin name="K4" direction="in"/>
<pin name="K5" direction="in"/>
<pin name="K6" direction="in"/>
<pin name="K7" direction="in"/>
<pin name="ANODE" direction="in"/>
<pin name="K8" direction="in"/>
<pin name="K9" direction="in"/>
</symbol>
<symbol name="IC_INA138">
<pin name="V+" direction="sup"/>
<pin name="OUT" direction="out"/>
<pin name="VIN-" direction="in"/>
<pin name="GND" direction="sup"/>
<pin name="VIN+" direction="in"/>
</symbol>
<symbol name="DISP_D8035E">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="-" direction="in"/>
<pin name="GRID" direction="in"/>
<pin name="F+" direction="pwr"/>
<pin name="F-" direction="pwr"/>
<pin name="DP" direction="in"/>
</symbol>
<symbol name="IC_MIC2027">
<pin name="OUT_A" direction="out"/>
<pin name="EN_A" direction="in"/>
<pin name="EN_C" direction="in"/>
<pin name="FLG_C" direction="out"/>
<pin name="IN_AB" direction="in"/>
<pin name="OUT_B" direction="out"/>
<pin name="OUT_C" direction="out"/>
<pin name="OUT_D" direction="out"/>
<pin name="IN_CD" direction="in"/>
<pin name="FLG_A" direction="out"/>
<pin name="EN_B" direction="in"/>
<pin name="FLG_B" direction="out"/>
<pin name="EN_D" direction="in"/>
<pin name="FLG_D" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="IC_TD62783">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="IN8" direction="in"/>
<pin name="OUT8" direction="out"/>
</symbol>
<symbol name="JOYSTICK_SF303GJ26-3">
<pin name="CENTER"/>
<pin name="B"/>
<pin name="COMMON"/>
<pin name="A"/>
<pin name="C"/>
<pin name="D"/>
</symbol>
<symbol name="PIC24F16KA102">
<pin name="RA5/!MCLR!/VPP" direction="in"/>
<pin name="RA0/AN0/CN2/VREF+"/>
<pin name="RA1/AN1/CN3/VREF-"/>
<pin name="RB0/AN2/CN4/C2INB/C1IND/PGD1/U2TX"/>
<pin name="RB1/AN3/CN5/C2INA/C1INC/PGC1/U2RX"/>
<pin name="RB2/AN4/CN6/C2IND/C1INB/U1RX"/>
<pin name="RB3/AN5/CN7/C2INC/C1INA"/>
<pin name="VSS@1" direction="sup"/>
<pin name="RA2/CN30/OSCI/CLKI"/>
<pin name="RA3/CN29/OSCO/CLKO"/>
<pin name="RB4/CN1/SOSCI/!U2RTS!/U2BCLK"/>
<pin name="RA4/CN0/SOSCO/T1CK/!U2CTS!"/>
<pin name="VDD@1" direction="sup"/>
<pin name="RB5/CN27/PGD3/SDA1"/>
<pin name="SCL1/PGC3/CN24/RB6"/>
<pin name="U1TX/INT0/CN23/RB7"/>
<pin name="!U1CTS!/SCL1/CN22/RB8"/>
<pin name="!U1RTS!/U1BCLK/SDA1/CN21/RB9"/>
<pin name="IC1/CN9/RA7" direction="pwr"/>
<pin name="OC1/C2OUT/INT2/CTED1/CN8/RA6" direction="pwr"/>
<pin name="SDI1/PMD2/PGD2/CN16/RB10"/>
<pin name="SCK1/PGC2/CN15/RB11"/>
<pin name="HLVDIN/CTED2/CN14/AN12/RB12"/>
<pin name="SDO1/CTPLS/CN13/AN11/RB13"/>
<pin name="OCFA/C1OUT/RTCC/CVREF/CN12/AN10/RB14"/>
<pin name="REFO/!SS1!/T2CK/T3CK/CN11/RB15"/>
<pin name="VSS@2" direction="sup"/>
<pin name="VDD@2" direction="sup"/>
</symbol>
<symbol name="CON_MICROSD">
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="VSS"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
</symbol>
<symbol name="JUMP_SOLDER_1X2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DIL-28">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
</symbol>
<symbol name="SWITCH_3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="BB_XQFP_050">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="63"/>
<pin name="64"/>
<pin name="65"/>
<pin name="66"/>
<pin name="67"/>
<pin name="68"/>
<pin name="69"/>
<pin name="70"/>
<pin name="71"/>
<pin name="72"/>
<pin name="73"/>
<pin name="74"/>
<pin name="75"/>
<pin name="76"/>
<pin name="77"/>
<pin name="78"/>
<pin name="79"/>
<pin name="80"/>
</symbol>
<symbol name="BB_XQFP_065">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="63"/>
<pin name="64"/>
<pin name="65"/>
<pin name="66"/>
<pin name="67"/>
<pin name="68"/>
<pin name="69"/>
<pin name="70"/>
<pin name="71"/>
<pin name="72"/>
<pin name="73"/>
<pin name="74"/>
<pin name="75"/>
<pin name="76"/>
<pin name="77"/>
<pin name="78"/>
<pin name="79"/>
<pin name="80"/>
</symbol>
<symbol name="BB_XQFP_080">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="63"/>
<pin name="64"/>
<pin name="65"/>
<pin name="66"/>
<pin name="67"/>
<pin name="68"/>
<pin name="69"/>
<pin name="70"/>
<pin name="71"/>
<pin name="72"/>
<pin name="73"/>
<pin name="74"/>
<pin name="75"/>
<pin name="76"/>
<pin name="77"/>
<pin name="78"/>
<pin name="79"/>
<pin name="80"/>
</symbol>
<symbol name="BB_XQFP_050_065">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="63"/>
<pin name="64"/>
<pin name="65"/>
<pin name="66"/>
<pin name="67"/>
<pin name="68"/>
<pin name="69"/>
<pin name="70"/>
<pin name="71"/>
<pin name="72"/>
<pin name="73"/>
<pin name="74"/>
<pin name="75"/>
<pin name="76"/>
<pin name="77"/>
<pin name="78"/>
<pin name="79"/>
<pin name="80"/>
</symbol>
<symbol name="BB_XQFP_050_080">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="63"/>
<pin name="64"/>
<pin name="65"/>
<pin name="66"/>
<pin name="67"/>
<pin name="68"/>
<pin name="69"/>
<pin name="70"/>
<pin name="71"/>
<pin name="72"/>
<pin name="73"/>
<pin name="74"/>
<pin name="75"/>
<pin name="76"/>
<pin name="77"/>
<pin name="78"/>
<pin name="79"/>
<pin name="80"/>
</symbol>
<symbol name="BB_XQFP_080_065">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="39"/>
<pin name="40"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="49"/>
<pin name="50"/>
<pin name="51"/>
<pin name="52"/>
<pin name="53"/>
<pin name="54"/>
<pin name="55"/>
<pin name="56"/>
<pin name="57"/>
<pin name="58"/>
<pin name="59"/>
<pin name="60"/>
<pin name="61"/>
<pin name="62"/>
<pin name="63"/>
<pin name="64"/>
<pin name="65"/>
<pin name="66"/>
<pin name="67"/>
<pin name="68"/>
<pin name="69"/>
<pin name="70"/>
<pin name="71"/>
<pin name="72"/>
<pin name="73"/>
<pin name="74"/>
<pin name="75"/>
<pin name="76"/>
<pin name="77"/>
<pin name="78"/>
<pin name="79"/>
<pin name="80"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BATTERY_2032" prefix="BATT">
<description>BATTERY</description>
<gates>
<gate name="BATT" symbol="2032"/>
</gates>
<devices>
<device name="" package="BATT2032">
<connects>
<connect gate="BATT" pin="V-" pad="V-"/>
<connect gate="BATT" pin="V1" pad="V1"/>
<connect gate="BATT" pin="V2" pad="V2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR_NPOL" prefix="C" uservalue="yes">
<description>Non-Polarized capacitor in various packages</description>
<gates>
<gate name="C" symbol="CAP"/>
</gates>
<devices>
<device name="-0805" package="C805">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="C402">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="C603">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="C1206">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH_0.1&quot;" package="C0.1PTH">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR_POL" prefix="C" uservalue="yes">
<description>Polarized capacitor in various packages</description>
<gates>
<gate name="C" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-SMC_A" package="SMC_A">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMC_B" package="SMC_B">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CASE_A" package="CASE_A">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CASE_B" package="CASE_B">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-EDGE-F-06X2" prefix="CON">
<description>Female 6x2 Edge connector</description>
<gates>
<gate name="CON" symbol="EDGE_CONNECTOR_6X2"/>
</gates>
<devices>
<device name="" package="EDGE_CONNECTOR_6X2">
<connects>
<connect gate="CON" pin="A1" pad="1"/>
<connect gate="CON" pin="A2" pad="2"/>
<connect gate="CON" pin="A3" pad="3"/>
<connect gate="CON" pin="A4" pad="4"/>
<connect gate="CON" pin="A5" pad="5"/>
<connect gate="CON" pin="A6" pad="6"/>
<connect gate="CON" pin="B1" pad="7"/>
<connect gate="CON" pin="B2" pad="8"/>
<connect gate="CON" pin="B3" pad="9"/>
<connect gate="CON" pin="B4" pad="10"/>
<connect gate="CON" pin="B5" pad="11"/>
<connect gate="CON" pin="B6" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-EDGE-M-06X2" prefix="CON" uservalue="yes">
<description>Male 6x2 PCB Edge connector</description>
<gates>
<gate name="G$1" symbol="EDGE_CONNECTOR_6X2"/>
</gates>
<devices>
<device name="" package="PCB_EDGE_CONNECTOR_6X2">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-RJ45-F" prefix="ETH">
<description>HR911105A Female Ethernet RJ-45 with internal transformer and 2 LEDs</description>
<gates>
<gate name="ETH" symbol="HR911105A"/>
</gates>
<devices>
<device name="" package="HR911105A">
<connects>
<connect gate="ETH" pin="1" pad="1"/>
<connect gate="ETH" pin="10" pad="10"/>
<connect gate="ETH" pin="11" pad="11"/>
<connect gate="ETH" pin="12" pad="12"/>
<connect gate="ETH" pin="13" pad="13"/>
<connect gate="ETH" pin="14" pad="14"/>
<connect gate="ETH" pin="2" pad="2"/>
<connect gate="ETH" pin="3" pad="3"/>
<connect gate="ETH" pin="4" pad="4"/>
<connect gate="ETH" pin="5" pad="5"/>
<connect gate="ETH" pin="6" pad="6"/>
<connect gate="ETH" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-USB-F" prefix="USB">
<description>USB Female connector</description>
<gates>
<gate name="USB" symbol="CONN_USB"/>
<gate name="BODY" symbol="USB_BODY_PINS"/>
</gates>
<devices>
<device name="-MINI-B" package="CONN_USB_MINI-B">
<connects>
<connect gate="BODY" pin="BODY@1" pad="BODY@1"/>
<connect gate="BODY" pin="BODY@2" pad="BODY@2"/>
<connect gate="BODY" pin="BODY@3" pad="BODY@3"/>
<connect gate="BODY" pin="BODY@4" pad="BODY@4"/>
<connect gate="USB" pin="D+" pad="D+"/>
<connect gate="USB" pin="D-" pad="D-"/>
<connect gate="USB" pin="GND" pad="GND"/>
<connect gate="USB" pin="USBID" pad="ID"/>
<connect gate="USB" pin="VUSB" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICRO-B" package="CONN_USB_MICRO-B">
<connects>
<connect gate="BODY" pin="BODY@1" pad="BODY@1"/>
<connect gate="BODY" pin="BODY@2" pad="BODY@2"/>
<connect gate="BODY" pin="BODY@3" pad="BODY@3"/>
<connect gate="BODY" pin="BODY@4" pad="BODY@4"/>
<connect gate="USB" pin="D+" pad="P3"/>
<connect gate="USB" pin="D-" pad="P2"/>
<connect gate="USB" pin="GND" pad="P5"/>
<connect gate="USB" pin="USBID" pad="P4"/>
<connect gate="USB" pin="VUSB" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-USB-M" prefix="USB" uservalue="yes">
<description>USB Male connector</description>
<gates>
<gate name="USB" symbol="CONN_USB_4P"/>
<gate name="BODY" symbol="USB_BODY_PINS2"/>
</gates>
<devices>
<device name="-A" package="CONN_USB_A_MALE">
<connects>
<connect gate="BODY" pin="BODY@1" pad="BODY@1"/>
<connect gate="BODY" pin="BODY@2" pad="BODY@2"/>
<connect gate="BODY" pin="BODY@3" pad="BODY@3"/>
<connect gate="BODY" pin="BODY@4" pad="BODY@4"/>
<connect gate="USB" pin="D+" pad="D+"/>
<connect gate="USB" pin="D-" pad="D-"/>
<connect gate="USB" pin="GND" pad="GND"/>
<connect gate="USB" pin="VUSB" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_ARDUINO" prefix="ARDUINO">
<description>Arduino board connector layout</description>
<gates>
<gate name="G$1" symbol="ARDUINO"/>
</gates>
<devices>
<device name="" package="CON_ARDUINO">
<connects>
<connect gate="G$1" pin="3V3" pad="3V3"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="AN0" pad="A_0"/>
<connect gate="G$1" pin="AN1" pad="A_1"/>
<connect gate="G$1" pin="AN2" pad="A_2"/>
<connect gate="G$1" pin="AN3" pad="A_3"/>
<connect gate="G$1" pin="AN4" pad="A_4"/>
<connect gate="G$1" pin="AN5" pad="A_5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="DIG0_RX" pad="D_0"/>
<connect gate="G$1" pin="DIG10_PWM" pad="D_10"/>
<connect gate="G$1" pin="DIG11_PWM" pad="D_11"/>
<connect gate="G$1" pin="DIG12" pad="D_12"/>
<connect gate="G$1" pin="DIG13" pad="D_13"/>
<connect gate="G$1" pin="DIG1_TX" pad="D_1"/>
<connect gate="G$1" pin="DIG2" pad="D_2"/>
<connect gate="G$1" pin="DIG3_PWM" pad="D_3"/>
<connect gate="G$1" pin="DIG4" pad="D_4"/>
<connect gate="G$1" pin="DIG5_PWM" pad="D_5"/>
<connect gate="G$1" pin="DIG6_PWM" pad="D_6"/>
<connect gate="G$1" pin="DIG7" pad="D_7"/>
<connect gate="G$1" pin="DIG8" pad="D_8"/>
<connect gate="G$1" pin="DIG9_PWM" pad="D_9"/>
<connect gate="G$1" pin="GND0" pad="GND0"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="RESET" pad="RESET"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_ATX_PWR" prefix="J">
<gates>
<gate name="J" symbol="HEADER2X10"/>
</gates>
<devices>
<device name="-90DEG" package="CON_ATX_PWR_90DEG">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="15"/>
<connect gate="J" pin="11" pad="6"/>
<connect gate="J" pin="12" pad="16"/>
<connect gate="J" pin="13" pad="7"/>
<connect gate="J" pin="14" pad="17"/>
<connect gate="J" pin="15" pad="8"/>
<connect gate="J" pin="16" pad="18"/>
<connect gate="J" pin="17" pad="9"/>
<connect gate="J" pin="18" pad="19"/>
<connect gate="J" pin="19" pad="10"/>
<connect gate="J" pin="2" pad="11"/>
<connect gate="J" pin="20" pad="20"/>
<connect gate="J" pin="3" pad="2"/>
<connect gate="J" pin="4" pad="12"/>
<connect gate="J" pin="5" pad="3"/>
<connect gate="J" pin="6" pad="13"/>
<connect gate="J" pin="7" pad="4"/>
<connect gate="J" pin="8" pad="14"/>
<connect gate="J" pin="9" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_BUSPIRATE" prefix="J" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="HDR-BUSPIRATE"/>
</gates>
<devices>
<device name="" package="HDR-BUSPIRATE">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_DC_M" prefix="J" uservalue="yes">
<description>DC power connector</description>
<gates>
<gate name="J" symbol="DC_JACK"/>
</gates>
<devices>
<device name="-DC_SMD" package="DC_BARREL_JACK_SMD_2MM">
<connects>
<connect gate="J" pin="P1" pad="P1@2"/>
<connect gate="J" pin="P2" pad="P2"/>
<connect gate="J" pin="P3" pad="P3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DC_PTH" package="DC_BARREL_JACK_PTH_2MM">
<connects>
<connect gate="J" pin="P1" pad="P1"/>
<connect gate="J" pin="P2" pad="P3"/>
<connect gate="J" pin="P3" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DC_PTH2" package="DC_BARREL_JACK_PTH_2MM_2">
<connects>
<connect gate="J" pin="P1" pad="P1"/>
<connect gate="J" pin="P2" pad="P3"/>
<connect gate="J" pin="P3" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_1X01" prefix="J">
<gates>
<gate name="J" symbol="HEADER1X1"/>
</gates>
<devices>
<device name="-PTH" package="M1X1">
<connects>
<connect gate="J" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="SMDPAD05X05">
<connects>
<connect gate="J" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH_08_17" package="M1X2_08_17">
<connects>
<connect gate="J" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH_10_17" package="M1X2_10_17">
<connects>
<connect gate="J" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_1X02" prefix="J">
<gates>
<gate name="G$1" symbol="HEADER1X2"/>
</gates>
<devices>
<device name="-PTH" package="M1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_1X03" prefix="J">
<gates>
<gate name="G$1" symbol="HEADER1X3"/>
</gates>
<devices>
<device name="-PTH" package="M1X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_1X04" prefix="J">
<gates>
<gate name="J" symbol="HEADER1X4"/>
</gates>
<devices>
<device name="" package="M1X4">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_1X05" prefix="J">
<gates>
<gate name="G$1" symbol="HEADER1X5"/>
</gates>
<devices>
<device name="-PTH" package="M1X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_1X06" prefix="J">
<gates>
<gate name="J" symbol="HEADER1X6"/>
</gates>
<devices>
<device name="-PTH" package="M1X6">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="M1X6_SMD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH-RIGHT-ANGLED" package="M1X6_MALE_RIGHT_ANGLED">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-RIGHT-ANGLED" package="M1X6_MALE_RIGHT_ANGLED_SMD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_1X08" prefix="J">
<gates>
<gate name="J" symbol="HEADER1X8"/>
</gates>
<devices>
<device name="-PTH" package="M1X8">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="M1X8_SMD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X02" prefix="J">
<gates>
<gate name="J" symbol="HEADER2X2"/>
</gates>
<devices>
<device name="-PTH" package="M2X2">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X03" prefix="J">
<gates>
<gate name="J" symbol="HEADER2X3"/>
</gates>
<devices>
<device name="-PTH" package="M2X3">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="M2X3_SMD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X04" prefix="J">
<gates>
<gate name="G$1" symbol="HEADER2X4"/>
</gates>
<devices>
<device name="-PTH" package="M2X4">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X05" prefix="J">
<description>2x05 pin header</description>
<gates>
<gate name="J" symbol="HEADER2X5"/>
</gates>
<devices>
<device name="-PTH+SHROUDED_A" package="PINSHRD_PTH_2X05">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH+SHROUDED_B" package="PINSHRD_PTH_2X05B">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD+SHROUDED" package="PINSHRD_SMT_2X05">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH" package="M2X5">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X06" prefix="J">
<description>2x5 Pin header</description>
<gates>
<gate name="J" symbol="HEADER2X6"/>
</gates>
<devices>
<device name="-PTH+SHROUDED" package="PINSHRD_PTH_2X06">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD+SHROUDED" package="PINSHRD_SMT_2X06">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X10" prefix="J">
<gates>
<gate name="J" symbol="HEADER2X10"/>
</gates>
<devices>
<device name="-PTH" package="M2X10">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="13" pad="13"/>
<connect gate="J" pin="14" pad="14"/>
<connect gate="J" pin="15" pad="15"/>
<connect gate="J" pin="16" pad="16"/>
<connect gate="J" pin="17" pad="17"/>
<connect gate="J" pin="18" pad="18"/>
<connect gate="J" pin="19" pad="19"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="20" pad="20"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SHROUDED" package="PINSHRD_PTH_2X10">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="13" pad="13"/>
<connect gate="J" pin="14" pad="14"/>
<connect gate="J" pin="15" pad="15"/>
<connect gate="J" pin="16" pad="16"/>
<connect gate="J" pin="17" pad="17"/>
<connect gate="J" pin="18" pad="18"/>
<connect gate="J" pin="19" pad="19"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="20" pad="20"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_PRG_AVR_ICSP" prefix="J">
<description>2x3 AVR ICSP programming header</description>
<gates>
<gate name="J" symbol="PRG_ICSP_AVR"/>
</gates>
<devices>
<device name="-PTH" package="HEADER_PRG_2X03">
<connects>
<connect gate="J" pin="+V" pad="2"/>
<connect gate="J" pin="GND" pad="6"/>
<connect gate="J" pin="MISO" pad="1"/>
<connect gate="J" pin="MOSI" pad="4"/>
<connect gate="J" pin="RST" pad="5"/>
<connect gate="J" pin="SCK" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="M2X3_SMD">
<connects>
<connect gate="J" pin="+V" pad="2"/>
<connect gate="J" pin="GND" pad="6"/>
<connect gate="J" pin="MISO" pad="1"/>
<connect gate="J" pin="MOSI" pad="4"/>
<connect gate="J" pin="RST" pad="5"/>
<connect gate="J" pin="SCK" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_PRG_MSP_SBW" prefix="J">
<description>4-pin MSP Spy-Bi-Wire programming header</description>
<gates>
<gate name="J" symbol="PRG_SBW_MSP"/>
</gates>
<devices>
<device name="" package="HEADER_PRG_1X04">
<connects>
<connect gate="J" pin="+V" pad="3"/>
<connect gate="J" pin="GND" pad="4"/>
<connect gate="J" pin="SBWTCK" pad="1"/>
<connect gate="J" pin="SBWTDIO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_PRG_PIC_ICSP" prefix="J">
<description>5-pin PIC In Circuit Serial Programming header</description>
<gates>
<gate name="J" symbol="PRG_ICSP_PIC"/>
</gates>
<devices>
<device name="0.1INCH_A" package="HEADER_PRG_1X05">
<connects>
<connect gate="J" pin="+V" pad="2"/>
<connect gate="J" pin="/MCLR" pad="1"/>
<connect gate="J" pin="GND" pad="3"/>
<connect gate="J" pin="PGC" pad="5"/>
<connect gate="J" pin="PGD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.1INCH_B" package="HEADER_PRG_1X05_ICSP_B">
<connects>
<connect gate="J" pin="+V" pad="2"/>
<connect gate="J" pin="/MCLR" pad="1"/>
<connect gate="J" pin="GND" pad="3"/>
<connect gate="J" pin="PGC" pad="5"/>
<connect gate="J" pin="PGD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO-PROG" package="CON_POGO_ICSP_PROG">
<connects>
<connect gate="J" pin="+V" pad="VCC"/>
<connect gate="J" pin="/MCLR" pad="MCLR"/>
<connect gate="J" pin="GND" pad="GND"/>
<connect gate="J" pin="PGC" pad="PGC"/>
<connect gate="J" pin="PGD" pad="PGD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-POGO-FOOTPRINT" package="CON_POGO_ICSP_TARGET">
<connects>
<connect gate="J" pin="+V" pad="VCC"/>
<connect gate="J" pin="/MCLR" pad="MCLR"/>
<connect gate="J" pin="GND" pad="GND"/>
<connect gate="J" pin="PGC" pad="PGC"/>
<connect gate="J" pin="PGD" pad="PGD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_PRG_XILINX_JTAG6" prefix="J">
<description>6-pin Xilinx JTAG programming header</description>
<gates>
<gate name="J" symbol="XILINX_JTAG6"/>
</gates>
<devices>
<device name="" package="HEADER_PRG_1X06">
<connects>
<connect gate="J" pin="+V" pad="1"/>
<connect gate="J" pin="GND" pad="2"/>
<connect gate="J" pin="TCK" pad="3"/>
<connect gate="J" pin="TDI" pad="6"/>
<connect gate="J" pin="TDO" pad="4"/>
<connect gate="J" pin="TMS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>Various Diode Packages</description>
<gates>
<gate name="D" symbol="DIODE"/>
</gates>
<devices>
<device name="-DO323" package="DO323">
<connects>
<connect gate="D" pin="A" pad="A"/>
<connect gate="D" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT23" package="SOT-23">
<connects>
<connect gate="D" pin="A" pad="1"/>
<connect gate="D" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOD-123" package="SOD-123">
<connects>
<connect gate="D" pin="A" pad="A"/>
<connect gate="D" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DO-214AC" package="DO-214AC">
<connects>
<connect gate="D" pin="A" pad="2"/>
<connect gate="D" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_PHOTO_QSE15X" prefix="D">
<gates>
<gate name="G$1" symbol="QSE15X"/>
</gates>
<devices>
<device name="" package="QSE15X">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_7SEG" prefix="7SEG">
<gates>
<gate name="G$1" symbol="7SEGCC"/>
</gates>
<devices>
<device name="" package="DISP_7SEG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="DP" pad="DP"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="F" pad="F"/>
<connect gate="G$1" pin="G" pad="G"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_OLED_96X16" prefix="DISP">
<gates>
<gate name="G$1" symbol="OLED96X16"/>
</gates>
<devices>
<device name="" package="OLED96X16">
<connects>
<connect gate="G$1" pin="IREF" pad="5"/>
<connect gate="G$1" pin="RES#" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VCOMH" pad="6"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITE" prefix="L" uservalue="yes">
<description>Ferrite bead in various packages</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-1206" package="FB1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="FB402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="FB805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="FB603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME_DINA4_L">
<description>&lt;h4&gt;A4 DP frame&lt;/h4&gt;

Standard Dangerous Prototypes schematic frame. Automagically adds the DP logo and standard texts to the PCB&lt;BR&gt;
&lt;BR&gt;
Use the atrribute in the schematic editor to change the fields.</description>
<gates>
<gate name="G$1" symbol="DINA4_L"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="" package="DP_LOGO">
<technologies>
<technology name="">
<attribute name="FF1" value="fulfillment by"/>
<attribute name="FF2" value="Seeed Studio"/>
<attribute name="FF3" value="www.seeedstudio.com"/>
<attribute name="LICENSE" value="CC-BY-SA"/>
<attribute name="PROJECT" value="Projectname"/>
<attribute name="URL1" value="http://"/>
<attribute name="URL2" value="DangerousPrototypes.com"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FUSE_PTC" prefix="F" uservalue="yes">
<description>Resettable PTC</description>
<gates>
<gate name="G$1" symbol="FUSE_PTC"/>
</gates>
<devices>
<device name="-0805" package="PTC0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1812" package="PTC1812L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_ADC_ADS831" prefix="IC">
<description>8-bit 80MHz ADC</description>
<gates>
<gate name="G$1" symbol="ADS831"/>
</gates>
<devices>
<device name="" package="SSOP-20-DBQ">
<connects>
<connect gate="G$1" pin="!IN" pad="P16"/>
<connect gate="G$1" pin="!INT!/EXT" pad="P12"/>
<connect gate="G$1" pin="+VS" pad="P19"/>
<connect gate="G$1" pin="BIT1" pad="P2"/>
<connect gate="G$1" pin="BIT2" pad="P3"/>
<connect gate="G$1" pin="BIT3" pad="P4"/>
<connect gate="G$1" pin="BIT4" pad="P5"/>
<connect gate="G$1" pin="BIT5" pad="P6"/>
<connect gate="G$1" pin="BIT6" pad="P7"/>
<connect gate="G$1" pin="BIT7" pad="P8"/>
<connect gate="G$1" pin="BIT8" pad="P9"/>
<connect gate="G$1" pin="CLK" pad="P10"/>
<connect gate="G$1" pin="CM" pad="P15"/>
<connect gate="G$1" pin="GND@1" pad="P1"/>
<connect gate="G$1" pin="GND@2" pad="P18"/>
<connect gate="G$1" pin="IN" pad="P17"/>
<connect gate="G$1" pin="REFB" pad="P13"/>
<connect gate="G$1" pin="REFT" pad="P14"/>
<connect gate="G$1" pin="RSEL" pad="P11"/>
<connect gate="G$1" pin="VDRV" pad="P20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_ADC_MAX111**" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX111**"/>
</gates>
<devices>
<device name="-SOT-23-6" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="AIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCLK" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_74*16245" prefix="IC">
<description>16-bit &lt;B&gt;BUS TRANSCEIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416245"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP-48DL">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1A5" pad="41"/>
<connect gate="G$1" pin="1A6" pad="40"/>
<connect gate="G$1" pin="1A7" pad="38"/>
<connect gate="G$1" pin="1A8" pad="37"/>
<connect gate="G$1" pin="1B1" pad="2"/>
<connect gate="G$1" pin="1B2" pad="3"/>
<connect gate="G$1" pin="1B3" pad="5"/>
<connect gate="G$1" pin="1B4" pad="6"/>
<connect gate="G$1" pin="1B5" pad="8"/>
<connect gate="G$1" pin="1B6" pad="9"/>
<connect gate="G$1" pin="1B7" pad="11"/>
<connect gate="G$1" pin="1B8" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="1"/>
<connect gate="G$1" pin="1G" pad="48"/>
<connect gate="G$1" pin="2A1" pad="36"/>
<connect gate="G$1" pin="2A2" pad="35"/>
<connect gate="G$1" pin="2A3" pad="33"/>
<connect gate="G$1" pin="2A4" pad="32"/>
<connect gate="G$1" pin="2A5" pad="30"/>
<connect gate="G$1" pin="2A6" pad="29"/>
<connect gate="G$1" pin="2A7" pad="27"/>
<connect gate="G$1" pin="2A8" pad="26"/>
<connect gate="G$1" pin="2B1" pad="13"/>
<connect gate="G$1" pin="2B2" pad="14"/>
<connect gate="G$1" pin="2B3" pad="16"/>
<connect gate="G$1" pin="2B4" pad="17"/>
<connect gate="G$1" pin="2B5" pad="19"/>
<connect gate="G$1" pin="2B6" pad="20"/>
<connect gate="G$1" pin="2B7" pad="22"/>
<connect gate="G$1" pin="2B8" pad="23"/>
<connect gate="G$1" pin="2DIR" pad="24"/>
<connect gate="G$1" pin="2G" pad="25"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TSSOP48" package="TSSOP-48">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1A5" pad="41"/>
<connect gate="G$1" pin="1A6" pad="40"/>
<connect gate="G$1" pin="1A7" pad="38"/>
<connect gate="G$1" pin="1A8" pad="37"/>
<connect gate="G$1" pin="1B1" pad="2"/>
<connect gate="G$1" pin="1B2" pad="3"/>
<connect gate="G$1" pin="1B3" pad="5"/>
<connect gate="G$1" pin="1B4" pad="6"/>
<connect gate="G$1" pin="1B5" pad="8"/>
<connect gate="G$1" pin="1B6" pad="9"/>
<connect gate="G$1" pin="1B7" pad="11"/>
<connect gate="G$1" pin="1B8" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="1"/>
<connect gate="G$1" pin="1G" pad="48"/>
<connect gate="G$1" pin="2A1" pad="36"/>
<connect gate="G$1" pin="2A2" pad="35"/>
<connect gate="G$1" pin="2A3" pad="33"/>
<connect gate="G$1" pin="2A4" pad="32"/>
<connect gate="G$1" pin="2A5" pad="30"/>
<connect gate="G$1" pin="2A6" pad="29"/>
<connect gate="G$1" pin="2A7" pad="27"/>
<connect gate="G$1" pin="2A8" pad="26"/>
<connect gate="G$1" pin="2B1" pad="13"/>
<connect gate="G$1" pin="2B2" pad="14"/>
<connect gate="G$1" pin="2B3" pad="16"/>
<connect gate="G$1" pin="2B4" pad="17"/>
<connect gate="G$1" pin="2B5" pad="19"/>
<connect gate="G$1" pin="2B6" pad="20"/>
<connect gate="G$1" pin="2B7" pad="22"/>
<connect gate="G$1" pin="2B8" pad="23"/>
<connect gate="G$1" pin="2DIR" pad="24"/>
<connect gate="G$1" pin="2G" pad="25"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_74LVC1G125" prefix="IC">
<gates>
<gate name="G$1" symbol="74LVC1G125"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OE" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_74LVC245A" prefix="IC">
<description>Octal Bus transceiver with 3-state, 3.3V supply</description>
<gates>
<gate name="G$1" symbol="74LVC245A"/>
<gate name="SUPPLY" symbol="SUPPLY"/>
</gates>
<devices>
<device name="-SOIC20" package="SOIC-20">
<connects>
<connect gate="G$1" pin="!OE" pad="19"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="B0" pad="18"/>
<connect gate="G$1" pin="B1" pad="17"/>
<connect gate="G$1" pin="B2" pad="16"/>
<connect gate="G$1" pin="B3" pad="15"/>
<connect gate="G$1" pin="B4" pad="14"/>
<connect gate="G$1" pin="B5" pad="13"/>
<connect gate="G$1" pin="B6" pad="12"/>
<connect gate="G$1" pin="B7" pad="11"/>
<connect gate="G$1" pin="DIR" pad="1"/>
<connect gate="SUPPLY" pin="GND" pad="10"/>
<connect gate="SUPPLY" pin="V+" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SSOP20" package="SSOP-20">
<connects>
<connect gate="G$1" pin="!OE" pad="19"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="B0" pad="18"/>
<connect gate="G$1" pin="B1" pad="17"/>
<connect gate="G$1" pin="B2" pad="16"/>
<connect gate="G$1" pin="B3" pad="15"/>
<connect gate="G$1" pin="B4" pad="14"/>
<connect gate="G$1" pin="B5" pad="13"/>
<connect gate="G$1" pin="B6" pad="12"/>
<connect gate="G$1" pin="B7" pad="11"/>
<connect gate="G$1" pin="DIR" pad="1"/>
<connect gate="SUPPLY" pin="GND" pad="10"/>
<connect gate="SUPPLY" pin="V+" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_SN74AVC2T45" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="2T45"/>
</gates>
<devices>
<device name="DCT" package="DCT_R_PDSO_G8">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCU" package="DCU_R_PDSO_G8">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_SN74AVC4T245" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="SN74AVC4T245"/>
</gates>
<devices>
<device name="" package="SOIC-16W">
<connects>
<connect gate="G$1" pin="1A1" pad="4"/>
<connect gate="G$1" pin="1A2" pad="5"/>
<connect gate="G$1" pin="1B1" pad="13"/>
<connect gate="G$1" pin="1B2" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="2"/>
<connect gate="G$1" pin="1OE" pad="15"/>
<connect gate="G$1" pin="2A1" pad="6"/>
<connect gate="G$1" pin="2A2" pad="7"/>
<connect gate="G$1" pin="2B1" pad="11"/>
<connect gate="G$1" pin="2B2" pad="10"/>
<connect gate="G$1" pin="2DIR" pad="3"/>
<connect gate="G$1" pin="2OE" pad="14"/>
<connect gate="G$1" pin="GNDA" pad="8"/>
<connect gate="G$1" pin="GNDB" pad="9"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="SN74AVC4T245" value=""/>
</technology>
</technologies>
</device>
<device name="PW" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="1A1" pad="4"/>
<connect gate="G$1" pin="1A2" pad="5"/>
<connect gate="G$1" pin="1B1" pad="13"/>
<connect gate="G$1" pin="1B2" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="2"/>
<connect gate="G$1" pin="1OE" pad="15"/>
<connect gate="G$1" pin="2A1" pad="6"/>
<connect gate="G$1" pin="2A2" pad="7"/>
<connect gate="G$1" pin="2B1" pad="11"/>
<connect gate="G$1" pin="2B2" pad="10"/>
<connect gate="G$1" pin="2DIR" pad="3"/>
<connect gate="G$1" pin="2OE" pad="14"/>
<connect gate="G$1" pin="GNDA" pad="8"/>
<connect gate="G$1" pin="GNDB" pad="9"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_SN74LVC1T45DBV" prefix="IC">
<gates>
<gate name="G$1" symbol="SN74LVC1T45"/>
</gates>
<devices>
<device name="" package="DBV-R-PDSO-G6">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="4"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_SN74LVC2G17" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="DUAL_SCHMITT"/>
</gates>
<devices>
<device name="DBV" package="DBV-R-PDSO-G6">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1Y" pad="6"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCK" package="DCK_R_PDSO_G6">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1Y" pad="6"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_SN74LVC2T45DCT" prefix="IC">
<gates>
<gate name="G$1" symbol="SN74LVC2T45"/>
</gates>
<devices>
<device name="" package="DCT_R_PDSO_G8">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_BUFF_SN74LVC8T245" prefix="IC">
<gates>
<gate name="G$1" symbol="SN74LVC8T245"/>
</gates>
<devices>
<device name="" package="SOIC-24">
<connects>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="B1" pad="21"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="19"/>
<connect gate="G$1" pin="B4" pad="18"/>
<connect gate="G$1" pin="B5" pad="17"/>
<connect gate="G$1" pin="B6" pad="16"/>
<connect gate="G$1" pin="B7" pad="15"/>
<connect gate="G$1" pin="B8" pad="14"/>
<connect gate="G$1" pin="DIR" pad="2"/>
<connect gate="G$1" pin="GND1" pad="11"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="OE" pad="22"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB1" pad="24"/>
<connect gate="G$1" pin="VCCB2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_CPLD_EPM3064A" prefix="IC">
<description>64 Macrocells 3.3V CPLD</description>
<gates>
<gate name="G$1" symbol="EPM3064A"/>
</gates>
<devices>
<device name="-TQFP44" package="TQFP-44">
<connects>
<connect gate="G$1" pin="A-(1)I/O/TDI" pad="P1"/>
<connect gate="G$1" pin="A-(2)I/O" pad="P2"/>
<connect gate="G$1" pin="A-(3)I/O" pad="P3"/>
<connect gate="G$1" pin="A-(4)I/O" pad="P5"/>
<connect gate="G$1" pin="A-(5)I/O" pad="P6"/>
<connect gate="G$1" pin="A-(6)I/O" pad="P42"/>
<connect gate="G$1" pin="A-(7)I/O" pad="P43"/>
<connect gate="G$1" pin="A-(8)I/O" pad="P44"/>
<connect gate="G$1" pin="B-(1)I/O/TMS" pad="P7"/>
<connect gate="G$1" pin="B-(2)I/O" pad="P8"/>
<connect gate="G$1" pin="B-(3)I/O" pad="P10"/>
<connect gate="G$1" pin="B-(4)I/O" pad="P12"/>
<connect gate="G$1" pin="B-(5)I/O" pad="P13"/>
<connect gate="G$1" pin="B-(6)I/O" pad="P14"/>
<connect gate="G$1" pin="B-(7)I/O" pad="P15"/>
<connect gate="G$1" pin="C-(1)I/O" pad="P18"/>
<connect gate="G$1" pin="C-(2)I/O" pad="P19"/>
<connect gate="G$1" pin="C-(3)I/O" pad="P20"/>
<connect gate="G$1" pin="C-(4)I/O" pad="P21"/>
<connect gate="G$1" pin="C-(5)I/O" pad="P22"/>
<connect gate="G$1" pin="C-(6)I/O" pad="P23"/>
<connect gate="G$1" pin="C-(7)I/O" pad="P25"/>
<connect gate="G$1" pin="C-(8)I/O/TCK" pad="P26"/>
<connect gate="G$1" pin="D-(1)I/O" pad="P27"/>
<connect gate="G$1" pin="D-(2)I/O" pad="P28"/>
<connect gate="G$1" pin="D-(3)I/O" pad="P31"/>
<connect gate="G$1" pin="D-(4)I/O" pad="P33"/>
<connect gate="G$1" pin="D-(4)I/O/TDO" pad="P32"/>
<connect gate="G$1" pin="D-(5)I/O" pad="P34"/>
<connect gate="G$1" pin="D-(6)I/O" pad="P35"/>
<connect gate="G$1" pin="GNDINT@1" pad="P16"/>
<connect gate="G$1" pin="GNDINT@2" pad="P36"/>
<connect gate="G$1" pin="GNDIO@1" pad="P4"/>
<connect gate="G$1" pin="GNDIO@2" pad="P11"/>
<connect gate="G$1" pin="GNDIO@3" pad="P24"/>
<connect gate="G$1" pin="GNDIO@4" pad="P30"/>
<connect gate="G$1" pin="I/GCLK1" pad="P37"/>
<connect gate="G$1" pin="I/GCLRN" pad="P39"/>
<connect gate="G$1" pin="I/OE1" pad="P38"/>
<connect gate="G$1" pin="I/OE2/GCLK2" pad="P40"/>
<connect gate="G$1" pin="VCCINT@1" pad="P17"/>
<connect gate="G$1" pin="VCCINT@2" pad="P41"/>
<connect gate="G$1" pin="VCCIO@1" pad="P9"/>
<connect gate="G$1" pin="VCCIO@2" pad="P29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_CPLD_LC4032V" prefix="IC">
<description>32 Macrocells 3.3V CPLD</description>
<gates>
<gate name="G$1" symbol="LC4032V"/>
</gates>
<devices>
<device name="-TQFP44" package="TQFP-44">
<connects>
<connect gate="G$1" pin="A-A0/GOE" pad="P40"/>
<connect gate="G$1" pin="A-CLK/I" pad="P39"/>
<connect gate="G$1" pin="A-GND" pad="P5"/>
<connect gate="G$1" pin="A-VCCO" pad="P6"/>
<connect gate="G$1" pin="A1" pad="P41"/>
<connect gate="G$1" pin="A10" pad="P9"/>
<connect gate="G$1" pin="A12" pad="P13"/>
<connect gate="G$1" pin="A13" pad="P14"/>
<connect gate="G$1" pin="A14" pad="P15"/>
<connect gate="G$1" pin="A15" pad="P16"/>
<connect gate="G$1" pin="A2" pad="P42"/>
<connect gate="G$1" pin="A3" pad="P43"/>
<connect gate="G$1" pin="A4" pad="P44"/>
<connect gate="G$1" pin="A5" pad="P2"/>
<connect gate="G$1" pin="A6" pad="P3"/>
<connect gate="G$1" pin="A7" pad="P4"/>
<connect gate="G$1" pin="A8" pad="P7"/>
<connect gate="G$1" pin="A9" pad="P8"/>
<connect gate="G$1" pin="B-B15/GOE" pad="P38"/>
<connect gate="G$1" pin="B-CLK2/I" pad="P17"/>
<connect gate="G$1" pin="B-GND" pad="P27"/>
<connect gate="G$1" pin="B-VCCO" pad="P28"/>
<connect gate="G$1" pin="B0" pad="P18"/>
<connect gate="G$1" pin="B1" pad="P19"/>
<connect gate="G$1" pin="B10" pad="P31"/>
<connect gate="G$1" pin="B12" pad="P35"/>
<connect gate="G$1" pin="B13" pad="P36"/>
<connect gate="G$1" pin="B14" pad="P37"/>
<connect gate="G$1" pin="B2" pad="P20"/>
<connect gate="G$1" pin="B3" pad="P21"/>
<connect gate="G$1" pin="B4" pad="P22"/>
<connect gate="G$1" pin="B5" pad="P24"/>
<connect gate="G$1" pin="B6" pad="P25"/>
<connect gate="G$1" pin="B7" pad="P26"/>
<connect gate="G$1" pin="B8" pad="P29"/>
<connect gate="G$1" pin="B9" pad="P30"/>
<connect gate="G$1" pin="GND@1" pad="P12"/>
<connect gate="G$1" pin="GND@2" pad="P34"/>
<connect gate="G$1" pin="TCK" pad="P10"/>
<connect gate="G$1" pin="TDI" pad="P1"/>
<connect gate="G$1" pin="TDO" pad="P32"/>
<connect gate="G$1" pin="TMS" pad="P23"/>
<connect gate="G$1" pin="VCC@1" pad="P11"/>
<connect gate="G$1" pin="VCC@2" pad="P33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_CPLD_XC2C32A" prefix="IC">
<description>&lt;b&gt;xc2c32a_vq44-ian&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: xc2c32a_vq44-ian.bsd</description>
<gates>
<gate name="G$1" symbol="XC2C32A_VQ44-IAN"/>
</gates>
<devices>
<device name="" package="VQ-44">
<connects>
<connect gate="G$1" pin="GND@0" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="IN_32" pad="18"/>
<connect gate="G$1" pin="IO_0" pad="38"/>
<connect gate="G$1" pin="IO_1" pad="37"/>
<connect gate="G$1" pin="IO_10" pad="27"/>
<connect gate="G$1" pin="IO_11" pad="23"/>
<connect gate="G$1" pin="IO_12" pad="22"/>
<connect gate="G$1" pin="IO_13" pad="21"/>
<connect gate="G$1" pin="IO_14" pad="20"/>
<connect gate="G$1" pin="IO_15" pad="19"/>
<connect gate="G$1" pin="IO_16" pad="39"/>
<connect gate="G$1" pin="IO_17" pad="40"/>
<connect gate="G$1" pin="IO_18" pad="41"/>
<connect gate="G$1" pin="IO_19" pad="42"/>
<connect gate="G$1" pin="IO_2" pad="36"/>
<connect gate="G$1" pin="IO_20" pad="43"/>
<connect gate="G$1" pin="IO_21" pad="44"/>
<connect gate="G$1" pin="IO_22" pad="1"/>
<connect gate="G$1" pin="IO_23" pad="2"/>
<connect gate="G$1" pin="IO_24" pad="3"/>
<connect gate="G$1" pin="IO_25" pad="5"/>
<connect gate="G$1" pin="IO_26" pad="6"/>
<connect gate="G$1" pin="IO_27" pad="8"/>
<connect gate="G$1" pin="IO_28" pad="12"/>
<connect gate="G$1" pin="IO_29" pad="13"/>
<connect gate="G$1" pin="IO_3" pad="34"/>
<connect gate="G$1" pin="IO_30" pad="14"/>
<connect gate="G$1" pin="IO_31" pad="16"/>
<connect gate="G$1" pin="IO_4" pad="33"/>
<connect gate="G$1" pin="IO_5" pad="32"/>
<connect gate="G$1" pin="IO_6" pad="31"/>
<connect gate="G$1" pin="IO_7" pad="30"/>
<connect gate="G$1" pin="IO_8" pad="29"/>
<connect gate="G$1" pin="IO_9" pad="28"/>
<connect gate="G$1" pin="TCK" pad="11"/>
<connect gate="G$1" pin="TDI" pad="9"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="10"/>
<connect gate="G$1" pin="VDDAUX" pad="35"/>
<connect gate="G$1" pin="VDDINT" pad="15"/>
<connect gate="G$1" pin="VDDIO1" pad="7"/>
<connect gate="G$1" pin="VDDIO2" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_CPLD_XC3S250E_2" prefix="IC">
<description>&lt;b&gt;XC3S250E_VQ100&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: XC3S250E_VQ100.bsdl</description>
<gates>
<gate name="G$1" symbol="XC3S250E_VQ100"/>
</gates>
<devices>
<device name="" package="VQ-100">
<connects>
<connect gate="G$1" pin="DONE" pad="51"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@10" pad="81"/>
<connect gate="G$1" pin="GND@11" pad="87"/>
<connect gate="G$1" pin="GND@12" pad="93"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="GND@3" pad="19"/>
<connect gate="G$1" pin="GND@4" pad="29"/>
<connect gate="G$1" pin="GND@5" pad="37"/>
<connect gate="G$1" pin="GND@6" pad="52"/>
<connect gate="G$1" pin="GND@7" pad="59"/>
<connect gate="G$1" pin="GND@8" pad="64"/>
<connect gate="G$1" pin="GND@9" pad="72"/>
<connect gate="G$1" pin="IPAD107" pad="39"/>
<connect gate="G$1" pin="IPAD108" pad="38"/>
<connect gate="G$1" pin="IPAD114" pad="30"/>
<connect gate="G$1" pin="IPAD152" pad="13"/>
<connect gate="G$1" pin="IPAD21" pad="89"/>
<connect gate="G$1" pin="IPAD22" pad="88"/>
<connect gate="G$1" pin="IPAD61" pad="69"/>
<connect gate="G$1" pin="P10" pad="10"/>
<connect gate="G$1" pin="P11" pad="11"/>
<connect gate="G$1" pin="P12" pad="12"/>
<connect gate="G$1" pin="P15" pad="15"/>
<connect gate="G$1" pin="P16" pad="16"/>
<connect gate="G$1" pin="P17" pad="17"/>
<connect gate="G$1" pin="P18" pad="18"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P22" pad="22"/>
<connect gate="G$1" pin="P23" pad="23"/>
<connect gate="G$1" pin="P24" pad="24"/>
<connect gate="G$1" pin="P25" pad="25"/>
<connect gate="G$1" pin="P26" pad="26"/>
<connect gate="G$1" pin="P27" pad="27"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P32" pad="32"/>
<connect gate="G$1" pin="P33" pad="33"/>
<connect gate="G$1" pin="P34" pad="34"/>
<connect gate="G$1" pin="P35" pad="35"/>
<connect gate="G$1" pin="P36" pad="36"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P40" pad="40"/>
<connect gate="G$1" pin="P41" pad="41"/>
<connect gate="G$1" pin="P42" pad="42"/>
<connect gate="G$1" pin="P43" pad="43"/>
<connect gate="G$1" pin="P44" pad="44"/>
<connect gate="G$1" pin="P47" pad="47"/>
<connect gate="G$1" pin="P48" pad="48"/>
<connect gate="G$1" pin="P49" pad="49"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P50" pad="50"/>
<connect gate="G$1" pin="P53" pad="53"/>
<connect gate="G$1" pin="P54" pad="54"/>
<connect gate="G$1" pin="P57" pad="57"/>
<connect gate="G$1" pin="P58" pad="58"/>
<connect gate="G$1" pin="P60" pad="60"/>
<connect gate="G$1" pin="P61" pad="61"/>
<connect gate="G$1" pin="P62" pad="62"/>
<connect gate="G$1" pin="P63" pad="63"/>
<connect gate="G$1" pin="P65" pad="65"/>
<connect gate="G$1" pin="P66" pad="66"/>
<connect gate="G$1" pin="P67" pad="67"/>
<connect gate="G$1" pin="P68" pad="68"/>
<connect gate="G$1" pin="P70" pad="70"/>
<connect gate="G$1" pin="P71" pad="71"/>
<connect gate="G$1" pin="P78" pad="78"/>
<connect gate="G$1" pin="P79" pad="79"/>
<connect gate="G$1" pin="P83" pad="83"/>
<connect gate="G$1" pin="P84" pad="84"/>
<connect gate="G$1" pin="P85" pad="85"/>
<connect gate="G$1" pin="P86" pad="86"/>
<connect gate="G$1" pin="P9" pad="9"/>
<connect gate="G$1" pin="P90" pad="90"/>
<connect gate="G$1" pin="P91" pad="91"/>
<connect gate="G$1" pin="P92" pad="92"/>
<connect gate="G$1" pin="P94" pad="94"/>
<connect gate="G$1" pin="P95" pad="95"/>
<connect gate="G$1" pin="P98" pad="98"/>
<connect gate="G$1" pin="PROG_B" pad="1"/>
<connect gate="G$1" pin="PUDC_B" pad="99"/>
<connect gate="G$1" pin="TCK" pad="77"/>
<connect gate="G$1" pin="TDI" pad="100"/>
<connect gate="G$1" pin="TDO" pad="76"/>
<connect gate="G$1" pin="TMS" pad="75"/>
<connect gate="G$1" pin="VCCAUX@1" pad="21"/>
<connect gate="G$1" pin="VCCAUX@2" pad="46"/>
<connect gate="G$1" pin="VCCAUX@3" pad="74"/>
<connect gate="G$1" pin="VCCAUX@4" pad="96"/>
<connect gate="G$1" pin="VCCINT@1" pad="6"/>
<connect gate="G$1" pin="VCCINT@2" pad="28"/>
<connect gate="G$1" pin="VCCINT@3" pad="56"/>
<connect gate="G$1" pin="VCCINT@4" pad="80"/>
<connect gate="G$1" pin="VCCO_0@1" pad="82"/>
<connect gate="G$1" pin="VCCO_0@2" pad="97"/>
<connect gate="G$1" pin="VCCO_1@1" pad="55"/>
<connect gate="G$1" pin="VCCO_1@2" pad="73"/>
<connect gate="G$1" pin="VCCO_2@1" pad="31"/>
<connect gate="G$1" pin="VCCO_2@2" pad="45"/>
<connect gate="G$1" pin="VCCO_3@1" pad="8"/>
<connect gate="G$1" pin="VCCO_3@2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_CPLD_XC9572" prefix="IC">
<gates>
<gate name="G$1" symbol="XC9572XL"/>
</gates>
<devices>
<device name="VQ44" package="VQ-44">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="17"/>
<connect gate="G$1" pin="GND3" pad="25"/>
<connect gate="G$1" pin="IO1-11/GCK2" pad="44"/>
<connect gate="G$1" pin="IO1-14/GCK3" pad="1"/>
<connect gate="G$1" pin="IO1-15" pad="2"/>
<connect gate="G$1" pin="IO1-17" pad="3"/>
<connect gate="G$1" pin="IO1-2" pad="39"/>
<connect gate="G$1" pin="IO1-5" pad="40"/>
<connect gate="G$1" pin="IO1-6" pad="41"/>
<connect gate="G$1" pin="IO1-8" pad="42"/>
<connect gate="G$1" pin="IO1-9/GCK1" pad="43"/>
<connect gate="G$1" pin="IO2-11/GTS2" pad="34"/>
<connect gate="G$1" pin="IO2-14/GTS1" pad="36"/>
<connect gate="G$1" pin="IO2-15" pad="37"/>
<connect gate="G$1" pin="IO2-17" pad="38"/>
<connect gate="G$1" pin="IO2-2" pad="29"/>
<connect gate="G$1" pin="IO2-5" pad="30"/>
<connect gate="G$1" pin="IO2-6" pad="31"/>
<connect gate="G$1" pin="IO2-8" pad="32"/>
<connect gate="G$1" pin="IO2-9/GSR" pad="33"/>
<connect gate="G$1" pin="IO3-11" pad="12"/>
<connect gate="G$1" pin="IO3-14" pad="13"/>
<connect gate="G$1" pin="IO3-15" pad="14"/>
<connect gate="G$1" pin="IO3-16" pad="18"/>
<connect gate="G$1" pin="IO3-17" pad="16"/>
<connect gate="G$1" pin="IO3-2" pad="5"/>
<connect gate="G$1" pin="IO3-5" pad="6"/>
<connect gate="G$1" pin="IO3-8" pad="7"/>
<connect gate="G$1" pin="IO3-9" pad="8"/>
<connect gate="G$1" pin="IO4-11" pad="22"/>
<connect gate="G$1" pin="IO4-14" pad="23"/>
<connect gate="G$1" pin="IO4-15" pad="27"/>
<connect gate="G$1" pin="IO4-17" pad="28"/>
<connect gate="G$1" pin="IO4-2" pad="19"/>
<connect gate="G$1" pin="IO4-5" pad="20"/>
<connect gate="G$1" pin="IO4-8" pad="21"/>
<connect gate="G$1" pin="TCK" pad="11"/>
<connect gate="G$1" pin="TDI" pad="9"/>
<connect gate="G$1" pin="TDO" pad="24"/>
<connect gate="G$1" pin="TMS" pad="10"/>
<connect gate="G$1" pin="VCCINT1" pad="15"/>
<connect gate="G$1" pin="VCCINT2" pad="35"/>
<connect gate="G$1" pin="VCCIO" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_DIL14" prefix="IC">
<description>Universal 14pins IC</description>
<gates>
<gate name="G$1" symbol="DIL-14"/>
</gates>
<devices>
<device name="-PTH" package="DIP14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTHW" package="DIP14W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_DIL18" prefix="IC">
<description>Universal 18pins IC</description>
<gates>
<gate name="G$1" symbol="DIL-18"/>
</gates>
<devices>
<device name="-EDGE" package="EGDE2X9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH" package="DIP18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_DIL20" prefix="IC">
<description>Universal 20pins IC</description>
<gates>
<gate name="G$1" symbol="DIL-20"/>
</gates>
<devices>
<device name="-EDGE" package="EGDE2X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH" package="DIP20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_DIL8" prefix="IC">
<description>Universal 8pins IC</description>
<gates>
<gate name="G$1" symbol="DIL-8"/>
</gates>
<devices>
<device name="-PTH" package="DIP8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO8" package="SO-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_DS1085" prefix="IC">
<gates>
<gate name="IC" symbol="DS1085"/>
</gates>
<devices>
<device name="-SO-8" package="SO-8">
<connects>
<connect gate="IC" pin="CTRL0" pad="5"/>
<connect gate="IC" pin="CTRL1" pad="6"/>
<connect gate="IC" pin="GND" pad="4"/>
<connect gate="IC" pin="OUT0" pad="2"/>
<connect gate="IC" pin="OUT1" pad="1"/>
<connect gate="IC" pin="SCL" pad="8"/>
<connect gate="IC" pin="SDA" pad="7"/>
<connect gate="IC" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_ENC424J600" prefix="IC">
<description>Stand-Alone 10/100 Ethernet Controller with SPI or Parallel Interface

Source: http://ww1.microchip.com/downloads/en/DeviceDoc/39935c.pdf</description>
<gates>
<gate name="G$1" symbol="ENC424J600"/>
</gates>
<devices>
<device name="-TQFP44" package="TQFP-44">
<connects>
<connect gate="G$1" pin="AD0" pad="P38"/>
<connect gate="G$1" pin="AD1" pad="P39"/>
<connect gate="G$1" pin="AD10" pad="P27"/>
<connect gate="G$1" pin="AD11" pad="P28"/>
<connect gate="G$1" pin="AD12" pad="P29"/>
<connect gate="G$1" pin="AD13" pad="P30"/>
<connect gate="G$1" pin="AD14" pad="P31"/>
<connect gate="G$1" pin="AD2" pad="P40"/>
<connect gate="G$1" pin="AD3" pad="P41"/>
<connect gate="G$1" pin="AD4" pad="P5"/>
<connect gate="G$1" pin="AD5" pad="P6"/>
<connect gate="G$1" pin="AD6" pad="P7"/>
<connect gate="G$1" pin="AD7" pad="P8"/>
<connect gate="G$1" pin="AD8" pad="P25"/>
<connect gate="G$1" pin="AD9" pad="P26"/>
<connect gate="G$1" pin="CLKOUT" pad="P23"/>
<connect gate="G$1" pin="CS" pad="P34"/>
<connect gate="G$1" pin="INT/SPISEL" pad="P24"/>
<connect gate="G$1" pin="LEDA" pad="P10"/>
<connect gate="G$1" pin="LEDB" pad="P9"/>
<connect gate="G$1" pin="OSC1" pad="P3"/>
<connect gate="G$1" pin="OSC2" pad="P2"/>
<connect gate="G$1" pin="PSPCFG0" pad="P32"/>
<connect gate="G$1" pin="RBIAS" pad="P11"/>
<connect gate="G$1" pin="SCK/AL" pad="P37"/>
<connect gate="G$1" pin="SI/RD/RW" pad="P36"/>
<connect gate="G$1" pin="SO/WR/EN" pad="P35"/>
<connect gate="G$1" pin="TPIN+" pad="P16"/>
<connect gate="G$1" pin="TPIN-" pad="P17"/>
<connect gate="G$1" pin="TPOUT+" pad="P20"/>
<connect gate="G$1" pin="TPOUT-" pad="P21"/>
<connect gate="G$1" pin="VCAP" pad="P43"/>
<connect gate="G$1" pin="VDD" pad="P44"/>
<connect gate="G$1" pin="VDDOSC" pad="P4"/>
<connect gate="G$1" pin="VDDPLL" pad="P12"/>
<connect gate="G$1" pin="VDDRX" pad="P15"/>
<connect gate="G$1" pin="VDDTX" pad="P18"/>
<connect gate="G$1" pin="VSS1" pad="P42"/>
<connect gate="G$1" pin="VSS2" pad="P33"/>
<connect gate="G$1" pin="VSSOSC" pad="P1"/>
<connect gate="G$1" pin="VSSPLL" pad="P13"/>
<connect gate="G$1" pin="VSSRX" pad="P14"/>
<connect gate="G$1" pin="VSSTX1" pad="P19"/>
<connect gate="G$1" pin="VSSTX2" pad="P22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FAN5331" prefix="IC">
<gates>
<gate name="G$1" symbol="FAN5331"/>
</gates>
<devices>
<device name="-SOT-23-5" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="!SHDN" pad="4"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FPGA_XC3S250E" prefix="IC">
<description>&lt;b&gt;xc3s250e_vq100_1532&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: xc3s250e_vq100_1532.bsd</description>
<gates>
<gate name="G$1" symbol="XC3S250E_VQ100_1532"/>
</gates>
<devices>
<device name="" package="VQ-100">
<connects>
<connect gate="G$1" pin="DONE" pad="51"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@10" pad="81"/>
<connect gate="G$1" pin="GND@11" pad="87"/>
<connect gate="G$1" pin="GND@12" pad="93"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="GND@3" pad="19"/>
<connect gate="G$1" pin="GND@4" pad="29"/>
<connect gate="G$1" pin="GND@5" pad="37"/>
<connect gate="G$1" pin="GND@6" pad="52"/>
<connect gate="G$1" pin="GND@7" pad="59"/>
<connect gate="G$1" pin="GND@8" pad="64"/>
<connect gate="G$1" pin="GND@9" pad="72"/>
<connect gate="G$1" pin="IPAD107" pad="39"/>
<connect gate="G$1" pin="IPAD108" pad="38"/>
<connect gate="G$1" pin="IPAD114" pad="30"/>
<connect gate="G$1" pin="IPAD152" pad="13"/>
<connect gate="G$1" pin="IPAD21" pad="89"/>
<connect gate="G$1" pin="IPAD22" pad="88"/>
<connect gate="G$1" pin="IPAD61" pad="69"/>
<connect gate="G$1" pin="P10" pad="10"/>
<connect gate="G$1" pin="P11" pad="11"/>
<connect gate="G$1" pin="P12" pad="12"/>
<connect gate="G$1" pin="P15" pad="15"/>
<connect gate="G$1" pin="P16" pad="16"/>
<connect gate="G$1" pin="P17" pad="17"/>
<connect gate="G$1" pin="P18" pad="18"/>
<connect gate="G$1" pin="P2" pad="2"/>
<connect gate="G$1" pin="P22" pad="22"/>
<connect gate="G$1" pin="P23" pad="23"/>
<connect gate="G$1" pin="P24" pad="24"/>
<connect gate="G$1" pin="P25" pad="25"/>
<connect gate="G$1" pin="P26" pad="26"/>
<connect gate="G$1" pin="P27" pad="27"/>
<connect gate="G$1" pin="P3" pad="3"/>
<connect gate="G$1" pin="P32" pad="32"/>
<connect gate="G$1" pin="P33" pad="33"/>
<connect gate="G$1" pin="P34" pad="34"/>
<connect gate="G$1" pin="P35" pad="35"/>
<connect gate="G$1" pin="P36" pad="36"/>
<connect gate="G$1" pin="P4" pad="4"/>
<connect gate="G$1" pin="P40" pad="40"/>
<connect gate="G$1" pin="P41" pad="41"/>
<connect gate="G$1" pin="P42" pad="42"/>
<connect gate="G$1" pin="P43" pad="43"/>
<connect gate="G$1" pin="P44" pad="44"/>
<connect gate="G$1" pin="P47" pad="47"/>
<connect gate="G$1" pin="P48" pad="48"/>
<connect gate="G$1" pin="P49" pad="49"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P50" pad="50"/>
<connect gate="G$1" pin="P53" pad="53"/>
<connect gate="G$1" pin="P54" pad="54"/>
<connect gate="G$1" pin="P57" pad="57"/>
<connect gate="G$1" pin="P58" pad="58"/>
<connect gate="G$1" pin="P60" pad="60"/>
<connect gate="G$1" pin="P61" pad="61"/>
<connect gate="G$1" pin="P62" pad="62"/>
<connect gate="G$1" pin="P63" pad="63"/>
<connect gate="G$1" pin="P65" pad="65"/>
<connect gate="G$1" pin="P66" pad="66"/>
<connect gate="G$1" pin="P67" pad="67"/>
<connect gate="G$1" pin="P68" pad="68"/>
<connect gate="G$1" pin="P70" pad="70"/>
<connect gate="G$1" pin="P71" pad="71"/>
<connect gate="G$1" pin="P78" pad="78"/>
<connect gate="G$1" pin="P79" pad="79"/>
<connect gate="G$1" pin="P83" pad="83"/>
<connect gate="G$1" pin="P84" pad="84"/>
<connect gate="G$1" pin="P85" pad="85"/>
<connect gate="G$1" pin="P86" pad="86"/>
<connect gate="G$1" pin="P9" pad="9"/>
<connect gate="G$1" pin="P90" pad="90"/>
<connect gate="G$1" pin="P91" pad="91"/>
<connect gate="G$1" pin="P92" pad="92"/>
<connect gate="G$1" pin="P94" pad="94"/>
<connect gate="G$1" pin="P95" pad="95"/>
<connect gate="G$1" pin="P98" pad="98"/>
<connect gate="G$1" pin="PROG_B" pad="1"/>
<connect gate="G$1" pin="PUDC_B" pad="99"/>
<connect gate="G$1" pin="TCK" pad="77"/>
<connect gate="G$1" pin="TDI" pad="100"/>
<connect gate="G$1" pin="TDO" pad="76"/>
<connect gate="G$1" pin="TMS" pad="75"/>
<connect gate="G$1" pin="VCCAUX@1" pad="21"/>
<connect gate="G$1" pin="VCCAUX@2" pad="46"/>
<connect gate="G$1" pin="VCCAUX@3" pad="74"/>
<connect gate="G$1" pin="VCCAUX@4" pad="96"/>
<connect gate="G$1" pin="VCCINT@1" pad="6"/>
<connect gate="G$1" pin="VCCINT@2" pad="28"/>
<connect gate="G$1" pin="VCCINT@3" pad="56"/>
<connect gate="G$1" pin="VCCINT@4" pad="80"/>
<connect gate="G$1" pin="VCCO_0@1" pad="82"/>
<connect gate="G$1" pin="VCCO_0@2" pad="97"/>
<connect gate="G$1" pin="VCCO_1@1" pad="55"/>
<connect gate="G$1" pin="VCCO_1@2" pad="73"/>
<connect gate="G$1" pin="VCCO_2@1" pad="31"/>
<connect gate="G$1" pin="VCCO_2@2" pad="45"/>
<connect gate="G$1" pin="VCCO_3@1" pad="8"/>
<connect gate="G$1" pin="VCCO_3@2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FPGA_XC6SLX9" prefix="IC">
<gates>
<gate name="G$1" symbol="XC6SLX9-3TQG144C"/>
</gates>
<devices>
<device name="3TQG144C" package="TQFP-144">
<connects>
<connect gate="G$1" pin="CMPCS_B_2" pad="72"/>
<connect gate="G$1" pin="DONE_2" pad="71"/>
<connect gate="G$1" pin="GND_A" pad="3"/>
<connect gate="G$1" pin="GND_B" pad="13"/>
<connect gate="G$1" pin="GND_C" pad="25"/>
<connect gate="G$1" pin="GND_D" pad="49"/>
<connect gate="G$1" pin="GND_E" pad="54"/>
<connect gate="G$1" pin="GND_F" pad="68"/>
<connect gate="G$1" pin="GND_G" pad="77"/>
<connect gate="G$1" pin="GND_H" pad="91"/>
<connect gate="G$1" pin="GND_I" pad="96"/>
<connect gate="G$1" pin="GND_J" pad="108"/>
<connect gate="G$1" pin="GND_K" pad="113"/>
<connect gate="G$1" pin="GND_L" pad="130"/>
<connect gate="G$1" pin="GND_M" pad="136"/>
<connect gate="G$1" pin="IO_L12N_D2_MISO3_2" pad="61"/>
<connect gate="G$1" pin="IO_L12P_D1_MISO2_2" pad="62"/>
<connect gate="G$1" pin="IO_L13N_D10_2" pad="59"/>
<connect gate="G$1" pin="IO_L13P_M1_2" pad="60"/>
<connect gate="G$1" pin="IO_L14N_D12_2" pad="57"/>
<connect gate="G$1" pin="IO_L14P_D11_2" pad="58"/>
<connect gate="G$1" pin="IO_L1N_M0_CMPMISO_2" pad="69"/>
<connect gate="G$1" pin="IO_L1N_VREF_0" pad="143"/>
<connect gate="G$1" pin="IO_L1N_VREF_1" pad="104"/>
<connect gate="G$1" pin="IO_L1N_VREF_3" pad="34"/>
<connect gate="G$1" pin="IO_L1P_1" pad="105"/>
<connect gate="G$1" pin="IO_L1P_3" pad="35"/>
<connect gate="G$1" pin="IO_L1P_CCLK_2" pad="70"/>
<connect gate="G$1" pin="IO_L1P_HSWAPEN_0" pad="144"/>
<connect gate="G$1" pin="IO_L2N_0" pad="141"/>
<connect gate="G$1" pin="IO_L2N_3" pad="32"/>
<connect gate="G$1" pin="IO_L2N_CMPMOSI_2" pad="66"/>
<connect gate="G$1" pin="IO_L2P_0" pad="142"/>
<connect gate="G$1" pin="IO_L2P_3" pad="33"/>
<connect gate="G$1" pin="IO_L2P_CMPCLK_2" pad="67"/>
<connect gate="G$1" pin="IO_L30N_GCLK0_USERCCLK_2" pad="55"/>
<connect gate="G$1" pin="IO_L30P_GCLK1_D13_2" pad="56"/>
<connect gate="G$1" pin="IO_L31N_GCLK30_D15_2" pad="50"/>
<connect gate="G$1" pin="IO_L31P_GCLK31_D14_2" pad="51"/>
<connect gate="G$1" pin="IO_L32N_1" pad="101"/>
<connect gate="G$1" pin="IO_L32P_1" pad="102"/>
<connect gate="G$1" pin="IO_L33N_1" pad="99"/>
<connect gate="G$1" pin="IO_L33P_1" pad="100"/>
<connect gate="G$1" pin="IO_L34N_1" pad="97"/>
<connect gate="G$1" pin="IO_L34N_GCLK18_0" pad="133"/>
<connect gate="G$1" pin="IO_L34P_1" pad="98"/>
<connect gate="G$1" pin="IO_L34P_GCLK19_0" pad="134"/>
<connect gate="G$1" pin="IO_L35N_GCLK16_0" pad="131"/>
<connect gate="G$1" pin="IO_L35P_GCLK17_0" pad="132"/>
<connect gate="G$1" pin="IO_L36N_3" pad="29"/>
<connect gate="G$1" pin="IO_L36N_GCLK14_0" pad="126"/>
<connect gate="G$1" pin="IO_L36P_3" pad="30"/>
<connect gate="G$1" pin="IO_L36P_GCLK15_0" pad="127"/>
<connect gate="G$1" pin="IO_L37N_3" pad="26"/>
<connect gate="G$1" pin="IO_L37N_GCLK12_0" pad="123"/>
<connect gate="G$1" pin="IO_L37P_3" pad="27"/>
<connect gate="G$1" pin="IO_L37P_GCLK13_0" pad="124"/>
<connect gate="G$1" pin="IO_L3N_0" pad="139"/>
<connect gate="G$1" pin="IO_L3N_MOSI_CSI_B_MISO0_2" pad="64"/>
<connect gate="G$1" pin="IO_L3P_0" pad="140"/>
<connect gate="G$1" pin="IO_L3P_D0_DIN_MISO_MISO1_2" pad="65"/>
<connect gate="G$1" pin="IO_L40N_GCLK10_1" pad="94"/>
<connect gate="G$1" pin="IO_L40P_GCLK11_1" pad="95"/>
<connect gate="G$1" pin="IO_L41N_GCLK26_3" pad="23"/>
<connect gate="G$1" pin="IO_L41N_GCLK8_1" pad="92"/>
<connect gate="G$1" pin="IO_L41P_GCLK27_3" pad="24"/>
<connect gate="G$1" pin="IO_L41P_GCLK9_IRDY1_1" pad="93"/>
<connect gate="G$1" pin="IO_L42N_GCLK24_3" pad="21"/>
<connect gate="G$1" pin="IO_L42N_GCLK6_TRDY1_1" pad="87"/>
<connect gate="G$1" pin="IO_L42P_GCLK25_TRDY2_3" pad="22"/>
<connect gate="G$1" pin="IO_L42P_GCLK7_1" pad="88"/>
<connect gate="G$1" pin="IO_L43N_GCLK22_IRDY2_3" pad="16"/>
<connect gate="G$1" pin="IO_L43N_GCLK4_1" pad="84"/>
<connect gate="G$1" pin="IO_L43P_GCLK23_3" pad="17"/>
<connect gate="G$1" pin="IO_L43P_GCLK5_1" pad="85"/>
<connect gate="G$1" pin="IO_L44N_GCLK20_3" pad="14"/>
<connect gate="G$1" pin="IO_L44P_GCLK21_3" pad="15"/>
<connect gate="G$1" pin="IO_L45N_1" pad="82"/>
<connect gate="G$1" pin="IO_L45P_1" pad="83"/>
<connect gate="G$1" pin="IO_L46N_1" pad="80"/>
<connect gate="G$1" pin="IO_L46P_1" pad="81"/>
<connect gate="G$1" pin="IO_L47N_1" pad="78"/>
<connect gate="G$1" pin="IO_L47P_1" pad="79"/>
<connect gate="G$1" pin="IO_L48N_RDWR_B_VREF_2" pad="47"/>
<connect gate="G$1" pin="IO_L48P_D7_2" pad="48"/>
<connect gate="G$1" pin="IO_L49N_3" pad="11"/>
<connect gate="G$1" pin="IO_L49N_D4_2" pad="45"/>
<connect gate="G$1" pin="IO_L49P_3" pad="12"/>
<connect gate="G$1" pin="IO_L49P_D3_2" pad="46"/>
<connect gate="G$1" pin="IO_L4N_0" pad="137"/>
<connect gate="G$1" pin="IO_L4P_0" pad="138"/>
<connect gate="G$1" pin="IO_L50N_3" pad="9"/>
<connect gate="G$1" pin="IO_L50P_3" pad="10"/>
<connect gate="G$1" pin="IO_L51N_3" pad="7"/>
<connect gate="G$1" pin="IO_L51P_3" pad="8"/>
<connect gate="G$1" pin="IO_L52N_3" pad="5"/>
<connect gate="G$1" pin="IO_L52P_3" pad="6"/>
<connect gate="G$1" pin="IO_L62N_D6_2" pad="43"/>
<connect gate="G$1" pin="IO_L62N_VREF_0" pad="120"/>
<connect gate="G$1" pin="IO_L62P_0" pad="121"/>
<connect gate="G$1" pin="IO_L62P_D5_2" pad="44"/>
<connect gate="G$1" pin="IO_L63N_SCP6_0" pad="118"/>
<connect gate="G$1" pin="IO_L63P_SCP7_0" pad="119"/>
<connect gate="G$1" pin="IO_L64N_D9_2" pad="40"/>
<connect gate="G$1" pin="IO_L64N_SCP4_0" pad="116"/>
<connect gate="G$1" pin="IO_L64P_D8_2" pad="41"/>
<connect gate="G$1" pin="IO_L64P_SCP5_0" pad="117"/>
<connect gate="G$1" pin="IO_L65N_CSO_B_2" pad="38"/>
<connect gate="G$1" pin="IO_L65N_SCP2_0" pad="114"/>
<connect gate="G$1" pin="IO_L65P_INIT_B_2" pad="39"/>
<connect gate="G$1" pin="IO_L65P_SCP3_0" pad="115"/>
<connect gate="G$1" pin="IO_L66N_SCP0_0" pad="111"/>
<connect gate="G$1" pin="IO_L66P_SCP1_0" pad="112"/>
<connect gate="G$1" pin="IO_L74N_DOUT_BUSY_1" pad="74"/>
<connect gate="G$1" pin="IO_L74P_AWAKE_1" pad="75"/>
<connect gate="G$1" pin="IO_L83N_VREF_3" pad="1"/>
<connect gate="G$1" pin="IO_L83P_3" pad="2"/>
<connect gate="G$1" pin="PROGRAM_B_2" pad="37"/>
<connect gate="G$1" pin="SUSPEND" pad="73"/>
<connect gate="G$1" pin="TCK" pad="109"/>
<connect gate="G$1" pin="TDI" pad="110"/>
<connect gate="G$1" pin="TDO" pad="106"/>
<connect gate="G$1" pin="TMS" pad="107"/>
<connect gate="G$1" pin="VCCAUX_A" pad="20"/>
<connect gate="G$1" pin="VCCAUX_B" pad="36"/>
<connect gate="G$1" pin="VCCAUX_C" pad="53"/>
<connect gate="G$1" pin="VCCAUX_D" pad="90"/>
<connect gate="G$1" pin="VCCAUX_E" pad="129"/>
<connect gate="G$1" pin="VCCINT_A" pad="19"/>
<connect gate="G$1" pin="VCCINT_B" pad="28"/>
<connect gate="G$1" pin="VCCINT_C" pad="52"/>
<connect gate="G$1" pin="VCCINT_D" pad="89"/>
<connect gate="G$1" pin="VCCINT_E" pad="128"/>
<connect gate="G$1" pin="VCCO_BANK0_A" pad="122"/>
<connect gate="G$1" pin="VCCO_BANK0_B" pad="125"/>
<connect gate="G$1" pin="VCCO_BANK0_C" pad="135"/>
<connect gate="G$1" pin="VCCO_BANK1_A" pad="76"/>
<connect gate="G$1" pin="VCCO_BANK1_B" pad="86"/>
<connect gate="G$1" pin="VCCO_BANK1_C" pad="103"/>
<connect gate="G$1" pin="VCCO_BANK2_A" pad="42"/>
<connect gate="G$1" pin="VCCO_BANK2_B" pad="63"/>
<connect gate="G$1" pin="VCCO_BANK3_A" pad="4"/>
<connect gate="G$1" pin="VCCO_BANK3_B" pad="18"/>
<connect gate="G$1" pin="VCCO_BANK3_C" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FT2232H" prefix="IC" uservalue="yes">
<description>DUAL HIGH SPEED USB TO MULTIPURPOSE UART/FIFO IC</description>
<gates>
<gate name="G$1" symbol="FT-2232"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="ACBUS0/TXDEN/GPIOH0" pad="26"/>
<connect gate="G$1" pin="ACBUS1/GPIOH1" pad="27"/>
<connect gate="G$1" pin="ACBUS2/GPIOH2" pad="28"/>
<connect gate="G$1" pin="ACBUS3/RXLED#/GPIOH3" pad="29"/>
<connect gate="G$1" pin="ACBUS4/TXLED#/GPIOH4" pad="30"/>
<connect gate="G$1" pin="ACBUS5/GPIOH5" pad="32"/>
<connect gate="G$1" pin="ACBUS6/GPIOH6" pad="33"/>
<connect gate="G$1" pin="ACBUS7/GPIOH7" pad="34"/>
<connect gate="G$1" pin="ADBUS0/TXD/TCK/SK" pad="16"/>
<connect gate="G$1" pin="ADBUS1/RXD/TDI/DO" pad="17"/>
<connect gate="G$1" pin="ADBUS2/RTS#/TDO/DI" pad="18"/>
<connect gate="G$1" pin="ADBUS3/CTS#/TMS/CS" pad="19"/>
<connect gate="G$1" pin="ADBUS4/DTR#/GPIOL0" pad="21"/>
<connect gate="G$1" pin="ADBUS5/DSR#/GPIOL1" pad="22"/>
<connect gate="G$1" pin="ADBUS6/DCD#/GPIOL2" pad="23"/>
<connect gate="G$1" pin="ADBUS7/RI#/GPIOL3" pad="24"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCBUS0/GPIOH1" pad="48"/>
<connect gate="G$1" pin="BCBUS1/GPIOH2" pad="52"/>
<connect gate="G$1" pin="BCBUS2" pad="53"/>
<connect gate="G$1" pin="BCBUS3/RXLED#/GPIOH3" pad="54"/>
<connect gate="G$1" pin="BCBUS4/TXLED#/GPIOH4" pad="55"/>
<connect gate="G$1" pin="BCBUS5/GPIOH5" pad="57"/>
<connect gate="G$1" pin="BCBUS6/GPIOH6" pad="58"/>
<connect gate="G$1" pin="BCBUS7/GPIOH7" pad="59"/>
<connect gate="G$1" pin="BDBUS0/TXD/TCK/SK" pad="38"/>
<connect gate="G$1" pin="BDBUS1/RXD/TDI/DO" pad="39"/>
<connect gate="G$1" pin="BDBUS2/RTS#/TDO/DI" pad="40"/>
<connect gate="G$1" pin="BDBUS3/CTS#/TMS/CS" pad="41"/>
<connect gate="G$1" pin="BDBUS4/DTR#/GPIOL0" pad="43"/>
<connect gate="G$1" pin="BDBUS5/DSR#/GPIOL1" pad="44"/>
<connect gate="G$1" pin="BDBUS6/DCD#/GPIOL2" pad="45"/>
<connect gate="G$1" pin="BDBUS7/RI#/GPIOL3" pad="46"/>
<connect gate="G$1" pin="DM" pad="7"/>
<connect gate="G$1" pin="DP" pad="8"/>
<connect gate="G$1" pin="EECLK" pad="62"/>
<connect gate="G$1" pin="EECS" pad="63"/>
<connect gate="G$1" pin="EEDATA" pad="61"/>
<connect gate="G$1" pin="GND0" pad="1"/>
<connect gate="G$1" pin="GND1" pad="5"/>
<connect gate="G$1" pin="GND2" pad="11"/>
<connect gate="G$1" pin="GND3" pad="15"/>
<connect gate="G$1" pin="GND4" pad="25"/>
<connect gate="G$1" pin="GND5" pad="35"/>
<connect gate="G$1" pin="GND6" pad="47"/>
<connect gate="G$1" pin="GND7" pad="51"/>
<connect gate="G$1" pin="OSC0" pad="3"/>
<connect gate="G$1" pin="OSCI" pad="2"/>
<connect gate="G$1" pin="PWREN#" pad="60"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="RESET#" pad="14"/>
<connect gate="G$1" pin="SUSPEND#" pad="36"/>
<connect gate="G$1" pin="TEST" pad="13"/>
<connect gate="G$1" pin="VCCIO0" pad="20"/>
<connect gate="G$1" pin="VCCIO1" pad="31"/>
<connect gate="G$1" pin="VCCIO2" pad="42"/>
<connect gate="G$1" pin="VCCIO3" pad="56"/>
<connect gate="G$1" pin="VCORE0" pad="12"/>
<connect gate="G$1" pin="VCORE1" pad="37"/>
<connect gate="G$1" pin="VCORE2" pad="64"/>
<connect gate="G$1" pin="VPHY" pad="4"/>
<connect gate="G$1" pin="VPLL" pad="9"/>
<connect gate="G$1" pin="VREGIN" pad="50"/>
<connect gate="G$1" pin="VREGOUT" pad="49"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FT232RL-VER2" prefix="IC">
<gates>
<gate name="G$1" symbol="FT232RL-VER2"/>
</gates>
<devices>
<device name="" package="SSOP-28">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="CBUS0" pad="23"/>
<connect gate="G$1" pin="CBUS1" pad="22"/>
<connect gate="G$1" pin="CBUS2" pad="13"/>
<connect gate="G$1" pin="CBUS3" pad="14"/>
<connect gate="G$1" pin="CBUS4" pad="12"/>
<connect gate="G$1" pin="CTS#" pad="11"/>
<connect gate="G$1" pin="DCD#" pad="10"/>
<connect gate="G$1" pin="DSR#" pad="9"/>
<connect gate="G$1" pin="DTR#" pad="2"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="NC1" pad="8"/>
<connect gate="G$1" pin="NC2" pad="24"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="RESET#" pad="19"/>
<connect gate="G$1" pin="RI#" pad="6"/>
<connect gate="G$1" pin="RTS#" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FT232RL" prefix="IC">
<description>USB to serial UART interface</description>
<gates>
<gate name="G$1" symbol="FT232RL"/>
</gates>
<devices>
<device name="" package="SSOP-28">
<connects>
<connect gate="G$1" pin="!CTS" pad="11"/>
<connect gate="G$1" pin="!DCD" pad="10"/>
<connect gate="G$1" pin="!DSR" pad="9"/>
<connect gate="G$1" pin="!DTR" pad="2"/>
<connect gate="G$1" pin="!PWREN" pad="14"/>
<connect gate="G$1" pin="!RESET" pad="19"/>
<connect gate="G$1" pin="!RI" pad="6"/>
<connect gate="G$1" pin="!RTS" pad="3"/>
<connect gate="G$1" pin="!RXLED" pad="22"/>
<connect gate="G$1" pin="!SLEEP" pad="12"/>
<connect gate="G$1" pin="!TXLED" pad="23"/>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="21"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="TXDEN" pad="13"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_LM4910" prefix="IC">
<gates>
<gate name="G$1" symbol="LM4910"/>
</gates>
<devices>
<device name="-SO-8" package="SO-8">
<connects>
<connect gate="G$1" pin="!SHUTDOWN" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VO1" pad="8"/>
<connect gate="G$1" pin="VO2" pad="7"/>
<connect gate="G$1" pin="VO3" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MAX14500" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX14500"/>
</gates>
<devices>
<device name="-TQFN40-5X5" package="TQFN-40-5X5">
<connects>
<connect gate="G$1" pin="!BERR" pad="6"/>
<connect gate="G$1" pin="!BUSY" pad="7"/>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="ADD" pad="4"/>
<connect gate="G$1" pin="CCLK1" pad="32"/>
<connect gate="G$1" pin="CCMD1" pad="34"/>
<connect gate="G$1" pin="CCPRS" pad="33"/>
<connect gate="G$1" pin="CD+" pad="22"/>
<connect gate="G$1" pin="CD-" pad="21"/>
<connect gate="G$1" pin="CDAT1_0" pad="13"/>
<connect gate="G$1" pin="CDAT1_1" pad="12"/>
<connect gate="G$1" pin="CDAT1_2" pad="11"/>
<connect gate="G$1" pin="CDAT1_3" pad="10"/>
<connect gate="G$1" pin="CLDO" pad="38"/>
<connect gate="G$1" pin="EXPAD" pad="EP"/>
<connect gate="G$1" pin="FREF" pad="25"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="GND3" pad="26"/>
<connect gate="G$1" pin="GND4" pad="37"/>
<connect gate="G$1" pin="HCKL1" pad="29"/>
<connect gate="G$1" pin="HCMD1" pad="31"/>
<connect gate="G$1" pin="HCPRS" pad="30"/>
<connect gate="G$1" pin="HD+" pad="20"/>
<connect gate="G$1" pin="HD-" pad="19"/>
<connect gate="G$1" pin="HDAT1_0" pad="17"/>
<connect gate="G$1" pin="HDAT1_1" pad="16"/>
<connect gate="G$1" pin="HDAT1_2" pad="15"/>
<connect gate="G$1" pin="HDAT1_3" pad="14"/>
<connect gate="G$1" pin="I2C_SEL" pad="1"/>
<connect gate="G$1" pin="KVBUS" pad="28"/>
<connect gate="G$1" pin="MODE" pad="8"/>
<connect gate="G$1" pin="NC1" pad="35"/>
<connect gate="G$1" pin="NC2" pad="36"/>
<connect gate="G$1" pin="RREF" pad="27"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VCC" pad="39"/>
<connect gate="G$1" pin="VIO" pad="5"/>
<connect gate="G$1" pin="VSD" pad="40"/>
<connect gate="G$1" pin="VTM" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MAX1896" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX1896"/>
</gates>
<devices>
<device name="" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="!SHDN" pad="4"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="LX" pad="1"/>
<connect gate="G$1" pin="SS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MAX31855" prefix="IC">
<gates>
<gate name="G$1" symbol="MAX31855"/>
</gates>
<devices>
<device name="-SO-8" package="SO-8">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="DNC" pad="8"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SO" pad="7"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MCP2200" prefix="IC">
<gates>
<gate name="G$1" symbol="MCP2200"/>
</gates>
<devices>
<device name="-SOIC-20" package="SOIC-20">
<connects>
<connect gate="G$1" pin="/CTS" pad="13"/>
<connect gate="G$1" pin="/RST" pad="4"/>
<connect gate="G$1" pin="/RTS" pad="11"/>
<connect gate="G$1" pin="D+" pad="19"/>
<connect gate="G$1" pin="D-" pad="18"/>
<connect gate="G$1" pin="GP0" pad="16"/>
<connect gate="G$1" pin="GP1" pad="15"/>
<connect gate="G$1" pin="GP2" pad="14"/>
<connect gate="G$1" pin="GP3" pad="9"/>
<connect gate="G$1" pin="GP4" pad="8"/>
<connect gate="G$1" pin="GP5" pad="7"/>
<connect gate="G$1" pin="GP6" pad="6"/>
<connect gate="G$1" pin="GP7" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="2"/>
<connect gate="G$1" pin="OSC2" pad="3"/>
<connect gate="G$1" pin="RXD" pad="12"/>
<connect gate="G$1" pin="TXD" pad="10"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="20"/>
<connect gate="G$1" pin="VUSB" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SSOP-20" package="SSOP-20">
<connects>
<connect gate="G$1" pin="/CTS" pad="13"/>
<connect gate="G$1" pin="/RST" pad="4"/>
<connect gate="G$1" pin="/RTS" pad="11"/>
<connect gate="G$1" pin="D+" pad="19"/>
<connect gate="G$1" pin="D-" pad="18"/>
<connect gate="G$1" pin="GP0" pad="16"/>
<connect gate="G$1" pin="GP1" pad="15"/>
<connect gate="G$1" pin="GP2" pad="14"/>
<connect gate="G$1" pin="GP3" pad="9"/>
<connect gate="G$1" pin="GP4" pad="8"/>
<connect gate="G$1" pin="GP5" pad="7"/>
<connect gate="G$1" pin="GP6" pad="6"/>
<connect gate="G$1" pin="GP7" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="2"/>
<connect gate="G$1" pin="OSC2" pad="3"/>
<connect gate="G$1" pin="RXD" pad="12"/>
<connect gate="G$1" pin="TXD" pad="10"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="20"/>
<connect gate="G$1" pin="VUSB" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-QFN-25-5X5" package="QFN25_5X5">
<connects>
<connect gate="G$1" pin="/CTS" pad="10"/>
<connect gate="G$1" pin="/RST" pad="1"/>
<connect gate="G$1" pin="/RTS" pad="8"/>
<connect gate="G$1" pin="D+" pad="16"/>
<connect gate="G$1" pin="D-" pad="15"/>
<connect gate="G$1" pin="GP0" pad="13"/>
<connect gate="G$1" pin="GP1" pad="12"/>
<connect gate="G$1" pin="GP2" pad="11"/>
<connect gate="G$1" pin="GP3" pad="6"/>
<connect gate="G$1" pin="GP4" pad="5"/>
<connect gate="G$1" pin="GP5" pad="4"/>
<connect gate="G$1" pin="GP6" pad="3"/>
<connect gate="G$1" pin="GP7" pad="2"/>
<connect gate="G$1" pin="OSC1" pad="19"/>
<connect gate="G$1" pin="OSC2" pad="20"/>
<connect gate="G$1" pin="RXD" pad="9"/>
<connect gate="G$1" pin="TXD" pad="7"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VSS" pad="17"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MCP3021" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="MCP3021"/>
</gates>
<devices>
<device name="SOT-23-5" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MCP3021" value="MCP3021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MCP4019" prefix="IC">
<description>7-Bit Single I2C Digital Rheostat

Source: http://ww1.microchip.com/downloads/en/DeviceDoc/22147a.pdf</description>
<gates>
<gate name="G$1" symbol="MCP4019"/>
</gates>
<devices>
<device name="" package="SOT-23-5LT">
<connects>
<connect gate="G$1" pin="SCL" pad="P3"/>
<connect gate="G$1" pin="SDA" pad="P4"/>
<connect gate="G$1" pin="VDD" pad="P1"/>
<connect gate="G$1" pin="VSS/B" pad="P2"/>
<connect gate="G$1" pin="W" pad="P5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MCP4725" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="MCP4725"/>
</gates>
<devices>
<device name="" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MCP73831" prefix="IC">
<gates>
<gate name="G$1" symbol="MCP73831"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="BAT" pad="3"/>
<connect gate="G$1" pin="PROG" pad="5"/>
<connect gate="G$1" pin="STAT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MEM_23A**" prefix="IC">
<gates>
<gate name="G$1" symbol="23AXX"/>
</gates>
<devices>
<device name="SO8" package="SO-8">
<connects>
<connect gate="G$1" pin="+" pad="8"/>
<connect gate="G$1" pin="/CS" pad="1"/>
<connect gate="G$1" pin="/HOLD" pad="7"/>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="DO" pad="2"/>
<connect gate="G$1" pin="G" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MEM_23K256" prefix="IC">
<description>256K SPI Bus Low power Serial SRAM</description>
<gates>
<gate name="G$1" symbol="SRAM"/>
</gates>
<devices>
<device name="" package="SOIC-8">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MEM_24AA*" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="24AA"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="24AA" value="24AA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MEM_93C46" prefix="IC" uservalue="yes">
<description>Serial EEPROM 1K</description>
<gates>
<gate name="G$1" symbol="3WIRE"/>
</gates>
<devices>
<device name="" package="SOIC-8">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DC" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="93C46" value="93C46"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MMA7455L" prefix="IC">
<gates>
<gate name="G$1" symbol="MMA7455L"/>
</gates>
<devices>
<device name="" package="LGA-14">
<connects>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="6"/>
<connect gate="G$1" pin="DVDD_IO" pad="1"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="IADDR0" pad="4"/>
<connect gate="G$1" pin="INT1/DRDY" pad="8"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="10"/>
<connect gate="G$1" pin="NC3" pad="11"/>
<connect gate="G$1" pin="SCL/SPC" pad="14"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="13"/>
<connect gate="G$1" pin="SDO" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_OP-AMP_LM358" prefix="IC">
<description>Dual op-amp</description>
<gates>
<gate name="A" symbol="OPAMP_V+-"/>
<gate name="B" symbol="OPAMP"/>
</gates>
<devices>
<device name="-SO8" package="SO-8">
<connects>
<connect gate="A" pin="+" pad="3"/>
<connect gate="A" pin="-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+" pad="5"/>
<connect gate="B" pin="-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_OP-AMP_LMV321" prefix="IC">
<description>Low voltage op-amp (2.7 - 5.0V)</description>
<gates>
<gate name="OPAMP" symbol="OPAMP_V+GND"/>
</gates>
<devices>
<device name="-SOT-23-5" package="SOT-23-5">
<connects>
<connect gate="OPAMP" pin="+" pad="1"/>
<connect gate="OPAMP" pin="-" pad="3"/>
<connect gate="OPAMP" pin="GND" pad="2"/>
<connect gate="OPAMP" pin="OUT" pad="4"/>
<connect gate="OPAMP" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_OPA2830" prefix="IC">
<gates>
<gate name="G$1" symbol="OPA2830"/>
</gates>
<devices>
<device name="" package="DGK_S_PDSO_G8">
<connects>
<connect gate="G$1" pin="INPUT1+" pad="3"/>
<connect gate="G$1" pin="INPUT1-" pad="2"/>
<connect gate="G$1" pin="INPUT2+" pad="5"/>
<connect gate="G$1" pin="INPUT2-" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="VS+" pad="8"/>
<connect gate="G$1" pin="VS-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_PCF8563" prefix="IC">
<gates>
<gate name="G$1" symbol="PCF8563"/>
</gates>
<devices>
<device name="" package="SO-8">
<connects>
<connect gate="G$1" pin="!INT" pad="3"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_RTC_DS1307" prefix="IC">
<gates>
<gate name="G$1" symbol="DS1307"/>
</gates>
<devices>
<device name="" package="SO-8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SQW/OUT" pad="7"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_SI4707" prefix="IC">
<gates>
<gate name="G$1" symbol="SI4707"/>
</gates>
<devices>
<device name="" package="QFN-20">
<connects>
<connect gate="G$1" pin="!RST" pad="5"/>
<connect gate="G$1" pin="!SEN" pad="6"/>
<connect gate="G$1" pin="FMI" pad="2"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="GPO1" pad="19"/>
<connect gate="G$1" pin="GPO2/!INT" pad="18"/>
<connect gate="G$1" pin="GPO3" pad="17"/>
<connect gate="G$1" pin="LOUT" pad="14"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="20"/>
<connect gate="G$1" pin="NP1" pad="4"/>
<connect gate="G$1" pin="NP2" pad="15"/>
<connect gate="G$1" pin="NP3" pad="16"/>
<connect gate="G$1" pin="PAD" pad="0"/>
<connect gate="G$1" pin="RCLK" pad="9"/>
<connect gate="G$1" pin="RFGND" pad="3"/>
<connect gate="G$1" pin="ROUT" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="SDIO" pad="8"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VIO" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_TC74" prefix="IC">
<gates>
<gate name="G$1" symbol="TC74"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_TMP006" prefix="IC">
<gates>
<gate name="G$1" symbol="TMP006"/>
</gates>
<devices>
<device name="" package="DSBGA-8">
<connects>
<connect gate="G$1" pin="!DRDY" pad="C2"/>
<connect gate="G$1" pin="ADR0" pad="C1"/>
<connect gate="G$1" pin="ADR1" pad="B1"/>
<connect gate="G$1" pin="AGND" pad="A2"/>
<connect gate="G$1" pin="DGND" pad="A1"/>
<connect gate="G$1" pin="SCL" pad="B3"/>
<connect gate="G$1" pin="SDA" pad="C3"/>
<connect gate="G$1" pin="V+" pad="A3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_TPIC6B595" prefix="IC">
<gates>
<gate name="G$1" symbol="TPIC6B595"/>
</gates>
<devices>
<device name="DW" package="SOIC-20">
<connects>
<connect gate="G$1" pin="!G" pad="9"/>
<connect gate="G$1" pin="!SCLR" pad="8"/>
<connect gate="G$1" pin="DRAIN0" pad="4"/>
<connect gate="G$1" pin="DRAIN1" pad="5"/>
<connect gate="G$1" pin="DRAIN2" pad="6"/>
<connect gate="G$1" pin="DRAIN3" pad="7"/>
<connect gate="G$1" pin="DRAIN4" pad="14"/>
<connect gate="G$1" pin="DRAIN5" pad="15"/>
<connect gate="G$1" pin="DRAIN6" pad="16"/>
<connect gate="G$1" pin="DRAIN7" pad="17"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="GND1" pad="11"/>
<connect gate="G$1" pin="GND2" pad="19"/>
<connect gate="G$1" pin="RCK" pad="12"/>
<connect gate="G$1" pin="SERIN" pad="3"/>
<connect gate="G$1" pin="SEROUT" pad="18"/>
<connect gate="G$1" pin="SRCK" pad="13"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_TPS2041B" prefix="IC">
<description>High side power distribution switch</description>
<gates>
<gate name="G$1" symbol="TPS2041B"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="!EN" pad="4"/>
<connect gate="G$1" pin="!OC" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_TXB0108" prefix="IC">
<description>&lt;b&gt;8-Bit bidirectional voltage level translator&lt;/b&gt;
&lt;br&gt; Mfr no: TXB0108PWR
&lt;br&gt;&lt;a href="http://www.digikey.com/product-detail/en/TXB0108PWR/296-21527-2-ND/1305699"&gt; TXB0108PWR &lt;/a&gt;</description>
<gates>
<gate name="IC" symbol="TXB0108"/>
</gates>
<devices>
<device name="PW" package="SSOP-20">
<connects>
<connect gate="IC" pin="A1" pad="1"/>
<connect gate="IC" pin="A2" pad="3"/>
<connect gate="IC" pin="A3" pad="4"/>
<connect gate="IC" pin="A4" pad="5"/>
<connect gate="IC" pin="A5" pad="6"/>
<connect gate="IC" pin="A6" pad="7"/>
<connect gate="IC" pin="A7" pad="8"/>
<connect gate="IC" pin="A8" pad="9"/>
<connect gate="IC" pin="B1" pad="20"/>
<connect gate="IC" pin="B2" pad="18"/>
<connect gate="IC" pin="B3" pad="17"/>
<connect gate="IC" pin="B4" pad="16"/>
<connect gate="IC" pin="B5" pad="15"/>
<connect gate="IC" pin="B6" pad="14"/>
<connect gate="IC" pin="B7" pad="13"/>
<connect gate="IC" pin="B8" pad="12"/>
<connect gate="IC" pin="GND" pad="11"/>
<connect gate="IC" pin="OE" pad="10"/>
<connect gate="IC" pin="VA" pad="2"/>
<connect gate="IC" pin="VB" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TSSOP-20" package="TSSOP-20">
<connects>
<connect gate="IC" pin="A1" pad="1"/>
<connect gate="IC" pin="A2" pad="3"/>
<connect gate="IC" pin="A3" pad="4"/>
<connect gate="IC" pin="A4" pad="5"/>
<connect gate="IC" pin="A5" pad="6"/>
<connect gate="IC" pin="A6" pad="7"/>
<connect gate="IC" pin="A7" pad="8"/>
<connect gate="IC" pin="A8" pad="9"/>
<connect gate="IC" pin="B1" pad="20"/>
<connect gate="IC" pin="B2" pad="18"/>
<connect gate="IC" pin="B3" pad="17"/>
<connect gate="IC" pin="B4" pad="16"/>
<connect gate="IC" pin="B5" pad="15"/>
<connect gate="IC" pin="B6" pad="14"/>
<connect gate="IC" pin="B7" pad="13"/>
<connect gate="IC" pin="B8" pad="12"/>
<connect gate="IC" pin="GND" pad="11"/>
<connect gate="IC" pin="OE" pad="10"/>
<connect gate="IC" pin="VA" pad="2"/>
<connect gate="IC" pin="VB" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_ATMEGA328P" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="ATMEGA328P"/>
</gates>
<devices>
<device name="DIL" package="DIL28-N">
<connects>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND2" pad="22"/>
<connect gate="G$1" pin="PB0/PCINT0/CLKO/ICP1" pad="14"/>
<connect gate="G$1" pin="PB1/OC1A/PCINT1" pad="15"/>
<connect gate="G$1" pin="PB2/SS/OCIB/PCINT2" pad="16"/>
<connect gate="G$1" pin="PB3/MOSI/OC2A/PCINT3" pad="17"/>
<connect gate="G$1" pin="PB4/MISO/PCINT4" pad="18"/>
<connect gate="G$1" pin="PB5/SCK/PCINT5" pad="19"/>
<connect gate="G$1" pin="PB6/PCINT6/XTAL1/TOSC1" pad="9"/>
<connect gate="G$1" pin="PB7/PCINT7/XTAL2/TOSC2" pad="10"/>
<connect gate="G$1" pin="PC0/ADC0/PCINT8" pad="23"/>
<connect gate="G$1" pin="PC1/ADC1/PCINT9" pad="24"/>
<connect gate="G$1" pin="PC2/ADC2/PCINT10" pad="25"/>
<connect gate="G$1" pin="PC3/ADC3/PCINT11" pad="26"/>
<connect gate="G$1" pin="PC4/ADC4/SDA/PCINT12" pad="27"/>
<connect gate="G$1" pin="PC5/ADC5/SCL/PCINT13" pad="28"/>
<connect gate="G$1" pin="PC6/PCINT14/RESET" pad="1"/>
<connect gate="G$1" pin="PD0/PCINT16/RXD" pad="2"/>
<connect gate="G$1" pin="PD1/PCINT17/TXD" pad="3"/>
<connect gate="G$1" pin="PD2/PCINT18/INT0" pad="4"/>
<connect gate="G$1" pin="PD3/PCINT19/OC2B/INT1" pad="5"/>
<connect gate="G$1" pin="PD4/PCINT20/XCK/T0" pad="6"/>
<connect gate="G$1" pin="PD5/PCINT21/OCOB/T1" pad="11"/>
<connect gate="G$1" pin="PD6/PCINT22/OC0A/AIN0" pad="12"/>
<connect gate="G$1" pin="PD7/PCINT23/AIN1" pad="13"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_LPC1343" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="LPC1343"/>
</gates>
<devices>
<device name="-LQFP48" package="LQFP48">
<connects>
<connect gate="G$1" pin="PIO0_1/USB_FTOGGLE" pad="4"/>
<connect gate="G$1" pin="PIO0_10" pad="29"/>
<connect gate="G$1" pin="PIO0_11" pad="32"/>
<connect gate="G$1" pin="PIO0_2" pad="10"/>
<connect gate="G$1" pin="PIO0_3/USB_VBUS" pad="14"/>
<connect gate="G$1" pin="PIO0_4" pad="15"/>
<connect gate="G$1" pin="PIO0_5" pad="16"/>
<connect gate="G$1" pin="PIO0_6/USB_CONNECT" pad="22"/>
<connect gate="G$1" pin="PIO0_7" pad="23"/>
<connect gate="G$1" pin="PIO0_8" pad="27"/>
<connect gate="G$1" pin="PIO0_9" pad="28"/>
<connect gate="G$1" pin="PIO1_0" pad="33"/>
<connect gate="G$1" pin="PIO1_1" pad="34"/>
<connect gate="G$1" pin="PIO1_10" pad="30"/>
<connect gate="G$1" pin="PIO1_11" pad="42"/>
<connect gate="G$1" pin="PIO1_2" pad="35"/>
<connect gate="G$1" pin="PIO1_3" pad="39"/>
<connect gate="G$1" pin="PIO1_4" pad="40"/>
<connect gate="G$1" pin="PIO1_5" pad="45"/>
<connect gate="G$1" pin="PIO1_6" pad="46"/>
<connect gate="G$1" pin="PIO1_7" pad="47"/>
<connect gate="G$1" pin="PIO1_8" pad="9"/>
<connect gate="G$1" pin="PIO1_9" pad="17"/>
<connect gate="G$1" pin="PIO2_0" pad="2"/>
<connect gate="G$1" pin="PIO2_1" pad="13"/>
<connect gate="G$1" pin="PIO2_10" pad="25"/>
<connect gate="G$1" pin="PIO2_11" pad="31"/>
<connect gate="G$1" pin="PIO2_2" pad="26"/>
<connect gate="G$1" pin="PIO2_3" pad="38"/>
<connect gate="G$1" pin="PIO2_4" pad="18"/>
<connect gate="G$1" pin="PIO2_5" pad="21"/>
<connect gate="G$1" pin="PIO2_6" pad="1"/>
<connect gate="G$1" pin="PIO2_7" pad="11"/>
<connect gate="G$1" pin="PIO2_8" pad="12"/>
<connect gate="G$1" pin="PIO2_9" pad="24"/>
<connect gate="G$1" pin="PIO3_0" pad="36"/>
<connect gate="G$1" pin="PIO3_1" pad="37"/>
<connect gate="G$1" pin="PIO3_2" pad="43"/>
<connect gate="G$1" pin="PIO3_3" pad="48"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="3"/>
<connect gate="G$1" pin="USB_DM" pad="19"/>
<connect gate="G$1" pin="USB_DP" pad="20"/>
<connect gate="G$1" pin="VDD" pad="44"/>
<connect gate="G$1" pin="VDD." pad="8"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="VSS." pad="5"/>
<connect gate="G$1" pin="XTALIN" pad="6"/>
<connect gate="G$1" pin="XTALOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_MSP430F2132" prefix="IC">
<description>16-bit Ultra-Low-Power Microcontroller, 8kB Flash, 512B RAM, 10 bit ADC, 1 USCI</description>
<gates>
<gate name="G$1" symbol="MSP430F21X2"/>
</gates>
<devices>
<device name="" package="TSSOP-28">
<connects>
<connect gate="G$1" pin="!RST!/NMI/SBWTDIO" pad="7"/>
<connect gate="G$1" pin="A6/TA1.0/P3.6" pad="17"/>
<connect gate="G$1" pin="A7/TA1.1/P3.7" pad="18"/>
<connect gate="G$1" pin="CA0/VEREF-/VREF-/A3/TA0.1/P2.3" pad="19"/>
<connect gate="G$1" pin="CA1/VEREF+/VREF+/A4/TA0.2/P2.4" pad="20"/>
<connect gate="G$1" pin="CAOUT/ADC10CLK/TACLK/P1.0" pad="21"/>
<connect gate="G$1" pin="DVCC" pad="2"/>
<connect gate="G$1" pin="DVSS" pad="4"/>
<connect gate="G$1" pin="P2.0/ACLK/A0/CA2" pad="8"/>
<connect gate="G$1" pin="P2.1/TAINCLK/SMCLK/A1/CA3" pad="9"/>
<connect gate="G$1" pin="P2.2/TA0.0/A2/CA4/CAOUT" pad="10"/>
<connect gate="G$1" pin="P2.5/ROSC/CA5" pad="3"/>
<connect gate="G$1" pin="P3.0/UCB0STE/UCA0CLK/A5" pad="11"/>
<connect gate="G$1" pin="P3.1/UCB0SIMO/UCB0SDA" pad="12"/>
<connect gate="G$1" pin="P3.2/UCB0SOMI/UCB0SCL" pad="13"/>
<connect gate="G$1" pin="P3.3/UCB0CLK/UCA0STE" pad="14"/>
<connect gate="G$1" pin="TA0.1/P1.2" pad="23"/>
<connect gate="G$1" pin="TA0.2/P1.3" pad="24"/>
<connect gate="G$1" pin="TA1.0/TA0.0/P1.1" pad="22"/>
<connect gate="G$1" pin="TCK/SMCLK/P1.4" pad="25"/>
<connect gate="G$1" pin="TCLK/TDI/TA0.1/P1.6" pad="27"/>
<connect gate="G$1" pin="TDI/TDO/TA0.2/P1.7" pad="28"/>
<connect gate="G$1" pin="TEST/SBWTCK" pad="1"/>
<connect gate="G$1" pin="TMS/TA0.0/P1.5" pad="26"/>
<connect gate="G$1" pin="UCA0SIMO/UCA0TXD/P3.4" pad="15"/>
<connect gate="G$1" pin="UCA0SOMI/UCA0RXD/P3.5" pad="16"/>
<connect gate="G$1" pin="XIN/P2.6/CA6" pad="6"/>
<connect gate="G$1" pin="XOUT/P2.7/CA7" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_MSP430G2231" prefix="IC">
<description>Ultra Low Power Mixed signal microcontroller</description>
<gates>
<gate name="G$1" symbol="MSP430G2XX1"/>
</gates>
<devices>
<device name="" package="DIP14">
<connects>
<connect gate="G$1" pin="DVCC" pad="1"/>
<connect gate="G$1" pin="DVSS" pad="14"/>
<connect gate="G$1" pin="P1.0/TA0CLK/ACLK/A0" pad="2"/>
<connect gate="G$1" pin="P1.1/TA0.0/A1" pad="3"/>
<connect gate="G$1" pin="P1.2/TA0.1/A2" pad="4"/>
<connect gate="G$1" pin="P1.3/ADC10CLK/A3/VREF-/VEREF-" pad="5"/>
<connect gate="G$1" pin="P1.4/SMCLK/A4/VREF+/VEREF+/TCK" pad="6"/>
<connect gate="G$1" pin="P1.5/TA0.0/A5/SCLK/TMS" pad="7"/>
<connect gate="G$1" pin="SBWTCK/TEST" pad="11"/>
<connect gate="G$1" pin="SBWTDIO/NMI/!RST" pad="10"/>
<connect gate="G$1" pin="TA0.1/XIN/P2.6" pad="13"/>
<connect gate="G$1" pin="TCLK/TDI/SCL/SDO/A6/TA0.1/P1.6" pad="8"/>
<connect gate="G$1" pin="TDI/TDO/SDA/SDI/A7/P1.7" pad="9"/>
<connect gate="G$1" pin="XOUT/P2.7" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC10F22*" prefix="IC">
<gates>
<gate name="G$1" symbol="PIC10F22X"/>
</gates>
<devices>
<device name="" package="SOT-23-6">
<connects>
<connect gate="G$1" pin="GP0" pad="1"/>
<connect gate="G$1" pin="GP1" pad="3"/>
<connect gate="G$1" pin="GP2" pad="4"/>
<connect gate="G$1" pin="GP3" pad="6"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC12F1822" prefix="IC">
<gates>
<gate name="G$1" symbol="PIC12F1822"/>
</gates>
<devices>
<device name="DFN6_3X3" package="DFN6_3X3">
<connects>
<connect gate="G$1" pin="RA0" pad="7"/>
<connect gate="G$1" pin="RA1" pad="6"/>
<connect gate="G$1" pin="RA2" pad="5"/>
<connect gate="G$1" pin="RA3" pad="4"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RA5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP8" package="DIP8">
<connects>
<connect gate="G$1" pin="RA0" pad="7"/>
<connect gate="G$1" pin="RA1" pad="6"/>
<connect gate="G$1" pin="RA2" pad="5"/>
<connect gate="G$1" pin="RA3" pad="4"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RA5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC12F508" prefix="IC">
<gates>
<gate name="G$1" symbol="PIC12F508"/>
</gates>
<devices>
<device name="DIP" package="DIP8">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3" pad="4"/>
<connect gate="G$1" pin="GP4" pad="3"/>
<connect gate="G$1" pin="GP5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MSOP" package="MSOP8">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3" pad="4"/>
<connect gate="G$1" pin="GP4" pad="3"/>
<connect gate="G$1" pin="GP5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SO-8">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3" pad="4"/>
<connect gate="G$1" pin="GP4" pad="3"/>
<connect gate="G$1" pin="GP5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DFN" package="DFN8_3X2">
<connects>
<connect gate="G$1" pin="GP0" pad="7"/>
<connect gate="G$1" pin="GP1" pad="6"/>
<connect gate="G$1" pin="GP2" pad="5"/>
<connect gate="G$1" pin="GP3" pad="4"/>
<connect gate="G$1" pin="GP4" pad="3"/>
<connect gate="G$1" pin="GP5" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC16F1823" prefix="IC">
<gates>
<gate name="IC" symbol="PIC16F1823"/>
</gates>
<devices>
<device name="-DIL14" package="DIP14">
<connects>
<connect gate="IC" pin="RA0" pad="13"/>
<connect gate="IC" pin="RA1" pad="12"/>
<connect gate="IC" pin="RA2" pad="11"/>
<connect gate="IC" pin="RA3" pad="4"/>
<connect gate="IC" pin="RA4" pad="3"/>
<connect gate="IC" pin="RA5" pad="2"/>
<connect gate="IC" pin="RC0" pad="10"/>
<connect gate="IC" pin="RC1" pad="9"/>
<connect gate="IC" pin="RC2" pad="8"/>
<connect gate="IC" pin="RC3" pad="7"/>
<connect gate="IC" pin="RC4" pad="6"/>
<connect gate="IC" pin="RC5" pad="5"/>
<connect gate="IC" pin="VDD" pad="1"/>
<connect gate="IC" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="PTH"/>
</technologies>
</device>
<device name="-QFN16_4X4" package="QFN16_4X4">
<connects>
<connect gate="IC" pin="RA0" pad="12"/>
<connect gate="IC" pin="RA1" pad="11"/>
<connect gate="IC" pin="RA2" pad="10"/>
<connect gate="IC" pin="RA3" pad="3"/>
<connect gate="IC" pin="RA4" pad="2"/>
<connect gate="IC" pin="RA5" pad="1"/>
<connect gate="IC" pin="RC0" pad="9"/>
<connect gate="IC" pin="RC1" pad="8"/>
<connect gate="IC" pin="RC2" pad="7"/>
<connect gate="IC" pin="RC3" pad="6"/>
<connect gate="IC" pin="RC4" pad="5"/>
<connect gate="IC" pin="RC5" pad="4"/>
<connect gate="IC" pin="VDD" pad="16"/>
<connect gate="IC" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOIC14" package="SOIC-14">
<connects>
<connect gate="IC" pin="RA0" pad="13"/>
<connect gate="IC" pin="RA1" pad="12"/>
<connect gate="IC" pin="RA2" pad="11"/>
<connect gate="IC" pin="RA3" pad="4"/>
<connect gate="IC" pin="RA4" pad="3"/>
<connect gate="IC" pin="RA5" pad="2"/>
<connect gate="IC" pin="RC0" pad="10"/>
<connect gate="IC" pin="RC1" pad="9"/>
<connect gate="IC" pin="RC2" pad="8"/>
<connect gate="IC" pin="RC3" pad="7"/>
<connect gate="IC" pin="RC4" pad="6"/>
<connect gate="IC" pin="RC5" pad="5"/>
<connect gate="IC" pin="VDD" pad="1"/>
<connect gate="IC" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC16F1829" prefix="IC">
<gates>
<gate name="G$1" symbol="PIC16(L)F1829"/>
</gates>
<devices>
<device name="-SSOP-20" package="SSOP-20">
<connects>
<connect gate="G$1" pin="RA0/PGD" pad="19"/>
<connect gate="G$1" pin="RA1/PGC" pad="18"/>
<connect gate="G$1" pin="RA2" pad="17"/>
<connect gate="G$1" pin="RA3/!MCLR" pad="4"/>
<connect gate="G$1" pin="RA4" pad="3"/>
<connect gate="G$1" pin="RA5" pad="2"/>
<connect gate="G$1" pin="RB4" pad="13"/>
<connect gate="G$1" pin="RB5" pad="12"/>
<connect gate="G$1" pin="RB6" pad="11"/>
<connect gate="G$1" pin="RB7" pad="10"/>
<connect gate="G$1" pin="RC0" pad="16"/>
<connect gate="G$1" pin="RC1" pad="15"/>
<connect gate="G$1" pin="RC2" pad="14"/>
<connect gate="G$1" pin="RC3" pad="7"/>
<connect gate="G$1" pin="RC4" pad="6"/>
<connect gate="G$1" pin="RC5" pad="5"/>
<connect gate="G$1" pin="RC6" pad="8"/>
<connect gate="G$1" pin="RC7" pad="9"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC18F44J50" prefix="IC">
<description>44-Pin Low Power USB Microcontrollers</description>
<gates>
<gate name="G$1" symbol="PIC18F44J50"/>
</gates>
<devices>
<device name="" package="TQFP-44">
<connects>
<connect gate="G$1" pin="!MCLR!/5V" pad="P18"/>
<connect gate="G$1" pin="CTEDG2/PMA2/VPO/RP6/AN9/RB3" pad="P11"/>
<connect gate="G$1" pin="INT0/RP3/AN12/RB0" pad="P8"/>
<connect gate="G$1" pin="KBI2/PGC/5V/RP9/RB6" pad="P16"/>
<connect gate="G$1" pin="KBI3/PGD/5V/RP10/RB7" pad="P17"/>
<connect gate="G$1" pin="PMA0/KBI1/SDI1/SDA1/5V/RP8/RB5" pad="P15"/>
<connect gate="G$1" pin="PMA1/KBI0/SCK1/SCL1/5V/RP7/RB4" pad="P14"/>
<connect gate="G$1" pin="PMCS/AN7/RE2" pad="P27"/>
<connect gate="G$1" pin="PMD0/SCL2/5V/RD0" pad="P38"/>
<connect gate="G$1" pin="PMD1/SDA2/5V/RD1" pad="P39"/>
<connect gate="G$1" pin="PMD2/5V/RP19/RD2" pad="P40"/>
<connect gate="G$1" pin="PMD3/5V/RP20/RD3" pad="P41"/>
<connect gate="G$1" pin="PMD4/5V/RP21/RD4" pad="P2"/>
<connect gate="G$1" pin="PMD5/5V/RP22/RD5" pad="P3"/>
<connect gate="G$1" pin="PMD6/5V/RP23/RD6" pad="P4"/>
<connect gate="G$1" pin="PMD7/5V/RP24/RD7" pad="P5"/>
<connect gate="G$1" pin="PMRD/AN5/RE0" pad="P25"/>
<connect gate="G$1" pin="PMWR/AN6/RE1" pad="P26"/>
<connect gate="G$1" pin="RA0/AN0/RP0/C1INA/ULPWU/PMA6" pad="P19"/>
<connect gate="G$1" pin="RA1/AN1/RP1/C2INA/PMA7" pad="P20"/>
<connect gate="G$1" pin="RA2/AN2/C2INB/VREF-/CVREF" pad="P21"/>
<connect gate="G$1" pin="RA3/AN3/C1INB/VREF+" pad="P22"/>
<connect gate="G$1" pin="RA5/AN4//RP2/!SS1!/HLVDIN/RCV" pad="P24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="P31"/>
<connect gate="G$1" pin="RA7/OSC1/CLKI" pad="P30"/>
<connect gate="G$1" pin="RC0/RP11/TIOSO/T1CKI" pad="P32"/>
<connect gate="G$1" pin="RC1/RP12/T1OSI/!UOE!" pad="P35"/>
<connect gate="G$1" pin="RC2/AN11/RP13/CTPLS" pad="P36"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="P42"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="P43"/>
<connect gate="G$1" pin="RC6/RP17/5V/PMA5/TX1/CK1" pad="P44"/>
<connect gate="G$1" pin="RC7/RP18/5V/PMA4/RX1/DT1/SDO1" pad="P1"/>
<connect gate="G$1" pin="REFO/VMO/PMA3/CTEDG1/RP5/AN8/RB2" pad="P10"/>
<connect gate="G$1" pin="RTCC/PMBE/RP4/AN10/RB1" pad="P9"/>
<connect gate="G$1" pin="VDD@0" pad="P7"/>
<connect gate="G$1" pin="VDD@1" pad="P28"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="P23"/>
<connect gate="G$1" pin="VSS@0" pad="P6"/>
<connect gate="G$1" pin="VSS@1" pad="P29"/>
<connect gate="G$1" pin="VUSB" pad="P37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC18FJ2*50" prefix="IC">
<gates>
<gate name="G$1" symbol="PIC18FJ2X50"/>
</gates>
<devices>
<device name="-SSOP-28" package="SSOP-28">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3/5V" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="9"/>
<connect gate="G$1" pin="RA0/AN0/RP0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/RP1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA5/AN4/!SS1!/HLVDIN/RP2" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT0/RP3" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/RTCC/RP4" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/VMO/RP5" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/VPO/RP6" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/SCK1/RP7/5V" pad="25"/>
<connect gate="G$1" pin="RB5/KBI1/PGM/SDI1/RP8/5V" pad="26"/>
<connect gate="G$1" pin="RB6/KBI2/PGC/PR9/5V" pad="27"/>
<connect gate="G$1" pin="RB7/BKI3/PGD/RP10/5V" pad="28"/>
<connect gate="G$1" pin="RC0/TIOSO/T1CKI/RP11" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI/!UOE!/RP12" pad="12"/>
<connect gate="G$1" pin="RC2/AN11/RP13" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/TX1/CK1/RP17/5V" pad="17"/>
<connect gate="G$1" pin="RC7/RX1/DT1/SDO1/RP18/5V" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="6"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PIC18FJ2X50" value="PIC18FJ2X50"/>
</technology>
</technologies>
</device>
<device name="-SOIC-28-W" package="SOIC-28W">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3/5V" pad="1"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="9"/>
<connect gate="G$1" pin="RA0/AN0/RP0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/RP1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="4"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="5"/>
<connect gate="G$1" pin="RA5/AN4/!SS1!/HLVDIN/RP2" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="10"/>
<connect gate="G$1" pin="RB0/AN12/INT0/RP3" pad="21"/>
<connect gate="G$1" pin="RB1/AN10/RTCC/RP4" pad="22"/>
<connect gate="G$1" pin="RB2/AN8/VMO/RP5" pad="23"/>
<connect gate="G$1" pin="RB3/AN9/VPO/RP6" pad="24"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/SCK1/RP7/5V" pad="25"/>
<connect gate="G$1" pin="RB5/KBI1/PGM/SDI1/RP8/5V" pad="26"/>
<connect gate="G$1" pin="RB6/KBI2/PGC/PR9/5V" pad="27"/>
<connect gate="G$1" pin="RB7/BKI3/PGD/RP10/5V" pad="28"/>
<connect gate="G$1" pin="RC0/TIOSO/T1CKI/RP11" pad="11"/>
<connect gate="G$1" pin="RC1/T1OSI/!UOE!/RP12" pad="12"/>
<connect gate="G$1" pin="RC2/AN11/RP13" pad="13"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="15"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="16"/>
<connect gate="G$1" pin="RC6/TX1/CK1/RP17/5V" pad="17"/>
<connect gate="G$1" pin="RC7/RX1/DT1/SDO1/RP18/5V" pad="18"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDCORE/VCAP" pad="6"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VUSB" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC24FJ256GB106" prefix="IC">
<description>16-Bit Flash Microcontroller with USB On-The-Go(OTG)</description>
<gates>
<gate name="G$1" symbol="PIC24FJ256GB106"/>
</gates>
<devices>
<device name="" package="TQFP-64-10X10">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="RB0/CN2/PMA6/RP0/VREF+/AN0/PGED1" pad="16"/>
<connect gate="G$1" pin="RB1/CN3/RP1/VREF-/AN1/PGEC1" pad="15"/>
<connect gate="G$1" pin="RB10/CN28/PMA13/AN10/CVREF/TMS" pad="23"/>
<connect gate="G$1" pin="RB11/CN29/PMA12/AN11/TDO" pad="24"/>
<connect gate="G$1" pin="RB12/CN30/CTED2/PMA11/AN12/TCK" pad="27"/>
<connect gate="G$1" pin="RB13/CN31/CTED1/PMA10/AN13/TDI" pad="28"/>
<connect gate="G$1" pin="RB14/CN32/PMA1/RP14/CTPLS/AN14" pad="29"/>
<connect gate="G$1" pin="RB15/CN12/PMA0/REFO/RP29/AN15" pad="30"/>
<connect gate="G$1" pin="RB2/CN4/RP13/VMIO/C2INB/AN2" pad="14"/>
<connect gate="G$1" pin="RB3/CN5/VPIO/C2INA/AN3" pad="13"/>
<connect gate="G$1" pin="RB4/CN6/RP28/USBOEN/C1INB/AN4/PGED3" pad="12"/>
<connect gate="G$1" pin="RB5/CN7/RP18/VBUSON/C1INA/AN5/PGEC3" pad="11"/>
<connect gate="G$1" pin="RB6/CN24/RP6/AN6/PGEC2" pad="17"/>
<connect gate="G$1" pin="RB7/CN25/RCV/RP7/AN7/PGED2" pad="18"/>
<connect gate="G$1" pin="RB8/CN26/RP8/AN8" pad="21"/>
<connect gate="G$1" pin="RB9/CN27/PMA7/RP9/AN9" pad="22"/>
<connect gate="G$1" pin="RC12/CN23/CLKI/OSCI" pad="39"/>
<connect gate="G$1" pin="RC13/CN1/C3IND/SOSCI" pad="47"/>
<connect gate="G$1" pin="RC14/CN0/RPI37/C3INC/T1CK/SOSCO" pad="48"/>
<connect gate="G$1" pin="RC15/CN22/CLKO/OSCO" pad="40"/>
<connect gate="G$1" pin="RD0/CN49/INT0/RP11/DMH" pad="46"/>
<connect gate="G$1" pin="RD1/CN50/RP24/VCPCON" pad="49"/>
<connect gate="G$1" pin="RD10/CN55/PMCS2/RP3/SCL1" pad="44"/>
<connect gate="G$1" pin="RD11/CN56/PMCS1/RP12" pad="45"/>
<connect gate="G$1" pin="RD2/CN51/RP23/DPH" pad="50"/>
<connect gate="G$1" pin="RD3/CN52/PMBE/RP22" pad="51"/>
<connect gate="G$1" pin="RD4/CN13/PMWR/RP25" pad="52"/>
<connect gate="G$1" pin="RD5/CN14/PMRD/RP20" pad="53"/>
<connect gate="G$1" pin="RD6/CN15/C3INB" pad="54"/>
<connect gate="G$1" pin="RD7/CN16/C3INA" pad="55"/>
<connect gate="G$1" pin="RD8/CN53/RP2/DMLN/RTCC" pad="42"/>
<connect gate="G$1" pin="RD9/CN54/RP4/SDA1/DPLN" pad="43"/>
<connect gate="G$1" pin="RE0/CN58/PMD0" pad="60"/>
<connect gate="G$1" pin="RE1/CN59/PMD1" pad="61"/>
<connect gate="G$1" pin="RE2/CN60/PMD2" pad="62"/>
<connect gate="G$1" pin="RE3/CN61/PMD3" pad="63"/>
<connect gate="G$1" pin="RE4/CN62/PMD4" pad="64"/>
<connect gate="G$1" pin="RE5/CN63/PMD5" pad="1"/>
<connect gate="G$1" pin="RE6/CN64/PMD6/SCL3" pad="2"/>
<connect gate="G$1" pin="RE7/CN65/PMD7/SDA3" pad="3"/>
<connect gate="G$1" pin="RF0/CN68/VCMPST1/VBUSST" pad="58"/>
<connect gate="G$1" pin="RF1/CN69/VCMPST2" pad="59"/>
<connect gate="G$1" pin="RF3/CN71/USBID/RP16" pad="33"/>
<connect gate="G$1" pin="RF4/CN17/PMA9/RP10/SDA2" pad="31"/>
<connect gate="G$1" pin="RF5/CN18/PMA8/RP17/SCL2" pad="32"/>
<connect gate="G$1" pin="RG2/D+" pad="37"/>
<connect gate="G$1" pin="RG3/D-" pad="36"/>
<connect gate="G$1" pin="RG6/CN8/PMA5/RP21/C1IND" pad="4"/>
<connect gate="G$1" pin="RG7/CN9/PMA4/RP26/C1INC" pad="5"/>
<connect gate="G$1" pin="RG8/CN10/PMA3/RP19/C2IND" pad="6"/>
<connect gate="G$1" pin="RG9/CN11/C2INC/PMA2/RP27" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="56"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC24FJ256GB110" prefix="IC">
<description>16-bit Flash Microcontroller with USB OTG</description>
<gates>
<gate name="G$1" symbol="PIC24FJ256GB110"/>
</gates>
<devices>
<device name="-TQFP100" package="TQFP-100">
<connects>
<connect gate="G$1" pin="!MCLR" pad="P13"/>
<connect gate="G$1" pin="AVDD" pad="P30"/>
<connect gate="G$1" pin="AVSS" pad="P31"/>
<connect gate="G$1" pin="C1INC/RP26/PMA4/CN9/RG7" pad="P11"/>
<connect gate="G$1" pin="C1IND/RP21/PMA5/CN8/RG6" pad="P10"/>
<connect gate="G$1" pin="C2INC/RP27/PMA2/CN11/RG9" pad="P14"/>
<connect gate="G$1" pin="C2IND/RP19/PMA3/CN10/RG8" pad="P12"/>
<connect gate="G$1" pin="CLKI/OSCI/CN23/RC12" pad="P63"/>
<connect gate="G$1" pin="CLKO/OSCO/CN22/RC15" pad="P64"/>
<connect gate="G$1" pin="CN77/5V/RG0" pad="P90"/>
<connect gate="G$1" pin="CN78/5V/RG1" pad="P89"/>
<connect gate="G$1" pin="CN79/5V/RG12" pad="P96"/>
<connect gate="G$1" pin="CN80/5V/RG13" pad="P97"/>
<connect gate="G$1" pin="CN81/5V/RG14" pad="P95"/>
<connect gate="G$1" pin="CN82/5V/RG15" pad="P1"/>
<connect gate="G$1" pin="D+/RG2" pad="P57"/>
<connect gate="G$1" pin="D-/RG3" pad="P56"/>
<connect gate="G$1" pin="ENVREG" pad="P86"/>
<connect gate="G$1" pin="PMD0/CN58/5V/RE0" pad="P93"/>
<connect gate="G$1" pin="PMD1/CN59/5V/RE1" pad="P94"/>
<connect gate="G$1" pin="PMD2/CN60/5V/RE2" pad="P98"/>
<connect gate="G$1" pin="PMD3/CN61/5V/RE3" pad="P99"/>
<connect gate="G$1" pin="PMD4/CN62/5V/RE4" pad="P100"/>
<connect gate="G$1" pin="PMD5/CN63/5V/RE5" pad="P3"/>
<connect gate="G$1" pin="RA0/5V/CN33/TMS" pad="P17"/>
<connect gate="G$1" pin="RA1/5V/CN34/TCK" pad="P38"/>
<connect gate="G$1" pin="RA10/CN42/PMA6/VREF+" pad="P29"/>
<connect gate="G$1" pin="RA14/5V/CN43/SCL1/RPI36" pad="P66"/>
<connect gate="G$1" pin="RA15/5V/CN44/SDA1/RPI35" pad="P67"/>
<connect gate="G$1" pin="RA2/5V/CN35/SCL2" pad="P58"/>
<connect gate="G$1" pin="RA3/5V/CN36/SDA2" pad="P59"/>
<connect gate="G$1" pin="RA4/5V/CN37/TDI" pad="P60"/>
<connect gate="G$1" pin="RA5/5V/CN38/TDO" pad="P61"/>
<connect gate="G$1" pin="RA6/CN39" pad="P91"/>
<connect gate="G$1" pin="RA7/5V/CN40" pad="P92"/>
<connect gate="G$1" pin="RA9/CN41/PMA7/VREF-" pad="P28"/>
<connect gate="G$1" pin="RB0/AN0/CN2/PGED1/RP0" pad="P25"/>
<connect gate="G$1" pin="RB1/AN1/CN3/RP1/PGEC1" pad="P24"/>
<connect gate="G$1" pin="RB10/AN10/CN28/PMA13/CVREF" pad="P34"/>
<connect gate="G$1" pin="RB11/AN11/CN29/PMA12" pad="P35"/>
<connect gate="G$1" pin="RB12/AN12/CN30/CTED2/PMA11" pad="P41"/>
<connect gate="G$1" pin="RB13/AN13/CN31/CTED1/PMA10" pad="P42"/>
<connect gate="G$1" pin="RB14/AN14/CN32/PMA1/CTPLS/RP14" pad="P43"/>
<connect gate="G$1" pin="RB15/AN15/CN12/PMA0/REFO/RP29" pad="P44"/>
<connect gate="G$1" pin="RB2/AN2/CN4/RP13/C2INB/VMIO" pad="P23"/>
<connect gate="G$1" pin="RB3/AN3/CN5/C2INA/VPIO" pad="P22"/>
<connect gate="G$1" pin="RB4/AN4/CN6/RP28/USBOEN/C1INB/PGED3" pad="P21"/>
<connect gate="G$1" pin="RB5/AN5/CN7/RP18/VBUSON/C1INA/PGEC3" pad="P20"/>
<connect gate="G$1" pin="RB6/AN6/CN24/PGEC2/RP6" pad="P26"/>
<connect gate="G$1" pin="RB7/AN7/CN25/PGED2/RCV/RP7" pad="P27"/>
<connect gate="G$1" pin="RB8/AN8/CN26/RP8" pad="P32"/>
<connect gate="G$1" pin="RB9/AN9/CN27/RP9" pad="P33"/>
<connect gate="G$1" pin="RD0/5V/CN49/INT0/DMH/RP11" pad="P72"/>
<connect gate="G$1" pin="RD1/5V/CN50/VCPCON/RP24" pad="P76"/>
<connect gate="G$1" pin="RD10/5V/CN55/PMCS2/RP3" pad="P70"/>
<connect gate="G$1" pin="RD11/5V/CN56/PMCS1/RP12" pad="P71"/>
<connect gate="G$1" pin="RD12/5V/CN57/RPI42" pad="P79"/>
<connect gate="G$1" pin="RD13/5V/CN19" pad="P80"/>
<connect gate="G$1" pin="RD14/5V/CN20/RPI43" pad="P47"/>
<connect gate="G$1" pin="RD15/5V/CN21/RP5" pad="P48"/>
<connect gate="G$1" pin="RD2/5V/CN51/DPH/RP23" pad="P77"/>
<connect gate="G$1" pin="RD3/5V/CN52/PMBE/RP22" pad="P78"/>
<connect gate="G$1" pin="RD4/5V/CN13/PMWR/RP25" pad="P81"/>
<connect gate="G$1" pin="RD5/5V/CN14/PMRD/RP20" pad="P82"/>
<connect gate="G$1" pin="RD6/CN15/C3INB" pad="P83"/>
<connect gate="G$1" pin="RD7/CN16/C3INA" pad="P84"/>
<connect gate="G$1" pin="RD8/5V/CN53/DMLN/RTCC/RP2" pad="P68"/>
<connect gate="G$1" pin="RD9/5V/CN54/DPLN/RP4" pad="P69"/>
<connect gate="G$1" pin="RP10/PMA9/CN17/5V/RF4" pad="P49"/>
<connect gate="G$1" pin="RP15/CN74/5V/RF8" pad="P53"/>
<connect gate="G$1" pin="RP16/USBID/CN71/5V/RF3" pad="P51"/>
<connect gate="G$1" pin="RP17/PMA8/CN18/5V/RF5" pad="P50"/>
<connect gate="G$1" pin="RP30/CN70/5V/RF2" pad="P52"/>
<connect gate="G$1" pin="RP31/CN76/5V/RF13" pad="P39"/>
<connect gate="G$1" pin="RPI32/CN75/5V/RF12" pad="P40"/>
<connect gate="G$1" pin="RPI33/CN66/5V/RE8" pad="P18"/>
<connect gate="G$1" pin="RPI34/CN67/5V/RE9" pad="P19"/>
<connect gate="G$1" pin="RPI37/SOSCO/C3INC/T1CK/CN0/RC14" pad="P74"/>
<connect gate="G$1" pin="RPI38/CN45/5V/RC1" pad="P6"/>
<connect gate="G$1" pin="RPI39/CN46/5V/RC2" pad="P7"/>
<connect gate="G$1" pin="RPI40/CN47/5V/RC3" pad="P8"/>
<connect gate="G$1" pin="RPI41/CN48/5V/RC4" pad="P9"/>
<connect gate="G$1" pin="SCL3/PMD6/CN64/5V/RE6" pad="P4"/>
<connect gate="G$1" pin="SDA3/PMD7/CN65/5V/RE7" pad="P5"/>
<connect gate="G$1" pin="SOSCI/C3IND/CN1/RC13" pad="P73"/>
<connect gate="G$1" pin="VBUS" pad="P54"/>
<connect gate="G$1" pin="VBUSST/VCMPST1/CN68/RF0" pad="P87"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="P85"/>
<connect gate="G$1" pin="VCMPST2/CN69/5V/RF1" pad="P88"/>
<connect gate="G$1" pin="VDD" pad="P2"/>
<connect gate="G$1" pin="VDD@1" pad="P16"/>
<connect gate="G$1" pin="VDD@2" pad="P37"/>
<connect gate="G$1" pin="VDD@3" pad="P46"/>
<connect gate="G$1" pin="VDD@4" pad="P62"/>
<connect gate="G$1" pin="VSS" pad="P15"/>
<connect gate="G$1" pin="VSS@1" pad="P36"/>
<connect gate="G$1" pin="VSS@2" pad="P45"/>
<connect gate="G$1" pin="VSS@3" pad="P65"/>
<connect gate="G$1" pin="VSS@4" pad="P75"/>
<connect gate="G$1" pin="VUSB" pad="P55"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC24FJ64GA002" prefix="IC">
<description>16-bit General Purpose Flash Microcontroller</description>
<gates>
<gate name="G$1" symbol="PIC24FJ64GA002"/>
</gates>
<devices>
<device name="" package="SSOP-28">
<connects>
<connect gate="G$1" pin="DISVREG" pad="19"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="PMCS1/CN11/RP15/AN9/RB15" pad="26"/>
<connect gate="G$1" pin="PMD0/CN14/RP12/AN12/RB12" pad="23"/>
<connect gate="G$1" pin="PMD1/TMS/EMUC2/PGC2/CN15/RP11/RB11" pad="22"/>
<connect gate="G$1" pin="PMD2/TDI/EMUD2/PGD2/CN16/RP10/RB10" pad="21"/>
<connect gate="G$1" pin="PMD3/SDA1/TDO/CN21/RP9/RB9" pad="18"/>
<connect gate="G$1" pin="PMD4/SCL1/TCK/CN22/RP8/RB8" pad="17"/>
<connect gate="G$1" pin="PMD5/INT0/CN23/RP7/RB7" pad="16"/>
<connect gate="G$1" pin="PMD6/ASCL1/EMUC3/PGC3/CN24/RP6/RB6" pad="15"/>
<connect gate="G$1" pin="PMRD/CN13/RP13/AN11/RB13" pad="24"/>
<connect gate="G$1" pin="PMWR/RTCC/CVREF/CN12/RP14/AN10/RB14" pad="25"/>
<connect gate="G$1" pin="RA0/AN0/CN2/VREF+" pad="2"/>
<connect gate="G$1" pin="RA1/AN1/CN3/VREF-" pad="3"/>
<connect gate="G$1" pin="RA2/CN30/OSCI/CLKI" pad="9"/>
<connect gate="G$1" pin="RA3/CN29/OSCO/CLKO/PMA0" pad="10"/>
<connect gate="G$1" pin="RA4/CN0/SOSCO/T1CK/PMA1" pad="12"/>
<connect gate="G$1" pin="RB0/AN2/RP0/CN4/C2IN-/PGD1/EMUD1" pad="4"/>
<connect gate="G$1" pin="RB1/AN3/RP1/CN5/C2IN+/PGC1/EMUC1" pad="5"/>
<connect gate="G$1" pin="RB2/AN4/RP2/CN6/C1IN-/SDA2" pad="6"/>
<connect gate="G$1" pin="RB3/AN5/RP3/CN7/C1IN+/SCL2" pad="7"/>
<connect gate="G$1" pin="RB4/RP4/CN1/SOSCI/PMBE" pad="11"/>
<connect gate="G$1" pin="RB5/RP5/CN27/PGD3/EMUD3/ASDA1/PMD7" pad="14"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC24FJ64GB002" prefix="IC">
<gates>
<gate name="G$1" symbol="PIC24FJ64GB002"/>
</gates>
<devices>
<device name="SP" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="DISVREG" pad="19"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="9"/>
<connect gate="G$1" pin="RA3" pad="10"/>
<connect gate="G$1" pin="RA4" pad="12"/>
<connect gate="G$1" pin="RB0" pad="4"/>
<connect gate="G$1" pin="RB1" pad="5"/>
<connect gate="G$1" pin="RB10/D+" pad="21"/>
<connect gate="G$1" pin="RB11/D-" pad="22"/>
<connect gate="G$1" pin="RB13" pad="24"/>
<connect gate="G$1" pin="RB14" pad="25"/>
<connect gate="G$1" pin="RB15" pad="26"/>
<connect gate="G$1" pin="RB2" pad="6"/>
<connect gate="G$1" pin="RB3" pad="7"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="14"/>
<connect gate="G$1" pin="RB7" pad="16"/>
<connect gate="G$1" pin="RB8" pad="17"/>
<connect gate="G$1" pin="RB9" pad="18"/>
<connect gate="G$1" pin="VBUS" pad="15"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
<connect gate="G$1" pin="VUSB" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SOIC-28W">
<connects>
<connect gate="G$1" pin="!MCLR" pad="1"/>
<connect gate="G$1" pin="DISVREG" pad="19"/>
<connect gate="G$1" pin="RA0" pad="2"/>
<connect gate="G$1" pin="RA1" pad="3"/>
<connect gate="G$1" pin="RA2" pad="9"/>
<connect gate="G$1" pin="RA3" pad="10"/>
<connect gate="G$1" pin="RA4" pad="12"/>
<connect gate="G$1" pin="RB0" pad="4"/>
<connect gate="G$1" pin="RB1" pad="5"/>
<connect gate="G$1" pin="RB10/D+" pad="21"/>
<connect gate="G$1" pin="RB11/D-" pad="22"/>
<connect gate="G$1" pin="RB13" pad="24"/>
<connect gate="G$1" pin="RB14" pad="25"/>
<connect gate="G$1" pin="RB15" pad="26"/>
<connect gate="G$1" pin="RB2" pad="6"/>
<connect gate="G$1" pin="RB3" pad="7"/>
<connect gate="G$1" pin="RB4" pad="11"/>
<connect gate="G$1" pin="RB5" pad="14"/>
<connect gate="G$1" pin="RB7" pad="16"/>
<connect gate="G$1" pin="RB8" pad="17"/>
<connect gate="G$1" pin="RB9" pad="18"/>
<connect gate="G$1" pin="VBUS" pad="15"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD@1" pad="13"/>
<connect gate="G$1" pin="VDD@2" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="27"/>
<connect gate="G$1" pin="VUSB" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC24J***GP106" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="PIC24FJ128GA"/>
</gates>
<devices>
<device name="" package="TQFP-64-10X10">
<connects>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="CLKI/OSC1/CN23/RC12" pad="39"/>
<connect gate="G$1" pin="CLKO/OSC2/CN22/RC15" pad="40"/>
<connect gate="G$1" pin="CN58/RE0" pad="60"/>
<connect gate="G$1" pin="CN59/RE1" pad="61"/>
<connect gate="G$1" pin="CN60/RE2" pad="62"/>
<connect gate="G$1" pin="CN61/RE3" pad="63"/>
<connect gate="G$1" pin="CN62/RE4" pad="64"/>
<connect gate="G$1" pin="CN63/RE5" pad="1"/>
<connect gate="G$1" pin="CN68/RF0" pad="58"/>
<connect gate="G$1" pin="CN69/RF1" pad="59"/>
<connect gate="G$1" pin="MCLR" pad="7"/>
<connect gate="G$1" pin="RB0/AN0/CN2/VR+/PGD1/RP0" pad="16"/>
<connect gate="G$1" pin="RB1/AN1/CN3/VR-/PGC1/RP1" pad="15"/>
<connect gate="G$1" pin="RB10/AN10/CN28/TMS" pad="23"/>
<connect gate="G$1" pin="RB11/AN11/CN29/TDO" pad="24"/>
<connect gate="G$1" pin="RB12/AN12/CN30/TCK" pad="27"/>
<connect gate="G$1" pin="RB13/AN13/CN31/TDI" pad="28"/>
<connect gate="G$1" pin="RB14/AN14/CN32/RP14" pad="29"/>
<connect gate="G$1" pin="RB15/AN15/CN12/RP29" pad="30"/>
<connect gate="G$1" pin="RB2/AN2/CN4/RP13" pad="14"/>
<connect gate="G$1" pin="RB3/AN3/CN5" pad="13"/>
<connect gate="G$1" pin="RB4/AN4/CN6/RP28" pad="12"/>
<connect gate="G$1" pin="RB5/AN5/CN7/RP18" pad="11"/>
<connect gate="G$1" pin="RB6/AN6/CN24/PGC2/RP6" pad="17"/>
<connect gate="G$1" pin="RB7/AN7/CN25/PGD2/RP7" pad="18"/>
<connect gate="G$1" pin="RB8/AN8/CN26/RP8" pad="21"/>
<connect gate="G$1" pin="RB9/AN9/CN27/RP9" pad="22"/>
<connect gate="G$1" pin="RD0/CN49/RP11" pad="46"/>
<connect gate="G$1" pin="RD1/CN50/RP24" pad="49"/>
<connect gate="G$1" pin="RD10/CN55/RP3" pad="44"/>
<connect gate="G$1" pin="RD11/CN56/RP12" pad="45"/>
<connect gate="G$1" pin="RD2/CN51/RP23" pad="50"/>
<connect gate="G$1" pin="RD3/CN52/RP22" pad="51"/>
<connect gate="G$1" pin="RD4/CN13/RP25" pad="52"/>
<connect gate="G$1" pin="RD5/CN14/RP20" pad="53"/>
<connect gate="G$1" pin="RD6/CN15" pad="54"/>
<connect gate="G$1" pin="RD7/CN16" pad="55"/>
<connect gate="G$1" pin="RD8/CN53/RP2" pad="42"/>
<connect gate="G$1" pin="RD9/CN54/RP4" pad="43"/>
<connect gate="G$1" pin="RP10/SDA2/CN17/RF4" pad="31"/>
<connect gate="G$1" pin="RP16/CN71/RF3" pad="33"/>
<connect gate="G$1" pin="RP17/SCL2/CN18/RF5" pad="32"/>
<connect gate="G$1" pin="RP19/CN10/RG8" pad="6"/>
<connect gate="G$1" pin="RP21/CN8/RG6" pad="4"/>
<connect gate="G$1" pin="RP26/CN9/RG7" pad="5"/>
<connect gate="G$1" pin="RP27/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="RP30/CN70/RF2" pad="34"/>
<connect gate="G$1" pin="RPI45/CN72/RF6" pad="35"/>
<connect gate="G$1" pin="SCL1/CN83/RG2" pad="37"/>
<connect gate="G$1" pin="SCL3/CN64/RE6" pad="2"/>
<connect gate="G$1" pin="SDA1/CN84/RG3" pad="36"/>
<connect gate="G$1" pin="SDA3/CN65/RE7" pad="3"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="VCEN" pad="57"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDD@1" pad="26"/>
<connect gate="G$1" pin="VDD@2" pad="38"/>
<connect gate="G$1" pin="VDDC" pad="56"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="VSS@1" pad="25"/>
<connect gate="G$1" pin="VSS@2" pad="41"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_STM32" prefix="IC" uservalue="yes">
<description>STM32F102C6</description>
<gates>
<gate name="G$1" symbol="STM32-48"/>
</gates>
<devices>
<device name="" package="LQFP48">
<connects>
<connect gate="G$1" pin="BOOT0" pad="44"/>
<connect gate="G$1" pin="NRST" pad="7"/>
<connect gate="G$1" pin="PA0-WKUP" pad="10"/>
<connect gate="G$1" pin="PA1" pad="11"/>
<connect gate="G$1" pin="PA10.USART1_RX" pad="31"/>
<connect gate="G$1" pin="PA11/USART1_CTS/USBDM" pad="32"/>
<connect gate="G$1" pin="PA12/USART1_RTS/USBDP" pad="33"/>
<connect gate="G$1" pin="PA13/JTMS-SWDIO" pad="34"/>
<connect gate="G$1" pin="PA14/JTCK/SWCLK" pad="37"/>
<connect gate="G$1" pin="PA15/JTDI" pad="38"/>
<connect gate="G$1" pin="PA2" pad="12"/>
<connect gate="G$1" pin="PA3" pad="13"/>
<connect gate="G$1" pin="PA4" pad="14"/>
<connect gate="G$1" pin="PA5" pad="15"/>
<connect gate="G$1" pin="PA6" pad="16"/>
<connect gate="G$1" pin="PA7" pad="17"/>
<connect gate="G$1" pin="PA8/USART1_CK/MCO" pad="29"/>
<connect gate="G$1" pin="PA9/USART1_TX" pad="30"/>
<connect gate="G$1" pin="PB0" pad="18"/>
<connect gate="G$1" pin="PB1" pad="19"/>
<connect gate="G$1" pin="PB10" pad="21"/>
<connect gate="G$1" pin="PB11" pad="22"/>
<connect gate="G$1" pin="PB12" pad="25"/>
<connect gate="G$1" pin="PB13" pad="26"/>
<connect gate="G$1" pin="PB14" pad="27"/>
<connect gate="G$1" pin="PB15" pad="28"/>
<connect gate="G$1" pin="PB2" pad="20"/>
<connect gate="G$1" pin="PB3/JTDO" pad="39"/>
<connect gate="G$1" pin="PB4/JNTRST" pad="40"/>
<connect gate="G$1" pin="PB5/I2C_SMBA" pad="41"/>
<connect gate="G$1" pin="PB6/I2C_SCL" pad="42"/>
<connect gate="G$1" pin="PB7/I2C_SDA" pad="43"/>
<connect gate="G$1" pin="PB8" pad="45"/>
<connect gate="G$1" pin="PB9" pad="46"/>
<connect gate="G$1" pin="PC13-TAMPER-RTC" pad="2"/>
<connect gate="G$1" pin="PC14-0SC32_IN" pad="3"/>
<connect gate="G$1" pin="PC15-OSC32_OUT" pad="4"/>
<connect gate="G$1" pin="PD0-OSC_IN" pad="5"/>
<connect gate="G$1" pin="PD1-OSC_OUT" pad="6"/>
<connect gate="G$1" pin="VBAT" pad="1"/>
<connect gate="G$1" pin="VDDA" pad="9"/>
<connect gate="G$1" pin="VDD_1" pad="24"/>
<connect gate="G$1" pin="VDD_2" pad="36"/>
<connect gate="G$1" pin="VDD_3" pad="48"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="VSS_1" pad="23"/>
<connect gate="G$1" pin="VSS_2" pad="35"/>
<connect gate="G$1" pin="VSS_3" pad="47"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_STM32F103RBTXX" prefix="IC">
<description>32-bit ARM-based MCU with 64 or 128KB Flash</description>
<gates>
<gate name="G$1" symbol="STM32F103RX"/>
</gates>
<devices>
<device name="-LQFP64" package="LQFP64">
<connects>
<connect gate="G$1" pin="5V/PC10" pad="51"/>
<connect gate="G$1" pin="5V/PC11" pad="52"/>
<connect gate="G$1" pin="5V/PC12" pad="53"/>
<connect gate="G$1" pin="5V/PC6" pad="37"/>
<connect gate="G$1" pin="5V/PC7" pad="38"/>
<connect gate="G$1" pin="5V/PC8" pad="39"/>
<connect gate="G$1" pin="5V/PC9" pad="40"/>
<connect gate="G$1" pin="ADC10/PC0" pad="8"/>
<connect gate="G$1" pin="ADC11/PC1" pad="9"/>
<connect gate="G$1" pin="ADC12/PC2" pad="10"/>
<connect gate="G$1" pin="ADC13/PC3" pad="11"/>
<connect gate="G$1" pin="ADC14/PC4" pad="24"/>
<connect gate="G$1" pin="ADC15/PC5" pad="25"/>
<connect gate="G$1" pin="BOOT0" pad="60"/>
<connect gate="G$1" pin="BOOT1/5V/PB2" pad="28"/>
<connect gate="G$1" pin="I2C1_SCL/TIM4_CH1/5V/PB6" pad="58"/>
<connect gate="G$1" pin="I2C1_SDA/TIM4_CH2/5V/PB7" pad="59"/>
<connect gate="G$1" pin="I2C1_SMBAI/PB5" pad="57"/>
<connect gate="G$1" pin="I2C2_SCL/USART3_TX/5V/PB10" pad="29"/>
<connect gate="G$1" pin="I2C2_SDA/USART3_RX/5V/PB11" pad="30"/>
<connect gate="G$1" pin="JNTRST/5V/PB4" pad="56"/>
<connect gate="G$1" pin="JTDO/5V/PB3" pad="55"/>
<connect gate="G$1" pin="NRST" pad="7"/>
<connect gate="G$1" pin="OSC32_IN/PC14" pad="3"/>
<connect gate="G$1" pin="OSC32_OUT/PC15" pad="4"/>
<connect gate="G$1" pin="PA0/ADC0/USART2_CTS/TIM2_CH1_ETR/WKUP" pad="14"/>
<connect gate="G$1" pin="PA1/ADC1/USART2_RTS/TIM2_CH2" pad="15"/>
<connect gate="G$1" pin="PA10/5V/USART1_RX/TIM1_CH3" pad="43"/>
<connect gate="G$1" pin="PA11/5V/USART1_CTS/TIM1_CH4/CAN_RX/USB_D-" pad="44"/>
<connect gate="G$1" pin="PA12/5V/USART1_RTS/TIM1_ETR/CAN_TX/USB_D+" pad="45"/>
<connect gate="G$1" pin="PA13/5V/JTMS/SWDIO" pad="46"/>
<connect gate="G$1" pin="PA14/5V/JTCK/SWCLK" pad="49"/>
<connect gate="G$1" pin="PA15/5V/JTDI" pad="50"/>
<connect gate="G$1" pin="PA2/ADC2/USART2_TX/TIM2_CH4" pad="16"/>
<connect gate="G$1" pin="PA3/ADC3/USART2_RX/TIM2_CH4" pad="17"/>
<connect gate="G$1" pin="PA4/ADC4/USART2_CK/SPI1_NSS" pad="20"/>
<connect gate="G$1" pin="PA5/ADC5/SPI1_SCK" pad="21"/>
<connect gate="G$1" pin="PA6/ADC6/SPI1_MISO/TIM3_CH1" pad="22"/>
<connect gate="G$1" pin="PA7/ADC7/SPI1_MOSI/TIM3_CH2" pad="23"/>
<connect gate="G$1" pin="PA8/5V/USART1_CK/TIM1_CH1/MCO" pad="41"/>
<connect gate="G$1" pin="PA9/5V/USART1_TX/TIM1_CH2" pad="42"/>
<connect gate="G$1" pin="PD0/5V/OSC_IN" pad="5"/>
<connect gate="G$1" pin="PD1/5V/OSC_OUT" pad="6"/>
<connect gate="G$1" pin="PD2/5V/TIM3_ETR" pad="54"/>
<connect gate="G$1" pin="SPI2_MISO/USART3_RTS/TIM1_CH2N/5V/PB14" pad="35"/>
<connect gate="G$1" pin="SPI2_MOSI/TIM1_CH3N/5V/PB15" pad="36"/>
<connect gate="G$1" pin="SPI2_NSS/I2C2_SMBAI/USART3_CK/TIM1_BKIN/5V/PB12" pad="33"/>
<connect gate="G$1" pin="SPI2_SCK/USART3_CTS/TIM1_CH1N/5V/PB13" pad="34"/>
<connect gate="G$1" pin="TAMPER-RTC/PC13" pad="2"/>
<connect gate="G$1" pin="TIM3_CH3/ADC8/PB0" pad="26"/>
<connect gate="G$1" pin="TIM3_CH4/ADC9/PB1" pad="27"/>
<connect gate="G$1" pin="TIM4_CH3/5V/PB8" pad="61"/>
<connect gate="G$1" pin="TIM4_CH4/5V/PB9" pad="62"/>
<connect gate="G$1" pin="VBAT" pad="1"/>
<connect gate="G$1" pin="VDDA" pad="13"/>
<connect gate="G$1" pin="VDD_1" pad="32"/>
<connect gate="G$1" pin="VDD_2" pad="48"/>
<connect gate="G$1" pin="VDD_3" pad="64"/>
<connect gate="G$1" pin="VDD_4" pad="19"/>
<connect gate="G$1" pin="VSSA" pad="12"/>
<connect gate="G$1" pin="VSS_1" pad="31"/>
<connect gate="G$1" pin="VSS_2" pad="47"/>
<connect gate="G$1" pin="VSS_3" pad="63"/>
<connect gate="G$1" pin="VSS_4" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_ULN2803A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;DRIVER ARRAY&lt;/b&gt;</description>
<gates>
<gate name="IC" symbol="2801A"/>
</gates>
<devices>
<device name="N" package="DIL18">
<connects>
<connect gate="IC" pin="CD+" pad="10"/>
<connect gate="IC" pin="GND" pad="9"/>
<connect gate="IC" pin="I1" pad="1"/>
<connect gate="IC" pin="I2" pad="2"/>
<connect gate="IC" pin="I3" pad="3"/>
<connect gate="IC" pin="I4" pad="4"/>
<connect gate="IC" pin="I5" pad="5"/>
<connect gate="IC" pin="I6" pad="6"/>
<connect gate="IC" pin="I7" pad="7"/>
<connect gate="IC" pin="I8" pad="8"/>
<connect gate="IC" pin="O1" pad="18"/>
<connect gate="IC" pin="O2" pad="17"/>
<connect gate="IC" pin="O3" pad="16"/>
<connect gate="IC" pin="O4" pad="15"/>
<connect gate="IC" pin="O5" pad="14"/>
<connect gate="IC" pin="O6" pad="13"/>
<connect gate="IC" pin="O7" pad="12"/>
<connect gate="IC" pin="O8" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DW" package="SO-18L">
<connects>
<connect gate="IC" pin="CD+" pad="10"/>
<connect gate="IC" pin="GND" pad="9"/>
<connect gate="IC" pin="I1" pad="1"/>
<connect gate="IC" pin="I2" pad="2"/>
<connect gate="IC" pin="I3" pad="3"/>
<connect gate="IC" pin="I4" pad="4"/>
<connect gate="IC" pin="I5" pad="5"/>
<connect gate="IC" pin="I6" pad="6"/>
<connect gate="IC" pin="I7" pad="7"/>
<connect gate="IC" pin="I8" pad="8"/>
<connect gate="IC" pin="O1" pad="18"/>
<connect gate="IC" pin="O2" pad="17"/>
<connect gate="IC" pin="O3" pad="16"/>
<connect gate="IC" pin="O4" pad="15"/>
<connect gate="IC" pin="O5" pad="14"/>
<connect gate="IC" pin="O6" pad="13"/>
<connect gate="IC" pin="O7" pad="12"/>
<connect gate="IC" pin="O8" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO-18" package="SO-18">
<connects>
<connect gate="IC" pin="CD+" pad="10"/>
<connect gate="IC" pin="GND" pad="9"/>
<connect gate="IC" pin="I1" pad="1"/>
<connect gate="IC" pin="I2" pad="2"/>
<connect gate="IC" pin="I3" pad="3"/>
<connect gate="IC" pin="I4" pad="4"/>
<connect gate="IC" pin="I5" pad="5"/>
<connect gate="IC" pin="I6" pad="6"/>
<connect gate="IC" pin="I7" pad="7"/>
<connect gate="IC" pin="I8" pad="8"/>
<connect gate="IC" pin="O1" pad="18"/>
<connect gate="IC" pin="O2" pad="17"/>
<connect gate="IC" pin="O3" pad="16"/>
<connect gate="IC" pin="O4" pad="15"/>
<connect gate="IC" pin="O5" pad="14"/>
<connect gate="IC" pin="O6" pad="13"/>
<connect gate="IC" pin="O7" pad="12"/>
<connect gate="IC" pin="O8" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_USB2514" prefix="IC">
<gates>
<gate name="G$1" symbol="USB2514"/>
</gates>
<devices>
<device name="" package="QFN36_6X6">
<connects>
<connect gate="G$1" pin="!RESET" pad="26"/>
<connect gate="G$1" pin="HS_IND/CFG_SEL1" pad="25"/>
<connect gate="G$1" pin="OCS1" pad="13"/>
<connect gate="G$1" pin="OCS2" pad="17"/>
<connect gate="G$1" pin="OCS3" pad="19"/>
<connect gate="G$1" pin="OCS4" pad="21"/>
<connect gate="G$1" pin="PRTPWR1" pad="12"/>
<connect gate="G$1" pin="PRTPWR2" pad="16"/>
<connect gate="G$1" pin="PRTPWR3" pad="18"/>
<connect gate="G$1" pin="PRTPWR4" pad="20"/>
<connect gate="G$1" pin="RBIAS" pad="35"/>
<connect gate="G$1" pin="SCL/CFG_SEL0" pad="24"/>
<connect gate="G$1" pin="SDA/NON_REM1" pad="22"/>
<connect gate="G$1" pin="SUSPEND/NON_REM0" pad="28"/>
<connect gate="G$1" pin="TEST" pad="11"/>
<connect gate="G$1" pin="USBDN_DM1" pad="1"/>
<connect gate="G$1" pin="USBDN_DM2" pad="3"/>
<connect gate="G$1" pin="USBDN_DM3" pad="6"/>
<connect gate="G$1" pin="USBDN_DM4" pad="8"/>
<connect gate="G$1" pin="USBDN_DP1" pad="2"/>
<connect gate="G$1" pin="USBDN_DP2" pad="4"/>
<connect gate="G$1" pin="USBDN_DP3" pad="7"/>
<connect gate="G$1" pin="USBDN_DP4" pad="9"/>
<connect gate="G$1" pin="USBUP_DM" pad="30"/>
<connect gate="G$1" pin="USBUP_DP" pad="31"/>
<connect gate="G$1" pin="VBUS" pad="27"/>
<connect gate="G$1" pin="VDD18" pad="14"/>
<connect gate="G$1" pin="VDD18PLL" pad="34"/>
<connect gate="G$1" pin="VDD33CR_1" pad="15"/>
<connect gate="G$1" pin="VDD33CR_2" pad="23"/>
<connect gate="G$1" pin="VDD33PLL" pad="36"/>
<connect gate="G$1" pin="VDDA33_1" pad="5"/>
<connect gate="G$1" pin="VDDA33_2" pad="10"/>
<connect gate="G$1" pin="VDDA33_3" pad="29"/>
<connect gate="G$1" pin="VSS" pad="P$1"/>
<connect gate="G$1" pin="XTAL1" pad="33"/>
<connect gate="G$1" pin="XTAL2" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_USBLC6-2" prefix="IC">
<gates>
<gate name="G$1" symbol="USBLC"/>
</gates>
<devices>
<device name="" package="SOT-23-6L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I/O1" pad="6"/>
<connect gate="G$1" pin="I/O2" pad="4"/>
<connect gate="G$1" pin="I/O_1" pad="1"/>
<connect gate="G$1" pin="I/O_2" pad="3"/>
<connect gate="G$1" pin="VBUS" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_3PINS" prefix="VREG" uservalue="yes">
<description>Various 3 pin voltage regulators in different packages &lt;br&gt; Double check the right pinout for the right part</description>
<gates>
<gate name="VREG" symbol="LD-1117"/>
</gates>
<devices>
<device name="-SOT-223" package="SOT-223">
<connects>
<connect gate="VREG" pin="GND" pad="1"/>
<connect gate="VREG" pin="VIN" pad="3"/>
<connect gate="VREG" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-220" package="TO-220V">
<connects>
<connect gate="VREG" pin="GND" pad="1"/>
<connect gate="VREG" pin="VIN" pad="3"/>
<connect gate="VREG" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DPAK" package="DPAK">
<connects>
<connect gate="VREG" pin="GND" pad="1"/>
<connect gate="VREG" pin="VIN" pad="3"/>
<connect gate="VREG" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D2PAK" package="D2PAK">
<connects>
<connect gate="VREG" pin="GND" pad="2"/>
<connect gate="VREG" pin="VIN" pad="1"/>
<connect gate="VREG" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_5PINS" prefix="VREG" uservalue="yes">
<description>5 pins voltage regulator</description>
<gates>
<gate name="G$1" symbol="MIC5205"/>
</gates>
<devices>
<device name="-SOT-23-5" package="SOT-23-5">
<connects>
<connect gate="G$1" pin="BYP" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_W25X10" prefix="IC">
<gates>
<gate name="G$1" symbol="W25X10"/>
</gates>
<devices>
<device name="" package="SOIC-8W">
<connects>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DIO" pad="5"/>
<connect gate="G$1" pin="DO" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK" prefix="JOY">
<gates>
<gate name="G$1" symbol="JOYSTICK"/>
</gates>
<devices>
<device name="" package="JOYSTICK">
<connects>
<connect gate="G$1" pin="ACT" pad="3"/>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="DOWN" pad="4"/>
<connect gate="G$1" pin="LEFT" pad="2"/>
<connect gate="G$1" pin="RIGHT" pad="5"/>
<connect gate="G$1" pin="UP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER_1X3" prefix="J">
<gates>
<gate name="G$1" symbol="JUMP3"/>
</gates>
<devices>
<device name="0805" package="JP3_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="J12" value="optA"/>
<attribute name="J23" value="optB"/>
</technology>
</technologies>
</device>
<device name="ALT" package="JUMPER_SOLDER">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LABEL_JUMPER_1X2">
<description>Nice formatted two legged jumperdescription&lt;br&gt;
&lt;br&gt;
Use attributes to change the values&lt;br&gt;
ON =  With jumper&lt;br&gt;
OFF =  Without jumper&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="JUMP2_DESC"/>
</gates>
<devices>
<device name="" package="JUMP2_DESC">
<technologies>
<technology name="">
<attribute name="OFF" value="off"/>
<attribute name="ON" value="on"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LABEL_JUMPER_1X3">
<description>Nice formatted three legged jumperdescription&lt;br&gt;
&lt;br&gt;
Use attributes to change the values&lt;br&gt;
LEFT =  With jumper to the left&lt;br&gt;
RIGHT =  With jumper to the right&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="JUMP3_DESC"/>
</gates>
<devices>
<device name="" package="JUMP3_DESC">
<technologies>
<technology name="">
<attribute name="LEFT" value="left"/>
<attribute name="RIGHT" value="right"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LABEL_JUMPER_2X2">
<gates>
<gate name="G$1" symbol="JUMP2X2_DESC"/>
</gates>
<devices>
<device name="" package="JUMP2X2_DESC">
<technologies>
<technology name="">
<attribute name="OPT1" value="option1"/>
<attribute name="OPT2" value="option2"/>
<attribute name="OPT3" value="option3"/>
<attribute name="OPT4" value="option4"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>Light Emitting Diode</description>
<gates>
<gate name="LED" symbol="LED"/>
</gates>
<devices>
<device name="-3MM" package="LED-3MM">
<connects>
<connect gate="LED" pin="A" pad="A"/>
<connect gate="LED" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5MM" package="LED-5MM">
<connects>
<connect gate="LED" pin="A" pad="A"/>
<connect gate="LED" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="LED-805">
<connects>
<connect gate="LED" pin="A" pad="A"/>
<connect gate="LED" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5MM-90DEG" package="LED-5MM-90DEG">
<connects>
<connect gate="LED" pin="A" pad="A"/>
<connect gate="LED" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB" prefix="LED">
<gates>
<gate name="G$1" symbol="RGB"/>
</gates>
<devices>
<device name="" package="PLCC4">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="R" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB2" prefix="LED">
<gates>
<gate name="G$1" symbol="RGBLED"/>
</gates>
<devices>
<device name="1206" package="RGBLED1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="R" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RGB3" prefix="LED">
<gates>
<gate name="G$1" symbol="RGB3"/>
</gates>
<devices>
<device name="" package="RGBLED">
<connects>
<connect gate="G$1" pin="AB" pad="AB"/>
<connect gate="G$1" pin="AG" pad="AG"/>
<connect gate="G$1" pin="AR" pad="AR"/>
<connect gate="G$1" pin="CB" pad="CB"/>
<connect gate="G$1" pin="CG" pad="CG"/>
<connect gate="G$1" pin="CR" pad="CR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO_CC-0" prefix="LOGO">
<gates>
<gate name="LOGO" symbol="LOGO_CC-0"/>
</gates>
<devices>
<device name="" package="LOGO_CC-0">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO_CC-BY-SA" prefix="LOGO">
<gates>
<gate name="LOGO" symbol="LOGO_CC_BY_SA"/>
</gates>
<devices>
<device name="" package="LOGO_CC-BY-SA">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO_DP">
<gates>
<gate name="G$1" symbol="DP_LOGO"/>
</gates>
<devices>
<device name="" package="DP_LOGO">
<technologies>
<technology name="">
<attribute name="FF1" value="fullfillment by"/>
<attribute name="FF2" value="Seeed studio"/>
<attribute name="FF3" value="www.seeedstudio.com"/>
<attribute name="LICENSE" value="CC-BY-SA"/>
<attribute name="PROJECT" value="project"/>
<attribute name="URL1" value="DangerousPrototypes.com"/>
<attribute name="URL2" value="DangerousPrototypes.com"/>
</technology>
</technologies>
</device>
<device name="2X2" package="DP_LOGO_ART_2X2">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.5X0.5" package="DP_LOGO_ART_0.5X0.5">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X1" package="DP_LOGO_ART_1X1">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3X3" package="DP_LOGO_ART_3X3">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5X2.5" package="DP_LOGO_ART_2.5X2.5">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.5X1.5" package="DP_LOGO_ART_1.5X1.5">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MODULE_MRF24WBOMA" prefix="MOD">
<gates>
<gate name="G$1" symbol="MRF24WBOMA"/>
</gates>
<devices>
<device name="" package="MRF24WBOMA">
<connects>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="!INT" pad="33"/>
<connect gate="G$1" pin="!RESET" pad="7"/>
<connect gate="G$1" pin="!WP" pad="16"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="18"/>
<connect gate="G$1" pin="GND4" pad="19"/>
<connect gate="G$1" pin="GND5" pad="25"/>
<connect gate="G$1" pin="GND6" pad="28"/>
<connect gate="G$1" pin="GND7" pad="30"/>
<connect gate="G$1" pin="GND8" pad="36"/>
<connect gate="G$1" pin="HBRNT" pad="20"/>
<connect gate="G$1" pin="JT_EN" pad="21"/>
<connect gate="G$1" pin="JT_RST" pad="9"/>
<connect gate="G$1" pin="JT_TCK" pad="4"/>
<connect gate="G$1" pin="JT_TDI" pad="6"/>
<connect gate="G$1" pin="JT_TDO" pad="3"/>
<connect gate="G$1" pin="JT_TMS" pad="5"/>
<connect gate="G$1" pin="RXD" pad="26"/>
<connect gate="G$1" pin="SCK" pad="34"/>
<connect gate="G$1" pin="SDI" pad="35"/>
<connect gate="G$1" pin="SDO" pad="32"/>
<connect gate="G$1" pin="TXD" pad="27"/>
<connect gate="G$1" pin="VDD1" pad="17"/>
<connect gate="G$1" pin="VDD2" pad="29"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSC-OSCILLATOR" prefix="XTAL">
<description>Oscillator</description>
<gates>
<gate name="G$1" symbol="OSCILLATOR"/>
</gates>
<devices>
<device name="" package="OSCILLATOR_7X5_SMD">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSC-XTAL" prefix="XTAL" uservalue="yes">
<gates>
<gate name="X" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="-HC-49U-SMD" package="HC-49U">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC-26" package="TC-26">
<connects>
<connect gate="X" pin="1" pad="P1"/>
<connect gate="X" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TC-38" package="TC-38">
<connects>
<connect gate="X" pin="1" pad="P1"/>
<connect gate="X" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-12M" package="XTAL_4X6">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-8M" package="XTAL_5X8">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC-49U-PTH" package="HC-49U-PTH">
<connects>
<connect gate="X" pin="1" pad="P1"/>
<connect gate="X" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAD_TERMINAL" prefix="T">
<description>Terminal connection pad</description>
<gates>
<gate name="T" symbol="TERMINAL"/>
</gates>
<devices>
<device name="-4.1MMROUND" package="PAD_ROUND_4.1MM">
<connects>
<connect gate="T" pin="P" pad="P"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCB_DP_RECTANGLE" prefix="PCB">
<description>Dangerous Prototypes Standard Rectangular PCB sizes</description>
<gates>
<gate name="PCB" symbol="PCB_STANDARD"/>
</gates>
<devices>
<device name="-6.2X10" package="DP10062_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP10062_V1"/>
</technology>
</technologies>
</device>
<device name="-43X70" package="DP7043_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP7043_V1"/>
</technology>
</technologies>
</device>
<device name="-31X50" package="DP5031_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP5031_V1"/>
</technology>
</technologies>
</device>
<device name="-37X60" package="DP6037_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP6037_V1"/>
</technology>
</technologies>
</device>
<device name="-80X49" package="DP8049_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP8049_V1"/>
</technology>
</technologies>
</device>
<device name="-56X90" package="DP9056_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP9056_V1"/>
</technology>
</technologies>
</device>
<device name="-50X100" package="DP10050_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP10050_V1"/>
</technology>
</technologies>
</device>
<device name="-80X100" package="DP10080_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP10080_V1"/>
</technology>
</technologies>
</device>
<device name="-85X56" package="DP8654_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP8654_V1"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCB_DP_SQUARE" prefix="PCB">
<description>Dangerous Prototypes Standard Square PCB sizes</description>
<gates>
<gate name="PCB" symbol="PCB_STANDARD"/>
</gates>
<devices>
<device name="-3X3" package="DP3030_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP3030_V1"/>
</technology>
</technologies>
</device>
<device name="-4X4" package="DP4040_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP4040_V1"/>
</technology>
</technologies>
</device>
<device name="-5X5" package="DP5050_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP5050_V1"/>
</technology>
</technologies>
</device>
<device name="-6X6" package="DP6060_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP6060_V1"/>
</technology>
</technologies>
</device>
<device name="-7X7" package="DP7070_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP7070_V1"/>
</technology>
</technologies>
</device>
<device name="-8X8" package="DP8080_V1">
<technologies>
<technology name="">
<attribute name="PCB_SIZE" value="DP8080_V1"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PROTO_VIAS_05X05">
<description>5x5 square pad 0.04 inch prototyping block</description>
<gates>
</gates>
<devices>
<device name="" package="PROTO_VIAS_05X05">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="-0805" package="R805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="R805"/>
</technologies>
</device>
<device name="-0603" package="R603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="R402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PTH-0.4" package="RTH025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-220-2" package="TO-220-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR_ARRAY_4" prefix="RN" uservalue="yes">
<description>4 Resistor Array 0603</description>
<gates>
<gate name="B" symbol="RESISTOR"/>
<gate name="C" symbol="RESISTOR"/>
<gate name="D" symbol="RESISTOR"/>
<gate name="A" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="RN8P-4R-CRA06S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="7"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="6"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR_ARRAY_8" prefix="RN">
<gates>
<gate name="A" symbol="RESISTOR"/>
<gate name="B" symbol="RESISTOR"/>
<gate name="C" symbol="RESISTOR"/>
<gate name="D" symbol="RESISTOR"/>
<gate name="E" symbol="RESISTOR"/>
<gate name="F" symbol="RESISTOR"/>
<gate name="G" symbol="RESISTOR"/>
<gate name="H" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="CAT16-F8/CAT16-J8">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="16"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="15"/>
<connect gate="C" pin="1" pad="3"/>
<connect gate="C" pin="2" pad="14"/>
<connect gate="D" pin="1" pad="4"/>
<connect gate="D" pin="2" pad="13"/>
<connect gate="E" pin="1" pad="5"/>
<connect gate="E" pin="2" pad="12"/>
<connect gate="F" pin="1" pad="6"/>
<connect gate="F" pin="2" pad="11"/>
<connect gate="G" pin="1" pad="7"/>
<connect gate="G" pin="2" pad="10"/>
<connect gate="H" pin="1" pad="8"/>
<connect gate="H" pin="2" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_MEMBRANE" prefix="SW">
<gates>
<gate name="G$1" symbol="SW_MEMBRANE"/>
</gates>
<devices>
<device name="" package="SW_MEMBRANE">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_PUSH_DPDT" prefix="SW">
<gates>
<gate name="SW" symbol="SW_DPDT"/>
</gates>
<devices>
<device name="" package="SW_PUSH_BUTTON_MINI">
<connects>
<connect gate="SW" pin="COM1" pad="2"/>
<connect gate="SW" pin="COM2" pad="5"/>
<connect gate="SW" pin="NC1" pad="1"/>
<connect gate="SW" pin="NC2" pad="4"/>
<connect gate="SW" pin="NO1" pad="3"/>
<connect gate="SW" pin="NO2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_SLIDE" prefix="SW">
<gates>
<gate name="G$1" symbol="SLIDE_SWITCH_SMD"/>
</gates>
<devices>
<device name="" package="SLIDE_SWITCH_SMD">
<connects>
<connect gate="G$1" pin="COM" pad="COM"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_TACT_4P" prefix="SW" uservalue="yes">
<gates>
<gate name="G$1" symbol="SWITCH_2"/>
</gates>
<devices>
<device name="" package="SW_TACT_SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_BJT_NPN" prefix="Q" uservalue="yes">
<description>&lt;p&gt;Most commonly used is &lt;b&gt;SOT23-BEC&lt;/b&gt;</description>
<gates>
<gate name="Q" symbol="NPN"/>
</gates>
<devices>
<device name="-SOT-23-BCE" package="SOT-23">
<connects>
<connect gate="Q" pin="B" pad="1"/>
<connect gate="Q" pin="C" pad="2"/>
<connect gate="Q" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT-23-BEC" package="SOT-23">
<connects>
<connect gate="Q" pin="B" pad="1"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT-23-EBC" package="SOT-23">
<connects>
<connect gate="Q" pin="B" pad="2"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-92-EBC" package="TO-92">
<connects>
<connect gate="Q" pin="B" pad="2"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-92-ECB" package="TO-92">
<connects>
<connect gate="Q" pin="B" pad="3"/>
<connect gate="Q" pin="C" pad="2"/>
<connect gate="Q" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_BJT_PNP" prefix="Q" uservalue="yes">
<description>&lt;p&gt;Most commonly used is &lt;b&gt;SOT23-BEC&lt;/b&gt;</description>
<gates>
<gate name="Q" symbol="PNP"/>
</gates>
<devices>
<device name="-SOT-23-BCE" package="SOT-23">
<connects>
<connect gate="Q" pin="B" pad="1"/>
<connect gate="Q" pin="C" pad="2"/>
<connect gate="Q" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT-23-BEC" package="SOT-23">
<connects>
<connect gate="Q" pin="B" pad="1"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT-23-EBC" package="SOT-23">
<connects>
<connect gate="Q" pin="B" pad="2"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-92-EBC" package="TO-92">
<connects>
<connect gate="Q" pin="B" pad="2"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-92-ECB" package="TO-92">
<connects>
<connect gate="Q" pin="B" pad="3"/>
<connect gate="Q" pin="C" pad="2"/>
<connect gate="Q" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_FET-N" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="FET"/>
</gates>
<devices>
<device name="" package="SOT-23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_FET_BS170" prefix="Q" uservalue="yes">
<description>N-Channel Enhancement Mode Field Effect Transistor</description>
<gates>
<gate name="G$1" symbol="N-MOSFET"/>
</gates>
<devices>
<device name="-SOT-23" package="SOT-23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_FET_TSM2301CX" prefix="Q" uservalue="yes">
<description>20V P-Channel Enhancement Mode MOSFET</description>
<gates>
<gate name="G$1" symbol="P-MOSFET"/>
</gates>
<devices>
<device name="" package="SOT-23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMMER" prefix="R" uservalue="yes">
<description>Trimmer resistor</description>
<gates>
<gate name="R" symbol="POT"/>
</gates>
<devices>
<device name="-3362P" package="TRIMMER_3362P">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
<connect gate="R" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3306F" package="TRIMMER_3306F">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
<connect gate="R" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3314G" package="TRIMMER_3314G">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
<connect gate="R" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZENER" prefix="ZD" uservalue="yes">
<description>Zener Diode SOD-323</description>
<gates>
<gate name="G$1" symbol="ZENER"/>
</gates>
<devices>
<device name="SOD-323F" package="SOD-323F">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD-123" package="SOD-123">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_LCD" prefix="LCD">
<gates>
<gate name="LCD" symbol="DISP_LCD"/>
</gates>
<devices>
<device name="-4X20" package="DISP_LCD_4X20">
<connects>
<connect gate="LCD" pin="A" pad="15"/>
<connect gate="LCD" pin="CONTR" pad="3"/>
<connect gate="LCD" pin="D0" pad="7"/>
<connect gate="LCD" pin="D1" pad="8"/>
<connect gate="LCD" pin="D2" pad="9"/>
<connect gate="LCD" pin="D3" pad="10"/>
<connect gate="LCD" pin="D4" pad="11"/>
<connect gate="LCD" pin="D5" pad="12"/>
<connect gate="LCD" pin="D6" pad="13"/>
<connect gate="LCD" pin="D7" pad="14"/>
<connect gate="LCD" pin="E" pad="6"/>
<connect gate="LCD" pin="GND" pad="1"/>
<connect gate="LCD" pin="K" pad="16"/>
<connect gate="LCD" pin="R/W" pad="5"/>
<connect gate="LCD" pin="RS" pad="4"/>
<connect gate="LCD" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_VFD_IV-22" prefix="DISP">
<description>7-segment VFD Display &lt;br&gt;
&lt;B&gt;Dangerousprototypes.com&lt;/B&gt;</description>
<gates>
<gate name="DISP" symbol="DISP_VFD_IV-22"/>
</gates>
<devices>
<device name="" package="DISP_IN-12_SOCKET">
<connects>
<connect gate="DISP" pin="A" pad="7"/>
<connect gate="DISP" pin="B" pad="8"/>
<connect gate="DISP" pin="C" pad="4"/>
<connect gate="DISP" pin="D" pad="3"/>
<connect gate="DISP" pin="E" pad="10"/>
<connect gate="DISP" pin="F" pad="2"/>
<connect gate="DISP" pin="FA" pad="5"/>
<connect gate="DISP" pin="FB" pad="12"/>
<connect gate="DISP" pin="G" pad="11"/>
<connect gate="DISP" pin="GRID" pad="6"/>
<connect gate="DISP" pin="H" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MAX6921" prefix="IC">
<description>20-outputs, 76V, serial VFD driver&lt;br&gt;
&lt;b&gt;Dangerousprototypes.com&lt;/b&gt;</description>
<gates>
<gate name="IC" symbol="MAX6921"/>
</gates>
<devices>
<device name="-TSSOP28" package="TSSOP-28">
<connects>
<connect gate="IC" pin="BLANK" pad="20"/>
<connect gate="IC" pin="CLK" pad="22"/>
<connect gate="IC" pin="DIN" pad="6"/>
<connect gate="IC" pin="DOUT" pad="9"/>
<connect gate="IC" pin="GND" pad="21"/>
<connect gate="IC" pin="LOAD" pad="23"/>
<connect gate="IC" pin="OUT0" pad="5"/>
<connect gate="IC" pin="OUT1" pad="4"/>
<connect gate="IC" pin="OUT10" pad="19"/>
<connect gate="IC" pin="OUT11" pad="18"/>
<connect gate="IC" pin="OUT12" pad="17"/>
<connect gate="IC" pin="OUT13" pad="16"/>
<connect gate="IC" pin="OUT14" pad="15"/>
<connect gate="IC" pin="OUT15" pad="14"/>
<connect gate="IC" pin="OUT16" pad="13"/>
<connect gate="IC" pin="OUT17" pad="12"/>
<connect gate="IC" pin="OUT18" pad="11"/>
<connect gate="IC" pin="OUT19" pad="10"/>
<connect gate="IC" pin="OUT2" pad="3"/>
<connect gate="IC" pin="OUT3" pad="2"/>
<connect gate="IC" pin="OUT4" pad="1"/>
<connect gate="IC" pin="OUT5" pad="28"/>
<connect gate="IC" pin="OUT6" pad="27"/>
<connect gate="IC" pin="OUT7" pad="26"/>
<connect gate="IC" pin="OUT8" pad="25"/>
<connect gate="IC" pin="OUT9" pad="24"/>
<connect gate="IC" pin="VBB" pad="8"/>
<connect gate="IC" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_ATMEGA32U4" prefix="IC">
<gates>
<gate name="IC" symbol="ATMEGA32U4"/>
</gates>
<devices>
<device name="-TQFP44" package="TQFP-44">
<connects>
<connect gate="IC" pin="!RESET" pad="P13"/>
<connect gate="IC" pin="AREF" pad="P42"/>
<connect gate="IC" pin="AVCC@0" pad="P24"/>
<connect gate="IC" pin="AVCC@1" pad="P44"/>
<connect gate="IC" pin="D+" pad="P4"/>
<connect gate="IC" pin="D-" pad="P3"/>
<connect gate="IC" pin="GND@0" pad="P15"/>
<connect gate="IC" pin="GND@1" pad="P23"/>
<connect gate="IC" pin="GND@2" pad="P35"/>
<connect gate="IC" pin="GND@3" pad="P43"/>
<connect gate="IC" pin="PB0" pad="P8"/>
<connect gate="IC" pin="PB1" pad="P9"/>
<connect gate="IC" pin="PB2" pad="P10"/>
<connect gate="IC" pin="PB3" pad="P11"/>
<connect gate="IC" pin="PB4" pad="P28"/>
<connect gate="IC" pin="PB5" pad="P29"/>
<connect gate="IC" pin="PB6" pad="P30"/>
<connect gate="IC" pin="PB7" pad="P12"/>
<connect gate="IC" pin="PC6" pad="P31"/>
<connect gate="IC" pin="PC7" pad="P32"/>
<connect gate="IC" pin="PD0" pad="P18"/>
<connect gate="IC" pin="PD1" pad="P19"/>
<connect gate="IC" pin="PD2" pad="P20"/>
<connect gate="IC" pin="PD3" pad="P21"/>
<connect gate="IC" pin="PD4" pad="P25"/>
<connect gate="IC" pin="PD5" pad="P22"/>
<connect gate="IC" pin="PD6" pad="P26"/>
<connect gate="IC" pin="PD7" pad="P27"/>
<connect gate="IC" pin="PE2" pad="P33"/>
<connect gate="IC" pin="PE6" pad="P1"/>
<connect gate="IC" pin="PF0" pad="P41"/>
<connect gate="IC" pin="PF1" pad="P40"/>
<connect gate="IC" pin="PF4" pad="P39"/>
<connect gate="IC" pin="PF5" pad="P38"/>
<connect gate="IC" pin="PF6" pad="P37"/>
<connect gate="IC" pin="PF7" pad="P36"/>
<connect gate="IC" pin="UCAP" pad="P6"/>
<connect gate="IC" pin="UGND" pad="P5"/>
<connect gate="IC" pin="UVCC" pad="P2"/>
<connect gate="IC" pin="VBUS" pad="P7"/>
<connect gate="IC" pin="VCC@0" pad="P14"/>
<connect gate="IC" pin="VCC@1" pad="P34"/>
<connect gate="IC" pin="XTAL1" pad="P17"/>
<connect gate="IC" pin="XTAL2" pad="P16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L">
<description>Inductor</description>
<gates>
<gate name="L" symbol="COIL"/>
</gates>
<devices>
<device name="-L1812" package="L1812">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_ENC28J60" prefix="IC">
<description>Ethernet Controller with SPI Interface</description>
<gates>
<gate name="IC" symbol="ENC28J60"/>
</gates>
<devices>
<device name="-SOIC-28" package="SOIC-28W">
<connects>
<connect gate="IC" pin="!CS" pad="9"/>
<connect gate="IC" pin="!INT" pad="4"/>
<connect gate="IC" pin="!RESET" pad="10"/>
<connect gate="IC" pin="CLKOUT" pad="3"/>
<connect gate="IC" pin="LEDA" pad="27"/>
<connect gate="IC" pin="LEDB" pad="26"/>
<connect gate="IC" pin="OSC1" pad="23"/>
<connect gate="IC" pin="OSC2" pad="24"/>
<connect gate="IC" pin="RBIAS" pad="14"/>
<connect gate="IC" pin="SCK" pad="8"/>
<connect gate="IC" pin="SI" pad="7"/>
<connect gate="IC" pin="SO" pad="6"/>
<connect gate="IC" pin="TPIN+" pad="13"/>
<connect gate="IC" pin="TPIN-" pad="12"/>
<connect gate="IC" pin="TPOUT+" pad="17"/>
<connect gate="IC" pin="TPOUT-" pad="16"/>
<connect gate="IC" pin="VCAP" pad="1"/>
<connect gate="IC" pin="VDD" pad="28"/>
<connect gate="IC" pin="VDDOSC" pad="25"/>
<connect gate="IC" pin="VDDPLL" pad="20"/>
<connect gate="IC" pin="VDDRX" pad="19"/>
<connect gate="IC" pin="VDDTX" pad="15"/>
<connect gate="IC" pin="VSS" pad="2"/>
<connect gate="IC" pin="VSSOSC" pad="22"/>
<connect gate="IC" pin="VSSPLL" pad="21"/>
<connect gate="IC" pin="VSSRX" pad="11"/>
<connect gate="IC" pin="VSSTX" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_LTC4053" prefix="IC">
<description>USB Compatible Li-Ion Battery Charger</description>
<gates>
<gate name="IC" symbol="LTC4053"/>
</gates>
<devices>
<device name="-MSOP-10" package="MSOP-10">
<connects>
<connect gate="IC" pin="!ACPR" pad="P10"/>
<connect gate="IC" pin="!CHRG" pad="P1"/>
<connect gate="IC" pin="!FAULT" pad="P3"/>
<connect gate="IC" pin="!SHDN" pad="P8"/>
<connect gate="IC" pin="BAT" pad="P9"/>
<connect gate="IC" pin="GND@1" pad="P5"/>
<connect gate="IC" pin="GND@2" pad="P11"/>
<connect gate="IC" pin="NTC" pad="P6"/>
<connect gate="IC" pin="PROG" pad="P7"/>
<connect gate="IC" pin="TIMER" pad="P4"/>
<connect gate="IC" pin="VCC" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER_SW1" prefix="SW">
<description>Incremental Encoder with push switch</description>
<gates>
<gate name="ENCODER" symbol="ENCODER"/>
<gate name="SW" symbol="SW_MEMBRANE"/>
</gates>
<devices>
<device name="-PEC12" package="PEC12_INCREMENTAL_ENCODER">
<connects>
<connect gate="ENCODER" pin="A" pad="A"/>
<connect gate="ENCODER" pin="B" pad="B"/>
<connect gate="ENCODER" pin="C" pad="C"/>
<connect gate="SW" pin="1" pad="P1"/>
<connect gate="SW" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X07" prefix="J">
<description>2x07 pin header</description>
<gates>
<gate name="J" symbol="HEADER2X7"/>
</gates>
<devices>
<device name="-PTH-SHROUDED" package="PINSHRD_PTH_2X07">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="13" pad="13"/>
<connect gate="J" pin="14" pad="14"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FT230X" prefix="IC">
<description>BASIC USB to UART IC</description>
<gates>
<gate name="IC" symbol="FT230X"/>
</gates>
<devices>
<device name="-SSOP-16" package="SSOP-16-FTDI">
<connects>
<connect gate="IC" pin="!CTS" pad="6"/>
<connect gate="IC" pin="!RESET" pad="11"/>
<connect gate="IC" pin="!RTS" pad="2"/>
<connect gate="IC" pin="3V3OUT" pad="10"/>
<connect gate="IC" pin="CBUS0" pad="15"/>
<connect gate="IC" pin="CBUS1" pad="14"/>
<connect gate="IC" pin="CBUS2" pad="7"/>
<connect gate="IC" pin="CBUS3" pad="16"/>
<connect gate="IC" pin="GND@1" pad="5"/>
<connect gate="IC" pin="GND@2" pad="13"/>
<connect gate="IC" pin="RXD" pad="4"/>
<connect gate="IC" pin="TXD" pad="1"/>
<connect gate="IC" pin="USB+" pad="8"/>
<connect gate="IC" pin="USB-" pad="9"/>
<connect gate="IC" pin="VCC" pad="12"/>
<connect gate="IC" pin="VCCIO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VREG_3PINS_ADJ-*" prefix="VREG">
<description>Adjustable 3 pins voltage regulators</description>
<gates>
<gate name="VREG" symbol="VREG-ADJ"/>
</gates>
<devices>
<device name="-TO-220VA" package="TO-220V">
<connects>
<connect gate="VREG" pin="ADJ" pad="1"/>
<connect gate="VREG" pin="VIN" pad="3"/>
<connect gate="VREG" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="LM317T"/>
</technologies>
</device>
<device name="-TO-220VB" package="TO-220V">
<connects>
<connect gate="VREG" pin="ADJ" pad="1"/>
<connect gate="VREG" pin="VIN" pad="2"/>
<connect gate="VREG" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="LM337T"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_74HC595" prefix="IC">
<description>8-bit serial-in parallel out shift register, output latch 3-state</description>
<gates>
<gate name="IC" symbol="74595"/>
<gate name="SUP" symbol="SUPPLY"/>
</gates>
<devices>
<device name="-TSSOP-16" package="TSSOP-16">
<connects>
<connect gate="IC" pin="!OE" pad="13"/>
<connect gate="IC" pin="!RST" pad="10"/>
<connect gate="IC" pin="LATCH" pad="12"/>
<connect gate="IC" pin="Q0" pad="15"/>
<connect gate="IC" pin="Q1" pad="1"/>
<connect gate="IC" pin="Q2" pad="2"/>
<connect gate="IC" pin="Q3" pad="3"/>
<connect gate="IC" pin="Q4" pad="4"/>
<connect gate="IC" pin="Q5" pad="5"/>
<connect gate="IC" pin="Q6" pad="6"/>
<connect gate="IC" pin="Q7" pad="7"/>
<connect gate="IC" pin="Q7S" pad="9"/>
<connect gate="IC" pin="SCLK" pad="11"/>
<connect gate="IC" pin="SDA" pad="14"/>
<connect gate="SUP" pin="GND" pad="8"/>
<connect gate="SUP" pin="V+" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOIC-16" package="SOIC-16">
<connects>
<connect gate="IC" pin="!OE" pad="13"/>
<connect gate="IC" pin="!RST" pad="10"/>
<connect gate="IC" pin="LATCH" pad="12"/>
<connect gate="IC" pin="Q0" pad="15"/>
<connect gate="IC" pin="Q1" pad="1"/>
<connect gate="IC" pin="Q2" pad="2"/>
<connect gate="IC" pin="Q3" pad="3"/>
<connect gate="IC" pin="Q4" pad="4"/>
<connect gate="IC" pin="Q5" pad="5"/>
<connect gate="IC" pin="Q6" pad="6"/>
<connect gate="IC" pin="Q7" pad="7"/>
<connect gate="IC" pin="Q7S" pad="9"/>
<connect gate="IC" pin="SCLK" pad="11"/>
<connect gate="IC" pin="SDA" pad="14"/>
<connect gate="SUP" pin="GND" pad="8"/>
<connect gate="SUP" pin="V+" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DIP-16" package="DIL16">
<connects>
<connect gate="IC" pin="!OE" pad="13"/>
<connect gate="IC" pin="!RST" pad="10"/>
<connect gate="IC" pin="LATCH" pad="12"/>
<connect gate="IC" pin="Q0" pad="15"/>
<connect gate="IC" pin="Q1" pad="1"/>
<connect gate="IC" pin="Q2" pad="2"/>
<connect gate="IC" pin="Q3" pad="3"/>
<connect gate="IC" pin="Q4" pad="4"/>
<connect gate="IC" pin="Q5" pad="5"/>
<connect gate="IC" pin="Q6" pad="6"/>
<connect gate="IC" pin="Q7" pad="7"/>
<connect gate="IC" pin="Q7S" pad="9"/>
<connect gate="IC" pin="SCLK" pad="11"/>
<connect gate="IC" pin="SDA" pad="14"/>
<connect gate="SUP" pin="GND" pad="8"/>
<connect gate="SUP" pin="V+" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_ULN2003" prefix="IC">
<description>7 Darlington Array Driver</description>
<gates>
<gate name="IC" symbol="ULN2003"/>
</gates>
<devices>
<device name="-TSSOP-16" package="TSSOP-16">
<connects>
<connect gate="IC" pin="1B" pad="1"/>
<connect gate="IC" pin="1C" pad="16"/>
<connect gate="IC" pin="2B" pad="2"/>
<connect gate="IC" pin="2C" pad="15"/>
<connect gate="IC" pin="3B" pad="3"/>
<connect gate="IC" pin="3C" pad="14"/>
<connect gate="IC" pin="4B" pad="4"/>
<connect gate="IC" pin="4C" pad="13"/>
<connect gate="IC" pin="5B" pad="5"/>
<connect gate="IC" pin="5C" pad="12"/>
<connect gate="IC" pin="6B" pad="6"/>
<connect gate="IC" pin="6C" pad="11"/>
<connect gate="IC" pin="7B" pad="7"/>
<connect gate="IC" pin="7C" pad="10"/>
<connect gate="IC" pin="COM" pad="9"/>
<connect gate="IC" pin="GND" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_74HC4017" prefix="IC">
<description>Decade counter</description>
<gates>
<gate name="IC" symbol="74HC4017"/>
<gate name="SUPPLY" symbol="SUPPLY"/>
</gates>
<devices>
<device name="-TSSOP-16" package="TSSOP-16">
<connects>
<connect gate="IC" pin="!CP1" pad="13"/>
<connect gate="IC" pin="!Q5-9" pad="12"/>
<connect gate="IC" pin="CP0" pad="14"/>
<connect gate="IC" pin="MR" pad="15"/>
<connect gate="IC" pin="Q0" pad="3"/>
<connect gate="IC" pin="Q1" pad="2"/>
<connect gate="IC" pin="Q2" pad="4"/>
<connect gate="IC" pin="Q3" pad="7"/>
<connect gate="IC" pin="Q4" pad="10"/>
<connect gate="IC" pin="Q5" pad="1"/>
<connect gate="IC" pin="Q6" pad="5"/>
<connect gate="IC" pin="Q7" pad="6"/>
<connect gate="IC" pin="Q8" pad="9"/>
<connect gate="IC" pin="Q9" pad="11"/>
<connect gate="SUPPLY" pin="GND" pad="8"/>
<connect gate="SUPPLY" pin="V+" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_555" prefix="IC">
<description>Classic 555 IC</description>
<gates>
<gate name="IC" symbol="555"/>
</gates>
<devices>
<device name="-SOIC8" package="SOIC-8">
<connects>
<connect gate="IC" pin="CTRL" pad="5"/>
<connect gate="IC" pin="DIS" pad="7"/>
<connect gate="IC" pin="GND" pad="1"/>
<connect gate="IC" pin="OUT" pad="3"/>
<connect gate="IC" pin="RST" pad="4"/>
<connect gate="IC" pin="THR" pad="6"/>
<connect gate="IC" pin="TRIG" pad="2"/>
<connect gate="IC" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_KSZ8851SNL" prefix="IC">
<description>Fast Ethernet Controller with PHY, MAC and SPI</description>
<gates>
<gate name="IC" symbol="IC_KSZ8851SNL"/>
<gate name="SUP" symbol="QFN25_GND"/>
</gates>
<devices>
<device name="" package="QFN32_5X5">
<connects>
<connect gate="IC" pin="!CS" pad="26"/>
<connect gate="IC" pin="!INT" pad="3"/>
<connect gate="IC" pin="!RST" pad="19"/>
<connect gate="IC" pin="AGND@1" pad="8"/>
<connect gate="IC" pin="AGND@2" pad="13"/>
<connect gate="IC" pin="AGND@3" pad="18"/>
<connect gate="IC" pin="DGND@1" pad="4"/>
<connect gate="IC" pin="DGND@2" pad="22"/>
<connect gate="IC" pin="DGND@3" pad="24"/>
<connect gate="IC" pin="DGND@4" pad="29"/>
<connect gate="IC" pin="EDD_IO" pad="6"/>
<connect gate="IC" pin="EECS" pad="10"/>
<connect gate="IC" pin="EESK" pad="7"/>
<connect gate="IC" pin="ISET" pad="17"/>
<connect gate="IC" pin="LED0" pad="1"/>
<connect gate="IC" pin="LED1" pad="32"/>
<connect gate="IC" pin="PME" pad="2"/>
<connect gate="IC" pin="RXM" pad="12"/>
<connect gate="IC" pin="RXP" pad="11"/>
<connect gate="IC" pin="SCLK" pad="28"/>
<connect gate="IC" pin="SI" pad="31"/>
<connect gate="IC" pin="SO" pad="27"/>
<connect gate="IC" pin="TXM" pad="15"/>
<connect gate="IC" pin="TXP" pad="14"/>
<connect gate="IC" pin="VDD_A18" pad="9"/>
<connect gate="IC" pin="VDD_A33" pad="16"/>
<connect gate="IC" pin="VDD_CO18" pad="5"/>
<connect gate="IC" pin="VDD_D18" pad="23"/>
<connect gate="IC" pin="VDD_IO@1" pad="25"/>
<connect gate="IC" pin="VDD_IO@2" pad="30"/>
<connect gate="IC" pin="X1" pad="20"/>
<connect gate="IC" pin="X2" pad="21"/>
<connect gate="SUP" pin="GND@0" pad="EP"/>
<connect gate="SUP" pin="GND@1" pad="EP1"/>
<connect gate="SUP" pin="GND@2" pad="EP2"/>
<connect gate="SUP" pin="GND@3" pad="EP3"/>
<connect gate="SUP" pin="GND@4" pad="EP4"/>
<connect gate="SUP" pin="GND@5" pad="EP5"/>
<connect gate="SUP" pin="GND@6" pad="EP6"/>
<connect gate="SUP" pin="GND@7" pad="EP7"/>
<connect gate="SUP" pin="GND@8" pad="PAD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_TPS6120X" prefix="IC">
<description>Low input voltage Synchronous Boost converter</description>
<gates>
<gate name="IC" symbol="TPS6120X"/>
<gate name="GND" symbol="QFN-10-GND"/>
</gates>
<devices>
<device name="-QFN10" package="QFN-10">
<connects>
<connect gate="GND" pin="GND@0" pad="P0"/>
<connect gate="GND" pin="GND@1" pad="P1"/>
<connect gate="GND" pin="GND@2" pad="P2"/>
<connect gate="GND" pin="GND@3" pad="P3"/>
<connect gate="GND" pin="GND@4" pad="P4"/>
<connect gate="GND" pin="GND@5" pad="V0"/>
<connect gate="GND" pin="GND@6" pad="V1"/>
<connect gate="IC" pin="EN" pad="6"/>
<connect gate="IC" pin="FB" pad="10"/>
<connect gate="IC" pin="GND" pad="9"/>
<connect gate="IC" pin="L" pad="3"/>
<connect gate="IC" pin="PGND" pad="4"/>
<connect gate="IC" pin="PS" pad="8"/>
<connect gate="IC" pin="UVLO" pad="7"/>
<connect gate="IC" pin="VAUX" pad="1"/>
<connect gate="IC" pin="VIN" pad="5"/>
<connect gate="IC" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_HEADER_2X08" prefix="J">
<gates>
<gate name="J" symbol="HEADER2X8"/>
</gates>
<devices>
<device name="" package="M2X8">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="13" pad="13"/>
<connect gate="J" pin="14" pad="14"/>
<connect gate="J" pin="15" pad="15"/>
<connect gate="J" pin="16" pad="16"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_TACT_2P" prefix="SW">
<gates>
<gate name="SW" symbol="SWITCH_1"/>
</gates>
<devices>
<device name="-3X6" package="SW_TACT_3X6">
<connects>
<connect gate="SW" pin="1" pad="1"/>
<connect gate="SW" pin="3" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_TFT18">
<gates>
<gate name="G$1" symbol="LCD_SPI"/>
</gates>
<devices>
<device name="" package="TFT18">
<connects>
<connect gate="G$1" pin="CS" pad="12"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="LEDA" pad="4"/>
<connect gate="G$1" pin="LEDK" pad="3"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="14"/>
<connect gate="G$1" pin="RS" pad="7"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="8"/>
<connect gate="G$1" pin="VCC1" pad="10"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_TERMINAL_BLOCK_02" prefix="J">
<description>2 poles wire to board terminal block</description>
<gates>
<gate name="CON" symbol="HEADER1X2"/>
</gates>
<devices>
<device name="-5MM" package="TERMINAL_BLOCK_2P_5">
<connects>
<connect gate="CON" pin="1" pad="1"/>
<connect gate="CON" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY_+5V" prefix="+5V">
<gates>
<gate name="SUPPLY" symbol="SUPPLY_+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY_VUSB" prefix="VUSB">
<gates>
<gate name="G$1" symbol="SUPPLY_VUSB"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY_+3V3" prefix="+3V3">
<gates>
<gate name="G$1" symbol="SUPPLY_+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY_GND" prefix="GND">
<gates>
<gate name="G$1" symbol="SUPPLY_GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_TERMINAL_BLOCK_03" prefix="J">
<description>3 poles, wire to board connector</description>
<gates>
<gate name="CON" symbol="HEADER1X3"/>
</gates>
<devices>
<device name="-5MM" package="TERMINAL_BLOCK_3P_5">
<connects>
<connect gate="CON" pin="1" pad="1"/>
<connect gate="CON" pin="2" pad="2"/>
<connect gate="CON" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-USB-F-2PB" prefix="USB">
<description>USB Female connector with 2 body pins</description>
<gates>
<gate name="USB" symbol="CONN_USB_4P"/>
<gate name="B" symbol="USB_BODY_PINS_2P"/>
</gates>
<devices>
<device name="" package="CONN_USB_A_F">
<connects>
<connect gate="B" pin="BODY@1" pad="B1"/>
<connect gate="B" pin="BODY@2" pad="B2"/>
<connect gate="USB" pin="D+" pad="3"/>
<connect gate="USB" pin="D-" pad="2"/>
<connect gate="USB" pin="GND" pad="4"/>
<connect gate="USB" pin="VUSB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_74AC573" prefix="IC">
<description>8 Transparent Latch with 3-state output
&lt;br&gt; Mfr no: SN74AC573NSR
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/SN74AC573NSR/296-29119-1-ND/2690568"&gt; Digikey &lt;/a&gt;</description>
<gates>
<gate name="IC" symbol="74AC573"/>
<gate name="PWR" symbol="SUPPLY"/>
</gates>
<devices>
<device name="" package="SOIC-20">
<connects>
<connect gate="IC" pin="!OE" pad="1"/>
<connect gate="IC" pin="1D" pad="2"/>
<connect gate="IC" pin="1Q" pad="19"/>
<connect gate="IC" pin="2D" pad="3"/>
<connect gate="IC" pin="2Q" pad="18"/>
<connect gate="IC" pin="3D" pad="4"/>
<connect gate="IC" pin="3Q" pad="17"/>
<connect gate="IC" pin="4D" pad="5"/>
<connect gate="IC" pin="4Q" pad="16"/>
<connect gate="IC" pin="5D" pad="6"/>
<connect gate="IC" pin="5Q" pad="15"/>
<connect gate="IC" pin="6D" pad="7"/>
<connect gate="IC" pin="6Q" pad="14"/>
<connect gate="IC" pin="7D" pad="8"/>
<connect gate="IC" pin="7Q" pad="13"/>
<connect gate="IC" pin="8D" pad="9"/>
<connect gate="IC" pin="8Q" pad="12"/>
<connect gate="IC" pin="LE" pad="11"/>
<connect gate="PWR" pin="GND" pad="10"/>
<connect gate="PWR" pin="V+" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_FT311D" prefix="IC">
<description>&lt;b&gt;USB Android Host&lt;/b&gt;
&lt;br&gt; Mfr no: FT311D-32L1C
&lt;br&gt;&lt;a href="http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT311D.pdf"&gt; FT311D &lt;/a&gt;</description>
<gates>
<gate name="IC" symbol="FT311D"/>
</gates>
<devices>
<device name="-LQFP-32" package="LQFP-32">
<connects>
<connect gate="IC" pin="!RESET" pad="10"/>
<connect gate="IC" pin="!USB_ERROR" pad="32"/>
<connect gate="IC" pin="AVCC" pad="3"/>
<connect gate="IC" pin="CNFG0" pad="12"/>
<connect gate="IC" pin="CNFG1" pad="14"/>
<connect gate="IC" pin="CNFG2" pad="15"/>
<connect gate="IC" pin="GND@1" pad="1"/>
<connect gate="IC" pin="GND@2" pad="6"/>
<connect gate="IC" pin="GND@3" pad="16"/>
<connect gate="IC" pin="GND@4" pad="19"/>
<connect gate="IC" pin="GND@5" pad="27"/>
<connect gate="IC" pin="IOBUS0" pad="23"/>
<connect gate="IC" pin="IOBUS1" pad="24"/>
<connect gate="IC" pin="IOBUS2" pad="25"/>
<connect gate="IC" pin="IOBUS3" pad="26"/>
<connect gate="IC" pin="IOBUS4" pad="29"/>
<connect gate="IC" pin="IOBUS5" pad="30"/>
<connect gate="IC" pin="IOBUS6" pad="31"/>
<connect gate="IC" pin="TEST0" pad="11"/>
<connect gate="IC" pin="TEST1" pad="8"/>
<connect gate="IC" pin="TEST2" pad="9"/>
<connect gate="IC" pin="USB+" pad="17"/>
<connect gate="IC" pin="USB-" pad="18"/>
<connect gate="IC" pin="VCC" pad="2"/>
<connect gate="IC" pin="VCCIO@1" pad="13"/>
<connect gate="IC" pin="VCCIO@2" pad="22"/>
<connect gate="IC" pin="VCCIO@3" pad="28"/>
<connect gate="IC" pin="VREGOUT" pad="7"/>
<connect gate="IC" pin="XTIN" pad="4"/>
<connect gate="IC" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MEM_23LC1024" prefix="IC">
<description>1Mbit SPI SRAM with Serial dual interface and Serial quad interface</description>
<gates>
<gate name="IC" symbol="SRAM-23LCXXXX"/>
<gate name="SUP" symbol="SUPPLY"/>
</gates>
<devices>
<device name="" package="SOIC-8">
<connects>
<connect gate="IC" pin="!CS" pad="1"/>
<connect gate="IC" pin="!HOLD/SIO3" pad="7"/>
<connect gate="IC" pin="SCK" pad="6"/>
<connect gate="IC" pin="SI/SIO0" pad="5"/>
<connect gate="IC" pin="SIO2" pad="3"/>
<connect gate="IC" pin="SO/SIO1" pad="2"/>
<connect gate="SUP" pin="GND" pad="4"/>
<connect gate="SUP" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_74141" prefix="IC">
<description>BCD to decimal decoder</description>
<gates>
<gate name="IC" symbol="74141"/>
<gate name="SUPPLY" symbol="SUPPLY"/>
</gates>
<devices>
<device name="-DIP-16" package="DIL16">
<connects>
<connect gate="IC" pin="A" pad="3"/>
<connect gate="IC" pin="B" pad="6"/>
<connect gate="IC" pin="C" pad="7"/>
<connect gate="IC" pin="D" pad="4"/>
<connect gate="IC" pin="Q0" pad="16"/>
<connect gate="IC" pin="Q1" pad="15"/>
<connect gate="IC" pin="Q2" pad="8"/>
<connect gate="IC" pin="Q3" pad="9"/>
<connect gate="IC" pin="Q4" pad="13"/>
<connect gate="IC" pin="Q5" pad="14"/>
<connect gate="IC" pin="Q6" pad="11"/>
<connect gate="IC" pin="Q7" pad="10"/>
<connect gate="IC" pin="Q8" pad="1"/>
<connect gate="IC" pin="Q9" pad="2"/>
<connect gate="SUPPLY" pin="GND" pad="12"/>
<connect gate="SUPPLY" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY_+12V" prefix="+12V">
<gates>
<gate name="SUPPLY" symbol="SUPPLY_+12V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY_-12V" prefix="-12V">
<gates>
<gate name="SUPPLY" symbol="SUPPLY_-12V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY_-5V" prefix="-5V">
<gates>
<gate name="SUPPLY" symbol="SUPPLY_-5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_IN12A" prefix="DISP">
<description>IN-12A Nixie Display</description>
<gates>
<gate name="DISP" symbol="DISP_IN-12"/>
</gates>
<devices>
<device name="" package="DISP_IN-12_SOCKET">
<connects>
<connect gate="DISP" pin="ANODE" pad="1"/>
<connect gate="DISP" pin="K0" pad="2"/>
<connect gate="DISP" pin="K1" pad="11"/>
<connect gate="DISP" pin="K2" pad="10"/>
<connect gate="DISP" pin="K3" pad="9"/>
<connect gate="DISP" pin="K4" pad="8"/>
<connect gate="DISP" pin="K5" pad="7"/>
<connect gate="DISP" pin="K6" pad="6"/>
<connect gate="DISP" pin="K7" pad="5"/>
<connect gate="DISP" pin="K8" pad="4"/>
<connect gate="DISP" pin="K9" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_INA138" prefix="IC">
<description>&lt;b&gt;High Side Current  Shunt Monitor&lt;/b&gt;
&lt;br&gt; Mfr no: INA138NA/3K
&lt;br&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/ina138.pdf"&gt; INA138 &lt;/a&gt;</description>
<gates>
<gate name="IC" symbol="IC_INA138"/>
</gates>
<devices>
<device name="" package="SOT-23-5">
<connects>
<connect gate="IC" pin="GND" pad="2"/>
<connect gate="IC" pin="OUT" pad="1"/>
<connect gate="IC" pin="V+" pad="5"/>
<connect gate="IC" pin="VIN+" pad="3"/>
<connect gate="IC" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISP_D8035E" prefix="DISP">
<description>VFD 7-Segment Display
&lt;br&gt; Mfr no: NEC LD8035E
&lt;br&gt; &lt;a href="http://www.tube-tester.com/sites/nixie/dat_arch/D-8035-E_LD8035.pdf"&gt; D-8035-E PDF&lt;/a&gt;</description>
<gates>
<gate name="DISP" symbol="DISP_D8035E"/>
</gates>
<devices>
<device name="" package="DISP_D8035E">
<connects>
<connect gate="DISP" pin="-" pad="5"/>
<connect gate="DISP" pin="A" pad="7"/>
<connect gate="DISP" pin="B" pad="6"/>
<connect gate="DISP" pin="C" pad="12"/>
<connect gate="DISP" pin="D" pad="11"/>
<connect gate="DISP" pin="DP" pad="2"/>
<connect gate="DISP" pin="E" pad="10"/>
<connect gate="DISP" pin="F" pad="9"/>
<connect gate="DISP" pin="F+" pad="1"/>
<connect gate="DISP" pin="F-" pad="4"/>
<connect gate="DISP" pin="G" pad="8"/>
<connect gate="DISP" pin="GRID" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MIC2027" prefix="IC">
<description>&lt;b&gt;Quad USB Power Distribution Switch&lt;/b&gt;
&lt;br&gt; Mfr no: MIC2027-2YM
&lt;br&gt;&lt;a href="http://www.digikey.com/product-detail/en/MIC2027-2YM/576-2139-ND/1027902"&gt; MIC2027 &lt;/a&gt;</description>
<gates>
<gate name="IC" symbol="IC_MIC2027"/>
</gates>
<devices>
<device name="-SOIC-16" package="SOIC-16">
<connects>
<connect gate="IC" pin="EN_A" pad="2"/>
<connect gate="IC" pin="EN_B" pad="15"/>
<connect gate="IC" pin="EN_C" pad="7"/>
<connect gate="IC" pin="EN_D" pad="10"/>
<connect gate="IC" pin="FLG_A" pad="1"/>
<connect gate="IC" pin="FLG_B" pad="16"/>
<connect gate="IC" pin="FLG_C" pad="8"/>
<connect gate="IC" pin="FLG_D" pad="9"/>
<connect gate="IC" pin="GND@1" pad="4"/>
<connect gate="IC" pin="GND@2" pad="12"/>
<connect gate="IC" pin="IN_AB" pad="13"/>
<connect gate="IC" pin="IN_CD" pad="5"/>
<connect gate="IC" pin="OUT_A" pad="3"/>
<connect gate="IC" pin="OUT_B" pad="14"/>
<connect gate="IC" pin="OUT_C" pad="6"/>
<connect gate="IC" pin="OUT_D" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOIC-16W" package="SOIC-16W">
<connects>
<connect gate="IC" pin="EN_A" pad="2"/>
<connect gate="IC" pin="EN_B" pad="15"/>
<connect gate="IC" pin="EN_C" pad="7"/>
<connect gate="IC" pin="EN_D" pad="10"/>
<connect gate="IC" pin="FLG_A" pad="1"/>
<connect gate="IC" pin="FLG_B" pad="16"/>
<connect gate="IC" pin="FLG_C" pad="8"/>
<connect gate="IC" pin="FLG_D" pad="9"/>
<connect gate="IC" pin="GND@1" pad="4"/>
<connect gate="IC" pin="GND@2" pad="12"/>
<connect gate="IC" pin="IN_AB" pad="13"/>
<connect gate="IC" pin="IN_CD" pad="5"/>
<connect gate="IC" pin="OUT_A" pad="3"/>
<connect gate="IC" pin="OUT_B" pad="14"/>
<connect gate="IC" pin="OUT_C" pad="6"/>
<connect gate="IC" pin="OUT_D" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_TD62783" prefix="IC">
<description>8 Channel High voltage Source driver
&lt;br&gt; Mfr no: TD62783
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/TD62783AFG%28O,S%29/TD62783AFG%28OS%29-ND/871116"&gt; TD62783AFG&lt;/a&gt;</description>
<gates>
<gate name="IC" symbol="IC_TD62783"/>
</gates>
<devices>
<device name="-SO-18W" package="SO-18L">
<connects>
<connect gate="IC" pin="GND" pad="9"/>
<connect gate="IC" pin="IN1" pad="1"/>
<connect gate="IC" pin="IN2" pad="2"/>
<connect gate="IC" pin="IN3" pad="3"/>
<connect gate="IC" pin="IN4" pad="4"/>
<connect gate="IC" pin="IN5" pad="5"/>
<connect gate="IC" pin="IN6" pad="6"/>
<connect gate="IC" pin="IN7" pad="7"/>
<connect gate="IC" pin="IN8" pad="8"/>
<connect gate="IC" pin="OUT1" pad="18"/>
<connect gate="IC" pin="OUT2" pad="17"/>
<connect gate="IC" pin="OUT3" pad="16"/>
<connect gate="IC" pin="OUT4" pad="15"/>
<connect gate="IC" pin="OUT5" pad="14"/>
<connect gate="IC" pin="OUT6" pad="13"/>
<connect gate="IC" pin="OUT7" pad="12"/>
<connect gate="IC" pin="OUT8" pad="11"/>
<connect gate="IC" pin="VS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK_SF303GJ26-3" prefix="SW">
<description>Multi way switch
&lt;br&gt; Mfr no: SF303GJ26-3
&lt;br&gt; &lt;a href="https://www.sparkfun.com/products/10063?"&gt; SF303GJ26-3&lt;/a&gt;</description>
<gates>
<gate name="SW" symbol="JOYSTICK_SF303GJ26-3"/>
</gates>
<devices>
<device name="" package="JOYSTICK_SF303GJ26-3">
<connects>
<connect gate="SW" pin="A" pad="1"/>
<connect gate="SW" pin="B" pad="4"/>
<connect gate="SW" pin="C" pad="3"/>
<connect gate="SW" pin="CENTER" pad="2"/>
<connect gate="SW" pin="COMMON" pad="5"/>
<connect gate="SW" pin="D" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_UC_PIC24F16KA102" prefix="IC">
<description>16-Bit Flash PIC Microcontroller
&lt;br&gt; Mfr no: PIC24F16KA102
&lt;br&gt; &lt;a href="http://www.microchip.com/wwwproducts/Devices.aspx?dDocName=en539800"&gt; PIC24F16KA102&lt;/a&gt;</description>
<gates>
<gate name="IC" symbol="PIC24F16KA102"/>
</gates>
<devices>
<device name="-SSOP" package="SSOP-28">
<connects>
<connect gate="IC" pin="!U1CTS!/SCL1/CN22/RB8" pad="17"/>
<connect gate="IC" pin="!U1RTS!/U1BCLK/SDA1/CN21/RB9" pad="18"/>
<connect gate="IC" pin="HLVDIN/CTED2/CN14/AN12/RB12" pad="23"/>
<connect gate="IC" pin="IC1/CN9/RA7" pad="19"/>
<connect gate="IC" pin="OC1/C2OUT/INT2/CTED1/CN8/RA6" pad="20"/>
<connect gate="IC" pin="OCFA/C1OUT/RTCC/CVREF/CN12/AN10/RB14" pad="25"/>
<connect gate="IC" pin="RA0/AN0/CN2/VREF+" pad="2"/>
<connect gate="IC" pin="RA1/AN1/CN3/VREF-" pad="3"/>
<connect gate="IC" pin="RA2/CN30/OSCI/CLKI" pad="9"/>
<connect gate="IC" pin="RA3/CN29/OSCO/CLKO" pad="10"/>
<connect gate="IC" pin="RA4/CN0/SOSCO/T1CK/!U2CTS!" pad="12"/>
<connect gate="IC" pin="RA5/!MCLR!/VPP" pad="1"/>
<connect gate="IC" pin="RB0/AN2/CN4/C2INB/C1IND/PGD1/U2TX" pad="4"/>
<connect gate="IC" pin="RB1/AN3/CN5/C2INA/C1INC/PGC1/U2RX" pad="5"/>
<connect gate="IC" pin="RB2/AN4/CN6/C2IND/C1INB/U1RX" pad="6"/>
<connect gate="IC" pin="RB3/AN5/CN7/C2INC/C1INA" pad="7"/>
<connect gate="IC" pin="RB4/CN1/SOSCI/!U2RTS!/U2BCLK" pad="11"/>
<connect gate="IC" pin="RB5/CN27/PGD3/SDA1" pad="14"/>
<connect gate="IC" pin="REFO/!SS1!/T2CK/T3CK/CN11/RB15" pad="26"/>
<connect gate="IC" pin="SCK1/PGC2/CN15/RB11" pad="22"/>
<connect gate="IC" pin="SCL1/PGC3/CN24/RB6" pad="15"/>
<connect gate="IC" pin="SDI1/PMD2/PGD2/CN16/RB10" pad="21"/>
<connect gate="IC" pin="SDO1/CTPLS/CN13/AN11/RB13" pad="24"/>
<connect gate="IC" pin="U1TX/INT0/CN23/RB7" pad="16"/>
<connect gate="IC" pin="VDD@1" pad="13"/>
<connect gate="IC" pin="VDD@2" pad="28"/>
<connect gate="IC" pin="VSS@1" pad="8"/>
<connect gate="IC" pin="VSS@2" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOIC" package="SOIC-28W">
<connects>
<connect gate="IC" pin="!U1CTS!/SCL1/CN22/RB8" pad="17"/>
<connect gate="IC" pin="!U1RTS!/U1BCLK/SDA1/CN21/RB9" pad="18"/>
<connect gate="IC" pin="HLVDIN/CTED2/CN14/AN12/RB12" pad="23"/>
<connect gate="IC" pin="IC1/CN9/RA7" pad="19"/>
<connect gate="IC" pin="OC1/C2OUT/INT2/CTED1/CN8/RA6" pad="20"/>
<connect gate="IC" pin="OCFA/C1OUT/RTCC/CVREF/CN12/AN10/RB14" pad="25"/>
<connect gate="IC" pin="RA0/AN0/CN2/VREF+" pad="2"/>
<connect gate="IC" pin="RA1/AN1/CN3/VREF-" pad="3"/>
<connect gate="IC" pin="RA2/CN30/OSCI/CLKI" pad="9"/>
<connect gate="IC" pin="RA3/CN29/OSCO/CLKO" pad="10"/>
<connect gate="IC" pin="RA4/CN0/SOSCO/T1CK/!U2CTS!" pad="12"/>
<connect gate="IC" pin="RA5/!MCLR!/VPP" pad="1"/>
<connect gate="IC" pin="RB0/AN2/CN4/C2INB/C1IND/PGD1/U2TX" pad="4"/>
<connect gate="IC" pin="RB1/AN3/CN5/C2INA/C1INC/PGC1/U2RX" pad="5"/>
<connect gate="IC" pin="RB2/AN4/CN6/C2IND/C1INB/U1RX" pad="6"/>
<connect gate="IC" pin="RB3/AN5/CN7/C2INC/C1INA" pad="7"/>
<connect gate="IC" pin="RB4/CN1/SOSCI/!U2RTS!/U2BCLK" pad="11"/>
<connect gate="IC" pin="RB5/CN27/PGD3/SDA1" pad="14"/>
<connect gate="IC" pin="REFO/!SS1!/T2CK/T3CK/CN11/RB15" pad="26"/>
<connect gate="IC" pin="SCK1/PGC2/CN15/RB11" pad="22"/>
<connect gate="IC" pin="SCL1/PGC3/CN24/RB6" pad="15"/>
<connect gate="IC" pin="SDI1/PMD2/PGD2/CN16/RB10" pad="21"/>
<connect gate="IC" pin="SDO1/CTPLS/CN13/AN11/RB13" pad="24"/>
<connect gate="IC" pin="U1TX/INT0/CN23/RB7" pad="16"/>
<connect gate="IC" pin="VDD@1" pad="13"/>
<connect gate="IC" pin="VDD@2" pad="28"/>
<connect gate="IC" pin="VSS@1" pad="8"/>
<connect gate="IC" pin="VSS@2" pad="27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_MICROSD">
<gates>
<gate name="CON" symbol="CON_MICROSD"/>
</gates>
<devices>
<device name="HINGED" package="CON_MICROSD_HINGED">
<connects>
<connect gate="CON" pin="CD/DAT3" pad="2"/>
<connect gate="CON" pin="CLK" pad="5"/>
<connect gate="CON" pin="CMD" pad="3"/>
<connect gate="CON" pin="DAT0" pad="7"/>
<connect gate="CON" pin="DAT1" pad="8"/>
<connect gate="CON" pin="DAT2" pad="1"/>
<connect gate="CON" pin="VDD" pad="4"/>
<connect gate="CON" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER_SOLDER_1X2" prefix="J">
<gates>
<gate name="J" symbol="JUMP_SOLDER_1X2"/>
</gates>
<devices>
<device name="" package="JUMPER_SOLDER_1X2">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_DIL28" prefix="IC">
<description>universal DIP-28</description>
<gates>
<gate name="IC" symbol="DIL-28"/>
</gates>
<devices>
<device name="-DIL28-SMD" package="DIL28-SMD">
<connects>
<connect gate="IC" pin="1" pad="1"/>
<connect gate="IC" pin="10" pad="10"/>
<connect gate="IC" pin="11" pad="11"/>
<connect gate="IC" pin="12" pad="12"/>
<connect gate="IC" pin="13" pad="13"/>
<connect gate="IC" pin="14" pad="14"/>
<connect gate="IC" pin="15" pad="15"/>
<connect gate="IC" pin="16" pad="16"/>
<connect gate="IC" pin="17" pad="17"/>
<connect gate="IC" pin="18" pad="18"/>
<connect gate="IC" pin="19" pad="19"/>
<connect gate="IC" pin="2" pad="2"/>
<connect gate="IC" pin="20" pad="20"/>
<connect gate="IC" pin="21" pad="21"/>
<connect gate="IC" pin="22" pad="22"/>
<connect gate="IC" pin="23" pad="23"/>
<connect gate="IC" pin="24" pad="24"/>
<connect gate="IC" pin="25" pad="25"/>
<connect gate="IC" pin="26" pad="26"/>
<connect gate="IC" pin="27" pad="27"/>
<connect gate="IC" pin="28" pad="28"/>
<connect gate="IC" pin="3" pad="3"/>
<connect gate="IC" pin="4" pad="4"/>
<connect gate="IC" pin="5" pad="5"/>
<connect gate="IC" pin="6" pad="6"/>
<connect gate="IC" pin="7" pad="7"/>
<connect gate="IC" pin="8" pad="8"/>
<connect gate="IC" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_TACT_4P_B" prefix="SW">
<gates>
<gate name="SW" symbol="SWITCH_3"/>
</gates>
<devices>
<device name="" package="SW_TACT_STANDARD_RIGHT_ANGLE">
<connects>
<connect gate="SW" pin="1" pad="1"/>
<connect gate="SW" pin="2" pad="2"/>
<connect gate="SW" pin="3" pad="3"/>
<connect gate="SW" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB_XQFP_050">
<gates>
<gate name="G$1" symbol="BB_XQFP_050"/>
</gates>
<devices>
<device name="" package="BB_QFP_050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="73" pad="73"/>
<connect gate="G$1" pin="74" pad="74"/>
<connect gate="G$1" pin="75" pad="75"/>
<connect gate="G$1" pin="76" pad="76"/>
<connect gate="G$1" pin="77" pad="77"/>
<connect gate="G$1" pin="78" pad="78"/>
<connect gate="G$1" pin="79" pad="79"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="80" pad="80"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BB" package="BB_QFP_050_BREAKOUT_BOARD">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="13" pad="P$13"/>
<connect gate="G$1" pin="14" pad="P$14"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="19" pad="P$19"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="20" pad="P$20"/>
<connect gate="G$1" pin="21" pad="P$21"/>
<connect gate="G$1" pin="22" pad="P$22"/>
<connect gate="G$1" pin="23" pad="P$23"/>
<connect gate="G$1" pin="24" pad="P$24"/>
<connect gate="G$1" pin="25" pad="P$25"/>
<connect gate="G$1" pin="26" pad="P$26"/>
<connect gate="G$1" pin="27" pad="P$27"/>
<connect gate="G$1" pin="28" pad="P$28"/>
<connect gate="G$1" pin="29" pad="P$29"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="30" pad="P$30"/>
<connect gate="G$1" pin="31" pad="P$31"/>
<connect gate="G$1" pin="32" pad="P$32"/>
<connect gate="G$1" pin="33" pad="P$33"/>
<connect gate="G$1" pin="34" pad="P$34"/>
<connect gate="G$1" pin="35" pad="P$35"/>
<connect gate="G$1" pin="36" pad="P$36"/>
<connect gate="G$1" pin="37" pad="P$37"/>
<connect gate="G$1" pin="38" pad="P$38"/>
<connect gate="G$1" pin="39" pad="P$39"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="40" pad="P$40"/>
<connect gate="G$1" pin="41" pad="P$41"/>
<connect gate="G$1" pin="42" pad="P$42"/>
<connect gate="G$1" pin="43" pad="P$43"/>
<connect gate="G$1" pin="44" pad="P$44"/>
<connect gate="G$1" pin="45" pad="P$45"/>
<connect gate="G$1" pin="46" pad="P$46"/>
<connect gate="G$1" pin="47" pad="P$47"/>
<connect gate="G$1" pin="48" pad="P$48"/>
<connect gate="G$1" pin="49" pad="P$49"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="50" pad="P$50"/>
<connect gate="G$1" pin="51" pad="P$51"/>
<connect gate="G$1" pin="52" pad="P$52"/>
<connect gate="G$1" pin="53" pad="P$53"/>
<connect gate="G$1" pin="54" pad="P$54"/>
<connect gate="G$1" pin="55" pad="P$55"/>
<connect gate="G$1" pin="56" pad="P$56"/>
<connect gate="G$1" pin="57" pad="P$57"/>
<connect gate="G$1" pin="58" pad="P$58"/>
<connect gate="G$1" pin="59" pad="P$59"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="60" pad="P$60"/>
<connect gate="G$1" pin="61" pad="P$61"/>
<connect gate="G$1" pin="62" pad="P$62"/>
<connect gate="G$1" pin="63" pad="P$63"/>
<connect gate="G$1" pin="64" pad="P$64"/>
<connect gate="G$1" pin="65" pad="P$65"/>
<connect gate="G$1" pin="66" pad="P$66"/>
<connect gate="G$1" pin="67" pad="P$67"/>
<connect gate="G$1" pin="68" pad="P$68"/>
<connect gate="G$1" pin="69" pad="P$69"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="70" pad="P$70"/>
<connect gate="G$1" pin="71" pad="P$71"/>
<connect gate="G$1" pin="72" pad="P$72"/>
<connect gate="G$1" pin="73" pad="P$73"/>
<connect gate="G$1" pin="74" pad="P$74"/>
<connect gate="G$1" pin="75" pad="P$75"/>
<connect gate="G$1" pin="76" pad="P$76"/>
<connect gate="G$1" pin="77" pad="P$77"/>
<connect gate="G$1" pin="78" pad="P$78"/>
<connect gate="G$1" pin="79" pad="P$79"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="80" pad="P$80"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB_XQFP_065">
<gates>
<gate name="G$1" symbol="BB_XQFP_065"/>
</gates>
<devices>
<device name="" package="BB_QFP_065">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="73" pad="73"/>
<connect gate="G$1" pin="74" pad="74"/>
<connect gate="G$1" pin="75" pad="75"/>
<connect gate="G$1" pin="76" pad="76"/>
<connect gate="G$1" pin="77" pad="77"/>
<connect gate="G$1" pin="78" pad="78"/>
<connect gate="G$1" pin="79" pad="79"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="80" pad="80"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BB" package="BB_QFP_065_BREAKOUT_BOARD">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="13" pad="P$13"/>
<connect gate="G$1" pin="14" pad="P$14"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="19" pad="P$19"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="20" pad="P$20"/>
<connect gate="G$1" pin="21" pad="P$21"/>
<connect gate="G$1" pin="22" pad="P$22"/>
<connect gate="G$1" pin="23" pad="P$23"/>
<connect gate="G$1" pin="24" pad="P$24"/>
<connect gate="G$1" pin="25" pad="P$25"/>
<connect gate="G$1" pin="26" pad="P$26"/>
<connect gate="G$1" pin="27" pad="P$27"/>
<connect gate="G$1" pin="28" pad="P$28"/>
<connect gate="G$1" pin="29" pad="P$29"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="30" pad="P$30"/>
<connect gate="G$1" pin="31" pad="P$31"/>
<connect gate="G$1" pin="32" pad="P$32"/>
<connect gate="G$1" pin="33" pad="P$33"/>
<connect gate="G$1" pin="34" pad="P$34"/>
<connect gate="G$1" pin="35" pad="P$35"/>
<connect gate="G$1" pin="36" pad="P$36"/>
<connect gate="G$1" pin="37" pad="P$37"/>
<connect gate="G$1" pin="38" pad="P$38"/>
<connect gate="G$1" pin="39" pad="P$39"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="40" pad="P$40"/>
<connect gate="G$1" pin="41" pad="P$41"/>
<connect gate="G$1" pin="42" pad="P$42"/>
<connect gate="G$1" pin="43" pad="P$43"/>
<connect gate="G$1" pin="44" pad="P$44"/>
<connect gate="G$1" pin="45" pad="P$45"/>
<connect gate="G$1" pin="46" pad="P$46"/>
<connect gate="G$1" pin="47" pad="P$47"/>
<connect gate="G$1" pin="48" pad="P$48"/>
<connect gate="G$1" pin="49" pad="P$49"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="50" pad="P$50"/>
<connect gate="G$1" pin="51" pad="P$51"/>
<connect gate="G$1" pin="52" pad="P$52"/>
<connect gate="G$1" pin="53" pad="P$53"/>
<connect gate="G$1" pin="54" pad="P$54"/>
<connect gate="G$1" pin="55" pad="P$55"/>
<connect gate="G$1" pin="56" pad="P$56"/>
<connect gate="G$1" pin="57" pad="P$57"/>
<connect gate="G$1" pin="58" pad="P$58"/>
<connect gate="G$1" pin="59" pad="P$59"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="60" pad="P$60"/>
<connect gate="G$1" pin="61" pad="P$61"/>
<connect gate="G$1" pin="62" pad="P$62"/>
<connect gate="G$1" pin="63" pad="P$63"/>
<connect gate="G$1" pin="64" pad="P$64"/>
<connect gate="G$1" pin="65" pad="P$65"/>
<connect gate="G$1" pin="66" pad="P$66"/>
<connect gate="G$1" pin="67" pad="P$67"/>
<connect gate="G$1" pin="68" pad="P$68"/>
<connect gate="G$1" pin="69" pad="P$69"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="70" pad="P$70"/>
<connect gate="G$1" pin="71" pad="P$71"/>
<connect gate="G$1" pin="72" pad="P$72"/>
<connect gate="G$1" pin="73" pad="P$73"/>
<connect gate="G$1" pin="74" pad="P$74"/>
<connect gate="G$1" pin="75" pad="P$75"/>
<connect gate="G$1" pin="76" pad="P$76"/>
<connect gate="G$1" pin="77" pad="P$77"/>
<connect gate="G$1" pin="78" pad="P$78"/>
<connect gate="G$1" pin="79" pad="P$79"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="80" pad="P$80"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB_XQFP_080">
<gates>
<gate name="G$1" symbol="BB_XQFP_080"/>
</gates>
<devices>
<device name="" package="BB_QFP_080">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="53" pad="53"/>
<connect gate="G$1" pin="54" pad="54"/>
<connect gate="G$1" pin="55" pad="55"/>
<connect gate="G$1" pin="56" pad="56"/>
<connect gate="G$1" pin="57" pad="57"/>
<connect gate="G$1" pin="58" pad="58"/>
<connect gate="G$1" pin="59" pad="59"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="60" pad="60"/>
<connect gate="G$1" pin="61" pad="61"/>
<connect gate="G$1" pin="62" pad="62"/>
<connect gate="G$1" pin="63" pad="63"/>
<connect gate="G$1" pin="64" pad="64"/>
<connect gate="G$1" pin="65" pad="65"/>
<connect gate="G$1" pin="66" pad="66"/>
<connect gate="G$1" pin="67" pad="67"/>
<connect gate="G$1" pin="68" pad="68"/>
<connect gate="G$1" pin="69" pad="69"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="70" pad="70"/>
<connect gate="G$1" pin="71" pad="71"/>
<connect gate="G$1" pin="72" pad="72"/>
<connect gate="G$1" pin="73" pad="73"/>
<connect gate="G$1" pin="74" pad="74"/>
<connect gate="G$1" pin="75" pad="75"/>
<connect gate="G$1" pin="76" pad="76"/>
<connect gate="G$1" pin="77" pad="77"/>
<connect gate="G$1" pin="78" pad="78"/>
<connect gate="G$1" pin="79" pad="79"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="80" pad="80"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BB" package="BB_QFP_080_BREAKOUT_BOARD">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="13" pad="P$13"/>
<connect gate="G$1" pin="14" pad="P$14"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="19" pad="P$19"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="20" pad="P$20"/>
<connect gate="G$1" pin="21" pad="P$21"/>
<connect gate="G$1" pin="22" pad="P$22"/>
<connect gate="G$1" pin="23" pad="P$23"/>
<connect gate="G$1" pin="24" pad="P$24"/>
<connect gate="G$1" pin="25" pad="P$25"/>
<connect gate="G$1" pin="26" pad="P$26"/>
<connect gate="G$1" pin="27" pad="P$27"/>
<connect gate="G$1" pin="28" pad="P$28"/>
<connect gate="G$1" pin="29" pad="P$29"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="30" pad="P$30"/>
<connect gate="G$1" pin="31" pad="P$31"/>
<connect gate="G$1" pin="32" pad="P$32"/>
<connect gate="G$1" pin="33" pad="P$33"/>
<connect gate="G$1" pin="34" pad="P$34"/>
<connect gate="G$1" pin="35" pad="P$35"/>
<connect gate="G$1" pin="36" pad="P$36"/>
<connect gate="G$1" pin="37" pad="P$37"/>
<connect gate="G$1" pin="38" pad="P$38"/>
<connect gate="G$1" pin="39" pad="P$39"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="40" pad="P$40"/>
<connect gate="G$1" pin="41" pad="P$41"/>
<connect gate="G$1" pin="42" pad="P$42"/>
<connect gate="G$1" pin="43" pad="P$43"/>
<connect gate="G$1" pin="44" pad="P$44"/>
<connect gate="G$1" pin="45" pad="P$45"/>
<connect gate="G$1" pin="46" pad="P$46"/>
<connect gate="G$1" pin="47" pad="P$47"/>
<connect gate="G$1" pin="48" pad="P$48"/>
<connect gate="G$1" pin="49" pad="P$49"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="50" pad="P$50"/>
<connect gate="G$1" pin="51" pad="P$51"/>
<connect gate="G$1" pin="52" pad="P$52"/>
<connect gate="G$1" pin="53" pad="P$53"/>
<connect gate="G$1" pin="54" pad="P$54"/>
<connect gate="G$1" pin="55" pad="P$55"/>
<connect gate="G$1" pin="56" pad="P$56"/>
<connect gate="G$1" pin="57" pad="P$57"/>
<connect gate="G$1" pin="58" pad="P$58"/>
<connect gate="G$1" pin="59" pad="P$59"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="60" pad="P$60"/>
<connect gate="G$1" pin="61" pad="P$61"/>
<connect gate="G$1" pin="62" pad="P$62"/>
<connect gate="G$1" pin="63" pad="P$63"/>
<connect gate="G$1" pin="64" pad="P$64"/>
<connect gate="G$1" pin="65" pad="P$65"/>
<connect gate="G$1" pin="66" pad="P$66"/>
<connect gate="G$1" pin="67" pad="P$67"/>
<connect gate="G$1" pin="68" pad="P$68"/>
<connect gate="G$1" pin="69" pad="P$69"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="70" pad="P$70"/>
<connect gate="G$1" pin="71" pad="P$71"/>
<connect gate="G$1" pin="72" pad="P$72"/>
<connect gate="G$1" pin="73" pad="P$73"/>
<connect gate="G$1" pin="74" pad="P$74"/>
<connect gate="G$1" pin="75" pad="P$75"/>
<connect gate="G$1" pin="76" pad="P$76"/>
<connect gate="G$1" pin="77" pad="P$77"/>
<connect gate="G$1" pin="78" pad="P$78"/>
<connect gate="G$1" pin="79" pad="P$79"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="80" pad="P$80"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON_SOLO_STACKER_6" prefix="J">
<description>SOLO Staggard Stocker
&lt;br&gt; Mfr no: 009188006020062
&lt;br&gt; &lt;a href="http://www.digikey.com/product-detail/en/009188006020062/478-5491-1-ND/2024954?cur=USD"&gt;  009188006020062&lt;/a&gt;</description>
<gates>
<gate name="J" symbol="HEADER2X3"/>
</gates>
<devices>
<device name="-FOOTPRINT" package="CON_SOLO_STACKER_6_FOOTPRINT">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CONNECTOR" package="CON_SOLO_STACKER_6_CONNECTOR">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB_XQFP_050_065" prefix="IC">
<gates>
<gate name="IC" symbol="BB_XQFP_050_065"/>
</gates>
<devices>
<device name="" package="BB_QFP_050_065_BREAKOUT_BOARD">
<connects>
<connect gate="IC" pin="1" pad="1"/>
<connect gate="IC" pin="10" pad="10"/>
<connect gate="IC" pin="11" pad="11"/>
<connect gate="IC" pin="12" pad="12"/>
<connect gate="IC" pin="13" pad="13"/>
<connect gate="IC" pin="14" pad="14"/>
<connect gate="IC" pin="15" pad="15"/>
<connect gate="IC" pin="16" pad="16"/>
<connect gate="IC" pin="17" pad="17"/>
<connect gate="IC" pin="18" pad="18"/>
<connect gate="IC" pin="19" pad="19"/>
<connect gate="IC" pin="2" pad="2"/>
<connect gate="IC" pin="20" pad="20"/>
<connect gate="IC" pin="21" pad="21"/>
<connect gate="IC" pin="22" pad="22"/>
<connect gate="IC" pin="23" pad="23"/>
<connect gate="IC" pin="24" pad="24"/>
<connect gate="IC" pin="25" pad="25"/>
<connect gate="IC" pin="26" pad="26"/>
<connect gate="IC" pin="27" pad="27"/>
<connect gate="IC" pin="28" pad="28"/>
<connect gate="IC" pin="29" pad="29"/>
<connect gate="IC" pin="3" pad="3"/>
<connect gate="IC" pin="30" pad="30"/>
<connect gate="IC" pin="31" pad="31"/>
<connect gate="IC" pin="32" pad="32"/>
<connect gate="IC" pin="33" pad="33"/>
<connect gate="IC" pin="34" pad="34"/>
<connect gate="IC" pin="35" pad="35"/>
<connect gate="IC" pin="36" pad="36"/>
<connect gate="IC" pin="37" pad="37"/>
<connect gate="IC" pin="38" pad="38"/>
<connect gate="IC" pin="39" pad="39"/>
<connect gate="IC" pin="4" pad="4"/>
<connect gate="IC" pin="40" pad="40"/>
<connect gate="IC" pin="41" pad="41"/>
<connect gate="IC" pin="42" pad="42"/>
<connect gate="IC" pin="43" pad="43"/>
<connect gate="IC" pin="44" pad="44"/>
<connect gate="IC" pin="45" pad="45"/>
<connect gate="IC" pin="46" pad="46"/>
<connect gate="IC" pin="47" pad="47"/>
<connect gate="IC" pin="48" pad="48"/>
<connect gate="IC" pin="49" pad="49"/>
<connect gate="IC" pin="5" pad="5"/>
<connect gate="IC" pin="50" pad="50"/>
<connect gate="IC" pin="51" pad="51"/>
<connect gate="IC" pin="52" pad="52"/>
<connect gate="IC" pin="53" pad="53"/>
<connect gate="IC" pin="54" pad="54"/>
<connect gate="IC" pin="55" pad="55"/>
<connect gate="IC" pin="56" pad="56"/>
<connect gate="IC" pin="57" pad="57"/>
<connect gate="IC" pin="58" pad="58"/>
<connect gate="IC" pin="59" pad="59"/>
<connect gate="IC" pin="6" pad="6"/>
<connect gate="IC" pin="60" pad="60"/>
<connect gate="IC" pin="61" pad="61"/>
<connect gate="IC" pin="62" pad="62"/>
<connect gate="IC" pin="63" pad="63"/>
<connect gate="IC" pin="64" pad="64"/>
<connect gate="IC" pin="65" pad="65"/>
<connect gate="IC" pin="66" pad="66"/>
<connect gate="IC" pin="67" pad="67"/>
<connect gate="IC" pin="68" pad="68"/>
<connect gate="IC" pin="69" pad="69"/>
<connect gate="IC" pin="7" pad="7"/>
<connect gate="IC" pin="70" pad="70"/>
<connect gate="IC" pin="71" pad="71"/>
<connect gate="IC" pin="72" pad="72"/>
<connect gate="IC" pin="73" pad="73"/>
<connect gate="IC" pin="74" pad="74"/>
<connect gate="IC" pin="75" pad="75"/>
<connect gate="IC" pin="76" pad="76"/>
<connect gate="IC" pin="77" pad="77"/>
<connect gate="IC" pin="78" pad="78"/>
<connect gate="IC" pin="79" pad="79"/>
<connect gate="IC" pin="8" pad="8"/>
<connect gate="IC" pin="80" pad="80"/>
<connect gate="IC" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB_XQFP_050_080" prefix="IC">
<gates>
<gate name="IC" symbol="BB_XQFP_050_080"/>
</gates>
<devices>
<device name="" package="BB_QFP_080_050_BREAKOUT_BOARD">
<connects>
<connect gate="IC" pin="1" pad="1"/>
<connect gate="IC" pin="10" pad="10"/>
<connect gate="IC" pin="11" pad="11"/>
<connect gate="IC" pin="12" pad="12"/>
<connect gate="IC" pin="13" pad="13"/>
<connect gate="IC" pin="14" pad="14"/>
<connect gate="IC" pin="15" pad="15"/>
<connect gate="IC" pin="16" pad="16"/>
<connect gate="IC" pin="17" pad="17"/>
<connect gate="IC" pin="18" pad="18"/>
<connect gate="IC" pin="19" pad="19"/>
<connect gate="IC" pin="2" pad="2"/>
<connect gate="IC" pin="20" pad="20"/>
<connect gate="IC" pin="21" pad="21"/>
<connect gate="IC" pin="22" pad="22"/>
<connect gate="IC" pin="23" pad="23"/>
<connect gate="IC" pin="24" pad="24"/>
<connect gate="IC" pin="25" pad="25"/>
<connect gate="IC" pin="26" pad="26"/>
<connect gate="IC" pin="27" pad="27"/>
<connect gate="IC" pin="28" pad="28"/>
<connect gate="IC" pin="29" pad="29"/>
<connect gate="IC" pin="3" pad="3"/>
<connect gate="IC" pin="30" pad="30"/>
<connect gate="IC" pin="31" pad="31"/>
<connect gate="IC" pin="32" pad="32"/>
<connect gate="IC" pin="33" pad="33"/>
<connect gate="IC" pin="34" pad="34"/>
<connect gate="IC" pin="35" pad="35"/>
<connect gate="IC" pin="36" pad="36"/>
<connect gate="IC" pin="37" pad="37"/>
<connect gate="IC" pin="38" pad="38"/>
<connect gate="IC" pin="39" pad="39"/>
<connect gate="IC" pin="4" pad="4"/>
<connect gate="IC" pin="40" pad="40"/>
<connect gate="IC" pin="41" pad="41"/>
<connect gate="IC" pin="42" pad="42"/>
<connect gate="IC" pin="43" pad="43"/>
<connect gate="IC" pin="44" pad="44"/>
<connect gate="IC" pin="45" pad="45"/>
<connect gate="IC" pin="46" pad="46"/>
<connect gate="IC" pin="47" pad="47"/>
<connect gate="IC" pin="48" pad="48"/>
<connect gate="IC" pin="49" pad="49"/>
<connect gate="IC" pin="5" pad="5"/>
<connect gate="IC" pin="50" pad="50"/>
<connect gate="IC" pin="51" pad="51"/>
<connect gate="IC" pin="52" pad="52"/>
<connect gate="IC" pin="53" pad="53"/>
<connect gate="IC" pin="54" pad="54"/>
<connect gate="IC" pin="55" pad="55"/>
<connect gate="IC" pin="56" pad="56"/>
<connect gate="IC" pin="57" pad="57"/>
<connect gate="IC" pin="58" pad="58"/>
<connect gate="IC" pin="59" pad="59"/>
<connect gate="IC" pin="6" pad="6"/>
<connect gate="IC" pin="60" pad="60"/>
<connect gate="IC" pin="61" pad="61"/>
<connect gate="IC" pin="62" pad="62"/>
<connect gate="IC" pin="63" pad="63"/>
<connect gate="IC" pin="64" pad="64"/>
<connect gate="IC" pin="65" pad="65"/>
<connect gate="IC" pin="66" pad="66"/>
<connect gate="IC" pin="67" pad="67"/>
<connect gate="IC" pin="68" pad="68"/>
<connect gate="IC" pin="69" pad="69"/>
<connect gate="IC" pin="7" pad="7"/>
<connect gate="IC" pin="70" pad="70"/>
<connect gate="IC" pin="71" pad="71"/>
<connect gate="IC" pin="72" pad="72"/>
<connect gate="IC" pin="73" pad="73"/>
<connect gate="IC" pin="74" pad="74"/>
<connect gate="IC" pin="75" pad="75"/>
<connect gate="IC" pin="76" pad="76"/>
<connect gate="IC" pin="77" pad="77"/>
<connect gate="IC" pin="78" pad="78"/>
<connect gate="IC" pin="79" pad="79"/>
<connect gate="IC" pin="8" pad="8"/>
<connect gate="IC" pin="80" pad="80"/>
<connect gate="IC" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BB_XQFP_080_065" prefix="IC">
<gates>
<gate name="IC" symbol="BB_XQFP_080_065"/>
</gates>
<devices>
<device name="" package="BB_QFP_080_065_BREAKOUT_BOARD">
<connects>
<connect gate="IC" pin="1" pad="1"/>
<connect gate="IC" pin="10" pad="10"/>
<connect gate="IC" pin="11" pad="11"/>
<connect gate="IC" pin="12" pad="12"/>
<connect gate="IC" pin="13" pad="13"/>
<connect gate="IC" pin="14" pad="14"/>
<connect gate="IC" pin="15" pad="15"/>
<connect gate="IC" pin="16" pad="16"/>
<connect gate="IC" pin="17" pad="17"/>
<connect gate="IC" pin="18" pad="18"/>
<connect gate="IC" pin="19" pad="19"/>
<connect gate="IC" pin="2" pad="2"/>
<connect gate="IC" pin="20" pad="20"/>
<connect gate="IC" pin="21" pad="21"/>
<connect gate="IC" pin="22" pad="22"/>
<connect gate="IC" pin="23" pad="23"/>
<connect gate="IC" pin="24" pad="24"/>
<connect gate="IC" pin="25" pad="25"/>
<connect gate="IC" pin="26" pad="26"/>
<connect gate="IC" pin="27" pad="27"/>
<connect gate="IC" pin="28" pad="28"/>
<connect gate="IC" pin="29" pad="29"/>
<connect gate="IC" pin="3" pad="3"/>
<connect gate="IC" pin="30" pad="30"/>
<connect gate="IC" pin="31" pad="31"/>
<connect gate="IC" pin="32" pad="32"/>
<connect gate="IC" pin="33" pad="33"/>
<connect gate="IC" pin="34" pad="34"/>
<connect gate="IC" pin="35" pad="35"/>
<connect gate="IC" pin="36" pad="36"/>
<connect gate="IC" pin="37" pad="37"/>
<connect gate="IC" pin="38" pad="38"/>
<connect gate="IC" pin="39" pad="39"/>
<connect gate="IC" pin="4" pad="4"/>
<connect gate="IC" pin="40" pad="40"/>
<connect gate="IC" pin="41" pad="41"/>
<connect gate="IC" pin="42" pad="42"/>
<connect gate="IC" pin="43" pad="43"/>
<connect gate="IC" pin="44" pad="44"/>
<connect gate="IC" pin="45" pad="45"/>
<connect gate="IC" pin="46" pad="46"/>
<connect gate="IC" pin="47" pad="47"/>
<connect gate="IC" pin="48" pad="48"/>
<connect gate="IC" pin="49" pad="49"/>
<connect gate="IC" pin="5" pad="5"/>
<connect gate="IC" pin="50" pad="50"/>
<connect gate="IC" pin="51" pad="51"/>
<connect gate="IC" pin="52" pad="52"/>
<connect gate="IC" pin="53" pad="53"/>
<connect gate="IC" pin="54" pad="54"/>
<connect gate="IC" pin="55" pad="55"/>
<connect gate="IC" pin="56" pad="56"/>
<connect gate="IC" pin="57" pad="57"/>
<connect gate="IC" pin="58" pad="58"/>
<connect gate="IC" pin="59" pad="59"/>
<connect gate="IC" pin="6" pad="6"/>
<connect gate="IC" pin="60" pad="60"/>
<connect gate="IC" pin="61" pad="61"/>
<connect gate="IC" pin="62" pad="62"/>
<connect gate="IC" pin="63" pad="63"/>
<connect gate="IC" pin="64" pad="64"/>
<connect gate="IC" pin="65" pad="65"/>
<connect gate="IC" pin="66" pad="66"/>
<connect gate="IC" pin="67" pad="67"/>
<connect gate="IC" pin="68" pad="68"/>
<connect gate="IC" pin="69" pad="69"/>
<connect gate="IC" pin="7" pad="7"/>
<connect gate="IC" pin="70" pad="70"/>
<connect gate="IC" pin="71" pad="71"/>
<connect gate="IC" pin="72" pad="72"/>
<connect gate="IC" pin="73" pad="73"/>
<connect gate="IC" pin="74" pad="74"/>
<connect gate="IC" pin="75" pad="75"/>
<connect gate="IC" pin="76" pad="76"/>
<connect gate="IC" pin="77" pad="77"/>
<connect gate="IC" pin="78" pad="78"/>
<connect gate="IC" pin="79" pad="79"/>
<connect gate="IC" pin="8" pad="8"/>
<connect gate="IC" pin="80" pad="80"/>
<connect gate="IC" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PROTO_VIAS_01X01" prefix="P">
<description>Single Pad for Protoboard Filling</description>
<gates>
<gate name="P" symbol="HEADER1X1"/>
</gates>
<devices>
<device name="" package="PROTO_VIAS_01X01">
<connects>
<connect gate="P" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
