{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Roland+memser","Sheet2"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Roland+memser","index":0,"n_rows":60,"n_cols":12,"rows_kept":60,"flags":["formulas_cached_only"]}
[1,"SW_DIP-8","SW_DIP-8","EDG-08","32KOmnibus",null,"S1","DIP SWITCH"]
[2,"100K","R-US_0207/10","0207/10","32KOmnibus",null,"R15, R24","RESISTOR, American symbol"]
[13,"100nF","C-US050-025X075","C050-025X075","32KOmnibus",null,"C1, C2, C3, C4, C5, C6, C8, C10, C11, C12, C13, C14, C15, C16, C17, C18, C19, C20, C21, C23, C24, C25, C26, C27, C28, C29, C31, C32, C33, C36, C37","CAPACITOR, American symbol"]
[1,"10K","8R-P","DIL16","32KOmnibus",null,"R23","DIL RESISTOR"]
[1,"200pF","C-US050-025X075","C050-025X075","32KOmnibus",null,"C22","CAPACITOR, American symbol"]
[1,"2N3904","2N3904","TO92","32KOmnibus",null,"Q3","NPN TRANSISTOR"]
[2,"5K","G08R","SIL9","32KOmnibus",null,"RN1, RN2","SIL RESISTOR","unknown","unknown"]
[7,"14 Pin DIP Socket","575-199314","DIL14","32KOmnibus"]
[2,"16 Pin DIP Socket","575-199316","DIL16","32KOmnibus"]
[3,"20 Pin DIP Socket","575-199320","DIL20","32KOmnibus"]
[2,"28 Pin Wide DIP Socket","575-199628","DIL28-6","32KOmnibus"]
[2,"28 Pin Narrow DIP Socket","575-199328","DIL28-3","32KOmnibus"]
[1,"74LS10N","74LS10N","DIL14","32KOmnibus",null,"E8","Triple 3-input NAND gate"]
[1,"74LS151N","74LS151N","DIL16","32KOmnibus",null,"E9","Data SELECTOR/MULTIPLEXER"]
[2,"74LS244N","74LS244N","DIL20","32KOmnibus",null,"E1, E7","Octal BUFFER and LINE DRIVER, 3-state"]
[6,"74LS38N","74LS38N","DIL14","32KOmnibus",null,"E3, E4, E10, E11, E12, E13","Quad 2-input NAND gate, open collector output"]
[1,"74LS540N","74LS540N","DIL20","32KOmnibus",null,"E6","Octal BUFFER and LINE DRIVER, 3-state"]
[2,"BAT86","BAT19","DO35-10","32KOmnibus",null,"D2, D3","DIODE"]
[1,"CR2032","B2430UNI","B2430UNI","32KOmnibus",null,"B1","LI BATTERY"]
[1,"CR2032 Socket","534-1066",1066,"32KOmnibus"]
[2,62256,"58C256P","DIL28-6","32KOmnibus","Stock","E2, E5","MEMORY"]
[2,62256,"62832P","DIL28-3","32KOmnibus","Stock","E2A, E5A","MEMORY","unknown","unknown"]
[3,"6.8uF","CPOL-USE20-8AXIAL","E12-8","Board","Stock","C30, C34, C35","A 0.8 inch electrolytic."]
[1,"PCB","QUAD","EDGE-CON8","Board","Stock","J1","Quad-Height DEC board"]
[1,"ML10","ML10","ML10","CPLDSerial",null,"SV2","HARTING","unknown","unknown"]
[5,"0.22uF","C-US","C063-025X075","CPLDSerial",null,"C41, C42, C43, C44, C45","Capacitors with funky DEC lead spacing."]
[1,"19.661 MHz","QG5460","DIL08S","CPLDSerial",null,"OSC","CRYSTAL RESONATOR","unknown","unknown"]
[1,"47K","G10R","SIL11","CPLDSerial",null,"RN3","SIL RESISTOR","unknown","unknown"]
[1,"ATF150X84","ATF150X84","PLCC84","CPLDSerial",null,"E14","ATF150x in 84 pin package."]
[1,"PCLCC84 Socket","ATF150X84","S84","CPLDSerial",null,"E14"]
[1,"CONF","DP06","DP-06","CPLDSerial",null,"SERIAL","DIL/CODE SWITCH","MCDP06",9471618,"26M1097"]
[1,"D-SUB9-HM","DB9-USB-M","H5M09RA","CPLDSerial",null,"J5","D-Subminiatur Connector","unknown","unknown"]
[1,"M837","9070-1W","9070-1W","CPLDSerial",null,"TS_DISABLE","TOGGLE SWITCH"]
[1,"MAX232","MAX232","DIL16","CPLDSerial",null,"U10","RS232 TRANSCEIVER","MAXIM","MAX232ACPE+",9723773,"68K4544"]
[1,"Serial","DEC40PINH","DEC40PINH","CPLDSerial",null,"J4","PIN HEADER"]
[1,"COMM","MA04-1","MA04-1","CPLDSerial","Stock","J2","PIN HEADER","unknown","unknown"]
[1,"ICSP","MA03-2","MA03-2","CPLDSerial","Stock","J3","PIN HEADER","unknown","unknown"]
["Qty","Value","Device","Package","Project","Stock","Parts","Description","MF","MPN","OC_FARNELL","OC_NEWARK"]
[1,"10-XX","10-XX","B3F-10XX","Roland",null,"SW2","OMRON SWITCH","B3F-1000",176432,"36M3542"]
[20,"100nF","C-US050-025X075","C050-025X075","Roland",null,"C1, C2, C3, C4, C5, C6, C8, C10, C11, C12, C13, C14, C15, C16, C17, C18, C19, C20, C21, C23, C24, C25, C26, C27, C28, C29, C31, C32, C33, C36, C37","CAPACITOR, American symbol"]
[1,"10K","R-US_0207/10","0207/10","Roland",null,"R19","RESISTOR, American symbol"]
[1,"16.000MHz","CRYSTALHC49U-H","HC49U-H","Roland",null,"Y1","CRYSTAL",1666973,"unknown"]
[9,"1K","R-US_0207/10","0207/10","Roland",null,"R1, R2, R3, R4, R8, R9, R16, R17, R20","RESISTOR, American symbol"]
[1,"1M","R-US_0207/10","0207/10","Roland",null,"R18","RESISTOR, American symbol"]
[1,"1N4148","1N4148DO35-10","DO35-10","Roland",null,"D1","DIODE"]
[2,"22pF","C-US050-025X075","C050-025X075","Roland",null,"C7, C9","CAPACITOR, American symbol"]
[1,"24LC1025P","24LC025P","DIL8","Roland",null,"U11","Serial EEPROM","MICROCHIP","24LC025-I/P","unknown","92C7098"]
[4,"27R","R-US_0207/10","0207/10","Roland",null,"R5, R6, R10, R11","RESISTOR, American symbol"]
[3,"4.7K","R-US_0207/10","0207/10","Roland",null,"R7, R21, R22","RESISTOR, American symbol"]
[1,"47R","R-US_0207/10","0207/10","Roland",null,"R12","RESISTOR, American symbol"]
[2,"470R","R-US_0207/10","0207/10","Roland",null,"R13, R14","RESISTOR, American symbol"]
[2,"28 Pin Narrow DIP Socket","575-199328","DIL28-3","Roland"]
[1,"74LS00N (132 OK?)","74LS00N","DIL14","Roland",null,"U9","Quad 2-input NAND gate"]
[1,"74LS10N","74LS10N","DIL14","Roland",null,"U8","Triple 3-input NAND gate"]
[5,"74LS38N","74LS38N","DIL14","Roland",null,"U3, U4, U5, U6, U7","Quad 2-input NAND gate, open collector output"]
[2,"BC547","-NPN-TO5","TO5","Roland",null,"Q1, Q2","NPN Transistror"]
[1,"DIP-4","DIP04S","DIP04S","Roland",null,"SW3","DIL/CODE SWITCH","unknown","unknown"]
[1,"MEGA328-P","MEGA8-P","DIL28-3","Roland",null,"U1","MICROCONTROLLER","unknown","unknown"]
[1,"ARDEBUG","MA03-2","MA03-2","Roland","Stock","SV1","PIN HEADER","unknown","unknown"]
[1,"MCP23017SP","MCP23017SP","DIL28-3","Roland","Stock","U2","I2C GPIO Expander","MICROCHIP","MCP23017-E/SP",1332088,"31K2959"]

{"sheet":"Sheet2","index":1,"n_rows":28,"n_cols":10,"rows_kept":28,"flags":["formulas_cached_only"]}
[19660800,3686400,9830400,614400,230400,225986.2068965517,{"v":14124.137931034482,"d":"14,124"},109.0909090909091,1228800,409600]
[9830400,null,4915200,307200,115200,{"v":112993.10344827586,"d":"112,993"},{"v":7062.068965517241,"d":"7,062"}]
[4915200,null,2457600,153600,38400,{"v":56496.55172413793,"d":"56,497"},{"v":3531.0344827586205,"d":"3,531"},57600]
[2457600,null,1228800,76800,19200,{"v":28248.275862068964,"d":"28,248"},{"v":1765.5172413793102,"d":"1,766"},null,57600]
[1228800,19660800,614400,38400,9600,{"v":14124.137931034482,"d":"14,124"},{"v":882.7586206896551,"d":"883"}]
[614400,9830400,307200,19200,4800,{"v":7062.068965517241,"d":"7,062"},{"v":441.37931034482756,"d":"441"}]
[307200,4915200,153600,9600,2400,{"v":3531.0344827586205,"d":"3,531"},{"v":220.68965517241378,"d":"221"}]
[153600,2457600,76800,4800,1200,{"v":1765.5172413793102,"d":"1,766"},{"v":110.34482758620689,"d":"110"}]
[76800,1228800,38400,2400,600,{"v":882.7586206896551,"d":"883"},{"v":55.172413793103445,"d":"55"}]
[38400,614400,19200,1200,300,{"v":441.37931034482756,"d":"441"},{"v":27.586206896551722,"d":"28"}]
[19200,307200,9600,600,150,{"v":220.68965517241378,"d":"221"},{"v":13.793103448275861,"d":"14"}]
[9600,153600,4800,300]
[4800,76800,2400,150]
[2400,38400]
[1200,19200]
[600,9600]
[300,4800]
[150,2400]
[]
[5068800,337920,28160,460800,38400]
[10137600,null,14080,null,19200]
[20275200,null,7040,null,9600]
[null,null,3520,null,4800]
[null,null,1760,null,2400]
[null,null,880,null,1200]
[null,null,440,null,600]
[null,null,220,null,300]
[null,null,110,null,150]