<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>A1</text>
<text>V1</text>
<text>8i/8L Bus Connector</text>
<text>8i/8L Bus Connector</text>
<text>8i/8L Bus Connector</text>
<text>M901/M903/M904 - Use both</text>
<text>M901</text>
<text>M901</text>
<text>Jumper unless M901</text>
<text>10ohm</text>
<text>10ohm</text>
<text>M90x/W0x1 - always used</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>* - Posibus/Negibus Signal</text>
<text>VRS</text>
<text>VRS</text>
<text>Component Side</text>
<text>Solder Side</text>
</plain>
<libraries>
<library name="con-lstb">
<packages>
<package name="MA17-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA12-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dec-con">
<packages>
<package name="EDGE-CON2">
<description>Single-Height DEC edge connector</description>
</package>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV2" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV1" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV4" library="con-lstb" package="MA12-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV3" library="con-lstb" package="MA12-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="PAD1" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD7" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD8" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="dec-con" package="EDGE-CON2" value=""/>
<element name="U$1" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
</elements>
<signals>
<signal name="S1">
<contactref element="SV1" pad="32"/>
<contactref element="U$4" pad="S1"/>
</signal>
<signal name="B1">
<contactref element="U$4" pad="B1"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="D1">
<contactref element="U$4" pad="D1"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="E1">
<contactref element="SV1" pad="12"/>
<contactref element="U$4" pad="E1"/>
</signal>
<signal name="H1">
<contactref element="SV1" pad="16"/>
<contactref element="U$4" pad="H1"/>
</signal>
<signal name="J1">
<contactref element="U$4" pad="J1"/>
<contactref element="SV1" pad="20"/>
</signal>
<signal name="L1">
<contactref element="U$4" pad="L1"/>
<contactref element="SV1" pad="24"/>
</signal>
<signal name="M1">
<contactref element="U$4" pad="M1"/>
<contactref element="SV1" pad="28"/>
</signal>
<signal name="P1">
<contactref element="U$4" pad="P1"/>
<contactref element="SV1" pad="30"/>
</signal>
<signal name="U1">
<contactref element="PAD5" pad="1"/>
<contactref element="U$4" pad="U1"/>
</signal>
<signal name="V1">
<contactref element="PAD7" pad="1"/>
<contactref element="U$4" pad="V1"/>
</signal>
<signal name="A2">
<contactref element="PAD1" pad="1"/>
<contactref element="U$4" pad="A2"/>
</signal>
<signal name="B2">
<contactref element="PAD3" pad="1"/>
<contactref element="U$4" pad="B2"/>
</signal>
<signal name="D2">
<contactref element="SV2" pad="6"/>
<contactref element="U$4" pad="D2"/>
</signal>
<signal name="E2">
<contactref element="SV2" pad="8"/>
<contactref element="U$4" pad="E2"/>
</signal>
<signal name="H2">
<contactref element="SV2" pad="12"/>
<contactref element="U$4" pad="H2"/>
</signal>
<signal name="K2">
<contactref element="SV2" pad="16"/>
<contactref element="U$4" pad="K2"/>
</signal>
<signal name="N2">
<contactref element="SV2" pad="22"/>
<contactref element="SV3" pad="10"/>
<contactref element="U$4" pad="N2"/>
</signal>
<signal name="P2">
<contactref element="SV2" pad="24"/>
<contactref element="U$4" pad="P2"/>
</signal>
<signal name="V2">
<contactref element="SV2" pad="32"/>
<contactref element="U$4" pad="V2"/>
</signal>
<signal name="T2">
<contactref element="SV2" pad="30"/>
<contactref element="U$4" pad="T2"/>
</signal>
<signal name="S2">
<contactref element="SV2" pad="28"/>
<contactref element="U$4" pad="S2"/>
</signal>
<signal name="F2">
<contactref element="SV2" pad="10"/>
<contactref element="SV3" pad="7"/>
<contactref element="U$4" pad="F2"/>
</signal>
<signal name="J2">
<contactref element="SV2" pad="14"/>
<contactref element="SV3" pad="8"/>
<contactref element="U$4" pad="J2"/>
</signal>
<signal name="L2">
<contactref element="SV2" pad="18"/>
<contactref element="SV3" pad="9"/>
<contactref element="U$4" pad="L2"/>
</signal>
<signal name="M2">
<contactref element="SV2" pad="20"/>
<contactref element="U$4" pad="M2"/>
</signal>
<signal name="R2">
<contactref element="SV2" pad="26"/>
<contactref element="SV3" pad="11"/>
<contactref element="U$4" pad="R2"/>
</signal>
<signal name="U2">
<contactref element="SV2" pad="34"/>
<contactref element="SV3" pad="12"/>
<contactref element="U$4" pad="U2"/>
</signal>
<signal name="C2">
<contactref element="SV2" pad="33"/>
<contactref element="SV2" pad="31"/>
<contactref element="SV2" pad="29"/>
<contactref element="SV2" pad="27"/>
<contactref element="SV2" pad="25"/>
<contactref element="SV2" pad="23"/>
<contactref element="SV2" pad="21"/>
<contactref element="SV2" pad="19"/>
<contactref element="SV2" pad="17"/>
<contactref element="SV2" pad="15"/>
<contactref element="SV2" pad="13"/>
<contactref element="SV2" pad="11"/>
<contactref element="SV2" pad="9"/>
<contactref element="SV2" pad="7"/>
<contactref element="SV2" pad="5"/>
<contactref element="SV2" pad="3"/>
<contactref element="SV2" pad="1"/>
<contactref element="SV4" pad="7"/>
<contactref element="SV4" pad="8"/>
<contactref element="SV4" pad="9"/>
<contactref element="SV4" pad="10"/>
<contactref element="SV4" pad="11"/>
<contactref element="SV4" pad="12"/>
<contactref element="U$4" pad="C2"/>
</signal>
<signal name="C1">
<contactref element="SV1" pad="3"/>
<contactref element="SV1" pad="5"/>
<contactref element="SV1" pad="7"/>
<contactref element="SV1" pad="9"/>
<contactref element="SV1" pad="11"/>
<contactref element="SV1" pad="13"/>
<contactref element="SV1" pad="15"/>
<contactref element="SV1" pad="17"/>
<contactref element="SV1" pad="19"/>
<contactref element="SV1" pad="21"/>
<contactref element="SV1" pad="23"/>
<contactref element="SV1" pad="25"/>
<contactref element="SV1" pad="27"/>
<contactref element="SV1" pad="29"/>
<contactref element="SV1" pad="31"/>
<contactref element="SV1" pad="33"/>
<contactref element="SV1" pad="1"/>
<contactref element="SV4" pad="6"/>
<contactref element="SV4" pad="5"/>
<contactref element="SV4" pad="4"/>
<contactref element="SV4" pad="3"/>
<contactref element="SV4" pad="2"/>
<contactref element="SV4" pad="1"/>
<contactref element="U$4" pad="C1"/>
</signal>
<signal name="A1">
<contactref element="SV3" pad="1"/>
<contactref element="U$4" pad="A1"/>
<contactref element="SV1" pad="10"/>
</signal>
<signal name="F1">
<contactref element="SV3" pad="2"/>
<contactref element="SV1" pad="14"/>
<contactref element="U$4" pad="F1"/>
</signal>
<signal name="K1">
<contactref element="SV3" pad="3"/>
<contactref element="U$4" pad="K1"/>
<contactref element="SV1" pad="18"/>
</signal>
<signal name="N1">
<contactref element="SV3" pad="4"/>
<contactref element="U$4" pad="N1"/>
<contactref element="SV1" pad="22"/>
</signal>
<signal name="T1">
<contactref element="SV3" pad="6"/>
<contactref element="SV1" pad="34"/>
<contactref element="U$4" pad="T1"/>
</signal>
<signal name="R1">
<contactref element="SV3" pad="5"/>
<contactref element="U$4" pad="R1"/>
<contactref element="SV1" pad="26"/>
</signal>
<signal name="JU1">
<contactref element="PAD6" pad="1"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="JV1">
<contactref element="PAD8" pad="1"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="JA2">
<contactref element="SV2" pad="2"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="JB2">
<contactref element="SV2" pad="4"/>
<contactref element="PAD4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
