{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["board1-bom"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"board1-bom","index":0,"n_rows":39,"n_cols":5,"rows_kept":39,"flags":["formulas_cached_only"]}
["Qty","Value","Device","Package","Parts"]
[2,null,"3,81/1,4","3,81/1,4","GND, VCC"]
[20,null,"40-XX","B3F-40XX","!SHLT, BOOT, DISP, DNEXT, DTHIS, ENEXT, ETHIS, INIT, KEY0, KEY1, KEY2, KEY3, KEY4, KEY5, KEY6, KEY7, LA, LSR, LXA, RUN"]
[2,null,"DIL16S","SOCKET-16","J1, J2"]
[16,0.01,"C-US050-025X075","C050-025X075","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16"]
[1,"1.0uf","CPOL-USE15-5AXIAL","E15-5","C17"]
[4,10,"R-US_0207/10","0207/10","R29, R30, R31, R32"]
[2,"10K","R-US_0207/10","0207/10","R1, R4"]
[20,"1K","R-US_0207/10","0207/10","R3, R5, R6, R7, R8, R9, R10, R11, R12, R13, R14, R15, R16, R17, R18, R19, R20, R21, R22, R23"]
[1,"220uf","CPOL-USE22-6AXIAL","E22-6","C19"]
[6,27,"R-US_0207/10","0207/10","R33, R34, R35, R36, R37, R38"]
[8,330,"R-US_0207/10","0207/10","R39, R40, R41, R42, R43, R44, R45, R46"]
[1,"33pf","C-US050-025X075","C050-025X075","C21"]
[5,470,"R-US_0207/10","0207/10","R24, R25, R26, R27, R28"]
[1,"47pf","C-US050-025X075","C050-025X075","C18"]
[1,"6.8K","R-US_0207/10","0207/10","R2"]
[1,"6.8uf","CPOL-USE22-6AXIAL","E22-6","C20"]
[1,"7416N","7416N","DIL14","E19"]
[3,"7446N","7446N","DIL16","E8, E13, E16"]
[1,"74LS04N","74LS04N","DIL14","E20"]
[2,"74LS08N","74LS08N","DIL14","E2, E10"]
[1,"74LS123N","74LS123N","DIL16","E18"]
[1,"74LS145N","74LS145N","DIL16","E17"]
[2,"74LS148N","74LS148N","DIL16","E1, E6"]
[1,"74LS20N","74LS20N","DIL14","E21"]
[1,"74LS42N","74LS42N","DIL16","E22"]
[1,"74LS74N","74LS74N","DIL14","E23"]
[1,"74LS90N","74LS90N","DIL14","E25"]
[1,"74LS95N","74LS95N","DIL14","E24"]
[1,"AC","LED5MM","LED5MM","D4"]
[1,"BUS","LED5MM","LED5MM","D7"]
[9,"HD-H101","HD-H101","HDSP-M","E3, E4, E5, E7, E9, E11, E12, E14, E15"]
[1,"MD","LED5MM","LED5MM","D3"]
[5,"MPSA05","2N2222A","TO18","Q1, Q2, Q3, Q4, Q5"]
[1,"MQ","LED5MM","LED5MM","D1"]
[1,"RUN","LED5MM","LED5MM","D8"]
[1,"SR","LED5MM","LED5MM","D2"]
[1,"STATE","LED5MM","LED5MM","D6"]
[1,"STATUS","LED5MM","LED5MM","D5"]