<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="7.9375" x2="0" y2="201.6125" width="0" layer="20"/>
<wire x1="7.9375" y1="0" x2="463.55" y2="0" width="0" layer="20"/>
<wire x1="7.9375" y1="209.55" x2="463.55" y2="209.55" width="0" layer="20"/>
<wire x1="471.4875" y1="201.6125" x2="471.4875" y2="7.9375" width="0" layer="20"/>
<text>1/8" Thick Plastic Stock</text>
<wire x1="7.9375" y1="0" x2="0" y2="7.9375" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="201.6125" x2="7.9375" y2="209.55" width="0" layer="20" curve="-90"/>
<wire x1="463.55" y1="209.55" x2="471.4875" y2="201.6125" width="0" layer="20" curve="-90"/>
<wire x1="471.4875" y1="7.9375" x2="463.55" y2="0" width="0" layer="20" curve="-90"/>
<text>Fonts and lettering are inaccurate/missing.</text>
<text>MEMORY ADDRESS</text>
<text>LINK</text>
<text>ION</text>
<text>PAR</text>
<text>PROT</text>
<text>RUN</text>
<text>1/4" Bulb aperture</text>
<text>MEMORY BUFFER</text>
<text>ACCUMULATOR</text>
<wire x1="408.78125" y1="46.0375" x2="408.78125" y2="23.8125" width="0" layer="20"/>
<wire x1="408.78125" y1="23.8125" x2="423.8625" y2="23.8125" width="0" layer="20"/>
<wire x1="423.8625" y1="23.8125" x2="423.8625" y2="46.0375" width="0" layer="20"/>
<wire x1="423.8625" y1="46.0375" x2="408.78125" y2="46.0375" width="0" layer="20"/>
<wire x1="330.2" y1="46.0375" x2="330.2" y2="23.8125" width="0" layer="20"/>
<wire x1="330.2" y1="23.8125" x2="403.621875" y2="23.8125" width="0" layer="20"/>
<wire x1="403.621875" y1="23.8125" x2="403.621875" y2="46.0375" width="0" layer="20"/>
<wire x1="403.621875" y1="46.0375" x2="330.2" y2="46.0375" width="0" layer="20"/>
<wire x1="308.76875" y1="46.0375" x2="308.76875" y2="23.8125" width="0" layer="20"/>
<wire x1="308.76875" y1="23.8125" x2="323.85" y2="23.8125" width="0" layer="20"/>
<wire x1="323.85" y1="23.8125" x2="323.85" y2="46.0375" width="0" layer="20"/>
<wire x1="323.85" y1="46.0375" x2="308.76875" y2="46.0375" width="0" layer="20"/>
<wire x1="130.175" y1="46.0375" x2="130.175" y2="23.8125" width="0" layer="20"/>
<wire x1="130.175" y1="23.8125" x2="302.41875" y2="23.8125" width="0" layer="20"/>
<wire x1="302.41875" y1="23.8125" x2="302.41875" y2="46.0375" width="0" layer="20"/>
<wire x1="302.41875" y1="46.0375" x2="130.175" y2="46.0375" width="0" layer="20"/>
<text>INSTRUCTION</text>
<text>MAJOR STATES</text>
<text>F</text>
<text>E</text>
<text>D</text>
<text>WC</text>
<text>CA</text>
<text>B</text>
<text>EA</text>
<wire x1="73.025" y1="46.0375" x2="73.025" y2="23.8125" width="0" layer="20"/>
<wire x1="73.025" y1="23.8125" x2="88.10625" y2="23.8125" width="0" layer="20"/>
<wire x1="88.10625" y1="23.8125" x2="88.10625" y2="46.0375" width="0" layer="20"/>
<wire x1="88.10625" y1="46.0375" x2="73.025" y2="46.0375" width="0" layer="20"/>
<wire x1="94.45625" y1="46.0375" x2="94.45625" y2="23.8125" width="0" layer="20"/>
<wire x1="94.45625" y1="23.8125" x2="123.825" y2="23.8125" width="0" layer="20"/>
<wire x1="123.825" y1="23.8125" x2="123.825" y2="46.0375" width="0" layer="20"/>
<wire x1="123.825" y1="46.0375" x2="94.45625" y2="46.0375" width="0" layer="20"/>
<hole x="45.24375" y="36.5125" drill="19.84375"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="BULB">
<description>&lt;B&gt;Panel Bulb&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IF2" library="dec-con" package="BULB" value=""/>
<element name="MA0" library="dec-con" package="BULB" value=""/>
<element name="MA1" library="dec-con" package="BULB" value=""/>
<element name="MA2" library="dec-con" package="BULB" value=""/>
<element name="MA3" library="dec-con" package="BULB" value=""/>
<element name="MA4" library="dec-con" package="BULB" value=""/>
<element name="MA5" library="dec-con" package="BULB" value=""/>
<element name="MA6" library="dec-con" package="BULB" value=""/>
<element name="MA7" library="dec-con" package="BULB" value=""/>
<element name="MA8" library="dec-con" package="BULB" value=""/>
<element name="MA9" library="dec-con" package="BULB" value=""/>
<element name="MA10" library="dec-con" package="BULB" value=""/>
<element name="MA11" library="dec-con" package="BULB" value=""/>
<element name="MB0" library="dec-con" package="BULB" value=""/>
<element name="MB1" library="dec-con" package="BULB" value=""/>
<element name="MB2" library="dec-con" package="BULB" value=""/>
<element name="MB3" library="dec-con" package="BULB" value=""/>
<element name="MB4" library="dec-con" package="BULB" value=""/>
<element name="MB5" library="dec-con" package="BULB" value=""/>
<element name="MB6" library="dec-con" package="BULB" value=""/>
<element name="MB7" library="dec-con" package="BULB" value=""/>
<element name="MB8" library="dec-con" package="BULB" value=""/>
<element name="MB9" library="dec-con" package="BULB" value=""/>
<element name="MB10" library="dec-con" package="BULB" value=""/>
<element name="MB11" library="dec-con" package="BULB" value=""/>
<element name="AC0" library="dec-con" package="BULB" value=""/>
<element name="AC1" library="dec-con" package="BULB" value=""/>
<element name="AC2" library="dec-con" package="BULB" value=""/>
<element name="AC3" library="dec-con" package="BULB" value=""/>
<element name="AC4" library="dec-con" package="BULB" value=""/>
<element name="AC5" library="dec-con" package="BULB" value=""/>
<element name="AC6" library="dec-con" package="BULB" value=""/>
<element name="AC7" library="dec-con" package="BULB" value=""/>
<element name="AC8" library="dec-con" package="BULB" value=""/>
<element name="AC9" library="dec-con" package="BULB" value=""/>
<element name="AC10" library="dec-con" package="BULB" value=""/>
<element name="AC11" library="dec-con" package="BULB" value=""/>
<element name="LINK" library="dec-con" package="BULB" value=""/>
<element name="ION" library="dec-con" package="BULB" value=""/>
<element name="PAR" library="dec-con" package="BULB" value=""/>
<element name="RUN" library="dec-con" package="BULB" value=""/>
<element name="FETCH" library="dec-con" package="BULB" value=""/>
<element name="EXECUTE" library="dec-con" package="BULB" value=""/>
<element name="DEFER" library="dec-con" package="BULB" value=""/>
<element name="WC" library="dec-con" package="BULB" value=""/>
<element name="CA" library="dec-con" package="BULB" value=""/>
<element name="BREAK" library="dec-con" package="BULB" value=""/>
<element name="IR0" library="dec-con" package="BULB" value=""/>
<element name="IR2" library="dec-con" package="BULB" value=""/>
<element name="IR1" library="dec-con" package="BULB" value=""/>
<element name="PROT" library="dec-con" package="BULB" value=""/>
</elements>
<signals>
<signal name="N$6">
<contactref element="IF2" pad="B"/>
</signal>
<signal name="N$19">
<contactref element="MA0" pad="B"/>
</signal>
<signal name="N$20">
<contactref element="MA1" pad="B"/>
</signal>
<signal name="N$21">
<contactref element="MA2" pad="B"/>
</signal>
<signal name="N$22">
<contactref element="MA3" pad="B"/>
</signal>
<signal name="N$24">
<contactref element="MA5" pad="B"/>
</signal>
<signal name="N$25">
<contactref element="MA6" pad="B"/>
</signal>
<signal name="N$26">
<contactref element="MA7" pad="B"/>
</signal>
<signal name="N$27">
<contactref element="MA8" pad="B"/>
</signal>
<signal name="N$28">
<contactref element="MA9" pad="B"/>
</signal>
<signal name="N$29">
<contactref element="MA10" pad="B"/>
</signal>
<signal name="N$30">
<contactref element="MA11" pad="B"/>
</signal>
<signal name="N$31">
<contactref element="MB0" pad="B"/>
</signal>
<signal name="N$32">
<contactref element="MB1" pad="B"/>
</signal>
<signal name="N$33">
<contactref element="MB2" pad="B"/>
</signal>
<signal name="N$34">
<contactref element="MB3" pad="B"/>
</signal>
<signal name="N$35">
<contactref element="MB4" pad="B"/>
</signal>
<signal name="N$36">
<contactref element="MB5" pad="B"/>
</signal>
<signal name="N$37">
<contactref element="MB6" pad="B"/>
</signal>
<signal name="N$38">
<contactref element="MB7" pad="B"/>
</signal>
<signal name="N$39">
<contactref element="MB8" pad="B"/>
</signal>
<signal name="N$40">
<contactref element="MB9" pad="B"/>
</signal>
<signal name="N$41">
<contactref element="MB10" pad="B"/>
</signal>
<signal name="N$42">
<contactref element="MB11" pad="B"/>
</signal>
<signal name="N$43">
<contactref element="AC0" pad="B"/>
</signal>
<signal name="N$44">
<contactref element="AC1" pad="B"/>
</signal>
<signal name="N$45">
<contactref element="AC2" pad="B"/>
</signal>
<signal name="N$46">
<contactref element="AC3" pad="B"/>
</signal>
<signal name="N$47">
<contactref element="AC4" pad="B"/>
</signal>
<signal name="N$48">
<contactref element="AC5" pad="B"/>
</signal>
<signal name="N$49">
<contactref element="AC6" pad="B"/>
</signal>
<signal name="N$50">
<contactref element="AC7" pad="B"/>
</signal>
<signal name="N$51">
<contactref element="AC8" pad="B"/>
</signal>
<signal name="N$52">
<contactref element="AC9" pad="B"/>
</signal>
<signal name="N$53">
<contactref element="AC10" pad="B"/>
</signal>
<signal name="N$54">
<contactref element="AC11" pad="B"/>
</signal>
<signal name="N$72">
<contactref element="LINK" pad="B"/>
</signal>
<signal name="N$73">
<contactref element="ION" pad="B"/>
</signal>
<signal name="N$74">
<contactref element="PAR" pad="B"/>
</signal>
<signal name="N$75">
<contactref element="RUN" pad="B"/>
</signal>
<signal name="N$76">
<contactref element="FETCH" pad="B"/>
</signal>
<signal name="N$77">
<contactref element="EXECUTE" pad="B"/>
</signal>
<signal name="N$78">
<contactref element="DEFER" pad="B"/>
</signal>
<signal name="N$79">
<contactref element="WC" pad="B"/>
</signal>
<signal name="N$80">
<contactref element="CA" pad="B"/>
</signal>
<signal name="N$81">
<contactref element="BREAK" pad="B"/>
</signal>
<signal name="N$82">
<contactref element="IR0" pad="B"/>
</signal>
<signal name="N$83">
<contactref element="IR2" pad="B"/>
</signal>
<signal name="N$84">
<contactref element="IR1" pad="B"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
