<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="136.525" x2="101.6" y2="136.525" width="0" layer="20"/>
<wire x1="101.6" y1="136.525" x2="101.6" y2="0" width="0" layer="20"/>
<wire x1="101.6" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="136.525" width="0" layer="20"/>
</plain>
<libraries>
<library name="dec-m">
<description>DEC Flip-Chips
&lt;BR&gt;Vincent R. Slyngstad
&lt;BR&gt;vrs@msn.com</description>
<packages>
<package name="H807-2">
<description>Two-wide Female Edge Connector</description>
</package>
<package name="H807">
<description>One-wide female edge connector</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B06" library="dec-m" package="H807" value="M040"/>
<element name="B03" library="dec-m" package="H807" value="M040"/>
<element name="B04" library="dec-m" package="H807" value="M040"/>
<element name="B05" library="dec-m" package="H807" value="M040"/>
<element name="AB07" library="dec-m" package="H807-2" value="G918"/>
<element name="A06" library="dec-m" package="H807" value="M113"/>
<element name="A02" library="dec-m" package="H807" value="EMPTY"/>
<element name="A01" library="dec-m" package="H807" value="W033"/>
<element name="B01" library="dec-m" package="H807" value="W033"/>
<element name="B08" library="dec-m" package="H807" value="W033"/>
<element name="B02" library="dec-m" package="H807" value="W033"/>
<element name="A08" library="dec-m" package="H807" value="W033"/>
<element name="A03" library="dec-m" package="H807" value="M044"/>
<element name="A04" library="dec-m" package="H807" value="M044"/>
<element name="A05" library="dec-m" package="H807" value="M044"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="B06" pad="A2"/>
<contactref element="B03" pad="A2"/>
<contactref element="B04" pad="A2"/>
<contactref element="B05" pad="A2"/>
<contactref element="A06" pad="A2"/>
<contactref element="AB07" pad="AA2"/>
<contactref element="AB07" pad="BA2"/>
<contactref element="B08" pad="R2"/>
<contactref element="A08" pad="A2"/>
<contactref element="A03" pad="A2"/>
<contactref element="A04" pad="A2"/>
<contactref element="A05" pad="A2"/>
<contactref element="B08" pad="A2"/>
</signal>
<signal name="GND">
<contactref element="B06" pad="C2"/>
<contactref element="B03" pad="C2"/>
<contactref element="B04" pad="C2"/>
<contactref element="B05" pad="C2"/>
<contactref element="A06" pad="C2"/>
<contactref element="A06" pad="T1"/>
<contactref element="A02" pad="C2"/>
<contactref element="A01" pad="C2"/>
<contactref element="AB07" pad="AC2"/>
<contactref element="AB07" pad="BC2"/>
<contactref element="B01" pad="B2"/>
<contactref element="B01" pad="D2"/>
<contactref element="A08" pad="C2"/>
<contactref element="A03" pad="C2"/>
<contactref element="A04" pad="C2"/>
<contactref element="A05" pad="C2"/>
<contactref element="B02" pad="C2"/>
<contactref element="B02" pad="E2"/>
<contactref element="B08" pad="C2"/>
<contactref element="A03" pad="M2"/>
<contactref element="A04" pad="M2"/>
<contactref element="A05" pad="M2"/>
</signal>
<signal name="-15V">
<contactref element="B06" pad="B2"/>
<contactref element="B03" pad="B2"/>
<contactref element="B04" pad="B2"/>
<contactref element="B05" pad="B2"/>
<contactref element="AB07" pad="AB2"/>
<contactref element="AB07" pad="BB2"/>
<contactref element="A03" pad="B2"/>
<contactref element="A04" pad="B2"/>
<contactref element="A05" pad="B2"/>
<contactref element="B08" pad="B2"/>
<contactref element="A08" pad="B2"/>
<contactref element="A06" pad="B2"/>
</signal>
<signal name="PUN_FEED">
<contactref element="B01" pad="A2"/>
<contactref element="B02" pad="U2"/>
</signal>
<signal name="PUN_SYNC">
<contactref element="B01" pad="C2"/>
<contactref element="B02" pad="F2"/>
</signal>
<signal name="PUN_DONE">
<contactref element="B01" pad="E2"/>
<contactref element="A06" pad="E2"/>
</signal>
<signal name="PHOTO2">
<contactref element="B08" pad="N2"/>
<contactref element="AB07" pad="BN2"/>
</signal>
<signal name="PHOTO8">
<contactref element="B08" pad="F2"/>
<contactref element="AB07" pad="BF2"/>
</signal>
<signal name="PHOTO7">
<contactref element="B08" pad="H2"/>
<contactref element="AB07" pad="BH2"/>
</signal>
<signal name="PHOTO6">
<contactref element="B08" pad="J2"/>
<contactref element="AB07" pad="BJ2"/>
</signal>
<signal name="PHOTO5">
<contactref element="B08" pad="K2"/>
<contactref element="AB07" pad="BK2"/>
</signal>
<signal name="PHOTO4">
<contactref element="B08" pad="L2"/>
<contactref element="AB07" pad="BL2"/>
</signal>
<signal name="FEED">
<contactref element="B08" pad="S2"/>
<contactref element="AB07" pad="BE2"/>
</signal>
<signal name="PHOTO1">
<contactref element="B08" pad="P2"/>
<contactref element="AB07" pad="BP2"/>
</signal>
<signal name="PHOTO3">
<contactref element="B08" pad="M2"/>
<contactref element="AB07" pad="BM2"/>
</signal>
<signal name="RD_HOLE1">
<contactref element="AB07" pad="AE2"/>
<contactref element="A01" pad="D2"/>
</signal>
<signal name="RD_HOLE2">
<contactref element="AB07" pad="AF2"/>
<contactref element="A01" pad="E2"/>
</signal>
<signal name="RD_HOLE3">
<contactref element="AB07" pad="AJ2"/>
<contactref element="A01" pad="F2"/>
</signal>
<signal name="RD_HOLE4">
<contactref element="AB07" pad="BD2"/>
<contactref element="A01" pad="H2"/>
</signal>
<signal name="FEED_HOLE">
<contactref element="AB07" pad="AT2"/>
<contactref element="A01" pad="N2"/>
</signal>
<signal name="RD_HOLE5">
<contactref element="AB07" pad="AL2"/>
<contactref element="A01" pad="J2"/>
</signal>
<signal name="RD_HOLE6">
<contactref element="AB07" pad="AN2"/>
<contactref element="A01" pad="K2"/>
</signal>
<signal name="RD_HOLE7">
<contactref element="AB07" pad="AP2"/>
<contactref element="A01" pad="L2"/>
</signal>
<signal name="RD_HOLE8">
<contactref element="AB07" pad="AR2"/>
<contactref element="A01" pad="M2"/>
</signal>
<signal name="OFF_LINE">
<contactref element="A01" pad="B2"/>
</signal>
<signal name="BA(0)">
<contactref element="B03" pad="K2"/>
<contactref element="B03" pad="D2"/>
<contactref element="A01" pad="P2"/>
</signal>
<signal name="BA(1)">
<contactref element="B04" pad="K2"/>
<contactref element="B04" pad="D2"/>
<contactref element="A01" pad="R2"/>
</signal>
<signal name="BB(0)">
<contactref element="B05" pad="K2"/>
<contactref element="B05" pad="D2"/>
<contactref element="A01" pad="S2"/>
</signal>
<signal name="BB(1)">
<contactref element="B06" pad="K2"/>
<contactref element="B06" pad="D2"/>
<contactref element="A01" pad="T2"/>
</signal>
<signal name="-18V">
<contactref element="B06" pad="V2"/>
<contactref element="B05" pad="V2"/>
<contactref element="B04" pad="V2"/>
<contactref element="B03" pad="V2"/>
</signal>
<signal name="PWR">
<contactref element="B03" pad="E2"/>
<contactref element="B04" pad="E2"/>
<contactref element="B05" pad="E2"/>
<contactref element="B06" pad="E2"/>
<contactref element="A01" pad="U2"/>
</signal>
<signal name="!RDR_FEED_SW">
<contactref element="A01" pad="V2"/>
</signal>
<signal name="N$4">
<contactref element="A06" pad="J2"/>
<contactref element="A06" pad="F2"/>
<contactref element="A06" pad="H2"/>
</signal>
<signal name="+5V_BIAS">
<contactref element="A06" pad="D2"/>
<contactref element="B01" pad="M2"/>
<contactref element="B02" pad="V2"/>
</signal>
<signal name="PUN">
<contactref element="A06" pad="K2"/>
<contactref element="A03" pad="E2"/>
<contactref element="A03" pad="F2"/>
<contactref element="A03" pad="H2"/>
<contactref element="A03" pad="D2"/>
<contactref element="A04" pad="E2"/>
<contactref element="A04" pad="P2"/>
<contactref element="A04" pad="K2"/>
<contactref element="A04" pad="H2"/>
<contactref element="A05" pad="E2"/>
<contactref element="A05" pad="P2"/>
<contactref element="A05" pad="K2"/>
<contactref element="A05" pad="H2"/>
</signal>
<signal name="PUN_FEED_HOLE">
<contactref element="A03" pad="U2"/>
<contactref element="A03" pad="T2"/>
<contactref element="B02" pad="H2"/>
</signal>
<signal name="PUNCH8">
<contactref element="A04" pad="N2"/>
<contactref element="B01" pad="H2"/>
</signal>
<signal name="PUNCH1">
<contactref element="A05" pad="D2"/>
<contactref element="B01" pad="S2"/>
</signal>
<signal name="PUNCH2">
<contactref element="A05" pad="F2"/>
<contactref element="B01" pad="R2"/>
</signal>
<signal name="PUNCH3">
<contactref element="A05" pad="J2"/>
<contactref element="B01" pad="P2"/>
</signal>
<signal name="PUNCH4">
<contactref element="A05" pad="N2"/>
<contactref element="B01" pad="N2"/>
</signal>
<signal name="PUNCH6">
<contactref element="A04" pad="F2"/>
<contactref element="B01" pad="K2"/>
</signal>
<signal name="PUNCH7">
<contactref element="A04" pad="J2"/>
<contactref element="B01" pad="J2"/>
</signal>
<signal name="PUNCH5">
<contactref element="A04" pad="D2"/>
<contactref element="B01" pad="L2"/>
</signal>
<signal name="OUTOFTAPE">
<contactref element="B02" pad="T2"/>
<contactref element="B01" pad="T2"/>
</signal>
<signal name="HOLE2">
<contactref element="A05" pad="T2"/>
<contactref element="B02" pad="S2"/>
</signal>
<signal name="HOLE8">
<contactref element="A04" pad="R2"/>
<contactref element="B02" pad="K2"/>
</signal>
<signal name="HOLE7">
<contactref element="A04" pad="S2"/>
<contactref element="B02" pad="L2"/>
</signal>
<signal name="HOLE6">
<contactref element="A04" pad="T2"/>
<contactref element="B02" pad="M2"/>
</signal>
<signal name="HOLE5">
<contactref element="A04" pad="U2"/>
<contactref element="B02" pad="N2"/>
</signal>
<signal name="HOLE4">
<contactref element="A05" pad="R2"/>
<contactref element="B02" pad="P2"/>
</signal>
<signal name="HOLE3">
<contactref element="A05" pad="S2"/>
<contactref element="B02" pad="R2"/>
</signal>
<signal name="HOLE1">
<contactref element="A05" pad="U2"/>
<contactref element="B02" pad="J2"/>
</signal>
<signal name="-36V">
<contactref element="A05" pad="V2"/>
<contactref element="B02" pad="D2"/>
<contactref element="A03" pad="V2"/>
<contactref element="A04" pad="V2"/>
</signal>
<signal name="NC">
<contactref element="A02" pad="A2"/>
</signal>
<signal name="***">
<contactref element="A02" pad="B2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
