<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.79375" y1="212.725" x2="405.60625" y2="212.725" width="0" layer="20"/>
<wire x1="405.60625" y1="212.725" x2="405.60625" y2="15.875" width="0" layer="20"/>
<wire x1="405.60625" y1="15.875" x2="399.25625" y2="15.875" width="0" layer="20"/>
<wire x1="-0.79375" y1="212.725" x2="-0.79375" y2="18.415" width="0" layer="20"/>
<wire x1="-0.79375" y1="18.415" x2="3.96875" y2="18.415" width="0" layer="20"/>
<wire x1="134.77875" y1="18.415" x2="137.31875" y2="18.415" width="0" layer="20"/>
<wire x1="203.99375" y1="18.415" x2="206.53375" y2="18.415" width="0" layer="20"/>
<wire x1="267.81125" y1="18.415" x2="270.03375" y2="18.415" width="0" layer="20"/>
<wire x1="337.34375" y1="18.415" x2="339.88375" y2="18.415" width="0" layer="20"/>
<wire x1="330.99375" y1="15.875" x2="337.34375" y2="15.875" width="0" layer="20"/>
<wire x1="337.34375" y1="15.875" x2="337.34375" y2="18.415" width="0" layer="20"/>
<wire x1="267.81125" y1="15.875" x2="267.81125" y2="18.415" width="0" layer="20"/>
<wire x1="203.99375" y1="15.875" x2="203.99375" y2="18.415" width="0" layer="20"/>
<wire x1="134.77875" y1="15.875" x2="134.77875" y2="18.415" width="0" layer="20"/>
<wire x1="72.23125" y1="15.875" x2="72.23125" y2="18.415" width="0" layer="20"/>
<wire x1="72.23125" y1="18.415" x2="72.54875" y2="18.415" width="0" layer="20"/>
<wire x1="64.29375" y1="15.875" x2="72.23125" y2="15.875" width="0" layer="20"/>
<wire x1="197.64375" y1="15.875" x2="203.99375" y2="15.875" width="0" layer="20"/>
<hole x="12.7" y="107.95" drill="3.175"/>
<hole x="12.7" y="184.15" drill="3.175"/>
<hole x="393.7" y="184.15" drill="3.175"/>
<hole x="393.7" y="107.95" drill="3.175"/>
<text>PDP-8/S CONTROL PANEL</text>
<text>5403833B</text>
<text>D-IA-5003835</text>
</plain>
<libraries>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
<package name="BULB">
<description>&lt;B&gt;Panel Bulb&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="A" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="B" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="C" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="D" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="E" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="F" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="AC0" library="dec-con" package="BULB" value=""/>
<element name="AC1" library="dec-con" package="BULB" value=""/>
<element name="AC2" library="dec-con" package="BULB" value=""/>
<element name="AC3" library="dec-con" package="BULB" value=""/>
<element name="AC4" library="dec-con" package="BULB" value=""/>
<element name="AC5" library="dec-con" package="BULB" value=""/>
<element name="AC6" library="dec-con" package="BULB" value=""/>
<element name="AC7" library="dec-con" package="BULB" value=""/>
<element name="AC8" library="dec-con" package="BULB" value=""/>
<element name="AC9" library="dec-con" package="BULB" value=""/>
<element name="AC10" library="dec-con" package="BULB" value=""/>
<element name="AC11" library="dec-con" package="BULB" value=""/>
<element name="MB0" library="dec-con" package="BULB" value=""/>
<element name="MB1" library="dec-con" package="BULB" value=""/>
<element name="MB2" library="dec-con" package="BULB" value=""/>
<element name="MB3" library="dec-con" package="BULB" value=""/>
<element name="MB4" library="dec-con" package="BULB" value=""/>
<element name="MB5" library="dec-con" package="BULB" value=""/>
<element name="MB6" library="dec-con" package="BULB" value=""/>
<element name="MB7" library="dec-con" package="BULB" value=""/>
<element name="MB8" library="dec-con" package="BULB" value=""/>
<element name="MB9" library="dec-con" package="BULB" value=""/>
<element name="MB10" library="dec-con" package="BULB" value=""/>
<element name="MB11" library="dec-con" package="BULB" value=""/>
<element name="MA0" library="dec-con" package="BULB" value=""/>
<element name="MA1" library="dec-con" package="BULB" value=""/>
<element name="MA2" library="dec-con" package="BULB" value=""/>
<element name="MA3" library="dec-con" package="BULB" value=""/>
<element name="MA4" library="dec-con" package="BULB" value=""/>
<element name="MA5" library="dec-con" package="BULB" value=""/>
<element name="MA6" library="dec-con" package="BULB" value=""/>
<element name="MA7" library="dec-con" package="BULB" value=""/>
<element name="MA8" library="dec-con" package="BULB" value=""/>
<element name="MA9" library="dec-con" package="BULB" value=""/>
<element name="MA10" library="dec-con" package="BULB" value=""/>
<element name="MA11" library="dec-con" package="BULB" value=""/>
<element name="PC0" library="dec-con" package="BULB" value=""/>
<element name="PC1" library="dec-con" package="BULB" value=""/>
<element name="PC2" library="dec-con" package="BULB" value=""/>
<element name="PC3" library="dec-con" package="BULB" value=""/>
<element name="PC4" library="dec-con" package="BULB" value=""/>
<element name="PC5" library="dec-con" package="BULB" value=""/>
<element name="PC6" library="dec-con" package="BULB" value=""/>
<element name="PC7" library="dec-con" package="BULB" value=""/>
<element name="PC8" library="dec-con" package="BULB" value=""/>
<element name="PC9" library="dec-con" package="BULB" value=""/>
<element name="PC10" library="dec-con" package="BULB" value=""/>
<element name="PC11" library="dec-con" package="BULB" value=""/>
<element name="DF0" library="dec-con" package="BULB" value=""/>
<element name="DF1" library="dec-con" package="BULB" value=""/>
<element name="DF2" library="dec-con" package="BULB" value=""/>
<element name="IF0" library="dec-con" package="BULB" value=""/>
<element name="IF1" library="dec-con" package="BULB" value=""/>
<element name="IF2" library="dec-con" package="BULB" value=""/>
<element name="AND" library="dec-con" package="BULB" value=""/>
<element name="TAD" library="dec-con" package="BULB" value=""/>
<element name="ISZ" library="dec-con" package="BULB" value=""/>
<element name="DCA" library="dec-con" package="BULB" value=""/>
<element name="JMS" library="dec-con" package="BULB" value=""/>
<element name="JMP" library="dec-con" package="BULB" value=""/>
<element name="IOT" library="dec-con" package="BULB" value=""/>
<element name="OPR" library="dec-con" package="BULB" value=""/>
<element name="FETCH" library="dec-con" package="BULB" value=""/>
<element name="INDEX" library="dec-con" package="BULB" value=""/>
<element name="DEFER" library="dec-con" package="BULB" value=""/>
<element name="EXEC" library="dec-con" package="BULB" value=""/>
<element name="END" library="dec-con" package="BULB" value=""/>
<element name="BREAK" library="dec-con" package="BULB" value=""/>
<element name="PAUSE" library="dec-con" package="BULB" value=""/>
<element name="RUN" library="dec-con" package="BULB" value=""/>
<element name="ION" library="dec-con" package="BULB" value=""/>
<element name="SPARE1" library="dec-con" package="BULB" value=""/>
<element name="PARITY" library="dec-con" package="BULB" value=""/>
<element name="SPARE2" library="dec-con" package="BULB" value=""/>
<element name="PERR" library="dec-con" package="BULB" value=""/>
<element name="SPARE3" library="dec-con" package="BULB" value=""/>
<element name="SPARE4" library="dec-con" package="BULB" value=""/>
<element name="MQ0" library="dec-con" package="BULB" value=""/>
<element name="MQ1" library="dec-con" package="BULB" value=""/>
<element name="MQ2" library="dec-con" package="BULB" value=""/>
<element name="MQ3" library="dec-con" package="BULB" value=""/>
<element name="MQ4" library="dec-con" package="BULB" value=""/>
<element name="MQ5" library="dec-con" package="BULB" value=""/>
<element name="MQ6" library="dec-con" package="BULB" value=""/>
<element name="MQ7" library="dec-con" package="BULB" value=""/>
<element name="MQ8" library="dec-con" package="BULB" value=""/>
<element name="MQ9" library="dec-con" package="BULB" value=""/>
<element name="MQ10" library="dec-con" package="BULB" value=""/>
<element name="MQ11" library="dec-con" package="BULB" value=""/>
<element name="LINK" library="dec-con" package="BULB" value=""/>
</elements>
<signals>
<signal name="AV2">
<contactref element="A" pad="V2"/>
<contactref element="IOT" pad="A"/>
</signal>
<signal name="AD2">
<contactref element="A" pad="D2"/>
<contactref element="RUN" pad="A"/>
</signal>
<signal name="AE2">
<contactref element="A" pad="E2"/>
<contactref element="PAUSE" pad="A"/>
</signal>
<signal name="AF2">
<contactref element="A" pad="F2"/>
<contactref element="BREAK" pad="A"/>
</signal>
<signal name="AH2">
<contactref element="A" pad="H2"/>
<contactref element="END" pad="A"/>
</signal>
<signal name="AJ2">
<contactref element="A" pad="J2"/>
<contactref element="EXEC" pad="A"/>
</signal>
<signal name="AK2">
<contactref element="A" pad="K2"/>
<contactref element="DEFER" pad="A"/>
</signal>
<signal name="AL2">
<contactref element="A" pad="L2"/>
<contactref element="INDEX" pad="A"/>
</signal>
<signal name="AM2">
<contactref element="A" pad="M2"/>
<contactref element="FETCH" pad="A"/>
</signal>
<signal name="AN2">
<contactref element="A" pad="N2"/>
<contactref element="AND" pad="A"/>
</signal>
<signal name="AP2">
<contactref element="A" pad="P2"/>
<contactref element="TAD" pad="A"/>
</signal>
<signal name="AR2">
<contactref element="A" pad="R2"/>
<contactref element="ISZ" pad="A"/>
</signal>
<signal name="AS2">
<contactref element="A" pad="S2"/>
<contactref element="DCA" pad="A"/>
</signal>
<signal name="AT2">
<contactref element="A" pad="T2"/>
<contactref element="JMS" pad="A"/>
</signal>
<signal name="AU2">
<contactref element="A" pad="U2"/>
<contactref element="JMP" pad="A"/>
</signal>
<signal name="BV2">
<contactref element="B" pad="V2"/>
<contactref element="AC10" pad="A"/>
</signal>
<signal name="BU2">
<contactref element="B" pad="U2"/>
<contactref element="MB10" pad="A"/>
</signal>
<signal name="BT2">
<contactref element="B" pad="T2"/>
<contactref element="MA10" pad="A"/>
</signal>
<signal name="BS2">
<contactref element="B" pad="S2"/>
<contactref element="MQ11" pad="A"/>
</signal>
<signal name="BR2">
<contactref element="B" pad="R2"/>
<contactref element="AC11" pad="A"/>
</signal>
<signal name="BP2">
<contactref element="B" pad="P2"/>
<contactref element="MB11" pad="A"/>
</signal>
<signal name="BN2">
<contactref element="B" pad="N2"/>
<contactref element="MA11" pad="A"/>
</signal>
<signal name="BM2">
<contactref element="B" pad="M2"/>
<contactref element="PC5" pad="A"/>
</signal>
<signal name="BL2">
<contactref element="B" pad="L2"/>
<contactref element="PC6" pad="A"/>
</signal>
<signal name="BK2">
<contactref element="B" pad="K2"/>
<contactref element="PC7" pad="A"/>
</signal>
<signal name="BJ2">
<contactref element="B" pad="J2"/>
<contactref element="PC8" pad="A"/>
</signal>
<signal name="BH2">
<contactref element="B" pad="H2"/>
<contactref element="PC9" pad="A"/>
</signal>
<signal name="BF2">
<contactref element="B" pad="F2"/>
<contactref element="PC10" pad="A"/>
</signal>
<signal name="BE2">
<contactref element="B" pad="E2"/>
<contactref element="PC11" pad="A"/>
</signal>
<signal name="BD2">
<contactref element="B" pad="D2"/>
<contactref element="OPR" pad="A"/>
</signal>
<signal name="CV2">
<contactref element="C" pad="V2"/>
<contactref element="MB6" pad="A"/>
</signal>
<signal name="CU2">
<contactref element="C" pad="U2"/>
<contactref element="MA6" pad="A"/>
</signal>
<signal name="CT2">
<contactref element="C" pad="T2"/>
<contactref element="MQ7" pad="A"/>
</signal>
<signal name="CS2">
<contactref element="C" pad="S2"/>
<contactref element="AC7" pad="A"/>
</signal>
<signal name="CR2">
<contactref element="C" pad="R2"/>
<contactref element="MB7" pad="A"/>
</signal>
<signal name="CP2">
<contactref element="C" pad="P2"/>
<contactref element="MA7" pad="A"/>
</signal>
<signal name="CN2">
<contactref element="C" pad="N2"/>
<contactref element="MQ8" pad="A"/>
</signal>
<signal name="CM2">
<contactref element="C" pad="M2"/>
<contactref element="AC8" pad="A"/>
</signal>
<signal name="CL2">
<contactref element="C" pad="L2"/>
<contactref element="MB8" pad="A"/>
</signal>
<signal name="CK2">
<contactref element="C" pad="K2"/>
<contactref element="MA8" pad="A"/>
</signal>
<signal name="CJ2">
<contactref element="C" pad="J2"/>
<contactref element="MQ9" pad="A"/>
</signal>
<signal name="CH2">
<contactref element="C" pad="H2"/>
<contactref element="AC9" pad="A"/>
</signal>
<signal name="CF2">
<contactref element="C" pad="F2"/>
<contactref element="MB9" pad="A"/>
</signal>
<signal name="CE2">
<contactref element="C" pad="E2"/>
<contactref element="MA9" pad="A"/>
</signal>
<signal name="CD2">
<contactref element="C" pad="D2"/>
<contactref element="MQ10" pad="A"/>
</signal>
<signal name="DV2">
<contactref element="D" pad="V2"/>
<contactref element="MQ2" pad="A"/>
</signal>
<signal name="DU2">
<contactref element="D" pad="U2"/>
<contactref element="MA3" pad="A"/>
</signal>
<signal name="DT2">
<contactref element="D" pad="T2"/>
<contactref element="MB3" pad="A"/>
</signal>
<signal name="DS2">
<contactref element="D" pad="S2"/>
<contactref element="MQ3" pad="A"/>
</signal>
<signal name="DR2">
<contactref element="D" pad="R2"/>
<contactref element="AC3" pad="A"/>
</signal>
<signal name="DP2">
<contactref element="D" pad="P2"/>
<contactref element="MA4" pad="A"/>
</signal>
<signal name="DN2">
<contactref element="D" pad="N2"/>
<contactref element="MB4" pad="A"/>
</signal>
<signal name="DM2">
<contactref element="D" pad="M2"/>
<contactref element="MQ4" pad="A"/>
</signal>
<signal name="DL2">
<contactref element="D" pad="L2"/>
<contactref element="AC4" pad="A"/>
</signal>
<signal name="DK2">
<contactref element="D" pad="K2"/>
<contactref element="MA5" pad="A"/>
</signal>
<signal name="DJ2">
<contactref element="D" pad="J2"/>
<contactref element="MB5" pad="A"/>
</signal>
<signal name="DH2">
<contactref element="D" pad="H2"/>
<contactref element="MQ5" pad="A"/>
</signal>
<signal name="DF2">
<contactref element="D" pad="F2"/>
<contactref element="AC5" pad="A"/>
</signal>
<signal name="DE2">
<contactref element="D" pad="E2"/>
<contactref element="AC6" pad="A"/>
</signal>
<signal name="DD2">
<contactref element="D" pad="D2"/>
<contactref element="MQ6" pad="A"/>
</signal>
<signal name="ES2">
<contactref element="E" pad="S2"/>
<contactref element="LINK" pad="A"/>
</signal>
<signal name="ER2">
<contactref element="E" pad="R2"/>
<contactref element="MA0" pad="A"/>
</signal>
<signal name="EP2">
<contactref element="E" pad="P2"/>
<contactref element="MB0" pad="A"/>
</signal>
<signal name="EN2">
<contactref element="E" pad="N2"/>
<contactref element="AC0" pad="A"/>
</signal>
<signal name="EM2">
<contactref element="E" pad="M2"/>
<contactref element="MQ0" pad="A"/>
</signal>
<signal name="EL2">
<contactref element="E" pad="L2"/>
<contactref element="MA1" pad="A"/>
</signal>
<signal name="EK2">
<contactref element="E" pad="K2"/>
<contactref element="MB1" pad="A"/>
</signal>
<signal name="EJ2">
<contactref element="E" pad="J2"/>
<contactref element="AC1" pad="A"/>
</signal>
<signal name="EH2">
<contactref element="E" pad="H2"/>
<contactref element="MQ1" pad="A"/>
</signal>
<signal name="EF2">
<contactref element="E" pad="F2"/>
<contactref element="MA2" pad="A"/>
</signal>
<signal name="EE2">
<contactref element="E" pad="E2"/>
<contactref element="MB2" pad="A"/>
</signal>
<signal name="ED2">
<contactref element="E" pad="D2"/>
<contactref element="AC2" pad="A"/>
</signal>
<signal name="FV2">
<contactref element="F" pad="V2"/>
<contactref element="ION" pad="A"/>
</signal>
<signal name="FU2">
<contactref element="F" pad="U2"/>
<contactref element="SPARE1" pad="A"/>
</signal>
<signal name="FT2">
<contactref element="F" pad="T2"/>
<contactref element="PARITY" pad="A"/>
</signal>
<signal name="FS2">
<contactref element="F" pad="S2"/>
<contactref element="SPARE2" pad="A"/>
</signal>
<signal name="FR2">
<contactref element="F" pad="R2"/>
<contactref element="PERR" pad="A"/>
</signal>
<signal name="FP2">
<contactref element="F" pad="P2"/>
<contactref element="SPARE3" pad="A"/>
</signal>
<signal name="FN2">
<contactref element="F" pad="N2"/>
<contactref element="SPARE4" pad="A"/>
</signal>
<signal name="FM2">
<contactref element="F" pad="M2"/>
<contactref element="IF0" pad="A"/>
</signal>
<signal name="FL2">
<contactref element="F" pad="L2"/>
<contactref element="IF1" pad="A"/>
</signal>
<signal name="FK2">
<contactref element="F" pad="K2"/>
<contactref element="IF2" pad="A"/>
</signal>
<signal name="FJ2">
<contactref element="F" pad="J2"/>
<contactref element="DF0" pad="A"/>
</signal>
<signal name="FH2">
<contactref element="F" pad="H2"/>
<contactref element="DF1" pad="A"/>
</signal>
<signal name="FF2">
<contactref element="F" pad="F2"/>
<contactref element="DF2" pad="A"/>
</signal>
<signal name="FE2">
<contactref element="PC0" pad="A"/>
<contactref element="F" pad="E2"/>
</signal>
<signal name="FD2">
<contactref element="PC1" pad="A"/>
<contactref element="F" pad="D2"/>
</signal>
<signal name="EV2">
<contactref element="PC2" pad="A"/>
<contactref element="E" pad="V2"/>
</signal>
<signal name="EU2">
<contactref element="PC3" pad="A"/>
<contactref element="E" pad="U2"/>
</signal>
<signal name="ET2">
<contactref element="PC4" pad="A"/>
<contactref element="E" pad="T2"/>
</signal>
<signal name="AB2">
<contactref element="A" pad="B2"/>
<contactref element="PC11" pad="B"/>
<contactref element="PC7" pad="B"/>
<contactref element="PC8" pad="B"/>
<contactref element="PC9" pad="B"/>
<contactref element="PC10" pad="B"/>
<contactref element="PC6" pad="B"/>
<contactref element="PC5" pad="B"/>
<contactref element="FETCH" pad="B"/>
<contactref element="INDEX" pad="B"/>
<contactref element="DEFER" pad="B"/>
<contactref element="EXEC" pad="B"/>
<contactref element="END" pad="B"/>
<contactref element="BREAK" pad="B"/>
<contactref element="PAUSE" pad="B"/>
<contactref element="RUN" pad="B"/>
</signal>
<signal name="BB2">
<contactref element="B" pad="B2"/>
<contactref element="AND" pad="B"/>
<contactref element="TAD" pad="B"/>
<contactref element="ISZ" pad="B"/>
<contactref element="DCA" pad="B"/>
<contactref element="JMS" pad="B"/>
<contactref element="JMP" pad="B"/>
<contactref element="IOT" pad="B"/>
<contactref element="OPR" pad="B"/>
</signal>
<signal name="CB2">
<contactref element="C" pad="B2"/>
<contactref element="AC11" pad="B"/>
<contactref element="AC7" pad="B"/>
<contactref element="AC8" pad="B"/>
<contactref element="AC9" pad="B"/>
<contactref element="AC10" pad="B"/>
<contactref element="MQ11" pad="B"/>
<contactref element="MQ7" pad="B"/>
<contactref element="MQ8" pad="B"/>
<contactref element="MQ9" pad="B"/>
<contactref element="MQ10" pad="B"/>
<contactref element="MA11" pad="B"/>
<contactref element="MA7" pad="B"/>
<contactref element="MA8" pad="B"/>
<contactref element="MA9" pad="B"/>
<contactref element="MA10" pad="B"/>
<contactref element="MB11" pad="B"/>
<contactref element="MB7" pad="B"/>
<contactref element="MB8" pad="B"/>
<contactref element="MB9" pad="B"/>
<contactref element="MB10" pad="B"/>
</signal>
<signal name="DB2">
<contactref element="D" pad="B2"/>
<contactref element="MB6" pad="B"/>
<contactref element="MB5" pad="B"/>
<contactref element="MB4" pad="B"/>
<contactref element="MB3" pad="B"/>
<contactref element="MQ6" pad="B"/>
<contactref element="MQ5" pad="B"/>
<contactref element="MQ4" pad="B"/>
<contactref element="MQ3" pad="B"/>
<contactref element="AC3" pad="B"/>
<contactref element="AC4" pad="B"/>
<contactref element="AC5" pad="B"/>
<contactref element="AC6" pad="B"/>
<contactref element="MA6" pad="B"/>
<contactref element="MA5" pad="B"/>
<contactref element="MA4" pad="B"/>
<contactref element="MA3" pad="B"/>
</signal>
<signal name="EB2">
<contactref element="E" pad="B2"/>
<contactref element="LINK" pad="B"/>
<contactref element="MQ0" pad="B"/>
<contactref element="MQ2" pad="B"/>
<contactref element="MQ1" pad="B"/>
<contactref element="AC0" pad="B"/>
<contactref element="AC1" pad="B"/>
<contactref element="AC2" pad="B"/>
<contactref element="MA0" pad="B"/>
<contactref element="MA2" pad="B"/>
<contactref element="MA1" pad="B"/>
<contactref element="MB0" pad="B"/>
<contactref element="MB2" pad="B"/>
<contactref element="MB1" pad="B"/>
</signal>
<signal name="FB2">
<contactref element="F" pad="B2"/>
<contactref element="IF0" pad="B"/>
<contactref element="IF2" pad="B"/>
<contactref element="IF1" pad="B"/>
<contactref element="PC4" pad="B"/>
<contactref element="PC3" pad="B"/>
<contactref element="PC0" pad="B"/>
<contactref element="PC2" pad="B"/>
<contactref element="PC1" pad="B"/>
<contactref element="DF0" pad="B"/>
<contactref element="DF2" pad="B"/>
<contactref element="DF1" pad="B"/>
<contactref element="PERR" pad="B"/>
<contactref element="SPARE2" pad="B"/>
<contactref element="PARITY" pad="B"/>
<contactref element="SPARE1" pad="B"/>
<contactref element="ION" pad="B"/>
<contactref element="SPARE3" pad="B"/>
<contactref element="SPARE4" pad="B"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
