<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>TSC8-75</text>
<text>EDUCOMP</text>
<text>CORPORATION</text>
<text>COPYRIGHT 1975</text>
<text>+</text>
<text>+</text>
<text>+</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="OMNIBUS">
<description>Quad-Height DEC board</description>
</package>
<package name="EDGE-CON8">
<description>Quad-Height DEC edge connector</description>
</package>
<package name="E12-8">
<description>A 0.8 inch electrolytic.</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
</packages>
</library>
<library name="atmel-cpld">
<packages>
<package name="PQFP-100">
<description>PQFP100
Quad flat pack 14mm x 20mm</description>
</package>
</packages>
</library>
<library name="con-harting-ml">
<packages>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="OMNIBUS" value="OUTLINE-OMNIBUS"/>
<element name="EDGE" library="dec-con" package="EDGE-CON8" value=""/>
<element name="R10" library="rcl" package="0204/7" value="39K"/>
<element name="C47" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="C46" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="C48" library="dec-con" package="E12-8" value="6.8uF"/>
<element name="C1" library="rcl" package="C050-025X075" value=".22uF"/>
<element name="C2" library="rcl" package="C050-025X075" value=".22uF"/>
<element name="C49" library="rcl" package="C050-025X075" value=""/>
<element name="E1" library="atmel-cpld" package="PQFP-100" value="ATF150X100PQFP"/>
<element name="ISP" library="con-harting-ml" package="ML10" value=""/>
</elements>
<signals>
<signal name="!DATA06">
<contactref element="EDGE" pad="BU1"/>
<contactref element="E1" pad="46"/>
</signal>
<signal name="!DATA09">
<contactref element="EDGE" pad="DS1"/>
<contactref element="E1" pad="2"/>
</signal>
<signal name="!DATA00">
<contactref element="EDGE" pad="AR1"/>
<contactref element="E1" pad="66"/>
</signal>
<signal name="!DATA03">
<contactref element="EDGE" pad="AV1"/>
<contactref element="E1" pad="62"/>
</signal>
<signal name="!DATA05">
<contactref element="EDGE" pad="BS1"/>
<contactref element="E1" pad="47"/>
</signal>
<signal name="!DATA02">
<contactref element="EDGE" pad="AU1"/>
<contactref element="E1" pad="63"/>
</signal>
<signal name="!DATA11">
<contactref element="EDGE" pad="DV1"/>
<contactref element="E1" pad="3"/>
</signal>
<signal name="!DATA08">
<contactref element="EDGE" pad="DR1"/>
<contactref element="E1" pad="4"/>
</signal>
<signal name="!DATA04">
<contactref element="EDGE" pad="BR1"/>
<contactref element="E1" pad="48"/>
</signal>
<signal name="!DATA01">
<contactref element="EDGE" pad="AS1"/>
<contactref element="E1" pad="65"/>
</signal>
<signal name="!DATA07">
<contactref element="EDGE" pad="BV1"/>
<contactref element="E1" pad="44"/>
</signal>
<signal name="!DATA10">
<contactref element="EDGE" pad="DU1"/>
<contactref element="E1" pad="1"/>
</signal>
<signal name="!SKIP">
<contactref element="EDGE" pad="CS1"/>
<contactref element="E1" pad="26"/>
</signal>
<signal name="!MD04">
<contactref element="EDGE" pad="BK1"/>
<contactref element="E1" pad="52"/>
</signal>
<signal name="!MD05">
<contactref element="EDGE" pad="BL1"/>
<contactref element="E1" pad="51"/>
</signal>
<signal name="!MD08">
<contactref element="EDGE" pad="DK1"/>
<contactref element="E1" pad="10"/>
</signal>
<signal name="!MD07">
<contactref element="EDGE" pad="BP1"/>
<contactref element="E1" pad="49"/>
</signal>
<signal name="!IO_PAUSE">
<contactref element="EDGE" pad="CD1"/>
<contactref element="E1" pad="38"/>
</signal>
<signal name="!INTERNAL_IO">
<contactref element="EDGE" pad="CL1"/>
<contactref element="E1" pad="30"/>
</signal>
<signal name="!MD10">
<contactref element="EDGE" pad="DM1"/>
<contactref element="E1" pad="8"/>
</signal>
<signal name="!MD11">
<contactref element="EDGE" pad="DP1"/>
<contactref element="E1" pad="7"/>
</signal>
<signal name="!MD09">
<contactref element="EDGE" pad="DL1"/>
<contactref element="E1" pad="9"/>
</signal>
<signal name="TP3">
<contactref element="EDGE" pad="CH2"/>
<contactref element="E1" pad="32"/>
</signal>
<signal name="!C0">
<contactref element="EDGE" pad="CE1"/>
<contactref element="E1" pad="35"/>
</signal>
<signal name="!C1">
<contactref element="EDGE" pad="CH1"/>
<contactref element="E1" pad="33"/>
</signal>
<signal name="TP4">
<contactref element="EDGE" pad="CJ2"/>
<contactref element="E1" pad="31"/>
</signal>
<signal name="INITIALIZE">
<contactref element="EDGE" pad="CR1"/>
<contactref element="E1" pad="27"/>
</signal>
<signal name="!MD03">
<contactref element="EDGE" pad="AP1"/>
<contactref element="E1" pad="67"/>
</signal>
<signal name="!INT_RQST">
<contactref element="EDGE" pad="CP1"/>
<contactref element="E1" pad="29"/>
</signal>
<signal name="!MA01">
<contactref element="EDGE" pad="AE1"/>
<contactref element="E1" pad="77"/>
</signal>
<signal name="!MD02">
<contactref element="EDGE" pad="AM1"/>
<contactref element="E1" pad="69"/>
</signal>
<signal name="!MD01">
<contactref element="EDGE" pad="AL1"/>
<contactref element="E1" pad="70"/>
</signal>
<signal name="!MD00">
<contactref element="EDGE" pad="AK1"/>
<contactref element="E1" pad="71"/>
</signal>
<signal name="!MA03">
<contactref element="EDGE" pad="AJ1"/>
<contactref element="E1" pad="73"/>
</signal>
<signal name="!MA02">
<contactref element="EDGE" pad="AH1"/>
<contactref element="E1" pad="74"/>
</signal>
<signal name="!MA00">
<contactref element="EDGE" pad="AD1"/>
<contactref element="E1" pad="78"/>
</signal>
<signal name="!MA04">
<contactref element="EDGE" pad="BD1"/>
<contactref element="E1" pad="57"/>
</signal>
<signal name="!MA07">
<contactref element="EDGE" pad="BJ1"/>
<contactref element="E1" pad="54"/>
</signal>
<signal name="!MA05">
<contactref element="EDGE" pad="BE1"/>
<contactref element="E1" pad="56"/>
</signal>
<signal name="!MA06">
<contactref element="EDGE" pad="BH1"/>
<contactref element="E1" pad="55"/>
</signal>
<signal name="!MA11">
<contactref element="EDGE" pad="DJ1"/>
<contactref element="E1" pad="15"/>
</signal>
<signal name="!MA08">
<contactref element="EDGE" pad="DD1"/>
<contactref element="E1" pad="19"/>
</signal>
<signal name="!MA09">
<contactref element="EDGE" pad="DE1"/>
<contactref element="E1" pad="18"/>
</signal>
<signal name="!MA10">
<contactref element="EDGE" pad="DH1"/>
<contactref element="E1" pad="16"/>
</signal>
<signal name="!MD_DIR">
<contactref element="EDGE" pad="AK2"/>
<contactref element="E1" pad="72"/>
</signal>
<signal name="TP2">
<contactref element="EDGE" pad="CE2"/>
<contactref element="E1" pad="34"/>
</signal>
<signal name="TP1">
<contactref element="EDGE" pad="CD2"/>
<contactref element="E1" pad="37"/>
</signal>
<signal name="!IR0">
<contactref element="EDGE" pad="DD2"/>
<contactref element="E1" pad="22"/>
</signal>
<signal name="USER_MODE">
<contactref element="EDGE" pad="DM2"/>
<contactref element="E1" pad="11"/>
</signal>
<signal name="!F">
<contactref element="EDGE" pad="DJ2"/>
<contactref element="E1" pad="14"/>
</signal>
<signal name="!E">
<contactref element="EDGE" pad="DL2"/>
<contactref element="E1" pad="12"/>
</signal>
<signal name="VCC">
<contactref element="EDGE" pad="BA2"/>
<contactref element="EDGE" pad="CA2"/>
<contactref element="C47" pad="+"/>
<contactref element="C46" pad="+"/>
<contactref element="C48" pad="+"/>
<contactref element="EDGE" pad="AA2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="E1" pad="84"/>
<contactref element="E1" pad="41"/>
<contactref element="E1" pad="93"/>
<contactref element="E1" pad="20"/>
<contactref element="E1" pad="36"/>
<contactref element="E1" pad="53"/>
<contactref element="E1" pad="68"/>
<contactref element="E1" pad="5"/>
<contactref element="ISP" pad="4"/>
</signal>
<signal name="GND">
<contactref element="EDGE" pad="AC2"/>
<contactref element="EDGE" pad="AF1"/>
<contactref element="EDGE" pad="AF2"/>
<contactref element="EDGE" pad="AN1"/>
<contactref element="EDGE" pad="AN2"/>
<contactref element="EDGE" pad="AT1"/>
<contactref element="EDGE" pad="AT2"/>
<contactref element="EDGE" pad="BF1"/>
<contactref element="EDGE" pad="BF2"/>
<contactref element="EDGE" pad="BN1"/>
<contactref element="EDGE" pad="BN2"/>
<contactref element="EDGE" pad="DC1"/>
<contactref element="EDGE" pad="DC2"/>
<contactref element="EDGE" pad="DF1"/>
<contactref element="EDGE" pad="DF2"/>
<contactref element="EDGE" pad="DT1"/>
<contactref element="EDGE" pad="DT2"/>
<contactref element="EDGE" pad="DN2"/>
<contactref element="EDGE" pad="DN1"/>
<contactref element="EDGE" pad="CT2"/>
<contactref element="EDGE" pad="CT1"/>
<contactref element="EDGE" pad="BT2"/>
<contactref element="EDGE" pad="BT1"/>
<contactref element="EDGE" pad="CN2"/>
<contactref element="EDGE" pad="CN1"/>
<contactref element="EDGE" pad="CC2"/>
<contactref element="EDGE" pad="CF2"/>
<contactref element="EDGE" pad="CF1"/>
<contactref element="EDGE" pad="BC2"/>
<contactref element="EDGE" pad="BC1"/>
<contactref element="C47" pad="-"/>
<contactref element="C46" pad="-"/>
<contactref element="C48" pad="-"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="EDGE" pad="CC1"/>
<contactref element="E1" pad="13"/>
<contactref element="E1" pad="28"/>
<contactref element="E1" pad="40"/>
<contactref element="E1" pad="45"/>
<contactref element="E1" pad="61"/>
<contactref element="E1" pad="76"/>
<contactref element="E1" pad="88"/>
<contactref element="E1" pad="97"/>
<contactref element="ISP" pad="2"/>
<contactref element="ISP" pad="10"/>
</signal>
<signal name="!MD06">
<contactref element="EDGE" pad="BM1"/>
<contactref element="E1" pad="50"/>
</signal>
<signal name="N$63">
<contactref element="R10" pad="1"/>
<contactref element="E1" pad="83"/>
</signal>
<signal name="!IR1">
<contactref element="EDGE" pad="DE2"/>
<contactref element="E1" pad="21"/>
</signal>
<signal name="N$558">
<contactref element="E1" pad="82"/>
<contactref element="R10" pad="2"/>
<contactref element="C49" pad="2"/>
</signal>
<signal name="TDI">
<contactref element="ISP" pad="9"/>
<contactref element="E1" pad="6"/>
</signal>
<signal name="TDO">
<contactref element="ISP" pad="3"/>
<contactref element="E1" pad="75"/>
</signal>
<signal name="TCK">
<contactref element="ISP" pad="1"/>
<contactref element="E1" pad="64"/>
</signal>
<signal name="TMS">
<contactref element="ISP" pad="5"/>
<contactref element="E1" pad="17"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
