<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="68.58" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="62.23" width="0" layer="20"/>
<wire x1="0" y1="62.23" x2="71.755" y2="62.23" width="0" layer="20"/>
<text>C:/Users/Vince/Documents/websvn/trunk/Eagle/projects/DEC/Wxxx/W021/W021Abackfb.bmp</text>
<text>SIGNAL CABLE CONNECTOR W011B</text>
<text>10-69</text>
<text>FLIP CHIP</text>
<hole x="5.08" y="56.515" drill="3.2512"/>
<hole x="5.08" y="5.715" drill="3.2512"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
<package name="0465">
<description>Drill 0.0465" (#56)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="GND1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BLK1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="WHT1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND3" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BLU1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND4" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GRN1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND5" library="dec-con" package="0465" value="PAD-0465"/>
<element name="RED1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND6" library="dec-con" package="0465" value="PAD-0465"/>
<element name="WHT2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND7" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GRN2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND8" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BLU2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GND9" library="dec-con" package="0465" value="PAD-0465"/>
<element name="RED2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="NC" library="dec-con" package="0465" value="PAD-0465"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="C2"/>
<contactref element="U$2" pad="U2"/>
<contactref element="U$2" pad="R2"/>
<contactref element="U$2" pad="L2"/>
<contactref element="U$2" pad="N2"/>
<contactref element="U$2" pad="J2"/>
<contactref element="U$2" pad="F2"/>
<contactref element="GND1" pad="P$1"/>
<contactref element="GND2" pad="P$1"/>
<contactref element="GND3" pad="P$1"/>
<contactref element="GND4" pad="P$1"/>
<contactref element="GND5" pad="P$1"/>
<contactref element="GND6" pad="P$1"/>
<contactref element="GND7" pad="P$1"/>
<contactref element="GND8" pad="P$1"/>
<contactref element="GND9" pad="P$1"/>
<contactref element="NC" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="E2"/>
<contactref element="WHT1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="H2"/>
<contactref element="BLU1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="K2"/>
<contactref element="GRN1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="M2"/>
<contactref element="RED1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="P2"/>
<contactref element="WHT2" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="S2"/>
<contactref element="GRN2" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="T2"/>
<contactref element="BLU2" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="V2"/>
<contactref element="RED2" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="D2"/>
<contactref element="BLK1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
