<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="22.86" y1="40.64" x2="27.94" y2="40.64" width="0" layer="20" curve="-180"/>
<wire x1="49.53" y1="40.64" x2="54.61" y2="40.64" width="0" layer="20" curve="-180"/>
<wire x1="27.94" y1="20.32" x2="22.86" y2="20.32" width="0" layer="20" curve="-180"/>
<wire x1="54.61" y1="20.32" x2="49.53" y2="20.32" width="0" layer="20" curve="-180"/>
<wire x1="22.86" y1="40.64" x2="22.86" y2="20.32" width="0" layer="20"/>
<wire x1="27.94" y1="40.64" x2="27.94" y2="20.32" width="0" layer="20"/>
<wire x1="49.53" y1="40.64" x2="49.53" y2="20.32" width="0" layer="20"/>
<wire x1="54.61" y1="40.64" x2="54.61" y2="20.32" width="0" layer="20"/>
<text>C:/Users/Vince/Documents/websvn/trunk/Eagle/projects/DEC/Wxxx/W021/W021Abackfb.bmp</text>
<text>W021B</text>
<text>1-68</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
<package name="0465">
<description>Drill 0.0465" (#56)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="U$2" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="BLK1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BRN1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="RED1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="ORN1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="YEL1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GRN1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BLU1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="VIO1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GRY1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="WHT1" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BLK2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BRN2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="RED2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="ORN2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="YEL2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GRN2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BLU2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="VIO2" library="dec-con" package="0465" value="PAD-0465"/>
<element name="GRY2" library="dec-con" package="0465" value="PAD-0465"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="C2"/>
<contactref element="U$2" pad="U2"/>
<contactref element="U$2" pad="R2"/>
<contactref element="U$2" pad="L2"/>
<contactref element="U$2" pad="N2"/>
<contactref element="U$2" pad="J2"/>
<contactref element="U$2" pad="F2"/>
<contactref element="BLK1" pad="P$1"/>
<contactref element="RED1" pad="P$1"/>
<contactref element="YEL1" pad="P$1"/>
<contactref element="BLU1" pad="P$1"/>
<contactref element="GRY1" pad="P$1"/>
<contactref element="BLK2" pad="P$1"/>
<contactref element="RED2" pad="P$1"/>
<contactref element="YEL2" pad="P$1"/>
<contactref element="BLU2" pad="P$1"/>
<contactref element="GRY2" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="E2"/>
<contactref element="ORN1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="H2"/>
<contactref element="GRN1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="K2"/>
<contactref element="VIO1" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="M2"/>
<contactref element="WHT1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="P2"/>
<contactref element="BRN2" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="S2"/>
<contactref element="ORN2" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="T2"/>
<contactref element="GRN2" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="V2"/>
<contactref element="VIO2" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="D2"/>
<contactref element="BRN1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
