<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>CONNECTOR BOARD W025A</text>
<text>10-68</text>
<hole x="88.9" y="126.365" drill="3.175"/>
<hole x="88.9" y="5.715" drill="3.175"/>
<hole x="88.9" y="56.515" drill="3.175"/>
<hole x="88.9" y="75.565" drill="3.175"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="DOUBLE">
<description>Double-Height DEC board</description>
</package>
<package name="EDGE-CON4">
<description>Double-Height DEC edge connector</description>
</package>
<package name="0465">
<description>Drill 0.0465" (#56)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BC" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BD" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BE" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BF" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BH" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BJ" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BK" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BL" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BM" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BN" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BP" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BR" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BS" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BT" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BU" library="dec-con" package="0465" value="PAD-0465"/>
<element name="BV" library="dec-con" package="0465" value="PAD-0465"/>
<element name="U$1" library="dec-con" package="DOUBLE" value="OUTLINE-DOUBLE"/>
<element name="U$3" library="dec-con" package="EDGE-CON4" value=""/>
<element name="AC" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AD" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AE" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AF" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AH" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AJ" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AK" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AL" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AM" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AN" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AP" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AR" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AS" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AT" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AU" library="dec-con" package="0465" value="PAD-0465"/>
<element name="AV" library="dec-con" package="0465" value="PAD-0465"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="BE" pad="P$1"/>
<contactref element="U$3" pad="BE2"/>
</signal>
<signal name="N$2">
<contactref element="BH" pad="P$1"/>
<contactref element="U$3" pad="BH2"/>
</signal>
<signal name="N$3">
<contactref element="BK" pad="P$1"/>
<contactref element="U$3" pad="BK2"/>
</signal>
<signal name="N$4">
<contactref element="BM" pad="P$1"/>
<contactref element="U$3" pad="BM2"/>
</signal>
<signal name="N$5">
<contactref element="BP" pad="P$1"/>
<contactref element="U$3" pad="BP2"/>
</signal>
<signal name="N$6">
<contactref element="BS" pad="P$1"/>
<contactref element="U$3" pad="BS2"/>
</signal>
<signal name="N$7">
<contactref element="BT" pad="P$1"/>
<contactref element="U$3" pad="BT2"/>
</signal>
<signal name="N$9">
<contactref element="BD" pad="P$1"/>
<contactref element="U$3" pad="BD2"/>
</signal>
<signal name="N$15">
<contactref element="BF" pad="P$1"/>
<contactref element="U$3" pad="BF2"/>
</signal>
<signal name="N$16">
<contactref element="BJ" pad="P$1"/>
<contactref element="U$3" pad="BJ2"/>
</signal>
<signal name="N$17">
<contactref element="BL" pad="P$1"/>
<contactref element="U$3" pad="BL2"/>
</signal>
<signal name="N$18">
<contactref element="BN" pad="P$1"/>
<contactref element="U$3" pad="BN2"/>
</signal>
<signal name="N$19">
<contactref element="BR" pad="P$1"/>
<contactref element="U$3" pad="BR2"/>
</signal>
<signal name="N$20">
<contactref element="BU" pad="P$1"/>
<contactref element="U$3" pad="BU2"/>
</signal>
<signal name="N$12">
<contactref element="BV" pad="P$1"/>
<contactref element="U$3" pad="BV2"/>
</signal>
<signal name="N$13">
<contactref element="BC" pad="P$1"/>
<contactref element="U$3" pad="BC2"/>
</signal>
<signal name="N$8">
<contactref element="AE" pad="P$1"/>
<contactref element="U$3" pad="AE2"/>
</signal>
<signal name="N$14">
<contactref element="AH" pad="P$1"/>
<contactref element="U$3" pad="AH2"/>
</signal>
<signal name="N$21">
<contactref element="AK" pad="P$1"/>
<contactref element="U$3" pad="AK2"/>
</signal>
<signal name="N$22">
<contactref element="AM" pad="P$1"/>
<contactref element="U$3" pad="AM2"/>
</signal>
<signal name="N$23">
<contactref element="AP" pad="P$1"/>
<contactref element="U$3" pad="AP2"/>
</signal>
<signal name="N$24">
<contactref element="AS" pad="P$1"/>
<contactref element="U$3" pad="AS2"/>
</signal>
<signal name="N$25">
<contactref element="AT" pad="P$1"/>
<contactref element="U$3" pad="AT2"/>
</signal>
<signal name="N$26">
<contactref element="AD" pad="P$1"/>
<contactref element="U$3" pad="AD2"/>
</signal>
<signal name="N$29">
<contactref element="AF" pad="P$1"/>
<contactref element="U$3" pad="AF2"/>
</signal>
<signal name="N$30">
<contactref element="AJ" pad="P$1"/>
<contactref element="U$3" pad="AJ2"/>
</signal>
<signal name="N$31">
<contactref element="AL" pad="P$1"/>
<contactref element="U$3" pad="AL2"/>
</signal>
<signal name="N$32">
<contactref element="AN" pad="P$1"/>
<contactref element="U$3" pad="AN2"/>
</signal>
<signal name="N$33">
<contactref element="AR" pad="P$1"/>
<contactref element="U$3" pad="AR2"/>
</signal>
<signal name="N$34">
<contactref element="AU" pad="P$1"/>
<contactref element="U$3" pad="AU2"/>
</signal>
<signal name="N$35">
<contactref element="AV" pad="P$1"/>
<contactref element="U$3" pad="AV2"/>
</signal>
<signal name="N$36">
<contactref element="AC" pad="P$1"/>
<contactref element="U$3" pad="AC2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
