<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="19.05" y1="62.23" x2="63.5" y2="62.23" width="0" layer="20"/>
<wire x1="63.5" y1="62.23" x2="63.5" y2="0" width="0" layer="20"/>
<wire x1="63.5" y1="0" x2="15.875" y2="0" width="0" layer="20"/>
<text>W404</text>
<text>CS*ABCDEFHJKLMNPRSTUV</text>
<text>FLIP CHIP</text>
<text>5009588C</text>
<text>C:/Users/Vince/Documents/eagle/projects/DEC/Wxxx/W404/W404Cbackfb.bmp</text>
<text>6-74P</text>
<text>DTR JUMPER</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
<package name="0818/25">
<description>One inch resistor package</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="R1" library="dec-con" package="0818/25" value="1K"/>
<element name="R2" library="dec-con" package="0818/25" value="1K"/>
</elements>
<signals>
<signal name="N$10">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="R2"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="T2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="N2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
