<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
<package name="C063-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
<element name="U$2" library="dec-con" package="EDGE-CON1" value="EDGE-1"/>
<element name="C1" library="dec-con" package="C063-025X075" value=".01uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="C2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="A2"/>
</signal>
<signal name="P2">
<contactref element="U$2" pad="P2"/>
</signal>
<signal name="V2">
<contactref element="U$2" pad="V2"/>
</signal>
<signal name="U2">
<contactref element="U$2" pad="U2"/>
</signal>
<signal name="T2">
<contactref element="U$2" pad="T2"/>
</signal>
<signal name="S2">
<contactref element="U$2" pad="S2"/>
</signal>
<signal name="D2">
<contactref element="U$2" pad="D2"/>
</signal>
<signal name="E2">
<contactref element="U$2" pad="E2"/>
</signal>
<signal name="F2">
<contactref element="U$2" pad="F2"/>
</signal>
<signal name="H2">
<contactref element="U$2" pad="H2"/>
</signal>
<signal name="J2">
<contactref element="U$2" pad="J2"/>
</signal>
<signal name="K2">
<contactref element="U$2" pad="K2"/>
</signal>
<signal name="L2">
<contactref element="U$2" pad="L2"/>
</signal>
<signal name="M2">
<contactref element="U$2" pad="M2"/>
</signal>
<signal name="N2">
<contactref element="U$2" pad="N2"/>
</signal>
<signal name="R2">
<contactref element="U$2" pad="R2"/>
</signal>
<signal name="-15V">
<contactref element="U$2" pad="B2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
