<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="SD_CARD">
<description>SD Card Receptacle</description>
</package>
</packages>
<symbols>
<symbol name="SD_CARD">
<pin name="CD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="CMD" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="GND$1" direction="pwr"/>
<pin name="GND$2" direction="pwr"/>
<pin name="SW1" direction="in"/>
<pin name="SW2" direction="out"/>
<pin name="SW3" direction="out"/>
<pin name="VDD" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SD_CARD" prefix="SD">
<description>SD Card Socket</description>
<gates>
<gate name="G$1" symbol="SD_CARD"/>
</gates>
<devices>
<device name="" package="SD_CARD">
<connects>
<connect gate="G$1" pin="CD" pad="DAT3"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="D0" pad="DAT0"/>
<connect gate="G$1" pin="D1" pad="DAT1"/>
<connect gate="G$1" pin="D2" pad="DAT2"/>
<connect gate="G$1" pin="GND$1" pad="VSS$1"/>
<connect gate="G$1" pin="GND$2" pad="VSS$2"/>
<connect gate="G$1" pin="SW1" pad="SW1"/>
<connect gate="G$1" pin="SW2" pad="SW2"/>
<connect gate="G$1" pin="SW3" pad="SW3"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
