<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.9525" y1="21.59" x2="-0.9525" y2="93.98" width="0" layer="20"/>
<wire x1="-0.9525" y1="93.98" x2="264.4775" y2="93.98" width="0" layer="20"/>
<wire x1="264.4775" y1="93.98" x2="264.4775" y2="21.59" width="0" layer="20"/>
<text>JTAG - ISP</text>
<text>RX ADDR</text>
<text>TX ADDR</text>
</plain>
<libraries>
<library name="alan_common">
<description>Alan's frequently used manually inputted parts</description>
<packages>
<package name="DEC_OMNIBUS_QUAD">
<description>Quad-Height DEC board</description>
</package>
<package name="PLCC84">
</package>
<package name="C_TH_5MM">
<description>CAPACITOR
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="RN_SIP9">
</package>
<package name="SW_DIP-6_ROUND">
</package>
<package name="LED_TH_3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="R_204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="HDR_2X5">
</package>
<package name="XTAL_CAN_HALFSIZE">
</package>
<package name="AMP_DB-9RA">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="OMNI" library="alan_common" package="DEC_OMNIBUS_QUAD" value="DEC_OMNIBUS_QUAD"/>
<element name="D1" library="alan_common" package="LED_TH_3MM" value="LED">
<attribute name="NAME"/>
</element>
<element name="D2" library="alan_common" package="LED_TH_3MM" value="LED">
<attribute name="NAME"/>
</element>
<element name="D3" library="alan_common" package="LED_TH_3MM" value="LED">
<attribute name="NAME"/>
</element>
<element name="U$6" library="alan_common" package="SW_DIP-6_ROUND" value="SW_DIP-6R"/>
<element name="U$7" library="alan_common" package="SW_DIP-6_ROUND" value="SW_DIP-6R"/>
<element name="RN1" library="alan_common" package="RN_SIP9" value="47K">
<attribute name="NAME"/>
</element>
<element name="RN2" library="alan_common" package="RN_SIP9" value="RNET_X8_SIP">
<attribute name="NAME"/>
</element>
<element name="R1" library="alan_common" package="R_204/7" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="alan_common" package="R_204/7" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="alan_common" package="R_204/7" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="alan_common" package="PLCC84" value="ATF1508AS">
<attribute name="NAME"/>
</element>
<element name="J3" library="alan_common" package="HDR_2X5" value="HDR_2X5&quot;"/>
<element name="C5" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="XO1" library="alan_common" package="XTAL_CAN_HALFSIZE" value="XTAL_CAN_HALFSIZE"/>
<element name="C2" library="alan_common" package="C_TH_5MM" value="10uF">
<attribute name="NAME"/>
</element>
<element name="USB" library="alan_common" package="AMP_DB-9RA" value="DB9">
<attribute name="MANF" value="TE/AMP"/>
<attribute name="MOUSER#" value="571-1734352-1"/>
<attribute name="MANF#" value="1734352-1"/>
</element>
<element name="C1" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="OMNI" pad="A1F"/>
<contactref element="OMNI" pad="A2F"/>
<contactref element="OMNI" pad="A2N"/>
<contactref element="OMNI" pad="A2T"/>
<contactref element="OMNI" pad="A2C"/>
<contactref element="OMNI" pad="C1C"/>
<contactref element="OMNI" pad="C1F"/>
<contactref element="OMNI" pad="C1T"/>
<contactref element="OMNI" pad="C2T"/>
<contactref element="OMNI" pad="C2C"/>
<contactref element="OMNI" pad="C2F"/>
<contactref element="OMNI" pad="C2N"/>
<contactref element="OMNI" pad="D1C"/>
<contactref element="OMNI" pad="D1F"/>
<contactref element="OMNI" pad="D2C"/>
<contactref element="OMNI" pad="D2N"/>
<contactref element="OMNI" pad="D2F"/>
<contactref element="OMNI" pad="B1F"/>
<contactref element="OMNI" pad="B1C"/>
<contactref element="OMNI" pad="B2C"/>
<contactref element="OMNI" pad="B2F"/>
<contactref element="OMNI" pad="B2N"/>
<contactref element="OMNI" pad="B2T"/>
<contactref element="U1" pad="72"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="82"/>
<contactref element="U1" pad="59"/>
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="42"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="10"/>
<contactref element="D1" pad="K"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="XO1" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$7" pad="6"/>
<contactref element="U$7" pad="5"/>
<contactref element="U$7" pad="4"/>
<contactref element="U$7" pad="3"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$6" pad="6"/>
<contactref element="U$6" pad="5"/>
<contactref element="U$6" pad="4"/>
<contactref element="U$6" pad="3"/>
<contactref element="U$6" pad="2"/>
<contactref element="U$6" pad="1"/>
<contactref element="USB" pad="G1"/>
<contactref element="USB" pad="5"/>
<contactref element="USB" pad="G2"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="78"/>
<contactref element="U1" pad="66"/>
<contactref element="U1" pad="43"/>
<contactref element="U1" pad="53"/>
<contactref element="J3" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="RN1" pad="1"/>
<contactref element="RN2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="XO1" pad="8"/>
<contactref element="OMNI" pad="A2A"/>
</signal>
<signal name="MD0">
<contactref element="OMNI" pad="A1K"/>
<contactref element="U1" pad="63"/>
</signal>
<signal name="MD1">
<contactref element="OMNI" pad="A1L"/>
<contactref element="U1" pad="60"/>
</signal>
<signal name="MD2">
<contactref element="OMNI" pad="A1M"/>
<contactref element="U1" pad="61"/>
</signal>
<signal name="MD3">
<contactref element="OMNI" pad="A1P"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="DATA0">
<contactref element="OMNI" pad="A1R"/>
<contactref element="U1" pad="65"/>
</signal>
<signal name="DATA1">
<contactref element="OMNI" pad="A1S"/>
<contactref element="U1" pad="56"/>
</signal>
<signal name="DATA2">
<contactref element="OMNI" pad="A1U"/>
<contactref element="U1" pad="57"/>
</signal>
<signal name="DATA3">
<contactref element="OMNI" pad="A1V"/>
<contactref element="U1" pad="54"/>
</signal>
<signal name="DATA5">
<contactref element="OMNI" pad="B1S"/>
<contactref element="U1" pad="48"/>
</signal>
<signal name="DATA6">
<contactref element="OMNI" pad="B1U"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="DATA7">
<contactref element="OMNI" pad="B1V"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="MD4">
<contactref element="OMNI" pad="B1K"/>
<contactref element="U1" pad="55"/>
</signal>
<signal name="MD5">
<contactref element="OMNI" pad="B1L"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="MD6">
<contactref element="OMNI" pad="B1M"/>
<contactref element="U1" pad="52"/>
</signal>
<signal name="MD7">
<contactref element="OMNI" pad="B1P"/>
<contactref element="U1" pad="49"/>
</signal>
<signal name="DATA4">
<contactref element="OMNI" pad="B1R"/>
<contactref element="U1" pad="50"/>
</signal>
<signal name="IO_PAUSE">
<contactref element="OMNI" pad="C1D"/>
<contactref element="U1" pad="41"/>
</signal>
<signal name="C0">
<contactref element="OMNI" pad="C1E"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="C1">
<contactref element="OMNI" pad="C1H"/>
<contactref element="U1" pad="37"/>
</signal>
<signal name="TP3">
<contactref element="OMNI" pad="C2H"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="INT_IO">
<contactref element="OMNI" pad="C1L"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="TS3">
<contactref element="OMNI" pad="C2M"/>
<contactref element="U1" pad="35"/>
</signal>
<signal name="INT_RQST">
<contactref element="OMNI" pad="C1P"/>
<contactref element="U1" pad="34"/>
</signal>
<signal name="INIT">
<contactref element="OMNI" pad="C1R"/>
<contactref element="U1" pad="33"/>
</signal>
<signal name="SKIP">
<contactref element="OMNI" pad="C1S"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="MD8">
<contactref element="OMNI" pad="D1K"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="MD9">
<contactref element="OMNI" pad="D1L"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="MD10">
<contactref element="OMNI" pad="D1M"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="MD11">
<contactref element="OMNI" pad="D1P"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="DATA8">
<contactref element="OMNI" pad="D1R"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="DATA9">
<contactref element="OMNI" pad="D1S"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="DATA10">
<contactref element="OMNI" pad="D1U"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="DATA11">
<contactref element="OMNI" pad="D1V"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="SW">
<contactref element="OMNI" pad="D2V"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="M_TCK">
<contactref element="U1" pad="62"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="M_TMS">
<contactref element="U1" pad="23"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="M_TDI">
<contactref element="U1" pad="14"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="M_TDO">
<contactref element="U1" pad="71"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="U3">
<contactref element="U1" pad="9"/>
<contactref element="USB" pad="3"/>
</signal>
<signal name="U2">
<contactref element="U1" pad="11"/>
<contactref element="USB" pad="2"/>
</signal>
<signal name="RX5">
<contactref element="RN1" pad="7"/>
<contactref element="U$6" pad="7"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="RX4">
<contactref element="RN1" pad="6"/>
<contactref element="U$6" pad="8"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="RX3">
<contactref element="RN1" pad="5"/>
<contactref element="U$6" pad="9"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="RX2">
<contactref element="RN1" pad="4"/>
<contactref element="U$6" pad="10"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="RX1">
<contactref element="RN1" pad="3"/>
<contactref element="U$6" pad="11"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="RX0">
<contactref element="RN1" pad="2"/>
<contactref element="U$6" pad="12"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="TX5">
<contactref element="RN2" pad="2"/>
<contactref element="U$7" pad="7"/>
<contactref element="U1" pad="76"/>
</signal>
<signal name="TX4">
<contactref element="RN2" pad="3"/>
<contactref element="U$7" pad="8"/>
<contactref element="U1" pad="73"/>
</signal>
<signal name="TX3">
<contactref element="RN2" pad="4"/>
<contactref element="U$7" pad="9"/>
<contactref element="U1" pad="70"/>
</signal>
<signal name="TX2">
<contactref element="RN2" pad="5"/>
<contactref element="U$7" pad="10"/>
<contactref element="U1" pad="69"/>
</signal>
<signal name="TX1">
<contactref element="RN2" pad="6"/>
<contactref element="U$7" pad="11"/>
<contactref element="U1" pad="68"/>
</signal>
<signal name="TX0">
<contactref element="RN2" pad="7"/>
<contactref element="U$7" pad="12"/>
<contactref element="U1" pad="67"/>
</signal>
<signal name="SYSCLK">
<contactref element="XO1" pad="5"/>
<contactref element="U1" pad="81"/>
</signal>
<signal name="LED0">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="79"/>
</signal>
<signal name="LED1">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="75"/>
</signal>
<signal name="LED2">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="77"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
