<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Microcontroller based on the amazing AVR RISC Core&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;/ul&gt;
&lt;author&gt;Revised by info@embedit.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="DIL20">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="S44">
<description>&lt;B&gt;Throughhole Plastic J-Leaded Chip Carrier Socket&lt;/B&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;B&gt;Plastic J-Leaded Chip Carrier&lt;/B&gt;</description>
</package>
<package name="PLCC-SM44">
<description>&lt;B&gt;SMD Plastic J-Leaded Chip Carrier Socket&lt;/B&gt;</description>
</package>
<package name="SSOP20D8">
<description>&lt;B&gt;Plastic Shrink Small Outline Package&lt;/B&gt;</description>
</package>
<package name="TQFP64">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="TQFP32-0762">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.762 mm</description>
</package>
<package name="SO20L">
<description>&lt;B&gt;Small Outline Package&lt;/B&gt;</description>
</package>
<package name="TQFP48">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="SOIC20S">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="LOGO">
<description>&lt;B&gt;Logo&lt;/B&gt;</description>
</package>
<package name="PQFP44">
<description>&lt;B&gt;Plastic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="TQFP44">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="PLCC32R">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
rectangle</description>
</package>
<package name="TSOP32">
<description>&lt;b&gt;TSOP32&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO32X">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
extra wide body 8.9 mm/JEDEC MO-120AC</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;100-lead Thin Quad Flat Pack Package Outline&lt;/b&gt;</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF64">
<description>&lt;b&gt;64M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF44">
<description>&lt;b&gt;44M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="PSSO20">
<description>&lt;b&gt;PSSO20&lt;/b&gt;</description>
</package>
<package name="MLF16">
<description>&lt;b&gt;HP-VFQFP-N16&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="D24-3/16">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.4 inch</description>
</package>
<package name="DD-3">
<description>&lt;b&gt;DPAC&lt;/b&gt;</description>
</package>
<package name="DD-7">
<description>&lt;b&gt;DPAC&lt;b&gt;</description>
</package>
<package name="DIL08$">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL14/7">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL16/8">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL20$">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL24-3/12">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL24-4">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.4 inch</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL24/12">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="DIL24/16">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL28-3$">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL28/3">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL28S">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.3 inch</description>
</package>
<package name="MSOP08">
<description>&lt;b&gt;Mini Small Outline Package&lt;/b&gt;</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
 square</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
 square</description>
</package>
<package name="PLCC_S28">
<description>&lt;b&gt;SOCKET&lt;/b&gt;&lt;p&gt;
 Plastic leaded chip carrier, square</description>
</package>
<package name="QSOP20">
<description>&lt;b&gt;Quarter-Size Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO08-GW">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, gull wing</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO16-1">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO16-1/8">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO18L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="SO20L$">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="SO24L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="SO28-3">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO28-3/8">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO28-3/12">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOJ28-4">
<description>&lt;b&gt;Small Outline J-Lead Package&lt;/b&gt;</description>
</package>
<package name="SOP08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOP16">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOP20">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOT23/5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SSOP16BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP16DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP20BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP20DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP24BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP24DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP28BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP28DL">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP48DL">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP56DL">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="TO-220G5">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="TO99">
<description>&lt;b&gt;Metal can Package&lt;/b&gt;</description>
</package>
<package name="TO220-5">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="TO220-7">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="TSSOP024">
<description>&lt;b&gt;Thin Shrink Small Outline Package&lt;/b&gt;</description>
</package>
<package name="ZZ326">
<description>&lt;b&gt;Special Package&lt;/b&gt;</description>
</package>
<package name="TINY13M">
</package>
</packages>
<symbols>
<symbol name="6-I/O-1">
<pin name="(XTAL2)PB4"/>
<pin name="(XTAL1)PB3"/>
<pin name="(RESET)PB5"/>
<pin name="(T0)PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="6-I/O-2">
<pin name="(XTAL2)PB4"/>
<pin name="(XTAL1)PB3"/>
<pin name="(RESET)PB5"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="5-I/O-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PB4"/>
<pin name="(CLOCK)PB3"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
</symbol>
<symbol name="6-I/O-3">
<pin name="(ADC3)PB4"/>
<pin name="(ADC2)PB3"/>
<pin name="(ADC0)PB5"/>
<pin name="(ADC1)PB2"/>
<pin name="(OCP)PB1"/>
<pin name="(AREF)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="16-I/O-1">
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="(ADC3)PB4"/>
<pin name="(ADC2)PB3"/>
<pin name="(ADC1)PB2"/>
<pin name="(OCP)PB1"/>
<pin name="(AVREF)PB0"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PC7"/>
<pin name="(ADC0)PB5"/>
</symbol>
<symbol name="15-I/O-1">
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="PB4"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="(T0)PD4"/>
<pin name="PD3"/>
<pin name="(INT0)PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" function="dot"/>
</symbol>
<symbol name="3-I/O-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
</symbol>
<symbol name="20-I/O-1">
<pin name="(ADC5)PC5"/>
<pin name="(ADC4)PC4"/>
<pin name="(ADC3)PC3"/>
<pin name="(ADC2)PC2"/>
<pin name="(ADC1)PC1"/>
<pin name="(ADC0)PC0"/>
<pin name="(SCK)PB5"/>
<pin name="(MISO)PB4"/>
<pin name="(MOSI)PB3"/>
<pin name="(SS)PB2"/>
<pin name="(OC1)PB1"/>
<pin name="(ICP)PB0"/>
<pin name="(AIN1)PD7"/>
<pin name="(AIN0)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="NC4" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="32-I/O-1">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="OC1B"/>
<pin name="ALE"/>
<pin name="ICP"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
</symbol>
<symbol name="32-I/O-2">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="OC1B"/>
<pin name="ALE"/>
<pin name="ICP"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="48-I/O-1">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4)" direction="in"/>
<pin name="PF5(ADC5)" direction="in"/>
<pin name="PF6(ADC6)" direction="in"/>
<pin name="PF7(ADC7)" direction="in"/>
<pin name="(RXD)PE0"/>
<pin name="(TXD)PE1"/>
<pin name="(AC+)PE2"/>
<pin name="(AC-)PE3"/>
<pin name="(INT4)PE4"/>
<pin name="(INT5)PE5"/>
<pin name="(INT6)PE6"/>
<pin name="(INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(INT3)PD3"/>
<pin name="(INT2)PD2"/>
<pin name="(INT1)PD1"/>
<pin name="(INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2"/>
<pin name="TOSC1"/>
<pin name="WR" function="dot"/>
<pin name="RD" function="dot"/>
<pin name="ALE"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="15-I/O-2">
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="PB4"/>
<pin name="(OCI)PB3"/>
<pin name="PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="(ICP)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" function="dot"/>
</symbol>
<symbol name="20-I/O-2">
<pin name="(ADC5)PC5"/>
<pin name="(ADC4)PC4"/>
<pin name="(ADC3)PC3"/>
<pin name="(ADC2)PC2"/>
<pin name="(ADC1)PC1"/>
<pin name="(ADC0)PC0)"/>
<pin name="(SCK)PB5"/>
<pin name="(MISO)PB4"/>
<pin name="(MOSI)PB3"/>
<pin name="(SS)PB2"/>
<pin name="(OC1)PB1"/>
<pin name="(ICP)PB0"/>
<pin name="(AIN1)PD7"/>
<pin name="(AIN0)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-3">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-4">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="15-I/O-3">
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="INT1" direction="in"/>
<pin name="INT0" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ADIN5" direction="in"/>
<pin name="ADIN4" direction="in"/>
<pin name="ADIN3" direction="in"/>
<pin name="ADIN2" direction="in"/>
<pin name="ADIN1" direction="in"/>
<pin name="ADIN0" direction="in"/>
<pin name="NC13" direction="nc"/>
<pin name="NC12" direction="nc"/>
<pin name="NC11" direction="nc"/>
<pin name="NC10" direction="nc"/>
<pin name="NC9" direction="nc"/>
<pin name="NC8" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="NC6" direction="nc"/>
<pin name="NC5" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC14" direction="nc"/>
<pin name="NC15" direction="nc"/>
<pin name="NC16" direction="nc"/>
<pin name="NC17" direction="nc"/>
<pin name="NC18" direction="nc"/>
<pin name="NC19" direction="nc"/>
<pin name="NC20" direction="nc"/>
<pin name="NC21" direction="nc"/>
<pin name="NC22" direction="nc"/>
<pin name="NC23" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="NC24" direction="nc"/>
<pin name="NC25" direction="nc"/>
<pin name="NC26" direction="nc"/>
</symbol>
<symbol name="35-I/O-1">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(TXD1)PB3"/>
<pin name="(RXD1)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(RD)PD7"/>
<pin name="(WR)PD6"/>
<pin name="(TOSC2)PD5"/>
<pin name="(TOSC1)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD0)PD1"/>
<pin name="(RXD0)PD0"/>
<pin name="(OC1B)PE2"/>
<pin name="(ALE)PE1"/>
<pin name="(INT2)PE0"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="in"/>
</symbol>
<symbol name="35-I/O-2">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(TXD1)PB3"/>
<pin name="(RXD1)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(RD)PD7"/>
<pin name="(WR)PD6"/>
<pin name="(TOSC2)PD5"/>
<pin name="(TOSC1)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD0)PD1"/>
<pin name="(RXD0)PD0"/>
<pin name="(OC1B)PE2"/>
<pin name="(ALE)PE1"/>
<pin name="(INT2)PE0"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="32-I/O-5">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-6">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="20-I/O-3">
<pin name="PB5" direction="in"/>
<pin name="PB4(INT1)" direction="in"/>
<pin name="PB3(INT0)" direction="in"/>
<pin name="PB2(T0)" direction="in"/>
<pin name="PB1(AIN1)" direction="in"/>
<pin name="PB0(AIN0)" direction="in"/>
<pin name="PA3"/>
<pin name="(IR)PA2" direction="out"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="PB7" direction="in"/>
<pin name="PB6" direction="in"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC1" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="20-I/O-4">
<pin name="PB5" direction="in"/>
<pin name="PB4(INT1)" direction="in"/>
<pin name="PB3(INT0)" direction="in"/>
<pin name="PB2(T0)" direction="in"/>
<pin name="PB1(AIN1)" direction="in"/>
<pin name="PB0(AIN0)" direction="in"/>
<pin name="PA3"/>
<pin name="(IR)PA2" direction="out"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="PB7" direction="in"/>
<pin name="PB6" direction="in"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC1" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC5" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="24CXX">
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="250X0">
<pin name="HOLD/" direction="in"/>
<pin name="CS/" direction="in"/>
<pin name="SO" direction="in"/>
<pin name="WP/" direction="in"/>
<pin name="SCK"/>
<pin name="SI"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SDE2506">
<pin name="CLK" direction="in"/>
<pin name="CE/" direction="in"/>
<pin name="D"/>
<pin name="NC" direction="nc"/>
<pin name="TP" direction="in"/>
<pin name="TG"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="93CX6">
<pin name="DO" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SK"/>
<pin name="ORG" direction="in"/>
<pin name="DC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="15IO-1">
<pin name="AIN0-PB0"/>
<pin name="AIN1-PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="MOSI-PB5"/>
<pin name="MISO-PB6"/>
<pin name="SCK-PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="INT0-PD2"/>
<pin name="PD3"/>
<pin name="T0-PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="RST/"/>
</symbol>
<symbol name="5IO-1">
<pin name="MOSI-PB0"/>
<pin name="MISO-PB1"/>
<pin name="SCK-PB2"/>
<pin name="CLK-PB3"/>
<pin name="PB4"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RST/"/>
</symbol>
<symbol name="32IO-1">
<pin name="AD7-PA7"/>
<pin name="AD6-PA6"/>
<pin name="AD5-PA5"/>
<pin name="AD4-PA4"/>
<pin name="AD3-PA3"/>
<pin name="AD2-PA2"/>
<pin name="AD1-PA1"/>
<pin name="AD0-PA0"/>
<pin name="A15-PC7"/>
<pin name="A14-PC6"/>
<pin name="A13-PC5"/>
<pin name="A12-PC4"/>
<pin name="A11-PC3"/>
<pin name="A10-PC2"/>
<pin name="A9-PC1"/>
<pin name="A8-PC0"/>
<pin name="PB7-SCK"/>
<pin name="PB6-MISO"/>
<pin name="PB5-MOSI"/>
<pin name="PB4-SS/"/>
<pin name="PB3-AIN1"/>
<pin name="PB2-AIN0"/>
<pin name="PB1-T1"/>
<pin name="PB0-T0"/>
<pin name="PD0-RXD"/>
<pin name="PD1-TXD"/>
<pin name="PD2-INT0"/>
<pin name="PD3-INT1"/>
<pin name="PD4"/>
<pin name="PD5-OC1A"/>
<pin name="PD6-WR/"/>
<pin name="PD7-RD/"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RST/" direction="in"/>
<pin name="ICP"/>
<pin name="ALE"/>
<pin name="OC1B"/>
</symbol>
<symbol name="89C2051">
<pin name="P3.7"/>
<pin name="P3.5-T1"/>
<pin name="P3.4-T0"/>
<pin name="P3.3-INT1/"/>
<pin name="P3.2-INTO/"/>
<pin name="P3.1-TXD"/>
<pin name="P3.0-RXD"/>
<pin name="P1.7"/>
<pin name="P1.6"/>
<pin name="P1.5"/>
<pin name="P1.4"/>
<pin name="P1.3"/>
<pin name="P1.2"/>
<pin name="AIN1-P1.1"/>
<pin name="AIN0-P1.0"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RST-VPP" direction="in"/>
</symbol>
<symbol name="48-I/O-2">
<pin name="ADC0-PF0" direction="in"/>
<pin name="ADC1-PF1" direction="in"/>
<pin name="ADC2-PF2" direction="in"/>
<pin name="ADC3-PF3" direction="in"/>
<pin name="ADC4-PF4" direction="in"/>
<pin name="ADC5-PF5" direction="in"/>
<pin name="ADC6-PF6" direction="in"/>
<pin name="ADC7-PF7" direction="in"/>
<pin name="RXD-PE0" direction="out"/>
<pin name="TXD-PE1" direction="out"/>
<pin name="AC+_PE2" direction="out"/>
<pin name="AC-_PE3" direction="out"/>
<pin name="INT4-PE4" direction="out"/>
<pin name="INT5-PE5" direction="out"/>
<pin name="INT6-PE6" direction="out"/>
<pin name="INT7-PE7" direction="out"/>
<pin name="PD7-T2"/>
<pin name="PD6-T1"/>
<pin name="PD5"/>
<pin name="PD4-IC1"/>
<pin name="PD3-INT3"/>
<pin name="PD2-INT2"/>
<pin name="PD1-INT1"/>
<pin name="PD0-INT0"/>
<pin name="A15-PC7"/>
<pin name="A14-PC6"/>
<pin name="A13-PC5"/>
<pin name="A12-PC4"/>
<pin name="A11-PC3"/>
<pin name="A10-PC2"/>
<pin name="A9-PC1"/>
<pin name="A8-PC0"/>
<pin name="OC2-PB7"/>
<pin name="OC1B-PB6"/>
<pin name="OC1A-PB5"/>
<pin name="OC0-PB4"/>
<pin name="MISO-PB3"/>
<pin name="MOSI-PB2"/>
<pin name="SCK-PB1"/>
<pin name="SS-PB0"/>
<pin name="AD6-PA6"/>
<pin name="AD7-PA7"/>
<pin name="AD5-PA5"/>
<pin name="AD4-PA4"/>
<pin name="AD3-PA3"/>
<pin name="AD2-PA2"/>
<pin name="AD1-PA1"/>
<pin name="AD0-PA0"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="AVREF"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="01" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="02" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2"/>
<pin name="TOSC1"/>
<pin name="WR/"/>
<pin name="RD/"/>
<pin name="ALE"/>
<pin name="RESET/" direction="in"/>
<pin name="PEN/" direction="in"/>
</symbol>
<symbol name="AT89C52">
<pin name="EA" direction="in"/>
<pin name="P0.0AD0"/>
<pin name="P0.1AD1"/>
<pin name="P0.2AD2"/>
<pin name="P0.3AD3"/>
<pin name="P0.4AD4"/>
<pin name="P0.5AD5"/>
<pin name="P0.6AD6"/>
<pin name="P0.7AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0_T2"/>
<pin name="P1.1_T2EX"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR"/>
<pin name="P3.7/RD"/>
</symbol>
<symbol name="VCCGND">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="27C080">
<pin name="A16" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OEVPP" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
</symbol>
<symbol name="AT91R4008">
<pin name="NCS0" direction="out"/>
<pin name="NCS1" direction="out"/>
<pin name="NWAIT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NWDOVF" direction="out"/>
<pin name="MCKI" direction="in"/>
<pin name="NRW0/NWE" direction="out"/>
<pin name="NRD/NOE" direction="out"/>
<pin name="NRW1/NUB" direction="out"/>
<pin name="NRST" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
</symbol>
<symbol name="ICE-TEST">
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
</symbol>
<symbol name="AT91R4008-PARPORT">
<pin name="P0/TCLK0"/>
<pin name="P1/TIOA0"/>
<pin name="P2/TIOB0"/>
<pin name="P3/TCLK1"/>
<pin name="P4/TIOA1"/>
<pin name="P5/TIOB1"/>
<pin name="P6/TCLK2"/>
<pin name="P7/TIOA2"/>
<pin name="P8/TIOB2"/>
<pin name="P9/IRQ0"/>
<pin name="P10/IRQ1"/>
<pin name="P11/IRQ2"/>
<pin name="P12/FIQ"/>
<pin name="P13/SCK0"/>
<pin name="P14/TXD0"/>
<pin name="P15/RXD0"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20/SCK1"/>
<pin name="P21/TXD1/NTRI"/>
<pin name="P22/RXD1"/>
<pin name="P23"/>
<pin name="P24/BMS"/>
<pin name="P25/MCKO"/>
<pin name="P26/NCS2"/>
<pin name="P27/NCS3"/>
</symbol>
<symbol name="AT91R4008-ADR">
<pin name="P31/CS4/A23" direction="out"/>
<pin name="P30/CS5/A22" direction="out"/>
<pin name="P29/CS6/A21" direction="out"/>
<pin name="P28/CS7/A20" direction="out"/>
<pin name="NLB/A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
</symbol>
<symbol name="D0-32">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="D16" direction="hiz"/>
<pin name="D17" direction="hiz"/>
<pin name="D18" direction="hiz"/>
<pin name="D19" direction="hiz"/>
<pin name="D20" direction="hiz"/>
<pin name="D21" direction="hiz"/>
<pin name="D22" direction="hiz"/>
<pin name="D23" direction="hiz"/>
<pin name="D24" direction="hiz"/>
<pin name="D25" direction="hiz"/>
<pin name="D26" direction="hiz"/>
<pin name="D27" direction="hiz"/>
<pin name="D28" direction="hiz"/>
<pin name="D29" direction="hiz"/>
<pin name="D30" direction="hiz"/>
<pin name="D31" direction="hiz"/>
</symbol>
<symbol name="D0-15">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="VDDIO">
<pin name="VDDIO" direction="pwr"/>
</symbol>
<symbol name="VDDCORE">
<pin name="VDDCORE" direction="pwr"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="L4960">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
</symbol>
<symbol name="23-I/O-2">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="VCC@1"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="32-I/O-7">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
</symbol>
<symbol name="32-I/O-M8535-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M8535-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/INT2)PB3"/>
<pin name="(AIN0/OC0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-M8515-A">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="32-I/O-M16-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-M16-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M32-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M32-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="MEGA64">
<pin name="PF0(ADC0)"/>
<pin name="PF1(ADC1)"/>
<pin name="PF2(ADC2)"/>
<pin name="PF3(ADC3)"/>
<pin name="PF4(ADC4/TCK)"/>
<pin name="PF5(ADC5/TMS)"/>
<pin name="PF6(ADC6/TDO)"/>
<pin name="PF7(ADC7/TDI)"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="MEGA128">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="MEGA169">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PCINT0)PE0"/>
<pin name="(TXD/PCINT1)PE1"/>
<pin name="(XCK0/AIN0/PCINT2)PE2"/>
<pin name="(AIN1/PCINT3)PE3"/>
<pin name="(USCK/SCL/PCINT4)PE4"/>
<pin name="(DI/SDA/PCINT5)PE5"/>
<pin name="(DO/PCINT6)PE6"/>
<pin name="(CLKO/PCINT7)PE7"/>
<pin name="(SEG15)PD7"/>
<pin name="(SEG16)PD6"/>
<pin name="(SEG17)PD5"/>
<pin name="(SEG18)PD4"/>
<pin name="(SEG19)PD3"/>
<pin name="(SEG20)PD2"/>
<pin name="(SEG21/INT0)PD1"/>
<pin name="(SEG22/ICP)PD0"/>
<pin name="(SEG5)PC7" direction="out"/>
<pin name="(SEG6)PC6" direction="out"/>
<pin name="(SEG7)PC5" direction="out"/>
<pin name="(SEG8)PC4" direction="out"/>
<pin name="(SEG9)PC3" direction="out"/>
<pin name="(SEG10)PC2" direction="out"/>
<pin name="(SEG11)PC1" direction="out"/>
<pin name="(SEG12)PC0" direction="out"/>
<pin name="(OC2A/PCINT15)PB7"/>
<pin name="(OC1B/PCINT14)PB6"/>
<pin name="(OC1A/PCINT13)PB5"/>
<pin name="(OC0A/PCINT12)PB4"/>
<pin name="(MISO/PCINT11)PB3"/>
<pin name="(MOSI/PCINT10)PB2"/>
<pin name="(SCK/PCINT9)PB1"/>
<pin name="(SS/PCINT8)PB0"/>
<pin name="(SEG2)PA6"/>
<pin name="(SEG3)PA7"/>
<pin name="(SEG1)PA5"/>
<pin name="(SEG0)PA4"/>
<pin name="(COM3)PA3"/>
<pin name="(COM2)PA2"/>
<pin name="(COM1)PA1"/>
<pin name="(COM0)PA0"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(T1/SEG24)"/>
<pin name="PG4(T0/SEG23)"/>
<pin name="PG0(SEG14)"/>
<pin name="PG1(SEG13)"/>
<pin name="PG2(SEG4)"/>
<pin name="PG5(RESET)" direction="in" function="dot"/>
<pin name="LCDCAP" direction="in"/>
</symbol>
<symbol name="MEGA323">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="MEGA323-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MEGA162">
<pin name="(AD7/PCINT7)PA7"/>
<pin name="(AD6/PCINT6)PA6"/>
<pin name="(AD5/PCINT5)PA5"/>
<pin name="(AD4/PCINT4)PA4"/>
<pin name="(AD3/PCINT3)PA3"/>
<pin name="(AD2/PCINT2)PA2"/>
<pin name="(AD1/PCINT1)PA1"/>
<pin name="(AD0/PCINT0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS/OC3B)PB4"/>
<pin name="(AIN1/TXD1)PB3"/>
<pin name="(AIN0/RXD1)PB2"/>
<pin name="(T1/OC2)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15/PCINT15/TDI)PC7"/>
<pin name="(A14/PCINT14/TDO)PC6"/>
<pin name="(A13/PCINT13/TMS)PC5"/>
<pin name="(A12/PCINT12/TCK)PC4"/>
<pin name="(A11/PCINT11)PC3"/>
<pin name="(A10/PCINT10)PC2"/>
<pin name="(A9/PCINT9)PC1"/>
<pin name="(A8/PCINT8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP1/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD0)PD0"/>
<pin name="(TXD0)PD1"/>
<pin name="(INT0/XCK1)PD2"/>
<pin name="(INT1/ICP3)PD3"/>
<pin name="(XCK0/TOSC1/OC3A)PD4"/>
<pin name="(OC1A/TOSC2)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
</symbol>
<symbol name="MEGA2560">
<pin name="(AD0)PA0"/>
<pin name="(AD1)PA1"/>
<pin name="(AD2)PA2"/>
<pin name="(AD3)PA3"/>
<pin name="(AD4)PA4"/>
<pin name="(AD5)PA5"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(SS/PCINT0)PB0"/>
<pin name="(SCK/PCINT1)PB1"/>
<pin name="(MOSI/PCINT2)PB2"/>
<pin name="(MISO/PCINT3)PB3"/>
<pin name="(OC2A/PCINT4)PB4"/>
<pin name="(OC1A/PCINT5)PB5"/>
<pin name="(OC1B/PCINT6)PB6"/>
<pin name="(OC0A/OC1C/PCINT7)PB7"/>
<pin name="(A8)PC0"/>
<pin name="(A9)PC1"/>
<pin name="(A10)PC2"/>
<pin name="(A11)PC3"/>
<pin name="(A12)PC4"/>
<pin name="(A13)PC5"/>
<pin name="(A14)PC6"/>
<pin name="(A15)PC7"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(ICP1)PD4"/>
<pin name="(XCK1)PD5"/>
<pin name="(T1)PD6"/>
<pin name="(T0)PD7"/>
<pin name="(RXD0/PCINT8)PE0"/>
<pin name="(TXD0)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(CLKO/ICP2/INT7)PE7"/>
<pin name="(ADC0)PF0"/>
<pin name="(ADC1)PF1"/>
<pin name="(ADC2)PF2"/>
<pin name="(ADC3)PF3"/>
<pin name="(TCK/ADC4)PF4"/>
<pin name="(TMS/ADC5)PF5"/>
<pin name="(TDO/ADC6)PF6"/>
<pin name="(TDI/ADC7)PF7"/>
<pin name="PL0(ICP4)"/>
<pin name="PL1(ICP5)"/>
<pin name="PL2(T5)"/>
<pin name="PL3(PC5A)"/>
<pin name="PL4(OC5B)"/>
<pin name="PL5(OC5C)"/>
<pin name="PL6"/>
<pin name="PL7"/>
<pin name="(PCINT16/ADC8)PK0"/>
<pin name="(PCINT17/ADC9)PK1"/>
<pin name="(PCINT18/ADC10)PK2"/>
<pin name="(PCINT19/ADC11)PK3"/>
<pin name="(PCINT20/ADC12)PK4"/>
<pin name="(PCINT21/ADC13)PK5"/>
<pin name="(PCINT22/ADC14)PK6"/>
<pin name="(PCINT23/ADC15)PK7"/>
<pin name="PJ0(PCINT9/RXD3)"/>
<pin name="PJ1(PCINT10/TXD3)"/>
<pin name="PJ2((PCINT11/XCK3)"/>
<pin name="PJ3(PCINT12"/>
<pin name="PJ4(PCINT13)"/>
<pin name="PJ5(PCINT14)"/>
<pin name="PJ6(PCINT15)"/>
<pin name="PJ7"/>
<pin name="PH0(RXD2)"/>
<pin name="PH1(TXD2)"/>
<pin name="PH2(XCK2)"/>
<pin name="PH3(OC4A)"/>
<pin name="PH4(OC4B)"/>
<pin name="PH5(OC4C)"/>
<pin name="PH6(OC2B)"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="PG0(WR)"/>
<pin name="PG1(RD)"/>
<pin name="PG2(ALE)"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG5(OC0B)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="PH7(T4)"/>
</symbol>
<symbol name="MEGA162-A">
<pin name="(AD7/PCINT7)PA7"/>
<pin name="(AD6/PCINT6)PA6"/>
<pin name="(AD5/PCINT5)PA5"/>
<pin name="(AD4/PCINT4)PA4"/>
<pin name="(AD3/PCINT3)PA3"/>
<pin name="(AD2/PCINT2)PA2"/>
<pin name="(AD1/PCINT1)PA1"/>
<pin name="(AD0/PCINT0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS/OC3B)PB4"/>
<pin name="(AIN1/TXD1)PB3"/>
<pin name="(AIN0/RXD1)PB2"/>
<pin name="(T1/OC2)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15/PCINT15/TDI)PC7"/>
<pin name="(A14/PCINT14/TDO)PC6"/>
<pin name="(A13/PCINT13/TMS)PC5"/>
<pin name="(A12/PCINT12/TCK)PC4"/>
<pin name="(A11/PCINT11)PC3"/>
<pin name="(A10/PCINT10)PC2"/>
<pin name="(A9/PCINT9)PC1"/>
<pin name="(A8/PCINT8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP1/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD0)PD0"/>
<pin name="(TXD0)PD1"/>
<pin name="(INT0/XCK1)PD2"/>
<pin name="(INT1/ICP3)PD3"/>
<pin name="(XCK0/TOSC1/OC3A)PD4"/>
<pin name="(OC1A/TOSC2)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="CAN128">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD0/PDI)PE0"/>
<pin name="(TXD0/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(RXCAN/T1)PD6"/>
<pin name="(TXCAN/XCK1)PD5"/>
<pin name="(ICP1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(CLKO/A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC0A/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC2A)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="MEGA164">
<pin name="(PCI7/ADC7)PA7"/>
<pin name="(PCI6/ADC6)PA6"/>
<pin name="(PCI5/ADC5)PA5"/>
<pin name="(PCI4/ADC4)PA4"/>
<pin name="(PCI3/ADC3)PA3"/>
<pin name="(PCI2/ADC2)PA2"/>
<pin name="(PCI1/ADC1)PA1"/>
<pin name="(PCI0/ADC0)PA0"/>
<pin name="(PCI15/SCK)PB7"/>
<pin name="(PCI14/MISO)PB6"/>
<pin name="(PCI13/MOSI)PB5"/>
<pin name="(PCI12/OC0B/SS)PB4"/>
<pin name="(PCI11/AIN1/OC0A)PB3"/>
<pin name="(PCI10/AIN0/INT2)PB2"/>
<pin name="(PCI9/CLK0/T1)PB1"/>
<pin name="(PCI8/T0/XCK0)PB0"/>
<pin name="(PCI23/TOSC2)PC7"/>
<pin name="(PCI22/TOSC1)PC6"/>
<pin name="(PCI21/TDI)PC5"/>
<pin name="(PCI20/TDO)PC4"/>
<pin name="(PCI19/TMS)PC3"/>
<pin name="(PCI18/TCK)PC2"/>
<pin name="(PCI17/SDA)PC1"/>
<pin name="(PCI16/SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(PCI24/RXD)PD0"/>
<pin name="(PCI25/TXD)PD1"/>
<pin name="(PCI26/RXD1/INT0)PD2"/>
<pin name="(PCI27/TXD1/INT1)PD3"/>
<pin name="(PCI28/XCK1/OC1B)PD4"/>
<pin name="(PCI29OC1A)PD5"/>
<pin name="(PCI30/OC2B/ICP)PD6"/>
<pin name="(PCI31/OC2)PD7"/>
</symbol>
<symbol name="MEGA644">
<pin name="(PCI7/ADC7)PA7"/>
<pin name="(PCI6/ADC6)PA6"/>
<pin name="(PCI5/ADC5)PA5"/>
<pin name="(PCI4/ADC4)PA4"/>
<pin name="(PCI3/ADC3)PA3"/>
<pin name="(PCI2/ADC2)PA2"/>
<pin name="(PCI1/ADC1)PA1"/>
<pin name="(PCI0/ADC0)PA0"/>
<pin name="(PCI15/SCK)PB7"/>
<pin name="(PCI14/MISO)PB6"/>
<pin name="(PCI13/MOSI)PB5"/>
<pin name="(PCI12/OC0B/SS)PB4"/>
<pin name="(PCI11/AIN1/OC0A)PB3"/>
<pin name="(PCI10/AIN0/INT2)PB2"/>
<pin name="(PCI9/CLK0/T1)PB1"/>
<pin name="(PCI8/T0/XCK0)PB0"/>
<pin name="(PCI23/TOSC2)PC7"/>
<pin name="(PCI22/TOSC1)PC6"/>
<pin name="(PCI21/TDI)PC5"/>
<pin name="(PCI20/TDO)PC4"/>
<pin name="(PCI19/TMS)PC3"/>
<pin name="(PCI18/TCK)PC2"/>
<pin name="(PCI17/SDA)PC1"/>
<pin name="(PCI16/SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(PCI24/RXD)PD0"/>
<pin name="(PCI25/TXD)PD1"/>
<pin name="(PCI26/INT0)PD2"/>
<pin name="(PCI27/INT1)PD3"/>
<pin name="(PCI28/XCK1/OC1B)PD4"/>
<pin name="(PCI29OC1A)PD5"/>
<pin name="(PCI30/OC2B/ICP)PD6"/>
<pin name="(PCI31/OC2)PD7"/>
</symbol>
<symbol name="MEGA164-A">
<pin name="(PCI7/ADC7)PA7"/>
<pin name="(PCI6/ADC6)PA6"/>
<pin name="(PCI5/ADC5)PA5"/>
<pin name="(PCI4/ADC4)PA4"/>
<pin name="(PCI3/ADC3)PA3"/>
<pin name="(PCI2/ADC2)PA2"/>
<pin name="(PCI1/ADC1)PA1"/>
<pin name="(PCI0/ADC0)PA0"/>
<pin name="(PCI15/SCK)PB7"/>
<pin name="(PCI14/MISO)PB6"/>
<pin name="(PCI13/MOSI)PB5"/>
<pin name="(PCI12/OC0B/SS)PB4"/>
<pin name="(PCI11/AIN1/OC0A)PB3"/>
<pin name="(PCI10/AIN0/INT2)PB2"/>
<pin name="(PCI9/CLK0/T1)PB1"/>
<pin name="(PCI8/T0/XCK0)PB0"/>
<pin name="(PCI23/TOSC2)PC7"/>
<pin name="(PCI22/TOSC1)PC6"/>
<pin name="(PCI21/TDI)PC5"/>
<pin name="(PCI20/TDO)PC4"/>
<pin name="(PCI19/TMS)PC3"/>
<pin name="(PCI18/TCK)PC2"/>
<pin name="(PCI17/SDA)PC1"/>
<pin name="(PCI16/SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(PCI24/RXD)PD0"/>
<pin name="(PCI25/TXD)PD1"/>
<pin name="(PCI26/RXD1/INT0)PD2"/>
<pin name="(PCI27/TXD1/INT1)PD3"/>
<pin name="(PCI28/XCK1/OC1B)PD4"/>
<pin name="(PCI29OC1A)PD5"/>
<pin name="(PCI30/OC2B/ICP)PD6"/>
<pin name="(PCI31/OC2)PD7"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="MEGA644-A">
<pin name="(PCI7/ADC7)PA7"/>
<pin name="(PCI6/ADC6)PA6"/>
<pin name="(PCI5/ADC5)PA5"/>
<pin name="(PCI4/ADC4)PA4"/>
<pin name="(PCI3/ADC3)PA3"/>
<pin name="(PCI2/ADC2)PA2"/>
<pin name="(PCI1/ADC1)PA1"/>
<pin name="(PCI0/ADC0)PA0"/>
<pin name="(PCI15/SCK)PB7"/>
<pin name="(PCI14/MISO)PB6"/>
<pin name="(PCI13/MOSI)PB5"/>
<pin name="(PCI12/OC0B/SS)PB4"/>
<pin name="(PCI11/AIN1/OC0A)PB3"/>
<pin name="(PCI10/AIN0/INT2)PB2"/>
<pin name="(PCI9/CLK0/T1)PB1"/>
<pin name="(PCI8/T0/XCK0)PB0"/>
<pin name="(PCI23/TOSC2)PC7"/>
<pin name="(PCI22/TOSC1)PC6"/>
<pin name="(PCI21/TDI)PC5"/>
<pin name="(PCI20/TDO)PC4"/>
<pin name="(PCI19/TMS)PC3"/>
<pin name="(PCI18/TCK)PC2"/>
<pin name="(PCI17/SDA)PC1"/>
<pin name="(PCI16/SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(PCI24/RXD)PD0"/>
<pin name="(PCI25/TXD)PD1"/>
<pin name="(PCI26/INT0)PD2"/>
<pin name="(PCI27/INT1)PD3"/>
<pin name="(PCI28/XCK1/OC1B)PD4"/>
<pin name="(PCI29OC1A)PD5"/>
<pin name="(PCI30/OC2B/ICP)PD6"/>
<pin name="(PCI31/OC2)PD7"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="MEGA168">
<pin name="(PCI5/SCK)PB5"/>
<pin name="PB7(XTAL2/TOSC2/PCI7)"/>
<pin name="PB6(XTAL1/TOSC1/PCI6)"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="(PCI4/MISO)PB4"/>
<pin name="(PCI3/MOSI/OC2A)PB3"/>
<pin name="(PCI2/SS/OC1B)PB2"/>
<pin name="(PCI1/OC1A/OC1S)PB1"/>
<pin name="(PCI0/ICP/CLKO)PB0"/>
<pin name="(PCI23/AIN1)PD7"/>
<pin name="(PCI22/AIN0OC0A)PD6"/>
<pin name="(PCI21/T1/OC0B)PD5"/>
<pin name="(PCI20/XCK/T0)PD4"/>
<pin name="(PCI19/INT1/OC2B)PD3"/>
<pin name="(PCI18/INT0)PD2"/>
<pin name="(PCI17/TXD)PD1"/>
<pin name="(PCI16/RXD)PD0"/>
<pin name="(PCI13/ADC5/SCL)PC5"/>
<pin name="(PCI12/ADC4/SDA)PC4"/>
<pin name="(PCI11/ADC3)PC3"/>
<pin name="(PCI10/ADC2)PC2"/>
<pin name="(PCI9/ADC1)PC1"/>
<pin name="(PCI8/ADC0)PC0"/>
<pin name="PC6(/RESET/PCI14)" function="dot"/>
</symbol>
<symbol name="MEGA168-A">
<pin name="(PCI5/SCK)PB5"/>
<pin name="PB7(XTAL2/TOSC2/PCI7)"/>
<pin name="PB6(XTAL1/TOSC1/PCI6)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="(PCI4/MISO)PB4"/>
<pin name="(PCI3/MOSI/OC2A)PB3"/>
<pin name="(PCI2/SS/OC1B)PB2"/>
<pin name="(PCI1/OC1A/OC1S)PB1"/>
<pin name="(PCI0/ICP/CLKO)PB0"/>
<pin name="(PCI23/AIN1)PD7"/>
<pin name="(PCI22/AIN0OC0A)PD6"/>
<pin name="(PCI21/T1/OC0B)PD5"/>
<pin name="(PCI20/XCK/T0)PD4"/>
<pin name="(PCI19/INT1/OC2B)PD3"/>
<pin name="(PCI18/INT0)PD2"/>
<pin name="(PCI17/TXD)PD1"/>
<pin name="(PCI16/RXD)PD0"/>
<pin name="(PCI13/ADC5/SCL)PC5"/>
<pin name="(PCI12/ADC4/SDA)PC4"/>
<pin name="(PCI11/ADC3)PC3"/>
<pin name="(PCI10/ADC2)PC2"/>
<pin name="(PCI9/ADC1)PC1"/>
<pin name="(PCI8/ADC0)PC0"/>
<pin name="PC6(/RESET/PCI14)" function="dot"/>
<pin name="ADC6"/>
<pin name="ADC7"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="TINY13">
<pin name="(ADC2/PCI4)PB4"/>
<pin name="(CLKI/ADC3/PCI3)PB3"/>
<pin name="(RESET/DW/ADC0/PCI5)PB5"/>
<pin name="(T0/SCK/ADC1/PCI2)PB2"/>
<pin name="(AIN1/MISO/OC0B/INT0/PCI2)PB1"/>
<pin name="(AIN0/MOSI/OC0A/PCI0)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TINY13M">
<pin name="(ADC2/PCI4)PB4"/>
<pin name="(CLKI/ADC3/PCI3)PB3"/>
<pin name="(RESET/DW/ADC0/PCI5)PB5"/>
<pin name="(T0/SCK/ADC1/PCI2)PB2"/>
<pin name="(AIN1/MISO/OC0B/INT0/PCI2)PB1"/>
<pin name="(AIN0/MOSI/OC0A/PCI0)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="P$1" direction="nc"/>
<pin name="P$2" direction="nc"/>
<pin name="P$3" direction="nc"/>
<pin name="P$4" direction="nc"/>
<pin name="P$5" direction="nc"/>
<pin name="P$6" direction="nc"/>
<pin name="P$7" direction="nc"/>
<pin name="P$8" direction="nc"/>
<pin name="P$9" direction="nc"/>
<pin name="P$10" direction="nc"/>
<pin name="P$11" direction="nc"/>
<pin name="P$12" direction="nc"/>
</symbol>
<symbol name="TINY2313">
<pin name="(SCK/UCSK/PCI7)PB7"/>
<pin name="(MISO/DO/PCI6)PB6"/>
<pin name="(MOSI/DI/SDA/PCI5)PB5"/>
<pin name="(OC1B/PCI4)PB4"/>
<pin name="(OC1A/PCI3)PB3"/>
<pin name="(OC0A/PCI2)PB2"/>
<pin name="(AIN1/PCI1)PB1"/>
<pin name="(AIN0/PCI0)PB0"/>
<pin name="(ICP)PD6"/>
<pin name="(OC0B/T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(CKOUT/XCK/INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1(PA0)"/>
<pin name="XTAL2(PA1)"/>
<pin name="RESET/DW/PA2" function="dot"/>
</symbol>
<symbol name="TINY26">
<pin name="(ADC9/INT0/T0)PB6"/>
<pin name="(OC1B)PB3"/>
<pin name="(SCK/SCL/OC1B)PB2"/>
<pin name="(MISO/DO/OC1A)PB1"/>
<pin name="(MOSI/DI/SDA/OC1A)PB0"/>
<pin name="(AIN0/ADC5)PA6"/>
<pin name="(ADC4)PA5"/>
<pin name="(ADC3)PA4"/>
<pin name="(AREF)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1(PB4/ADC7)"/>
<pin name="XTAL2(PB5/ADC8)"/>
<pin name="(RESET/ADC10)PB7" function="dot"/>
<pin name="(AIN1/ADC6)PA7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="TINY26M">
<pin name="(ADC9/INT0/T0)PB6"/>
<pin name="(OC1B)PB3"/>
<pin name="(SCK/SCL/OC1B)PB2"/>
<pin name="(MISO/DO/OC1A)PB1"/>
<pin name="(MOSI/DI/SDA/OC1A)PB0"/>
<pin name="(AIN0/ADC5)PA6"/>
<pin name="(ADC4)PA5"/>
<pin name="(ADC3)PA4"/>
<pin name="(AREF)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1(PB4/ADC7)"/>
<pin name="XTAL2(PB5/ADC8)"/>
<pin name="(RESET/ADC10)PB7" function="dot"/>
<pin name="(AIN1/ADC6)PA7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="P$1" direction="nc"/>
<pin name="P$2" direction="nc"/>
<pin name="P$3" direction="nc"/>
<pin name="P$4" direction="nc"/>
<pin name="P$5" direction="nc"/>
<pin name="P$6" direction="nc"/>
<pin name="P$7" direction="nc"/>
<pin name="P$8" direction="nc"/>
<pin name="P$9" direction="nc"/>
<pin name="P$10" direction="nc"/>
<pin name="P$11" direction="nc"/>
<pin name="P$12" direction="nc"/>
</symbol>
<symbol name="MEGA32906490">
<pin name="(COM0)PA0"/>
<pin name="(COM1)PA1"/>
<pin name="(COM2)PA2"/>
<pin name="(COM3)PA3"/>
<pin name="(SEG0)PA4"/>
<pin name="(SEG1)PA5"/>
<pin name="(SEG2)PA6"/>
<pin name="(SEG3)PA7"/>
<pin name="(SEG4)PG2"/>
<pin name="(SEG5)PC7"/>
<pin name="(SEG6)PC6"/>
<pin name="(SEG7/PCINT19)PH3"/>
<pin name="(SEG8/PCINT18)PH2"/>
<pin name="(SEG9/PCINT17)PH1"/>
<pin name="(SEG10/PCINT16)PH0"/>
<pin name="(RXD/PCINT0)PE0"/>
<pin name="(SEG11)PC5"/>
<pin name="(SEG12)PC4"/>
<pin name="(SEG13)PC3"/>
<pin name="(SEG14)PC2"/>
<pin name="(SEG15)PC1"/>
<pin name="(SEG16)PC0"/>
<pin name="(SEG17)PG1"/>
<pin name="(SEG18)PG0"/>
<pin name="(SEG19)PD7"/>
<pin name="(SEG20)PD6"/>
<pin name="(SEG21)PD5"/>
<pin name="(SEG22)PD4"/>
<pin name="(SEG23)PD3"/>
<pin name="(SEG24)PD2"/>
<pin name="(SEG25/INT0)PD1"/>
<pin name="(SEG26/ICP1)PD0"/>
<pin name="(SEG27/PCINT30)PJ6"/>
<pin name="(SEG28/PCINT29)PJ5"/>
<pin name="(SEG29/PCINT28)PJ4"/>
<pin name="(SEG30/PCINT27)PJ3"/>
<pin name="(SEG31/PCINT26)PJ2"/>
<pin name="(SEG32/T0)PG4"/>
<pin name="(SEG33/T1)PG3"/>
<pin name="(SEG34/PCINT25)PJ1"/>
<pin name="(SEG35/PCINT24)PJ0"/>
<pin name="(SEG36/PCINT23)PH7"/>
<pin name="(SEG37/PCINT22)PH6"/>
<pin name="(SEG38/PCINT21)PH5"/>
<pin name="(SEG39/PCINT20)PH4"/>
<pin name="(TXD/PCINT1)PE1"/>
<pin name="(XCK/AIN0/PCINT2)PE2"/>
<pin name="(AIN1/PCINT3)PE3"/>
<pin name="(USCK/SCL/PCINT4)PE4"/>
<pin name="(DI/SDA/PCINT5)PE5"/>
<pin name="(DO/PCINT6)PE6"/>
<pin name="(CLKO/PCINT7)PE7"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="LCDCAP"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="PB7(PCINT15/OC2A)"/>
<pin name="P$57" direction="nc"/>
<pin name="P$58" direction="nc"/>
<pin name="P$59" direction="nc"/>
<pin name="P$60" direction="nc"/>
<pin name="P$61" direction="nc"/>
<pin name="P$62" direction="nc"/>
<pin name="P$63" direction="nc"/>
<pin name="P$64" direction="nc"/>
<pin name="P$65" direction="nc"/>
<pin name="P$66" direction="nc"/>
<pin name="P$67" direction="nc"/>
<pin name="P$68" direction="nc"/>
<pin name="P$69" direction="nc"/>
<pin name="P$70" direction="nc"/>
<pin name="P$71" direction="nc"/>
<pin name="P$72" direction="nc"/>
<pin name="P$73" direction="nc"/>
<pin name="P$74" direction="nc"/>
<pin name="P$75" direction="nc"/>
<pin name="PB7/RESET" direction="nc"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="PB0(PCINT8/SS)" direction="nc"/>
<pin name="PB1(PCINT9/SCK)" direction="nc"/>
<pin name="PB2(PCINT10/MOSI)" direction="nc"/>
<pin name="PB3(PCINT11/MISO)" direction="nc"/>
<pin name="PB4(PCINT12/OC0A)" direction="nc"/>
<pin name="PB5(PCINT13/OC1A)" direction="nc"/>
<pin name="PB6(PCINT14/OC1B)" direction="nc"/>
<pin name="PF0(ADC0)" direction="nc"/>
<pin name="PF1(ADC1)" direction="nc"/>
<pin name="PF2(ADC2)" direction="nc"/>
<pin name="PF3(ADC3)" direction="nc"/>
<pin name="PF4(ADC4/TCK)" direction="nc"/>
<pin name="PF5(ADC5/TMS)" direction="nc"/>
<pin name="PF6(ADC6/TDO)" direction="nc"/>
<pin name="PF7(ADC7/TDI)" direction="nc"/>
</symbol>
<symbol name="MEGA329649">
<pin name="(COM0)PA0"/>
<pin name="(COM1)PA1"/>
<pin name="(COM2)PA2"/>
<pin name="(COM3)PA3"/>
<pin name="(SEG0)PA4"/>
<pin name="(SEG1)PA5"/>
<pin name="(SEG2)PA6"/>
<pin name="(SEG3)PA7"/>
<pin name="(SEG4)PG2"/>
<pin name="(SEG5)PC7"/>
<pin name="(SEG6)PC6"/>
<pin name="(SEG7)PC5"/>
<pin name="(SEG8)PC4"/>
<pin name="(SEG9)PC3"/>
<pin name="(SEG10)PC2"/>
<pin name="(SEG11)PC1"/>
<pin name="(SEG12)PC0"/>
<pin name="(SEG13)PG1"/>
<pin name="(SEG14)PG0"/>
<pin name="(SEG15)PD7"/>
<pin name="(SEG16)PD6"/>
<pin name="(SEG17)PD5"/>
<pin name="(SEG18)PD4"/>
<pin name="(SEG19)PD3"/>
<pin name="(SEG20)PD2"/>
<pin name="(SEG21)PD1"/>
<pin name="(SEG22)PD0"/>
<pin name="(SEG23/T0)PG4"/>
<pin name="(SEG24/T1)PG3"/>
<pin name="LCDCAP"/>
<pin name="(RXD/PCINT0)PE0"/>
<pin name="(TXD/PCINT1)PE1"/>
<pin name="RESET/PG5"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="(CLKO/PCINT7)PE7"/>
<pin name="(DO/PCINT6)PE6"/>
<pin name="(DI/SDA/PCINT5)PE5"/>
<pin name="(USCK/SCL/PCINT4)PE4"/>
<pin name="(AIN1/PCINT3)PE3"/>
<pin name="(XCK/AIN0/PCINT2)PE2"/>
<pin name="PB7(PCINT15/OC2A)"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="PB0(PCINT8/SS)" direction="nc"/>
<pin name="PB1(PCINT9/SCK)" direction="nc"/>
<pin name="PB2(PCINT10/MOSI)" direction="nc"/>
<pin name="PB3(PCINT11/MISO)" direction="nc"/>
<pin name="PB4(PCINT12/OC0A)" direction="nc"/>
<pin name="PB5(PCINT13/OC1A)" direction="nc"/>
<pin name="PB6(PCINT14/OC1B)" direction="nc"/>
<pin name="PF0(ADC0)" direction="nc"/>
<pin name="PF1(ADC1)" direction="nc"/>
<pin name="PF2(ADC2)" direction="nc"/>
<pin name="PF3(ADC3)" direction="nc"/>
<pin name="PF4(ADC4/TCK)" direction="nc"/>
<pin name="PF5(ADC5/TMS)" direction="nc"/>
<pin name="PF6(ADC6/TDO)" direction="nc"/>
<pin name="PF7(ADC7/TDI)" direction="nc"/>
</symbol>
<symbol name="TINY25_45_85">
<pin name="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0"/>
<pin name="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1"/>
<pin name="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2"/>
<pin name="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3"/>
<pin name="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4"/>
<pin name="(RESET/DW/ADC0/PCINT5)PB5"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="TINY25_45_85*M">
<pin name="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0"/>
<pin name="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1"/>
<pin name="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2"/>
<pin name="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3"/>
<pin name="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4"/>
<pin name="(RESET/DW/ADC0/PCINT5)PB5"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="P$1" direction="nc"/>
<pin name="P$2" direction="nc"/>
<pin name="P$3" direction="nc"/>
<pin name="P$4" direction="nc"/>
<pin name="P$5" direction="nc"/>
<pin name="P$6" direction="nc"/>
<pin name="P$7" direction="nc"/>
<pin name="P$8" direction="nc"/>
<pin name="P$9" direction="nc"/>
<pin name="P$10" direction="nc"/>
<pin name="P$11" direction="nc"/>
<pin name="P$12" direction="nc"/>
</symbol>
<symbol name="MEGA165">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PCI0)PE0"/>
<pin name="(TXD/PCI2)PE1"/>
<pin name="(XCK0/AIN0/PCI2)PE2"/>
<pin name="(AIN1/PCI3)PE3"/>
<pin name="(USCK/SCL/PCI4)PE4"/>
<pin name="(DI/SDA/PCI5)PE5"/>
<pin name="(DO/PCI6)PE6"/>
<pin name="(CLKO/PCI7)PE7"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="(INT0)PD1"/>
<pin name="(ICP1)PD0"/>
<pin name="PC7"/>
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="(OC2A/PCI15)PB7"/>
<pin name="(OC1B/PCI14)PB6"/>
<pin name="(OC1A/PCI13)PB5"/>
<pin name="(OC0A/PCI12)PB4"/>
<pin name="(MISO/PCI11)PB3"/>
<pin name="(MOSI/PCI10)PB2"/>
<pin name="(SCK/PCI9)PB1"/>
<pin name="(SS/PCI8)PB0"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="PG3(T1)"/>
<pin name="PG4(T0)"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="MEGA1281">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD0/PDI/PCI8)PE0"/>
<pin name="(TXD0/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(ICP3/CLKO/INT7)PE7"/>
<pin name="(T0)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(ICP1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(OC0A/OC1C/PCI7)PB7"/>
<pin name="(OC1B/PCI6)PB6"/>
<pin name="(OC1A/PCI5)PB5"/>
<pin name="(OC2A/PCI4)PB4"/>
<pin name="(MISO/PCI3)PB3"/>
<pin name="(MOSI/PCI2)PB2"/>
<pin name="(SCK/PCI1)PB1"/>
<pin name="(SS/PCI0)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PG5(OC0B)"/>
</symbol>
<symbol name="MEGA406">
<pin name="(ADC0/PCI0)PA0"/>
<pin name="(ADC1/PCI1)PA1"/>
<pin name="(ADC2/PCI2)PA2"/>
<pin name="(ADC3/PCI3)PA3"/>
<pin name="(ADC4/INT0/PCI4)PA4"/>
<pin name="(INT1/PCI5)PA5"/>
<pin name="(INT2/PCI6)PA6"/>
<pin name="(INT3/PCI7)PA7"/>
<pin name="(TDO/PCINT8)PB0"/>
<pin name="(TDI/PCINT9)PB1"/>
<pin name="(TMS/PCINT10)PB2"/>
<pin name="(TCK/PCINT11)PB3"/>
<pin name="(PCINT12)PB4"/>
<pin name="(PCINT13)PB5"/>
<pin name="(OC0A/PCINT14)PB6"/>
<pin name="(OC0B/PCINT15)PB7"/>
<pin name="(T0)PD0"/>
<pin name="PD1"/>
<pin name="PC0"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="OC"/>
<pin name="OPC"/>
<pin name="BATT"/>
<pin name="RESET"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SGND"/>
<pin name="GND@4" direction="pwr"/>
<pin name="VREFGND"/>
<pin name="VREF"/>
<pin name="VREG"/>
<pin name="NNI"/>
<pin name="NI"/>
<pin name="PI"/>
<pin name="PPI"/>
<pin name="NV"/>
<pin name="PV1"/>
<pin name="PV2"/>
<pin name="PV4"/>
<pin name="PV3"/>
<pin name="PVT"/>
<pin name="OD"/>
<pin name="VFET"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AT90*4434P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC0" pad="22"/>
<connect gate="G$1" pin="PC1" pad="23"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*4434" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (LS)&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-4"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="44"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0" pad="19"/>
<connect gate="G$1" pin="PC1" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*8535P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC0" pad="22"/>
<connect gate="G$1" pin="PC1" pad="23"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*8535" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-4"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0" pad="19"/>
<connect gate="G$1" pin="PC1" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S4414" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="ICP" pad="31"/>
<connect gate="G$1" pin="OC1B" pad="29"/>
<connect gate="G$1" pin="PD4" pad="14"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J1" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J2" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J3" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515-A" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-2"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-2"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-1"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="ICP" pad="31"/>
<connect gate="G$1" pin="OC1B" pad="29"/>
<connect gate="G$1" pin="PD4" pad="14"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2333A" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10-bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-1"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="10"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(ICP)PB0" pad="12"/>
<connect gate="G$1" pin="(INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(INT1)PD3" pad="1"/>
<connect gate="G$1" pin="(MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1)PB1" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(SS)PB2" pad="14"/>
<connect gate="G$1" pin="(T0)PD4" pad="2"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="31"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC3" pad="19"/>
<connect gate="G$1" pin="NC4" pad="22"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2333P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10-bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-2"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="12"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(ICP)PB0" pad="14"/>
<connect gate="G$1" pin="(INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="17"/>
<connect gate="G$1" pin="(OC1)PB1" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(SS)PB2" pad="16"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(T1)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S4433" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="12"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(ICP)PB0" pad="14"/>
<connect gate="G$1" pin="(INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="17"/>
<connect gate="G$1" pin="(OC1)PB1" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(SS)PB2" pad="16"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(T1)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="10"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(ICP)PB0" pad="12"/>
<connect gate="G$1" pin="(INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(INT1)PD3" pad="1"/>
<connect gate="G$1" pin="(MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1)PB1" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(SS)PB2" pad="14"/>
<connect gate="G$1" pin="(T0)PD4" pad="2"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="31"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*2323" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="3-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*2343" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="5-I/O-1"/>
</gates>
<devices>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2313" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="15-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OCI)PB3" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OCI)PB3" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S1200" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="15-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Y" package="SSOP20D8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY10" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes ROM</description>
<gates>
<gate name="G$1" symbol="6-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY11*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="6-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-6"/>
<technology name="L-2"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-6"/>
<technology name="L-2"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY12*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="6-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
<technology name="V-1"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
<technology name="V-1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY22" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1K ROM&lt;p&gt;
128 bytes RAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="5-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA103*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (L)&lt;p&gt;
128 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
2 Kbytes EEPROM&lt;p&gt;
UART&lt;p&gt;
RTC&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="48-I/O-1"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AC+)PE2" pad="4"/>
<connect gate="G$1" pin="(AC-)PE3" pad="5"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(TXD)PE1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="ALE" pad="43"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="53"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="54"/>
<connect gate="G$1" pin="RD" pad="34"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="TOSC1" pad="19"/>
<connect gate="G$1" pin="TOSC2" pad="18"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC1" pad="52"/>
<connect gate="G$1" pin="WR" pad="33"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90C8534" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
256 bytes SRAM&lt;p&gt;
6-channel&lt;p&gt;
10-bit A/D</description>
<gates>
<gate name="G$1" symbol="15-I/O-3"/>
</gates>
<devices>
<device name="A" package="TQFP48">
<connects>
<connect gate="G$1" pin="ADIN0" pad="1"/>
<connect gate="G$1" pin="ADIN1" pad="13"/>
<connect gate="G$1" pin="ADIN2" pad="14"/>
<connect gate="G$1" pin="ADIN3" pad="15"/>
<connect gate="G$1" pin="ADIN4" pad="16"/>
<connect gate="G$1" pin="ADIN5" pad="17"/>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="31"/>
<connect gate="G$1" pin="INT0" pad="35"/>
<connect gate="G$1" pin="INT1" pad="34"/>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC10" pad="12"/>
<connect gate="G$1" pin="NC11" pad="19"/>
<connect gate="G$1" pin="NC12" pad="21"/>
<connect gate="G$1" pin="NC13" pad="25"/>
<connect gate="G$1" pin="NC14" pad="26"/>
<connect gate="G$1" pin="NC15" pad="27"/>
<connect gate="G$1" pin="NC16" pad="28"/>
<connect gate="G$1" pin="NC17" pad="29"/>
<connect gate="G$1" pin="NC18" pad="30"/>
<connect gate="G$1" pin="NC19" pad="32"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="NC20" pad="36"/>
<connect gate="G$1" pin="NC21" pad="37"/>
<connect gate="G$1" pin="NC22" pad="40"/>
<connect gate="G$1" pin="NC23" pad="41"/>
<connect gate="G$1" pin="NC24" pad="42"/>
<connect gate="G$1" pin="NC25" pad="43"/>
<connect gate="G$1" pin="NC26" pad="48"/>
<connect gate="G$1" pin="NC3" pad="4"/>
<connect gate="G$1" pin="NC4" pad="5"/>
<connect gate="G$1" pin="NC5" pad="6"/>
<connect gate="G$1" pin="NC6" pad="7"/>
<connect gate="G$1" pin="NC7" pad="8"/>
<connect gate="G$1" pin="NC8" pad="9"/>
<connect gate="G$1" pin="NC9" pad="10"/>
<connect gate="G$1" pin="PA0" pad="47"/>
<connect gate="G$1" pin="PA1" pad="46"/>
<connect gate="G$1" pin="PA2" pad="45"/>
<connect gate="G$1" pin="PA3" pad="44"/>
<connect gate="G$1" pin="PA4" pad="39"/>
<connect gate="G$1" pin="PA5" pad="38"/>
<connect gate="G$1" pin="PA6" pad="33"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA161*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH,&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
dual UART&lt;p&gt;
hardware multiplier</description>
<gates>
<gate name="G$1" symbol="35-I/O-1"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(ALE)PE1" pad="30"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(INT2)PE0" pad="31"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="29"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="10"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="3"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="14"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="15"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="11"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="4"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA161*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH,&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
dual UART&lt;p&gt;
hardware multiplier</description>
<gates>
<gate name="G$1" symbol="35-I/O-2"/>
</gates>
<devices>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(ALE)PE1" pad="27"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(INT2)PE0" pad="29"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="26"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="5"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="42"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="10"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="7"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="43"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY15L" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2.7 V&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM&lt;p&gt;
4-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="6-I/O-3"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(ADC0)PB5" pad="1"/>
<connect gate="G$1" pin="(ADC1)PB2" pad="7"/>
<connect gate="G$1" pin="(ADC2)PB3" pad="3"/>
<connect gate="G$1" pin="(ADC3)PB4" pad="2"/>
<connect gate="G$1" pin="(AREF)PB0" pad="5"/>
<connect gate="G$1" pin="(OCP)PB1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-1"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(ADC0)PB5" pad="1"/>
<connect gate="G$1" pin="(ADC1)PB2" pad="7"/>
<connect gate="G$1" pin="(ADC2)PB3" pad="3"/>
<connect gate="G$1" pin="(ADC3)PB4" pad="2"/>
<connect gate="G$1" pin="(AREF)PB0" pad="5"/>
<connect gate="G$1" pin="(OCP)PB1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA163*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH,&lt;p&gt;
1 Kbytes &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
hardware multiplier</description>
<gates>
<gate name="G$1" symbol="32-I/O-5"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA163*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH,&lt;p&gt;
1 Kbytes EEPROM&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
hardware multiplier</description>
<gates>
<gate name="G$1" symbol="32-I/O-6"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY28*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1.8 V&lt;p&gt;
2 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="20-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(IR)PA2" pad="25"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="22"/>
<connect gate="G$1" pin="NC1" pad="21"/>
<connect gate="G$1" pin="PA0" pad="28"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PB0(AIN0)" pad="14"/>
<connect gate="G$1" pin="PB1(AIN1)" pad="15"/>
<connect gate="G$1" pin="PB2(T0)" pad="16"/>
<connect gate="G$1" pin="PB3(INT0)" pad="17"/>
<connect gate="G$1" pin="PB4(INT1)" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="23"/>
<connect gate="G$1" pin="PB7" pad="24"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD2" pad="4"/>
<connect gate="G$1" pin="PD3" pad="5"/>
<connect gate="G$1" pin="PD4" pad="6"/>
<connect gate="G$1" pin="PD5" pad="11"/>
<connect gate="G$1" pin="PD6" pad="12"/>
<connect gate="G$1" pin="PD7" pad="13"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name="L-4"/>
<technology name="V-1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY28*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1.8 V&lt;p&gt;
2 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="20-I/O-4"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(IR)PA2" pad="25"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND1" pad="21"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC3" pad="19"/>
<connect gate="G$1" pin="NC4" pad="20"/>
<connect gate="G$1" pin="NC5" pad="22"/>
<connect gate="G$1" pin="PA0" pad="28"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PB0(AIN0)" pad="12"/>
<connect gate="G$1" pin="PB1(AIN1)" pad="13"/>
<connect gate="G$1" pin="PB2(T0)" pad="14"/>
<connect gate="G$1" pin="PB3(INT0)" pad="15"/>
<connect gate="G$1" pin="PB4(INT1)" pad="16"/>
<connect gate="G$1" pin="PB5" pad="17"/>
<connect gate="G$1" pin="PB6" pad="23"/>
<connect gate="G$1" pin="PB7" pad="24"/>
<connect gate="G$1" pin="PD0" pad="30"/>
<connect gate="G$1" pin="PD1" pad="31"/>
<connect gate="G$1" pin="PD2" pad="32"/>
<connect gate="G$1" pin="PD3" pad="1"/>
<connect gate="G$1" pin="PD4" pad="2"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="10"/>
<connect gate="G$1" pin="PD7" pad="11"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCC1" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="L-4"/>
<technology name="V-1"/>
</technologies>
</device>
<device name="M" package="MLF32">
<connects>
<connect gate="G$1" pin="(IR)PA2" pad="25"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND1" pad="21"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC3" pad="19"/>
<connect gate="G$1" pin="NC4" pad="20"/>
<connect gate="G$1" pin="NC5" pad="22"/>
<connect gate="G$1" pin="PA0" pad="28"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PB0(AIN0)" pad="12"/>
<connect gate="G$1" pin="PB1(AIN1)" pad="13"/>
<connect gate="G$1" pin="PB2(T0)" pad="14"/>
<connect gate="G$1" pin="PB3(INT0)" pad="15"/>
<connect gate="G$1" pin="PB4(INT1)" pad="16"/>
<connect gate="G$1" pin="PB5" pad="17"/>
<connect gate="G$1" pin="PB6" pad="23"/>
<connect gate="G$1" pin="PB7" pad="24"/>
<connect gate="G$1" pin="PD0" pad="30"/>
<connect gate="G$1" pin="PD1" pad="31"/>
<connect gate="G$1" pin="PD2" pad="32"/>
<connect gate="G$1" pin="PD3" pad="1"/>
<connect gate="G$1" pin="PD4" pad="2"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="10"/>
<connect gate="G$1" pin="PD7" pad="11"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCC1" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="L-4"/>
<technology name="V-1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA103*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (L)&lt;p&gt;
128 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
2 Kbytes EEPROM&lt;p&gt;
UART&lt;p&gt;
RTC&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="48-I/O-2"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="01" pad="21"/>
<connect gate="G$1" pin="02" pad="22"/>
<connect gate="G$1" pin="A10-PC2" pad="37"/>
<connect gate="G$1" pin="A11-PC3" pad="38"/>
<connect gate="G$1" pin="A12-PC4" pad="39"/>
<connect gate="G$1" pin="A13-PC5" pad="40"/>
<connect gate="G$1" pin="A14-PC6" pad="41"/>
<connect gate="G$1" pin="A15-PC7" pad="42"/>
<connect gate="G$1" pin="A8-PC0" pad="35"/>
<connect gate="G$1" pin="A9-PC1" pad="36"/>
<connect gate="G$1" pin="AC+_PE2" pad="4"/>
<connect gate="G$1" pin="AC-_PE3" pad="5"/>
<connect gate="G$1" pin="AD0-PA0" pad="51"/>
<connect gate="G$1" pin="AD1-PA1" pad="50"/>
<connect gate="G$1" pin="AD2-PA2" pad="49"/>
<connect gate="G$1" pin="AD3-PA3" pad="48"/>
<connect gate="G$1" pin="AD4-PA4" pad="47"/>
<connect gate="G$1" pin="AD5-PA5" pad="46"/>
<connect gate="G$1" pin="AD6-PA6" pad="45"/>
<connect gate="G$1" pin="AD7-PA7" pad="44"/>
<connect gate="G$1" pin="ADC0-PF0" pad="61"/>
<connect gate="G$1" pin="ADC1-PF1" pad="60"/>
<connect gate="G$1" pin="ADC2-PF2" pad="59"/>
<connect gate="G$1" pin="ADC3-PF3" pad="58"/>
<connect gate="G$1" pin="ADC4-PF4" pad="57"/>
<connect gate="G$1" pin="ADC5-PF5" pad="56"/>
<connect gate="G$1" pin="ADC6-PF6" pad="55"/>
<connect gate="G$1" pin="ADC7-PF7" pad="54"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="ALE" pad="43"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVREF" pad="62"/>
<connect gate="G$1" pin="GND" pad="53"/>
<connect gate="G$1" pin="INT4-PE4" pad="6"/>
<connect gate="G$1" pin="INT5-PE5" pad="7"/>
<connect gate="G$1" pin="INT6-PE6" pad="8"/>
<connect gate="G$1" pin="INT7-PE7" pad="9"/>
<connect gate="G$1" pin="MISO-PB3" pad="13"/>
<connect gate="G$1" pin="MOSI-PB2" pad="12"/>
<connect gate="G$1" pin="OC0-PB4" pad="14"/>
<connect gate="G$1" pin="OC1A-PB5" pad="15"/>
<connect gate="G$1" pin="OC1B-PB6" pad="16"/>
<connect gate="G$1" pin="OC2-PB7" pad="17"/>
<connect gate="G$1" pin="PD0-INT0" pad="25"/>
<connect gate="G$1" pin="PD1-INT1" pad="26"/>
<connect gate="G$1" pin="PD2-INT2" pad="27"/>
<connect gate="G$1" pin="PD3-INT3" pad="28"/>
<connect gate="G$1" pin="PD4-IC1" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6-T1" pad="31"/>
<connect gate="G$1" pin="PD7-T2" pad="32"/>
<connect gate="G$1" pin="PEN/" pad="1"/>
<connect gate="G$1" pin="RD/" pad="34"/>
<connect gate="G$1" pin="RESET/" pad="20"/>
<connect gate="G$1" pin="RXD-PE0" pad="2"/>
<connect gate="G$1" pin="SCK-PB1" pad="11"/>
<connect gate="G$1" pin="SS-PB0" pad="10"/>
<connect gate="G$1" pin="TOSC1" pad="19"/>
<connect gate="G$1" pin="TOSC2" pad="18"/>
<connect gate="G$1" pin="TXD-PE1" pad="3"/>
<connect gate="G$1" pin="VCC" pad="52"/>
<connect gate="G$1" pin="WR/" pad="33"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
6-channel 10 bit ADC&lt;p&gt;
2-channel 8 bit ADC</description>
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="M" package="MLF32">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
2-channel 8 bit ADC</description>
<gates>
<gate name="G$1" symbol="23-I/O-2"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8535" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-A"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="PC0(SCL)" pad="25"/>
<connect gate="G$1" pin="PC1(SDA)" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="J-SMD" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="PC0(SCL)" pad="25"/>
<connect gate="G$1" pin="PC1(SDA)" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="J-SO" package="S44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="PC0(SCL)" pad="25"/>
<connect gate="G$1" pin="PC1(SDA)" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8535*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/OC0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/INT2)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8515*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-7"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="(XCK)PD4" pad="14"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="31"/>
<connect gate="G$1" pin="PE1(ALE)" pad="30"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="29"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8515" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8515-A"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="(XCK)PD4" pad="16"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="35"/>
<connect gate="G$1" pin="PE1(ALE)" pad="33"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="32"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="J-SMD" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="(XCK)PD4" pad="16"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="35"/>
<connect gate="G$1" pin="PE1(ALE)" pad="33"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="32"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="J-SO" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="(XCK)PD4" pad="16"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="35"/>
<connect gate="G$1" pin="PE1(ALE)" pad="33"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="32"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA16" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-A"/>
</gates>
<devices>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA16*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;p&gt;
1 kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;p&gt;
2 Kbytes SRAM&lt;p&gt;
1 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-M32-A"/>
</gates>
<devices>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;p&gt;
2 Kbytes SRAM&lt;p&gt;
1 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="32-I/O-M32-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA64" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
2 Kbytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA64"/>
</gates>
<devices>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA128" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
4 Kbytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA128"/>
</gates>
<devices>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA169" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
4x25 Segment LCD Driver</description>
<gates>
<gate name="G$1" symbol="MEGA169"/>
</gates>
<devices>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA323*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;p&gt;
2 Kbytes SRAM&lt;p&gt;
1 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA323"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA323" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;p&gt;
2 Kbytes SRAM&lt;p&gt;
1 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA323-A"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-8"/>
<technology name="L-4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA162*P" prefix="IC">
<description>MIKROCONTROLLER&lt;br&gt;&lt;br&gt;
&lt;b&gt;ATmega162&lt;/b&gt;&lt;br&gt;&lt;br&gt;
16kB Flash&lt;br&gt;&lt;br&gt;
2kB RAM&lt;br&gt;&lt;br&gt;
2 USARTS&lt;br&gt;&lt;br&gt;
ATmega162 = 2,7-5,5V or ATmega162V = 1,8-5,5V</description>
<gates>
<gate name="G$1" symbol="MEGA162"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10/PCINT10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11/PCINT11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12/PCINT12/TCK)PC4" pad="25"/>
<connect gate="G$1" pin="(A13/PCINT13/TMS)PC5" pad="26"/>
<connect gate="G$1" pin="(A14/PCINT14/TDO)PC6" pad="27"/>
<connect gate="G$1" pin="(A15/PCINT15/TDI)PC7" pad="28"/>
<connect gate="G$1" pin="(A8/PCINT8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9/PCINT9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0/PCINT0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1/PCINT1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2/PCINT2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3/PCINT3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4/PCINT4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5/PCINT5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6/PCINT6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7/PCINT7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0/RXD1)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/TXD1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0/XCK1)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1/ICP3)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A/TOSC2)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS/OC3B)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1/OC2)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="(XCK0/TOSC1/OC3A)PD4" pad="14"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="PE0(ICP1/INT2)" pad="31"/>
<connect gate="G$1" pin="PE1(ALE)" pad="30"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="29"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA162" prefix="IC">
<description>MIKROCONTROLLER&lt;br&gt;&lt;br&gt;
&lt;b&gt;ATmega162&lt;/b&gt;&lt;br&gt;&lt;br&gt;
16kB Flash&lt;br&gt;&lt;br&gt;
2kB RAM&lt;br&gt;&lt;br&gt;
2 USARTS&lt;br&gt;&lt;br&gt;
ATmega162 = 2,7-5,5V or ATmega162V = 1,8-5,5V</description>
<gates>
<gate name="G$1" symbol="MEGA162-A"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10/PCINT10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11/PCINT11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12/PCINT12/TCK)PC4" pad="22"/>
<connect gate="G$1" pin="(A13/PCINT13/TMS)PC5" pad="23"/>
<connect gate="G$1" pin="(A14/PCINT14/TDO)PC6" pad="24"/>
<connect gate="G$1" pin="(A15/PCINT15/TDI)PC7" pad="25"/>
<connect gate="G$1" pin="(A8/PCINT8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9/PCINT9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0/PCINT0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1/PCINT1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2/PCINT2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3/PCINT3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4/PCINT4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5/PCINT5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6/PCINT6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7/PCINT7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/RXD1)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/TXD1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0/XCK1)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1/ICP3)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A/TOSC2)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS/OC3B)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1/OC2)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK0/TOSC1/OC3A)PD4" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="PE0(ICP1/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="6"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(A10/PCINT10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11/PCINT11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12/PCINT12/TCK)PC4" pad="22"/>
<connect gate="G$1" pin="(A13/PCINT13/TMS)PC5" pad="23"/>
<connect gate="G$1" pin="(A14/PCINT14/TDO)PC6" pad="24"/>
<connect gate="G$1" pin="(A15/PCINT15/TDI)PC7" pad="25"/>
<connect gate="G$1" pin="(A8/PCINT8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9/PCINT9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0/PCINT0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1/PCINT1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2/PCINT2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3/PCINT3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4/PCINT4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5/PCINT5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6/PCINT6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7/PCINT7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/RXD1)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/TXD1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0/XCK1)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1/ICP3)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A/TOSC2)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS/OC3B)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1/OC2)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK0/TOSC1/OC3A)PD4" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="PE0(ICP1/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="6"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90CAN128" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
4 Kbytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
CAN 2.0 A&amp;B Interface&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="CAN128"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(CLKO/A15)PC7" pad="42"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="29"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A)PB4" pad="14"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXCAN/T1)PD6" pad="31"/>
<connect gate="G$1" pin="(RXD0/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXCAN/XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="(TXD0/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="53"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(CLKO/A15)PC7" pad="42"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="29"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A)PB4" pad="14"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXCAN/T1)PD6" pad="31"/>
<connect gate="G$1" pin="(RXD0/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXCAN/XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="(TXD0/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="53"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA164*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
512 Bytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA164"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="4"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="5"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="15"/>
<connect gate="G$1" pin="(PCI26/RXD1/INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(PCI27/TXD1/INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="1"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="2"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA324" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;p&gt;
1 kBytes SRAM&lt;p&gt;
1 kBytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA164-A"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="43"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="44"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="10"/>
<connect gate="G$1" pin="(PCI26/RXD1/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCI27/TXD1/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="5"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="43"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="44"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="10"/>
<connect gate="G$1" pin="(PCI26/RXD1/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCI27/TXD1/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="5"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA164" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
512 Bytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA164-A"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="43"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="44"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="10"/>
<connect gate="G$1" pin="(PCI26/RXD1/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCI27/TXD1/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="5"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="43"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="44"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="10"/>
<connect gate="G$1" pin="(PCI26/RXD1/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCI27/TXD1/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="5"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA324*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 kBytes FLASH&lt;p&gt;
2 kBytes SRAM&lt;p&gt;
1 kBytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA164"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="4"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="5"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="15"/>
<connect gate="G$1" pin="(PCI26/RXD1/INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(PCI27/TXD1/INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="1"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="2"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 kBytes FLASH&lt;p&gt;
4 kBytes SRAM&lt;p&gt;
2 kBytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA644-A"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="43"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="44"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="10"/>
<connect gate="G$1" pin="(PCI26/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCI27/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="5"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="M" package="MLF44">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="43"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="44"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="10"/>
<connect gate="G$1" pin="(PCI26/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCI27/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="18"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="5"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 kBytes FLASH&lt;p&gt;
4 kBytes SRAM&lt;p&gt;
2 kBytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA644"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(PCI0/ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(PCI1/ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(PCI10/AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(PCI11/AIN1/OC0A)PB3" pad="4"/>
<connect gate="G$1" pin="(PCI12/OC0B/SS)PB4" pad="5"/>
<connect gate="G$1" pin="(PCI13/MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(PCI14/MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(PCI15/SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(PCI16/SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(PCI17/SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(PCI18/TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(PCI19/TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(PCI2/ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(PCI20/TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(PCI21/TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(PCI22/TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(PCI23/TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(PCI24/RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(PCI25/TXD)PD1" pad="15"/>
<connect gate="G$1" pin="(PCI26/INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(PCI27/INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(PCI28/XCK1/OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(PCI29OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(PCI3/ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(PCI30/OC2B/ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(PCI31/OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(PCI4/ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(PCI5/ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(PCI6/ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(PCI7/ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(PCI8/T0/XCK0)PB0" pad="1"/>
<connect gate="G$1" pin="(PCI9/CLK0/T1)PB1" pad="2"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA48" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
512 Bytes SRAM&lt;p&gt;
256 Bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA168-A"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="12"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="13"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="31"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="1"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="14"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="2"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="9"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="10"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="15"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="8"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="29"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="M" package="MLF32">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="12"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="13"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="31"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="1"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="14"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="2"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="9"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="10"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="15"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="8"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="29"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA48*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
512 Bytes SRAM&lt;p&gt;
256 Bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA168"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="14"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="15"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="3"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="5"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="16"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="6"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="11"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="12"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="17"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="10"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA88" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 kBytes FLASH&lt;p&gt;
1 kBytes SRAM&lt;p&gt;
512 Bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA168-A"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="12"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="13"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="31"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="1"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="14"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="2"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="9"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="10"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="15"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="8"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="29"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="M" package="MLF32">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="12"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="13"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="31"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="1"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="14"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="2"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="9"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="10"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="15"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="8"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="29"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA88*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 kBytes FLASH&lt;p&gt;
1 kBytes SRAM&lt;p&gt;
512 Bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA168"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="14"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="15"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="3"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="5"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="16"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="6"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="11"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="12"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="17"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="10"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA168" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 kBytes FLASH&lt;p&gt;
1 kBytes SRAM&lt;p&gt;
512 Bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA168-A"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="12"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="13"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="31"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="1"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="14"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="2"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="9"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="10"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="15"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="8"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="29"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="M" package="MLF32">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="12"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="13"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="31"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="1"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="14"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="2"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="9"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="10"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="15"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="8"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="29"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA168*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 kBytes FLASH&lt;p&gt;
1 kBytes SRAM&lt;p&gt;
512 Bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA168"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(PCI0/ICP/CLKO)PB0" pad="14"/>
<connect gate="G$1" pin="(PCI1/OC1A/OC1S)PB1" pad="15"/>
<connect gate="G$1" pin="(PCI10/ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(PCI11/ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(PCI12/ADC4/SDA)PC4" pad="27"/>
<connect gate="G$1" pin="(PCI13/ADC5/SCL)PC5" pad="28"/>
<connect gate="G$1" pin="(PCI16/RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(PCI17/TXD)PD1" pad="3"/>
<connect gate="G$1" pin="(PCI18/INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(PCI19/INT1/OC2B)PD3" pad="5"/>
<connect gate="G$1" pin="(PCI2/SS/OC1B)PB2" pad="16"/>
<connect gate="G$1" pin="(PCI20/XCK/T0)PD4" pad="6"/>
<connect gate="G$1" pin="(PCI21/T1/OC0B)PD5" pad="11"/>
<connect gate="G$1" pin="(PCI22/AIN0OC0A)PD6" pad="12"/>
<connect gate="G$1" pin="(PCI23/AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(PCI3/MOSI/OC2A)PB3" pad="17"/>
<connect gate="G$1" pin="(PCI4/MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(PCI5/SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(PCI8/ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(PCI9/ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1/PCI6)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2/PCI7)" pad="10"/>
<connect gate="G$1" pin="PC6(/RESET/PCI14)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM&lt;p&gt;
64 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="TINY13"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(ADC2/PCI4)PB4" pad="3"/>
<connect gate="G$1" pin="(AIN0/MOSI/OC0A/PCI0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1/MISO/OC0B/INT0/PCI2)PB1" pad="6"/>
<connect gate="G$1" pin="(CLKI/ADC3/PCI3)PB3" pad="2"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCI5)PB5" pad="1"/>
<connect gate="G$1" pin="(T0/SCK/ADC1/PCI2)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="SS" package="SO08">
<connects>
<connect gate="G$1" pin="(ADC2/PCI4)PB4" pad="3"/>
<connect gate="G$1" pin="(AIN0/MOSI/OC0A/PCI0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1/MISO/OC0B/INT0/PCI2)PB1" pad="6"/>
<connect gate="G$1" pin="(CLKI/ADC3/PCI3)PB3" pad="2"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCI5)PB5" pad="1"/>
<connect gate="G$1" pin="(T0/SCK/ADC1/PCI2)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(ADC2/PCI4)PB4" pad="3"/>
<connect gate="G$1" pin="(AIN0/MOSI/OC0A/PCI0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1/MISO/OC0B/INT0/PCI2)PB1" pad="6"/>
<connect gate="G$1" pin="(CLKI/ADC3/PCI3)PB3" pad="2"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCI5)PB5" pad="1"/>
<connect gate="G$1" pin="(T0/SCK/ADC1/PCI2)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13*M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM&lt;p&gt;
64 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="TINY13M"/>
</gates>
<devices>
<device name="" package="MLF20">
<connects>
<connect gate="G$1" pin="(ADC2/PCI4)PB4" pad="5"/>
<connect gate="G$1" pin="(AIN0/MOSI/OC0A/PCI0)PB0" pad="11"/>
<connect gate="G$1" pin="(AIN1/MISO/OC0B/INT0/PCI2)PB1" pad="12"/>
<connect gate="G$1" pin="(CLKI/ADC3/PCI3)PB3" pad="2"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCI5)PB5" pad="1"/>
<connect gate="G$1" pin="(T0/SCK/ADC1/PCI2)PB2" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="P$1" pad="3"/>
<connect gate="G$1" pin="P$10" pad="18"/>
<connect gate="G$1" pin="P$11" pad="19"/>
<connect gate="G$1" pin="P$12" pad="20"/>
<connect gate="G$1" pin="P$2" pad="4"/>
<connect gate="G$1" pin="P$3" pad="6"/>
<connect gate="G$1" pin="P$4" pad="7"/>
<connect gate="G$1" pin="P$5" pad="9"/>
<connect gate="G$1" pin="P$6" pad="10"/>
<connect gate="G$1" pin="P$7" pad="13"/>
<connect gate="G$1" pin="P$8" pad="16"/>
<connect gate="G$1" pin="P$9" pad="17"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY2313" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="TINY2313"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0/PCI0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1/PCI1)PB1" pad="13"/>
<connect gate="G$1" pin="(CKOUT/XCK/INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO/DO/PCI6)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/PCI5)PB5" pad="17"/>
<connect gate="G$1" pin="(OC0A/PCI2)PB2" pad="14"/>
<connect gate="G$1" pin="(OC0B/T1)PD5" pad="9"/>
<connect gate="G$1" pin="(OC1A/PCI3)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCI4)PB4" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK/UCSK/PCI7)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RESET/DW/PA2" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1(PA0)" pad="5"/>
<connect gate="G$1" pin="XTAL2(PA1)" pad="4"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(AIN0/PCI0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1/PCI1)PB1" pad="13"/>
<connect gate="G$1" pin="(CKOUT/XCK/INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO/DO/PCI6)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/PCI5)PB5" pad="17"/>
<connect gate="G$1" pin="(OC0A/PCI2)PB2" pad="14"/>
<connect gate="G$1" pin="(OC0B/T1)PD5" pad="9"/>
<connect gate="G$1" pin="(OC1A/PCI3)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCI4)PB4" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK/UCSK/PCI7)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RESET/DW/PA2" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1(PA0)" pad="5"/>
<connect gate="G$1" pin="XTAL2(PA1)" pad="4"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="M" package="MLF20">
<connects>
<connect gate="G$1" pin="(AIN0/PCI0)PB0" pad="10"/>
<connect gate="G$1" pin="(AIN1/PCI1)PB1" pad="11"/>
<connect gate="G$1" pin="(CKOUT/XCK/INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="9"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO/DO/PCI6)PB6" pad="16"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/PCI5)PB5" pad="15"/>
<connect gate="G$1" pin="(OC0A/PCI2)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0B/T1)PD5" pad="7"/>
<connect gate="G$1" pin="(OC1A/PCI3)PB3" pad="13"/>
<connect gate="G$1" pin="(OC1B/PCI4)PB4" pad="14"/>
<connect gate="G$1" pin="(RXD)PD0" pad="20"/>
<connect gate="G$1" pin="(SCK/UCSK/PCI7)PB7" pad="17"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(TXD)PD1" pad="1"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RESET/DW/PA2" pad="19"/>
<connect gate="G$1" pin="VCC" pad="18"/>
<connect gate="G$1" pin="XTAL1(PA0)" pad="3"/>
<connect gate="G$1" pin="XTAL2(PA1)" pad="2"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY26" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
USI&lt;p&gt;
10-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="TINY26"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="20"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="19"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="18"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="14"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="13"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="9"/>
<connect gate="G$1" pin="(AIN0/ADC5)PA6" pad="12"/>
<connect gate="G$1" pin="(AIN1/ADC6)PA7" pad="11"/>
<connect gate="G$1" pin="(AREF)PA3" pad="17"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="2"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/OC1A)PB0" pad="1"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="4"/>
<connect gate="G$1" pin="(RESET/ADC10)PB7" pad="10"/>
<connect gate="G$1" pin="(SCK/SCL/OC1B)PB2" pad="3"/>
<connect gate="G$1" pin="AGND" pad="16"/>
<connect gate="G$1" pin="AVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="XTAL1(PB4/ADC7)" pad="7"/>
<connect gate="G$1" pin="XTAL2(PB5/ADC8)" pad="8"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="20"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="19"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="18"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="14"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="13"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="9"/>
<connect gate="G$1" pin="(AIN0/ADC5)PA6" pad="12"/>
<connect gate="G$1" pin="(AIN1/ADC6)PA7" pad="11"/>
<connect gate="G$1" pin="(AREF)PA3" pad="17"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="2"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/OC1A)PB0" pad="1"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="4"/>
<connect gate="G$1" pin="(RESET/ADC10)PB7" pad="10"/>
<connect gate="G$1" pin="(SCK/SCL/OC1B)PB2" pad="3"/>
<connect gate="G$1" pin="AGND" pad="16"/>
<connect gate="G$1" pin="AVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="XTAL1(PB4/ADC7)" pad="7"/>
<connect gate="G$1" pin="XTAL2(PB5/ADC8)" pad="8"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY26*M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
USI&lt;p&gt;
10-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="TINY26M"/>
</gates>
<devices>
<device name="" package="MLF32">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="26"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="25"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="23"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="17"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="15"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="10"/>
<connect gate="G$1" pin="(AIN0/ADC5)PA6" pad="14"/>
<connect gate="G$1" pin="(AIN1/ADC6)PA7" pad="13"/>
<connect gate="G$1" pin="(AREF)PA3" pad="22"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="31"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/OC1A)PB0" pad="30"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="2"/>
<connect gate="G$1" pin="(RESET/ADC10)PB7" pad="11"/>
<connect gate="G$1" pin="(SCK/SCL/OC1B)PB2" pad="32"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="27"/>
<connect gate="G$1" pin="P$11" pad="28"/>
<connect gate="G$1" pin="P$12" pad="29"/>
<connect gate="G$1" pin="P$2" pad="3"/>
<connect gate="G$1" pin="P$3" pad="6"/>
<connect gate="G$1" pin="P$4" pad="9"/>
<connect gate="G$1" pin="P$5" pad="12"/>
<connect gate="G$1" pin="P$6" pad="16"/>
<connect gate="G$1" pin="P$7" pad="19"/>
<connect gate="G$1" pin="P$8" pad="20"/>
<connect gate="G$1" pin="P$9" pad="24"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1(PB4/ADC7)" pad="7"/>
<connect gate="G$1" pin="XTAL2(PB5/ADC8)" pad="8"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="L-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA3290" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;p&gt;
2 Kbytes SRAM&lt;p&gt;
1 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
LCD Driver</description>
<gates>
<gate name="G$1" symbol="MEGA32906490"/>
</gates>
<devices>
<device name="A" package="TQFP100">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="78"/>
<connect gate="G$1" pin="(COM1)PA1" pad="77"/>
<connect gate="G$1" pin="(COM2)PA2" pad="76"/>
<connect gate="G$1" pin="(COM3)PA3" pad="75"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="74"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="73"/>
<connect gate="G$1" pin="(SEG10/PCINT16)PH0" pad="63"/>
<connect gate="G$1" pin="(SEG11)PC5" pad="58"/>
<connect gate="G$1" pin="(SEG12)PC4" pad="57"/>
<connect gate="G$1" pin="(SEG13)PC3" pad="56"/>
<connect gate="G$1" pin="(SEG14)PC2" pad="55"/>
<connect gate="G$1" pin="(SEG15)PC1" pad="54"/>
<connect gate="G$1" pin="(SEG16)PC0" pad="53"/>
<connect gate="G$1" pin="(SEG17)PG1" pad="52"/>
<connect gate="G$1" pin="(SEG18)PG0" pad="51"/>
<connect gate="G$1" pin="(SEG19)PD7" pad="50"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="72"/>
<connect gate="G$1" pin="(SEG20)PD6" pad="49"/>
<connect gate="G$1" pin="(SEG21)PD5" pad="48"/>
<connect gate="G$1" pin="(SEG22)PD4" pad="47"/>
<connect gate="G$1" pin="(SEG23)PD3" pad="46"/>
<connect gate="G$1" pin="(SEG24)PD2" pad="45"/>
<connect gate="G$1" pin="(SEG25/INT0)PD1" pad="44"/>
<connect gate="G$1" pin="(SEG26/ICP1)PD0" pad="43"/>
<connect gate="G$1" pin="(SEG27/PCINT30)PJ6" pad="41"/>
<connect gate="G$1" pin="(SEG28/PCINT29)PJ5" pad="40"/>
<connect gate="G$1" pin="(SEG29/PCINT28)PJ4" pad="39"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="71"/>
<connect gate="G$1" pin="(SEG30/PCINT27)PJ3" pad="38"/>
<connect gate="G$1" pin="(SEG31/PCINT26)PJ2" pad="37"/>
<connect gate="G$1" pin="(SEG32/T0)PG4" pad="29"/>
<connect gate="G$1" pin="(SEG33/T1)PG3" pad="28"/>
<connect gate="G$1" pin="(SEG34/PCINT25)PJ1" pad="14"/>
<connect gate="G$1" pin="(SEG35/PCINT24)PJ0" pad="13"/>
<connect gate="G$1" pin="(SEG36/PCINT23)PH7" pad="87"/>
<connect gate="G$1" pin="(SEG37/PCINT22)PH6" pad="86"/>
<connect gate="G$1" pin="(SEG38/PCINT21)PH5" pad="85"/>
<connect gate="G$1" pin="(SEG39/PCINT20)PH4" pad="84"/>
<connect gate="G$1" pin="(SEG4)PG2" pad="70"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="69"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="68"/>
<connect gate="G$1" pin="(SEG7/PCINT19)PH3" pad="66"/>
<connect gate="G$1" pin="(SEG8/PCINT18)PH2" pad="65"/>
<connect gate="G$1" pin="(SEG9/PCINT17)PH1" pad="64"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="99"/>
<connect gate="G$1" pin="AREF" pad="98"/>
<connect gate="G$1" pin="AVCC" pad="100"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="32"/>
<connect gate="G$1" pin="GND@3" pad="81"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="P$57" pad="12"/>
<connect gate="G$1" pin="P$58" pad="15"/>
<connect gate="G$1" pin="P$59" pad="16"/>
<connect gate="G$1" pin="P$60" pad="17"/>
<connect gate="G$1" pin="P$61" pad="18"/>
<connect gate="G$1" pin="P$62" pad="27"/>
<connect gate="G$1" pin="P$63" pad="35"/>
<connect gate="G$1" pin="P$64" pad="36"/>
<connect gate="G$1" pin="P$65" pad="42"/>
<connect gate="G$1" pin="P$66" pad="59"/>
<connect gate="G$1" pin="P$67" pad="60"/>
<connect gate="G$1" pin="P$68" pad="61"/>
<connect gate="G$1" pin="P$69" pad="62"/>
<connect gate="G$1" pin="P$70" pad="67"/>
<connect gate="G$1" pin="P$71" pad="79"/>
<connect gate="G$1" pin="P$72" pad="82"/>
<connect gate="G$1" pin="P$73" pad="83"/>
<connect gate="G$1" pin="P$74" pad="88"/>
<connect gate="G$1" pin="P$75" pad="89"/>
<connect gate="G$1" pin="PB0(PCINT8/SS)" pad="19"/>
<connect gate="G$1" pin="PB1(PCINT9/SCK)" pad="20"/>
<connect gate="G$1" pin="PB2(PCINT10/MOSI)" pad="21"/>
<connect gate="G$1" pin="PB3(PCINT11/MISO)" pad="22"/>
<connect gate="G$1" pin="PB4(PCINT12/OC0A)" pad="23"/>
<connect gate="G$1" pin="PB5(PCINT13/OC1A)" pad="24"/>
<connect gate="G$1" pin="PB6(PCINT14/OC1B)" pad="25"/>
<connect gate="G$1" pin="PB7(PCINT15/OC2A)" pad="26"/>
<connect gate="G$1" pin="PB7/RESET" pad="30"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="97"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="96"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="95"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="94"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="93"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="92"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="91"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="90"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="31"/>
<connect gate="G$1" pin="VCC@3" pad="80"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="34"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="33"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA6490" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
2 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
LCD Driver</description>
<gates>
<gate name="G$1" symbol="MEGA32906490"/>
</gates>
<devices>
<device name="A" package="TQFP100">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="78"/>
<connect gate="G$1" pin="(COM1)PA1" pad="77"/>
<connect gate="G$1" pin="(COM2)PA2" pad="76"/>
<connect gate="G$1" pin="(COM3)PA3" pad="75"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="74"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="73"/>
<connect gate="G$1" pin="(SEG10/PCINT16)PH0" pad="63"/>
<connect gate="G$1" pin="(SEG11)PC5" pad="58"/>
<connect gate="G$1" pin="(SEG12)PC4" pad="57"/>
<connect gate="G$1" pin="(SEG13)PC3" pad="56"/>
<connect gate="G$1" pin="(SEG14)PC2" pad="55"/>
<connect gate="G$1" pin="(SEG15)PC1" pad="54"/>
<connect gate="G$1" pin="(SEG16)PC0" pad="53"/>
<connect gate="G$1" pin="(SEG17)PG1" pad="52"/>
<connect gate="G$1" pin="(SEG18)PG0" pad="51"/>
<connect gate="G$1" pin="(SEG19)PD7" pad="50"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="72"/>
<connect gate="G$1" pin="(SEG20)PD6" pad="49"/>
<connect gate="G$1" pin="(SEG21)PD5" pad="48"/>
<connect gate="G$1" pin="(SEG22)PD4" pad="47"/>
<connect gate="G$1" pin="(SEG23)PD3" pad="46"/>
<connect gate="G$1" pin="(SEG24)PD2" pad="45"/>
<connect gate="G$1" pin="(SEG25/INT0)PD1" pad="44"/>
<connect gate="G$1" pin="(SEG26/ICP1)PD0" pad="43"/>
<connect gate="G$1" pin="(SEG27/PCINT30)PJ6" pad="41"/>
<connect gate="G$1" pin="(SEG28/PCINT29)PJ5" pad="40"/>
<connect gate="G$1" pin="(SEG29/PCINT28)PJ4" pad="39"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="71"/>
<connect gate="G$1" pin="(SEG30/PCINT27)PJ3" pad="38"/>
<connect gate="G$1" pin="(SEG31/PCINT26)PJ2" pad="37"/>
<connect gate="G$1" pin="(SEG32/T0)PG4" pad="29"/>
<connect gate="G$1" pin="(SEG33/T1)PG3" pad="28"/>
<connect gate="G$1" pin="(SEG34/PCINT25)PJ1" pad="14"/>
<connect gate="G$1" pin="(SEG35/PCINT24)PJ0" pad="13"/>
<connect gate="G$1" pin="(SEG36/PCINT23)PH7" pad="87"/>
<connect gate="G$1" pin="(SEG37/PCINT22)PH6" pad="86"/>
<connect gate="G$1" pin="(SEG38/PCINT21)PH5" pad="85"/>
<connect gate="G$1" pin="(SEG39/PCINT20)PH4" pad="84"/>
<connect gate="G$1" pin="(SEG4)PG2" pad="70"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="69"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="68"/>
<connect gate="G$1" pin="(SEG7/PCINT19)PH3" pad="66"/>
<connect gate="G$1" pin="(SEG8/PCINT18)PH2" pad="65"/>
<connect gate="G$1" pin="(SEG9/PCINT17)PH1" pad="64"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="99"/>
<connect gate="G$1" pin="AREF" pad="98"/>
<connect gate="G$1" pin="AVCC" pad="100"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="32"/>
<connect gate="G$1" pin="GND@3" pad="81"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="P$57" pad="12"/>
<connect gate="G$1" pin="P$58" pad="15"/>
<connect gate="G$1" pin="P$59" pad="16"/>
<connect gate="G$1" pin="P$60" pad="17"/>
<connect gate="G$1" pin="P$61" pad="18"/>
<connect gate="G$1" pin="P$62" pad="27"/>
<connect gate="G$1" pin="P$63" pad="35"/>
<connect gate="G$1" pin="P$64" pad="36"/>
<connect gate="G$1" pin="P$65" pad="42"/>
<connect gate="G$1" pin="P$66" pad="59"/>
<connect gate="G$1" pin="P$67" pad="60"/>
<connect gate="G$1" pin="P$68" pad="61"/>
<connect gate="G$1" pin="P$69" pad="62"/>
<connect gate="G$1" pin="P$70" pad="67"/>
<connect gate="G$1" pin="P$71" pad="79"/>
<connect gate="G$1" pin="P$72" pad="82"/>
<connect gate="G$1" pin="P$73" pad="83"/>
<connect gate="G$1" pin="P$74" pad="88"/>
<connect gate="G$1" pin="P$75" pad="89"/>
<connect gate="G$1" pin="PB0(PCINT8/SS)" pad="19"/>
<connect gate="G$1" pin="PB1(PCINT9/SCK)" pad="20"/>
<connect gate="G$1" pin="PB2(PCINT10/MOSI)" pad="21"/>
<connect gate="G$1" pin="PB3(PCINT11/MISO)" pad="22"/>
<connect gate="G$1" pin="PB4(PCINT12/OC0A)" pad="23"/>
<connect gate="G$1" pin="PB5(PCINT13/OC1A)" pad="24"/>
<connect gate="G$1" pin="PB6(PCINT14/OC1B)" pad="25"/>
<connect gate="G$1" pin="PB7(PCINT15/OC2A)" pad="26"/>
<connect gate="G$1" pin="PB7/RESET" pad="30"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="97"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="96"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="95"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="94"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="93"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="92"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="91"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="90"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="31"/>
<connect gate="G$1" pin="VCC@3" pad="80"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="34"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="33"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA329" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;p&gt;
2 Kbytes SRAM&lt;p&gt;
1 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
LCD Driver</description>
<gates>
<gate name="G$1" symbol="MEGA329649"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG13)PG1" pad="34"/>
<connect gate="G$1" pin="(SEG14)PG0" pad="33"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG23/T0)PG4" pad="19"/>
<connect gate="G$1" pin="(SEG24/T1)PG3" pad="18"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG4)PG2" pad="43"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PB0(PCINT8/SS)" pad="10"/>
<connect gate="G$1" pin="PB1(PCINT9/SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(PCINT10/MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(PCINT11/MISO)" pad="13"/>
<connect gate="G$1" pin="PB4(PCINT12/OC0A)" pad="14"/>
<connect gate="G$1" pin="PB5(PCINT13/OC1A)" pad="15"/>
<connect gate="G$1" pin="PB6(PCINT14/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB7(PCINT15/OC2A)" pad="17"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="RESET/PG5" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG13)PG1" pad="34"/>
<connect gate="G$1" pin="(SEG14)PG0" pad="33"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG23/T0)PG4" pad="19"/>
<connect gate="G$1" pin="(SEG24/T1)PG3" pad="18"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG4)PG2" pad="43"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PB0(PCINT8/SS)" pad="10"/>
<connect gate="G$1" pin="PB1(PCINT9/SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(PCINT10/MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(PCINT11/MISO)" pad="13"/>
<connect gate="G$1" pin="PB4(PCINT12/OC0A)" pad="14"/>
<connect gate="G$1" pin="PB5(PCINT13/OC1A)" pad="15"/>
<connect gate="G$1" pin="PB6(PCINT14/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB7(PCINT15/OC2A)" pad="17"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="RESET/PG5" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA649" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
2 Kbytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
LCD Driver</description>
<gates>
<gate name="G$1" symbol="MEGA329649"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG13)PG1" pad="34"/>
<connect gate="G$1" pin="(SEG14)PG0" pad="33"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG23/T0)PG4" pad="19"/>
<connect gate="G$1" pin="(SEG24/T1)PG3" pad="18"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG4)PG2" pad="43"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PB0(PCINT8/SS)" pad="10"/>
<connect gate="G$1" pin="PB1(PCINT9/SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(PCINT10/MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(PCINT11/MISO)" pad="13"/>
<connect gate="G$1" pin="PB4(PCINT12/OC0A)" pad="14"/>
<connect gate="G$1" pin="PB5(PCINT13/OC1A)" pad="15"/>
<connect gate="G$1" pin="PB6(PCINT14/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB7(PCINT15/OC2A)" pad="17"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="RESET/PG5" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG13)PG1" pad="34"/>
<connect gate="G$1" pin="(SEG14)PG0" pad="33"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG23/T0)PG4" pad="19"/>
<connect gate="G$1" pin="(SEG24/T1)PG3" pad="18"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG4)PG2" pad="43"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PB0(PCINT8/SS)" pad="10"/>
<connect gate="G$1" pin="PB1(PCINT9/SCK)" pad="11"/>
<connect gate="G$1" pin="PB2(PCINT10/MOSI)" pad="12"/>
<connect gate="G$1" pin="PB3(PCINT11/MISO)" pad="13"/>
<connect gate="G$1" pin="PB4(PCINT12/OC0A)" pad="14"/>
<connect gate="G$1" pin="PB5(PCINT13/OC1A)" pad="15"/>
<connect gate="G$1" pin="PB6(PCINT14/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB7(PCINT15/OC2A)" pad="17"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="RESET/PG5" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY25" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
128 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="TINY25_45_85"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY25*M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
128 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="TINY25_45_85*M"/>
</gates>
<devices>
<device name="" package="MLF20">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="12"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="11"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="14"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="5"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="P$1" pad="3"/>
<connect gate="G$1" pin="P$10" pad="18"/>
<connect gate="G$1" pin="P$11" pad="19"/>
<connect gate="G$1" pin="P$12" pad="20"/>
<connect gate="G$1" pin="P$2" pad="4"/>
<connect gate="G$1" pin="P$3" pad="6"/>
<connect gate="G$1" pin="P$4" pad="7"/>
<connect gate="G$1" pin="P$5" pad="9"/>
<connect gate="G$1" pin="P$6" pad="10"/>
<connect gate="G$1" pin="P$7" pad="13"/>
<connect gate="G$1" pin="P$8" pad="16"/>
<connect gate="G$1" pin="P$9" pad="17"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
256 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="TINY25_45_85"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45*M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
256 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="TINY25_45_85*M"/>
</gates>
<devices>
<device name="" package="MLF20">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="12"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="11"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="14"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="5"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="P$1" pad="3"/>
<connect gate="G$1" pin="P$10" pad="18"/>
<connect gate="G$1" pin="P$11" pad="19"/>
<connect gate="G$1" pin="P$12" pad="20"/>
<connect gate="G$1" pin="P$2" pad="4"/>
<connect gate="G$1" pin="P$3" pad="6"/>
<connect gate="G$1" pin="P$4" pad="7"/>
<connect gate="G$1" pin="P$5" pad="9"/>
<connect gate="G$1" pin="P$6" pad="10"/>
<connect gate="G$1" pin="P$7" pad="13"/>
<connect gate="G$1" pin="P$8" pad="16"/>
<connect gate="G$1" pin="P$9" pad="17"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
512 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="TINY25_45_85"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85*M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
512 bytes RAM&lt;p&gt;
4-channel 10 bit ADC&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="TINY25_45_85*M"/>
</gates>
<devices>
<device name="" package="MLF20">
<connects>
<connect gate="G$1" pin="(MISO/DO/AIN1/OC0B/OC1A/PCINT1)PB1" pad="12"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/AIN0/OC0A/OC1A/AREF/PCINT0)PB0" pad="11"/>
<connect gate="G$1" pin="(RESET/DW/ADC0/PCINT5)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)PB2" pad="14"/>
<connect gate="G$1" pin="(XTAL1/CLKI/OC1B/ADC3/PCINT3)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2/CLKO/OC1B/ADC2/PCINT4)PB4" pad="5"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="P$1" pad="3"/>
<connect gate="G$1" pin="P$10" pad="18"/>
<connect gate="G$1" pin="P$11" pad="19"/>
<connect gate="G$1" pin="P$12" pad="20"/>
<connect gate="G$1" pin="P$2" pad="4"/>
<connect gate="G$1" pin="P$3" pad="6"/>
<connect gate="G$1" pin="P$4" pad="7"/>
<connect gate="G$1" pin="P$5" pad="9"/>
<connect gate="G$1" pin="P$6" pad="10"/>
<connect gate="G$1" pin="P$7" pad="13"/>
<connect gate="G$1" pin="P$8" pad="16"/>
<connect gate="G$1" pin="P$9" pad="17"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name="-20"/>
<technology name="V-10"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA165" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;p&gt;
1 Kbytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;
USI</description>
<gates>
<gate name="G$1" symbol="MEGA165"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(AIN1/PCI3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCI7)PE7" pad="9"/>
<connect gate="G$1" pin="(DI/SDA/PCI5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCI6)PE6" pad="8"/>
<connect gate="G$1" pin="(ICP1)PD0" pad="25"/>
<connect gate="G$1" pin="(INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(MISO/PCI11)PB3" pad="17"/>
<connect gate="G$1" pin="(MOSI/PCI10)PB2" pad="16"/>
<connect gate="G$1" pin="(OC0A/PCI12)PB4" pad="15"/>
<connect gate="G$1" pin="(OC1A/PCI13)PB5" pad="14"/>
<connect gate="G$1" pin="(OC1B/PCI14)PB6" pad="13"/>
<connect gate="G$1" pin="(OC2A/PCI15)PB7" pad="12"/>
<connect gate="G$1" pin="(RXD/PCI0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCI9)PB1" pad="11"/>
<connect gate="G$1" pin="(SS/PCI8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCI2)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCI4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCI2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="PG3(T1)" pad="18"/>
<connect gate="G$1" pin="PG4(T0)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(AIN1/PCI3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCI7)PE7" pad="9"/>
<connect gate="G$1" pin="(DI/SDA/PCI5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCI6)PE6" pad="8"/>
<connect gate="G$1" pin="(ICP1)PD0" pad="25"/>
<connect gate="G$1" pin="(INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(MISO/PCI11)PB3" pad="17"/>
<connect gate="G$1" pin="(MOSI/PCI10)PB2" pad="16"/>
<connect gate="G$1" pin="(OC0A/PCI12)PB4" pad="15"/>
<connect gate="G$1" pin="(OC1A/PCI13)PB5" pad="14"/>
<connect gate="G$1" pin="(OC1B/PCI14)PB6" pad="13"/>
<connect gate="G$1" pin="(OC2A/PCI15)PB7" pad="12"/>
<connect gate="G$1" pin="(RXD/PCI0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCI9)PB1" pad="11"/>
<connect gate="G$1" pin="(SS/PCI8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCI2)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCI4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCI2)PE2" pad="4"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="PG3(T1)" pad="18"/>
<connect gate="G$1" pin="PG4(T0)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA2560" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
256 kBytes FLASH&lt;p&gt;
8 kBytes SRAM&lt;p&gt;
4 kBytes EEPROM&lt;p&gt;
QUAD USART&lt;p&gt;
16-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA2560"/>
</gates>
<devices>
<device name="A" package="TQFP100">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="55"/>
<connect gate="G$1" pin="(A11)PC3" pad="56"/>
<connect gate="G$1" pin="(A12)PC4" pad="57"/>
<connect gate="G$1" pin="(A13)PC5" pad="58"/>
<connect gate="G$1" pin="(A14)PC6" pad="59"/>
<connect gate="G$1" pin="(A15)PC7" pad="60"/>
<connect gate="G$1" pin="(A8)PC0" pad="53"/>
<connect gate="G$1" pin="(A9)PC1" pad="54"/>
<connect gate="G$1" pin="(AD0)PA0" pad="78"/>
<connect gate="G$1" pin="(AD1)PA1" pad="77"/>
<connect gate="G$1" pin="(AD2)PA2" pad="76"/>
<connect gate="G$1" pin="(AD3)PA3" pad="75"/>
<connect gate="G$1" pin="(AD4)PA4" pad="74"/>
<connect gate="G$1" pin="(AD5)PA5" pad="73"/>
<connect gate="G$1" pin="(AD6)PA6" pad="72"/>
<connect gate="G$1" pin="(AD7)PA7" pad="71"/>
<connect gate="G$1" pin="(ADC0)PF0" pad="97"/>
<connect gate="G$1" pin="(ADC1)PF1" pad="96"/>
<connect gate="G$1" pin="(ADC2)PF2" pad="95"/>
<connect gate="G$1" pin="(ADC3)PF3" pad="94"/>
<connect gate="G$1" pin="(CLKO/ICP2/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="47"/>
<connect gate="G$1" pin="(MISO/PCINT3)PB3" pad="22"/>
<connect gate="G$1" pin="(MOSI/PCINT2)PB2" pad="21"/>
<connect gate="G$1" pin="(OC0A/OC1C/PCINT7)PB7" pad="26"/>
<connect gate="G$1" pin="(OC1A/PCINT5)PB5" pad="24"/>
<connect gate="G$1" pin="(OC1B/PCINT6)PB6" pad="25"/>
<connect gate="G$1" pin="(OC2A/PCINT4)PB4" pad="23"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(PCINT16/ADC8)PK0" pad="89"/>
<connect gate="G$1" pin="(PCINT17/ADC9)PK1" pad="88"/>
<connect gate="G$1" pin="(PCINT18/ADC10)PK2" pad="87"/>
<connect gate="G$1" pin="(PCINT19/ADC11)PK3" pad="86"/>
<connect gate="G$1" pin="(PCINT20/ADC12)PK4" pad="85"/>
<connect gate="G$1" pin="(PCINT21/ADC13)PK5" pad="84"/>
<connect gate="G$1" pin="(PCINT22/ADC14)PK6" pad="83"/>
<connect gate="G$1" pin="(PCINT23/ADC15)PK7" pad="82"/>
<connect gate="G$1" pin="(RXD0/PCINT8)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="45"/>
<connect gate="G$1" pin="(SCK/PCINT1)PB1" pad="20"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="43"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="44"/>
<connect gate="G$1" pin="(SS/PCINT0)PB0" pad="19"/>
<connect gate="G$1" pin="(T0)PD7" pad="50"/>
<connect gate="G$1" pin="(T1)PD6" pad="49"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TCK/ADC4)PF4" pad="93"/>
<connect gate="G$1" pin="(TDI/ADC7)PF7" pad="90"/>
<connect gate="G$1" pin="(TDO/ADC6)PF6" pad="91"/>
<connect gate="G$1" pin="(TMS/ADC5)PF5" pad="92"/>
<connect gate="G$1" pin="(TXD0)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="46"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="48"/>
<connect gate="G$1" pin="AGND" pad="99"/>
<connect gate="G$1" pin="AREF" pad="98"/>
<connect gate="G$1" pin="AVCC" pad="100"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="32"/>
<connect gate="G$1" pin="GND@3" pad="62"/>
<connect gate="G$1" pin="GND@4" pad="81"/>
<connect gate="G$1" pin="PG0(WR)" pad="51"/>
<connect gate="G$1" pin="PG1(RD)" pad="52"/>
<connect gate="G$1" pin="PG2(ALE)" pad="70"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="28"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="29"/>
<connect gate="G$1" pin="PG5(OC0B)" pad="1"/>
<connect gate="G$1" pin="PH0(RXD2)" pad="12"/>
<connect gate="G$1" pin="PH1(TXD2)" pad="13"/>
<connect gate="G$1" pin="PH2(XCK2)" pad="14"/>
<connect gate="G$1" pin="PH3(OC4A)" pad="15"/>
<connect gate="G$1" pin="PH4(OC4B)" pad="16"/>
<connect gate="G$1" pin="PH5(OC4C)" pad="17"/>
<connect gate="G$1" pin="PH6(OC2B)" pad="18"/>
<connect gate="G$1" pin="PH7(T4)" pad="27"/>
<connect gate="G$1" pin="PJ0(PCINT9/RXD3)" pad="63"/>
<connect gate="G$1" pin="PJ1(PCINT10/TXD3)" pad="64"/>
<connect gate="G$1" pin="PJ2((PCINT11/XCK3)" pad="65"/>
<connect gate="G$1" pin="PJ3(PCINT12" pad="66"/>
<connect gate="G$1" pin="PJ4(PCINT13)" pad="67"/>
<connect gate="G$1" pin="PJ5(PCINT14)" pad="68"/>
<connect gate="G$1" pin="PJ6(PCINT15)" pad="69"/>
<connect gate="G$1" pin="PJ7" pad="79"/>
<connect gate="G$1" pin="PL0(ICP4)" pad="35"/>
<connect gate="G$1" pin="PL1(ICP5)" pad="36"/>
<connect gate="G$1" pin="PL2(T5)" pad="37"/>
<connect gate="G$1" pin="PL3(PC5A)" pad="38"/>
<connect gate="G$1" pin="PL4(OC5B)" pad="39"/>
<connect gate="G$1" pin="PL5(OC5C)" pad="40"/>
<connect gate="G$1" pin="PL6" pad="41"/>
<connect gate="G$1" pin="PL7" pad="42"/>
<connect gate="G$1" pin="RESET" pad="30"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="31"/>
<connect gate="G$1" pin="VCC@3" pad="61"/>
<connect gate="G$1" pin="VCC@4" pad="80"/>
<connect gate="G$1" pin="XTAL1" pad="34"/>
<connect gate="G$1" pin="XTAL2" pad="33"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA1280" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 kBytes FLASH&lt;p&gt;
8 kBytes SRAM&lt;p&gt;
4 kBytes EEPROM&lt;p&gt;
QUAD USART&lt;p&gt;
16-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA2560"/>
</gates>
<devices>
<device name="A" package="TQFP100">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="55"/>
<connect gate="G$1" pin="(A11)PC3" pad="56"/>
<connect gate="G$1" pin="(A12)PC4" pad="57"/>
<connect gate="G$1" pin="(A13)PC5" pad="58"/>
<connect gate="G$1" pin="(A14)PC6" pad="59"/>
<connect gate="G$1" pin="(A15)PC7" pad="60"/>
<connect gate="G$1" pin="(A8)PC0" pad="53"/>
<connect gate="G$1" pin="(A9)PC1" pad="54"/>
<connect gate="G$1" pin="(AD0)PA0" pad="78"/>
<connect gate="G$1" pin="(AD1)PA1" pad="77"/>
<connect gate="G$1" pin="(AD2)PA2" pad="76"/>
<connect gate="G$1" pin="(AD3)PA3" pad="75"/>
<connect gate="G$1" pin="(AD4)PA4" pad="74"/>
<connect gate="G$1" pin="(AD5)PA5" pad="73"/>
<connect gate="G$1" pin="(AD6)PA6" pad="72"/>
<connect gate="G$1" pin="(AD7)PA7" pad="71"/>
<connect gate="G$1" pin="(ADC0)PF0" pad="97"/>
<connect gate="G$1" pin="(ADC1)PF1" pad="96"/>
<connect gate="G$1" pin="(ADC2)PF2" pad="95"/>
<connect gate="G$1" pin="(ADC3)PF3" pad="94"/>
<connect gate="G$1" pin="(CLKO/ICP2/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="47"/>
<connect gate="G$1" pin="(MISO/PCINT3)PB3" pad="22"/>
<connect gate="G$1" pin="(MOSI/PCINT2)PB2" pad="21"/>
<connect gate="G$1" pin="(OC0A/OC1C/PCINT7)PB7" pad="26"/>
<connect gate="G$1" pin="(OC1A/PCINT5)PB5" pad="24"/>
<connect gate="G$1" pin="(OC1B/PCINT6)PB6" pad="25"/>
<connect gate="G$1" pin="(OC2A/PCINT4)PB4" pad="23"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(PCINT16/ADC8)PK0" pad="89"/>
<connect gate="G$1" pin="(PCINT17/ADC9)PK1" pad="88"/>
<connect gate="G$1" pin="(PCINT18/ADC10)PK2" pad="87"/>
<connect gate="G$1" pin="(PCINT19/ADC11)PK3" pad="86"/>
<connect gate="G$1" pin="(PCINT20/ADC12)PK4" pad="85"/>
<connect gate="G$1" pin="(PCINT21/ADC13)PK5" pad="84"/>
<connect gate="G$1" pin="(PCINT22/ADC14)PK6" pad="83"/>
<connect gate="G$1" pin="(PCINT23/ADC15)PK7" pad="82"/>
<connect gate="G$1" pin="(RXD0/PCINT8)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="45"/>
<connect gate="G$1" pin="(SCK/PCINT1)PB1" pad="20"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="43"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="44"/>
<connect gate="G$1" pin="(SS/PCINT0)PB0" pad="19"/>
<connect gate="G$1" pin="(T0)PD7" pad="50"/>
<connect gate="G$1" pin="(T1)PD6" pad="49"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TCK/ADC4)PF4" pad="93"/>
<connect gate="G$1" pin="(TDI/ADC7)PF7" pad="90"/>
<connect gate="G$1" pin="(TDO/ADC6)PF6" pad="91"/>
<connect gate="G$1" pin="(TMS/ADC5)PF5" pad="92"/>
<connect gate="G$1" pin="(TXD0)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="46"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="48"/>
<connect gate="G$1" pin="AGND" pad="99"/>
<connect gate="G$1" pin="AREF" pad="98"/>
<connect gate="G$1" pin="AVCC" pad="100"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="32"/>
<connect gate="G$1" pin="GND@3" pad="62"/>
<connect gate="G$1" pin="GND@4" pad="81"/>
<connect gate="G$1" pin="PG0(WR)" pad="51"/>
<connect gate="G$1" pin="PG1(RD)" pad="52"/>
<connect gate="G$1" pin="PG2(ALE)" pad="70"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="28"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="29"/>
<connect gate="G$1" pin="PG5(OC0B)" pad="1"/>
<connect gate="G$1" pin="PH0(RXD2)" pad="12"/>
<connect gate="G$1" pin="PH1(TXD2)" pad="13"/>
<connect gate="G$1" pin="PH2(XCK2)" pad="14"/>
<connect gate="G$1" pin="PH3(OC4A)" pad="15"/>
<connect gate="G$1" pin="PH4(OC4B)" pad="16"/>
<connect gate="G$1" pin="PH5(OC4C)" pad="17"/>
<connect gate="G$1" pin="PH6(OC2B)" pad="18"/>
<connect gate="G$1" pin="PH7(T4)" pad="27"/>
<connect gate="G$1" pin="PJ0(PCINT9/RXD3)" pad="63"/>
<connect gate="G$1" pin="PJ1(PCINT10/TXD3)" pad="64"/>
<connect gate="G$1" pin="PJ2((PCINT11/XCK3)" pad="65"/>
<connect gate="G$1" pin="PJ3(PCINT12" pad="66"/>
<connect gate="G$1" pin="PJ4(PCINT13)" pad="67"/>
<connect gate="G$1" pin="PJ5(PCINT14)" pad="68"/>
<connect gate="G$1" pin="PJ6(PCINT15)" pad="69"/>
<connect gate="G$1" pin="PJ7" pad="79"/>
<connect gate="G$1" pin="PL0(ICP4)" pad="35"/>
<connect gate="G$1" pin="PL1(ICP5)" pad="36"/>
<connect gate="G$1" pin="PL2(T5)" pad="37"/>
<connect gate="G$1" pin="PL3(PC5A)" pad="38"/>
<connect gate="G$1" pin="PL4(OC5B)" pad="39"/>
<connect gate="G$1" pin="PL5(OC5C)" pad="40"/>
<connect gate="G$1" pin="PL6" pad="41"/>
<connect gate="G$1" pin="PL7" pad="42"/>
<connect gate="G$1" pin="RESET" pad="30"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="31"/>
<connect gate="G$1" pin="VCC@3" pad="61"/>
<connect gate="G$1" pin="VCC@4" pad="80"/>
<connect gate="G$1" pin="XTAL1" pad="34"/>
<connect gate="G$1" pin="XTAL2" pad="33"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA640" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 kBytes FLASH&lt;p&gt;
8 kBytes SRAM&lt;p&gt;
4 kBytes EEPROM&lt;p&gt;
QUAD USART&lt;p&gt;
16-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA2560"/>
</gates>
<devices>
<device name="A" package="TQFP100">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="55"/>
<connect gate="G$1" pin="(A11)PC3" pad="56"/>
<connect gate="G$1" pin="(A12)PC4" pad="57"/>
<connect gate="G$1" pin="(A13)PC5" pad="58"/>
<connect gate="G$1" pin="(A14)PC6" pad="59"/>
<connect gate="G$1" pin="(A15)PC7" pad="60"/>
<connect gate="G$1" pin="(A8)PC0" pad="53"/>
<connect gate="G$1" pin="(A9)PC1" pad="54"/>
<connect gate="G$1" pin="(AD0)PA0" pad="78"/>
<connect gate="G$1" pin="(AD1)PA1" pad="77"/>
<connect gate="G$1" pin="(AD2)PA2" pad="76"/>
<connect gate="G$1" pin="(AD3)PA3" pad="75"/>
<connect gate="G$1" pin="(AD4)PA4" pad="74"/>
<connect gate="G$1" pin="(AD5)PA5" pad="73"/>
<connect gate="G$1" pin="(AD6)PA6" pad="72"/>
<connect gate="G$1" pin="(AD7)PA7" pad="71"/>
<connect gate="G$1" pin="(ADC0)PF0" pad="97"/>
<connect gate="G$1" pin="(ADC1)PF1" pad="96"/>
<connect gate="G$1" pin="(ADC2)PF2" pad="95"/>
<connect gate="G$1" pin="(ADC3)PF3" pad="94"/>
<connect gate="G$1" pin="(CLKO/ICP2/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="47"/>
<connect gate="G$1" pin="(MISO/PCINT3)PB3" pad="22"/>
<connect gate="G$1" pin="(MOSI/PCINT2)PB2" pad="21"/>
<connect gate="G$1" pin="(OC0A/OC1C/PCINT7)PB7" pad="26"/>
<connect gate="G$1" pin="(OC1A/PCINT5)PB5" pad="24"/>
<connect gate="G$1" pin="(OC1B/PCINT6)PB6" pad="25"/>
<connect gate="G$1" pin="(OC2A/PCINT4)PB4" pad="23"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(PCINT16/ADC8)PK0" pad="89"/>
<connect gate="G$1" pin="(PCINT17/ADC9)PK1" pad="88"/>
<connect gate="G$1" pin="(PCINT18/ADC10)PK2" pad="87"/>
<connect gate="G$1" pin="(PCINT19/ADC11)PK3" pad="86"/>
<connect gate="G$1" pin="(PCINT20/ADC12)PK4" pad="85"/>
<connect gate="G$1" pin="(PCINT21/ADC13)PK5" pad="84"/>
<connect gate="G$1" pin="(PCINT22/ADC14)PK6" pad="83"/>
<connect gate="G$1" pin="(PCINT23/ADC15)PK7" pad="82"/>
<connect gate="G$1" pin="(RXD0/PCINT8)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="45"/>
<connect gate="G$1" pin="(SCK/PCINT1)PB1" pad="20"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="43"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="44"/>
<connect gate="G$1" pin="(SS/PCINT0)PB0" pad="19"/>
<connect gate="G$1" pin="(T0)PD7" pad="50"/>
<connect gate="G$1" pin="(T1)PD6" pad="49"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TCK/ADC4)PF4" pad="93"/>
<connect gate="G$1" pin="(TDI/ADC7)PF7" pad="90"/>
<connect gate="G$1" pin="(TDO/ADC6)PF6" pad="91"/>
<connect gate="G$1" pin="(TMS/ADC5)PF5" pad="92"/>
<connect gate="G$1" pin="(TXD0)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="46"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="48"/>
<connect gate="G$1" pin="AGND" pad="99"/>
<connect gate="G$1" pin="AREF" pad="98"/>
<connect gate="G$1" pin="AVCC" pad="100"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="32"/>
<connect gate="G$1" pin="GND@3" pad="62"/>
<connect gate="G$1" pin="GND@4" pad="81"/>
<connect gate="G$1" pin="PG0(WR)" pad="51"/>
<connect gate="G$1" pin="PG1(RD)" pad="52"/>
<connect gate="G$1" pin="PG2(ALE)" pad="70"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="28"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="29"/>
<connect gate="G$1" pin="PG5(OC0B)" pad="1"/>
<connect gate="G$1" pin="PH0(RXD2)" pad="12"/>
<connect gate="G$1" pin="PH1(TXD2)" pad="13"/>
<connect gate="G$1" pin="PH2(XCK2)" pad="14"/>
<connect gate="G$1" pin="PH3(OC4A)" pad="15"/>
<connect gate="G$1" pin="PH4(OC4B)" pad="16"/>
<connect gate="G$1" pin="PH5(OC4C)" pad="17"/>
<connect gate="G$1" pin="PH6(OC2B)" pad="18"/>
<connect gate="G$1" pin="PH7(T4)" pad="27"/>
<connect gate="G$1" pin="PJ0(PCINT9/RXD3)" pad="63"/>
<connect gate="G$1" pin="PJ1(PCINT10/TXD3)" pad="64"/>
<connect gate="G$1" pin="PJ2((PCINT11/XCK3)" pad="65"/>
<connect gate="G$1" pin="PJ3(PCINT12" pad="66"/>
<connect gate="G$1" pin="PJ4(PCINT13)" pad="67"/>
<connect gate="G$1" pin="PJ5(PCINT14)" pad="68"/>
<connect gate="G$1" pin="PJ6(PCINT15)" pad="69"/>
<connect gate="G$1" pin="PJ7" pad="79"/>
<connect gate="G$1" pin="PL0(ICP4)" pad="35"/>
<connect gate="G$1" pin="PL1(ICP5)" pad="36"/>
<connect gate="G$1" pin="PL2(T5)" pad="37"/>
<connect gate="G$1" pin="PL3(PC5A)" pad="38"/>
<connect gate="G$1" pin="PL4(OC5B)" pad="39"/>
<connect gate="G$1" pin="PL5(OC5C)" pad="40"/>
<connect gate="G$1" pin="PL6" pad="41"/>
<connect gate="G$1" pin="PL7" pad="42"/>
<connect gate="G$1" pin="RESET" pad="30"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="31"/>
<connect gate="G$1" pin="VCC@3" pad="61"/>
<connect gate="G$1" pin="VCC@4" pad="80"/>
<connect gate="G$1" pin="XTAL1" pad="34"/>
<connect gate="G$1" pin="XTAL2" pad="33"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA1281" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 Kbytes FLASH&lt;p&gt;
8 Kbytes SRAM&lt;p&gt;
4 Kbytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA1281"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="29"/>
<connect gate="G$1" pin="(ICP3/CLKO/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO/PCI3)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCI2)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/OC1C/PCI7)PB7" pad="17"/>
<connect gate="G$1" pin="(OC1A/PCI5)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCI6)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCI4)PB4" pad="14"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD0/PDI/PCI8)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK/PCI1)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS/PCI0)PB0" pad="10"/>
<connect gate="G$1" pin="(T0)PD7" pad="32"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD0/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="PG5(OC0B)" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="29"/>
<connect gate="G$1" pin="(ICP3/CLKO/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO/PCI3)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCI2)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/OC1C/PCI7)PB7" pad="17"/>
<connect gate="G$1" pin="(OC1A/PCI5)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCI6)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCI4)PB4" pad="14"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD0/PDI/PCI8)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK/PCI1)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS/PCI0)PB0" pad="10"/>
<connect gate="G$1" pin="(T0)PD7" pad="32"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD0/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="PG5(OC0B)" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA2561" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
256 Kbytes FLASH&lt;p&gt;
8 Kbytes SRAM&lt;p&gt;
4 Kbytes EEPROM&lt;p&gt;
DUAL USART&lt;p&gt;
8-channel 10 bit ADC&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="MEGA1281"/>
</gates>
<devices>
<device name="A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="29"/>
<connect gate="G$1" pin="(ICP3/CLKO/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO/PCI3)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCI2)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/OC1C/PCI7)PB7" pad="17"/>
<connect gate="G$1" pin="(OC1A/PCI5)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCI6)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCI4)PB4" pad="14"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD0/PDI/PCI8)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK/PCI1)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS/PCI0)PB0" pad="10"/>
<connect gate="G$1" pin="(T0)PD7" pad="32"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD0/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="PG5(OC0B)" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
<device name="M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(ICP1)PD4" pad="29"/>
<connect gate="G$1" pin="(ICP3/CLKO/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO/PCI3)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCI2)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/OC1C/PCI7)PB7" pad="17"/>
<connect gate="G$1" pin="(OC1A/PCI5)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCI6)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCI4)PB4" pad="14"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD0/PDI/PCI8)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK/PCI1)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS/PCI0)PB0" pad="10"/>
<connect gate="G$1" pin="(T0)PD7" pad="32"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD0/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND@1" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="PG5(OC0B)" pad="1"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC@1" pad="21"/>
<connect gate="G$1" pin="VCC@2" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="-16"/>
<technology name="V-8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA406" prefix="IC">
<gates>
<gate name="G$1" symbol="MEGA406"/>
</gates>
<devices>
<device name="AAU" package="TQFP48">
<connects>
<connect gate="G$1" pin="(ADC0/PCI0)PA0" pad="2"/>
<connect gate="G$1" pin="(ADC1/PCI1)PA1" pad="3"/>
<connect gate="G$1" pin="(ADC2/PCI2)PA2" pad="4"/>
<connect gate="G$1" pin="(ADC3/PCI3)PA3" pad="5"/>
<connect gate="G$1" pin="(ADC4/INT0/PCI4)PA4" pad="9"/>
<connect gate="G$1" pin="(INT1/PCI5)PA5" pad="10"/>
<connect gate="G$1" pin="(INT2/PCI6)PA6" pad="11"/>
<connect gate="G$1" pin="(INT3/PCI7)PA7" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT14)PB6" pad="25"/>
<connect gate="G$1" pin="(OC0B/PCINT15)PB7" pad="26"/>
<connect gate="G$1" pin="(PCINT12)PB4" pad="21"/>
<connect gate="G$1" pin="(PCINT13)PB5" pad="22"/>
<connect gate="G$1" pin="(T0)PD0" pad="27"/>
<connect gate="G$1" pin="(TCK/PCINT11)PB3" pad="20"/>
<connect gate="G$1" pin="(TDI/PCINT9)PB1" pad="18"/>
<connect gate="G$1" pin="(TDO/PCINT8)PB0" pad="17"/>
<connect gate="G$1" pin="(TMS/PCINT10)PB2" pad="19"/>
<connect gate="G$1" pin="BATT" pad="31"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="16"/>
<connect gate="G$1" pin="GND@3" pad="29"/>
<connect gate="G$1" pin="GND@4" pad="37"/>
<connect gate="G$1" pin="NI" pad="47"/>
<connect gate="G$1" pin="NNI" pad="48"/>
<connect gate="G$1" pin="NV" pad="42"/>
<connect gate="G$1" pin="OC" pad="33"/>
<connect gate="G$1" pin="OD" pad="35"/>
<connect gate="G$1" pin="OPC" pad="32"/>
<connect gate="G$1" pin="PC0" pad="30"/>
<connect gate="G$1" pin="PD1" pad="28"/>
<connect gate="G$1" pin="PI" pad="46"/>
<connect gate="G$1" pin="PPI" pad="45"/>
<connect gate="G$1" pin="PV1" pad="41"/>
<connect gate="G$1" pin="PV2" pad="40"/>
<connect gate="G$1" pin="PV3" pad="39"/>
<connect gate="G$1" pin="PV4" pad="38"/>
<connect gate="G$1" pin="PVT" pad="36"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="G$1" pin="SCL" pad="23"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="SGND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFET" pad="34"/>
<connect gate="G$1" pin="VREF" pad="43"/>
<connect gate="G$1" pin="VREFGND" pad="44"/>
<connect gate="G$1" pin="VREG" pad="6"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="15"/>
</connects>
<technologies>
<technology name="-1"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
