{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["iob16avrs"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"iob16avrs","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"flags":["formulas_cached_only"]}
["Qty","Value","Device","Package","Parts","Description"]
[1,null,"F25HS","F25H","LPT","SUB-D"]
[1,null,"HF15H","HDF15H","VGA","SUB-D"]
[2,null,"JP1E","JP1","CPREQ, HS2","JUMPER"]
[1,null,"JP2E","JP2","J3","JUMPER"]
[1,null,"MA03-2","MA03-2","JTAG","PIN HEADER"]
[2,null,"MA13-2","MA13-2","IO1, IO2","PIN HEADER"]
[1,null,"MINI_DIN_6","M_DIN6","KBD"]
[3,null,"ML10","ML10","SER1, SER2, SER3","HARTING"]
[4,"0.1uF","C-USC1206","C1206","C11, C12, C15, C16","CAPACITOR, American symbol"]
[19,"0u1","C-USC0805","C0805","C3, C4, C5, C6, C7, C8, C9, C10, C13, C14, C17, C100, C101, C102, C103, C104, C105, C106, C107","CAPACITOR, American symbol"]
[1,"100ohm","R-US_M1206","M1206","R4","RESISTOR, American symbol"]
[4,"10K","R-US_M0805","M0805","R1, R2, R3, R7","RESISTOR, American symbol"]
[1,"10K","R-US_R0805","R0805","R5","RESISTOR, American symbol"]
[2,"10u","CPOL-USD/7343-31W","D/7343-31W","C1, C2","POLARIZED CAPACITOR, American symbol"]
[1,"2550-","2550-","PAK100/2500-50","SBC","3M (TM) Pak 100 4-Wall Header"]
[1,"28F400E","AM29F400E","TSOP48","IC1","4-Megabit FLASH MEMORY"]
[1,"29.4912MHz","OSC-OE-5V","SG636","X1"]
[1,0,"CRYSTALTC26H","TC26H","X2","CRYSTAL"]
[2,"470ohm","R-US_M0805","M0805","R8, R11","RESISTOR, American symbol"]
[3,"4K7","R-US_M0805","M0805","R6, R9, R10","RESISTOR, American symbol"]
[4,0,"TC554001AF","SOP32","IC2, IC3, IC4, IC5"]
[1,"74ACT04D","74ALS04D","SO14","IC17","Hex INVERTER"]
[1,"74ACT05D","74ALS05D","SO14","IC15","Hex INVERTER, open collector"]
[2,"74ACT245DW","74LS245DW","SO20W","IC9, IC13","Octal BUS TRANSCEIVER, 3-state"]
[1,"74ACT32D","74LS32D","SO14","IC10","Quad 2-input OR gate"]
[1,"74ACT373DW","74LS373DW","SO20W","IC8","Octal D type transparent LATCH, edge triggered"]
[1,"74AHC138D","74LS138D","SO16","IC6","3-line to 8-line DECODER/DEMULTIPLEXER"]
[1,"74HC367D","74HCT367D","SO16","IC7","Hex BUS DRIVER, 3-state"]
[1,"CF_CMM_SOCKET2","CF_CMM_SOCKET2","CF_SOCKET2_SMT","CF1"]
[2,"CR2032","CR2032HOLDER","CR2032HOLDER","BATA, BATB"]
[1,"DS1302","DS1302","SO08","IC16"]
[1,"DS1321D","DS1321D","SO16","IC14","DS1321 Battery Monitor"]
[1,"KSS1201","KSS1201","KSS1201","SPKR","SPEAKER"]
[1,"MAX208ECWG","MAX208ECWG","SO24L","IC11","RS232 TRANSCEIVER"]
[1,"RN2","RN-4-SMT","RN-CTS-744C043","RN2","4 resistor package"]
[1,"TPS77725D","TPS77XXXD","SO08","REG2.5"]
[1,"TPS77733D","TPS77XXXD","SO08","REG3.3"]
[1,"XC2S100-5TQ144C","XC2S30-IOB1-5TQ144","TQFP144","IC12"]