<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="-0.63" y1="-0.47" x2="159.37" y2="-0.47" width="0" layer="20"/>
<wire x1="159.37" y1="-0.47" x2="159.37" y2="99.53" width="0" layer="20"/>
<wire x1="159.37" y1="99.53" x2="-0.63" y2="99.53" width="0" layer="20"/>
<wire x1="-0.63" y1="99.53" x2="-0.63" y2="-0.47" width="0" layer="20"/>
</plain>
<libraries>
<library name="74xx-us">
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pal">
<packages>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="dec-con">
<packages>
<package name="OMNIBUS">
<description>Quad-Height DEC board</description>
</package>
<package name="EDGE-CON8">
<description>Quad-Height DEC edge connector</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="A20" library="74xx-us" package="DIL14" value="7430N"/>
<element name="A49" library="74xx-us" package="DIL14" value="7400N"/>
<element name="A47" library="74xx-us" package="DIL14" value="7404N"/>
<element name="A25" library="74xx-us" package="DIL14" value="7402N"/>
<element name="A28" library="74xx-us" package="DIL14" value="7402N"/>
<element name="A26" library="74xx-us" package="DIL14" value="7404N"/>
<element name="A21" library="74xx-us" package="DIL14" value="7430N"/>
<element name="A59" library="74xx-us" package="DIL14" value="74LS74N"/>
<element name="A60" library="74xx-us" package="DIL14" value="7400N"/>
<element name="IC1" library="pal" package="DIL24-3" value="">
<attribute name="MF"/>
<attribute name="MPN" value="GAL22V10D-7LPN"/>
<attribute name="OC_FARNELL" value="1571925"/>
<attribute name="OC_NEWARK" value="97M0480"/>
</element>
<element name="IC2" library="pal" package="DIL24-3" value="">
<attribute name="MF"/>
<attribute name="MPN" value="GAL22V10D-7LPN"/>
<attribute name="OC_NEWARK" value="97M0480"/>
<attribute name="OC_FARNELL" value="1571925"/>
</element>
<element name="U$1" library="dec-con" package="OMNIBUS" value="OUTLINE-OMNIBUS"/>
<element name="U$2" library="dec-con" package="EDGE-CON8" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="A20" pad="7"/>
<contactref element="A49" pad="7"/>
<contactref element="A47" pad="7"/>
<contactref element="A25" pad="7"/>
<contactref element="A28" pad="7"/>
<contactref element="A26" pad="7"/>
<contactref element="A21" pad="7"/>
<contactref element="A59" pad="7"/>
<contactref element="A60" pad="7"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
<contactref element="U$2" pad="AN1"/>
<contactref element="U$2" pad="AT1"/>
<contactref element="U$2" pad="AF1"/>
<contactref element="U$2" pad="BT1"/>
<contactref element="U$2" pad="BN1"/>
<contactref element="U$2" pad="AT2"/>
<contactref element="U$2" pad="AN2"/>
<contactref element="U$2" pad="AF2"/>
<contactref element="U$2" pad="AC2"/>
<contactref element="U$2" pad="BN2"/>
<contactref element="U$2" pad="CC1"/>
<contactref element="U$2" pad="DT1"/>
<contactref element="U$2" pad="DN1"/>
<contactref element="U$2" pad="DF1"/>
<contactref element="U$2" pad="DC1"/>
<contactref element="U$2" pad="CC2"/>
<contactref element="U$2" pad="DT2"/>
<contactref element="U$2" pad="DN2"/>
<contactref element="U$2" pad="DF2"/>
<contactref element="U$2" pad="DC2"/>
<contactref element="U$2" pad="BF2"/>
<contactref element="U$2" pad="BC2"/>
<contactref element="U$2" pad="CT2"/>
<contactref element="U$2" pad="CN2"/>
<contactref element="U$2" pad="CF2"/>
<contactref element="U$2" pad="BF1"/>
<contactref element="U$2" pad="BC1"/>
<contactref element="U$2" pad="CT1"/>
<contactref element="U$2" pad="CN1"/>
</signal>
<signal name="VCC">
<contactref element="A20" pad="14"/>
<contactref element="A49" pad="14"/>
<contactref element="A47" pad="14"/>
<contactref element="A25" pad="14"/>
<contactref element="A28" pad="14"/>
<contactref element="A26" pad="14"/>
<contactref element="A21" pad="14"/>
<contactref element="A59" pad="14"/>
<contactref element="A60" pad="14"/>
<contactref element="A59" pad="10"/>
<contactref element="IC1" pad="24"/>
<contactref element="IC2" pad="24"/>
<contactref element="U$2" pad="CA2"/>
<contactref element="U$2" pad="BA2"/>
<contactref element="U$2" pad="AA2"/>
</signal>
<signal name="DEP">
<contactref element="A20" pad="12"/>
<contactref element="A20" pad="1"/>
<contactref element="A20" pad="6"/>
<contactref element="A20" pad="11"/>
</signal>
<signal name="ISZ">
<contactref element="A20" pad="5"/>
</signal>
<signal name="JMS">
<contactref element="A20" pad="3"/>
</signal>
<signal name="DCA">
<contactref element="A20" pad="2"/>
</signal>
<signal name="LDM">
<contactref element="A20" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="A49" pad="10"/>
<contactref element="A20" pad="8"/>
<contactref element="A25" pad="12"/>
</signal>
<signal name="CP1H">
<contactref element="A49" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="A47" pad="12"/>
<contactref element="A25" pad="11"/>
</signal>
<signal name="LDMB">
<contactref element="A47" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="A49" pad="13"/>
<contactref element="A49" pad="8"/>
</signal>
<signal name="F7">
<contactref element="A49" pad="12"/>
<contactref element="A21" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="A28" pad="8"/>
<contactref element="A25" pad="13"/>
</signal>
<signal name="CPO">
<contactref element="A28" pad="9"/>
</signal>
<signal name="WRITE">
<contactref element="A49" pad="11"/>
</signal>
<signal name="N$5">
<contactref element="A28" pad="10"/>
<contactref element="A26" pad="9"/>
</signal>
<signal name="F10">
<contactref element="A21" pad="12"/>
<contactref element="A21" pad="5"/>
<contactref element="A21" pad="6"/>
<contactref element="A21" pad="11"/>
</signal>
<signal name="N$6">
<contactref element="A26" pad="8"/>
<contactref element="A21" pad="4"/>
</signal>
<signal name="F5">
<contactref element="A21" pad="2"/>
</signal>
<signal name="F0">
<contactref element="A21" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="A59" pad="12"/>
<contactref element="A21" pad="8"/>
</signal>
<signal name="CLK">
<contactref element="A59" pad="11"/>
<contactref element="A60" pad="9"/>
</signal>
<signal name="N$8">
<contactref element="A60" pad="8"/>
<contactref element="A59" pad="13"/>
</signal>
<signal name="MBL">
<contactref element="A59" pad="9"/>
<contactref element="A60" pad="10"/>
</signal>
<signal name="DATA_ENAB">
<contactref element="U$2" pad="AB1"/>
</signal>
<signal name="!DATA10">
<contactref element="U$2" pad="DU1"/>
</signal>
<signal name="!DATA00">
<contactref element="U$2" pad="AR1"/>
</signal>
<signal name="!DATA01">
<contactref element="U$2" pad="AS1"/>
</signal>
<signal name="!DATA02">
<contactref element="U$2" pad="AU1"/>
</signal>
<signal name="!DATA03">
<contactref element="U$2" pad="AV1"/>
</signal>
<signal name="!DATA04">
<contactref element="U$2" pad="BR1"/>
</signal>
<signal name="!DATA05">
<contactref element="U$2" pad="BS1"/>
</signal>
<signal name="!DATA06">
<contactref element="U$2" pad="BU1"/>
</signal>
<signal name="!DATA07">
<contactref element="U$2" pad="BV1"/>
</signal>
<signal name="!DATA08">
<contactref element="U$2" pad="DR1"/>
</signal>
<signal name="!DATA09">
<contactref element="U$2" pad="DS1"/>
</signal>
<signal name="!DATA11">
<contactref element="U$2" pad="DV1"/>
</signal>
<signal name="-15V">
<contactref element="U$2" pad="DB2"/>
</signal>
<signal name="!MEM_START">
<contactref element="U$2" pad="AJ2"/>
</signal>
<signal name="!LA_ENABLE">
<contactref element="U$2" pad="BM2"/>
</signal>
<signal name="!RUN">
<contactref element="U$2" pad="BU2"/>
</signal>
<signal name="!POWER_OK">
<contactref element="U$2" pad="BV2"/>
</signal>
<signal name="!START_ADD">
<contactref element="U$2" pad="CB1"/>
</signal>
<signal name="TP4">
<contactref element="U$2" pad="CJ2"/>
</signal>
<signal name="!TS1">
<contactref element="U$2" pad="CK2"/>
</signal>
<signal name="!TS3">
<contactref element="U$2" pad="CM2"/>
</signal>
<signal name="INITIALIZE">
<contactref element="U$2" pad="CR1"/>
</signal>
<signal name="!MSIR_DISABLE">
<contactref element="U$2" pad="CV1"/>
</signal>
<signal name="!INIT_ADD">
<contactref element="U$2" pad="DA1"/>
</signal>
<signal name="PULSE_LA">
<contactref element="U$2" pad="DR2"/>
</signal>
<signal name="!STOP">
<contactref element="U$2" pad="DS2"/>
</signal>
<signal name="!KEY_CONTROL">
<contactref element="U$2" pad="DU2"/>
</signal>
<signal name="SW">
<contactref element="U$2" pad="DV2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
