<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>12 N24</text>
<text>12 N24</text>
<text>12 N24</text>
<text>8i H05</text>
<text>8i H05</text>
<text>8i H05</text>
<text>R1, R2 are needed if cabling was used.</text>
</plain>
<libraries>
<library name="con-ml">
<packages>
<package name="ML50L">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-us">
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="EDGE-CON1">
<description>Single-sided Edge Connector</description>
</package>
<package name="SINGLE">
<description>Single-Height DEC board</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E5" library="74xx-us" package="DIL14" value="74LS00N"/>
<element name="H05" library="dec-con" package="EDGE-CON1" value=" "/>
<element name="C5" library="rcl" package="C050-025X075" value="0.1uF"/>
<element name="C4" library="rcl" package="C050-025X075" value="0.1uF"/>
<element name="C2" library="rcl" package="C050-025X075" value="0.1uF"/>
<element name="SV5" library="con-ml" package="ML50L" value=" ">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C6" library="rcl" package="C050-025X075" value="0.1uF"/>
<element name="C3" library="rcl" package="C050-025X075" value="0.1uF"/>
<element name="E4" library="dec-con" package="DIL14" value="7438N"/>
<element name="R1" library="rcl" package="0207/10" value="100"/>
<element name="R2" library="rcl" package="0207/10" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="SparkFun-Hardware" package="STAND-OFF" value=""/>
<element name="U$8" library="SparkFun-Hardware" package="STAND-OFF" value=""/>
<element name="U$16" library="SparkFun-Hardware" package="STAND-OFF" value=""/>
<element name="E3" library="74xx-us" package="DIL16" value="74HCT123N"/>
<element name="E2" library="74xx-us" package="DIL16" value="74HCT123N"/>
<element name="E1" library="74xx-us" package="DIL16" value="74HCT123N"/>
<element name="R4" library="rcl" package="0207/10" value="2K"/>
<element name="C17" library="rcl" package="C050-025X075" value="470pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="0207/10" value="2K"/>
<element name="C18" library="rcl" package="C050-025X075" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="0207/10" value="2K"/>
<element name="C19" library="rcl" package="C050-025X075" value="180pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="0207/10" value="1.5K"/>
<element name="C20" library="rcl" package="C050-025X075" value="470pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="0207/10" value="2K"/>
<element name="C21" library="rcl" package="C050-025X075" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="0207/10" value="2K"/>
<element name="C22" library="rcl" package="C050-025X075" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="dec-con" package="SINGLE" value="OUTLINE-SINGLE"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="E5" pad="14"/>
<contactref element="C5" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="E4" pad="14"/>
<contactref element="SV5" pad="49"/>
<contactref element="SV5" pad="50"/>
<contactref element="E3" pad="16"/>
<contactref element="E2" pad="16"/>
<contactref element="E1" pad="16"/>
<contactref element="R4" pad="1"/>
<contactref element="E3" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="E1" pad="11"/>
<contactref element="E1" pad="3"/>
<contactref element="E3" pad="11"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="E2" pad="3"/>
<contactref element="E2" pad="11"/>
<contactref element="E3" pad="2"/>
<contactref element="E3" pad="10"/>
<contactref element="E1" pad="2"/>
<contactref element="E1" pad="10"/>
<contactref element="E2" pad="10"/>
<contactref element="E2" pad="2"/>
<contactref element="E4" pad="1"/>
<contactref element="E4" pad="2"/>
<contactref element="E4" pad="4"/>
<contactref element="E4" pad="5"/>
</signal>
<signal name="GND">
<contactref element="E5" pad="7"/>
<contactref element="H05" pad="C2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="SV5" pad="1"/>
<contactref element="SV5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="E4" pad="7"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="E3" pad="8"/>
<contactref element="E2" pad="8"/>
<contactref element="E1" pad="8"/>
</signal>
<signal name="MEM08">
<contactref element="H05" pad="D2"/>
<contactref element="SV5" pad="41"/>
</signal>
<signal name="MEM10">
<contactref element="H05" pad="H2"/>
<contactref element="SV5" pad="40"/>
</signal>
<signal name="MEMSTART(0)">
<contactref element="E5" pad="6"/>
<contactref element="E3" pad="1"/>
<contactref element="E3" pad="9"/>
</signal>
<signal name="MEMSTART(1)">
<contactref element="E5" pad="5"/>
<contactref element="H05" pad="M2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="MEMDONE(1)">
<contactref element="E4" pad="13"/>
<contactref element="E4" pad="12"/>
<contactref element="E2" pad="5"/>
</signal>
<signal name="BTP2(1)">
<contactref element="H05" pad="V2"/>
<contactref element="E5" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="MEM09">
<contactref element="H05" pad="E2"/>
<contactref element="SV5" pad="39"/>
</signal>
<signal name="MEM11">
<contactref element="H05" pad="K2"/>
<contactref element="SV5" pad="37"/>
</signal>
<signal name="STROBE(0)">
<contactref element="H05" pad="P2"/>
<contactref element="E4" pad="8"/>
</signal>
<signal name="MBODD_P">
<contactref element="H05" pad="T2"/>
<contactref element="SV5" pad="42"/>
</signal>
<signal name="OE(0)">
<contactref element="SV5" pad="22"/>
<contactref element="E3" pad="4"/>
<contactref element="E5" pad="10"/>
</signal>
<signal name="CS(0)">
<contactref element="SV5" pad="18"/>
<contactref element="E5" pad="11"/>
</signal>
<signal name="WE(0)">
<contactref element="SV5" pad="32"/>
<contactref element="E1" pad="4"/>
<contactref element="E5" pad="9"/>
</signal>
<signal name="FS(1)">
<contactref element="SV5" pad="34"/>
<contactref element="E5" pad="4"/>
<contactref element="E5" pad="2"/>
</signal>
<signal name="BTP2(0)">
<contactref element="E5" pad="3"/>
<contactref element="E1" pad="1"/>
<contactref element="E1" pad="9"/>
</signal>
<signal name="MEMDONE(0)">
<contactref element="E4" pad="11"/>
<contactref element="H05" pad="S2"/>
</signal>
<signal name="STROBE(1)">
<contactref element="E4" pad="10"/>
<contactref element="E4" pad="9"/>
<contactref element="E2" pad="13"/>
</signal>
<signal name="SDELAY">
<contactref element="E3" pad="5"/>
<contactref element="E2" pad="1"/>
</signal>
<signal name="DDELAY">
<contactref element="E1" pad="5"/>
<contactref element="E2" pad="9"/>
</signal>
<signal name="CS(1)">
<contactref element="E5" pad="8"/>
<contactref element="E5" pad="12"/>
<contactref element="E5" pad="13"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="E3" pad="15"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="E3" pad="14"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="E3" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="C18" pad="2"/>
<contactref element="E3" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="E1" pad="15"/>
</signal>
<signal name="N$10">
<contactref element="C19" pad="2"/>
<contactref element="E1" pad="14"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="E1" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="C20" pad="2"/>
<contactref element="E1" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="E2" pad="15"/>
</signal>
<signal name="N$14">
<contactref element="C21" pad="2"/>
<contactref element="E2" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="R9" pad="2"/>
<contactref element="C22" pad="1"/>
<contactref element="E2" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="C22" pad="2"/>
<contactref element="E2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
