{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet1","TD8Edaughter"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":40,"n_cols":12,"rows_kept":40,"flags":["formulas_cached_only"]}
["Parts","Device","Package","Description","Qty","Value","Order","Qty","Mouser #"]
["C3, C4, C5, C41, C44, C47, C48","C-US050-025X075","C050-025X075","CAPACITOR, American symbol",7,".01uF",0,0]
["C1, C2","C-US050-025X075","C050-025X075","CAPACITOR, American symbol",2,".22uF",0,0,"594-K224K20X7RF53H5"]
["R35","R-US_0207/15","0207/15","RESISTOR, American symbol",1,"1.21K 1%",1,15,"660-MF1/4DCT52R1211F "]
["R27, R29, R37, R39, R44","R-US_0207/10","0207/10","RESISTOR, American symbol",5,"1.5K",4,60,"603-CFR-25JR-52-1K5"]
["R24","R-US_0207/10","0207/10","RESISTOR, American symbol",1,"10K",0,0,"71-CCF0710K0JKE36"]
["R9","R-US_0207/10","0207/10","RESISTOR, American symbol",1,"120 ohm",1,15,"603-CFR-25JR-52-120R"]
["R1, R2, R3, R4, R5, R6, R7, R8","R-US_0207/10","0207/10","RESISTOR, American symbol",8,"180 ohm",8,120,"71-CCF07180RGKE36"]
["R30, R31, R32, R33, R34, R38, R40, R42, R45","R-US_0207/10","0207/10","RESISTOR, American symbol",9,"1K",7,105,"71-CCF071K00GKE36 "]
["D2, D3, D4, D6","1N4148DO35-10","DO35-10","DIODE",4,"1N4154",4,60,"78-1N4154-TAP ","0.88V","833-1N914B-TP ",".72V"]
["D1, D5, D7, D8, D9, D10","1N4148DO35-10","DO35-10","DIODE",6,"1N4148",6,90,"78-1N4150-TAP",".55V"]
["R46","275P","3006Y","Trimpot with 275P (3006Y) footprint.",1,"20K",0,0,"Use R46A"]
["R46A","R-TRIMM3006P","RTRIM3006P","Trimm resistor",1,"20K",1,15,"652-3006P-1-203-LF"]
["R28","R-US_0207/10","0207/10","RESISTOR, American symbol",1,"220 ohm",0,0,"71-CCF07220RJKE36 "]
["R18, R19, R20, R21, R23","R-US_0207/10","0207/10","RESISTOR, American symbol",5,"270 ohm",5,75,"71-CCF07270RGKE36"]
["C37, C39","C-US102-043X133","C102-043X133","CAPACITOR, American symbol",2,"2700pF",2,30,"871-B32671L1272J"]
["C38","C-US050-025X075","C050-025X075","CAPACITOR, American symbol",1,"27pF",1,15,"140-100N5-270J-RC"]
["R10, R11, R12, R13, R14, R15, R16, R17","R-US_0207/10","0207/10","RESISTOR, American symbol",8,"390 ohm",7,105,"603-CFR-25JR-52390R"]
["R41","R-US_0207/10","0207/10","RESISTOR, American symbol",1,"3K",1,15,"71-CCF073K00GKE36"]
["R25, R43","R-US_0207/10","0207/10","RESISTOR, American symbol",2,"4.7K",1,15,"71-CCF07-J-4.7K-E3"]
["R48","R-US_0207/10","0207/10","RESISTOR, American symbol",1,"470 ohm",0,0,"71-CCF07470RGKE36"]
["R26","R-US_0207/10","0207/10","RESISTOR, American symbol",1,"51K",1,15,"71-CCF0751K0GKE36"]
["C40","C-US075-032X103","C075-032X103","CAPACITOR, American symbol",1,"560pF",1,15,"594-D561K20Y5PH63J5R"]
["R36","R-US_0207/15","0207/15","RESISTOR, American symbol",1,"562 1%",1,15,"660-MF1/4DCT52R5620F"]
["R22","R-US_0207/10","0207/10","RESISTOR, American symbol",1,"6.8K",0,0,"71-CCF076K80GKE36"]
["C6, C7, C36","CPOL-USE20-8AXIAL","E12-8","A 0.8 inch electrolytic.",3,"6.8uF",2,30,"80-T322D685K035"]
["E04, E08","74123N","DIL16","Retriggerable monostable MULTIVIBRATOR",2,"74123N",2,30,"595-SN74123N "]
["E1","ATF150X100PQFP","PQFP-100","ATF150x in 100 pin package.",1,"ATF150X100PQFP",1,15,"556-ATF1508AS10QU100"]
["IC1, IC2","DS75453N","DIL08","Quad 2-input OR gate, open collector output",2,"DS75453N",2,30,"595-SN75453BP"]
["Q1, Q2, Q3, Q4, Q5","MPS6534","TO5","NPN Transistor",5,"MPS6534",5,75,"610-MPS6534"]
["W2W1, W4W3","0R2","0R2/10","Bridge switch 0R 2 x 10mm",2,"0 ohm",0,0,"STOCK"]
["WTM","9070-1W","9070-1W","TOGGLE SWITCH",1,"SPDT",1,15,"633-B12AH"]
["DRIVE","DEC40PINH","DEC40PINH","PIN HEADER",1,"Drives",1,15,"517-D3432-5302-AR"]
["GND1, GND4, GND6, GND7, GND8, GND11, GND12, GND13, GND14, GND15, GND16, GND17, GND21, GND24, GND27, VCC1, VCC4, VCC6, VCC7, VCC8, VCC11, VCC12, VCC13, VCC14, VCC15, VCC16, VCC17, VCC21, VCC24, VCC27","MA01-2","JP1","JUMPER",30,null,0,0]
["CA2, etc","MA01-1","1.6/0.9","PIN HEADER",39,null,0,0]
[null,"MA01-36","MA01-36","Breakaway Pin Header",3,"100x1",3,45,"538-22-28-5363"]
["SV2, SV3","MA08-2","MA08-2","PIN HEADER",2,null,0,0]
[null,"MA36-2","MA36-2","Breakaway Pin Header",1,"16x2",1,15,"710-61307221121"]
["ISP","ML10","ML10","HARTING",1,"STOCK",0,0]
["E31","SW_DIP-8","EDG-08","DIP SWITCH",1,"SW_DIP-8",1,15,"774-2088"]

{"sheet":"TD8Edaughter","index":1,"n_rows":40,"n_cols":10,"rows_kept":40,"flags":["formulas_cached_only"]}
["Qty","Value","Device","Package","Parts","Description","MF","MPN","OC_FARNELL","OC_NEWARK"]
[2,null,"0R2","0R2/10","W2W1, W4W3","Bridge switch 0R 2 x 10mm"]
[39,null,"1,6/0,9","1,6/0,9","CA2, CB1, CB2, CC1, CC2, CD1, CE1, CF1, CF2, CH1, CH2, CJ2, CL1, CN1, CN2, CP1, CR1, CS1, CT1, CT2, DA2, DB1, DB2, DC1, DC2, DF1, DF2, DK1, DL1, DM1, DN1, DN2, DP1, DR1, DS1, DT1, DT2, DU1, DV1","THROUGH-HOLE PAD"]
[1,null,"9070-1W","9070-1W","WTM","TOGGLE SWITCH"]
[1,null,"DEC40PINH","DEC40PINH","DRIVE","PIN HEADER"]
[30,null,"JP1E","JP1","GND1, GND4, GND6, GND7, GND8, GND11, GND12, GND13, GND14, GND15, GND16, GND17, GND21, GND24, GND27, VCC1, VCC4, VCC6, VCC7, VCC8, VCC11, VCC12, VCC13, VCC14, VCC15, VCC16, VCC17, VCC21, VCC24, VCC27","JUMPER"]
[2,null,"MA08-2","MA08-2","SV2, SV3","PIN HEADER",null,null,"unknown","unknown"]
[1,null,"ML10","ML10","ISP","HARTING",null,null,"unknown","unknown"]
[1,null,"SW_DIP-8","EDG-08","E31","DIP SWITCH"]
[7,".01uF","C-US050-025X075","C050-025X075","C3, C4, C5, C41, C44, C47, C48","CAPACITOR, American symbol"]
[2,".22uF","C-US050-025X075","C050-025X075","C1, C2","CAPACITOR, American symbol"]
[1,"1.21K 1%","R-US_0207/15","0207/15","R35","RESISTOR, American symbol"]
[5,"1.5K","R-US_0207/10","0207/10","R27, R29, R37, R39, R44","RESISTOR, American symbol"]
[1,"10K","R-US_0207/10","0207/10","R24","RESISTOR, American symbol"]
[1,120,"R-US_0207/10","0207/10","R9","RESISTOR, American symbol"]
[8,180,"R-US_0207/10","0207/10","R1, R2, R3, R4, R5, R6, R7, R8","RESISTOR, American symbol"]
[9,"1K","R-US_0207/10","0207/10","R30, R31, R32, R33, R34, R38, R40, R42, R45","RESISTOR, American symbol"]
[4,"1N4148","1N4148DO35-10","DO35-10","D2, D3, D4, D6","DIODE"]
[6,"1N4154","1N4148DO35-10","DO35-10","D1, D5, D7, D8, D9, D10","DIODE"]
[1,"20K","275P","3006Y","R46","Trimpot with 275P (3006Y) footprint."]
[1,"20K","R-TRIMM3006P","RTRIM3006P","R46A","Trimm resistor"]
[1,220,"R-US_0207/10","0207/10","R28","RESISTOR, American symbol"]
[5,270,"R-US_0207/10","0207/10","R18, R19, R20, R21, R23","RESISTOR, American symbol"]
[2,"2700pF","C-US102-043X133","C102-043X133","C37, C39","CAPACITOR, American symbol"]
[1,"27pF","C-US050-025X075","C050-025X075","C38","CAPACITOR, American symbol"]
[8,390,"R-US_0207/10","0207/10","R10, R11, R12, R13, R14, R15, R16, R17","RESISTOR, American symbol"]
[1,"3K","R-US_0207/10","0207/10","R41","RESISTOR, American symbol"]
[2,"4.7K","R-US_0207/10","0207/10","R25, R43","RESISTOR, American symbol"]
[1,470,"R-US_0207/10","0207/10","R48","RESISTOR, American symbol"]
[1,"51K","R-US_0207/10","0207/10","R26","RESISTOR, American symbol"]
[1,"560pF","C-US075-032X103","C075-032X103","C40","CAPACITOR, American symbol"]
[1,"562 1%","R-US_0207/15","0207/15","R36","RESISTOR, American symbol"]
[1,"6.8K","R-US_0207/10","0207/10","R22","RESISTOR, American symbol"]
[3,"6.8uF","CPOL-USE20-8AXIAL","E12-8","C6, C7, C36","A 0.8 inch electrolytic."]
[2,"74123N","74123N","DIL16","E04, E08","Retriggerable monostable MULTIVIBRATOR"]
[1,"ATF150X100PQFP","ATF150X100PQFP","PQFP-100","E1","ATF150x in 100 pin package."]
[2,"DS75453N","DS75453N","DIL08","IC1, IC2","Quad 2-input OR gate, open collector output"]
[2,"JUMPER-NC","JUMPER-NC1","NC1","J1, J2","Normally closed SMD Jumper"]
[4,"JUMPER-NC2","JUMPER-NC2","NC2","J3, J4, J5, J6","Normally closed SMD Jumper"]
[5,"MPS6534","2N2219","TO5","Q1, Q2, Q3, Q4, Q5","NPN Transistor"]