<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<text>JTAG - ISP</text>
</plain>
<libraries>
<library name="alan_common">
<description>Alan's frequently used manually inputted parts</description>
<packages>
<package name="C_TH_5MM">
<description>CAPACITOR
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="LED_TH_3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="R_204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="HDR_2X5">
</package>
<package name="XTAL_CAN_HALFSIZE">
</package>
<package name="AMP_DB-9RA">
</package>
</packages>
</library>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="EDGE-CON8">
<description>Quad-Height DEC edge connector</description>
</package>
<package name="OMNIBUS">
<description>Quad-Height DEC board</description>
</package>
<package name="NC1">
<description>NC Jumper, circular lobes</description>
</package>
</packages>
</library>
<library name="atmel-cpld">
<description>5V CPLD w/ISP 

32 Macrocell, low power w/ISP, 5V</description>
<packages>
<package name="S84">
<description>&lt;b&gt;84 Pin PLCC Socket&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor-sil">
<description>&lt;b&gt;Resistors in Single Inline Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIL9">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-06">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="19inch">
<description>&lt;b&gt;19-Inch Slot Eurocards&lt;/b&gt;&lt;p&gt;
100 x 160 mm with DIN 41612 connectors&lt;br&gt;
 VME-BUS-Cards - http://www.interfacebus.com/COTs_Cards_VME.html&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="VG96B">
<description>&lt;b&gt;EUROCARD&lt;/b&gt;, 4 holes, C/ABC, 2.54</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="alan_common" package="LED_TH_3MM" value="LED">
<attribute name="NAME"/>
</element>
<element name="D2" library="alan_common" package="LED_TH_3MM" value="LED">
<attribute name="NAME"/>
</element>
<element name="D3" library="alan_common" package="LED_TH_3MM" value="LED">
<attribute name="NAME"/>
</element>
<element name="RN1" library="resistor-sil" package="SIL9" value="47K">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN2" library="resistor-sil" package="SIL9" value="">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="alan_common" package="R_204/7" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="alan_common" package="R_204/7" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="alan_common" package="R_204/7" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="alan_common" package="HDR_2X5" value="HDR_2X5&quot;"/>
<element name="C5" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="XO1" library="alan_common" package="XTAL_CAN_HALFSIZE" value="XTAL_CAN_HALFSIZE">
<attribute name="NAME"/>
</element>
<element name="C2" library="alan_common" package="C_TH_5MM" value="10uF">
<attribute name="NAME"/>
</element>
<element name="USB" library="alan_common" package="AMP_DB-9RA" value="DB9">
<attribute name="MANF" value="TE/AMP"/>
<attribute name="MOUSER#" value="571-1734352-1"/>
<attribute name="MANF#" value="1734352-1"/>
</element>
<element name="C1" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="U$1" library="dec-con" package="EDGE-CON8" value="QUAD"/>
<element name="U$2" library="dec-con" package="OMNIBUS" value="OUTLINE-OMNIBUS"/>
<element name="E1" library="atmel-cpld" package="S84" value="ATF150X84"/>
<element name="J1" library="dec-con" package="NC1" value="JUMPER-NC1">
<attribute name="NAME"/>
</element>
<element name="J2" library="dec-con" package="NC1" value="JUMPER-NC1">
<attribute name="NAME"/>
</element>
<element name="TX_ADDR" library="special" package="EDG-06" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RX_ADDR" library="special" package="EDG-06" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J4" library="19inch" package="VG96B" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="10"/>
<contactref element="D1" pad="K"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="XO1" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="USB" pad="G1"/>
<contactref element="USB" pad="5"/>
<contactref element="USB" pad="G2"/>
<contactref element="U$1" pad="AA1"/>
<contactref element="U$1" pad="CU2"/>
<contactref element="U$1" pad="AL2"/>
<contactref element="U$1" pad="AN2"/>
<contactref element="U$1" pad="AR2"/>
<contactref element="U$1" pad="AJ2"/>
<contactref element="U$1" pad="AF2"/>
<contactref element="U$1" pad="AC2"/>
<contactref element="U$1" pad="AU2"/>
<contactref element="U$1" pad="AK1"/>
<contactref element="U$1" pad="AN1"/>
<contactref element="U$1" pad="AR1"/>
<contactref element="U$1" pad="AT1"/>
<contactref element="U$1" pad="AU1"/>
<contactref element="U$1" pad="AV1"/>
<contactref element="U$1" pad="AF1"/>
<contactref element="U$1" pad="AC1"/>
<contactref element="U$1" pad="BV1"/>
<contactref element="U$1" pad="BU1"/>
<contactref element="U$1" pad="BT1"/>
<contactref element="U$1" pad="BR1"/>
<contactref element="U$1" pad="BN1"/>
<contactref element="U$1" pad="BK1"/>
<contactref element="U$1" pad="BF1"/>
<contactref element="U$1" pad="BC1"/>
<contactref element="U$1" pad="BA1"/>
<contactref element="U$1" pad="BU2"/>
<contactref element="U$1" pad="BR2"/>
<contactref element="U$1" pad="BN2"/>
<contactref element="U$1" pad="BL2"/>
<contactref element="U$1" pad="BJ2"/>
<contactref element="U$1" pad="BF2"/>
<contactref element="U$1" pad="BC2"/>
<contactref element="U$1" pad="CV1"/>
<contactref element="U$1" pad="CU1"/>
<contactref element="U$1" pad="CT1"/>
<contactref element="U$1" pad="CR1"/>
<contactref element="U$1" pad="CN1"/>
<contactref element="U$1" pad="CK1"/>
<contactref element="U$1" pad="CF1"/>
<contactref element="U$1" pad="CC1"/>
<contactref element="U$1" pad="CA1"/>
<contactref element="U$1" pad="CR2"/>
<contactref element="U$1" pad="CN2"/>
<contactref element="U$1" pad="CL2"/>
<contactref element="U$1" pad="CJ2"/>
<contactref element="U$1" pad="CF2"/>
<contactref element="U$1" pad="CC2"/>
<contactref element="E1" pad="7"/>
<contactref element="E1" pad="19"/>
<contactref element="E1" pad="32"/>
<contactref element="E1" pad="42"/>
<contactref element="E1" pad="47"/>
<contactref element="E1" pad="59"/>
<contactref element="E1" pad="72"/>
<contactref element="E1" pad="82"/>
<contactref element="TX_ADDR" pad="1"/>
<contactref element="TX_ADDR" pad="2"/>
<contactref element="TX_ADDR" pad="3"/>
<contactref element="TX_ADDR" pad="4"/>
<contactref element="TX_ADDR" pad="5"/>
<contactref element="TX_ADDR" pad="6"/>
<contactref element="RX_ADDR" pad="1"/>
<contactref element="RX_ADDR" pad="2"/>
<contactref element="RX_ADDR" pad="3"/>
<contactref element="RX_ADDR" pad="4"/>
<contactref element="RX_ADDR" pad="5"/>
<contactref element="RX_ADDR" pad="6"/>
</signal>
<signal name="M_TCK">
<contactref element="J3" pad="1"/>
<contactref element="E1" pad="62"/>
</signal>
<signal name="M_TMS">
<contactref element="J3" pad="5"/>
<contactref element="E1" pad="23"/>
</signal>
<signal name="M_TDI">
<contactref element="J3" pad="9"/>
<contactref element="E1" pad="14"/>
</signal>
<signal name="M_TDO">
<contactref element="J3" pad="3"/>
<contactref element="E1" pad="71"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="U3">
<contactref element="USB" pad="3"/>
<contactref element="E1" pad="8"/>
</signal>
<signal name="U2">
<contactref element="USB" pad="2"/>
<contactref element="E1" pad="12"/>
</signal>
<signal name="RX5">
<contactref element="RN1" pad="7"/>
<contactref element="E1" pad="84"/>
<contactref element="RX_ADDR" pad="7"/>
</signal>
<signal name="RX4">
<contactref element="RN1" pad="6"/>
<contactref element="E1" pad="1"/>
<contactref element="RX_ADDR" pad="8"/>
</signal>
<signal name="RX3">
<contactref element="RN1" pad="5"/>
<contactref element="E1" pad="2"/>
<contactref element="RX_ADDR" pad="9"/>
</signal>
<signal name="RX2">
<contactref element="RN1" pad="4"/>
<contactref element="E1" pad="4"/>
<contactref element="RX_ADDR" pad="10"/>
</signal>
<signal name="RX1">
<contactref element="RN1" pad="3"/>
<contactref element="E1" pad="5"/>
<contactref element="RX_ADDR" pad="11"/>
</signal>
<signal name="RX0">
<contactref element="RN1" pad="2"/>
<contactref element="E1" pad="6"/>
<contactref element="RX_ADDR" pad="12"/>
</signal>
<signal name="TX5">
<contactref element="RN2" pad="2"/>
<contactref element="E1" pad="83"/>
<contactref element="TX_ADDR" pad="7"/>
</signal>
<signal name="TX4">
<contactref element="RN2" pad="3"/>
<contactref element="E1" pad="80"/>
<contactref element="TX_ADDR" pad="8"/>
</signal>
<signal name="TX3">
<contactref element="RN2" pad="4"/>
<contactref element="E1" pad="79"/>
<contactref element="TX_ADDR" pad="9"/>
</signal>
<signal name="TX2">
<contactref element="RN2" pad="5"/>
<contactref element="E1" pad="77"/>
<contactref element="TX_ADDR" pad="10"/>
</signal>
<signal name="TX1">
<contactref element="RN2" pad="6"/>
<contactref element="E1" pad="76"/>
<contactref element="TX_ADDR" pad="11"/>
</signal>
<signal name="TX0">
<contactref element="RN2" pad="7"/>
<contactref element="E1" pad="75"/>
<contactref element="TX_ADDR" pad="12"/>
</signal>
<signal name="SYSCLK">
<contactref element="XO1" pad="5"/>
<contactref element="E1" pad="81"/>
</signal>
<signal name="LED0">
<contactref element="R1" pad="1"/>
<contactref element="E1" pad="10"/>
</signal>
<signal name="LED1">
<contactref element="R2" pad="1"/>
<contactref element="E1" pad="9"/>
</signal>
<signal name="LED2">
<contactref element="R3" pad="1"/>
<contactref element="E1" pad="11"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="AA2"/>
<contactref element="U$1" pad="BA2"/>
<contactref element="U$1" pad="CA2"/>
<contactref element="J3" pad="4"/>
<contactref element="RN1" pad="1"/>
<contactref element="RN2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="XO1" pad="8"/>
<contactref element="XO1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="-15V">
<contactref element="U$1" pad="AB2"/>
<contactref element="U$1" pad="BB2"/>
<contactref element="U$1" pad="CB2"/>
</signal>
<signal name="IOP_2">
<contactref element="U$1" pad="AM2"/>
<contactref element="E1" pad="58"/>
</signal>
<signal name="IOP_4">
<contactref element="U$1" pad="AP2"/>
<contactref element="E1" pad="56"/>
</signal>
<signal name="TS03">
<contactref element="U$1" pad="AS2"/>
<contactref element="E1" pad="55"/>
</signal>
<signal name="TS04">
<contactref element="U$1" pad="AT2"/>
<contactref element="E1" pad="52"/>
</signal>
<signal name="IOP_1">
<contactref element="U$1" pad="AK2"/>
<contactref element="E1" pad="63"/>
</signal>
<signal name="BAC_11">
<contactref element="U$1" pad="AH2"/>
<contactref element="E1" pad="64"/>
</signal>
<signal name="BAC_10">
<contactref element="U$1" pad="AE2"/>
<contactref element="E1" pad="69"/>
</signal>
<signal name="BAC_09">
<contactref element="U$1" pad="AD2"/>
<contactref element="E1" pad="70"/>
</signal>
<signal name="PWR_CLR">
<contactref element="U$1" pad="AV2"/>
<contactref element="E1" pad="51"/>
</signal>
<signal name="BAC_05">
<contactref element="U$1" pad="AL1"/>
<contactref element="E1" pad="60"/>
</signal>
<signal name="BAC_06">
<contactref element="U$1" pad="AM1"/>
<contactref element="E1" pad="61"/>
</signal>
<signal name="BAC_07">
<contactref element="U$1" pad="AP1"/>
<contactref element="E1" pad="57"/>
</signal>
<signal name="BAC_08">
<contactref element="U$1" pad="AS1"/>
<contactref element="E1" pad="54"/>
</signal>
<signal name="BAC_04">
<contactref element="U$1" pad="AJ1"/>
<contactref element="E1" pad="65"/>
</signal>
<signal name="BAC_03">
<contactref element="U$1" pad="AH1"/>
<contactref element="E1" pad="67"/>
</signal>
<signal name="BAC_02">
<contactref element="U$1" pad="AE1"/>
<contactref element="E1" pad="68"/>
</signal>
<signal name="BAC_01">
<contactref element="U$1" pad="AD1"/>
<contactref element="E1" pad="73"/>
</signal>
<signal name="BAC_00">
<contactref element="U$1" pad="AB1"/>
<contactref element="E1" pad="74"/>
</signal>
<signal name="BMB_05">
<contactref element="U$1" pad="BS1"/>
<contactref element="E1" pad="40"/>
</signal>
<signal name="!BMB_05">
<contactref element="U$1" pad="BP1"/>
</signal>
<signal name="BMB_04">
<contactref element="U$1" pad="BM1"/>
<contactref element="E1" pad="41"/>
</signal>
<signal name="!BMB_04">
<contactref element="U$1" pad="BL1"/>
</signal>
<signal name="BMB_03">
<contactref element="U$1" pad="BJ1"/>
<contactref element="E1" pad="45"/>
</signal>
<signal name="!BMB_03">
<contactref element="U$1" pad="BH1"/>
</signal>
<signal name="BMB_02">
<contactref element="U$1" pad="BE1"/>
<contactref element="E1" pad="48"/>
</signal>
<signal name="BMB_01">
<contactref element="U$1" pad="BD1"/>
<contactref element="E1" pad="49"/>
</signal>
<signal name="BMB_00">
<contactref element="U$1" pad="BB1"/>
<contactref element="E1" pad="50"/>
</signal>
<signal name="BMB_11">
<contactref element="U$1" pad="BV2"/>
<contactref element="E1" pad="35"/>
</signal>
<signal name="BMB_10">
<contactref element="U$1" pad="BT2"/>
<contactref element="E1" pad="36"/>
</signal>
<signal name="BMB_09">
<contactref element="U$1" pad="BS2"/>
<contactref element="E1" pad="37"/>
</signal>
<signal name="BMB_08">
<contactref element="U$1" pad="BP2"/>
<contactref element="E1" pad="39"/>
</signal>
<signal name="!BMB_08">
<contactref element="U$1" pad="BM2"/>
</signal>
<signal name="BMB_07">
<contactref element="U$1" pad="BK2"/>
<contactref element="E1" pad="44"/>
</signal>
<signal name="!BMB_07">
<contactref element="U$1" pad="BH2"/>
</signal>
<signal name="BMB_06">
<contactref element="U$1" pad="BE2"/>
<contactref element="E1" pad="46"/>
</signal>
<signal name="!BMB_06">
<contactref element="U$1" pad="BD2"/>
</signal>
<signal name="!IN_08">
<contactref element="U$1" pad="CS1"/>
<contactref element="E1" pad="16"/>
</signal>
<signal name="!IN_07">
<contactref element="U$1" pad="CP1"/>
<contactref element="E1" pad="18"/>
</signal>
<signal name="!IN_06">
<contactref element="U$1" pad="CM1"/>
<contactref element="E1" pad="21"/>
</signal>
<signal name="!IN_05">
<contactref element="U$1" pad="CL1"/>
<contactref element="E1" pad="22"/>
</signal>
<signal name="!IN_04">
<contactref element="U$1" pad="CJ1"/>
<contactref element="E1" pad="25"/>
</signal>
<signal name="!IN_03">
<contactref element="U$1" pad="CH1"/>
<contactref element="E1" pad="28"/>
</signal>
<signal name="!IN_02">
<contactref element="U$1" pad="CE1"/>
<contactref element="E1" pad="30"/>
</signal>
<signal name="!IN_01">
<contactref element="U$1" pad="CD1"/>
<contactref element="E1" pad="31"/>
</signal>
<signal name="!IN_00">
<contactref element="U$1" pad="CB1"/>
<contactref element="E1" pad="33"/>
</signal>
<signal name="!BRUN">
<contactref element="U$1" pad="CS2"/>
<contactref element="E1" pad="15"/>
</signal>
<signal name="!0_TO_AC">
<contactref element="U$1" pad="CP2"/>
<contactref element="E1" pad="17"/>
</signal>
<signal name="!INT_RQ">
<contactref element="U$1" pad="CM2"/>
<contactref element="E1" pad="20"/>
</signal>
<signal name="!SKP_RQ">
<contactref element="U$1" pad="CK2"/>
<contactref element="E1" pad="24"/>
</signal>
<signal name="!IN_11">
<contactref element="U$1" pad="CH2"/>
<contactref element="E1" pad="27"/>
</signal>
<signal name="!IN_10">
<contactref element="U$1" pad="CE2"/>
<contactref element="E1" pad="29"/>
</signal>
<signal name="!IN_09">
<contactref element="U$1" pad="CD2"/>
<contactref element="E1" pad="34"/>
</signal>
<signal name="VCCINT">
<contactref element="E1" pad="3"/>
<contactref element="E1" pad="43"/>
<contactref element="J2" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="VCCIO">
<contactref element="E1" pad="13"/>
<contactref element="E1" pad="26"/>
<contactref element="E1" pad="38"/>
<contactref element="E1" pad="53"/>
<contactref element="E1" pad="66"/>
<contactref element="E1" pad="78"/>
<contactref element="J1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
