<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0.005" y1="0.165" x2="276.695" y2="-0.015" width="0" layer="20"/>
<wire x1="213.345" y1="0.165" x2="213.345" y2="152.235" width="0" layer="20"/>
<wire x1="0.005" y1="152.235" x2="0.005" y2="0.165" width="0" layer="20"/>
<wire x1="215.9" y1="88.9" x2="215.9" y2="0" width="0" layer="20"/>
<wire x1="215.9" y1="88.9" x2="276.86" y2="88.9" width="0" layer="20"/>
<wire x1="276.86" y1="88.9" x2="276.86" y2="0" width="0" layer="20"/>
<wire x1="215.9" y1="111.76" x2="276.86" y2="111.76" width="0" layer="20"/>
<wire x1="215.9" y1="200.66" x2="215.9" y2="111.76" width="0" layer="20"/>
<wire x1="215.9" y1="200.66" x2="276.86" y2="200.66" width="0" layer="20"/>
<wire x1="276.86" y1="200.66" x2="0" y2="200.66" width="0" layer="20"/>
<wire x1="276.86" y1="200.66" x2="276.86" y2="130.81" width="0" layer="20"/>
<wire x1="213.36" y1="154.94" x2="0" y2="154.94" width="0" layer="20"/>
<wire x1="0" y1="157.48" x2="0" y2="200.66" width="0" layer="20"/>
<wire x1="213.36" y1="200.66" x2="213.36" y2="154.94" width="0" layer="20"/>
<text>VRS</text>
<text>RF08</text>
<text>RF08</text>
<text>VRS</text>
<text>RS08</text>
<text>RS08</text>
<text>VRS</text>
<text>VRS</text>
<text>VRS</text>
<text>VRS</text>
<text>RS08</text>
<text>RS08</text>
<text>RF08 Debug</text>
<text>RF08 Debug</text>
<text>VRS</text>
<text>VRS</text>
</plain>
<libraries>
<library name="wirepad">
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA13-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="resistor-sil">
<packages>
<package name="SIL8">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
<package name="SIL6">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pcb">
<packages>
<package name="SIERRA-PROTO">
<description>Sierra Proto -- not to exceed 85 sq".</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="holes" package="2,8" value=""/>
<element name="U$1" library="holes" package="2,8" value=""/>
<element name="U$3" library="holes" package="2,8" value=""/>
<element name="U$4" library="holes" package="2,8" value=""/>
<element name="U$5" library="holes" package="2,8" value=""/>
<element name="U$6" library="holes" package="2,8" value=""/>
<element name="U$7" library="holes" package="2,8" value=""/>
<element name="U$8" library="holes" package="2,8" value=""/>
<element name="U$9" library="holes" package="2,8" value=""/>
<element name="U$10" library="holes" package="2,8" value=""/>
<element name="U$11" library="holes" package="2,8" value=""/>
<element name="U$12" library="holes" package="2,8" value=""/>
<element name="F.3" library="led" package="LED5MM" value=""/>
<element name="F.2" library="led" package="LED5MM" value=""/>
<element name="F.1" library="led" package="LED5MM" value=""/>
<element name="DEA8" library="led" package="LED5MM" value=""/>
<element name="DEA7" library="led" package="LED5MM" value=""/>
<element name="DEA6" library="led" package="LED5MM" value=""/>
<element name="DEA5" library="led" package="LED5MM" value=""/>
<element name="DEA4" library="led" package="LED5MM" value=""/>
<element name="DEA3" library="led" package="LED5MM" value=""/>
<element name="DEA2" library="led" package="LED5MM" value=""/>
<element name="DEA1" library="led" package="LED5MM" value=""/>
<element name="DEA0" library="led" package="LED5MM" value=""/>
<element name="DMA00" library="led" package="LED5MM" value=""/>
<element name="DMA01" library="led" package="LED5MM" value=""/>
<element name="DMA02" library="led" package="LED5MM" value=""/>
<element name="DMA03" library="led" package="LED5MM" value=""/>
<element name="DMA04" library="led" package="LED5MM" value=""/>
<element name="DMA05" library="led" package="LED5MM" value=""/>
<element name="DMA06" library="led" package="LED5MM" value=""/>
<element name="DMA07" library="led" package="LED5MM" value=""/>
<element name="DMA08" library="led" package="LED5MM" value=""/>
<element name="DMA09" library="led" package="LED5MM" value=""/>
<element name="DMA10" library="led" package="LED5MM" value=""/>
<element name="DMA11" library="led" package="LED5MM" value=""/>
<element name="DMB00" library="led" package="LED5MM" value=""/>
<element name="DMB01" library="led" package="LED5MM" value=""/>
<element name="DMB02" library="led" package="LED5MM" value=""/>
<element name="DMB03" library="led" package="LED5MM" value=""/>
<element name="DMB04" library="led" package="LED5MM" value=""/>
<element name="DMB05" library="led" package="LED5MM" value=""/>
<element name="DMB06" library="led" package="LED5MM" value=""/>
<element name="DMB07" library="led" package="LED5MM" value=""/>
<element name="DMB08" library="led" package="LED5MM" value=""/>
<element name="DMB09" library="led" package="LED5MM" value=""/>
<element name="DMB10" library="led" package="LED5MM" value=""/>
<element name="DMB11" library="led" package="LED5MM" value=""/>
<element name="CIE" library="led" package="LED5MM" value=""/>
<element name="EIE" library="led" package="LED5MM" value=""/>
<element name="PIE" library="led" package="LED5MM" value=""/>
<element name="DRE" library="led" package="LED5MM" value=""/>
<element name="R/W" library="led" package="LED5MM" value=""/>
<element name="DBR" library="led" package="LED5MM" value=""/>
<element name="DRL" library="led" package="LED5MM" value=""/>
<element name="WLS" library="led" package="LED5MM" value=""/>
<element name="NXD" library="led" package="LED5MM" value=""/>
<element name="WCO" library="led" package="LED5MM" value=""/>
<element name="PER" library="led" package="LED5MM" value=""/>
<element name="DCF" library="led" package="LED5MM" value=""/>
<element name="PAD10" library="wirepad" package="1,6/0,8" value=""/>
<element name="PAD11" library="wirepad" package="1,6/0,8" value=""/>
<element name="SV3" library="con-lstb" package="MA13-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV4" library="con-lstb" package="MA13-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$13" library="holes" package="2,8" value=""/>
<element name="U$14" library="holes" package="2,8" value=""/>
<element name="U$16" library="holes" package="2,8" value=""/>
<element name="U$17" library="holes" package="2,8" value=""/>
<element name="IC33" library="74xx-us" package="DIL20" value="74LS240N"/>
<element name="IC40" library="74xx-us" package="DIL20" value="74LS240N"/>
<element name="IC56" library="74xx-us" package="DIL20" value="74LS240N"/>
<element name="IC47" library="74xx-us" package="DIL20" value="74LS240N"/>
<element name="IC48" library="74xx-us" package="DIL20" value="74LS240N"/>
<element name="IC49" library="74xx-us" package="DIL20" value="74LS240N"/>
<element name="U$18" library="pcb" package="SIERRA-PROTO" value=""/>
<element name="RN5" library="resistor-sil" package="SIL8" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN6" library="resistor-sil" package="SIL8" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN7" library="resistor-sil" package="SIL8" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN8" library="resistor-sil" package="SIL8" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN9" library="resistor-sil" package="SIL6" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN10" library="resistor-sil" package="SIL6" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN11" library="resistor-sil" package="SIL6" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN12" library="resistor-sil" package="SIL6" value="330">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SV4" pad="26"/>
<contactref element="SV4" pad="25"/>
<contactref element="IC33" pad="10"/>
<contactref element="IC40" pad="10"/>
<contactref element="IC56" pad="10"/>
<contactref element="IC33" pad="1"/>
<contactref element="IC33" pad="19"/>
<contactref element="IC40" pad="1"/>
<contactref element="IC40" pad="19"/>
<contactref element="IC56" pad="1"/>
<contactref element="IC56" pad="19"/>
<contactref element="IC47" pad="10"/>
<contactref element="IC47" pad="1"/>
<contactref element="IC47" pad="19"/>
<contactref element="IC48" pad="10"/>
<contactref element="IC48" pad="1"/>
<contactref element="IC48" pad="19"/>
<contactref element="IC49" pad="10"/>
<contactref element="IC49" pad="1"/>
<contactref element="IC49" pad="19"/>
</signal>
<signal name="VCC">
<contactref element="SV3" pad="25"/>
<contactref element="SV3" pad="26"/>
<contactref element="IC33" pad="20"/>
<contactref element="IC40" pad="20"/>
<contactref element="IC56" pad="20"/>
<contactref element="IC47" pad="20"/>
<contactref element="IC48" pad="20"/>
<contactref element="IC49" pad="20"/>
<contactref element="RN5" pad="1"/>
<contactref element="RN9" pad="1"/>
<contactref element="RN6" pad="1"/>
<contactref element="RN10" pad="1"/>
<contactref element="RN7" pad="1"/>
<contactref element="RN11" pad="1"/>
<contactref element="RN8" pad="1"/>
<contactref element="RN12" pad="1"/>
</signal>
<signal name="DMA11">
<contactref element="SV4" pad="23"/>
<contactref element="IC49" pad="13"/>
</signal>
<signal name="DMA00">
<contactref element="SV4" pad="1"/>
<contactref element="SV4" pad="24"/>
<contactref element="IC33" pad="4"/>
<contactref element="IC49" pad="11"/>
</signal>
<signal name="DMA01">
<contactref element="SV4" pad="3"/>
<contactref element="IC33" pad="13"/>
</signal>
<signal name="DMA02">
<contactref element="SV4" pad="5"/>
<contactref element="IC40" pad="4"/>
</signal>
<signal name="DMA03">
<contactref element="SV4" pad="7"/>
<contactref element="IC40" pad="13"/>
</signal>
<signal name="DMA04">
<contactref element="SV4" pad="9"/>
<contactref element="IC56" pad="2"/>
</signal>
<signal name="DMA05">
<contactref element="SV4" pad="11"/>
<contactref element="IC56" pad="11"/>
</signal>
<signal name="DMA06">
<contactref element="SV4" pad="13"/>
<contactref element="IC47" pad="4"/>
</signal>
<signal name="DMA07">
<contactref element="SV4" pad="15"/>
<contactref element="IC47" pad="11"/>
</signal>
<signal name="DMA08">
<contactref element="SV4" pad="17"/>
<contactref element="IC48" pad="2"/>
</signal>
<signal name="DMA09">
<contactref element="SV4" pad="19"/>
<contactref element="IC48" pad="11"/>
</signal>
<signal name="DMA10">
<contactref element="SV4" pad="21"/>
<contactref element="IC49" pad="4"/>
</signal>
<signal name="DAR08">
<contactref element="SV4" pad="16"/>
<contactref element="IC47" pad="8"/>
</signal>
<signal name="DAR09">
<contactref element="SV4" pad="18"/>
<contactref element="IC47" pad="17"/>
</signal>
<signal name="DAR10">
<contactref element="SV4" pad="20"/>
<contactref element="IC48" pad="8"/>
</signal>
<signal name="DAR11">
<contactref element="SV4" pad="22"/>
<contactref element="IC49" pad="2"/>
</signal>
<signal name="DAR07">
<contactref element="SV4" pad="14"/>
<contactref element="IC47" pad="2"/>
</signal>
<signal name="DAR06">
<contactref element="SV4" pad="12"/>
<contactref element="IC56" pad="8"/>
</signal>
<signal name="DAR04">
<contactref element="SV4" pad="8"/>
<contactref element="IC40" pad="11"/>
</signal>
<signal name="DAR05">
<contactref element="SV4" pad="10"/>
<contactref element="IC40" pad="17"/>
</signal>
<signal name="!BRK_RQ">
<contactref element="SV3" pad="11"/>
<contactref element="IC56" pad="17"/>
</signal>
<signal name="!BWC0">
<contactref element="SV3" pad="19"/>
<contactref element="IC48" pad="17"/>
</signal>
<signal name="DIO05">
<contactref element="SV3" pad="12"/>
<contactref element="IC56" pad="13"/>
</signal>
<signal name="DIO11">
<contactref element="SV3" pad="24"/>
<contactref element="IC49" pad="15"/>
</signal>
<signal name="DIO10">
<contactref element="SV3" pad="22"/>
<contactref element="IC49" pad="6"/>
</signal>
<signal name="DIO09">
<contactref element="SV3" pad="20"/>
<contactref element="IC48" pad="13"/>
</signal>
<signal name="DIO08">
<contactref element="SV3" pad="18"/>
<contactref element="IC48" pad="4"/>
</signal>
<signal name="DIO07">
<contactref element="SV3" pad="16"/>
<contactref element="IC47" pad="13"/>
</signal>
<signal name="DIO06">
<contactref element="SV3" pad="14"/>
<contactref element="IC47" pad="6"/>
</signal>
<signal name="DIO04">
<contactref element="SV3" pad="10"/>
<contactref element="IC56" pad="4"/>
</signal>
<signal name="DIO03">
<contactref element="SV3" pad="8"/>
<contactref element="IC40" pad="15"/>
</signal>
<signal name="DIO02">
<contactref element="SV3" pad="6"/>
<contactref element="IC40" pad="6"/>
</signal>
<signal name="DIO01">
<contactref element="SV3" pad="4"/>
<contactref element="IC33" pad="15"/>
</signal>
<signal name="DIO00">
<contactref element="SV3" pad="2"/>
<contactref element="IC33" pad="6"/>
</signal>
<signal name="F.2">
<contactref element="SV4" pad="4"/>
<contactref element="IC33" pad="11"/>
</signal>
<signal name="F.3">
<contactref element="SV4" pad="2"/>
<contactref element="IC33" pad="2"/>
</signal>
<signal name="PIE">
<contactref element="SV3" pad="5"/>
<contactref element="IC40" pad="8"/>
</signal>
<signal name="PER">
<contactref element="SV3" pad="21"/>
<contactref element="IC49" pad="8"/>
</signal>
<signal name="F.1">
<contactref element="SV4" pad="6"/>
<contactref element="IC40" pad="2"/>
</signal>
<signal name="CIE">
<contactref element="SV3" pad="1"/>
<contactref element="IC33" pad="8"/>
</signal>
<signal name="EIE">
<contactref element="SV3" pad="3"/>
<contactref element="IC33" pad="17"/>
</signal>
<signal name="WLS">
<contactref element="SV3" pad="15"/>
<contactref element="IC47" pad="15"/>
</signal>
<signal name="WRITING">
<contactref element="SV3" pad="9"/>
<contactref element="IC56" pad="6"/>
</signal>
<signal name="DONE">
<contactref element="SV3" pad="23"/>
<contactref element="IC49" pad="17"/>
</signal>
<signal name="NXD">
<contactref element="SV3" pad="17"/>
<contactref element="IC48" pad="6"/>
</signal>
<signal name="N$169">
<contactref element="DRE" pad="K"/>
<contactref element="PAD10" pad="1"/>
</signal>
<signal name="N$170">
<contactref element="DRL" pad="K"/>
<contactref element="PAD11" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="F.3" pad="A"/>
<contactref element="RN5" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="F.2" pad="A"/>
<contactref element="RN5" pad="3"/>
</signal>
<signal name="N$44">
<contactref element="F.1" pad="A"/>
<contactref element="RN5" pad="4"/>
</signal>
<signal name="N$86">
<contactref element="DMA00" pad="A"/>
<contactref element="RN5" pad="5"/>
</signal>
<signal name="N$87">
<contactref element="DMA01" pad="A"/>
<contactref element="RN5" pad="6"/>
</signal>
<signal name="N$88">
<contactref element="DMA02" pad="A"/>
<contactref element="RN5" pad="7"/>
</signal>
<signal name="N$98">
<contactref element="PIE" pad="A"/>
<contactref element="RN9" pad="2"/>
</signal>
<signal name="N$99">
<contactref element="EIE" pad="A"/>
<contactref element="RN9" pad="3"/>
</signal>
<signal name="N$100">
<contactref element="CIE" pad="A"/>
<contactref element="RN9" pad="4"/>
</signal>
<signal name="N$110">
<contactref element="DMB02" pad="A"/>
<contactref element="RN9" pad="5"/>
</signal>
<signal name="N$111">
<contactref element="DMB01" pad="A"/>
<contactref element="RN9" pad="6"/>
</signal>
<signal name="N$112">
<contactref element="DMB00" pad="A"/>
<contactref element="RN5" pad="8"/>
</signal>
<signal name="N$122">
<contactref element="IC33" pad="18"/>
<contactref element="F.3" pad="K"/>
</signal>
<signal name="N$123">
<contactref element="IC33" pad="16"/>
<contactref element="DMA00" pad="K"/>
</signal>
<signal name="N$124">
<contactref element="CIE" pad="K"/>
<contactref element="IC33" pad="12"/>
</signal>
<signal name="N$125">
<contactref element="IC33" pad="14"/>
<contactref element="DMB00" pad="K"/>
</signal>
<signal name="N$126">
<contactref element="DMA01" pad="K"/>
<contactref element="IC33" pad="7"/>
</signal>
<signal name="N$127">
<contactref element="F.2" pad="K"/>
<contactref element="IC33" pad="9"/>
</signal>
<signal name="N$128">
<contactref element="IC33" pad="5"/>
<contactref element="DMB01" pad="K"/>
</signal>
<signal name="N$129">
<contactref element="IC33" pad="3"/>
<contactref element="EIE" pad="K"/>
</signal>
<signal name="N$132">
<contactref element="F.1" pad="K"/>
<contactref element="IC40" pad="18"/>
</signal>
<signal name="N$133">
<contactref element="IC40" pad="16"/>
<contactref element="DMA02" pad="K"/>
</signal>
<signal name="N$134">
<contactref element="IC40" pad="14"/>
<contactref element="DMB02" pad="K"/>
</signal>
<signal name="N$135">
<contactref element="IC40" pad="12"/>
<contactref element="PIE" pad="K"/>
</signal>
<signal name="N$45">
<contactref element="DEA8" pad="A"/>
<contactref element="RN6" pad="2"/>
</signal>
<signal name="N$89">
<contactref element="DEA7" pad="A"/>
<contactref element="RN6" pad="3"/>
</signal>
<signal name="N$90">
<contactref element="DEA6" pad="A"/>
<contactref element="RN6" pad="4"/>
</signal>
<signal name="N$91">
<contactref element="DMA03" pad="A"/>
<contactref element="RN6" pad="5"/>
</signal>
<signal name="N$101">
<contactref element="DMA04" pad="A"/>
<contactref element="RN6" pad="6"/>
</signal>
<signal name="N$102">
<contactref element="DMA05" pad="A"/>
<contactref element="RN6" pad="7"/>
</signal>
<signal name="N$103">
<contactref element="DMB03" pad="A"/>
<contactref element="RN6" pad="8"/>
</signal>
<signal name="N$172">
<contactref element="DMB04" pad="A"/>
<contactref element="RN10" pad="6"/>
</signal>
<signal name="N$173">
<contactref element="DMB05" pad="A"/>
<contactref element="RN10" pad="5"/>
</signal>
<signal name="N$113">
<contactref element="DRE" pad="A"/>
<contactref element="RN10" pad="4"/>
</signal>
<signal name="N$114">
<contactref element="R/W" pad="A"/>
<contactref element="RN10" pad="3"/>
</signal>
<signal name="N$115">
<contactref element="DBR" pad="A"/>
<contactref element="RN10" pad="2"/>
</signal>
<signal name="N$136">
<contactref element="IC40" pad="5"/>
<contactref element="DMB03" pad="K"/>
</signal>
<signal name="N$137">
<contactref element="IC40" pad="7"/>
<contactref element="DMA03" pad="K"/>
</signal>
<signal name="N$138">
<contactref element="IC40" pad="9"/>
<contactref element="DEA8" pad="K"/>
</signal>
<signal name="N$139">
<contactref element="DEA7" pad="K"/>
<contactref element="IC40" pad="3"/>
</signal>
<signal name="N$140">
<contactref element="DMA04" pad="K"/>
<contactref element="IC56" pad="18"/>
</signal>
<signal name="N$141">
<contactref element="DMB04" pad="K"/>
<contactref element="IC56" pad="16"/>
</signal>
<signal name="N$142">
<contactref element="IC56" pad="14"/>
<contactref element="R/W" pad="K"/>
</signal>
<signal name="N$144">
<contactref element="DEA6" pad="K"/>
<contactref element="IC56" pad="12"/>
</signal>
<signal name="N$171">
<contactref element="DMA05" pad="K"/>
<contactref element="IC56" pad="9"/>
</signal>
<signal name="N$143">
<contactref element="IC56" pad="7"/>
<contactref element="DMB05" pad="K"/>
</signal>
<signal name="N$145">
<contactref element="IC56" pad="5"/>
<contactref element="DBR" pad="K"/>
</signal>
<signal name="N$175">
<contactref element="IC56" pad="3"/>
<contactref element="IC56" pad="15"/>
</signal>
<signal name="N$48">
<contactref element="DEA5" pad="A"/>
<contactref element="RN7" pad="2"/>
</signal>
<signal name="N$49">
<contactref element="DEA4" pad="A"/>
<contactref element="RN7" pad="3"/>
</signal>
<signal name="N$50">
<contactref element="DEA3" pad="A"/>
<contactref element="RN7" pad="4"/>
</signal>
<signal name="N$92">
<contactref element="DMA07" pad="A"/>
<contactref element="RN7" pad="6"/>
</signal>
<signal name="N$93">
<contactref element="DMA06" pad="A"/>
<contactref element="RN7" pad="5"/>
</signal>
<signal name="N$94">
<contactref element="DMA08" pad="A"/>
<contactref element="RN7" pad="7"/>
</signal>
<signal name="N$104">
<contactref element="DMB06" pad="A"/>
<contactref element="RN7" pad="8"/>
</signal>
<signal name="N$105">
<contactref element="DMB07" pad="A"/>
<contactref element="RN11" pad="6"/>
</signal>
<signal name="N$106">
<contactref element="DMB08" pad="A"/>
<contactref element="RN11" pad="5"/>
</signal>
<signal name="N$116">
<contactref element="DRL" pad="A"/>
<contactref element="RN11" pad="4"/>
</signal>
<signal name="N$117">
<contactref element="WLS" pad="A"/>
<contactref element="RN11" pad="3"/>
</signal>
<signal name="N$118">
<contactref element="NXD" pad="A"/>
<contactref element="RN11" pad="2"/>
</signal>
<signal name="N$146">
<contactref element="DMA06" pad="K"/>
<contactref element="IC47" pad="16"/>
</signal>
<signal name="N$149">
<contactref element="IC47" pad="18"/>
<contactref element="DEA5" pad="K"/>
</signal>
<signal name="N$152">
<contactref element="IC47" pad="14"/>
<contactref element="DMB06" pad="K"/>
</signal>
<signal name="N$147">
<contactref element="IC47" pad="12"/>
<contactref element="DEA4" pad="K"/>
</signal>
<signal name="N$148">
<contactref element="IC47" pad="7"/>
<contactref element="DMB07" pad="K"/>
</signal>
<signal name="N$150">
<contactref element="IC47" pad="9"/>
<contactref element="DMA07" pad="K"/>
</signal>
<signal name="N$151">
<contactref element="IC47" pad="5"/>
<contactref element="WLS" pad="K"/>
</signal>
<signal name="N$153">
<contactref element="DEA3" pad="K"/>
<contactref element="IC47" pad="3"/>
</signal>
<signal name="N$154">
<contactref element="DMA08" pad="K"/>
<contactref element="IC48" pad="18"/>
</signal>
<signal name="N$155">
<contactref element="IC48" pad="16"/>
<contactref element="DMB08" pad="K"/>
</signal>
<signal name="N$156">
<contactref element="IC48" pad="14"/>
<contactref element="NXD" pad="K"/>
</signal>
<signal name="N$46">
<contactref element="DEA2" pad="A"/>
<contactref element="RN8" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="DEA1" pad="A"/>
<contactref element="RN8" pad="3"/>
</signal>
<signal name="N$51">
<contactref element="DEA0" pad="A"/>
<contactref element="RN8" pad="4"/>
</signal>
<signal name="N$52">
<contactref element="DMA09" pad="A"/>
<contactref element="RN8" pad="5"/>
</signal>
<signal name="N$85">
<contactref element="DMA10" pad="A"/>
<contactref element="RN8" pad="6"/>
</signal>
<signal name="N$95">
<contactref element="DMA11" pad="A"/>
<contactref element="RN8" pad="7"/>
</signal>
<signal name="N$96">
<contactref element="DMB09" pad="A"/>
<contactref element="RN8" pad="8"/>
</signal>
<signal name="N$97">
<contactref element="DMB10" pad="A"/>
<contactref element="RN12" pad="6"/>
</signal>
<signal name="N$107">
<contactref element="DMB11" pad="A"/>
<contactref element="RN12" pad="5"/>
</signal>
<signal name="N$108">
<contactref element="WCO" pad="A"/>
<contactref element="RN12" pad="4"/>
</signal>
<signal name="N$109">
<contactref element="PER" pad="A"/>
<contactref element="RN12" pad="3"/>
</signal>
<signal name="N$119">
<contactref element="DCF" pad="A"/>
<contactref element="RN12" pad="2"/>
</signal>
<signal name="N$120">
<contactref element="DMA09" pad="K"/>
<contactref element="IC48" pad="9"/>
</signal>
<signal name="N$121">
<contactref element="IC48" pad="7"/>
<contactref element="DMB09" pad="K"/>
</signal>
<signal name="N$157">
<contactref element="IC48" pad="5"/>
<contactref element="WCO" pad="K"/>
</signal>
<signal name="N$160">
<contactref element="DEA2" pad="K"/>
<contactref element="IC48" pad="12"/>
</signal>
<signal name="N$163">
<contactref element="IC48" pad="3"/>
<contactref element="IC48" pad="15"/>
</signal>
<signal name="N$158">
<contactref element="IC49" pad="12"/>
<contactref element="PER" pad="K"/>
</signal>
<signal name="N$159">
<contactref element="IC49" pad="14"/>
<contactref element="DMB10" pad="K"/>
</signal>
<signal name="N$161">
<contactref element="IC49" pad="16"/>
<contactref element="DMA10" pad="K"/>
</signal>
<signal name="N$162">
<contactref element="IC49" pad="18"/>
<contactref element="DEA1" pad="K"/>
</signal>
<signal name="N$164">
<contactref element="DMA11" pad="K"/>
<contactref element="IC49" pad="7"/>
</signal>
<signal name="N$165">
<contactref element="IC49" pad="9"/>
<contactref element="DEA0" pad="K"/>
</signal>
<signal name="N$166">
<contactref element="DMB11" pad="K"/>
<contactref element="IC49" pad="5"/>
</signal>
<signal name="N$167">
<contactref element="DCF" pad="K"/>
<contactref element="IC49" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
