<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.6" y2="0" width="0.254" layer="20"/>
<wire x1="101.6" y1="0" x2="101.6" y2="81.28" width="0.254" layer="20"/>
<wire x1="101.6" y1="81.28" x2="0" y2="81.28" width="0.254" layer="20"/>
<wire x1="0" y1="81.28" x2="0" y2="0" width="0.254" layer="20"/>
<text>11-11-08</text>
<text>Nordic USB Serial Converter</text>
<text>DNP</text>
<text>nRF24L01</text>
<text>nRF2401A</text>
<text>RF-24G</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>VCC</text>
<text>STAT0</text>
<text>STAT1</text>
<text>STAT2</text>
<text>TX</text>
<text>RX</text>
<text>POWER</text>
<text>3.3V</text>
<text>P. Dokter</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="2X3">
</package>
<package name="SFE-NEW-WEBLOGO">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="EIA3216">
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="1X08">
</package>
<package name="FIDUCIAL-1X2">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="LED-0603">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="TRF-24G-SOCKET">
</package>
<package name="1X07">
</package>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun" package="SFE-NEW-WEBLOGO" value="LOGO-SFENEW"/>
<element name="C8" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$3" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="JP1" library="SparkFun" package="2X3" value="AVR_PRG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="TQFP32-08" value="ATMEGA168">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="C0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X08" value="nRF24L01"/>
<element name="U$4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$5" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$6" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$7" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="C3" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFun" package="USB-MINIB" value="USBSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun" package="SSOP28DB" value="FT232RL-BASICSSOP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="C0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun" package="LED-0603" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$8" library="SparkFun" package="TRF-24G-SOCKET" value="TRF-24G"/>
<element name="JP3" library="SparkFun" package="1X07" value="">
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun" package="C0402" value="0.1uF"/>
<element name="C7" library="SparkFun" package="C0402" value="0.1uF"/>
<element name="R2" library="SparkFun" package="C0402" value="330"/>
<element name="R3" library="SparkFun" package="C0402" value="330"/>
<element name="LED2" library="SparkFun" package="LED-0603" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun" package="LED-0603" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="SparkFun" package="LED-0603" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="SparkFun" package="LED-0603" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="SparkFun" package="LED-0603" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="C0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="C0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="C0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun" package="C0402" value="0.1uF"/>
<element name="U$9" library="SparkFun" package="CREATIVE_COMMONS" value="CREATIVE_COMMONS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C8" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="21"/>
<contactref element="U2" pad="25"/>
<contactref element="U2" pad="26"/>
<contactref element="X1" pad="GND"/>
<contactref element="C2" pad="C"/>
<contactref element="C5" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP2" pad="1"/>
<contactref element="U$8" pad="P$10"/>
<contactref element="JP3" pad="7"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="20"/>
<contactref element="C2" pad="A"/>
<contactref element="JP2" pad="8"/>
<contactref element="X1" pad="VBUS"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="JP2" pad="5"/>
<contactref element="U$8" pad="P$6"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="29"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="IRQ">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="CSN">
<contactref element="JP2" pad="6"/>
<contactref element="U1" pad="14"/>
<contactref element="U$8" pad="P$7"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="CE">
<contactref element="JP2" pad="7"/>
<contactref element="U1" pad="13"/>
<contactref element="U$8" pad="P$9"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="20"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="2"/>
<contactref element="C5" pad="A"/>
<contactref element="R1" pad="2"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="C9" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED6" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="U2" pad="4"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="X1" pad="D-"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="N$17">
<contactref element="X1" pad="D+"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="RXI">
<contactref element="U1" pad="30"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="TXO">
<contactref element="U1" pad="31"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="DATA">
<contactref element="U$8" pad="P$5"/>
<contactref element="U1" pad="11"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="DR2">
<contactref element="U$8" pad="P$2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="DOUT2">
<contactref element="U$8" pad="P$3"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="DR1">
<contactref element="U$8" pad="P$4"/>
<contactref element="U1" pad="10"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="CLK2">
<contactref element="U$8" pad="P$8"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="STAT0">
<contactref element="U1" pad="23"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="STAT1">
<contactref element="U1" pad="24"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="STAT2">
<contactref element="U1" pad="25"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="23"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="22"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="2"/>
<contactref element="LED5" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="2"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="2"/>
<contactref element="LED6" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
