<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="377.825" y2="0" width="0" layer="20"/>
<wire x1="377.825" y1="0" x2="377.825" y2="146.05" width="0" layer="20"/>
<wire x1="377.825" y1="146.05" x2="0" y2="146.05" width="0" layer="20"/>
<wire x1="0" y1="146.05" x2="0" y2="0" width="0" layer="20"/>
<text>PDP-8/I Light Board 50045108</text>
<text>5404519</text>
<hole x="50.8" y="7.9375" drill="6.35"/>
<hole x="333.375" y="7.9375" drill="6.35"/>
<wire x1="49.2125" y1="152.4" x2="63.5" y2="152.4" width="0.381" layer="20"/>
<wire x1="63.5" y1="152.4" x2="63.5" y2="174.625" width="0.381" layer="20"/>
<wire x1="336.55" y1="150.8125" x2="365.125" y2="150.8125" width="0.381" layer="20"/>
<wire x1="365.125" y1="161.925" x2="365.125" y2="150.8125" width="0.381" layer="20"/>
<wire x1="250.825" y1="150.8125" x2="307.975" y2="150.8125" width="0.381" layer="20"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="FLEX19">
<description>19 SMT pads on 0.0625" centers</description>
</package>
<package name="SPADELUG">
<description>Spade Lug Mounting Hole</description>
</package>
<package name="BULB">
<description>&lt;B&gt;Panel Bulb&lt;/B&gt;</description>
</package>
<package name="STRAIN-RELIEF">
</package>
</packages>
</library>
<library name="transistor">
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA17-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DF0" library="dec-con" package="BULB" value=""/>
<element name="T1" library="transistor" package="TO92" value="2N2222"/>
<element name="DF1" library="dec-con" package="BULB" value=""/>
<element name="T2" library="transistor" package="TO92" value="2N2222"/>
<element name="DF2" library="dec-con" package="BULB" value=""/>
<element name="T3" library="transistor" package="TO92" value="2N2222"/>
<element name="IF0" library="dec-con" package="BULB" value=""/>
<element name="T4" library="transistor" package="TO92" value="2N2222"/>
<element name="IF1" library="dec-con" package="BULB" value=""/>
<element name="T5" library="transistor" package="TO92" value="2N2222"/>
<element name="IF2" library="dec-con" package="BULB" value=""/>
<element name="T6" library="transistor" package="TO92" value="2N2222"/>
<element name="PC0" library="dec-con" package="BULB" value=""/>
<element name="T7" library="transistor" package="TO92" value="2N2222"/>
<element name="PC1" library="dec-con" package="BULB" value=""/>
<element name="T8" library="transistor" package="TO92" value="2N2222"/>
<element name="PC2" library="dec-con" package="BULB" value=""/>
<element name="T9" library="transistor" package="TO92" value="2N2222"/>
<element name="PC3" library="dec-con" package="BULB" value=""/>
<element name="T10" library="transistor" package="TO92" value="2N2222"/>
<element name="PC4" library="dec-con" package="BULB" value=""/>
<element name="T11" library="transistor" package="TO92" value="2N2222"/>
<element name="PC5" library="dec-con" package="BULB" value=""/>
<element name="T12" library="transistor" package="TO92" value="2N2222"/>
<element name="PC6" library="dec-con" package="BULB" value=""/>
<element name="T13" library="transistor" package="TO92" value="2N2222"/>
<element name="PC7" library="dec-con" package="BULB" value=""/>
<element name="T14" library="transistor" package="TO92" value="2N2222"/>
<element name="PC8" library="dec-con" package="BULB" value=""/>
<element name="T15" library="transistor" package="TO92" value="2N2222"/>
<element name="PC9" library="dec-con" package="BULB" value=""/>
<element name="T16" library="transistor" package="TO92" value="2N2222"/>
<element name="PC10" library="dec-con" package="BULB" value=""/>
<element name="T17" library="transistor" package="TO92" value="2N2222"/>
<element name="PC11" library="dec-con" package="BULB" value=""/>
<element name="T18" library="transistor" package="TO92" value="2N2222"/>
<element name="MA0" library="dec-con" package="BULB" value=""/>
<element name="T19" library="transistor" package="TO92" value="2N2222"/>
<element name="MA1" library="dec-con" package="BULB" value=""/>
<element name="T20" library="transistor" package="TO92" value="2N2222"/>
<element name="MA2" library="dec-con" package="BULB" value=""/>
<element name="T21" library="transistor" package="TO92" value="2N2222"/>
<element name="MA3" library="dec-con" package="BULB" value=""/>
<element name="T22" library="transistor" package="TO92" value="2N2222"/>
<element name="MA4" library="dec-con" package="BULB" value=""/>
<element name="T23" library="transistor" package="TO92" value="2N2222"/>
<element name="MA5" library="dec-con" package="BULB" value=""/>
<element name="T24" library="transistor" package="TO92" value="2N2222"/>
<element name="MA6" library="dec-con" package="BULB" value=""/>
<element name="T25" library="transistor" package="TO92" value="2N2222"/>
<element name="MA7" library="dec-con" package="BULB" value=""/>
<element name="T26" library="transistor" package="TO92" value="2N2222"/>
<element name="MA8" library="dec-con" package="BULB" value=""/>
<element name="T27" library="transistor" package="TO92" value="2N2222"/>
<element name="MA9" library="dec-con" package="BULB" value=""/>
<element name="T28" library="transistor" package="TO92" value="2N2222"/>
<element name="MA10" library="dec-con" package="BULB" value=""/>
<element name="T29" library="transistor" package="TO92" value="2N2222"/>
<element name="MA11" library="dec-con" package="BULB" value=""/>
<element name="T30" library="transistor" package="TO92" value="2N2222"/>
<element name="MB0" library="dec-con" package="BULB" value=""/>
<element name="T31" library="transistor" package="TO92" value="2N2222"/>
<element name="MB1" library="dec-con" package="BULB" value=""/>
<element name="T32" library="transistor" package="TO92" value="2N2222"/>
<element name="MB2" library="dec-con" package="BULB" value=""/>
<element name="T33" library="transistor" package="TO92" value="2N2222"/>
<element name="MB3" library="dec-con" package="BULB" value=""/>
<element name="T34" library="transistor" package="TO92" value="2N2222"/>
<element name="MB4" library="dec-con" package="BULB" value=""/>
<element name="T35" library="transistor" package="TO92" value="2N2222"/>
<element name="MB5" library="dec-con" package="BULB" value=""/>
<element name="T36" library="transistor" package="TO92" value="2N2222"/>
<element name="MB6" library="dec-con" package="BULB" value=""/>
<element name="T37" library="transistor" package="TO92" value="2N2222"/>
<element name="MB7" library="dec-con" package="BULB" value=""/>
<element name="T38" library="transistor" package="TO92" value="2N2222"/>
<element name="MB8" library="dec-con" package="BULB" value=""/>
<element name="T39" library="transistor" package="TO92" value="2N2222"/>
<element name="MB9" library="dec-con" package="BULB" value=""/>
<element name="T40" library="transistor" package="TO92" value="2N2222"/>
<element name="MB10" library="dec-con" package="BULB" value=""/>
<element name="T41" library="transistor" package="TO92" value="2N2222"/>
<element name="MB11" library="dec-con" package="BULB" value=""/>
<element name="T42" library="transistor" package="TO92" value="2N2222"/>
<element name="AC0" library="dec-con" package="BULB" value=""/>
<element name="T43" library="transistor" package="TO92" value="2N2222"/>
<element name="AC1" library="dec-con" package="BULB" value=""/>
<element name="T44" library="transistor" package="TO92" value="2N2222"/>
<element name="AC2" library="dec-con" package="BULB" value=""/>
<element name="T45" library="transistor" package="TO92" value="2N2222"/>
<element name="AC3" library="dec-con" package="BULB" value=""/>
<element name="T46" library="transistor" package="TO92" value="2N2222"/>
<element name="AC4" library="dec-con" package="BULB" value=""/>
<element name="T47" library="transistor" package="TO92" value="2N2222"/>
<element name="AC5" library="dec-con" package="BULB" value=""/>
<element name="T48" library="transistor" package="TO92" value="2N2222"/>
<element name="AC6" library="dec-con" package="BULB" value=""/>
<element name="T49" library="transistor" package="TO92" value="2N2222"/>
<element name="AC7" library="dec-con" package="BULB" value=""/>
<element name="T50" library="transistor" package="TO92" value="2N2222"/>
<element name="AC8" library="dec-con" package="BULB" value=""/>
<element name="T51" library="transistor" package="TO92" value="2N2222"/>
<element name="AC9" library="dec-con" package="BULB" value=""/>
<element name="T52" library="transistor" package="TO92" value="2N2222"/>
<element name="AC10" library="dec-con" package="BULB" value=""/>
<element name="T53" library="transistor" package="TO92" value="2N2222"/>
<element name="AC11" library="dec-con" package="BULB" value=""/>
<element name="T54" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ0" library="dec-con" package="BULB" value=""/>
<element name="T55" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ1" library="dec-con" package="BULB" value=""/>
<element name="T56" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ2" library="dec-con" package="BULB" value=""/>
<element name="T57" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ3" library="dec-con" package="BULB" value=""/>
<element name="T58" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ4" library="dec-con" package="BULB" value=""/>
<element name="T59" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ5" library="dec-con" package="BULB" value=""/>
<element name="T60" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ6" library="dec-con" package="BULB" value=""/>
<element name="T61" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ7" library="dec-con" package="BULB" value=""/>
<element name="T62" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ8" library="dec-con" package="BULB" value=""/>
<element name="T63" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ9" library="dec-con" package="BULB" value=""/>
<element name="T64" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ10" library="dec-con" package="BULB" value=""/>
<element name="T65" library="transistor" package="TO92" value="2N2222"/>
<element name="MQ11" library="dec-con" package="BULB" value=""/>
<element name="T66" library="transistor" package="TO92" value="2N2222"/>
<element name="SC0" library="dec-con" package="BULB" value=""/>
<element name="T67" library="transistor" package="TO92" value="2N2222"/>
<element name="SC1" library="dec-con" package="BULB" value=""/>
<element name="T68" library="transistor" package="TO92" value="2N2222"/>
<element name="SC2" library="dec-con" package="BULB" value=""/>
<element name="T69" library="transistor" package="TO92" value="2N2222"/>
<element name="SC3" library="dec-con" package="BULB" value=""/>
<element name="T70" library="transistor" package="TO92" value="2N2222"/>
<element name="SC4" library="dec-con" package="BULB" value=""/>
<element name="T71" library="transistor" package="TO92" value="2N2222"/>
<element name="LINK" library="dec-con" package="BULB" value=""/>
<element name="T72" library="transistor" package="TO92" value="2N2222"/>
<element name="ION" library="dec-con" package="BULB" value=""/>
<element name="T73" library="transistor" package="TO92" value="2N2222"/>
<element name="PAUSE" library="dec-con" package="BULB" value=""/>
<element name="T74" library="transistor" package="TO92" value="2N2222"/>
<element name="RUN" library="dec-con" package="BULB" value=""/>
<element name="T75" library="transistor" package="TO92" value="2N2222"/>
<element name="FETCH" library="dec-con" package="BULB" value=""/>
<element name="T76" library="transistor" package="TO92" value="2N2222"/>
<element name="EXECUTE" library="dec-con" package="BULB" value=""/>
<element name="T77" library="transistor" package="TO92" value="2N2222"/>
<element name="DEFER" library="dec-con" package="BULB" value=""/>
<element name="T78" library="transistor" package="TO92" value="2N2222"/>
<element name="WORDCOUNT" library="dec-con" package="BULB" value=""/>
<element name="T79" library="transistor" package="TO92" value="2N2222"/>
<element name="CURRENTADDRESS" library="dec-con" package="BULB" value=""/>
<element name="T80" library="transistor" package="TO92" value="2N2222"/>
<element name="BREAK" library="dec-con" package="BULB" value=""/>
<element name="T81" library="transistor" package="TO92" value="2N2222"/>
<element name="AND" library="dec-con" package="BULB" value=""/>
<element name="T82" library="transistor" package="TO92" value="2N2222"/>
<element name="TAD" library="dec-con" package="BULB" value=""/>
<element name="T83" library="transistor" package="TO92" value="2N2222"/>
<element name="ISZ" library="dec-con" package="BULB" value=""/>
<element name="T84" library="transistor" package="TO92" value="2N2222"/>
<element name="DCA" library="dec-con" package="BULB" value=""/>
<element name="T85" library="transistor" package="TO92" value="2N2222"/>
<element name="JMS" library="dec-con" package="BULB" value=""/>
<element name="T86" library="transistor" package="TO92" value="2N2222"/>
<element name="JMP" library="dec-con" package="BULB" value=""/>
<element name="T87" library="transistor" package="TO92" value="2N2222"/>
<element name="IOT" library="dec-con" package="BULB" value=""/>
<element name="T88" library="transistor" package="TO92" value="2N2222"/>
<element name="OPR" library="dec-con" package="BULB" value=""/>
<element name="T89" library="transistor" package="TO92" value="2N2222"/>
<element name="U$1" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$2" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$3" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$4" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="C40TOP" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="C40BOT" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="D40TOP" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="D40BOT" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="E40TOP" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="E40BOT" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="F40TOP" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="F40BOT" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="U$5" library="holes" package="3,6" value=""/>
<element name="U$6" library="holes" package="3,6" value=""/>
<element name="U$7" library="holes" package="3,6" value=""/>
<element name="U$8" library="holes" package="3,6" value=""/>
<element name="U$9" library="holes" package="3,6" value=""/>
<element name="U$11" library="holes" package="3,6" value=""/>
<element name="C40" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="D40" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="E40" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="F40" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="LUG1" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="LUG2" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="LUG3" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="LUG4" library="dec-con" package="SPADELUG" value="LUG"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="DF0" pad="B"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="+15V">
<contactref element="DF0" pad="A"/>
<contactref element="DF1" pad="A"/>
<contactref element="DF2" pad="A"/>
<contactref element="IF0" pad="A"/>
<contactref element="IF1" pad="A"/>
<contactref element="IF2" pad="A"/>
<contactref element="PC0" pad="A"/>
<contactref element="PC1" pad="A"/>
<contactref element="PC2" pad="A"/>
<contactref element="PC3" pad="A"/>
<contactref element="PC4" pad="A"/>
<contactref element="PC5" pad="A"/>
<contactref element="PC6" pad="A"/>
<contactref element="PC7" pad="A"/>
<contactref element="PC8" pad="A"/>
<contactref element="PC9" pad="A"/>
<contactref element="PC10" pad="A"/>
<contactref element="PC11" pad="A"/>
<contactref element="MA0" pad="A"/>
<contactref element="MA1" pad="A"/>
<contactref element="MA2" pad="A"/>
<contactref element="MA3" pad="A"/>
<contactref element="MA4" pad="A"/>
<contactref element="MA5" pad="A"/>
<contactref element="MA6" pad="A"/>
<contactref element="MA7" pad="A"/>
<contactref element="MA8" pad="A"/>
<contactref element="MA9" pad="A"/>
<contactref element="MA10" pad="A"/>
<contactref element="MA11" pad="A"/>
<contactref element="MB0" pad="A"/>
<contactref element="MB1" pad="A"/>
<contactref element="MB2" pad="A"/>
<contactref element="MB3" pad="A"/>
<contactref element="MB4" pad="A"/>
<contactref element="MB5" pad="A"/>
<contactref element="MB6" pad="A"/>
<contactref element="MB7" pad="A"/>
<contactref element="MB8" pad="A"/>
<contactref element="MB9" pad="A"/>
<contactref element="MB10" pad="A"/>
<contactref element="MB11" pad="A"/>
<contactref element="AC0" pad="A"/>
<contactref element="AC1" pad="A"/>
<contactref element="AC2" pad="A"/>
<contactref element="AC3" pad="A"/>
<contactref element="AC4" pad="A"/>
<contactref element="AC5" pad="A"/>
<contactref element="AC6" pad="A"/>
<contactref element="AC7" pad="A"/>
<contactref element="AC8" pad="A"/>
<contactref element="AC9" pad="A"/>
<contactref element="AC10" pad="A"/>
<contactref element="AC11" pad="A"/>
<contactref element="MQ0" pad="A"/>
<contactref element="MQ1" pad="A"/>
<contactref element="MQ2" pad="A"/>
<contactref element="MQ3" pad="A"/>
<contactref element="MQ4" pad="A"/>
<contactref element="MQ5" pad="A"/>
<contactref element="MQ6" pad="A"/>
<contactref element="MQ7" pad="A"/>
<contactref element="MQ8" pad="A"/>
<contactref element="MQ9" pad="A"/>
<contactref element="MQ10" pad="A"/>
<contactref element="MQ11" pad="A"/>
<contactref element="SC0" pad="A"/>
<contactref element="SC1" pad="A"/>
<contactref element="SC2" pad="A"/>
<contactref element="SC3" pad="A"/>
<contactref element="SC4" pad="A"/>
<contactref element="LINK" pad="A"/>
<contactref element="ION" pad="A"/>
<contactref element="PAUSE" pad="A"/>
<contactref element="RUN" pad="A"/>
<contactref element="FETCH" pad="A"/>
<contactref element="EXECUTE" pad="A"/>
<contactref element="DEFER" pad="A"/>
<contactref element="WORDCOUNT" pad="A"/>
<contactref element="CURRENTADDRESS" pad="A"/>
<contactref element="BREAK" pad="A"/>
<contactref element="AND" pad="A"/>
<contactref element="TAD" pad="A"/>
<contactref element="ISZ" pad="A"/>
<contactref element="DCA" pad="A"/>
<contactref element="JMS" pad="A"/>
<contactref element="JMP" pad="A"/>
<contactref element="IOT" pad="A"/>
<contactref element="OPR" pad="A"/>
<contactref element="LUG3" pad="1"/>
<contactref element="LUG4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="T1" pad="1"/>
<contactref element="T2" pad="1"/>
<contactref element="T3" pad="1"/>
<contactref element="T4" pad="1"/>
<contactref element="T5" pad="1"/>
<contactref element="T6" pad="1"/>
<contactref element="T7" pad="1"/>
<contactref element="T8" pad="1"/>
<contactref element="T9" pad="1"/>
<contactref element="T10" pad="1"/>
<contactref element="T11" pad="1"/>
<contactref element="T12" pad="1"/>
<contactref element="T13" pad="1"/>
<contactref element="T14" pad="1"/>
<contactref element="T15" pad="1"/>
<contactref element="T16" pad="1"/>
<contactref element="T17" pad="1"/>
<contactref element="T18" pad="1"/>
<contactref element="T19" pad="1"/>
<contactref element="T20" pad="1"/>
<contactref element="T21" pad="1"/>
<contactref element="T22" pad="1"/>
<contactref element="T23" pad="1"/>
<contactref element="T24" pad="1"/>
<contactref element="T25" pad="1"/>
<contactref element="T26" pad="1"/>
<contactref element="T27" pad="1"/>
<contactref element="T28" pad="1"/>
<contactref element="T29" pad="1"/>
<contactref element="T30" pad="1"/>
<contactref element="T31" pad="1"/>
<contactref element="T32" pad="1"/>
<contactref element="T33" pad="1"/>
<contactref element="T34" pad="1"/>
<contactref element="T35" pad="1"/>
<contactref element="T36" pad="1"/>
<contactref element="T37" pad="1"/>
<contactref element="T38" pad="1"/>
<contactref element="T39" pad="1"/>
<contactref element="T40" pad="1"/>
<contactref element="T41" pad="1"/>
<contactref element="T42" pad="1"/>
<contactref element="T43" pad="1"/>
<contactref element="T44" pad="1"/>
<contactref element="T45" pad="1"/>
<contactref element="T46" pad="1"/>
<contactref element="T47" pad="1"/>
<contactref element="T48" pad="1"/>
<contactref element="T49" pad="1"/>
<contactref element="T50" pad="1"/>
<contactref element="T51" pad="1"/>
<contactref element="T52" pad="1"/>
<contactref element="T53" pad="1"/>
<contactref element="T54" pad="1"/>
<contactref element="T55" pad="1"/>
<contactref element="T56" pad="1"/>
<contactref element="T57" pad="1"/>
<contactref element="T58" pad="1"/>
<contactref element="T59" pad="1"/>
<contactref element="T60" pad="1"/>
<contactref element="T61" pad="1"/>
<contactref element="T62" pad="1"/>
<contactref element="T63" pad="1"/>
<contactref element="T64" pad="1"/>
<contactref element="T65" pad="1"/>
<contactref element="T66" pad="1"/>
<contactref element="T67" pad="1"/>
<contactref element="T68" pad="1"/>
<contactref element="T69" pad="1"/>
<contactref element="T70" pad="1"/>
<contactref element="T71" pad="1"/>
<contactref element="T72" pad="1"/>
<contactref element="T73" pad="1"/>
<contactref element="T74" pad="1"/>
<contactref element="T75" pad="1"/>
<contactref element="T76" pad="1"/>
<contactref element="T77" pad="1"/>
<contactref element="T78" pad="1"/>
<contactref element="T79" pad="1"/>
<contactref element="T80" pad="1"/>
<contactref element="T81" pad="1"/>
<contactref element="T82" pad="1"/>
<contactref element="T83" pad="1"/>
<contactref element="T84" pad="1"/>
<contactref element="T85" pad="1"/>
<contactref element="T86" pad="1"/>
<contactref element="T87" pad="1"/>
<contactref element="T88" pad="1"/>
<contactref element="T89" pad="1"/>
<contactref element="C40BOT" pad="13"/>
<contactref element="D40BOT" pad="13"/>
<contactref element="E40BOT" pad="13"/>
<contactref element="F40BOT" pad="13"/>
<contactref element="C40" pad="17"/>
<contactref element="C40" pad="19"/>
<contactref element="C40" pad="20"/>
<contactref element="C40" pad="18"/>
<contactref element="D40" pad="17"/>
<contactref element="D40" pad="19"/>
<contactref element="D40" pad="20"/>
<contactref element="D40" pad="18"/>
<contactref element="E40" pad="17"/>
<contactref element="E40" pad="19"/>
<contactref element="E40" pad="20"/>
<contactref element="E40" pad="18"/>
<contactref element="F40" pad="17"/>
<contactref element="F40" pad="19"/>
<contactref element="F40" pad="20"/>
<contactref element="F40" pad="18"/>
<contactref element="LUG1" pad="1"/>
<contactref element="LUG2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="DF1" pad="B"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="DF2" pad="B"/>
<contactref element="T3" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IF0" pad="B"/>
<contactref element="T4" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="IF1" pad="B"/>
<contactref element="T5" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="IF2" pad="B"/>
<contactref element="T6" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="PC0" pad="B"/>
<contactref element="T7" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="PC1" pad="B"/>
<contactref element="T8" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="PC2" pad="B"/>
<contactref element="T9" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="PC3" pad="B"/>
<contactref element="T10" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="PC4" pad="B"/>
<contactref element="T11" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="PC5" pad="B"/>
<contactref element="T12" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="PC6" pad="B"/>
<contactref element="T13" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="PC7" pad="B"/>
<contactref element="T14" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="PC8" pad="B"/>
<contactref element="T15" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="PC9" pad="B"/>
<contactref element="T16" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="PC10" pad="B"/>
<contactref element="T17" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="PC11" pad="B"/>
<contactref element="T18" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="MA0" pad="B"/>
<contactref element="T19" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="MA1" pad="B"/>
<contactref element="T20" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="MA2" pad="B"/>
<contactref element="T21" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="MA3" pad="B"/>
<contactref element="T22" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="MA4" pad="B"/>
<contactref element="T23" pad="3"/>
</signal>
<signal name="N$24">
<contactref element="MA5" pad="B"/>
<contactref element="T24" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="MA6" pad="B"/>
<contactref element="T25" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="MA7" pad="B"/>
<contactref element="T26" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="MA8" pad="B"/>
<contactref element="T27" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="MA9" pad="B"/>
<contactref element="T28" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="MA10" pad="B"/>
<contactref element="T29" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="MA11" pad="B"/>
<contactref element="T30" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="MB0" pad="B"/>
<contactref element="T31" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="MB1" pad="B"/>
<contactref element="T32" pad="3"/>
</signal>
<signal name="N$33">
<contactref element="MB2" pad="B"/>
<contactref element="T33" pad="3"/>
</signal>
<signal name="N$34">
<contactref element="MB3" pad="B"/>
<contactref element="T34" pad="3"/>
</signal>
<signal name="N$35">
<contactref element="MB4" pad="B"/>
<contactref element="T35" pad="3"/>
</signal>
<signal name="N$36">
<contactref element="MB5" pad="B"/>
<contactref element="T36" pad="3"/>
</signal>
<signal name="N$37">
<contactref element="MB6" pad="B"/>
<contactref element="T37" pad="3"/>
</signal>
<signal name="N$38">
<contactref element="MB7" pad="B"/>
<contactref element="T38" pad="3"/>
</signal>
<signal name="N$39">
<contactref element="MB8" pad="B"/>
<contactref element="T39" pad="3"/>
</signal>
<signal name="N$40">
<contactref element="MB9" pad="B"/>
<contactref element="T40" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="MB10" pad="B"/>
<contactref element="T41" pad="3"/>
</signal>
<signal name="N$42">
<contactref element="MB11" pad="B"/>
<contactref element="T42" pad="3"/>
</signal>
<signal name="N$43">
<contactref element="AC0" pad="B"/>
<contactref element="T43" pad="3"/>
</signal>
<signal name="N$44">
<contactref element="AC1" pad="B"/>
<contactref element="T44" pad="3"/>
</signal>
<signal name="N$45">
<contactref element="AC2" pad="B"/>
<contactref element="T45" pad="3"/>
</signal>
<signal name="N$46">
<contactref element="AC3" pad="B"/>
<contactref element="T46" pad="3"/>
</signal>
<signal name="N$47">
<contactref element="AC4" pad="B"/>
<contactref element="T47" pad="3"/>
</signal>
<signal name="N$48">
<contactref element="AC5" pad="B"/>
<contactref element="T48" pad="3"/>
</signal>
<signal name="N$49">
<contactref element="AC6" pad="B"/>
<contactref element="T49" pad="3"/>
</signal>
<signal name="N$50">
<contactref element="AC7" pad="B"/>
<contactref element="T50" pad="3"/>
</signal>
<signal name="N$51">
<contactref element="AC8" pad="B"/>
<contactref element="T51" pad="3"/>
</signal>
<signal name="N$52">
<contactref element="AC9" pad="B"/>
<contactref element="T52" pad="3"/>
</signal>
<signal name="N$53">
<contactref element="AC10" pad="B"/>
<contactref element="T53" pad="3"/>
</signal>
<signal name="N$54">
<contactref element="AC11" pad="B"/>
<contactref element="T54" pad="3"/>
</signal>
<signal name="N$55">
<contactref element="MQ0" pad="B"/>
<contactref element="T55" pad="3"/>
</signal>
<signal name="N$56">
<contactref element="MQ1" pad="B"/>
<contactref element="T56" pad="3"/>
</signal>
<signal name="N$57">
<contactref element="MQ2" pad="B"/>
<contactref element="T57" pad="3"/>
</signal>
<signal name="N$58">
<contactref element="MQ3" pad="B"/>
<contactref element="T58" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="MQ4" pad="B"/>
<contactref element="T59" pad="3"/>
</signal>
<signal name="N$60">
<contactref element="MQ5" pad="B"/>
<contactref element="T60" pad="3"/>
</signal>
<signal name="N$61">
<contactref element="MQ6" pad="B"/>
<contactref element="T61" pad="3"/>
</signal>
<signal name="N$62">
<contactref element="MQ7" pad="B"/>
<contactref element="T62" pad="3"/>
</signal>
<signal name="N$63">
<contactref element="MQ8" pad="B"/>
<contactref element="T63" pad="3"/>
</signal>
<signal name="N$64">
<contactref element="MQ9" pad="B"/>
<contactref element="T64" pad="3"/>
</signal>
<signal name="N$65">
<contactref element="MQ10" pad="B"/>
<contactref element="T65" pad="3"/>
</signal>
<signal name="N$66">
<contactref element="MQ11" pad="B"/>
<contactref element="T66" pad="3"/>
</signal>
<signal name="N$67">
<contactref element="SC0" pad="B"/>
<contactref element="T67" pad="3"/>
</signal>
<signal name="N$68">
<contactref element="SC1" pad="B"/>
<contactref element="T68" pad="3"/>
</signal>
<signal name="N$69">
<contactref element="SC2" pad="B"/>
<contactref element="T69" pad="3"/>
</signal>
<signal name="N$70">
<contactref element="SC3" pad="B"/>
<contactref element="T70" pad="3"/>
</signal>
<signal name="N$71">
<contactref element="SC4" pad="B"/>
<contactref element="T71" pad="3"/>
</signal>
<signal name="N$72">
<contactref element="LINK" pad="B"/>
<contactref element="T72" pad="3"/>
</signal>
<signal name="N$73">
<contactref element="ION" pad="B"/>
<contactref element="T73" pad="3"/>
</signal>
<signal name="N$74">
<contactref element="PAUSE" pad="B"/>
<contactref element="T74" pad="3"/>
</signal>
<signal name="N$75">
<contactref element="RUN" pad="B"/>
<contactref element="T75" pad="3"/>
</signal>
<signal name="N$76">
<contactref element="FETCH" pad="B"/>
<contactref element="T76" pad="3"/>
</signal>
<signal name="N$77">
<contactref element="EXECUTE" pad="B"/>
<contactref element="T77" pad="3"/>
</signal>
<signal name="N$78">
<contactref element="DEFER" pad="B"/>
<contactref element="T78" pad="3"/>
</signal>
<signal name="N$79">
<contactref element="WORDCOUNT" pad="B"/>
<contactref element="T79" pad="3"/>
</signal>
<signal name="N$80">
<contactref element="CURRENTADDRESS" pad="B"/>
<contactref element="T80" pad="3"/>
</signal>
<signal name="N$81">
<contactref element="BREAK" pad="B"/>
<contactref element="T81" pad="3"/>
</signal>
<signal name="N$82">
<contactref element="AND" pad="B"/>
<contactref element="T82" pad="3"/>
</signal>
<signal name="N$83">
<contactref element="TAD" pad="B"/>
<contactref element="T83" pad="3"/>
</signal>
<signal name="N$84">
<contactref element="ISZ" pad="B"/>
<contactref element="T84" pad="3"/>
</signal>
<signal name="N$85">
<contactref element="DCA" pad="B"/>
<contactref element="T85" pad="3"/>
</signal>
<signal name="N$86">
<contactref element="JMS" pad="B"/>
<contactref element="T86" pad="3"/>
</signal>
<signal name="N$87">
<contactref element="JMP" pad="B"/>
<contactref element="T87" pad="3"/>
</signal>
<signal name="N$88">
<contactref element="IOT" pad="B"/>
<contactref element="T88" pad="3"/>
</signal>
<signal name="N$89">
<contactref element="OPR" pad="B"/>
<contactref element="T89" pad="3"/>
</signal>
<signal name="DF0">
<contactref element="T1" pad="2"/>
<contactref element="C40TOP" pad="1"/>
<contactref element="C40" pad="1"/>
</signal>
<signal name="DF1">
<contactref element="T2" pad="2"/>
<contactref element="C40BOT" pad="5"/>
<contactref element="C40" pad="10"/>
</signal>
<signal name="DF2">
<contactref element="T3" pad="2"/>
<contactref element="C40TOP" pad="6"/>
<contactref element="C40" pad="11"/>
</signal>
<signal name="IF0">
<contactref element="T4" pad="2"/>
<contactref element="C40BOT" pad="14"/>
<contactref element="C40" pad="24"/>
</signal>
<signal name="ION">
<contactref element="T73" pad="2"/>
<contactref element="F40BOT" pad="19"/>
<contactref element="D40" pad="34"/>
</signal>
<signal name="PAUSE">
<contactref element="T74" pad="2"/>
<contactref element="F40TOP" pad="17"/>
<contactref element="D40" pad="31"/>
</signal>
<signal name="RUN">
<contactref element="T75" pad="2"/>
<contactref element="F40TOP" pad="18"/>
<contactref element="D40" pad="33"/>
</signal>
<signal name="IF1">
<contactref element="T5" pad="2"/>
<contactref element="C40TOP" pad="14"/>
<contactref element="C40" pad="25"/>
</signal>
<signal name="IF2">
<contactref element="T6" pad="2"/>
<contactref element="C40BOT" pad="19"/>
<contactref element="C40" pad="34"/>
</signal>
<signal name="FETCH">
<contactref element="T76" pad="2"/>
<contactref element="F40BOT" pad="14"/>
<contactref element="D40" pad="24"/>
</signal>
<signal name="EXECUTE">
<contactref element="T77" pad="2"/>
<contactref element="F40BOT" pad="16"/>
<contactref element="D40" pad="28"/>
</signal>
<signal name="DEFER">
<contactref element="T78" pad="2"/>
<contactref element="F40BOT" pad="15"/>
<contactref element="D40" pad="26"/>
</signal>
<signal name="WC">
<contactref element="T79" pad="2"/>
<contactref element="F40BOT" pad="17"/>
<contactref element="D40" pad="30"/>
</signal>
<signal name="CA">
<contactref element="T80" pad="2"/>
<contactref element="F40BOT" pad="18"/>
<contactref element="D40" pad="32"/>
</signal>
<signal name="BREAK">
<contactref element="T81" pad="2"/>
<contactref element="F40BOT" pad="12"/>
<contactref element="D40" pad="22"/>
</signal>
<signal name="LINK">
<contactref element="T72" pad="2"/>
<contactref element="C40BOT" pad="16"/>
<contactref element="C40" pad="28"/>
</signal>
<signal name="SC0">
<contactref element="T67" pad="2"/>
<contactref element="C40TOP" pad="5"/>
<contactref element="C40" pad="9"/>
</signal>
<signal name="SC1">
<contactref element="T68" pad="2"/>
<contactref element="C40BOT" pad="1"/>
<contactref element="C40" pad="2"/>
</signal>
<signal name="SC2">
<contactref element="T69" pad="2"/>
<contactref element="C40TOP" pad="13"/>
<contactref element="C40" pad="23"/>
</signal>
<signal name="SC3">
<contactref element="T70" pad="2"/>
<contactref element="C40BOT" pad="6"/>
<contactref element="C40" pad="12"/>
</signal>
<signal name="SC4">
<contactref element="T71" pad="2"/>
<contactref element="C40TOP" pad="18"/>
<contactref element="C40" pad="33"/>
</signal>
<signal name="AND">
<contactref element="T82" pad="2"/>
<contactref element="F40BOT" pad="1"/>
<contactref element="D40" pad="2"/>
</signal>
<signal name="TAD">
<contactref element="T83" pad="2"/>
<contactref element="F40BOT" pad="2"/>
<contactref element="D40" pad="4"/>
</signal>
<signal name="ISZ">
<contactref element="T84" pad="2"/>
<contactref element="F40BOT" pad="3"/>
<contactref element="D40" pad="6"/>
</signal>
<signal name="DCA">
<contactref element="T85" pad="2"/>
<contactref element="F40BOT" pad="4"/>
<contactref element="D40" pad="8"/>
</signal>
<signal name="JMS">
<contactref element="T86" pad="2"/>
<contactref element="F40BOT" pad="5"/>
<contactref element="D40" pad="10"/>
</signal>
<signal name="JMP">
<contactref element="T87" pad="2"/>
<contactref element="F40BOT" pad="6"/>
<contactref element="D40" pad="12"/>
</signal>
<signal name="IOT">
<contactref element="T88" pad="2"/>
<contactref element="F40TOP" pad="13"/>
<contactref element="D40" pad="23"/>
</signal>
<signal name="OPR">
<contactref element="T89" pad="2"/>
<contactref element="F40BOT" pad="11"/>
<contactref element="D40" pad="16"/>
</signal>
<signal name="PC0">
<contactref element="T7" pad="2"/>
<contactref element="D40TOP" pad="1"/>
<contactref element="E40" pad="1"/>
</signal>
<signal name="PC1">
<contactref element="T8" pad="2"/>
<contactref element="D40BOT" pad="5"/>
<contactref element="E40" pad="10"/>
</signal>
<signal name="PC2">
<contactref element="T9" pad="2"/>
<contactref element="D40TOP" pad="6"/>
<contactref element="E40" pad="11"/>
</signal>
<signal name="PC3">
<contactref element="T10" pad="2"/>
<contactref element="D40BOT" pad="14"/>
<contactref element="E40" pad="24"/>
</signal>
<signal name="PC4">
<contactref element="T11" pad="2"/>
<contactref element="D40TOP" pad="14"/>
<contactref element="E40" pad="25"/>
</signal>
<signal name="PC5">
<contactref element="T12" pad="2"/>
<contactref element="D40BOT" pad="19"/>
<contactref element="E40" pad="34"/>
</signal>
<signal name="PC6">
<contactref element="T13" pad="2"/>
<contactref element="E40TOP" pad="1"/>
<contactref element="F40" pad="1"/>
</signal>
<signal name="PC7">
<contactref element="T14" pad="2"/>
<contactref element="E40BOT" pad="5"/>
<contactref element="F40" pad="10"/>
</signal>
<signal name="PC8">
<contactref element="T15" pad="2"/>
<contactref element="E40TOP" pad="6"/>
<contactref element="F40" pad="11"/>
</signal>
<signal name="MA0">
<contactref element="T19" pad="2"/>
<contactref element="D40TOP" pad="2"/>
<contactref element="E40" pad="3"/>
</signal>
<signal name="MA1">
<contactref element="T20" pad="2"/>
<contactref element="D40BOT" pad="4"/>
<contactref element="E40" pad="8"/>
</signal>
<signal name="MA2">
<contactref element="T21" pad="2"/>
<contactref element="D40TOP" pad="7"/>
<contactref element="E40" pad="13"/>
</signal>
<signal name="MA3">
<contactref element="T22" pad="2"/>
<contactref element="D40BOT" pad="12"/>
<contactref element="E40" pad="22"/>
</signal>
<signal name="MA4">
<contactref element="T23" pad="2"/>
<contactref element="D40TOP" pad="15"/>
<contactref element="E40" pad="27"/>
</signal>
<signal name="MA5">
<contactref element="T24" pad="2"/>
<contactref element="D40BOT" pad="18"/>
<contactref element="E40" pad="32"/>
</signal>
<signal name="MA6">
<contactref element="T25" pad="2"/>
<contactref element="E40TOP" pad="2"/>
<contactref element="F40" pad="3"/>
</signal>
<signal name="MA7">
<contactref element="T26" pad="2"/>
<contactref element="E40BOT" pad="4"/>
<contactref element="F40" pad="8"/>
</signal>
<signal name="MA8">
<contactref element="T27" pad="2"/>
<contactref element="E40TOP" pad="7"/>
<contactref element="F40" pad="13"/>
</signal>
<signal name="MB0">
<contactref element="T31" pad="2"/>
<contactref element="D40TOP" pad="3"/>
<contactref element="E40" pad="5"/>
</signal>
<signal name="MB1">
<contactref element="T32" pad="2"/>
<contactref element="D40BOT" pad="3"/>
<contactref element="E40" pad="6"/>
</signal>
<signal name="MB2">
<contactref element="T33" pad="2"/>
<contactref element="D40TOP" pad="8"/>
<contactref element="E40" pad="15"/>
</signal>
<signal name="MB3">
<contactref element="T34" pad="2"/>
<contactref element="D40BOT" pad="11"/>
<contactref element="E40" pad="16"/>
</signal>
<signal name="MB4">
<contactref element="T35" pad="2"/>
<contactref element="D40TOP" pad="16"/>
<contactref element="E40" pad="29"/>
</signal>
<signal name="MB5">
<contactref element="T36" pad="2"/>
<contactref element="D40BOT" pad="17"/>
<contactref element="E40" pad="30"/>
</signal>
<signal name="MB6">
<contactref element="T37" pad="2"/>
<contactref element="E40TOP" pad="3"/>
<contactref element="F40" pad="5"/>
</signal>
<signal name="MB7">
<contactref element="T38" pad="2"/>
<contactref element="E40BOT" pad="3"/>
<contactref element="F40" pad="6"/>
</signal>
<signal name="MB8">
<contactref element="T39" pad="2"/>
<contactref element="E40TOP" pad="8"/>
<contactref element="F40" pad="15"/>
</signal>
<signal name="PC9">
<contactref element="T16" pad="2"/>
<contactref element="E40BOT" pad="14"/>
<contactref element="F40" pad="24"/>
</signal>
<signal name="PC10">
<contactref element="T17" pad="2"/>
<contactref element="E40TOP" pad="14"/>
<contactref element="F40" pad="25"/>
</signal>
<signal name="PC11">
<contactref element="T18" pad="2"/>
<contactref element="E40BOT" pad="19"/>
<contactref element="F40" pad="34"/>
</signal>
<signal name="MA11">
<contactref element="T30" pad="2"/>
<contactref element="E40BOT" pad="18"/>
<contactref element="F40" pad="32"/>
</signal>
<signal name="MA10">
<contactref element="T29" pad="2"/>
<contactref element="E40TOP" pad="15"/>
<contactref element="F40" pad="27"/>
</signal>
<signal name="MA9">
<contactref element="T28" pad="2"/>
<contactref element="E40BOT" pad="12"/>
<contactref element="F40" pad="22"/>
</signal>
<signal name="MB9">
<contactref element="T40" pad="2"/>
<contactref element="E40BOT" pad="11"/>
<contactref element="F40" pad="16"/>
</signal>
<signal name="MB10">
<contactref element="T41" pad="2"/>
<contactref element="E40TOP" pad="16"/>
<contactref element="F40" pad="29"/>
</signal>
<signal name="MB11">
<contactref element="T42" pad="2"/>
<contactref element="E40BOT" pad="17"/>
<contactref element="F40" pad="30"/>
</signal>
<signal name="AC0">
<contactref element="T43" pad="2"/>
<contactref element="D40TOP" pad="4"/>
<contactref element="E40" pad="7"/>
</signal>
<signal name="AC1">
<contactref element="T44" pad="2"/>
<contactref element="D40BOT" pad="2"/>
<contactref element="E40" pad="4"/>
</signal>
<signal name="AC2">
<contactref element="T45" pad="2"/>
<contactref element="D40TOP" pad="12"/>
<contactref element="E40" pad="21"/>
</signal>
<signal name="AC3">
<contactref element="T46" pad="2"/>
<contactref element="D40BOT" pad="9"/>
<contactref element="E40" pad="14"/>
</signal>
<signal name="AC4">
<contactref element="T47" pad="2"/>
<contactref element="D40TOP" pad="17"/>
<contactref element="E40" pad="31"/>
</signal>
<signal name="AC5">
<contactref element="T48" pad="2"/>
<contactref element="D40BOT" pad="16"/>
<contactref element="E40" pad="28"/>
</signal>
<signal name="AC6">
<contactref element="T49" pad="2"/>
<contactref element="E40TOP" pad="4"/>
<contactref element="F40" pad="7"/>
</signal>
<signal name="AC7">
<contactref element="T50" pad="2"/>
<contactref element="E40BOT" pad="2"/>
<contactref element="F40" pad="4"/>
</signal>
<signal name="AC8">
<contactref element="T51" pad="2"/>
<contactref element="E40TOP" pad="12"/>
<contactref element="F40" pad="21"/>
</signal>
<signal name="MQ8">
<contactref element="T63" pad="2"/>
<contactref element="E40TOP" pad="13"/>
<contactref element="F40" pad="23"/>
</signal>
<signal name="MQ7">
<contactref element="T62" pad="2"/>
<contactref element="E40BOT" pad="1"/>
<contactref element="F40" pad="2"/>
</signal>
<signal name="MQ6">
<contactref element="T61" pad="2"/>
<contactref element="E40TOP" pad="5"/>
<contactref element="F40" pad="9"/>
</signal>
<signal name="MQ0">
<contactref element="T55" pad="2"/>
<contactref element="D40TOP" pad="5"/>
<contactref element="E40" pad="9"/>
</signal>
<signal name="MQ1">
<contactref element="T56" pad="2"/>
<contactref element="D40BOT" pad="1"/>
<contactref element="E40" pad="2"/>
</signal>
<signal name="MQ2">
<contactref element="T57" pad="2"/>
<contactref element="D40TOP" pad="13"/>
<contactref element="E40" pad="23"/>
</signal>
<signal name="MQ3">
<contactref element="T58" pad="2"/>
<contactref element="D40BOT" pad="6"/>
<contactref element="E40" pad="12"/>
</signal>
<signal name="MQ4">
<contactref element="T59" pad="2"/>
<contactref element="D40TOP" pad="18"/>
<contactref element="E40" pad="33"/>
</signal>
<signal name="MQ5">
<contactref element="T60" pad="2"/>
<contactref element="D40BOT" pad="15"/>
<contactref element="E40" pad="26"/>
</signal>
<signal name="AC9">
<contactref element="T52" pad="2"/>
<contactref element="E40BOT" pad="9"/>
<contactref element="F40" pad="14"/>
</signal>
<signal name="AC10">
<contactref element="T53" pad="2"/>
<contactref element="E40TOP" pad="17"/>
<contactref element="F40" pad="31"/>
</signal>
<signal name="AC11">
<contactref element="T54" pad="2"/>
<contactref element="E40BOT" pad="16"/>
<contactref element="F40" pad="28"/>
</signal>
<signal name="MQ11">
<contactref element="T66" pad="2"/>
<contactref element="E40BOT" pad="15"/>
<contactref element="F40" pad="26"/>
</signal>
<signal name="MQ10">
<contactref element="T65" pad="2"/>
<contactref element="E40TOP" pad="18"/>
<contactref element="F40" pad="33"/>
</signal>
<signal name="MQ9">
<contactref element="T64" pad="2"/>
<contactref element="E40BOT" pad="6"/>
<contactref element="F40" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
