<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.6" y2="0" width="0" layer="20"/>
<wire x1="101.6" y1="0" x2="376.2375" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="82.55" width="0" layer="20"/>
<wire x1="0" y1="82.55" x2="376.2375" y2="82.55" width="0" layer="20"/>
<wire x1="376.2375" y1="0" x2="376.2375" y2="82.55" width="0" layer="20"/>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="DPDT8I">
<description>DPDT, 8/i non-momentary</description>
</package>
<package name="FLEX19">
<description>19 SMT pads on 0.0625" centers</description>
</package>
<package name="STRAIN-RELIEF">
</package>
<package name="SPDT8I">
<description>SPDT momentary, 8/I style</description>
</package>
<package name="SPADELUG">
<description>Spade Lug Mounting Hole</description>
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA17-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="START" library="dec-con" package="SPDT8I" value="SPDT8I"/>
<element name="IF0" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="IF1" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="IF2" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="DF0" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="DF1" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="DF2" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR0" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR1" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR2" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SS" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SI" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR3" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR4" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR5" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR6" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR7" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR8" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR9" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR10" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="SR11" library="dec-con" package="DPDT8I" value="DPDT8I"/>
<element name="LA" library="dec-con" package="SPDT8I" value="SPDT8I"/>
<element name="DEP" library="dec-con" package="SPDT8I" value="SPDT8I"/>
<element name="EXAM" library="dec-con" package="SPDT8I" value="SPDT8I"/>
<element name="CONT" library="dec-con" package="SPDT8I" value="SPDT8I"/>
<element name="STOP" library="dec-con" package="SPDT8I" value="SPDT8I"/>
<element name="U$1" library="holes" package="3,6" value=""/>
<element name="U$2" library="holes" package="3,6" value=""/>
<element name="U$3" library="holes" package="3,6" value=""/>
<element name="U$4" library="holes" package="3,6" value=""/>
<element name="U$5" library="holes" package="3,6" value=""/>
<element name="U$6" library="holes" package="3,6" value=""/>
<element name="U$7" library="holes" package="3,6" value=""/>
<element name="U$10" library="holes" package="3,6" value=""/>
<element name="U$11" library="holes" package="3,6" value=""/>
<element name="U$12" library="holes" package="3,6" value=""/>
<element name="U$13" library="holes" package="3,6" value=""/>
<element name="U$14" library="holes" package="3,6" value=""/>
<element name="U$15" library="holes" package="3,6" value=""/>
<element name="U$16" library="holes" package="3,6" value=""/>
<element name="U$18" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$17" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="FLEXB" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="FLEXA" library="dec-con" package="FLEX19" value="FLEX19"/>
<element name="A40" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="B40" library="con-lstb" package="MA17-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="V-" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="LOCK-" library="dec-con" package="SPADELUG" value="LUG"/>
</elements>
<signals>
<signal name="DF1">
<contactref element="IF1" pad="L2"/>
<contactref element="IF1" pad="R2"/>
<contactref element="FLEXA" pad="15"/>
<contactref element="A40" pad="8"/>
</signal>
<signal name="IF2">
<contactref element="DF2" pad="L2"/>
<contactref element="DF2" pad="R2"/>
<contactref element="FLEXA" pad="11"/>
<contactref element="A40" pad="16"/>
</signal>
<signal name="IF1">
<contactref element="DF1" pad="L2"/>
<contactref element="DF1" pad="R2"/>
<contactref element="FLEXA" pad="12"/>
<contactref element="A40" pad="14"/>
</signal>
<signal name="DF2">
<contactref element="IF2" pad="R2"/>
<contactref element="IF2" pad="L2"/>
<contactref element="FLEXA" pad="14"/>
<contactref element="A40" pad="10"/>
</signal>
<signal name="DF0">
<contactref element="IF0" pad="R2"/>
<contactref element="IF0" pad="L2"/>
<contactref element="FLEXA" pad="16"/>
<contactref element="A40" pad="6"/>
</signal>
<signal name="IF0">
<contactref element="DF0" pad="R2"/>
<contactref element="DF0" pad="L2"/>
<contactref element="FLEXA" pad="13"/>
<contactref element="A40" pad="12"/>
</signal>
<signal name="SS">
<contactref element="SS" pad="L2"/>
<contactref element="SS" pad="R2"/>
<contactref element="FLEXB" pad="3"/>
<contactref element="B40" pad="34"/>
</signal>
<signal name="SI">
<contactref element="SI" pad="R2"/>
<contactref element="SI" pad="L2"/>
<contactref element="FLEXB" pad="2"/>
<contactref element="B40" pad="32"/>
</signal>
<signal name="STOP">
<contactref element="FLEXB" pad="4"/>
<contactref element="STOP" pad="A2"/>
<contactref element="B40" pad="30"/>
</signal>
<signal name="CONT">
<contactref element="CONT" pad="A2"/>
<contactref element="FLEXB" pad="5"/>
<contactref element="B40" pad="28"/>
</signal>
<signal name="EXAM">
<contactref element="EXAM" pad="A2"/>
<contactref element="FLEXB" pad="6"/>
<contactref element="B40" pad="26"/>
</signal>
<signal name="START">
<contactref element="START" pad="A2"/>
<contactref element="FLEXB" pad="11"/>
<contactref element="B40" pad="16"/>
</signal>
<signal name="SR8">
<contactref element="SR8" pad="R2"/>
<contactref element="SR8" pad="L2"/>
<contactref element="FLEXB" pad="15"/>
<contactref element="B40" pad="8"/>
</signal>
<signal name="DEP">
<contactref element="DEP" pad="A2"/>
<contactref element="FLEXB" pad="9"/>
<contactref element="B40" pad="20"/>
</signal>
<signal name="LA">
<contactref element="LA" pad="A2"/>
<contactref element="FLEXB" pad="10"/>
<contactref element="B40" pad="18"/>
</signal>
<signal name="SR11">
<contactref element="SR11" pad="R2"/>
<contactref element="SR11" pad="L2"/>
<contactref element="FLEXB" pad="12"/>
<contactref element="B40" pad="14"/>
</signal>
<signal name="SR10">
<contactref element="SR10" pad="R2"/>
<contactref element="SR10" pad="L2"/>
<contactref element="FLEXB" pad="13"/>
<contactref element="B40" pad="12"/>
</signal>
<signal name="SR9">
<contactref element="SR9" pad="R2"/>
<contactref element="SR9" pad="L2"/>
<contactref element="FLEXB" pad="14"/>
<contactref element="B40" pad="10"/>
</signal>
<signal name="SR6">
<contactref element="SR6" pad="R2"/>
<contactref element="SR6" pad="L2"/>
<contactref element="FLEXA" pad="2"/>
<contactref element="A40" pad="32"/>
</signal>
<signal name="SR7">
<contactref element="SR7" pad="R2"/>
<contactref element="SR7" pad="L2"/>
<contactref element="FLEXB" pad="16"/>
<contactref element="B40" pad="6"/>
</signal>
<signal name="SR5">
<contactref element="SR5" pad="R2"/>
<contactref element="SR5" pad="L2"/>
<contactref element="FLEXA" pad="3"/>
<contactref element="A40" pad="34"/>
</signal>
<signal name="SR4">
<contactref element="SR4" pad="L2"/>
<contactref element="SR4" pad="R2"/>
<contactref element="FLEXA" pad="4"/>
<contactref element="A40" pad="30"/>
</signal>
<signal name="SR3">
<contactref element="SR3" pad="R2"/>
<contactref element="SR3" pad="L2"/>
<contactref element="FLEXA" pad="5"/>
<contactref element="A40" pad="28"/>
</signal>
<signal name="SR2">
<contactref element="SR2" pad="L2"/>
<contactref element="SR2" pad="R2"/>
<contactref element="FLEXA" pad="6"/>
<contactref element="A40" pad="26"/>
</signal>
<signal name="SR1">
<contactref element="SR1" pad="L2"/>
<contactref element="SR1" pad="R2"/>
<contactref element="FLEXA" pad="9"/>
<contactref element="A40" pad="20"/>
</signal>
<signal name="SR0">
<contactref element="SR0" pad="L2"/>
<contactref element="SR0" pad="R2"/>
<contactref element="FLEXA" pad="10"/>
<contactref element="A40" pad="18"/>
</signal>
<signal name="LOCK-">
<contactref element="START" pad="A1"/>
<contactref element="CONT" pad="A1"/>
<contactref element="STOP" pad="A1"/>
<contactref element="SS" pad="R1"/>
<contactref element="SS" pad="L1"/>
<contactref element="SI" pad="L1"/>
<contactref element="SI" pad="R1"/>
<contactref element="LOCK-" pad="1"/>
</signal>
<signal name="V-">
<contactref element="LA" pad="A1"/>
<contactref element="DEP" pad="A1"/>
<contactref element="EXAM" pad="A1"/>
<contactref element="SR6" pad="R3"/>
<contactref element="IF0" pad="L3"/>
<contactref element="IF1" pad="L3"/>
<contactref element="IF0" pad="R3"/>
<contactref element="IF2" pad="L3"/>
<contactref element="DF2" pad="L3"/>
<contactref element="IF1" pad="R3"/>
<contactref element="IF2" pad="R3"/>
<contactref element="DF0" pad="R3"/>
<contactref element="DF0" pad="L3"/>
<contactref element="DF1" pad="L3"/>
<contactref element="DF1" pad="R3"/>
<contactref element="DF2" pad="R3"/>
<contactref element="SR3" pad="R3"/>
<contactref element="SR3" pad="L3"/>
<contactref element="SR4" pad="L3"/>
<contactref element="SR5" pad="L3"/>
<contactref element="SR5" pad="R3"/>
<contactref element="SR6" pad="L3"/>
<contactref element="SR7" pad="L3"/>
<contactref element="SR8" pad="L3"/>
<contactref element="SR8" pad="R3"/>
<contactref element="SR7" pad="R3"/>
<contactref element="SR4" pad="R3"/>
<contactref element="SR0" pad="L3"/>
<contactref element="SR0" pad="R3"/>
<contactref element="SR9" pad="L3"/>
<contactref element="SR9" pad="R3"/>
<contactref element="SR1" pad="L3"/>
<contactref element="SR1" pad="R3"/>
<contactref element="SR10" pad="R3"/>
<contactref element="SR10" pad="L3"/>
<contactref element="SR2" pad="L3"/>
<contactref element="SR2" pad="R3"/>
<contactref element="SR11" pad="L3"/>
<contactref element="SR11" pad="R3"/>
<contactref element="A40" pad="4"/>
<contactref element="B40" pad="4"/>
<contactref element="FLEXA" pad="18"/>
<contactref element="FLEXB" pad="18"/>
<contactref element="V-" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
