<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="377.825" y1="0" x2="377.825" y2="138.1125" width="0" layer="20"/>
<wire x1="0" y1="138.1125" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="377.825" y2="0" width="0" layer="20"/>
<wire x1="174.625" y1="0" x2="377.825" y2="0" width="0" layer="20"/>
<wire x1="377.825" y1="138.1125" x2="0" y2="138.1125" width="0" layer="20"/>
<text>PuDP-8/I Interface Board</text>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="SPADELUG">
<description>Spade Lug Mounting Hole</description>
</package>
<package name="STRAIN-RELIEF">
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA17-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
<library name="raspberrypi_bastelstube_v13">
<packages>
<package name="RASPI_BOARD_B+_FULL">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes</description>
</package>
</packages>
</library>
<library name="74xx-us">
<packages>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$2" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$3" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$4" library="dec-con" package="STRAIN-RELIEF" value=""/>
<element name="U$5" library="holes" package="3,6" value=""/>
<element name="U$6" library="holes" package="3,6" value=""/>
<element name="U$7" library="holes" package="3,6" value=""/>
<element name="U$8" library="holes" package="3,6" value=""/>
<element name="U$9" library="holes" package="3,6" value=""/>
<element name="U$11" library="holes" package="3,6" value=""/>
<element name="C40" library="con-lstb" package="MA17-2" value=""/>
<element name="D40" library="con-lstb" package="MA17-2" value=""/>
<element name="E40" library="con-lstb" package="MA17-2" value=""/>
<element name="F40" library="con-lstb" package="MA17-2" value=""/>
<element name="GND1" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="GND2" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="+V1" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="+V2" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="+V3" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="GND3" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="+V4" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="GND4" library="dec-con" package="SPADELUG" value="LUG"/>
<element name="X1" library="raspberrypi_bastelstube_v13" package="RASPI_BOARD_B+_FULL" value="RASPI_BOARD_B+_F"/>
<element name="R90" library="rcl" package="0207/10" value=""/>
<element name="R91" library="rcl" package="0207/10" value=""/>
<element name="R92" library="rcl" package="0207/10" value=""/>
<element name="R93" library="rcl" package="0207/10" value="4K"/>
<element name="R94" library="rcl" package="0207/10" value=""/>
<element name="R95" library="rcl" package="0207/10" value=""/>
<element name="R96" library="rcl" package="0207/10" value=""/>
<element name="R97" library="rcl" package="0207/10" value=""/>
<element name="R98" library="rcl" package="0207/10" value=""/>
<element name="R99" library="rcl" package="0207/10" value="4K"/>
<element name="R100" library="rcl" package="0207/10" value=""/>
<element name="R101" library="rcl" package="0207/10" value=""/>
<element name="R102" library="rcl" package="0207/10" value=""/>
<element name="R103" library="rcl" package="0207/10" value="4K"/>
<element name="R104" library="rcl" package="0207/10" value=""/>
<element name="R1" library="rcl" package="0207/10" value="4.7K"/>
<element name="R2" library="rcl" package="0207/10" value="4.7K"/>
<element name="R3" library="rcl" package="0207/10" value="4.7K"/>
<element name="R4" library="rcl" package="0207/10" value="4.7K"/>
<element name="R5" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC4" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R6" library="rcl" package="0207/10" value="4.7K"/>
<element name="R7" library="rcl" package="0207/10" value="4.7K"/>
<element name="R8" library="rcl" package="0207/10" value="4.7K"/>
<element name="R9" library="rcl" package="0207/10" value="4.7K"/>
<element name="R10" library="rcl" package="0207/10" value="4.7K"/>
<element name="R11" library="rcl" package="0207/10" value="4.7K"/>
<element name="R12" library="rcl" package="0207/10" value="4.7K"/>
<element name="R13" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC5" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R14" library="rcl" package="0207/10" value="4.7K"/>
<element name="R15" library="rcl" package="0207/10" value="4.7K"/>
<element name="R16" library="rcl" package="0207/10" value="4.7K"/>
<element name="R17" library="rcl" package="0207/10" value="4.7K"/>
<element name="R18" library="rcl" package="0207/10" value="4.7K"/>
<element name="R19" library="rcl" package="0207/10" value="4.7K"/>
<element name="R20" library="rcl" package="0207/10" value="4.7K"/>
<element name="R21" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC6" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R22" library="rcl" package="0207/10" value="4.7K"/>
<element name="R23" library="rcl" package="0207/10" value="4.7K"/>
<element name="R24" library="rcl" package="0207/10" value="4.7K"/>
<element name="R25" library="rcl" package="0207/10" value="4.7K"/>
<element name="R26" library="rcl" package="0207/10" value="4.7K"/>
<element name="R27" library="rcl" package="0207/10" value="4.7K"/>
<element name="R28" library="rcl" package="0207/10" value="4.7K"/>
<element name="R29" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC7" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R30" library="rcl" package="0207/10" value="4.7K"/>
<element name="R31" library="rcl" package="0207/10" value="4.7K"/>
<element name="R32" library="rcl" package="0207/10" value="4.7K"/>
<element name="R33" library="rcl" package="0207/10" value="4.7K"/>
<element name="R34" library="rcl" package="0207/10" value="4.7K"/>
<element name="R35" library="rcl" package="0207/10" value="4.7K"/>
<element name="R36" library="rcl" package="0207/10" value="4.7K"/>
<element name="R37" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC8" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R38" library="rcl" package="0207/10" value="4.7K"/>
<element name="R39" library="rcl" package="0207/10" value="4.7K"/>
<element name="R40" library="rcl" package="0207/10" value="4.7K"/>
<element name="R41" library="rcl" package="0207/10" value="4.7K"/>
<element name="R42" library="rcl" package="0207/10" value="4.7K"/>
<element name="R43" library="rcl" package="0207/10" value="4.7K"/>
<element name="R44" library="rcl" package="0207/10" value="4.7K"/>
<element name="R45" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC9" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R46" library="rcl" package="0207/10" value="4.7K"/>
<element name="R47" library="rcl" package="0207/10" value="4.7K"/>
<element name="R48" library="rcl" package="0207/10" value="4.7K"/>
<element name="R49" library="rcl" package="0207/10" value="4.7K"/>
<element name="R50" library="rcl" package="0207/10" value="4.7K"/>
<element name="R51" library="rcl" package="0207/10" value="4.7K"/>
<element name="R52" library="rcl" package="0207/10" value="4.7K"/>
<element name="R53" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC10" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R54" library="rcl" package="0207/10" value="4.7K"/>
<element name="R55" library="rcl" package="0207/10" value="4.7K"/>
<element name="R56" library="rcl" package="0207/10" value="4.7K"/>
<element name="R57" library="rcl" package="0207/10" value="4.7K"/>
<element name="R58" library="rcl" package="0207/10" value="4.7K"/>
<element name="R59" library="rcl" package="0207/10" value="4.7K"/>
<element name="R60" library="rcl" package="0207/10" value="4.7K"/>
<element name="R61" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC11" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R62" library="rcl" package="0207/10" value="4.7K"/>
<element name="R63" library="rcl" package="0207/10" value="4.7K"/>
<element name="R65" library="rcl" package="0207/10" value="4.7K"/>
<element name="R66" library="rcl" package="0207/10" value="4.7K"/>
<element name="R67" library="rcl" package="0207/10" value="4.7K"/>
<element name="R68" library="rcl" package="0207/10" value="4.7K"/>
<element name="R69" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC12" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R70" library="rcl" package="0207/10" value="4.7K"/>
<element name="R71" library="rcl" package="0207/10" value="4.7K"/>
<element name="R73" library="rcl" package="0207/10" value="4.7K"/>
<element name="R74" library="rcl" package="0207/10" value="4.7K"/>
<element name="R75" library="rcl" package="0207/10" value="4.7K"/>
<element name="R76" library="rcl" package="0207/10" value="4.7K"/>
<element name="R77" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC13" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R78" library="rcl" package="0207/10" value="4.7K"/>
<element name="R79" library="rcl" package="0207/10" value="4.7K"/>
<element name="R81" library="rcl" package="0207/10" value="4.7K"/>
<element name="R82" library="rcl" package="0207/10" value="4.7K"/>
<element name="R83" library="rcl" package="0207/10" value="4.7K"/>
<element name="R84" library="rcl" package="0207/10" value="4.7K"/>
<element name="R85" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC14" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R86" library="rcl" package="0207/10" value="4.7K"/>
<element name="R89" library="rcl" package="0207/10" value="4.7K"/>
<element name="R187" library="rcl" package="0207/10" value="4.7K"/>
<element name="R188" library="rcl" package="0207/10" value="4.7K"/>
<element name="R196" library="rcl" package="0207/10" value="4.7K"/>
<element name="R197" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC15" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="R198" library="rcl" package="0207/10" value="4.7K"/>
<element name="IC1" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="IC2" library="74xx-us" package="DIL20" value="74LS244N"/>
<element name="IC3" library="74xx-us" package="DIL20" value="74LS244N"/>
</elements>
<signals>
<signal name="+15V">
<contactref element="+V1" pad="1"/>
<contactref element="+V2" pad="1"/>
<contactref element="+V3" pad="1"/>
<contactref element="+V4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C40" pad="17"/>
<contactref element="C40" pad="19"/>
<contactref element="C40" pad="20"/>
<contactref element="C40" pad="18"/>
<contactref element="D40" pad="17"/>
<contactref element="D40" pad="19"/>
<contactref element="D40" pad="20"/>
<contactref element="D40" pad="18"/>
<contactref element="E40" pad="17"/>
<contactref element="E40" pad="19"/>
<contactref element="E40" pad="20"/>
<contactref element="E40" pad="18"/>
<contactref element="F40" pad="17"/>
<contactref element="F40" pad="19"/>
<contactref element="F40" pad="20"/>
<contactref element="F40" pad="18"/>
<contactref element="GND1" pad="1"/>
<contactref element="GND2" pad="1"/>
<contactref element="GND3" pad="1"/>
<contactref element="GND4" pad="1"/>
<contactref element="X1" pad="6"/>
<contactref element="X1" pad="9"/>
<contactref element="X1" pad="39"/>
<contactref element="X1" pad="30"/>
<contactref element="X1" pad="20"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC6" pad="10"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC8" pad="10"/>
<contactref element="IC9" pad="10"/>
<contactref element="IC10" pad="10"/>
<contactref element="IC11" pad="10"/>
<contactref element="IC12" pad="10"/>
<contactref element="IC13" pad="10"/>
<contactref element="IC14" pad="10"/>
<contactref element="IC15" pad="10"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="DF0">
<contactref element="C40" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="DF1">
<contactref element="C40" pad="10"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="DF2">
<contactref element="C40" pad="11"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="IF0">
<contactref element="C40" pad="24"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="ION">
<contactref element="D40" pad="34"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="PAUSE">
<contactref element="D40" pad="31"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="RUN">
<contactref element="D40" pad="33"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="IF1">
<contactref element="C40" pad="25"/>
<contactref element="R40" pad="2"/>
</signal>
<signal name="IF2">
<contactref element="C40" pad="34"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="FETCH">
<contactref element="D40" pad="24"/>
<contactref element="R70" pad="2"/>
</signal>
<signal name="EXECUTE">
<contactref element="D40" pad="28"/>
<contactref element="R78" pad="2"/>
</signal>
<signal name="DEFER">
<contactref element="D40" pad="26"/>
<contactref element="R86" pad="2"/>
</signal>
<signal name="WC">
<contactref element="D40" pad="30"/>
<contactref element="R198" pad="2"/>
</signal>
<signal name="CA">
<contactref element="D40" pad="32"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="BREAK">
<contactref element="D40" pad="22"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="LINK">
<contactref element="C40" pad="28"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="SC0">
<contactref element="C40" pad="9"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="SC1">
<contactref element="C40" pad="2"/>
<contactref element="R55" pad="2"/>
</signal>
<signal name="SC2">
<contactref element="C40" pad="23"/>
<contactref element="R63" pad="2"/>
</signal>
<signal name="SC3">
<contactref element="C40" pad="12"/>
<contactref element="R71" pad="2"/>
</signal>
<signal name="SC4">
<contactref element="C40" pad="33"/>
<contactref element="R79" pad="2"/>
</signal>
<signal name="AND">
<contactref element="D40" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="TAD">
<contactref element="D40" pad="4"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="ISZ">
<contactref element="D40" pad="6"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="DCA">
<contactref element="D40" pad="8"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="JMS">
<contactref element="D40" pad="10"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="JMP">
<contactref element="D40" pad="12"/>
<contactref element="R46" pad="2"/>
</signal>
<signal name="IOT">
<contactref element="D40" pad="23"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="OPR">
<contactref element="D40" pad="16"/>
<contactref element="R62" pad="2"/>
</signal>
<signal name="PC0">
<contactref element="E40" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PC1">
<contactref element="E40" pad="10"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="PC2">
<contactref element="E40" pad="11"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="PC3">
<contactref element="E40" pad="24"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="PC4">
<contactref element="E40" pad="25"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="PC5">
<contactref element="E40" pad="34"/>
<contactref element="R41" pad="2"/>
</signal>
<signal name="PC6">
<contactref element="F40" pad="1"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="PC7">
<contactref element="F40" pad="10"/>
<contactref element="R57" pad="2"/>
</signal>
<signal name="PC8">
<contactref element="F40" pad="11"/>
<contactref element="R65" pad="2"/>
</signal>
<signal name="MA0">
<contactref element="E40" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="MA1">
<contactref element="E40" pad="8"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="MA2">
<contactref element="E40" pad="13"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="MA3">
<contactref element="E40" pad="22"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="MA4">
<contactref element="E40" pad="27"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="MA5">
<contactref element="E40" pad="32"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="MA6">
<contactref element="F40" pad="3"/>
<contactref element="R50" pad="2"/>
</signal>
<signal name="MA7">
<contactref element="F40" pad="8"/>
<contactref element="R58" pad="2"/>
</signal>
<signal name="MA8">
<contactref element="F40" pad="13"/>
<contactref element="R66" pad="2"/>
</signal>
<signal name="MB0">
<contactref element="E40" pad="5"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="MB1">
<contactref element="E40" pad="6"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="MB2">
<contactref element="E40" pad="15"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="MB3">
<contactref element="E40" pad="16"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="MB4">
<contactref element="E40" pad="29"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="MB5">
<contactref element="E40" pad="30"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="MB6">
<contactref element="F40" pad="5"/>
<contactref element="R51" pad="2"/>
</signal>
<signal name="MB7">
<contactref element="F40" pad="6"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="MB8">
<contactref element="F40" pad="15"/>
<contactref element="R67" pad="2"/>
</signal>
<signal name="PC9">
<contactref element="F40" pad="24"/>
<contactref element="R73" pad="2"/>
</signal>
<signal name="PC10">
<contactref element="F40" pad="25"/>
<contactref element="R81" pad="2"/>
</signal>
<signal name="PC11">
<contactref element="F40" pad="34"/>
<contactref element="R89" pad="2"/>
</signal>
<signal name="MA11">
<contactref element="F40" pad="32"/>
<contactref element="R187" pad="2"/>
</signal>
<signal name="MA10">
<contactref element="F40" pad="27"/>
<contactref element="R82" pad="2"/>
</signal>
<signal name="MA9">
<contactref element="F40" pad="22"/>
<contactref element="R74" pad="2"/>
</signal>
<signal name="MB9">
<contactref element="F40" pad="16"/>
<contactref element="R75" pad="2"/>
</signal>
<signal name="MB10">
<contactref element="F40" pad="29"/>
<contactref element="R83" pad="2"/>
</signal>
<signal name="MB11">
<contactref element="F40" pad="30"/>
<contactref element="R188" pad="2"/>
</signal>
<signal name="AC0">
<contactref element="E40" pad="7"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="AC1">
<contactref element="E40" pad="4"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="AC2">
<contactref element="E40" pad="21"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="AC3">
<contactref element="E40" pad="14"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="AC4">
<contactref element="E40" pad="31"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="AC5">
<contactref element="E40" pad="28"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="AC6">
<contactref element="F40" pad="7"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="AC7">
<contactref element="F40" pad="4"/>
<contactref element="R60" pad="2"/>
</signal>
<signal name="AC8">
<contactref element="F40" pad="21"/>
<contactref element="R68" pad="2"/>
</signal>
<signal name="MQ8">
<contactref element="F40" pad="23"/>
<contactref element="R69" pad="2"/>
</signal>
<signal name="MQ7">
<contactref element="F40" pad="2"/>
<contactref element="R61" pad="2"/>
</signal>
<signal name="MQ6">
<contactref element="F40" pad="9"/>
<contactref element="R53" pad="2"/>
</signal>
<signal name="MQ0">
<contactref element="E40" pad="9"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="MQ1">
<contactref element="E40" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="MQ2">
<contactref element="E40" pad="23"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="MQ3">
<contactref element="E40" pad="12"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="MQ4">
<contactref element="E40" pad="33"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="MQ5">
<contactref element="E40" pad="26"/>
<contactref element="R45" pad="2"/>
</signal>
<signal name="AC9">
<contactref element="F40" pad="14"/>
<contactref element="R76" pad="2"/>
</signal>
<signal name="AC10">
<contactref element="F40" pad="31"/>
<contactref element="R84" pad="2"/>
</signal>
<signal name="AC11">
<contactref element="F40" pad="28"/>
<contactref element="R196" pad="2"/>
</signal>
<signal name="MQ11">
<contactref element="F40" pad="26"/>
<contactref element="R197" pad="2"/>
</signal>
<signal name="MQ10">
<contactref element="F40" pad="33"/>
<contactref element="R85" pad="2"/>
</signal>
<signal name="MQ9">
<contactref element="F40" pad="12"/>
<contactref element="R77" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="X1" pad="1"/>
<contactref element="X1" pad="17"/>
</signal>
<signal name="N$179">
<contactref element="X1" pad="3"/>
<contactref element="R91" pad="2"/>
</signal>
<signal name="N$180">
<contactref element="R90" pad="2"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="COL1">
<contactref element="IC4" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="COL2">
<contactref element="IC4" pad="19"/>
<contactref element="IC5" pad="19"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="N$181">
<contactref element="R92" pad="2"/>
<contactref element="X1" pad="7"/>
</signal>
<signal name="COL3">
<contactref element="IC6" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$182">
<contactref element="R93" pad="2"/>
<contactref element="X1" pad="11"/>
</signal>
<signal name="ROW2">
<contactref element="R93" pad="1"/>
</signal>
<signal name="SPARE">
<contactref element="X1" pad="35"/>
</signal>
<signal name="TX">
<contactref element="X1" pad="8"/>
</signal>
<signal name="RX">
<contactref element="X1" pad="10"/>
</signal>
<signal name="XLED8">
<contactref element="X1" pad="13"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="XLED3">
<contactref element="X1" pad="15"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$183">
<contactref element="X1" pad="26"/>
<contactref element="R94" pad="1"/>
</signal>
<signal name="COL6">
<contactref element="IC8" pad="19"/>
<contactref element="IC9" pad="19"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$184">
<contactref element="X1" pad="19"/>
<contactref element="R95" pad="1"/>
</signal>
<signal name="N$185">
<contactref element="X1" pad="21"/>
<contactref element="R96" pad="1"/>
</signal>
<signal name="N$186">
<contactref element="X1" pad="23"/>
<contactref element="R97" pad="1"/>
</signal>
<signal name="N$187">
<contactref element="X1" pad="24"/>
<contactref element="R98" pad="1"/>
</signal>
<signal name="COL10">
<contactref element="IC12" pad="19"/>
<contactref element="IC13" pad="19"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="COL9">
<contactref element="IC12" pad="1"/>
<contactref element="IC13" pad="1"/>
<contactref element="IC3" pad="18"/>
</signal>
<signal name="COL8">
<contactref element="IC10" pad="19"/>
<contactref element="IC11" pad="19"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="COL7">
<contactref element="IC10" pad="1"/>
<contactref element="IC11" pad="1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$188">
<contactref element="X1" pad="12"/>
<contactref element="R99" pad="2"/>
</signal>
<signal name="ROW3">
<contactref element="R99" pad="1"/>
</signal>
<signal name="COL4">
<contactref element="IC6" pad="19"/>
<contactref element="IC7" pad="19"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="COL5">
<contactref element="IC8" pad="1"/>
<contactref element="IC9" pad="1"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$191">
<contactref element="X1" pad="29"/>
<contactref element="R100" pad="2"/>
</signal>
<signal name="N$192">
<contactref element="X1" pad="31"/>
<contactref element="R101" pad="2"/>
</signal>
<signal name="COL12">
<contactref element="IC14" pad="19"/>
<contactref element="IC15" pad="19"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="N$190">
<contactref element="X1" pad="33"/>
<contactref element="R102" pad="2"/>
</signal>
<signal name="XLED7">
<contactref element="X1" pad="37"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="XLED1">
<contactref element="X1" pad="38"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="XLED2">
<contactref element="X1" pad="40"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$189">
<contactref element="R104" pad="2"/>
<contactref element="X1" pad="32"/>
</signal>
<signal name="COL11">
<contactref element="IC14" pad="1"/>
<contactref element="IC15" pad="1"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="N$194">
<contactref element="X1" pad="36"/>
<contactref element="R103" pad="2"/>
</signal>
<signal name="ROW1">
<contactref element="R103" pad="1"/>
</signal>
<signal name="XLED6">
<contactref element="X1" pad="22"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="XLED5">
<contactref element="X1" pad="18"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="XLED4">
<contactref element="X1" pad="16"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC5" pad="20"/>
<contactref element="IC6" pad="20"/>
<contactref element="IC7" pad="20"/>
<contactref element="IC8" pad="20"/>
<contactref element="IC9" pad="20"/>
<contactref element="IC10" pad="20"/>
<contactref element="IC11" pad="20"/>
<contactref element="IC12" pad="20"/>
<contactref element="IC13" pad="20"/>
<contactref element="IC14" pad="20"/>
<contactref element="IC15" pad="20"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC3" pad="20"/>
</signal>
<signal name="LED2">
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC6" pad="13"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC8" pad="13"/>
<contactref element="IC10" pad="4"/>
<contactref element="IC10" pad="13"/>
<contactref element="IC12" pad="4"/>
<contactref element="IC12" pad="13"/>
<contactref element="IC14" pad="4"/>
<contactref element="IC14" pad="13"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="LED3">
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="15"/>
<contactref element="IC6" pad="6"/>
<contactref element="IC6" pad="15"/>
<contactref element="IC8" pad="6"/>
<contactref element="IC8" pad="15"/>
<contactref element="IC10" pad="6"/>
<contactref element="IC10" pad="15"/>
<contactref element="IC12" pad="6"/>
<contactref element="IC12" pad="15"/>
<contactref element="IC14" pad="6"/>
<contactref element="IC14" pad="15"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="LED4">
<contactref element="IC4" pad="8"/>
<contactref element="IC4" pad="17"/>
<contactref element="IC6" pad="8"/>
<contactref element="IC6" pad="17"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC8" pad="17"/>
<contactref element="IC10" pad="8"/>
<contactref element="IC10" pad="17"/>
<contactref element="IC12" pad="8"/>
<contactref element="IC12" pad="17"/>
<contactref element="IC14" pad="8"/>
<contactref element="IC14" pad="17"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="LED7">
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="15"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="15"/>
<contactref element="IC9" pad="6"/>
<contactref element="IC9" pad="15"/>
<contactref element="IC11" pad="6"/>
<contactref element="IC11" pad="15"/>
<contactref element="IC13" pad="6"/>
<contactref element="IC13" pad="15"/>
<contactref element="IC15" pad="6"/>
<contactref element="IC15" pad="15"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="LED8">
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="17"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC7" pad="17"/>
<contactref element="IC9" pad="8"/>
<contactref element="IC9" pad="17"/>
<contactref element="IC11" pad="8"/>
<contactref element="IC11" pad="17"/>
<contactref element="IC13" pad="8"/>
<contactref element="IC13" pad="17"/>
<contactref element="IC15" pad="8"/>
<contactref element="IC15" pad="17"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="LED5">
<contactref element="IC5" pad="2"/>
<contactref element="IC5" pad="11"/>
<contactref element="IC7" pad="2"/>
<contactref element="IC7" pad="11"/>
<contactref element="IC9" pad="2"/>
<contactref element="IC9" pad="11"/>
<contactref element="IC11" pad="2"/>
<contactref element="IC11" pad="11"/>
<contactref element="IC13" pad="2"/>
<contactref element="IC13" pad="11"/>
<contactref element="IC15" pad="2"/>
<contactref element="IC15" pad="11"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="LED6">
<contactref element="IC5" pad="4"/>
<contactref element="IC5" pad="13"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC7" pad="13"/>
<contactref element="IC9" pad="4"/>
<contactref element="IC9" pad="13"/>
<contactref element="IC11" pad="4"/>
<contactref element="IC11" pad="13"/>
<contactref element="IC13" pad="4"/>
<contactref element="IC13" pad="13"/>
<contactref element="IC15" pad="4"/>
<contactref element="IC15" pad="13"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="XCOL7">
<contactref element="R98" pad="2"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="XCOL1">
<contactref element="R91" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="XCOL2">
<contactref element="R90" pad="1"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="XCOL3">
<contactref element="R92" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="XCOL4">
<contactref element="R100" pad="1"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="XCOL5">
<contactref element="R101" pad="1"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="XCOL6">
<contactref element="R94" pad="2"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="XCOL8">
<contactref element="R96" pad="2"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="XCOL9">
<contactref element="R95" pad="2"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="XCOL10">
<contactref element="R97" pad="2"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="XCOL11">
<contactref element="R104" pad="1"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="XCOL12">
<contactref element="R102" pad="1"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="LED1">
<contactref element="IC4" pad="2"/>
<contactref element="IC4" pad="11"/>
<contactref element="IC6" pad="2"/>
<contactref element="IC6" pad="11"/>
<contactref element="IC8" pad="2"/>
<contactref element="IC8" pad="11"/>
<contactref element="IC10" pad="2"/>
<contactref element="IC10" pad="11"/>
<contactref element="IC12" pad="2"/>
<contactref element="IC12" pad="11"/>
<contactref element="IC14" pad="2"/>
<contactref element="IC14" pad="11"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="IC4" pad="18"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="1"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="1"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="IC4" pad="16"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="IC5" pad="18"/>
</signal>
<signal name="N$6">
<contactref element="IC5" pad="16"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC5" pad="14"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="1"/>
<contactref element="IC5" pad="12"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="1"/>
<contactref element="IC4" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="R12" pad="1"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="R11" pad="1"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="R10" pad="1"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="R13" pad="1"/>
<contactref element="IC5" pad="9"/>
</signal>
<signal name="N$14">
<contactref element="IC5" pad="7"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC5" pad="5"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R16" pad="1"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="R17" pad="1"/>
<contactref element="IC6" pad="18"/>
</signal>
<signal name="N$18">
<contactref element="R20" pad="1"/>
<contactref element="IC6" pad="12"/>
</signal>
<signal name="N$19">
<contactref element="R19" pad="1"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="N$20">
<contactref element="R18" pad="1"/>
<contactref element="IC6" pad="16"/>
</signal>
<signal name="N$21">
<contactref element="R21" pad="1"/>
<contactref element="IC7" pad="18"/>
</signal>
<signal name="N$22">
<contactref element="IC7" pad="16"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="IC7" pad="14"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R24" pad="1"/>
<contactref element="IC7" pad="12"/>
</signal>
<signal name="N$25">
<contactref element="R25" pad="1"/>
<contactref element="IC6" pad="9"/>
</signal>
<signal name="N$26">
<contactref element="R28" pad="1"/>
<contactref element="IC6" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="R27" pad="1"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$28">
<contactref element="R26" pad="1"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="N$29">
<contactref element="R29" pad="1"/>
<contactref element="IC7" pad="9"/>
</signal>
<signal name="N$30">
<contactref element="IC7" pad="7"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="IC7" pad="5"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R32" pad="1"/>
<contactref element="IC7" pad="3"/>
</signal>
<signal name="N$33">
<contactref element="R33" pad="1"/>
<contactref element="IC8" pad="18"/>
</signal>
<signal name="N$34">
<contactref element="R36" pad="1"/>
<contactref element="IC8" pad="12"/>
</signal>
<signal name="N$35">
<contactref element="R35" pad="1"/>
<contactref element="IC8" pad="14"/>
</signal>
<signal name="N$36">
<contactref element="R34" pad="1"/>
<contactref element="IC8" pad="16"/>
</signal>
<signal name="N$37">
<contactref element="R37" pad="1"/>
<contactref element="IC9" pad="18"/>
</signal>
<signal name="N$38">
<contactref element="IC9" pad="16"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="IC9" pad="14"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="R40" pad="1"/>
<contactref element="IC9" pad="12"/>
</signal>
<signal name="N$41">
<contactref element="R41" pad="1"/>
<contactref element="IC8" pad="9"/>
</signal>
<signal name="N$42">
<contactref element="R44" pad="1"/>
<contactref element="IC8" pad="3"/>
</signal>
<signal name="N$43">
<contactref element="R43" pad="1"/>
<contactref element="IC8" pad="5"/>
</signal>
<signal name="N$44">
<contactref element="R42" pad="1"/>
<contactref element="IC8" pad="7"/>
</signal>
<signal name="N$45">
<contactref element="R45" pad="1"/>
<contactref element="IC9" pad="9"/>
</signal>
<signal name="N$46">
<contactref element="IC9" pad="7"/>
<contactref element="R46" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="IC9" pad="5"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="R48" pad="1"/>
<contactref element="IC9" pad="3"/>
</signal>
<signal name="N$49">
<contactref element="R49" pad="1"/>
<contactref element="IC10" pad="18"/>
</signal>
<signal name="N$50">
<contactref element="R52" pad="1"/>
<contactref element="IC10" pad="12"/>
</signal>
<signal name="N$51">
<contactref element="R51" pad="1"/>
<contactref element="IC10" pad="14"/>
</signal>
<signal name="N$52">
<contactref element="R50" pad="1"/>
<contactref element="IC10" pad="16"/>
</signal>
<signal name="N$53">
<contactref element="R53" pad="1"/>
<contactref element="IC11" pad="18"/>
</signal>
<signal name="N$54">
<contactref element="IC11" pad="16"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="IC11" pad="14"/>
<contactref element="R55" pad="1"/>
</signal>
<signal name="N$56">
<contactref element="R56" pad="1"/>
<contactref element="IC11" pad="12"/>
</signal>
<signal name="N$57">
<contactref element="R57" pad="1"/>
<contactref element="IC10" pad="9"/>
</signal>
<signal name="N$58">
<contactref element="R60" pad="1"/>
<contactref element="IC10" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="R59" pad="1"/>
<contactref element="IC10" pad="5"/>
</signal>
<signal name="N$60">
<contactref element="R58" pad="1"/>
<contactref element="IC10" pad="7"/>
</signal>
<signal name="N$61">
<contactref element="R61" pad="1"/>
<contactref element="IC11" pad="9"/>
</signal>
<signal name="N$62">
<contactref element="IC11" pad="7"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="IC11" pad="5"/>
<contactref element="R63" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="R65" pad="1"/>
<contactref element="IC12" pad="18"/>
</signal>
<signal name="N$66">
<contactref element="R68" pad="1"/>
<contactref element="IC12" pad="12"/>
</signal>
<signal name="N$67">
<contactref element="R67" pad="1"/>
<contactref element="IC12" pad="14"/>
</signal>
<signal name="N$68">
<contactref element="R66" pad="1"/>
<contactref element="IC12" pad="16"/>
</signal>
<signal name="N$69">
<contactref element="R69" pad="1"/>
<contactref element="IC13" pad="18"/>
</signal>
<signal name="N$70">
<contactref element="IC13" pad="16"/>
<contactref element="R70" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="IC13" pad="14"/>
<contactref element="R71" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="R73" pad="1"/>
<contactref element="IC12" pad="9"/>
</signal>
<signal name="N$74">
<contactref element="R76" pad="1"/>
<contactref element="IC12" pad="3"/>
</signal>
<signal name="N$75">
<contactref element="R75" pad="1"/>
<contactref element="IC12" pad="5"/>
</signal>
<signal name="N$76">
<contactref element="R74" pad="1"/>
<contactref element="IC12" pad="7"/>
</signal>
<signal name="N$77">
<contactref element="R77" pad="1"/>
<contactref element="IC13" pad="9"/>
</signal>
<signal name="N$78">
<contactref element="IC13" pad="7"/>
<contactref element="R78" pad="1"/>
</signal>
<signal name="N$79">
<contactref element="IC13" pad="5"/>
<contactref element="R79" pad="1"/>
</signal>
<signal name="N$81">
<contactref element="R81" pad="1"/>
<contactref element="IC14" pad="18"/>
</signal>
<signal name="N$82">
<contactref element="R84" pad="1"/>
<contactref element="IC14" pad="12"/>
</signal>
<signal name="N$83">
<contactref element="R83" pad="1"/>
<contactref element="IC14" pad="14"/>
</signal>
<signal name="N$84">
<contactref element="R82" pad="1"/>
<contactref element="IC14" pad="16"/>
</signal>
<signal name="N$85">
<contactref element="R85" pad="1"/>
<contactref element="IC15" pad="18"/>
</signal>
<signal name="N$86">
<contactref element="IC15" pad="16"/>
<contactref element="R86" pad="1"/>
</signal>
<signal name="N$89">
<contactref element="R89" pad="1"/>
<contactref element="IC14" pad="9"/>
</signal>
<signal name="N$90">
<contactref element="R196" pad="1"/>
<contactref element="IC14" pad="3"/>
</signal>
<signal name="N$91">
<contactref element="R188" pad="1"/>
<contactref element="IC14" pad="5"/>
</signal>
<signal name="N$92">
<contactref element="R187" pad="1"/>
<contactref element="IC14" pad="7"/>
</signal>
<signal name="N$93">
<contactref element="R197" pad="1"/>
<contactref element="IC15" pad="9"/>
</signal>
<signal name="N$94">
<contactref element="IC15" pad="7"/>
<contactref element="R198" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
