<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="20.955" width="0" layer="20"/>
<wire x1="0" y1="20.955" x2="12.065" y2="20.955" width="0" layer="20"/>
<wire x1="12.065" y1="20.955" x2="12.065" y2="0" width="0" layer="20"/>
<wire x1="12.065" y1="0" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="dec-con">
<description>DEC Edge Connectors and Parts</description>
<packages>
<package name="FSM4JAH">
<description>Footprint for the FSM4JAH 6mm SMD tactile switch.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SW2" library="dec-con" package="FSM4JAH" value="FSM4JAH"/>
<element name="SW1" library="dec-con" package="FSM4JAH" value="FSM4JAH"/>
</elements>
<signals>
<signal name="CENTER">
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="TOP">
<contactref element="SW2" pad="3"/>
<contactref element="SW2" pad="4"/>
</signal>
<signal name="BOT">
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
