<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="dec-m">
<packages>
<package name="H807">
<description>One-wide female edge connector</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C40" library="dec-m" package="H807" value="M900"/>
<element name="E40" library="dec-m" package="H807" value="M900"/>
<element name="F40" library="dec-m" package="H807" value="M900"/>
<element name="D40" library="dec-m" package="H807" value="M900"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C40" pad="T1"/>
<contactref element="C40" pad="C2"/>
<contactref element="E40" pad="T1"/>
<contactref element="E40" pad="C2"/>
<contactref element="F40" pad="T1"/>
<contactref element="F40" pad="C2"/>
<contactref element="D40" pad="T1"/>
<contactref element="D40" pad="C2"/>
</signal>
<signal name="VCC">
<contactref element="C40" pad="A2"/>
<contactref element="E40" pad="A2"/>
<contactref element="F40" pad="A2"/>
<contactref element="D40" pad="A2"/>
</signal>
<signal name="PC11">
<contactref element="F40" pad="D1"/>
</signal>
<signal name="MA1">
<contactref element="E40" pad="R2"/>
</signal>
<signal name="AND">
<contactref element="D40" pad="M2"/>
</signal>
<signal name="TAD">
<contactref element="D40" pad="T2"/>
</signal>
<signal name="OPR">
<contactref element="D40" pad="D2"/>
</signal>
<signal name="IOT">
<contactref element="D40" pad="N2"/>
</signal>
<signal name="JMP">
<contactref element="D40" pad="L2"/>
</signal>
<signal name="JMS">
<contactref element="D40" pad="S1"/>
</signal>
<signal name="DCA">
<contactref element="D40" pad="R2"/>
</signal>
<signal name="ISZ">
<contactref element="D40" pad="P1"/>
</signal>
<signal name="MB11">
<contactref element="F40" pad="A1"/>
</signal>
<signal name="CURRENT_ADDRESS">
<contactref element="D40" pad="E1"/>
</signal>
<signal name="ION">
<contactref element="D40" pad="D1"/>
</signal>
<signal name="RUN">
<contactref element="D40" pad="F1"/>
</signal>
<signal name="PAUSE">
<contactref element="D40" pad="M1"/>
</signal>
<signal name="FETCH">
<contactref element="D40" pad="N1"/>
</signal>
<signal name="EXECUTE">
<contactref element="D40" pad="B1"/>
</signal>
<signal name="DEFER">
<contactref element="D40" pad="H1"/>
</signal>
<signal name="WORD_COUNT">
<contactref element="D40" pad="A1"/>
</signal>
<signal name="BREAK">
<contactref element="D40" pad="E2"/>
</signal>
<signal name="AC0">
<contactref element="E40" pad="V2"/>
</signal>
<signal name="MQ11">
<contactref element="F40" pad="H1"/>
</signal>
<signal name="SC0">
<contactref element="C40" pad="S2"/>
</signal>
<signal name="DC1">
<contactref element="C40" pad="M2"/>
</signal>
<signal name="SC2">
<contactref element="C40" pad="N2"/>
</signal>
<signal name="SC3">
<contactref element="C40" pad="L2"/>
</signal>
<signal name="SC4">
<contactref element="C40" pad="F1"/>
</signal>
<signal name="MQ0">
<contactref element="E40" pad="S2"/>
</signal>
<signal name="MQ1">
<contactref element="E40" pad="M2"/>
</signal>
<signal name="MQ2">
<contactref element="E40" pad="N2"/>
</signal>
<signal name="MQ3">
<contactref element="E40" pad="L2"/>
</signal>
<signal name="MQ5">
<contactref element="E40" pad="H1"/>
</signal>
<signal name="MQ4">
<contactref element="E40" pad="F1"/>
</signal>
<signal name="MQ6">
<contactref element="F40" pad="S2"/>
</signal>
<signal name="MQ7">
<contactref element="F40" pad="M2"/>
</signal>
<signal name="MQ8">
<contactref element="F40" pad="N2"/>
</signal>
<signal name="MQ9">
<contactref element="F40" pad="L2"/>
</signal>
<signal name="MQ10">
<contactref element="F40" pad="F1"/>
</signal>
<signal name="AC11">
<contactref element="F40" pad="B1"/>
</signal>
<signal name="AC10">
<contactref element="F40" pad="M1"/>
</signal>
<signal name="AC9">
<contactref element="F40" pad="H2"/>
</signal>
<signal name="AC8">
<contactref element="F40" pad="J1"/>
</signal>
<signal name="AC7">
<contactref element="F40" pad="T2"/>
</signal>
<signal name="AC6">
<contactref element="F40" pad="V2"/>
</signal>
<signal name="AC5">
<contactref element="E40" pad="B1"/>
</signal>
<signal name="AC4">
<contactref element="E40" pad="M1"/>
</signal>
<signal name="AC3">
<contactref element="E40" pad="H2"/>
</signal>
<signal name="AC2">
<contactref element="E40" pad="J1"/>
</signal>
<signal name="AC1">
<contactref element="E40" pad="T2"/>
</signal>
<signal name="LINK">
<contactref element="C40" pad="B1"/>
</signal>
<signal name="MB0">
<contactref element="E40" pad="R1"/>
</signal>
<signal name="MB1">
<contactref element="E40" pad="P1"/>
</signal>
<signal name="MB2">
<contactref element="E40" pad="F2"/>
</signal>
<signal name="MB3">
<contactref element="E40" pad="D2"/>
</signal>
<signal name="MB4">
<contactref element="E40" pad="K1"/>
</signal>
<signal name="MB5">
<contactref element="E40" pad="A1"/>
</signal>
<signal name="MB6">
<contactref element="F40" pad="R1"/>
</signal>
<signal name="MB7">
<contactref element="F40" pad="P1"/>
</signal>
<signal name="MB8">
<contactref element="F40" pad="F2"/>
</signal>
<signal name="MB9">
<contactref element="F40" pad="D2"/>
</signal>
<signal name="MB10">
<contactref element="F40" pad="K1"/>
</signal>
<signal name="MA11">
<contactref element="F40" pad="E1"/>
</signal>
<signal name="MA10">
<contactref element="F40" pad="L1"/>
</signal>
<signal name="MA9">
<contactref element="F40" pad="E2"/>
</signal>
<signal name="MA7">
<contactref element="F40" pad="R2"/>
</signal>
<signal name="MA8">
<contactref element="F40" pad="K2"/>
</signal>
<signal name="MA6">
<contactref element="F40" pad="U2"/>
</signal>
<signal name="MA5">
<contactref element="E40" pad="E1"/>
</signal>
<signal name="MA4">
<contactref element="E40" pad="L1"/>
</signal>
<signal name="MA3">
<contactref element="E40" pad="E2"/>
</signal>
<signal name="MA2">
<contactref element="E40" pad="K2"/>
</signal>
<signal name="MA0">
<contactref element="E40" pad="U2"/>
</signal>
<signal name="DF0">
<contactref element="C40" pad="J2"/>
</signal>
<signal name="DF1">
<contactref element="C40" pad="S1"/>
</signal>
<signal name="DF2">
<contactref element="C40" pad="P2"/>
</signal>
<signal name="IF0">
<contactref element="C40" pad="N1"/>
</signal>
<signal name="IF1">
<contactref element="C40" pad="C1"/>
</signal>
<signal name="IF2">
<contactref element="C40" pad="D1"/>
</signal>
<signal name="PC0">
<contactref element="E40" pad="J2"/>
</signal>
<signal name="PC1">
<contactref element="E40" pad="S1"/>
</signal>
<signal name="PC2">
<contactref element="E40" pad="P2"/>
</signal>
<signal name="PC3">
<contactref element="E40" pad="N1"/>
</signal>
<signal name="PC4">
<contactref element="E40" pad="C1"/>
</signal>
<signal name="PC5">
<contactref element="E40" pad="D1"/>
</signal>
<signal name="PC6">
<contactref element="F40" pad="J2"/>
</signal>
<signal name="PC7">
<contactref element="F40" pad="S1"/>
</signal>
<signal name="PC8">
<contactref element="F40" pad="P2"/>
</signal>
<signal name="PC9">
<contactref element="F40" pad="N1"/>
</signal>
<signal name="PC10">
<contactref element="F40" pad="C1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
