<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>&lt;b&gt;Raspberry Pi&lt;/b&gt; by &lt;b&gt;Martin's Bastelstube&lt;/b&gt;
&lt;p&gt;
Different shapes of piggyback boards for the famous &amp;amp; fabulous
&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt; computer.
&lt;p&gt;
The outline of the Raspberry Pi board is drawn on layer 52 bDocu, so you can make it invisible if necessary.&lt;br/&gt;
Recommendation: Start your design with RASPI_BOARD_*_FULL, so you are aware of all the big components and
connectors when you're drawing the dimensions of your board and placing your own components.&lt;br/&gt;
Later, you can simply change the package of your Raspberry Pi connector to the RASPI_BOARD_*_EDGES type,
so you can concentrate on your own design.
&lt;p&gt;
Most of my board packages don't have the outline drawn in layer 20 Dimension (except the HATs). This allows you to deviate from the original Raspberry Pi board shape, e.g. when you need more space behind the GPIO connector for the routing of the power supply lines. If you want to stick exactly to the Raspberry Pi board shape, then just draw the Dimension layer right on the lines in layer bDocu.

&lt;hr&gt;&lt;br/&gt;

Version 1.3
&lt;ul&gt;
&lt;li&gt;Added the shape and dimensions of the HAT board with &amp;amp; without the camera and display flex cutout&lt;/li&gt;
&lt;li&gt;New GPIO connector version (suffix &amp;quot;#&amp;quot;) with all pins connected (no more &amp;quot;n.c.&amp;quot; pins)&lt;/li&gt;
&lt;li&gt;Two more &amp;quot;AB-&amp;quot; boards with 5 and 6 drill holes / pads, mechanically compatible with all RasPi versions&lt;/li&gt;
&lt;/ul&gt;

Version 1.2
&lt;ul&gt;
&lt;li&gt;Added a 26-pin GPIO connector with board dimensions of model B+&lt;br/&gt;
       for backwards compatibility with models A and B, named &amp;quot;B-&amp;quot;&lt;/li&gt;
&lt;/ul&gt;

Version 1.1
&lt;ul&gt;
&lt;li&gt;New GPIO connector and board dimensions of model B+&lt;/li&gt;
&lt;li&gt;Old connector and board (for models A and B) renamed to AB&lt;/li&gt;
&lt;li&gt;GPIO pin numbers on connector changed to match Rev2 board design&lt;/li&gt;
&lt;/ul&gt;

Version 1.0
&lt;ul&gt;
&lt;li&gt;More detailed descriptions for all components&lt;/li&gt;
&lt;li&gt;Published on Cadsoft webpage&lt;/li&gt;
&lt;/ul&gt;

&lt;hr&gt;&lt;br/&gt;

Designed by &lt;a href="http://bastelstube.rocci.net/"&gt;Martin's Bastelstube&lt;/a&gt;&lt;br&gt;
Comments / complaints / bug reports / suggestions to &lt;author&gt;eightbit@web.de&lt;/author&gt;</description>
<packages>
<package name="RASPI_GPIO_AB_PIN">
<description>26-pin connector for Raspberry Pi GPIO&lt;br/&gt;
 &amp;nbsp; just the two rows of pins</description>
</package>
<package name="RASPI_BOARD_AB_EDGES_2DRILL">
<description>Raspberry Pi board model A / B, outline is only marked by its edges&lt;br&gt;
including 2 drill holes for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_AB_FULL">
<description>Raspberry Pi board, full outline with position of big connectors + components&lt;br&gt;
including drill holes for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_AB_EDGES_1DRILL">
<description>Raspberry Pi board model A / B, outline is only marked by its edges&lt;br&gt;
including 1 drill hole for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_AB_THIN_DRILL">
<description>Raspberry Pi board
 - 
Thin version with only the width of the GPIO connector and 1 drill hole</description>
</package>
<package name="RASPI_GPIO_AB_BOX">
<description>26-pin box header for Raspberry Pi GPIO&lt;br/&gt;
 &amp;nbsp; for use with flat ribbon cables</description>
</package>
<package name="RASPI_BOARD_AB_EDGES_2DRILL_PAD">
<description>Raspberry Pi board model A / B, outline is only marked by its edges&lt;br&gt;
including 2 mounting pads for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_AB_EDGES_1DRILL_PAD">
<description>Raspberry Pi board model A / B, outline is only marked by its edges&lt;br&gt;
including 1 mounting pad for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_AB_FULL_PAD">
<description>Raspberry Pi board, full outline with position of big connectors + components&lt;br&gt;
including mounting pads for Model B Revision 2.0</description>
</package>
<package name="RASPI_BOARD_AB_THIN_PAD">
<description>Raspberry Pi board
 - 
Thin version with only the width of the GPIO connector and 1 mounting pad</description>
</package>
<package name="RASPI_BOARD_AB_THIN_BOT">
<description>Raspberry Pi board - Thin version with only the width of the GPIO connector and 1 drill hole&lt;p/&gt;
Pads are in "Offset" shape to make them easy to solder from the bottom side&lt;br/&gt;
for single-side PCBs</description>
</package>
<package name="RASPI_BOARD_AB_EDGES_0DRILL">
<description>Raspberry Pi board model A / B, outline is only marked by its edges&lt;br&gt;
without any drill holes</description>
</package>
<package name="RASPI_BOARD_AB_THIN">
<description>Raspberry Pi board
 - 
Thin version with only the width of the GPIO connector</description>
</package>
<package name="RASPI_GPIO_B+_PIN">
<description>40-pin connector for Raspberry Pi GPIO model B+&lt;br/&gt;
 &amp;nbsp; just the two rows of pins</description>
</package>
<package name="RASPI_GPIO_B+_BOX">
<description>40-pin box header for Raspberry Pi GPIO model B+&lt;br/&gt;
 &amp;nbsp; for use with flat ribbon cables</description>
</package>
<package name="RASPI_BOARD_B+_FULL">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes</description>
</package>
<package name="RASPI_BOARD_B+_FULL_PAD">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; mounting pads</description>
</package>
<package name="RASPI_BOARD_B+_EDGES_4DRILL">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
with all 4 drill holes</description>
</package>
<package name="RASPI_BOARD_B+_EDGES_0DRILL">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br&gt;
without any drill holes</description>
</package>
<package name="RASPI_BOARD_B+_EDGES_4DRILL_PAD">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
with all 4 mounting pads</description>
</package>
<package name="RASPI_BOARD_B+_EDGES_3DRILL">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br&gt;
with 3 drill holes (top left hole is missing to allow routing of power supply lines)</description>
</package>
<package name="RASPI_BOARD_B+_EDGES_3DRILL_PAD">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br&gt;
with 3 mounting pads (top left pad is missing to allow routing of power supply lines)</description>
</package>
<package name="RASPI_BOARD_B-_FULL">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B</description>
</package>
<package name="RASPI_BOARD_B-_FULL_PAD">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; mounting pads&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B</description>
</package>
<package name="RASPI_BOARD_B-_EDGES_3DRILL">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with only 3 drill holes (top left hole is missing to allow routing of power supply lines)</description>
</package>
<package name="RASPI_BOARD_B-_EDGES_3DRILL_PAD">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with only 3 mounting pads (top left hole is missing to allow routing of power supply lines)</description>
</package>
<package name="RASPI_BOARD_B-_EDGES_4DRILL">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with all 4 drill holes</description>
</package>
<package name="RASPI_BOARD_B-_EDGES_4DRILL_PAD">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with all 4 mounting pads</description>
</package>
<package name="RASPI_BOARD_B-_EDGES_2DRILL">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with only 2 drill holes (both top holes are missing)</description>
</package>
<package name="RASPI_BOARD_B-_EDGES_2DRILL_PAD">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with only 2 mounting pads (both top pads are missing)</description>
</package>
<package name="RASPI_BOARD_B+HAT_DF_CF">
<description>Raspberry Pi board model B+ HAT board&lt;br/&gt;
Official outline with cutouts for display &amp;amp; camera flex connector</description>
</package>
<package name="RASPI_BOARD_B+HAT_DF">
<description>Raspberry Pi board model B+ HAT board&lt;br/&gt;
Official outline with cutout for display flex connector</description>
</package>
<package name="RASPI_BOARD_B+HAT">
<description>Raspberry Pi board model B+ HAT board&lt;br/&gt;
Official outline, but without cutouts for display &amp;amp; camera flex connector</description>
</package>
<package name="RASPI_BOARD_AB+_FULL">
<description>Raspberry Pi board model A, B, B+, full outline with position of big connectors &amp;amp; all 6 drill holes</description>
</package>
<package name="RASPI_BOARD_AB+_FULL_PAD">
<description>Raspberry Pi board model A, B, B+, full outline with position of big connectors &amp;amp; all 6 mounting pads</description>
</package>
<package name="RASPI_BOARD_AB-_FULL">
<description>Raspberry Pi board model A, B, B+, full outline with position of big connectors &amp;amp; all 6 drill holes&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B</description>
</package>
<package name="RASPI_BOARD_AB-_FULL_PAD">
<description>Raspberry Pi board model A, B, B+, full outline with position of big connectors &amp;amp; all 6 mounting pads&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B</description>
</package>
<package name="RASPI_BOARD_AB-_EDGES_6DRILL">
<description>Raspberry Pi board model A, B, B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with all 6 drill holes</description>
</package>
<package name="RASPI_BOARD_AB-_EDGES_6DRILL_PAD">
<description>Raspberry Pi board model A, B, B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with all 6 mounting pads</description>
</package>
<package name="RASPI_BOARD_AB-_EDGES_5DRILL">
<description>Raspberry Pi board model A, B, B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with 5 drill holes</description>
</package>
<package name="RASPI_BOARD_AB-_EDGES_5DRILL_PAD">
<description>Raspberry Pi board model A, B, B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with 5 mounting pads</description>
</package>
<package name="RASPI_BOARD_B-_EDGES_0DRILL">
<description>Raspberry Pi board model A, B, B+, outline is only marked by its edges&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
without any drill holes</description>
</package>
</packages>
<symbols>
<symbol name="RASPI_GPIO_AB">
<pin name="5V0" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO27"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO24"/>
<pin name="GPIO25"/>
<pin name="GPIO04"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="SPI_SCLK"/>
<pin name="SPI_CE0"/>
<pin name="SPI_CE1"/>
<pin name="N.C.0" direction="nc"/>
<pin name="N.C.1" direction="nc"/>
<pin name="N.C.2" direction="nc"/>
<pin name="N.C.3" direction="nc"/>
<pin name="N.C.4" direction="nc"/>
<pin name="N.C.5" direction="nc"/>
</symbol>
<symbol name="RASPI_GPIO_B+">
<pin name="5V0" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO27"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO24"/>
<pin name="GPIO25"/>
<pin name="GPIO04"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="SPI_SCLK"/>
<pin name="SPI_CE0"/>
<pin name="SPI_CE1"/>
<pin name="N.C.0" direction="nc"/>
<pin name="N.C.1" direction="nc"/>
<pin name="N.C.2" direction="nc"/>
<pin name="N.C.3" direction="nc"/>
<pin name="N.C.4" direction="nc"/>
<pin name="N.C.5" direction="nc"/>
<pin name="ID_SC" direction="nc"/>
<pin name="ID_SD" direction="nc"/>
<pin name="GPIO05" direction="nc"/>
<pin name="GPIO06" direction="nc"/>
<pin name="GPIO12" direction="nc"/>
<pin name="GPIO13" direction="nc"/>
<pin name="GPIO19" direction="nc"/>
<pin name="GPIO16" direction="nc"/>
<pin name="GPIO26" direction="nc"/>
<pin name="GPIO20" direction="nc"/>
<pin name="GPIO21" direction="nc"/>
<pin name="N.C.6" direction="nc"/>
<pin name="N.C.7" direction="nc"/>
<pin name="N.C.8" direction="nc"/>
</symbol>
<symbol name="RASPI_GPIO_AB#">
<pin name="5V0A" direction="pwr"/>
<pin name="3V3A" direction="pwr"/>
<pin name="GND_F" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO27"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO24"/>
<pin name="GPIO25"/>
<pin name="GPIO04"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="SPI_SCLK"/>
<pin name="SPI_CE0"/>
<pin name="SPI_CE1"/>
<pin name="5V0B" direction="pwr"/>
<pin name="3V3B" direction="pwr"/>
<pin name="GND_A" direction="pwr"/>
<pin name="GND_B" direction="pwr"/>
<pin name="GND_C" direction="pwr"/>
<pin name="GND_E" direction="pwr"/>
</symbol>
<symbol name="RASPI_GPIO_B+#">
<pin name="5V0A" direction="pwr"/>
<pin name="3V3A" direction="pwr"/>
<pin name="GND_A" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO27"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO24"/>
<pin name="GPIO25"/>
<pin name="GPIO04"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="SPI_SCLK"/>
<pin name="SPI_CE0"/>
<pin name="SPI_CE1"/>
<pin name="5V0B" direction="pwr"/>
<pin name="3V3B" direction="pwr"/>
<pin name="GND_B" direction="pwr"/>
<pin name="GND_C" direction="pwr"/>
<pin name="GND_D" direction="pwr"/>
<pin name="GND_E" direction="pwr"/>
<pin name="ID_SC" direction="nc"/>
<pin name="ID_SD" direction="nc"/>
<pin name="GPIO05" direction="nc"/>
<pin name="GPIO06" direction="nc"/>
<pin name="GPIO12" direction="nc"/>
<pin name="GPIO13" direction="nc"/>
<pin name="GPIO19" direction="nc"/>
<pin name="GPIO16" direction="nc"/>
<pin name="GPIO26" direction="nc"/>
<pin name="GPIO20" direction="nc"/>
<pin name="GPIO21" direction="nc"/>
<pin name="GND_F" direction="pwr"/>
<pin name="GND_G" direction="pwr"/>
<pin name="GND_H" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RASPI_GPIO_AB" prefix="X">
<description>Only the 2x13 header connector, nothing else</description>
<gates>
<gate name="G$1" symbol="RASPI_GPIO_AB"/>
</gates>
<devices>
<device name="_PIN" package="RASPI_GPIO_AB_PIN">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_BOX" package="RASPI_GPIO_AB_BOX">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_BOARD_AB" prefix="X">
<description>Raspberry Pi GPIO connector with markings for the outer dimensions of the Raspberry Pi board model A or B&lt;br&gt;
with different sets of drill holes or mounting pads for model B Revision 2.0</description>
<gates>
<gate name="G$1" symbol="RASPI_GPIO_AB"/>
</gates>
<devices>
<device name="_E2" package="RASPI_BOARD_AB_EDGES_2DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_F" package="RASPI_BOARD_AB_FULL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E1" package="RASPI_BOARD_AB_EDGES_1DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TD" package="RASPI_BOARD_AB_THIN_DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E1P" package="RASPI_BOARD_AB_EDGES_1DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E2P" package="RASPI_BOARD_AB_EDGES_2DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_FP" package="RASPI_BOARD_AB_FULL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TP" package="RASPI_BOARD_AB_THIN_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TB" package="RASPI_BOARD_AB_THIN_BOT">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E0" package="RASPI_BOARD_AB_EDGES_0DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_T" package="RASPI_BOARD_AB_THIN">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_GPIO_B+" prefix="X">
<description>Only the 2x20 header connector, nothing else</description>
<gates>
<gate name="G$1" symbol="RASPI_GPIO_B+"/>
</gates>
<devices>
<device name="_BOX" package="RASPI_GPIO_B+_BOX">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PIN" package="RASPI_GPIO_B+_PIN">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_BOARD_B+" prefix="X">
<description>Raspberry Pi GPIO connector with markings for the outer dimensions of the Raspberry Pi board model B+&lt;br&gt;
with different sets of drill holes or mounting pads</description>
<gates>
<gate name="G$1" symbol="RASPI_GPIO_B+"/>
</gates>
<devices>
<device name="_F" package="RASPI_BOARD_B+_FULL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_FP" package="RASPI_BOARD_B+_FULL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E0" package="RASPI_BOARD_B+_EDGES_0DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4" package="RASPI_BOARD_B+_EDGES_4DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4P" package="RASPI_BOARD_B+_EDGES_4DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3" package="RASPI_BOARD_B+_EDGES_3DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3P" package="RASPI_BOARD_B+_EDGES_3DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_H" package="RASPI_BOARD_B+HAT">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HD" package="RASPI_BOARD_B+HAT_DF">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HDC" package="RASPI_BOARD_B+HAT_DF_CF">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO05" pad="29"/>
<connect gate="G$1" pin="GPIO06" pad="31"/>
<connect gate="G$1" pin="GPIO12" pad="32"/>
<connect gate="G$1" pin="GPIO13" pad="33"/>
<connect gate="G$1" pin="GPIO16" pad="36"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO19" pad="35"/>
<connect gate="G$1" pin="GPIO20" pad="38"/>
<connect gate="G$1" pin="GPIO21" pad="40"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO26" pad="37"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="N.C.6" pad="30"/>
<connect gate="G$1" pin="N.C.7" pad="34"/>
<connect gate="G$1" pin="N.C.8" pad="39"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_BOARD_B-" prefix="X">
<description>Raspberry Pi GPIO connector with markings for the outer dimensions of the Raspberry Pi board model B+&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with different sets of drill holes or mounting pads</description>
<gates>
<gate name="G$1" symbol="RASPI_GPIO_AB"/>
</gates>
<devices>
<device name="_F" package="RASPI_BOARD_B-_FULL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_FP" package="RASPI_BOARD_B-_FULL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3" package="RASPI_BOARD_B-_EDGES_3DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3P" package="RASPI_BOARD_B-_EDGES_3DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4" package="RASPI_BOARD_B-_EDGES_4DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4P" package="RASPI_BOARD_B-_EDGES_4DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E2" package="RASPI_BOARD_B-_EDGES_2DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E2P" package="RASPI_BOARD_B-_EDGES_2DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E6" package="RASPI_BOARD_AB-_EDGES_6DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E6P" package="RASPI_BOARD_AB-_EDGES_6DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E5" package="RASPI_BOARD_AB-_EDGES_5DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E5P" package="RASPI_BOARD_AB-_EDGES_5DRILL_PAD">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E0" package="RASPI_BOARD_B-_EDGES_0DRILL">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_GPIO_AB#" prefix="X">
<description>2x13 header connector, all pins connected</description>
<gates>
</gates>
<devices>
<device name="_BOX" package="RASPI_GPIO_AB_BOX">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PIN" package="RASPI_GPIO_AB_PIN">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_GPIO_B+#" prefix="X">
<description>2x20 header connector, all pins connected</description>
<gates>
</gates>
<devices>
<device name="_BOX" package="RASPI_GPIO_B+_BOX">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PIN" package="RASPI_GPIO_B+_PIN">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_BOARD_B+#" prefix="X">
<description>Raspberry Pi GPIO connector with markings for the outer dimensions of the Raspberry Pi board model B+&lt;br&gt;
with different sets of drill holes or mounting pads&lt;br/&gt;
All pins connected</description>
<gates>
</gates>
<devices>
<device name="_F" package="RASPI_BOARD_B+_FULL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_FP" package="RASPI_BOARD_B+_FULL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E0" package="RASPI_BOARD_B+_EDGES_0DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3" package="RASPI_BOARD_B+_EDGES_3DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3P" package="RASPI_BOARD_B+_EDGES_3DRILL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4" package="RASPI_BOARD_B+_EDGES_4DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4P" package="RASPI_BOARD_B+_EDGES_4DRILL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_H" package="RASPI_BOARD_B+HAT">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HD" package="RASPI_BOARD_B+HAT_DF">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HDC" package="RASPI_BOARD_B+HAT_DF_CF">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPI_BOARD_B-#" prefix="X">
<description>Raspberry Pi GPIO connector with markings for the outer dimensions of the Raspberry Pi board model B+&lt;br/&gt;
GPIO connector reduced to 26 pins to match models A and B&lt;br/&gt;
with different sets of drill holes or mounting pads&lt;br/&gt;
All pins connected</description>
<gates>
</gates>
<devices>
<device name="_F" package="RASPI_BOARD_B-_FULL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_FP" package="RASPI_BOARD_B-_FULL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E0" package="RASPI_BOARD_B-_EDGES_0DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E2" package="RASPI_BOARD_B-_EDGES_2DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E2P" package="RASPI_BOARD_B-_EDGES_2DRILL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3" package="RASPI_BOARD_B-_EDGES_3DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E3P" package="RASPI_BOARD_B-_EDGES_3DRILL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4" package="RASPI_BOARD_B-_EDGES_4DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E4P" package="RASPI_BOARD_B-_EDGES_4DRILL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E5" package="RASPI_BOARD_AB-_EDGES_5DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E5P" package="RASPI_BOARD_AB-_EDGES_5DRILL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E6" package="RASPI_BOARD_AB-_EDGES_6DRILL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_E6P" package="RASPI_BOARD_AB-_EDGES_6DRILL_PAD">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
