<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="266.7" width="0" layer="20"/>
<wire x1="0" y1="266.7" x2="406.4" y2="266.7" width="0" layer="20"/>
<wire x1="406.4" y1="266.7" x2="406.4" y2="0" width="0" layer="20"/>
<wire x1="406.4" y1="0" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="dec-m">
<packages>
<package name="H807">
<description>One-wide female edge connector</description>
</package>
<package name="H807-2">
<description>Two-wide Female Edge Connector</description>
</package>
<package name="CBLOCK">
<description>Connector block outline with mounting holes.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B08" library="dec-m" package="H807" value="M216"/>
<element name="B07" library="dec-m" package="H807" value=""/>
<element name="A32" library="dec-m" package="H807" value="W033"/>
<element name="AB02" library="dec-m" package="H807-2" value="G826"/>
<element name="AB01" library="dec-m" package="H807-2" value="G805"/>
<element name="A25" library="dec-m" package="H807" value="G624"/>
<element name="B24" library="dec-m" package="H807" value="G624"/>
<element name="B25" library="dec-m" package="H807" value="G624"/>
<element name="A24" library="dec-m" package="H807" value="G624"/>
<element name="A03" library="dec-m" package="H807" value="H807"/>
<element name="A04" library="dec-m" package="H807" value="H807"/>
<element name="A05" library="dec-m" package="H807" value="H807"/>
<element name="A06" library="dec-m" package="H807" value="H807"/>
<element name="B03" library="dec-m" package="H807" value="H807"/>
<element name="B04" library="dec-m" package="H807" value="H807"/>
<element name="B05" library="dec-m" package="H807" value="H807"/>
<element name="D01" library="dec-m" package="H807" value="H807"/>
<element name="D02" library="dec-m" package="H807" value="H807"/>
<element name="D03" library="dec-m" package="H807" value="H807"/>
<element name="D04" library="dec-m" package="H807" value="H807"/>
<element name="D05" library="dec-m" package="H807" value="H807"/>
<element name="D06" library="dec-m" package="H807" value="H807"/>
<element name="D07" library="dec-m" package="H807" value="H807"/>
<element name="D08" library="dec-m" package="H807" value="H807"/>
<element name="D09" library="dec-m" package="H807" value="H807"/>
<element name="D10" library="dec-m" package="H807" value="H807"/>
<element name="C01" library="dec-m" package="H807" value="H807"/>
<element name="C02" library="dec-m" package="H807" value="H807"/>
<element name="C03" library="dec-m" package="H807" value="H807"/>
<element name="C04" library="dec-m" package="H807" value="H807"/>
<element name="C05" library="dec-m" package="H807" value="H807"/>
<element name="C06" library="dec-m" package="H807" value="H807"/>
<element name="C07" library="dec-m" package="H807" value="H807"/>
<element name="C08" library="dec-m" package="H807" value="H807"/>
<element name="C09" library="dec-m" package="H807" value="H807"/>
<element name="C10" library="dec-m" package="H807" value="H807"/>
<element name="A26" library="dec-m" package="H807" value="H807"/>
<element name="A27" library="dec-m" package="H807" value="H807"/>
<element name="B26" library="dec-m" package="H807" value="H807"/>
<element name="B27" library="dec-m" package="H807" value="H807"/>
<element name="C26" library="dec-m" package="H807" value="H807"/>
<element name="C27" library="dec-m" package="H807" value="H807"/>
<element name="C28" library="dec-m" package="H807" value="H807"/>
<element name="C29" library="dec-m" package="H807" value="H807"/>
<element name="C30" library="dec-m" package="H807" value="H807"/>
<element name="C31" library="dec-m" package="H807" value="H807"/>
<element name="C32" library="dec-m" package="H807" value="H807"/>
<element name="B28" library="dec-m" package="H807" value="H807"/>
<element name="B29" library="dec-m" package="H807" value="H807"/>
<element name="B30" library="dec-m" package="H807" value="H807"/>
<element name="B31" library="dec-m" package="H807" value="H807"/>
<element name="B32" library="dec-m" package="H807" value="H807"/>
<element name="D27" library="dec-m" package="H807" value="H807"/>
<element name="B16" library="dec-m" package="H807" value=""/>
<element name="D32" library="dec-m" package="H807" value="W033"/>
<element name="A07" library="dec-m" package="H807" value="M310"/>
<element name="A08" library="dec-m" package="H807" value="M310"/>
<element name="C25" library="dec-m" package="H807" value="G228"/>
<element name="D25" library="dec-m" package="H807" value="G228"/>
<element name="A09" library="dec-m" package="H807" value="M310"/>
<element name="B06" library="dec-m" package="H807" value=""/>
<element name="A10" library="dec-m" package="H807" value="M310"/>
<element name="U$1" library="dec-m" package="CBLOCK" value=""/>
<element name="U$2" library="dec-m" package="CBLOCK" value=""/>
<element name="U$3" library="dec-m" package="CBLOCK" value=""/>
<element name="U$4" library="dec-m" package="CBLOCK" value=""/>
<element name="U$5" library="dec-m" package="CBLOCK" value=""/>
<element name="U$6" library="dec-m" package="CBLOCK" value=""/>
<element name="U$7" library="dec-m" package="CBLOCK" value=""/>
<element name="U$8" library="dec-m" package="CBLOCK" value=""/>
<element name="U$9" library="dec-m" package="CBLOCK" value=""/>
<element name="U$10" library="dec-m" package="CBLOCK" value=""/>
<element name="U$11" library="dec-m" package="CBLOCK" value=""/>
<element name="U$12" library="dec-m" package="CBLOCK" value=""/>
<element name="U$13" library="dec-m" package="CBLOCK" value=""/>
<element name="U$14" library="dec-m" package="CBLOCK" value=""/>
<element name="U$15" library="dec-m" package="CBLOCK" value=""/>
<element name="U$16" library="dec-m" package="CBLOCK" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="B08" pad="A2"/>
<contactref element="B07" pad="A2"/>
<contactref element="AB02" pad="AA2"/>
<contactref element="AB02" pad="BA2"/>
<contactref element="B16" pad="A2"/>
<contactref element="A07" pad="A2"/>
<contactref element="A08" pad="A2"/>
<contactref element="C25" pad="A2"/>
<contactref element="D25" pad="A2"/>
<contactref element="A09" pad="A2"/>
<contactref element="B06" pad="A2"/>
<contactref element="A10" pad="A2"/>
</signal>
<signal name="GND">
<contactref element="AB01" pad="BC2"/>
<contactref element="B08" pad="J1"/>
<contactref element="A24" pad="E2"/>
<contactref element="B25" pad="E2"/>
<contactref element="B08" pad="P1"/>
<contactref element="B08" pad="M2"/>
<contactref element="B08" pad="C2"/>
<contactref element="B08" pad="T1"/>
<contactref element="B07" pad="T1"/>
<contactref element="B07" pad="C2"/>
<contactref element="A32" pad="C2"/>
<contactref element="A32" pad="F2"/>
<contactref element="A32" pad="J2"/>
<contactref element="A32" pad="L2"/>
<contactref element="A32" pad="N2"/>
<contactref element="A32" pad="R2"/>
<contactref element="A32" pad="U2"/>
<contactref element="AB02" pad="AC2"/>
<contactref element="AB02" pad="BC2"/>
<contactref element="AB01" pad="BD2"/>
<contactref element="AB01" pad="BE2"/>
<contactref element="AB01" pad="BF2"/>
<contactref element="AB01" pad="BH2"/>
<contactref element="AB01" pad="BJ2"/>
<contactref element="AB01" pad="BK2"/>
<contactref element="AB01" pad="BL2"/>
<contactref element="B16" pad="C2"/>
<contactref element="B16" pad="T1"/>
<contactref element="D32" pad="C2"/>
<contactref element="D32" pad="F2"/>
<contactref element="D32" pad="J2"/>
<contactref element="D32" pad="L2"/>
<contactref element="D32" pad="N2"/>
<contactref element="D32" pad="R2"/>
<contactref element="D32" pad="U2"/>
<contactref element="A07" pad="C2"/>
<contactref element="A07" pad="T1"/>
<contactref element="A08" pad="C2"/>
<contactref element="A08" pad="T1"/>
<contactref element="C25" pad="C2"/>
<contactref element="D25" pad="C2"/>
<contactref element="A09" pad="C2"/>
<contactref element="A09" pad="T1"/>
<contactref element="B06" pad="T1"/>
<contactref element="B06" pad="C2"/>
<contactref element="A10" pad="C2"/>
<contactref element="A10" pad="T1"/>
<contactref element="AB01" pad="AP2"/>
<contactref element="AB01" pad="AR2"/>
<contactref element="AB01" pad="AS2"/>
<contactref element="AB01" pad="AT2"/>
<contactref element="AB01" pad="AU2"/>
<contactref element="C25" pad="T1"/>
<contactref element="D25" pad="T1"/>
</signal>
<signal name="-30V@4">
<contactref element="AB02" pad="BV2"/>
<contactref element="AB01" pad="AE2"/>
</signal>
<signal name="-6V@3">
<contactref element="AB01" pad="BM2"/>
<contactref element="AB02" pad="BM2"/>
<contactref element="B24" pad="E2"/>
<contactref element="A25" pad="E2"/>
</signal>
<signal name="N$1">
<contactref element="AB01" pad="AV2"/>
<contactref element="AB02" pad="BJ2"/>
<contactref element="AB02" pad="BK2"/>
</signal>
<signal name="-15V">
<contactref element="AB02" pad="AB2"/>
<contactref element="B25" pad="B2"/>
<contactref element="A24" pad="B2"/>
<contactref element="B24" pad="B2"/>
<contactref element="A25" pad="B2"/>
</signal>
<signal name="STOP_OK">
<contactref element="AB02" pad="AH2"/>
</signal>
<signal name="!SHUT_DOWN">
<contactref element="AB02" pad="AF2"/>
</signal>
<signal name="!PWR_CLR">
<contactref element="AB02" pad="AS2"/>
<contactref element="B08" pad="A1"/>
<contactref element="B08" pad="K2"/>
</signal>
<signal name="!PWR_OK">
<contactref element="AB02" pad="AJ2"/>
</signal>
<signal name="EA1">
<contactref element="B07" pad="M1"/>
</signal>
<signal name="!EA0">
<contactref element="B07" pad="L1"/>
<contactref element="B07" pad="K2"/>
</signal>
<signal name="N$5">
<contactref element="B07" pad="N1"/>
<contactref element="B16" pad="R2"/>
</signal>
<signal name="+3V@B07V1">
<contactref element="B16" pad="S2"/>
<contactref element="B16" pad="T2"/>
<contactref element="B16" pad="U2"/>
<contactref element="B07" pad="V1"/>
<contactref element="B16" pad="B1"/>
<contactref element="B16" pad="C1"/>
<contactref element="B16" pad="D1"/>
<contactref element="B16" pad="F2"/>
<contactref element="B16" pad="E2"/>
<contactref element="B16" pad="D2"/>
<contactref element="B16" pad="H1"/>
<contactref element="B16" pad="J1"/>
<contactref element="B16" pad="K1"/>
<contactref element="B16" pad="N1"/>
<contactref element="B16" pad="P1"/>
<contactref element="B16" pad="R1"/>
<contactref element="B16" pad="L2"/>
<contactref element="B16" pad="M2"/>
<contactref element="B16" pad="N2"/>
</signal>
<signal name="N$6">
<contactref element="B16" pad="V2"/>
<contactref element="B08" pad="B1"/>
<contactref element="B07" pad="D1"/>
</signal>
<signal name="MEM_START">
<contactref element="B07" pad="E1"/>
<contactref element="A32" pad="M2"/>
<contactref element="B08" pad="C1"/>
<contactref element="D32" pad="M2"/>
</signal>
<signal name="N$7">
<contactref element="B07" pad="F1"/>
<contactref element="B07" pad="A1"/>
</signal>
<signal name="+3V@B07U1">
<contactref element="B07" pad="B1"/>
<contactref element="B07" pad="U1"/>
<contactref element="B08" pad="D1"/>
<contactref element="B07" pad="J2"/>
<contactref element="B07" pad="E2"/>
<contactref element="B07" pad="H1"/>
<contactref element="B08" pad="F2"/>
</signal>
<signal name="MEM_ENABLE">
<contactref element="B08" pad="E1"/>
<contactref element="B06" pad="B1"/>
</signal>
<signal name="!MEM_ENABLE">
<contactref element="B08" pad="F1"/>
<contactref element="B16" pad="A1"/>
</signal>
<signal name="B_MEM_ENABLE">
<contactref element="B16" pad="E1"/>
</signal>
<signal name="EA0">
<contactref element="B07" pad="H2"/>
</signal>
<signal name="!EA2">
<contactref element="B08" pad="E2"/>
</signal>
<signal name="N$8">
<contactref element="B07" pad="C1"/>
<contactref element="B08" pad="D2"/>
</signal>
<signal name="!FIELD">
<contactref element="B08" pad="J2"/>
<contactref element="B16" pad="H2"/>
</signal>
<signal name="FIELD">
<contactref element="B08" pad="H2"/>
<contactref element="B16" pad="F1"/>
</signal>
<signal name="B_FIELD">
<contactref element="B16" pad="J2"/>
</signal>
<signal name="!B_FIELD">
<contactref element="B16" pad="L1"/>
</signal>
<signal name="!READ">
<contactref element="B08" pad="M1"/>
</signal>
<signal name="READ">
<contactref element="B08" pad="L1"/>
<contactref element="C25" pad="D2"/>
<contactref element="C25" pad="M2"/>
<contactref element="D25" pad="D1"/>
<contactref element="D25" pad="L1"/>
</signal>
<signal name="N$9">
<contactref element="A07" pad="H1"/>
<contactref element="A07" pad="M2"/>
</signal>
<signal name="N$10">
<contactref element="A07" pad="E1"/>
<contactref element="A07" pad="K2"/>
</signal>
<signal name="N$11">
<contactref element="A07" pad="F1"/>
<contactref element="B16" pad="M1"/>
</signal>
<signal name="!MEM_BEGIN">
<contactref element="B16" pad="S1"/>
<contactref element="B08" pad="K1"/>
</signal>
<signal name="N$12">
<contactref element="A07" pad="J1"/>
<contactref element="A08" pad="H2"/>
</signal>
<signal name="N$13">
<contactref element="A08" pad="E1"/>
<contactref element="A08" pad="T2"/>
</signal>
<signal name="N$14">
<contactref element="A08" pad="F1"/>
<contactref element="B08" pad="H1"/>
</signal>
<signal name="-30V@3">
<contactref element="AB01" pad="AN2"/>
<contactref element="AB01" pad="AM2"/>
<contactref element="B24" pad="U2"/>
<contactref element="B24" pad="J2"/>
<contactref element="B25" pad="U2"/>
<contactref element="B25" pad="J2"/>
<contactref element="B25" pad="H2"/>
</signal>
<signal name="-30V@2">
<contactref element="AB01" pad="AL2"/>
<contactref element="AB01" pad="AK2"/>
<contactref element="A25" pad="M2"/>
<contactref element="B24" pad="H2"/>
</signal>
<signal name="-30V@1">
<contactref element="AB01" pad="AJ2"/>
<contactref element="A25" pad="H2"/>
</signal>
<signal name="-30V@6">
<contactref element="AB01" pad="AH2"/>
</signal>
<signal name="-30V@5">
<contactref element="AB01" pad="AF2"/>
</signal>
<signal name="-6V@1">
<contactref element="AB01" pad="BN2"/>
<contactref element="AB01" pad="BP2"/>
<contactref element="A24" pad="H2"/>
</signal>
<signal name="-6V@2">
<contactref element="AB01" pad="BR2"/>
<contactref element="AB01" pad="BS2"/>
<contactref element="A24" pad="U2"/>
<contactref element="A24" pad="J2"/>
<contactref element="A25" pad="J2"/>
<contactref element="A25" pad="U2"/>
</signal>
<signal name="-6V@4">
<contactref element="AB01" pad="BT2"/>
</signal>
<signal name="-6V@5">
<contactref element="AB01" pad="BU2"/>
</signal>
<signal name="-6V@6">
<contactref element="AB01" pad="BV2"/>
</signal>
<signal name="NEG_CLAMP">
<contactref element="A25" pad="R2"/>
</signal>
<signal name="X_SOURCE">
<contactref element="C25" pad="F2"/>
<contactref element="C25" pad="K1"/>
<contactref element="A25" pad="D2"/>
</signal>
<signal name="Y_SOURCE">
<contactref element="C25" pad="P2"/>
<contactref element="C25" pad="S1"/>
<contactref element="B24" pad="D2"/>
</signal>
<signal name="Y_RETURN">
<contactref element="D25" pad="S1"/>
<contactref element="D25" pad="P2"/>
<contactref element="A24" pad="D2"/>
</signal>
<signal name="X_RETURN">
<contactref element="D25" pad="F2"/>
<contactref element="D25" pad="K1"/>
<contactref element="B25" pad="D2"/>
</signal>
<signal name="N$19">
<contactref element="C25" pad="M1"/>
<contactref element="B25" pad="F2"/>
<contactref element="D25" pad="M1"/>
</signal>
<signal name="N$20">
<contactref element="B24" pad="F2"/>
<contactref element="C25" pad="E1"/>
<contactref element="D25" pad="E1"/>
</signal>
<signal name="N$3">
<contactref element="D25" pad="L2"/>
<contactref element="C25" pad="L2"/>
<contactref element="A25" pad="F2"/>
</signal>
<signal name="N$4">
<contactref element="C25" pad="U2"/>
<contactref element="D25" pad="U2"/>
<contactref element="A24" pad="F2"/>
</signal>
<signal name="V2">
<contactref element="C25" pad="V2"/>
<contactref element="D25" pad="V2"/>
</signal>
<signal name="WRITE">
<contactref element="C25" pad="D1"/>
<contactref element="C25" pad="L1"/>
<contactref element="D25" pad="D2"/>
<contactref element="D25" pad="M2"/>
<contactref element="B08" pad="S1"/>
</signal>
<signal name="+3V@B16U1">
<contactref element="D25" pad="N2"/>
<contactref element="D25" pad="E2"/>
<contactref element="D25" pad="A1"/>
<contactref element="C25" pad="N2"/>
<contactref element="C25" pad="E2"/>
<contactref element="C25" pad="A1"/>
<contactref element="B16" pad="U1"/>
</signal>
<signal name="BTP2">
<contactref element="A32" pad="V2"/>
<contactref element="D32" pad="V2"/>
<contactref element="B06" pad="A1"/>
</signal>
<signal name="N$2">
<contactref element="B06" pad="C1"/>
<contactref element="B06" pad="E1"/>
<contactref element="B06" pad="D1"/>
</signal>
<signal name="N$15">
<contactref element="B06" pad="F1"/>
<contactref element="A09" pad="H2"/>
</signal>
<signal name="N$16">
<contactref element="A09" pad="K2"/>
<contactref element="A09" pad="E1"/>
</signal>
<signal name="N$17">
<contactref element="A09" pad="L2"/>
<contactref element="A09" pad="H1"/>
</signal>
<signal name="N$18">
<contactref element="A09" pad="F1"/>
<contactref element="B07" pad="D2"/>
</signal>
<signal name="N$21">
<contactref element="B08" pad="N2"/>
<contactref element="B07" pad="F2"/>
</signal>
<signal name="N$22">
<contactref element="B08" pad="R2"/>
<contactref element="B16" pad="K2"/>
</signal>
<signal name="B_INHIBIT">
<contactref element="B16" pad="P2"/>
</signal>
<signal name="INHIBIT">
<contactref element="B08" pad="P2"/>
</signal>
<signal name="N$23">
<contactref element="A09" pad="J1"/>
<contactref element="A10" pad="H2"/>
<contactref element="B07" pad="J1"/>
</signal>
<signal name="N$24">
<contactref element="A10" pad="E1"/>
<contactref element="A10" pad="T2"/>
</signal>
<signal name="MEM_FINISH">
<contactref element="A10" pad="F1"/>
<contactref element="B08" pad="L2"/>
<contactref element="B08" pad="N1"/>
</signal>
<signal name="!MEM_DONE">
<contactref element="D32" pad="S2"/>
<contactref element="A32" pad="S2"/>
</signal>
<signal name="N$25">
<contactref element="B07" pad="K1"/>
<contactref element="B08" pad="R1"/>
</signal>
<signal name="!WRITE">
<contactref element="B08" pad="U1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
