<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="dec-con">
<packages>
<package name="OMNIBUS">
<description>Quad-Height DEC board</description>
</package>
<package name="EDGE-CON8">
<description>Quad-Height DEC edge connector</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL40">
<description>40 pin wide DIP</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="memory-hitachi">
<packages>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="memory">
<packages>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pal">
<packages>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="XILINX">
<packages>
<package name="PLCC-S44">
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="dec-con" package="OMNIBUS" value="OUTLINE-OMNIBUS"/>
<element name="U$2" library="dec-con" package="EDGE-CON8" value=""/>
<element name="E1" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="E2" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="E3" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="IC2" library="74xx-us" package="DIL20" value="74HC244N"/>
<element name="IC3" library="74xx-us" package="DIL20" value="74HC244N"/>
<element name="IC4" library="74xx-us" package="DIL20" value="74HC244N"/>
<element name="IC5" library="dec-con" package="DIL40" value="IM6102"/>
<element name="IC1" library="dec-con" package="DIL40" value="IM6100"/>
<element name="E4" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="E5" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="E6" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="IC8" library="74xx-us" package="DIL20" value="74LS373N"/>
<element name="IC9" library="74xx-us" package="DIL20" value="74LS373N"/>
<element name="E7" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="IC6" library="74xx-us" package="DIL14" value="74LS04N"/>
<element name="IC7" library="74xx-us" package="DIL14" value="74AS02N"/>
<element name="E8" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="IC11" library="74xx-us" package="DIL14" value="74LS08N"/>
<element name="IC10" library="74xx-us" package="DIL14" value="74LS74N"/>
<element name="E9" library="dec-con" package="DIL16" value="AM26S10"/>
<element name="IC12" library="74xx-us" package="DIL20" value="74LS373N"/>
<element name="IC13" library="74xx-us" package="DIL20" value="74LS373N"/>
<element name="IC16" library="memory" package="DIL28" value=""/>
<element name="IC17" library="memory" package="DIL28" value=""/>
<element name="U$3" library="dec-con" package="DIL32" value="628512P"/>
<element name="U$4" library="dec-con" package="DIL32" value="628512P"/>
<element name="IC20" library="memory-hitachi" package="DIL32" value="628128P">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC14" library="memory-hitachi" package="DIL28-3" value="CY7C199">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC15" library="memory-hitachi" package="DIL28-3" value="CY7C199">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC18" library="74xx-us" package="DIL14" value="74LS74N"/>
<element name="IC24" library="pal" package="DIL24-3" value="22V10">
<attribute name="OC_NEWARK" value="97M0480"/>
<attribute name="MPN" value="GAL22V10D-7LPN"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1571925"/>
</element>
<element name="IC25" library="pal" package="DIL24-3" value="22V10">
<attribute name="OC_NEWARK" value="97M0480"/>
<attribute name="MPN" value="GAL22V10D-7LPN"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1571925"/>
</element>
<element name="IC19" library="pal" package="DIL20" value="16V8">
<attribute name="OC_NEWARK" value="97K0449"/>
<attribute name="MPN" value="GAL16V8D-7LPN"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9699740"/>
</element>
<element name="IC21" library="74xx-us" package="DIL14" value="74HC05N"/>
<element name="IC22" library="74xx-us" package="DIL14" value="74LS74N"/>
<element name="IC23" library="74xx-us" package="DIL14" value="74AS02N"/>
<element name="IC26" library="XILINX" package="PLCC-S44" value=""/>
</elements>
<signals>
<signal name="MA0_L">
<contactref element="U$2" pad="AD1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="AF1"/>
<contactref element="U$2" pad="AN1"/>
<contactref element="U$2" pad="AT1"/>
<contactref element="U$2" pad="AC2"/>
<contactref element="U$2" pad="AF2"/>
<contactref element="U$2" pad="AN2"/>
<contactref element="U$2" pad="AT2"/>
<contactref element="U$2" pad="BC1"/>
<contactref element="U$2" pad="BF1"/>
<contactref element="U$2" pad="BN1"/>
<contactref element="U$2" pad="BT1"/>
<contactref element="U$2" pad="BC2"/>
<contactref element="U$2" pad="BF2"/>
<contactref element="U$2" pad="BN2"/>
<contactref element="U$2" pad="BT2"/>
<contactref element="U$2" pad="CC1"/>
<contactref element="U$2" pad="CF1"/>
<contactref element="U$2" pad="CN1"/>
<contactref element="U$2" pad="CT1"/>
<contactref element="U$2" pad="CT2"/>
<contactref element="U$2" pad="CN2"/>
<contactref element="U$2" pad="CF2"/>
<contactref element="U$2" pad="CC2"/>
<contactref element="U$2" pad="DC1"/>
<contactref element="U$2" pad="DF1"/>
<contactref element="U$2" pad="DN1"/>
<contactref element="U$2" pad="DT1"/>
<contactref element="U$2" pad="DC2"/>
<contactref element="U$2" pad="DF2"/>
<contactref element="U$2" pad="DN2"/>
<contactref element="U$2" pad="DT2"/>
<contactref element="E1" pad="8"/>
<contactref element="E1" pad="1"/>
<contactref element="E2" pad="8"/>
<contactref element="E2" pad="1"/>
<contactref element="E3" pad="8"/>
<contactref element="E3" pad="1"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC5" pad="29"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC1" pad="26"/>
<contactref element="E4" pad="8"/>
<contactref element="E4" pad="1"/>
<contactref element="E5" pad="8"/>
<contactref element="E5" pad="1"/>
<contactref element="E6" pad="8"/>
<contactref element="E6" pad="1"/>
<contactref element="E4" pad="12"/>
<contactref element="E6" pad="12"/>
<contactref element="E5" pad="12"/>
<contactref element="IC8" pad="10"/>
<contactref element="IC9" pad="10"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC8" pad="17"/>
<contactref element="IC8" pad="18"/>
<contactref element="IC9" pad="1"/>
<contactref element="IC9" pad="17"/>
<contactref element="IC9" pad="18"/>
<contactref element="E7" pad="8"/>
<contactref element="E7" pad="1"/>
<contactref element="IC6" pad="7"/>
<contactref element="IC7" pad="7"/>
<contactref element="E8" pad="8"/>
<contactref element="E8" pad="1"/>
<contactref element="E8" pad="12"/>
<contactref element="IC5" pad="26"/>
<contactref element="IC11" pad="7"/>
<contactref element="IC10" pad="7"/>
<contactref element="E9" pad="8"/>
<contactref element="E9" pad="1"/>
<contactref element="E9" pad="12"/>
<contactref element="IC12" pad="10"/>
<contactref element="IC13" pad="10"/>
<contactref element="IC12" pad="1"/>
<contactref element="IC13" pad="1"/>
<contactref element="IC16" pad="14"/>
<contactref element="IC17" pad="14"/>
<contactref element="IC13" pad="18"/>
<contactref element="IC18" pad="7"/>
<contactref element="IC10" pad="2"/>
<contactref element="IC24" pad="12"/>
<contactref element="IC25" pad="12"/>
<contactref element="IC19" pad="10"/>
<contactref element="IC21" pad="7"/>
<contactref element="IC22" pad="7"/>
<contactref element="IC23" pad="7"/>
<contactref element="IC26" pad="23"/>
<contactref element="IC26" pad="10"/>
<contactref element="IC26" pad="31"/>
</signal>
<signal name="MA1_L">
<contactref element="U$2" pad="AE1"/>
</signal>
<signal name="MA3_L">
<contactref element="U$2" pad="AJ1"/>
</signal>
<signal name="MD0_L">
<contactref element="U$2" pad="AK1"/>
<contactref element="E6" pad="9"/>
</signal>
<signal name="DATA3_L">
<contactref element="U$2" pad="AV1"/>
<contactref element="E1" pad="2"/>
</signal>
<signal name="DATA2_L">
<contactref element="U$2" pad="AU1"/>
<contactref element="E1" pad="7"/>
</signal>
<signal name="DATA1_L">
<contactref element="U$2" pad="AS1"/>
<contactref element="E1" pad="15"/>
</signal>
<signal name="DATA0_L">
<contactref element="U$2" pad="AR1"/>
<contactref element="E1" pad="9"/>
</signal>
<signal name="MD3_L">
<contactref element="U$2" pad="AP1"/>
<contactref element="E6" pad="2"/>
</signal>
<signal name="MD1_L">
<contactref element="U$2" pad="AL1"/>
<contactref element="E6" pad="15"/>
</signal>
<signal name="MA2_L">
<contactref element="U$2" pad="AH1"/>
</signal>
<signal name="MD2_L">
<contactref element="U$2" pad="AM1"/>
<contactref element="E6" pad="7"/>
</signal>
<signal name="-15V">
<contactref element="U$2" pad="AB2"/>
<contactref element="U$2" pad="BB2"/>
<contactref element="U$2" pad="CB2"/>
<contactref element="U$2" pad="DB2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="AA2"/>
<contactref element="U$2" pad="BA2"/>
<contactref element="U$2" pad="CA2"/>
<contactref element="U$2" pad="DA2"/>
<contactref element="E1" pad="16"/>
<contactref element="E2" pad="16"/>
<contactref element="E3" pad="16"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC3" pad="20"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="34"/>
<contactref element="E4" pad="16"/>
<contactref element="E5" pad="16"/>
<contactref element="E6" pad="16"/>
<contactref element="IC8" pad="20"/>
<contactref element="IC9" pad="20"/>
<contactref element="E7" pad="16"/>
<contactref element="IC6" pad="14"/>
<contactref element="E7" pad="12"/>
<contactref element="E7" pad="4"/>
<contactref element="E7" pad="5"/>
<contactref element="E7" pad="11"/>
<contactref element="E7" pad="13"/>
<contactref element="IC7" pad="14"/>
<contactref element="E8" pad="16"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC11" pad="14"/>
<contactref element="IC10" pad="14"/>
<contactref element="E9" pad="16"/>
<contactref element="IC12" pad="20"/>
<contactref element="IC13" pad="20"/>
<contactref element="IC16" pad="28"/>
<contactref element="IC17" pad="28"/>
<contactref element="IC18" pad="14"/>
<contactref element="IC24" pad="24"/>
<contactref element="IC25" pad="24"/>
<contactref element="IC18" pad="10"/>
<contactref element="IC19" pad="20"/>
<contactref element="IC21" pad="14"/>
<contactref element="IC22" pad="14"/>
<contactref element="IC22" pad="2"/>
<contactref element="IC22" pad="4"/>
<contactref element="IC23" pad="14"/>
<contactref element="IC26" pad="21"/>
<contactref element="IC26" pad="41"/>
<contactref element="IC26" pad="32"/>
<contactref element="IC20" pad="32"/>
<contactref element="IC14" pad="28"/>
<contactref element="IC15" pad="28"/>
<contactref element="U$3" pad="32"/>
<contactref element="U$4" pad="32"/>
</signal>
<signal name="INHIBIT_H">
<contactref element="U$2" pad="AP2"/>
</signal>
<signal name="EMA0_L">
<contactref element="U$2" pad="AD2"/>
<contactref element="E9" pad="9"/>
</signal>
<signal name="EMA1_L">
<contactref element="U$2" pad="AE2"/>
<contactref element="E9" pad="7"/>
</signal>
<signal name="EMA2_L">
<contactref element="U$2" pad="AH2"/>
<contactref element="E9" pad="2"/>
</signal>
<signal name="MEM_START_L">
<contactref element="U$2" pad="AJ2"/>
</signal>
<signal name="MD_DIR_L">
<contactref element="U$2" pad="AK2"/>
</signal>
<signal name="SOURCE_H">
<contactref element="U$2" pad="AL2"/>
</signal>
<signal name="STROBE_H">
<contactref element="U$2" pad="AM2"/>
</signal>
<signal name="WRITE_H">
<contactref element="U$2" pad="AS2"/>
</signal>
<signal name="LINK_L">
<contactref element="U$2" pad="AV2"/>
</signal>
<signal name="ROM_ADDRESS_L">
<contactref element="U$2" pad="AU2"/>
</signal>
<signal name="RETURN_H">
<contactref element="U$2" pad="AR2"/>
</signal>
<signal name="MA4_L">
<contactref element="U$2" pad="BD1"/>
</signal>
<signal name="DATA7_L">
<contactref element="U$2" pad="BV1"/>
<contactref element="E2" pad="2"/>
</signal>
<signal name="DATA6_L">
<contactref element="U$2" pad="BU1"/>
<contactref element="E2" pad="7"/>
</signal>
<signal name="DATA5_L">
<contactref element="U$2" pad="BS1"/>
<contactref element="E2" pad="15"/>
</signal>
<signal name="DATA4_L">
<contactref element="U$2" pad="BR1"/>
<contactref element="E2" pad="9"/>
</signal>
<signal name="MD7_L">
<contactref element="U$2" pad="BP1"/>
<contactref element="E5" pad="2"/>
</signal>
<signal name="MD6_L">
<contactref element="U$2" pad="BM1"/>
<contactref element="E5" pad="7"/>
</signal>
<signal name="MD5_L">
<contactref element="U$2" pad="BL1"/>
<contactref element="E5" pad="15"/>
</signal>
<signal name="MD4_L">
<contactref element="U$2" pad="BK1"/>
<contactref element="E5" pad="9"/>
</signal>
<signal name="MA7_L">
<contactref element="U$2" pad="BJ1"/>
</signal>
<signal name="MA6_L">
<contactref element="U$2" pad="BH1"/>
</signal>
<signal name="MA5_L">
<contactref element="U$2" pad="BE1"/>
</signal>
<signal name="BREAK_CYCLE_L">
<contactref element="U$2" pad="BL2"/>
</signal>
<signal name="POWER_OK_H">
<contactref element="U$2" pad="BV2"/>
</signal>
<signal name="RUN_L">
<contactref element="U$2" pad="BU2"/>
</signal>
<signal name="RES2_H">
<contactref element="U$2" pad="BS2"/>
</signal>
<signal name="RES1_H">
<contactref element="U$2" pad="BR2"/>
</signal>
<signal name="INT_IN_PROG_H">
<contactref element="U$2" pad="BP2"/>
</signal>
<signal name="LA_ENABLE_L">
<contactref element="U$2" pad="BM2"/>
</signal>
<signal name="INT_STROBE_H">
<contactref element="U$2" pad="BD2"/>
</signal>
<signal name="BRK_IN_PROG_L">
<contactref element="U$2" pad="BE2"/>
</signal>
<signal name="MA_MS_LOAD_CONT_L">
<contactref element="U$2" pad="BH2"/>
</signal>
<signal name="OVERFLOW_L">
<contactref element="U$2" pad="BJ2"/>
</signal>
<signal name="BREAK_DATA_CONT_L">
<contactref element="U$2" pad="BK2"/>
</signal>
<signal name="MS_IR_DISABLE_L">
<contactref element="U$2" pad="CV1"/>
</signal>
<signal name="IO_PAUSE_L">
<contactref element="U$2" pad="CD1"/>
<contactref element="E8" pad="2"/>
</signal>
<signal name="C1_L">
<contactref element="U$2" pad="CH1"/>
<contactref element="E7" pad="7"/>
</signal>
<signal name="C2_L">
<contactref element="U$2" pad="CJ1"/>
</signal>
<signal name="BUS_STROBE_L">
<contactref element="U$2" pad="CK1"/>
</signal>
<signal name="INTERNAL_IO_L">
<contactref element="U$2" pad="CL1"/>
</signal>
<signal name="NOT_LAST_XFER_L">
<contactref element="U$2" pad="CM1"/>
</signal>
<signal name="INT_RQST_L">
<contactref element="U$2" pad="CP1"/>
<contactref element="E7" pad="15"/>
</signal>
<signal name="INITIALIZE_H">
<contactref element="U$2" pad="CR1"/>
</signal>
<signal name="SKIP_L">
<contactref element="U$2" pad="CS1"/>
<contactref element="E7" pad="9"/>
</signal>
<signal name="CPMA_DISABLE_L">
<contactref element="U$2" pad="CU1"/>
</signal>
<signal name="C0_L">
<contactref element="U$2" pad="CE1"/>
<contactref element="E7" pad="2"/>
</signal>
<signal name="IND2_L">
<contactref element="U$2" pad="CV2"/>
</signal>
<signal name="IND1_L">
<contactref element="U$2" pad="CU2"/>
</signal>
<signal name="LINK_LOAD_L">
<contactref element="U$2" pad="CS2"/>
</signal>
<signal name="LINK_DATA_L">
<contactref element="U$2" pad="CR2"/>
</signal>
<signal name="TS4_L">
<contactref element="U$2" pad="CP2"/>
</signal>
<signal name="TS3_L">
<contactref element="U$2" pad="CM2"/>
</signal>
<signal name="TS2_L">
<contactref element="U$2" pad="CL2"/>
</signal>
<signal name="TS1_L">
<contactref element="U$2" pad="CK2"/>
</signal>
<signal name="TP4_H">
<contactref element="U$2" pad="CJ2"/>
</signal>
<signal name="TP3_H">
<contactref element="U$2" pad="CH2"/>
<contactref element="E8" pad="7"/>
</signal>
<signal name="TP2_H">
<contactref element="U$2" pad="CE2"/>
</signal>
<signal name="TP1_H">
<contactref element="U$2" pad="CD2"/>
</signal>
<signal name="MA8_L">
<contactref element="U$2" pad="DD1"/>
</signal>
<signal name="DATA11_L">
<contactref element="U$2" pad="DV1"/>
<contactref element="E3" pad="2"/>
</signal>
<signal name="DATA10_L">
<contactref element="U$2" pad="DU1"/>
<contactref element="E3" pad="7"/>
</signal>
<signal name="DATA9_L">
<contactref element="U$2" pad="DS1"/>
<contactref element="E3" pad="15"/>
</signal>
<signal name="DATA8_L">
<contactref element="U$2" pad="DR1"/>
<contactref element="E3" pad="9"/>
</signal>
<signal name="MD11_L">
<contactref element="U$2" pad="DP1"/>
<contactref element="E4" pad="2"/>
</signal>
<signal name="MD10_L">
<contactref element="U$2" pad="DM1"/>
<contactref element="E4" pad="15"/>
</signal>
<signal name="MD9_L">
<contactref element="U$2" pad="DL1"/>
<contactref element="E4" pad="7"/>
</signal>
<signal name="MD8_L">
<contactref element="U$2" pad="DK1"/>
<contactref element="E4" pad="9"/>
</signal>
<signal name="MA11_L">
<contactref element="U$2" pad="DJ1"/>
</signal>
<signal name="MA10_L">
<contactref element="U$2" pad="DH1"/>
</signal>
<signal name="MA9_L">
<contactref element="U$2" pad="DE1"/>
</signal>
<signal name="SW">
<contactref element="U$2" pad="DV2"/>
</signal>
<signal name="IR0_L">
<contactref element="U$2" pad="DD2"/>
</signal>
<signal name="IR1_L">
<contactref element="U$2" pad="DE2"/>
</signal>
<signal name="F_L">
<contactref element="U$2" pad="DJ2"/>
</signal>
<signal name="D_L">
<contactref element="U$2" pad="DK2"/>
</signal>
<signal name="USER_MODE_H">
<contactref element="U$2" pad="DM2"/>
</signal>
<signal name="E_L">
<contactref element="U$2" pad="DL2"/>
</signal>
<signal name="F_SET_L">
<contactref element="U$2" pad="DP2"/>
</signal>
<signal name="PULSE_LA_H">
<contactref element="U$2" pad="DR2"/>
</signal>
<signal name="STOP_L">
<contactref element="U$2" pad="DS2"/>
</signal>
<signal name="KEY_CONTROL_L">
<contactref element="U$2" pad="DU2"/>
</signal>
<signal name="IR2_L">
<contactref element="U$2" pad="DH2"/>
</signal>
<signal name="SP_GND">
<contactref element="U$2" pad="AC1"/>
</signal>
<signal name="DX11">
<contactref element="E3" pad="4"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC5" pad="28"/>
<contactref element="IC1" pad="28"/>
<contactref element="IC12" pad="3"/>
<contactref element="IC25" pad="6"/>
</signal>
<signal name="DX0">
<contactref element="E1" pad="11"/>
<contactref element="IC4" pad="12"/>
<contactref element="IC5" pad="16"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC13" pad="3"/>
<contactref element="IC25" pad="13"/>
</signal>
<signal name="DX1">
<contactref element="E1" pad="13"/>
<contactref element="IC4" pad="14"/>
<contactref element="IC5" pad="17"/>
<contactref element="IC1" pad="17"/>
<contactref element="IC13" pad="4"/>
<contactref element="IC25" pad="11"/>
</signal>
<signal name="DX2">
<contactref element="E1" pad="5"/>
<contactref element="IC4" pad="16"/>
<contactref element="IC5" pad="18"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC13" pad="7"/>
<contactref element="IC25" pad="10"/>
</signal>
<signal name="DX3">
<contactref element="E1" pad="4"/>
<contactref element="IC4" pad="18"/>
<contactref element="IC5" pad="19"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC13" pad="8"/>
<contactref element="IC25" pad="9"/>
</signal>
<signal name="DX4">
<contactref element="E2" pad="11"/>
<contactref element="IC3" pad="12"/>
<contactref element="IC5" pad="20"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC12" pad="18"/>
</signal>
<signal name="DX5">
<contactref element="E2" pad="13"/>
<contactref element="IC3" pad="14"/>
<contactref element="IC5" pad="21"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC12" pad="17"/>
<contactref element="IC18" pad="2"/>
</signal>
<signal name="DX6">
<contactref element="E2" pad="5"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC5" pad="22"/>
<contactref element="IC1" pad="22"/>
<contactref element="IC12" pad="14"/>
</signal>
<signal name="DX7">
<contactref element="E2" pad="4"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC5" pad="23"/>
<contactref element="IC1" pad="23"/>
<contactref element="IC12" pad="13"/>
</signal>
<signal name="DX8">
<contactref element="E3" pad="11"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC5" pad="24"/>
<contactref element="IC1" pad="24"/>
<contactref element="IC12" pad="8"/>
</signal>
<signal name="DX9">
<contactref element="E3" pad="13"/>
<contactref element="IC2" pad="14"/>
<contactref element="IC5" pad="25"/>
<contactref element="IC1" pad="25"/>
<contactref element="IC12" pad="7"/>
<contactref element="IC25" pad="8"/>
</signal>
<signal name="DX10">
<contactref element="E3" pad="5"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC5" pad="27"/>
<contactref element="IC1" pad="27"/>
<contactref element="IC12" pad="4"/>
<contactref element="IC25" pad="7"/>
</signal>
<signal name="!XTB">
<contactref element="E3" pad="12"/>
<contactref element="E2" pad="12"/>
<contactref element="E1" pad="12"/>
<contactref element="IC6" pad="12"/>
</signal>
<signal name="!SKP!/!INT">
<contactref element="IC5" pad="35"/>
<contactref element="IC1" pad="35"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="!C0">
<contactref element="IC5" pad="32"/>
<contactref element="IC1" pad="32"/>
<contactref element="IC21" pad="2"/>
</signal>
<signal name="!C1">
<contactref element="IC5" pad="33"/>
<contactref element="IC1" pad="33"/>
<contactref element="IC21" pad="4"/>
</signal>
<signal name="!RESET">
<contactref element="IC5" pad="7"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC10" pad="1"/>
<contactref element="IC10" pad="13"/>
<contactref element="IC18" pad="13"/>
</signal>
<signal name="!DEVSEL">
<contactref element="IC1" pad="30"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC11" pad="2"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="!MEMSEL">
<contactref element="IC5" pad="4"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="IFETCH">
<contactref element="IC5" pad="5"/>
<contactref element="IC1" pad="36"/>
<contactref element="IC25" pad="2"/>
</signal>
<signal name="LXMAR">
<contactref element="IC5" pad="10"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC13" pad="11"/>
<contactref element="IC12" pad="11"/>
</signal>
<signal name="XTC">
<contactref element="IC5" pad="13"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC7" pad="6"/>
</signal>
<signal name="XTA">
<contactref element="IC5" pad="9"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC6" pad="11"/>
<contactref element="IC24" pad="1"/>
<contactref element="IC25" pad="3"/>
</signal>
<signal name="INTGNT">
<contactref element="IC5" pad="39"/>
<contactref element="IC1" pad="39"/>
</signal>
<signal name="DMAGNT">
<contactref element="IC5" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC5" pad="14"/>
<contactref element="IC5" pad="31"/>
</signal>
<signal name="OSCIN">
<contactref element="IC1" pad="15"/>
</signal>
<signal name="OSCOUT">
<contactref element="IC1" pad="14"/>
</signal>
<signal name="RUN/!HLT">
<contactref element="IC1" pad="6"/>
</signal>
<signal name="!DMAREQ">
<contactref element="IC1" pad="4"/>
</signal>
<signal name="!CPREQ">
<contactref element="IC1" pad="5"/>
<contactref element="IC10" pad="4"/>
<contactref element="IC10" pad="10"/>
<contactref element="IC21" pad="6"/>
</signal>
<signal name="!WAIT">
<contactref element="IC1" pad="11"/>
</signal>
<signal name="!CPSEL">
<contactref element="IC1" pad="38"/>
<contactref element="IC25" pad="5"/>
</signal>
<signal name="DATAF">
<contactref element="IC1" pad="40"/>
</signal>
<signal name="XTB">
<contactref element="IC1" pad="12"/>
<contactref element="IC6" pad="13"/>
</signal>
<signal name="RUN">
<contactref element="IC1" pad="2"/>
<contactref element="IC6" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="E6" pad="11"/>
<contactref element="IC8" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="E6" pad="13"/>
<contactref element="IC8" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="E6" pad="5"/>
<contactref element="IC8" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="E6" pad="4"/>
<contactref element="IC8" pad="9"/>
</signal>
<signal name="N$7">
<contactref element="E5" pad="11"/>
<contactref element="IC8" pad="12"/>
</signal>
<signal name="N$8">
<contactref element="E5" pad="13"/>
<contactref element="IC8" pad="15"/>
</signal>
<signal name="N$9">
<contactref element="E5" pad="5"/>
<contactref element="IC9" pad="15"/>
</signal>
<signal name="N$10">
<contactref element="E5" pad="4"/>
<contactref element="IC9" pad="12"/>
</signal>
<signal name="N$11">
<contactref element="E4" pad="11"/>
<contactref element="IC9" pad="9"/>
</signal>
<signal name="N$12">
<contactref element="E4" pad="5"/>
<contactref element="IC9" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="E4" pad="13"/>
<contactref element="IC9" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="E4" pad="4"/>
<contactref element="IC9" pad="2"/>
</signal>
<signal name="!XTA">
<contactref element="IC4" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="DATA0">
<contactref element="IC8" pad="3"/>
<contactref element="E1" pad="10"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="DATA1">
<contactref element="IC8" pad="4"/>
<contactref element="E1" pad="14"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="DATA2">
<contactref element="IC8" pad="7"/>
<contactref element="E1" pad="6"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="DATA3">
<contactref element="IC8" pad="8"/>
<contactref element="E1" pad="3"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="DATA4">
<contactref element="IC8" pad="13"/>
<contactref element="E2" pad="10"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="DATA5">
<contactref element="IC8" pad="14"/>
<contactref element="E2" pad="14"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="DATA6">
<contactref element="IC9" pad="14"/>
<contactref element="E2" pad="6"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="DATA7">
<contactref element="IC9" pad="13"/>
<contactref element="E2" pad="3"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="DATA8">
<contactref element="IC9" pad="8"/>
<contactref element="E3" pad="10"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="DATA9">
<contactref element="IC9" pad="7"/>
<contactref element="E3" pad="14"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="DATA10">
<contactref element="IC9" pad="4"/>
<contactref element="E3" pad="6"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="DATA11">
<contactref element="IC9" pad="3"/>
<contactref element="E3" pad="3"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="!LXMAR">
<contactref element="IC9" pad="11"/>
<contactref element="IC8" pad="11"/>
</signal>
<signal name="INT_RQST">
<contactref element="E7" pad="14"/>
<contactref element="IC11" pad="1"/>
</signal>
<signal name="C0">
<contactref element="E7" pad="3"/>
<contactref element="IC21" pad="1"/>
</signal>
<signal name="C1">
<contactref element="E7" pad="6"/>
<contactref element="IC21" pad="3"/>
</signal>
<signal name="SKIP">
<contactref element="E7" pad="10"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="!TP3">
<contactref element="IC6" pad="8"/>
<contactref element="E8" pad="5"/>
</signal>
<signal name="DEVSEL">
<contactref element="E8" pad="4"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC24" pad="2"/>
</signal>
<signal name="TP3">
<contactref element="IC6" pad="9"/>
<contactref element="IC7" pad="4"/>
</signal>
<signal name="!SKPX!/!INTX">
<contactref element="IC7" pad="1"/>
<contactref element="IC5" pad="15"/>
</signal>
<signal name="N$2">
<contactref element="IC7" pad="3"/>
<contactref element="IC11" pad="3"/>
</signal>
<signal name="!FZ">
<contactref element="IC11" pad="13"/>
<contactref element="IC11" pad="10"/>
<contactref element="IC11" pad="5"/>
<contactref element="IC10" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="IC11" pad="9"/>
<contactref element="IC5" pad="37"/>
</signal>
<signal name="N$17">
<contactref element="IC5" pad="36"/>
<contactref element="IC11" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="IC11" pad="12"/>
<contactref element="IC5" pad="38"/>
</signal>
<signal name="EA1">
<contactref element="IC11" pad="8"/>
<contactref element="E9" pad="5"/>
<contactref element="IC13" pad="14"/>
</signal>
<signal name="EA0">
<contactref element="IC11" pad="6"/>
<contactref element="E9" pad="11"/>
<contactref element="IC13" pad="13"/>
</signal>
<signal name="EA2">
<contactref element="IC11" pad="11"/>
<contactref element="E9" pad="4"/>
<contactref element="IC13" pad="17"/>
</signal>
<signal name="PDF">
<contactref element="IC10" pad="9"/>
</signal>
<signal name="!PDF">
<contactref element="IC10" pad="8"/>
</signal>
<signal name="CPDSPD">
<contactref element="IC10" pad="11"/>
<contactref element="IC10" pad="3"/>
<contactref element="IC24" pad="15"/>
</signal>
<signal name="VSS">
<contactref element="IC20" pad="16"/>
<contactref element="IC14" pad="14"/>
<contactref element="IC15" pad="14"/>
<contactref element="U$3" pad="16"/>
<contactref element="U$4" pad="16"/>
</signal>
<signal name="EMA1">
<contactref element="IC13" pad="15"/>
<contactref element="IC16" pad="26"/>
</signal>
<signal name="MA11">
<contactref element="IC12" pad="2"/>
<contactref element="IC16" pad="10"/>
<contactref element="IC24" pad="4"/>
</signal>
<signal name="MA10">
<contactref element="IC12" pad="5"/>
<contactref element="IC16" pad="9"/>
<contactref element="IC24" pad="5"/>
</signal>
<signal name="MA9">
<contactref element="IC12" pad="6"/>
<contactref element="IC16" pad="8"/>
<contactref element="IC24" pad="6"/>
</signal>
<signal name="MA8">
<contactref element="IC12" pad="9"/>
<contactref element="IC16" pad="7"/>
<contactref element="IC10" pad="12"/>
<contactref element="IC24" pad="7"/>
</signal>
<signal name="MA7">
<contactref element="IC12" pad="12"/>
<contactref element="IC16" pad="6"/>
<contactref element="IC24" pad="8"/>
</signal>
<signal name="MA6">
<contactref element="IC12" pad="15"/>
<contactref element="IC16" pad="5"/>
<contactref element="IC24" pad="9"/>
</signal>
<signal name="MA5">
<contactref element="IC12" pad="16"/>
<contactref element="IC16" pad="4"/>
<contactref element="IC24" pad="10"/>
</signal>
<signal name="MA4">
<contactref element="IC12" pad="19"/>
<contactref element="IC16" pad="3"/>
<contactref element="IC24" pad="11"/>
</signal>
<signal name="MA0">
<contactref element="IC13" pad="2"/>
<contactref element="IC16" pad="23"/>
</signal>
<signal name="MA1">
<contactref element="IC13" pad="5"/>
<contactref element="IC16" pad="21"/>
</signal>
<signal name="MA2">
<contactref element="IC13" pad="6"/>
<contactref element="IC16" pad="24"/>
</signal>
<signal name="MA3">
<contactref element="IC13" pad="9"/>
<contactref element="IC16" pad="25"/>
<contactref element="IC24" pad="13"/>
</signal>
<signal name="EMA0">
<contactref element="IC13" pad="12"/>
<contactref element="IC16" pad="27"/>
</signal>
<signal name="EMA2">
<contactref element="IC13" pad="16"/>
<contactref element="IC16" pad="2"/>
</signal>
<signal name="!UF">
<contactref element="IC18" pad="8"/>
</signal>
<signal name="UF">
<contactref element="IC18" pad="9"/>
<contactref element="IC25" pad="4"/>
</signal>
<signal name="!CUF">
<contactref element="IC18" pad="1"/>
<contactref element="IC24" pad="21"/>
</signal>
<signal name="!CINT">
<contactref element="IC24" pad="23"/>
<contactref element="IC22" pad="1"/>
</signal>
<signal name="!SINT">
<contactref element="IC24" pad="22"/>
<contactref element="IC23" pad="3"/>
</signal>
<signal name="!SUF">
<contactref element="IC18" pad="4"/>
<contactref element="IC24" pad="20"/>
</signal>
<signal name="!RTF">
<contactref element="IC24" pad="18"/>
</signal>
<signal name="!CAF">
<contactref element="IC24" pad="17"/>
</signal>
<signal name="!GTF">
<contactref element="IC24" pad="19"/>
</signal>
<signal name="!NDEVSEL">
<contactref element="IC5" pad="30"/>
<contactref element="IC24" pad="16"/>
</signal>
<signal name="RTF">
<contactref element="IC18" pad="3"/>
</signal>
<signal name="!IOT">
<contactref element="IC24" pad="3"/>
<contactref element="IC25" pad="20"/>
</signal>
<signal name="XTAFETCH">
<contactref element="IC25" pad="1"/>
<contactref element="IC25" pad="23"/>
</signal>
<signal name="!HLT">
<contactref element="IC25" pad="22"/>
</signal>
<signal name="!PRV">
<contactref element="IC25" pad="19"/>
</signal>
<signal name="!OSR">
<contactref element="IC25" pad="21"/>
</signal>
<signal name="!IBIF">
<contactref element="IC25" pad="18"/>
<contactref element="IC18" pad="11"/>
</signal>
<signal name="UB">
<contactref element="IC18" pad="5"/>
<contactref element="IC18" pad="12"/>
</signal>
<signal name="TSIOT">
<contactref element="IC24" pad="14"/>
</signal>
<signal name="FNOP">
<contactref element="IC25" pad="17"/>
<contactref element="IC7" pad="9"/>
<contactref element="IC7" pad="11"/>
<contactref element="IC22" pad="3"/>
</signal>
<signal name="!SWSEL">
<contactref element="IC7" pad="12"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="SWSEL">
<contactref element="IC7" pad="13"/>
</signal>
<signal name="!RUN">
<contactref element="IC6" pad="2"/>
<contactref element="IC21" pad="5"/>
<contactref element="IC23" pad="2"/>
</signal>
<signal name="UINT">
<contactref element="IC22" pad="5"/>
</signal>
<signal name="!UINT">
<contactref element="IC22" pad="6"/>
</signal>
<signal name="!RUN!/!HLT">
<contactref element="IC23" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
