<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="48.26" y1="43.18" x2="2.54" y2="43.18" width="0" layer="20"/>
<wire x1="0" y1="40.64" x2="2.54" y2="43.18" width="0" layer="20" curve="-90"/>
<wire x1="48.26" y1="43.18" x2="50.8" y2="40.64" width="0" layer="20" curve="-90"/>
<wire x1="50.8" y1="40.64" x2="50.8" y2="2.54" width="0" layer="20"/>
<wire x1="50.8" y1="2.54" x2="48.26" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="2.54" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="0" y1="40.64" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="17.562103125" x2="3.81" y2="25.617896875" width="0" layer="46"/>
<wire x1="11.847103125" y1="33.02" x2="40.857896875" y2="33.02" width="0" layer="46"/>
<wire x1="45.085" y1="28.792896875" x2="45.085" y2="14.387103125" width="0" layer="46"/>
<text>1.2 mm PCB strength</text>
<hole x="7.62" y="6.35" drill="3.2"/>
<hole x="7.62" y="36.83" drill="3.2"/>
<hole x="43.18" y="36.83" drill="3.2"/>
<hole x="43.18" y="6.35" drill="3.2"/>
<text>need 4 per device</text>
<wire x1="38.1" y1="10.16" x2="11.847103125" y2="10.16" width="0" layer="46"/>
<wire x1="3.81" y1="25.617896875" x2="4.55395" y2="28.04895" width="0" layer="46" curve="-45.00005"/>
<wire x1="4.55395" y1="28.04895" x2="8.14605" y2="31.64105" width="0" layer="46"/>
<wire x1="8.14605" y1="31.64105" x2="11.847103125" y2="33.02" width="0" layer="46" curve="-45.00007"/>
<wire x1="3.81" y1="17.562103125" x2="4.55395" y2="15.13105" width="0" layer="46" curve="45.00005"/>
<wire x1="4.55395" y1="15.13105" x2="8.14605" y2="11.53895" width="0" layer="46"/>
<wire x1="8.14605" y1="11.53895" x2="11.847103125" y2="10.16" width="0" layer="46" curve="45.00007"/>
<wire x1="40.857896875" y1="33.02" x2="42.65395" y2="32.27605" width="0" layer="46" curve="-45.00005"/>
<wire x1="42.65395" y1="32.27605" x2="44.34105" y2="30.58895" width="0" layer="46"/>
<wire x1="44.34105" y1="30.58895" x2="45.085" y2="28.792896875" width="0" layer="46" curve="-45.00007"/>
<wire x1="45.085" y1="14.387103125" x2="44.34105" y2="12.59105" width="0" layer="46" curve="-45.00005"/>
<wire x1="44.34105" y1="12.59105" x2="43.18" y2="11.43" width="0" layer="46"/>
<wire x1="43.18" y1="11.43" x2="42.65395" y2="10.90395" width="0" layer="46"/>
<wire x1="42.65395" y1="10.90395" x2="40.857896875" y2="10.16" width="0" layer="46" curve="-45.00007"/>
<wire x1="40.857896875" y1="10.16" x2="38.1" y2="10.16" width="0" layer="46"/>
</plain>
<libraries>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
</elements>
<signals>
<signal name="N$1">
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
