<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<packages>
<package name="PETAL-NOHOLE">
</package>
<package name="BUTTONHOLE-SM">
</package>
<package name="BUTTONHOLE">
</package>
<package name="LOGO-LILYPAD">
</package>
<package name="LOGO-A">
</package>
<package name="LOGO-LPA">
</package>
<package name="LOGO-L">
</package>
<package name="PETAL-LONG-1">
</package>
<package name="PETAL-LONG-2">
</package>
<package name="PETAL-MEDIUM">
</package>
<package name="PETAL-LARGE">
</package>
<package name="PETAL-SMALL">
</package>
<package name="LED-1206">
</package>
<package name="PETAL-SMALL-2SIDE">
</package>
<package name="PETAL-NOHOLE-2SIDE">
</package>
<package name="PETAL-LARGE-2SIDE">
</package>
<package name="PETAL-MEDIUM-2SIDE">
</package>
<package name="PETAL-LONG-1-2SIDE">
</package>
<package name="PETAL-LONG-2-2SIDE">
</package>
<package name="LOGO-L-TINY">
</package>
<package name="PETAL-TINY">
</package>
<package name="PETAL-MEDIUM-2SIDE-NOHOLE">
</package>
<package name="PETAL-MEDIUM-NOHOLE">
</package>
<package name="SIMPLE_HOLE">
</package>
<package name="SIMPLE_HOLE_SM">
</package>
</packages>
<symbols>
<symbol name="BUTTONHOLE">
<pin name="P$1"/>
</symbol>
<symbol name="LETTER_L">
</symbol>
<symbol name="DOCFIELD">
</symbol>
<symbol name="SEWTAP-NOHOLE">
</symbol>
<symbol name="SEWTAP">
<pin name="1"/>
</symbol>
<symbol name="LOGO-LP">
</symbol>
<symbol name="SEWTAP-NEW">
<pin name="1"/>
</symbol>
<symbol name="LED">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SIMPLE_HOLE">
<pin name="P$1"/>
</symbol>
<symbol name="SIMPLE_HOLE_SM">
<pin name="P$1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BUTTONHOLE" prefix="BH">
<gates>
<gate name="G$1" symbol="BUTTONHOLE"/>
</gates>
<devices>
<device name="LARGE" package="BUTTONHOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL" package="BUTTONHOLE-SM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEWTAP-NOHOLE">
<gates>
<gate name="G$1" symbol="SEWTAP-NOHOLE"/>
</gates>
<devices>
<device name="1" package="PETAL-NOHOLE">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="PETAL-NOHOLE-2SIDE">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3" package="PETAL-MEDIUM-2SIDE-NOHOLE">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4" package="PETAL-MEDIUM-NOHOLE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LEDs&lt;/b&gt;
Standard schematic elements and footprints for 5mm, 3mm, 1206, and 0603 sized LEDs. 5mm - Spark Fun Electronics SKU : Comp-SBL</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-LP">
<gates>
<gate name="G$1" symbol="LOGO-LP"/>
</gates>
<devices>
<device name="LP" package="LOGO-LILYPAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LPA" package="LOGO-LPA">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="LOGO-L">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L-TINY" package="LOGO-L-TINY">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ARDUINO_ONLY" package="LOGO-A">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEWTAP">
<gates>
<gate name="G$1" symbol="SEWTAP"/>
</gates>
<devices>
<device name="1" package="PETAL-LONG-1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="PETAL-LONG-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3" package="PETAL-MEDIUM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5" package="PETAL-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4" package="PETAL-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6" package="PETAL-SMALL-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="7" package="PETAL-LARGE-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8" package="PETAL-MEDIUM-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="9" package="PETAL-LONG-1-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10" package="PETAL-LONG-2-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="11" package="PETAL-TINY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEW_HOLE" prefix="H">
<description>Simple sew-hole&lt;br&gt;
.1" diameter hole with 20mil annular ring</description>
<gates>
<gate name="G$1" symbol="SIMPLE_HOLE"/>
</gates>
<devices>
<device name="" package="SIMPLE_HOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEW_HOLE-SMALL" prefix="H">
<description>.070" hole with 20mil annular ring</description>
<gates>
<gate name="G$1" symbol="SIMPLE_HOLE_SM"/>
</gates>
<devices>
<device name="" package="SIMPLE_HOLE_SM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
