<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT363">
</package>
<package name="CNZ1120">
</package>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="DIODE-1N4001">
</package>
<package name="SOD-323">
</package>
<package name="SOT23-3">
</package>
<package name="DIODE-1N4148">
</package>
<package name="SMB-DIODE">
<description>&lt;b&gt;Diode&lt;/b&gt;&lt;p&gt;
Basic small signal diode good up to 200mA. SMB footprint. Common part #: BAS16</description>
</package>
<package name="DIODE-HV">
</package>
<package name="SMA-DIODE_ALT">
</package>
<package name="SMA-DIODE-KIT">
</package>
<package name="DIODE-ZENER">
</package>
<package name="GP1A57HR">
</package>
<package name="SC70">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="DIL06">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="DPAK">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="8-SMD">
</package>
<package name="SSOP-4">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOT89">
</package>
<package name="TO-92-AMMO">
</package>
<package name="V18ZA2P">
</package>
<package name="0603-RES">
</package>
<package name="DIP8SMD">
</package>
<package name="SMC">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT23-6">
</package>
<package name="POWERPAK1212-8">
<description>Vishay PowerPAK 1212-8 single device package&lt;br&gt;
High-power, low thermal resistance package.</description>
</package>
<package name="SOD-523">
</package>
<package name="SOD523">
</package>
<package name="SOT323">
</package>
</packages>
<symbols>
<symbol name="BAV99">
<pin name="A1"/>
<pin name="C2"/>
<pin name="COM"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="CNZ1120">
<pin name="2"/>
<pin name="1"/>
<pin name="4"/>
<pin name="3"/>
</symbol>
<symbol name="DIODE">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DIODE-SCHOTTKY">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DIODE-ZENER">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="GP1A57HR">
<pin name="2"/>
<pin name="1"/>
<pin name="5"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="HALL-EFFECT">
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="ILD213T">
<pin name="C2"/>
<pin name="A2"/>
<pin name="C1"/>
<pin name="A1"/>
<pin name="ET2"/>
<pin name="CT2"/>
<pin name="ET1"/>
<pin name="CT1"/>
</symbol>
<symbol name="IRF7507">
<pin name="S1"/>
<pin name="G1"/>
<pin name="S2"/>
<pin name="G2"/>
<pin name="D2@5"/>
<pin name="D2@6"/>
<pin name="D1@7"/>
<pin name="D1@8"/>
</symbol>
<symbol name="TVS">
<pin name="A1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="MOC3031-M">
<pin name="1"/>
<pin name="2"/>
<pin name="6"/>
<pin name="4"/>
</symbol>
<symbol name="MOSFET-NCHANNEL">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="IRF9410">
<pin name="S@1"/>
<pin name="S@2"/>
<pin name="S@3"/>
<pin name="G"/>
<pin name="D@1"/>
<pin name="D@2"/>
<pin name="D@3"/>
<pin name="D@4"/>
</symbol>
<symbol name="MOSFET-PCHANNEL">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="NDS8434-1">
<pin name="D@1"/>
<pin name="D@2"/>
<pin name="D@3"/>
<pin name="D@4"/>
<pin name="G"/>
<pin name="S@1"/>
<pin name="S@2"/>
<pin name="S@3"/>
</symbol>
<symbol name="OPTOTRIAC_ZC">
<pin name="A"/>
<pin name="K"/>
<pin name="T2"/>
<pin name="T1"/>
</symbol>
<symbol name="NDS8434">
<pin name="S@1"/>
<pin name="S@2"/>
<pin name="S@3"/>
<pin name="G"/>
<pin name="D@1"/>
<pin name="D@2"/>
<pin name="D@3"/>
<pin name="D@4"/>
</symbol>
<symbol name="OPTO_DARLINGTON_6N138-39">
<pin name="C"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="VOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="TCMT1103">
<pin name="C"/>
<pin name="E"/>
<pin name="K"/>
<pin name="A"/>
</symbol>
<symbol name="TRIAC">
<pin name="M2"/>
<pin name="M1"/>
<pin name="G"/>
</symbol>
<symbol name="SCHOTTKY_BRIDGE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="V18ZA2P">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="VARISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="XN04312">
<pin name="E2"/>
<pin name="B2"/>
<pin name="C1"/>
<pin name="E1"/>
<pin name="B1"/>
<pin name="C2"/>
</symbol>
<symbol name="IRF7509_NMOS">
<pin name="G1"/>
<pin name="S1"/>
<pin name="D1"/>
</symbol>
<symbol name="IRF7509_PMOS">
<pin name="G2"/>
<pin name="S2"/>
<pin name="D2"/>
</symbol>
<symbol name="MOSFET-NCHANNEL-1">
<pin name="D" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BAV99" prefix="D" uservalue="yes">
<description>Two small signal silicon diodes connected anode to cathode.&lt;br&gt;
Connections to all three nodes available.&lt;br&gt;
DIO-10647</description>
<gates>
<gate name="G$1" symbol="BAV99"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="C2" pad="2"/>
<connect gate="G$1" pin="COM" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10647"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC847PN">
<description>NPN/PNP transistor pair in SOT-363 package</description>
<gates>
<gate name="G1" symbol="PNP"/>
<gate name="G2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G1" pin="B" pad="2"/>
<connect gate="G1" pin="C" pad="6"/>
<connect gate="G1" pin="E" pad="1"/>
<connect gate="G2" pin="B" pad="5"/>
<connect gate="G2" pin="C" pad="3"/>
<connect gate="G2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CNZ1120">
<description>LED-to-NPN optoisolator</description>
<gates>
<gate name="G$1" symbol="CNZ1120"/>
</gates>
<devices>
<device name="PTH" package="CNZ1120">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-SCHOTTKY" prefix="D">
<description>Commonly MBRA140.</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="_" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOD-523">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-ZENER">
<description>Zener Diode
Production Part - 8199
3.4V Zener Voltage</description>
<gates>
<gate name="G$1" symbol="DIODE-ZENER"/>
</gates>
<devices>
<device name="PTH" package="DIODE-ZENER">
<connects>
<connect gate="G$1" pin="A" pad="P$2"/>
<connect gate="G$1" pin="C" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BZT52" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GP1A57HR">
<description>Optoisolator with 15k built-in bias resistor.</description>
<gates>
<gate name="G$1" symbol="GP1A57HR"/>
</gates>
<devices>
<device name="" package="GP1A57HR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ILD213T" prefix="IC">
<description>Dual optoisolator.</description>
<gates>
<gate name="G$1" symbol="ILD213T"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="4"/>
<connect gate="G$1" pin="CT1" pad="6"/>
<connect gate="G$1" pin="CT2" pad="8"/>
<connect gate="G$1" pin="ET1" pad="5"/>
<connect gate="G$1" pin="ET2" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOC3063*" prefix="U" uservalue="yes">
<description>&lt;b&gt;Optotriac in DIP and SMD&lt;/b&gt;
&lt;p&gt;
LED:&lt;br&gt;
Vf: 1.2V&lt;br&gt;
If: 5 mA&lt;br&gt;
&lt;p&gt;
TRIAC&lt;br&gt;
Vdrm: 600V&lt;br&gt;
Itsm: 1A&lt;br&gt;
Viso: 5000V&lt;br&gt;
DV/dt: 1500V/us&lt;br&gt;
&lt;p&gt;
DIP: MOC3063&lt;br&gt;
SMD: MOC3063S</description>
<gates>
<gate name="G$1" symbol="OPTOTRIAC_ZC"/>
</gates>
<devices>
<device name="S" package="DIP8SMD">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="T1" pad="6"/>
<connect gate="G$1" pin="T2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMBZ27VCLT1">
<description>40W Zener-diode transient voltage suppressor (ESD protection)</description>
<gates>
<gate name="G$1" symbol="TVS"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MMDT3904">
<description>Dual NPN transistor</description>
<gates>
<gate name="G$1" symbol="NPN"/>
<gate name="G$2" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT363">
<connects>
<connect gate="G$1" pin="B" pad="5"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$2" pin="B" pad="2"/>
<connect gate="G$2" pin="C" pad="6"/>
<connect gate="G$2" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOC3031-M">
<description>Opto-isolated TRIAC</description>
<gates>
<gate name="G$1" symbol="MOC3031-M"/>
</gates>
<devices>
<device name="" package="DIL06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-NCHANNEL-SOIC8">
<description>IRF9410 and NDS8434 SOIC-8 parts.</description>
<gates>
<gate name="G$1" symbol="IRF9410"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="D@1" pad="8"/>
<connect gate="G$1" pin="D@2" pad="7"/>
<connect gate="G$1" pin="D@3" pad="6"/>
<connect gate="G$1" pin="D@4" pad="5"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S@1" pad="1"/>
<connect gate="G$1" pin="S@2" pad="2"/>
<connect gate="G$1" pin="S@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-PCHANNEL" prefix="Q">
<description>Generic PMOSFET</description>
<gates>
<gate name="G$1" symbol="MOSFET-PCHANNEL"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-PCHANNEL-SOIC8">
<description>Generic 8-pin PMOSFET</description>
<gates>
<gate name="G$1" symbol="NDS8434-1"/>
</gates>
<devices>
<device name="SOIC8" package="SO08">
<connects>
<connect gate="G$1" pin="D@1" pad="5"/>
<connect gate="G$1" pin="D@2" pad="6"/>
<connect gate="G$1" pin="D@3" pad="7"/>
<connect gate="G$1" pin="D@4" pad="8"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S@1" pad="1"/>
<connect gate="G$1" pin="S@2" pad="2"/>
<connect gate="G$1" pin="S@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NDS8434">
<description>8-SOIC NMOSFET</description>
<gates>
<gate name="G$1" symbol="NDS8434"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="D@1" pad="7"/>
<connect gate="G$1" pin="D@2" pad="8"/>
<connect gate="G$1" pin="D@3" pad="6"/>
<connect gate="G$1" pin="D@4" pad="5"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S@1" pad="1"/>
<connect gate="G$1" pin="S@2" pad="2"/>
<connect gate="G$1" pin="S@3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPTO_DARL_6N138S">
<description>Optoisolator, darlington pair output</description>
<gates>
<gate name="G$1" symbol="OPTO_DARLINGTON_6N138-39"/>
</gates>
<devices>
<device name="" package="8-SMD">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCMT1103-OPTO">
<description>Optoisolator- NPN output</description>
<gates>
<gate name="G$1" symbol="TCMT1103"/>
</gates>
<devices>
<device name="" package="SSOP-4">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_NPN" prefix="Q" uservalue="yes">
<description>Generic NPN BJT. MMBT2222 is the common NPN we use. Double check against datasheet- not all devices are the same!</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23-3" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="&quot;" package="SOT223">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT89" package="SOT89">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO-92-AMMO" package="TO-92-AMMO">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_NPN_2">
<description>Alternate TO-92 NPN BJT</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSISTOR_PNP" prefix="Q">
<description>Generic PNP BJT. Double check pinouts against datasheets- not all devices are the same!</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO92" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SOT89">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIAC">
<description>Low-power generic TRIAC packages</description>
<gates>
<gate name="G$1" symbol="TRIAC"/>
</gates>
<devices>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="M1" pad="1"/>
<connect gate="G$1" pin="M2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOT223">
<connects>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="M1" pad="1"/>
<connect gate="G$1" pin="M2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVS">
<description>Transient voltage suppressor- prevents ESD on inputs.&lt;br&gt;
Ignore package description- MBRA140 is NOT this type of part!!!</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY_BRIDGE"/>
</gates>
<devices>
<device name="" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="1" pad="A"/>
<connect gate="G$1" pin="2" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V-REFERENCE">
<description>Zener diode</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V18ZA2P">
<description>Varistor</description>
<gates>
<gate name="G$1" symbol="V18ZA2P"/>
</gates>
<devices>
<device name="" package="V18ZA2P">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VARISTOR" prefix="Z" uservalue="yes">
<description>&lt;h3&gt;Varistor&lt;/h3&gt;
Varistor (Variable resistor) is a nonlinear resistive element of the
voltage dependence that resistance changes with applied voltage.
Varistor is equivalent with Zener diode of two series connection.</description>
<gates>
<gate name="G$1" symbol="VARISTOR"/>
</gates>
<devices>
<device name="-0603" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XN04312">
<description>&lt;b&gt;NPN/PNP Transistor Array&lt;/b&gt;
Handy dandy transistor array for level shifting and inverting signals. Spark Fun Electronics SKU : COM-00588</description>
<gates>
<gate name="G$1" symbol="XN04312"/>
</gates>
<devices>
<device name="SOT" package="SOT23-6">
<connects>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="2"/>
<connect gate="G$1" pin="C1" pad="1"/>
<connect gate="G$1" pin="C2" pad="4"/>
<connect gate="G$1" pin="E1" pad="6"/>
<connect gate="G$1" pin="E2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;b&gt;Diode&lt;/b&gt;
These are standard reverse protection diodes and small signal diodes. SMA package can handle up to about 1A. SOD-323 can handle about 200mA. What the SOD-323 package when ordering, there are some mfgs out there that are 5-pin packages.</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="SMA" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="DIODE-1N4001">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1N4148" package="DIODE-1N4148">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMB" package="SMB-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HV" package="DIODE-HV">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMA-ALT" package="SMA-DIODE_ALT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMA-KIT" package="SMA-DIODE-KIT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD523" package="SOD523">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMC/DO-214AB" package="SMC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-NCHANNEL" prefix="Q">
<description>Generic NMOS footprint</description>
<gates>
<gate name="G$1" symbol="MOSFET-NCHANNEL-1"/>
</gates>
<devices>
<device name="FDD8580" package="DPAK">
<connects>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="TO220V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT323" package="SOT323">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SI7820DN" package="POWERPAK1212-8">
<connects>
<connect gate="G$1" pin="D" pad="D1 D2 D3 D4 DPAD"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S1 S2 S3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF7509" prefix="Q" uservalue="yes">
<description>30V Dual PMOS/NMOS MSOP-8&lt;BR&gt;
NMOS RDS .11-ohm&lt;BR&gt;
PMOS RDS .20-ohm&lt;BR&gt;
TRANS-07913</description>
<gates>
<gate name="NMOS" symbol="MOSFET-NCHANNEL"/>
<gate name="PMOS" symbol="MOSFET-PCHANNEL"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="NMOS" pin="D" pad="7 8"/>
<connect gate="NMOS" pin="G" pad="2"/>
<connect gate="NMOS" pin="S" pad="1"/>
<connect gate="PMOS" pin="D" pad="5 6"/>
<connect gate="PMOS" pin="G" pad="4"/>
<connect gate="PMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-07913"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBRA140" prefix="D">
<description>40V, 1A Schottky rectifier&lt;br&gt;
SMA/DO-214AC package&lt;br&gt;
DIO-08053</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08053"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BSS138" prefix="Q" uservalue="yes">
<description>NMOSFET, Enh Mode&lt;br&gt;
50V/6-ohm 200mA (SOT-23)&lt;br&gt;
TRANS-00830</description>
<gates>
<gate name="G$1" symbol="MOSFET-NCHANNEL"/>
</gates>
<devices>
<device name="TRANS-00830" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE" value="BSS138"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="B340A" prefix="D" uservalue="yes">
<description>Schottky Diode&lt;br&gt;
3A-40V</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09886"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RB751" prefix="D" uservalue="yes">
<description>40V 120mA SOD-523 Schottky&lt;br&gt;
DIO-11018</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="" package="SOD-523">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11018"/>
<attribute name="VALUE" value="RB751"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
